(kicad_pcb
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(general
		(thickness 1.6)
		(legacy_teardrops no)
	)
	(paper "A4")
	(layers
		(0 "F.Cu" signal)
		(4 "In1.Cu" signal "GND")
		(6 "In2.Cu" signal "VCC")
		(2 "B.Cu" signal)
		(9 "F.Adhes" user "F.Adhesive")
		(11 "B.Adhes" user "B.Adhesive")
		(13 "F.Paste" user)
		(15 "B.Paste" user)
		(5 "F.SilkS" user "F.Silkscreen")
		(7 "B.SilkS" user "B.Silkscreen")
		(1 "F.Mask" user)
		(3 "B.Mask" user)
		(17 "Dwgs.User" user "User.Drawings")
		(19 "Cmts.User" user "User.Comments")
		(21 "Eco1.User" user "User.Eco1")
		(23 "Eco2.User" user "User.Eco2")
		(25 "Edge.Cuts" user)
		(27 "Margin" user)
		(31 "F.CrtYd" user "F.Courtyard")
		(29 "B.CrtYd" user "B.Courtyard")
		(35 "F.Fab" user)
		(33 "B.Fab" user)
		(39 "User.1" user)
		(41 "User.2" user)
		(43 "User.3" user)
		(45 "User.4" user)
	)
	(setup
		(stackup
			(layer "F.SilkS"
				(type "Top Silk Screen")
			)
			(layer "F.Paste"
				(type "Top Solder Paste")
			)
			(layer "F.Mask"
				(type "Top Solder Mask")
				(color "Purple")
				(thickness 0.01)
			)
			(layer "F.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "dielectric 1"
				(type "prepreg")
				(thickness 0.1)
				(material "FR4")
				(epsilon_r 4.5)
				(loss_tangent 0.02)
			)
			(layer "In1.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "dielectric 2"
				(type "core")
				(thickness 1.24)
				(material "FR4")
				(epsilon_r 4.5)
				(loss_tangent 0.02)
			)
			(layer "In2.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "dielectric 3"
				(type "prepreg")
				(thickness 0.1)
				(material "FR4")
				(epsilon_r 4.5)
				(loss_tangent 0.02)
			)
			(layer "B.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "B.Mask"
				(type "Bottom Solder Mask")
				(color "Purple")
				(thickness 0.01)
			)
			(layer "B.Paste"
				(type "Bottom Solder Paste")
			)
			(layer "B.SilkS"
				(type "Bottom Silk Screen")
			)
			(copper_finish "ENIG")
			(dielectric_constraints no)
		)
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(tenting front back)
		(grid_origin 150.3 100.275)
		(pcbplotparams
			(layerselection 0x00000000_00000000_55555555_5755f5ff)
			(plot_on_all_layers_selection 0x00000000_00000000_00000000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 4)
			(plotframeref no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(pdf_metadata yes)
			(pdf_single_document no)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plot_black_and_white yes)
			(sketchpadsonfab no)
			(plotpadnumbers no)
			(hidednponfab no)
			(sketchdnponfab yes)
			(crossoutdnponfab yes)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 1)
			(scaleselection 1)
			(outputdirectory "")
		)
	)
	(net 0 "")
	(net 1 "GND")
	(net 2 "+3.0V")
	(net 3 "VBUS")
	(net 4 "/+BAT")
	(net 5 "Net-(IC4-DEC)")
	(net 6 "/VSYS")
	(net 7 "+8.7V")
	(net 8 "Net-(IC1-REG)")
	(net 9 "OLED_VDD")
	(net 10 "Net-(ANT1-PadFEED)")
	(net 11 "/VDD_D")
	(net 12 "Net-(O1-VCOMH)")
	(net 13 "/AGDC")
	(net 14 "/VDD_A")
	(net 15 "/VDD_DR")
	(net 16 "/VDD_AM")
	(net 17 "/VDD")
	(net 18 "/XTO")
	(net 19 "/XTI")
	(net 20 "Net-(C1-Pad4)")
	(net 21 "Net-(C42-Pad1)")
	(net 22 "/RFI-")
	(net 23 "Net-(C43-Pad4)")
	(net 24 "/RFI+")
	(net 25 "Net-(C1-Pad3)")
	(net 26 "Net-(IC1-OUT+)")
	(net 27 "/DECD")
	(net 28 "LRA_TRIG")
	(net 29 "Net-(IC1-OUT-)")
	(net 30 "/DECA")
	(net 31 "unconnected-(IC4-NC_4-Pad24)")
	(net 32 "unconnected-(IC4-NC_1-Pad4)")
	(net 33 "BAT_ERR")
	(net 34 "Net-(IC4-NTC)")
	(net 35 "unconnected-(IC4-NC_3-Pad18)")
	(net 36 "Net-(IC4-SW)")
	(net 37 "unconnected-(IC4-NC_2-Pad13)")
	(net 38 "unconnected-(IC4-D+-Pad20)")
	(net 39 "BAT_CHG")
	(net 40 "unconnected-(IC4-D--Pad19)")
	(net 41 "Net-(IC4-ICHG)")
	(net 42 "unconnected-(J2-PadMP2)")
	(net 43 "unconnected-(J2-PadMP1)")
	(net 44 "Net-(PS1-SW)")
	(net 45 "/RFO1")
	(net 46 "/RFO2")
	(net 47 "SH1107_RESET")
	(net 48 "Net-(O1-IREF)")
	(net 49 "unconnected-(O1-NC-Pad13)")
	(net 50 "unconnected-(O1-NC-Pad1)")
	(net 51 "+8.7V_EN")
	(net 52 "Net-(PS1-FB)")
	(net 53 "ENC_OUT_A")
	(net 54 "ENC_OUT_B")
	(net 55 "Net-(AE1-Pad2)")
	(net 56 "Net-(AE1-Pad1)")
	(net 57 "Net-(U2-NRESET)")
	(net 58 "Net-(C53-Pad2)")
	(net 59 "Net-(C54-Pad2)")
	(net 60 "TWIM_SCL")
	(net 61 "TWIM_SDA")
	(net 62 "ACCEL_INT")
	(net 63 "NFC_IRQ")
	(net 64 "BTN_A")
	(net 65 "Net-(J3-Pin_2)")
	(net 66 "BTN_B")
	(net 67 "Net-(J3-Pin_1)")
	(net 68 "/DCC")
	(net 69 "/ANT")
	(net 70 "Net-(R3-Pad2)")
	(net 71 "unconnected-(U2-P1.12{slash}AIN5-Pad40)")
	(net 72 "unconnected-(U2-P2.07{slash}TRACEDATA[0]{slash}SWO{slash}SPI.DCX-Pad18)")
	(net 73 "unconnected-(U2-P0.01-Pad24)")
	(net 74 "unconnected-(U2-P1.13{slash}AIN6-Pad41)")
	(net 75 "unconnected-(U2-P2.04{slash}SPI.SDI{slash}SDO-Pad15)")
	(net 76 "unconnected-(U2-P2.09{slash}TRACEDATA[2]{slash}SPI.SDI{slash}SDO-Pad20)")
	(net 77 "unconnected-(U2-P0.02-Pad27)")
	(net 78 "unconnected-(IC2-EXT_LM-Pad17)")
	(net 79 "unconnected-(IC2-TAD1-Pad25)")
	(net 80 "/AAT_PARALLEL")
	(net 81 "/AAT_SERIES")
	(net 82 "unconnected-(IC2-MOSI-Pad31)")
	(net 83 "unconnected-(IC2-BSS-Pad29)")
	(net 84 "unconnected-(IC2-TAD2-Pad2)")
	(net 85 "unconnected-(IC2-MCU_CLK-Pad28)")
	(net 86 "unconnected-(IC3-INT2-Pad9)")
	(net 87 "unconnected-(Y1-NC_2-Pad4)")
	(net 88 "unconnected-(Y1-NC_1-Pad2)")
	(net 89 "unconnected-(U2-P0.00-Pad23)")
	(net 90 "unconnected-(U2-P0.03{slash}GRTC_PWMOUT-Pad28)")
	(net 91 "unconnected-(U2-P2.08{slash}TRACEDATA[1]{slash}SPI.SDI{slash}SDO-Pad19)")
	(net 92 "unconnected-(U2-P2.03-Pad14)")
	(net 93 "unconnected-(U2-P1.09{slash}TAMPC-Pad37)")
	(net 94 "unconnected-(U2-P0.04{slash}GRTC_CLKOUT32K-Pad29)")
	(net 95 "unconnected-(U2-P1.14{slash}AIN7-Pad42)")
	(net 96 "unconnected-(U2-P2.06{slash}TRACECLK{slash}SPI.SCK-Pad17)")
	(net 97 "unconnected-(U2-P2.05{slash}SPI.CS-Pad16)")
	(net 98 "Net-(U2-XC2)")
	(net 99 "unconnected-(U2-P2.10{slash}TRACEDATA[3]{slash}SPIM.CS-Pad21)")
	(net 100 "Net-(U2-XC1)")
	(net 101 "unconnected-(J4-Pin_9-Pad9)")
	(net 102 "unconnected-(J4-Pin_15-Pad15)")
	(net 103 "unconnected-(J4-Pin_16-Pad16)")
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 162.1 68 90)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C41"
			(at 1.1 0 180)
			(layer "F.SilkS")
		)
		(property "Value" "620pF"
			(at 0 1.16 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "watch.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 90)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 90)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 20 "Net-(C1-Pad4)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 193 72.5)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R7"
			(at 0.4 0.8 0)
			(layer "F.SilkS")
		)
		(property "Value" "R10K"
			(at 0 1.17 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "watch.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "+3.0V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 53 "ENC_OUT_A")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 170 93 90)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C24"
			(at 0.5 0.8 90)
			(layer "F.SilkS")
		)
		(property "Value" "C0.1uF"
			(at 0 1.16 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "watch.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 90)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "+3.0V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 90)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 162.75 77.525 90)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R1"
			(at 0 -0.95 90)
			(layer "F.SilkS")
		)
		(property "Value" "R15k"
			(at 0 1.17 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "watch.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.509999 0 90)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 41 "Net-(IC4-ICHG)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.509999 0 90)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 161 63.75)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C38"
			(at -1.65 0.025 0)
			(layer "F.SilkS")
		)
		(property "Value" "C1uF"
			(at 0 1.16 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "watch.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 17 "/VDD")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "rotary_enc:PUI_HD-LA0503-LW28"
		(layer "F.Cu")
		(at 177.750001 63.8 -90)
		(property "Reference" "B1"
			(at 2.8 0.350001 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "HD-LA0503-LW28"
			(at 8.43 4.115 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTREV" "A"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "STANDARD" "Manufacturer Recommendations"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MAXIMUM_PACKAGE_HEIGHT" "3.2mm"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER" "PUI Audio"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "watch.kicad_sch")
		(attr through_hole)
		(pad "N" thru_hole circle
			(at 10.1 0.750001 270)
			(size 1.008 1.008)
			(drill 0.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 29 "Net-(IC1-OUT-)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "P" thru_hole circle
			(at 10.1 -0.750001 270)
			(size 1.008 1.008)
			(drill 0.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 26 "Net-(IC1-OUT+)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
		(model "${KIPRJMOD}/symbols/HD_LA0503_LW28/HD-LA0503-LW28.step"
			(offset
				(xyz 2 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 -0 90)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0201_0603Metric"
		(layer "F.Cu")
		(at 155.5 96.75 90)
		(descr "Capacitor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C55"
			(at -0.025 -0.7 90)
			(layer "F.SilkS")
		)
		(property "Value" "C0.3pF"
			(at 0 1.05 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Capacitor, C0G, ±0.1 pF, 50 V"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "watch.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -0.68 90)
			(layer "F.Fab")
		)
		(pad "" smd roundrect
			(at -0.345 0 90)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0.345 0 90)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "1" smd roundrect
			(at -0.32 0 90)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.32 0 90)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 10 "Net-(ANT1-PadFEED)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0201_0603Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0201_0603Metric"
		(layer "F.Cu")
		(at 170.1 72.9 180)
		(descr "Capacitor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C30"
			(at -1.6 -0.025 180)
			(layer "F.SilkS")
		)
		(property "Value" "C10nF"
			(at 0 1.05 180)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "watch.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -0.68 180)
			(layer "F.Fab")
		)
		(pad "" smd roundrect
			(at -0.345 0 180)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0.345 0 180)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "1" smd roundrect
			(at -0.32 0 180)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.32 0 180)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 13 "/AGDC")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0201_0603Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "varicap:LXRW0YV201059"
		(layer "F.Cu")
		(at 157.8 67.8)
		(descr "LXRW0YV201-059-2")
		(tags "Capacitor")
		(property "Reference" "C44"
			(at 1.1 -0.225 0)
			(layer "F.SilkS")
		)
		(property "Value" "LXRW0YV201-059"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTREV" "July, 2018"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "STANDARD" "Manufacturer Recommendations"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MAXIMUM_PACKAGE_HEIGHT" "0.3mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER" "Murata"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "watch.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -0.2 0.2 90)
			(size 0.2 0.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pintype "power_in")
		)
		(pad "2" smd rect
			(at -0.2 -0.2 90)
			(size 0.2 0.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 80 "/AAT_PARALLEL")
			(pintype "input")
		)
		(pad "3" smd rect
			(at 0.2 -0.2 90)
			(size 0.2 0.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 25 "Net-(C1-Pad3)")
			(pintype "passive")
		)
		(pad "4" smd rect
			(at 0.2 0.2 90)
			(size 0.2 0.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KIPRJMOD}/symbols/LIB_LXRW0YV201-059(1)/LXRW0YV201-059/3D/LXRW0YV201-059.stp"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "rotary_enc:QFN50P400X400X90-25N-D"
		(layer "F.Cu")
		(at 164 81.275 180)
		(descr "NPM1100-QDAA-R*")
		(tags "Integrated Circuit")
		(property "Reference" "IC4"
			(at -3.8 0.8 0)
			(layer "F.SilkS")
		)
		(property "Value" "NPM1100-QDAA-R"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Battery Management Extremely compact Power Management IC (PMIC) QFN"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Height" "0.9"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Part Number" "949-NPM1100-QDAA-R"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Price/Stock" "https://www.mouser.co.uk/ProductDetail/Nordic-Semiconductor/NPM1100-QDAA-R?qs=amGC7iS6iy9SVRzpFaPmEA%3D%3D"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Name" "Nordic Semiconductor"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Part_Number" "NPM1100-QDAA-R"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "watch.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -2 -1.25 270)
			(size 0.3 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "+3.0V")
			(pinfunction "VOUTB")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -2 -0.75 270)
			(size 0.3 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 6 "/VSYS")
			(pinfunction "VOUTBSET1")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at -2 -0.25 270)
			(size 0.3 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 6 "/VSYS")
			(pinfunction "VOUTBSET2")
			(pintype "passive")
		)
		(pad "4" smd rect
			(at -2 0.25 270)
			(size 0.3 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 32 "unconnected-(IC4-NC_1-Pad4)")
			(pinfunction "NC_1")
			(pintype "passive+no_connect")
		)
		(pad "5" smd rect
			(at -2 0.75 270)
			(size 0.3 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "ISET")
			(pintype "passive")
		)
		(pad "6" smd rect
			(at -2 1.25 270)
			(size 0.3 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "SHPACT")
			(pintype "passive")
		)
		(pad "7" smd rect
			(at -1.25 2 180)
			(size 0.3 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "MODE")
			(pintype "passive")
		)
		(pad "8" smd rect
			(at -0.75 2 180)
			(size 0.3 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 39 "BAT_CHG")
			(pinfunction "CHG")
			(pintype "passive")
		)
		(pad "9" smd rect
			(at -0.25 2 180)
			(size 0.3 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 6 "/VSYS")
			(pinfunction "VTERMSET")
			(pintype "passive")
		)
		(pad "10" smd rect
			(at 0.25 2 180)
			(size 0.3 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 33 "BAT_ERR")
			(pinfunction "ERR")
			(pintype "passive")
		)
		(pad "11" smd rect
			(at 0.75 2 180)
			(size 0.3 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "SHPHLD")
			(pintype "passive")
		)
		(pad "12" smd rect
			(at 1.25 2 180)
			(size 0.3 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 41 "Net-(IC4-ICHG)")
			(pinfunction "ICHG")
			(pintype "passive")
		)
		(pad "13" smd rect
			(at 2 1.25 270)
			(size 0.3 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 37 "unconnected-(IC4-NC_2-Pad13)")
			(pinfunction "NC_2")
			(pintype "passive+no_connect")
		)
		(pad "14" smd rect
			(at 2 0.75 270)
			(size 0.3 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 34 "Net-(IC4-NTC)")
			(pinfunction "NTC")
			(pintype "passive")
		)
		(pad "15" smd rect
			(at 2 0.25 270)
			(size 0.3 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 4 "/+BAT")
			(pinfunction "VBAT")
			(pintype "passive")
		)
		(pad "16" smd rect
			(at 2 -0.25 270)
			(size 0.3 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 6 "/VSYS")
			(pinfunction "VSYS")
			(pintype "passive")
		)
		(pad "17" smd rect
			(at 2 -0.75 270)
			(size 0.3 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 3 "VBUS")
			(pinfunction "VBUS")
			(pintype "passive")
		)
		(pad "18" smd rect
			(at 2 -1.25 270)
			(size 0.3 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 35 "unconnected-(IC4-NC_3-Pad18)")
			(pinfunction "NC_3")
			(pintype "passive+no_connect")
		)
		(pad "19" smd rect
			(at 1.25 -2 180)
			(size 0.3 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 40 "unconnected-(IC4-D--Pad19)")
			(pinfunction "D-")
			(pintype "passive+no_connect")
		)
		(pad "20" smd rect
			(at 0.75 -2 180)
			(size 0.3 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 38 "unconnected-(IC4-D+-Pad20)")
			(pinfunction "D+")
			(pintype "passive+no_connect")
		)
		(pad "21" smd rect
			(at 0.25 -2 180)
			(size 0.3 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 5 "Net-(IC4-DEC)")
			(pinfunction "DEC")
			(pintype "passive")
		)
		(pad "22" smd rect
			(at -0.25 -2 180)
			(size 0.3 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 36 "Net-(IC4-SW)")
			(pinfunction "SW")
			(pintype "passive")
		)
		(pad "23" smd rect
			(at -0.75 -2 180)
			(size 0.3 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "PVSS")
			(pintype "passive")
		)
		(pad "24" smd rect
			(at -1.25 -2 180)
			(size 0.3 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 31 "unconnected-(IC4-NC_4-Pad24)")
			(pinfunction "NC_4")
			(pintype "passive+no_connect")
		)
		(pad "25" smd rect
			(at 0 0 180)
			(size 2.8 2.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "EP")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KIPRJMOD}/symbols/LIB_NPM1100-QDAA-R/NPM1100-QDAA-R/3D/NPM1100-QDAA-R.stp"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 158 81.5 90)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C4"
			(at -0.1 -0.7 90)
			(layer "F.SilkS")
		)
		(property "Value" "C2.2uF"
			(at 0 1.16 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "watch.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 90)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 90)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 4 "/+BAT")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 156.1 65.5 90)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C49"
			(at 0.225 -1.45 180)
			(layer "F.SilkS")
		)
		(property "Value" "220pF"
			(at 0 1.16 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "watch.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 90)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 24 "/RFI+")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 90)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 155.5 85.725)
		(descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x02 2.54mm single row")
		(property "Reference" "J3"
			(at 0 -2.38 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Conn_01x02_Pin"
			(at 0 4.92 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x02, script generated"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "/")
		(sheetfile "watch.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 1.27 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 67 "Net-(J3-Pin_1)")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 0 2.54)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 65 "Net-(J3-Pin_2)")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "beepy:Trans Rights now Front"
		(layer "F.Cu")
		(at 189.96 107.7)
		(property "Reference" "TRNSRTS"
			(at -0.03 -2.75 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Trans Rights now Front"
			(at 0 2.4 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd allow_soldermask_bridges)
		(fp_text user "TRANS"
			(at -4.86 -0.27 0)
			(unlocked yes)
			(layer "F.Cu")
		)
		(fp_text user "NOW"
			(at 0.39 -1.79 270)
			(unlocked yes)
			(layer "F.Cu")
		)
		(fp_text user "RIGHTS"
			(at -5.21 1.21 0)
			(unlocked yes)
			(layer "F.Cu")
		)
		(fp_text user "TRANS"
			(at -4.860007 -0.27 0)
			(unlocked yes)
			(layer "F.Mask")
		)
		(fp_text user "NOW"
			(at 0.389993 -1.79 270)
			(unlocked yes)
			(layer "F.Mask")
		)
		(fp_text user "RIGHTS"
			(at -5.210007 1.21 0)
			(unlocked yes)
			(layer "F.Mask")
		)
		(fp_text user "${REFERENCE}"
			(at 0 3.9 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(embedded_fonts no)
	)
	(footprint "varicap:LXRW0YV201059"
		(layer "F.Cu")
		(at 160.3 70.5 -90)
		(descr "LXRW0YV201-059-2")
		(tags "Capacitor")
		(property "Reference" "C43"
			(at -0.6 -0.8 180)
			(layer "F.SilkS")
		)
		(property "Value" "LXRW0YV201-059"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTREV" "July, 2018"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "STANDARD" "Manufacturer Recommendations"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MAXIMUM_PACKAGE_HEIGHT" "0.3mm"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER" "Murata"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "watch.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -0.2 0.2)
			(size 0.2 0.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pintype "power_in")
		)
		(pad "2" smd rect
			(at -0.2 -0.2)
			(size 0.2 0.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 81 "/AAT_SERIES")
			(pintype "input")
		)
		(pad "3" smd rect
			(at 0.2 -0.2)
			(size 0.2 0.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 21 "Net-(C42-Pad1)")
			(pintype "passive")
		)
		(pad "4" smd rect
			(at 0.2 0.2)
			(size 0.2 0.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 23 "Net-(C43-Pad4)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KIPRJMOD}/symbols/LIB_LXRW0YV201-059(1)/LXRW0YV201-059/3D/LXRW0YV201-059.stp"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 163.5 100.75 90)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C51"
			(at 0 0.75 90)
			(layer "F.SilkS")
		)
		(property "Value" "C2.2uF"
			(at 0 1.16 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "watch.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 90)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 30 "/DECA")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 90)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 156.1 70.9 90)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C46"
			(at -0.475 1.3 180)
			(layer "F.SilkS")
		)
		(property "Value" "10pF"
			(at 0 1.16 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "watch.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 90)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 22 "/RFI-")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 90)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 23 "Net-(C43-Pad4)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 176.73 85.75)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C18"
			(at -0.03 -0.775 0)
			(layer "F.SilkS")
		)
		(property "Value" "C0.1uF"
			(at 0 1.16 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "watch.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "+3.0V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 179 96.5 -90)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C7"
			(at -1.2 -0.05 180)
			(layer "F.SilkS")
		)
		(property "Value" "C4.7uF"
			(at 0 1.16 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol 10V"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "watch.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 270)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 7 "+8.7V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 270)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Crystal:Crystal_SMD_2016-4Pin_2.0x1.6mm"
		(layer "F.Cu")
		(at 158.5 98.25 90)
		(descr "SMD2016/4, Crystal, 2.0x1.6mm package, SMD, generated with kicad-footprint-generator make_crystal.py, http://www.q-crystal.com/upload/5/2015552223166229.pdf")
		(property "Reference" "Y2"
			(at 0 -1.6 90)
			(layer "F.SilkS")
		)
		(property "Value" "32MHz"
			(at 0 2 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Crystal SMD 2016, 32 MHz, Cl = 8 pF, Total Tol: ±40 ppm."
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Crystal*")
		(sheetname "/")
		(sheetfile "watch.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.7 0.55 90)
			(size 0.9 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 98 "Net-(U2-XC2)")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.7 0.55 90)
			(size 0.9 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 100 "Net-(U2-XC1)")
			(pinfunction "2")
			(pintype "passive")
		)
		(pad "3" smd roundrect
			(at 0.7 -0.55 90)
			(size 0.9 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "4" smd roundrect
			(at -0.7 -0.55 90)
			(size 0.9 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Crystal.3dshapes/Crystal_SMD_2016-4Pin_2.0x1.6mm.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 159.48 82.25 90)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C6"
			(at -1.15 -0.08 180)
			(layer "F.SilkS")
		)
		(property "Value" "C10uF"
			(at 0 1.16 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "watch.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 90)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 90)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 6 "/VSYS")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "accel:LSM6DS3USTR"
		(layer "F.Cu")
		(at 176.873 82.838)
		(descr "LGA-14(2.5x3x0.86)")
		(tags "Integrated Circuit")
		(property "Reference" "IC3"
			(at 0.027 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "ISM330DHCXTR"
			(at -0.209 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/ism330dhcx.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "IMUs - Inertial Measurement Units VFLGA2.5X3X.86 14L P.5 L.475X.25"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Height" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Part Number" "511-ISM330DHCXTR"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Price/Stock" "https://www.mouser.co.uk/ProductDetail/STMicroelectronics/ISM330DHCXTR?qs=%252B6g0mu59x7Jv2Xps2dM6Xw%3D%3D"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Name" "STMicroelectronics"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Part_Number" "ISM330DHCXTR"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "watch.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at -0.209 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.163 -0.75 90)
			(size 0.25 0.475)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "SDO/SA0")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -1.163 -0.25 90)
			(size 0.25 0.475)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "+3.0V")
			(pinfunction "SDX")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at -1.163 0.25 90)
			(size 0.25 0.475)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "+3.0V")
			(pinfunction "SCX")
			(pintype "passive")
		)
		(pad "4" smd rect
			(at -1.163 0.75 90)
			(size 0.25 0.475)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 62 "ACCEL_INT")
			(pinfunction "INT1")
			(pintype "passive")
		)
		(pad "5" smd rect
			(at -0.5 0.912)
			(size 0.25 0.475)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "+3.0V")
			(pinfunction "VDDIO")
			(pintype "passive")
		)
		(pad "6" smd rect
			(at 0 0.912)
			(size 0.25 0.475)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND_1")
			(pintype "passive")
		)
		(pad "7" smd rect
			(at 0.5 0.912)
			(size 0.25 0.475)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND_2")
			(pintype "passive")
		)
		(pad "8" smd rect
			(at 1.163 0.75 90)
			(size 0.25 0.475)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "+3.0V")
			(pinfunction "VDD")
			(pintype "passive")
		)
		(pad "9" smd rect
			(at 1.163 0.25 90)
			(size 0.25 0.475)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 86 "unconnected-(IC3-INT2-Pad9)")
			(pinfunction "INT2")
			(pintype "passive+no_connect")
		)
		(pad "10" smd rect
			(at 1.163 -0.25 90)
			(size 0.25 0.475)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "OCS_AUX")
			(pintype "passive")
		)
		(pad "11" smd rect
			(at 1.163 -0.75 90)
			(size 0.25 0.475)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "SDO_AUX")
			(pintype "passive")
		)
		(pad "12" smd rect
			(at 0.5 -0.912)
			(size 0.25 0.475)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "+3.0V")
			(pinfunction "CS")
			(pintype "passive")
		)
		(pad "13" smd rect
			(at 0 -0.912)
			(size 0.25 0.475)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 60 "TWIM_SCL")
			(pinfunction "SCL")
			(pintype "passive")
		)
		(pad "14" smd rect
			(at -0.5 -0.912)
			(size 0.25 0.475)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 61 "TWIM_SDA")
			(pinfunction "SDA")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KIPRJMOD}/symbols/LIB_ISM330DHCXTR(1)/ISM330DHCXTR/3D/ISM330DHCXTR.stp"
			(offset
				(xyz 0 0 0.8600000014)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 90 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 189.740001 72.5)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R15"
			(at -1.640001 0.1 0)
			(layer "F.SilkS")
		)
		(property "Value" "R10K"
			(at 0 1.17 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "watch.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.509999 0)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.509999 0)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 64 "BTN_A")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 154.7 68.3 180)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R12"
			(at 0.1 -0.8 0)
			(layer "F.SilkS")
		)
		(property "Value" "R1.6"
			(at 0 1.17 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "watch.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.509999 0 180)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 25 "Net-(C1-Pad3)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.509999 0 180)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 56 "Net-(AE1-Pad1)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0201_0603Metric"
		(layer "F.Cu")
		(at 170.08 71.9 180)
		(descr "Capacitor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C29"
			(at -1.62 -0.025 180)
			(layer "F.SilkS")
		)
		(property "Value" "C2.2uF"
			(at 0 1.05 180)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "watch.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -0.68 180)
			(layer "F.Fab")
		)
		(pad "" smd roundrect
			(at -0.345 0 180)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0.345 0 180)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "1" smd roundrect
			(at -0.32 0 180)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.32 0 180)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 13 "/AGDC")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0201_0603Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 174.5 93.48 -90)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C8"
			(at 0.02 -1 180)
			(layer "F.SilkS")
		)
		(property "Value" "C2.2uF"
			(at 0 1.16 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "watch.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 270)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "+3.0V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 270)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0201_0603Metric"
		(layer "F.Cu")
		(at 163.5 62.75)
		(descr "Capacitor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C31"
			(at 1.6 -0.025 0)
			(layer "F.SilkS")
		)
		(property "Value" "C2.2uF"
			(at 0 1.05 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "watch.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -0.68 0)
			(layer "F.Fab")
		)
		(pad "" smd roundrect
			(at -0.345 0)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0.345 0)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "1" smd roundrect
			(at -0.32 0)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.32 0)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 14 "/VDD_A")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0201_0603Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0201_0603Metric"
		(layer "F.Cu")
		(at 162.5 64.75)
		(descr "Capacitor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C33"
			(at -1.6 0.075 0)
			(layer "F.SilkS")
		)
		(property "Value" "C2.2uF"
			(at 0 1.05 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "watch.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -0.68 0)
			(layer "F.Fab")
		)
		(pad "" smd roundrect
			(at -0.345 0)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0.345 0)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "1" smd roundrect
			(at -0.32 0)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.32 0)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 15 "/VDD_DR")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0201_0603Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 180.75 92.25)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C17"
			(at 0 0.775 0)
			(layer "F.SilkS")
		)
		(property "Value" "C4.7uF"
			(at 0 1.16 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol, 16V X7R"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "watch.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 12 "Net-(O1-VCOMH)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "rotary_enc:BGA6C40P2X3_88X123X62"
		(layer "F.Cu")
		(at 177.2 93.6)
		(descr "WCSP")
		(tags "Power Supply")
		(property "Reference" "PS1"
			(at 1.7 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "TPS61046YFFR"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/tps61046"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "28-V Output Voltage Boost Converter in WCSP Package"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Height" "0.625"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Part Number" "595-TPS61046YFFR"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Price/Stock" "https://www.mouser.co.uk/ProductDetail/Texas-Instruments/TPS61046YFFR?qs=MiqG6Kq1qKNwq3TLqYBDaw%3D%3D"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Name" "Texas Instruments"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Part_Number" "TPS61046YFFR"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "watch.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "A1" smd circle
			(at -0.2 -0.4 90)
			(size 0.2 0.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "+3.0V")
			(pinfunction "VIN")
			(pintype "power_in")
		)
		(pad "A2" smd circle
			(at 0.2 -0.4 90)
			(size 0.2 0.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "B1" smd circle
			(at -0.2 0 90)
			(size 0.2 0.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 52 "Net-(PS1-FB)")
			(pinfunction "FB")
			(pintype "input")
		)
		(pad "B2" smd circle
			(at 0.2 0 90)
			(size 0.2 0.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 44 "Net-(PS1-SW)")
			(pinfunction "SW")
			(pintype "bidirectional")
		)
		(pad "C1" smd circle
			(at -0.2 0.4 90)
			(size 0.2 0.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 51 "+8.7V_EN")
			(pinfunction "EN")
			(pintype "input")
		)
		(pad "C2" smd circle
			(at 0.2 0.4 90)
			(size 0.2 0.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 7 "+8.7V")
			(pinfunction "VOUT")
			(pintype "power_in")
		)
		(embedded_fonts no)
		(model "${KIPRJMOD}/symbols/LIB_TPS61046YFFR/TPS61046YFFR/3D/TPS61046YFFR.stp"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 162.25 100.75 90)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C50"
			(at -0.25 -0.75 270)
			(layer "F.SilkS")
		)
		(property "Value" "C2.2nF"
			(at 0 1.16 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "watch.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 90)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 30 "/DECA")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 90)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Inductor_SMD:L_0402_1005Metric"
		(layer "F.Cu")
		(at 163.5 70.4 -135)
		(descr "Inductor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
		(tags "inductor")
		(property "Reference" "L4"
			(at -0.070711 0.636396 45)
			(layer "F.SilkS")
		)
		(property "Value" "LEMC1"
			(at 0 1.17 45)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://www.mouser.com/ProductDetail/Wurth-Elektronik/7447650227?qs=sGAEpiMZZMv126LJFLh8y52c8U8kZLUYkGOIYgN%2FHZk%3D"
			(at 0 0 45)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Inductor"
			(at 0 0 45)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Choke_* *Coil* Inductor_* L_*")
		(sheetname "/")
		(sheetfile "watch.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 45)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.485 0 225)
			(size 0.59 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 46 "/RFO2")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.485 0 225)
			(size 0.59 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 21 "Net-(C42-Pad1)")
			(pinfunction "2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_0402_1005Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "varicap:LXRW0YV201059"
		(layer "F.Cu")
		(at 157.8 70.5)
		(descr "LXRW0YV201-059-2")
		(tags "Capacitor")
		(property "Reference" "C45"
			(at 0.9 -0.6 0)
			(layer "F.SilkS")
		)
		(property "Value" "LXRW0YV201-059"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTREV" "July, 2018"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "STANDARD" "Manufacturer Recommendations"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MAXIMUM_PACKAGE_HEIGHT" "0.3mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER" "Murata"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "watch.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -0.2 0.2 90)
			(size 0.2 0.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pintype "power_in")
		)
		(pad "2" smd rect
			(at -0.2 -0.2 90)
			(size 0.2 0.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 80 "/AAT_PARALLEL")
			(pintype "input")
		)
		(pad "3" smd rect
			(at 0.2 -0.2 90)
			(size 0.2 0.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pintype "passive")
		)
		(pad "4" smd rect
			(at 0.2 0.2 90)
			(size 0.2 0.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 23 "Net-(C43-Pad4)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KIPRJMOD}/symbols/LIB_LXRW0YV201-059(1)/LXRW0YV201-059/3D/LXRW0YV201-059.stp"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 159.5 92.75 90)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "R3"
			(at 0.175 -0.9 180)
			(layer "F.SilkS")
		)
		(property "Value" "R1k"
			(at 0 1.16 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "watch.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 90)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 57 "Net-(U2-NRESET)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 90)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 70 "Net-(R3-Pad2)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_PinHeader_2.54mm:PinHeader_2x10_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 157.18 106.765 90)
		(descr "Through hole straight pin header, 2x10, 2.54mm pitch, double rows")
		(tags "Through hole pin header THT 2x10 2.54mm double row")
		(property "Reference" "J4"
			(at 1.27 -2.38 90)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_02x10_Odd_Even"
			(at 1.27 25.24 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, double row, 02x10, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_2x??_*")
		(sheetname "/")
		(sheetfile "watch.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 1.27 11.43 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 33 "BAT_ERR")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 2.54 0 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 39 "BAT_CHG")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole circle
			(at 0 2.54 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 53 "ENC_OUT_A")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole circle
			(at 2.54 2.54 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 54 "ENC_OUT_B")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(pad "5" thru_hole circle
			(at 0 5.08 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 64 "BTN_A")
			(pinfunction "Pin_5")
			(pintype "passive")
		)
		(pad "6" thru_hole circle
			(at 2.54 5.08 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 66 "BTN_B")
			(pinfunction "Pin_6")
			(pintype "passive")
		)
		(pad "7" thru_hole circle
			(at 0 7.62 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 28 "LRA_TRIG")
			(pinfunction "Pin_7")
			(pintype "passive")
		)
		(pad "8" thru_hole circle
			(at 2.54 7.62 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 62 "ACCEL_INT")
			(pinfunction "Pin_8")
			(pintype "passive")
		)
		(pad "9" thru_hole circle
			(at 0 10.16 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 101 "unconnected-(J4-Pin_9-Pad9)")
			(pinfunction "Pin_9")
			(pintype "passive+no_connect")
		)
		(pad "10" thru_hole circle
			(at 2.54 10.16 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 51 "+8.7V_EN")
			(pinfunction "Pin_10")
			(pintype "passive")
		)
		(pad "11" thru_hole circle
			(at 0 12.7 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 9 "OLED_VDD")
			(pinfunction "Pin_11")
			(pintype "passive")
		)
		(pad "12" thru_hole circle
			(at 2.54 12.7 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 47 "SH1107_RESET")
			(pinfunction "Pin_12")
			(pintype "passive")
		)
		(pad "13" thru_hole circle
			(at 0 15.24 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 61 "TWIM_SDA")
			(pinfunction "Pin_13")
			(pintype "passive")
		)
		(pad "14" thru_hole circle
			(at 2.54 15.24 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 60 "TWIM_SCL")
			(pinfunction "Pin_14")
			(pintype "passive")
		)
		(pad "15" thru_hole circle
			(at 0 17.78 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 102 "unconnected-(J4-Pin_15-Pad15)")
			(pinfunction "Pin_15")
			(pintype "passive+no_connect")
		)
		(pad "16" thru_hole circle
			(at 2.54 17.78 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 103 "unconnected-(J4-Pin_16-Pad16)")
			(pinfunction "Pin_16")
			(pintype "passive+no_connect")
		)
		(pad "17" thru_hole circle
			(at 0 20.32 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "+3.0V")
			(pinfunction "Pin_17")
			(pintype "passive")
		)
		(pad "18" thru_hole circle
			(at 2.54 20.32 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_18")
			(pintype "passive")
		)
		(pad "19" thru_hole circle
			(at 0 22.86 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "+3.0V")
			(pinfunction "Pin_19")
			(pintype "passive")
		)
		(pad "20" thru_hole circle
			(at 2.54 22.86 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_20")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x10_P2.54mm_Vertical.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 161 61.75 180)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C37"
			(at 1.7 -0.05 0)
			(layer "F.SilkS")
		)
		(property "Value" "C0.1uF"
			(at 0 1.16 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "watch.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 180)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 180)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "+3.0V")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 160.5 93.25 -90)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C52"
			(at 0.05 -0.8 270)
			(layer "F.SilkS")
		)
		(property "Value" "C3.9pF"
			(at 0 1.16 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "watch.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 270)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 270)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 57 "Net-(U2-NRESET)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "w3008:ANTENNA_W3008"
		(layer "F.Cu")
		(at 151.575 94.585 -90)
		(property "Reference" "ANT1"
			(at 0.015 -0.125 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "W3008"
			(at 2.049931 2.158873 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "STANDARD" "Manufacturer recommendations"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER" "PulseLarsen Antennas"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "watch.kicad_sch")
		(attr smd)
		(pad "FEED" smd rect
			(at 1.6 -0.475 270)
			(size 0.8 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 10 "Net-(ANT1-PadFEED)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "G1" smd rect
			(at 1.6 0.475 270)
			(size 0.8 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "G2" smd rect
			(at -1.6 0 270)
			(size 0.8 1.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(zone
			(net 0)
			(net_name "")
			(layer "F.Cu")
			(hatch full 0.508)
			(connect_pads
				(clearance 0)
			)
			(min_thickness 0.127)
			(filled_areas_thickness no)
			(keepout
				(tracks not_allowed)
				(vias not_allowed)
				(pads not_allowed)
				(copperpour not_allowed)
				(footprints allowed)
			)
			(placement
				(enabled no)
				(sheetname "")
			)
			(fill
				(thermal_gap 0.508)
				(thermal_bridge_width 0.508)
			)
			(polygon
				(pts
					(xy 150.375 92.585) (xy 150.375 96.585) (xy 150.65 96.585) (xy 150.65 95.685) (xy 152.55 95.685)
					(xy 152.55 96.585) (xy 154.625 96.585) (xy 154.625 92.585) (xy 152.45 92.585) (xy 152.45 93.485)
					(xy 150.65 93.485) (xy 150.65 92.585)
				)
			)
		)
		(zone
			(net 0)
			(net_name "")
			(layer "B.Cu")
			(hatch full 0.508)
			(connect_pads
				(clearance 0)
			)
			(min_thickness 0.127)
			(filled_areas_thickness no)
			(keepout
				(tracks not_allowed)
				(vias not_allowed)
				(pads not_allowed)
				(copperpour not_allowed)
				(footprints allowed)
			)
			(placement
				(enabled no)
				(sheetname "")
			)
			(fill
				(thermal_gap 0.508)
				(thermal_bridge_width 0.508)
			)
			(polygon
				(pts
					(xy 150.375 92.585) (xy 150.65 92.585) (xy 150.65 93.485) (xy 152.45 93.485) (xy 152.45 92.585)
					(xy 154.625 92.585) (xy 154.625 96.585) (xy 152.55 96.585) (xy 152.55 95.685) (xy 150.65 95.685)
					(xy 150.65 96.585) (xy 150.375 96.585)
				)
			)
		)
		(embedded_fonts no)
		(model "${KIPRJMOD}/symbols/W3008(1)/W3008.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 -0 -0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0201_0603Metric"
		(layer "F.Cu")
		(at 159 64.25)
		(descr "Capacitor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C35"
			(at -1.5 0.025 0)
			(layer "F.SilkS")
		)
		(property "Value" "C2.2uF"
			(at 0 1.05 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "watch.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -0.68 0)
			(layer "F.Fab")
		)
		(pad "" smd roundrect
			(at -0.345 0)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0.345 0)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "1" smd roundrect
			(at -0.32 0)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.32 0)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 16 "/VDD_AM")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0201_0603Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 172.25 65.75 180)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C15"
			(at -0.55 -0.85 0)
			(layer "F.SilkS")
		)
		(property "Value" "C0.1uF"
			(at 0 1.16 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "watch.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 180)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 180)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "+3.0V")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0201_0603Metric"
		(layer "F.Cu")
		(at 158.25 80 180)
		(descr "Capacitor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "TH1"
			(at 0.05 0.7 0)
			(layer "F.SilkS")
		)
		(property "Value" "NTC"
			(at 0 1 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://www.mouser.com/ProductDetail/TDK/NTCG063JF103FT?qs=4JX4e57RtWxzWoQTVVBI1Q%3D%3D"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Temperature dependent resistor, negative temperature coefficient"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*NTC* *Thermistor* PIN?ARRAY* bornier* *Terminal?Block* R_*")
		(sheetname "/")
		(sheetfile "watch.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -0.680001 0)
			(layer "F.Fab")
		)
		(pad "" smd roundrect
			(at -0.345 0 180)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0.345 0 180)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "1" smd roundrect
			(at -0.32 0 180)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 34 "Net-(IC4-NTC)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.32 0 180)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0201_0603Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 160.75 99 -90)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C23"
			(at 0 -0.85 90)
			(layer "F.SilkS")
		)
		(property "Value" "C0.1uF"
			(at 0 1.16 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "watch.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 270)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "+3.0V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 270)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 166 99.5 -90)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C26"
			(at 0.025 -0.8 90)
			(layer "F.SilkS")
		)
		(property "Value" "C2.2uF"
			(at 0 1.16 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "watch.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 270)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 27 "/DECD")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 270)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 156.1 67.4 90)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C48"
			(at 0.375 -1.3 180)
			(layer "F.SilkS")
		)
		(property "Value" "10pF"
			(at 0 1.16 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "watch.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 90)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 25 "Net-(C1-Pad3)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 90)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 24 "/RFI+")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 170 63.92 90)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C39"
			(at 1.72 0.1 90)
			(layer "F.SilkS")
		)
		(property "Value" "C12pF"
			(at 0 1.16 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "watch.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 90)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 18 "/XTO")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 90)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "rotary_enc:XRCGB"
		(layer "F.Cu")
		(at 167.5 63.42)
		(descr "XRCGB")
		(tags "Crystal or Oscillator")
		(property "Reference" "Y1"
			(at 0 -1.22 0)
			(layer "F.SilkS")
		)
		(property "Value" "XRCGB27M120F3M13R0"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" "https://www.murata.com/products/productdata/8801063141406/SPEC-XRCGB27M120F3M13R0.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Crystals 2.0x1.6x0.65mm 27.12MHz Crystal +/-30ppm Initial tolerance"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Height" "0.7"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Part Number" "81-XRCGB27M120F3M13R"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Price/Stock" "https://www.mouser.co.uk/ProductDetail/Murata-Electronics/XRCGB27M120F3M13R0?qs=rrS6PyfT74fcMlJ2scmJMQ%3D%3D"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Name" "Murata Electronics"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Part_Number" "XRCGB27M120F3M13R0"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "watch.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -0.675 0.5 90)
			(size 0.7 0.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 19 "/XTI")
			(pinfunction "XTAL_1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 0.675 0.5 90)
			(size 0.7 0.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 88 "unconnected-(Y1-NC_1-Pad2)")
			(pinfunction "NC_1")
			(pintype "passive+no_connect")
		)
		(pad "3" smd rect
			(at 0.675 -0.5 90)
			(size 0.7 0.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 18 "/XTO")
			(pinfunction "XTAL_2")
			(pintype "passive")
		)
		(pad "4" smd rect
			(at -0.675 -0.5 90)
			(size 0.7 0.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 87 "unconnected-(Y1-NC_2-Pad4)")
			(pinfunction "NC_2")
			(pintype "passive+no_connect")
		)
		(embedded_fonts no)
		(model "XRCGB27M120F3M13R0.stp"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0201_0603Metric"
		(layer "F.Cu")
		(at 158.5 95.5 90)
		(descr "Capacitor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C53"
			(at -0.675 1 0)
			(layer "F.SilkS")
		)
		(property "Value" "C1.5pF"
			(at 0 1.05 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Capacitor, NP0, ±0.05 pF, 25 V, High Q"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "watch.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -0.68 90)
			(layer "F.Fab")
		)
		(pad "" smd roundrect
			(at -0.345 0 90)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0.345 0 90)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "1" smd roundrect
			(at -0.32 0 90)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.32 0 90)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 58 "Net-(C53-Pad2)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0201_0603Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0201_0603Metric"
		(layer "F.Cu")
		(at 171.5 63.4 180)
		(descr "Capacitor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C16"
			(at -1.65 -0.025 180)
			(layer "F.SilkS")
		)
		(property "Value" "C2.2uF"
			(at 0 1.05 180)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "watch.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -0.68 180)
			(layer "F.Fab")
		)
		(pad "" smd roundrect
			(at -0.345 0 180)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0.345 0 180)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "1" smd roundrect
			(at -0.32 0 180)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.32 0 180)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 11 "/VDD_D")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0201_0603Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 171.5 95.05 90)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R4"
			(at 0.05 0.9 90)
			(layer "F.SilkS")
		)
		(property "Value" "R10K"
			(at 0 1.17 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "watch.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 90)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "+3.0V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 90)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 61 "TWIM_SDA")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 169.5 83 -90)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C2"
			(at 0.275 -1.05 90)
			(layer "F.SilkS")
		)
		(property "Value" "C10uF"
			(at 0 1.16 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "watch.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 270)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "+3.0V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 270)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0201_0603Metric"
		(layer "F.Cu")
		(at 163.5 61.875)
		(descr "Capacitor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C32"
			(at 1.6 -0.05 0)
			(layer "F.SilkS")
		)
		(property "Value" "C10nF"
			(at 0 1.05 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "watch.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -0.68 0)
			(layer "F.Fab")
		)
		(pad "" smd roundrect
			(at -0.345 0)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0.345 0)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "1" smd roundrect
			(at -0.32 0)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.32 0)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 14 "/VDD_A")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0201_0603Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Inductor_SMD:L_1008_2520Metric"
		(layer "F.Cu")
		(at 177 90.235)
		(descr "Inductor SMD 1008 (2520 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: https://ecsxtal.com/store/pdf/ECS-MPI2520-SMD-POWER-INDUCTOR.pdf), generated with kicad-footprint-generator")
		(tags "inductor")
		(property "Reference" "L2"
			(at 0 -1.535 0)
			(layer "F.SilkS")
		)
		(property "Value" "L10uH"
			(at 0 2.05 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://www.mouser.com/ProductDetail/Murata-Electronics/1239AS-H-100M%3DP2?qs=KuGPmAKtFKWZyoO25uKvSg%3D%3D"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Inductor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Choke_* *Coil* Inductor_* L_*")
		(sheetname "/")
		(sheetfile "watch.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.075 0)
			(size 1.25 2.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.2)
			(net 2 "+3.0V")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.075 0)
			(size 1.25 2.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.2)
			(net 44 "Net-(PS1-SW)")
			(pinfunction "2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_1008_2520Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "F.Cu")
		(at 151.8 69.1 -90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "AE1"
			(at 1.175 -0.5 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Antenna_Loop"
			(at 0 1.68 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "watch.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0 270)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 56 "Net-(AE1-Pad1)")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at 0.95 0 270)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 55 "Net-(AE1-Pad2)")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 169.75 98.75 90)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C21"
			(at -1.45 0.05 90)
			(layer "F.SilkS")
		)
		(property "Value" "C10uF"
			(at 0 1.16 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "watch.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 90)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 90)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "+3.0V")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 163.25 84.5)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C5"
			(at 0 0.8 0)
			(layer "F.SilkS")
		)
		(property "Value" "C10uF"
			(at 0 1.16 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "watch.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 5 "Net-(IC4-DEC)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Inductor_SMD:L_0402_1005Metric"
		(layer "F.Cu")
		(at 165.5 101.25 180)
		(descr "Inductor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
		(tags "inductor")
		(property "Reference" "FB2"
			(at -0.05 0.725 180)
			(layer "F.SilkS")
		)
		(property "Value" "FerriteBead"
			(at 0 1.17 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "81-BLM15AG121SN1D"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Ferrite bead, 120 Ω at 100 MHz, 200 mA, 500 mΩ Max"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Inductor_* L_* *Ferrite*")
		(sheetname "/")
		(sheetfile "watch.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.485 0 180)
			(size 0.59 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 27 "/DECD")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.485 0 180)
			(size 0.59 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 30 "/DECA")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_0402_1005Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Inductor_SMD:L_0402_1005Metric"
		(layer "F.Cu")
		(at 161 62.75)
		(descr "Inductor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
		(tags "inductor")
		(property "Reference" "FB1"
			(at -1.7 -0.05 0)
			(layer "F.SilkS")
		)
		(property "Value" "FerriteBead"
			(at 0 1.17 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Ferrite bead"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Inductor_* L_* *Ferrite*")
		(sheetname "/")
		(sheetfile "watch.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.485 0)
			(size 0.59 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "+3.0V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.485 0)
			(size 0.59 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 17 "/VDD")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_0402_1005Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "beepy:Trans Rights now Back"
		(layer "F.Cu")
		(at 189.7625 107.7)
		(property "Reference" "TRNSRTS"
			(at -0.01 -2.69 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Trans Rights now Back"
			(at 0.01 2.68 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd allow_soldermask_bridges)
		(fp_text user "NOW"
			(at -0.39 -1.79 90)
			(unlocked yes)
			(layer "B.Cu")
		)
		(fp_text user "TRANS"
			(at 4.86 -0.27 0)
			(unlocked yes)
			(layer "B.Cu")
		)
		(fp_text user "RIGHTS"
			(at 5.21 1.21 0)
			(unlocked yes)
			(layer "B.Cu")
		)
		(fp_text user "RIGHTS"
			(at 5.2075 1.21 0)
			(unlocked yes)
			(layer "B.Mask")
		)
		(fp_text user "TRANS"
			(at 4.8575 -0.27 0)
			(unlocked yes)
			(layer "B.Mask")
		)
		(fp_text user "NOW"
			(at -0.3925 -1.79 90)
			(unlocked yes)
			(layer "B.Mask")
		)
		(fp_text user "${REFERENCE}"
			(at 0 3.9 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(embedded_fonts no)
	)
	(footprint "Capacitor_SMD:C_0201_0603Metric"
		(layer "F.Cu")
		(at 171.5 64.4 180)
		(descr "Capacitor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C28"
			(at -1.65 -0.025 180)
			(layer "F.SilkS")
		)
		(property "Value" "C10nF"
			(at 0 1.05 180)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "watch.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -0.68 180)
			(layer "F.Fab")
		)
		(pad "" smd roundrect
			(at -0.345 0 180)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0.345 0 180)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "1" smd roundrect
			(at -0.32 0 180)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.32 0 180)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 11 "/VDD_D")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0201_0603Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 180.740001 88.75 180)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R6"
			(at -0.059999 0.975 180)
			(layer "F.SilkS")
		)
		(property "Value" "R510K"
			(at 0 1.17 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "watch.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.509999 0 180)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 48 "Net-(O1-IREF)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.509999 0 180)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Inductor_SMD:L_0201_0603Metric"
		(layer "F.Cu")
		(at 156 95.25 180)
		(descr "Inductor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
		(tags "inductor")
		(property "Reference" "L8"
			(at 0 0.675 180)
			(layer "F.SilkS")
		)
		(property "Value" "L3.5nH"
			(at 0 1.05 180)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Inductor, 500 mA, ±0.1 nH, 170 mΩ"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Choke_* *Coil* Inductor_* L_*")
		(sheetname "/")
		(sheetfile "watch.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -0.68 180)
			(layer "F.Fab")
		)
		(pad "" smd roundrect
			(at -0.345 0 180)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0.345 0 180)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "1" smd roundrect
			(at -0.32 0 180)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 59 "Net-(C54-Pad2)")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.32 0 180)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 10 "Net-(ANT1-PadFEED)")
			(pinfunction "2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_0201_0603Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 176 96.5 90)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R5"
			(at 1.2 0 180)
			(layer "F.SilkS")
		)
		(property "Value" "R75K"
			(at 0 1.17 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "watch.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.509999 0 90)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.509999 0 90)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 52 "Net-(PS1-FB)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Inductor_SMD:L_0201_0603Metric"
		(layer "F.Cu")
		(at 159.7 95.25 180)
		(descr "Inductor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
		(tags "inductor")
		(property "Reference" "L6"
			(at 0 0.575 180)
			(layer "F.SilkS")
		)
		(property "Value" "L2.7nH"
			(at 0 1.05 180)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Inductor, 600 mA, ±0.1 nH, 120 mΩ"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Choke_* *Coil* Inductor_* L_*")
		(sheetname "/")
		(sheetfile "watch.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -0.68 180)
			(layer "F.Fab")
		)
		(pad "" smd roundrect
			(at -0.345 0 180)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0.345 0 180)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "1" smd roundrect
			(at -0.32 0 180)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 69 "/ANT")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.32 0 180)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 58 "Net-(C53-Pad2)")
			(pinfunction "2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_0201_0603Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "buttons:SW_B3U-1100P"
		(layer "F.Cu")
		(at 185.25 69.5 -90)
		(property "Reference" "SW4"
			(at 0 2.75 270)
			(layer "F.SilkS")
		)
		(property "Value" "SW_Push"
			(at 3.0949 -2.627906 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Push button switch, generic, two pins"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "watch.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at 1.700001 0 270)
			(size 0.8 1.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 66 "BTN_B")
			(pinfunction "1")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd rect
			(at -1.700001 0 270)
			(size 0.8 1.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "+3.0V")
			(pinfunction "2")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "3" smd rect
			(at 0 1.65 270)
			(size 0.8 1.1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
		(model "${KIPRJMOD}/symbols/B3U_1100P/B3U-1100P.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 -0 -0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 156.1 72.8 90)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C47"
			(at -0.475 1.3 180)
			(layer "F.SilkS")
		)
		(property "Value" "220pF"
			(at 0 1.16 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "watch.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 90)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 90)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 22 "/RFI-")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 180 100.275 -90)
		(descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x02 2.54mm single row")
		(property "Reference" "J6"
			(at 0 -2.38 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Conn_01x02_Pin"
			(at 0 4.92 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x02, script generated"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "/")
		(sheetfile "watch.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 1.27 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 0 2.54 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 7 "+8.7V")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 165 63.9 90)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C40"
			(at 0 -0.8 90)
			(layer "F.SilkS")
		)
		(property "Value" "C12pF"
			(at 0 1.16 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "watch.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 90)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 19 "/XTI")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 90)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "buttons:SW_B3U-1100P"
		(layer "F.Cu")
		(at 190.25 69.5 -90)
		(property "Reference" "SW3"
			(at 0 2.85 90)
			(layer "F.SilkS")
		)
		(property "Value" "SW_Push"
			(at 3.0949 -2.627906 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Push button switch, generic, two pins"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "watch.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at 1.700001 0 270)
			(size 0.8 1.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 64 "BTN_A")
			(pinfunction "1")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd rect
			(at -1.700001 0 270)
			(size 0.8 1.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "+3.0V")
			(pinfunction "2")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "3" smd rect
			(at 0 1.65 270)
			(size 0.8 1.1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
		(model "${KIPRJMOD}/symbols/B3U_1100P/B3U-1100P.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 -0 -0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 175.5 78.25 90)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C10"
			(at 0 -0.8 90)
			(layer "F.SilkS")
		)
		(property "Value" "C0.1uF"
			(at 0 1.16 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "watch.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 90)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 90)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 8 "Net-(IC1-REG)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0201_0603Metric"
		(layer "F.Cu")
		(at 162.5 65.75)
		(descr "Capacitor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C34"
			(at -1.6 0.075 0)
			(layer "F.SilkS")
		)
		(property "Value" "C10nF"
			(at 0 1.05 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "watch.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -0.68 0)
			(layer "F.Fab")
		)
		(pad "" smd roundrect
			(at -0.345 0)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0.345 0)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "1" smd roundrect
			(at -0.32 0)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.32 0)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 15 "/VDD_DR")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0201_0603Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 160.5 84 -90)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C3"
			(at 0 -0.9 90)
			(layer "F.SilkS")
		)
		(property "Value" "C2.2uF"
			(at 0 1.16 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "watch.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 270)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 3 "VBUS")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 270)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "buttons:SW_B3U-1100P"
		(layer "F.Cu")
		(at 163.5 88 180)
		(property "Reference" "SW2"
			(at 2.7 0.1 90)
			(layer "F.SilkS")
		)
		(property "Value" "SW_Push"
			(at 3.0949 -2.627906 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Push button switch, generic, two pins"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "watch.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at 1.7 0 180)
			(size 0.8 1.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 70 "Net-(R3-Pad2)")
			(pinfunction "1")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd rect
			(at -1.7 0 180)
			(size 0.8 1.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "2")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "3" smd rect
			(at 0 1.65 180)
			(size 0.8 1.1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
		(model "${KIPRJMOD}/symbols/B3U_1100P/B3U-1100P.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 -0 -0)
			)
		)
	)
	(footprint "nfc:QFN50P500X500X60-33N-D"
		(layer "F.Cu")
		(at 167.55 68.35 -90)
		(descr "UFQFPN32_2024")
		(tags "Integrated Circuit")
		(property "Reference" "IC2"
			(at 0 -4.05 180)
			(layer "F.SilkS")
		)
		(property "Value" "ST25R3916B-AQET"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" "https://www.st.com/en/nfc/st25r3916b.html"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "RFID Reader/Transponder IC 13.56MHz FeliCa, ISO 14443, ISO 15693, MIFARE, NFC I2C, SPI 2.6V ~ 5.5V 36-UFBGA, WLCSP"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Height" "0.6"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Part Number" "511-ST25R3916B-AQET"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Price/Stock" "https://www.mouser.co.uk/ProductDetail/STMicroelectronics/ST25R3916B-AQET?qs=rQFj71Wb1eX4vi6O4DqiQQ%3D%3D"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Name" "STMicroelectronics"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Part_Number" "ST25R3916B-AQET"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "watch.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -2.45 -1.75)
			(size 0.3 0.85)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "+3.0V")
			(pinfunction "VDD_IO")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -2.45 -1.25)
			(size 0.3 0.85)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 84 "unconnected-(IC2-TAD2-Pad2)")
			(pinfunction "TAD2")
			(pintype "passive+no_connect")
		)
		(pad "3" smd rect
			(at -2.45 -0.75)
			(size 0.3 0.85)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 11 "/VDD_D")
			(pinfunction "VDD_D")
			(pintype "passive")
		)
		(pad "4" smd rect
			(at -2.45 -0.25)
			(size 0.3 0.85)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 18 "/XTO")
			(pinfunction "XTO")
			(pintype "passive")
		)
		(pad "5" smd rect
			(at -2.45 0.25)
			(size 0.3 0.85)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 19 "/XTI")
			(pinfunction "XTI")
			(pintype "passive")
		)
		(pad "6" smd rect
			(at -2.45 0.75)
			(size 0.3 0.85)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND_D")
			(pintype "passive")
		)
		(pad "7" smd rect
			(at -2.45 1.25)
			(size 0.3 0.85)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 14 "/VDD_A")
			(pinfunction "VDD_A")
			(pintype "passive")
		)
		(pad "8" smd rect
			(at -2.45 1.75)
			(size 0.3 0.85)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 17 "/VDD")
			(pinfunction "VDD")
			(pintype "passive")
		)
		(pad "9" smd rect
			(at -1.75 2.45 270)
			(size 0.3 0.85)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 15 "/VDD_DR")
			(pinfunction "VDD_RF")
			(pintype "passive")
		)
		(pad "10" smd rect
			(at -1.25 2.45 270)
			(size 0.3 0.85)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 17 "/VDD")
			(pinfunction "VDD_TX")
			(pintype "passive")
		)
		(pad "11" smd rect
			(at -0.75 2.45 270)
			(size 0.3 0.85)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 16 "/VDD_AM")
			(pinfunction "VDD_AM")
			(pintype "passive")
		)
		(pad "12" smd rect
			(at -0.25 2.45 270)
			(size 0.3 0.85)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND_DR1")
			(pintype "passive")
		)
		(pad "13" smd rect
			(at 0.25 2.45 270)
			(size 0.3 0.85)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 45 "/RFO1")
			(pinfunction "RFO1")
			(pintype "passive")
		)
		(pad "14" smd rect
			(at 0.75 2.45 270)
			(size 0.3 0.85)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 15 "/VDD_DR")
			(pinfunction "VDD_DR")
			(pintype "passive")
		)
		(pad "15" smd rect
			(at 1.25 2.45 270)
			(size 0.3 0.85)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 46 "/RFO2")
			(pinfunction "RFO2")
			(pintype "passive")
		)
		(pad "16" smd rect
			(at 1.75 2.45 270)
			(size 0.3 0.85)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND_DR2")
			(pintype "passive")
		)
		(pad "17" smd rect
			(at 2.45 1.75)
			(size 0.3 0.85)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 78 "unconnected-(IC2-EXT_LM-Pad17)")
			(pinfunction "EXT_LM")
			(pintype "passive+no_connect")
		)
		(pad "18" smd rect
			(at 2.45 1.25)
			(size 0.3 0.85)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 81 "/AAT_SERIES")
			(pinfunction "AAT_A")
			(pintype "passive")
		)
		(pad "19" smd rect
			(at 2.45 0.75)
			(size 0.3 0.85)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 80 "/AAT_PARALLEL")
			(pinfunction "AAT_B")
			(pintype "passive")
		)
		(pad "20" smd rect
			(at 2.45 0.25)
			(size 0.3 0.85)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 11 "/VDD_D")
			(pinfunction "I2C_EN")
			(pintype "passive")
		)
		(pad "21" smd rect
			(at 2.45 -0.25)
			(size 0.3 0.85)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "VSS")
			(pintype "passive")
		)
		(pad "22" smd rect
			(at 2.45 -0.75)
			(size 0.3 0.85)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 24 "/RFI+")
			(pinfunction "RFI1")
			(pintype "passive")
		)
		(pad "23" smd rect
			(at 2.45 -1.25)
			(size 0.3 0.85)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 22 "/RFI-")
			(pinfunction "RFI2")
			(pintype "passive")
		)
		(pad "24" smd rect
			(at 2.45 -1.75)
			(size 0.3 0.85)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 13 "/AGDC")
			(pinfunction "AGDC")
			(pintype "passive")
		)
		(pad "25" smd rect
			(at 1.75 -2.45 270)
			(size 0.3 0.85)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 79 "unconnected-(IC2-TAD1-Pad25)")
			(pinfunction "TAD1")
			(pintype "passive+no_connect")
		)
		(pad "26" smd rect
			(at 1.25 -2.45 270)
			(size 0.3 0.85)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND_A")
			(pintype "passive")
		)
		(pad "27" smd rect
			(at 0.75 -2.45 270)
			(size 0.3 0.85)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 63 "NFC_IRQ")
			(pinfunction "IRQ")
			(pintype "passive")
		)
		(pad "28" smd rect
			(at 0.25 -2.45 270)
			(size 0.3 0.85)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 85 "unconnected-(IC2-MCU_CLK-Pad28)")
			(pinfunction "MCU_CLK")
			(pintype "passive+no_connect")
		)
		(pad "29" smd rect
			(at -0.25 -2.45 270)
			(size 0.3 0.85)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 83 "unconnected-(IC2-BSS-Pad29)")
			(pinfunction "BSS")
			(pintype "passive+no_connect")
		)
		(pad "30" smd rect
			(at -0.75 -2.45 270)
			(size 0.3 0.85)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 60 "TWIM_SCL")
			(pinfunction "SCLK/SCL")
			(pintype "passive")
		)
		(pad "31" smd rect
			(at -1.25 -2.45 270)
			(size 0.3 0.85)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 82 "unconnected-(IC2-MOSI-Pad31)")
			(pinfunction "MOSI")
			(pintype "passive+no_connect")
		)
		(pad "32" smd rect
			(at -1.75 -2.45 270)
			(size 0.3 0.85)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 61 "TWIM_SDA")
			(pinfunction "MISO/SDA")
			(pintype "passive")
		)
		(pad "33" smd rect
			(at 0 0 270)
			(size 3.6 3.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KIPRJMOD}/symbols/LIB_ST25R3916B-AQET(1)/ST25R3916B-AQET/3D/ST25R3916B-AQET.stp"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "rotary_enc:2121340002"
		(layer "F.Cu")
		(at 153.5 80.5 -90)
		(descr "212134-0002-1")
		(tags "Connector")
		(property "Reference" "J2"
			(at 0 -0.14 90)
			(layer "F.SilkS")
		)
		(property "Value" "212134-0002"
			(at 0 -0.14 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" "https://www.molex.com/pdm_docs/sd/2121340002_sd.pdf"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "PICO-EZMATE PLUS1.0 PLUGASSY ETP LH 2CKT - Tape and Reel"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Height" "1.4"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Part Number" "538-212134-0002"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Price/Stock" "https://www.mouser.co.uk/ProductDetail/Molex/212134-0002?qs=hd1VzrDQEGhMEPSgG43Vcg%3D%3D"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Name" "Molex"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Part_Number" "212134-0002"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "watch.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -0.14 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -0.5 -2.24 270)
			(size 0.7 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 0.5 -2.24 270)
			(size 0.7 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 4 "/+BAT")
			(pinfunction "2")
			(pintype "passive")
		)
		(pad "MP1" smd rect
			(at -1.525 1.76 270)
			(size 0.55 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 43 "unconnected-(J2-PadMP1)")
			(pinfunction "MP1")
			(pintype "passive+no_connect")
		)
		(pad "MP2" smd rect
			(at 1.525 1.76 270)
			(size 0.55 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 42 "unconnected-(J2-PadMP2)")
			(pinfunction "MP2")
			(pintype "passive+no_connect")
		)
		(embedded_fonts no)
		(model "${KIPRJMOD}/symbols/LIB_212134-0002(1)/212134-0002/3D/212134-0002.stp"
			(offset
				(xyz 0 0.1399999985 0.6000000148)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 -180)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 180 82.98 90)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C14"
			(at -0.095 1.2 90)
			(layer "F.SilkS")
		)
		(property "Value" "C0.1uF"
			(at 0 1.16 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "watch.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 90)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "+3.0V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 90)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0201_0603Metric"
		(layer "F.Cu")
		(at 157.5 95.5 90)
		(descr "Capacitor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C54"
			(at -0.675 -1 0)
			(layer "F.SilkS")
		)
		(property "Value" "C2.0pF"
			(at 0 1.05 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Capacitor, NP0, ±0.05 pF, 25 V"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "watch.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -0.68 90)
			(layer "F.Fab")
		)
		(pad "" smd roundrect
			(at -0.345 0 90)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0.345 0 90)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "1" smd roundrect
			(at -0.32 0 90)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.32 0 90)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 59 "Net-(C54-Pad2)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0201_0603Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Inductor_SMD:L_0201_0603Metric"
		(layer "F.Cu")
		(at 158 94.175 180)
		(descr "Inductor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
		(tags "inductor")
		(property "Reference" "L7"
			(at 0 0.6 180)
			(layer "F.SilkS")
		)
		(property "Value" "L3.5nH"
			(at 0 1.05 180)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Inductor, 500 mA, ±0.1 nH, 170 mΩ"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Choke_* *Coil* Inductor_* L_*")
		(sheetname "/")
		(sheetfile "watch.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -0.68 180)
			(layer "F.Fab")
		)
		(pad "" smd roundrect
			(at -0.345 0 180)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0.345 0 180)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "1" smd roundrect
			(at -0.32 0 180)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 58 "Net-(C53-Pad2)")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.32 0 180)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 59 "Net-(C54-Pad2)")
			(pinfunction "2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_0201_0603Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 180.5 96.5 -90)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C13"
			(at 0 -1.16 270)
			(layer "F.SilkS")
		)
		(property "Value" "C4.7uF"
			(at 0 1.16 270)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol, 16V X7R"
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "watch.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 270)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 270)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 7 "+8.7V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 270)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 152 88.275 180)
		(descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x02 2.54mm single row")
		(property "Reference" "J5"
			(at 0 -2.38 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Conn_01x02_Pin"
			(at 0 4.92 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x02, script generated"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "/")
		(sheetfile "watch.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 5.475 1.27 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 0 2.54 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "VBUS")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 171.5 93 -90)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R14"
			(at -0.5 -0.9 90)
			(layer "F.SilkS")
		)
		(property "Value" "R10K"
			(at 0 1.17 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "watch.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 270)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "+3.0V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 270)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 60 "TWIM_SCL")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 168.75 98.75 -90)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C22"
			(at 1.55 -0.05 90)
			(layer "F.SilkS")
		)
		(property "Value" "C0.1uF"
			(at 0 1.16 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "watch.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 270)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "+3.0V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 270)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "rotary_enc:P0.7_FPC"
		(layer "F.Cu")
		(at 189.5 96.5)
		(property "Reference" "O1"
			(at -0.25 -10.5 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "~"
			(at -0.05 -7.05 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "watch.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at -0.05 -5.55 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -4.2 -0.9)
			(size 0.4 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 50 "unconnected-(O1-NC-Pad1)")
			(pinfunction "NC")
			(pintype "input+no_connect")
			(thermal_bridge_angle 45)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd rect
			(at -3.5 -0.9)
			(size 0.4 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 7 "+8.7V")
			(pinfunction "VPP")
			(pintype "input")
			(thermal_bridge_angle 45)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "3" smd rect
			(at -2.8 -0.9)
			(size 0.4 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 12 "Net-(O1-VCOMH)")
			(pinfunction "VCOMH")
			(pintype "input")
			(thermal_bridge_angle 45)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "4" smd rect
			(at -2.1 -0.9)
			(size 0.4 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 9 "OLED_VDD")
			(pinfunction "VDD")
			(pintype "input")
			(thermal_bridge_angle 45)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "5" smd rect
			(at -1.4 -0.9)
			(size 0.4 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 9 "OLED_VDD")
			(pinfunction "IM1")
			(pintype "input")
			(thermal_bridge_angle 45)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "6" smd rect
			(at -0.7 -0.9)
			(size 0.4 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 48 "Net-(O1-IREF)")
			(pinfunction "IREF")
			(pintype "input")
			(thermal_bridge_angle 45)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "7" smd rect
			(at 0 -0.9)
			(size 0.4 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 1 "GND")
			(pinfunction "CS")
			(pintype "input")
			(thermal_bridge_angle 45)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "8" smd rect
			(at 0.7 -0.9)
			(size 0.4 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 47 "SH1107_RESET")
			(pinfunction "RES")
			(pintype "input")
			(thermal_bridge_angle 45)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "9" smd rect
			(at 1.4 -0.9)
			(size 0.4 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 1 "GND")
			(pinfunction "A0")
			(pintype "input")
			(thermal_bridge_angle 45)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "10" smd rect
			(at 2.1 -0.9)
			(size 0.4 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 60 "TWIM_SCL")
			(pinfunction "D0")
			(pintype "input")
			(thermal_bridge_angle 45)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "11" smd rect
			(at 2.8 -0.9)
			(size 0.4 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 61 "TWIM_SDA")
			(pinfunction "D1")
			(pintype "input")
			(thermal_bridge_angle 45)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "12" smd rect
			(at 3.5 -0.9)
			(size 0.4 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "input")
			(thermal_bridge_angle 45)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "13" smd rect
			(at 4.2 -0.9)
			(size 0.4 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 49 "unconnected-(O1-NC-Pad13)")
			(pinfunction "NC")
			(pintype "input+no_connect")
			(thermal_bridge_angle 45)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KIPRJMOD}/symbols/disp.obj"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Inductor_SMD:L_0402_1005Metric"
		(layer "F.Cu")
		(at 163.5 67.9 135)
		(descr "Inductor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
		(tags "inductor")
		(property "Reference" "L3"
			(at 0 -0.848528 135)
			(layer "F.SilkS")
		)
		(property "Value" "LEMC1"
			(at 0 1.17 135)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://www.mouser.com/ProductDetail/Wurth-Elektronik/7447650227?qs=sGAEpiMZZMv126LJFLh8y52c8U8kZLUYkGOIYgN%2FHZk%3D"
			(at 0 0 135)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Inductor"
			(at 0 0 135)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Choke_* *Coil* Inductor_* L_*")
		(sheetname "/")
		(sheetfile "watch.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 135)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.485 0 135)
			(size 0.59 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 45 "/RFO1")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.485 0 135)
			(size 0.59 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 20 "Net-(C1-Pad4)")
			(pinfunction "2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_0402_1005Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 179.75 78.5 90)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C9"
			(at 0.025 1.15 90)
			(layer "F.SilkS")
		)
		(property "Value" "C0.1uF"
			(at 0 1.16 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "watch.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 90)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 90)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "+3.0V")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Inductor_SMD:L_0805_2012Metric"
		(layer "F.Cu")
		(at 168 83.5 -90)
		(descr "Inductor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 80, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "inductor")
		(property "Reference" "L1"
			(at 2.025 -0.05 90)
			(layer "F.SilkS")
		)
		(property "Value" "L2.2uH"
			(at 0 1.550001 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://www.mouser.com/ProductDetail/Murata-Electronics/DFE201210U-2R2M%3DP2?qs=AQlKX63v8Rt%252B2GxwUyA5Fw%3D%3D"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Inductor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Choke_* *Coil* Inductor_* L_*")
		(sheetname "/")
		(sheetfile "watch.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.0625 0 270)
			(size 0.875 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "+3.0V")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.0625 0 270)
			(size 0.875 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 36 "Net-(IC4-SW)")
			(pinfunction "2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 193 71)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R8"
			(at -0.3 -0.8 0)
			(layer "F.SilkS")
		)
		(property "Value" "R10K"
			(at 0 1.17 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "watch.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.509999 0)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "+3.0V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.509999 0)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 54 "ENC_OUT_B")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0201_0603Metric"
		(layer "F.Cu")
		(at 164.5 99.25)
		(descr "Capacitor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C27"
			(at 0.1 -0.475 0)
			(layer "F.SilkS")
		)
		(property "Value" "C10nF"
			(at 0 1.05 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "watch.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -0.68 0)
			(layer "F.Fab")
		)
		(pad "" smd roundrect
			(at -0.345 0)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0.345 0)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "1" smd roundrect
			(at -0.32 0)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.32 0)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 30 "/DECA")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0201_0603Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 184.76 72.5)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R16"
			(at -1.56 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "R10K"
			(at 0 1.17 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "watch.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 66 "BTN_B")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 180.75 90.25)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C11"
			(at 0 0.925 0)
			(layer "F.SilkS")
		)
		(property "Value" "C4.7uF"
			(at 0 1.16 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol, 16V X7R"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "watch.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 9 "OLED_VDD")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0201_0603Metric"
		(layer "F.Cu")
		(at 159 65.25)
		(descr "Capacitor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C36"
			(at -1.55 0.025 0)
			(layer "F.SilkS")
		)
		(property "Value" "C10nF"
			(at 0 1.05 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "watch.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -0.68 0)
			(layer "F.Fab")
		)
		(pad "" smd roundrect
			(at -0.345 0)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0.345 0)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "1" smd roundrect
			(at -0.32 0)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.32 0)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 16 "/VDD_AM")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0201_0603Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 154.7 69.9 180)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R11"
			(at 0.1 -0.9 0)
			(layer "F.SilkS")
		)
		(property "Value" "R1.6"
			(at 0 1.17 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "watch.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.509999 0 180)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 23 "Net-(C43-Pad4)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.509999 0 180)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 55 "Net-(AE1-Pad2)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Inductor_SMD:L_0603_1608Metric"
		(layer "F.Cu")
		(at 167.5 100.25 -90)
		(descr "Inductor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
		(tags "inductor")
		(property "Reference" "L5"
			(at -1.75 0 180)
			(layer "F.SilkS")
		)
		(property "Value" "L4.7uH"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Inductor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Choke_* *Coil* Inductor_* L_*")
		(sheetname "/")
		(sheetfile "watch.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.787501 0 270)
			(size 0.875 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 68 "/DCC")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.787501 0 270)
			(size 0.875 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 27 "/DECD")
			(pinfunction "2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 177.5 96.5 90)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R2"
			(at 1.2 0.1 180)
			(layer "F.SilkS")
		)
		(property "Value" "R750K"
			(at 0 1.17 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "watch.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.509999 0 90)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 52 "Net-(PS1-FB)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.509999 0 90)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 7 "+8.7V")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_DFN_QFN:QFN-48-1EP_6x6mm_P0.4mm_EP4.6x4.6mm"
		(layer "F.Cu")
		(at 165 95 180)
		(descr "QFN, 48 Pin (http://infocenter.nordicsemi.com/pdf/nRF51822_PS_v3.3.pdf#page=67), generated with kicad-footprint-generator ipc_noLead_generator.py")
		(tags "QFN NoLead")
		(property "Reference" "U2"
			(at 0.7 -3 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "NRF54L15-QFAA-R"
			(at 0 4.3 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "NRF54L15-QFAA-R"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "QFN48_6X6_NOR QFN48_6X6_NOR-M QFN48_6X6_NOR-L")
		(sheetname "/")
		(sheetfile "watch.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "" smd roundrect
			(at -1.53 -1.53 180)
			(size 1.24 1.24)
			(layers "F.Paste")
			(roundrect_rratio 0.201613)
		)
		(pad "" smd roundrect
			(at -1.53 0 180)
			(size 1.24 1.24)
			(layers "F.Paste")
			(roundrect_rratio 0.201613)
		)
		(pad "" smd roundrect
			(at -1.53 1.53 180)
			(size 1.24 1.24)
			(layers "F.Paste")
			(roundrect_rratio 0.201613)
		)
		(pad "" smd roundrect
			(at 0 -1.53 180)
			(size 1.24 1.24)
			(layers "F.Paste")
			(roundrect_rratio 0.201613)
		)
		(pad "" smd roundrect
			(at 0 0 180)
			(size 1.24 1.24)
			(layers "F.Paste")
			(roundrect_rratio 0.201613)
		)
		(pad "" smd roundrect
			(at 0 1.53 180)
			(size 1.24 1.24)
			(layers "F.Paste")
			(roundrect_rratio 0.201613)
		)
		(pad "" smd roundrect
			(at 1.53 -1.53 180)
			(size 1.24 1.24)
			(layers "F.Paste")
			(roundrect_rratio 0.201613)
		)
		(pad "" smd roundrect
			(at 1.53 0 180)
			(size 1.24 1.24)
			(layers "F.Paste")
			(roundrect_rratio 0.201613)
		)
		(pad "" smd roundrect
			(at 1.53 1.53 180)
			(size 1.24 1.24)
			(layers "F.Paste")
			(roundrect_rratio 0.201613)
		)
		(pad "1" smd roundrect
			(at -2.95 -2.2 180)
			(size 0.8 0.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 62 "ACCEL_INT")
			(pinfunction "P1.00/XL1")
			(pintype "bidirectional")
		)
		(pad "2" smd roundrect
			(at -2.95 -1.8 180)
			(size 0.8 0.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 28 "LRA_TRIG")
			(pinfunction "P1.01/XL2")
			(pintype "bidirectional")
		)
		(pad "3" smd roundrect
			(at -2.95 -1.4 180)
			(size 0.8 0.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 64 "BTN_A")
			(pinfunction "P1.02/NFC1")
			(pintype "bidirectional")
		)
		(pad "4" smd roundrect
			(at -2.95 -1 180)
			(size 0.8 0.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 66 "BTN_B")
			(pinfunction "P1.03/NFC2")
			(pintype "bidirectional")
		)
		(pad "5" smd roundrect
			(at -2.95 -0.6 180)
			(size 0.8 0.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 63 "NFC_IRQ")
			(pinfunction "P1.04/AIN0/TAMPC")
			(pintype "bidirectional")
		)
		(pad "6" smd roundrect
			(at -2.95 -0.2 180)
			(size 0.8 0.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 53 "ENC_OUT_A")
			(pinfunction "P1.05/AIN1/TAMPC")
			(pintype "input")
		)
		(pad "7" smd roundrect
			(at -2.95 0.2 180)
			(size 0.8 0.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 54 "ENC_OUT_B")
			(pinfunction "P1.06/AIN2/TAMPC")
			(pintype "input")
		)
		(pad "8" smd roundrect
			(at -2.95 0.6 180)
			(size 0.8 0.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 61 "TWIM_SDA")
			(pinfunction "P1.07/AIN3/TAMPC")
			(pintype "input")
		)
		(pad "9" smd roundrect
			(at -2.95 1 180)
			(size 0.8 0.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 60 "TWIM_SCL")
			(pinfunction "P1.08/CLK16M/TAMPC")
			(pintype "bidirectional")
		)
		(pad "10" smd roundrect
			(at -2.95 1.4 180)
			(size 0.8 0.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "+3.0V")
			(pinfunction "VDD")
			(pintype "power_in")
		)
		(pad "11" smd roundrect
			(at -2.95 1.8 180)
			(size 0.8 0.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 51 "+8.7V_EN")
			(pinfunction "P2.00/SPI.DCX")
			(pintype "bidirectional")
		)
		(pad "12" smd roundrect
			(at -2.95 2.2 180)
			(size 0.8 0.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 47 "SH1107_RESET")
			(pinfunction "P2.01/SPI.SCK")
			(pintype "bidirectional")
		)
		(pad "13" smd roundrect
			(at -2.2 2.95 180)
			(size 0.2 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 9 "OLED_VDD")
			(pinfunction "P2.02/SPI.SDI/SDO")
			(pintype "bidirectional")
		)
		(pad "14" smd roundrect
			(at -1.8 2.95 180)
			(size 0.2 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 92 "unconnected-(U2-P2.03-Pad14)")
			(pinfunction "P2.03")
			(pintype "bidirectional+no_connect")
		)
		(pad "15" smd roundrect
			(at -1.4 2.95 180)
			(size 0.2 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 75 "unconnected-(U2-P2.04{slash}SPI.SDI{slash}SDO-Pad15)")
			(pinfunction "P2.04/SPI.SDI/SDO")
			(pintype "bidirectional+no_connect")
		)
		(pad "16" smd roundrect
			(at -1 2.95 180)
			(size 0.2 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 97 "unconnected-(U2-P2.05{slash}SPI.CS-Pad16)")
			(pinfunction "P2.05/SPI.CS")
			(pintype "bidirectional+no_connect")
		)
		(pad "17" smd roundrect
			(at -0.6 2.95 180)
			(size 0.2 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 96 "unconnected-(U2-P2.06{slash}TRACECLK{slash}SPI.SCK-Pad17)")
			(pinfunction "P2.06/TRACECLK/SPI.SCK")
			(pintype "bidirectional+no_connect")
		)
		(pad "18" smd roundrect
			(at -0.2 2.95 180)
			(size 0.2 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 72 "unconnected-(U2-P2.07{slash}TRACEDATA[0]{slash}SWO{slash}SPI.DCX-Pad18)")
			(pinfunction "P2.07/TRACEDATA[0]/SWO/SPI.DCX")
			(pintype "bidirectional+no_connect")
		)
		(pad "19" smd roundrect
			(at 0.2 2.95 180)
			(size 0.2 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 91 "unconnected-(U2-P2.08{slash}TRACEDATA[1]{slash}SPI.SDI{slash}SDO-Pad19)")
			(pinfunction "P2.08/TRACEDATA[1]/SPI.SDI/SDO")
			(pintype "bidirectional+no_connect")
		)
		(pad "20" smd roundrect
			(at 0.6 2.95 180)
			(size 0.2 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 76 "unconnected-(U2-P2.09{slash}TRACEDATA[2]{slash}SPI.SDI{slash}SDO-Pad20)")
			(pinfunction "P2.09/TRACEDATA[2]/SPI.SDI/SDO")
			(pintype "bidirectional+no_connect")
		)
		(pad "21" smd roundrect
			(at 1 2.95 180)
			(size 0.2 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 99 "unconnected-(U2-P2.10{slash}TRACEDATA[3]{slash}SPIM.CS-Pad21)")
			(pinfunction "P2.10/TRACEDATA[3]/SPIM.CS")
			(pintype "bidirectional+no_connect")
		)
		(pad "22" smd roundrect
			(at 1.4 2.95 180)
			(size 0.2 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "+3.0V")
			(pinfunction "VDD")
			(pintype "power_in")
		)
		(pad "23" smd roundrect
			(at 1.8 2.95 180)
			(size 0.2 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 89 "unconnected-(U2-P0.00-Pad23)")
			(pinfunction "P0.00")
			(pintype "bidirectional+no_connect")
		)
		(pad "24" smd roundrect
			(at 2.2 2.95 180)
			(size 0.2 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 73 "unconnected-(U2-P0.01-Pad24)")
			(pinfunction "P0.01")
			(pintype "bidirectional+no_connect")
		)
		(pad "25" smd roundrect
			(at 2.95 2.2 180)
			(size 0.8 0.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 67 "Net-(J3-Pin_1)")
			(pinfunction "SWDIO")
			(pintype "unspecified")
		)
		(pad "26" smd roundrect
			(at 2.95 1.8 180)
			(size 0.8 0.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 65 "Net-(J3-Pin_2)")
			(pinfunction "SWDCLK")
			(pintype "unspecified")
		)
		(pad "27" smd roundrect
			(at 2.95 1.4 180)
			(size 0.8 0.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 77 "unconnected-(U2-P0.02-Pad27)")
			(pinfunction "P0.02")
			(pintype "bidirectional+no_connect")
		)
		(pad "28" smd roundrect
			(at 2.95 1 180)
			(size 0.8 0.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 90 "unconnected-(U2-P0.03{slash}GRTC_PWMOUT-Pad28)")
			(pinfunction "P0.03/GRTC_PWMOUT")
			(pintype "output+no_connect")
		)
		(pad "29" smd roundrect
			(at 2.95 0.6 180)
			(size 0.8 0.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 94 "unconnected-(U2-P0.04{slash}GRTC_CLKOUT32K-Pad29)")
			(pinfunction "P0.04/GRTC_CLKOUT32K")
			(pintype "output+no_connect")
		)
		(pad "30" smd roundrect
			(at 2.95 0.2 180)
			(size 0.8 0.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 57 "Net-(U2-NRESET)")
			(pinfunction "NRESET")
			(pintype "unspecified")
		)
		(pad "31" smd roundrect
			(at 2.95 -0.2 180)
			(size 0.8 0.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 69 "/ANT")
			(pinfunction "ANT")
			(pintype "unspecified")
		)
		(pad "32" smd roundrect
			(at 2.95 -0.6 180)
			(size 0.8 0.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "VSS_PA")
			(pintype "power_out")
		)
		(pad "33" smd roundrect
			(at 2.95 -1 180)
			(size 0.8 0.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 30 "/DECA")
			(pinfunction "DECRF")
			(pintype "unspecified")
		)
		(pad "34" smd roundrect
			(at 2.95 -1.4 180)
			(size 0.8 0.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 100 "Net-(U2-XC1)")
			(pinfunction "XC1")
			(pintype "bidirectional")
		)
		(pad "35" smd roundrect
			(at 2.95 -1.8 180)
			(size 0.8 0.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 98 "Net-(U2-XC2)")
			(pinfunction "XC2")
			(pintype "unspecified")
		)
		(pad "36" smd roundrect
			(at 2.95 -2.2 180)
			(size 0.8 0.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "+3.0V")
			(pinfunction "VDD")
			(pintype "power_in")
		)
		(pad "37" smd roundrect
			(at 2.2 -2.95 180)
			(size 0.2 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 93 "unconnected-(U2-P1.09{slash}TAMPC-Pad37)")
			(pinfunction "P1.09/TAMPC")
			(pintype "bidirectional+no_connect")
		)
		(pad "38" smd roundrect
			(at 1.8 -2.95 180)
			(size 0.2 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 39 "BAT_CHG")
			(pinfunction "P1.10/TAMPC")
			(pintype "bidirectional")
		)
		(pad "39" smd roundrect
			(at 1.4 -2.95 180)
			(size 0.2 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 33 "BAT_ERR")
			(pinfunction "P1.11/AIN4")
			(pintype "input")
		)
		(pad "40" smd roundrect
			(at 1 -2.95 180)
			(size 0.2 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 71 "unconnected-(U2-P1.12{slash}AIN5-Pad40)")
			(pinfunction "P1.12/AIN5")
			(pintype "input+no_connect")
		)
		(pad "41" smd roundrect
			(at 0.6 -2.95 180)
			(size 0.2 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 74 "unconnected-(U2-P1.13{slash}AIN6-Pad41)")
			(pinfunction "P1.13/AIN6")
			(pintype "input+no_connect")
		)
		(pad "42" smd roundrect
			(at 0.2 -2.95 180)
			(size 0.2 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 95 "unconnected-(U2-P1.14{slash}AIN7-Pad42)")
			(pinfunction "P1.14/AIN7")
			(pintype "input+no_connect")
		)
		(pad "43" smd roundrect
			(at -0.2 -2.95 180)
			(size 0.2 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 30 "/DECA")
			(pinfunction "DECA")
			(pintype "unspecified")
		)
		(pad "44" smd roundrect
			(at -0.6 -2.95 180)
			(size 0.2 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "VSS")
			(pintype "power_out")
		)
		(pad "45" smd roundrect
			(at -1 -2.95 180)
			(size 0.2 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 27 "/DECD")
			(pinfunction "DECD")
			(pintype "unspecified")
		)
		(pad "46" smd roundrect
			(at -1.4 -2.95 180)
			(size 0.2 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 68 "/DCC")
			(pinfunction "DCC")
			(pintype "unspecified")
		)
		(pad "47" smd roundrect
			(at -1.8 -2.95 180)
			(size 0.2 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "+3.0V")
			(pinfunction "VDD")
			(pintype "power_in")
		)
		(pad "48" smd roundrect
			(at -2.2 -2.95 180)
			(size 0.2 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "+3.0V")
			(pinfunction "VDD")
			(pintype "power_in")
		)
		(pad "49" smd rect
			(at 0 0 180)
			(size 4.6 4.6)
			(property pad_prop_heatsink)
			(layers "F.Cu" "F.Mask")
			(net 1 "GND")
			(pinfunction "VSS")
			(pintype "power_out")
			(zone_connect 2)
		)
		(embedded_fonts no)
		(model "${KIPRJMOD}/symbols/NRF54L15_QFAA_R/QFN48_6X6_NOR.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "rotary_enc:alps_ec05e"
		(layer "F.Cu")
		(at 195 69.5 -90)
		(property "Reference" "SW1"
			(at 0 -3 270)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "RotaryEncoder"
			(at 0.1 -9.4 270)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Rotary encoder, dual channel, incremental quadrate outputs"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "RotaryEncoder*")
		(sheetname "/")
		(sheetfile "watch.kicad_sch")
		(attr smd)
		(fp_line
			(start -3.3 -3.8)
			(end -2.3 -3.8)
			(layer "Edge.Cuts")
		)
		(fp_line
			(start 3.3 -3.8)
			(end 2.3 -3.8)
			(layer "Edge.Cuts")
		)
		(fp_line
			(start -3.3 -4.2)
			(end -2.3 -4.2)
			(layer "Edge.Cuts")
		)
		(fp_line
			(start 3.3 -4.2)
			(end 2.3 -4.2)
			(layer "Edge.Cuts")
		)
		(fp_arc
			(start -3.3 -3.8)
			(mid -3.5 -4)
			(end -3.3 -4.2)
			(layer "Edge.Cuts")
		)
		(fp_arc
			(start 2.3 -3.8)
			(mid 2.1 -4)
			(end 2.3 -4.2)
			(layer "Edge.Cuts")
		)
		(fp_arc
			(start -2.3 -4.2)
			(mid -2.1 -4)
			(end -2.3 -3.8)
			(layer "Edge.Cuts")
		)
		(fp_arc
			(start 3.3 -4.2)
			(mid 3.5 -4)
			(end 3.3 -3.8)
			(layer "Edge.Cuts")
		)
		(fp_text user "${REFERENCE}"
			(at 0.1 -7.9 270)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "4" smd roundrect
			(at -3.550001 -1.85 270)
			(size 1.1 2.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.2)
			(thermal_bridge_angle 45)
		)
		(pad "5" smd roundrect
			(at 3.550001 -1.85 270)
			(size 1.1 2.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.2)
			(thermal_bridge_angle 45)
		)
		(pad "A" smd rect
			(at -2 -1 270)
			(size 1 2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 53 "ENC_OUT_A")
			(pinfunction "A")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "B" smd rect
			(at 2 -1 270)
			(size 1 2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 54 "ENC_OUT_B")
			(pinfunction "B")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "C" smd rect
			(at 0 -1 270)
			(size 1 2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "C")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(embedded_fonts no)
		(model "${KIPRJMOD}/symbols/alps/LIB_EC05E1220202/EC05E1220202/3D/EC05E1220202.stp"
			(offset
				(xyz 0 4 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -0 -0 -180)
			)
		)
	)
	(footprint "lra_driver:BGA9C40P3X3_147X133X62"
		(layer "F.Cu")
		(at 177.65 77.85 90)
		(descr "YFF0009-C01")
		(tags "Integrated Circuit")
		(property "Reference" "IC1"
			(at -1.625 0.25 180)
			(layer "F.SilkS")
		)
		(property "Value" "DRV2625YFFR"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" "https://componentsearchengine.com/Datasheets/1/DRV2625YFFR.pdf"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Motor / Motion / Ignition Controllers & Drivers Advanced ERM & LRA Haptics Driver with Smart Loop and Embedded Effects Library 9-DSBGA -40 to 85"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Height" "0.625"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Part Number" "595-DRV2625YFFR"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Price/Stock" "https://www.mouser.co.uk/ProductDetail/Texas-Instruments/DRV2625YFFR?qs=n%252BTO0c4TDSZ6D6FykI88sg%3D%3D"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Name" "Texas Instruments"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Part_Number" "DRV2625YFFR"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "watch.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "A1" smd circle
			(at -0.4 -0.4 180)
			(size 0.2 0.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 28 "LRA_TRIG")
			(pinfunction "TRIG/_INTZ")
			(pintype "passive")
		)
		(pad "A2" smd circle
			(at 0 -0.4 180)
			(size 0.2 0.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 8 "Net-(IC1-REG)")
			(pinfunction "REG")
			(pintype "passive")
		)
		(pad "A3" smd circle
			(at 0.4 -0.4 180)
			(size 0.2 0.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 26 "Net-(IC1-OUT+)")
			(pinfunction "OUT+")
			(pintype "passive")
		)
		(pad "B1" smd circle
			(at -0.4 0 180)
			(size 0.2 0.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 61 "TWIM_SDA")
			(pinfunction "SDA")
			(pintype "passive")
		)
		(pad "B2" smd circle
			(at 0 0 180)
			(size 0.2 0.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "+3.0V")
			(pinfunction "NRST")
			(pintype "passive")
		)
		(pad "B3" smd circle
			(at 0.4 0 180)
			(size 0.2 0.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "C1" smd circle
			(at -0.4 0.4 180)
			(size 0.2 0.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 60 "TWIM_SCL")
			(pinfunction "SCL")
			(pintype "passive")
		)
		(pad "C2" smd circle
			(at 0 0.4 180)
			(size 0.2 0.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "+3.0V")
			(pinfunction "VDD")
			(pintype "passive")
		)
		(pad "C3" smd circle
			(at 0.4 0.4 180)
			(size 0.2 0.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 29 "Net-(IC1-OUT-)")
			(pinfunction "OUT-")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KIPRJMOD}/symbols/LIB_DRV2625YFFR/DRV2625YFFR/3D/DRV2625YFFR.stp"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "varicap:LXRW0YV201059"
		(layer "F.Cu")
		(at 160.3 67.8 90)
		(descr "LXRW0YV201-059-2")
		(tags "Capacitor")
		(property "Reference" "C1"
			(at 0.2 0.9 180)
			(layer "F.SilkS")
		)
		(property "Value" "LXRW0YV201-059"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTREV" "July, 2018"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "STANDARD" "Manufacturer Recommendations"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MAXIMUM_PACKAGE_HEIGHT" "0.3mm"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER" "Murata"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "watch.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -0.2 0.2 180)
			(size 0.2 0.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pintype "power_in")
		)
		(pad "2" smd rect
			(at -0.2 -0.2 180)
			(size 0.2 0.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 81 "/AAT_SERIES")
			(pintype "input")
		)
		(pad "3" smd rect
			(at 0.2 -0.2 180)
			(size 0.2 0.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 25 "Net-(C1-Pad3)")
			(pintype "passive")
		)
		(pad "4" smd rect
			(at 0.2 0.2 180)
			(size 0.2 0.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 20 "Net-(C1-Pad4)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KIPRJMOD}/symbols/LIB_LXRW0YV201-059(1)/LXRW0YV201-059/3D/LXRW0YV201-059.stp"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 162.1 70.3 90)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C42"
			(at -1.2 0 180)
			(layer "F.SilkS")
		)
		(property "Value" "620pF"
			(at 0 1.16 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "watch.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 90)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 21 "Net-(C42-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 90)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 164 91)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C25"
			(at 0 -1.16 0)
			(layer "F.SilkS")
		)
		(property "Value" "C0.1uF"
			(at 0 1.16 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "watch.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "+3.0V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(gr_arc
		(start 150 62.5)
		(mid 150.732233 60.732233)
		(end 152.5 60)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 150 62.5)
		(end 150 107.5)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 183.5 105.5)
		(mid 183 105)
		(end 183.5 104.5)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 200 107.5)
		(end 200 62.5)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 195.5 105.5)
		(end 183.5 105.5)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 197.5 60)
		(mid 199.267767 60.732233)
		(end 200 62.5)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 152.5 110)
		(end 197.5 110)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 197.5 60)
		(end 152.5 60)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 183.5 104.5)
		(end 195.5 104.5)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 195.5 104.5)
		(mid 196 105)
		(end 195.5 105.5)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 200 107.5)
		(mid 199.267767 109.267767)
		(end 197.5 110)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 152.5 110)
		(mid 150.732233 109.267767)
		(end 150 107.5)
		(layer "Edge.Cuts")
	)
	(gr_text "INT"
		(at 164.75 102.5 0)
		(layer "F.SilkS")
	)
	(gr_text "SWDIO"
		(at 155.5 84 0)
		(layer "F.SilkS")
	)
	(gr_text "NC"
		(at 167.25 108.75 0)
		(layer "F.SilkS")
	)
	(gr_text "SWDCLK"
		(at 155.5 90.6 0)
		(layer "F.SilkS")
	)
	(gr_text "BTNA"
		(at 162.25 108.75 0)
		(layer "F.SilkS")
	)
	(gr_text "SDA"
		(at 172.5 108.75 0)
		(layer "F.SilkS")
	)
	(gr_text "ENCA"
		(at 159.5 108.75 0)
		(layer "F.SilkS")
	)
	(gr_text "TRIG"
		(at 164.75 108.75 0)
		(layer "F.SilkS")
	)
	(gr_text "ENCB"
		(at 159.6 102.5 0)
		(layer "F.SilkS")
	)
	(gr_text "CHG"
		(at 157 102.5 0)
		(layer "F.SilkS")
	)
	(gr_text "NC"
		(at 175 102.5 0)
		(layer "F.SilkS")
	)
	(gr_text "8.7V"
		(at 177.5 98.5 0)
		(layer "F.SilkS")
	)
	(gr_text "GND"
		(at 180 102.5 0)
		(layer "F.SilkS")
	)
	(gr_text "3V"
		(at 180 108.75 0)
		(layer "F.SilkS")
	)
	(gr_text "3V"
		(at 177.5 108.75 0)
		(layer "F.SilkS")
	)
	(gr_text "OVDD"
		(at 170 108.75 0)
		(layer "F.SilkS")
	)
	(gr_text "GND"
		(at 177.5 102.5 0)
		(layer "F.SilkS")
	)
	(gr_text "ORST"
		(at 169.9 102.5 0)
		(layer "F.SilkS")
	)
	(gr_text "ERR"
		(at 157 108.75 0)
		(layer "F.SilkS")
	)
	(gr_text "ANT"
		(at 151.9 66.8 0)
		(layer "F.SilkS")
	)
	(gr_text "GND"
		(at 152 90.6 0)
		(layer "F.SilkS")
	)
	(gr_text "SH1107 OLED"
		(at 189.4 100.3 0)
		(layer "F.SilkS")
	)
	(gr_text "87EN"
		(at 167.25 102.5 0)
		(layer "F.SilkS")
	)
	(gr_text "T4T DEVICE"
		(at 163.75 74.225 0)
		(layer "F.SilkS")
	)
	(gr_text "5V"
		(at 152 84 0)
		(layer "F.SilkS")
	)
	(gr_text "LRA"
		(at 177.8 65.8 0)
		(layer "F.SilkS")
	)
	(gr_text "NC"
		(at 175 108.75 0)
		(layer "F.SilkS")
	)
	(gr_text "GND"
		(at 180 98.5 0)
		(layer "F.SilkS")
	)
	(gr_text "BTNB"
		(at 162.25 102.5 0)
		(layer "F.SilkS")
	)
	(gr_text "CERN-OHL-S"
		(at 187.1 65 0)
		(layer "F.SilkS")
	)
	(gr_text "PHW-1-1-2"
		(at 188.1 63.3 0)
		(layer "F.SilkS")
	)
	(gr_text "SCL"
		(at 172.4 102.5 0)
		(layer "F.SilkS")
	)
	(gr_text "NFC"
		(at 152.2 67.6 90)
		(layer "B.SilkS")
	)
	(gr_text "2.4G"
		(at 152.199999 92.8 90)
		(layer "B.SilkS")
	)
	(gr_text "6.4mm to end of connector\n\n"
		(at 200.9 100.7 0)
		(layer "Dwgs.User")
	)
	(gr_text "9.4mm of flex connector\nused to bend around radius 3mm"
		(at 200.7 105 0)
		(layer "Cmts.User")
	)
	(zone
		(net 66)
		(net_name "BTN_B")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30106)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 174.333891 98.856) (xy 174.333891 98.656) (xy 174.191473 98.661767) (xy 174.249 98.956003) (xy 174.416671 98.706562)
			)
		)
	)
	(zone
		(net 1)
		(net_name "GND")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30025)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 158.85 82.155764) (xy 158.65 82.155764) (xy 158.455764 82.691473) (xy 158.75 82.751) (xy 159.044236 82.691473)
			)
		)
	)
	(zone
		(net 60)
		(net_name "TWIM_SCL")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30109)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 171.948 91.083269) (xy 172.148 91.083269) (xy 172.143236 90.941854) (xy 171.849 90.999381) (xy 172.098441 91.167052)
			)
		)
	)
	(zone
		(net 51)
		(net_name "+8.7V_EN")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30063)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 168.483888 93.1) (xy 168.483888 93.3) (xy 169.058527 93.294236) (xy 169.001 93) (xy 168.833329 92.750559)
			)
		)
	)
	(zone
		(net 1)
		(net_name "GND")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30092)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 167.064364 68) (xy 167.064364 68.2) (xy 167.250559 68.566671) (xy 167.501 68.4) (xy 167.558527 68.105764)
			)
		)
	)
	(zone
		(net 54)
		(net_name "ENC_OUT_B")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30058)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 174.624477 97.965898) (xy 174.765898 97.824477) (xy 174.499441 97.333329) (xy 174.249293 97.499293)
				(xy 174.191473 97.794236)
			)
		)
	)
	(zone
		(net 1)
		(net_name "GND")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30098)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 162.227 69.005764) (xy 161.973 69.005764) (xy 162.433329 69.349441) (xy 162.6 69.101) (xy 162.541473 68.805764)
			)
		)
	)
	(zone
		(net 11)
		(net_name "/VDD_D")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30019)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 167.4 71.105764) (xy 167.2 71.105764) (xy 167.005764 71.641473) (xy 167.3 71.701) (xy 167.594236 71.641473)
			)
		)
	)
	(zone
		(net 1)
		(net_name "GND")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30020)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 159.344236 82.83) (xy 159.344236 82.63) (xy 158.808527 82.455764) (xy 158.749 82.75) (xy 158.808527 83.044236)
			)
		)
	)
	(zone
		(net 6)
		(net_name "/VSYS")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30070)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 164.15 78.694046) (xy 164.35 78.694046) (xy 164.628443 78.295673) (xy 164.379002 78.128002)
				(xy 164.084766 78.187529)
			)
		)
	)
	(zone
		(net 9)
		(net_name "OLED_VDD")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30021)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 168.155764 90.65) (xy 168.155764 90.85) (xy 168.691473 91.044236) (xy 168.751 90.75) (xy 168.691473 90.455764)
			)
		)
	)
	(zone
		(net 24)
		(net_name "/RFI+")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30071)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 168.4 71.237027) (xy 168.2 71.237027) (xy 167.916556 71.633329) (xy 168.165997 71.801) (xy 168.460233 71.741473)
			)
		)
	)
	(zone
		(net 7)
		(net_name "+8.7V")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30006)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 178.148 96.978765) (xy 177.948 96.978765) (xy 177.758252 97.514474) (xy 178.052488 97.574001)
				(xy 178.346724 97.514474)
			)
		)
	)
	(zone
		(net 1)
		(net_name "GND")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 3)
		(connect_pads thru_hole_only
			(clearance 0.2)
		)
		(min_thickness 0.2)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 110 20) (xy 240 20) (xy 240 150) (xy 110 150)
			)
		)
	)
	(zone
		(net 60)
		(net_name "TWIM_SCL")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30091)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 173.257055 80.428) (xy 173.257055 80.228) (xy 172.736329 80.500559) (xy 172.902 80.75) (xy 173.197236 80.808527)
			)
		)
	)
	(zone
		(net 47)
		(net_name "SH1107_RESET")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30102)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 167.95 92.7) (xy 167.95 92.9) (xy 168.316473 92.919236) (xy 168.376 92.625) (xy 168.125559 92.458329)
			)
		)
	)
	(zone
		(net 1)
		(net_name "GND")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30093)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 167.7 68.835636) (xy 167.9 68.835636) (xy 167.794236 68.341473) (xy 167.5 68.399) (xy 167.333329 68.649441)
			)
		)
	)
	(zone
		(net 60)
		(net_name "TWIM_SCL")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30111)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 171.948 80.832888) (xy 172.148 80.832888) (xy 172.143236 80.691473) (xy 171.849 80.749) (xy 172.098441 80.916671)
			)
		)
	)
	(zone
		(net 55)
		(net_name "Net-(AE1-Pad2)")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30001)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 153.025 70) (xy 153.025 69.8) (xy 152.370671 69.56903) (xy 151.799 70.05) (xy 152.453898 70.473602)
			)
		)
	)
	(zone
		(net 1)
		(net_name "GND")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30100)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 155.834236 80.1) (xy 155.834236 79.9) (xy 156.034236 79.558527) (xy 155.739 79.5) (xy 155.490559 79.666671)
			)
		)
	)
	(zone
		(net 11)
		(net_name "/VDD_D")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30107)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 169.917112 64.808) (xy 169.917112 65.008) (xy 169.833329 64.857559) (xy 170.001 65.107) (xy 170.058527 64.812764)
			)
		)
	)
	(zone
		(net 1)
		(net_name "GND")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30083)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 166.269673 79.925) (xy 166.269673 80.125) (xy 166.808527 80.044236) (xy 166.751 79.75) (xy 166.500559 79.583329)
			)
		)
	)
	(zone
		(net 1)
		(net_name "GND")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30101)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 162.043578 68.876817) (xy 162.223183 69.056422) (xy 162.350559 69.266671) (xy 162.600707 69.099293)
				(xy 162.541473 68.805764)
			)
		)
	)
	(zone
		(net 2)
		(net_name "+3.0V")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30016)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 169.655764 98.15) (xy 169.655764 98.35) (xy 170.191473 98.544236) (xy 170.251 98.25) (xy 170.191473 97.955764)
			)
		)
	)
	(zone
		(net 66)
		(net_name "BTN_B")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30096)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 185.32071 72.40929) (xy 185.17929 72.55071) (xy 185.010559 72.833329) (xy 185.260707 73.000707)
				(xy 185.509441 72.833329)
			)
		)
	)
	(zone
		(net 9)
		(net_name "OLED_VDD")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30052)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 181.23 90.15) (xy 181.23 90.35) (xy 181.741473 90.544236) (xy 181.801 90.25) (xy 181.741473 89.955764)
			)
		)
	)
	(zone
		(net 1)
		(net_name "GND")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30051)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 162.337326 68.537721) (xy 162.157721 68.717326) (xy 162.305764 69.158527) (xy 162.600707 69.100707)
				(xy 162.766671 68.850559)
			)
		)
	)
	(zone
		(net 1)
		(net_name "GND")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30065)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 177.55 77.077057) (xy 177.75 77.077057) (xy 177.999441 76.666671) (xy 177.75 76.499) (xy 177.455764 76.558527)
			)
		)
	)
	(zone
		(net 6)
		(net_name "/VSYS")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30010)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 166.155764 81.4) (xy 166.155764 81.6) (xy 166.691473 81.794236) (xy 166.751 81.5) (xy 166.691473 81.205764)
			)
		)
	)
	(zone
		(net 1)
		(net_name "GND")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30055)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 178.949142 97.037721) (xy 178.807721 97.179142) (xy 178.955764 97.631527) (xy 179.250707 97.573707)
				(xy 179.416671 97.323559)
			)
		)
	)
	(zone
		(net 1)
		(net_name "GND")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30043)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 164.509102 95.349477) (xy 164.650523 95.490898) (xy 165.166671 95.249441) (xy 165.000707 94.999293)
				(xy 164.750559 94.833329)
			)
		)
	)
	(zone
		(net 66)
		(net_name "BTN_B")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30074)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 194.556 75.303861) (xy 194.756 75.303861) (xy 194.794236 74.808527) (xy 194.5 74.749) (xy 194.250559 74.916671)
			)
		)
	)
	(zone
		(net 1)
		(net_name "GND")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30046)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 165.259102 78.599477) (xy 165.400523 78.740898) (xy 165.916671 78.499441) (xy 165.750707 78.249293)
				(xy 165.500559 78.083329)
			)
		)
	)
	(zone
		(net 1)
		(net_name "GND")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30005)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 180.405764 97.175) (xy 180.405764 97.375) (xy 180.941473 97.544236) (xy 181.001 97.25) (xy 180.941473 96.955764)
			)
		)
	)
	(zone
		(net 2)
		(net_name "+3.0V")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30088)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 174.240682 93.1) (xy 174.240682 92.9) (xy 173.691473 92.955764) (xy 173.749 93.25) (xy 173.999441 93.416671)
			)
		)
	)
	(zone
		(net 56)
		(net_name "Net-(AE1-Pad1)")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30000)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 153.025 68.4) (xy 153.025 68.2) (xy 152.453898 67.726397) (xy 151.799 68.15) (xy 152.370671 68.63097)
			)
		)
	)
	(zone
		(net 1)
		(net_name "GND")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30064)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 158.1 68.583888) (xy 157.9 68.583888) (xy 157.905764 69.158527) (xy 158.2 69.101) (xy 158.449441 68.933329)
			)
		)
	)
	(zone
		(net 1)
		(net_name "GND")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30086)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 160.157848 63.529269) (xy 160.299269 63.387848) (xy 159.866671 63.050559) (xy 159.699293 63.299293)
				(xy 159.758527 63.594236)
			)
		)
	)
	(zone
		(net 1)
		(net_name "GND")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30028)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 158.155764 81.88) (xy 158.155764 82.08) (xy 158.691473 82.294236) (xy 158.751 82) (xy 158.691473 81.705764)
			)
		)
	)
	(zone
		(net 28)
		(net_name "LRA_TRIG")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30080)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 177.137345 78.504075) (xy 176.995925 78.362655) (xy 176.558527 78.205764) (xy 176.499293 78.500707)
				(xy 176.666671 78.749441)
			)
		)
	)
	(zone
		(net 26)
		(net_name "Net-(IC1-OUT+)")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30040)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 177.149477 77.490898) (xy 177.290898 77.349477) (xy 177.049441 76.833329) (xy 176.799293 76.999293)
				(xy 176.633329 77.249441)
			)
		)
	)
	(zone
		(net 80)
		(net_name "/AAT_PARALLEL")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30078)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 157.5 69.52855) (xy 157.7 69.52855) (xy 157.449441 68.933329) (xy 157.2 69.099) (xy 157.141473 69.394236)
			)
		)
	)
	(zone
		(net 1)
		(net_name "GND")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30018)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 158.1 69.694236) (xy 158.3 69.694236) (xy 158.494236 69.158527) (xy 158.2 69.099) (xy 157.905764 69.158527)
			)
		)
	)
	(zone
		(net 1)
		(net_name "GND")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30077)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 174.67358 82.188) (xy 174.67358 81.988) (xy 174.083329 82.250559) (xy 174.249 82.5) (xy 174.544236 82.558527)
			)
		)
	)
	(zone
		(net 28)
		(net_name "LRA_TRIG")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30068)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 169.823987 97.135) (xy 169.823987 96.935) (xy 169.308527 96.848176) (xy 169.249 97.142412) (xy 169.416671 97.391853)
			)
		)
	)
	(zone
		(net 1)
		(net_name "GND")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30062)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 160.6 64.683888) (xy 160.4 64.683888) (xy 160.405764 65.258527) (xy 160.7 65.201) (xy 160.949441 65.033329)
			)
		)
	)
	(zone
		(net 9)
		(net_name "OLED_VDD")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30085)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 186.921942 93.280521) (xy 186.780521 93.421942) (xy 187.217174 93.749441) (xy 187.384552 93.500707)
				(xy 187.325318 93.205764)
			)
		)
	)
	(zone
		(net 62)
		(net_name "ACCEL_INT")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30084)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 170.384277 97.778994) (xy 170.525699 97.637572) (xy 170.087602 97.313559) (xy 169.920224 97.562293)
				(xy 169.979458 97.857236)
			)
		)
	)
	(zone
		(net 62)
		(net_name "ACCEL_INT")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30048)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 173.618252 83.777877) (xy 173.476831 83.636456) (xy 172.960683 83.877913) (xy 173.126647 84.128061)
				(xy 173.376795 84.294025)
			)
		)
	)
	(zone
		(net 1)
		(net_name "GND")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30103)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 162.269615 69.09001) (xy 162.09001 69.269615) (xy 162.541473 69.394236) (xy 162.600707 69.100707)
				(xy 162.350559 68.933329)
			)
		)
	)
	(zone
		(net 1)
		(net_name "GND")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30022)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 174.4 95.094236) (xy 174.6 95.094236) (xy 174.794236 94.558527) (xy 174.5 94.499) (xy 174.205764 94.558527)
			)
		)
	)
	(zone
		(net 64)
		(net_name "BTN_A")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30009)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 190.35 72.405764) (xy 190.15 72.405764) (xy 189.955764 72.941473) (xy 190.25 73.001) (xy 190.544236 72.941473)
			)
		)
	)
	(zone
		(net 64)
		(net_name "BTN_A")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30054)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 173.867026 99.225605) (xy 173.725605 99.367026) (xy 174.000559 99.849677) (xy 174.250707 99.683713)
				(xy 174.308527 99.38877)
			)
		)
	)
	(zone
		(net 39)
		(net_name "BAT_CHG")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30056)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 162.844236 98.678) (xy 162.844236 98.478) (xy 162.308527 98.328764) (xy 162.249 98.623) (xy 162.416671 98.872441)
			)
		)
	)
	(zone
		(net 2)
		(net_name "+3.0V")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30087)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 174.240682 93.1) (xy 174.240682 92.9) (xy 173.999441 92.583329) (xy 173.749 92.75) (xy 173.691473 93.044236)
			)
		)
	)
	(zone
		(net 66)
		(net_name "BTN_B")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30099)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 185.34071 72.57071) (xy 185.19929 72.42929) (xy 185.010559 72.833329) (xy 185.259293 73.000707)
				(xy 185.509441 72.833329)
			)
		)
	)
	(zone
		(net 33)
		(net_name "BAT_ERR")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30072)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 163.444562 98.910547) (xy 163.303141 98.769126) (xy 162.816474 98.834407) (xy 162.874294 99.12935)
				(xy 163.124442 99.295314)
			)
		)
	)
	(zone
		(net 1)
		(net_name "GND")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30042)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 160.910523 99.499102) (xy 160.769102 99.640523) (xy 161.000559 100.166671) (xy 161.250707 100.000707)
				(xy 161.416671 99.750559)
			)
		)
	)
	(zone
		(net 17)
		(net_name "/VDD")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30060)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 164.279645 66.821066) (xy 164.421066 66.679645) (xy 164.294236 66.218473) (xy 163.999293 66.276293)
				(xy 163.833329 66.526441)
			)
		)
	)
	(zone
		(net 1)
		(net_name "GND")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30023)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 163.4 100.094236) (xy 163.6 100.094236) (xy 163.794236 99.558527) (xy 163.5 99.499) (xy 163.205764 99.558527)
			)
		)
	)
	(zone
		(net 80)
		(net_name "/AAT_PARALLEL")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30026)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 166.795098 71.509032) (xy 166.595098 71.509032) (xy 166.400862 72.044741) (xy 166.695098 72.104268)
				(xy 166.989334 72.044741)
			)
		)
	)
	(zone
		(net 28)
		(net_name "LRA_TRIG")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30079)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 168.744698 97.027706) (xy 168.603277 97.169127) (xy 169.083329 97.391853) (xy 169.250707 97.143119)
				(xy 169.191473 96.848176)
			)
		)
	)
	(zone
		(net 51)
		(net_name "+8.7V_EN")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30015)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 176.85 94.405764) (xy 176.65 94.405764) (xy 176.455764 94.941473) (xy 176.75 95.001) (xy 177.044236 94.941473)
			)
		)
	)
	(zone
		(net 2)
		(net_name "+3.0V")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30081)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 159.651487 99.759934) (xy 159.510066 99.618513) (xy 159.250559 100.083329) (xy 159.499293 100.250707)
				(xy 159.794236 100.191473)
			)
		)
	)
	(zone
		(net 2)
		(net_name "+3.0V")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30003)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 169.721234 81.938391) (xy 169.438391 82.221234) (xy 169.750559 82.666671) (xy 170.000707 82.500707)
				(xy 170.166671 82.250559)
			)
		)
	)
	(zone
		(net 39)
		(net_name "BAT_CHG")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30035)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 167.650523 78.259102) (xy 167.509102 78.400523) (xy 167.750559 78.916671) (xy 168.000707 78.750707)
				(xy 168.166671 78.500559)
			)
		)
	)
	(zone
		(net 53)
		(net_name "ENC_OUT_A")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30110)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 174.332888 98.528) (xy 174.332888 98.328) (xy 174.416671 98.478441) (xy 174.249 98.229) (xy 174.191473 98.523236)
			)
		)
	)
	(zone
		(net 1)
		(net_name "GND")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30075)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 177.32929 93.129289) (xy 177.470711 93.27071) (xy 177.916671 92.999441) (xy 177.750707 92.749293)
				(xy 177.455764 92.691473)
			)
		)
	)
	(zone
		(net 1)
		(net_name "GND")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30095)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 164.48 90.9) (xy 164.48 91.1) (xy 164.833329 91.249441) (xy 165.001 91) (xy 164.833329 90.750559)
			)
		)
	)
	(zone
		(net 1)
		(net_name "GND")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30047)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 155.849477 69.590898) (xy 155.990898 69.449477) (xy 155.749441 68.933329) (xy 155.499293 69.099293)
				(xy 155.333329 69.349441)
			)
		)
	)
	(zone
		(net 22)
		(net_name "/RFI-")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30061)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 168.9 71.220043) (xy 168.7 71.220043) (xy 168.598764 71.741473) (xy 168.893 71.801) (xy 169.142441 71.633329)
			)
		)
	)
	(zone
		(net 54)
		(net_name "ENC_OUT_B")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30017)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 191.6 71.094236) (xy 191.8 71.094236) (xy 191.994236 70.558527) (xy 191.7 70.499) (xy 191.405764 70.558527)
			)
		)
	)
	(zone
		(net 2)
		(net_name "+3.0V")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30011)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 185.15 67.594236) (xy 185.35 67.594236) (xy 185.544236 67.058527) (xy 185.25 66.999) (xy 184.955764 67.058527)
			)
		)
	)
	(zone
		(net 80)
		(net_name "/AAT_PARALLEL")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30029)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 157.3 68.505764) (xy 157.1 68.505764) (xy 156.905764 69.041473) (xy 157.2 69.101) (xy 157.494236 69.041473)
			)
		)
	)
	(zone
		(net 1)
		(net_name "GND")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30027)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 157.594236 80.1) (xy 157.594236 79.9) (xy 157.058527 79.705764) (xy 156.999 80) (xy 157.058527 80.294236)
			)
		)
	)
	(zone
		(net 1)
		(net_name "GND")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30031)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 158.794236 69.2) (xy 158.794236 69) (xy 158.258527 68.805764) (xy 158.199 69.1) (xy 158.258527 69.394236)
			)
		)
	)
	(zone
		(net 64)
		(net_name "BTN_A")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30044)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 195.009102 74.849477) (xy 195.150523 74.990898) (xy 195.666671 74.749441) (xy 195.500707 74.499293)
				(xy 195.250559 74.333329)
			)
		)
	)
	(zone
		(net 30)
		(net_name "/DECA")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30089)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 161.248966 101.33) (xy 161.248966 101.13) (xy 160.999441 100.833329) (xy 160.749 101) (xy 160.691473 101.294236)
			)
		)
	)
	(zone
		(net 62)
		(net_name "ACCEL_INT")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30069)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 169.346944 97.570412) (xy 169.346944 97.770412) (xy 169.862404 97.857236) (xy 169.921931 97.563)
				(xy 169.75426 97.313559)
			)
		)
	)
	(zone
		(net 81)
		(net_name "/AAT_SERIES")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30067)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 160.4 69.677057) (xy 160.6 69.677057) (xy 160.694236 69.158527) (xy 160.4 69.099) (xy 160.150559 69.266671)
			)
		)
	)
	(zone
		(net 1)
		(net_name "GND")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30050)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 164.349477 81.765898) (xy 164.490898 81.624477) (xy 164.249441 81.108329) (xy 163.999293 81.274293)
				(xy 163.833329 81.524441)
			)
		)
	)
	(zone
		(net 33)
		(net_name "BAT_ERR")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30037)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 168.400523 78.009102) (xy 168.259102 78.150523) (xy 168.500559 78.666671) (xy 168.750707 78.500707)
				(xy 168.916671 78.250559)
			)
		)
	)
	(zone
		(net 51)
		(net_name "+8.7V_EN")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30014)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 183.194236 97.073) (xy 183.194236 96.873) (xy 182.658527 96.678764) (xy 182.599 96.973) (xy 182.658527 97.267236)
			)
		)
	)
	(zone
		(net 1)
		(net_name "GND")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30012)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 164.65 82.594236) (xy 164.85 82.594236) (xy 165.044236 82.058527) (xy 164.75 81.999) (xy 164.455764 82.058527)
			)
		)
	)
	(zone
		(net 12)
		(net_name "Net-(O1-VCOMH)")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30039)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 186.377526 93.509102) (xy 186.236105 93.650523) (xy 186.477562 94.166671) (xy 186.72771 94.000707)
				(xy 186.893674 93.750559)
			)
		)
	)
	(zone
		(net 2)
		(net_name "+3.0V")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30004)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 190.15 67.594236) (xy 190.35 67.594236) (xy 190.544236 67.058527) (xy 190.25 66.999) (xy 189.955764 67.058527)
			)
		)
	)
	(zone
		(net 2)
		(net_name "+3.0V")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30094)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 171.736502 95.655081) (xy 171.595081 95.796502) (xy 172.083329 95.999441) (xy 172.250707 95.750707)
				(xy 172.083329 95.500559)
			)
		)
	)
	(zone
		(net 1)
		(net_name "GND")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30032)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 170.85 70.155764) (xy 170.65 70.155764) (xy 170.455764 70.691473) (xy 170.75 70.751) (xy 171.044236 70.691473)
			)
		)
	)
	(zone
		(net 81)
		(net_name "/AAT_SERIES")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30090)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 166.4 71.18606) (xy 166.2 71.18606) (xy 165.926592 71.445994) (xy 166.093263 71.696435) (xy 166.387499 71.753962)
			)
		)
	)
	(zone
		(net 60)
		(net_name "TWIM_SCL")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30049)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 173.252477 81.240898) (xy 173.393898 81.099477) (xy 173.152441 80.583329) (xy 172.902293 80.749293)
				(xy 172.736329 80.999441)
			)
		)
	)
	(zone
		(net 1)
		(net_name "GND")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30104)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 179.473523 97.082102) (xy 179.332102 97.223523) (xy 179.083329 97.323559) (xy 179.250707 97.573707)
				(xy 179.544236 97.514473)
			)
		)
	)
	(zone
		(net 1)
		(net_name "GND")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30008)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 156.405764 79.9) (xy 156.405764 80.1) (xy 156.941473 80.294236) (xy 157.001 80) (xy 156.941473 79.705764)
			)
		)
	)
	(zone
		(net 30)
		(net_name "/DECA")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30013)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 160.594236 96.85) (xy 160.594236 96.65) (xy 160.058527 96.455764) (xy 159.999 96.75) (xy 160.058527 97.044236)
			)
		)
	)
	(zone
		(net 51)
		(net_name "+8.7V_EN")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30036)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 183.850523 97.082102) (xy 183.709102 97.223523) (xy 183.950559 97.739671) (xy 184.200707 97.573707)
				(xy 184.366671 97.323559)
			)
		)
	)
	(zone
		(net 63)
		(net_name "NFC_IRQ")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30073)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 168.443654 95.5) (xy 168.443654 95.7) (xy 168.833329 95.999441) (xy 169.001 95.75) (xy 168.941473 95.455764)
			)
		)
	)
	(zone
		(net 2)
		(net_name "+3.0V")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30066)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 163.5 90.827057) (xy 163.7 90.827057) (xy 163.794236 90.308527) (xy 163.5 90.249) (xy 163.250559 90.416671)
			)
		)
	)
	(zone
		(net 7)
		(net_name "+8.7V")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30007)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 185.405764 94.4) (xy 185.405764 94.6) (xy 185.941473 94.794236) (xy 186.001 94.5) (xy 185.941473 94.205764)
			)
		)
	)
	(zone
		(net 9)
		(net_name "OLED_VDD")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30076)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 182.235657 90.577078) (xy 182.377078 90.435657) (xy 182.049441 90.083329) (xy 181.799293 90.249293)
				(xy 181.741473 90.544236)
			)
		)
	)
	(zone
		(net 1)
		(net_name "GND")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30038)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 164.388023 81.521602) (xy 164.246602 81.663023) (xy 164.500559 82.166671) (xy 164.750707 82.000707)
				(xy 164.916671 81.750559)
			)
		)
	)
	(zone
		(net 1)
		(net_name "GND")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30057)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 167.204091 67.86267) (xy 167.06267 68.004091) (xy 167.205764 68.458527) (xy 167.500707 68.400707)
				(xy 167.666671 68.150559)
			)
		)
	)
	(zone
		(net 1)
		(net_name "GND")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30030)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 158.405764 69) (xy 158.405764 69.2) (xy 158.941473 69.394236) (xy 159.001 69.1) (xy 158.941473 68.805764)
			)
		)
	)
	(zone
		(net 2)
		(net_name "+3.0V")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30097)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 171.4 92.49) (xy 171.6 92.49) (xy 171.749441 92.166671) (xy 171.5 91.999) (xy 171.250559 92.166671)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layer "F.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(keepout
			(tracks allowed)
			(vias allowed)
			(pads allowed)
			(copperpour not_allowed)
			(footprints allowed)
		)
		(placement
			(enabled no)
			(sheetname "")
		)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 173.4 80.575) (xy 176.4 80.575) (xy 176.4 80.975) (xy 173.4 80.975)
			)
		)
	)
	(zone
		(net 63)
		(net_name "NFC_IRQ")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30059)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 168.594236 91.572) (xy 168.594236 91.372) (xy 168.058527 91.205764) (xy 167.999 91.5) (xy 168.166671 91.749441)
			)
		)
	)
	(zone
		(net 9)
		(net_name "OLED_VDD")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30041)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 188.950523 97.009102) (xy 188.809102 97.150523) (xy 189.050559 97.666671) (xy 189.300707 97.500707)
				(xy 189.466671 97.250559)
			)
		)
	)
	(zone
		(net 2)
		(net_name "+3.0V")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30002)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 169.778766 82.561609) (xy 170.061609 82.278766) (xy 169.749441 81.833329) (xy 169.499293 81.999293)
				(xy 169.333329 82.249441)
			)
		)
	)
	(zone
		(net 1)
		(net_name "GND")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30045)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 165.349477 95.490898) (xy 165.490898 95.349477) (xy 165.249441 94.833329) (xy 164.999293 94.999293)
				(xy 164.833329 95.249441)
			)
		)
	)
	(zone
		(net 9)
		(net_name "OLED_VDD")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30033)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 187.283845 94.094236) (xy 187.483845 94.094236) (xy 187.678081 93.558527) (xy 187.383845 93.499)
				(xy 187.089609 93.558527)
			)
		)
	)
	(zone
		(net 81)
		(net_name "/AAT_SERIES")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30082)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 160.2 68.630028) (xy 160 68.630028) (xy 160.105764 69.158527) (xy 160.4 69.101) (xy 160.566671 68.850559)
			)
		)
	)
	(zone
		(net 15)
		(net_name "/VDD_DR")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30105)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 163.194236 65.65) (xy 163.194236 65.85) (xy 162.905764 65.808527) (xy 163.201 65.75) (xy 162.905764 65.808527)
			)
		)
	)
	(zone
		(net 1)
		(net_name "GND")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30024)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 158.65 82.594236) (xy 158.85 82.594236) (xy 159.044236 82.058527) (xy 158.75 81.999) (xy 158.455764 82.058527)
			)
		)
	)
	(zone
		(net 48)
		(net_name "Net-(O1-IREF)")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30034)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 188.400523 93.009102) (xy 188.259102 93.150523) (xy 188.500559 93.666671) (xy 188.750707 93.500707)
				(xy 188.916671 93.250559)
			)
		)
	)
	(zone
		(net 61)
		(net_name "TWIM_SDA")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30108)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 172.276 90.582888) (xy 172.476 90.582888) (xy 172.325559 90.666671) (xy 172.575 90.499) (xy 172.280764 90.441473)
			)
		)
	)
	(zone
		(net 64)
		(net_name "BTN_A")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30053)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 174.774395 99.367026) (xy 174.632974 99.225605) (xy 174.191473 99.38877) (xy 174.249293 99.683713)
				(xy 174.499441 99.849677)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layers "F.Cu" "B.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(keepout
			(tracks allowed)
			(vias allowed)
			(pads allowed)
			(copperpour not_allowed)
			(footprints allowed)
		)
		(placement
			(enabled no)
			(sheetname "/")
		)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 176.4 103.3) (xy 181.1 103.3) (xy 181.1 107.8) (xy 176.4 107.8)
			)
		)
	)
	(zone
		(net 81)
		(net_name "/AAT_SERIES")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30036)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 160.749477 69.590898) (xy 160.890898 69.449477) (xy 160.649441 68.933329) (xy 160.399293 69.099293)
				(xy 160.233329 69.349441)
			)
		)
	)
	(zone
		(net 22)
		(net_name "/RFI-")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30053)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 156.449477 72.390898) (xy 156.590898 72.249477) (xy 156.349441 71.733329) (xy 156.099293 71.899293)
				(xy 155.933329 72.149441)
			)
		)
	)
	(zone
		(net 63)
		(net_name "NFC_IRQ")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30066)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 167.747 92.055104) (xy 167.947 92.055104) (xy 168.249441 91.666671) (xy 168 91.499) (xy 167.705764 91.558527)
			)
		)
	)
	(zone
		(net 39)
		(net_name "BAT_CHG")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30046)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 168.349477 79.240898) (xy 168.490898 79.099477) (xy 168.249441 78.583329) (xy 167.999293 78.749293)
				(xy 167.833329 78.999441)
			)
		)
	)
	(zone
		(net 12)
		(net_name "Net-(O1-VCOMH)")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30057)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 186.827003 94.5) (xy 186.627003 94.5) (xy 186.522038 94.7) (xy 186.7 95.601) (xy 186.9 94.7)
			)
		)
	)
	(zone
		(net 33)
		(net_name "BAT_ERR")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30030)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 168.65 79.094236) (xy 168.85 79.094236) (xy 169.044236 78.558527) (xy 168.75 78.499) (xy 168.455764 78.558527)
			)
		)
	)
	(zone
		(net 63)
		(net_name "NFC_IRQ")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30008)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 169.1 95.155764) (xy 168.9 95.155764) (xy 168.705764 95.691473) (xy 169 95.751) (xy 169.294236 95.691473)
			)
		)
	)
	(zone
		(net 30)
		(net_name "/DECA")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30027)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 159.9 97.344236) (xy 160.1 97.344236) (xy 160.294236 96.808527) (xy 160 96.749) (xy 159.705764 96.808527)
			)
		)
	)
	(zone
		(net 60)
		(net_name "TWIM_SCL")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30054)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 172.198477 91.491279) (xy 172.339898 91.349858) (xy 172.098441 90.83371) (xy 171.848293 90.999674)
				(xy 171.682329 91.249822)
			)
		)
	)
	(zone
		(net 9)
		(net_name "OLED_VDD")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30022)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 187.3 94.094236) (xy 187.5 94.094236) (xy 187.678081 93.558527) (xy 187.383845 93.499) (xy 187.089609 93.558527)
			)
		)
	)
	(zone
		(net 62)
		(net_name "ACCEL_INT")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30062)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 172.831706 84.563011) (xy 172.973127 84.704432) (xy 173.376795 84.294025) (xy 173.128061 84.126647)
				(xy 172.833118 84.068827)
			)
		)
	)
	(zone
		(net 9)
		(net_name "OLED_VDD")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30072)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 187.8 95.7) (xy 187.8 95.5) (xy 187.6 95.4) (xy 187.399 95.6) (xy 187.6 95.8)
			)
		)
	)
	(zone
		(net 61)
		(net_name "TWIM_SDA")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30056)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 172.924477 90.990898) (xy 173.065898 90.849477) (xy 172.824441 90.333329) (xy 172.574293 90.499293)
				(xy 172.408329 90.749441)
			)
		)
	)
	(zone
		(net 60)
		(net_name "TWIM_SCL")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30004)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 191.7 94.5) (xy 191.5 94.5) (xy 191.4 94.7) (xy 191.6 95.601) (xy 191.8 94.7)
			)
		)
	)
	(zone
		(net 11)
		(net_name "/VDD_D")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30017)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 169.9 65.701236) (xy 170.1 65.701236) (xy 170.294236 65.165527) (xy 170 65.106) (xy 169.705764 65.165527)
			)
		)
	)
	(zone
		(net 17)
		(net_name "/VDD")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30020)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 164.1 65.682764) (xy 163.9 65.682764) (xy 163.705764 66.218473) (xy 164 66.278) (xy 164.294236 66.218473)
			)
		)
	)
	(zone
		(net 39)
		(net_name "BAT_CHG")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30059)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 162.178 99.217236) (xy 162.378 99.217236) (xy 162.544236 98.681527) (xy 162.25 98.622) (xy 162.000559 98.789671)
			)
		)
	)
	(zone
		(net 9)
		(net_name "OLED_VDD")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30034)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 188.705764 97.4) (xy 188.705764 97.6) (xy 189.241473 97.794236) (xy 189.301 97.5) (xy 189.241473 97.205764)
			)
		)
	)
	(zone
		(net 70)
		(net_name "Net-(R3-Pad2)")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30031)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 161.7 88.594236) (xy 161.9 88.594236) (xy 162.094236 88.058527) (xy 161.8 87.999) (xy 161.505764 88.058527)
			)
		)
	)
	(zone
		(net 9)
		(net_name "OLED_VDD")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30073)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 187.7 95.5) (xy 187.7 95.7) (xy 187.9 95.8) (xy 188.101 95.6) (xy 187.9 95.4)
			)
		)
	)
	(zone
		(net 51)
		(net_name "+8.7V_EN")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30060)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 176.155764 94.928) (xy 176.155764 95.128) (xy 176.691473 95.294236) (xy 176.751 95) (xy 176.583329 94.750559)
			)
		)
	)
	(zone
		(net 33)
		(net_name "BAT_ERR")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30067)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 163.452079 98.941164) (xy 163.310658 98.799743) (xy 162.816474 98.834407) (xy 162.874294 99.12935)
				(xy 163.124442 99.295314)
			)
		)
	)
	(zone
		(net 47)
		(net_name "SH1107_RESET")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30000)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 189.987868 96.57071) (xy 190.12929 96.712132) (xy 190.279718 96.5) (xy 190.200707 95.599293)
				(xy 190 95.590898)
			)
		)
	)
	(zone
		(net 54)
		(net_name "ENC_OUT_B")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30011)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 192.294236 70.6) (xy 192.294236 70.4) (xy 191.758527 70.205764) (xy 191.699 70.5) (xy 191.758527 70.794236)
			)
		)
	)
	(zone
		(net 47)
		(net_name "SH1107_RESET")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30070)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 168.370925 93.262345) (xy 168.512345 93.120925) (xy 168.669236 92.683527) (xy 168.374293 92.624293)
				(xy 168.125559 92.791671)
			)
		)
	)
	(zone
		(net 66)
		(net_name "BTN_B")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30033)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 173.655764 98.856003) (xy 173.655764 99.056003) (xy 174.191473 99.250239) (xy 174.251 98.956003)
				(xy 174.191473 98.661767)
			)
		)
	)
	(zone
		(net 26)
		(net_name "Net-(IC1-OUT+)")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30025)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 176.9 76.405764) (xy 176.7 76.405764) (xy 176.505764 76.941473) (xy 176.8 77.001) (xy 177.094236 76.941473)
			)
		)
	)
	(zone
		(net 9)
		(net_name "OLED_VDD")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30048)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 169.240898 90.400523) (xy 169.099477 90.259102) (xy 168.583329 90.500559) (xy 168.749293 90.750707)
				(xy 168.999441 90.916671)
			)
		)
	)
	(zone
		(net 17)
		(net_name "/VDD")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30021)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 161.994236 64.3) (xy 161.994236 64.1) (xy 161.458527 63.905764) (xy 161.399 64.2) (xy 161.458527 64.494236)
			)
		)
	)
	(zone
		(net 9)
		(net_name "OLED_VDD")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30007)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 187.5 94.5) (xy 187.3 94.5) (xy 187.2 94.7) (xy 187.4 95.601) (xy 187.6 94.7)
			)
		)
	)
	(zone
		(net 6)
		(net_name "/VSYS")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30045)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 164.728479 78.6199) (xy 164.8699 78.478479) (xy 164.628443 77.962331) (xy 164.378295 78.128295)
				(xy 164.212331 78.378443)
			)
		)
	)
	(zone
		(net 62)
		(net_name "ACCEL_INT")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30063)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 169.346944 97.570412) (xy 169.346944 97.770412) (xy 169.862404 97.857236) (xy 169.921931 97.563)
				(xy 169.75426 97.313559)
			)
		)
	)
	(zone
		(net 80)
		(net_name "/AAT_PARALLEL")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30038)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 157.549477 69.590898) (xy 157.690898 69.449477) (xy 157.449441 68.933329) (xy 157.199293 69.099293)
				(xy 157.033329 69.349441)
			)
		)
	)
	(zone
		(net 22)
		(net_name "/RFI-")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30055)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 168.411953 72.159328) (xy 168.553374 72.300749) (xy 169.059671 72.049441) (xy 168.893707 71.799293)
				(xy 168.643559 71.633329)
			)
		)
	)
	(zone
		(net 7)
		(net_name "+8.7V")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30024)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 185.9 95.094236) (xy 186.1 95.094236) (xy 186.294236 94.558527) (xy 186 94.499) (xy 185.705764 94.558527)
			)
		)
	)
	(zone
		(net 48)
		(net_name "Net-(O1-IREF)")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30003)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 188.9 94.5) (xy 188.7 94.5) (xy 188.6 94.7) (xy 188.8 95.601) (xy 189 94.7)
			)
		)
	)
	(zone
		(net 6)
		(net_name "/VSYS")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30049)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 166.259102 81.849477) (xy 166.400523 81.990898) (xy 166.916671 81.749441) (xy 166.750707 81.499293)
				(xy 166.500559 81.333329)
			)
		)
	)
	(zone
		(net 1)
		(net_name "GND")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30065)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 190.8 94.056346) (xy 191 94.056346) (xy 191.044236 93.558527) (xy 190.75 93.499) (xy 190.500559 93.666671)
			)
		)
	)
	(zone
		(net 51)
		(net_name "+8.7V_EN")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30013)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 184.1 98.167236) (xy 184.3 98.167236) (xy 184.494236 97.631527) (xy 184.2 97.572) (xy 183.905764 97.631527)
			)
		)
	)
	(zone
		(net 28)
		(net_name "LRA_TRIG")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30050)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 168.900523 96.651514) (xy 168.759102 96.792935) (xy 169.000559 97.309083) (xy 169.250707 97.143119)
				(xy 169.416671 96.892971)
			)
		)
	)
	(zone
		(net 60)
		(net_name "TWIM_SCL")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30014)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 172.308764 80.65) (xy 172.308764 80.85) (xy 172.844473 81.044236) (xy 172.904 80.75) (xy 172.844473 80.455764)
			)
		)
	)
	(zone
		(net 51)
		(net_name "+8.7V_EN")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30061)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 177.344236 95.128) (xy 177.344236 94.928) (xy 176.916671 94.750559) (xy 176.749 95) (xy 176.808527 95.294236)
			)
		)
	)
	(zone
		(net 1)
		(net_name "GND")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30015)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 189.4 94.094236) (xy 189.6 94.094236) (xy 189.794236 93.558527) (xy 189.5 93.499) (xy 189.205764 93.558527)
			)
		)
	)
	(zone
		(net 70)
		(net_name "Net-(R3-Pad2)")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30039)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 159.990898 91.400523) (xy 159.849477 91.259102) (xy 159.333329 91.500559) (xy 159.499293 91.750707)
				(xy 159.749441 91.916671)
			)
		)
	)
	(zone
		(net 7)
		(net_name "+8.7V")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30006)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 186.1 94.5) (xy 185.9 94.5) (xy 185.8 94.7) (xy 186 95.601) (xy 186.2 94.7)
			)
		)
	)
	(zone
		(net 28)
		(net_name "LRA_TRIG")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30026)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 176.4 79.094236) (xy 176.6 79.094236) (xy 176.794236 78.558527) (xy 176.5 78.499) (xy 176.205764 78.558527)
			)
		)
	)
	(zone
		(net 54)
		(net_name "ENC_OUT_B")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30010)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 192.932764 70.4) (xy 192.932764 70.6) (xy 193.468473 70.794236) (xy 193.528 70.5) (xy 193.468473 70.205764)
			)
		)
	)
	(zone
		(net 64)
		(net_name "BTN_A")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30037)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 195.150523 74.009102) (xy 195.009102 74.150523) (xy 195.250559 74.666671) (xy 195.500707 74.500707)
				(xy 195.666671 74.250559)
			)
		)
	)
	(zone
		(net 81)
		(net_name "/AAT_SERIES")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30016)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 165.499027 71.595435) (xy 165.499027 71.795435) (xy 166.034736 71.989671) (xy 166.094263 71.695435)
				(xy 166.034736 71.401199)
			)
		)
	)
	(zone
		(net 48)
		(net_name "Net-(O1-IREF)")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30058)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 188.7 94.094236) (xy 188.9 94.094236) (xy 189.044236 93.558527) (xy 188.75 93.499) (xy 188.500559 93.666671)
			)
		)
	)
	(zone
		(net 64)
		(net_name "BTN_A")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30042)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 190.599477 73.490898) (xy 190.740898 73.349477) (xy 190.499441 72.833329) (xy 190.249293 72.999293)
				(xy 190.083329 73.249441)
			)
		)
	)
	(zone
		(net 60)
		(net_name "TWIM_SCL")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30012)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 172.443236 80.85) (xy 172.443236 80.65) (xy 171.907527 80.455764) (xy 171.848 80.75) (xy 171.907527 81.044236)
			)
		)
	)
	(zone
		(net 30)
		(net_name "/DECA")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30028)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 160.85 100.405764) (xy 160.65 100.405764) (xy 160.455764 100.941473) (xy 160.75 101.001) (xy 161.044236 100.941473)
			)
		)
	)
	(zone
		(net 24)
		(net_name "/RFI+")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30023)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 156 67.094236) (xy 156.2 67.094236) (xy 156.394236 66.558527) (xy 156.1 66.499) (xy 155.805764 66.558527)
			)
		)
	)
	(zone
		(net 51)
		(net_name "+8.7V_EN")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30035)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 182.237023 96.495602) (xy 182.095602 96.637023) (xy 182.350559 97.139671) (xy 182.600707 96.973707)
				(xy 182.766671 96.723559)
			)
		)
	)
	(zone
		(net 33)
		(net_name "BAT_ERR")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30032)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 162.775001 99.722879) (xy 162.975001 99.722879) (xy 163.169237 99.18717) (xy 162.875001 99.127643)
				(xy 162.580765 99.18717)
			)
		)
	)
	(zone
		(net 66)
		(net_name "BTN_B")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30040)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 194.150523 74.259102) (xy 194.009102 74.400523) (xy 194.250559 74.916671) (xy 194.500707 74.750707)
				(xy 194.666671 74.500559)
			)
		)
	)
	(zone
		(net 1)
		(net_name "GND")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30009)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 192.9 94.094236) (xy 193.1 94.094236) (xy 193.294236 93.558527) (xy 193 93.499) (xy 192.705764 93.558527)
			)
		)
	)
	(zone
		(net 66)
		(net_name "BTN_B")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30041)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 185.609477 73.490898) (xy 185.750898 73.349477) (xy 185.509441 72.833329) (xy 185.259293 72.999293)
				(xy 185.093329 73.249441)
			)
		)
	)
	(zone
		(net 11)
		(net_name "/VDD_D")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30018)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 167.4 71.105764) (xy 167.2 71.105764) (xy 167.005764 71.641473) (xy 167.3 71.701) (xy 167.594236 71.641473)
			)
		)
	)
	(zone
		(net 61)
		(net_name "TWIM_SDA")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30001)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 192.4 94.5) (xy 192.2 94.5) (xy 192.1 94.7) (xy 192.3 95.601) (xy 192.5 94.7)
			)
		)
	)
	(zone
		(net 12)
		(net_name "Net-(O1-VCOMH)")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30019)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 186.627003 94.594236) (xy 186.827003 94.594236) (xy 187.021239 94.058527) (xy 186.727003 93.999)
				(xy 186.432767 94.058527)
			)
		)
	)
	(zone
		(net 80)
		(net_name "/AAT_PARALLEL")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30064)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 166.126394 72.123435) (xy 166.126394 72.323435) (xy 166.636571 72.397504) (xy 166.696098 72.103268)
				(xy 166.528427 71.853827)
			)
		)
	)
	(zone
		(net 1)
		(net_name "GND")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 2)
		(connect_pads
			(clearance 0.2)
		)
		(min_thickness 0.2)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 120 30) (xy 230 30) (xy 230 140) (xy 121 140)
			)
		)
	)
	(zone
		(net 39)
		(net_name "BAT_CHG")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30068)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 162.689734 98.35) (xy 162.689734 98.15) (xy 162.191473 98.328764) (xy 162.249 98.623) (xy 162.499441 98.789671)
			)
		)
	)
	(zone
		(net 24)
		(net_name "/RFI+")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30043)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 167.675099 72.149477) (xy 167.81652 72.290898) (xy 168.332668 72.049441) (xy 168.166704 71.799293)
				(xy 167.916556 71.633329)
			)
		)
	)
	(zone
		(net 15)
		(net_name "/VDD_DR")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30071)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 163.215516 66.37923) (xy 163.356938 66.237808) (xy 163.494236 65.808527) (xy 163.199293 65.749293)
				(xy 162.950559 65.916671)
			)
		)
	)
	(zone
		(net 15)
		(net_name "/VDD_DR")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30069)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 164.9 68.658784) (xy 164.7 68.658784) (xy 164.263459 68.850373) (xy 164.43013 69.100814) (xy 164.724366 69.158341)
			)
		)
	)
	(zone
		(net 6)
		(net_name "/VSYS")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30029)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 166.85 80.905764) (xy 166.65 80.905764) (xy 166.455764 81.441473) (xy 166.75 81.501) (xy 167.044236 81.441473)
			)
		)
	)
	(zone
		(net 60)
		(net_name "TWIM_SCL")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30002)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 191.5 96.7) (xy 191.7 96.7) (xy 191.8 96.5) (xy 191.6 95.599) (xy 191.4 96.5)
			)
		)
	)
	(zone
		(net 7)
		(net_name "+8.7V")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30047)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 177.56159 97.922478) (xy 177.703011 98.063899) (xy 178.219159 97.822442) (xy 178.053195 97.572294)
				(xy 177.803047 97.40633)
			)
		)
	)
	(zone
		(net 6)
		(net_name "/VSYS")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30044)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 160.599477 82.731198) (xy 160.740898 82.589777) (xy 160.499441 82.073629) (xy 160.249293 82.239593)
				(xy 160.083329 82.489741)
			)
		)
	)
	(zone
		(net 61)
		(net_name "TWIM_SDA")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30005)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 192.2 96.7) (xy 192.4 96.7) (xy 192.5 96.5) (xy 192.3 95.599) (xy 192.1 96.5)
			)
		)
	)
	(zone
		(net 9)
		(net_name "OLED_VDD")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30051)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 181.302852 90.593227) (xy 181.444273 90.734648) (xy 181.966671 90.499441) (xy 181.800707 90.249293)
				(xy 181.550559 90.083329)
			)
		)
	)
	(zone
		(net 51)
		(net_name "+8.7V_EN")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30052)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 169.349477 93.490898) (xy 169.490898 93.349477) (xy 169.249441 92.833329) (xy 168.999293 92.999293)
				(xy 168.833329 93.249441)
			)
		)
	)
	(zone
		(net 1)
		(net_name "GND")
		(layer "In1.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0.4)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 140 50) (xy 210 50) (xy 210 120) (xy 140 120)
			)
		)
	)
	(zone
		(net 2)
		(net_name "+3.0V")
		(layer "In2.Cu")
		(hatch edge 0.5)
		(priority 1)
		(connect_pads
			(clearance 0.4)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 130 40) (xy 220 40) (xy 220 130) (xy 130 130)
			)
		)
	)
	(embedded_fonts no)
)
