(kicad_pcb
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(general
		(thickness 1.6)
		(legacy_teardrops no)
	)
	(paper "A4")
	(layers
		(0 "F.Cu" signal)
		(2 "B.Cu" signal)
		(9 "F.Adhes" user "F.Adhesive")
		(11 "B.Adhes" user "B.Adhesive")
		(13 "F.Paste" user)
		(15 "B.Paste" user)
		(5 "F.SilkS" user "F.Silkscreen")
		(7 "B.SilkS" user "B.Silkscreen")
		(1 "F.Mask" user)
		(3 "B.Mask" user)
		(17 "Dwgs.User" user "User.Drawings")
		(19 "Cmts.User" user "User.Comments")
		(21 "Eco1.User" user "User.Eco1")
		(23 "Eco2.User" user "User.Eco2")
		(25 "Edge.Cuts" user)
		(27 "Margin" user)
		(31 "F.CrtYd" user "F.Courtyard")
		(29 "B.CrtYd" user "B.Courtyard")
		(35 "F.Fab" user)
		(33 "B.Fab" user)
		(39 "User.1" user)
		(41 "User.2" user)
		(43 "User.3" user)
		(45 "User.4" user)
	)
	(setup
		(stackup
			(layer "F.SilkS"
				(type "Top Silk Screen")
			)
			(layer "F.Paste"
				(type "Top Solder Paste")
			)
			(layer "F.Mask"
				(type "Top Solder Mask")
				(thickness 0.01)
			)
			(layer "F.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "dielectric 1"
				(type "core")
				(thickness 1.51)
				(material "FR4")
				(epsilon_r 4.5)
				(loss_tangent 0.02)
			)
			(layer "B.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "B.Mask"
				(type "Bottom Solder Mask")
				(thickness 0.01)
			)
			(layer "B.Paste"
				(type "Bottom Solder Paste")
			)
			(layer "B.SilkS"
				(type "Bottom Silk Screen")
			)
			(copper_finish "None")
			(dielectric_constraints no)
		)
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(tenting front back)
		(pcbplotparams
			(layerselection 0x00000000_00000000_55555555_5755f5ff)
			(plot_on_all_layers_selection 0x00000000_00000000_00000000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 4)
			(plotframeref no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(pdf_metadata yes)
			(pdf_single_document no)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plot_black_and_white yes)
			(sketchpadsonfab no)
			(plotpadnumbers no)
			(hidednponfab no)
			(sketchdnponfab yes)
			(crossoutdnponfab yes)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 0)
			(scaleselection 1)
			(outputdirectory "")
		)
	)
	(net 0 "")
	(net 1 "GND")
	(net 2 "Net-(D3-K)")
	(net 3 "Net-(U1-VREG_2V7)")
	(net 4 "Net-(U1-VREG_1V2)")
	(net 5 "Net-(D4-K)")
	(net 6 "Net-(C6-Pad1)")
	(net 7 "Net-(R1-Pad2)")
	(net 8 "Net-(U2-G)")
	(net 9 "unconnected-(U1-POWER_OK3-Pad14)")
	(net 10 "unconnected-(U1-GPIO-Pad15)")
	(net 11 "unconnected-(U1-A_B_SIDE-Pad17)")
	(net 12 "unconnected-(U1-POWER_OK2-Pad20)")
	(net 13 "unconnected-(U1-NC-Pad3)")
	(net 14 "unconnected-(U1-ATTACH-Pad11)")
	(net 15 "/VBUS_EN_SNK")
	(net 16 "/DISCH")
	(net 17 "/VDD")
	(net 18 "/VBUS_VS_DISCH")
	(net 19 "/RESET")
	(net 20 "/CC2")
	(net 21 "/CC1")
	(net 22 "/SCL")
	(net 23 "/SDA")
	(net 24 "Net-(U2-S)")
	(net 25 "Net-(U1-SCL)")
	(net 26 "Net-(U1-SDA)")
	(net 27 "/Vbus")
	(net 28 "unconnected-(U1-ALERT-Pad19)")
	(footprint "Diode_SMD:D_0603_1608Metric_Pad1.05x0.95mm_HandSolder"
		(layer "F.Cu")
		(at 338.4 118.4 180)
		(descr "Diode SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
		(tags "diode handsolder")
		(property "Reference" "D5"
			(at 0 1.4 0)
			(layer "F.SilkS")
		)
		(property "Value" "D"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Diode"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Device" "D"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TO-???* *_Diode_* *SingleDiode* D_*")
		(sheetname "/")
		(sheetfile "USB_PD_Sink_Controller_Min_VBUS.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.875 0 180)
			(size 1.05 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 17 "/VDD")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.875 0 180)
			(size 1.05 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 27 "/Vbus")
			(pinfunction "A")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Diode_SMD.3dshapes/D_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "ST_1610:ST_1610"
		(layer "F.Cu")
		(at 341.5 124.575 -90)
		(property "Reference" "D4"
			(at -1.475 2 0)
			(layer "F.SilkS")
		)
		(property "Value" "ESDA25P35-1U1M"
			(at -0.137 1.75 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "kicad-embed://esda25p35-1u1m.pdf"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*ST_1610*")
		(sheetname "/")
		(sheetfile "USB_PD_Sink_Controller_Min_VBUS.kicad_sch")
		(pad "1" smd rect
			(at -0.625 0 270)
			(size 0.55 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 5 "Net-(D4-K)")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 0.625 0 270)
			(size 0.55 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "A")
			(pintype "passive")
		)
		(embedded_fonts no)
		(embedded_files
			(file
				(name "ST_1610.step")
				(type model)
			)
		)
		(model "kicad-embed://ST_1610.step"
			(offset
				(xyz 0 -0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -0 -0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder"
		(layer "F.Cu")
		(at 325.25 120.5 180)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C1"
			(at -1.65 -1.2 90)
			(layer "F.SilkS")
		)
		(property "Value" "4.7 μF"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor - VBUS – DEVICE Capacitor CVBUS 4.7 μF Range: 1.0 μF to 10.0 μF"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "USB_PD_Sink_Controller_Min_VBUS.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.8625 0 180)
			(size 1.075 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 27 "/Vbus")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.8625 0 180)
			(size 1.075 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder"
		(layer "F.Cu")
		(at 327.7 116.2 90)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C3"
			(at 2.2 -0.4 0)
			(layer "F.SilkS")
		)
		(property "Value" "1μF"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "USB_PD_Sink_Controller_Min_VBUS.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.8625 0 90)
			(size 1.075 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 17 "/VDD")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.8625 0 90)
			(size 1.075 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "STL6P3LLH6:POWERFLAT_3P3X3P3_STM2"
		(layer "F.Cu")
		(at 342.3998 113.974999 180)
		(tags "STL6P3LLH6 ")
		(property "Reference" "U2"
			(at 0 2.525001 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "STL6P3LLH6"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stl6p3llh6.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SOT?23*")
		(sheetname "/")
		(sheetfile "USB_PD_Sink_Controller_Min_VBUS.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.6002 0.974999 180)
			(size 0.9144 0.3302)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 8 "Net-(U2-G)")
			(pinfunction "G")
			(pintype "input")
		)
		(pad "2" smd rect
			(at -1.6002 -0.974999 180)
			(size 0.9144 0.3302)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 24 "Net-(U2-S)")
			(pinfunction "S")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -1.6002 -0.325001 180)
			(size 0.9144 0.3302)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 24 "Net-(U2-S)")
			(pinfunction "S")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -1.6002 0.325001 180)
			(size 0.9144 0.3302)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 24 "Net-(U2-S)")
			(pinfunction "S")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at 0.4445 0 180)
			(size 2.1082 2.3622)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 27 "/Vbus")
			(pinfunction "D")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at 1.6002 -0.974999 180)
			(size 0.9144 0.3302)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 27 "/Vbus")
			(pinfunction "D")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at 1.6002 -0.325001 180)
			(size 0.9144 0.3302)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 27 "/Vbus")
			(pinfunction "D")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at 1.6002 0.325001 180)
			(size 0.9144 0.3302)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 27 "/Vbus")
			(pinfunction "D")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at 1.6002 0.974999 180)
			(size 0.9144 0.3302)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 27 "/Vbus")
			(pinfunction "D")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder"
		(layer "F.Cu")
		(at 347 118.25 180)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R5"
			(at -2.5 -0.05 0)
			(layer "F.SilkS")
		)
		(property "Value" "100R"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "USB_PD_Sink_Controller_Min_VBUS.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 180)
			(size 0.975 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 6 "Net-(C6-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 180)
			(size 0.975 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 8 "Net-(U2-G)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder"
		(layer "F.Cu")
		(at 343.5 116.75)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R4"
			(at -2.5 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "100kR"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "USB_PD_Sink_Controller_Min_VBUS.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0)
			(size 0.975 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 8 "Net-(U2-G)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0)
			(size 0.975 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 24 "Net-(U2-S)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder"
		(layer "F.Cu")
		(at 347 116.75)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C6"
			(at 2.5 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "100nF"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "USB_PD_Sink_Controller_Min_VBUS.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.8625 0)
			(size 1.075 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 6 "Net-(C6-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.8625 0)
			(size 1.075 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 5 "Net-(D4-K)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder"
		(layer "F.Cu")
		(at 337 115.25)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C2"
			(at 0 -1.43 0)
			(layer "F.SilkS")
		)
		(property "Value" "1μF"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "USB_PD_Sink_Controller_Min_VBUS.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.8625 0)
			(size 1.075 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "Net-(D3-K)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.8625 0)
			(size 1.075 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_DFN_QFN:QFN-24-1EP_4x4mm_P0.5mm_EP2.7x2.7mm"
		(layer "F.Cu")
		(at 330 121)
		(descr "QFN, 24 Pin (http://www.alfarzpp.lv/eng/sc/AS3330.pdf), generated with kicad-footprint-generator ipc_noLead_generator.py")
		(tags "QFN NoLead")
		(property "Reference" "U1"
			(at 3 3 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "STUSB4500QTR"
			(at 0 3.33 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stusb4500.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Stand-alone USB PD controller (with sink Auto-run mode), QFN-24"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "QFN*4x4mm*P0.5mm*")
		(sheetname "/")
		(sheetfile "USB_PD_Sink_Controller_Min_VBUS.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "" smd roundrect
			(at -0.675 -0.675)
			(size 1.09 1.09)
			(layers "F.Paste")
			(roundrect_rratio 0.229358)
		)
		(pad "" smd roundrect
			(at -0.675 0.675)
			(size 1.09 1.09)
			(layers "F.Paste")
			(roundrect_rratio 0.229358)
		)
		(pad "" smd roundrect
			(at 0.675 -0.675)
			(size 1.09 1.09)
			(layers "F.Paste")
			(roundrect_rratio 0.229358)
		)
		(pad "" smd roundrect
			(at 0.675 0.675)
			(size 1.09 1.09)
			(layers "F.Paste")
			(roundrect_rratio 0.229358)
		)
		(pad "1" smd roundrect
			(at -1.9625 -1.25)
			(size 0.825 0.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 21 "/CC1")
			(pinfunction "CC1DB")
			(pintype "bidirectional")
		)
		(pad "2" smd roundrect
			(at -1.9625 -0.75)
			(size 0.825 0.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 21 "/CC1")
			(pinfunction "CC1")
			(pintype "bidirectional")
		)
		(pad "3" smd roundrect
			(at -1.9625 -0.25)
			(size 0.825 0.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 13 "unconnected-(U1-NC-Pad3)")
			(pinfunction "NC")
			(pintype "no_connect")
		)
		(pad "4" smd roundrect
			(at -1.9625 0.25)
			(size 0.825 0.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 20 "/CC2")
			(pinfunction "CC2")
			(pintype "bidirectional")
		)
		(pad "5" smd roundrect
			(at -1.9625 0.75)
			(size 0.825 0.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 20 "/CC2")
			(pinfunction "CC2DB")
			(pintype "bidirectional")
		)
		(pad "6" smd roundrect
			(at -1.9625 1.25)
			(size 0.825 0.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 19 "/RESET")
			(pinfunction "RESET")
			(pintype "input")
		)
		(pad "7" smd roundrect
			(at -1.25 1.9625)
			(size 0.25 0.825)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 25 "Net-(U1-SCL)")
			(pinfunction "SCL")
			(pintype "input")
		)
		(pad "8" smd roundrect
			(at -0.75 1.9625)
			(size 0.25 0.825)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 26 "Net-(U1-SDA)")
			(pinfunction "SDA")
			(pintype "bidirectional")
		)
		(pad "9" smd roundrect
			(at -0.25 1.9625)
			(size 0.25 0.825)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 16 "/DISCH")
			(pinfunction "DISCH")
			(pintype "bidirectional")
		)
		(pad "10" smd roundrect
			(at 0.25 1.9625)
			(size 0.25 0.825)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "11" smd roundrect
			(at 0.75 1.9625)
			(size 0.25 0.825)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 14 "unconnected-(U1-ATTACH-Pad11)")
			(pinfunction "ATTACH")
			(pintype "open_collector+no_connect")
		)
		(pad "12" smd roundrect
			(at 1.25 1.9625)
			(size 0.25 0.825)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "ADDR0")
			(pintype "input")
		)
		(pad "13" smd roundrect
			(at 1.9625 1.25)
			(size 0.825 0.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "ADDR1")
			(pintype "input")
		)
		(pad "14" smd roundrect
			(at 1.9625 0.75)
			(size 0.825 0.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 9 "unconnected-(U1-POWER_OK3-Pad14)")
			(pinfunction "POWER_OK3")
			(pintype "open_collector+no_connect")
		)
		(pad "15" smd roundrect
			(at 1.9625 0.25)
			(size 0.825 0.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 10 "unconnected-(U1-GPIO-Pad15)")
			(pinfunction "GPIO")
			(pintype "open_collector+no_connect")
		)
		(pad "16" smd roundrect
			(at 1.9625 -0.25)
			(size 0.825 0.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 15 "/VBUS_EN_SNK")
			(pinfunction "VBUS_EN_SNK")
			(pintype "open_collector")
		)
		(pad "17" smd roundrect
			(at 1.9625 -0.75)
			(size 0.825 0.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 11 "unconnected-(U1-A_B_SIDE-Pad17)")
			(pinfunction "A_B_SIDE")
			(pintype "open_collector+no_connect")
		)
		(pad "18" smd roundrect
			(at 1.9625 -1.25)
			(size 0.825 0.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 18 "/VBUS_VS_DISCH")
			(pinfunction "VBUS_VS_DISCH")
			(pintype "input")
		)
		(pad "19" smd roundrect
			(at 1.25 -1.9625)
			(size 0.25 0.825)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 28 "unconnected-(U1-ALERT-Pad19)")
			(pinfunction "ALERT")
			(pintype "open_collector+no_connect")
		)
		(pad "20" smd roundrect
			(at 0.75 -1.9625)
			(size 0.25 0.825)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 12 "unconnected-(U1-POWER_OK2-Pad20)")
			(pinfunction "POWER_OK2")
			(pintype "open_collector+no_connect")
		)
		(pad "21" smd roundrect
			(at 0.25 -1.9625)
			(size 0.25 0.825)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 4 "Net-(U1-VREG_1V2)")
			(pinfunction "VREG_1V2")
			(pintype "power_out")
		)
		(pad "22" smd roundrect
			(at -0.25 -1.9625)
			(size 0.25 0.825)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "VSYS")
			(pintype "power_in")
		)
		(pad "23" smd roundrect
			(at -0.75 -1.9625)
			(size 0.25 0.825)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 3 "Net-(U1-VREG_2V7)")
			(pinfunction "VREG_2V7")
			(pintype "power_out")
		)
		(pad "24" smd roundrect
			(at -1.25 -1.9625)
			(size 0.25 0.825)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 17 "/VDD")
			(pinfunction "VDD")
			(pintype "power_in")
		)
		(pad "25" smd rect
			(at 0 0)
			(size 2.7 2.7)
			(property pad_prop_heatsink)
			(layers "F.Cu" "F.Mask")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "passive")
			(zone_connect 2)
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Package_DFN_QFN.3dshapes/QFN-24-1EP_4x4mm_P0.5mm_EP2.7x2.7mm.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder"
		(layer "F.Cu")
		(at 328.9125 124.5 180)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R7"
			(at -2.8375 0.25 0)
			(layer "F.SilkS")
		)
		(property "Value" "10kR"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "USB_PD_Sink_Controller_Min_VBUS.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 180)
			(size 0.975 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 180)
			(size 0.975 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 19 "/RESET")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "STL6P3LLH6:POWERFLAT_3P3X3P3_STM2"
		(layer "F.Cu")
		(at 347.5 114)
		(tags "STL6P3LLH6 ")
		(property "Reference" "U3"
			(at -0.1498 -2.525001 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "STL6P3LLH6"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stl6p3llh6.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SOT?23*")
		(sheetname "/")
		(sheetfile "USB_PD_Sink_Controller_Min_VBUS.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.6002 0.974999)
			(size 0.9144 0.3302)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 8 "Net-(U2-G)")
			(pinfunction "G")
			(pintype "input")
		)
		(pad "2" smd rect
			(at -1.6002 -0.974999)
			(size 0.9144 0.3302)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 24 "Net-(U2-S)")
			(pinfunction "S")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -1.6002 -0.325001)
			(size 0.9144 0.3302)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 24 "Net-(U2-S)")
			(pinfunction "S")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -1.6002 0.325001)
			(size 0.9144 0.3302)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 24 "Net-(U2-S)")
			(pinfunction "S")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at 0.4445 0)
			(size 2.1082 2.3622)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 5 "Net-(D4-K)")
			(pinfunction "D")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at 1.6002 -0.974999)
			(size 0.9144 0.3302)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 5 "Net-(D4-K)")
			(pinfunction "D")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at 1.6002 -0.325001)
			(size 0.9144 0.3302)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 5 "Net-(D4-K)")
			(pinfunction "D")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at 1.6002 0.325001)
			(size 0.9144 0.3302)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 5 "Net-(D4-K)")
			(pinfunction "D")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at 1.6002 0.974999)
			(size 0.9144 0.3302)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 5 "Net-(D4-K)")
			(pinfunction "D")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder"
		(layer "F.Cu")
		(at 338.7 125.1 180)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R8"
			(at 2.6 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "4.7kR"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "USB_PD_Sink_Controller_Min_VBUS.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 180)
			(size 0.975 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 22 "/SCL")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 180)
			(size 0.975 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 25 "Net-(U1-SCL)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder"
		(layer "F.Cu")
		(at 343.5 118.25 180)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R3"
			(at 2.5 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "22kR"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "USB_PD_Sink_Controller_Min_VBUS.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 180)
			(size 0.975 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 8 "Net-(U2-G)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 180)
			(size 0.975 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 15 "/VBUS_EN_SNK")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder"
		(layer "F.Cu")
		(at 334.5 119.5 180)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R2"
			(at 0 -1.49 0)
			(layer "F.SilkS")
		)
		(property "Value" "1kR"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "USB_PD_Sink_Controller_Min_VBUS.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 180)
			(size 0.975 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 7 "Net-(R1-Pad2)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 180)
			(size 0.975 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 18 "/VBUS_VS_DISCH")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "ST_1610:ST_1610"
		(layer "F.Cu")
		(at 325 122.25 180)
		(property "Reference" "D1"
			(at 0.8 -1.75 0)
			(layer "F.SilkS")
		)
		(property "Value" "ESDA25P35-1U1M"
			(at -0.137 1.75 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "kicad-embed://esda25p35-1u1m.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*ST_1610*")
		(sheetname "/")
		(sheetfile "USB_PD_Sink_Controller_Min_VBUS.kicad_sch")
		(pad "1" smd rect
			(at -0.625 0 180)
			(size 0.55 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 27 "/Vbus")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 0.625 0 180)
			(size 0.55 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "A")
			(pintype "passive")
		)
		(embedded_fonts no)
		(embedded_files
			(file
				(name "ST_1610.step")
				(type model)
			)
		)
		(model "kicad-embed://ST_1610.step"
			(offset
				(xyz 0 -0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -0 -0 0)
			)
		)
	)
	(footprint "Connector_USB:USB_C_Receptacle_GCT_USB4105-xx-A_16P_TopMnt_Horizontal"
		(layer "F.Cu")
		(at 318.25 120 -90)
		(descr "USB 2.0 Type C Receptacle, GCT, 16P, top mounted, horizontal, 5A: https://gct.co/files/drawings/usb4105.pdf")
		(tags "USB C Type-C Receptacle SMD USB 2.0 16P 16C USB4105-15-A USB4105-15-A-060 USB4105-15-A-120 USB4105-GF-A USB4105-GF-A-060 USB4105-GF-A-120")
		(property "Reference" "J1"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "USB_C_Receptacle_PowerOnly_6P"
			(at 0 5 270)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://www.usb.org/sites/default/files/documents/usb_type-c.zip"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "USB Power-Only 6P Type-C Receptacle connector"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "USB*C*Receptacle*")
		(sheetname "/")
		(sheetfile "USB_PD_Sink_Controller_Min_VBUS.kicad_sch")
		(attr smd)
		(fp_text user "PCB Edge"
			(at 0 3.1 270)
			(unlocked yes)
			(layer "Dwgs.User")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole circle
			(at -2.89 -2.605 270)
			(size 0.65 0.65)
			(drill 0.65)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 2.89 -2.605 270)
			(size 0.65 0.65)
			(drill 0.65)
			(layers "*.Cu" "*.Mask")
		)
		(pad "A5" smd roundrect
			(at -1.25 -3.68 270)
			(size 0.3 1.15)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 21 "/CC1")
			(pinfunction "CC1")
			(pintype "bidirectional")
		)
		(pad "A6" smd roundrect
			(at -0.25 -3.68 270)
			(size 0.3 1.15)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "A7" smd roundrect
			(at 0.25 -3.68 270)
			(size 0.3 1.15)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "A8" smd roundrect
			(at 1.25 -3.68 270)
			(size 0.3 1.15)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "A9" smd roundrect
			(at 2.4 -3.68 270)
			(size 0.6 1.15)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 27 "/Vbus")
			(pinfunction "VBUS")
			(pintype "passive")
		)
		(pad "A12" smd roundrect
			(at 3.2 -3.68 270)
			(size 0.6 1.15)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "B5" smd roundrect
			(at 1.75 -3.68 270)
			(size 0.3 1.15)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 20 "/CC2")
			(pinfunction "CC2")
			(pintype "bidirectional")
		)
		(pad "B6" smd roundrect
			(at 0.75 -3.68 270)
			(size 0.3 1.15)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "B7" smd roundrect
			(at -0.75 -3.68 270)
			(size 0.3 1.15)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "B8" smd roundrect
			(at -1.75 -3.68 270)
			(size 0.3 1.15)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "B9" smd roundrect
			(at -2.4 -3.68 270)
			(size 0.6 1.15)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 27 "/Vbus")
			(pinfunction "VBUS")
			(pintype "passive")
		)
		(pad "B12" smd roundrect
			(at -3.2 -3.68 270)
			(size 0.6 1.15)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "S1" thru_hole oval
			(at -4.32 -3.105 270)
			(size 1 2.1)
			(drill oval 0.6 1.7)
			(property pad_prop_heatsink)
			(layers "*.Cu" "*.Mask" "F.Paste")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "SHIELD")
			(pintype "passive")
		)
		(pad "S1" thru_hole oval
			(at -4.32 1.075 270)
			(size 1 1.8)
			(drill oval 0.6 1.4)
			(property pad_prop_heatsink)
			(layers "*.Cu" "*.Mask" "F.Paste")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "SHIELD")
			(pintype "passive")
		)
		(pad "S1" thru_hole oval
			(at 4.32 -3.105 270)
			(size 1 2.1)
			(drill oval 0.6 1.7)
			(property pad_prop_heatsink)
			(layers "*.Cu" "*.Mask" "F.Paste")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "SHIELD")
			(pintype "passive")
		)
		(pad "S1" thru_hole oval
			(at 4.32 1.075 270)
			(size 1 1.8)
			(drill oval 0.6 1.4)
			(property pad_prop_heatsink)
			(layers "*.Cu" "*.Mask" "F.Paste")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "SHIELD")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_USB.3dshapes/USB_C_Receptacle_GCT_USB4105-xx-A_16P_TopMnt_Horizontal.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder"
		(layer "F.Cu")
		(at 340.5 121.6)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R10"
			(at -3 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "4.7kR"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "USB_PD_Sink_Controller_Min_VBUS.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0)
			(size 0.975 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 26 "Net-(U1-SDA)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0)
			(size 0.975 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 23 "/SDA")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_JST:JST_XH_S5B-XH-A_1x05_P2.50mm_Horizontal"
		(layer "F.Cu")
		(at 345.5 122)
		(descr "JST XH series connector, S5B-XH-A (http://www.jst-mfg.com/product/pdf/eng/eXH.pdf), generated with kicad-footprint-generator")
		(tags "connector JST XH horizontal")
		(property "Reference" "J3"
			(at 1.3 -2 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "JST_01x05_Socket"
			(at 5 10.4 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x05, script generated"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "/")
		(sheetfile "USB_PD_Sink_Controller_Min_VBUS.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 1 5.5 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole roundrect
			(at 0 0)
			(size 1.7 1.95)
			(drill 0.95)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.147059)
			(net 1 "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 2.5 0)
			(size 1.7 1.95)
			(drill 0.95)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 17 "/VDD")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 5 0)
			(size 1.7 1.95)
			(drill 0.95)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 23 "/SDA")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole oval
			(at 7.5 0)
			(size 1.7 1.95)
			(drill 0.95)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 22 "/SCL")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(pad "5" thru_hole oval
			(at 10 0)
			(size 1.7 1.95)
			(drill 0.95)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 19 "/RESET")
			(pinfunction "Pin_5")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_JST.3dshapes/JST_XH_S5B-XH-A_1x05_P2.50mm_Horizontal.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder"
		(layer "F.Cu")
		(at 334 118)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R1"
			(at 0 -1.3 0)
			(layer "F.SilkS")
		)
		(property "Value" "470R"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "USB_PD_Sink_Controller_Min_VBUS.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0)
			(size 0.975 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 27 "/Vbus")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0)
			(size 0.975 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 7 "Net-(R1-Pad2)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "ST_SOT323-3L:ST_SOT323-3L"
		(layer "F.Cu")
		(at 325 118.25)
		(property "Reference" "D2"
			(at 0 -2.25 0)
			(layer "F.SilkS")
		)
		(property "Value" "ESDA25W"
			(at -0.289 2.324 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*ST_SOT323-3L*")
		(sheetname "/")
		(sheetfile "USB_PD_Sink_Controller_Min_VBUS.kicad_sch")
		(pad "1" smd rect
			(at -0.975 -0.65 90)
			(size 0.5 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 21 "/CC1")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.975 0.65 90)
			(size 0.5 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 20 "/CC2")
			(pinfunction "2")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at 0.975 0 90)
			(size 0.5 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "3")
			(pintype "passive")
		)
		(embedded_fonts no)
		(embedded_files
			(file
				(name "ST_SOT323-3L.step")
				(type model)
			)
		)
		(model "kicad-embed://ST_SOT323-3L.step"
			(offset
				(xyz 0 -0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -0 -0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder"
		(layer "F.Cu")
		(at 340.5 120)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R6"
			(at -2.6 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "1kR"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "USB_PD_Sink_Controller_Min_VBUS.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0)
			(size 0.975 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 16 "/DISCH")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0)
			(size 0.975 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 5 "Net-(D4-K)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_JST:JST_XH_S2B-XH-A_1x02_P2.50mm_Horizontal"
		(layer "F.Cu")
		(at 355.35 116.345 180)
		(descr "JST XH series connector, S2B-XH-A (http://www.jst-mfg.com/product/pdf/eng/eXH.pdf), generated with kicad-footprint-generator")
		(tags "connector JST XH horizontal")
		(property "Reference" "J2"
			(at 1.45 -1.855 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "JST_01x02_Socket"
			(at 1.25 10.4 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x02, script generated"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "/")
		(sheetfile "USB_PD_Sink_Controller_Min_VBUS.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 1.25 3.45 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole roundrect
			(at 0 0 180)
			(size 1.7 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.147059)
			(net 1 "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 2.5 0 180)
			(size 1.7 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "Net-(D4-K)")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_JST.3dshapes/JST_XH_S2B-XH-A_1x02_P2.50mm_Horizontal.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Diode_SMD:D_0603_1608Metric_Pad1.05x0.95mm_HandSolder"
		(layer "F.Cu")
		(at 333.625 115.25)
		(descr "Diode SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
		(tags "diode handsolder")
		(property "Reference" "D3"
			(at 0 -1.43 0)
			(layer "F.SilkS")
		)
		(property "Value" "D"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Diode"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Device" "D"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TO-???* *_Diode_* *SingleDiode* D_*")
		(sheetname "/")
		(sheetfile "USB_PD_Sink_Controller_Min_VBUS.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.875 0)
			(size 1.05 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "Net-(D3-K)")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.875 0)
			(size 1.05 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 27 "/Vbus")
			(pinfunction "A")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Diode_SMD.3dshapes/D_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder"
		(layer "F.Cu")
		(at 330.7 116.2375 90)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C5"
			(at 2.2375 0.2 0)
			(layer "F.SilkS")
		)
		(property "Value" "1μF"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "USB_PD_Sink_Controller_Min_VBUS.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.8625 0 90)
			(size 1.075 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 4 "Net-(U1-VREG_1V2)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.8625 0 90)
			(size 1.075 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder"
		(layer "F.Cu")
		(at 329.2 116.2375 90)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C4"
			(at 2.2375 -0.1 0)
			(layer "F.SilkS")
		)
		(property "Value" "1μF"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "USB_PD_Sink_Controller_Min_VBUS.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.8625 0 90)
			(size 1.075 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 3 "Net-(U1-VREG_2V7)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.8625 0 90)
			(size 1.075 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(gr_rect
		(start 314.75 112)
		(end 358.25 125.975)
		(fill no)
		(layer "Edge.Cuts")
	)
	(gr_text "RST"
		(at 356.25 123.25 90)
		(layer "B.SilkS")
	)
	(gr_text "STUSB-1-0"
		(at 315 114.5 0)
		(layer "B.SilkS")
	)
	(gr_text "VBUS"
		(at 353.25 117.75 90)
		(layer "B.SilkS")
	)
	(gr_text "VDD"
		(at 348.5 123.5 90)
		(layer "B.SilkS")
	)
	(gr_text "GND"
		(at 346 123.25 90)
		(layer "B.SilkS")
	)
	(gr_text "GND"
		(at 355.75 117.75 90)
		(layer "B.SilkS")
	)
	(gr_text "SDA"
		(at 351 123.25 90)
		(layer "B.SilkS")
	)
	(gr_text "SCL"
		(at 353.75 123.25 90)
		(layer "B.SilkS")
	)
	(zone
		(net 1)
		(net_name "GND")
		(layer "B.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 310 110) (xy 360 110) (xy 360 145) (xy 310 145)
			)
		)
	)
	(embedded_fonts no)
	(embedded_files
		(file
			(name "ST_1610.step")
			(type model)
		)
		(file
			(name "ST_SOT323-3L.step")
			(type model)
		)
	)
)
