(kicad_pcb (version 20221018) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )
  (setup
    (pad_to_mask_clearance 0)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (plot_on_all_layers_selection 0x0000000_00000000)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (dashed_line_dash_ratio 12.000000)
      (dashed_line_gap_ratio 3.000000)
      (svgprecision 4)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "")
    )
  )
  (net 0 "")
  (net 1 "Net-(J1-Pin_1)")
  (net 2 "Net-(J1-Pin_2)")
  (net 3 "Net-(J1-Pin_3)")
  (net 4 "Net-(J1-Pin_4)")
  (net 5 "Net-(Q1-B)")
  (net 6 "Net-(Q1-C)")
  (net 7 "Net-(Q2-B)")
  (net 8 "Net-(Q3-B)")
  (net 9 "Net-(U1-GPIO15)")
  (net 10 "Net-(U1-GPIO17)")
  (net 11 "Net-(U1-GPIO16)")
  (net 12 "unconnected-(U1-GPIO0-Pad1)")
  (net 13 "unconnected-(U1-GPIO1-Pad2)")
  (net 14 "unconnected-(U1-GND-Pad3)")
  (net 15 "unconnected-(U1-GPIO2-Pad4)")
  (net 16 "unconnected-(U1-GPIO3-Pad5)")
  (net 17 "unconnected-(U1-GPIO4-Pad6)")
  (net 18 "unconnected-(U1-GPIO5-Pad7)")
  (net 19 "unconnected-(U1-GND-Pad8)")
  (net 20 "unconnected-(U1-GPIO6-Pad9)")
  (net 21 "unconnected-(U1-GPIO7-Pad10)")
  (net 22 "unconnected-(U1-GPIO8-Pad11)")
  (net 23 "unconnected-(U1-GPIO9-Pad12)")
  (net 24 "unconnected-(U1-GND-Pad13)")
  (net 25 "unconnected-(U1-GPIO10-Pad14)")
  (net 26 "unconnected-(U1-GPIO11-Pad15)")
  (net 27 "unconnected-(U1-GPIO12-Pad16)")
  (net 28 "unconnected-(U1-GPIO13-Pad17)")
  (net 29 "unconnected-(U1-GND-Pad18)")
  (net 30 "unconnected-(U1-GPIO14-Pad19)")
  (net 31 "unconnected-(U1-GND-Pad23)")
  (net 32 "unconnected-(U1-GPIO18-Pad24)")
  (net 33 "unconnected-(U1-GPIO19-Pad25)")
  (net 34 "unconnected-(U1-GPIO20-Pad26)")
  (net 35 "unconnected-(U1-GPIO21-Pad27)")
  (net 36 "unconnected-(U1-GND-Pad28)")
  (net 37 "unconnected-(U1-GPIO22-Pad29)")
  (net 38 "unconnected-(U1-RUN-Pad30)")
  (net 39 "unconnected-(U1-GPIO26_ADC0-Pad31)")
  (net 40 "unconnected-(U1-GPIO27_ADC1-Pad32)")
  (net 41 "unconnected-(U1-AGND-Pad33)")
  (net 42 "unconnected-(U1-GPIO28_ADC2-Pad34)")
  (net 43 "unconnected-(U1-ADC_VREF-Pad35)")
  (net 44 "unconnected-(U1-3V3-Pad36)")
  (net 45 "unconnected-(U1-3V3_EN-Pad37)")
  (net 46 "unconnected-(U1-VSYS-Pad39)")
  (net 47 "unconnected-(U1-SWCLK-Pad41)")
  (net 48 "unconnected-(U1-GND-Pad42)")
  (net 49 "unconnected-(U1-SWDIO-Pad43)")
  (footprint "Package_TO_SOT_THT:TO-92_Inline" (layer "F.Cu")
    (at 127 111.76 180)
    (descr "TO-92 leads in-line, narrow, oval pads, drill 0.75mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (property "Sheetfile" "LED Strip Controller.kicad_sch")
    (property "Sheetname" "")
    (property "Sim.Device" "NPN")
    (property "Sim.Pins" "1=C 2=B 3=E")
    (property "Sim.Type" "GUMMELPOON")
    (property "ki_description" "Bipolar transistor symbol for simulation only, substrate tied to the emitter")
    (property "ki_keywords" "simulation")
    (attr through_hole)
    (fp_text reference "Q1" (at 1.27 -3.56) (layer "F.SilkS"))
    (fp_text value "2N3904" (at 1.27 2.79) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.27 0) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 180) (size 1.05 1.5) (drill 0.75) (layers "*.Cu" "*.Mask")
      (net 6 "Net-(Q1-C)") (pinfunction "C") (pintype "open_collector"))
    (pad "2" thru_hole oval (at 1.27 0 180) (size 1.05 1.5) (drill 0.75) (layers "*.Cu" "*.Mask")
      (net 5 "Net-(Q1-B)") (pinfunction "B") (pintype "input"))
    (pad "3" thru_hole oval (at 2.54 0 180) (size 1.05 1.5) (drill 0.75) (layers "*.Cu" "*.Mask")
      (net 4 "Net-(J1-Pin_4)") (pinfunction "E") (pintype "open_emitter"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_THT.3dshapes/TO-92_Inline.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (layer "F.Cu")
    (at 139.7 97.79 -90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "LED Strip Controller.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R3" (at 3.81 -2.37 90) (layer "F.SilkS"))
    (fp_text value "1K" (at 3.81 2.37 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 0 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 11 "Net-(U1-GPIO16)") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 8 "Net-(Q3-B)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (layer "F.Cu")
    (at 124.46 97.79 -90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "LED Strip Controller.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R1" (at 3.81 -2.37 90) (layer "F.SilkS"))
    (fp_text value "1K" (at 3.81 2.37 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 0 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 9 "Net-(U1-GPIO15)") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 5 "Net-(Q1-B)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal" (layer "F.Cu")
    (at 132.08 97.79 -90)
    (descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
    (property "Sheetfile" "LED Strip Controller.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr through_hole)
    (fp_text reference "R2" (at 3.81 -2.37 90) (layer "F.SilkS"))
    (fp_text value "1K" (at 3.81 2.37 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 0 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 10 "Net-(U1-GPIO17)") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 7 "Net-(Q2-B)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_THT:TO-92_Inline" (layer "F.Cu")
    (at 134.62 111.76 180)
    (descr "TO-92 leads in-line, narrow, oval pads, drill 0.75mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (property "Sheetfile" "LED Strip Controller.kicad_sch")
    (property "Sheetname" "")
    (property "Sim.Device" "NPN")
    (property "Sim.Pins" "1=C 2=B 3=E")
    (property "Sim.Type" "GUMMELPOON")
    (property "ki_description" "Bipolar transistor symbol for simulation only, substrate tied to the emitter")
    (property "ki_keywords" "simulation")
    (attr through_hole)
    (fp_text reference "Q2" (at 1.27 -3.56) (layer "F.SilkS"))
    (fp_text value "2N3904" (at 1.27 2.79) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.27 0) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 180) (size 1.05 1.5) (drill 0.75) (layers "*.Cu" "*.Mask")
      (net 6 "Net-(Q1-C)") (pinfunction "C") (pintype "open_collector"))
    (pad "2" thru_hole oval (at 1.27 0 180) (size 1.05 1.5) (drill 0.75) (layers "*.Cu" "*.Mask")
      (net 7 "Net-(Q2-B)") (pinfunction "B") (pintype "input"))
    (pad "3" thru_hole oval (at 2.54 0 180) (size 1.05 1.5) (drill 0.75) (layers "*.Cu" "*.Mask")
      (net 3 "Net-(J1-Pin_3)") (pinfunction "E") (pintype "open_emitter"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_THT.3dshapes/TO-92_Inline.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_PinSocket_2.54mm:PinSocket_1x04_P2.54mm_Vertical" (layer "F.Cu")
    (at 137.16 121.92 -90)
    (descr "Through hole straight socket strip, 1x04, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
    (tags "Through hole socket strip THT 1x04 2.54mm single row")
    (property "Sheetfile" "LED Strip Controller.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x04, script generated")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J1" (at 0 -2.77 90) (layer "F.SilkS"))
    (fp_text value "Conn_01x04_Socket" (at -1.27 23.09 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 3.81) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 1 "Net-(J1-Pin_1)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 2.54 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 2 "Net-(J1-Pin_2)") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 5.08 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 3 "Net-(J1-Pin_3)") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 0 7.62 270) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 4 "Net-(J1-Pin_4)") (pinfunction "Pin_4") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x04_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_THT:TO-92_Inline" (layer "F.Cu")
    (at 142.24 111.76 180)
    (descr "TO-92 leads in-line, narrow, oval pads, drill 0.75mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (property "Sheetfile" "LED Strip Controller.kicad_sch")
    (property "Sheetname" "")
    (property "Sim.Device" "NPN")
    (property "Sim.Pins" "1=C 2=B 3=E")
    (property "Sim.Type" "GUMMELPOON")
    (property "ki_description" "Bipolar transistor symbol for simulation only, substrate tied to the emitter")
    (property "ki_keywords" "simulation")
    (attr through_hole)
    (fp_text reference "Q3" (at 1.27 -3.56) (layer "F.SilkS"))
    (fp_text value "2N3904" (at 1.27 2.79) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.27 0) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 180) (size 1.05 1.5) (drill 0.75) (layers "*.Cu" "*.Mask")
      (net 6 "Net-(Q1-C)") (pinfunction "C") (pintype "open_collector"))
    (pad "2" thru_hole oval (at 1.27 0 180) (size 1.05 1.5) (drill 0.75) (layers "*.Cu" "*.Mask")
      (net 8 "Net-(Q3-B)") (pinfunction "B") (pintype "input"))
    (pad "3" thru_hole oval (at 2.54 0 180) (size 1.05 1.5) (drill 0.75) (layers "*.Cu" "*.Mask")
      (net 2 "Net-(J1-Pin_2)") (pinfunction "E") (pintype "open_emitter"))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_THT.3dshapes/TO-92_Inline.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Raspberry Pi Pico:RPi_Pico_SMD_TH" (layer "F.Cu")
    (at 133.35 67.31)
    (descr "Through hole straight pin header, 2x20, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x20 2.54mm double row")
    (property "Sheetfile" "LED Strip Controller.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "U1" (at 0 0) (layer "F.SilkS"))
    (fp_text value "Pico" (at 0 2.159) (layer "F.Fab"))
    (fp_text user "GP17" (at 13.054 21.59 45) (layer "F.SilkS"))
    (fp_text user "VSYS" (at 13.2 -21.59 45) (layer "F.SilkS"))
    (fp_text user "3V3_EN" (at 13.7 -17.2 45) (layer "F.SilkS"))
    (fp_text user "GP28" (at 13.054 -9.144 45) (layer "F.SilkS"))
    (fp_text user "VBUS" (at 13.3 -24.2 45) (layer "F.SilkS"))
    (fp_text user "GP0" (at -12.8 -24.13 45) (layer "F.SilkS"))
    (fp_text user "GP9" (at -12.8 3.81 45) (layer "F.SilkS"))
    (fp_text user "GND" (at -12.8 19.05 45) (layer "F.SilkS"))
    (fp_text user "GP21" (at 13.054 8.9 45) (layer "F.SilkS"))
    (fp_text user "GP4" (at -12.8 -11.43 45) (layer "F.SilkS"))
    (fp_text user "GND" (at 12.8 -19.05 45) (layer "F.SilkS"))
    (fp_text user "GND" (at -12.8 6.35 45) (layer "F.SilkS"))
    (fp_text user "GP7" (at -12.7 -1.3 45) (layer "F.SilkS"))
    (fp_text user "GP2" (at -12.9 -16.51 45) (layer "F.SilkS"))
    (fp_text user "GND" (at 12.8 6.35 45) (layer "F.SilkS"))
    (fp_text user "GP22" (at 13.054 3.81 45) (layer "F.SilkS"))
    (fp_text user "RUN" (at 13 1.27 45) (layer "F.SilkS"))
    (fp_text user "GP12" (at -13.2 13.97 45) (layer "F.SilkS"))
    (fp_text user "GP1" (at -12.9 -21.6 45) (layer "F.SilkS"))
    (fp_text user "GP15" (at -13.054 24.13 45) (layer "F.SilkS"))
    (fp_text user "GP14" (at -13.1 21.59 45) (layer "F.SilkS"))
    (fp_text user "GP18" (at 13.054 16.51 45) (layer "F.SilkS"))
    (fp_text user "GP26" (at 13.054 -1.27 45) (layer "F.SilkS"))
    (fp_text user "GP11" (at -13.2 11.43 45) (layer "F.SilkS"))
    (fp_text user "GP6" (at -12.8 -3.81 45) (layer "F.SilkS"))
    (fp_text user "GP13" (at -13.054 16.51 45) (layer "F.SilkS"))
    (fp_text user "GP10" (at -13.054 8.89 45) (layer "F.SilkS"))
    (fp_text user "SWDIO" (at 5.6 26.2) (layer "F.SilkS"))
    (fp_text user "AGND" (at 13.054 -6.35 45) (layer "F.SilkS"))
    (fp_text user "GP5" (at -12.8 -8.89 45) (layer "F.SilkS"))
    (fp_text user "GP20" (at 13.054 11.43 45) (layer "F.SilkS"))
    (fp_text user "GP19" (at 13.054 13.97 45) (layer "F.SilkS"))
    (fp_text user "GND" (at 12.8 19.05 45) (layer "F.SilkS"))
    (fp_text user "ADC_VREF" (at 14 -12.5 45) (layer "F.SilkS"))
    (fp_text user "GND" (at -12.8 -6.35 45) (layer "F.SilkS"))
    (fp_text user "GP27" (at 13.054 -3.8 45) (layer "F.SilkS"))
    (fp_text user "GP8" (at -12.8 1.27 45) (layer "F.SilkS"))
    (fp_text user "GND" (at -12.8 -19.05 45) (layer "F.SilkS"))
    (fp_text user "GP3" (at -12.8 -13.97 45) (layer "F.SilkS"))
    (fp_text user "3V3" (at 12.9 -13.9 45) (layer "F.SilkS"))
    (fp_text user "GP16" (at 13.054 24.13 45) (layer "F.SilkS"))
    (fp_text user "SWCLK" (at -5.7 26.2) (layer "F.SilkS"))
    (fp_text user "Copper Keepouts shown on Dwgs layer" (at 0.1 -30.2) (layer "Cmts.User"))
    (fp_text user "${REFERENCE}" (at 0 0 180) (layer "F.Fab"))
    (pad "" np_thru_hole oval (at -2.725 -24) (size 1.8 1.8) (drill 1.8) (layers "*.Cu" "*.Mask"))
    (pad "" np_thru_hole oval (at -2.425 -20.97) (size 1.5 1.5) (drill 1.5) (layers "*.Cu" "*.Mask"))
    (pad "" np_thru_hole oval (at 2.425 -20.97) (size 1.5 1.5) (drill 1.5) (layers "*.Cu" "*.Mask"))
    (pad "" np_thru_hole oval (at 2.725 -24) (size 1.8 1.8) (drill 1.8) (layers "*.Cu" "*.Mask"))
    (pad "1" thru_hole oval (at -8.89 -24.13) (size 1.7 1.7) (drill 1.02) (layers "*.Cu" "*.Mask")
      (net 12 "unconnected-(U1-GPIO0-Pad1)") (pinfunction "GPIO0") (pintype "bidirectional"))
    (pad "1" smd rect (at -8.89 -24.13) (size 3.5 1.7) (drill (offset -0.9 0)) (layers "F.Cu" "F.Mask")
      (net 12 "unconnected-(U1-GPIO0-Pad1)") (pinfunction "GPIO0") (pintype "bidirectional"))
    (pad "2" thru_hole oval (at -8.89 -21.59) (size 1.7 1.7) (drill 1.02) (layers "*.Cu" "*.Mask")
      (net 13 "unconnected-(U1-GPIO1-Pad2)") (pinfunction "GPIO1") (pintype "bidirectional"))
    (pad "2" smd rect (at -8.89 -21.59) (size 3.5 1.7) (drill (offset -0.9 0)) (layers "F.Cu" "F.Mask")
      (net 13 "unconnected-(U1-GPIO1-Pad2)") (pinfunction "GPIO1") (pintype "bidirectional"))
    (pad "3" thru_hole rect (at -8.89 -19.05) (size 1.7 1.7) (drill 1.02) (layers "*.Cu" "*.Mask")
      (net 14 "unconnected-(U1-GND-Pad3)") (pinfunction "GND") (pintype "power_in"))
    (pad "3" smd rect (at -8.89 -19.05) (size 3.5 1.7) (drill (offset -0.9 0)) (layers "F.Cu" "F.Mask")
      (net 14 "unconnected-(U1-GND-Pad3)") (pinfunction "GND") (pintype "power_in"))
    (pad "4" thru_hole oval (at -8.89 -16.51) (size 1.7 1.7) (drill 1.02) (layers "*.Cu" "*.Mask")
      (net 15 "unconnected-(U1-GPIO2-Pad4)") (pinfunction "GPIO2") (pintype "bidirectional"))
    (pad "4" smd rect (at -8.89 -16.51) (size 3.5 1.7) (drill (offset -0.9 0)) (layers "F.Cu" "F.Mask")
      (net 15 "unconnected-(U1-GPIO2-Pad4)") (pinfunction "GPIO2") (pintype "bidirectional"))
    (pad "5" thru_hole oval (at -8.89 -13.97) (size 1.7 1.7) (drill 1.02) (layers "*.Cu" "*.Mask")
      (net 16 "unconnected-(U1-GPIO3-Pad5)") (pinfunction "GPIO3") (pintype "bidirectional"))
    (pad "5" smd rect (at -8.89 -13.97) (size 3.5 1.7) (drill (offset -0.9 0)) (layers "F.Cu" "F.Mask")
      (net 16 "unconnected-(U1-GPIO3-Pad5)") (pinfunction "GPIO3") (pintype "bidirectional"))
    (pad "6" thru_hole oval (at -8.89 -11.43) (size 1.7 1.7) (drill 1.02) (layers "*.Cu" "*.Mask")
      (net 17 "unconnected-(U1-GPIO4-Pad6)") (pinfunction "GPIO4") (pintype "bidirectional"))
    (pad "6" smd rect (at -8.89 -11.43) (size 3.5 1.7) (drill (offset -0.9 0)) (layers "F.Cu" "F.Mask")
      (net 17 "unconnected-(U1-GPIO4-Pad6)") (pinfunction "GPIO4") (pintype "bidirectional"))
    (pad "7" thru_hole oval (at -8.89 -8.89) (size 1.7 1.7) (drill 1.02) (layers "*.Cu" "*.Mask")
      (net 18 "unconnected-(U1-GPIO5-Pad7)") (pinfunction "GPIO5") (pintype "bidirectional"))
    (pad "7" smd rect (at -8.89 -8.89) (size 3.5 1.7) (drill (offset -0.9 0)) (layers "F.Cu" "F.Mask")
      (net 18 "unconnected-(U1-GPIO5-Pad7)") (pinfunction "GPIO5") (pintype "bidirectional"))
    (pad "8" thru_hole rect (at -8.89 -6.35) (size 1.7 1.7) (drill 1.02) (layers "*.Cu" "*.Mask")
      (net 19 "unconnected-(U1-GND-Pad8)") (pinfunction "GND") (pintype "power_in"))
    (pad "8" smd rect (at -8.89 -6.35) (size 3.5 1.7) (drill (offset -0.9 0)) (layers "F.Cu" "F.Mask")
      (net 19 "unconnected-(U1-GND-Pad8)") (pinfunction "GND") (pintype "power_in"))
    (pad "9" thru_hole oval (at -8.89 -3.81) (size 1.7 1.7) (drill 1.02) (layers "*.Cu" "*.Mask")
      (net 20 "unconnected-(U1-GPIO6-Pad9)") (pinfunction "GPIO6") (pintype "bidirectional"))
    (pad "9" smd rect (at -8.89 -3.81) (size 3.5 1.7) (drill (offset -0.9 0)) (layers "F.Cu" "F.Mask")
      (net 20 "unconnected-(U1-GPIO6-Pad9)") (pinfunction "GPIO6") (pintype "bidirectional"))
    (pad "10" thru_hole oval (at -8.89 -1.27) (size 1.7 1.7) (drill 1.02) (layers "*.Cu" "*.Mask")
      (net 21 "unconnected-(U1-GPIO7-Pad10)") (pinfunction "GPIO7") (pintype "bidirectional"))
    (pad "10" smd rect (at -8.89 -1.27) (size 3.5 1.7) (drill (offset -0.9 0)) (layers "F.Cu" "F.Mask")
      (net 21 "unconnected-(U1-GPIO7-Pad10)") (pinfunction "GPIO7") (pintype "bidirectional"))
    (pad "11" thru_hole oval (at -8.89 1.27) (size 1.7 1.7) (drill 1.02) (layers "*.Cu" "*.Mask")
      (net 22 "unconnected-(U1-GPIO8-Pad11)") (pinfunction "GPIO8") (pintype "bidirectional"))
    (pad "11" smd rect (at -8.89 1.27) (size 3.5 1.7) (drill (offset -0.9 0)) (layers "F.Cu" "F.Mask")
      (net 22 "unconnected-(U1-GPIO8-Pad11)") (pinfunction "GPIO8") (pintype "bidirectional"))
    (pad "12" thru_hole oval (at -8.89 3.81) (size 1.7 1.7) (drill 1.02) (layers "*.Cu" "*.Mask")
      (net 23 "unconnected-(U1-GPIO9-Pad12)") (pinfunction "GPIO9") (pintype "bidirectional"))
    (pad "12" smd rect (at -8.89 3.81) (size 3.5 1.7) (drill (offset -0.9 0)) (layers "F.Cu" "F.Mask")
      (net 23 "unconnected-(U1-GPIO9-Pad12)") (pinfunction "GPIO9") (pintype "bidirectional"))
    (pad "13" thru_hole rect (at -8.89 6.35) (size 1.7 1.7) (drill 1.02) (layers "*.Cu" "*.Mask")
      (net 24 "unconnected-(U1-GND-Pad13)") (pinfunction "GND") (pintype "power_in"))
    (pad "13" smd rect (at -8.89 6.35) (size 3.5 1.7) (drill (offset -0.9 0)) (layers "F.Cu" "F.Mask")
      (net 24 "unconnected-(U1-GND-Pad13)") (pinfunction "GND") (pintype "power_in"))
    (pad "14" thru_hole oval (at -8.89 8.89) (size 1.7 1.7) (drill 1.02) (layers "*.Cu" "*.Mask")
      (net 25 "unconnected-(U1-GPIO10-Pad14)") (pinfunction "GPIO10") (pintype "bidirectional"))
    (pad "14" smd rect (at -8.89 8.89) (size 3.5 1.7) (drill (offset -0.9 0)) (layers "F.Cu" "F.Mask")
      (net 25 "unconnected-(U1-GPIO10-Pad14)") (pinfunction "GPIO10") (pintype "bidirectional"))
    (pad "15" thru_hole oval (at -8.89 11.43) (size 1.7 1.7) (drill 1.02) (layers "*.Cu" "*.Mask")
      (net 26 "unconnected-(U1-GPIO11-Pad15)") (pinfunction "GPIO11") (pintype "bidirectional"))
    (pad "15" smd rect (at -8.89 11.43) (size 3.5 1.7) (drill (offset -0.9 0)) (layers "F.Cu" "F.Mask")
      (net 26 "unconnected-(U1-GPIO11-Pad15)") (pinfunction "GPIO11") (pintype "bidirectional"))
    (pad "16" thru_hole oval (at -8.89 13.97) (size 1.7 1.7) (drill 1.02) (layers "*.Cu" "*.Mask")
      (net 27 "unconnected-(U1-GPIO12-Pad16)") (pinfunction "GPIO12") (pintype "bidirectional"))
    (pad "16" smd rect (at -8.89 13.97) (size 3.5 1.7) (drill (offset -0.9 0)) (layers "F.Cu" "F.Mask")
      (net 27 "unconnected-(U1-GPIO12-Pad16)") (pinfunction "GPIO12") (pintype "bidirectional"))
    (pad "17" thru_hole oval (at -8.89 16.51) (size 1.7 1.7) (drill 1.02) (layers "*.Cu" "*.Mask")
      (net 28 "unconnected-(U1-GPIO13-Pad17)") (pinfunction "GPIO13") (pintype "bidirectional"))
    (pad "17" smd rect (at -8.89 16.51) (size 3.5 1.7) (drill (offset -0.9 0)) (layers "F.Cu" "F.Mask")
      (net 28 "unconnected-(U1-GPIO13-Pad17)") (pinfunction "GPIO13") (pintype "bidirectional"))
    (pad "18" thru_hole rect (at -8.89 19.05) (size 1.7 1.7) (drill 1.02) (layers "*.Cu" "*.Mask")
      (net 29 "unconnected-(U1-GND-Pad18)") (pinfunction "GND") (pintype "power_in"))
    (pad "18" smd rect (at -8.89 19.05) (size 3.5 1.7) (drill (offset -0.9 0)) (layers "F.Cu" "F.Mask")
      (net 29 "unconnected-(U1-GND-Pad18)") (pinfunction "GND") (pintype "power_in"))
    (pad "19" thru_hole oval (at -8.89 21.59) (size 1.7 1.7) (drill 1.02) (layers "*.Cu" "*.Mask")
      (net 30 "unconnected-(U1-GPIO14-Pad19)") (pinfunction "GPIO14") (pintype "bidirectional"))
    (pad "19" smd rect (at -8.89 21.59) (size 3.5 1.7) (drill (offset -0.9 0)) (layers "F.Cu" "F.Mask")
      (net 30 "unconnected-(U1-GPIO14-Pad19)") (pinfunction "GPIO14") (pintype "bidirectional"))
    (pad "20" thru_hole oval (at -8.89 24.13) (size 1.7 1.7) (drill 1.02) (layers "*.Cu" "*.Mask")
      (net 9 "Net-(U1-GPIO15)") (pinfunction "GPIO15") (pintype "bidirectional"))
    (pad "20" smd rect (at -8.89 24.13) (size 3.5 1.7) (drill (offset -0.9 0)) (layers "F.Cu" "F.Mask")
      (net 9 "Net-(U1-GPIO15)") (pinfunction "GPIO15") (pintype "bidirectional"))
    (pad "21" thru_hole oval (at 8.89 24.13) (size 1.7 1.7) (drill 1.02) (layers "*.Cu" "*.Mask")
      (net 11 "Net-(U1-GPIO16)") (pinfunction "GPIO16") (pintype "bidirectional"))
    (pad "21" smd rect (at 8.89 24.13) (size 3.5 1.7) (drill (offset 0.9 0)) (layers "F.Cu" "F.Mask")
      (net 11 "Net-(U1-GPIO16)") (pinfunction "GPIO16") (pintype "bidirectional"))
    (pad "22" thru_hole oval (at 8.89 21.59) (size 1.7 1.7) (drill 1.02) (layers "*.Cu" "*.Mask")
      (net 10 "Net-(U1-GPIO17)") (pinfunction "GPIO17") (pintype "bidirectional"))
    (pad "22" smd rect (at 8.89 21.59) (size 3.5 1.7) (drill (offset 0.9 0)) (layers "F.Cu" "F.Mask")
      (net 10 "Net-(U1-GPIO17)") (pinfunction "GPIO17") (pintype "bidirectional"))
    (pad "23" thru_hole rect (at 8.89 19.05) (size 1.7 1.7) (drill 1.02) (layers "*.Cu" "*.Mask")
      (net 31 "unconnected-(U1-GND-Pad23)") (pinfunction "GND") (pintype "power_in"))
    (pad "23" smd rect (at 8.89 19.05) (size 3.5 1.7) (drill (offset 0.9 0)) (layers "F.Cu" "F.Mask")
      (net 31 "unconnected-(U1-GND-Pad23)") (pinfunction "GND") (pintype "power_in"))
    (pad "24" thru_hole oval (at 8.89 16.51) (size 1.7 1.7) (drill 1.02) (layers "*.Cu" "*.Mask")
      (net 32 "unconnected-(U1-GPIO18-Pad24)") (pinfunction "GPIO18") (pintype "bidirectional"))
    (pad "24" smd rect (at 8.89 16.51) (size 3.5 1.7) (drill (offset 0.9 0)) (layers "F.Cu" "F.Mask")
      (net 32 "unconnected-(U1-GPIO18-Pad24)") (pinfunction "GPIO18") (pintype "bidirectional"))
    (pad "25" thru_hole oval (at 8.89 13.97) (size 1.7 1.7) (drill 1.02) (layers "*.Cu" "*.Mask")
      (net 33 "unconnected-(U1-GPIO19-Pad25)") (pinfunction "GPIO19") (pintype "bidirectional"))
    (pad "25" smd rect (at 8.89 13.97) (size 3.5 1.7) (drill (offset 0.9 0)) (layers "F.Cu" "F.Mask")
      (net 33 "unconnected-(U1-GPIO19-Pad25)") (pinfunction "GPIO19") (pintype "bidirectional"))
    (pad "26" thru_hole oval (at 8.89 11.43) (size 1.7 1.7) (drill 1.02) (layers "*.Cu" "*.Mask")
      (net 34 "unconnected-(U1-GPIO20-Pad26)") (pinfunction "GPIO20") (pintype "bidirectional"))
    (pad "26" smd rect (at 8.89 11.43) (size 3.5 1.7) (drill (offset 0.9 0)) (layers "F.Cu" "F.Mask")
      (net 34 "unconnected-(U1-GPIO20-Pad26)") (pinfunction "GPIO20") (pintype "bidirectional"))
    (pad "27" thru_hole oval (at 8.89 8.89) (size 1.7 1.7) (drill 1.02) (layers "*.Cu" "*.Mask")
      (net 35 "unconnected-(U1-GPIO21-Pad27)") (pinfunction "GPIO21") (pintype "bidirectional"))
    (pad "27" smd rect (at 8.89 8.89) (size 3.5 1.7) (drill (offset 0.9 0)) (layers "F.Cu" "F.Mask")
      (net 35 "unconnected-(U1-GPIO21-Pad27)") (pinfunction "GPIO21") (pintype "bidirectional"))
    (pad "28" thru_hole rect (at 8.89 6.35) (size 1.7 1.7) (drill 1.02) (layers "*.Cu" "*.Mask")
      (net 36 "unconnected-(U1-GND-Pad28)") (pinfunction "GND") (pintype "power_in"))
    (pad "28" smd rect (at 8.89 6.35) (size 3.5 1.7) (drill (offset 0.9 0)) (layers "F.Cu" "F.Mask")
      (net 36 "unconnected-(U1-GND-Pad28)") (pinfunction "GND") (pintype "power_in"))
    (pad "29" thru_hole oval (at 8.89 3.81) (size 1.7 1.7) (drill 1.02) (layers "*.Cu" "*.Mask")
      (net 37 "unconnected-(U1-GPIO22-Pad29)") (pinfunction "GPIO22") (pintype "bidirectional"))
    (pad "29" smd rect (at 8.89 3.81) (size 3.5 1.7) (drill (offset 0.9 0)) (layers "F.Cu" "F.Mask")
      (net 37 "unconnected-(U1-GPIO22-Pad29)") (pinfunction "GPIO22") (pintype "bidirectional"))
    (pad "30" thru_hole oval (at 8.89 1.27) (size 1.7 1.7) (drill 1.02) (layers "*.Cu" "*.Mask")
      (net 38 "unconnected-(U1-RUN-Pad30)") (pinfunction "RUN") (pintype "input"))
    (pad "30" smd rect (at 8.89 1.27) (size 3.5 1.7) (drill (offset 0.9 0)) (layers "F.Cu" "F.Mask")
      (net 38 "unconnected-(U1-RUN-Pad30)") (pinfunction "RUN") (pintype "input"))
    (pad "31" thru_hole oval (at 8.89 -1.27) (size 1.7 1.7) (drill 1.02) (layers "*.Cu" "*.Mask")
      (net 39 "unconnected-(U1-GPIO26_ADC0-Pad31)") (pinfunction "GPIO26_ADC0") (pintype "bidirectional"))
    (pad "31" smd rect (at 8.89 -1.27) (size 3.5 1.7) (drill (offset 0.9 0)) (layers "F.Cu" "F.Mask")
      (net 39 "unconnected-(U1-GPIO26_ADC0-Pad31)") (pinfunction "GPIO26_ADC0") (pintype "bidirectional"))
    (pad "32" thru_hole oval (at 8.89 -3.81) (size 1.7 1.7) (drill 1.02) (layers "*.Cu" "*.Mask")
      (net 40 "unconnected-(U1-GPIO27_ADC1-Pad32)") (pinfunction "GPIO27_ADC1") (pintype "bidirectional"))
    (pad "32" smd rect (at 8.89 -3.81) (size 3.5 1.7) (drill (offset 0.9 0)) (layers "F.Cu" "F.Mask")
      (net 40 "unconnected-(U1-GPIO27_ADC1-Pad32)") (pinfunction "GPIO27_ADC1") (pintype "bidirectional"))
    (pad "33" thru_hole rect (at 8.89 -6.35) (size 1.7 1.7) (drill 1.02) (layers "*.Cu" "*.Mask")
      (net 41 "unconnected-(U1-AGND-Pad33)") (pinfunction "AGND") (pintype "power_in"))
    (pad "33" smd rect (at 8.89 -6.35) (size 3.5 1.7) (drill (offset 0.9 0)) (layers "F.Cu" "F.Mask")
      (net 41 "unconnected-(U1-AGND-Pad33)") (pinfunction "AGND") (pintype "power_in"))
    (pad "34" thru_hole oval (at 8.89 -8.89) (size 1.7 1.7) (drill 1.02) (layers "*.Cu" "*.Mask")
      (net 42 "unconnected-(U1-GPIO28_ADC2-Pad34)") (pinfunction "GPIO28_ADC2") (pintype "bidirectional"))
    (pad "34" smd rect (at 8.89 -8.89) (size 3.5 1.7) (drill (offset 0.9 0)) (layers "F.Cu" "F.Mask")
      (net 42 "unconnected-(U1-GPIO28_ADC2-Pad34)") (pinfunction "GPIO28_ADC2") (pintype "bidirectional"))
    (pad "35" thru_hole oval (at 8.89 -11.43) (size 1.7 1.7) (drill 1.02) (layers "*.Cu" "*.Mask")
      (net 43 "unconnected-(U1-ADC_VREF-Pad35)") (pinfunction "ADC_VREF") (pintype "power_in"))
    (pad "35" smd rect (at 8.89 -11.43) (size 3.5 1.7) (drill (offset 0.9 0)) (layers "F.Cu" "F.Mask")
      (net 43 "unconnected-(U1-ADC_VREF-Pad35)") (pinfunction "ADC_VREF") (pintype "power_in"))
    (pad "36" thru_hole oval (at 8.89 -13.97) (size 1.7 1.7) (drill 1.02) (layers "*.Cu" "*.Mask")
      (net 44 "unconnected-(U1-3V3-Pad36)") (pinfunction "3V3") (pintype "power_in"))
    (pad "36" smd rect (at 8.89 -13.97) (size 3.5 1.7) (drill (offset 0.9 0)) (layers "F.Cu" "F.Mask")
      (net 44 "unconnected-(U1-3V3-Pad36)") (pinfunction "3V3") (pintype "power_in"))
    (pad "37" thru_hole oval (at 8.89 -16.51) (size 1.7 1.7) (drill 1.02) (layers "*.Cu" "*.Mask")
      (net 45 "unconnected-(U1-3V3_EN-Pad37)") (pinfunction "3V3_EN") (pintype "input"))
    (pad "37" smd rect (at 8.89 -16.51) (size 3.5 1.7) (drill (offset 0.9 0)) (layers "F.Cu" "F.Mask")
      (net 45 "unconnected-(U1-3V3_EN-Pad37)") (pinfunction "3V3_EN") (pintype "input"))
    (pad "38" thru_hole rect (at 8.89 -19.05) (size 1.7 1.7) (drill 1.02) (layers "*.Cu" "*.Mask")
      (net 6 "Net-(Q1-C)") (pinfunction "GND") (pintype "bidirectional"))
    (pad "38" smd rect (at 8.89 -19.05) (size 3.5 1.7) (drill (offset 0.9 0)) (layers "F.Cu" "F.Mask")
      (net 6 "Net-(Q1-C)") (pinfunction "GND") (pintype "bidirectional"))
    (pad "39" thru_hole oval (at 8.89 -21.59) (size 1.7 1.7) (drill 1.02) (layers "*.Cu" "*.Mask")
      (net 46 "unconnected-(U1-VSYS-Pad39)") (pinfunction "VSYS") (pintype "power_in"))
    (pad "39" smd rect (at 8.89 -21.59) (size 3.5 1.7) (drill (offset 0.9 0)) (layers "F.Cu" "F.Mask")
      (net 46 "unconnected-(U1-VSYS-Pad39)") (pinfunction "VSYS") (pintype "power_in"))
    (pad "40" thru_hole oval (at 8.89 -24.13) (size 1.7 1.7) (drill 1.02) (layers "*.Cu" "*.Mask")
      (net 1 "Net-(J1-Pin_1)") (pinfunction "VBUS") (pintype "power_in"))
    (pad "40" smd rect (at 8.89 -24.13) (size 3.5 1.7) (drill (offset 0.9 0)) (layers "F.Cu" "F.Mask")
      (net 1 "Net-(J1-Pin_1)") (pinfunction "VBUS") (pintype "power_in"))
    (pad "41" thru_hole oval (at -2.54 23.9) (size 1.7 1.7) (drill 1.02) (layers "*.Cu" "*.Mask")
      (net 47 "unconnected-(U1-SWCLK-Pad41)") (pinfunction "SWCLK") (pintype "input"))
    (pad "41" smd rect (at -2.54 23.9 90) (size 3.5 1.7) (drill (offset -0.9 0)) (layers "F.Cu" "F.Mask")
      (net 47 "unconnected-(U1-SWCLK-Pad41)") (pinfunction "SWCLK") (pintype "input"))
    (pad "42" thru_hole rect (at 0 23.9) (size 1.7 1.7) (drill 1.02) (layers "*.Cu" "*.Mask")
      (net 48 "unconnected-(U1-GND-Pad42)") (pinfunction "GND") (pintype "power_in"))
    (pad "42" smd rect (at 0 23.9 90) (size 3.5 1.7) (drill (offset -0.9 0)) (layers "F.Cu" "F.Mask")
      (net 48 "unconnected-(U1-GND-Pad42)") (pinfunction "GND") (pintype "power_in"))
    (pad "43" thru_hole oval (at 2.54 23.9) (size 1.7 1.7) (drill 1.02) (layers "*.Cu" "*.Mask")
      (net 49 "unconnected-(U1-SWDIO-Pad43)") (pinfunction "SWDIO") (pintype "bidirectional"))
    (pad "43" smd rect (at 2.54 23.9 90) (size 3.5 1.7) (drill (offset -0.9 0)) (layers "F.Cu" "F.Mask")
      (net 49 "unconnected-(U1-SWDIO-Pad43)") (pinfunction "SWDIO") (pintype "bidirectional"))
    (model "C:/Users/ncara/OneDrive/IoT/Tools/KiCad/RP-Pico Libraries/Pico.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_rect (start 116.84 40.64) (end 152.4 124.46)
    (fill none) (layer "Edge.Cuts"))
)
