(kicad_pcb
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(general
		(thickness 1.6)
		(legacy_teardrops no)
	)
	(paper "A4")
	(title_block
		(title "ATF150x_uPRG_j")
		(date "2026-09-06")
		(rev "004")
		(company "Brian K. White")
		(comment 1 "CC-BY-SA")
		(comment 2 "github.com/bkw777/ATF150x_uPRG")
	)
	(layers
		(0 "F.Cu" signal)
		(2 "B.Cu" signal)
		(9 "F.Adhes" user "F.Adhesive")
		(11 "B.Adhes" user "B.Adhesive")
		(13 "F.Paste" user)
		(15 "B.Paste" user)
		(5 "F.SilkS" user "F.Silkscreen")
		(7 "B.SilkS" user "B.Silkscreen")
		(1 "F.Mask" user)
		(3 "B.Mask" user)
		(17 "Dwgs.User" user "User.Drawings")
		(19 "Cmts.User" user "User.Comments")
		(21 "Eco1.User" user "User.Eco1")
		(23 "Eco2.User" user "User.Eco2")
		(25 "Edge.Cuts" user)
		(27 "Margin" user)
		(31 "F.CrtYd" user "F.Courtyard")
		(29 "B.CrtYd" user "B.Courtyard")
		(35 "F.Fab" user)
		(33 "B.Fab" user)
	)
	(setup
		(stackup
			(layer "F.SilkS"
				(type "Top Silk Screen")
			)
			(layer "F.Paste"
				(type "Top Solder Paste")
			)
			(layer "F.Mask"
				(type "Top Solder Mask")
				(thickness 0.01)
			)
			(layer "F.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "dielectric 1"
				(type "core")
				(thickness 1.51)
				(material "FR4")
				(epsilon_r 4.5)
				(loss_tangent 0.02)
			)
			(layer "B.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "B.Mask"
				(type "Bottom Solder Mask")
				(thickness 0.01)
			)
			(layer "B.Paste"
				(type "Bottom Solder Paste")
			)
			(layer "B.SilkS"
				(type "Bottom Silk Screen")
			)
			(copper_finish "ENIG")
			(dielectric_constraints no)
		)
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(tenting front back)
		(pcbplotparams
			(layerselection 0x00000000_00000000_55555555_f755f5ff)
			(plot_on_all_layers_selection 0x00000000_00000000_00000000_00000000)
			(disableapertmacros no)
			(usegerberextensions yes)
			(usegerberattributes no)
			(usegerberadvancedattributes no)
			(creategerberjobfile no)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 4)
			(plotframeref no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(pdf_metadata yes)
			(pdf_single_document no)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plot_black_and_white yes)
			(sketchpadsonfab no)
			(plotpadnumbers no)
			(hidednponfab no)
			(sketchdnponfab yes)
			(crossoutdnponfab yes)
			(subtractmaskfromsilk yes)
			(outputformat 1)
			(mirror no)
			(drillshape 0)
			(scaleselection 1)
			(outputdirectory "GERBER_${TITLE}_${REVISION}")
		)
	)
	(net 0 "")
	(net 1 "TCK")
	(net 2 "TDI")
	(net 3 "TDO")
	(net 4 "TMS")
	(net 5 "Net-(C7-Pad1)")
	(net 6 "Net-(C7-Pad2)")
	(net 7 "unconnected-(J1-AC1-Pad13)")
	(net 8 "unconnected-(J1-AD4-Pad8)")
	(net 9 "+5V")
	(net 10 "GND")
	(net 11 "unconnected-(J1-AD6-Pad10)")
	(net 12 "unconnected-(J1-AC0-Pad12)")
	(net 13 "unconnected-(J1-AC5-Pad17)")
	(net 14 "unconnected-(J1-AC3-Pad15)")
	(net 15 "unconnected-(J1-AC6-Pad18)")
	(net 16 "unconnected-(J1-AC4-Pad16)")
	(net 17 "unconnected-(J1-AC8-Pad20)")
	(net 18 "unconnected-(J1-AD5-Pad9)")
	(net 19 "unconnected-(J1-AC9-Pad21)")
	(net 20 "unconnected-(J1-AC7-Pad19)")
	(net 21 "unconnected-(J1-AC2-Pad14)")
	(net 22 "+12V")
	(net 23 "unconnected-(J1-AD7-Pad11)")
	(net 24 "+3V3")
	(net 25 "unconnected-(JP1-Pad1)")
	(net 26 "unconnected-(JP2-Pad1)")
	(net 27 "Net-(JP2-Pad3)")
	(net 28 "Net-(LED1-A)")
	(net 29 "Net-(LED2-A)")
	(net 30 "Net-(LED3-A)")
	(net 31 "VCC")
	(net 32 "Net-(C6-Pad2)")
	(net 33 "Net-(C6-Pad1)")
	(net 34 "VPP")
	(net 35 "unconnected-(J2-nc-Pad7)")
	(net 36 "unconnected-(J2-nc-Pad8)")
	(footprint "000_LOCAL:R_0805"
		(layer "F.Cu")
		(at 131.572 95.885)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "R2"
			(at 1.905 -0.508 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "10k"
			(at 1.905 0.635 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "ATF150x_uPRG.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0)
			(size 0.9 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 28 "Net-(LED1-A)")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at 0.95 0)
			(size 0.9 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 31 "VCC")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KIPRJMOD}/000_LOCAL.pretty/3dshapes/R_0805.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "000_LOCAL:C_0805"
		(layer "F.Cu")
		(at 140.649999 99.441)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C1"
			(at 2.479001 -0.508 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "1u"
			(at 2.479001 0.508 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "ATF150x_uPRG.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -1.270001 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.949999 0)
			(size 0.9 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 9 "+5V")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at 0.949999 0)
			(size 0.9 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 10 "GND")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KIPRJMOD}/000_LOCAL.pretty/3dshapes/C_0805.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "000_LOCAL:Fiducial_0.5_1.0"
		(layer "F.Cu")
		(at 159.76 87.23)
		(descr "Circular Fiducial, 0.5mm bare copper, 1mm soldermask opening (Level C)")
		(tags "fiducial")
		(property "Reference" "REF**"
			(at 0 -1.5 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Fiducial_0.5_1.0"
			(at 0 1.5 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "" smd circle
			(at 0 0)
			(size 0.5 0.5)
			(layers "F.Cu" "F.Mask")
			(solder_mask_margin 0.25)
			(clearance 0.25)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
	)
	(footprint "000_LOCAL:SOIC-8"
		(layer "F.Cu")
		(at 137.225 91.186)
		(descr "SOIC, 8 Pin (JEDEC MS-012AA, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_narrow-r/r_8.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOIC SO")
		(property "Reference" "U2"
			(at -1.208 -2.427 270)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "MAX662A"
			(at 0.443 0 270)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "ATF150x_uPRG.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -2.667 -1.905)
			(size 1.5 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 33 "Net-(C6-Pad1)")
			(pinfunction "C1-")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at -2.667 -0.635)
			(size 1.5 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 32 "Net-(C6-Pad2)")
			(pinfunction "C1+")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "3" smd roundrect
			(at -2.667 0.635)
			(size 1.5 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 5 "Net-(C7-Pad1)")
			(pinfunction "C1-")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "4" smd roundrect
			(at -2.667 1.905)
			(size 1.5 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 6 "Net-(C7-Pad2)")
			(pinfunction "C1+")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "5" smd roundrect
			(at 2.667 1.905)
			(size 1.5 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 9 "+5V")
			(pinfunction "Vcc")
			(pintype "power_in")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "6" smd roundrect
			(at 2.667 0.635)
			(size 1.5 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 22 "+12V")
			(pinfunction "Vout")
			(pintype "power_out")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "7" smd roundrect
			(at 2.667 -0.635)
			(size 1.5 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 10 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "8" smd roundrect
			(at 2.667 -1.905)
			(size 1.5 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 10 "GND")
			(pinfunction "SHDN")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KIPRJMOD}/000_LOCAL.pretty/3dshapes/SO-8_3.9x4.9mm_P1.27mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "000_LOCAL:Fiducial_0.5_1.0"
		(layer "F.Cu")
		(at 128.16 88.79)
		(descr "Circular Fiducial, 0.5mm bare copper, 1mm soldermask opening (Level C)")
		(tags "fiducial")
		(property "Reference" "REF**"
			(at 0 -1.5 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Fiducial_0.5_1.0"
			(at 0 1.5 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "" smd circle
			(at 0 0)
			(size 0.5 0.5)
			(layers "F.Cu" "F.Mask")
			(solder_mask_margin 0.25)
			(clearance 0.25)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
	)
	(footprint "000_LOCAL:C_0805"
		(layer "F.Cu")
		(at 142.177998 90.7186 90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C4"
			(at 3.3426 -0.064998 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "1u"
			(at 2.1996 -0.064998 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "ATF150x_uPRG.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -1.270001 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.949999 0 90)
			(size 0.9 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 22 "+12V")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at 0.949999 0 90)
			(size 0.9 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 10 "GND")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KIPRJMOD}/000_LOCAL.pretty/3dshapes/C_0805.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "000_LOCAL:IDC-Header_2x05_P2.54mm pcb-edge"
		(layer "F.Cu")
		(at 165.09 95.25)
		(descr "Through hole IDC box header, 2x05, 2.54mm pitch, DIN 41651 / IEC 60603-13, double rows, https://docs.google.com/spreadsheets/d/16SsEcesNF15N3Lb4niX7dcUr-NY5_MFPQhobNuNppn4/edit#gid=0")
		(tags "Through hole horizontal IDC box header THT 2x05 2.54mm double row")
		(property "Reference" "J2"
			(at -4.689 -6.985 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Altera JTAG-A+VPP"
			(at -6.096 0 270)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "datasheets/JTAG-A.pdf"
			(at -4.318 -5.08 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, double row, 02x05, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at -4.318 -5.08 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_2x??_*")
		(sheetname "Root")
		(sheetfile "ATF150x_uPRG.kicad_sch")
		(attr through_hole)
		(fp_text user "PCB EDGE"
			(at 4.445 11.303 0)
			(unlocked yes)
			(layer "Dwgs.User")
		)
		(fp_text user "PCB EDGE"
			(at -0.889 9.271 270)
			(unlocked yes)
			(layer "Dwgs.User")
		)
		(fp_text user "${REFERENCE}"
			(at 4.512 0 90)
			(layer "F.Fab")
		)
		(pad "1" connect roundrect
			(at -1.905 -5.08)
			(size 3.81 1.905)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(chamfer_ratio 0)
			(chamfer top_right bottom_right)
			(net 1 "TCK")
			(pinfunction "TCK")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" connect roundrect
			(at -1.905 -5.08)
			(size 3.81 1.905)
			(layers "B.Cu" "B.Mask")
			(roundrect_rratio 0.25)
			(chamfer_ratio 0)
			(chamfer top_right bottom_right)
			(net 10 "GND")
			(pinfunction "GND")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "3" connect roundrect
			(at -1.905 -2.54)
			(size 3.81 1.905)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(chamfer_ratio 0)
			(chamfer top_right bottom_right)
			(net 3 "TDO")
			(pinfunction "TDO")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "4" connect roundrect
			(at -1.905 -2.54)
			(size 3.81 1.905)
			(layers "B.Cu" "B.Mask")
			(roundrect_rratio 0.25)
			(chamfer_ratio 0)
			(chamfer top_right bottom_right)
			(net 31 "VCC")
			(pinfunction "VREF")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "5" connect roundrect
			(at -1.905 0)
			(size 3.81 1.905)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(chamfer_ratio 0)
			(chamfer top_right bottom_right)
			(net 4 "TMS")
			(pinfunction "TMS")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "6" connect roundrect
			(at -1.905 0)
			(size 3.81 1.905)
			(layers "B.Cu" "B.Mask")
			(roundrect_rratio 0.25)
			(chamfer_ratio 0)
			(chamfer top_right bottom_right)
			(net 34 "VPP")
			(pinfunction "VPP")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "7" connect roundrect
			(at -1.905 2.54)
			(size 3.81 1.905)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(chamfer_ratio 0)
			(chamfer top_right bottom_right)
			(net 35 "unconnected-(J2-nc-Pad7)")
			(pinfunction "nc")
			(pintype "passive+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "8" connect roundrect
			(at -1.905 2.54)
			(size 3.81 1.905)
			(layers "B.Cu" "B.Mask")
			(roundrect_rratio 0.25)
			(chamfer_ratio 0)
			(chamfer top_right bottom_right)
			(net 36 "unconnected-(J2-nc-Pad8)")
			(pinfunction "nc")
			(pintype "passive+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "9" connect roundrect
			(at -1.905 5.08)
			(size 3.81 1.905)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(chamfer_ratio 0)
			(chamfer top_right bottom_right)
			(net 2 "TDI")
			(pinfunction "TDI")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "10" connect roundrect
			(at -1.905 5.08)
			(size 3.81 1.905)
			(layers "B.Cu" "B.Mask")
			(roundrect_rratio 0.25)
			(chamfer_ratio 0)
			(chamfer top_right bottom_right)
			(net 10 "GND")
			(pinfunction "GND")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KIPRJMOD}/000_LOCAL.pretty/3dshapes/IDC-Header_2x05_P2.54mm_Vertical.step"
			(offset
				(xyz -0.2032 5.08 0.4318)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 -90 0)
			)
		)
	)
	(footprint "000_LOCAL:R_0805"
		(layer "F.Cu")
		(at 146.812 92.618597 90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "R1"
			(at 0.416597 1.016 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "2k2"
			(at -0.726403 1.016 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "ATF150x_uPRG.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -1.270001 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.949999 0 90)
			(size 0.9 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 27 "Net-(JP2-Pad3)")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at 0.949999 0 90)
			(size 0.9 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 22 "+12V")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KIPRJMOD}/000_LOCAL.pretty/3dshapes/R_0805.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "000_LOCAL:Fiducial_0.5_1.0"
		(layer "F.Cu")
		(at 131.86 102.67)
		(descr "Circular Fiducial, 0.5mm bare copper, 1mm soldermask opening (Level C)")
		(tags "fiducial")
		(property "Reference" "REF**"
			(at 0 -1.5 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Fiducial_0.5_1.0"
			(at 0 1.5 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "" smd circle
			(at 0 0)
			(size 0.5 0.5)
			(layers "F.Cu" "F.Mask")
			(solder_mask_margin 0.25)
			(clearance 0.25)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
	)
	(footprint "000_LOCAL:Adafruit_2264"
		(layer "F.Cu")
		(at 146.05 95.251)
		(property "Reference" "J1"
			(at 8.89 -6.604 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Adafruit_2264"
			(at 4.445 0.381 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Adafruit FT232H Breakout v2"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "ATF150x_uPRG.kicad_sch")
		(fp_line
			(start -19.05 -8.89)
			(end -19.05 8.89)
			(layer "Edge.Cuts")
		)
		(fp_line
			(start -16.51 11.43)
			(end 16.51 11.43)
			(layer "Edge.Cuts")
		)
		(fp_line
			(start 16.51 -11.43)
			(end -16.51 -11.43)
			(layer "Edge.Cuts")
		)
		(fp_line
			(start 19.05 8.89)
			(end 19.05 -8.89)
			(layer "Edge.Cuts")
		)
		(fp_arc
			(start -19.05 -8.89)
			(mid -18.306051 -10.686051)
			(end -16.51 -11.43)
			(layer "Edge.Cuts")
		)
		(fp_arc
			(start -16.51 11.43)
			(mid -18.306051 10.686051)
			(end -19.05 8.89)
			(layer "Edge.Cuts")
		)
		(fp_arc
			(start 16.51 -11.43)
			(mid 18.306051 -10.686051)
			(end 19.05 -8.89)
			(layer "Edge.Cuts")
		)
		(fp_arc
			(start 19.05 8.89)
			(mid 18.306051 10.686051)
			(end 16.51 11.43)
			(layer "Edge.Cuts")
		)
		(pad "1" thru_hole circle
			(at -12.7 10.033)
			(size 1.6 1.6)
			(drill 0.94)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 24 "+3V3")
			(pinfunction "3V3")
			(pintype "power_out")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" thru_hole circle
			(at -10.16 10.287)
			(size 1.6 1.6)
			(drill 0.94)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 9 "+5V")
			(pinfunction "5V")
			(pintype "power_out")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "3" thru_hole circle
			(at -7.62 10.033)
			(size 1.6 1.6)
			(drill 0.94)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 10 "GND")
			(pinfunction "GND")
			(pintype "power_out")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "4" thru_hole circle
			(at -5.08 10.287)
			(size 1.6 1.6)
			(drill 0.94)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "TCK")
			(pinfunction "AD0")
			(pintype "bidirectional")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "5" thru_hole circle
			(at -2.54 10.033)
			(size 1.6 1.6)
			(drill 0.94)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "TDI")
			(pinfunction "AD1")
			(pintype "bidirectional")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "6" thru_hole circle
			(at 0 10.287)
			(size 1.6 1.6)
			(drill 0.94)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "TDO")
			(pinfunction "AD2")
			(pintype "bidirectional")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "7" thru_hole circle
			(at 2.54 10.033)
			(size 1.6 1.6)
			(drill 0.94)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "TMS")
			(pinfunction "AD3")
			(pintype "bidirectional")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "8" thru_hole circle
			(at 5.08 10.287)
			(size 1.6 1.6)
			(drill 0.94)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 8 "unconnected-(J1-AD4-Pad8)")
			(pinfunction "AD4")
			(pintype "bidirectional+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "9" thru_hole circle
			(at 7.62 10.033)
			(size 1.6 1.6)
			(drill 0.94)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 18 "unconnected-(J1-AD5-Pad9)")
			(pinfunction "AD5")
			(pintype "bidirectional+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "10" thru_hole circle
			(at 10.16 10.287)
			(size 1.6 1.6)
			(drill 0.94)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 11 "unconnected-(J1-AD6-Pad10)")
			(pinfunction "AD6")
			(pintype "bidirectional+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "11" thru_hole circle
			(at 12.7 10.033)
			(size 1.6 1.6)
			(drill 0.94)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 23 "unconnected-(J1-AD7-Pad11)")
			(pinfunction "AD7")
			(pintype "bidirectional+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "12" thru_hole circle
			(at 12.7 -10.287)
			(size 1.6 1.6)
			(drill 0.94)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 12 "unconnected-(J1-AC0-Pad12)")
			(pinfunction "AC0")
			(pintype "bidirectional+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "13" thru_hole circle
			(at 10.16 -10.033)
			(size 1.6 1.6)
			(drill 0.94)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 7 "unconnected-(J1-AC1-Pad13)")
			(pinfunction "AC1")
			(pintype "bidirectional+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "14" thru_hole circle
			(at 7.62 -10.287)
			(size 1.6 1.6)
			(drill 0.94)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 21 "unconnected-(J1-AC2-Pad14)")
			(pinfunction "AC2")
			(pintype "bidirectional+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "15" thru_hole circle
			(at 5.08 -10.033)
			(size 1.6 1.6)
			(drill 0.94)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 14 "unconnected-(J1-AC3-Pad15)")
			(pinfunction "AC3")
			(pintype "bidirectional+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "16" thru_hole circle
			(at 2.54 -10.287)
			(size 1.6 1.6)
			(drill 0.94)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 16 "unconnected-(J1-AC4-Pad16)")
			(pinfunction "AC4")
			(pintype "bidirectional+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "17" thru_hole circle
			(at 0 -10.033)
			(size 1.6 1.6)
			(drill 0.94)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 13 "unconnected-(J1-AC5-Pad17)")
			(pinfunction "AC5")
			(pintype "bidirectional+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "18" thru_hole circle
			(at -2.54 -10.287)
			(size 1.6 1.6)
			(drill 0.94)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 15 "unconnected-(J1-AC6-Pad18)")
			(pinfunction "AC6")
			(pintype "bidirectional+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "19" thru_hole circle
			(at -5.08 -10.033)
			(size 1.6 1.6)
			(drill 0.94)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 20 "unconnected-(J1-AC7-Pad19)")
			(pinfunction "AC7")
			(pintype "bidirectional+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "20" thru_hole circle
			(at -7.62 -10.287)
			(size 1.6 1.6)
			(drill 0.94)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 17 "unconnected-(J1-AC8-Pad20)")
			(pinfunction "AC8")
			(pintype "bidirectional+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "21" thru_hole circle
			(at -10.16 -10.033)
			(size 1.6 1.6)
			(drill 0.94)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 19 "unconnected-(J1-AC9-Pad21)")
			(pinfunction "AC9")
			(pintype "bidirectional+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "22" thru_hole circle
			(at -12.7 -10.287)
			(size 1.6 1.6)
			(drill 0.94)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 10 "GND")
			(pinfunction "GND")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "M" thru_hole circle
			(at -16.51 -8.89)
			(size 3.2 3.2)
			(drill 2.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 10 "GND")
			(pinfunction "M")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "M" thru_hole circle
			(at -16.51 8.89)
			(size 3.2 3.2)
			(drill 2.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 10 "GND")
			(pinfunction "M")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "M" thru_hole circle
			(at 16.51 -8.89)
			(size 3.2 3.2)
			(drill 2.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 10 "GND")
			(pinfunction "M")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "M" thru_hole circle
			(at 16.51 8.89)
			(size 3.2 3.2)
			(drill 2.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 10 "GND")
			(pinfunction "M")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KIPRJMOD}/000_LOCAL.pretty/3dshapes/Adafruit_2264.step"
			(offset
				(xyz 0 0 2.54)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
		(model "${KIPRJMOD}/000_LOCAL.pretty/3dshapes/PinHeader_1x11_P2.54mm_Vertical.step"
			(offset
				(xyz 12.7 -10.16 2.54)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 180 90)
			)
		)
		(model "${KIPRJMOD}/000_LOCAL.pretty/3dshapes/PinHeader_1x11_P2.54mm_Vertical.step"
			(offset
				(xyz 12.7 10.16 2.54)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 180 90)
			)
		)
	)
	(footprint "000_LOCAL:R_0805"
		(layer "F.Cu")
		(at 131.572 100.711)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "R4"
			(at -1.778 0 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "10k"
			(at -1.651 1.143 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "ATF150x_uPRG.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.949999 0)
			(size 0.9 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 30 "Net-(LED3-A)")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at 0.949999 0)
			(size 0.9 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 9 "+5V")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KIPRJMOD}/000_LOCAL.pretty/3dshapes/R_0805.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "000_LOCAL:C_0805"
		(layer "F.Cu")
		(at 132.271997 89.448602 -90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C6"
			(at -0.548602 1.842997 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "1u"
			(at 0.594398 1.842997 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "ATF150x_uPRG.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -1.270001 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.949999 0 270)
			(size 0.9 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 33 "Net-(C6-Pad1)")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at 0.949999 0 270)
			(size 0.9 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 32 "Net-(C6-Pad2)")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KIPRJMOD}/000_LOCAL.pretty/3dshapes/C_0805.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "000_LOCAL:C_0805"
		(layer "F.Cu")
		(at 132.271997 92.923401 -90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C7"
			(at -0.594401 1.842997 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "1u"
			(at 0.548599 1.842997 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "ATF150x_uPRG.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -1.270001 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.949999 0 270)
			(size 0.9 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 5 "Net-(C7-Pad1)")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at 0.949999 0 270)
			(size 0.9 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 6 "Net-(C7-Pad2)")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KIPRJMOD}/000_LOCAL.pretty/3dshapes/C_0805.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "000_LOCAL:Fiducial_0.5_1.0"
		(layer "F.Cu")
		(at 160.38 102.43)
		(descr "Circular Fiducial, 0.5mm bare copper, 1mm soldermask opening (Level C)")
		(tags "fiducial")
		(property "Reference" "REF**"
			(at 0 -1.5 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Fiducial_0.5_1.0"
			(at 0 1.5 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "" smd circle
			(at 0 0)
			(size 0.5 0.5)
			(layers "F.Cu" "F.Mask")
			(solder_mask_margin 0.25)
			(clearance 0.25)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
	)
	(footprint "000_LOCAL:C_0805"
		(layer "F.Cu")
		(at 144.464998 90.718599 90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C5"
			(at 3.342599 -0.064998 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "1u"
			(at 2.199599 -0.064998 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "ATF150x_uPRG.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -1.270001 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.949999 0 90)
			(size 0.9 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 22 "+12V")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at 0.949999 0 90)
			(size 0.9 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 10 "GND")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KIPRJMOD}/000_LOCAL.pretty/3dshapes/C_0805.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "000_LOCAL:C_0805"
		(layer "F.Cu")
		(at 140.649999 97.282)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C2"
			(at 2.479001 -0.508 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "1u"
			(at 2.479001 0.508 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "ATF150x_uPRG.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -1.270001 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.949999 0)
			(size 0.9 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 9 "+5V")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at 0.949999 0)
			(size 0.9 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 10 "GND")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KIPRJMOD}/000_LOCAL.pretty/3dshapes/C_0805.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "000_LOCAL:C_0805"
		(layer "F.Cu")
		(at 140.649999 95.123)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C3"
			(at 2.479001 -0.508 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "1u"
			(at 2.479001 0.508 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "ATF150x_uPRG.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -1.270001 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.949999 0)
			(size 0.9 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 9 "+5V")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at 0.949999 0)
			(size 0.9 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 10 "GND")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KIPRJMOD}/000_LOCAL.pretty/3dshapes/C_0805.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "000_LOCAL:R_0805"
		(layer "F.Cu")
		(at 131.572 98.298)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "R3"
			(at 1.905 -0.508 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "10k"
			(at 1.905 0.635 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "ATF150x_uPRG.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0)
			(size 0.9 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 29 "Net-(LED2-A)")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at 0.95 0)
			(size 0.9 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 34 "VPP")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KIPRJMOD}/000_LOCAL.pretty/3dshapes/R_0805.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "000_LOCAL:LED_0805"
		(layer "B.Cu")
		(at 128.778 99.06)
		(descr "LED SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "LED")
		(property "Reference" "LED3"
			(at 0 1.65 180)
			(unlocked yes)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "PWR"
			(at 1.524 0 0)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Light emitting diode"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "LED* LED_SMD:* LED_THT:*")
		(sheetname "Root")
		(sheetfile "ATF150x_uPRG.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9375 0)
			(size 0.975 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 10 "GND")
			(pinfunction "K")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at 0.9375 0)
			(size 0.975 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 30 "Net-(LED3-A)")
			(pinfunction "A")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KIPRJMOD}/000_LOCAL.pretty/3dshapes/LED_0805.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "000_LOCAL:LED_0805"
		(layer "B.Cu")
		(at 128.778 95.25)
		(descr "LED SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "LED")
		(property "Reference" "LED2"
			(at 0 1.65 180)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "VPP"
			(at 1.524 0 0)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Light emitting diode"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "LED* LED_SMD:* LED_THT:*")
		(sheetname "Root")
		(sheetfile "ATF150x_uPRG.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9375 0)
			(size 0.975 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 10 "GND")
			(pinfunction "K")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at 0.9375 0)
			(size 0.975 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 29 "Net-(LED2-A)")
			(pinfunction "A")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KIPRJMOD}/000_LOCAL.pretty/3dshapes/LED_0805.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "000_LOCAL:LED_0805"
		(layer "B.Cu")
		(at 128.778 91.44)
		(descr "LED SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "LED")
		(property "Reference" "LED1"
			(at 0 1.65 180)
			(unlocked yes)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "VCC"
			(at 1.524 0 0)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Light emitting diode"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "LED* LED_SMD:* LED_THT:*")
		(sheetname "Root")
		(sheetfile "ATF150x_uPRG.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9375 0)
			(size 0.975 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 10 "GND")
			(pinfunction "K")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at 0.9375 0)
			(size 0.975 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 28 "Net-(LED1-A)")
			(pinfunction "A")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KIPRJMOD}/000_LOCAL.pretty/3dshapes/LED_0805.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "000_LOCAL:PinHeader_1x03_P2.54mm_Horizontal"
		(layer "B.Cu")
		(at 154.94 101.854 90)
		(descr "Through hole angled pin header, 1x03, 2.54mm pitch, 6mm pin length, single row")
		(tags "Through hole angled pin header THT 1x03 2.54mm single row")
		(property "Reference" "JP2"
			(at 2.794 -2.54 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "VPP"
			(at 14.732 -2.54 0)
			(unlocked yes)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Jumper, 3-pole, pins 1+2 closed/bridged"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Jumper* TestPoint*3Pads* TestPoint*Bridge*")
		(sheetname "Root")
		(sheetfile "ATF150x_uPRG.kicad_sch")
		(attr through_hole exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 2.77 -2.54 0)
			(layer "B.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 90)
			(size 1.6 1.6)
			(drill 0.95)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 26 "unconnected-(JP2-Pad1)")
			(pintype "passive+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" thru_hole circle
			(at 0 -2.54 90)
			(size 1.6 1.6)
			(drill 0.95)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 34 "VPP")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "3" thru_hole circle
			(at 0 -5.079999 90)
			(size 1.6 1.6)
			(drill 0.95)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 27 "Net-(JP2-Pad3)")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KIPRJMOD}/000_LOCAL.pretty/3dshapes/PinHeader_1x03_P2.54mm_Horizontal.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
		(model "${KIPRJMOD}/000_LOCAL.pretty/3dshapes/jumper.step"
			(offset
				(xyz 4.064 0 1.27)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 90 0 90)
			)
		)
	)
	(footprint "000_LOCAL:PinHeader_1x04_P2.54mm_Horizontal"
		(layer "B.Cu")
		(at 142.24 101.854 90)
		(descr "Through hole angled pin header, 1x04, 2.54mm pitch, 6mm pin length, single row")
		(tags "Through hole angled pin header THT 1x04 2.54mm single row")
		(property "Reference" "JP1"
			(at 4.385 2.27 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "VCC"
			(at 14.732 -3.81 0)
			(unlocked yes)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Jumper, 4-pole, pins 1+2 closed/bridged"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Jumper* TestPoint*3Pads* TestPoint*Bridge*")
		(sheetname "Root")
		(sheetfile "ATF150x_uPRG.kicad_sch")
		(attr through_hole exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 2.77 -3.81 0)
			(layer "B.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 90)
			(size 1.6 1.6)
			(drill 0.95)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 25 "unconnected-(JP1-Pad1)")
			(pintype "passive+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" thru_hole circle
			(at 0 -2.54 90)
			(size 1.6 1.6)
			(drill 0.95)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 9 "+5V")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "3" thru_hole circle
			(at 0 -5.079999 90)
			(size 1.6 1.6)
			(drill 0.95)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 31 "VCC")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "4" thru_hole circle
			(at 0 -7.62 90)
			(size 1.6 1.6)
			(drill 0.95)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 24 "+3V3")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KIPRJMOD}/000_LOCAL.pretty/3dshapes/PinHeader_1x04_P2.54mm_Horizontal.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
		(model "${KIPRJMOD}/000_LOCAL.pretty/3dshapes/jumper.step"
			(offset
				(xyz 4.064 0 1.27)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 90 0 90)
			)
		)
	)
	(gr_text "THIS SIDE\nFACE UP\n<-USB"
		(at 150.495 96.52 0)
		(layer "F.SilkS")
	)
	(gr_text "GND"
		(at 133.35 86.995 0)
		(layer "F.SilkS")
	)
	(gr_text "github.com/bkw777/\nATF150x_uPRG"
		(at 152.4 88.265 0)
		(layer "F.SilkS")
	)
	(gr_text "3V3"
		(at 133.477 104.013 90)
		(layer "F.SilkS")
	)
	(gr_text "5V"
		(at 135.89 104.013 90)
		(layer "F.SilkS")
	)
	(gr_text "GND"
		(at 138.43 104.013 90)
		(layer "F.SilkS")
	)
	(gr_text "TCK"
		(at 140.97 104.013 90)
		(layer "F.SilkS")
	)
	(gr_text "TDI"
		(at 143.51 104.013 90)
		(layer "F.SilkS")
	)
	(gr_text "TDO"
		(at 146.05 104.013 90)
		(layer "F.SilkS")
	)
	(gr_text "TMS"
		(at 148.59 104.013 90)
		(layer "F.SilkS")
	)
	(gr_text "TCK"
		(at 160.909 90.17 0)
		(layer "F.SilkS")
	)
	(gr_text "TDO"
		(at 160.909 92.71 0)
		(layer "F.SilkS")
	)
	(gr_text "TMS"
		(at 160.909 95.25 0)
		(layer "F.SilkS")
	)
	(gr_text "TDI"
		(at 160.909 100.33 0)
		(layer "F.SilkS")
	)
	(gr_text "USBC"
		(at 128.016 95.25 90)
		(layer "F.SilkS")
	)
	(gr_text "v${REVISION}"
		(at 160.655 102.743 0)
		(layer "B.SilkS")
	)
	(gr_text "3V3"
		(at 133.35 104.394 270)
		(layer "B.SilkS")
	)
	(gr_text "5V"
		(at 135.89 104.394 270)
		(layer "B.SilkS")
	)
	(gr_text "GND"
		(at 138.43 104.394 270)
		(layer "B.SilkS")
	)
	(gr_text "TCK"
		(at 140.97 104.394 270)
		(layer "B.SilkS")
	)
	(gr_text "TDI"
		(at 143.51 104.394 270)
		(layer "B.SilkS")
	)
	(gr_text "TDO"
		(at 146.05 104.394 270)
		(layer "B.SilkS")
	)
	(gr_text "TMS"
		(at 148.336 104.394 270)
		(layer "B.SilkS")
	)
	(gr_text "GND"
		(at 132.334 85.725 270)
		(layer "B.SilkS")
	)
	(gr_text "12V"
		(at 147.701 100.711 -90)
		(layer "B.SilkS")
	)
	(gr_text "GND"
		(at 160.909 90.17 0)
		(layer "B.SilkS")
	)
	(gr_text "VCC"
		(at 160.909 92.71 0)
		(layer "B.SilkS")
	)
	(gr_text "VPP"
		(at 160.909 95.25 0)
		(layer "B.SilkS")
	)
	(gr_text "GND"
		(at 160.909 100.33 0)
		(layer "B.SilkS")
	)
	(gr_text "ATF150x_uPRG"
		(at 155.194 103.632 0)
		(layer "B.SilkS")
	)
	(gr_text "3V3"
		(at 134.62 90.805 270)
		(layer "B.SilkS")
	)
	(gr_text "VCC"
		(at 137.16 90.805 270)
		(layer "B.SilkS")
	)
	(gr_text "5V"
		(at 139.7 90.805 270)
		(layer "B.SilkS")
	)
	(gr_text "N/C"
		(at 142.24 90.805 270)
		(layer "B.SilkS")
	)
	(gr_text "12V"
		(at 149.86 90.805 270)
		(layer "B.SilkS")
	)
	(gr_text "VPP"
		(at 152.4 90.805 270)
		(layer "B.SilkS")
	)
	(gr_text "N/C"
		(at 154.94 90.805 270)
		(layer "B.SilkS")
	)
	(gr_text "BKW JTAG-A+VPP"
		(at 145.415 93.98 270)
		(layer "B.SilkS")
	)
	(zone
		(net 33)
		(net_name "Net-(C6-Pad1)")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30014)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 133.549461 88.567423) (xy 133.390255 88.509608) (xy 133.254098 88.463675) (xy 133.125367 88.406807)
				(xy 133.071595 88.372617) (xy 133.029049 88.333707) (xy 133.000852 88.289414) (xy 132.990129 88.239077)
				(xy 132.271131 88.498104) (xy 132.208551 88.948603) (xy 132.378746 88.899568) (xy 132.560959 88.885791)
				(xy 132.75788 88.907657) (xy 132.971175 88.966783) (xy 133.199588 89.062746) (xy 133.249462 89.087038)
			)
		)
	)
	(zone
		(net 9)
		(net_name "+5V")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30016)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 140 98.457) (xy 139.993465 98.349555) (xy 139.984542 98.208783) (xy 139.992164 98.064592) (xy 140.008103 97.999196)
				(xy 140.035288 97.942521) (xy 140.076088 97.897759) (xy 140.132873 97.868104) (xy 139.7 97.281)
				(xy 139.267127 97.868104) (xy 139.30646 97.885787) (xy 139.338502 97.910503) (xy 139.385208 97.981557)
				(xy 139.411236 98.089285) (xy 139.413942 98.247175) (xy 139.406535 98.349554) (xy 139.4 98.457)
			)
		)
	)
	(zone
		(net 9)
		(net_name "+5V")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30021)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 139.4 96.107) (xy 139.406535 96.214446) (xy 139.415459 96.355218) (xy 139.407837 96.499408)
				(xy 139.391897 96.564805) (xy 139.364712 96.621479) (xy 139.323912 96.666241) (xy 139.267127 96.695896)
				(xy 139.7 97.283) (xy 140.132873 96.695896) (xy 140.09354 96.678213) (xy 140.061499 96.653497) (xy 140.014793 96.582443)
				(xy 139.988764 96.474715) (xy 139.986058 96.316824) (xy 139.993465 96.214445) (xy 140 96.107)
			)
		)
	)
	(zone
		(net 2)
		(net_name "TDI")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30037)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 158.895196 100.992) (xy 158.815664 100.987332) (xy 158.755069 100.974658) (xy 158.652813 100.926439)
				(xy 158.571184 100.883714) (xy 158.448773 100.846804) (xy 158.399 101.092) (xy 158.448773 101.337196)
				(xy 158.585415 101.293905) (xy 158.652813 101.257561) (xy 158.747709 101.211647) (xy 158.810872 101.197319)
				(xy 158.895196 101.192)
			)
		)
	)
	(zone
		(net 4)
		(net_name "TMS")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30003)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 160.432906 94.588) (xy 160.559847 94.607388) (xy 160.709763 94.671096) (xy 160.871722 94.78405)
				(xy 160.951185 94.857957) (xy 161.025931 94.941516) (xy 161.092762 95.031572) (xy 161.151996 95.129225)
				(xy 161.199469 95.227449) (xy 161.237562 95.331051) (xy 161.263428 95.431561) (xy 161.279061 95.535613)
				(xy 161.28 95.710769) (xy 163.186 95.25) (xy 161.75625 94.2975) (xy 161.651147 94.330603) (xy 161.416504 94.362262)
				(xy 160.990319 94.383534) (xy 160.478206 94.388018) (xy 160.432906 94.388)
			)
		)
	)
	(zone
		(net 28)
		(net_name "Net-(LED1-A)")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30028)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 129.937272 95.074404) (xy 130.023122 95.188845) (xy 130.09837 95.356407) (xy 130.153545 95.577966)
				(xy 130.177432 95.841759) (xy 130.172 96.025912) (xy 130.622587 95.885808) (xy 130.666353 95.16)
				(xy 130.536192 95.163384) (xy 130.388879 95.13029) (xy 130.234263 95.058997) (xy 130.161456 95.010616)
				(xy 130.103616 94.961376) (xy 130.09907 94.956844)
			)
		)
	)
	(zone
		(net 1)
		(net_name "TCK")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30007)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 142.09079 104.417788) (xy 141.990975 104.510668) (xy 141.899365 104.582017) (xy 141.820603 104.631056)
				(xy 141.745584 104.666391) (xy 141.599942 104.704742) (xy 141.423863 104.714158) (xy 141.351316 104.713222)
				(xy 141.114706 104.715436) (xy 140.973945 104.727667) (xy 140.813928 104.753372) (xy 140.969293 105.538707)
				(xy 141.635176 105.982456) (xy 141.70524 105.869028) (xy 141.759562 105.763735) (xy 141.832902 105.565018)
				(xy 141.873406 105.361328) (xy 141.88352 105.284109) (xy 141.908673 105.116734) (xy 141.958214 104.947143)
				(xy 142.000079 104.858227) (xy 142.057581 104.76481) (xy 142.133898 104.665576) (xy 142.232212 104.55921)
			)
		)
	)
	(zone
		(net 9)
		(net_name "+5V")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30022)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 139.4 98.266) (xy 139.406535 98.373446) (xy 139.415459 98.514218) (xy 139.407837 98.658408)
				(xy 139.391897 98.723805) (xy 139.364712 98.780479) (xy 139.323912 98.825241) (xy 139.267127 98.854896)
				(xy 139.7 99.442) (xy 140.132873 98.854896) (xy 140.09354 98.837213) (xy 140.061499 98.812497) (xy 140.014793 98.741443)
				(xy 139.988764 98.633715) (xy 139.986058 98.475824) (xy 139.993465 98.373445) (xy 140 98.266)
			)
		)
	)
	(zone
		(net 1)
		(net_name "TCK")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30000)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 160.3275 90.27) (xy 160.497392 90.289344) (xy 160.723335 90.355972) (xy 160.850533 90.409171)
				(xy 160.977807 90.473413) (xy 161.099267 90.546108) (xy 161.214493 90.627643) (xy 161.311481 90.708958)
				(xy 161.398329 90.796253) (xy 161.464619 90.877674) (xy 161.519562 90.962789) (xy 161.573997 91.086248)
				(xy 163.186 90.17) (xy 161.573997 89.253752) (xy 161.508072 89.396995) (xy 161.39718 89.545023)
				(xy 161.236618 89.694984) (xy 161.026893 89.838652) (xy 160.781605 89.960994) (xy 160.655468 90.007966)
				(xy 160.534569 90.042404) (xy 160.427746 90.062651) (xy 160.331527 90.069986) (xy 160.3275 90.07)
			)
		)
	)
	(zone
		(net 9)
		(net_name "+5V")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30004)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 139.4 100.269372) (xy 139.395183 100.416808) (xy 139.381465 100.543337) (xy 139.360366 100.65064)
				(xy 139.332769 100.74422) (xy 139.256054 100.914512) (xy 139.180851 101.041488) (xy 139.108574 101.162556)
				(xy 139.03725 101.303132) (xy 138.971358 101.476996) (xy 138.915372 101.697928) (xy 139.7 101.855)
				(xy 140.484628 101.697928) (xy 140.4513 101.554563) (xy 140.413505 101.43133) (xy 140.32257 101.219993)
				(xy 140.219149 101.041489) (xy 140.135695 100.899257) (xy 140.06583 100.74016) (xy 140.038582 100.646318)
				(xy 140.017838 100.538697) (xy 140.004632 100.414111) (xy 140 100.269372)
			)
		)
	)
	(zone
		(net 22)
		(net_name "+12V")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30017)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 145.637 91.968598) (xy 145.744445 91.962063) (xy 145.885217 91.95314) (xy 146.029408 91.960762)
				(xy 146.094804 91.976701) (xy 146.151479 92.003886) (xy 146.196241 92.044686) (xy 146.225896 92.101471)
				(xy 146.813 91.668598) (xy 146.225896 91.235725) (xy 146.208213 91.275058) (xy 146.183497 91.3071)
				(xy 146.112443 91.353806) (xy 146.004715 91.379834) (xy 145.846825 91.38254) (xy 145.744446 91.375133)
				(xy 145.637 91.368598)
			)
		)
	)
	(zone
		(net 31)
		(net_name "VCC")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30032)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 133.422 95.404) (xy 133.310895 95.398365) (xy 133.172652 95.378916) (xy 133.070911 95.353259)
				(xy 132.984371 95.316303) (xy 132.943436 95.286505) (xy 132.91687 95.251207) (xy 132.910097 95.231885)
				(xy 132.521 95.885) (xy 132.972 96.182867) (xy 132.990616 96.02992) (xy 133.04519 95.887069) (xy 133.132619 95.761225)
				(xy 133.244242 95.664703) (xy 133.303203 95.632337) (xy 133.361463 95.611868) (xy 133.422 95.604)
			)
		)
	)
	(zone
		(net 22)
		(net_name "+12V")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30020)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 143.289998 91.968599) (xy 143.397444 91.962064) (xy 143.538216 91.95314) (xy 143.682406 91.960762)
				(xy 143.747803 91.976702) (xy 143.804477 92.003886) (xy 143.849239 92.044686) (xy 143.878894 92.101471)
				(xy 144.465998 91.668598) (xy 143.878894 91.235725) (xy 143.861211 91.275058) (xy 143.836495 91.3071)
				(xy 143.765441 91.353806) (xy 143.657713 91.379834) (xy 143.499823 91.382541) (xy 143.397443 91.375134)
				(xy 143.289998 91.368599)
			)
		)
	)
	(zone
		(net 3)
		(net_name "TDO")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30009)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 146.585 104.216397) (xy 146.580097 104.311219) (xy 146.565777 104.390381) (xy 146.545056 104.450245)
				(xy 146.517461 104.499858) (xy 146.44498 104.572402) (xy 146.339741 104.624281) (xy 146.139063 104.67491)
				(xy 146.014657 104.702441) (xy 145.882573 104.739611) (xy 145.745355 104.79391) (xy 145.605544 104.872824)
				(xy 146.05 105.539) (xy 146.834628 105.381928) (xy 146.792638 105.145539) (xy 146.772086 104.967697)
				(xy 146.769698 104.71384) (xy 146.773722 104.627267) (xy 146.785 104.216397)
			)
		)
	)
	(zone
		(net 30)
		(net_name "Net-(LED3-A)")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30038)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 130.289196 100.103) (xy 130.209664 100.098332) (xy 130.149069 100.085658) (xy 130.046813 100.037439)
				(xy 129.965184 99.994714) (xy 129.842773 99.957804) (xy 129.793 100.203) (xy 129.842773 100.448196)
				(xy 129.979415 100.404905) (xy 130.046813 100.368561) (xy 130.141709 100.322647) (xy 130.204872 100.308319)
				(xy 130.289196 100.303)
			)
		)
	)
	(zone
		(net 31)
		(net_name "VCC")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30005)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 136.860001 100.269372) (xy 136.855184 100.416808) (xy 136.841466 100.543337) (xy 136.820367 100.65064)
				(xy 136.79277 100.74422) (xy 136.716055 100.914512) (xy 136.640852 101.041488) (xy 136.568575 101.162556)
				(xy 136.497251 101.303132) (xy 136.431359 101.476996) (xy 136.375373 101.697928) (xy 137.160001 101.855)
				(xy 137.944629 101.697928) (xy 137.911301 101.554563) (xy 137.873506 101.43133) (xy 137.782571 101.219993)
				(xy 137.67915 101.041489) (xy 137.595696 100.899257) (xy 137.525831 100.74016) (xy 137.498583 100.646318)
				(xy 137.477839 100.538697) (xy 137.464633 100.414111) (xy 137.460001 100.269372)
			)
		)
	)
	(zone
		(net 30)
		(net_name "Net-(LED3-A)")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30031)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 129.794 100.303) (xy 129.881226 100.322339) (xy 129.96994 100.383108) (xy 130.055003 100.491057)
				(xy 130.124777 100.646776) (xy 130.149535 100.73982) (xy 130.165614 100.840796) (xy 130.172001 100.962402)
				(xy 130.623001 100.711) (xy 130.324632 100.000394) (xy 130.270745 100.042055) (xy 130.162234 100.076752)
				(xy 129.97944 100.098647) (xy 129.794 100.103)
			)
		)
	)
	(zone
		(net 34)
		(net_name "VPP")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30006)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 152.1 100.269372) (xy 152.095183 100.416808) (xy 152.081465 100.543337) (xy 152.060366 100.65064)
				(xy 152.032769 100.74422) (xy 151.956054 100.914512) (xy 151.880851 101.041488) (xy 151.808574 101.162556)
				(xy 151.73725 101.303132) (xy 151.671358 101.476996) (xy 151.615372 101.697928) (xy 152.4 101.855)
				(xy 153.184628 101.697928) (xy 153.1513 101.554563) (xy 153.113505 101.43133) (xy 153.02257 101.219993)
				(xy 152.919149 101.041489) (xy 152.835695 100.899257) (xy 152.76583 100.74016) (xy 152.738582 100.646318)
				(xy 152.717838 100.538697) (xy 152.704632 100.414111) (xy 152.7 100.269372)
			)
		)
	)
	(zone
		(net 22)
		(net_name "+12V")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30023)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 145.639998 91.368598) (xy 145.532552 91.375133) (xy 145.39178 91.384057) (xy 145.24759 91.376435)
				(xy 145.182193 91.360495) (xy 145.125519 91.33331) (xy 145.080757 91.29251) (xy 145.051102 91.235725)
				(xy 144.463998 91.668598) (xy 145.051102 92.101471) (xy 145.068785 92.062138) (xy 145.093501 92.030097)
				(xy 145.164555 91.983391) (xy 145.272283 91.957362) (xy 145.430174 91.954656) (xy 145.532553 91.962063)
				(xy 145.639998 91.968598)
			)
		)
	)
	(zone
		(net 2)
		(net_name "TDI")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30002)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 160.432906 101.192) (xy 160.478206 101.191982) (xy 160.802488 101.19322) (xy 161.183609 101.20298)
				(xy 161.53154 101.229871) (xy 161.664924 101.25243) (xy 161.75625 101.2825) (xy 163.186 100.33)
				(xy 161.28 99.86923) (xy 161.277397 100.060303) (xy 161.236775 100.25147) (xy 161.157948 100.439667)
				(xy 161.042093 100.618231) (xy 160.894817 100.775863) (xy 160.813037 100.842322) (xy 160.729366 100.897683)
				(xy 160.647144 100.940339) (xy 160.566233 100.97073) (xy 160.432906 100.992)
			)
		)
	)
	(zone
		(net 34)
		(net_name "VPP")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30035)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 134.251804 97.89) (xy 134.331336 97.894668) (xy 134.391931 97.907342) (xy 134.494187 97.955561)
				(xy 134.575815 97.998285) (xy 134.698227 98.035196) (xy 134.748 97.79) (xy 134.698227 97.544804)
				(xy 134.561585 97.588094) (xy 134.494186 97.624439) (xy 134.39929 97.670353) (xy 134.336128 97.684681)
				(xy 134.251804 97.69)
			)
		)
	)
	(zone
		(net 2)
		(net_name "TDI")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30034)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 145.008554 103.925867) (xy 145.068092 103.87293) (xy 145.119901 103.839045) (xy 145.226304 103.800835)
				(xy 145.314235 103.773326) (xy 145.426893 103.712867) (xy 145.288707 103.504293) (xy 145.080133 103.366107)
				(xy 145.014123 103.493338) (xy 144.992164 103.566697) (xy 144.957529 103.666264) (xy 144.922998 103.721059)
				(xy 144.867133 103.784446)
			)
		)
	)
	(zone
		(net 9)
		(net_name "+5V")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30033)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 134.274439 99.699988) (xy 134.344692 99.690852) (xy 134.399737 99.693385) (xy 134.481981 99.722165)
				(xy 134.514378 99.740397) (xy 134.58975 99.779824) (xy 134.698227 99.813196) (xy 134.74798 99.567805)
				(xy 134.698227 99.322804) (xy 134.611142 99.344754) (xy 134.546306 99.369657) (xy 134.466821 99.413318)
				(xy 134.376273 99.461912) (xy 134.235419 99.503832)
			)
		)
	)
	(zone
		(net 9)
		(net_name "+5V")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30018)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 140 96.298) (xy 139.993465 96.190555) (xy 139.984542 96.049783) (xy 139.992164 95.905592) (xy 140.008103 95.840196)
				(xy 140.035288 95.783521) (xy 140.076088 95.738759) (xy 140.132873 95.709104) (xy 139.7 95.122)
				(xy 139.267127 95.709104) (xy 139.30646 95.726787) (xy 139.338502 95.751503) (xy 139.385208 95.822557)
				(xy 139.411236 95.930285) (xy 139.413942 96.088175) (xy 139.406535 96.190554) (xy 139.4 96.298)
			)
		)
	)
	(zone
		(net 22)
		(net_name "+12V")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30012)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 141.002998 92.121) (xy 141.219075 92.105177) (xy 141.330136 92.091693) (xy 141.54882 92.066598)
				(xy 141.775891 92.053227) (xy 141.99956 92.065816) (xy 142.106433 92.086293) (xy 142.208033 92.118599)
				(xy 142.178998 91.668599) (xy 141.507282 91.301885) (xy 141.497205 91.35197) (xy 141.47904 91.393979)
				(xy 141.42187 91.45712) (xy 141.333957 91.499207) (xy 141.207103 91.520768) (xy 141.053456 91.521973)
				(xy 141.002998 91.521)
			)
		)
	)
	(zone
		(net 34)
		(net_name "VPP")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30030)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 133.420409 97.69) (xy 133.403274 97.690012) (xy 133.258989 97.688709) (xy 133.088536 97.678767)
				(xy 132.935905 97.651478) (xy 132.88002 97.628607) (xy 132.845086 97.598133) (xy 132.521 98.298)
				(xy 132.972 98.560086) (xy 132.99033 98.379652) (xy 133.044539 98.212023) (xy 133.129984 98.06772)
				(xy 133.181441 98.008668) (xy 133.23641 97.960527) (xy 133.291608 97.925168) (xy 133.347528 97.901629)
				(xy 133.420409 97.89)
			)
		)
	)
	(zone
		(net 2)
		(net_name "TDI")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30008)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 144.55929 104.092288) (xy 144.446344 104.198231) (xy 144.345059 104.278779) (xy 144.262335 104.331992)
				(xy 144.183714 104.37093) (xy 144.029508 104.41657) (xy 143.80339 104.441806) (xy 143.603562 104.460174)
				(xy 143.353928 104.499372) (xy 143.509293 105.284707) (xy 144.294628 105.440072) (xy 144.339574 105.136223)
				(xy 144.352052 104.989141) (xy 144.371312 104.79676) (xy 144.388774 104.709586) (xy 144.416334 104.624083)
				(xy 144.457651 104.536999) (xy 144.516381 104.445078) (xy 144.596182 104.345066) (xy 144.700712 104.23371)
			)
		)
	)
	(zone
		(net 29)
		(net_name "Net-(LED2-A)")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30040)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 129.865749 97.472167) (xy 129.80067 97.433599) (xy 129.757278 97.3961) (xy 129.710473 97.321553)
				(xy 129.697302 97.290532) (xy 129.667998 97.224483) (xy 129.620867 97.143107) (xy 129.41211 97.281546)
				(xy 129.364227 97.527196) (xy 129.47656 97.547989) (xy 129.611107 97.57787) (xy 129.774942 97.650363)
			)
		)
	)
	(zone
		(net 28)
		(net_name "Net-(LED1-A)")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30039)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 129.8155 93.205196) (xy 129.820168 93.125664) (xy 129.832842 93.065069) (xy 129.881061 92.962813)
				(xy 129.923785 92.881184) (xy 129.960696 92.758773) (xy 129.7155 92.709) (xy 129.470304 92.758773)
				(xy 129.513594 92.895415) (xy 129.549939 92.962813) (xy 129.595853 93.057709) (xy 129.610181 93.120872)
				(xy 129.6155 93.205196)
			)
		)
	)
	(zone
		(net 6)
		(net_name "Net-(C7-Pad2)")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30015)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 133.249456 93.28498) (xy 132.999758 93.394888) (xy 132.849664 93.443024) (xy 132.687727 93.476081)
				(xy 132.578355 93.485721) (xy 132.466601 93.483592) (xy 132.370231 93.470878) (xy 132.273494 93.446731)
				(xy 132.208556 93.4234) (xy 132.271131 93.8739) (xy 132.990128 94.132932) (xy 133.009935 94.064653)
				(xy 133.068046 94.002088) (xy 133.177841 93.93924) (xy 133.390247 93.86241) (xy 133.549461 93.804592)
			)
		)
	)
	(zone
		(net 22)
		(net_name "+12V")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30024)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 143.352998 91.368599) (xy 143.245552 91.375134) (xy 143.10478 91.384058) (xy 142.96059 91.376436)
				(xy 142.895193 91.360496) (xy 142.838519 91.333311) (xy 142.793757 91.292511) (xy 142.764102 91.235726)
				(xy 142.176998 91.668599) (xy 142.764102 92.101472) (xy 142.781785 92.062139) (xy 142.806501 92.030098)
				(xy 142.877555 91.983392) (xy 142.985283 91.957363) (xy 143.143174 91.954657) (xy 143.245553 91.962064)
				(xy 143.352998 91.968599)
			)
		)
	)
	(zone
		(net 31)
		(net_name "VCC")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30036)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 134.251804 95.604) (xy 134.331336 95.608668) (xy 134.391931 95.621342) (xy 134.494187 95.669561)
				(xy 134.575815 95.712285) (xy 134.698227 95.749196) (xy 134.748 95.504) (xy 134.698227 95.258804)
				(xy 134.561585 95.302094) (xy 134.494186 95.338439) (xy 134.39929 95.384353) (xy 134.336128 95.398681)
				(xy 134.251804 95.404)
			)
		)
	)
	(zone
		(net 29)
		(net_name "Net-(LED2-A)")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30027)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 129.742125 97.63364) (xy 129.843161 97.682493) (xy 129.947692 97.777719) (xy 130.046397 97.922537)
				(xy 130.089135 98.012173) (xy 130.124348 98.109623) (xy 130.150755 98.212709) (xy 130.16757 98.320834)
				(xy 130.172 98.497692) (xy 130.62289 98.298454) (xy 130.490714 97.573) (xy 130.403996 97.583821)
				(xy 130.245119 97.564849) (xy 129.99139 97.501744) (xy 129.900816 97.47528) (xy 129.832931 97.455443)
			)
		)
	)
	(zone
		(net 9)
		(net_name "+5V")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30019)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 140 100.616) (xy 139.993465 100.508555) (xy 139.984542 100.367783) (xy 139.992164 100.223592)
				(xy 140.008103 100.158196) (xy 140.035288 100.101521) (xy 140.076088 100.056759) (xy 140.132873 100.027104)
				(xy 139.7 99.44) (xy 139.267127 100.027104) (xy 139.30646 100.044787) (xy 139.338502 100.069503)
				(xy 139.385208 100.140557) (xy 139.411236 100.248285) (xy 139.413942 100.406175) (xy 139.406535 100.508554)
				(xy 139.4 100.616)
			)
		)
	)
	(zone
		(net 3)
		(net_name "TDO")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30001)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 160.3275 92.81) (xy 160.497392 92.829344) (xy 160.723335 92.895972) (xy 160.850533 92.949171)
				(xy 160.977807 93.013413) (xy 161.099267 93.086108) (xy 161.214493 93.167643) (xy 161.311481 93.248958)
				(xy 161.398329 93.336253) (xy 161.464619 93.417674) (xy 161.519562 93.502789) (xy 161.573997 93.626248)
				(xy 163.186 92.71) (xy 161.573997 91.793752) (xy 161.508072 91.936995) (xy 161.39718 92.085023)
				(xy 161.236618 92.234984) (xy 161.026893 92.378652) (xy 160.781605 92.500994) (xy 160.655468 92.547966)
				(xy 160.534569 92.582404) (xy 160.427746 92.602651) (xy 160.331527 92.609986) (xy 160.3275 92.61)
			)
		)
	)
	(zone
		(net 9)
		(net_name "+5V")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30025)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 139.4 93.948) (xy 139.406535 94.055446) (xy 139.415459 94.196218) (xy 139.407837 94.340408)
				(xy 139.391897 94.405805) (xy 139.364712 94.462479) (xy 139.323912 94.507241) (xy 139.267127 94.536896)
				(xy 139.7 95.124) (xy 140.132873 94.536896) (xy 140.09354 94.519213) (xy 140.061499 94.494497) (xy 140.014793 94.423443)
				(xy 139.988764 94.315715) (xy 139.986058 94.157824) (xy 139.993465 94.055445) (xy 140 93.948)
			)
		)
	)
	(zone
		(net 32)
		(net_name "Net-(C6-Pad2)")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30011)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 133.446997 90.251001) (xy 133.396539 90.251974) (xy 133.263167 90.251971) (xy 133.120164 90.230439)
				(xy 133.055788 90.204498) (xy 133.001891 90.164653) (xy 132.962767 90.108063) (xy 132.942712 90.031887)
				(xy 132.270998 90.398601) (xy 132.241963 90.848601) (xy 132.409916 90.802209) (xy 132.618134 90.783372)
				(xy 132.882272 90.794828) (xy 133.119861 90.821693) (xy 133.295113 90.842082) (xy 133.446996 90.851)
			)
		)
	)
	(zone
		(net 5)
		(net_name "Net-(C7-Pad1)")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30013)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 133.446997 91.521) (xy 133.230921 91.536823) (xy 133.119858 91.550307) (xy 132.901175 91.575402)
				(xy 132.674104 91.588773) (xy 132.450436 91.576185) (xy 132.343563 91.555708) (xy 132.241963 91.523402)
				(xy 132.270998 91.973402) (xy 132.942713 92.340114) (xy 132.95279 92.290029) (xy 132.970955 92.24802)
				(xy 133.028125 92.184879) (xy 133.116038 92.142792) (xy 133.242892 92.121232) (xy 133.396539 92.120026)
				(xy 133.446996 92.120999)
			)
		)
	)
	(zone
		(net 4)
		(net_name "TMS")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30010)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 147.855 103.962397) (xy 147.866277 104.373266) (xy 147.872615 104.53381) (xy 147.869551 104.68978)
				(xy 147.849625 104.876158) (xy 147.805372 105.127928) (xy 148.59 105.285) (xy 149.034456 104.618824)
				(xy 148.863487 104.525827) (xy 148.671236 104.460079) (xy 148.500936 104.42091) (xy 148.322087 104.377556)
				(xy 148.246118 104.348031) (xy 148.180926 104.307955) (xy 148.127865 104.253342) (xy 148.088287 104.180203)
				(xy 148.063547 104.08455) (xy 148.055 103.962397)
			)
		)
	)
	(zone
		(net 9)
		(net_name "+5V")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30029)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 133.346552 100.029515) (xy 133.203929 100.050963) (xy 133.028123 100.060507) (xy 132.92889 100.053684)
				(xy 132.843526 100.033479) (xy 132.776937 99.991955) (xy 132.521076 100.711382) (xy 132.971999 100.94845)
				(xy 132.990369 100.767944) (xy 133.045918 100.591487) (xy 133.135249 100.431815) (xy 133.189608 100.363859)
				(xy 133.247933 100.306755) (xy 133.306458 100.263176) (xy 133.366019 100.231851) (xy 133.423096 100.214287)
			)
		)
	)
	(zone
		(net 27)
		(net_name "Net-(JP2-Pad3)")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30026)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 147.112 94.468596) (xy 147.107182 94.390452) (xy 147.100085 94.270963) (xy 147.110294 94.149958)
				(xy 147.128089 94.097887) (xy 147.157652 94.056236) (xy 147.201462 94.028606) (xy 147.262 94.018596)
				(xy 146.812 93.567596) (xy 146.362 94.018596) (xy 146.405475 94.023402) (xy 146.440701 94.037043)
				(xy 146.489013 94.085164) (xy 146.516896 94.165792) (xy 146.523401 94.291665) (xy 146.516818 94.390452)
				(xy 146.512 94.468596)
			)
		)
	)
	(zone
		(net 10)
		(net_name "GND")
		(layers "F.Cu" "B.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0.2032)
		)
		(min_thickness 0.2032)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.2032)
			(thermal_bridge_width 0.4064)
			(smoothing fillet)
			(radius 0.1016)
		)
		(polygon
			(pts
				(xy 165.1 106.68) (xy 127 106.68) (xy 127 83.82) (xy 165.1 83.82)
			)
		)
	)
	(zone
		(net 24)
		(net_name "+3V3")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30004)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 133.802366 103.121411) (xy 133.857319 103.024301) (xy 133.913365 102.945396) (xy 133.967694 102.885529)
				(xy 134.023345 102.838433) (xy 134.14068 102.775014) (xy 134.282443 102.739412) (xy 134.42387 102.723106)
				(xy 134.565949 102.70726) (xy 134.719227 102.676979) (xy 134.884973 102.618779) (xy 135.064456 102.519176)
				(xy 134.620454 101.85311) (xy 133.954824 101.409544) (xy 133.826383 101.610334) (xy 133.730994 101.777046)
				(xy 133.606724 102.044893) (xy 133.545303 102.207589) (xy 133.440743 102.478147) (xy 133.26777 102.849003)
			)
		)
	)
	(zone
		(net 28)
		(net_name "Net-(LED1-A)")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30007)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 129.8155 92.6275) (xy 129.835119 92.481032) (xy 129.863207 92.384663) (xy 129.903046 92.286321)
				(xy 129.949346 92.199902) (xy 130.00478 92.121477) (xy 130.056949 92.06625) (xy 130.114895 92.022084)
				(xy 130.184446 91.989529) (xy 129.7155 91.439) (xy 129.246554 91.989529) (xy 129.341826 92.039636)
				(xy 129.433922 92.131046) (xy 129.519328 92.268392) (xy 129.586404 92.444258) (xy 129.607061 92.536247)
				(xy 129.615349 92.616594) (xy 129.6155 92.6275)
			)
		)
	)
	(zone
		(net 2)
		(net_name "TDI")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30011)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 158.120554 101.512867) (xy 158.180092 101.45993) (xy 158.231901 101.426045) (xy 158.338304 101.387835)
				(xy 158.426235 101.360326) (xy 158.538893 101.299867) (xy 158.400707 101.091293) (xy 158.192133 100.953107)
				(xy 158.126123 101.080338) (xy 158.104164 101.153697) (xy 158.069529 101.253264) (xy 158.034998 101.308059)
				(xy 157.979133 101.371446)
			)
		)
	)
	(zone
		(net 30)
		(net_name "Net-(LED3-A)")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30009)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 129.894 100.203) (xy 129.914088 100.041048) (xy 129.942003 99.938242) (xy 129.981996 99.835731)
				(xy 130.024191 99.757212) (xy 130.074732 99.689269) (xy 130.119972 99.646639) (xy 130.17034 99.615523)
				(xy 130.184446 99.609529) (xy 129.7155 99.059) (xy 129.299393 99.688607) (xy 129.404429 99.722499)
				(xy 129.503227 99.793658) (xy 129.592913 99.903799) (xy 129.662621 100.046222) (xy 129.684256 100.121286)
				(xy 129.69363 100.188536) (xy 129.694 100.203)
			)
		)
	)
	(zone
		(net 24)
		(net_name "+3V3")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30002)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 133.05 103.699372) (xy 133.045183 103.846808) (xy 133.031465 103.973337) (xy 133.010366 104.08064)
				(xy 132.982769 104.17422) (xy 132.906054 104.344512) (xy 132.830851 104.471488) (xy 132.758574 104.592556)
				(xy 132.68725 104.733132) (xy 132.621358 104.906996) (xy 132.565372 105.127928) (xy 133.35 105.285)
				(xy 134.134628 105.127928) (xy 134.1013 104.984563) (xy 134.063505 104.86133) (xy 133.97257 104.649993)
				(xy 133.869149 104.471489) (xy 133.785695 104.329257) (xy 133.71583 104.17016) (xy 133.688582 104.076318)
				(xy 133.667838 103.968697) (xy 133.654632 103.844111) (xy 133.65 103.699372)
			)
		)
	)
	(zone
		(net 9)
		(net_name "+5V")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30006)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 138.855829 103.122387) (xy 138.959089 103.028872) (xy 139.054243 102.955573) (xy 139.141707 102.90005)
				(xy 139.224227 102.858282) (xy 139.393696 102.800748) (xy 139.519293 102.77283) (xy 139.650927 102.743646)
				(xy 139.794694 102.7003) (xy 139.957051 102.629806) (xy 140.144456 102.519176) (xy 139.700717 101.853304)
				(xy 139.034824 101.409544) (xy 138.964203 101.523747) (xy 138.909894 101.628608) (xy 138.835742 101.826623)
				(xy 138.789709 102.032572) (xy 138.757372 102.184827) (xy 138.703479 102.338488) (xy 138.661178 102.419111)
				(xy 138.604763 102.504005) (xy 138.531325 102.594474) (xy 138.437957 102.691827)
			)
		)
	)
	(zone
		(net 31)
		(net_name "VCC")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30016)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 136.664805 95.604) (xy 136.744337 95.608668) (xy 136.804932 95.621342) (xy 136.907188 95.669561)
				(xy 136.988816 95.712285) (xy 137.111228 95.749196) (xy 137.161001 95.504) (xy 137.111228 95.258804)
				(xy 136.974586 95.302094) (xy 136.907187 95.338439) (xy 136.812291 95.384353) (xy 136.749129 95.398681)
				(xy 136.664805 95.404)
			)
		)
	)
	(zone
		(net 31)
		(net_name "VCC")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30001)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 160.359077 92.375) (xy 160.522104 92.395023) (xy 160.62032 92.42249) (xy 160.721864 92.461663)
				(xy 160.820814 92.510933) (xy 160.917318 92.571285) (xy 161.000681 92.635845) (xy 161.077668 92.709611)
				(xy 161.139501 92.783498) (xy 161.19307 92.864792) (xy 161.233263 92.944946) (xy 161.26432 93.031211)
				(xy 161.284036 93.116963) (xy 161.293987 93.208018) (xy 161.294959 93.261457) (xy 163.186 92.71)
				(xy 161.75625 91.7575) (xy 161.66662 91.79836) (xy 161.509515 91.82582) (xy 161.253121 91.831887)
				(xy 160.75503 91.799727) (xy 160.359077 91.775)
			)
		)
	)
	(zone
		(net 9)
		(net_name "+5V")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30005)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 136.325181 103.975555) (xy 136.018123 104.26067) (xy 135.85054 104.399164) (xy 135.703814 104.520883)
				(xy 135.562508 104.655823) (xy 135.408789 104.836028) (xy 135.224824 105.093544) (xy 135.889293 105.538707)
				(xy 136.674628 105.694072) (xy 136.695411 105.497208) (xy 136.679851 105.312908) (xy 136.631302 105.120475)
				(xy 136.614321 105.066717) (xy 136.568079 104.90471) (xy 136.556008 104.826399) (xy 136.55608 104.747818)
				(xy 136.571878 104.667418) (xy 136.606983 104.583651) (xy 136.664978 104.494968) (xy 136.749445 104.399819)
			)
		)
	)
	(zone
		(net 31)
		(net_name "VCC")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30017)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 135.242196 95.404) (xy 135.162664 95.399332) (xy 135.102069 95.386658) (xy 134.999813 95.338439)
				(xy 134.918184 95.295714) (xy 134.795773 95.258804) (xy 134.746 95.504) (xy 134.795773 95.749196)
				(xy 134.932415 95.705905) (xy 134.999813 95.669561) (xy 135.094709 95.623647) (xy 135.157872 95.609319)
				(xy 135.242196 95.604)
			)
		)
	)
	(zone
		(net 2)
		(net_name "TDI")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30020)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 145.702425 103.6) (xy 145.651805 103.595159) (xy 145.615808 103.581273) (xy 145.575851 103.536893)
				(xy 145.552585 103.482606) (xy 145.529959 103.42745) (xy 145.495867 103.366107) (xy 145.287 103.505)
				(xy 145.239227 103.750196) (xy 145.289296 103.760203) (xy 145.482944 103.793638) (xy 145.702425 103.8)
			)
		)
	)
	(zone
		(net 27)
		(net_name "Net-(JP2-Pad3)")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30003)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 149.560001 100.269372) (xy 149.555184 100.416808) (xy 149.541466 100.543337) (xy 149.520367 100.65064)
				(xy 149.49277 100.74422) (xy 149.416055 100.914512) (xy 149.340852 101.041488) (xy 149.268575 101.162556)
				(xy 149.197251 101.303132) (xy 149.131359 101.476996) (xy 149.075373 101.697928) (xy 149.860001 101.855)
				(xy 150.644629 101.697928) (xy 150.611301 101.554563) (xy 150.573506 101.43133) (xy 150.482571 101.219993)
				(xy 150.37915 101.041489) (xy 150.295696 100.899257) (xy 150.225831 100.74016) (xy 150.198583 100.646318)
				(xy 150.177839 100.538697) (xy 150.164633 100.414111) (xy 150.160001 100.269372)
			)
		)
	)
	(zone
		(net 30)
		(net_name "Net-(LED3-A)")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30013)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 129.694 99.707804) (xy 129.689332 99.787336) (xy 129.676658 99.847931) (xy 129.628439 99.950186)
				(xy 129.585714 100.031815) (xy 129.548804 100.154227) (xy 129.794 100.204) (xy 130.039196 100.154227)
				(xy 129.995905 100.017584) (xy 129.959561 99.950187) (xy 129.913647 99.855291) (xy 129.899319 99.792128)
				(xy 129.894 99.707804)
			)
		)
	)
	(zone
		(net 34)
		(net_name "VPP")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30000)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 160.359077 96.185) (xy 160.75503 96.160273) (xy 161.049549 96.13756) (xy 161.33885 96.127111)
				(xy 161.470173 96.131133) (xy 161.586546 96.143799) (xy 161.683421 96.166968) (xy 161.75625 96.2025)
				(xy 163.186 95.25) (xy 161.294959 94.698542) (xy 161.278417 94.872627) (xy 161.225425 95.032649)
				(xy 161.136883 95.179989) (xy 161.012519 95.313826) (xy 160.853493 95.43012) (xy 160.667166 95.520806)
				(xy 160.474173 95.574499) (xy 160.359077 95.585)
			)
		)
	)
	(zone
		(net 9)
		(net_name "+5V")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30012)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 139.420554 98.769667) (xy 139.480092 98.71673) (xy 139.531901 98.682845) (xy 139.638304 98.644635)
				(xy 139.726235 98.617126) (xy 139.838893 98.556667) (xy 139.700707 98.348093) (xy 139.492133 98.209907)
				(xy 139.426123 98.337138) (xy 139.404164 98.410497) (xy 139.369529 98.510064) (xy 139.334998 98.564859)
				(xy 139.279133 98.628246)
			)
		)
	)
	(zone
		(net 34)
		(net_name "VPP")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30018)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 135.242196 97.69) (xy 135.162664 97.685332) (xy 135.102069 97.672658) (xy 134.999813 97.624439)
				(xy 134.918184 97.581714) (xy 134.795773 97.544804) (xy 134.746 97.79) (xy 134.795773 98.035196)
				(xy 134.932415 97.991905) (xy 134.999813 97.955561) (xy 135.094709 97.909647) (xy 135.157872 97.895319)
				(xy 135.242196 97.89)
			)
		)
	)
	(zone
		(net 29)
		(net_name "Net-(LED2-A)")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30014)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 129.313 96.786804) (xy 129.308332 96.866336) (xy 129.295658 96.926931) (xy 129.247439 97.029186)
				(xy 129.204714 97.110815) (xy 129.167804 97.233227) (xy 129.413 97.283) (xy 129.658196 97.233227)
				(xy 129.614905 97.096584) (xy 129.578561 97.029187) (xy 129.532647 96.934291) (xy 129.518319 96.871128)
				(xy 129.513 96.786804)
			)
		)
	)
	(zone
		(net 28)
		(net_name "Net-(LED1-A)")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30015)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 129.6155 92.214804) (xy 129.610832 92.294336) (xy 129.598158 92.354931) (xy 129.549939 92.457186)
				(xy 129.507214 92.538815) (xy 129.470304 92.661227) (xy 129.7155 92.711) (xy 129.960696 92.661227)
				(xy 129.917405 92.524584) (xy 129.881061 92.457187) (xy 129.835147 92.362291) (xy 129.820819 92.299128)
				(xy 129.8155 92.214804)
			)
		)
	)
	(zone
		(net 34)
		(net_name "VPP")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30010)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 151.979133 98.780554) (xy 152.032069 98.840092) (xy 152.065954 98.891901) (xy 152.104164 98.998303)
				(xy 152.131674 99.086234) (xy 152.192133 99.198893) (xy 152.400707 99.060707) (xy 152.538893 98.852133)
				(xy 152.411662 98.786123) (xy 152.338303 98.764164) (xy 152.238735 98.729529) (xy 152.183941 98.694998)
				(xy 152.120554 98.639133)
			)
		)
	)
	(zone
		(net 29)
		(net_name "Net-(LED2-A)")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30008)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 129.513 96.425814) (xy 129.532372 96.320707) (xy 129.597819 96.190887) (xy 129.647171 96.126754)
				(xy 129.706403 96.067502) (xy 129.76918 96.019522) (xy 129.839187 95.980147) (xy 129.907321 95.954006)
				(xy 129.980364 95.937941) (xy 130.042934 95.933354) (xy 129.7155 95.249) (xy 129.228 95.70625) (xy 129.264661 95.781662)
				(xy 129.295137 95.933828) (xy 129.311675 96.191083) (xy 129.313066 96.387567) (xy 129.313 96.425814)
			)
		)
	)
	(zone
		(net 9)
		(net_name "+5V")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30019)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 135.242196 99.468) (xy 135.162664 99.463332) (xy 135.102069 99.450658) (xy 134.999813 99.402439)
				(xy 134.918184 99.359714) (xy 134.795773 99.322804) (xy 134.746 99.568) (xy 134.795773 99.813196)
				(xy 134.932415 99.769905) (xy 134.999813 99.733561) (xy 135.094709 99.687647) (xy 135.157872 99.673319)
				(xy 135.242196 99.668)
			)
		)
	)
	(embedded_fonts no)
)
