(kicad_pcb
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(general
		(thickness 1.542542)
		(legacy_teardrops no)
	)
	(paper "User" 440 290)
	(layers
		(0 "F.Cu" signal)
		(4 "In1.Cu" signal)
		(6 "In2.Cu" signal)
		(2 "B.Cu" signal)
		(9 "F.Adhes" user "F.Adhesive")
		(11 "B.Adhes" user "B.Adhesive")
		(13 "F.Paste" user)
		(15 "B.Paste" user)
		(5 "F.SilkS" user "F.Silkscreen")
		(7 "B.SilkS" user "B.Silkscreen")
		(1 "F.Mask" user)
		(3 "B.Mask" user)
		(17 "Dwgs.User" user "User.Drawings")
		(19 "Cmts.User" user "User.Comments")
		(21 "Eco1.User" user "User.Eco1")
		(23 "Eco2.User" user "User.Eco2")
		(25 "Edge.Cuts" user)
		(27 "Margin" user)
		(31 "F.CrtYd" user "F.Courtyard")
		(29 "B.CrtYd" user "B.Courtyard")
		(35 "F.Fab" user)
		(33 "B.Fab" user)
		(39 "User.1" user)
		(41 "User.2" user)
		(43 "User.3" user)
		(45 "User.4" user)
	)
	(setup
		(stackup
			(layer "F.SilkS"
				(type "Top Silk Screen")
				(color "White")
			)
			(layer "F.Paste"
				(type "Top Solder Paste")
			)
			(layer "F.Mask"
				(type "Top Solder Mask")
				(color "Purple")
				(thickness 0.01524)
			)
			(layer "F.Cu"
				(type "copper")
				(thickness 0.04572)
			)
			(layer "dielectric 1"
				(type "prepreg")
				(color "FR4 natural")
				(thickness 0.199898)
				(material "FR408HR")
				(epsilon_r 3.61)
				(loss_tangent 0.009)
			)
			(layer "In1.Cu"
				(type "copper")
				(thickness 0.01524)
			)
			(layer "dielectric 2"
				(type "core")
				(color "FR4 natural")
				(thickness 0.9906)
				(material "FR408HR")
				(epsilon_r 3.87)
				(loss_tangent 0.009)
			)
			(layer "In2.Cu"
				(type "copper")
				(thickness 0.01524)
			)
			(layer "dielectric 3"
				(type "prepreg")
				(color "FR4 natural")
				(thickness 0.199644)
				(material "FR408HR")
				(epsilon_r 3.61)
				(loss_tangent 0.009)
			)
			(layer "B.Cu"
				(type "copper")
				(thickness 0.04572)
			)
			(layer "B.Mask"
				(type "Bottom Solder Mask")
				(color "Purple")
				(thickness 0.01524)
			)
			(layer "B.Paste"
				(type "Bottom Solder Paste")
			)
			(layer "B.SilkS"
				(type "Bottom Silk Screen")
				(color "White")
			)
			(copper_finish "ENIG")
			(dielectric_constraints no)
		)
		(pad_to_mask_clearance 0.0381)
		(allow_soldermask_bridges_in_footprints no)
		(tenting front back)
		(pcbplotparams
			(layerselection 0x00000000_00000000_55555555_5755f5ff)
			(plot_on_all_layers_selection 0x00000000_00000000_00000000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 4)
			(plotframeref no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(pdf_metadata yes)
			(pdf_single_document no)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plot_black_and_white yes)
			(sketchpadsonfab no)
			(plotpadnumbers no)
			(hidednponfab no)
			(sketchdnponfab yes)
			(crossoutdnponfab yes)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 1)
			(scaleselection 1)
			(outputdirectory "")
		)
	)
	(net 0 "")
	(net 1 "/EPS_IN")
	(net 2 "Net-(C2-Pad1)")
	(net 3 "Net-(PS1-+V_INPUT)")
	(net 4 "/DC_POS.5V")
	(net 5 "/DC_POS.12V")
	(net 6 "/DC_POS.9V")
	(net 7 "/LCL_12V/12V_12A_LCL_1/OPAMP_Minus")
	(net 8 "Net-(Q1-B)")
	(net 9 "Net-(Q2-B)")
	(net 10 "/LCL_12V/12V_12A_LCL_2/OPAMP_Minus")
	(net 11 "/LCL_12V/12V_12A_LCL_3/OPAMP_Minus")
	(net 12 "Net-(Q3-B)")
	(net 13 "/LCL_12V/12V_12A_LCL_4/OPAMP_Minus")
	(net 14 "Net-(Q4-B)")
	(net 15 "Net-(Q5-B)")
	(net 16 "/LCL_12V/12V_3A_LCL_1/OPAMP_Minus")
	(net 17 "Net-(Q6-B)")
	(net 18 "/LCL_12V/12V_3A_LCL_2/OPAMP_Minus")
	(net 19 "/LCL_12V/12V_5A_LCL_1/OPAMP_Minus")
	(net 20 "Net-(Q7-B)")
	(net 21 "Net-(Q8-B)")
	(net 22 "/LCL_12V/12V_5A_LCL_2/OPAMP_Minus")
	(net 23 "Net-(Q9-B)")
	(net 24 "/LCL_5V/5V_6A_LCL_3/OPAMP_Minus")
	(net 25 "Net-(Q10-B)")
	(net 26 "/LCL_5V/5V_6A_LCL_1/OPAMP_Minus")
	(net 27 "/LCL_5V/5V_6A_LCL_2/OPAMP_Minus")
	(net 28 "Net-(Q11-B)")
	(net 29 "Net-(Q12-B)")
	(net 30 "/LCL_5V/5V_6A_LCL_4/OPAMP_Minus")
	(net 31 "Net-(Q13-B)")
	(net 32 "/LCL_9_and_3-3/9V_2A_LCL_1/OPAMP_Minus")
	(net 33 "/LCL_9_and_3-3/3-3V_1-5A_LCL_1/OPAMP_Minus")
	(net 34 "Net-(Q14-B)")
	(net 35 "/Digital Systems/3.3V+")
	(net 36 "Net-(U43-~{RST})")
	(net 37 "Net-(U43-OSC0)")
	(net 38 "Net-(U42-NR)")
	(net 39 "Net-(U44-REF)")
	(net 40 "Net-(U43-VDDC@1)")
	(net 41 "/Digital Systems/OSC1")
	(net 42 "Net-(D1-K)")
	(net 43 "/LCL_12.12A1")
	(net 44 "Net-(D2-K)")
	(net 45 "/LCL_12.12A2")
	(net 46 "Net-(D3-K)")
	(net 47 "/LCL_12.12A3")
	(net 48 "/LCL_12.12A4")
	(net 49 "Net-(D4-K)")
	(net 50 "/LCL_12.3A1")
	(net 51 "Net-(D5-K)")
	(net 52 "Net-(D6-K)")
	(net 53 "/LCL_12.3A2")
	(net 54 "/LCL_12.5A1")
	(net 55 "Net-(D7-K)")
	(net 56 "Net-(D8-K)")
	(net 57 "/LCL_12.5A2")
	(net 58 "Net-(D9-K)")
	(net 59 "/LCL_5.6A3")
	(net 60 "Net-(D10-K)")
	(net 61 "/LCL_5.6A1")
	(net 62 "Net-(D11-K)")
	(net 63 "/LCL_5.6A2")
	(net 64 "/LCL_5.6A4")
	(net 65 "Net-(D12-K)")
	(net 66 "/LCL_MIXED.9V2A")
	(net 67 "Net-(D13-K)")
	(net 68 "Net-(D14-K)")
	(net 69 "/LCL_MIXED.3.3V1.5A")
	(net 70 "Net-(U4--Vin)")
	(net 71 "Net-(U4-+Vin)")
	(net 72 "/DC_POS.3.3V")
	(net 73 "/JTAG.RESET")
	(net 74 "/JTAG.TDO")
	(net 75 "/JTAG.TDI")
	(net 76 "/JTAG.TMS")
	(net 77 "/JTAG.TCK")
	(net 78 "/ADC_AIN3")
	(net 79 "/ADC_AIN2")
	(net 80 "/ADC_AIN1")
	(net 81 "/USB.D+")
	(net 82 "/USB.VBUS")
	(net 83 "/USB.ID")
	(net 84 "/USB.D-")
	(net 85 "/ADC_AIN0")
	(net 86 "/UART.Tx")
	(net 87 "unconnected-(J23-Pad1)")
	(net 88 "/UART.Rx")
	(net 89 "Net-(LED1-Pad1)")
	(net 90 "unconnected-(PS1-ON{slash}OFF-Pad2)")
	(net 91 "Net-(U2-+On{slash}Off)")
	(net 92 "Net-(U3-+On{slash}Off)")
	(net 93 "Net-(U3--S)")
	(net 94 "Net-(U3-+S)")
	(net 95 "Net-(U2--S)")
	(net 96 "Net-(U2-+S)")
	(net 97 "Net-(U2-PC{slash}NC)")
	(net 98 "Net-(R7-Pad2)")
	(net 99 "Net-(U3-PC{slash}NC)")
	(net 100 "Net-(R10-Pad1)")
	(net 101 "Net-(R11-Pad2)")
	(net 102 "Net-(R13-Pad2)")
	(net 103 "Net-(R15-Pad2)")
	(net 104 "Net-(U5A-IN-)")
	(net 105 "Net-(U5B-IN-)")
	(net 106 "Net-(U5C-IN-)")
	(net 107 "Net-(U5D-IN-)")
	(net 108 "Net-(R21-Pad2)")
	(net 109 "Net-(R23-Pad2)")
	(net 110 "Net-(R25-Pad2)")
	(net 111 "Net-(R27-Pad2)")
	(net 112 "Net-(U6A-IN-)")
	(net 113 "Net-(U6B-IN-)")
	(net 114 "Net-(U6C-IN-)")
	(net 115 "Net-(U6D-IN-)")
	(net 116 "Net-(R33-Pad2)")
	(net 117 "Net-(R35-Pad2)")
	(net 118 "Net-(R37-Pad2)")
	(net 119 "Net-(R39-Pad2)")
	(net 120 "Net-(U7A-IN-)")
	(net 121 "Net-(U7B-IN-)")
	(net 122 "Net-(U7C-IN-)")
	(net 123 "Net-(U7D-IN-)")
	(net 124 "Net-(R45-Pad2)")
	(net 125 "Net-(R47-Pad2)")
	(net 126 "Net-(U8A-IN-)")
	(net 127 "Net-(U8B-IN-)")
	(net 128 "Net-(R55-Pad1)")
	(net 129 "Net-(R61-Pad1)")
	(net 130 "Net-(R67-Pad1)")
	(net 131 "Net-(R73-Pad1)")
	(net 132 "Net-(R79-Pad1)")
	(net 133 "Net-(R85-Pad1)")
	(net 134 "Net-(R91-Pad1)")
	(net 135 "Net-(R97-Pad1)")
	(net 136 "Net-(R103-Pad1)")
	(net 137 "Net-(R109-Pad1)")
	(net 138 "Net-(R115-Pad1)")
	(net 139 "Net-(R121-Pad1)")
	(net 140 "Net-(R127-Pad1)")
	(net 141 "Net-(R133-Pad1)")
	(net 142 "Net-(U41-~{CNVST}{slash}AIN15)")
	(net 143 "/Digital Systems/ADC1_CNVST")
	(net 144 "/Digital Systems/SSI0Tx")
	(net 145 "Net-(U41-DIN)")
	(net 146 "Net-(U41-SCLK)")
	(net 147 "/Digital Systems/SSI0CLK")
	(net 148 "Net-(U41-~{CS})")
	(net 149 "Net-(U41-~{EOC})")
	(net 150 "/Digital Systems/ADC1_EOC")
	(net 151 "Net-(R140-Pad2)")
	(net 152 "/Digital Systems/I2C0SCL")
	(net 153 "Net-(U43-PB2{slash}I2C0SCL)")
	(net 154 "Net-(U43-PB3{slash}I2C0SDA)")
	(net 155 "/Digital Systems/I2C0SDA")
	(net 156 "Net-(U43-PA2{slash}SSI0CLK)")
	(net 157 "Net-(U43-PA3{slash}SSI0FSS)")
	(net 158 "Net-(U43-PA5{slash}SSI0TX)")
	(net 159 "Net-(U43-PB6)")
	(net 160 "/Digital Systems/THM_CS")
	(net 161 "Net-(U43-PD6)")
	(net 162 "/Digital Systems/GPIO_INT")
	(net 163 "Net-(U43-PF0)")
	(net 164 "/Digital Systems/ADC2_EOC")
	(net 165 "Net-(U43-PF1)")
	(net 166 "/Digital Systems/ADC2_CNVST")
	(net 167 "Net-(U43-PF2)")
	(net 168 "Net-(U43-PF3)")
	(net 169 "Net-(U43-PF4)")
	(net 170 "/Digital Systems/SSI0Rx")
	(net 171 "Net-(U41-DOUT)")
	(net 172 "Net-(U43-OSC1)")
	(net 173 "Net-(U44-~{CNVST}{slash}AIN15)")
	(net 174 "Net-(U44-DIN)")
	(net 175 "Net-(U44-SCLK)")
	(net 176 "Net-(U44-~{CS})")
	(net 177 "Net-(U44-~{EOC})")
	(net 178 "/LCL_CTRL1")
	(net 179 "Net-(U45-P0_0)")
	(net 180 "Net-(U45-P0_1)")
	(net 181 "/LCL_CTRL2")
	(net 182 "/LCL_CTRL3")
	(net 183 "Net-(U45-P0_2)")
	(net 184 "/LCL_CTRL4")
	(net 185 "Net-(U45-P0_3)")
	(net 186 "/LCL_CTRL5")
	(net 187 "Net-(U45-P0_4)")
	(net 188 "Net-(U45-P0_5)")
	(net 189 "/LCL_CTRL6")
	(net 190 "/LCL_CTRL7")
	(net 191 "Net-(U45-P0_6)")
	(net 192 "Net-(U45-P0_7)")
	(net 193 "/LCL_CTRL8")
	(net 194 "Net-(U45-P1_0)")
	(net 195 "/LCL_CTRL9")
	(net 196 "/LCL_CTRL10")
	(net 197 "Net-(U45-P1_1)")
	(net 198 "/LCL_CTRL11")
	(net 199 "Net-(U45-P1_2)")
	(net 200 "Net-(U45-P1_3)")
	(net 201 "/LCL_CTRL12")
	(net 202 "/LCL_CTRL13")
	(net 203 "Net-(U45-P1_4)")
	(net 204 "Net-(U45-P1_5)")
	(net 205 "/LCL_CTRL14")
	(net 206 "Net-(U44-DOUT)")
	(net 207 "Net-(U46-SO)")
	(net 208 "Net-(U46-*CS)")
	(net 209 "Net-(U46-SCL)")
	(net 210 "unconnected-(S1-Pad3)")
	(net 211 "Net-(U42-EN)")
	(net 212 "unconnected-(SW1-Pad2)")
	(net 213 "unconnected-(SW1-Pad3)")
	(net 214 "unconnected-(U1-N.C.-Pad11)")
	(net 215 "unconnected-(U1-Remote_ON{slash}OFF-Pad1)")
	(net 216 "unconnected-(U2-AUX-Pad16)")
	(net 217 "unconnected-(U2-IOG-Pad15)")
	(net 218 "unconnected-(U2-TRIM-Pad13)")
	(net 219 "unconnected-(U3-AUX-Pad16)")
	(net 220 "unconnected-(U3-IOG-Pad15)")
	(net 221 "unconnected-(U3-TRIM-Pad13)")
	(net 222 "unconnected-(U4-TRIM-Pad8)")
	(net 223 "unconnected-(U4-NO_PIN-Pad5)")
	(net 224 "unconnected-(U4-Remote_On{slash}Off-Pad1)")
	(net 225 "/V_MEAS.12_2")
	(net 226 "/V_MEAS.12_1")
	(net 227 "/V_MEAS.12_3")
	(net 228 "/V_MEAS.12_4")
	(net 229 "/V_MEAS.12_7")
	(net 230 "/V_MEAS.12_8")
	(net 231 "/V_MEAS.12_6")
	(net 232 "/V_MEAS.12_5")
	(net 233 "/V_MEAS.5_2")
	(net 234 "/V_MEAS.5_1")
	(net 235 "/V_MEAS.5_4")
	(net 236 "/V_MEAS.5_3")
	(net 237 "/V_MEAS.3.3_")
	(net 238 "unconnected-(U8D-IN+-Pad12)")
	(net 239 "unconnected-(U8D-IN--Pad13)")
	(net 240 "/V_MEAS.9_")
	(net 241 "unconnected-(U8C-IN--Pad9)")
	(net 242 "unconnected-(U8C-OUT-Pad8)")
	(net 243 "unconnected-(U8C-IN+-Pad10)")
	(net 244 "unconnected-(U8D-OUT-Pad14)")
	(net 245 "/I_MEAS.12_3")
	(net 246 "/I_MEAS.12_4")
	(net 247 "/I_MEAS.12_1")
	(net 248 "/I_MEAS.12_2")
	(net 249 "/I_MEAS.12_8")
	(net 250 "/I_MEAS.12_7")
	(net 251 "/I_MEAS.12_6")
	(net 252 "/I_MEAS.12_5")
	(net 253 "unconnected-(U12-NC-Pad3)")
	(net 254 "unconnected-(U12-Pad6)")
	(net 255 "unconnected-(U14-NC-Pad3)")
	(net 256 "unconnected-(U14-Pad6)")
	(net 257 "unconnected-(U16-NC-Pad3)")
	(net 258 "unconnected-(U16-Pad6)")
	(net 259 "unconnected-(U18-Pad6)")
	(net 260 "unconnected-(U18-NC-Pad3)")
	(net 261 "unconnected-(U20-NC-Pad3)")
	(net 262 "unconnected-(U20-Pad6)")
	(net 263 "unconnected-(U22-Pad6)")
	(net 264 "unconnected-(U22-NC-Pad3)")
	(net 265 "unconnected-(U24-NC-Pad3)")
	(net 266 "unconnected-(U24-Pad6)")
	(net 267 "unconnected-(U26-NC-Pad3)")
	(net 268 "unconnected-(U26-Pad6)")
	(net 269 "/I_MEAS.5_2")
	(net 270 "/I_MEAS.5_4")
	(net 271 "/I_MEAS.5_3")
	(net 272 "/I_MEAS.5_1")
	(net 273 "unconnected-(U29-NC-Pad3)")
	(net 274 "unconnected-(U29-Pad6)")
	(net 275 "unconnected-(U31-Pad6)")
	(net 276 "unconnected-(U31-NC-Pad3)")
	(net 277 "unconnected-(U33-NC-Pad3)")
	(net 278 "unconnected-(U33-Pad6)")
	(net 279 "unconnected-(U35-Pad6)")
	(net 280 "unconnected-(U35-NC-Pad3)")
	(net 281 "unconnected-(U36-Pad9)")
	(net 282 "unconnected-(U36-Pad14)")
	(net 283 "/I_MEAS.9_")
	(net 284 "unconnected-(U36-Pad13)")
	(net 285 "unconnected-(U36-Pad8)")
	(net 286 "/I_MEAS.3.3_")
	(net 287 "unconnected-(U36-Pad10)")
	(net 288 "unconnected-(U36-Pad12)")
	(net 289 "unconnected-(U38-NC-Pad3)")
	(net 290 "unconnected-(U38-Pad6)")
	(net 291 "unconnected-(U40-NC-Pad3)")
	(net 292 "unconnected-(U40-Pad6)")
	(net 293 "unconnected-(U41-AIN4-Pad5)")
	(net 294 "unconnected-(U43-PE5-Pad60)")
	(net 295 "unconnected-(U43-XOSC1-Pad36)")
	(net 296 "unconnected-(U43-PE4-Pad59)")
	(net 297 "unconnected-(U43-PD7-Pad10)")
	(net 298 "unconnected-(U43-~{HIB}-Pad33)")
	(net 299 "unconnected-(U44-AIN12-Pad13)")
	(net 300 "unconnected-(U45-P1_7-Pad20)")
	(net 301 "unconnected-(U45-P1_6-Pad19)")
	(net 302 "unconnected-(U46-NC-Pad1)")
	(net 303 "/GNDREF")
	(net 304 "/Digital Systems/ADC1_CS")
	(net 305 "/Digital Systems/ADC2_CS")
	(footprint "EPS_Footprints:RESC1508X55N"
		(layer "F.Cu")
		(at 154.35905 251.05195 -90)
		(property "Reference" "R47"
			(at -2.01 0.3008 0)
			(layer "F.SilkS")
		)
		(property "Value" "100k"
			(at 1.54 1.07 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Power_Connectors/")
		(sheetfile "Power_Connectors.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -0.76 0 270)
			(size 0.9 0.97)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 69 "/LCL_MIXED.3.3V1.5A")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd rect
			(at 0.76 0 270)
			(size 0.9 0.97)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 125 "Net-(R47-Pad2)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:Terminal Block 691137710002"
		(layer "F.Cu")
		(at 185.85905 42.29195 180)
		(property "Reference" "J11"
			(at -1.1992 -4.25 0)
			(layer "F.SilkS")
		)
		(property "Value" "691137710002"
			(at 4.12 5.365 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/Power_Connectors/")
		(sheetfile "Power_Connectors.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole circle
			(at -2.5 0 180)
			(size 1.95 1.95)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 303 "/GNDREF")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" thru_hole circle
			(at 2.5 0 180)
			(size 1.95 1.95)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 61 "/LCL_5.6A1")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:RESC1508X55N"
		(layer "F.Cu")
		(at 278.65905 60.36695 90)
		(property "Reference" "R122"
			(at -2.675 -0.1008 90)
			(layer "F.SilkS")
		)
		(property "Value" "54.9k"
			(at 1.54 1.069999 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/LCL_5V/5V_6A_LCL_4/")
		(sheetfile "5V_6A_LCL.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -0.76 0 90)
			(size 0.9 0.97)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 139 "Net-(R121-Pad1)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd rect
			(at 0.76 0 90)
			(size 0.9 0.97)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 65 "Net-(D12-K)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:RESC1608X55N"
		(layer "F.Cu")
		(at 249.60905 60.54195 90)
		(property "Reference" "R103"
			(at -2.75 -0.0508 90)
			(layer "F.SilkS")
		)
		(property "Value" "5.1k"
			(at 1.54 1.049999 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/LCL_5V/5V_6A_LCL_3/")
		(sheetfile "5V_6A_LCL.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -0.82 0 90)
			(size 0.79 0.93)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 136 "Net-(R103-Pad1)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd rect
			(at 0.82 0 90)
			(size 0.79 0.93)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 58 "Net-(D9-K)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:RESC1508X55N"
		(layer "F.Cu")
		(at 42.35905 197.04195 -90)
		(property "Reference" "R11"
			(at -0.75 -1.4492 90)
			(layer "F.SilkS")
		)
		(property "Value" "100k"
			(at 1.54 1.07 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Power_Connectors/")
		(sheetfile "Power_Connectors.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -0.76 0 270)
			(size 0.9 0.97)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 45 "/LCL_12.12A2")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd rect
			(at 0.76 0 270)
			(size 0.9 0.97)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 101 "Net-(R11-Pad2)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:TO-263AB_SUM"
		(layer "F.Cu")
		(at 52.50935 113.54195 -90)
		(tags "SUM110P06-08L-E3 ")
		(property "Reference" "U17"
			(at 6.5 -0.0489 270)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "SUM110P06-08L-E3"
			(at -0.339999 3.193 270)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "SUM110P06-08L-E3"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TO-263AB_SUM TO-263AB_SUM-M TO-263AB_SUM-L")
		(sheetname "/LCL_12V/12V_12A_LCL_4/")
		(sheetfile "12V_12A_LCL.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
		)
		(fp_text user "*"
			(at -2.539999 5.2705 90)
			(layer "F.Fab")
		)
		(fp_text user "*"
			(at -2.539999 5.2705 270)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -2.54 8.8773 270)
			(size 0.9906 3.2004)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 49 "Net-(D4-K)")
			(pinfunction "G")
			(pintype "input")
		)
		(pad "2" smd rect
			(at 0 0.0508 270)
			(size 10.414 11.4554)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 13 "/LCL_12V/12V_12A_LCL_4/OPAMP_Minus")
			(pinfunction "D")
			(pintype "input")
		)
		(pad "3" smd rect
			(at 2.54 8.8773 270)
			(size 0.9906 3.2004)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 48 "/LCL_12.12A4")
			(pinfunction "S")
			(pintype "input")
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:RESC1508X55N"
		(layer "F.Cu")
		(at 234.59905 230.29195)
		(property "Reference" "R172"
			(at -2.7908 -0.5 0)
			(layer "F.SilkS")
		)
		(property "Value" "100"
			(at 1.54 1.07 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Digital Systems/")
		(sheetfile "Digital_Systems.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -0.76 0)
			(size 0.9 0.97)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 190 "/LCL_CTRL7")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd rect
			(at 0.76 0)
			(size 0.9 0.97)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 191 "Net-(U45-P0_6)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:RES_TLRP3A30DR018FTE_TEC"
		(layer "F.Cu")
		(at 157.35905 246.29195)
		(tags "TLRP3A30DR018FTE ")
		(property "Reference" "R129"
			(at -5.3008 1.5 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "0.01"
			(at 0 1 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/LCL_9_and_3-3/3-3V_1-5A_LCL_1/")
		(sheetfile "3-3V_1-5A_LCL.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -2.8321 0)
			(size 1.397 3.4544)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 72 "/DC_POS.3.3V")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 2.8321 0)
			(size 1.397 3.4544)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 33 "/LCL_9_and_3-3/3-3V_1-5A_LCL_1/OPAMP_Minus")
			(pintype "passive")
		)
		(zone
			(net 0)
			(net_name "")
			(layer "F.Cu")
			(hatch full 0.508)
			(connect_pads
				(clearance 0)
			)
			(min_thickness 0.254)
			(filled_areas_thickness no)
			(keepout
				(tracks not_allowed)
				(vias not_allowed)
				(pads allowed)
				(copperpour not_allowed)
				(footprints allowed)
			)
			(placement
				(enabled no)
				(sheetname "")
			)
			(fill
				(thermal_gap 0.508)
				(thermal_bridge_width 0.508)
			)
			(polygon
				(pts
					(xy 155.27625 244.61555) (xy 159.44185 244.61555) (xy 159.44185 247.96835) (xy 155.27625 247.96835)
				)
			)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:RESC1508X55N"
		(layer "F.Cu")
		(at 177.62825 62.79195 90)
		(property "Reference" "R106"
			(at -2.5 -0.07 90)
			(layer "F.SilkS")
		)
		(property "Value" "11.5k"
			(at 1.54 1.07 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/LCL_5V/5V_6A_LCL_1/")
		(sheetfile "5V_6A_LCL.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -0.76 0 90)
			(size 0.9 0.97)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 25 "Net-(Q10-B)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd rect
			(at 0.76 0 90)
			(size 0.9 0.97)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 26 "/LCL_5V/5V_6A_LCL_1/OPAMP_Minus")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:TO-263AB_SUM"
		(layer "F.Cu")
		(at 145.023741 51.813259 90)
		(tags "SUM110P06-08L-E3 ")
		(property "Reference" "U19"
			(at -4.228691 6.784509 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "SUM110P06-08L-E3"
			(at 0.43 0 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "SUM110P06-08L-E3"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TO-263AB_SUM TO-263AB_SUM-M TO-263AB_SUM-L")
		(sheetname "/LCL_12V/12V_3A_LCL_1/")
		(sheetfile "12V_3A_LCL.kicad_sch")
		(attr smd)
		(fp_text user "*"
			(at -2.539999 5.2705 90)
			(layer "F.Fab")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(fp_text user "*"
			(at -2.539999 5.2705 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -2.54 8.8773 90)
			(size 0.9906 3.2004)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 51 "Net-(D5-K)")
			(pinfunction "G")
			(pintype "input")
		)
		(pad "2" smd rect
			(at 0 0.0508 90)
			(size 10.414 11.4554)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 16 "/LCL_12V/12V_3A_LCL_1/OPAMP_Minus")
			(pinfunction "D")
			(pintype "input")
		)
		(pad "3" smd rect
			(at 2.54 8.8773 90)
			(size 0.9906 3.2004)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 50 "/LCL_12.3A1")
			(pinfunction "S")
			(pintype "input")
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:RESC1508X55N"
		(layer "F.Cu")
		(at 47.36905 236.80195 180)
		(property "Reference" "R45"
			(at -0.21 -1.07 0)
			(layer "F.SilkS")
		)
		(property "Value" "100k"
			(at 1.54 1.07 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Power_Connectors/")
		(sheetfile "Power_Connectors.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -0.76 0 180)
			(size 0.9 0.97)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 66 "/LCL_MIXED.9V2A")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd rect
			(at 0.76 0 180)
			(size 0.9 0.97)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 124 "Net-(R45-Pad2)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:RESC1508X55N"
		(layer "F.Cu")
		(at 38.10905 132.54195 90)
		(property "Reference" "R20"
			(at -0.21 -1.07 90)
			(layer "F.SilkS")
		)
		(property "Value" "1k"
			(at 1.54 1.07 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Power_Connectors/")
		(sheetfile "Power_Connectors.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -0.76 0 90)
			(size 0.9 0.97)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 107 "Net-(U5D-IN-)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd rect
			(at 0.76 0 90)
			(size 0.9 0.97)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 103 "Net-(R15-Pad2)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:RESC1508X55N"
		(layer "F.Cu")
		(at 234.35905 205.78195 -90)
		(property "Reference" "R183"
			(at -2.74 -0.6992 90)
			(layer "F.SilkS")
		)
		(property "Value" "470"
			(at 1.54 1.07 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Digital Systems/")
		(sheetfile "Digital_Systems.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -0.76 0 270)
			(size 0.9 0.97)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 160 "/Digital Systems/THM_CS")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd rect
			(at 0.76 0 270)
			(size 0.9 0.97)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 208 "Net-(U46-*CS)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:SOT91P240X120-3N"
		(layer "F.Cu")
		(at 148.509041 61.608258)
		(property "Reference" "Q5"
			(at -0.175999 -2.3698 0)
			(layer "F.SilkS")
		)
		(property "Value" "PNP"
			(at 3.1768 2.3698 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://ngspice.sourceforge.io/docs/ngspice-html-manual/manual.xhtml#cha_BJTs"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Bipolar transistor symbol for simulation only, substrate tied to the emitter"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Device" "PNP"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Type" "GUMMELPOON"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" "1=C 2=B 3=E"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/LCL_12V/12V_3A_LCL_1/")
		(sheetfile "12V_3A_LCL.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -0.915 1.025)
			(size 0.61 1.18)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 51 "Net-(D5-K)")
			(pinfunction "C")
			(pintype "open_collector")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd rect
			(at 0.915 1.025)
			(size 0.61 1.18)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 15 "Net-(Q5-B)")
			(pinfunction "B")
			(pintype "input")
			(solder_mask_margin 0.102)
		)
		(pad "3" smd rect
			(at 0 -1.025)
			(size 0.61 1.18)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 16 "/LCL_12V/12V_3A_LCL_1/OPAMP_Minus")
			(pinfunction "E")
			(pintype "open_emitter")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:TO-263AB_SUM"
		(layer "F.Cu")
		(at 80.857925 51.019375 90)
		(tags "SUM110P06-08L-E3 ")
		(property "Reference" "U23"
			(at -0.022575 -6.549675 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "SUM110P06-08L-E3"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "SUM110P06-08L-E3"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TO-263AB_SUM TO-263AB_SUM-M TO-263AB_SUM-L")
		(sheetname "/LCL_12V/12V_5A_LCL_1/")
		(sheetfile "12V_5A_LCL.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(fp_text user "*"
			(at -2.539999 5.2705 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(fp_text user "*"
			(at -2.539999 5.2705 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -2.54 8.8773 90)
			(size 0.9906 3.2004)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 55 "Net-(D7-K)")
			(pinfunction "G")
			(pintype "input")
		)
		(pad "2" smd rect
			(at 0 0.0508 90)
			(size 10.414 11.4554)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 19 "/LCL_12V/12V_5A_LCL_1/OPAMP_Minus")
			(pinfunction "D")
			(pintype "input")
		)
		(pad "3" smd rect
			(at 2.54 8.8773 90)
			(size 0.9906 3.2004)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 54 "/LCL_12.5A1")
			(pinfunction "S")
			(pintype "input")
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:DIP762W50P254L730H410Q6"
		(layer "F.Cu")
		(at 94.297925 60.979375 180)
		(property "Reference" "U24"
			(at -0.56 0.209999 0)
			(layer "F.SilkS")
		)
		(property "Value" "CNY17-1"
			(at -0.31 1.96 0)
			(layer "Dwgs.User")
		)
		(property "Datasheet" "http://www.vishay.com/docs/83606/cny17.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "DC Optocoupler Base Connected, Vce 70V, CTR 40-80%, Viso 5000V (RMS), DIP6"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "DIP*W7.62mm* DIP*W10.16mm* SMDIP*W9.53mm*")
		(sheetname "/LCL_12V/12V_5A_LCL_1/")
		(sheetfile "12V_5A_LCL.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole rect
			(at -3.81 -2.54 180)
			(size 1.4 1.4)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 190 "/LCL_CTRL7")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" thru_hole circle
			(at -3.81 0 180)
			(size 1.4 1.4)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 303 "/GNDREF")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "3" thru_hole circle
			(at -3.81 2.54 180)
			(size 1.4 1.4)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 265 "unconnected-(U24-NC-Pad3)")
			(pinfunction "NC")
			(pintype "no_connect")
			(solder_mask_margin 0.102)
		)
		(pad "4" thru_hole circle
			(at 3.81 2.54 180)
			(size 1.4 1.4)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 303 "/GNDREF")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "5" thru_hole circle
			(at 3.81 0 180)
			(size 1.4 1.4)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 134 "Net-(R91-Pad1)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "6" thru_hole circle
			(at 3.81 -2.54 180)
			(size 1.4 1.4)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 266 "unconnected-(U24-Pad6)")
			(pintype "passive+no_connect")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:RESC1508X55N"
		(layer "F.Cu")
		(at 64.10905 208.04195 180)
		(property "Reference" "R56"
			(at -2.1992 -0.5 0)
			(layer "F.SilkS")
		)
		(property "Value" "54.9k"
			(at 1.54 1.07 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/LCL_12V/12V_12A_LCL_1/")
		(sheetfile "12V_12A_LCL.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -0.76 0 180)
			(size 0.9 0.97)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 128 "Net-(R55-Pad1)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd rect
			(at 0.76 0 180)
			(size 0.9 0.97)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 42 "Net-(D1-K)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:RESC1508X55N"
		(layer "F.Cu")
		(at 223.61905 207.04195 180)
		(property "Reference" "R135"
			(at -0.21 -1.07 0)
			(layer "F.SilkS")
		)
		(property "Value" "0 Ohm"
			(at 1.54 1.07 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MF" "Stackpole Electronics Inc"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description_1" "0 Ohms Jumper 0.1W, 1/10W Chip Resistor 0603 (1608 Metric) Automotive AEC-Q200 Thick Film"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Package" "1508 Stackpole"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Price" "None"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SnapEDA_Link" "https://www.snapeda.com/parts/RMCF0603ZT0R00/Stackpole+Electronics/view-part/?ref=snap"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MP" "RMCF0603ZT0R00"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Purchase-URL" "https://www.snapeda.com/api/url_track_click_mouser/?unipart_id=3968849&manufacturer=Stackpole Electronics Inc&part_name=RMCF0603ZT0R00&search_term=rmcf0603zt0r00"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Availability" "In Stock"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Check_prices" "https://www.snapeda.com/parts/RMCF0603ZT0R00/Stackpole+Electronics/view-part/?ref=eda"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/Digital Systems/")
		(sheetfile "Digital_Systems.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -0.76 0 180)
			(size 0.9 0.97)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 143 "/Digital Systems/ADC1_CNVST")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd rect
			(at 0.76 0 180)
			(size 0.9 0.97)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 142 "Net-(U41-~{CNVST}{slash}AIN15)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:BAQ33GS08"
		(layer "F.Cu")
		(at 54.35905 230.66695 90)
		(descr "MiniMELF (SOD-80)")
		(tags "Zener Diode")
		(property "Reference" "ZD13"
			(at 0 0 90)
			(layer "F.SilkS")
		)
		(property "Value" "D_Zener"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Zener diode"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Library" "TZM5240B-GS08.txt"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Name" "TZM5240B-GS08"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Device" "D"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" "1=A 2=K"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TO-???* *_Diode_* *SingleDiode* D_*")
		(sheetname "/LCL_9_and_3-3/9V_2A_LCL_1/")
		(sheetfile "9V_2A_LCL.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.875 0 90)
			(size 1.25 2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 32 "/LCL_9_and_3-3/9V_2A_LCL_1/OPAMP_Minus")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.875 0 90)
			(size 1.25 2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 67 "Net-(D13-K)")
			(pinfunction "A")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "TZM5224B-GS08.stp"
			(offset
				(xyz 0 0 0.7999999999)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "EPS_Footprints:CAPC1608X90"
		(layer "F.Cu")
		(at 44.5828 59.9192 -90)
		(descr "<b>CAPACITOR</b>")
		(property "Reference" "C26"
			(at 2.62275 0.02455 90)
			(layer "F.SilkS")
		)
		(property "Value" "0.1uF"
			(at 1.56646 1.20613 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "SMD 0603 MLCC capacitor, Alternate KiCad Library"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/LCL_12V/12V_5A_LCL_2/")
		(sheetfile "12V_5A_LCL.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -0.85 0 270)
			(size 1.1 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 22 "/LCL_12V/12V_5A_LCL_2/OPAMP_Minus")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd rect
			(at 0.85 0 270)
			(size 1.1 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 21 "Net-(Q8-B)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:RESC1508X55N"
		(layer "F.Cu")
		(at 229.11905 201.54195 180)
		(property "Reference" "R137"
			(at -0.21 -1.07 0)
			(layer "F.SilkS")
		)
		(property "Value" "0 Ohm"
			(at 1.54 1.07 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MF" "Stackpole Electronics Inc"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description_1" "0 Ohms Jumper 0.1W, 1/10W Chip Resistor 0603 (1608 Metric) Automotive AEC-Q200 Thick Film"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Package" "1508 Stackpole"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Price" "None"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SnapEDA_Link" "https://www.snapeda.com/parts/RMCF0603ZT0R00/Stackpole+Electronics/view-part/?ref=snap"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MP" "RMCF0603ZT0R00"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Purchase-URL" "https://www.snapeda.com/api/url_track_click_mouser/?unipart_id=3968849&manufacturer=Stackpole Electronics Inc&part_name=RMCF0603ZT0R00&search_term=rmcf0603zt0r00"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Availability" "In Stock"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Check_prices" "https://www.snapeda.com/parts/RMCF0603ZT0R00/Stackpole+Electronics/view-part/?ref=eda"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/Digital Systems/")
		(sheetfile "Digital_Systems.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -0.76 0 180)
			(size 0.9 0.97)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 147 "/Digital Systems/SSI0CLK")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd rect
			(at 0.76 0 180)
			(size 0.9 0.97)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 146 "Net-(U41-SCLK)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:DIP762W50P254L730H410Q6"
		(layer "F.Cu")
		(at 64.70855 134.50245 -90)
		(property "Reference" "U16"
			(at -7.409999 -9.94 90)
			(layer "F.SilkS")
		)
		(property "Value" "CNY17-1"
			(at -0.21 9.94 90)
			(layer "Dwgs.User")
		)
		(property "Datasheet" "http://www.vishay.com/docs/83606/cny17.pdf"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "DC Optocoupler Base Connected, Vce 70V, CTR 40-80%, Viso 5000V (RMS), DIP6"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "DIP*W7.62mm* DIP*W10.16mm* SMDIP*W9.53mm*")
		(sheetname "/LCL_12V/12V_12A_LCL_3/")
		(sheetfile "12V_12A_LCL.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole rect
			(at -3.81 -2.54 270)
			(size 1.4 1.4)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 182 "/LCL_CTRL3")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" thru_hole circle
			(at -3.81 0 270)
			(size 1.4 1.4)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 303 "/GNDREF")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "3" thru_hole circle
			(at -3.81 2.54 270)
			(size 1.4 1.4)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 257 "unconnected-(U16-NC-Pad3)")
			(pinfunction "NC")
			(pintype "no_connect")
			(solder_mask_margin 0.102)
		)
		(pad "4" thru_hole circle
			(at 3.81 2.54 270)
			(size 1.4 1.4)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 303 "/GNDREF")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "5" thru_hole circle
			(at 3.81 0 270)
			(size 1.4 1.4)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 130 "Net-(R67-Pad1)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "6" thru_hole circle
			(at 3.81 -2.54 270)
			(size 1.4 1.4)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 258 "unconnected-(U16-Pad6)")
			(pintype "passive+no_connect")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:DIP762W50P254L730H410Q6"
		(layer "F.Cu")
		(at 50.10905 93.35195 -90)
		(property "Reference" "U18"
			(at 0 0 90)
			(layer "F.SilkS")
		)
		(property "Value" "CNY17-1"
			(at -0.1597 0.75 90)
			(layer "Dwgs.User")
		)
		(property "Datasheet" "http://www.vishay.com/docs/83606/cny17.pdf"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "DC Optocoupler Base Connected, Vce 70V, CTR 40-80%, Viso 5000V (RMS), DIP6"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "DIP*W7.62mm* DIP*W10.16mm* SMDIP*W9.53mm*")
		(sheetname "/LCL_12V/12V_12A_LCL_4/")
		(sheetfile "12V_12A_LCL.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole rect
			(at -3.81 -2.54 270)
			(size 1.4 1.4)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 184 "/LCL_CTRL4")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" thru_hole circle
			(at -3.81 0 270)
			(size 1.4 1.4)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 303 "/GNDREF")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "3" thru_hole circle
			(at -3.81 2.54 270)
			(size 1.4 1.4)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 260 "unconnected-(U18-NC-Pad3)")
			(pinfunction "NC")
			(pintype "no_connect")
			(solder_mask_margin 0.102)
		)
		(pad "4" thru_hole circle
			(at 3.81 2.54 270)
			(size 1.4 1.4)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 303 "/GNDREF")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "5" thru_hole circle
			(at 3.81 0 270)
			(size 1.4 1.4)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 131 "Net-(R73-Pad1)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "6" thru_hole circle
			(at 3.81 -2.54 270)
			(size 1.4 1.4)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 259 "unconnected-(U18-Pad6)")
			(pintype "passive+no_connect")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:RESC1508X55N"
		(layer "F.Cu")
		(at 225.35905 191.73695 90)
		(property "Reference" "R155"
			(at -0.21 -1.07 90)
			(layer "F.SilkS")
		)
		(property "Value" "30k"
			(at 1.54 1.07 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Digital Systems/")
		(sheetfile "Digital_Systems.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -0.76 0 90)
			(size 0.9 0.97)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 39 "Net-(U44-REF)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd rect
			(at 0.76 0 90)
			(size 0.9 0.97)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 35 "/Digital Systems/3.3V+")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:RESC1608X55N"
		(layer "F.Cu")
		(at 60.28905 252.04195 180)
		(property "Reference" "R124"
			(at -0.21 -1.05 0)
			(layer "F.SilkS")
		)
		(property "Value" "86.6k"
			(at 1.54 1.05 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/LCL_9_and_3-3/9V_2A_LCL_1/")
		(sheetfile "9V_2A_LCL.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -0.82 0 180)
			(size 0.79 0.93)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 31 "Net-(Q13-B)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd rect
			(at 0.82 0 180)
			(size 0.79 0.93)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 32 "/LCL_9_and_3-3/9V_2A_LCL_1/OPAMP_Minus")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:RESC1508X55N"
		(layer "F.Cu")
		(at 245.11905 229.54195)
		(property "Reference" "R175"
			(at -0.0608 1.25 0)
			(layer "F.SilkS")
		)
		(property "Value" "100"
			(at 1.54 1.07 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Digital Systems/")
		(sheetfile "Digital_Systems.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -0.76 0)
			(size 0.9 0.97)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 194 "Net-(U45-P1_0)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd rect
			(at 0.76 0)
			(size 0.9 0.97)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 195 "/LCL_CTRL9")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:BAQ33GS08"
		(layer "F.Cu")
		(at 64.9328 53.9192)
		(descr "MiniMELF (SOD-80)")
		(tags "Zener Diode")
		(property "Reference" "ZD8"
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "D_Zener"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Zener diode"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Library" "TZM5240B-GS08.txt"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Name" "TZM5240B-GS08"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Device" "D"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" "1=A 2=K"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TO-???* *_Diode_* *SingleDiode* D_*")
		(sheetname "/LCL_12V/12V_5A_LCL_2/")
		(sheetfile "12V_5A_LCL.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.875 0)
			(size 1.25 2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 22 "/LCL_12V/12V_5A_LCL_2/OPAMP_Minus")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.875 0)
			(size 1.25 2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 56 "Net-(D8-K)")
			(pinfunction "A")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "TZM5224B-GS08.stp"
			(offset
				(xyz 0 0 0.7999999999)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "EPS_Footprints:RESC1508X55N"
		(layer "F.Cu")
		(at 248.10905 223.54195)
		(property "Reference" "R178"
			(at 2.6992 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "100"
			(at 1.54 1.07 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Digital Systems/")
		(sheetfile "Digital_Systems.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -0.76 0)
			(size 0.9 0.97)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 200 "Net-(U45-P1_3)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd rect
			(at 0.76 0)
			(size 0.9 0.97)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 201 "/LCL_CTRL12")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:RESC1508X55N"
		(layer "F.Cu")
		(at 119.15295 61.79435 90)
		(property "Reference" "R86"
			(at -2.4976 -0.0947 90)
			(layer "F.SilkS")
		)
		(property "Value" "54.9k"
			(at 1.54 1.07 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/LCL_12V/12V_3A_LCL_2/")
		(sheetfile "12V_3A_LCL.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -0.76 0 90)
			(size 0.9 0.97)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 133 "Net-(R85-Pad1)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd rect
			(at 0.76 0 90)
			(size 0.9 0.97)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 52 "Net-(D6-K)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:SOT95P280X145-5N"
		(layer "F.Cu")
		(at 269.11405 176.84195 180)
		(property "Reference" "U42"
			(at -1.1942 -2.2 0)
			(layer "F.SilkS")
		)
		(property "Value" "TPS73633DBVR"
			(at 5.528 2.508 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DigiKey_Part_Number" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SnapEDA_Link" "https://www.snapeda.com/parts/TPS73633DBVR/Texas+Instruments/view-part/?ref=snap"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MAXIMUM_PACKAGE_HEIGHT" "1.45mm"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Package" "SOT-23-5 Texas Instruments"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Check_prices" "https://www.snapeda.com/parts/TPS73633DBVR/Texas+Instruments/view-part/?ref=eda"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "STANDARD" "IPC-7351B"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTREV" "U"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MF" "Texas Instruments"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MP" "TPS73633DBVR"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description_1" "400mA high-accuracy ultra-low-dropout voltage regulator with reverse current protection and enable"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER" "Texas Instruments"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/Digital Systems/")
		(sheetfile "Digital_Systems.kicad_sch")
		(attr smd)
		(pad "1" smd roundrect
			(at -1.255 -0.95 180)
			(size 1.21 0.59)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 211 "Net-(U42-EN)")
			(pinfunction "IN")
			(pintype "input")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd roundrect
			(at -1.255 0 180)
			(size 1.21 0.59)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 303 "/GNDREF")
			(pinfunction "GND")
			(pintype "power_in")
			(solder_mask_margin 0.102)
		)
		(pad "3" smd roundrect
			(at -1.255 0.95 180)
			(size 1.21 0.59)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 211 "Net-(U42-EN)")
			(pinfunction "EN")
			(pintype "input")
			(solder_mask_margin 0.102)
		)
		(pad "4" smd roundrect
			(at 1.255 0.95 180)
			(size 1.21 0.59)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 38 "Net-(U42-NR)")
			(pinfunction "NR")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "5" smd roundrect
			(at 1.255 -0.95 180)
			(size 1.21 0.59)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 35 "/Digital Systems/3.3V+")
			(pinfunction "OUT")
			(pintype "output")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:RESC1608X55N"
		(layer "F.Cu")
		(at 64.10905 206.29195 180)
		(property "Reference" "R55"
			(at -2.4492 -0.5 0)
			(layer "F.SilkS")
		)
		(property "Value" "8.87k"
			(at 1.54 1.05 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/LCL_12V/12V_12A_LCL_1/")
		(sheetfile "12V_12A_LCL.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -0.82 0 180)
			(size 0.79 0.93)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 128 "Net-(R55-Pad1)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd rect
			(at 0.82 0 180)
			(size 0.79 0.93)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 42 "Net-(D1-K)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:RESC1508X55N"
		(layer "F.Cu")
		(at 256.85905 181.54195 180)
		(property "Reference" "R143"
			(at -0.1992 1.25 0)
			(layer "F.SilkS")
		)
		(property "Value" "0 Ohm"
			(at 1.54 1.07 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MF" "Stackpole Electronics Inc"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description_1" "0 Ohms Jumper 0.1W, 1/10W Chip Resistor 0603 (1608 Metric) Automotive AEC-Q200 Thick Film"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Package" "1508 Stackpole"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Price" "None"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SnapEDA_Link" "https://www.snapeda.com/parts/RMCF0603ZT0R00/Stackpole+Electronics/view-part/?ref=snap"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MP" "RMCF0603ZT0R00"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Purchase-URL" "https://www.snapeda.com/api/url_track_click_mouser/?unipart_id=3968849&manufacturer=Stackpole Electronics Inc&part_name=RMCF0603ZT0R00&search_term=rmcf0603zt0r00"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Availability" "In Stock"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Check_prices" "https://www.snapeda.com/parts/RMCF0603ZT0R00/Stackpole+Electronics/view-part/?ref=eda"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/Digital Systems/")
		(sheetfile "Digital_Systems.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -0.76 0 180)
			(size 0.9 0.97)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 155 "/Digital Systems/I2C0SDA")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd rect
			(at 0.76 0 180)
			(size 0.9 0.97)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 154 "Net-(U43-PB3{slash}I2C0SDA)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:RESC1508X55N"
		(layer "F.Cu")
		(at 92.777925 42.059375 90)
		(property "Reference" "R26"
			(at 3.517425 0.030325 90)
			(layer "F.SilkS")
		)
		(property "Value" "13.7k"
			(at 1.54 1.07 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Power_Connectors/")
		(sheetfile "Power_Connectors.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -0.76 0 90)
			(size 0.9 0.97)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 110 "Net-(R25-Pad2)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd rect
			(at 0.76 0 90)
			(size 0.9 0.97)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 303 "/GNDREF")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:RESC1508X55N"
		(layer "F.Cu")
		(at 225.86905 202.79195 180)
		(property "Reference" "R138"
			(at -0.21 -1.07 0)
			(layer "F.SilkS")
		)
		(property "Value" "0 Ohm"
			(at 1.54 1.07 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MF" "Stackpole Electronics Inc"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description_1" "0 Ohms Jumper 0.1W, 1/10W Chip Resistor 0603 (1608 Metric) Automotive AEC-Q200 Thick Film"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Package" "1508 Stackpole"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Price" "None"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SnapEDA_Link" "https://www.snapeda.com/parts/RMCF0603ZT0R00/Stackpole+Electronics/view-part/?ref=snap"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MP" "RMCF0603ZT0R00"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Purchase-URL" "https://www.snapeda.com/api/url_track_click_mouser/?unipart_id=3968849&manufacturer=Stackpole Electronics Inc&part_name=RMCF0603ZT0R00&search_term=rmcf0603zt0r00"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Availability" "In Stock"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Check_prices" "https://www.snapeda.com/parts/RMCF0603ZT0R00/Stackpole+Electronics/view-part/?ref=eda"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/Digital Systems/")
		(sheetfile "Digital_Systems.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -0.76 0 180)
			(size 0.9 0.97)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 304 "/Digital Systems/ADC1_CS")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd rect
			(at 0.76 0 180)
			(size 0.9 0.97)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 148 "Net-(U41-~{CS})")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:RESC1608X55N"
		(layer "F.Cu")
		(at 48.53905 166.29195 180)
		(property "Reference" "R61"
			(at -2.5192 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "8.87k"
			(at 1.54 1.05 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/LCL_12V/12V_12A_LCL_2/")
		(sheetfile "12V_12A_LCL.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -0.82 0 180)
			(size 0.79 0.93)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 129 "Net-(R61-Pad1)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd rect
			(at 0.82 0 180)
			(size 0.79 0.93)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 44 "Net-(D2-K)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:CAPC1608X90"
		(layer "F.Cu")
		(at 63.65905 215.62195)
		(descr "<b>CAPACITOR</b>")
		(property "Reference" "C19"
			(at 2.8992 -0.08 0)
			(layer "F.SilkS")
		)
		(property "Value" "0.1uF"
			(at 1.56646 1.20613 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "SMD 0603 MLCC capacitor, Alternate KiCad Library"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/LCL_12V/12V_12A_LCL_1/")
		(sheetfile "12V_12A_LCL.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -0.85 0)
			(size 1.1 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 7 "/LCL_12V/12V_12A_LCL_1/OPAMP_Minus")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd rect
			(at 0.85 0)
			(size 1.1 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 8 "Net-(Q1-B)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:1301.9314.24_SCH"
		(layer "F.Cu")
		(at 265.4388 194.273251)
		(tags "1301.9314.24 ")
		(property "Reference" "SW1"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "1301.9314.24"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "1301.9314.24"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "1301.9314.24_SCH")
		(sheetname "/Digital Systems/")
		(sheetfile "Digital_Systems.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -5 -2.250001)
			(size 2.1082 1.397)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 151 "Net-(R140-Pad2)")
			(pinfunction "1")
			(pintype "unspecified")
		)
		(pad "2" smd rect
			(at 5 -2.250001)
			(size 2.1082 1.397)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 212 "unconnected-(SW1-Pad2)")
			(pinfunction "2")
			(pintype "unspecified+no_connect")
		)
		(pad "3" smd rect
			(at -5 2.250001)
			(size 2.1082 1.397)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 213 "unconnected-(SW1-Pad3)")
			(pinfunction "3")
			(pintype "unspecified+no_connect")
		)
		(pad "4" smd rect
			(at 5 2.250001)
			(size 2.1082 1.397)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 303 "/GNDREF")
			(pinfunction "4")
			(pintype "unspecified")
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:QFP50P1200X1200X160-64N"
		(layer "F.Cu")
		(at 247.30905 189.29195)
		(property "Reference" "U43"
			(at -2.028675 -7.348325 0)
			(layer "F.SilkS")
		)
		(property "Value" "TM4C123GH6PMIR"
			(at 9.11261 7.37114 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DigiKey_Part_Number" "296-46360-1-ND"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SnapEDA_Link" "https://www.snapeda.com/parts/TM4C123GH6PMIR/Texas+Instruments/view-part/?ref=snap"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description_1" "32-bit Arm Cortex-M4F based MCU with 80 -MHz, 256 -KB Flash, 32 -KB RAM, 2 CAN, RTC, USB, 64-Pin"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Package" "LQFP-64 Texas Instruments"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Check_prices" "https://www.snapeda.com/parts/TM4C123GH6PMIR/Texas+Instruments/view-part/?ref=eda"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MF" "Texas Instruments"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MP" "TM4C123GH6PMIR"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER" "TEXAS instruments"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/Digital Systems/")
		(sheetfile "Digital_Systems.kicad_sch")
		(attr smd allow_soldermask_bridges)
		(pad "1" smd rect
			(at -5.7 -3.75)
			(size 1.5 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 159 "Net-(U43-PB6)")
			(pinfunction "PB6")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd rect
			(at -5.7 -3.25)
			(size 1.5 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 35 "/Digital Systems/3.3V+")
			(pinfunction "VDDA")
			(pintype "power_in")
			(solder_mask_margin 0.102)
		)
		(pad "3" smd rect
			(at -5.7 -2.75)
			(size 1.5 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 303 "/GNDREF")
			(pinfunction "GNDA")
			(pintype "power_in")
			(solder_mask_margin 0.102)
		)
		(pad "4" smd rect
			(at -5.7 -2.25)
			(size 1.5 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 303 "/GNDREF")
			(pinfunction "PB7")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "5" smd rect
			(at -5.7 -1.75)
			(size 1.5 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 169 "Net-(U43-PF4)")
			(pinfunction "PF4")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "6" smd rect
			(at -5.7 -1.25)
			(size 1.5 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 85 "/ADC_AIN0")
			(pinfunction "PE3")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "7" smd rect
			(at -5.7 -0.75)
			(size 1.5 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 80 "/ADC_AIN1")
			(pinfunction "PE2")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "8" smd rect
			(at -5.7 -0.25)
			(size 1.5 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 79 "/ADC_AIN2")
			(pinfunction "PE1")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "9" smd rect
			(at -5.7 0.25)
			(size 1.5 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 78 "/ADC_AIN3")
			(pinfunction "PE0")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "10" smd rect
			(at -5.7 0.75)
			(size 1.5 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 297 "unconnected-(U43-PD7-Pad10)")
			(pinfunction "PD7")
			(pintype "bidirectional+no_connect")
			(solder_mask_margin 0.102)
		)
		(pad "11" smd rect
			(at -5.7 1.25)
			(size 1.5 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 35 "/Digital Systems/3.3V+")
			(pinfunction "VDD@1")
			(pintype "power_in")
			(solder_mask_margin 0.102)
		)
		(pad "12" smd rect
			(at -5.7 1.75)
			(size 1.5 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 303 "/GNDREF")
			(pinfunction "GND@1")
			(pintype "power_in")
			(solder_mask_margin 0.102)
		)
		(pad "13" smd rect
			(at -5.7 2.25)
			(size 1.5 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 303 "/GNDREF")
			(pinfunction "PC7")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "14" smd rect
			(at -5.7 2.75)
			(size 1.5 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 303 "/GNDREF")
			(pinfunction "PC6")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "15" smd rect
			(at -5.7 3.25)
			(size 1.5 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 86 "/UART.Tx")
			(pinfunction "PC5")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "16" smd rect
			(at -5.7 3.75)
			(size 1.5 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 88 "/UART.Rx")
			(pinfunction "PC4")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "17" smd rect
			(at -3.75 5.7)
			(size 0.3 1.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 303 "/GNDREF")
			(pinfunction "PA0/U0RX")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "18" smd rect
			(at -3.25 5.7)
			(size 0.3 1.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 303 "/GNDREF")
			(pinfunction "PA1/U0TX")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "19" smd rect
			(at -2.75 5.7)
			(size 0.3 1.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 156 "Net-(U43-PA2{slash}SSI0CLK)")
			(pinfunction "PA2/SSI0CLK")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "20" smd rect
			(at -2.25 5.7)
			(size 0.3 1.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 157 "Net-(U43-PA3{slash}SSI0FSS)")
			(pinfunction "PA3/SSI0FSS")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "21" smd rect
			(at -1.75 5.7)
			(size 0.3 1.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 170 "/Digital Systems/SSI0Rx")
			(pinfunction "PA4/SSI0RX")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "22" smd rect
			(at -1.25 5.7)
			(size 0.3 1.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 158 "Net-(U43-PA5{slash}SSI0TX)")
			(pinfunction "PA5/SSI0TX")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "23" smd rect
			(at -0.75 5.7)
			(size 0.3 1.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 303 "/GNDREF")
			(pinfunction "PA6")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "24" smd rect
			(at -0.25 5.7)
			(size 0.3 1.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 303 "/GNDREF")
			(pinfunction "PA7")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "25" smd rect
			(at 0.25 5.7)
			(size 0.3 1.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 40 "Net-(U43-VDDC@1)")
			(pinfunction "VDDC@1")
			(pintype "power_in")
			(solder_mask_margin 0.102)
		)
		(pad "26" smd rect
			(at 0.75 5.7)
			(size 0.3 1.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 35 "/Digital Systems/3.3V+")
			(pinfunction "VDD@2")
			(pintype "power_in")
			(solder_mask_margin 0.102)
		)
		(pad "27" smd rect
			(at 1.25 5.7)
			(size 0.3 1.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 303 "/GNDREF")
			(pinfunction "GND@2")
			(pintype "power_in")
			(solder_mask_margin 0.102)
		)
		(pad "28" smd rect
			(at 1.75 5.7)
			(size 0.3 1.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 163 "Net-(U43-PF0)")
			(pinfunction "PF0")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "29" smd rect
			(at 2.25 5.7)
			(size 0.3 1.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 165 "Net-(U43-PF1)")
			(pinfunction "PF1")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "30" smd rect
			(at 2.75 5.7)
			(size 0.3 1.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 167 "Net-(U43-PF2)")
			(pinfunction "PF2")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "31" smd rect
			(at 3.25 5.7)
			(size 0.3 1.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 168 "Net-(U43-PF3)")
			(pinfunction "PF3")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "32" smd rect
			(at 3.75 5.7)
			(size 0.3 1.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 303 "/GNDREF")
			(pinfunction "~{WAKE}")
			(pintype "input")
			(solder_mask_margin 0.102)
		)
		(pad "33" smd rect
			(at 5.7 3.75)
			(size 1.5 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 298 "unconnected-(U43-~{HIB}-Pad33)")
			(pinfunction "~{HIB}")
			(pintype "output+no_connect")
			(solder_mask_margin 0.102)
		)
		(pad "34" smd rect
			(at 5.7 3.25)
			(size 1.5 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 303 "/GNDREF")
			(pinfunction "XOSC0")
			(pintype "input")
			(solder_mask_margin 0.102)
		)
		(pad "35" smd rect
			(at 5.7 2.75)
			(size 1.5 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 303 "/GNDREF")
			(pinfunction "GNDX")
			(pintype "power_in")
			(solder_mask_margin 0.102)
		)
		(pad "36" smd rect
			(at 5.7 2.25)
			(size 1.5 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 295 "unconnected-(U43-XOSC1-Pad36)")
			(pinfunction "XOSC1")
			(pintype "output+no_connect")
			(solder_mask_margin 0.102)
		)
		(pad "37" smd rect
			(at 5.7 1.75)
			(size 1.5 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 35 "/Digital Systems/3.3V+")
			(pinfunction "VBAT")
			(pintype "power_in")
			(solder_mask_margin 0.102)
		)
		(pad "38" smd rect
			(at 5.7 1.25)
			(size 1.5 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 36 "Net-(U43-~{RST})")
			(pinfunction "~{RST}")
			(pintype "input")
			(solder_mask_margin 0.102)
		)
		(pad "39" smd rect
			(at 5.7 0.75)
			(size 1.5 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 303 "/GNDREF")
			(pinfunction "GND@3")
			(pintype "power_in")
			(solder_mask_margin 0.102)
		)
		(pad "40" smd rect
			(at 5.7 0.25)
			(size 1.5 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 37 "Net-(U43-OSC0)")
			(pinfunction "OSC0")
			(pintype "input")
			(solder_mask_margin 0.102)
		)
		(pad "41" smd rect
			(at 5.7 -0.25)
			(size 1.5 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 172 "Net-(U43-OSC1)")
			(pinfunction "OSC1")
			(pintype "output")
			(solder_mask_margin 0.102)
		)
		(pad "42" smd rect
			(at 5.7 -0.75)
			(size 1.5 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 35 "/Digital Systems/3.3V+")
			(pinfunction "VDD@3")
			(pintype "power_in")
			(solder_mask_margin 0.102)
		)
		(pad "43" smd rect
			(at 5.7 -1.25)
			(size 1.5 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 84 "/USB.D-")
			(pinfunction "PD4")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "44" smd rect
			(at 5.7 -1.75)
			(size 1.5 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 81 "/USB.D+")
			(pinfunction "PD5")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "45" smd rect
			(at 5.7 -2.25)
			(size 1.5 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 83 "/USB.ID")
			(pinfunction "PB0/USB0ID")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "46" smd rect
			(at 5.7 -2.75)
			(size 1.5 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 82 "/USB.VBUS")
			(pinfunction "PB1/USB0VBUS")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "47" smd rect
			(at 5.7 -3.25)
			(size 1.5 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 153 "Net-(U43-PB2{slash}I2C0SCL)")
			(pinfunction "PB2/I2C0SCL")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "48" smd rect
			(at 5.7 -3.75)
			(size 1.5 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 154 "Net-(U43-PB3{slash}I2C0SDA)")
			(pinfunction "PB3/I2C0SDA")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "49" smd rect
			(at 3.75 -5.7)
			(size 0.3 1.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 74 "/JTAG.TDO")
			(pinfunction "PC3/TDO/DWO")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "50" smd rect
			(at 3.25 -5.7)
			(size 0.3 1.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 75 "/JTAG.TDI")
			(pinfunction "PC2/TDI")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "51" smd rect
			(at 2.75 -5.7)
			(size 0.3 1.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 76 "/JTAG.TMS")
			(pinfunction "PC1/TMS/SWDIO")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "52" smd rect
			(at 2.25 -5.7)
			(size 0.3 1.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 77 "/JTAG.TCK")
			(pinfunction "PC0/TCK/SWCLK")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "53" smd rect
			(at 1.75 -5.7)
			(size 0.3 1.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 161 "Net-(U43-PD6)")
			(pinfunction "PD6")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "54" smd rect
			(at 1.25 -5.7)
			(size 0.3 1.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 35 "/Digital Systems/3.3V+")
			(pinfunction "VDD@4")
			(pintype "power_in")
			(solder_mask_margin 0.102)
		)
		(pad "55" smd rect
			(at 0.75 -5.7)
			(size 0.3 1.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 303 "/GNDREF")
			(pinfunction "GND@4")
			(pintype "power_in")
			(solder_mask_margin 0.102)
		)
		(pad "56" smd rect
			(at 0.25 -5.7)
			(size 0.3 1.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 40 "Net-(U43-VDDC@1)")
			(pinfunction "VDDC@2")
			(pintype "power_in")
			(solder_mask_margin 0.102)
		)
		(pad "57" smd rect
			(at -0.25 -5.7)
			(size 0.3 1.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 303 "/GNDREF")
			(pinfunction "PB5")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "58" smd rect
			(at -0.75 -5.7)
			(size 0.3 1.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 303 "/GNDREF")
			(pinfunction "PB4")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "59" smd rect
			(at -1.25 -5.7)
			(size 0.3 1.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 296 "unconnected-(U43-PE4-Pad59)")
			(pinfunction "PE4")
			(pintype "bidirectional+no_connect")
			(solder_mask_margin 0.102)
		)
		(pad "60" smd rect
			(at -1.75 -5.7)
			(size 0.3 1.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 294 "unconnected-(U43-PE5-Pad60)")
			(pinfunction "PE5")
			(pintype "bidirectional+no_connect")
			(solder_mask_margin 0.102)
		)
		(pad "61" smd rect
			(at -2.25 -5.7)
			(size 0.3 1.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 303 "/GNDREF")
			(pinfunction "PD0")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "62" smd rect
			(at -2.75 -5.7)
			(size 0.3 1.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 303 "/GNDREF")
			(pinfunction "PD1")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "63" smd rect
			(at -3.25 -5.7)
			(size 0.3 1.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 303 "/GNDREF")
			(pinfunction "PD2")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "64" smd rect
			(at -3.75 -5.7)
			(size 0.3 1.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 303 "/GNDREF")
			(pinfunction "PD3")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:RESC1608X55N"
		(layer "F.Cu")
		(at 42.9078 59.9192 90)
		(property "Reference" "R94"
			(at -0.21 -1.05 90)
			(layer "F.SilkS")
		)
		(property "Value" "86.6k"
			(at 1.54 1.05 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/LCL_12V/12V_5A_LCL_2/")
		(sheetfile "12V_5A_LCL.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -0.82 0 90)
			(size 0.79 0.93)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 21 "Net-(Q8-B)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd rect
			(at 0.82 0 90)
			(size 0.79 0.93)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 22 "/LCL_12V/12V_5A_LCL_2/OPAMP_Minus")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:CAPC1608X90"
		(layer "F.Cu")
		(at 144.174041 61.633258 -90)
		(descr "<b>CAPACITOR</b>")
		(property "Reference" "C23"
			(at 2.658692 0.115791 90)
			(layer "F.SilkS")
		)
		(property "Value" "0.1uF"
			(at 1.56646 1.20613 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "SMD 0603 MLCC capacitor, Alternate KiCad Library"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/LCL_12V/12V_3A_LCL_1/")
		(sheetfile "12V_3A_LCL.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -0.85 0 270)
			(size 1.1 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 16 "/LCL_12V/12V_3A_LCL_1/OPAMP_Minus")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd rect
			(at 0.85 0 270)
			(size 1.1 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 15 "Net-(Q5-B)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:CAPC17595_90N_KEM"
		(layer "F.Cu")
		(at 247.60905 180.54195 90)
		(tags "C0603C335K9PACTU ")
		(property "Reference" "C39"
			(at 1.25 -1.5508 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "3.3uF"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://content.kemet.com/datasheets/KEM_C1006_X5R_SMD.pdf"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "CAPC17595_90N_KEM CAPC17595_90N_KEM-M CAPC17595_90N_KEM-L")
		(sheetname "/Digital Systems/")
		(sheetfile "Digital_Systems.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -0.727799 0 90)
			(size 1.005599 0.949998)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 40 "Net-(U43-VDDC@1)")
			(pintype "unspecified")
		)
		(pad "2" smd rect
			(at 0.727799 0 90)
			(size 1.005599 0.949998)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 303 "/GNDREF")
			(pintype "unspecified")
		)
		(zone
			(net 0)
			(net_name "")
			(layer "F.Cu")
			(hatch full 0.508)
			(connect_pads
				(clearance 0)
			)
			(min_thickness 0.254)
			(filled_areas_thickness no)
			(keepout
				(tracks not_allowed)
				(vias not_allowed)
				(pads allowed)
				(copperpour not_allowed)
				(footprints allowed)
			)
			(placement
				(enabled no)
				(sheetname "")
			)
			(fill
				(thermal_gap 0.508)
				(thermal_bridge_width 0.508)
			)
			(polygon
				(pts
					(xy 247.184851 180.71615) (xy 247.184851 180.36775) (xy 248.033249 180.36775) (xy 248.033249 180.71615)
				)
			)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:RESC1508X55N"
		(layer "F.Cu")
		(at 87.607925 60.519375 90)
		(property "Reference" "R92"
			(at -2.522575 -0.049675 90)
			(layer "F.SilkS")
		)
		(property "Value" "54.9k"
			(at 1.54 1.069999 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/LCL_12V/12V_5A_LCL_1/")
		(sheetfile "12V_5A_LCL.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -0.76 0 90)
			(size 0.9 0.97)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 134 "Net-(R91-Pad1)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd rect
			(at 0.76 0 90)
			(size 0.9 0.97)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 55 "Net-(D7-K)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:Terminal Block 691137710002"
		(layer "F.Cu")
		(at 248.10905 42.54195 180)
		(property "Reference" "J13"
			(at 0 -5.135 0)
			(layer "F.SilkS")
		)
		(property "Value" "691137710002"
			(at 4.12 5.365 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/Power_Connectors/")
		(sheetfile "Power_Connectors.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole circle
			(at -2.5 0 180)
			(size 1.95 1.95)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 303 "/GNDREF")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" thru_hole circle
			(at 2.5 0 180)
			(size 1.95 1.95)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 59 "/LCL_5.6A3")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:RESC1508X55N"
		(layer "F.Cu")
		(at 225.35905 199.54195)
		(property "Reference" "R154"
			(at 2.6992 -0.25 0)
			(layer "F.SilkS")
		)
		(property "Value" "0 Ohm"
			(at 1.54 1.07 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MF" "Stackpole Electronics Inc"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description_1" "0 Ohms Jumper 0.1W, 1/10W Chip Resistor 0603 (1608 Metric) Automotive AEC-Q200 Thick Film"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Package" "1508 Stackpole"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Price" "None"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SnapEDA_Link" "https://www.snapeda.com/parts/RMCF0603ZT0R00/Stackpole+Electronics/view-part/?ref=snap"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MP" "RMCF0603ZT0R00"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Purchase-URL" "https://www.snapeda.com/api/url_track_click_mouser/?unipart_id=3968849&manufacturer=Stackpole Electronics Inc&part_name=RMCF0603ZT0R00&search_term=rmcf0603zt0r00"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Availability" "In Stock"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Check_prices" "https://www.snapeda.com/parts/RMCF0603ZT0R00/Stackpole+Electronics/view-part/?ref=eda"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/Digital Systems/")
		(sheetfile "Digital_Systems.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -0.76 0)
			(size 0.9 0.97)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 171 "Net-(U41-DOUT)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd rect
			(at 0.76 0)
			(size 0.9 0.97)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 170 "/Digital Systems/SSI0Rx")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:SOD3716X135N"
		(layer "F.Cu")
		(at 52.00905 237.29195 180)
		(descr "sod-123-ren1")
		(tags "Diode")
		(property "Reference" "D13"
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "D"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Diode"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Device" "D"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TO-???* *_Diode_* *SingleDiode* D_*")
		(sheetname "/LCL_9_and_3-3/9V_2A_LCL_1/")
		(sheetfile "9V_2A_LCL.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.65 0 270)
			(size 0.75 1.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 67 "Net-(D13-K)")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.65 0 270)
			(size 0.75 1.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 66 "/LCL_MIXED.9V2A")
			(pinfunction "A")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "1N4150W-E3-18.stp"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "EPS_Footprints:RESC1508X55N"
		(layer "F.Cu")
		(at 267.86905 179.79195 180)
		(property "Reference" "R157"
			(at -0.21 -1.07 0)
			(layer "F.SilkS")
		)
		(property "Value" "165"
			(at 1.54 1.07 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Digital Systems/")
		(sheetfile "Digital_Systems.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -0.76 0 180)
			(size 0.9 0.97)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 303 "/GNDREF")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd rect
			(at 0.76 0 180)
			(size 0.9 0.97)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 89 "Net-(LED1-Pad1)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:RESC1508X55N"
		(layer "F.Cu")
		(at 257.10905 195.29195)
		(property "Reference" "R141"
			(at -0.3008 1.25 0)
			(layer "F.SilkS")
		)
		(property "Value" "10k"
			(at 1.54 1.07 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Digital Systems/")
		(sheetfile "Digital_Systems.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -0.76 0)
			(size 0.9 0.97)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 36 "Net-(U43-~{RST})")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd rect
			(at 0.76 0)
			(size 0.9 0.97)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 73 "/JTAG.RESET")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:RESC1508X55N"
		(layer "F.Cu")
		(at 198.10905 244.54195 -90)
		(property "Reference" "R185"
			(at -0.21 -1.07 90)
			(layer "F.SilkS")
		)
		(property "Value" "4.7k"
			(at 1.54 1.07 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Digital_Connectors/")
		(sheetfile "Digital_Connectors.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -0.76 0 270)
			(size 0.9 0.97)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 72 "/DC_POS.3.3V")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd rect
			(at 0.76 0 270)
			(size 0.9 0.97)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 78 "/ADC_AIN3")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:DBV6"
		(layer "F.Cu")
		(at 234.309051 209.90955 90)
		(tags "TMP121AIDBVR ")
		(property "Reference" "U46"
			(at 0 2.499199 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "TMP121AIDBVR"
			(at -0.24 -0.75 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.ti.com/lit/gpn/tmp121"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "DBV6 DBV6-M DBV6-L")
		(sheetname "/Digital Systems/")
		(sheetfile "Digital_Systems.kicad_sch")
		(attr smd)
		(fp_text user "*"
			(at -0.6324 -2.750801 90)
			(layer "F.SilkS")
		)
		(fp_text user "*"
			(at -1.3716 -2.6518 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(fp_text user "*"
			(at -1.3716 -2.6518 90)
			(layer "F.Fab")
		)
		(fp_text user "*"
			(at -1.3716 -2.6518 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.1176 -0.950001 90)
			(size 1.4732 0.5588)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 302 "unconnected-(U46-NC-Pad1)")
			(pinfunction "NC")
			(pintype "unspecified+no_connect")
		)
		(pad "2" smd rect
			(at -1.1176 0 90)
			(size 1.4732 0.5588)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 303 "/GNDREF")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "3" smd rect
			(at -1.1176 0.950001 90)
			(size 1.4732 0.5588)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 35 "/Digital Systems/3.3V+")
			(pinfunction "V+")
			(pintype "power_in")
		)
		(pad "4" smd rect
			(at 1.1176 0.950001 90)
			(size 1.4732 0.5588)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 209 "Net-(U46-SCL)")
			(pinfunction "SCL")
			(pintype "unspecified")
		)
		(pad "5" smd rect
			(at 1.1176 0 90)
			(size 1.4732 0.5588)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 208 "Net-(U46-*CS)")
			(pinfunction "*CS")
			(pintype "unspecified")
		)
		(pad "6" smd rect
			(at 1.1176 -0.950001 90)
			(size 1.4732 0.5588)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 207 "Net-(U46-SO)")
			(pinfunction "SO")
			(pintype "unspecified")
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:BAQ33GS08"
		(layer "F.Cu")
		(at 43.60905 172.66695 90)
		(descr "MiniMELF (SOD-80)")
		(tags "Zener Diode")
		(property "Reference" "ZD2"
			(at 4.625 0 90)
			(layer "F.SilkS")
		)
		(property "Value" "D_Zener"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Zener diode"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Library" "TZM5240B-GS08.txt"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Name" "TZM5240B-GS08"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Device" "D"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" "1=A 2=K"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TO-???* *_Diode_* *SingleDiode* D_*")
		(sheetname "/LCL_12V/12V_12A_LCL_2/")
		(sheetfile "12V_12A_LCL.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.875 0 90)
			(size 1.25 2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 10 "/LCL_12V/12V_12A_LCL_2/OPAMP_Minus")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.875 0 90)
			(size 1.25 2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 44 "Net-(D2-K)")
			(pinfunction "A")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "TZM5224B-GS08.stp"
			(offset
				(xyz 0 0 0.7999999999)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "EPS_Footprints:RESC1508X55N"
		(layer "F.Cu")
		(at 53.8078 59.9192 90)
		(property "Reference" "R98"
			(at -2.37275 -0.24955 90)
			(layer "F.SilkS")
		)
		(property "Value" "54.9k"
			(at 1.54 1.07 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/LCL_12V/12V_5A_LCL_2/")
		(sheetfile "12V_5A_LCL.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -0.76 0 90)
			(size 0.9 0.97)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 135 "Net-(R97-Pad1)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd rect
			(at 0.76 0 90)
			(size 0.9 0.97)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 56 "Net-(D8-K)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:RESC1608X55N"
		(layer "F.Cu")
		(at 57.35905 247.86195 -90)
		(property "Reference" "R126"
			(at 1.68 -1.1992 90)
			(layer "F.SilkS")
		)
		(property "Value" "86.6k"
			(at 1.54 1.05 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/LCL_9_and_3-3/9V_2A_LCL_1/")
		(sheetfile "9V_2A_LCL.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -0.82 0 270)
			(size 0.79 0.93)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 67 "Net-(D13-K)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd rect
			(at 0.82 0 270)
			(size 0.79 0.93)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 32 "/LCL_9_and_3-3/9V_2A_LCL_1/OPAMP_Minus")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:RESC1508X55N"
		(layer "F.Cu")
		(at 92.857925 45.269375 90)
		(property "Reference" "R25"
			(at -1.022575 -1.299675 90)
			(layer "F.SilkS")
		)
		(property "Value" "100k"
			(at 1.54 1.07 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Power_Connectors/")
		(sheetfile "Power_Connectors.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -0.76 0 90)
			(size 0.9 0.97)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 54 "/LCL_12.5A1")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd rect
			(at 0.76 0 90)
			(size 0.9 0.97)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 110 "Net-(R25-Pad2)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:RESC1608X55N"
		(layer "F.Cu")
		(at 63.50855 151.52245 180)
		(property "Reference" "R64"
			(at -0.21 -1.05 0)
			(layer "F.SilkS")
		)
		(property "Value" "86.6k"
			(at 1.54 1.049999 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/LCL_12V/12V_12A_LCL_3/")
		(sheetfile "12V_12A_LCL.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -0.82 0 180)
			(size 0.79 0.93)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 12 "Net-(Q3-B)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd rect
			(at 0.82 0 180)
			(size 0.79 0.93)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 11 "/LCL_12V/12V_12A_LCL_3/OPAMP_Minus")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:RES_TLRP3A30DR018FTE_TEC"
		(layer "F.Cu")
		(at 131.82085 50.22435 180)
		(tags "TLRP3A30DR018FTE ")
		(property "Reference" "R81"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "0.01"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/LCL_12V/12V_3A_LCL_2/")
		(sheetfile "12V_3A_LCL.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -2.8321 0 180)
			(size 1.397 3.4544)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 5 "/DC_POS.12V")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 2.8321 0 180)
			(size 1.397 3.4544)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 18 "/LCL_12V/12V_3A_LCL_2/OPAMP_Minus")
			(pintype "passive")
		)
		(zone
			(net 0)
			(net_name "")
			(layer "F.Cu")
			(hatch full 0.508)
			(connect_pads
				(clearance 0)
			)
			(min_thickness 0.254)
			(filled_areas_thickness no)
			(keepout
				(tracks not_allowed)
				(vias not_allowed)
				(pads allowed)
				(copperpour not_allowed)
				(footprints allowed)
			)
			(placement
				(enabled no)
				(sheetname "")
			)
			(fill
				(thermal_gap 0.508)
				(thermal_bridge_width 0.508)
			)
			(polygon
				(pts
					(xy 133.90365 51.90075) (xy 129.73805 51.90075) (xy 129.73805 48.54795) (xy 133.90365 48.54795)
				)
			)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:RESC1508X55N"
		(layer "F.Cu")
		(at 254.35905 43.04195 90)
		(property "Reference" "R38"
			(at 1.5 1.1992 90)
			(layer "F.SilkS")
		)
		(property "Value" "37.5k (37.4k)"
			(at 1.54 1.07 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Power_Connectors/")
		(sheetfile "Power_Connectors.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -0.76 0 90)
			(size 0.9 0.97)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 118 "Net-(R37-Pad2)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd rect
			(at 0.76 0 90)
			(size 0.9 0.97)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 303 "/GNDREF")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:TO-263AB_SUM"
		(layer "F.Cu")
		(at 272.10905 51.79195 90)
		(tags "SUM110P06-08L-E3 ")
		(property "Reference" "U34"
			(at 4.25 -6.3008 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "SUM110P06-08L-E3"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "SUM110P06-08L-E3"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TO-263AB_SUM TO-263AB_SUM-M TO-263AB_SUM-L")
		(sheetname "/LCL_5V/5V_6A_LCL_4/")
		(sheetfile "5V_6A_LCL.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(fp_text user "*"
			(at -2.539999 5.2705 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(fp_text user "*"
			(at -2.539999 5.2705 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -2.54 8.8773 90)
			(size 0.9906 3.2004)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 65 "Net-(D12-K)")
			(pinfunction "G")
			(pintype "input")
		)
		(pad "2" smd rect
			(at 0 0.0508 90)
			(size 10.414 11.4554)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 30 "/LCL_5V/5V_6A_LCL_4/OPAMP_Minus")
			(pinfunction "D")
			(pintype "input")
		)
		(pad "3" smd rect
			(at 2.54 8.8773 90)
			(size 0.9906 3.2004)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 64 "/LCL_5.6A4")
			(pinfunction "S")
			(pintype "input")
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:DIP762W50P254L730H410Q6"
		(layer "F.Cu")
		(at 193.99825 61.33195 180)
		(property "Reference" "U31"
			(at -7.41 -9.94 0)
			(layer "F.SilkS")
		)
		(property "Value" "CNY17-1"
			(at -0.21 9.94 0)
			(layer "Dwgs.User")
		)
		(property "Datasheet" "http://www.vishay.com/docs/83606/cny17.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "DC Optocoupler Base Connected, Vce 70V, CTR 40-80%, Viso 5000V (RMS), DIP6"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "DIP*W7.62mm* DIP*W10.16mm* SMDIP*W9.53mm*")
		(sheetname "/LCL_5V/5V_6A_LCL_1/")
		(sheetfile "5V_6A_LCL.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole rect
			(at -3.81 -2.54 180)
			(size 1.4 1.4)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 195 "/LCL_CTRL9")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" thru_hole circle
			(at -3.81 0 180)
			(size 1.4 1.4)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 303 "/GNDREF")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "3" thru_hole circle
			(at -3.81 2.54 180)
			(size 1.4 1.4)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 276 "unconnected-(U31-NC-Pad3)")
			(pinfunction "NC")
			(pintype "no_connect")
			(solder_mask_margin 0.102)
		)
		(pad "4" thru_hole circle
			(at 3.81 2.54 180)
			(size 1.4 1.4)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 303 "/GNDREF")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "5" thru_hole circle
			(at 3.81 0 180)
			(size 1.4 1.4)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 137 "Net-(R109-Pad1)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "6" thru_hole circle
			(at 3.81 -2.54 180)
			(size 1.4 1.4)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 275 "unconnected-(U31-Pad6)")
			(pintype "passive+no_connect")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:RESC1508X55N"
		(layer "F.Cu")
		(at 261.85905 183.29195)
		(property "Reference" "R165"
			(at 2.6992 0.75 0)
			(layer "F.SilkS")
		)
		(property "Value" "10k"
			(at 1.54 1.07 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Digital Systems/")
		(sheetfile "Digital_Systems.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -0.76 0)
			(size 0.9 0.97)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 152 "/Digital Systems/I2C0SCL")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd rect
			(at 0.76 0)
			(size 0.9 0.97)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 35 "/Digital Systems/3.3V+")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:CAPC1608X90"
		(layer "F.Cu")
		(at 235.35905 213.04195 180)
		(descr "<b>CAPACITOR</b>")
		(property "Reference" "C48"
			(at -0.235423 -1.237214 0)
			(layer "F.SilkS")
		)
		(property "Value" "0.1uF"
			(at 1.56646 1.20613 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "SMD 0603 MLCC capacitor, Alternate KiCad Library"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/Digital Systems/")
		(sheetfile "Digital_Systems.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -0.85 0 180)
			(size 1.1 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 35 "/Digital Systems/3.3V+")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd rect
			(at 0.85 0 180)
			(size 1.1 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 303 "/GNDREF")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:AMPHENOL_20021112-00010T4LF"
		(layer "F.Cu")
		(at 276.55905 166.58195 90)
		(property "Reference" "J17"
			(at 0 -7.62 90)
			(layer "F.SilkS")
		)
		(property "Value" "20021112-00010T4LF"
			(at 13.97 -5.715 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DigiKey_Part_Number" "609-5926-ND"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SnapEDA_Link" "https://www.snapeda.com/parts/20021112-00010T4LF/Amphenol/view-part/?ref=snap"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MAXIMUM_PACKAGE_HEIGHT" "3.63mm"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Package" "None"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Check_prices" "https://www.snapeda.com/parts/20021112-00010T4LF/Amphenol/view-part/?ref=eda"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "STANDARD" "Manufacturer Recommendations"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTREV" "G"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MF" "Amphenol FCI"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MP" "20021112-00010T4LF"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description_1" "Minitek127, Board to Board connector, Unshrouded Right Angled Header, Through Hole, Double Row, 10 Positions, 1.27 mm (.050in) Pitch."
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER" "Amphenol"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/Digital_Connectors/")
		(sheetfile "Digital_Connectors.kicad_sch")
		(attr through_hole allow_soldermask_bridges)
		(pad "1" thru_hole rect
			(at -2.54 -2.45 90)
			(size 1.1 1.1)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 72 "/DC_POS.3.3V")
			(pinfunction "VRef")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" thru_hole circle
			(at -2.54 -3.72 90)
			(size 1.1 1.1)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 76 "/JTAG.TMS")
			(pinfunction "TMS")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "3" thru_hole circle
			(at -1.27 -2.45 90)
			(size 1.1 1.1)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 303 "/GNDREF")
			(pinfunction "GND")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "4" thru_hole circle
			(at -1.27 -3.72 90)
			(size 1.1 1.1)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 77 "/JTAG.TCK")
			(pinfunction "TCK")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "5" thru_hole circle
			(at 0 -2.45 90)
			(size 1.1 1.1)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 303 "/GNDREF")
			(pinfunction "GND")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "6" thru_hole circle
			(at 0 -3.72 90)
			(size 1.1 1.1)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 74 "/JTAG.TDO")
			(pinfunction "TDO")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "7" thru_hole circle
			(at 1.27 -2.45 90)
			(size 1.1 1.1)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 303 "/GNDREF")
			(pinfunction "GND")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "8" thru_hole circle
			(at 1.27 -3.72 90)
			(size 1.1 1.1)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 75 "/JTAG.TDI")
			(pinfunction "TDI")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "9" thru_hole circle
			(at 2.54 -2.45 90)
			(size 1.1 1.1)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 303 "/GNDREF")
			(pinfunction "GND")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "10" thru_hole circle
			(at 2.54 -3.72 90)
			(size 1.1 1.1)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 73 "/JTAG.RESET")
			(pinfunction "nRESET")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:RES_TLRP3A30DR018FTE_TEC"
		(layer "F.Cu")
		(at 99.275825 50.019375 180)
		(tags "TLRP3A30DR018FTE ")
		(property "Reference" "R87"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "0.01"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/LCL_12V/12V_5A_LCL_1/")
		(sheetfile "12V_5A_LCL.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -2.8321 0 180)
			(size 1.397 3.4544)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 5 "/DC_POS.12V")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 2.8321 0 180)
			(size 1.397 3.4544)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 19 "/LCL_12V/12V_5A_LCL_1/OPAMP_Minus")
			(pintype "passive")
		)
		(zone
			(net 0)
			(net_name "")
			(layer "F.Cu")
			(hatch full 0.508)
			(connect_pads
				(clearance 0)
			)
			(min_thickness 0.254)
			(filled_areas_thickness no)
			(keepout
				(tracks not_allowed)
				(vias not_allowed)
				(pads allowed)
				(copperpour not_allowed)
				(footprints allowed)
			)
			(placement
				(enabled no)
				(sheetname "")
			)
			(fill
				(thermal_gap 0.508)
				(thermal_bridge_width 0.508)
			)
			(polygon
				(pts
					(xy 101.358625 51.695775) (xy 97.193025 51.695775) (xy 97.193025 48.342975) (xy 101.358625 48.342975)
				)
			)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:RESC1508X55N"
		(layer "F.Cu")
		(at 186.60825 60.61695 90)
		(property "Reference" "R110"
			(at -2.675 -0.05 90)
			(layer "F.SilkS")
		)
		(property "Value" "54.9k"
			(at 1.54 1.07 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/LCL_5V/5V_6A_LCL_1/")
		(sheetfile "5V_6A_LCL.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -0.76 0 90)
			(size 0.9 0.97)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 137 "Net-(R109-Pad1)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd rect
			(at 0.76 0 90)
			(size 0.9 0.97)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 60 "Net-(D10-K)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:RES_TLRP3A30DR018FTE_TEC"
		(layer "F.Cu")
		(at 65.4757 49.4192 180)
		(tags "TLRP3A30DR018FTE ")
		(property "Reference" "R93"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "0.01"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/LCL_12V/12V_5A_LCL_2/")
		(sheetfile "12V_5A_LCL.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -2.8321 0 180)
			(size 1.397 3.4544)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 5 "/DC_POS.12V")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 2.8321 0 180)
			(size 1.397 3.4544)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 22 "/LCL_12V/12V_5A_LCL_2/OPAMP_Minus")
			(pintype "passive")
		)
		(zone
			(net 0)
			(net_name "")
			(layer "F.Cu")
			(hatch full 0.508)
			(connect_pads
				(clearance 0)
			)
			(min_thickness 0.254)
			(filled_areas_thickness no)
			(keepout
				(tracks not_allowed)
				(vias not_allowed)
				(pads allowed)
				(copperpour not_allowed)
				(footprints allowed)
			)
			(placement
				(enabled no)
				(sheetname "")
			)
			(fill
				(thermal_gap 0.508)
				(thermal_bridge_width 0.508)
			)
			(polygon
				(pts
					(xy 67.5585 51.0956) (xy 63.3929 51.0956) (xy 63.3929 47.7428) (xy 67.5585 47.7428)
				)
			)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:RESC1508X55N"
		(layer "F.Cu")
		(at 236.60905 244.79195 -90)
		(property "Reference" "R188"
			(at -0.21 -1.07 90)
			(layer "F.SilkS")
		)
		(property "Value" "4.7k"
			(at 1.54 1.07 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Digital_Connectors/")
		(sheetfile "Digital_Connectors.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -0.76 0 270)
			(size 0.9 0.97)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 72 "/DC_POS.3.3V")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd rect
			(at 0.76 0 270)
			(size 0.9 0.97)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 85 "/ADC_AIN0")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:RESC1508X55N"
		(layer "F.Cu")
		(at 238.10905 187.29195)
		(property "Reference" "R153"
			(at -2.8008 -1.213 0)
			(layer "F.SilkS")
		)
		(property "Value" "22"
			(at 1.54 1.07 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Digital Systems/")
		(sheetfile "Digital_Systems.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -0.76 0)
			(size 0.9 0.97)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 143 "/Digital Systems/ADC1_CNVST")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd rect
			(at 0.76 0)
			(size 0.9 0.97)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 169 "Net-(U43-PF4)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:CAPC1608X90"
		(layer "F.Cu")
		(at 78.382925 60.519375 -90)
		(descr "<b>CAPACITOR</b>")
		(property "Reference" "C25"
			(at 2.772575 0.824675 90)
			(layer "F.SilkS")
		)
		(property "Value" "0.1uF"
			(at 1.56646 1.20613 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "SMD 0603 MLCC capacitor, Alternate KiCad Library"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/LCL_12V/12V_5A_LCL_1/")
		(sheetfile "12V_5A_LCL.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -0.85 0 270)
			(size 1.1 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 19 "/LCL_12V/12V_5A_LCL_1/OPAMP_Minus")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd rect
			(at 0.85 0 270)
			(size 1.1 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 20 "Net-(Q7-B)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:Terminal Block 691137710002"
		(layer "F.Cu")
		(at 226.85905 250.79195)
		(property "Reference" "J20"
			(at 0 -5.135 0)
			(layer "F.SilkS")
		)
		(property "Value" "691137710002"
			(at 4.12 5.365 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/Digital_Connectors/")
		(sheetfile "Digital_Connectors.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole circle
			(at -2.5 0)
			(size 1.95 1.95)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 80 "/ADC_AIN1")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" thru_hole circle
			(at 2.5 0)
			(size 1.95 1.95)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 303 "/GNDREF")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:RESC1608X55N"
		(layer "F.Cu")
		(at 63.95855 140.44245 180)
		(property "Reference" "R67"
			(at -2.3497 -0.0995 0)
			(layer "F.SilkS")
		)
		(property "Value" "8.87k"
			(at 1.54 1.049999 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/LCL_12V/12V_12A_LCL_3/")
		(sheetfile "12V_12A_LCL.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -0.82 0 180)
			(size 0.79 0.93)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 130 "Net-(R67-Pad1)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd rect
			(at 0.82 0 180)
			(size 0.79 0.93)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 46 "Net-(D3-K)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:RESC1508X55N"
		(layer "F.Cu")
		(at 234.10905 218.29195)
		(property "Reference" "R166"
			(at -0.21 -1.25 0)
			(layer "F.SilkS")
		)
		(property "Value" "100"
			(at 1.54 1.07 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Digital Systems/")
		(sheetfile "Digital_Systems.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -0.76 0)
			(size 0.9 0.97)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 178 "/LCL_CTRL1")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd rect
			(at 0.76 0)
			(size 0.9 0.97)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 179 "Net-(U45-P0_0)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:RESC1508X55N"
		(layer "F.Cu")
		(at 236.10905 205.78195 -90)
		(property "Reference" "R184"
			(at -0.21 -1.07 90)
			(layer "F.SilkS")
		)
		(property "Value" "470"
			(at 1.54 1.07 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Digital Systems/")
		(sheetfile "Digital_Systems.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -0.76 0 270)
			(size 0.9 0.97)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 147 "/Digital Systems/SSI0CLK")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd rect
			(at 0.76 0 270)
			(size 0.9 0.97)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 209 "Net-(U46-SCL)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:RESC1608X55N"
		(layer "F.Cu")
		(at 110.40295 61.29435 90)
		(property "Reference" "R82"
			(at -2.4976 -0.0947 90)
			(layer "F.SilkS")
		)
		(property "Value" "86.6k"
			(at 1.54 1.05 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/LCL_12V/12V_3A_LCL_2/")
		(sheetfile "12V_3A_LCL.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -0.82 0 90)
			(size 0.79 0.93)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 17 "Net-(Q6-B)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd rect
			(at 0.82 0 90)
			(size 0.79 0.93)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 18 "/LCL_12V/12V_3A_LCL_2/OPAMP_Minus")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:RESC1508X55N"
		(layer "F.Cu")
		(at 227.85905 193.48695 180)
		(property "Reference" "R156"
			(at -0.21 -1.07 0)
			(layer "F.SilkS")
		)
		(property "Value" "10k"
			(at 1.54 1.07 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Digital Systems/")
		(sheetfile "Digital_Systems.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -0.76 0 180)
			(size 0.9 0.97)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 303 "/GNDREF")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd rect
			(at 0.76 0 180)
			(size 0.9 0.97)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 39 "Net-(U44-REF)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:HIROSE_ZX62-AB-5PA_31_"
		(layer "F.Cu")
		(at 276.85905 188.04195 90)
		(property "Reference" "J21"
			(at -1.975 -6.905 90)
			(layer "F.SilkS")
		)
		(property "Value" "ZX62-AB-5PA_31_"
			(at 5.82 8.475 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DigiKey_Part_Number" "H125279CT-ND"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SnapEDA_Link" "https://www.snapeda.com/parts/ZX62-AB-5PA(31)/Hirose/view-part/?ref=snap"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MAXIMUM_PACKAGE_HEIGHT" "3.00mm"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Package" "None"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Check_prices" "https://www.snapeda.com/parts/ZX62-AB-5PA(31)/Hirose/view-part/?ref=eda"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "STANDARD" "Manufacturer Recommendations"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTREV" "Jan 1, 2022"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MF" "Hirose Electric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MP" "ZX62-AB-5PA(31)"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description_1" "USB - micro AB USB 2.0 Receptacle Connector 5 Position Surface Mount, Right Angle"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER" "Hirose"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/Digital_Connectors/")
		(sheetfile "Digital_Connectors.kicad_sch")
		(attr smd)
		(fp_text user "PCB Edge"
			(at 6 1 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.3 -2.675 90)
			(size 0.4 1.35)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 82 "/USB.VBUS")
			(pinfunction "VCC")
			(pintype "power_in")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd rect
			(at -0.65 -2.675 90)
			(size 0.4 1.35)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 84 "/USB.D-")
			(pinfunction "D-")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "3" smd rect
			(at 0 -2.675 90)
			(size 0.4 1.35)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 81 "/USB.D+")
			(pinfunction "D+")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "4" smd rect
			(at 0.65 -2.675 90)
			(size 0.4 1.35)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 83 "/USB.ID")
			(pinfunction "ID")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "5" smd rect
			(at 1.3 -2.675 90)
			(size 0.4 1.35)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 303 "/GNDREF")
			(pinfunction "GND")
			(pintype "power_in")
			(solder_mask_margin 0.102)
		)
		(pad "S1" smd rect
			(at -3.1 -2.55 90)
			(size 2.1 1.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 303 "/GNDREF")
			(pinfunction "SHIELD")
			(pintype "power_in")
			(solder_mask_margin 0.102)
		)
		(pad "S2" smd rect
			(at 3.1 -2.55 90)
			(size 2.1 1.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 303 "/GNDREF")
			(pinfunction "SHIELD")
			(pintype "power_in")
			(solder_mask_margin 0.102)
		)
		(pad "S3" smd rect
			(at -4 0 90)
			(size 1.8 1.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 303 "/GNDREF")
			(pinfunction "SHIELD")
			(pintype "power_in")
			(solder_mask_margin 0.102)
		)
		(pad "S4" smd rect
			(at -1.2 0 90)
			(size 1.9 1.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 303 "/GNDREF")
			(pinfunction "SHIELD")
			(pintype "power_in")
			(solder_mask_margin 0.102)
		)
		(pad "S5" smd rect
			(at 1.2 0 90)
			(size 1.9 1.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 303 "/GNDREF")
			(pinfunction "SHIELD")
			(pintype "power_in")
			(solder_mask_margin 0.102)
		)
		(pad "S6" smd rect
			(at 4 0 90)
			(size 1.8 1.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 303 "/GNDREF")
			(pinfunction "SHIELD")
			(pintype "power_in")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:RESC1508X55N"
		(layer "F.Cu")
		(at 211.35905 244.54195 -90)
		(property "Reference" "R186"
			(at -0.21 -1.07 90)
			(layer "F.SilkS")
		)
		(property "Value" "4.7k"
			(at 1.54 1.07 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Digital_Connectors/")
		(sheetfile "Digital_Connectors.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -0.76 0 270)
			(size 0.9 0.97)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 72 "/DC_POS.3.3V")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd rect
			(at 0.76 0 270)
			(size 0.9 0.97)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 79 "/ADC_AIN2")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:RESC1508X55N"
		(layer "F.Cu")
		(at 223.35905 46.06195 90)
		(property "Reference" "R35"
			(at -0.98 -1.07 90)
			(layer "F.SilkS")
		)
		(property "Value" "100k"
			(at 1.54 1.07 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Power_Connectors/")
		(sheetfile "Power_Connectors.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -0.76 0 90)
			(size 0.9 0.97)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 63 "/LCL_5.6A2")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd rect
			(at 0.76 0 90)
			(size 0.9 0.97)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 117 "Net-(R35-Pad2)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:RESC1608X55N"
		(layer "F.Cu")
		(at 51.09905 174.94195)
		(property "Reference" "R60"
			(at 2.4592 -0.15 0)
			(layer "F.SilkS")
		)
		(property "Value" "86.6k"
			(at 1.54 1.05 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/LCL_12V/12V_12A_LCL_2/")
		(sheetfile "12V_12A_LCL.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -0.82 0)
			(size 0.79 0.93)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 44 "Net-(D2-K)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd rect
			(at 0.82 0)
			(size 0.79 0.93)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 10 "/LCL_12V/12V_12A_LCL_2/OPAMP_Minus")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:RES_TLRP3A30DR018FTE_TEC"
		(layer "F.Cu")
		(at 49.35905 229.70985 -90)
		(tags "TLRP3A30DR018FTE ")
		(property "Reference" "R123"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "0.01"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/LCL_9_and_3-3/9V_2A_LCL_1/")
		(sheetfile "9V_2A_LCL.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -2.8321 0 270)
			(size 1.397 3.4544)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 6 "/DC_POS.9V")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 2.8321 0 270)
			(size 1.397 3.4544)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 32 "/LCL_9_and_3-3/9V_2A_LCL_1/OPAMP_Minus")
			(pintype "passive")
		)
		(zone
			(net 0)
			(net_name "")
			(layer "F.Cu")
			(hatch full 0.508)
			(connect_pads
				(clearance 0)
			)
			(min_thickness 0.254)
			(filled_areas_thickness no)
			(keepout
				(tracks not_allowed)
				(vias not_allowed)
				(pads allowed)
				(copperpour not_allowed)
				(footprints allowed)
			)
			(placement
				(enabled no)
				(sheetname "")
			)
			(fill
				(thermal_gap 0.508)
				(thermal_bridge_width 0.508)
			)
			(polygon
				(pts
					(xy 51.03545 227.62705) (xy 51.03545 231.79265) (xy 47.68265 231.79265) (xy 47.68265 227.62705)
				)
			)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:RESC1608X55N"
		(layer "F.Cu")
		(at 152.924041 62.133258 90)
		(property "Reference" "R79"
			(at -2.408692 -0.115791 90)
			(layer "F.SilkS")
		)
		(property "Value" "8.87k"
			(at 1.54 1.049999 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/LCL_12V/12V_3A_LCL_1/")
		(sheetfile "12V_3A_LCL.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -0.82 0 90)
			(size 0.79 0.93)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 132 "Net-(R79-Pad1)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd rect
			(at 0.82 0 90)
			(size 0.79 0.93)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 51 "Net-(D5-K)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:Terminal Block 691137710002"
		(layer "F.Cu")
		(at 118.65295 41.72435 180)
		(property "Reference" "J8"
			(at -1.1553 -4.3176 0)
			(layer "F.SilkS")
		)
		(property "Value" "691137710002"
			(at -0.25 2.75 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/Power_Connectors/")
		(sheetfile "Power_Connectors.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole circle
			(at -2.5 0 180)
			(size 1.95 1.95)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 303 "/GNDREF")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" thru_hole circle
			(at 2.5 0 180)
			(size 1.95 1.95)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 53 "/LCL_12.3A2")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:RES_1206_OHM"
		(layer "F.Cu")
		(at 53.66855 128.71545 -90)
		(tags "MCS1632R005FER ")
		(property "Reference" "R63"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "0.005"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/LCL_12V/12V_12A_LCL_3/")
		(sheetfile "12V_12A_LCL.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.5266 0 270)
			(size 0.7032 1.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 5 "/DC_POS.12V")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.5266 0 270)
			(size 0.7032 1.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 11 "/LCL_12V/12V_12A_LCL_3/OPAMP_Minus")
			(pintype "passive")
		)
		(zone
			(net 0)
			(net_name "")
			(layer "F.Cu")
			(hatch full 0.508)
			(connect_pads
				(clearance 0)
			)
			(min_thickness 0.254)
			(filled_areas_thickness no)
			(keepout
				(tracks not_allowed)
				(vias not_allowed)
				(pads allowed)
				(copperpour not_allowed)
				(footprints allowed)
			)
			(placement
				(enabled no)
				(sheetname "")
			)
			(fill
				(thermal_gap 0.508)
				(thermal_bridge_width 0.508)
			)
			(polygon
				(pts
					(xy 54.46775 127.591249) (xy 54.46775 129.839651) (xy 52.86935 129.839651) (xy 52.86935 127.591249)
				)
			)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:RESC1508X55N"
		(layer "F.Cu")
		(at 242.35905 201.54195 90)
		(property "Reference" "R144"
			(at -0.21 -1.07 90)
			(layer "F.SilkS")
		)
		(property "Value" "22"
			(at 1.54 1.07 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Digital Systems/")
		(sheetfile "Digital_Systems.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -0.76 0 90)
			(size 0.9 0.97)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 147 "/Digital Systems/SSI0CLK")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd rect
			(at 0.76 0 90)
			(size 0.9 0.97)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 156 "Net-(U43-PA2{slash}SSI0CLK)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:RESC1508X55N"
		(layer "F.Cu")
		(at 234.10905 228.29195)
		(property "Reference" "R171"
			(at -2.5508 -0.75 0)
			(layer "F.SilkS")
		)
		(property "Value" "100"
			(at 0.1992 1 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Digital Systems/")
		(sheetfile "Digital_Systems.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -0.76 0)
			(size 0.9 0.97)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 189 "/LCL_CTRL6")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd rect
			(at 0.76 0)
			(size 0.9 0.97)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 188 "Net-(U45-P0_5)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:RESC1508X55N"
		(layer "F.Cu")
		(at 94.607925 43.769375 -90)
		(property "Reference" "R31"
			(at -0.21 -1.07 90)
			(layer "F.SilkS")
		)
		(property "Value" "1k"
			(at 1.54 1.07 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Power_Connectors/")
		(sheetfile "Power_Connectors.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -0.76 0 270)
			(size 0.9 0.97)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 114 "Net-(U6C-IN-)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd rect
			(at 0.76 0 270)
			(size 0.9 0.97)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 110 "Net-(R25-Pad2)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:TO-263AB_SUM"
		(layer "F.Cu")
		(at 180.05825 52.04195 90)
		(tags "SUM110P06-08L-E3 ")
		(property "Reference" "U30"
			(at -4.25 6.5 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "SUM110P06-08L-E3"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "SUM110P06-08L-E3"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TO-263AB_SUM TO-263AB_SUM-M TO-263AB_SUM-L")
		(sheetname "/LCL_5V/5V_6A_LCL_1/")
		(sheetfile "5V_6A_LCL.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(fp_text user "*"
			(at -2.54 5.2705 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(fp_text user "*"
			(at -2.54 5.2705 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -2.54 8.8773 90)
			(size 0.9906 3.2004)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 60 "Net-(D10-K)")
			(pinfunction "G")
			(pintype "input")
		)
		(pad "2" smd rect
			(at 0 0.0508 90)
			(size 10.414 11.4554)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 26 "/LCL_5V/5V_6A_LCL_1/OPAMP_Minus")
			(pinfunction "D")
			(pintype "input")
		)
		(pad "3" smd rect
			(at 2.54 8.8773 90)
			(size 0.9906 3.2004)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 61 "/LCL_5.6A1")
			(pinfunction "S")
			(pintype "input")
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:RESC1508X55N"
		(layer "F.Cu")
		(at 63.65905 213.87195)
		(property "Reference" "R53"
			(at 2.6492 -0.08 0)
			(layer "F.SilkS")
		)
		(property "Value" "54.9k"
			(at 1.54 1.07 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/LCL_12V/12V_12A_LCL_1/")
		(sheetfile "12V_12A_LCL.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -0.76 0)
			(size 0.9 0.97)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 42 "Net-(D1-K)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd rect
			(at 0.76 0)
			(size 0.9 0.97)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 8 "Net-(Q1-B)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:RES_1206_OHM"
		(layer "F.Cu")
		(at 53.81905 194.56495 -90)
		(tags "MCS1632R005FER ")
		(property "Reference" "R51"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "0.005"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/LCL_12V/12V_12A_LCL_1/")
		(sheetfile "12V_12A_LCL.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.5266 0 270)
			(size 0.7032 1.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 5 "/DC_POS.12V")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.5266 0 270)
			(size 0.7032 1.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 7 "/LCL_12V/12V_12A_LCL_1/OPAMP_Minus")
			(pintype "passive")
		)
		(zone
			(net 0)
			(net_name "")
			(layer "F.Cu")
			(hatch full 0.508)
			(connect_pads
				(clearance 0)
			)
			(min_thickness 0.254)
			(filled_areas_thickness no)
			(keepout
				(tracks not_allowed)
				(vias not_allowed)
				(pads allowed)
				(copperpour not_allowed)
				(footprints allowed)
			)
			(placement
				(enabled no)
				(sheetname "")
			)
			(fill
				(thermal_gap 0.508)
				(thermal_bridge_width 0.508)
			)
			(polygon
				(pts
					(xy 54.61825 193.440749) (xy 54.61825 195.689151) (xy 53.01985 195.689151) (xy 53.01985 193.440749)
				)
			)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:SOD3716X135N"
		(layer "F.Cu")
		(at 253.85905 52.791949 90)
		(descr "sod-123-ren1")
		(tags "Diode")
		(property "Reference" "D9"
			(at 0 0 90)
			(layer "F.SilkS")
		)
		(property "Value" "D"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Diode"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Device" "D"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TO-???* *_Diode_* *SingleDiode* D_*")
		(sheetname "/LCL_5V/5V_6A_LCL_3/")
		(sheetfile "5V_6A_LCL.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.65 0 180)
			(size 0.75 1.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 58 "Net-(D9-K)")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.65 0 180)
			(size 0.75 1.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 59 "/LCL_5.6A3")
			(pinfunction "A")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "1N4150W-E3-18.stp"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "EPS_Footprints:RESC1508X55N"
		(layer "F.Cu")
		(at 246.85905 199.29195 90)
		(property "Reference" "R146"
			(at -2.75 -0.0508 90)
			(layer "F.SilkS")
		)
		(property "Value" "22"
			(at 1.54 1.07 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Digital Systems/")
		(sheetfile "Digital_Systems.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -0.76 0 90)
			(size 0.9 0.97)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 144 "/Digital Systems/SSI0Tx")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd rect
			(at 0.76 0 90)
			(size 0.9 0.97)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 158 "Net-(U43-PA5{slash}SSI0TX)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:DIP762W50P254L730H410Q6"
		(layer "F.Cu")
		(at 48.60905 160.60195 -90)
		(property "Reference" "U14"
			(at -3.25 -5 90)
			(layer "F.SilkS")
		)
		(property "Value" "CNY17-1"
			(at 0.0903 0 90)
			(layer "Dwgs.User")
		)
		(property "Datasheet" "http://www.vishay.com/docs/83606/cny17.pdf"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "DC Optocoupler Base Connected, Vce 70V, CTR 40-80%, Viso 5000V (RMS), DIP6"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "DIP*W7.62mm* DIP*W10.16mm* SMDIP*W9.53mm*")
		(sheetname "/LCL_12V/12V_12A_LCL_2/")
		(sheetfile "12V_12A_LCL.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole rect
			(at -3.81 -2.54 270)
			(size 1.4 1.4)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 181 "/LCL_CTRL2")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" thru_hole circle
			(at -3.81 0 270)
			(size 1.4 1.4)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 303 "/GNDREF")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "3" thru_hole circle
			(at -3.81 2.54 270)
			(size 1.4 1.4)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 255 "unconnected-(U14-NC-Pad3)")
			(pinfunction "NC")
			(pintype "no_connect")
			(solder_mask_margin 0.102)
		)
		(pad "4" thru_hole circle
			(at 3.81 2.54 270)
			(size 1.4 1.4)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 303 "/GNDREF")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "5" thru_hole circle
			(at 3.81 0 270)
			(size 1.4 1.4)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 129 "Net-(R61-Pad1)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "6" thru_hole circle
			(at 3.81 -2.54 270)
			(size 1.4 1.4)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 256 "unconnected-(U14-Pad6)")
			(pintype "passive+no_connect")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "MountingHole:MountingHole_3.2mm_M3"
		(layer "F.Cu")
		(at 282.00825 96.44195)
		(descr "Mounting Hole 3.2mm, M3, no annular, generated by kicad-footprint-generator mountinghole.py")
		(tags "mountinghole M3")
		(property "Reference" "H2"
			(at 0 -4.15 0)
			(layer "F.SilkS")
		)
		(property "Value" "MountingHole"
			(at 0 4.15 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Mounting Hole without connection"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "MountingHole*")
		(sheetname "/")
		(sheetfile "PEEKbot_EPS.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 3.2 3.2)
			(drill 3.2)
			(layers "*.Cu" "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:RESC1608X55N"
		(layer "F.Cu")
		(at 79.287925 58.019375 180)
		(property "Reference" "R90"
			(at 2.479675 -0.522575 0)
			(layer "F.SilkS")
		)
		(property "Value" "86.6k"
			(at 1.54 1.05 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/LCL_12V/12V_5A_LCL_1/")
		(sheetfile "12V_5A_LCL.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -0.82 0 180)
			(size 0.79 0.93)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 55 "Net-(D7-K)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd rect
			(at 0.82 0 180)
			(size 0.79 0.93)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 19 "/LCL_12V/12V_5A_LCL_1/OPAMP_Minus")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:RESC1508X55N"
		(layer "F.Cu")
		(at 256.35905 191.79195)
		(property "Reference" "R140"
			(at 1.4492 -1.07 0)
			(layer "F.SilkS")
		)
		(property "Value" "470"
			(at 1.54 1.07 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Digital Systems/")
		(sheetfile "Digital_Systems.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -0.76 0)
			(size 0.9 0.97)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 36 "Net-(U43-~{RST})")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd rect
			(at 0.76 0)
			(size 0.9 0.97)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 151 "Net-(R140-Pad2)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:BAQ33GS08"
		(layer "F.Cu")
		(at 58.10905 194.16695 90)
		(descr "MiniMELF (SOD-80)")
		(tags "Zener Diode")
		(property "Reference" "ZD1"
			(at 0 0 90)
			(layer "F.SilkS")
		)
		(property "Value" "D_Zener"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Zener diode"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Library" "TZM5240B-GS08.txt"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Name" "TZM5240B-GS08"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Device" "D"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" "1=A 2=K"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TO-???* *_Diode_* *SingleDiode* D_*")
		(sheetname "/LCL_12V/12V_12A_LCL_1/")
		(sheetfile "12V_12A_LCL.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.875 0 90)
			(size 1.25 2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 7 "/LCL_12V/12V_12A_LCL_1/OPAMP_Minus")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.875 0 90)
			(size 1.25 2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 42 "Net-(D1-K)")
			(pinfunction "A")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "TZM5224B-GS08.stp"
			(offset
				(xyz 0 0 0.7999999999)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "EPS_Footprints:RESC1508X55N"
		(layer "F.Cu")
		(at 256.10905 44.54195 -90)
		(property "Reference" "R43"
			(at -0.21 -1.07 90)
			(layer "F.SilkS")
		)
		(property "Value" "1k"
			(at 1.54 1.07 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Power_Connectors/")
		(sheetfile "Power_Connectors.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -0.76 0 270)
			(size 0.9 0.97)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 122 "Net-(U7C-IN-)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd rect
			(at 0.76 0 270)
			(size 0.9 0.97)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 118 "Net-(R37-Pad2)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:RESC1508X55N"
		(layer "F.Cu")
		(at 40.10905 132.54195 -90)
		(property "Reference" "R16"
			(at -0.21 -1.07 90)
			(layer "F.SilkS")
		)
		(property "Value" "13.7k"
			(at 1.54 1.07 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Power_Connectors/")
		(sheetfile "Power_Connectors.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -0.76 0 270)
			(size 0.9 0.97)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 103 "Net-(R15-Pad2)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd rect
			(at 0.76 0 270)
			(size 0.9 0.97)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 303 "/GNDREF")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:RESC1508X55N"
		(layer "F.Cu")
		(at 258.35905 185.79195 180)
		(property "Reference" "R159"
			(at -2.6992 0.5 0)
			(layer "F.SilkS")
		)
		(property "Value" "2k"
			(at 1.54 1.07 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Digital Systems/")
		(sheetfile "Digital_Systems.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -0.76 0 180)
			(size 0.9 0.97)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 41 "/Digital Systems/OSC1")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd rect
			(at 0.76 0 180)
			(size 0.9 0.97)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 172 "Net-(U43-OSC1)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:RES_1206_OHM"
		(layer "F.Cu")
		(at 39.10905 103.54195 -90)
		(tags "MCS1632R005FER ")
		(property "Reference" "R69"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "0.005"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/LCL_12V/12V_12A_LCL_4/")
		(sheetfile "12V_12A_LCL.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.5266 0 270)
			(size 0.7032 1.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 5 "/DC_POS.12V")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.5266 0 270)
			(size 0.7032 1.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 13 "/LCL_12V/12V_12A_LCL_4/OPAMP_Minus")
			(pintype "passive")
		)
		(zone
			(net 0)
			(net_name "")
			(layer "F.Cu")
			(hatch full 0.508)
			(connect_pads
				(clearance 0)
			)
			(min_thickness 0.254)
			(filled_areas_thickness no)
			(keepout
				(tracks not_allowed)
				(vias not_allowed)
				(pads allowed)
				(copperpour not_allowed)
				(footprints allowed)
			)
			(placement
				(enabled no)
				(sheetname "")
			)
			(fill
				(thermal_gap 0.508)
				(thermal_bridge_width 0.508)
			)
			(polygon
				(pts
					(xy 39.90825 102.417749) (xy 39.90825 104.666151) (xy 38.30985 104.666151) (xy 38.30985 102.417749)
				)
			)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:TO-263AB_SUM"
		(layer "F.Cu")
		(at 181.75935 251.04195 -90)
		(tags "SUM110P06-08L-E3 ")
		(property "Reference" "U39"
			(at 0 -6.5489 270)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "SUM110P06-08L-E3"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "SUM110P06-08L-E3"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TO-263AB_SUM TO-263AB_SUM-M TO-263AB_SUM-L")
		(sheetname "/LCL_9_and_3-3/3-3V_1-5A_LCL_1/")
		(sheetfile "3-3V_1-5A_LCL.kicad_sch")
		(attr smd)
		(fp_text user "*"
			(at -5.715 8.8773 90)
			(layer "F.SilkS")
		)
		(fp_text user "*"
			(at -5.715 8.8773 270)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "*"
			(at -2.54 5.2705 90)
			(layer "F.Fab")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
		)
		(fp_text user "*"
			(at -2.54 5.2705 270)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -2.54 8.8773 270)
			(size 0.9906 3.2004)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 68 "Net-(D14-K)")
			(pinfunction "G")
			(pintype "input")
		)
		(pad "2" smd rect
			(at 0 0.0508 270)
			(size 10.414 11.4554)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 33 "/LCL_9_and_3-3/3-3V_1-5A_LCL_1/OPAMP_Minus")
			(pinfunction "D")
			(pintype "input")
		)
		(pad "3" smd rect
			(at 2.54 8.8773 270)
			(size 0.9906 3.2004)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 69 "/LCL_MIXED.3.3V1.5A")
			(pinfunction "S")
			(pintype "input")
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:RESC1508X55N"
		(layer "F.Cu")
		(at 50.85905 104.19195 90)
		(property "Reference" "R71"
			(at 2.4 0.1992 90)
			(layer "F.SilkS")
		)
		(property "Value" "54.9k"
			(at 1.54 1.07 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/LCL_12V/12V_12A_LCL_4/")
		(sheetfile "12V_12A_LCL.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -0.76 0 90)
			(size 0.9 0.97)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 49 "Net-(D4-K)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd rect
			(at 0.76 0 90)
			(size 0.9 0.97)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 14 "Net-(Q4-B)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:CAPC1608X90"
		(layer "F.Cu")
		(at 63.50855 149.77245)
		(descr "<b>CAPACITOR</b>")
		(property "Reference" "C21"
			(at 2.7997 0.0195 0)
			(layer "F.SilkS")
		)
		(property "Value" "0.1uF"
			(at 1.56646 1.20613 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "SMD 0603 MLCC capacitor, Alternate KiCad Library"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/LCL_12V/12V_12A_LCL_3/")
		(sheetfile "12V_12A_LCL.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -0.85 0)
			(size 1.1 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 11 "/LCL_12V/12V_12A_LCL_3/OPAMP_Minus")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd rect
			(at 0.85 0)
			(size 1.1 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 12 "Net-(Q3-B)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:Terminal Block 691137710002"
		(layer "F.Cu")
		(at 150.835609 42.145191 180)
		(property "Reference" "J7"
			(at -0.972641 -4.646759 0)
			(layer "F.SilkS")
		)
		(property "Value" "691137710002"
			(at 4.12 5.365 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/Power_Connectors/")
		(sheetfile "Power_Connectors.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole circle
			(at -2.5 0 180)
			(size 1.95 1.95)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 303 "/GNDREF")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" thru_hole circle
			(at 2.5 0 180)
			(size 1.95 1.95)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 50 "/LCL_12.3A1")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:CONN4_BM04B-SRSS_JST"
		(layer "F.Cu")
		(at 230.726849 180.04195 90)
		(tags "BM04B-SRSS-TB ")
		(property "Reference" "J23"
			(at 4.75 0.581401 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "BM04B-SRSS-TB"
			(at 22.5 -11.117799 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "BM04B-SRSS-TB"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "CONN4_BM04B-SRSS_JST")
		(sheetname "/Digital_Connectors/")
		(sheetfile "Digital_Connectors.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 1.882201 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.5 1.882201 90)
			(size 0.6604 1.5494)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 87 "unconnected-(J23-Pad1)")
			(pinfunction "1")
			(pintype "unspecified+no_connect")
		)
		(pad "2" smd rect
			(at -0.499999 1.882201 90)
			(size 0.6604 1.5494)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 86 "/UART.Tx")
			(pinfunction "2")
			(pintype "unspecified")
		)
		(pad "3" smd rect
			(at 0.499999 1.882201 90)
			(size 0.6604 1.5494)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 88 "/UART.Rx")
			(pinfunction "3")
			(pintype "unspecified")
		)
		(pad "4" smd rect
			(at 1.5 1.882201 90)
			(size 0.6604 1.5494)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 303 "/GNDREF")
			(pinfunction "4")
			(pintype "unspecified")
		)
		(pad "5" smd rect
			(at -2.799999 -0.697799 90)
			(size 1.2954 1.905)
			(layers "F.Cu" "F.Mask" "F.Paste")
		)
		(pad "6" smd rect
			(at 2.799999 -0.697799 90)
			(size 1.2954 1.905)
			(layers "F.Cu" "F.Mask" "F.Paste")
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:SW_JS202011SCQN"
		(layer "F.Cu")
		(at 276.60905 176.54195 90)
		(property "Reference" "S1"
			(at -3.75 -4.8008 90)
			(layer "F.SilkS")
		)
		(property "Value" "JS202011SCQN"
			(at 4.775 5.885 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DigiKey_Part_Number" "401-2002-1-ND"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SnapEDA_Link" "https://www.snapeda.com/parts/JS202011SCQN/C%2526K/view-part/?ref=snap"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MAXIMUM_PACKAGE_HEIGHT" "5.5 mm"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Package" "None"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Check_prices" "https://www.snapeda.com/parts/JS202011SCQN/C%2526K/view-part/?ref=eda"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "STANDARD" "Manufacturer Recommendations"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTREV" "26 May 22"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MF" "C&K"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MP" "JS202011SCQN"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description_1" "Slide Switch DPDT Surface Mount"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER" "C&K"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SNAPEDA_PN" "JS202011SCQN"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/Digital Systems/")
		(sheetfile "Digital_Systems.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -2.5 2.75 90)
			(size 1.2 2.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 72 "/DC_POS.3.3V")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd rect
			(at 0 2.75 90)
			(size 1.2 2.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 35 "/Digital Systems/3.3V+")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "3" smd rect
			(at 2.5 2.75 90)
			(size 1.2 2.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 210 "unconnected-(S1-Pad3)")
			(pintype "passive+no_connect")
			(solder_mask_margin 0.102)
		)
		(pad "4" smd rect
			(at -2.5 -2.75 90)
			(size 1.2 2.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 303 "/GNDREF")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "5" smd rect
			(at 0 -2.75 90)
			(size 1.2 2.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 211 "Net-(U42-EN)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "6" smd rect
			(at 2.5 -2.75 90)
			(size 1.2 2.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 82 "/USB.VBUS")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:RESC1508X55N"
		(layer "F.Cu")
		(at 246.60905 219.54195)
		(property "Reference" "R180"
			(at 2.9492 -0.25 0)
			(layer "F.SilkS")
		)
		(property "Value" "100"
			(at 1.54 1.07 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Digital Systems/")
		(sheetfile "Digital_Systems.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -0.76 0)
			(size 0.9 0.97)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 204 "Net-(U45-P1_5)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd rect
			(at 0.76 0)
			(size 0.9 0.97)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 205 "/LCL_CTRL14")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:CAPC1608X90"
		(layer "F.Cu")
		(at 269.11405 174.04195)
		(descr "<b>CAPACITOR</b>")
		(property "Reference" "C36"
			(at -0.235423 -1.237214 0)
			(layer "F.SilkS")
		)
		(property "Value" "0.1uF"
			(at 1.56646 1.20613 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "SMD 0603 MLCC capacitor, Alternate KiCad Library"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/Digital Systems/")
		(sheetfile "Digital_Systems.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -0.85 0)
			(size 1.1 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 38 "Net-(U42-NR)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd rect
			(at 0.85 0)
			(size 1.1 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 303 "/GNDREF")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:RESC1508X55N"
		(layer "F.Cu")
		(at 261.85905 181.54195)
		(property "Reference" "R158"
			(at -0.21 -1.07 0)
			(layer "F.SilkS")
		)
		(property "Value" "10k"
			(at 1.54 1.07 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Digital Systems/")
		(sheetfile "Digital_Systems.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -0.76 0)
			(size 0.9 0.97)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 155 "/Digital Systems/I2C0SDA")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd rect
			(at 0.76 0)
			(size 0.9 0.97)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 35 "/Digital Systems/3.3V+")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:RESC1508X55N"
		(layer "F.Cu")
		(at 193.85905 44.79195 -90)
		(property "Reference" "R41"
			(at -0.21 -1.07 90)
			(layer "F.SilkS")
		)
		(property "Value" "1k"
			(at 1.54 1.07 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Power_Connectors/")
		(sheetfile "Power_Connectors.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -0.76 0 270)
			(size 0.9 0.97)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 120 "Net-(U7A-IN-)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd rect
			(at 0.76 0 270)
			(size 0.9 0.97)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 116 "Net-(R33-Pad2)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:RESC1508X55N"
		(layer "F.Cu")
		(at 247.90905 60.61695 90)
		(property "Reference" "R104"
			(at -2.675 -0.1008 90)
			(layer "F.SilkS")
		)
		(property "Value" "54.9k"
			(at 1.54 1.069999 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/LCL_5V/5V_6A_LCL_3/")
		(sheetfile "5V_6A_LCL.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -0.76 0 90)
			(size 0.9 0.97)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 136 "Net-(R103-Pad1)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd rect
			(at 0.76 0 90)
			(size 0.9 0.97)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 58 "Net-(D9-K)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:Terminal Block 691137710002"
		(layer "F.Cu")
		(at 86.357925 41.519375 180)
		(property "Reference" "J9"
			(at -1.700325 -4.522575 0)
			(layer "F.SilkS")
		)
		(property "Value" "691137710002"
			(at 4.12 5.365 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/Power_Connectors/")
		(sheetfile "Power_Connectors.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole circle
			(at -2.5 0 180)
			(size 1.95 1.95)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 303 "/GNDREF")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" thru_hole circle
			(at 2.5 0 180)
			(size 1.95 1.95)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 54 "/LCL_12.5A1")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:SOD3716X135N"
		(layer "F.Cu")
		(at 54.45855 135.442449 180)
		(descr "sod-123-ren1")
		(tags "Diode")
		(property "Reference" "D3"
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "D"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Diode"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Device" "D"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TO-???* *_Diode_* *SingleDiode* D_*")
		(sheetname "/LCL_12V/12V_12A_LCL_3/")
		(sheetfile "12V_12A_LCL.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.65 0 270)
			(size 0.75 1.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 46 "Net-(D3-K)")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.65 0 270)
			(size 0.75 1.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 47 "/LCL_12.12A3")
			(pinfunction "A")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "1N4150W-E3-18.stp"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "EPS_Footprints:SOD3716X135N"
		(layer "F.Cu")
		(at 157.924042 51.313259 90)
		(descr "sod-123-ren1")
		(tags "Diode")
		(property "Reference" "D5"
			(at 0 0 90)
			(layer "F.SilkS")
		)
		(property "Value" "D"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Diode"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Device" "D"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TO-???* *_Diode_* *SingleDiode* D_*")
		(sheetname "/LCL_12V/12V_3A_LCL_1/")
		(sheetfile "12V_3A_LCL.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.65 0 180)
			(size 0.75 1.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 51 "Net-(D5-K)")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.65 0 180)
			(size 0.75 1.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 50 "/LCL_12.3A1")
			(pinfunction "A")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "1N4150W-E3-18.stp"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "EPS_Footprints:RES_TLRP3A30DR018FTE_TEC"
		(layer "F.Cu")
		(at 290.859049 50.541949 180)
		(tags "TLRP3A30DR018FTE ")
		(property "Reference" "R117"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "0.01"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/LCL_5V/5V_6A_LCL_4/")
		(sheetfile "5V_6A_LCL.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -2.8321 0 180)
			(size 1.397 3.4544)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 4 "/DC_POS.5V")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 2.8321 0 180)
			(size 1.397 3.4544)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 30 "/LCL_5V/5V_6A_LCL_4/OPAMP_Minus")
			(pintype "passive")
		)
		(zone
			(net 0)
			(net_name "")
			(layer "F.Cu")
			(hatch full 0.508)
			(connect_pads
				(clearance 0)
			)
			(min_thickness 0.254)
			(filled_areas_thickness no)
			(keepout
				(tracks not_allowed)
				(vias not_allowed)
				(pads allowed)
				(copperpour not_allowed)
				(footprints allowed)
			)
			(placement
				(enabled no)
				(sheetname "")
			)
			(fill
				(thermal_gap 0.508)
				(thermal_bridge_width 0.508)
			)
			(polygon
				(pts
					(xy 292.941849 52.218349) (xy 288.776249 52.218349) (xy 288.776249 48.865549) (xy 292.941849 48.865549)
				)
			)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:BAQ33GS08"
		(layer "F.Cu")
		(at 259.734049 55.041949)
		(descr "MiniMELF (SOD-80)")
		(tags "Zener Diode")
		(property "Reference" "ZD9"
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "D_Zener"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Zener diode"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Library" "TZM5240B-GS08.txt"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Name" "TZM5240B-GS08"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Device" "D"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" "1=A 2=K"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TO-???* *_Diode_* *SingleDiode* D_*")
		(sheetname "/LCL_5V/5V_6A_LCL_3/")
		(sheetfile "5V_6A_LCL.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.875 0)
			(size 1.25 2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 24 "/LCL_5V/5V_6A_LCL_3/OPAMP_Minus")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.875 0)
			(size 1.25 2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 58 "Net-(D9-K)")
			(pinfunction "A")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "TZM5224B-GS08.stp"
			(offset
				(xyz 0 0 0.7999999999)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "EPS_Footprints:RESC1508X55N"
		(layer "F.Cu")
		(at 40.62905 198.77195 -90)
		(property "Reference" "R12"
			(at -2.48 0.06 90)
			(layer "F.SilkS")
		)
		(property "Value" "13.7k"
			(at 1.54 1.07 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Power_Connectors/")
		(sheetfile "Power_Connectors.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -0.76 0 270)
			(size 0.9 0.97)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 101 "Net-(R11-Pad2)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd rect
			(at 0.76 0 270)
			(size 0.9 0.97)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 303 "/GNDREF")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:RESC1608X55N"
		(layer "F.Cu")
		(at 61.10905 214.61195 -90)
		(property "Reference" "R54"
			(at -0.11 1.3008 90)
			(layer "F.SilkS")
		)
		(property "Value" "86.6k"
			(at 1.54 1.05 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/LCL_12V/12V_12A_LCL_1/")
		(sheetfile "12V_12A_LCL.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -0.82 0 270)
			(size 0.79 0.93)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 42 "Net-(D1-K)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd rect
			(at 0.82 0 270)
			(size 0.79 0.93)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 7 "/LCL_12V/12V_12A_LCL_1/OPAMP_Minus")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:Current Sense Amplifier SOP65P640X120-14N"
		(layer "F.Cu")
		(at 101.73905 226.74195)
		(property "Reference" "U36"
			(at -0.73 -3.635 0)
			(layer "F.SilkS")
		)
		(property "Value" "INA4180A2IPWR"
			(at 6.89 3.635 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTREV" "H"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "STANDARD" "IPC 7351B"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SNAPEDA_PN" "INA4180A2IPWR"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MAXIMUM_PACKAGE_HEIGHT" "1.2 mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER" "Texas Instruments"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/LCL_9_and_3-3/")
		(sheetfile "LCL_9_and_3-3.kicad_sch")
		(attr smd)
		(pad "1" smd roundrect
			(at -2.87 -1.95)
			(size 1.57 0.41)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.125)
			(net 283 "/I_MEAS.9_")
			(pintype "output")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd roundrect
			(at -2.87 -1.3)
			(size 1.57 0.41)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.125)
			(net 32 "/LCL_9_and_3-3/9V_2A_LCL_1/OPAMP_Minus")
			(pintype "input")
			(solder_mask_margin 0.102)
		)
		(pad "3" smd roundrect
			(at -2.87 -0.65)
			(size 1.57 0.41)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.125)
			(net 6 "/DC_POS.9V")
			(pintype "input")
			(solder_mask_margin 0.102)
		)
		(pad "4" smd roundrect
			(at -2.87 0)
			(size 1.57 0.41)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.125)
			(net 72 "/DC_POS.3.3V")
			(pintype "power_in")
			(solder_mask_margin 0.102)
		)
		(pad "5" smd roundrect
			(at -2.87 0.65)
			(size 1.57 0.41)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.125)
			(net 72 "/DC_POS.3.3V")
			(pintype "input")
			(solder_mask_margin 0.102)
		)
		(pad "6" smd roundrect
			(at -2.87 1.3)
			(size 1.57 0.41)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.125)
			(net 33 "/LCL_9_and_3-3/3-3V_1-5A_LCL_1/OPAMP_Minus")
			(pintype "input")
			(solder_mask_margin 0.102)
		)
		(pad "7" smd roundrect
			(at -2.87 1.95)
			(size 1.57 0.41)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.125)
			(net 286 "/I_MEAS.3.3_")
			(pintype "output")
			(solder_mask_margin 0.102)
		)
		(pad "8" smd roundrect
			(at 2.87 1.95)
			(size 1.57 0.41)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.125)
			(net 285 "unconnected-(U36-Pad8)")
			(pintype "output+no_connect")
			(solder_mask_margin 0.102)
		)
		(pad "9" smd roundrect
			(at 2.87 1.3)
			(size 1.57 0.41)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.125)
			(net 281 "unconnected-(U36-Pad9)")
			(pintype "input+no_connect")
			(solder_mask_margin 0.102)
		)
		(pad "10" smd roundrect
			(at 2.87 0.65)
			(size 1.57 0.41)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.125)
			(net 287 "unconnected-(U36-Pad10)")
			(pintype "input+no_connect")
			(solder_mask_margin 0.102)
		)
		(pad "11" smd roundrect
			(at 2.87 0)
			(size 1.57 0.41)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.125)
			(net 303 "/GNDREF")
			(pintype "power_in")
			(solder_mask_margin 0.102)
		)
		(pad "12" smd roundrect
			(at 2.87 -0.65)
			(size 1.57 0.41)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.125)
			(net 288 "unconnected-(U36-Pad12)")
			(pintype "input+no_connect")
			(solder_mask_margin 0.102)
		)
		(pad "13" smd roundrect
			(at 2.87 -1.3)
			(size 1.57 0.41)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.125)
			(net 284 "unconnected-(U36-Pad13)")
			(pintype "input+no_connect")
			(solder_mask_margin 0.102)
		)
		(pad "14" smd roundrect
			(at 2.87 -1.95)
			(size 1.57 0.41)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.125)
			(net 282 "unconnected-(U36-Pad14)")
			(pintype "output+no_connect")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:RESC1508X55N"
		(layer "F.Cu")
		(at 43.95855 133.54195 180)
		(property "Reference" "R14"
			(at -0.21 -1.07 0)
			(layer "F.SilkS")
		)
		(property "Value" "13.7k"
			(at 1.54 1.07 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Power_Connectors/")
		(sheetfile "Power_Connectors.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -0.76 0 180)
			(size 0.9 0.97)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 102 "Net-(R13-Pad2)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd rect
			(at 0.76 0 180)
			(size 0.9 0.97)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 303 "/GNDREF")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:CAPC1608X87N"
		(layer "F.Cu")
		(at 255.85905 189.29195 -90)
		(property "Reference" "C35"
			(at -2.5 0.0508 90)
			(layer "F.SilkS")
		)
		(property "Value" "12pF"
			(at 1.51 1.07 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DigiKey_Part_Number" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SnapEDA_Link" "https://www.snapeda.com/parts/C0603C120K4HAC7867/Kemet/view-part/?ref=snap"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description_1" "CAP CER 0603 12PF 16V ULTRA STAB"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MF" "KEMET"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Package" "1608 KEMET"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Check_prices" "https://www.snapeda.com/parts/C0603C120K4HAC7867/Kemet/view-part/?ref=eda"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MP" "C0603C120K4HAC7867"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/Digital Systems/")
		(sheetfile "Digital_Systems.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -0.775 0 270)
			(size 0.92 0.97)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 37 "Net-(U43-OSC0)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd rect
			(at 0.775 0 270)
			(size 0.92 0.97)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 303 "/GNDREF")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:Current Sense Amplifier SOP65P640X120-14N"
		(layer "F.Cu")
		(at 148.73905 85.74195 180)
		(property "Reference" "U10"
			(at -0.73 -3.635 0)
			(layer "F.SilkS")
		)
		(property "Value" "INA4180A2IPWR"
			(at 6.89 3.635 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTREV" "H"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "STANDARD" "IPC 7351B"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SNAPEDA_PN" "INA4180A2IPWR"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MAXIMUM_PACKAGE_HEIGHT" "1.2 mm"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER" "Texas Instruments"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/LCL_12V/")
		(sheetfile "LCL_12V.kicad_sch")
		(attr smd)
		(pad "1" smd roundrect
			(at -2.87 -1.95 180)
			(size 1.57 0.41)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.125)
			(net 252 "/I_MEAS.12_5")
			(pintype "output")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd roundrect
			(at -2.87 -1.3 180)
			(size 1.57 0.41)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.125)
			(net 16 "/LCL_12V/12V_3A_LCL_1/OPAMP_Minus")
			(pintype "input")
			(solder_mask_margin 0.102)
		)
		(pad "3" smd roundrect
			(at -2.87 -0.65 180)
			(size 1.57 0.41)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.125)
			(net 5 "/DC_POS.12V")
			(pintype "input")
			(solder_mask_margin 0.102)
		)
		(pad "4" smd roundrect
			(at -2.87 0 180)
			(size 1.57 0.41)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.125)
			(net 72 "/DC_POS.3.3V")
			(pintype "power_in")
			(solder_mask_margin 0.102)
		)
		(pad "5" smd roundrect
			(at -2.87 0.65 180)
			(size 1.57 0.41)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.125)
			(net 5 "/DC_POS.12V")
			(pintype "input")
			(solder_mask_margin 0.102)
		)
		(pad "6" smd roundrect
			(at -2.87 1.3 180)
			(size 1.57 0.41)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.125)
			(net 18 "/LCL_12V/12V_3A_LCL_2/OPAMP_Minus")
			(pintype "input")
			(solder_mask_margin 0.102)
		)
		(pad "7" smd roundrect
			(at -2.87 1.95 180)
			(size 1.57 0.41)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.125)
			(net 251 "/I_MEAS.12_6")
			(pintype "output")
			(solder_mask_margin 0.102)
		)
		(pad "8" smd roundrect
			(at 2.87 1.95 180)
			(size 1.57 0.41)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.125)
			(net 250 "/I_MEAS.12_7")
			(pintype "output")
			(solder_mask_margin 0.102)
		)
		(pad "9" smd roundrect
			(at 2.87 1.3 180)
			(size 1.57 0.41)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.125)
			(net 19 "/LCL_12V/12V_5A_LCL_1/OPAMP_Minus")
			(pintype "input")
			(solder_mask_margin 0.102)
		)
		(pad "10" smd roundrect
			(at 2.87 0.65 180)
			(size 1.57 0.41)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.125)
			(net 5 "/DC_POS.12V")
			(pintype "input")
			(solder_mask_margin 0.102)
		)
		(pad "11" smd roundrect
			(at 2.87 0 180)
			(size 1.57 0.41)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.125)
			(net 303 "/GNDREF")
			(pintype "power_in")
			(solder_mask_margin 0.102)
		)
		(pad "12" smd roundrect
			(at 2.87 -0.65 180)
			(size 1.57 0.41)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.125)
			(net 5 "/DC_POS.12V")
			(pintype "input")
			(solder_mask_margin 0.102)
		)
		(pad "13" smd roundrect
			(at 2.87 -1.3 180)
			(size 1.57 0.41)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.125)
			(net 22 "/LCL_12V/12V_5A_LCL_2/OPAMP_Minus")
			(pintype "input")
			(solder_mask_margin 0.102)
		)
		(pad "14" smd roundrect
			(at 2.87 -1.95 180)
			(size 1.57 0.41)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.125)
			(net 249 "/I_MEAS.12_8")
			(pintype "output")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:CAPC1608X90"
		(layer "F.Cu")
		(at 60.75905 250.29195)
		(descr "<b>CAPACITOR</b>")
		(property "Reference" "C31"
			(at -0.235423 -1.237214 0)
			(layer "F.SilkS")
		)
		(property "Value" "0.1uF"
			(at 1.56646 1.20613 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "SMD 0603 MLCC capacitor, Alternate KiCad Library"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/LCL_9_and_3-3/9V_2A_LCL_1/")
		(sheetfile "9V_2A_LCL.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -0.85 0)
			(size 1.1 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 32 "/LCL_9_and_3-3/9V_2A_LCL_1/OPAMP_Minus")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd rect
			(at 0.85 0)
			(size 1.1 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 31 "Net-(Q13-B)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:RESC1608X55N"
		(layer "F.Cu")
		(at 80.107925 60.519375 -90)
		(property "Reference" "R89"
			(at 2.772575 0.049675 90)
			(layer "F.SilkS")
		)
		(property "Value" "45.3k"
			(at 1.54 1.05 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/LCL_12V/12V_5A_LCL_1/")
		(sheetfile "12V_5A_LCL.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -0.82 0 270)
			(size 0.79 0.93)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 55 "Net-(D7-K)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd rect
			(at 0.82 0 270)
			(size 0.79 0.93)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 20 "Net-(Q7-B)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:RESC1608X55N"
		(layer "F.Cu")
		(at 113.08295 58.54435 180)
		(property "Reference" "R84"
			(at -0.11 1.2524 0)
			(layer "F.SilkS")
		)
		(property "Value" "86.6k"
			(at 1.54 1.05 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/LCL_12V/12V_3A_LCL_2/")
		(sheetfile "12V_3A_LCL.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -0.82 0 180)
			(size 0.79 0.93)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 52 "Net-(D6-K)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd rect
			(at 0.82 0 180)
			(size 0.79 0.93)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 18 "/LCL_12V/12V_3A_LCL_2/OPAMP_Minus")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:Current Sense Amplifier SOP65P640X120-14N"
		(layer "F.Cu")
		(at 94.47905 144.49195)
		(property "Reference" "U9"
			(at -0.73 -3.635 0)
			(layer "F.SilkS")
		)
		(property "Value" "INA4180A2IPWR"
			(at 6.89 3.635 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTREV" "H"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "STANDARD" "IPC 7351B"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SNAPEDA_PN" "INA4180A2IPWR"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MAXIMUM_PACKAGE_HEIGHT" "1.2 mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER" "Texas Instruments"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/LCL_12V/")
		(sheetfile "LCL_12V.kicad_sch")
		(attr smd)
		(pad "1" smd roundrect
			(at -2.87 -1.95)
			(size 1.57 0.41)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.125)
			(net 247 "/I_MEAS.12_1")
			(pintype "output")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd roundrect
			(at -2.87 -1.3)
			(size 1.57 0.41)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.125)
			(net 7 "/LCL_12V/12V_12A_LCL_1/OPAMP_Minus")
			(pintype "input")
			(solder_mask_margin 0.102)
		)
		(pad "3" smd roundrect
			(at -2.87 -0.65)
			(size 1.57 0.41)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.125)
			(net 5 "/DC_POS.12V")
			(pintype "input")
			(solder_mask_margin 0.102)
		)
		(pad "4" smd roundrect
			(at -2.87 0)
			(size 1.57 0.41)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.125)
			(net 72 "/DC_POS.3.3V")
			(pintype "power_in")
			(solder_mask_margin 0.102)
		)
		(pad "5" smd roundrect
			(at -2.87 0.65)
			(size 1.57 0.41)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.125)
			(net 5 "/DC_POS.12V")
			(pintype "input")
			(solder_mask_margin 0.102)
		)
		(pad "6" smd roundrect
			(at -2.87 1.3)
			(size 1.57 0.41)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.125)
			(net 10 "/LCL_12V/12V_12A_LCL_2/OPAMP_Minus")
			(pintype "input")
			(solder_mask_margin 0.102)
		)
		(pad "7" smd roundrect
			(at -2.87 1.95)
			(size 1.57 0.41)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.125)
			(net 248 "/I_MEAS.12_2")
			(pintype "output")
			(solder_mask_margin 0.102)
		)
		(pad "8" smd roundrect
			(at 2.87 1.95)
			(size 1.57 0.41)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.125)
			(net 245 "/I_MEAS.12_3")
			(pintype "output")
			(solder_mask_margin 0.102)
		)
		(pad "9" smd roundrect
			(at 2.87 1.3)
			(size 1.57 0.41)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.125)
			(net 11 "/LCL_12V/12V_12A_LCL_3/OPAMP_Minus")
			(pintype "input")
			(solder_mask_margin 0.102)
		)
		(pad "10" smd roundrect
			(at 2.87 0.65)
			(size 1.57 0.41)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.125)
			(net 5 "/DC_POS.12V")
			(pintype "input")
			(solder_mask_margin 0.102)
		)
		(pad "11" smd roundrect
			(at 2.87 0)
			(size 1.57 0.41)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.125)
			(net 303 "/GNDREF")
			(pintype "power_in")
			(solder_mask_margin 0.102)
		)
		(pad "12" smd roundrect
			(at 2.87 -0.65)
			(size 1.57 0.41)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.125)
			(net 5 "/DC_POS.12V")
			(pintype "input")
			(solder_mask_margin 0.102)
		)
		(pad "13" smd roundrect
			(at 2.87 -1.3)
			(size 1.57 0.41)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.125)
			(net 13 "/LCL_12V/12V_12A_LCL_4/OPAMP_Minus")
			(pintype "input")
			(solder_mask_margin 0.102)
		)
		(pad "14" smd roundrect
			(at 2.87 -1.95)
			(size 1.57 0.41)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.125)
			(net 246 "/I_MEAS.12_4")
			(pintype "output")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:RESC1508X55N"
		(layer "F.Cu")
		(at 223.35905 42.79195 90)
		(property "Reference" "R36"
			(at 1.5 1.1992 90)
			(layer "F.SilkS")
		)
		(property "Value" "37.5k (37.4k)"
			(at 1.54 1.07 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Power_Connectors/")
		(sheetfile "Power_Connectors.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -0.76 0 90)
			(size 0.9 0.97)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 117 "Net-(R35-Pad2)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd rect
			(at 0.76 0 90)
			(size 0.9 0.97)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 303 "/GNDREF")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:RESC1508X55N"
		(layer "F.Cu")
		(at 182.35905 243.79195)
		(property "Reference" "R132"
			(at 2.6992 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "15k"
			(at 1.54 1.07 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/LCL_9_and_3-3/3-3V_1-5A_LCL_1/")
		(sheetfile "3-3V_1-5A_LCL.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -0.76 0)
			(size 0.9 0.97)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 68 "Net-(D14-K)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd rect
			(at 0.76 0)
			(size 0.9 0.97)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 33 "/LCL_9_and_3-3/3-3V_1-5A_LCL_1/OPAMP_Minus")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:SOT91P240X120-3N"
		(layer "F.Cu")
		(at 214.35905 62.291949)
		(property "Reference" "Q11"
			(at -0.175999 -2.3698 0)
			(layer "F.SilkS")
		)
		(property "Value" "PNP"
			(at 3.176799 2.3698 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://ngspice.sourceforge.io/docs/ngspice-html-manual/manual.xhtml#cha_BJTs"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Bipolar transistor symbol for simulation only, substrate tied to the emitter"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Device" "PNP"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Type" "GUMMELPOON"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" "1=C 2=B 3=E"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/LCL_5V/5V_6A_LCL_2/")
		(sheetfile "5V_6A_LCL.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -0.915 1.025)
			(size 0.61 1.18)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 62 "Net-(D11-K)")
			(pinfunction "C")
			(pintype "open_collector")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd rect
			(at 0.915 1.025)
			(size 0.61 1.18)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 28 "Net-(Q11-B)")
			(pinfunction "B")
			(pintype "input")
			(solder_mask_margin 0.102)
		)
		(pad "3" smd rect
			(at 0 -1.025)
			(size 0.61 1.18)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 27 "/LCL_5V/5V_6A_LCL_2/OPAMP_Minus")
			(pinfunction "E")
			(pintype "open_emitter")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:Terminal Block 691137710002"
		(layer "F.Cu")
		(at 161 252.75)
		(property "Reference" "J16"
			(at 0 -5.135 0)
			(layer "F.SilkS")
		)
		(property "Value" "691137710002"
			(at 4.12 5.365 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/Power_Connectors/")
		(sheetfile "Power_Connectors.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole circle
			(at -2.5 0)
			(size 1.95 1.95)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 303 "/GNDREF")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" thru_hole circle
			(at 2.5 0)
			(size 1.95 1.95)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 69 "/LCL_MIXED.3.3V1.5A")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:CAPC1608X90"
		(layer "F.Cu")
		(at 222.35905 193.23695)
		(descr "<b>CAPACITOR</b>")
		(property "Reference" "C38"
			(at -0.235423 -1.237214 0)
			(layer "F.SilkS")
		)
		(property "Value" "0.1uF"
			(at 1.56646 1.20613 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "SMD 0603 MLCC capacitor, Alternate KiCad Library"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/Digital Systems/")
		(sheetfile "Digital_Systems.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -0.85 0)
			(size 1.1 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 39 "Net-(U44-REF)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd rect
			(at 0.85 0)
			(size 1.1 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 303 "/GNDREF")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:SOD3716X135N"
		(layer "F.Cu")
		(at 284.60905 52.541949 90)
		(descr "sod-123-ren1")
		(tags "Diode")
		(property "Reference" "D12"
			(at 0 0 90)
			(layer "F.SilkS")
		)
		(property "Value" "D"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Diode"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Device" "D"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TO-???* *_Diode_* *SingleDiode* D_*")
		(sheetname "/LCL_5V/5V_6A_LCL_4/")
		(sheetfile "5V_6A_LCL.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.65 0 180)
			(size 0.75 1.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 65 "Net-(D12-K)")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.65 0 180)
			(size 0.75 1.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 64 "/LCL_5.6A4")
			(pinfunction "A")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "1N4150W-E3-18.stp"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "EPS_Footprints:TO-263AB_SUM"
		(layer "F.Cu")
		(at 210.60905 51.79195 90)
		(tags "SUM110P06-08L-E3 ")
		(property "Reference" "U32"
			(at -3.25 -6.5508 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "SUM110P06-08L-E3"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "SUM110P06-08L-E3"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TO-263AB_SUM TO-263AB_SUM-M TO-263AB_SUM-L")
		(sheetname "/LCL_5V/5V_6A_LCL_2/")
		(sheetfile "5V_6A_LCL.kicad_sch")
		(attr smd)
		(fp_text user "*"
			(at -2.539999 5.2705 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(fp_text user "*"
			(at -2.539999 5.2705 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -2.54 8.8773 90)
			(size 0.9906 3.2004)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 62 "Net-(D11-K)")
			(pinfunction "G")
			(pintype "input")
		)
		(pad "2" smd rect
			(at 0 0.0508 90)
			(size 10.414 11.4554)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 27 "/LCL_5V/5V_6A_LCL_2/OPAMP_Minus")
			(pinfunction "D")
			(pintype "input")
		)
		(pad "3" smd rect
			(at 2.54 8.8773 90)
			(size 0.9906 3.2004)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 63 "/LCL_5.6A2")
			(pinfunction "S")
			(pintype "input")
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:RESC1608X55N"
		(layer "F.Cu")
		(at 51.8078 59.9192 90)
		(property "Reference" "R97"
			(at -2.37275 0.00045 90)
			(layer "F.SilkS")
		)
		(property "Value" "8.87k"
			(at 1.54 1.05 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/LCL_12V/12V_5A_LCL_2/")
		(sheetfile "12V_5A_LCL.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -0.82 0 90)
			(size 0.79 0.93)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 135 "Net-(R97-Pad1)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd rect
			(at 0.82 0 90)
			(size 0.79 0.93)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 56 "Net-(D8-K)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:RESC1608X55N"
		(layer "F.Cu")
		(at 241.67905 60.29195 180)
		(property "Reference" "R102"
			(at -0.11 1.25 0)
			(layer "F.SilkS")
		)
		(property "Value" "86.6k"
			(at 1.54 1.049999 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/LCL_5V/5V_6A_LCL_3/")
		(sheetfile "5V_6A_LCL.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -0.82 0 180)
			(size 0.79 0.93)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 58 "Net-(D9-K)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd rect
			(at 0.82 0 180)
			(size 0.79 0.93)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 24 "/LCL_5V/5V_6A_LCL_3/OPAMP_Minus")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:CAPC1608X90"
		(layer "F.Cu")
		(at 112.15295 61.29435 -90)
		(descr "<b>CAPACITOR</b>")
		(property "Reference" "C24"
			(at 2.7476 -0.1553 90)
			(layer "F.SilkS")
		)
		(property "Value" "0.1uF"
			(at 1.56646 1.20613 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "SMD 0603 MLCC capacitor, Alternate KiCad Library"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/LCL_12V/12V_3A_LCL_2/")
		(sheetfile "12V_3A_LCL.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -0.85 0 270)
			(size 1.1 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 18 "/LCL_12V/12V_3A_LCL_2/OPAMP_Minus")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd rect
			(at 0.85 0 270)
			(size 1.1 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 17 "Net-(Q6-B)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:RESC1608X55N"
		(layer "F.Cu")
		(at 53.85905 172.39195 -90)
		(property "Reference" "R58"
			(at -0.85 -1.1992 90)
			(layer "F.SilkS")
		)
		(property "Value" "86.6k"
			(at 1.54 1.05 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/LCL_12V/12V_12A_LCL_2/")
		(sheetfile "12V_12A_LCL.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -0.82 0 270)
			(size 0.79 0.93)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 9 "Net-(Q2-B)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd rect
			(at 0.82 0 270)
			(size 0.79 0.93)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 10 "/LCL_12V/12V_12A_LCL_2/OPAMP_Minus")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:RESC1508X55N"
		(layer "F.Cu")
		(at 248.10905 225.54195)
		(property "Reference" "R177"
			(at 1.4492 1.25 0)
			(layer "F.SilkS")
		)
		(property "Value" "100"
			(at 1.54 1.07 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Digital Systems/")
		(sheetfile "Digital_Systems.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -0.76 0)
			(size 0.9 0.97)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 199 "Net-(U45-P1_2)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd rect
			(at 0.76 0)
			(size 0.9 0.97)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 198 "/LCL_CTRL11")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:CAPC1608X90"
		(layer "F.Cu")
		(at 52.60905 104.19195 90)
		(descr "<b>CAPACITOR</b>")
		(property "Reference" "C22"
			(at 2.9 -0.0508 90)
			(layer "F.SilkS")
		)
		(property "Value" "0.1uF"
			(at 1.56646 1.20613 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "SMD 0603 MLCC capacitor, Alternate KiCad Library"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/LCL_12V/12V_12A_LCL_4/")
		(sheetfile "12V_12A_LCL.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -0.85 0 90)
			(size 1.1 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 13 "/LCL_12V/12V_12A_LCL_4/OPAMP_Minus")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd rect
			(at 0.85 0 90)
			(size 1.1 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 14 "Net-(Q4-B)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:DIP762W50P254L730H410Q6"
		(layer "F.Cu")
		(at 59.60905 60.3792 180)
		(property "Reference" "U26"
			(at -0.56 0.21 0)
			(layer "F.SilkS")
		)
		(property "Value" "CNY17-1"
			(at -0.31 1.96 0)
			(layer "Dwgs.User")
		)
		(property "Datasheet" "http://www.vishay.com/docs/83606/cny17.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "DC Optocoupler Base Connected, Vce 70V, CTR 40-80%, Viso 5000V (RMS), DIP6"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "DIP*W7.62mm* DIP*W10.16mm* SMDIP*W9.53mm*")
		(sheetname "/LCL_12V/12V_5A_LCL_2/")
		(sheetfile "12V_5A_LCL.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole rect
			(at -3.81 -2.54 180)
			(size 1.4 1.4)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 193 "/LCL_CTRL8")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" thru_hole circle
			(at -3.81 0 180)
			(size 1.4 1.4)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 303 "/GNDREF")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "3" thru_hole circle
			(at -3.81 2.54 180)
			(size 1.4 1.4)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 267 "unconnected-(U26-NC-Pad3)")
			(pinfunction "NC")
			(pintype "no_connect")
			(solder_mask_margin 0.102)
		)
		(pad "4" thru_hole circle
			(at 3.81 2.54 180)
			(size 1.4 1.4)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 303 "/GNDREF")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "5" thru_hole circle
			(at 3.81 0 180)
			(size 1.4 1.4)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 135 "Net-(R97-Pad1)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "6" thru_hole circle
			(at 3.81 -2.54 180)
			(size 1.4 1.4)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 268 "unconnected-(U26-Pad6)")
			(pintype "passive+no_connect")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:RESC1508X55N"
		(layer "F.Cu")
		(at 252.85905 198.79195 180)
		(property "Reference" "R151"
			(at -2.6992 -0.25 0)
			(layer "F.SilkS")
		)
		(property "Value" "22"
			(at 1.54 1.07 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Digital Systems/")
		(sheetfile "Digital_Systems.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -0.76 0 180)
			(size 0.9 0.97)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 166 "/Digital Systems/ADC2_CNVST")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd rect
			(at 0.76 0 180)
			(size 0.9 0.97)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 167 "Net-(U43-PF2)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:RESC1508X55N"
		(layer "F.Cu")
		(at 250.10905 178.54195 -90)
		(property "Reference" "R148"
			(at -0.21 -1.07 90)
			(layer "F.SilkS")
		)
		(property "Value" "22"
			(at 1.54 1.07 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Digital Systems/")
		(sheetfile "Digital_Systems.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -0.76 0 270)
			(size 0.9 0.97)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 162 "/Digital Systems/GPIO_INT")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd rect
			(at 0.76 0 270)
			(size 0.9 0.97)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 161 "Net-(U43-PD6)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:RESC1608X55N"
		(layer "F.Cu")
		(at 63.65905 217.37195 180)
		(property "Reference" "R52"
			(at -2.3992 0.08 0)
			(layer "F.SilkS")
		)
		(property "Value" "86.6k"
			(at 1.54 1.05 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/LCL_12V/12V_12A_LCL_1/")
		(sheetfile "12V_12A_LCL.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -0.82 0 180)
			(size 0.79 0.93)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 8 "Net-(Q1-B)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd rect
			(at 0.82 0 180)
			(size 0.79 0.93)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 7 "/LCL_12V/12V_12A_LCL_1/OPAMP_Minus")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:SOT91P240X120-3N"
		(layer "F.Cu")
		(at 63.13405 210.70695 90)
		(property "Reference" "Q1"
			(at -0.176 -2.3698 90)
			(layer "F.SilkS")
		)
		(property "Value" "PNP"
			(at 3.1768 2.3698 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://ngspice.sourceforge.io/docs/ngspice-html-manual/manual.xhtml#cha_BJTs"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Bipolar transistor symbol for simulation only, substrate tied to the emitter"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Device" "PNP"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Type" "GUMMELPOON"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" "1=C 2=B 3=E"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/LCL_12V/12V_12A_LCL_1/")
		(sheetfile "12V_12A_LCL.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -0.915 1.025 90)
			(size 0.61 1.18)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 42 "Net-(D1-K)")
			(pinfunction "C")
			(pintype "open_collector")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd rect
			(at 0.915 1.025 90)
			(size 0.61 1.18)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 8 "Net-(Q1-B)")
			(pinfunction "B")
			(pintype "input")
			(solder_mask_margin 0.102)
		)
		(pad "3" smd rect
			(at 0 -1.025 90)
			(size 0.61 1.18)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 7 "/LCL_12V/12V_12A_LCL_1/OPAMP_Minus")
			(pinfunction "E")
			(pintype "open_emitter")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:SOD3716X135N"
		(layer "F.Cu")
		(at 223.10905 52.541949 90)
		(descr "sod-123-ren1")
		(tags "Diode")
		(property "Reference" "D11"
			(at 0 0 90)
			(layer "F.SilkS")
		)
		(property "Value" "D"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Diode"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Device" "D"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TO-???* *_Diode_* *SingleDiode* D_*")
		(sheetname "/LCL_5V/5V_6A_LCL_2/")
		(sheetfile "5V_6A_LCL.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.65 0 180)
			(size 0.75 1.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 62 "Net-(D11-K)")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.65 0 180)
			(size 0.75 1.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 63 "/LCL_5.6A2")
			(pinfunction "A")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "1N4150W-E3-18.stp"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "EPS_Footprints:RESC1508X55N"
		(layer "F.Cu")
		(at 181.60905 241.29195 90)
		(property "Reference" "R131"
			(at 2.75 -0.0508 90)
			(layer "F.SilkS")
		)
		(property "Value" "20k"
			(at 1.54 1.07 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/LCL_9_and_3-3/3-3V_1-5A_LCL_1/")
		(sheetfile "3-3V_1-5A_LCL.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -0.76 0 90)
			(size 0.9 0.97)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 68 "Net-(D14-K)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd rect
			(at 0.76 0 90)
			(size 0.9 0.97)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 34 "Net-(Q14-B)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:BAQ33GS08"
		(layer "F.Cu")
		(at 290.484049 54.791949)
		(descr "MiniMELF (SOD-80)")
		(tags "Zener Diode")
		(property "Reference" "ZD12"
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "D_Zener"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Zener diode"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Library" "TZM5240B-GS08.txt"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Name" "TZM5240B-GS08"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Device" "D"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" "1=A 2=K"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TO-???* *_Diode_* *SingleDiode* D_*")
		(sheetname "/LCL_5V/5V_6A_LCL_4/")
		(sheetfile "5V_6A_LCL.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.875 0)
			(size 1.25 2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 30 "/LCL_5V/5V_6A_LCL_4/OPAMP_Minus")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.875 0)
			(size 1.25 2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 65 "Net-(D12-K)")
			(pinfunction "A")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "TZM5224B-GS08.stp"
			(offset
				(xyz 0 0 0.7999999999)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "EPS_Footprints:RESC1508X55N"
		(layer "F.Cu")
		(at 44.06905 199.31495 180)
		(property "Reference" "R10"
			(at -0.21 -1.07 0)
			(layer "F.SilkS")
		)
		(property "Value" "13.7k"
			(at 1.54 1.07 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Power_Connectors/")
		(sheetfile "Power_Connectors.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -0.76 0 180)
			(size 0.9 0.97)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 100 "Net-(R10-Pad1)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd rect
			(at 0.76 0 180)
			(size 0.9 0.97)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 303 "/GNDREF")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:Terminal Block 691137710002"
		(layer "F.Cu")
		(at 40.81905 206.31495 -90)
		(property "Reference" "J3"
			(at 0 -5.135 90)
			(layer "F.SilkS")
		)
		(property "Value" "691137710002"
			(at 4.12 5.365 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/Power_Connectors/")
		(sheetfile "Power_Connectors.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole circle
			(at -2.5 0 270)
			(size 1.95 1.95)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 303 "/GNDREF")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" thru_hole circle
			(at 2.5 0 270)
			(size 1.95 1.95)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 43 "/LCL_12.12A1")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:SOD3716X135N"
		(layer "F.Cu")
		(at 54.60905 201.29195 180)
		(descr "sod-123-ren1")
		(tags "Diode")
		(property "Reference" "D1"
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "D"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Diode"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Device" "D"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TO-???* *_Diode_* *SingleDiode* D_*")
		(sheetname "/LCL_12V/12V_12A_LCL_1/")
		(sheetfile "12V_12A_LCL.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.65 0 270)
			(size 0.75 1.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 42 "Net-(D1-K)")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.65 0 270)
			(size 0.75 1.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 43 "/LCL_12.12A1")
			(pinfunction "A")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "1N4150W-E3-18.stp"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "EPS_Footprints:SOD3716X135N"
		(layer "F.Cu")
		(at 59.5578 50.1692 90)
		(descr "sod-123-ren1")
		(tags "Diode")
		(property "Reference" "D8"
			(at 0 0 90)
			(layer "F.SilkS")
		)
		(property "Value" "D"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Diode"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Device" "D"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TO-???* *_Diode_* *SingleDiode* D_*")
		(sheetname "/LCL_12V/12V_5A_LCL_2/")
		(sheetfile "12V_5A_LCL.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.65 0 180)
			(size 0.75 1.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 56 "Net-(D8-K)")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.65 0 180)
			(size 0.75 1.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 57 "/LCL_12.5A2")
			(pinfunction "A")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "1N4150W-E3-18.stp"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "EPS_Footprints:DIP762W50P254L730H410Q6"
		(layer "F.Cu")
		(at 158.674041 61.313259 180)
		(property "Reference" "U20"
			(at 0 0.5 0)
			(layer "F.SilkS")
		)
		(property "Value" "CNY17-1"
			(at -0.21 9.94 0)
			(layer "Dwgs.User")
		)
		(property "Datasheet" "http://www.vishay.com/docs/83606/cny17.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "DC Optocoupler Base Connected, Vce 70V, CTR 40-80%, Viso 5000V (RMS), DIP6"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "DIP*W7.62mm* DIP*W10.16mm* SMDIP*W9.53mm*")
		(sheetname "/LCL_12V/12V_3A_LCL_1/")
		(sheetfile "12V_3A_LCL.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole rect
			(at -3.81 -2.54 180)
			(size 1.4 1.4)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 186 "/LCL_CTRL5")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" thru_hole circle
			(at -3.81 0 180)
			(size 1.4 1.4)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 303 "/GNDREF")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "3" thru_hole circle
			(at -3.81 2.54 180)
			(size 1.4 1.4)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 261 "unconnected-(U20-NC-Pad3)")
			(pinfunction "NC")
			(pintype "no_connect")
			(solder_mask_margin 0.102)
		)
		(pad "4" thru_hole circle
			(at 3.81 2.54 180)
			(size 1.4 1.4)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 303 "/GNDREF")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "5" thru_hole circle
			(at 3.81 0 180)
			(size 1.4 1.4)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 132 "Net-(R79-Pad1)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "6" thru_hole circle
			(at 3.81 -2.54 180)
			(size 1.4 1.4)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 262 "unconnected-(U20-Pad6)")
			(pintype "passive+no_connect")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:M14A"
		(layer "F.Cu")
		(at 94.07285 155.35195)
		(tags "LPV324MX/NOPB ")
		(property "Reference" "U5"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "LPV324MX/NOPB"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://www.ti.com/lit/gpn/lpv324-n"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "M14A M14A-M M14A-L")
		(sheetname "/Power_Connectors/")
		(sheetfile "Power_Connectors.kicad_sch")
		(attr smd)
		(fp_text user "*"
			(at -2.7178 -5.5118 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(fp_text user "*"
			(at -2.7178 -5.5118 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -2.4638 -3.81)
			(size 1.9812 0.5588)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 226 "/V_MEAS.12_1")
			(pinfunction "OUT")
			(pintype "output")
		)
		(pad "2" smd rect
			(at -2.4638 -2.54)
			(size 1.9812 0.5588)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 104 "Net-(U5A-IN-)")
			(pinfunction "IN-")
			(pintype "input")
		)
		(pad "3" smd rect
			(at -2.4638 -1.27)
			(size 1.9812 0.5588)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 226 "/V_MEAS.12_1")
			(pinfunction "IN+")
			(pintype "input")
		)
		(pad "4" smd rect
			(at -2.4638 0)
			(size 1.9812 0.5588)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 72 "/DC_POS.3.3V")
			(pinfunction "V+")
			(pintype "input")
		)
		(pad "5" smd rect
			(at -2.4638 1.27)
			(size 1.9812 0.5588)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 225 "/V_MEAS.12_2")
			(pinfunction "IN+")
			(pintype "input")
		)
		(pad "6" smd rect
			(at -2.4638 2.54)
			(size 1.9812 0.5588)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 105 "Net-(U5B-IN-)")
			(pinfunction "IN-")
			(pintype "input")
		)
		(pad "7" smd rect
			(at -2.4638 3.81)
			(size 1.9812 0.5588)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 225 "/V_MEAS.12_2")
			(pinfunction "OUT")
			(pintype "output")
		)
		(pad "8" smd rect
			(at 2.4638 3.81)
			(size 1.9812 0.5588)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 227 "/V_MEAS.12_3")
			(pinfunction "OUT")
			(pintype "output")
		)
		(pad "9" smd rect
			(at 2.4638 2.54)
			(size 1.9812 0.5588)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 106 "Net-(U5C-IN-)")
			(pinfunction "IN-")
			(pintype "input")
		)
		(pad "10" smd rect
			(at 2.4638 1.27)
			(size 1.9812 0.5588)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 227 "/V_MEAS.12_3")
			(pinfunction "IN+")
			(pintype "input")
		)
		(pad "11" smd rect
			(at 2.4638 0)
			(size 1.9812 0.5588)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 303 "/GNDREF")
			(pinfunction "V-")
			(pintype "input")
		)
		(pad "12" smd rect
			(at 2.4638 -1.27)
			(size 1.9812 0.5588)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 228 "/V_MEAS.12_4")
			(pinfunction "IN+")
			(pintype "input")
		)
		(pad "13" smd rect
			(at 2.4638 -2.54)
			(size 1.9812 0.5588)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 107 "Net-(U5D-IN-)")
			(pinfunction "IN-")
			(pintype "input")
		)
		(pad "14" smd rect
			(at 2.4638 -3.81)
			(size 1.9812 0.5588)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 228 "/V_MEAS.12_4")
			(pinfunction "OUT")
			(pintype "output")
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:RESC1508X55N"
		(layer "F.Cu")
		(at 235.35905 232.29195)
		(property "Reference" "R173"
			(at -2.5508 -0.5 0)
			(layer "F.SilkS")
		)
		(property "Value" "100"
			(at 1.54 1.07 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Digital Systems/")
		(sheetfile "Digital_Systems.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -0.76 0)
			(size 0.9 0.97)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 193 "/LCL_CTRL8")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd rect
			(at 0.76 0)
			(size 0.9 0.97)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 192 "Net-(U45-P0_7)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:SOP63P602X175-24N"
		(layer "F.Cu")
		(at 215.99405 191.53445)
		(property "Reference" "U44"
			(at -0.46 -5.182 0)
			(layer "F.SilkS")
		)
		(property "Value" "MAX11643EEG_"
			(at 7.16 5.182 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DigiKey_Part_Number" "MAX11643EEG+-ND"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SnapEDA_Link" "https://www.snapeda.com/parts/MAX11643EEG+/Analog+Devices/view-part/?ref=snap"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description_1" "8-Bit, 16-/8-Channel, 300ksps ADCs with FIFO and Internal Reference"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MF" "Analog Devices"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Package" "QSOP-24 Maxim"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Check_prices" "https://www.snapeda.com/parts/MAX11643EEG+/Analog+Devices/view-part/?ref=eda"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MP" "MAX11643EEG+"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/Digital Systems/")
		(sheetfile "Digital_Systems.kicad_sch")
		(attr smd)
		(pad "1" smd roundrect
			(at -2.635 -3.4925)
			(size 1.64 0.41)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.125)
			(net 272 "/I_MEAS.5_1")
			(pinfunction "AIN0")
			(pintype "input")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd roundrect
			(at -2.635 -2.8575)
			(size 1.64 0.41)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.125)
			(net 269 "/I_MEAS.5_2")
			(pinfunction "AIN1")
			(pintype "input")
			(solder_mask_margin 0.102)
		)
		(pad "3" smd roundrect
			(at -2.635 -2.2225)
			(size 1.64 0.41)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.125)
			(net 271 "/I_MEAS.5_3")
			(pinfunction "AIN2")
			(pintype "input")
			(solder_mask_margin 0.102)
		)
		(pad "4" smd roundrect
			(at -2.635 -1.5875)
			(size 1.64 0.41)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.125)
			(net 270 "/I_MEAS.5_4")
			(pinfunction "AIN3")
			(pintype "input")
			(solder_mask_margin 0.102)
		)
		(pad "5" smd roundrect
			(at -2.635 -0.9525)
			(size 1.64 0.41)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.125)
			(net 250 "/I_MEAS.12_7")
			(pinfunction "AIN4")
			(pintype "input")
			(solder_mask_margin 0.102)
		)
		(pad "6" smd roundrect
			(at -2.635 -0.3175)
			(size 1.64 0.41)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.125)
			(net 249 "/I_MEAS.12_8")
			(pinfunction "AIN5")
			(pintype "input")
			(solder_mask_margin 0.102)
		)
		(pad "7" smd roundrect
			(at -2.635 0.3175)
			(size 1.64 0.41)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.125)
			(net 283 "/I_MEAS.9_")
			(pinfunction "AIN6")
			(pintype "input")
			(solder_mask_margin 0.102)
		)
		(pad "8" smd roundrect
			(at -2.635 0.9525)
			(size 1.64 0.41)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.125)
			(net 286 "/I_MEAS.3.3_")
			(pinfunction "AIN7")
			(pintype "input")
			(solder_mask_margin 0.102)
		)
		(pad "9" smd roundrect
			(at -2.635 1.5875)
			(size 1.64 0.41)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.125)
			(net 229 "/V_MEAS.12_7")
			(pinfunction "AIN8")
			(pintype "input")
			(solder_mask_margin 0.102)
		)
		(pad "10" smd roundrect
			(at -2.635 2.2225)
			(size 1.64 0.41)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.125)
			(net 230 "/V_MEAS.12_8")
			(pinfunction "AIN9")
			(pintype "input")
			(solder_mask_margin 0.102)
		)
		(pad "11" smd roundrect
			(at -2.635 2.8575)
			(size 1.64 0.41)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.125)
			(net 240 "/V_MEAS.9_")
			(pinfunction "AIN10")
			(pintype "input")
			(solder_mask_margin 0.102)
		)
		(pad "12" smd roundrect
			(at -2.635 3.4925)
			(size 1.64 0.41)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.125)
			(net 237 "/V_MEAS.3.3_")
			(pinfunction "AIN11")
			(pintype "input")
			(solder_mask_margin 0.102)
		)
		(pad "13" smd roundrect
			(at 2.635 3.4925)
			(size 1.64 0.41)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.125)
			(net 299 "unconnected-(U44-AIN12-Pad13)")
			(pinfunction "AIN12")
			(pintype "input+no_connect")
			(solder_mask_margin 0.102)
		)
		(pad "14" smd roundrect
			(at 2.635 2.8575)
			(size 1.64 0.41)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.125)
			(net 252 "/I_MEAS.12_5")
			(pinfunction "AIN13")
			(pintype "input")
			(solder_mask_margin 0.102)
		)
		(pad "15" smd roundrect
			(at 2.635 2.2225)
			(size 1.64 0.41)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.125)
			(net 251 "/I_MEAS.12_6")
			(pinfunction "AIN14")
			(pintype "input")
			(solder_mask_margin 0.102)
		)
		(pad "16" smd roundrect
			(at 2.635 1.5875)
			(size 1.64 0.41)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.125)
			(net 173 "Net-(U44-~{CNVST}{slash}AIN15)")
			(pinfunction "~{CNVST}/AIN15")
			(pintype "input")
			(solder_mask_margin 0.102)
		)
		(pad "17" smd roundrect
			(at 2.635 0.9525)
			(size 1.64 0.41)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.125)
			(net 39 "Net-(U44-REF)")
			(pinfunction "REF")
			(pintype "input")
			(solder_mask_margin 0.102)
		)
		(pad "18" smd roundrect
			(at 2.635 0.3175)
			(size 1.64 0.41)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.125)
			(net 303 "/GNDREF")
			(pinfunction "GND")
			(pintype "power_in")
			(solder_mask_margin 0.102)
		)
		(pad "19" smd roundrect
			(at 2.635 -0.3175)
			(size 1.64 0.41)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.125)
			(net 35 "/Digital Systems/3.3V+")
			(pinfunction "VDD")
			(pintype "power_in")
			(solder_mask_margin 0.102)
		)
		(pad "20" smd roundrect
			(at 2.635 -0.9525)
			(size 1.64 0.41)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.125)
			(net 176 "Net-(U44-~{CS})")
			(pinfunction "~{CS}")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "21" smd roundrect
			(at 2.635 -1.5875)
			(size 1.64 0.41)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.125)
			(net 175 "Net-(U44-SCLK)")
			(pinfunction "SCLK")
			(pintype "input")
			(solder_mask_margin 0.102)
		)
		(pad "22" smd roundrect
			(at 2.635 -2.2225)
			(size 1.64 0.41)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.125)
			(net 174 "Net-(U44-DIN)")
			(pinfunction "DIN")
			(pintype "input")
			(solder_mask_margin 0.102)
		)
		(pad "23" smd roundrect
			(at 2.635 -2.8575)
			(size 1.64 0.41)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.125)
			(net 206 "Net-(U44-DOUT)")
			(pinfunction "DOUT")
			(pintype "output")
			(solder_mask_margin 0.102)
		)
		(pad "24" smd roundrect
			(at 2.635 -3.4925)
			(size 1.64 0.41)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.125)
			(net 177 "Net-(U44-~{EOC})")
			(pinfunction "~{EOC}")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:SOD3716X135N"
		(layer "F.Cu")
		(at 93.508225 50.769375 90)
		(descr "sod-123-ren1")
		(tags "Diode")
		(property "Reference" "D7"
			(at 0 0 90)
			(layer "F.SilkS")
		)
		(property "Value" "D"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Diode"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Device" "D"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TO-???* *_Diode_* *SingleDiode* D_*")
		(sheetname "/LCL_12V/12V_5A_LCL_1/")
		(sheetfile "12V_5A_LCL.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.65 0 180)
			(size 0.75 1.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 55 "Net-(D7-K)")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.65 0 180)
			(size 0.75 1.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 54 "/LCL_12.5A1")
			(pinfunction "A")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "1N4150W-E3-18.stp"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "EPS_Footprints:RESC1608X55N"
		(layer "F.Cu")
		(at 120.90295 61.79435 90)
		(property "Reference" "R85"
			(at -2.2476 -0.0947 90)
			(layer "F.SilkS")
		)
		(property "Value" "8.87k"
			(at 1.54 1.05 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/LCL_12V/12V_3A_LCL_2/")
		(sheetfile "12V_3A_LCL.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -0.82 0 90)
			(size 0.79 0.93)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 133 "Net-(R85-Pad1)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd rect
			(at 0.82 0 90)
			(size 0.79 0.93)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 52 "Net-(D6-K)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:RESC1608X55N"
		(layer "F.Cu")
		(at 59.46405 241.51895 180)
		(property "Reference" "R127"
			(at -2.5942 -0.023 0)
			(layer "F.SilkS")
		)
		(property "Value" "8.87k"
			(at 1.54 1.05 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/LCL_9_and_3-3/9V_2A_LCL_1/")
		(sheetfile "9V_2A_LCL.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -0.82 0 180)
			(size 0.79 0.93)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 140 "Net-(R127-Pad1)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd rect
			(at 0.82 0 180)
			(size 0.79 0.93)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 67 "Net-(D13-K)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:SOT91P240X120-3N"
		(layer "F.Cu")
		(at 47.60905 172.29195 180)
		(property "Reference" "Q2"
			(at -0.176 -2.3698 0)
			(layer "F.SilkS")
		)
		(property "Value" "PNP"
			(at 3.1768 2.3698 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://ngspice.sourceforge.io/docs/ngspice-html-manual/manual.xhtml#cha_BJTs"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Bipolar transistor symbol for simulation only, substrate tied to the emitter"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Device" "PNP"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Type" "GUMMELPOON"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" "1=C 2=B 3=E"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/LCL_12V/12V_12A_LCL_2/")
		(sheetfile "12V_12A_LCL.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -0.915 1.025 180)
			(size 0.61 1.18)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 44 "Net-(D2-K)")
			(pinfunction "C")
			(pintype "open_collector")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd rect
			(at 0.915 1.025 180)
			(size 0.61 1.18)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 9 "Net-(Q2-B)")
			(pinfunction "B")
			(pintype "input")
			(solder_mask_margin 0.102)
		)
		(pad "3" smd rect
			(at 0 -1.025 180)
			(size 0.61 1.18)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 10 "/LCL_12V/12V_12A_LCL_2/OPAMP_Minus")
			(pinfunction "E")
			(pintype "open_emitter")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:RESC1508X55N"
		(layer "F.Cu")
		(at 50.35905 172.39195 90)
		(property "Reference" "R59"
			(at 2.35 0.1992 90)
			(layer "F.SilkS")
		)
		(property "Value" "54.9k"
			(at 1.54 1.07 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/LCL_12V/12V_12A_LCL_2/")
		(sheetfile "12V_12A_LCL.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -0.76 0 90)
			(size 0.9 0.97)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 44 "Net-(D2-K)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd rect
			(at 0.76 0 90)
			(size 0.9 0.97)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 9 "Net-(Q2-B)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:RES_TLRP3A30DR018FTE_TEC"
		(layer "F.Cu")
		(at 229.359049 50.541949 180)
		(tags "TLRP3A30DR018FTE ")
		(property "Reference" "R111"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "0.01"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/LCL_5V/5V_6A_LCL_2/")
		(sheetfile "5V_6A_LCL.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -2.8321 0 180)
			(size 1.397 3.4544)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 4 "/DC_POS.5V")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 2.8321 0 180)
			(size 1.397 3.4544)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 27 "/LCL_5V/5V_6A_LCL_2/OPAMP_Minus")
			(pintype "passive")
		)
		(zone
			(net 0)
			(net_name "")
			(layer "F.Cu")
			(hatch full 0.508)
			(connect_pads
				(clearance 0)
			)
			(min_thickness 0.254)
			(filled_areas_thickness no)
			(keepout
				(tracks not_allowed)
				(vias not_allowed)
				(pads allowed)
				(copperpour not_allowed)
				(footprints allowed)
			)
			(placement
				(enabled no)
				(sheetname "")
			)
			(fill
				(thermal_gap 0.508)
				(thermal_bridge_width 0.508)
			)
			(polygon
				(pts
					(xy 231.441849 52.218349) (xy 227.276249 52.218349) (xy 227.276249 48.865549) (xy 231.441849 48.865549)
				)
			)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:TO-263AB_SUM"
		(layer "F.Cu")
		(at 113.00265 51.47435 90)
		(tags "SUM110P06-08L-E3 ")
		(property "Reference" "U21"
			(at 1.1824 -6.4444 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "SUM110P06-08L-E3"
			(at 0.43 0 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "SUM110P06-08L-E3"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TO-263AB_SUM TO-263AB_SUM-M TO-263AB_SUM-L")
		(sheetname "/LCL_12V/12V_3A_LCL_2/")
		(sheetfile "12V_3A_LCL.kicad_sch")
		(attr smd)
		(fp_text user "*"
			(at -2.54 5.2705 90)
			(layer "F.Fab")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(fp_text user "*"
			(at -2.54 5.2705 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -2.54 8.8773 90)
			(size 0.9906 3.2004)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 52 "Net-(D6-K)")
			(pinfunction "G")
			(pintype "input")
		)
		(pad "2" smd rect
			(at 0 0.0508 90)
			(size 10.414 11.4554)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 18 "/LCL_12V/12V_3A_LCL_2/OPAMP_Minus")
			(pinfunction "D")
			(pintype "input")
		)
		(pad "3" smd rect
			(at 2.54 8.8773 90)
			(size 0.9906 3.2004)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 53 "/LCL_12.3A2")
			(pinfunction "S")
			(pintype "input")
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:RESC1508X55N"
		(layer "F.Cu")
		(at 238.92905 62.791949 90)
		(property "Reference" "R100"
			(at -0.21 -1.07 90)
			(layer "F.SilkS")
		)
		(property "Value" "11.5k"
			(at 1.54 1.069999 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/LCL_5V/5V_6A_LCL_3/")
		(sheetfile "5V_6A_LCL.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -0.76 0 90)
			(size 0.9 0.97)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 23 "Net-(Q9-B)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd rect
			(at 0.76 0 90)
			(size 0.9 0.97)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 24 "/LCL_5V/5V_6A_LCL_3/OPAMP_Minus")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:DIP762W50P254L730H410Q6"
		(layer "F.Cu")
		(at 126.65295 60.97435 180)
		(property "Reference" "U22"
			(at 0 0.5 0)
			(layer "F.SilkS")
		)
		(property "Value" "CNY17-1"
			(at -0.21 9.94 0)
			(layer "Dwgs.User")
		)
		(property "Datasheet" "http://www.vishay.com/docs/83606/cny17.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "DC Optocoupler Base Connected, Vce 70V, CTR 40-80%, Viso 5000V (RMS), DIP6"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "DIP*W7.62mm* DIP*W10.16mm* SMDIP*W9.53mm*")
		(sheetname "/LCL_12V/12V_3A_LCL_2/")
		(sheetfile "12V_3A_LCL.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole rect
			(at -3.81 -2.54 180)
			(size 1.4 1.4)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 189 "/LCL_CTRL6")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" thru_hole circle
			(at -3.81 0 180)
			(size 1.4 1.4)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 303 "/GNDREF")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "3" thru_hole circle
			(at -3.81 2.54 180)
			(size 1.4 1.4)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 264 "unconnected-(U22-NC-Pad3)")
			(pinfunction "NC")
			(pintype "no_connect")
			(solder_mask_margin 0.102)
		)
		(pad "4" thru_hole circle
			(at 3.81 2.54 180)
			(size 1.4 1.4)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 303 "/GNDREF")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "5" thru_hole circle
			(at 3.81 0 180)
			(size 1.4 1.4)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 133 "Net-(R85-Pad1)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "6" thru_hole circle
			(at 3.81 -2.54 180)
			(size 1.4 1.4)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 263 "unconnected-(U22-Pad6)")
			(pintype "passive+no_connect")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:M14A"
		(layer "F.Cu")
		(at 219.60905 81.04195)
		(tags "LPV324MX/NOPB ")
		(property "Reference" "U7"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "LPV324MX/NOPB"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://www.ti.com/lit/gpn/lpv324-n"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "M14A M14A-M M14A-L")
		(sheetname "/Power_Connectors/")
		(sheetfile "Power_Connectors.kicad_sch")
		(attr smd)
		(fp_text user "*"
			(at -2.7178 -5.5118 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(fp_text user "*"
			(at -2.7178 -5.5118 0)
			(layer "F.Fab")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -2.4638 -3.81)
			(size 1.9812 0.5588)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 234 "/V_MEAS.5_1")
			(pinfunction "OUT")
			(pintype "output")
		)
		(pad "2" smd rect
			(at -2.4638 -2.54)
			(size 1.9812 0.5588)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 120 "Net-(U7A-IN-)")
			(pinfunction "IN-")
			(pintype "input")
		)
		(pad "3" smd rect
			(at -2.4638 -1.27)
			(size 1.9812 0.5588)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 234 "/V_MEAS.5_1")
			(pinfunction "IN+")
			(pintype "input")
		)
		(pad "4" smd rect
			(at -2.4638 0)
			(size 1.9812 0.5588)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 72 "/DC_POS.3.3V")
			(pinfunction "V+")
			(pintype "input")
		)
		(pad "5" smd rect
			(at -2.4638 1.27)
			(size 1.9812 0.5588)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 233 "/V_MEAS.5_2")
			(pinfunction "IN+")
			(pintype "input")
		)
		(pad "6" smd rect
			(at -2.4638 2.54)
			(size 1.9812 0.5588)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 121 "Net-(U7B-IN-)")
			(pinfunction "IN-")
			(pintype "input")
		)
		(pad "7" smd rect
			(at -2.4638 3.81)
			(size 1.9812 0.5588)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 233 "/V_MEAS.5_2")
			(pinfunction "OUT")
			(pintype "output")
		)
		(pad "8" smd rect
			(at 2.4638 3.81)
			(size 1.9812 0.5588)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 236 "/V_MEAS.5_3")
			(pinfunction "OUT")
			(pintype "output")
		)
		(pad "9" smd rect
			(at 2.4638 2.54)
			(size 1.9812 0.5588)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 122 "Net-(U7C-IN-)")
			(pinfunction "IN-")
			(pintype "input")
		)
		(pad "10" smd rect
			(at 2.4638 1.27)
			(size 1.9812 0.5588)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 236 "/V_MEAS.5_3")
			(pinfunction "IN+")
			(pintype "input")
		)
		(pad "11" smd rect
			(at 2.4638 0)
			(size 1.9812 0.5588)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 303 "/GNDREF")
			(pinfunction "V-")
			(pintype "input")
		)
		(pad "12" smd rect
			(at 2.4638 -1.27)
			(size 1.9812 0.5588)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 235 "/V_MEAS.5_4")
			(pinfunction "IN+")
			(pintype "input")
		)
		(pad "13" smd rect
			(at 2.4638 -2.54)
			(size 1.9812 0.5588)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 123 "Net-(U7D-IN-)")
			(pinfunction "IN-")
			(pintype "input")
		)
		(pad "14" smd rect
			(at 2.4638 -3.81)
			(size 1.9812 0.5588)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 235 "/V_MEAS.5_4")
			(pinfunction "OUT")
			(pintype "output")
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:RESC1608X55N"
		(layer "F.Cu")
		(at 145.104041 58.883259 180)
		(property "Reference" "R78"
			(at 2.545791 -0.45 0)
			(layer "F.SilkS")
		)
		(property "Value" "86.6k"
			(at 1.54 1.05 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/LCL_12V/12V_3A_LCL_1/")
		(sheetfile "12V_3A_LCL.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -0.82 0 180)
			(size 0.79 0.93)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 51 "Net-(D5-K)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd rect
			(at 0.82 0 180)
			(size 0.79 0.93)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 16 "/LCL_12V/12V_3A_LCL_1/OPAMP_Minus")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:RESC1508X55N"
		(layer "F.Cu")
		(at 47.32905 199.31495 180)
		(property "Reference" "R9"
			(at -0.21 -1.07 0)
			(layer "F.SilkS")
		)
		(property "Value" "100k"
			(at 1.54 1.07 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Power_Connectors/")
		(sheetfile "Power_Connectors.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -0.76 0 180)
			(size 0.9 0.97)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 43 "/LCL_12.12A1")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd rect
			(at 0.76 0 180)
			(size 0.9 0.97)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 100 "Net-(R10-Pad1)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:RES_TLRP3A30DR018FTE_TEC"
		(layer "F.Cu")
		(at 198.80825 50.79195 180)
		(tags "TLRP3A30DR018FTE ")
		(property "Reference" "R105"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "0.01"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/LCL_5V/5V_6A_LCL_1/")
		(sheetfile "5V_6A_LCL.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -2.8321 0 180)
			(size 1.397 3.4544)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 4 "/DC_POS.5V")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 2.8321 0 180)
			(size 1.397 3.4544)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 26 "/LCL_5V/5V_6A_LCL_1/OPAMP_Minus")
			(pintype "passive")
		)
		(zone
			(net 0)
			(net_name "")
			(layer "F.Cu")
			(hatch full 0.508)
			(connect_pads
				(clearance 0)
			)
			(min_thickness 0.254)
			(filled_areas_thickness no)
			(keepout
				(tracks not_allowed)
				(vias not_allowed)
				(pads allowed)
				(copperpour not_allowed)
				(footprints allowed)
			)
			(placement
				(enabled no)
				(sheetname "")
			)
			(fill
				(thermal_gap 0.508)
				(thermal_bridge_width 0.508)
			)
			(polygon
				(pts
					(xy 200.89105 52.46835) (xy 196.72545 52.46835) (xy 196.72545 49.11555) (xy 200.89105 49.11555)
				)
			)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:TO-263AB_SUM"
		(layer "F.Cu")
		(at 52.95855 148.09275 180)
		(tags "SUM110P06-08L-E3 ")
		(property "Reference" "U15"
			(at -0.5997 -6.4492 180)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "SUM110P06-08L-E3"
			(at -0.339999 3.193 180)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "SUM110P06-08L-E3"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TO-263AB_SUM TO-263AB_SUM-M TO-263AB_SUM-L")
		(sheetname "/LCL_12V/12V_12A_LCL_3/")
		(sheetfile "12V_12A_LCL.kicad_sch")
		(attr smd)
		(fp_text user "*"
			(at -5.714999 8.8773 0)
			(layer "F.SilkS")
		)
		(fp_text user "*"
			(at -5.714999 8.8773 180)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "*"
			(at -2.539999 5.2705 0)
			(layer "F.Fab")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
		)
		(fp_text user "*"
			(at -2.539999 5.2705 180)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -2.54 8.8773 180)
			(size 0.9906 3.2004)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 46 "Net-(D3-K)")
			(pinfunction "G")
			(pintype "input")
		)
		(pad "2" smd rect
			(at 0 0.0508 180)
			(size 10.414 11.4554)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 11 "/LCL_12V/12V_12A_LCL_3/OPAMP_Minus")
			(pinfunction "D")
			(pintype "input")
		)
		(pad "3" smd rect
			(at 2.54 8.8773 180)
			(size 0.9906 3.2004)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 47 "/LCL_12.12A3")
			(pinfunction "S")
			(pintype "input")
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:RESC1608X55N"
		(layer "F.Cu")
		(at 218.85905 60.29195 90)
		(property "Reference" "R115"
			(at -2.75 -0.0508 90)
			(layer "F.SilkS")
		)
		(property "Value" "5.1k"
			(at 1.54 1.049999 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/LCL_5V/5V_6A_LCL_2/")
		(sheetfile "5V_6A_LCL.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -0.82 0 90)
			(size 0.79 0.93)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 138 "Net-(R115-Pad1)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd rect
			(at 0.82 0 90)
			(size 0.79 0.93)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 62 "Net-(D11-K)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:SOD3716X135N"
		(layer "F.Cu")
		(at 38.60905 113.04195 -90)
		(descr "sod-123-ren1")
		(tags "Diode")
		(property "Reference" "D4"
			(at 0 0 90)
			(layer "F.SilkS")
		)
		(property "Value" "D"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Diode"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Device" "D"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TO-???* *_Diode_* *SingleDiode* D_*")
		(sheetname "/LCL_12V/12V_12A_LCL_4/")
		(sheetfile "12V_12A_LCL.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.65 0)
			(size 0.75 1.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 49 "Net-(D4-K)")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.65 0)
			(size 0.75 1.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 48 "/LCL_12.12A4")
			(pinfunction "A")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "1N4150W-E3-18.stp"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "EPS_Footprints:CAPC1608X90"
		(layer "F.Cu")
		(at 222.10905 202.79195)
		(descr "<b>CAPACITOR</b>")
		(property "Reference" "C33"
			(at 0.1992 1.25 0)
			(layer "F.SilkS")
		)
		(property "Value" "0.1uF"
			(at 1.32646 0.45613 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "SMD 0603 MLCC capacitor, Alternate KiCad Library"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/Digital Systems/")
		(sheetfile "Digital_Systems.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -0.85 0)
			(size 1.1 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 35 "/Digital Systems/3.3V+")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd rect
			(at 0.85 0)
			(size 1.1 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 303 "/GNDREF")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:SOT91P240X120-3N"
		(layer "F.Cu")
		(at 116.48795 61.26935)
		(property "Reference" "Q6"
			(at -0.176 -2.3698 0)
			(layer "F.SilkS")
		)
		(property "Value" "PNP"
			(at 3.1768 2.3698 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://ngspice.sourceforge.io/docs/ngspice-html-manual/manual.xhtml#cha_BJTs"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Bipolar transistor symbol for simulation only, substrate tied to the emitter"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Device" "PNP"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Type" "GUMMELPOON"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" "1=C 2=B 3=E"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/LCL_12V/12V_3A_LCL_2/")
		(sheetfile "12V_3A_LCL.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -0.915 1.025)
			(size 0.61 1.18)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 52 "Net-(D6-K)")
			(pinfunction "C")
			(pintype "open_collector")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd rect
			(at 0.915 1.025)
			(size 0.61 1.18)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 17 "Net-(Q6-B)")
			(pinfunction "B")
			(pintype "input")
			(solder_mask_margin 0.102)
		)
		(pad "3" smd rect
			(at 0 -1.025)
			(size 0.61 1.18)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 18 "/LCL_12V/12V_3A_LCL_2/OPAMP_Minus")
			(pinfunction "E")
			(pintype "open_emitter")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:RESC1508X55N"
		(layer "F.Cu")
		(at 151.174041 62.133258 90)
		(property "Reference" "R80"
			(at -2.408692 -0.115791 90)
			(layer "F.SilkS")
		)
		(property "Value" "54.9k"
			(at 1.54 1.069999 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/LCL_12V/12V_3A_LCL_1/")
		(sheetfile "12V_3A_LCL.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -0.76 0 90)
			(size 0.9 0.97)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 132 "Net-(R79-Pad1)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd rect
			(at 0.76 0 90)
			(size 0.9 0.97)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 51 "Net-(D5-K)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:RESC1508X55N"
		(layer "F.Cu")
		(at 126.65295 44.22435 -90)
		(property "Reference" "R30"
			(at -0.21 -1.07 90)
			(layer "F.SilkS")
		)
		(property "Value" "1k"
			(at 1.54 1.07 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Power_Connectors/")
		(sheetfile "Power_Connectors.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -0.76 0 270)
			(size 0.9 0.97)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 113 "Net-(U6B-IN-)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd rect
			(at 0.76 0 270)
			(size 0.9 0.97)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 109 "Net-(R23-Pad2)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:RESC1508X55N"
		(layer "F.Cu")
		(at 45.85905 235.04195)
		(property "Reference" "R49"
			(at -0.21 -1.07 0)
			(layer "F.SilkS")
		)
		(property "Value" "1k"
			(at 1.54 1.07 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Power_Connectors/")
		(sheetfile "Power_Connectors.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -0.76 0)
			(size 0.9 0.97)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 126 "Net-(U8A-IN-)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd rect
			(at 0.76 0)
			(size 0.9 0.97)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 124 "Net-(R45-Pad2)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:RESC1508X55N"
		(layer "F.Cu")
		(at 185.10905 241.19195 -90)
		(property "Reference" "R130"
			(at -2.9 -0.1992 90)
			(layer "F.SilkS")
		)
		(property "Value" "10k"
			(at 1.54 1.07 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/LCL_9_and_3-3/3-3V_1-5A_LCL_1/")
		(sheetfile "3-3V_1-5A_LCL.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -0.76 0 270)
			(size 0.9 0.97)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 34 "Net-(Q14-B)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd rect
			(at 0.76 0 270)
			(size 0.9 0.97)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 33 "/LCL_9_and_3-3/3-3V_1-5A_LCL_1/OPAMP_Minus")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:BAQ33GS08"
		(layer "F.Cu")
		(at 228.984049 54.791949)
		(descr "MiniMELF (SOD-80)")
		(tags "Zener Diode")
		(property "Reference" "ZD11"
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "D_Zener"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Zener diode"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Library" "TZM5240B-GS08.txt"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Name" "TZM5240B-GS08"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Device" "D"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" "1=A 2=K"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TO-???* *_Diode_* *SingleDiode* D_*")
		(sheetname "/LCL_5V/5V_6A_LCL_2/")
		(sheetfile "5V_6A_LCL.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.875 0)
			(size 1.25 2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 27 "/LCL_5V/5V_6A_LCL_2/OPAMP_Minus")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.875 0)
			(size 1.25 2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 62 "Net-(D11-K)")
			(pinfunction "A")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "TZM5224B-GS08.stp"
			(offset
				(xyz 0 0 0.7999999999)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "EPS_Footprints:RESC1608X55N"
		(layer "F.Cu")
		(at 60.17905 247.54195)
		(property "Reference" "R125"
			(at 2.8792 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "45.3k"
			(at 1.54 1.05 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/LCL_9_and_3-3/9V_2A_LCL_1/")
		(sheetfile "9V_2A_LCL.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -0.82 0)
			(size 0.79 0.93)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 67 "Net-(D13-K)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd rect
			(at 0.82 0)
			(size 0.79 0.93)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 31 "Net-(Q13-B)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:RESC1608X55N"
		(layer "F.Cu")
		(at 54.35905 104.19195 -90)
		(property "Reference" "R70"
			(at -2.65 -0.1992 90)
			(layer "F.SilkS")
		)
		(property "Value" "86.6k"
			(at 1.54 1.049999 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/LCL_12V/12V_12A_LCL_4/")
		(sheetfile "12V_12A_LCL.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -0.82 0 270)
			(size 0.79 0.93)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 14 "Net-(Q4-B)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd rect
			(at 0.82 0 270)
			(size 0.79 0.93)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 13 "/LCL_12V/12V_12A_LCL_4/OPAMP_Minus")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:RESC1508X55N"
		(layer "F.Cu")
		(at 42.10905 130.80195 -90)
		(property "Reference" "R15"
			(at -0.21 -1.07 90)
			(layer "F.SilkS")
		)
		(property "Value" "100k"
			(at 1.54 1.07 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Power_Connectors/")
		(sheetfile "Power_Connectors.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -0.76 0 270)
			(size 0.9 0.97)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 48 "/LCL_12.12A4")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd rect
			(at 0.76 0 270)
			(size 0.9 0.97)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 103 "Net-(R15-Pad2)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:SOD3716X135N"
		(layer "F.Cu")
		(at 125.90295 50.97435 90)
		(descr "sod-123-ren1")
		(tags "Diode")
		(property "Reference" "D6"
			(at 0 0 90)
			(layer "F.SilkS")
		)
		(property "Value" "D"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Diode"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Device" "D"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TO-???* *_Diode_* *SingleDiode* D_*")
		(sheetname "/LCL_12V/12V_3A_LCL_2/")
		(sheetfile "12V_3A_LCL.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.65 0 180)
			(size 0.75 1.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 52 "Net-(D6-K)")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.65 0 180)
			(size 0.75 1.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 53 "/LCL_12.3A2")
			(pinfunction "A")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "1N4150W-E3-18.stp"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "EPS_Footprints:RESC1608X55N"
		(layer "F.Cu")
		(at 272.42905 60.04195 180)
		(property "Reference" "R120"
			(at -0.11 1.25 0)
			(layer "F.SilkS")
		)
		(property "Value" "86.6k"
			(at 1.54 1.049999 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/LCL_5V/5V_6A_LCL_4/")
		(sheetfile "5V_6A_LCL.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -0.82 0 180)
			(size 0.79 0.93)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 65 "Net-(D12-K)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd rect
			(at 0.82 0 180)
			(size 0.79 0.93)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 30 "/LCL_5V/5V_6A_LCL_4/OPAMP_Minus")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:RESC1508X55N"
		(layer "F.Cu")
		(at 157.085609 46.145191 90)
		(property "Reference" "R21"
			(at -0.646759 -1.07 90)
			(layer "F.SilkS")
		)
		(property "Value" "100k"
			(at 1.54 1.07 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Power_Connectors/")
		(sheetfile "Power_Connectors.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -0.76 0 90)
			(size 0.9 0.97)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 50 "/LCL_12.3A1")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd rect
			(at 0.76 0 90)
			(size 0.9 0.97)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 108 "Net-(R21-Pad2)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:RESC1508X55N"
		(layer "F.Cu")
		(at 208.17905 62.541949 90)
		(property "Reference" "R112"
			(at -2.500001 -0.1208 90)
			(layer "F.SilkS")
		)
		(property "Value" "11.5k"
			(at 1.54 1.069999 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/LCL_5V/5V_6A_LCL_2/")
		(sheetfile "5V_6A_LCL.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -0.76 0 90)
			(size 0.9 0.97)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 28 "Net-(Q11-B)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd rect
			(at 0.76 0 90)
			(size 0.9 0.97)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 27 "/LCL_5V/5V_6A_LCL_2/OPAMP_Minus")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:RESC1608X55N"
		(layer "F.Cu")
		(at 46.3078 59.9192 -90)
		(property "Reference" "R95"
			(at 2.37275 -0.00045 90)
			(layer "F.SilkS")
		)
		(property "Value" "45.3k"
			(at 1.54 1.05 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/LCL_12V/12V_5A_LCL_2/")
		(sheetfile "12V_5A_LCL.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -0.82 0 270)
			(size 0.79 0.93)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 56 "Net-(D8-K)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd rect
			(at 0.82 0 270)
			(size 0.79 0.93)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 21 "Net-(Q8-B)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:CAPC1608X90"
		(layer "F.Cu")
		(at 52.10905 172.39195 90)
		(descr "<b>CAPACITOR</b>")
		(property "Reference" "C20"
			(at 2.6 0.1992 90)
			(layer "F.SilkS")
		)
		(property "Value" "0.1uF"
			(at 1.56646 1.20613 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "SMD 0603 MLCC capacitor, Alternate KiCad Library"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/LCL_12V/12V_12A_LCL_2/")
		(sheetfile "12V_12A_LCL.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -0.85 0 90)
			(size 1.1 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 10 "/LCL_12V/12V_12A_LCL_2/OPAMP_Minus")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd rect
			(at 0.85 0 90)
			(size 1.1 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 9 "Net-(Q2-B)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:RESC1508X55N"
		(layer "F.Cu")
		(at 154.35905 254.29195 -90)
		(property "Reference" "R48"
			(at 2.5 0.5508 90)
			(layer "F.SilkS")
		)
		(property "Value" "75k"
			(at 1.54 1.07 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Power_Connectors/")
		(sheetfile "Power_Connectors.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -0.76 0 270)
			(size 0.9 0.97)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 125 "Net-(R47-Pad2)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd rect
			(at 0.76 0 270)
			(size 0.9 0.97)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 303 "/GNDREF")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:SOD3716X135N"
		(layer "F.Cu")
		(at 39.85905 180.54195 -90)
		(descr "sod-123-ren1")
		(tags "Diode")
		(property "Reference" "D2"
			(at 0 0 90)
			(layer "F.SilkS")
		)
		(property "Value" "D"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Diode"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Device" "D"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TO-???* *_Diode_* *SingleDiode* D_*")
		(sheetname "/LCL_12V/12V_12A_LCL_2/")
		(sheetfile "12V_12A_LCL.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.65 0)
			(size 0.75 1.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 44 "Net-(D2-K)")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.65 0)
			(size 0.75 1.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 45 "/LCL_12.12A2")
			(pinfunction "A")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "1N4150W-E3-18.stp"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "EPS_Footprints:RESC1508X55N"
		(layer "F.Cu")
		(at 181.12825 62.80195 -90)
		(property "Reference" "R107"
			(at 2.74 0.07 90)
			(layer "F.SilkS")
		)
		(property "Value" "11.5k"
			(at 1.54 1.07 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/LCL_5V/5V_6A_LCL_1/")
		(sheetfile "5V_6A_LCL.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -0.76 0 270)
			(size 0.9 0.97)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 60 "Net-(D10-K)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd rect
			(at 0.76 0 270)
			(size 0.9 0.97)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 25 "Net-(Q10-B)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:CAPC1608X90"
		(layer "F.Cu")
		(at 271.42905 62.641949 -90)
		(descr "<b>CAPACITOR</b>")
		(property "Reference" "C30"
			(at 2.650001 -0.1292 90)
			(layer "F.SilkS")
		)
		(property "Value" "0.1uF"
			(at 1.566459 1.20613 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "SMD 0603 MLCC capacitor, Alternate KiCad Library"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/LCL_5V/5V_6A_LCL_4/")
		(sheetfile "5V_6A_LCL.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -0.85 0 270)
			(size 1.1 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 30 "/LCL_5V/5V_6A_LCL_4/OPAMP_Minus")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd rect
			(at 0.85 0 270)
			(size 1.1 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 29 "Net-(Q12-B)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:SOT91P240X120-3N"
		(layer "F.Cu")
		(at 183.80825 62.54195)
		(property "Reference" "Q10"
			(at -0.176 -2.3698 0)
			(layer "F.SilkS")
		)
		(property "Value" "PNP"
			(at 3.1768 2.3698 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://ngspice.sourceforge.io/docs/ngspice-html-manual/manual.xhtml#cha_BJTs"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Bipolar transistor symbol for simulation only, substrate tied to the emitter"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Device" "PNP"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Type" "GUMMELPOON"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" "1=C 2=B 3=E"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/LCL_5V/5V_6A_LCL_1/")
		(sheetfile "5V_6A_LCL.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -0.915 1.025)
			(size 0.61 1.18)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 60 "Net-(D10-K)")
			(pinfunction "C")
			(pintype "open_collector")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd rect
			(at 0.915 1.025)
			(size 0.61 1.18)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 25 "Net-(Q10-B)")
			(pinfunction "B")
			(pintype "input")
			(solder_mask_margin 0.102)
		)
		(pad "3" smd rect
			(at 0 -1.025)
			(size 0.61 1.18)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 26 "/LCL_5V/5V_6A_LCL_1/OPAMP_Minus")
			(pinfunction "E")
			(pintype "open_emitter")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:DIP762W50P254L730H410Q6"
		(layer "F.Cu")
		(at 64.85905 200.35195 -90)
		(property "Reference" "U12"
			(at -7.41 -9.94 90)
			(layer "F.SilkS")
		)
		(property "Value" "CNY17-1"
			(at -0.21 9.94 90)
			(layer "Dwgs.User")
		)
		(property "Datasheet" "http://www.vishay.com/docs/83606/cny17.pdf"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "DC Optocoupler Base Connected, Vce 70V, CTR 40-80%, Viso 5000V (RMS), DIP6"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "DIP*W7.62mm* DIP*W10.16mm* SMDIP*W9.53mm*")
		(sheetname "/LCL_12V/12V_12A_LCL_1/")
		(sheetfile "12V_12A_LCL.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole rect
			(at -3.81 -2.54 270)
			(size 1.4 1.4)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 178 "/LCL_CTRL1")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" thru_hole circle
			(at -3.81 0 270)
			(size 1.4 1.4)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 303 "/GNDREF")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "3" thru_hole circle
			(at -3.81 2.54 270)
			(size 1.4 1.4)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 253 "unconnected-(U12-NC-Pad3)")
			(pinfunction "NC")
			(pintype "no_connect")
			(solder_mask_margin 0.102)
		)
		(pad "4" thru_hole circle
			(at 3.81 2.54 270)
			(size 1.4 1.4)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 303 "/GNDREF")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "5" thru_hole circle
			(at 3.81 0 270)
			(size 1.4 1.4)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 128 "Net-(R55-Pad1)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "6" thru_hole circle
			(at 3.81 -2.54 270)
			(size 1.4 1.4)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 254 "unconnected-(U12-Pad6)")
			(pintype "passive+no_connect")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:RESC1508X55N"
		(layer "F.Cu")
		(at 63.95855 142.19245 180)
		(property "Reference" "R68"
			(at -2.5997 -0.0995 0)
			(layer "F.SilkS")
		)
		(property "Value" "54.9k"
			(at 1.54 1.069999 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/LCL_12V/12V_12A_LCL_3/")
		(sheetfile "12V_12A_LCL.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -0.76 0 180)
			(size 0.9 0.97)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 130 "Net-(R67-Pad1)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd rect
			(at 0.76 0 180)
			(size 0.9 0.97)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 46 "Net-(D3-K)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:RESC1508X55N"
		(layer "F.Cu")
		(at 192.10905 46.29195 90)
		(property "Reference" "R33"
			(at -1 -1.07 90)
			(layer "F.SilkS")
		)
		(property "Value" "100k"
			(at 1.54 1.07 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Power_Connectors/")
		(sheetfile "Power_Connectors.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -0.76 0 90)
			(size 0.9 0.97)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 61 "/LCL_5.6A1")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd rect
			(at 0.76 0 90)
			(size 0.9 0.97)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 116 "Net-(R33-Pad2)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:RESC1508X55N"
		(layer "F.Cu")
		(at 45.81905 197.56495)
		(property "Reference" "R17"
			(at -0.0108 -1.273 0)
			(layer "F.SilkS")
		)
		(property "Value" "1k"
			(at 1.54 1.07 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Power_Connectors/")
		(sheetfile "Power_Connectors.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -0.76 0)
			(size 0.9 0.97)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 104 "Net-(U5A-IN-)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd rect
			(at 0.76 0)
			(size 0.9 0.97)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 100 "Net-(R10-Pad1)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:TO-263AB_SUM"
		(layer "F.Cu")
		(at 52.35905 181.29195 -90)
		(tags "SUM110P06-08L-E3 ")
		(property "Reference" "U13"
			(at 1.5 -6.4492 270)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "SUM110P06-08L-E3"
			(at -0.34 3.193 270)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "SUM110P06-08L-E3"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TO-263AB_SUM TO-263AB_SUM-M TO-263AB_SUM-L")
		(sheetname "/LCL_12V/12V_12A_LCL_2/")
		(sheetfile "12V_12A_LCL.kicad_sch")
		(attr smd)
		(fp_text user "*"
			(at -2.54 5.2705 90)
			(layer "F.Fab")
		)
		(fp_text user "*"
			(at -2.54 5.2705 270)
			(unlocked yes)
			(layer "F.Fab")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -2.54 8.8773 270)
			(size 0.9906 3.2004)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 44 "Net-(D2-K)")
			(pinfunction "G")
			(pintype "input")
		)
		(pad "2" smd rect
			(at 0 0.0508 270)
			(size 10.414 11.4554)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 10 "/LCL_12V/12V_12A_LCL_2/OPAMP_Minus")
			(pinfunction "D")
			(pintype "input")
		)
		(pad "3" smd rect
			(at 2.54 8.8773 270)
			(size 0.9906 3.2004)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 45 "/LCL_12.12A2")
			(pinfunction "S")
			(pintype "input")
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:DIP762W50P254L730H410Q6"
		(layer "F.Cu")
		(at 224.54905 61.081949 180)
		(property "Reference" "U33"
			(at -7.41 -9.94 0)
			(layer "F.SilkS")
		)
		(property "Value" "CNY17-1"
			(at -0.209999 9.94 0)
			(layer "Dwgs.User")
		)
		(property "Datasheet" "http://www.vishay.com/docs/83606/cny17.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "DC Optocoupler Base Connected, Vce 70V, CTR 40-80%, Viso 5000V (RMS), DIP6"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "DIP*W7.62mm* DIP*W10.16mm* SMDIP*W9.53mm*")
		(sheetname "/LCL_5V/5V_6A_LCL_2/")
		(sheetfile "5V_6A_LCL.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole rect
			(at -3.81 -2.54 180)
			(size 1.4 1.4)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 196 "/LCL_CTRL10")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" thru_hole circle
			(at -3.81 0 180)
			(size 1.4 1.4)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 303 "/GNDREF")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "3" thru_hole circle
			(at -3.81 2.54 180)
			(size 1.4 1.4)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 277 "unconnected-(U33-NC-Pad3)")
			(pinfunction "NC")
			(pintype "no_connect")
			(solder_mask_margin 0.102)
		)
		(pad "4" thru_hole circle
			(at 3.81 2.54 180)
			(size 1.4 1.4)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 303 "/GNDREF")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "5" thru_hole circle
			(at 3.81 0 180)
			(size 1.4 1.4)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 138 "Net-(R115-Pad1)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "6" thru_hole circle
			(at 3.81 -2.54 180)
			(size 1.4 1.4)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 278 "unconnected-(U33-Pad6)")
			(pintype "passive+no_connect")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:RESC1508X55N"
		(layer "F.Cu")
		(at 174.60905 242.29195 -90)
		(property "Reference" "R134"
			(at -2.75 -0.1992 90)
			(layer "F.SilkS")
		)
		(property "Value" "98.1k (100k)"
			(at 1.54 1.07 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/LCL_9_and_3-3/3-3V_1-5A_LCL_1/")
		(sheetfile "3-3V_1-5A_LCL.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -0.76 0 270)
			(size 0.9 0.97)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 141 "Net-(R133-Pad1)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd rect
			(at 0.76 0 270)
			(size 0.9 0.97)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 68 "Net-(D14-K)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:BAQ33GS08"
		(layer "F.Cu")
		(at 98.732925 54.519375)
		(descr "MiniMELF (SOD-80)")
		(tags "Zener Diode")
		(property "Reference" "ZD7"
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "D_Zener"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Zener diode"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Library" "TZM5240B-GS08.txt"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Name" "TZM5240B-GS08"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Device" "D"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" "1=A 2=K"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TO-???* *_Diode_* *SingleDiode* D_*")
		(sheetname "/LCL_12V/12V_5A_LCL_1/")
		(sheetfile "12V_5A_LCL.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.875 0)
			(size 1.25 2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 19 "/LCL_12V/12V_5A_LCL_1/OPAMP_Minus")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.875 0)
			(size 1.25 2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 55 "Net-(D7-K)")
			(pinfunction "A")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "TZM5224B-GS08.stp"
			(offset
				(xyz 0 0 0.7999999999)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "EPS_Footprints:SOP63P602X175-24N"
		(layer "F.Cu")
		(at 215.97405 203.53445)
		(property "Reference" "U41"
			(at -0.46 -5.182 0)
			(layer "F.SilkS")
		)
		(property "Value" "MAX11643EEG_"
			(at 7.16 5.182 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DigiKey_Part_Number" "MAX11643EEG+-ND"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SnapEDA_Link" "https://www.snapeda.com/parts/MAX11643EEG+/Analog+Devices/view-part/?ref=snap"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description_1" "8-Bit, 16-/8-Channel, 300ksps ADCs with FIFO and Internal Reference"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MF" "Analog Devices"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Package" "QSOP-24 Maxim"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Check_prices" "https://www.snapeda.com/parts/MAX11643EEG+/Analog+Devices/view-part/?ref=eda"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MP" "MAX11643EEG+"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/Digital Systems/")
		(sheetfile "Digital_Systems.kicad_sch")
		(attr smd)
		(pad "1" smd roundrect
			(at -2.635 -3.4925)
			(size 1.64 0.41)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.125)
			(net 247 "/I_MEAS.12_1")
			(pinfunction "AIN0")
			(pintype "input")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd roundrect
			(at -2.635 -2.8575)
			(size 1.64 0.41)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.125)
			(net 248 "/I_MEAS.12_2")
			(pinfunction "AIN1")
			(pintype "input")
			(solder_mask_margin 0.102)
		)
		(pad "3" smd roundrect
			(at -2.635 -2.2225)
			(size 1.64 0.41)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.125)
			(net 245 "/I_MEAS.12_3")
			(pinfunction "AIN2")
			(pintype "input")
			(solder_mask_margin 0.102)
		)
		(pad "4" smd roundrect
			(at -2.635 -1.5875)
			(size 1.64 0.41)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.125)
			(net 246 "/I_MEAS.12_4")
			(pinfunction "AIN3")
			(pintype "input")
			(solder_mask_margin 0.102)
		)
		(pad "5" smd roundrect
			(at -2.635 -0.9525)
			(size 1.64 0.41)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.125)
			(net 293 "unconnected-(U41-AIN4-Pad5)")
			(pinfunction "AIN4")
			(pintype "input+no_connect")
			(solder_mask_margin 0.102)
		)
		(pad "6" smd roundrect
			(at -2.635 -0.3175)
			(size 1.64 0.41)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.125)
			(net 226 "/V_MEAS.12_1")
			(pinfunction "AIN5")
			(pintype "input")
			(solder_mask_margin 0.102)
		)
		(pad "7" smd roundrect
			(at -2.635 0.3175)
			(size 1.64 0.41)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.125)
			(net 225 "/V_MEAS.12_2")
			(pinfunction "AIN6")
			(pintype "input")
			(solder_mask_margin 0.102)
		)
		(pad "8" smd roundrect
			(at -2.635 0.9525)
			(size 1.64 0.41)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.125)
			(net 227 "/V_MEAS.12_3")
			(pinfunction "AIN7")
			(pintype "input")
			(solder_mask_margin 0.102)
		)
		(pad "9" smd roundrect
			(at -2.635 1.5875)
			(size 1.64 0.41)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.125)
			(net 228 "/V_MEAS.12_4")
			(pinfunction "AIN8")
			(pintype "input")
			(solder_mask_margin 0.102)
		)
		(pad "10" smd roundrect
			(at -2.635 2.2225)
			(size 1.64 0.41)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.125)
			(net 232 "/V_MEAS.12_5")
			(pinfunction "AIN9")
			(pintype "input")
			(solder_mask_margin 0.102)
		)
		(pad "11" smd roundrect
			(at -2.635 2.8575)
			(size 1.64 0.41)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.125)
			(net 231 "/V_MEAS.12_6")
			(pinfunction "AIN10")
			(pintype "input")
			(solder_mask_margin 0.102)
		)
		(pad "12" smd roundrect
			(at -2.635 3.4925)
			(size 1.64 0.41)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.125)
			(net 234 "/V_MEAS.5_1")
			(pinfunction "AIN11")
			(pintype "input")
			(solder_mask_margin 0.102)
		)
		(pad "13" smd roundrect
			(at 2.635 3.4925)
			(size 1.64 0.41)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.125)
			(net 233 "/V_MEAS.5_2")
			(pinfunction "AIN12")
			(pintype "input")
			(solder_mask_margin 0.102)
		)
		(pad "14" smd roundrect
			(at 2.635 2.8575)
			(size 1.64 0.41)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.125)
			(net 236 "/V_MEAS.5_3")
			(pinfunction "AIN13")
			(pintype "input")
			(solder_mask_margin 0.102)
		)
		(pad "15" smd roundrect
			(at 2.635 2.2225)
			(size 1.64 0.41)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.125)
			(net 235 "/V_MEAS.5_4")
			(pinfunction "AIN14")
			(pintype "input")
			(solder_mask_margin 0.102)
		)
		(pad "16" smd roundrect
			(at 2.635 1.5875)
			(size 1.64 0.41)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.125)
			(net 142 "Net-(U41-~{CNVST}{slash}AIN15)")
			(pinfunction "~{CNVST}/AIN15")
			(pintype "input")
			(solder_mask_margin 0.102)
		)
		(pad "17" smd roundrect
			(at 2.635 0.9525)
			(size 1.64 0.41)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.125)
			(net 35 "/Digital Systems/3.3V+")
			(pinfunction "REF")
			(pintype "input")
			(solder_mask_margin 0.102)
		)
		(pad "18" smd roundrect
			(at 2.635 0.3175)
			(size 1.64 0.41)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.125)
			(net 303 "/GNDREF")
			(pinfunction "GND")
			(pintype "power_in")
			(solder_mask_margin 0.102)
		)
		(pad "19" smd roundrect
			(at 2.635 -0.3175)
			(size 1.64 0.41)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.125)
			(net 35 "/Digital Systems/3.3V+")
			(pinfunction "VDD")
			(pintype "power_in")
			(solder_mask_margin 0.102)
		)
		(pad "20" smd roundrect
			(at 2.635 -0.9525)
			(size 1.64 0.41)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.125)
			(net 148 "Net-(U41-~{CS})")
			(pinfunction "~{CS}")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "21" smd roundrect
			(at 2.635 -1.5875)
			(size 1.64 0.41)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.125)
			(net 146 "Net-(U41-SCLK)")
			(pinfunction "SCLK")
			(pintype "input")
			(solder_mask_margin 0.102)
		)
		(pad "22" smd roundrect
			(at 2.635 -2.2225)
			(size 1.64 0.41)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.125)
			(net 145 "Net-(U41-DIN)")
			(pinfunction "DIN")
			(pintype "input")
			(solder_mask_margin 0.102)
		)
		(pad "23" smd roundrect
			(at 2.635 -2.8575)
			(size 1.64 0.41)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.125)
			(net 171 "Net-(U41-DOUT)")
			(pinfunction "DOUT")
			(pintype "output")
			(solder_mask_margin 0.102)
		)
		(pad "24" smd roundrect
			(at 2.635 -3.4925)
			(size 1.64 0.41)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.125)
			(net 149 "Net-(U41-~{EOC})")
			(pinfunction "~{EOC}")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:RESC1608X55N"
		(layer "F.Cu")
		(at 210.92905 60.04195 180)
		(property "Reference" "R114"
			(at -0.11 1.25 0)
			(layer "F.SilkS")
		)
		(property "Value" "86.6k"
			(at 1.54 1.049999 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/LCL_5V/5V_6A_LCL_2/")
		(sheetfile "5V_6A_LCL.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -0.82 0 180)
			(size 0.79 0.93)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 62 "Net-(D11-K)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd rect
			(at 0.82 0 180)
			(size 0.79 0.93)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 27 "/LCL_5V/5V_6A_LCL_2/OPAMP_Minus")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:DIP762W50P254L730H410Q6"
		(layer "F.Cu")
		(at 286.04905 61.081949 180)
		(property "Reference" "U35"
			(at -0.06 -1.710001 0)
			(layer "F.SilkS")
		)
		(property "Value" "CNY17-1"
			(at -0.209999 9.94 0)
			(layer "Dwgs.User")
		)
		(property "Datasheet" "http://www.vishay.com/docs/83606/cny17.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "DC Optocoupler Base Connected, Vce 70V, CTR 40-80%, Viso 5000V (RMS), DIP6"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "DIP*W7.62mm* DIP*W10.16mm* SMDIP*W9.53mm*")
		(sheetname "/LCL_5V/5V_6A_LCL_4/")
		(sheetfile "5V_6A_LCL.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole rect
			(at -3.81 -2.54 180)
			(size 1.4 1.4)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 201 "/LCL_CTRL12")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" thru_hole circle
			(at -3.81 0 180)
			(size 1.4 1.4)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 303 "/GNDREF")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "3" thru_hole circle
			(at -3.81 2.54 180)
			(size 1.4 1.4)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 280 "unconnected-(U35-NC-Pad3)")
			(pinfunction "NC")
			(pintype "no_connect")
			(solder_mask_margin 0.102)
		)
		(pad "4" thru_hole circle
			(at 3.81 2.54 180)
			(size 1.4 1.4)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 303 "/GNDREF")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "5" thru_hole circle
			(at 3.81 0 180)
			(size 1.4 1.4)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 139 "Net-(R121-Pad1)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "6" thru_hole circle
			(at 3.81 -2.54 180)
			(size 1.4 1.4)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 279 "unconnected-(U35-Pad6)")
			(pintype "passive+no_connect")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:RESC1508X55N"
		(layer "F.Cu")
		(at 45.60905 131.54195)
		(property "Reference" "R19"
			(at -0.21 -1.07 0)
			(layer "F.SilkS")
		)
		(property "Value" "1k"
			(at 1.54 1.07 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Power_Connectors/")
		(sheetfile "Power_Connectors.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -0.76 0)
			(size 0.9 0.97)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 106 "Net-(U5C-IN-)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd rect
			(at 0.76 0)
			(size 0.9 0.97)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 102 "Net-(R13-Pad2)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:RESC1608X55N"
		(layer "F.Cu")
		(at 188.30825 60.54195 90)
		(property "Reference" "R109"
			(at -2.75 0 90)
			(layer "F.SilkS")
		)
		(property "Value" "5.1k"
			(at 1.54 1.05 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/LCL_5V/5V_6A_LCL_1/")
		(sheetfile "5V_6A_LCL.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -0.82 0 90)
			(size 0.79 0.93)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 137 "Net-(R109-Pad1)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd rect
			(at 0.82 0 90)
			(size 0.79 0.93)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 60 "Net-(D10-K)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:RESC1608X55N"
		(layer "F.Cu")
		(at 60.95855 148.76245 -90)
		(property "Reference" "R66"
			(at -0.11 1.4003 90)
			(layer "F.SilkS")
		)
		(property "Value" "86.6k"
			(at 1.54 1.05 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/LCL_12V/12V_12A_LCL_3/")
		(sheetfile "12V_12A_LCL.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -0.82 0 270)
			(size 0.79 0.93)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 46 "Net-(D3-K)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd rect
			(at 0.82 0 270)
			(size 0.79 0.93)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 11 "/LCL_12V/12V_12A_LCL_3/OPAMP_Minus")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:RESC1508X55N"
		(layer "F.Cu")
		(at 124.90295 45.72435 90)
		(property "Reference" "R23"
			(at -0.8176 -1.0947 90)
			(layer "F.SilkS")
		)
		(property "Value" "100k"
			(at 1.54 1.07 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Power_Connectors/")
		(sheetfile "Power_Connectors.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -0.76 0 90)
			(size 0.9 0.97)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 53 "/LCL_12.3A2")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd rect
			(at 0.76 0 90)
			(size 0.9 0.97)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 109 "Net-(R23-Pad2)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:Terminal Block 691137710002"
		(layer "F.Cu")
		(at 239.10905 250.79195)
		(property "Reference" "J22"
			(at 0 -5.135 0)
			(layer "F.SilkS")
		)
		(property "Value" "691137710002"
			(at 4.12 5.365 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/Digital_Connectors/")
		(sheetfile "Digital_Connectors.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole circle
			(at -2.5 0)
			(size 1.95 1.95)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 85 "/ADC_AIN0")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" thru_hole circle
			(at 2.5 0)
			(size 1.95 1.95)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 303 "/GNDREF")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:Terminal Block 691137710002"
		(layer "F.Cu")
		(at 278.60905 42.29195 180)
		(property "Reference" "J14"
			(at -0.6992 -4.5 0)
			(layer "F.SilkS")
		)
		(property "Value" "691137710002"
			(at 4.12 5.365 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/Power_Connectors/")
		(sheetfile "Power_Connectors.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole circle
			(at -2.5 0 180)
			(size 1.95 1.95)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 303 "/GNDREF")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" thru_hole circle
			(at 2.5 0 180)
			(size 1.95 1.95)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 64 "/LCL_5.6A4")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:RESC1508X55N"
		(layer "F.Cu")
		(at 242.42905 62.801949 -90)
		(property "Reference" "R101"
			(at 2.490001 0.1208 90)
			(layer "F.SilkS")
		)
		(property "Value" "11.5k"
			(at 1.539999 1.07 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/LCL_5V/5V_6A_LCL_3/")
		(sheetfile "5V_6A_LCL.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -0.76 0 270)
			(size 0.9 0.97)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 58 "Net-(D9-K)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd rect
			(at 0.76 0 270)
			(size 0.9 0.97)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 23 "Net-(Q9-B)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:RESC1508X55N"
		(layer "F.Cu")
		(at 273.17905 62.551949 -90)
		(property "Reference" "R119"
			(at 2.740001 0.1208 90)
			(layer "F.SilkS")
		)
		(property "Value" "11.5k"
			(at 1.539999 1.07 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/LCL_5V/5V_6A_LCL_4/")
		(sheetfile "5V_6A_LCL.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -0.76 0 270)
			(size 0.9 0.97)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 65 "Net-(D12-K)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd rect
			(at 0.76 0 270)
			(size 0.9 0.97)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 29 "Net-(Q12-B)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:RESC1508X55N"
		(layer "F.Cu")
		(at 124.90295 42.47435 90)
		(property "Reference" "R24"
			(at 0.9324 1.4053 90)
			(layer "F.SilkS")
		)
		(property "Value" "13.7k"
			(at 1.54 1.07 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Power_Connectors/")
		(sheetfile "Power_Connectors.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -0.76 0 90)
			(size 0.9 0.97)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 109 "Net-(R23-Pad2)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd rect
			(at 0.76 0 90)
			(size 0.9 0.97)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 303 "/GNDREF")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:RESC1508X55N"
		(layer "F.Cu")
		(at 229.85905 189.29195 180)
		(property "Reference" "R162"
			(at -0.21 -1.07 0)
			(layer "F.SilkS")
		)
		(property "Value" "0 Ohm"
			(at 1.54 1.07 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MF" "Stackpole Electronics Inc"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description_1" "0 Ohms Jumper 0.1W, 1/10W Chip Resistor 0603 (1608 Metric) Automotive AEC-Q200 Thick Film"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Package" "1508 Stackpole"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Price" "None"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SnapEDA_Link" "https://www.snapeda.com/parts/RMCF0603ZT0R00/Stackpole+Electronics/view-part/?ref=snap"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MP" "RMCF0603ZT0R00"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Purchase-URL" "https://www.snapeda.com/api/url_track_click_mouser/?unipart_id=3968849&manufacturer=Stackpole Electronics Inc&part_name=RMCF0603ZT0R00&search_term=rmcf0603zt0r00"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Availability" "In Stock"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Check_prices" "https://www.snapeda.com/parts/RMCF0603ZT0R00/Stackpole+Electronics/view-part/?ref=eda"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/Digital Systems/")
		(sheetfile "Digital_Systems.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -0.76 0 180)
			(size 0.9 0.97)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 147 "/Digital Systems/SSI0CLK")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd rect
			(at 0.76 0 180)
			(size 0.9 0.97)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 175 "Net-(U44-SCLK)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:RESC1508X55N"
		(layer "F.Cu")
		(at 240.85905 214.29195)
		(property "Reference" "R174"
			(at -0.21 -1.07 0)
			(layer "F.SilkS")
		)
		(property "Value" "10k"
			(at 1.54 1.07 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Digital Systems/")
		(sheetfile "Digital_Systems.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -0.76 0)
			(size 0.9 0.97)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 162 "/Digital Systems/GPIO_INT")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd rect
			(at 0.76 0)
			(size 0.9 0.97)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 35 "/Digital Systems/3.3V+")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:RESC1508X55N"
		(layer "F.Cu")
		(at 232.60905 222.29195)
		(property "Reference" "R168"
			(at -2.5508 -0.75 0)
			(layer "F.SilkS")
		)
		(property "Value" "100"
			(at 1.54 1.07 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Digital Systems/")
		(sheetfile "Digital_Systems.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -0.76 0)
			(size 0.9 0.97)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 182 "/LCL_CTRL3")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd rect
			(at 0.76 0)
			(size 0.9 0.97)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 183 "Net-(U45-P0_2)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:RESC1508X55N"
		(layer "F.Cu")
		(at 238.10905 185.49195)
		(property "Reference" "R147"
			(at -0.21 -1.07 0)
			(layer "F.SilkS")
		)
		(property "Value" "22"
			(at 1.54 1.07 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Digital Systems/")
		(sheetfile "Digital_Systems.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -0.76 0)
			(size 0.9 0.97)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 160 "/Digital Systems/THM_CS")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd rect
			(at 0.76 0)
			(size 0.9 0.97)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 159 "Net-(U43-PB6)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:RESC1508X55N"
		(layer "F.Cu")
		(at 63.50855 148.02245)
		(property "Reference" "R65"
			(at 2.5497 0.0195 0)
			(layer "F.SilkS")
		)
		(property "Value" "54.9k"
			(at 1.54 1.07 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/LCL_12V/12V_12A_LCL_3/")
		(sheetfile "12V_12A_LCL.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -0.76 0)
			(size 0.9 0.97)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 46 "Net-(D3-K)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd rect
			(at 0.76 0)
			(size 0.9 0.97)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 12 "Net-(Q3-B)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:RES_TLRP3A30DR018FTE_TEC"
		(layer "F.Cu")
		(at 260.109049 50.791949 180)
		(tags "TLRP3A30DR018FTE ")
		(property "Reference" "R99"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "0.01"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/LCL_5V/5V_6A_LCL_3/")
		(sheetfile "5V_6A_LCL.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -2.8321 0 180)
			(size 1.397 3.4544)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 4 "/DC_POS.5V")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 2.8321 0 180)
			(size 1.397 3.4544)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 24 "/LCL_5V/5V_6A_LCL_3/OPAMP_Minus")
			(pintype "passive")
		)
		(zone
			(net 0)
			(net_name "")
			(layer "F.Cu")
			(hatch full 0.508)
			(connect_pads
				(clearance 0)
			)
			(min_thickness 0.254)
			(filled_areas_thickness no)
			(keepout
				(tracks not_allowed)
				(vias not_allowed)
				(pads allowed)
				(copperpour not_allowed)
				(footprints allowed)
			)
			(placement
				(enabled no)
				(sheetname "")
			)
			(fill
				(thermal_gap 0.508)
				(thermal_bridge_width 0.508)
			)
			(polygon
				(pts
					(xy 262.191849 52.468349) (xy 258.026249 52.468349) (xy 258.026249 49.115549) (xy 262.191849 49.115549)
				)
			)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:SOT91P240X120-3N"
		(layer "F.Cu")
		(at 245.10905 62.541949)
		(property "Reference" "Q9"
			(at -0.175999 -2.3698 0)
			(layer "F.SilkS")
		)
		(property "Value" "PNP"
			(at 3.176799 2.3698 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://ngspice.sourceforge.io/docs/ngspice-html-manual/manual.xhtml#cha_BJTs"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Bipolar transistor symbol for simulation only, substrate tied to the emitter"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Device" "PNP"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Type" "GUMMELPOON"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" "1=C 2=B 3=E"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/LCL_5V/5V_6A_LCL_3/")
		(sheetfile "5V_6A_LCL.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -0.915 1.025)
			(size 0.61 1.18)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 58 "Net-(D9-K)")
			(pinfunction "C")
			(pintype "open_collector")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd rect
			(at 0.915 1.025)
			(size 0.61 1.18)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 23 "Net-(Q9-B)")
			(pinfunction "B")
			(pintype "input")
			(solder_mask_margin 0.102)
		)
		(pad "3" smd rect
			(at 0 -1.025)
			(size 0.61 1.18)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 24 "/LCL_5V/5V_6A_LCL_3/OPAMP_Minus")
			(pinfunction "E")
			(pintype "open_emitter")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:RESC1508X55N"
		(layer "F.Cu")
		(at 225.10905 44.55195 -90)
		(property "Reference" "R42"
			(at -0.21 -1.07 90)
			(layer "F.SilkS")
		)
		(property "Value" "1k"
			(at 1.54 1.07 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Power_Connectors/")
		(sheetfile "Power_Connectors.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -0.76 0 270)
			(size 0.9 0.97)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 121 "Net-(U7B-IN-)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd rect
			(at 0.76 0 270)
			(size 0.9 0.97)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 117 "Net-(R35-Pad2)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:RESC1508X55N"
		(layer "F.Cu")
		(at 38.85905 198.79195 90)
		(property "Reference" "R18"
			(at 2.25 0.1992 90)
			(layer "F.SilkS")
		)
		(property "Value" "1k"
			(at 1.54 1.07 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Power_Connectors/")
		(sheetfile "Power_Connectors.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -0.76 0 90)
			(size 0.9 0.97)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 105 "Net-(U5B-IN-)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd rect
			(at 0.76 0 90)
			(size 0.9 0.97)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 101 "Net-(R11-Pad2)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:RESC1508X55N"
		(layer "F.Cu")
		(at 246.85905 227.54195)
		(property "Reference" "R176"
			(at 0.9492 1 0)
			(layer "F.SilkS")
		)
		(property "Value" "100"
			(at 1.54 1.07 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Digital Systems/")
		(sheetfile "Digital_Systems.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -0.76 0)
			(size 0.9 0.97)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 197 "Net-(U45-P1_1)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd rect
			(at 0.76 0)
			(size 0.9 0.97)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 196 "/LCL_CTRL10")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:RESC1608X55N"
		(layer "F.Cu")
		(at 142.424041 61.633258 90)
		(property "Reference" "R76"
			(at -0.21 -1.05 90)
			(layer "F.SilkS")
		)
		(property "Value" "86.6k"
			(at 1.54 1.049999 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/LCL_12V/12V_3A_LCL_1/")
		(sheetfile "12V_3A_LCL.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -0.82 0 90)
			(size 0.79 0.93)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 15 "Net-(Q5-B)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd rect
			(at 0.82 0 90)
			(size 0.79 0.93)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 16 "/LCL_12V/12V_3A_LCL_1/OPAMP_Minus")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:RESC1508X55N"
		(layer "F.Cu")
		(at 47.34905 133.54195 180)
		(property "Reference" "R13"
			(at -0.21 -1.07 0)
			(layer "F.SilkS")
		)
		(property "Value" "100k"
			(at 1.54 1.07 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Power_Connectors/")
		(sheetfile "Power_Connectors.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -0.76 0 180)
			(size 0.9 0.97)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 47 "/LCL_12.12A3")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd rect
			(at 0.76 0 180)
			(size 0.9 0.97)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 102 "Net-(R13-Pad2)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:SOT91P240X120-3N"
		(layer "F.Cu")
		(at 82.692925 60.544375)
		(property "Reference" "Q7"
			(at -0.175999 -2.3698 0)
			(layer "F.SilkS")
		)
		(property "Value" "PNP"
			(at -0.085 -0.025 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://ngspice.sourceforge.io/docs/ngspice-html-manual/manual.xhtml#cha_BJTs"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Bipolar transistor symbol for simulation only, substrate tied to the emitter"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Device" "PNP"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Type" "GUMMELPOON"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" "1=C 2=B 3=E"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/LCL_12V/12V_5A_LCL_1/")
		(sheetfile "12V_5A_LCL.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -0.915 1.025)
			(size 0.61 1.18)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 55 "Net-(D7-K)")
			(pinfunction "C")
			(pintype "open_collector")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd rect
			(at 0.915 1.025)
			(size 0.61 1.18)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 20 "Net-(Q7-B)")
			(pinfunction "B")
			(pintype "input")
			(solder_mask_margin 0.102)
		)
		(pad "3" smd rect
			(at 0 -1.025)
			(size 0.61 1.18)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 19 "/LCL_12V/12V_5A_LCL_1/OPAMP_Minus")
			(pinfunction "E")
			(pintype "open_emitter")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:RESC1508X55N"
		(layer "F.Cu")
		(at 269.67905 62.541949 90)
		(property "Reference" "R118"
			(at -2.500001 -0.1208 90)
			(layer "F.SilkS")
		)
		(property "Value" "11.5k"
			(at 1.54 1.069999 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/LCL_5V/5V_6A_LCL_4/")
		(sheetfile "5V_6A_LCL.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -0.76 0 90)
			(size 0.9 0.97)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 29 "Net-(Q12-B)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd rect
			(at 0.76 0 90)
			(size 0.9 0.97)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 30 "/LCL_5V/5V_6A_LCL_4/OPAMP_Minus")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:RESC1508X55N"
		(layer "F.Cu")
		(at 225.60905 186.04195 180)
		(property "Reference" "R164"
			(at -0.21 -1.07 0)
			(layer "F.SilkS")
		)
		(property "Value" "0 Ohm"
			(at 1.54 1.07 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MF" "Stackpole Electronics Inc"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description_1" "0 Ohms Jumper 0.1W, 1/10W Chip Resistor 0603 (1608 Metric) Automotive AEC-Q200 Thick Film"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Package" "1508 Stackpole"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Price" "None"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SnapEDA_Link" "https://www.snapeda.com/parts/RMCF0603ZT0R00/Stackpole+Electronics/view-part/?ref=snap"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MP" "RMCF0603ZT0R00"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Purchase-URL" "https://www.snapeda.com/api/url_track_click_mouser/?unipart_id=3968849&manufacturer=Stackpole Electronics Inc&part_name=RMCF0603ZT0R00&search_term=rmcf0603zt0r00"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Availability" "In Stock"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Check_prices" "https://www.snapeda.com/parts/RMCF0603ZT0R00/Stackpole+Electronics/view-part/?ref=eda"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/Digital Systems/")
		(sheetfile "Digital_Systems.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -0.76 0 180)
			(size 0.9 0.97)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 164 "/Digital Systems/ADC2_EOC")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd rect
			(at 0.76 0 180)
			(size 0.9 0.97)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 177 "Net-(U44-~{EOC})")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:TO-263AB_SUM"
		(layer "F.Cu")
		(at 241.35905 52.04195 90)
		(tags "SUM110P06-08L-E3 ")
		(property "Reference" "U28"
			(at -2 -6.3008 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "SUM110P06-08L-E3"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "SUM110P06-08L-E3"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TO-263AB_SUM TO-263AB_SUM-M TO-263AB_SUM-L")
		(sheetname "/LCL_5V/5V_6A_LCL_3/")
		(sheetfile "5V_6A_LCL.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(fp_text user "*"
			(at -2.539999 5.2705 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(fp_text user "*"
			(at -2.539999 5.2705 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -2.54 8.8773 90)
			(size 0.9906 3.2004)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 58 "Net-(D9-K)")
			(pinfunction "G")
			(pintype "input")
		)
		(pad "2" smd rect
			(at 0 0.0508 90)
			(size 10.414 11.4554)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 24 "/LCL_5V/5V_6A_LCL_3/OPAMP_Minus")
			(pinfunction "D")
			(pintype "input")
		)
		(pad "3" smd rect
			(at 2.54 8.8773 90)
			(size 0.9906 3.2004)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 59 "/LCL_5.6A3")
			(pinfunction "S")
			(pintype "input")
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:RESC1508X55N"
		(layer "F.Cu")
		(at 224.35905 244.79195 -90)
		(property "Reference" "R187"
			(at -0.21 -1.07 90)
			(layer "F.SilkS")
		)
		(property "Value" "4.7k"
			(at 1.54 1.07 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Digital_Connectors/")
		(sheetfile "Digital_Connectors.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -0.76 0 270)
			(size 0.9 0.97)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 72 "/DC_POS.3.3V")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd rect
			(at 0.76 0 270)
			(size 0.9 0.97)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 80 "/ADC_AIN1")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:RESC1508X55N"
		(layer "F.Cu")
		(at 222.60905 194.98695 180)
		(property "Reference" "R160"
			(at -0.21 -1.07 0)
			(layer "F.SilkS")
		)
		(property "Value" "0 Ohm"
			(at 1.54 1.07 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MF" "Stackpole Electronics Inc"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description_1" "0 Ohms Jumper 0.1W, 1/10W Chip Resistor 0603 (1608 Metric) Automotive AEC-Q200 Thick Film"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Package" "1508 Stackpole"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Price" "None"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SnapEDA_Link" "https://www.snapeda.com/parts/RMCF0603ZT0R00/Stackpole+Electronics/view-part/?ref=snap"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MP" "RMCF0603ZT0R00"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Purchase-URL" "https://www.snapeda.com/api/url_track_click_mouser/?unipart_id=3968849&manufacturer=Stackpole Electronics Inc&part_name=RMCF0603ZT0R00&search_term=rmcf0603zt0r00"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Availability" "In Stock"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Check_prices" "https://www.snapeda.com/parts/RMCF0603ZT0R00/Stackpole+Electronics/view-part/?ref=eda"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/Digital Systems/")
		(sheetfile "Digital_Systems.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -0.76 0 180)
			(size 0.9 0.97)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 166 "/Digital Systems/ADC2_CNVST")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd rect
			(at 0.76 0 180)
			(size 0.9 0.97)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 173 "Net-(U44-~{CNVST}{slash}AIN15)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:RESC1608X55N"
		(layer "F.Cu")
		(at 49.10905 99.04195 180)
		(property "Reference" "R73"
			(at 2.5508 -0.25 0)
			(layer "F.SilkS")
		)
		(property "Value" "8.87k"
			(at 1.54 1.049999 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/LCL_12V/12V_12A_LCL_4/")
		(sheetfile "12V_12A_LCL.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -0.82 0 180)
			(size 0.79 0.93)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 131 "Net-(R73-Pad1)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd rect
			(at 0.82 0 180)
			(size 0.79 0.93)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 49 "Net-(D4-K)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:DIP762W50P254L730H410Q6"
		(layer "F.Cu")
		(at 62.10905 234.04195 -90)
		(property "Reference" "U38"
			(at -7.41 -9.94 90)
			(layer "F.SilkS")
		)
		(property "Value" "CNY17-1"
			(at -0.21 9.94 90)
			(layer "Dwgs.User")
		)
		(property "Datasheet" "http://www.vishay.com/docs/83606/cny17.pdf"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "DC Optocoupler Base Connected, Vce 70V, CTR 40-80%, Viso 5000V (RMS), DIP6"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "DIP*W7.62mm* DIP*W10.16mm* SMDIP*W9.53mm*")
		(sheetname "/LCL_9_and_3-3/9V_2A_LCL_1/")
		(sheetfile "9V_2A_LCL.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole rect
			(at -3.81 -2.54 270)
			(size 1.4 1.4)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 202 "/LCL_CTRL13")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" thru_hole circle
			(at -3.81 0 270)
			(size 1.4 1.4)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 303 "/GNDREF")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "3" thru_hole circle
			(at -3.81 2.54 270)
			(size 1.4 1.4)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 289 "unconnected-(U38-NC-Pad3)")
			(pinfunction "NC")
			(pintype "no_connect")
			(solder_mask_margin 0.102)
		)
		(pad "4" thru_hole circle
			(at 3.81 2.54 270)
			(size 1.4 1.4)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 303 "/GNDREF")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "5" thru_hole circle
			(at 3.81 0 270)
			(size 1.4 1.4)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 140 "Net-(R127-Pad1)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "6" thru_hole circle
			(at 3.81 -2.54 270)
			(size 1.4 1.4)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 290 "unconnected-(U38-Pad6)")
			(pintype "passive+no_connect")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:RESC1508X55N"
		(layer "F.Cu")
		(at 284.85905 46.04195 90)
		(property "Reference" "R39"
			(at -1 -1.0508 90)
			(layer "F.SilkS")
		)
		(property "Value" "100k"
			(at 1.54 1.07 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Power_Connectors/")
		(sheetfile "Power_Connectors.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -0.76 0 90)
			(size 0.9 0.97)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 64 "/LCL_5.6A4")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd rect
			(at 0.76 0 90)
			(size 0.9 0.97)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 119 "Net-(R39-Pad2)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:CAPC1608X90"
		(layer "F.Cu")
		(at 256.85905 193.54195)
		(descr "<b>CAPACITOR</b>")
		(property "Reference" "C34"
			(at -2.3008 0.25 270)
			(layer "F.SilkS")
		)
		(property "Value" "10nF"
			(at 1.56646 1.20613 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "SMD 0603 MLCC capacitor, Alternate KiCad Library"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/Digital Systems/")
		(sheetfile "Digital_Systems.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -0.85 0)
			(size 1.1 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 36 "Net-(U43-~{RST})")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd rect
			(at 0.85 0)
			(size 1.1 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 303 "/GNDREF")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:RESC1508X55N"
		(layer "F.Cu")
		(at 256.85905 183.29195 180)
		(property "Reference" "R142"
			(at -0.21 -1.07 0)
			(layer "F.SilkS")
		)
		(property "Value" "0 Ohm"
			(at 1.54 1.07 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MF" "Stackpole Electronics Inc"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description_1" "0 Ohms Jumper 0.1W, 1/10W Chip Resistor 0603 (1608 Metric) Automotive AEC-Q200 Thick Film"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Package" "1508 Stackpole"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Price" "None"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SnapEDA_Link" "https://www.snapeda.com/parts/RMCF0603ZT0R00/Stackpole+Electronics/view-part/?ref=snap"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MP" "RMCF0603ZT0R00"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Purchase-URL" "https://www.snapeda.com/api/url_track_click_mouser/?unipart_id=3968849&manufacturer=Stackpole Electronics Inc&part_name=RMCF0603ZT0R00&search_term=rmcf0603zt0r00"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Availability" "In Stock"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Check_prices" "https://www.snapeda.com/parts/RMCF0603ZT0R00/Stackpole+Electronics/view-part/?ref=eda"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/Digital Systems/")
		(sheetfile "Digital_Systems.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -0.76 0 180)
			(size 0.9 0.97)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 152 "/Digital Systems/I2C0SCL")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd rect
			(at 0.76 0 180)
			(size 0.9 0.97)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 153 "Net-(U43-PB2{slash}I2C0SCL)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:RESC1508X55N"
		(layer "F.Cu")
		(at 252.85905 197.04195 180)
		(property "Reference" "R152"
			(at -2.6992 -0.75 0)
			(layer "F.SilkS")
		)
		(property "Value" "22"
			(at 1.54 1.07 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Digital Systems/")
		(sheetfile "Digital_Systems.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -0.76 0 180)
			(size 0.9 0.97)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 150 "/Digital Systems/ADC1_EOC")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd rect
			(at 0.76 0 180)
			(size 0.9 0.97)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 168 "Net-(U43-PF3)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:RESC1508X55N"
		(layer "F.Cu")
		(at 157.085609 42.885191 90)
		(property "Reference" "R22"
			(at 1.093241 1.222641 90)
			(layer "F.SilkS")
		)
		(property "Value" "13.7k"
			(at 1.54 1.07 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Power_Connectors/")
		(sheetfile "Power_Connectors.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -0.76 0 90)
			(size 0.9 0.97)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 108 "Net-(R21-Pad2)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd rect
			(at 0.76 0 90)
			(size 0.9 0.97)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 303 "/GNDREF")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:CAPC1608X90"
		(layer "F.Cu")
		(at 179.37825 62.89195 -90)
		(descr "<b>CAPACITOR</b>")
		(property "Reference" "C28"
			(at 2.65 0.07 90)
			(layer "F.SilkS")
		)
		(property "Value" "0.1uF"
			(at 1.56646 1.20613 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "SMD 0603 MLCC capacitor, Alternate KiCad Library"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/LCL_5V/5V_6A_LCL_1/")
		(sheetfile "5V_6A_LCL.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -0.85 0 270)
			(size 1.1 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 26 "/LCL_5V/5V_6A_LCL_1/OPAMP_Minus")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd rect
			(at 0.85 0 270)
			(size 1.1 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 25 "Net-(Q10-B)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:RESC1508X55N"
		(layer "F.Cu")
		(at 222.10905 200.54195 180)
		(property "Reference" "R136"
			(at -0.21 -1.07 0)
			(layer "F.SilkS")
		)
		(property "Value" "0 Ohm"
			(at 1.54 1.07 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MF" "Stackpole Electronics Inc"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description_1" "0 Ohms Jumper 0.1W, 1/10W Chip Resistor 0603 (1608 Metric) Automotive AEC-Q200 Thick Film"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Package" "1508 Stackpole"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Price" "None"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SnapEDA_Link" "https://www.snapeda.com/parts/RMCF0603ZT0R00/Stackpole+Electronics/view-part/?ref=snap"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MP" "RMCF0603ZT0R00"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Purchase-URL" "https://www.snapeda.com/api/url_track_click_mouser/?unipart_id=3968849&manufacturer=Stackpole Electronics Inc&part_name=RMCF0603ZT0R00&search_term=rmcf0603zt0r00"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Availability" "In Stock"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Check_prices" "https://www.snapeda.com/parts/RMCF0603ZT0R00/Stackpole+Electronics/view-part/?ref=eda"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/Digital Systems/")
		(sheetfile "Digital_Systems.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -0.76 0 180)
			(size 0.9 0.97)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 144 "/Digital Systems/SSI0Tx")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd rect
			(at 0.76 0 180)
			(size 0.9 0.97)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 145 "Net-(U41-DIN)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:TO-263AB_SUM"
		(layer "F.Cu")
		(at 47.0578 50.4192 90)
		(tags "SUM110P06-08L-E3 ")
		(property "Reference" "U25"
			(at -0.12275 -6.49955 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "SUM110P06-08L-E3"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "SUM110P06-08L-E3"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TO-263AB_SUM TO-263AB_SUM-M TO-263AB_SUM-L")
		(sheetname "/LCL_12V/12V_5A_LCL_2/")
		(sheetfile "12V_5A_LCL.kicad_sch")
		(attr smd)
		(fp_text user "*"
			(at -2.54 5.2705 90)
			(layer "F.Fab")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(fp_text user "*"
			(at -2.54 5.2705 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -2.54 8.8773 90)
			(size 0.9906 3.2004)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 56 "Net-(D8-K)")
			(pinfunction "G")
			(pintype "input")
		)
		(pad "2" smd rect
			(at 0 0.0508 90)
			(size 10.414 11.4554)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 22 "/LCL_12V/12V_5A_LCL_2/OPAMP_Minus")
			(pinfunction "D")
			(pintype "input")
		)
		(pad "3" smd rect
			(at 2.54 8.8773 90)
			(size 0.9906 3.2004)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 57 "/LCL_12.5A2")
			(pinfunction "S")
			(pintype "input")
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:CAPC1608X90"
		(layer "F.Cu")
		(at 222.10905 205.29195)
		(descr "<b>CAPACITOR</b>")
		(property "Reference" "C37"
			(at 2.6992 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "0.1uF"
			(at 2.81646 1.20613 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "SMD 0603 MLCC capacitor, Alternate KiCad Library"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/Digital Systems/")
		(sheetfile "Digital_Systems.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -0.85 0)
			(size 1.1 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 35 "/Digital Systems/3.3V+")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd rect
			(at 0.85 0)
			(size 1.1 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 303 "/GNDREF")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:RESC1508X55N"
		(layer "F.Cu")
		(at 59.5578 41.4192 90)
		(property "Reference" "R28"
			(at 3.12725 0.00045 90)
			(layer "F.SilkS")
		)
		(property "Value" "13.7k"
			(at 1.54 1.07 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Power_Connectors/")
		(sheetfile "Power_Connectors.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -0.76 0 90)
			(size 0.9 0.97)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 111 "Net-(R27-Pad2)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd rect
			(at 0.76 0 90)
			(size 0.9 0.97)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 303 "/GNDREF")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:RESC1508X55N"
		(layer "F.Cu")
		(at 286.60905 44.29195 -90)
		(property "Reference" "R44"
			(at -0.21 -1.07 90)
			(layer "F.SilkS")
		)
		(property "Value" "1k"
			(at 1.54 1.07 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Power_Connectors/")
		(sheetfile "Power_Connectors.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -0.76 0 270)
			(size 0.9 0.97)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 123 "Net-(U7D-IN-)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd rect
			(at 0.76 0 270)
			(size 0.9 0.97)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 119 "Net-(R39-Pad2)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:CAPC1608X90"
		(layer "F.Cu")
		(at 183.35905 241.29195 90)
		(descr "<b>CAPACITOR</b>")
		(property "Reference" "C32"
			(at 2.75 0.1992 90)
			(layer "F.SilkS")
		)
		(property "Value" "0.1uF"
			(at 1.56646 1.20613 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "SMD 0603 MLCC capacitor, Alternate KiCad Library"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/LCL_9_and_3-3/3-3V_1-5A_LCL_1/")
		(sheetfile "3-3V_1-5A_LCL.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -0.85 0 90)
			(size 1.1 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 33 "/LCL_9_and_3-3/3-3V_1-5A_LCL_1/OPAMP_Minus")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd rect
			(at 0.85 0 90)
			(size 1.1 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 34 "Net-(Q14-B)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:RESC1508X55N"
		(layer "F.Cu")
		(at 284.85905 42.79195 90)
		(property "Reference" "R40"
			(at 1 1.4492 90)
			(layer "F.SilkS")
		)
		(property "Value" "37.5k (37.4k)"
			(at 1.54 1.07 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Power_Connectors/")
		(sheetfile "Power_Connectors.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -0.76 0 90)
			(size 0.9 0.97)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 119 "Net-(R39-Pad2)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd rect
			(at 0.76 0 90)
			(size 0.9 0.97)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 303 "/GNDREF")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:RESC1508X55N"
		(layer "F.Cu")
		(at 145.924041 61.643258 -90)
		(property "Reference" "R77"
			(at 2.398692 -0.134209 90)
			(layer "F.SilkS")
		)
		(property "Value" "51k"
			(at 1.54 1.07 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/LCL_12V/12V_3A_LCL_1/")
		(sheetfile "12V_3A_LCL.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -0.76 0 270)
			(size 0.9 0.97)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 51 "Net-(D5-K)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd rect
			(at 0.76 0 270)
			(size 0.9 0.97)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 15 "Net-(Q5-B)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:RESC1608X55N"
		(layer "F.Cu")
		(at 76.707925 60.519375 90)
		(property "Reference" "R88"
			(at -0.022575 -1.149675 90)
			(layer "F.SilkS")
		)
		(property "Value" "86.6k"
			(at 1.54 1.049999 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/LCL_12V/12V_5A_LCL_1/")
		(sheetfile "12V_5A_LCL.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -0.82 0 90)
			(size 0.79 0.93)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 20 "Net-(Q7-B)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd rect
			(at 0.82 0 90)
			(size 0.79 0.93)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 19 "/LCL_12V/12V_5A_LCL_1/OPAMP_Minus")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:RESC1508X55N"
		(layer "F.Cu")
		(at 248.60905 197.79195 90)
		(property "Reference" "R149"
			(at -2.75 -0.3008 90)
			(layer "F.SilkS")
		)
		(property "Value" "22"
			(at 1.54 1.07 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Digital Systems/")
		(sheetfile "Digital_Systems.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -0.76 0 90)
			(size 0.9 0.97)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 305 "/Digital Systems/ADC2_CS")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd rect
			(at 0.76 0 90)
			(size 0.9 0.97)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 163 "Net-(U43-PF0)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:RESC1608X55N"
		(layer "F.Cu")
		(at 180.37825 60.29195 180)
		(property "Reference" "R108"
			(at -0.11 1.25 0)
			(layer "F.SilkS")
		)
		(property "Value" "86.6k"
			(at 1.54 1.05 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/LCL_5V/5V_6A_LCL_1/")
		(sheetfile "5V_6A_LCL.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -0.82 0 180)
			(size 0.79 0.93)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 60 "Net-(D10-K)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd rect
			(at 0.82 0 180)
			(size 0.79 0.93)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 26 "/LCL_5V/5V_6A_LCL_1/OPAMP_Minus")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:SOD3716X135N"
		(layer "F.Cu")
		(at 168.85905 251.54195 -90)
		(descr "sod-123-ren1")
		(tags "Diode")
		(property "Reference" "D14"
			(at 0 0 90)
			(layer "F.SilkS")
		)
		(property "Value" "D"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Diode"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Device" "D"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TO-???* *_Diode_* *SingleDiode* D_*")
		(sheetname "/LCL_9_and_3-3/3-3V_1-5A_LCL_1/")
		(sheetfile "3-3V_1-5A_LCL.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.65 0)
			(size 0.75 1.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 68 "Net-(D14-K)")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.65 0)
			(size 0.75 1.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 69 "/LCL_MIXED.3.3V1.5A")
			(pinfunction "A")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "1N4150W-E3-18.stp"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "EPS_Footprints:RESC1508X55N"
		(layer "F.Cu")
		(at 192.10905 43.04195 90)
		(property "Reference" "R34"
			(at 1 1.1992 90)
			(layer "F.SilkS")
		)
		(property "Value" "37.5k (37.4k)"
			(at 1.54 1.07 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Power_Connectors/")
		(sheetfile "Power_Connectors.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -0.76 0 90)
			(size 0.9 0.97)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 116 "Net-(R33-Pad2)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd rect
			(at 0.76 0 90)
			(size 0.9 0.97)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 303 "/GNDREF")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:M14A"
		(layer "F.Cu")
		(at 101.39525 246.79195)
		(tags "LPV324MX/NOPB ")
		(property "Reference" "U8"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "LPV324MX/NOPB"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://www.ti.com/lit/gpn/lpv324-n"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "M14A M14A-M M14A-L")
		(sheetname "/Power_Connectors/")
		(sheetfile "Power_Connectors.kicad_sch")
		(attr smd)
		(fp_text user "*"
			(at -2.7178 -5.5118 0)
			(layer "F.Fab")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(fp_text user "*"
			(at -2.7178 -5.5118 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -2.4638 -3.81)
			(size 1.9812 0.5588)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 240 "/V_MEAS.9_")
			(pinfunction "OUT")
			(pintype "output")
		)
		(pad "2" smd rect
			(at -2.4638 -2.54)
			(size 1.9812 0.5588)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 126 "Net-(U8A-IN-)")
			(pinfunction "IN-")
			(pintype "input")
		)
		(pad "3" smd rect
			(at -2.4638 -1.27)
			(size 1.9812 0.5588)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 240 "/V_MEAS.9_")
			(pinfunction "IN+")
			(pintype "input")
		)
		(pad "4" smd rect
			(at -2.4638 0)
			(size 1.9812 0.5588)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 72 "/DC_POS.3.3V")
			(pinfunction "V+")
			(pintype "input")
		)
		(pad "5" smd rect
			(at -2.4638 1.27)
			(size 1.9812 0.5588)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 237 "/V_MEAS.3.3_")
			(pinfunction "IN+")
			(pintype "input")
		)
		(pad "6" smd rect
			(at -2.4638 2.54)
			(size 1.9812 0.5588)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 127 "Net-(U8B-IN-)")
			(pinfunction "IN-")
			(pintype "input")
		)
		(pad "7" smd rect
			(at -2.4638 3.81)
			(size 1.9812 0.5588)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 237 "/V_MEAS.3.3_")
			(pinfunction "OUT")
			(pintype "output")
		)
		(pad "8" smd rect
			(at 2.4638 3.81)
			(size 1.9812 0.5588)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 242 "unconnected-(U8C-OUT-Pad8)")
			(pinfunction "OUT")
			(pintype "output+no_connect")
		)
		(pad "9" smd rect
			(at 2.4638 2.54)
			(size 1.9812 0.5588)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 241 "unconnected-(U8C-IN--Pad9)")
			(pinfunction "IN-")
			(pintype "input+no_connect")
		)
		(pad "10" smd rect
			(at 2.4638 1.27)
			(size 1.9812 0.5588)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 243 "unconnected-(U8C-IN+-Pad10)")
			(pinfunction "IN+")
			(pintype "input+no_connect")
		)
		(pad "11" smd rect
			(at 2.4638 0)
			(size 1.9812 0.5588)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 303 "/GNDREF")
			(pinfunction "V-")
			(pintype "input")
		)
		(pad "12" smd rect
			(at 2.4638 -1.27)
			(size 1.9812 0.5588)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 238 "unconnected-(U8D-IN+-Pad12)")
			(pinfunction "IN+")
			(pintype "input+no_connect")
		)
		(pad "13" smd rect
			(at 2.4638 -2.54)
			(size 1.9812 0.5588)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 239 "unconnected-(U8D-IN--Pad13)")
			(pinfunction "IN-")
			(pintype "input+no_connect")
		)
		(pad "14" smd rect
			(at 2.4638 -3.81)
			(size 1.9812 0.5588)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 244 "unconnected-(U8D-OUT-Pad14)")
			(pinfunction "OUT")
			(pintype "output+no_connect")
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:RESC1508X55N"
		(layer "F.Cu")
		(at 44.11905 236.80195 180)
		(property "Reference" "R46"
			(at -0.21 -1.07 0)
			(layer "F.SilkS")
		)
		(property "Value" "18.7k"
			(at 1.54 1.07 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Power_Connectors/")
		(sheetfile "Power_Connectors.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -0.76 0 180)
			(size 0.9 0.97)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 124 "Net-(R45-Pad2)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd rect
			(at 0.76 0 180)
			(size 0.9 0.97)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 303 "/GNDREF")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:M14A"
		(layer "F.Cu")
		(at 114.10905 84.04195 180)
		(tags "LPV324MX/NOPB ")
		(property "Reference" "U6"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "LPV324MX/NOPB"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://www.ti.com/lit/gpn/lpv324-n"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "M14A M14A-M M14A-L")
		(sheetname "/Power_Connectors/")
		(sheetfile "Power_Connectors.kicad_sch")
		(attr smd)
		(fp_text user "*"
			(at -2.7178 -5.5118 0)
			(layer "F.SilkS")
		)
		(fp_text user "*"
			(at -2.7178 -5.5118 180)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
		)
		(fp_text user "*"
			(at -2.7178 -5.5118 0)
			(layer "F.Fab")
		)
		(fp_text user "*"
			(at -2.7178 -5.5118 180)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -2.4638 -3.81 180)
			(size 1.9812 0.5588)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 232 "/V_MEAS.12_5")
			(pinfunction "OUT")
			(pintype "output")
		)
		(pad "2" smd rect
			(at -2.4638 -2.54 180)
			(size 1.9812 0.5588)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 112 "Net-(U6A-IN-)")
			(pinfunction "IN-")
			(pintype "input")
		)
		(pad "3" smd rect
			(at -2.4638 -1.27 180)
			(size 1.9812 0.5588)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 232 "/V_MEAS.12_5")
			(pinfunction "IN+")
			(pintype "input")
		)
		(pad "4" smd rect
			(at -2.4638 0 180)
			(size 1.9812 0.5588)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 72 "/DC_POS.3.3V")
			(pinfunction "V+")
			(pintype "input")
		)
		(pad "5" smd rect
			(at -2.4638 1.27 180)
			(size 1.9812 0.5588)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 231 "/V_MEAS.12_6")
			(pinfunction "IN+")
			(pintype "input")
		)
		(pad "6" smd rect
			(at -2.4638 2.54 180)
			(size 1.9812 0.5588)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 113 "Net-(U6B-IN-)")
			(pinfunction "IN-")
			(pintype "input")
		)
		(pad "7" smd rect
			(at -2.4638 3.81 180)
			(size 1.9812 0.5588)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 231 "/V_MEAS.12_6")
			(pinfunction "OUT")
			(pintype "output")
		)
		(pad "8" smd rect
			(at 2.4638 3.81 180)
			(size 1.9812 0.5588)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 229 "/V_MEAS.12_7")
			(pinfunction "OUT")
			(pintype "output")
		)
		(pad "9" smd rect
			(at 2.4638 2.54 180)
			(size 1.9812 0.5588)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 114 "Net-(U6C-IN-)")
			(pinfunction "IN-")
			(pintype "input")
		)
		(pad "10" smd rect
			(at 2.4638 1.27 180)
			(size 1.9812 0.5588)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 229 "/V_MEAS.12_7")
			(pinfunction "IN+")
			(pintype "input")
		)
		(pad "11" smd rect
			(at 2.4638 0 180)
			(size 1.9812 0.5588)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 303 "/GNDREF")
			(pinfunction "V-")
			(pintype "input")
		)
		(pad "12" smd rect
			(at 2.4638 -1.27 180)
			(size 1.9812 0.5588)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 230 "/V_MEAS.12_8")
			(pinfunction "IN+")
			(pintype "input")
		)
		(pad "13" smd rect
			(at 2.4638 -2.54 180)
			(size 1.9812 0.5588)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 115 "Net-(U6D-IN-)")
			(pinfunction "IN-")
			(pintype "input")
		)
		(pad "14" smd rect
			(at 2.4638 -3.81 180)
			(size 1.9812 0.5588)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 230 "/V_MEAS.12_8")
			(pinfunction "OUT")
			(pintype "output")
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:Terminal Block 691137710002"
		(layer "F.Cu")
		(at 200.60905 250.54195)
		(property "Reference" "J18"
			(at 0 -5.135 0)
			(layer "F.SilkS")
		)
		(property "Value" "691137710002"
			(at 4.12 5.365 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/Digital_Connectors/")
		(sheetfile "Digital_Connectors.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole circle
			(at -2.5 0)
			(size 1.95 1.95)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 78 "/ADC_AIN3")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" thru_hole circle
			(at 2.5 0)
			(size 1.95 1.95)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 303 "/GNDREF")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:CAPC1608X90"
		(layer "F.Cu")
		(at 209.92905 62.641949 -90)
		(descr "<b>CAPACITOR</b>")
		(property "Reference" "C29"
			(at 2.650001 -0.1292 90)
			(layer "F.SilkS")
		)
		(property "Value" "0.1uF"
			(at 1.566459 1.20613 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "SMD 0603 MLCC capacitor, Alternate KiCad Library"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/LCL_5V/5V_6A_LCL_2/")
		(sheetfile "5V_6A_LCL.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -0.85 0 270)
			(size 1.1 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 27 "/LCL_5V/5V_6A_LCL_2/OPAMP_Minus")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd rect
			(at 0.85 0 270)
			(size 1.1 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 28 "Net-(Q11-B)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:RESC1508X55N"
		(layer "F.Cu")
		(at 59.5578 44.6692 90)
		(property "Reference" "R27"
			(at -0.62275 -1.24955 90)
			(layer "F.SilkS")
		)
		(property "Value" "100k"
			(at 1.54 1.07 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Power_Connectors/")
		(sheetfile "Power_Connectors.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -0.76 0 90)
			(size 0.9 0.97)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 57 "/LCL_12.5A2")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd rect
			(at 0.76 0 90)
			(size 0.9 0.97)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 111 "Net-(R27-Pad2)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:LED_LTST-C170GKT_LTO"
		(layer "F.Cu")
		(at 265.60905 176.79195 90)
		(tags "LTST-C170GKT ")
		(property "Reference" "LED1"
			(at -0.161413 -1.5508 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "LTST-C170GKT"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "LTST-C170GKT"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "LED_LTST-C170GKT_LTO")
		(sheetname "/Digital Systems/")
		(sheetfile "Digital_Systems.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.0541 0 90)
			(size 1.1938 1.1938)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 89 "Net-(LED1-Pad1)")
			(pintype "unspecified")
		)
		(pad "2" smd rect
			(at 1.0541 0 90)
			(size 1.1938 1.1938)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 35 "/Digital Systems/3.3V+")
			(pintype "unspecified")
		)
		(zone
			(net 0)
			(net_name "")
			(layer "F.Cu")
			(hatch full 0.508)
			(connect_pads
				(clearance 0)
			)
			(min_thickness 0.254)
			(filled_areas_thickness no)
			(keepout
				(tracks not_allowed)
				(vias not_allowed)
				(pads allowed)
				(copperpour not_allowed)
				(footprints allowed)
			)
			(placement
				(enabled no)
				(sheetname "")
			)
			(fill
				(thermal_gap 0.508)
				(thermal_bridge_width 0.508)
			)
			(polygon
				(pts
					(xy 265.03755 177.19835) (xy 265.03755 176.38555) (xy 266.18055 176.38555) (xy 266.18055 177.19835)
				)
			)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:RESC1508X55N"
		(layer "F.Cu")
		(at 113.90295 61.30435 -90)
		(property "Reference" "R83"
			(at 2.4876 0.0947 90)
			(layer "F.SilkS")
		)
		(property "Value" "51k"
			(at 1.54 1.07 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/LCL_12V/12V_3A_LCL_2/")
		(sheetfile "12V_3A_LCL.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -0.76 0 270)
			(size 0.9 0.97)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 52 "Net-(D6-K)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd rect
			(at 0.76 0 270)
			(size 0.9 0.97)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 17 "Net-(Q6-B)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:RESC1508X55N"
		(layer "F.Cu")
		(at 225.60905 188.23695 180)
		(property "Reference" "R161"
			(at -0.21 -1.07 0)
			(layer "F.SilkS")
		)
		(property "Value" "0 Ohm"
			(at 1.54 1.07 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MF" "Stackpole Electronics Inc"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description_1" "0 Ohms Jumper 0.1W, 1/10W Chip Resistor 0603 (1608 Metric) Automotive AEC-Q200 Thick Film"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Package" "1508 Stackpole"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Price" "None"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SnapEDA_Link" "https://www.snapeda.com/parts/RMCF0603ZT0R00/Stackpole+Electronics/view-part/?ref=snap"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MP" "RMCF0603ZT0R00"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Purchase-URL" "https://www.snapeda.com/api/url_track_click_mouser/?unipart_id=3968849&manufacturer=Stackpole Electronics Inc&part_name=RMCF0603ZT0R00&search_term=rmcf0603zt0r00"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Availability" "In Stock"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Check_prices" "https://www.snapeda.com/parts/RMCF0603ZT0R00/Stackpole+Electronics/view-part/?ref=eda"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/Digital Systems/")
		(sheetfile "Digital_Systems.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -0.76 0 180)
			(size 0.9 0.97)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 144 "/Digital Systems/SSI0Tx")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd rect
			(at 0.76 0 180)
			(size 0.9 0.97)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 174 "Net-(U44-DIN)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:RESC1508X55N"
		(layer "F.Cu")
		(at 232.60905 205.78195 -90)
		(property "Reference" "R182"
			(at -0.21 1.3008 90)
			(layer "F.SilkS")
		)
		(property "Value" "470"
			(at 1.54 1.07 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Digital Systems/")
		(sheetfile "Digital_Systems.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -0.76 0 270)
			(size 0.9 0.97)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 170 "/Digital Systems/SSI0Rx")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd rect
			(at 0.76 0 270)
			(size 0.9 0.97)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 207 "Net-(U46-SO)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:RESC1508X55N"
		(layer "F.Cu")
		(at 158.835609 44.395191 -90)
		(property "Reference" "R29"
			(at -0.21 -1.07 90)
			(layer "F.SilkS")
		)
		(property "Value" "1k"
			(at 1.54 1.07 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Power_Connectors/")
		(sheetfile "Power_Connectors.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -0.76 0 270)
			(size 0.9 0.97)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 112 "Net-(U6A-IN-)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd rect
			(at 0.76 0 270)
			(size 0.9 0.97)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 108 "Net-(R21-Pad2)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:RESC1508X55N"
		(layer "F.Cu")
		(at 254.35905 46.29195 90)
		(property "Reference" "R37"
			(at -1 -1.07 90)
			(layer "F.SilkS")
		)
		(property "Value" "100k"
			(at 1.54 1.07 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Power_Connectors/")
		(sheetfile "Power_Connectors.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -0.76 0 90)
			(size 0.9 0.97)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 59 "/LCL_5.6A3")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd rect
			(at 0.76 0 90)
			(size 0.9 0.97)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 118 "Net-(R37-Pad2)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:RESC1508X55N"
		(layer "F.Cu")
		(at 233.11905 224.29195)
		(property "Reference" "R169"
			(at -2.5608 -0.5 0)
			(layer "F.SilkS")
		)
		(property "Value" "100"
			(at 1.54 1.07 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Digital Systems/")
		(sheetfile "Digital_Systems.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -0.76 0)
			(size 0.9 0.97)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 184 "/LCL_CTRL4")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd rect
			(at 0.76 0)
			(size 0.9 0.97)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 185 "Net-(U45-P0_3)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:RESC1508X55N"
		(layer "F.Cu")
		(at 217.15905 60.36695 90)
		(property "Reference" "R116"
			(at -2.675 -0.1008 90)
			(layer "F.SilkS")
		)
		(property "Value" "54.9k"
			(at 1.54 1.069999 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/LCL_5V/5V_6A_LCL_2/")
		(sheetfile "5V_6A_LCL.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -0.76 0 90)
			(size 0.9 0.97)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 138 "Net-(R115-Pad1)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd rect
			(at 0.76 0 90)
			(size 0.9 0.97)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 62 "Net-(D11-K)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:BAQ33GS08"
		(layer "F.Cu")
		(at 157.60905 241.79195 180)
		(descr "MiniMELF (SOD-80)")
		(tags "Zener Diode")
		(property "Reference" "ZD14"
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "D_Zener"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Zener diode"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Library" "TZM5240B-GS08.txt"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Name" "TZM5240B-GS08"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Device" "D"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" "1=A 2=K"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TO-???* *_Diode_* *SingleDiode* D_*")
		(sheetname "/LCL_9_and_3-3/3-3V_1-5A_LCL_1/")
		(sheetfile "3-3V_1-5A_LCL.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.875 0 180)
			(size 1.25 2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 33 "/LCL_9_and_3-3/3-3V_1-5A_LCL_1/OPAMP_Minus")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.875 0 180)
			(size 1.25 2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 68 "Net-(D14-K)")
			(pinfunction "A")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "TZM5224B-GS08.stp"
			(offset
				(xyz 0 0 0.7999999999)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "EPS_Footprints:RESC1608X55N"
		(layer "F.Cu")
		(at 280.35905 60.29195 90)
		(property "Reference" "R121"
			(at -2.5 -0.0508 90)
			(layer "F.SilkS")
		)
		(property "Value" "5.1k"
			(at 1.54 1.049999 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/LCL_5V/5V_6A_LCL_4/")
		(sheetfile "5V_6A_LCL.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -0.82 0 90)
			(size 0.79 0.93)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 139 "Net-(R121-Pad1)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd rect
			(at 0.82 0 90)
			(size 0.79 0.93)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 65 "Net-(D12-K)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:SOP65P640X110-24N"
		(layer "F.Cu")
		(at 240.72905 219.86695)
		(property "Reference" "U45"
			(at -1.970183 -4.71161 0)
			(layer "F.SilkS")
		)
		(property "Value" "PCA9555APW_118"
			(at -0.330955 9.194005 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DigiKey_Part_Number" "568-9919-1-ND"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SnapEDA_Link" "https://www.snapeda.com/parts/PCA9555APW,118/NXP+Semiconductors/view-part/?ref=snap"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description_1" "I/O Expander 16 I2C, SMBus 400 kHz 24-TSSOP"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Package" "TSSOP-24 NXP Semiconductors"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Check_prices" "https://www.snapeda.com/parts/PCA9555APW,118/NXP+Semiconductors/view-part/?ref=eda"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "STANDARD" "IPC 7351B"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTREV" "1.1"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MF" "NXP USA"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MP" "PCA9555APW,118"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER" "NXP"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/Digital Systems/")
		(sheetfile "Digital_Systems.kicad_sch")
		(attr smd)
		(pad "1" smd roundrect
			(at -2.87 -3.575)
			(size 1.57 0.41)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.05)
			(net 162 "/Digital Systems/GPIO_INT")
			(pinfunction "~{INT}")
			(pintype "output")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd roundrect
			(at -2.87 -2.925)
			(size 1.57 0.41)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.05)
			(net 303 "/GNDREF")
			(pinfunction "A1")
			(pintype "input")
			(solder_mask_margin 0.102)
		)
		(pad "3" smd roundrect
			(at -2.87 -2.275)
			(size 1.57 0.41)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.05)
			(net 303 "/GNDREF")
			(pinfunction "A2")
			(pintype "input")
			(solder_mask_margin 0.102)
		)
		(pad "4" smd roundrect
			(at -2.87 -1.625)
			(size 1.57 0.41)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.05)
			(net 179 "Net-(U45-P0_0)")
			(pinfunction "P0_0")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "5" smd roundrect
			(at -2.87 -0.975)
			(size 1.57 0.41)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.05)
			(net 180 "Net-(U45-P0_1)")
			(pinfunction "P0_1")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "6" smd roundrect
			(at -2.87 -0.325)
			(size 1.57 0.41)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.05)
			(net 183 "Net-(U45-P0_2)")
			(pinfunction "P0_2")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "7" smd roundrect
			(at -2.87 0.325)
			(size 1.57 0.41)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.05)
			(net 185 "Net-(U45-P0_3)")
			(pinfunction "P0_3")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "8" smd roundrect
			(at -2.87 0.975)
			(size 1.57 0.41)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.05)
			(net 187 "Net-(U45-P0_4)")
			(pinfunction "P0_4")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "9" smd roundrect
			(at -2.87 1.625)
			(size 1.57 0.41)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.05)
			(net 188 "Net-(U45-P0_5)")
			(pinfunction "P0_5")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "10" smd roundrect
			(at -2.87 2.275)
			(size 1.57 0.41)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.05)
			(net 191 "Net-(U45-P0_6)")
			(pinfunction "P0_6")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "11" smd roundrect
			(at -2.87 2.925)
			(size 1.57 0.41)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.05)
			(net 192 "Net-(U45-P0_7)")
			(pinfunction "P0_7")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "12" smd roundrect
			(at -2.87 3.575)
			(size 1.57 0.41)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.05)
			(net 303 "/GNDREF")
			(pinfunction "VSS")
			(pintype "power_in")
			(solder_mask_margin 0.102)
		)
		(pad "13" smd roundrect
			(at 2.87 3.575)
			(size 1.57 0.41)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.05)
			(net 194 "Net-(U45-P1_0)")
			(pinfunction "P1_0")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "14" smd roundrect
			(at 2.87 2.925)
			(size 1.57 0.41)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.05)
			(net 197 "Net-(U45-P1_1)")
			(pinfunction "P1_1")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "15" smd roundrect
			(at 2.87 2.275)
			(size 1.57 0.41)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.05)
			(net 199 "Net-(U45-P1_2)")
			(pinfunction "P1_2")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "16" smd roundrect
			(at 2.87 1.625)
			(size 1.57 0.41)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.05)
			(net 200 "Net-(U45-P1_3)")
			(pinfunction "P1_3")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "17" smd roundrect
			(at 2.87 0.975)
			(size 1.57 0.41)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.05)
			(net 203 "Net-(U45-P1_4)")
			(pinfunction "P1_4")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "18" smd roundrect
			(at 2.87 0.325)
			(size 1.57 0.41)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.05)
			(net 204 "Net-(U45-P1_5)")
			(pinfunction "P1_5")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "19" smd roundrect
			(at 2.87 -0.325)
			(size 1.57 0.41)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.05)
			(net 301 "unconnected-(U45-P1_6-Pad19)")
			(pinfunction "P1_6")
			(pintype "bidirectional+no_connect")
			(solder_mask_margin 0.102)
		)
		(pad "20" smd roundrect
			(at 2.87 -0.975)
			(size 1.57 0.41)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.05)
			(net 300 "unconnected-(U45-P1_7-Pad20)")
			(pinfunction "P1_7")
			(pintype "bidirectional+no_connect")
			(solder_mask_margin 0.102)
		)
		(pad "21" smd roundrect
			(at 2.87 -1.625)
			(size 1.57 0.41)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.05)
			(net 303 "/GNDREF")
			(pinfunction "A0")
			(pintype "input")
			(solder_mask_margin 0.102)
		)
		(pad "22" smd roundrect
			(at 2.87 -2.275)
			(size 1.57 0.41)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.05)
			(net 152 "/Digital Systems/I2C0SCL")
			(pinfunction "SCL")
			(pintype "input")
			(solder_mask_margin 0.102)
		)
		(pad "23" smd roundrect
			(at 2.87 -2.925)
			(size 1.57 0.41)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.05)
			(net 155 "/Digital Systems/I2C0SDA")
			(pinfunction "SDA")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "24" smd roundrect
			(at 2.87 -3.575)
			(size 1.57 0.41)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.05)
			(net 35 "/Digital Systems/3.3V+")
			(pinfunction "VDD")
			(pintype "power_in")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:TO-263AB_SUM"
		(layer "F.Cu")
		(at 53.10905 213.94225 180)
		(tags "SUM110P06-08L-E3 ")
		(property "Reference" "U11"
			(at 0.0508 -6.3497 180)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "SUM110P06-08L-E3"
			(at -0.34 3.193 180)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "SUM110P06-08L-E3"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TO-263AB_SUM TO-263AB_SUM-M TO-263AB_SUM-L")
		(sheetname "/LCL_12V/12V_12A_LCL_1/")
		(sheetfile "12V_12A_LCL.kicad_sch")
		(attr smd)
		(fp_text user "*"
			(at -5.715 8.8773 0)
			(layer "F.SilkS")
		)
		(fp_text user "*"
			(at -5.715 8.8773 180)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "*"
			(at -2.54 5.2705 0)
			(layer "F.Fab")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
		)
		(fp_text user "*"
			(at -2.54 5.2705 180)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -2.54 8.8773 180)
			(size 0.9906 3.2004)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 42 "Net-(D1-K)")
			(pinfunction "G")
			(pintype "input")
		)
		(pad "2" smd rect
			(at 0 0.0508 180)
			(size 10.414 11.4554)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 7 "/LCL_12V/12V_12A_LCL_1/OPAMP_Minus")
			(pinfunction "D")
			(pintype "input")
		)
		(pad "3" smd rect
			(at 2.54 8.8773 180)
			(size 0.9906 3.2004)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 43 "/LCL_12.12A1")
			(pinfunction "S")
			(pintype "input")
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:Current Sense Amplifier SOP65P640X120-14N"
		(layer "F.Cu")
		(at 209.22905 79.49195)
		(property "Reference" "U27"
			(at -0.73 -3.635 0)
			(layer "F.SilkS")
		)
		(property "Value" "INA4180A2IPWR"
			(at 6.89 3.635 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTREV" "H"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "STANDARD" "IPC 7351B"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SNAPEDA_PN" "INA4180A2IPWR"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MAXIMUM_PACKAGE_HEIGHT" "1.2 mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER" "Texas Instruments"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/LCL_5V/")
		(sheetfile "LCL_5V.kicad_sch")
		(attr smd)
		(pad "1" smd roundrect
			(at -2.87 -1.95)
			(size 1.57 0.41)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.125)
			(net 272 "/I_MEAS.5_1")
			(pintype "output")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd roundrect
			(at -2.87 -1.3)
			(size 1.57 0.41)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.125)
			(net 26 "/LCL_5V/5V_6A_LCL_1/OPAMP_Minus")
			(pintype "input")
			(solder_mask_margin 0.102)
		)
		(pad "3" smd roundrect
			(at -2.87 -0.65)
			(size 1.57 0.41)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.125)
			(net 4 "/DC_POS.5V")
			(pintype "input")
			(solder_mask_margin 0.102)
		)
		(pad "4" smd roundrect
			(at -2.87 0)
			(size 1.57 0.41)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.125)
			(net 72 "/DC_POS.3.3V")
			(pintype "power_in")
			(solder_mask_margin 0.102)
		)
		(pad "5" smd roundrect
			(at -2.87 0.65)
			(size 1.57 0.41)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.125)
			(net 4 "/DC_POS.5V")
			(pintype "input")
			(solder_mask_margin 0.102)
		)
		(pad "6" smd roundrect
			(at -2.87 1.3)
			(size 1.57 0.41)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.125)
			(net 27 "/LCL_5V/5V_6A_LCL_2/OPAMP_Minus")
			(pintype "input")
			(solder_mask_margin 0.102)
		)
		(pad "7" smd roundrect
			(at -2.87 1.95)
			(size 1.57 0.41)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.125)
			(net 269 "/I_MEAS.5_2")
			(pintype "output")
			(solder_mask_margin 0.102)
		)
		(pad "8" smd roundrect
			(at 2.87 1.95)
			(size 1.57 0.41)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.125)
			(net 271 "/I_MEAS.5_3")
			(pintype "output")
			(solder_mask_margin 0.102)
		)
		(pad "9" smd roundrect
			(at 2.87 1.3)
			(size 1.57 0.41)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.125)
			(net 24 "/LCL_5V/5V_6A_LCL_3/OPAMP_Minus")
			(pintype "input")
			(solder_mask_margin 0.102)
		)
		(pad "10" smd roundrect
			(at 2.87 0.65)
			(size 1.57 0.41)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.125)
			(net 4 "/DC_POS.5V")
			(pintype "input")
			(solder_mask_margin 0.102)
		)
		(pad "11" smd roundrect
			(at 2.87 0)
			(size 1.57 0.41)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.125)
			(net 303 "/GNDREF")
			(pintype "power_in")
			(solder_mask_margin 0.102)
		)
		(pad "12" smd roundrect
			(at 2.87 -0.65)
			(size 1.57 0.41)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.125)
			(net 4 "/DC_POS.5V")
			(pintype "input")
			(solder_mask_margin 0.102)
		)
		(pad "13" smd roundrect
			(at 2.87 -1.3)
			(size 1.57 0.41)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.125)
			(net 30 "/LCL_5V/5V_6A_LCL_4/OPAMP_Minus")
			(pintype "input")
			(solder_mask_margin 0.102)
		)
		(pad "14" smd roundrect
			(at 2.87 -1.95)
			(size 1.57 0.41)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.125)
			(net 270 "/I_MEAS.5_4")
			(pintype "output")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:RESC1508X55N"
		(layer "F.Cu")
		(at 48.53905 168.04195 180)
		(property "Reference" "R62"
			(at -2.2692 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "54.9k"
			(at 1.54 1.07 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/LCL_12V/12V_12A_LCL_2/")
		(sheetfile "12V_12A_LCL.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -0.76 0 180)
			(size 0.9 0.97)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 129 "Net-(R61-Pad1)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd rect
			(at 0.76 0 180)
			(size 0.9 0.97)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 44 "Net-(D2-K)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:BAQ33GS08"
		(layer "F.Cu")
		(at 43.60905 104.66695 90)
		(descr "MiniMELF (SOD-80)")
		(tags "Zener Diode")
		(property "Reference" "ZD4"
			(at 4.625 0 90)
			(layer "F.SilkS")
		)
		(property "Value" "D_Zener"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Zener diode"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Library" "TZM5240B-GS08.txt"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Name" "TZM5240B-GS08"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Device" "D"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" "1=A 2=K"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TO-???* *_Diode_* *SingleDiode* D_*")
		(sheetname "/LCL_12V/12V_12A_LCL_4/")
		(sheetfile "12V_12A_LCL.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.875 0 90)
			(size 1.25 2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 13 "/LCL_12V/12V_12A_LCL_4/OPAMP_Minus")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.875 0 90)
			(size 1.25 2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 49 "Net-(D4-K)")
			(pinfunction "A")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "TZM5224B-GS08.stp"
			(offset
				(xyz 0 0 0.7999999999)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "EPS_Footprints:RESC1508X55N"
		(layer "F.Cu")
		(at 61.3078 43.1692 -90)
		(property "Reference" "R32"
			(at -0.21 -1.07 90)
			(layer "F.SilkS")
		)
		(property "Value" "1k"
			(at 1.54 1.07 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Power_Connectors/")
		(sheetfile "Power_Connectors.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -0.76 0 270)
			(size 0.9 0.97)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 115 "Net-(U6D-IN-)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd rect
			(at 0.76 0 270)
			(size 0.9 0.97)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 111 "Net-(R27-Pad2)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:RES_TLRP3A30DR018FTE_TEC"
		(layer "F.Cu")
		(at 163.841941 50.563259 180)
		(tags "TLRP3A30DR018FTE ")
		(property "Reference" "R75"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "0.01"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/LCL_12V/12V_3A_LCL_1/")
		(sheetfile "12V_3A_LCL.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -2.8321 0 180)
			(size 1.397 3.4544)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 5 "/DC_POS.12V")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 2.8321 0 180)
			(size 1.397 3.4544)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 16 "/LCL_12V/12V_3A_LCL_1/OPAMP_Minus")
			(pintype "passive")
		)
		(zone
			(net 0)
			(net_name "")
			(layer "F.Cu")
			(hatch full 0.508)
			(connect_pads
				(clearance 0)
			)
			(min_thickness 0.254)
			(filled_areas_thickness no)
			(keepout
				(tracks not_allowed)
				(vias not_allowed)
				(pads allowed)
				(copperpour not_allowed)
				(footprints allowed)
			)
			(placement
				(enabled no)
				(sheetname "")
			)
			(fill
				(thermal_gap 0.508)
				(thermal_bridge_width 0.508)
			)
			(polygon
				(pts
					(xy 165.924741 52.239659) (xy 161.759141 52.239659) (xy 161.759141 48.886859) (xy 165.924741 48.886859)
				)
			)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:SOD3716X135N"
		(layer "F.Cu")
		(at 192.55825 52.79195 90)
		(descr "sod-123-ren1")
		(tags "Diode")
		(property "Reference" "D10"
			(at 0 0 90)
			(layer "F.SilkS")
		)
		(property "Value" "D"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Diode"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Device" "D"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TO-???* *_Diode_* *SingleDiode* D_*")
		(sheetname "/LCL_5V/5V_6A_LCL_1/")
		(sheetfile "5V_6A_LCL.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.65 0 180)
			(size 0.75 1.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 60 "Net-(D10-K)")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.65 0 180)
			(size 0.75 1.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 61 "/LCL_5.6A1")
			(pinfunction "A")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "1N4150W-E3-18.stp"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "EPS_Footprints:SOT91P240X120-3N"
		(layer "F.Cu")
		(at 59.83405 244.62695 90)
		(property "Reference" "Q13"
			(at -0.176 -2.3698 90)
			(layer "F.SilkS")
		)
		(property "Value" "PNP"
			(at 3.1768 2.3698 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://ngspice.sourceforge.io/docs/ngspice-html-manual/manual.xhtml#cha_BJTs"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Bipolar transistor symbol for simulation only, substrate tied to the emitter"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Device" "PNP"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Type" "GUMMELPOON"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" "1=C 2=B 3=E"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/LCL_9_and_3-3/9V_2A_LCL_1/")
		(sheetfile "9V_2A_LCL.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -0.915 1.025 90)
			(size 0.61 1.18)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 67 "Net-(D13-K)")
			(pinfunction "C")
			(pintype "open_collector")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd rect
			(at 0.915 1.025 90)
			(size 0.61 1.18)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 31 "Net-(Q13-B)")
			(pinfunction "B")
			(pintype "input")
			(solder_mask_margin 0.102)
		)
		(pad "3" smd rect
			(at 0 -1.025 90)
			(size 0.61 1.18)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 32 "/LCL_9_and_3-3/9V_2A_LCL_1/OPAMP_Minus")
			(pinfunction "E")
			(pintype "open_emitter")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:BAQ33GS08"
		(layer "F.Cu")
		(at 57.95855 128.31745 90)
		(descr "MiniMELF (SOD-80)")
		(tags "Zener Diode")
		(property "Reference" "ZD3"
			(at 0 0 90)
			(layer "F.SilkS")
		)
		(property "Value" "D_Zener"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Zener diode"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Library" "TZM5240B-GS08.txt"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Name" "TZM5240B-GS08"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Device" "D"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" "1=A 2=K"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TO-???* *_Diode_* *SingleDiode* D_*")
		(sheetname "/LCL_12V/12V_12A_LCL_3/")
		(sheetfile "12V_12A_LCL.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.875 0 90)
			(size 1.25 2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 11 "/LCL_12V/12V_12A_LCL_3/OPAMP_Minus")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.875 0 90)
			(size 1.25 2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 46 "Net-(D3-K)")
			(pinfunction "A")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "TZM5224B-GS08.stp"
			(offset
				(xyz 0 0 0.7999999999)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "EPS_Footprints:RESC1508X55N"
		(layer "F.Cu")
		(at 222.10905 198.54195 180)
		(property "Reference" "R139"
			(at -2.6992 0.25 0)
			(layer "F.SilkS")
		)
		(property "Value" "0 Ohm"
			(at 1.54 1.07 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MF" "Stackpole Electronics Inc"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description_1" "0 Ohms Jumper 0.1W, 1/10W Chip Resistor 0603 (1608 Metric) Automotive AEC-Q200 Thick Film"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Package" "1508 Stackpole"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Price" "None"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SnapEDA_Link" "https://www.snapeda.com/parts/RMCF0603ZT0R00/Stackpole+Electronics/view-part/?ref=snap"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MP" "RMCF0603ZT0R00"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Purchase-URL" "https://www.snapeda.com/api/url_track_click_mouser/?unipart_id=3968849&manufacturer=Stackpole Electronics Inc&part_name=RMCF0603ZT0R00&search_term=rmcf0603zt0r00"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Availability" "In Stock"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Check_prices" "https://www.snapeda.com/parts/RMCF0603ZT0R00/Stackpole+Electronics/view-part/?ref=eda"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/Digital Systems/")
		(sheetfile "Digital_Systems.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -0.76 0 180)
			(size 0.9 0.97)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 150 "/Digital Systems/ADC1_EOC")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd rect
			(at 0.76 0 180)
			(size 0.9 0.97)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 149 "Net-(U41-~{EOC})")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:CAPC1608X90"
		(layer "F.Cu")
		(at 240.67905 62.891949 -90)
		(descr "<b>CAPACITOR</b>")
		(property "Reference" "C27"
			(at 2.650001 0.1208 90)
			(layer "F.SilkS")
		)
		(property "Value" "0.1uF"
			(at 1.566459 1.20613 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "SMD 0603 MLCC capacitor, Alternate KiCad Library"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/LCL_5V/5V_6A_LCL_3/")
		(sheetfile "5V_6A_LCL.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -0.85 0 270)
			(size 1.1 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 24 "/LCL_5V/5V_6A_LCL_3/OPAMP_Minus")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd rect
			(at 0.85 0 270)
			(size 1.1 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 23 "Net-(Q9-B)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:RESC1508X55N"
		(layer "F.Cu")
		(at 250.35905 199.79195 90)
		(property "Reference" "R150"
			(at -2.75 0.1992 90)
			(layer "F.SilkS")
		)
		(property "Value" "22"
			(at 1.54 1.07 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Digital Systems/")
		(sheetfile "Digital_Systems.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -0.76 0 90)
			(size 0.9 0.97)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 164 "/Digital Systems/ADC2_EOC")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd rect
			(at 0.76 0 90)
			(size 0.9 0.97)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 165 "Net-(U43-PF1)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:RESC1508X55N"
		(layer "F.Cu")
		(at 49.10905 100.79195 180)
		(property "Reference" "R74"
			(at 2.5508 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "54.9k"
			(at 1.54 1.069999 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/LCL_12V/12V_12A_LCL_4/")
		(sheetfile "12V_12A_LCL.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -0.76 0 180)
			(size 0.9 0.97)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 131 "Net-(R73-Pad1)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd rect
			(at 0.76 0 180)
			(size 0.9 0.97)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 49 "Net-(D4-K)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:Terminal Block 691137710002"
		(layer "F.Cu")
		(at 213.85905 250.54195)
		(property "Reference" "J19"
			(at 0 -5.135 0)
			(layer "F.SilkS")
		)
		(property "Value" "691137710002"
			(at 4.12 5.365 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/Digital_Connectors/")
		(sheetfile "Digital_Connectors.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole circle
			(at -2.5 0)
			(size 1.95 1.95)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 79 "/ADC_AIN2")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" thru_hole circle
			(at 2.5 0)
			(size 1.95 1.95)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 303 "/GNDREF")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:SOT91P240X120-3N"
		(layer "F.Cu")
		(at 179.02405 241.56695 180)
		(property "Reference" "Q14"
			(at -0.176 -2.3698 0)
			(layer "F.SilkS")
		)
		(property "Value" "PNP"
			(at 3.1768 2.3698 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://ngspice.sourceforge.io/docs/ngspice-html-manual/manual.xhtml#cha_BJTs"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Bipolar transistor symbol for simulation only, substrate tied to the emitter"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Device" "PNP"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Type" "GUMMELPOON"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" "1=C 2=B 3=E"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/LCL_9_and_3-3/3-3V_1-5A_LCL_1/")
		(sheetfile "3-3V_1-5A_LCL.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -0.915 1.025 180)
			(size 0.61 1.18)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 68 "Net-(D14-K)")
			(pinfunction "C")
			(pintype "open_collector")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd rect
			(at 0.915 1.025 180)
			(size 0.61 1.18)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 34 "Net-(Q14-B)")
			(pinfunction "B")
			(pintype "input")
			(solder_mask_margin 0.102)
		)
		(pad "3" smd rect
			(at 0 -1.025 180)
			(size 0.61 1.18)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 33 "/LCL_9_and_3-3/3-3V_1-5A_LCL_1/OPAMP_Minus")
			(pinfunction "E")
			(pintype "open_emitter")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:CAPC1608X87N"
		(layer "F.Cu")
		(at 264.30905 188.81695 -90)
		(property "Reference" "C40"
			(at -0.24 -1.07 90)
			(layer "F.SilkS")
		)
		(property "Value" "12pF"
			(at 1.51 1.07 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DigiKey_Part_Number" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SnapEDA_Link" "https://www.snapeda.com/parts/C0603C120K4HAC7867/Kemet/view-part/?ref=snap"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description_1" "CAP CER 0603 12PF 16V ULTRA STAB"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MF" "KEMET"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Package" "1608 KEMET"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Check_prices" "https://www.snapeda.com/parts/C0603C120K4HAC7867/Kemet/view-part/?ref=eda"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MP" "C0603C120K4HAC7867"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/Digital Systems/")
		(sheetfile "Digital_Systems.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -0.775 0 270)
			(size 0.92 0.97)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 41 "/Digital Systems/OSC1")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd rect
			(at 0.775 0 270)
			(size 0.92 0.97)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 303 "/GNDREF")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:RESC1508X55N"
		(layer "F.Cu")
		(at 211.67905 62.551949 -90)
		(property "Reference" "R113"
			(at 2.740001 -0.1292 90)
			(layer "F.SilkS")
		)
		(property "Value" "11.5k"
			(at 1.539999 1.07 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/LCL_5V/5V_6A_LCL_2/")
		(sheetfile "5V_6A_LCL.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -0.76 0 270)
			(size 0.9 0.97)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 62 "Net-(D11-K)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd rect
			(at 0.76 0 270)
			(size 0.9 0.97)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 28 "Net-(Q11-B)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:SOT91P240X120-3N"
		(layer "F.Cu")
		(at 62.98355 144.85745 90)
		(property "Reference" "Q3"
			(at -0.175999 -2.3698 90)
			(layer "F.SilkS")
		)
		(property "Value" "PNP"
			(at 3.1768 2.3698 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://ngspice.sourceforge.io/docs/ngspice-html-manual/manual.xhtml#cha_BJTs"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Bipolar transistor symbol for simulation only, substrate tied to the emitter"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Device" "PNP"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Type" "GUMMELPOON"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" "1=C 2=B 3=E"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/LCL_12V/12V_12A_LCL_3/")
		(sheetfile "12V_12A_LCL.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -0.915 1.025 90)
			(size 0.61 1.18)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 46 "Net-(D3-K)")
			(pinfunction "C")
			(pintype "open_collector")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd rect
			(at 0.915 1.025 90)
			(size 0.61 1.18)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 12 "Net-(Q3-B)")
			(pinfunction "B")
			(pintype "input")
			(solder_mask_margin 0.102)
		)
		(pad "3" smd rect
			(at 0 -1.025 90)
			(size 0.61 1.18)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 11 "/LCL_12V/12V_12A_LCL_3/OPAMP_Minus")
			(pinfunction "E")
			(pintype "open_emitter")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:RESC1508X55N"
		(layer "F.Cu")
		(at 152.60905 252.80195 90)
		(property "Reference" "R50"
			(at -0.21 -1.07 90)
			(layer "F.SilkS")
		)
		(property "Value" "1k"
			(at 1.54 1.07 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Power_Connectors/")
		(sheetfile "Power_Connectors.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -0.76 0 90)
			(size 0.9 0.97)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 127 "Net-(U8B-IN-)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd rect
			(at 0.76 0 90)
			(size 0.9 0.97)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 125 "Net-(R47-Pad2)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:RESC1608X55N"
		(layer "F.Cu")
		(at 51.59905 106.74195)
		(property "Reference" "R72"
			(at 2.4592 0.05 0)
			(layer "F.SilkS")
		)
		(property "Value" "86.6k"
			(at 1.54 1.05 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/LCL_12V/12V_12A_LCL_4/")
		(sheetfile "12V_12A_LCL.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -0.82 0)
			(size 0.79 0.93)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 49 "Net-(D4-K)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd rect
			(at 0.82 0)
			(size 0.79 0.93)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 13 "/LCL_12V/12V_12A_LCL_4/OPAMP_Minus")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:RESC1508X55N"
		(layer "F.Cu")
		(at 245.10905 200.29195 90)
		(property "Reference" "R145"
			(at -0.25 -1.3008 90)
			(layer "F.SilkS")
		)
		(property "Value" "22"
			(at 1.54 1.07 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Digital Systems/")
		(sheetfile "Digital_Systems.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -0.76 0 90)
			(size 0.9 0.97)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 304 "/Digital Systems/ADC1_CS")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd rect
			(at 0.76 0 90)
			(size 0.9 0.97)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 157 "Net-(U43-PA3{slash}SSI0FSS)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:RESC1608X55N"
		(layer "F.Cu")
		(at 85.607925 60.519375 90)
		(property "Reference" "R91"
			(at -2.272575 -0.049675 90)
			(layer "F.SilkS")
		)
		(property "Value" "8.87k"
			(at 1.54 1.049999 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/LCL_12V/12V_5A_LCL_1/")
		(sheetfile "12V_5A_LCL.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -0.82 0 90)
			(size 0.79 0.93)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 134 "Net-(R91-Pad1)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd rect
			(at 0.82 0 90)
			(size 0.79 0.93)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 55 "Net-(D7-K)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:SOT91P240X120-3N"
		(layer "F.Cu")
		(at 275.85905 62.291949)
		(property "Reference" "Q12"
			(at -0.175999 -2.3698 0)
			(layer "F.SilkS")
		)
		(property "Value" "PNP"
			(at 3.176799 2.3698 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://ngspice.sourceforge.io/docs/ngspice-html-manual/manual.xhtml#cha_BJTs"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Bipolar transistor symbol for simulation only, substrate tied to the emitter"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Device" "PNP"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Type" "GUMMELPOON"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" "1=C 2=B 3=E"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/LCL_5V/5V_6A_LCL_4/")
		(sheetfile "5V_6A_LCL.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -0.915 1.025)
			(size 0.61 1.18)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 65 "Net-(D12-K)")
			(pinfunction "C")
			(pintype "open_collector")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd rect
			(at 0.915 1.025)
			(size 0.61 1.18)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 29 "Net-(Q12-B)")
			(pinfunction "B")
			(pintype "input")
			(solder_mask_margin 0.102)
		)
		(pad "3" smd rect
			(at 0 -1.025)
			(size 0.61 1.18)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 30 "/LCL_5V/5V_6A_LCL_4/OPAMP_Minus")
			(pinfunction "E")
			(pintype "open_emitter")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:SOT91P240X120-3N"
		(layer "F.Cu")
		(at 47.60905 104.51695 180)
		(property "Reference" "Q4"
			(at -0.175999 -2.3698 0)
			(layer "F.SilkS")
		)
		(property "Value" "PNP"
			(at 3.1768 2.3698 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://ngspice.sourceforge.io/docs/ngspice-html-manual/manual.xhtml#cha_BJTs"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Bipolar transistor symbol for simulation only, substrate tied to the emitter"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Device" "PNP"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Type" "GUMMELPOON"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" "1=C 2=B 3=E"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/LCL_12V/12V_12A_LCL_4/")
		(sheetfile "12V_12A_LCL.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -0.915 1.025 180)
			(size 0.61 1.18)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 49 "Net-(D4-K)")
			(pinfunction "C")
			(pintype "open_collector")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd rect
			(at 0.915 1.025 180)
			(size 0.61 1.18)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 14 "Net-(Q4-B)")
			(pinfunction "B")
			(pintype "input")
			(solder_mask_margin 0.102)
		)
		(pad "3" smd rect
			(at 0 -1.025 180)
			(size 0.61 1.18)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 13 "/LCL_12V/12V_12A_LCL_4/OPAMP_Minus")
			(pinfunction "E")
			(pintype "open_emitter")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "MountingHole:MountingHole_3.2mm_M3"
		(layer "F.Cu")
		(at 42.00825 72.84195)
		(descr "Mounting Hole 3.2mm, M3, no annular, generated by kicad-footprint-generator mountinghole.py")
		(tags "mountinghole M3")
		(property "Reference" "H1"
			(at 0 -4.15 0)
			(layer "F.SilkS")
		)
		(property "Value" "MountingHole"
			(at 0 4.15 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Mounting Hole without connection"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "MountingHole*")
		(sheetname "/")
		(sheetfile "PEEKbot_EPS.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 3.2 3.2)
			(drill 3.2)
			(layers "*.Cu" "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:RESC1608X55N"
		(layer "F.Cu")
		(at 45.4878 57.4192 180)
		(property "Reference" "R96"
			(at 2.67955 0.12725 0)
			(layer "F.SilkS")
		)
		(property "Value" "86.6k"
			(at 1.54 1.05 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/LCL_12V/12V_5A_LCL_2/")
		(sheetfile "12V_5A_LCL.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -0.82 0 180)
			(size 0.79 0.93)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 56 "Net-(D8-K)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd rect
			(at 0.82 0 180)
			(size 0.79 0.93)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 22 "/LCL_12V/12V_5A_LCL_2/OPAMP_Minus")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:BAQ33GS08"
		(layer "F.Cu")
		(at 131.52795 54.47435)
		(descr "MiniMELF (SOD-80)")
		(tags "Zener Diode")
		(property "Reference" "ZD6"
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "D_Zener"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Zener diode"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Library" "TZM5240B-GS08.txt"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Name" "TZM5240B-GS08"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Device" "D"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" "1=A 2=K"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TO-???* *_Diode_* *SingleDiode* D_*")
		(sheetname "/LCL_12V/12V_3A_LCL_2/")
		(sheetfile "12V_3A_LCL.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.875 0)
			(size 1.25 2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 18 "/LCL_12V/12V_3A_LCL_2/OPAMP_Minus")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.875 0)
			(size 1.25 2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 52 "Net-(D6-K)")
			(pinfunction "A")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "TZM5224B-GS08.stp"
			(offset
				(xyz 0 0 0.7999999999)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "EPS_Footprints:SOT91P240X120-3N"
		(layer "F.Cu")
		(at 48.8928 59.9442)
		(property "Reference" "Q8"
			(at -0.176 -2.3698 0)
			(layer "F.SilkS")
		)
		(property "Value" "PNP"
			(at -0.085 -0.025 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://ngspice.sourceforge.io/docs/ngspice-html-manual/manual.xhtml#cha_BJTs"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Bipolar transistor symbol for simulation only, substrate tied to the emitter"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Device" "PNP"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Type" "GUMMELPOON"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" "1=C 2=B 3=E"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/LCL_12V/12V_5A_LCL_2/")
		(sheetfile "12V_5A_LCL.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -0.915 1.025)
			(size 0.61 1.18)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 56 "Net-(D8-K)")
			(pinfunction "C")
			(pintype "open_collector")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd rect
			(at 0.915 1.025)
			(size 0.61 1.18)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 21 "Net-(Q8-B)")
			(pinfunction "B")
			(pintype "input")
			(solder_mask_margin 0.102)
		)
		(pad "3" smd rect
			(at 0 -1.025)
			(size 0.61 1.18)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 22 "/LCL_12V/12V_5A_LCL_2/OPAMP_Minus")
			(pinfunction "E")
			(pintype "open_emitter")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:RESC1508X55N"
		(layer "F.Cu")
		(at 59.39405 239.76895 180)
		(property "Reference" "R128"
			(at -2.6642 -0.023 0)
			(layer "F.SilkS")
		)
		(property "Value" "54.9k"
			(at 1.54 1.07 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/LCL_9_and_3-3/9V_2A_LCL_1/")
		(sheetfile "9V_2A_LCL.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -0.76 0 180)
			(size 0.9 0.97)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 140 "Net-(R127-Pad1)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd rect
			(at 0.76 0 180)
			(size 0.9 0.97)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 67 "Net-(D13-K)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:BAQ33GS08"
		(layer "F.Cu")
		(at 198.43325 55.04195)
		(descr "MiniMELF (SOD-80)")
		(tags "Zener Diode")
		(property "Reference" "ZD10"
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "D_Zener"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Zener diode"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Library" "TZM5240B-GS08.txt"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Name" "TZM5240B-GS08"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Device" "D"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" "1=A 2=K"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TO-???* *_Diode_* *SingleDiode* D_*")
		(sheetname "/LCL_5V/5V_6A_LCL_1/")
		(sheetfile "5V_6A_LCL.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.875 0)
			(size 1.25 2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 26 "/LCL_5V/5V_6A_LCL_1/OPAMP_Minus")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.875 0)
			(size 1.25 2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 60 "Net-(D10-K)")
			(pinfunction "A")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "TZM5224B-GS08.stp"
			(offset
				(xyz 0 0 0.7999999999)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "EPS_Footprints:Terminal Block 691137710002"
		(layer "F.Cu")
		(at 40.85905 190.29195 -90)
		(property "Reference" "J4"
			(at 0 -5.135 90)
			(layer "F.SilkS")
		)
		(property "Value" "691137710002"
			(at 4.12 5.365 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/Power_Connectors/")
		(sheetfile "Power_Connectors.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole circle
			(at -2.5 0 270)
			(size 1.95 1.95)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 303 "/GNDREF")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" thru_hole circle
			(at 2.5 0 270)
			(size 1.95 1.95)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 45 "/LCL_12.12A2")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:RESC1508X55N"
		(layer "F.Cu")
		(at 233.59905 226.29195)
		(property "Reference" "R170"
			(at -2.5408 -0.5 0)
			(layer "F.SilkS")
		)
		(property "Value" "100"
			(at 1.54 1.07 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Digital Systems/")
		(sheetfile "Digital_Systems.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -0.76 0)
			(size 0.9 0.97)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 186 "/LCL_CTRL5")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd rect
			(at 0.76 0)
			(size 0.9 0.97)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 187 "Net-(U45-P0_4)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:RESC1508X55N"
		(layer "F.Cu")
		(at 232.10905 220.29195)
		(property "Reference" "R167"
			(at -1.3008 -1.25 0)
			(layer "F.SilkS")
		)
		(property "Value" "100"
			(at 1.54 1.07 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Digital Systems/")
		(sheetfile "Digital_Systems.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -0.76 0)
			(size 0.9 0.97)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 181 "/LCL_CTRL2")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd rect
			(at 0.76 0)
			(size 0.9 0.97)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 180 "Net-(U45-P0_1)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:XTAL_ABM3-16.000MHZ-B2-T"
		(layer "F.Cu")
		(at 260.05905 188.54195)
		(property "Reference" "Y1"
			(at 2.7492 -2.25 0)
			(layer "F.SilkS")
		)
		(property "Value" "ABM3-16.000MHZ-B2-T"
			(at 6.5036 2.5064 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DigiKey_Part_Number" "535-9103-1-ND"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SnapEDA_Link" "https://www.snapeda.com/parts/ABM3-16.000MHZ-B2-T/Abracon/view-part/?ref=snap"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MAXIMUM_PACKAGE_HEIGHT" "1.3 mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Package" "SMD-2 Abracon LLC"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Check_prices" "https://www.snapeda.com/parts/ABM3-16.000MHZ-B2-T/Abracon/view-part/?ref=eda"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "STANDARD" "Manufacturer Recommendations"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTREV" "4/25/2022"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MF" "Abracon"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MP" "ABM3-16.000MHZ-B2-T"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description_1" "16 MHz ±20ppm Crystal 18pF 40 Ohms 2-SMD, No Lead"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER" "Abracon"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/Digital Systems/")
		(sheetfile "Digital_Systems.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -2.05 0)
			(size 1.9 2.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 37 "Net-(U43-OSC0)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd rect
			(at 2.05 0)
			(size 1.9 2.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 41 "/Digital Systems/OSC1")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:Terminal Block 691137710002"
		(layer "F.Cu")
		(at 217.10905 42.29195 180)
		(property "Reference" "J12"
			(at -0.6992 -4.75 0)
			(layer "F.SilkS")
		)
		(property "Value" "691137710002"
			(at 4.12 5.365 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/Power_Connectors/")
		(sheetfile "Power_Connectors.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole circle
			(at -2.5 0 180)
			(size 1.95 1.95)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 303 "/GNDREF")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" thru_hole circle
			(at 2.5 0 180)
			(size 1.95 1.95)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 63 "/LCL_5.6A2")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:RESC1508X55N"
		(layer "F.Cu")
		(at 228.85905 191.79195 180)
		(property "Reference" "R163"
			(at -2.6992 -0.25 0)
			(layer "F.SilkS")
		)
		(property "Value" "0 Ohm"
			(at 1.54 1.07 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MF" "Stackpole Electronics Inc"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description_1" "0 Ohms Jumper 0.1W, 1/10W Chip Resistor 0603 (1608 Metric) Automotive AEC-Q200 Thick Film"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Package" "1508 Stackpole"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Price" "None"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SnapEDA_Link" "https://www.snapeda.com/parts/RMCF0603ZT0R00/Stackpole+Electronics/view-part/?ref=snap"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MP" "RMCF0603ZT0R00"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Purchase-URL" "https://www.snapeda.com/api/url_track_click_mouser/?unipart_id=3968849&manufacturer=Stackpole Electronics Inc&part_name=RMCF0603ZT0R00&search_term=rmcf0603zt0r00"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Availability" "In Stock"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Check_prices" "https://www.snapeda.com/parts/RMCF0603ZT0R00/Stackpole+Electronics/view-part/?ref=eda"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/Digital Systems/")
		(sheetfile "Digital_Systems.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -0.76 0 180)
			(size 0.9 0.97)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 305 "/Digital Systems/ADC2_CS")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd rect
			(at 0.76 0 180)
			(size 0.9 0.97)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 176 "Net-(U44-~{CS})")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:DIP762W50P254L730H410Q6"
		(layer "F.Cu")
		(at 168.79905 241.58195)
		(property "Reference" "U40"
			(at 0.06 -2.29 0)
			(layer "F.SilkS")
		)
		(property "Value" "CNY17-1"
			(at 0.06 1.46 0)
			(layer "Dwgs.User")
		)
		(property "Datasheet" "http://www.vishay.com/docs/83606/cny17.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "DC Optocoupler Base Connected, Vce 70V, CTR 40-80%, Viso 5000V (RMS), DIP6"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "DIP*W7.62mm* DIP*W10.16mm* SMDIP*W9.53mm*")
		(sheetname "/LCL_9_and_3-3/3-3V_1-5A_LCL_1/")
		(sheetfile "3-3V_1-5A_LCL.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole rect
			(at -3.81 -2.54)
			(size 1.4 1.4)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 205 "/LCL_CTRL14")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" thru_hole circle
			(at -3.81 0)
			(size 1.4 1.4)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 303 "/GNDREF")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "3" thru_hole circle
			(at -3.81 2.54)
			(size 1.4 1.4)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 291 "unconnected-(U40-NC-Pad3)")
			(pinfunction "NC")
			(pintype "no_connect")
			(solder_mask_margin 0.102)
		)
		(pad "4" thru_hole circle
			(at 3.81 2.54)
			(size 1.4 1.4)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 303 "/GNDREF")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "5" thru_hole circle
			(at 3.81 0)
			(size 1.4 1.4)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 141 "Net-(R133-Pad1)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "6" thru_hole circle
			(at 3.81 -2.54)
			(size 1.4 1.4)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 292 "unconnected-(U40-Pad6)")
			(pintype "passive+no_connect")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:CAPC1608X90"
		(layer "F.Cu")
		(at 222.35905 190.73695)
		(descr "<b>CAPACITOR</b>")
		(property "Reference" "C47"
			(at -0.235423 -1.237214 0)
			(layer "F.SilkS")
		)
		(property "Value" "0.1uF"
			(at 1.56646 1.20613 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "SMD 0603 MLCC capacitor, Alternate KiCad Library"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/Digital Systems/")
		(sheetfile "Digital_Systems.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -0.85 0)
			(size 1.1 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 35 "/Digital Systems/3.3V+")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd rect
			(at 0.85 0)
			(size 1.1 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 303 "/GNDREF")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:Terminal Block 691137710002"
		(layer "F.Cu")
		(at 40.85905 244.04195 -90)
		(property "Reference" "J15"
			(at -1.25 -4.6992 90)
			(layer "F.SilkS")
		)
		(property "Value" "691137710002"
			(at 38.365 0.38 180)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/Power_Connectors/")
		(sheetfile "Power_Connectors.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole circle
			(at -2.5 0 270)
			(size 1.95 1.95)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 303 "/GNDREF")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" thru_hole circle
			(at 2.5 0 270)
			(size 1.95 1.95)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 66 "/LCL_MIXED.9V2A")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "MountingHole:MountingHole_3.2mm_M3"
		(layer "F.Cu")
		(at 145.20825 256.84195)
		(descr "Mounting Hole 3.2mm, M3, no annular, generated by kicad-footprint-generator mountinghole.py")
		(tags "mountinghole M3")
		(property "Reference" "H4"
			(at 0 -4.15 0)
			(layer "F.SilkS")
		)
		(property "Value" "MountingHole"
			(at 0 4.15 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Mounting Hole without connection"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "MountingHole*")
		(sheetname "/")
		(sheetfile "PEEKbot_EPS.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 3.2 3.2)
			(drill 3.2)
			(layers "*.Cu" "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:DIP762W50P254L730H410Q6"
		(layer "F.Cu")
		(at 255.29905 61.331949 180)
		(property "Reference" "U29"
			(at -7.41 -9.94 0)
			(layer "F.SilkS")
		)
		(property "Value" "CNY17-1"
			(at -0.209999 9.94 0)
			(layer "Dwgs.User")
		)
		(property "Datasheet" "http://www.vishay.com/docs/83606/cny17.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "DC Optocoupler Base Connected, Vce 70V, CTR 40-80%, Viso 5000V (RMS), DIP6"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "DIP*W7.62mm* DIP*W10.16mm* SMDIP*W9.53mm*")
		(sheetname "/LCL_5V/5V_6A_LCL_3/")
		(sheetfile "5V_6A_LCL.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole rect
			(at -3.81 -2.54 180)
			(size 1.4 1.4)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 198 "/LCL_CTRL11")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" thru_hole circle
			(at -3.81 0 180)
			(size 1.4 1.4)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 303 "/GNDREF")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "3" thru_hole circle
			(at -3.81 2.54 180)
			(size 1.4 1.4)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 273 "unconnected-(U29-NC-Pad3)")
			(pinfunction "NC")
			(pintype "no_connect")
			(solder_mask_margin 0.102)
		)
		(pad "4" thru_hole circle
			(at 3.81 2.54 180)
			(size 1.4 1.4)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 303 "/GNDREF")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "5" thru_hole circle
			(at 3.81 0 180)
			(size 1.4 1.4)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 136 "Net-(R103-Pad1)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "6" thru_hole circle
			(at 3.81 -2.54 180)
			(size 1.4 1.4)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 274 "unconnected-(U29-Pad6)")
			(pintype "passive+no_connect")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:BAQ33GS08"
		(layer "F.Cu")
		(at 163.549041 54.813259)
		(descr "MiniMELF (SOD-80)")
		(tags "Zener Diode")
		(property "Reference" "ZD5"
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "D_Zener"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Zener diode"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Library" "TZM5240B-GS08.txt"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Name" "TZM5240B-GS08"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Device" "D"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" "1=A 2=K"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TO-???* *_Diode_* *SingleDiode* D_*")
		(sheetname "/LCL_12V/12V_3A_LCL_1/")
		(sheetfile "12V_3A_LCL.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.875 0)
			(size 1.25 2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 16 "/LCL_12V/12V_3A_LCL_1/OPAMP_Minus")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.875 0)
			(size 1.25 2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 51 "Net-(D5-K)")
			(pinfunction "A")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "TZM5224B-GS08.stp"
			(offset
				(xyz 0 0 0.7999999999)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MountingHole:MountingHole_3.2mm_M3"
		(layer "F.Cu")
		(at 281.40825 247.04195)
		(descr "Mounting Hole 3.2mm, M3, no annular, generated by kicad-footprint-generator mountinghole.py")
		(tags "mountinghole M3")
		(property "Reference" "H3"
			(at 0 -4.15 0)
			(layer "F.SilkS")
		)
		(property "Value" "MountingHole"
			(at 0 4.15 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Mounting Hole without connection"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "MountingHole*")
		(sheetname "/")
		(sheetfile "PEEKbot_EPS.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 3.2 3.2)
			(drill 3.2)
			(layers "*.Cu" "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:RES_1206_OHM"
		(layer "F.Cu")
		(at 39.60905 171.31855 -90)
		(tags "MCS1632R005FER ")
		(property "Reference" "R57"
			(at 0 1.8008 270)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "0.005"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/LCL_12V/12V_12A_LCL_2/")
		(sheetfile "12V_12A_LCL.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.5266 0 270)
			(size 0.7032 1.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 5 "/DC_POS.12V")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.5266 0 270)
			(size 0.7032 1.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 10 "/LCL_12V/12V_12A_LCL_2/OPAMP_Minus")
			(pintype "passive")
		)
		(zone
			(net 0)
			(net_name "")
			(layer "F.Cu")
			(hatch full 0.508)
			(connect_pads
				(clearance 0)
			)
			(min_thickness 0.254)
			(filled_areas_thickness no)
			(keepout
				(tracks not_allowed)
				(vias not_allowed)
				(pads allowed)
				(copperpour not_allowed)
				(footprints allowed)
			)
			(placement
				(enabled no)
				(sheetname "")
			)
			(fill
				(thermal_gap 0.508)
				(thermal_bridge_width 0.508)
			)
			(polygon
				(pts
					(xy 40.40825 170.194349) (xy 40.40825 172.442751) (xy 38.80985 172.442751) (xy 38.80985 170.194349)
				)
			)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:RESC1508X55N"
		(layer "F.Cu")
		(at 222.35905 187.73695)
		(property "Reference" "R181"
			(at -0.21 -1.07 0)
			(layer "F.SilkS")
		)
		(property "Value" "0 Ohm"
			(at 1.54 1.07 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MF" "Stackpole Electronics Inc"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description_1" "0 Ohms Jumper 0.1W, 1/10W Chip Resistor 0603 (1608 Metric) Automotive AEC-Q200 Thick Film"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Package" "1508 Stackpole"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Price" "None"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SnapEDA_Link" "https://www.snapeda.com/parts/RMCF0603ZT0R00/Stackpole+Electronics/view-part/?ref=snap"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MP" "RMCF0603ZT0R00"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Purchase-URL" "https://www.snapeda.com/api/url_track_click_mouser/?unipart_id=3968849&manufacturer=Stackpole Electronics Inc&part_name=RMCF0603ZT0R00&search_term=rmcf0603zt0r00"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Availability" "In Stock"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Check_prices" "https://www.snapeda.com/parts/RMCF0603ZT0R00/Stackpole+Electronics/view-part/?ref=eda"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/Digital Systems/")
		(sheetfile "Digital_Systems.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -0.76 0)
			(size 0.9 0.97)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 206 "Net-(U44-DOUT)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd rect
			(at 0.76 0)
			(size 0.9 0.97)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 170 "/Digital Systems/SSI0Rx")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:TO-263AB_SUM"
		(layer "F.Cu")
		(at 51.10905 250.19225 180)
		(tags "SUM110P06-08L-E3 ")
		(property "Reference" "U37"
			(at 0.0508 -6.3497 180)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "SUM110P06-08L-E3"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "SUM110P06-08L-E3"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TO-263AB_SUM TO-263AB_SUM-M TO-263AB_SUM-L")
		(sheetname "/LCL_9_and_3-3/9V_2A_LCL_1/")
		(sheetfile "9V_2A_LCL.kicad_sch")
		(attr smd)
		(fp_text user "*"
			(at -6.25 8.6503 0)
			(layer "F.SilkS")
		)
		(fp_text user "*"
			(at -6.25 8.6503 180)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
		)
		(fp_text user "*"
			(at -2.54 5.2705 0)
			(layer "F.Fab")
		)
		(fp_text user "*"
			(at -2.54 5.2705 180)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -2.54 8.8773 180)
			(size 0.9906 3.2004)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 67 "Net-(D13-K)")
			(pinfunction "G")
			(pintype "input")
		)
		(pad "2" smd rect
			(at 0 0.0508 180)
			(size 10.414 11.4554)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 32 "/LCL_9_and_3-3/9V_2A_LCL_1/OPAMP_Minus")
			(pinfunction "D")
			(pintype "input")
		)
		(pad "3" smd rect
			(at 2.54 8.8773 180)
			(size 0.9906 3.2004)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 66 "/LCL_MIXED.9V2A")
			(pinfunction "S")
			(pintype "input")
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:RESC1508X55N"
		(layer "F.Cu")
		(at 248.10905 221.54195)
		(property "Reference" "R179"
			(at 2.6992 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "100"
			(at 1.54 1.07 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Digital Systems/")
		(sheetfile "Digital_Systems.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -0.76 0)
			(size 0.9 0.97)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 203 "Net-(U45-P1_4)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd rect
			(at 0.76 0)
			(size 0.9 0.97)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 202 "/LCL_CTRL13")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:Terminal Block 691137710002"
		(layer "F.Cu")
		(at 41.20855 140.29195 -90)
		(property "Reference" "J5"
			(at 0 -5.135 90)
			(layer "F.SilkS")
		)
		(property "Value" "691137710002"
			(at 4.12 5.365 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/Power_Connectors/")
		(sheetfile "Power_Connectors.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole circle
			(at -2.5 0 270)
			(size 1.95 1.95)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 303 "/GNDREF")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" thru_hole circle
			(at 2.5 0 270)
			(size 1.95 1.95)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 47 "/LCL_12.12A3")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:Terminal Block 691137710002"
		(layer "F.Cu")
		(at 41.10905 122.54195 -90)
		(property "Reference" "J6"
			(at 0 -5.135 90)
			(layer "F.SilkS")
		)
		(property "Value" "691137710002"
			(at 4.12 5.365 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/Power_Connectors/")
		(sheetfile "Power_Connectors.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole circle
			(at -2.5 0 270)
			(size 1.95 1.95)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 303 "/GNDREF")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" thru_hole circle
			(at 2.5 0 270)
			(size 1.95 1.95)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 48 "/LCL_12.12A4")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:RESC1608X55N"
		(layer "F.Cu")
		(at 176.35905 242.29195 -90)
		(property "Reference" "R133"
			(at -2.75 0.0508 90)
			(layer "F.SilkS")
		)
		(property "Value" "5k (4.99k)"
			(at 1.54 1.05 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/LCL_9_and_3-3/3-3V_1-5A_LCL_1/")
		(sheetfile "3-3V_1-5A_LCL.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -0.82 0 270)
			(size 0.79 0.93)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 141 "Net-(R133-Pad1)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd rect
			(at 0.82 0 270)
			(size 0.79 0.93)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 68 "Net-(D14-K)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:Terminal Block 691137710002"
		(layer "F.Cu")
		(at 53.0578 40.4192 180)
		(property "Reference" "J10"
			(at -1.00045 -4.62275 0)
			(layer "F.SilkS")
		)
		(property "Value" "691137710002"
			(at 0.75 2.75 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/Power_Connectors/")
		(sheetfile "Power_Connectors.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole circle
			(at -2.5 0 180)
			(size 1.95 1.95)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 303 "/GNDREF")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" thru_hole circle
			(at 2.5 0 180)
			(size 1.95 1.95)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 57 "/LCL_12.5A2")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:RESC1508X55N"
		(layer "B.Cu")
		(at 81.97905 203.06195 180)
		(property "Reference" "R3"
			(at -0.21 -1.23 0)
			(layer "B.SilkS")
		)
		(property "Value" "0 Ohm"
			(at 1.54 -1.07 0)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MF" "Stackpole Electronics Inc"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description_1" "0 Ohms Jumper 0.1W, 1/10W Chip Resistor 0603 (1608 Metric) Automotive AEC-Q200 Thick Film"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Package" "1508 Stackpole"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Price" "None"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "SnapEDA_Link" "https://www.snapeda.com/parts/RMCF0603ZT0R00/Stackpole+Electronics/view-part/?ref=snap"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MP" "RMCF0603ZT0R00"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Purchase-URL" "https://www.snapeda.com/api/url_track_click_mouser/?unipart_id=3968849&manufacturer=Stackpole Electronics Inc&part_name=RMCF0603ZT0R00&search_term=rmcf0603zt0r00"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Availability" "In Stock"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Check_prices" "https://www.snapeda.com/parts/RMCF0603ZT0R00/Stackpole+Electronics/view-part/?ref=eda"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(sheetname "/DC-DC_Converters/")
		(sheetfile "DC-DC_Converters.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -0.76 0 180)
			(size 0.9 0.97)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 93 "Net-(U3--S)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd rect
			(at 0.76 0 180)
			(size 0.9 0.97)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 303 "/GNDREF")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:TAJD_AVX"
		(layer "B.Cu")
		(at 248.47905 69.14195 180)
		(tags "TAJD106K025RNJ ")
		(property "Reference" "C8"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "CP_SMD_Tantalum_AVX-N_7343"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "SMD Tantalum Electrolytic Capacitor, AVX-N, 7343, European Symbol, Alternate KiCad Library"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "CP_*")
		(sheetname "/DC-DC_Converters/")
		(sheetfile "DC-DC_Converters.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
		)
		(pad "1" smd rect
			(at -2.8829 0 90)
			(size 2.54 1.8796)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 4 "/DC_POS.5V")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 2.8829 0 90)
			(size 2.54 1.8796)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 303 "/GNDREF")
			(pintype "passive")
		)
		(zone
			(net 0)
			(net_name "")
			(layer "B.Cu")
			(hatch full 0.508)
			(connect_pads
				(clearance 0)
			)
			(min_thickness 0.254)
			(filled_areas_thickness no)
			(keepout
				(tracks not_allowed)
				(vias not_allowed)
				(pads allowed)
				(copperpour not_allowed)
				(footprints allowed)
			)
			(placement
				(enabled no)
				(sheetname "")
			)
			(fill
				(thermal_gap 0.508)
				(thermal_bridge_width 0.508)
			)
			(polygon
				(pts
					(xy 250.37135 67.79575) (xy 246.58675 67.79575) (xy 246.58675 70.48815) (xy 250.37135 70.48815)
				)
			)
		)
		(zone
			(net 0)
			(net_name "")
			(layer "B.Cu")
			(hatch full 0.508)
			(connect_pads
				(clearance 0)
			)
			(min_thickness 0.254)
			(filled_areas_thickness no)
			(keepout
				(tracks not_allowed)
				(vias not_allowed)
				(pads allowed)
				(copperpour not_allowed)
				(footprints allowed)
			)
			(placement
				(enabled no)
				(sheetname "")
			)
			(fill
				(thermal_gap 0.508)
				(thermal_bridge_width 0.508)
			)
			(polygon
				(pts
					(xy 252.17475 66.94485) (xy 244.78335 66.94485) (xy 244.78335 67.79575) (xy 252.17475 67.79575)
				)
			)
		)
		(zone
			(net 0)
			(net_name "")
			(layer "B.Cu")
			(hatch full 0.508)
			(connect_pads
				(clearance 0)
			)
			(min_thickness 0.254)
			(filled_areas_thickness no)
			(keepout
				(tracks not_allowed)
				(vias not_allowed)
				(pads allowed)
				(copperpour not_allowed)
				(footprints allowed)
			)
			(placement
				(enabled no)
				(sheetname "")
			)
			(fill
				(thermal_gap 0.508)
				(thermal_bridge_width 0.508)
			)
			(polygon
				(pts
					(xy 252.17475 70.48815) (xy 244.78335 70.48815) (xy 244.78335 71.33905) (xy 252.17475 71.33905)
				)
			)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:CAPPRD500W60D1000H1600"
		(layer "B.Cu")
		(at 60.70905 105.69195 -90)
		(property "Reference" "C16"
			(at 1.1 5.6508 90)
			(layer "B.SilkS")
		)
		(property "Value" "CP_SMD_Tantalum_AVX-N_7343"
			(at 0.25 -7.75 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "SMD Tantalum Electrolytic Capacitor, AVX-N, 7343, European Symbol, Alternate KiCad Library"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "CP_*")
		(sheetname "/DC-DC_Converters/")
		(sheetfile "DC-DC_Converters.kicad_sch")
		(attr through_hole)
		(pad "N" thru_hole circle
			(at 2.5 0 270)
			(size 1.2 1.2)
			(drill 0.85)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 303 "/GNDREF")
			(solder_mask_margin 0.102)
		)
		(pad "P" thru_hole rect
			(at -2.5 0 270)
			(size 1.2 1.2)
			(drill 0.85)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "/DC_POS.12V")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:CAP_EEHZU1V471P"
		(layer "B.Cu")
		(at 230.22905 139.74195 90)
		(property "Reference" "C5"
			(at -0.55 5.8292 90)
			(layer "B.SilkS")
		)
		(property "Value" "C_0603"
			(at 5.975 -6.535 90)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "SMD 0603 MLCC capacitor, Alternate KiCad Library"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/DC-DC_Converters/")
		(sheetfile "DC-DC_Converters.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -4.35 0 90)
			(size 4.1 2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 303 "/GNDREF")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd rect
			(at 4.35 0 90)
			(size 4.1 2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 3 "Net-(PS1-+V_INPUT)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:CAPPRD750W80D1800H3550"
		(layer "B.Cu")
		(at 200.20905 103.19195 90)
		(property "Reference" "C9"
			(at -1.45 10.335 90)
			(layer "B.SilkS")
		)
		(property "Value" "CP_SMD_Tantalum_AVX-N_7343"
			(at 9.345 -10.315 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "SMD Tantalum Electrolytic Capacitor, AVX-N, 7343, European Symbol, Alternate KiCad Library"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "CP_*")
		(sheetname "/DC-DC_Converters/")
		(sheetfile "DC-DC_Converters.kicad_sch")
		(attr through_hole)
		(pad "N" thru_hole circle
			(at 3.75 0 90)
			(size 1.4 1.4)
			(drill 1.05)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 303 "/GNDREF")
			(solder_mask_margin 0.102)
		)
		(pad "P" thru_hole rect
			(at -3.75 0 90)
			(size 1.4 1.4)
			(drill 1.05)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "/EPS_IN")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:TAJD_AVX"
		(layer "B.Cu")
		(at 52.13905 171.26195 -90)
		(tags "TAJD106K025RNJ ")
		(property "Reference" "C15"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "CP_SMD_Tantalum_AVX-N_7343"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "SMD Tantalum Electrolytic Capacitor, AVX-N, 7343, European Symbol, Alternate KiCad Library"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "CP_*")
		(sheetname "/DC-DC_Converters/")
		(sheetfile "DC-DC_Converters.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
		)
		(pad "1" smd rect
			(at -2.8829 0 180)
			(size 2.54 1.8796)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 5 "/DC_POS.12V")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 2.8829 0 180)
			(size 2.54 1.8796)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 303 "/GNDREF")
			(pintype "passive")
		)
		(zone
			(net 0)
			(net_name "")
			(layer "B.Cu")
			(hatch full 0.508)
			(connect_pads
				(clearance 0)
			)
			(min_thickness 0.254)
			(filled_areas_thickness no)
			(keepout
				(tracks not_allowed)
				(vias not_allowed)
				(pads allowed)
				(copperpour not_allowed)
				(footprints allowed)
			)
			(placement
				(enabled no)
				(sheetname "")
			)
			(fill
				(thermal_gap 0.508)
				(thermal_bridge_width 0.508)
			)
			(polygon
				(pts
					(xy 49.94195 167.56625) (xy 49.94195 174.95765) (xy 50.79285 174.95765) (xy 50.79285 167.56625)
				)
			)
		)
		(zone
			(net 0)
			(net_name "")
			(layer "B.Cu")
			(hatch full 0.508)
			(connect_pads
				(clearance 0)
			)
			(min_thickness 0.254)
			(filled_areas_thickness no)
			(keepout
				(tracks not_allowed)
				(vias not_allowed)
				(pads allowed)
				(copperpour not_allowed)
				(footprints allowed)
			)
			(placement
				(enabled no)
				(sheetname "")
			)
			(fill
				(thermal_gap 0.508)
				(thermal_bridge_width 0.508)
			)
			(polygon
				(pts
					(xy 50.79285 169.36965) (xy 50.79285 173.15425) (xy 53.48525 173.15425) (xy 53.48525 169.36965)
				)
			)
		)
		(zone
			(net 0)
			(net_name "")
			(layer "B.Cu")
			(hatch full 0.508)
			(connect_pads
				(clearance 0)
			)
			(min_thickness 0.254)
			(filled_areas_thickness no)
			(keepout
				(tracks not_allowed)
				(vias not_allowed)
				(pads allowed)
				(copperpour not_allowed)
				(footprints allowed)
			)
			(placement
				(enabled no)
				(sheetname "")
			)
			(fill
				(thermal_gap 0.508)
				(thermal_bridge_width 0.508)
			)
			(polygon
				(pts
					(xy 53.48525 167.56625) (xy 53.48525 174.95765) (xy 54.33615 174.95765) (xy 54.33615 167.56625)
				)
			)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:RESC1508X55N"
		(layer "B.Cu")
		(at 85.70905 138.54195 180)
		(property "Reference" "R6"
			(at -0.21 1.07 0)
			(layer "B.SilkS")
		)
		(property "Value" "0 Ohm"
			(at 1.54 -1.07 0)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MF" "Stackpole Electronics Inc"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description_1" "0 Ohms Jumper 0.1W, 1/10W Chip Resistor 0603 (1608 Metric) Automotive AEC-Q200 Thick Film"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Package" "1508 Stackpole"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Price" "None"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "SnapEDA_Link" "https://www.snapeda.com/parts/RMCF0603ZT0R00/Stackpole+Electronics/view-part/?ref=snap"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MP" "RMCF0603ZT0R00"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Purchase-URL" "https://www.snapeda.com/api/url_track_click_mouser/?unipart_id=3968849&manufacturer=Stackpole Electronics Inc&part_name=RMCF0603ZT0R00&search_term=rmcf0603zt0r00"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Availability" "In Stock"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Check_prices" "https://www.snapeda.com/parts/RMCF0603ZT0R00/Stackpole+Electronics/view-part/?ref=eda"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(sheetname "/DC-DC_Converters/")
		(sheetfile "DC-DC_Converters.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -0.76 0 180)
			(size 0.9 0.97)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 96 "Net-(U2-+S)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd rect
			(at 0.76 0 180)
			(size 0.9 0.97)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 5 "/DC_POS.12V")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:TE_796740-2"
		(layer "B.Cu")
		(at 208.46405 140.209694)
		(property "Reference" "J2"
			(at -0.03004 9.24952 0)
			(layer "B.SilkS")
		)
		(property "Value" "796740-2"
			(at 3.881995 -5.667885 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "https://www.te.com/commerce/DocumentDelivery/DDEController?Action=srchrtrv&DocNm=1-1773458-1_EURO_STYLE_QRG&DocType=Data+Sheet&DocLang=English&PartCntxt=796740-2&DocFormat=pdf"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "CONN2_796740-2_TEC")
		(sheetname "/")
		(sheetfile "PEEKbot_EPS.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.95 1.95)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "/EPS_IN")
			(pinfunction "1")
			(pintype "unspecified")
			(solder_mask_margin 0.102)
		)
		(pad "2" thru_hole circle
			(at 6.35 0)
			(size 1.95 1.95)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 303 "/GNDREF")
			(pinfunction "2")
			(pintype "unspecified")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:CAPC1608X95N"
		(layer "B.Cu")
		(at 67.70905 105.69195 -90)
		(property "Reference" "C11"
			(at -0.24 1.07 90)
			(layer "B.SilkS")
		)
		(property "Value" "C_0603"
			(at 1.51 -1.07 90)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "SMD 0603 MLCC capacitor, Alternate KiCad Library"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/DC-DC_Converters/")
		(sheetfile "DC-DC_Converters.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -0.763 0 270)
			(size 0.95 0.98)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 5 "/DC_POS.12V")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd rect
			(at 0.763 0 270)
			(size 0.95 0.98)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 303 "/GNDREF")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:RESC1508X55N"
		(layer "B.Cu")
		(at 188.69905 159.46195 180)
		(property "Reference" "R2"
			(at -0.21 1.07 0)
			(layer "B.SilkS")
		)
		(property "Value" "R_US"
			(at 1.54 -1.07 0)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/DC-DC_Converters/")
		(sheetfile "DC-DC_Converters.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -0.76 0 180)
			(size 0.9 0.97)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 1 "/EPS_IN")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd rect
			(at 0.76 0 180)
			(size 0.9 0.97)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 92 "Net-(U3-+On{slash}Off)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:TAJD_AVX"
		(layer "B.Cu")
		(at 52.20905 106.19195 -90)
		(tags "TAJD106K025RNJ ")
		(property "Reference" "C14"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "CP_SMD_Tantalum_AVX-N_7343"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "SMD Tantalum Electrolytic Capacitor, AVX-N, 7343, European Symbol, Alternate KiCad Library"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "CP_*")
		(sheetname "/DC-DC_Converters/")
		(sheetfile "DC-DC_Converters.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
		)
		(pad "1" smd rect
			(at -2.8829 0 180)
			(size 2.54 1.8796)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 5 "/DC_POS.12V")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 2.8829 0 180)
			(size 2.54 1.8796)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 303 "/GNDREF")
			(pintype "passive")
		)
		(zone
			(net 0)
			(net_name "")
			(layer "B.Cu")
			(hatch full 0.508)
			(connect_pads
				(clearance 0)
			)
			(min_thickness 0.254)
			(filled_areas_thickness no)
			(keepout
				(tracks not_allowed)
				(vias not_allowed)
				(pads allowed)
				(copperpour not_allowed)
				(footprints allowed)
			)
			(placement
				(enabled no)
				(sheetname "")
			)
			(fill
				(thermal_gap 0.508)
				(thermal_bridge_width 0.508)
			)
			(polygon
				(pts
					(xy 50.01195 102.49625) (xy 50.01195 109.88765) (xy 50.86285 109.88765) (xy 50.86285 102.49625)
				)
			)
		)
		(zone
			(net 0)
			(net_name "")
			(layer "B.Cu")
			(hatch full 0.508)
			(connect_pads
				(clearance 0)
			)
			(min_thickness 0.254)
			(filled_areas_thickness no)
			(keepout
				(tracks not_allowed)
				(vias not_allowed)
				(pads allowed)
				(copperpour not_allowed)
				(footprints allowed)
			)
			(placement
				(enabled no)
				(sheetname "")
			)
			(fill
				(thermal_gap 0.508)
				(thermal_bridge_width 0.508)
			)
			(polygon
				(pts
					(xy 50.86285 104.29965) (xy 50.86285 108.08425) (xy 53.55525 108.08425) (xy 53.55525 104.29965)
				)
			)
		)
		(zone
			(net 0)
			(net_name "")
			(layer "B.Cu")
			(hatch full 0.508)
			(connect_pads
				(clearance 0)
			)
			(min_thickness 0.254)
			(filled_areas_thickness no)
			(keepout
				(tracks not_allowed)
				(vias not_allowed)
				(pads allowed)
				(copperpour not_allowed)
				(footprints allowed)
			)
			(placement
				(enabled no)
				(sheetname "")
			)
			(fill
				(thermal_gap 0.508)
				(thermal_bridge_width 0.508)
			)
			(polygon
				(pts
					(xy 53.55525 102.49625) (xy 53.55525 109.88765) (xy 54.40615 109.88765) (xy 54.40615 102.49625)
				)
			)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:RESC1508X55N"
		(layer "B.Cu")
		(at 188.80825 94.24195 180)
		(property "Reference" "R1"
			(at -0.21 1.07 0)
			(layer "B.SilkS")
		)
		(property "Value" "R_US"
			(at 1.54 -1.07 0)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/DC-DC_Converters/")
		(sheetfile "DC-DC_Converters.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -0.76 0 180)
			(size 0.9 0.97)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 1 "/EPS_IN")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd rect
			(at 0.76 0 180)
			(size 0.9 0.97)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 91 "Net-(U2-+On{slash}Off)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:CAPC1608X90"
		(layer "B.Cu")
		(at 70.85905 233.79195 90)
		(descr "<b>CAPACITOR</b>")
		(property "Reference" "C13"
			(at -0.235423 -1.3008 90)
			(layer "B.SilkS")
		)
		(property "Value" "C_0603"
			(at 1.56646 -1.20613 90)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "SMD 0603 MLCC capacitor, Alternate KiCad Library"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/DC-DC_Converters/")
		(sheetfile "DC-DC_Converters.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -0.85 0 90)
			(size 1.1 1)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 6 "/DC_POS.9V")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd rect
			(at 0.85 0 90)
			(size 1.1 1)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 303 "/GNDREF")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:KAWS-12XXTEL"
		(layer "B.Cu")
		(at 102.61905 233.24195 180)
		(property "Reference" "U4"
			(at 0 0.5 0)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "KAWS-1209TEL"
			(at 0 -7.5 0)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Datasheet" "https://diwellshop.cafe24.com/web/DATASHEET/01_subtitle/4_POWER/2_DC-DC/KAW-EL/KAW-EL.pdf"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(sheetname "/DC-DC_Converters/")
		(sheetfile "DC-DC_Converters.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -9.5 0)
			(unlocked yes)
			(layer "B.Fab")
		)
		(pad "1" thru_hole circle
			(at -22.86 12.7 180)
			(size 2.1 2.1)
			(drill 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 224 "unconnected-(U4-Remote_On{slash}Off-Pad1)")
			(pinfunction "Remote_On/Off")
			(pintype "input+no_connect")
		)
		(pad "3" thru_hole circle
			(at -22.86 2.54 180)
			(size 2.1 2.1)
			(drill 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 70 "Net-(U4--Vin)")
			(pinfunction "-Vin")
			(pintype "input")
		)
		(pad "4" thru_hole circle
			(at -22.86 -2.54 180)
			(size 2.1 2.1)
			(drill 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 71 "Net-(U4-+Vin)")
			(pinfunction "+Vin")
			(pintype "input")
		)
		(pad "5" thru_hole circle
			(at 22.86 -15.24 180)
			(size 2.1 2.1)
			(drill 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 223 "unconnected-(U4-NO_PIN-Pad5)")
			(pinfunction "NO_PIN")
			(pintype "input+no_connect")
		)
		(pad "6" thru_hole circle
			(at 22.86 -5.08 180)
			(size 2.1 2.1)
			(drill 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "/DC_POS.9V")
			(pinfunction "+Vout")
			(pintype "output")
		)
		(pad "7" thru_hole circle
			(at 22.86 5.08 180)
			(size 2.1 2.1)
			(drill 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 303 "/GNDREF")
			(pinfunction "-Vout")
			(pintype "output")
		)
		(pad "8" thru_hole circle
			(at 22.86 15.24 180)
			(size 2.1 2.1)
			(drill 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 222 "unconnected-(U4-TRIM-Pad8)")
			(pinfunction "TRIM")
			(pintype "output+no_connect")
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:CAPC1608X90"
		(layer "B.Cu")
		(at 244.55905 188.79195)
		(descr "<b>CAPACITOR</b>")
		(property "Reference" "C43"
			(at 2.7492 0 0)
			(layer "B.SilkS")
		)
		(property "Value" "0.1uF"
			(at 1.56646 -1.20613 0)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "SMD 0603 MLCC capacitor, Alternate KiCad Library"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/Digital Systems/")
		(sheetfile "Digital_Systems.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -0.85 0)
			(size 1.1 1)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 35 "/Digital Systems/3.3V+")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd rect
			(at 0.85 0)
			(size 1.1 1)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 303 "/GNDREF")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:CAPC1608X95N"
		(layer "B.Cu")
		(at 67.78905 171.07495 -90)
		(property "Reference" "C12"
			(at -0.24 1.07 90)
			(layer "B.SilkS")
		)
		(property "Value" "C_0603"
			(at 1.51 -1.07 90)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "SMD 0603 MLCC capacitor, Alternate KiCad Library"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/DC-DC_Converters/")
		(sheetfile "DC-DC_Converters.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -0.763 0 270)
			(size 0.95 0.98)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 5 "/DC_POS.12V")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd rect
			(at 0.763 0 270)
			(size 0.95 0.98)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 303 "/GNDREF")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:CAPC1608X90"
		(layer "B.Cu")
		(at 244.55905 186.94155)
		(descr "<b>CAPACITOR</b>")
		(property "Reference" "C44"
			(at 2.4992 0.1004 0)
			(layer "B.SilkS")
		)
		(property "Value" "0.1uF"
			(at 1.56646 -1.20613 0)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "SMD 0603 MLCC capacitor, Alternate KiCad Library"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/Digital Systems/")
		(sheetfile "Digital_Systems.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -0.85 0)
			(size 1.1 1)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 35 "/Digital Systems/3.3V+")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd rect
			(at 0.85 0)
			(size 1.1 1)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 303 "/GNDREF")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:CONV_CFB400W-24S12"
		(layer "B.Cu")
		(at 128.38905 171.12195 180)
		(property "Reference" "U3"
			(at -54.675 31.585 0)
			(layer "B.SilkS")
		)
		(property "Value" "CFB400W-24S12"
			(at -47.22 -32.385 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "https://www.cincon.com/productdownload/Datasheet-CFB400W.pdf"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(sheetname "/DC-DC_Converters/")
		(sheetfile "DC-DC_Converters.kicad_sch")
		(attr through_hole)
		(pad "" np_thru_hole circle
			(at -53.35 -25.4 180)
			(size 3.5 3.5)
			(drill 3.5)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at -53.35 25.4 180)
			(size 3.5 3.5)
			(drill 3.5)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 53.35 -25.4 180)
			(size 3.5 3.5)
			(drill 3.5)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 53.35 25.4 180)
			(size 3.5 3.5)
			(drill 3.5)
			(layers "*.Cu" "*.Mask")
		)
		(pad "1" thru_hole rect
			(at -53.35 -12.7 180)
			(size 4.8 4.8)
			(drill 2.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 303 "/GNDREF")
			(pinfunction "-VIn")
			(pintype "input")
			(solder_mask_margin 0.102)
		)
		(pad "2" thru_hole circle
			(at -53.35 -2.54 180)
			(size 4.8 4.8)
			(drill 2.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "/EPS_IN")
			(pinfunction "+Vin")
			(pintype "input")
			(solder_mask_margin 0.102)
		)
		(pad "3" thru_hole circle
			(at -53.35 7.62 180)
			(size 2.8 2.8)
			(drill 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 303 "/GNDREF")
			(pinfunction "-On/Off")
			(pintype "input")
			(solder_mask_margin 0.102)
		)
		(pad "4" thru_hole circle
			(at -53.35 11.43 180)
			(size 2.8 2.8)
			(drill 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 92 "Net-(U3-+On{slash}Off)")
			(pinfunction "+On/Off")
			(pintype "input")
			(solder_mask_margin 0.102)
		)
		(pad "5" thru_hole circle
			(at 53.35 17.78 180)
			(size 4.8 4.8)
			(drill 2.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "/DC_POS.12V")
			(pinfunction "+Vout")
			(pintype "output")
			(solder_mask_margin 0.102)
		)
		(pad "6" thru_hole circle
			(at 53.35 11.43 180)
			(size 4.8 4.8)
			(drill 2.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "/DC_POS.12V")
			(pinfunction "+Vout")
			(pintype "output")
			(solder_mask_margin 0.102)
		)
		(pad "7" thru_hole circle
			(at 53.35 5.08 180)
			(size 4.8 4.8)
			(drill 2.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "/DC_POS.12V")
			(pinfunction "+Vout")
			(pintype "output")
			(solder_mask_margin 0.102)
		)
		(pad "8" thru_hole circle
			(at 53.35 -5.08 180)
			(size 4.8 4.8)
			(drill 2.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 303 "/GNDREF")
			(pinfunction "-Vout")
			(pintype "output")
			(solder_mask_margin 0.102)
		)
		(pad "9" thru_hole circle
			(at 53.35 -11.43 180)
			(size 4.8 4.8)
			(drill 2.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 303 "/GNDREF")
			(pinfunction "-Vout")
			(pintype "output")
			(solder_mask_margin 0.102)
		)
		(pad "10" thru_hole circle
			(at 53.35 -17.78 180)
			(size 4.8 4.8)
			(drill 2.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 303 "/GNDREF")
			(solder_mask_margin 0.102)
		)
		(pad "11" thru_hole circle
			(at 45.71 -26.67 180)
			(size 2.8 2.8)
			(drill 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 93 "Net-(U3--S)")
			(pinfunction "-S")
			(pintype "input")
			(solder_mask_margin 0.102)
		)
		(pad "12" thru_hole circle
			(at 41.9 -26.67 180)
			(size 2.8 2.8)
			(drill 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 94 "Net-(U3-+S)")
			(pinfunction "+S")
			(pintype "input")
			(solder_mask_margin 0.102)
		)
		(pad "13" thru_hole circle
			(at 38.09 -26.67 180)
			(size 2.8 2.8)
			(drill 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 221 "unconnected-(U3-TRIM-Pad13)")
			(pinfunction "TRIM")
			(pintype "input+no_connect")
			(solder_mask_margin 0.102)
		)
		(pad "14" thru_hole circle
			(at 34.28 -26.67 180)
			(size 2.8 2.8)
			(drill 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 99 "Net-(U3-PC{slash}NC)")
			(pinfunction "PC/NC")
			(pintype "input")
			(solder_mask_margin 0.102)
		)
		(pad "15" thru_hole circle
			(at 30.47 -26.67 180)
			(size 2.8 2.8)
			(drill 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 220 "unconnected-(U3-IOG-Pad15)")
			(pinfunction "IOG")
			(pintype "input+no_connect")
			(solder_mask_margin 0.102)
		)
		(pad "16" thru_hole circle
			(at 26.66 -26.67 180)
			(size 2.8 2.8)
			(drill 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 219 "unconnected-(U3-AUX-Pad16)")
			(pinfunction "AUX")
			(pintype "input+no_connect")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:RESC1508X55N"
		(layer "B.Cu")
		(at 94.10905 137.54195)
		(property "Reference" "R7"
			(at -0.21 1.07 0)
			(layer "B.SilkS")
		)
		(property "Value" "0 Ohm"
			(at 1.54 -1.07 0)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MF" "Stackpole Electronics Inc"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description_1" "0 Ohms Jumper 0.1W, 1/10W Chip Resistor 0603 (1608 Metric) Automotive AEC-Q200 Thick Film"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Package" "1508 Stackpole"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Price" "None"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "SnapEDA_Link" "https://www.snapeda.com/parts/RMCF0603ZT0R00/Stackpole+Electronics/view-part/?ref=snap"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MP" "RMCF0603ZT0R00"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Purchase-URL" "https://www.snapeda.com/api/url_track_click_mouser/?unipart_id=3968849&manufacturer=Stackpole Electronics Inc&part_name=RMCF0603ZT0R00&search_term=rmcf0603zt0r00"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Availability" "In Stock"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Check_prices" "https://www.snapeda.com/parts/RMCF0603ZT0R00/Stackpole+Electronics/view-part/?ref=eda"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(sheetname "/DC-DC_Converters/")
		(sheetfile "DC-DC_Converters.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -0.76 0)
			(size 0.9 0.97)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 97 "Net-(U2-PC{slash}NC)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd rect
			(at 0.76 0)
			(size 0.9 0.97)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 98 "Net-(R7-Pad2)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:WE-SI_7441501"
		(layer "B.Cu")
		(at 251.22905 146.14195 90)
		(property "Reference" "L2"
			(at 0.08 15.875 90)
			(layer "B.SilkS")
		)
		(property "Value" "L"
			(at 4.285 -15.625 90)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Inductor"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Choke_* *Coil* Inductor_* L_*")
		(sheetname "/DC-DC_Converters/")
		(sheetfile "DC-DC_Converters.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole circle
			(at -6 0 90)
			(size 2.1 2.1)
			(drill 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "/EPS_IN")
			(pinfunction "1")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" thru_hole circle
			(at 6 0 90)
			(size 2.1 2.1)
			(drill 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "Net-(PS1-+V_INPUT)")
			(pinfunction "2")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:CAPC1608X90"
		(layer "B.Cu")
		(at 244.55905 185.04195)
		(descr "<b>CAPACITOR</b>")
		(property "Reference" "C45"
			(at 2.7492 0.25 0)
			(layer "B.SilkS")
		)
		(property "Value" "0.1uF"
			(at 1.56646 -1.20613 0)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "SMD 0603 MLCC capacitor, Alternate KiCad Library"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/Digital Systems/")
		(sheetfile "Digital_Systems.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -0.85 0)
			(size 1.1 1)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 35 "/Digital Systems/3.3V+")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd rect
			(at 0.85 0)
			(size 1.1 1)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 303 "/GNDREF")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:CONV_CFB400W-24S12"
		(layer "B.Cu")
		(at 128.35905 105.79195 180)
		(property "Reference" "U2"
			(at -55.475 32.385 0)
			(layer "B.SilkS")
		)
		(property "Value" "CFB400W-24S12"
			(at -47.22 -32.385 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "https://www.cincon.com/productdownload/Datasheet-CFB400W.pdf"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(sheetname "/DC-DC_Converters/")
		(sheetfile "DC-DC_Converters.kicad_sch")
		(attr through_hole)
		(pad "" np_thru_hole circle
			(at -53.35 -25.4 180)
			(size 3.5 3.5)
			(drill 3.5)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at -53.35 25.4 180)
			(size 3.5 3.5)
			(drill 3.5)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 53.35 -25.4 180)
			(size 3.5 3.5)
			(drill 3.5)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 53.35 25.4 180)
			(size 3.5 3.5)
			(drill 3.5)
			(layers "*.Cu" "*.Mask")
		)
		(pad "1" thru_hole rect
			(at -53.35 -12.7 180)
			(size 4.8 4.8)
			(drill 2.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 303 "/GNDREF")
			(pinfunction "-VIn")
			(pintype "input")
			(solder_mask_margin 0.102)
		)
		(pad "2" thru_hole circle
			(at -53.35 -2.54 180)
			(size 4.8 4.8)
			(drill 2.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "/EPS_IN")
			(pinfunction "+Vin")
			(pintype "input")
			(solder_mask_margin 0.102)
		)
		(pad "3" thru_hole circle
			(at -53.35 7.62 180)
			(size 2.8 2.8)
			(drill 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 303 "/GNDREF")
			(pinfunction "-On/Off")
			(pintype "input")
			(solder_mask_margin 0.102)
		)
		(pad "4" thru_hole circle
			(at -53.35 11.43 180)
			(size 2.8 2.8)
			(drill 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 91 "Net-(U2-+On{slash}Off)")
			(pinfunction "+On/Off")
			(pintype "input")
			(solder_mask_margin 0.102)
		)
		(pad "5" thru_hole circle
			(at 53.35 17.78 180)
			(size 4.8 4.8)
			(drill 2.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "/DC_POS.12V")
			(pinfunction "+Vout")
			(pintype "output")
			(solder_mask_margin 0.102)
		)
		(pad "6" thru_hole circle
			(at 53.35 11.43 180)
			(size 4.8 4.8)
			(drill 2.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "/DC_POS.12V")
			(pinfunction "+Vout")
			(pintype "output")
			(solder_mask_margin 0.102)
		)
		(pad "7" thru_hole circle
			(at 53.35 5.08 180)
			(size 4.8 4.8)
			(drill 2.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "/DC_POS.12V")
			(pinfunction "+Vout")
			(pintype "output")
			(solder_mask_margin 0.102)
		)
		(pad "8" thru_hole circle
			(at 53.35 -5.08 180)
			(size 4.8 4.8)
			(drill 2.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 303 "/GNDREF")
			(pinfunction "-Vout")
			(pintype "output")
			(solder_mask_margin 0.102)
		)
		(pad "9" thru_hole circle
			(at 53.35 -11.43 180)
			(size 4.8 4.8)
			(drill 2.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 303 "/GNDREF")
			(pinfunction "-Vout")
			(pintype "output")
			(solder_mask_margin 0.102)
		)
		(pad "10" thru_hole circle
			(at 53.35 -17.78 180)
			(size 4.8 4.8)
			(drill 2.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 303 "/GNDREF")
			(solder_mask_margin 0.102)
		)
		(pad "11" thru_hole circle
			(at 45.71 -26.67 180)
			(size 2.8 2.8)
			(drill 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 95 "Net-(U2--S)")
			(pinfunction "-S")
			(pintype "input")
			(solder_mask_margin 0.102)
		)
		(pad "12" thru_hole circle
			(at 41.9 -26.67 180)
			(size 2.8 2.8)
			(drill 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 96 "Net-(U2-+S)")
			(pinfunction "+S")
			(pintype "input")
			(solder_mask_margin 0.102)
		)
		(pad "13" thru_hole circle
			(at 38.09 -26.67 180)
			(size 2.8 2.8)
			(drill 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 218 "unconnected-(U2-TRIM-Pad13)")
			(pinfunction "TRIM")
			(pintype "input+no_connect")
			(solder_mask_margin 0.102)
		)
		(pad "14" thru_hole circle
			(at 34.28 -26.67 180)
			(size 2.8 2.8)
			(drill 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 97 "Net-(U2-PC{slash}NC)")
			(pinfunction "PC/NC")
			(pintype "input")
			(solder_mask_margin 0.102)
		)
		(pad "15" thru_hole circle
			(at 30.47 -26.67 180)
			(size 2.8 2.8)
			(drill 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 217 "unconnected-(U2-IOG-Pad15)")
			(pinfunction "IOG")
			(pintype "input+no_connect")
			(solder_mask_margin 0.102)
		)
		(pad "16" thru_hole circle
			(at 26.66 -26.67 180)
			(size 2.8 2.8)
			(drill 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 216 "unconnected-(U2-AUX-Pad16)")
			(pinfunction "AUX")
			(pintype "input+no_connect")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:TE_796740-2"
		(layer "B.Cu")
		(at 214.75405 129.19195 180)
		(property "Reference" "J1"
			(at -0.03004 9.24952 0)
			(layer "B.SilkS")
		)
		(property "Value" "796740-2"
			(at 3.881995 -5.667885 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "https://www.te.com/commerce/DocumentDelivery/DDEController?Action=srchrtrv&DocNm=1-1773458-1_EURO_STYLE_QRG&DocType=Data+Sheet&DocLang=English&PartCntxt=796740-2&DocFormat=pdf"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "CONN2_796740-2_TEC")
		(sheetname "/")
		(sheetfile "PEEKbot_EPS.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole rect
			(at 0 0 180)
			(size 1.95 1.95)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "/EPS_IN")
			(pinfunction "1")
			(pintype "unspecified")
			(solder_mask_margin 0.102)
		)
		(pad "2" thru_hole circle
			(at 6.35 0 180)
			(size 1.95 1.95)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 303 "/GNDREF")
			(pinfunction "2")
			(pintype "unspecified")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:CAP_NTF_55_2.8T_NIP"
		(layer "B.Cu")
		(at 168.46845 211.93925 90)
		(tags "KTF500B106M55NHT00 ")
		(property "Reference" "C4"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "KTF500B106M55NHT00"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Datasheet" "KTF500B106M55NHT00"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "CAP_NTF_55_2.8T_NIP CAP_NTF_55_2.8T_NIP-M CAP_NTF_55_2.8T_NIP-L")
		(sheetname "/DC-DC_Converters/")
		(sheetfile "DC-DC_Converters.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
		)
		(pad "1" smd rect
			(at -2.5273 0 90)
			(size 1.7526 5.4102)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 2 "Net-(C2-Pad1)")
			(pintype "unspecified")
		)
		(pad "2" smd rect
			(at 2.5273 0 90)
			(size 1.7526 5.4102)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 303 "/GNDREF")
			(pintype "unspecified")
		)
		(zone
			(net 0)
			(net_name "")
			(layer "B.Cu")
			(hatch full 0.508)
			(connect_pads
				(clearance 0)
			)
			(min_thickness 0.254)
			(filled_areas_thickness no)
			(keepout
				(tracks not_allowed)
				(vias not_allowed)
				(pads allowed)
				(copperpour not_allowed)
				(footprints allowed)
			)
			(placement
				(enabled no)
				(sheetname "")
			)
			(fill
				(thermal_gap 0.508)
				(thermal_bridge_width 0.508)
			)
			(polygon
				(pts
					(xy 171.12275 213.53945) (xy 171.12275 210.33905) (xy 165.81415 210.33905) (xy 165.81415 213.53945)
				)
			)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:CONV_CQB150W-24S05"
		(layer "B.Cu")
		(at 246.72905 102.89195 90)
		(property "Reference" "PS1"
			(at -25.825 19.385 90)
			(layer "B.SilkS")
		)
		(property "Value" "CQB150W-24S05"
			(at -17.57 -19.365 90)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "DigiKey_Part_Number" "2034-2828-ND"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "SnapEDA_Link" "https://www.snapeda.com/parts/CQB150W-24S05/Cincon/view-part/?ref=snap"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MAXIMUM_PACKAGE_HEIGHT" "13.2mm"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Package" "None"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Check_prices" "https://www.snapeda.com/parts/CQB150W-24S05/Cincon/view-part/?ref=eda"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "STANDARD" "Manufacturer Recommendations"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "PARTREV" "V17"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MF" "Cincon Electronics Co. LTD"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MP" "CQB150W-24S05"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description_1" "Isolated Module DC DC Converter 1 Output 5V 30A 9V - 36V Input"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MANUFACTURER" "Cincon"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(sheetname "/DC-DC_Converters/")
		(sheetfile "DC-DC_Converters.kicad_sch")
		(attr through_hole)
		(pad "" np_thru_hole circle
			(at -23.6 13.075 90)
			(size 3.5 3.5)
			(drill 3.5)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 23.6 -13.075 90)
			(size 3.5 3.5)
			(drill 3.5)
			(layers "*.Cu" "*.Mask")
		)
		(pad "1" thru_hole rect
			(at -25.4 7.62 90)
			(size 2.5 2.5)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "Net-(PS1-+V_INPUT)")
			(pinfunction "+V_INPUT")
			(pintype "input")
			(solder_mask_margin 0.102)
		)
		(pad "2" thru_hole circle
			(at -25.4 0 90)
			(size 2.5 2.5)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 90 "unconnected-(PS1-ON{slash}OFF-Pad2)")
			(pinfunction "ON/OFF")
			(pintype "input+no_connect")
			(solder_mask_margin 0.102)
		)
		(pad "3" thru_hole circle
			(at -25.4 -7.62 90)
			(size 2.5 2.5)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 303 "/GNDREF")
			(pinfunction "-V_INPUT")
			(pintype "input")
			(solder_mask_margin 0.102)
		)
		(pad "4" thru_hole circle
			(at 25.4 -7.62 90)
			(size 3.3 3.3)
			(drill 1.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 303 "/GNDREF")
			(pinfunction "-V_OUTPUT")
			(pintype "output")
			(solder_mask_margin 0.102)
		)
		(pad "5" thru_hole circle
			(at 25.4 -3.81 90)
			(size 2.5 2.5)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 303 "/GNDREF")
			(pinfunction "-SENSE")
			(pintype "input")
			(solder_mask_margin 0.102)
		)
		(pad "6" thru_hole circle
			(at 25.4 0 90)
			(size 2.5 2.5)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 303 "/GNDREF")
			(pinfunction "TRIM")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "7" thru_hole circle
			(at 25.4 3.81 90)
			(size 2.5 2.5)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "/DC_POS.5V")
			(pinfunction "+SENSE")
			(pintype "input")
			(solder_mask_margin 0.102)
		)
		(pad "8" thru_hole circle
			(at 25.4 7.62 90)
			(size 3.3 3.3)
			(drill 1.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "/DC_POS.5V")
			(pinfunction "+V_OUTPUT")
			(pintype "output")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:RESC1508X55N"
		(layer "B.Cu")
		(at 81.70905 137.69195 180)
		(property "Reference" "R5"
			(at 0.1508 -1.35 0)
			(layer "B.SilkS")
		)
		(property "Value" "0 Ohm"
			(at 1.54 -1.07 0)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MF" "Stackpole Electronics Inc"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description_1" "0 Ohms Jumper 0.1W, 1/10W Chip Resistor 0603 (1608 Metric) Automotive AEC-Q200 Thick Film"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Package" "1508 Stackpole"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Price" "None"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "SnapEDA_Link" "https://www.snapeda.com/parts/RMCF0603ZT0R00/Stackpole+Electronics/view-part/?ref=snap"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MP" "RMCF0603ZT0R00"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Purchase-URL" "https://www.snapeda.com/api/url_track_click_mouser/?unipart_id=3968849&manufacturer=Stackpole Electronics Inc&part_name=RMCF0603ZT0R00&search_term=rmcf0603zt0r00"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Availability" "In Stock"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Check_prices" "https://www.snapeda.com/parts/RMCF0603ZT0R00/Stackpole+Electronics/view-part/?ref=eda"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(sheetname "/DC-DC_Converters/")
		(sheetfile "DC-DC_Converters.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -0.76 0 180)
			(size 0.9 0.97)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 95 "Net-(U2--S)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd rect
			(at 0.76 0 180)
			(size 0.9 0.97)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 303 "/GNDREF")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:FIL_BNX002-11"
		(layer "B.Cu")
		(at 136.35905 234.24195 180)
		(property "Reference" "FL1"
			(at -2.325 7.135 0)
			(layer "B.SilkS")
		)
		(property "Value" "BNX002-11"
			(at 1.485 -7.135 0)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "PARTREV" "N/A"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "STANDARD" "Manufacturer Recommendations"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MAXIMUM_PACKAGE_HEIGHT" "12.5 mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MANUFACTURER" "Murata Electronics"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(sheetname "/DC-DC_Converters/")
		(sheetfile "DC-DC_Converters.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole rect
			(at 2.5 2.5 180)
			(size 1.8 1.8)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "/EPS_IN")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" thru_hole circle
			(at 2.5 -2.5 180)
			(size 1.8 1.8)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 71 "Net-(U4-+Vin)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "3" thru_hole circle
			(at -2.5 2.5 180)
			(size 1.8 1.8)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 303 "/GNDREF")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "4_1" thru_hole circle
			(at -2.5 -2.5 180)
			(size 1.8 1.8)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 70 "Net-(U4--Vin)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "4_2" thru_hole circle
			(at 0 0 180)
			(size 1.8 1.8)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 70 "Net-(U4--Vin)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "4_3" thru_hole circle
			(at 5 0 180)
			(size 1.8 1.8)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 70 "Net-(U4--Vin)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:RL622_Series"
		(layer "B.Cu")
		(at 185.46845 218.93925 180)
		(tags "RL622-3R3K-RC ")
		(property "Reference" "L1"
			(at -2.0898 -2.8527 0)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "L"
			(at 2.5 0 0)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Inductor"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Choke_* *Coil* Inductor_* L_*")
		(sheetname "/DC-DC_Converters/")
		(sheetfile "DC-DC_Converters.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 2.5 0 0)
			(unlocked yes)
			(layer "B.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 180)
			(size 1.3716 1.3716)
			(drill 0.8636)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "/EPS_IN")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 5 0 180)
			(size 1.3716 1.3716)
			(drill 0.8636)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "Net-(C2-Pad1)")
			(pinfunction "2")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:DIP_RSDW08_MWU"
		(layer "B.Cu")
		(at 175.75905 234.28195 90)
		(tags "RSDW08F-12 ")
		(property "Reference" "U1"
			(at 7.62 -13.97 270)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "RSDW08F-03"
			(at 7.62 -13.97 270)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Datasheet" "https://www.meanwellusa.com/upload/pdf/RDDW08/RSDW08,RDDW08-spec.pdf"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(sheetname "/DC-DC_Converters/")
		(sheetfile "DC-DC_Converters.kicad_sch")
		(attr through_hole)
		(fp_text user "*"
			(at 1.74 -2.7008 270)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(fp_text user "*"
			(at 1.74 -1.2008 90)
			(layer "B.SilkS")
		)
		(fp_text user "*"
			(at 0 1.693334 270)
			(unlocked yes)
			(layer "B.Fab")
		)
		(fp_text user "*"
			(at 0 1.693334 90)
			(layer "B.Fab")
		)
		(fp_text user "${REFERENCE}"
			(at 7.62 -13.97 270)
			(unlocked yes)
			(layer "B.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 90)
			(size 1.27 1.27)
			(drill 0.762)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 215 "unconnected-(U1-Remote_ON{slash}OFF-Pad1)")
			(pinfunction "Remote_ON/OFF")
			(pintype "input+no_connect")
		)
		(pad "2" thru_hole circle
			(at 0 -2.54 90)
			(size 1.27 1.27)
			(drill 0.762)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 303 "/GNDREF")
			(pinfunction "-Vin")
			(pintype "input")
		)
		(pad "3" thru_hole circle
			(at 0 -5.08 90)
			(size 1.27 1.27)
			(drill 0.762)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 303 "/GNDREF")
			(pinfunction "-Vin")
			(pintype "input")
		)
		(pad "11" thru_hole circle
			(at 0 -25.4 90)
			(size 1.27 1.27)
			(drill 0.762)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 214 "unconnected-(U1-N.C.-Pad11)")
			(pinfunction "N.C.")
			(pintype "input+no_connect")
		)
		(pad "14" thru_hole circle
			(at 15.24 -25.4 90)
			(size 1.27 1.27)
			(drill 0.762)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 72 "/DC_POS.3.3V")
			(pinfunction "+Vout")
			(pintype "output")
		)
		(pad "16" thru_hole circle
			(at 15.24 -20.32 90)
			(size 1.27 1.27)
			(drill 0.762)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 303 "/GNDREF")
			(pinfunction "-Vout")
			(pintype "output")
		)
		(pad "22" thru_hole circle
			(at 15.24 -5.08 90)
			(size 1.27 1.27)
			(drill 0.762)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "Net-(C2-Pad1)")
			(pinfunction "+Vin")
			(pintype "input")
		)
		(pad "23" thru_hole circle
			(at 15.24 -2.54 90)
			(size 1.27 1.27)
			(drill 0.762)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "Net-(C2-Pad1)")
			(pinfunction "+Vin")
			(pintype "input")
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:CAP_NTF_55_2.8T_NIP"
		(layer "B.Cu")
		(at 181.85905 230.56925 90)
		(tags "KTF500B106M55NHT00 ")
		(property "Reference" "C6"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "KTF500B106M55NHT00"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Datasheet" "KTF500B106M55NHT00"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "CAP_NTF_55_2.8T_NIP CAP_NTF_55_2.8T_NIP-M CAP_NTF_55_2.8T_NIP-L")
		(sheetname "/DC-DC_Converters/")
		(sheetfile "DC-DC_Converters.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
		)
		(pad "1" smd rect
			(at -2.5273 0 90)
			(size 1.7526 5.4102)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 303 "/GNDREF")
			(pintype "unspecified")
		)
		(pad "2" smd rect
			(at 2.5273 0 90)
			(size 1.7526 5.4102)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 303 "/GNDREF")
			(pintype "unspecified")
		)
		(zone
			(net 0)
			(net_name "")
			(layer "B.Cu")
			(hatch full 0.508)
			(connect_pads
				(clearance 0)
			)
			(min_thickness 0.254)
			(filled_areas_thickness no)
			(keepout
				(tracks not_allowed)
				(vias not_allowed)
				(pads allowed)
				(copperpour not_allowed)
				(footprints allowed)
			)
			(placement
				(enabled no)
				(sheetname "")
			)
			(fill
				(thermal_gap 0.508)
				(thermal_bridge_width 0.508)
			)
			(polygon
				(pts
					(xy 184.51335 232.16945) (xy 184.51335 228.96905) (xy 179.20475 228.96905) (xy 179.20475 232.16945)
				)
			)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:CAPPRD500W60D1000H1600"
		(layer "B.Cu")
		(at 60.73905 170.99945 -90)
		(property "Reference" "C17"
			(at 2.5425 5.4308 90)
			(layer "B.SilkS")
		)
		(property "Value" "CP_SMD_Tantalum_AVX-N_7343"
			(at 11.345 -6.315 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "SMD Tantalum Electrolytic Capacitor, AVX-N, 7343, European Symbol, Alternate KiCad Library"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "CP_*")
		(sheetname "/DC-DC_Converters/")
		(sheetfile "DC-DC_Converters.kicad_sch")
		(attr through_hole)
		(pad "N" thru_hole circle
			(at 2.5 0 270)
			(size 1.2 1.2)
			(drill 0.85)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 303 "/GNDREF")
			(solder_mask_margin 0.102)
		)
		(pad "P" thru_hole rect
			(at -2.5 0 270)
			(size 1.2 1.2)
			(drill 0.85)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "/DC_POS.12V")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:CAPPRD750W80D1800H3550"
		(layer "B.Cu")
		(at 200.33905 168.41195 90)
		(property "Reference" "C10"
			(at -1.45 10.335 90)
			(layer "B.SilkS")
		)
		(property "Value" "CP_SMD_Tantalum_AVX-N_7343"
			(at 9.345 -10.315 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "SMD Tantalum Electrolytic Capacitor, AVX-N, 7343, European Symbol, Alternate KiCad Library"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "CP_*")
		(sheetname "/DC-DC_Converters/")
		(sheetfile "DC-DC_Converters.kicad_sch")
		(attr through_hole)
		(pad "N" thru_hole circle
			(at 3.75 0 90)
			(size 1.4 1.4)
			(drill 1.05)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 303 "/GNDREF")
			(solder_mask_margin 0.102)
		)
		(pad "P" thru_hole rect
			(at -3.75 0 90)
			(size 1.4 1.4)
			(drill 1.05)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "/EPS_IN")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:CAPC1608X90"
		(layer "B.Cu")
		(at 244.55905 190.79195)
		(descr "<b>CAPACITOR</b>")
		(property "Reference" "C42"
			(at 2.4992 0 0)
			(layer "B.SilkS")
		)
		(property "Value" "0.1uF"
			(at 1.56646 -1.20613 0)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "SMD 0603 MLCC capacitor, Alternate KiCad Library"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/Digital Systems/")
		(sheetfile "Digital_Systems.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -0.85 0)
			(size 1.1 1)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 35 "/Digital Systems/3.3V+")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd rect
			(at 0.85 0)
			(size 1.1 1)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 303 "/GNDREF")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:TAJD_AVX"
		(layer "B.Cu")
		(at 74.35905 233.54195 90)
		(tags "TAJD106K025RNJ ")
		(property "Reference" "C18"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "CP_SMD_Tantalum_AVX-N_7343"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "SMD Tantalum Electrolytic Capacitor, AVX-N, 7343, European Symbol, Alternate KiCad Library"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "CP_*")
		(sheetname "/DC-DC_Converters/")
		(sheetfile "DC-DC_Converters.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
		)
		(pad "1" smd rect
			(at -2.8829 0)
			(size 2.54 1.8796)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 6 "/DC_POS.9V")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 2.8829 0)
			(size 2.54 1.8796)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 303 "/GNDREF")
			(pintype "passive")
		)
		(zone
			(net 0)
			(net_name "")
			(layer "B.Cu")
			(hatch full 0.508)
			(connect_pads
				(clearance 0)
			)
			(min_thickness 0.254)
			(filled_areas_thickness no)
			(keepout
				(tracks not_allowed)
				(vias not_allowed)
				(pads allowed)
				(copperpour not_allowed)
				(footprints allowed)
			)
			(placement
				(enabled no)
				(sheetname "")
			)
			(fill
				(thermal_gap 0.508)
				(thermal_bridge_width 0.508)
			)
			(polygon
				(pts
					(xy 73.01285 237.23765) (xy 73.01285 229.84625) (xy 72.16195 229.84625) (xy 72.16195 237.23765)
				)
			)
		)
		(zone
			(net 0)
			(net_name "")
			(layer "B.Cu")
			(hatch full 0.508)
			(connect_pads
				(clearance 0)
			)
			(min_thickness 0.254)
			(filled_areas_thickness no)
			(keepout
				(tracks not_allowed)
				(vias not_allowed)
				(pads allowed)
				(copperpour not_allowed)
				(footprints allowed)
			)
			(placement
				(enabled no)
				(sheetname "")
			)
			(fill
				(thermal_gap 0.508)
				(thermal_bridge_width 0.508)
			)
			(polygon
				(pts
					(xy 75.70525 235.43425) (xy 75.70525 231.64965) (xy 73.01285 231.64965) (xy 73.01285 235.43425)
				)
			)
		)
		(zone
			(net 0)
			(net_name "")
			(layer "B.Cu")
			(hatch full 0.508)
			(connect_pads
				(clearance 0)
			)
			(min_thickness 0.254)
			(filled_areas_thickness no)
			(keepout
				(tracks not_allowed)
				(vias not_allowed)
				(pads allowed)
				(copperpour not_allowed)
				(footprints allowed)
			)
			(placement
				(enabled no)
				(sheetname "")
			)
			(fill
				(thermal_gap 0.508)
				(thermal_bridge_width 0.508)
			)
			(polygon
				(pts
					(xy 76.55615 237.23765) (xy 76.55615 229.84625) (xy 75.70525 229.84625) (xy 75.70525 237.23765)
				)
			)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:CAP_NTF_55_2.8T_NIP"
		(layer "B.Cu")
		(at 182.94115 210.93925 180)
		(tags "KTF500B106M55NHT00 ")
		(property "Reference" "C1"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "KTF500B106M55NHT00"
			(at 0.38 -1.1406 0)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Datasheet" "KTF500B106M55NHT00"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "CAP_NTF_55_2.8T_NIP CAP_NTF_55_2.8T_NIP-M CAP_NTF_55_2.8T_NIP-L")
		(sheetname "/DC-DC_Converters/")
		(sheetfile "DC-DC_Converters.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
		)
		(pad "1" smd rect
			(at -2.5273 0 180)
			(size 1.7526 5.4102)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 1 "/EPS_IN")
			(pintype "unspecified")
		)
		(pad "2" smd rect
			(at 2.5273 0 180)
			(size 1.7526 5.4102)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 303 "/GNDREF")
			(pintype "unspecified")
		)
		(zone
			(net 0)
			(net_name "")
			(layer "B.Cu")
			(hatch full 0.508)
			(connect_pads
				(clearance 0)
			)
			(min_thickness 0.254)
			(filled_areas_thickness no)
			(keepout
				(tracks not_allowed)
				(vias not_allowed)
				(pads allowed)
				(copperpour not_allowed)
				(footprints allowed)
			)
			(placement
				(enabled no)
				(sheetname "")
			)
			(fill
				(thermal_gap 0.508)
				(thermal_bridge_width 0.508)
			)
			(polygon
				(pts
					(xy 184.54135 208.28495) (xy 181.34095 208.28495) (xy 181.34095 213.59355) (xy 184.54135 213.59355)
				)
			)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:CAP_EEHZU1V471P"
		(layer "B.Cu")
		(at 230.22905 153.99195 -90)
		(property "Reference" "C3"
			(at -0.375 6.535 90)
			(layer "B.SilkS")
		)
		(property "Value" "C_0603"
			(at 5.975 -6.535 90)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "SMD 0603 MLCC capacitor, Alternate KiCad Library"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/DC-DC_Converters/")
		(sheetfile "DC-DC_Converters.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -4.35 0 270)
			(size 4.1 2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 303 "/GNDREF")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd rect
			(at 4.35 0 270)
			(size 4.1 2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 1 "/EPS_IN")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:RESC1508X55N"
		(layer "B.Cu")
		(at 94.85905 203.29195)
		(property "Reference" "R8"
			(at -0.21 1.07 0)
			(layer "B.SilkS")
		)
		(property "Value" "0 Ohm"
			(at 1.54 -1.07 0)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MF" "Stackpole Electronics Inc"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description_1" "0 Ohms Jumper 0.1W, 1/10W Chip Resistor 0603 (1608 Metric) Automotive AEC-Q200 Thick Film"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Package" "1508 Stackpole"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Price" "None"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "SnapEDA_Link" "https://www.snapeda.com/parts/RMCF0603ZT0R00/Stackpole+Electronics/view-part/?ref=snap"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MP" "RMCF0603ZT0R00"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Purchase-URL" "https://www.snapeda.com/api/url_track_click_mouser/?unipart_id=3968849&manufacturer=Stackpole Electronics Inc&part_name=RMCF0603ZT0R00&search_term=rmcf0603zt0r00"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Availability" "In Stock"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Check_prices" "https://www.snapeda.com/parts/RMCF0603ZT0R00/Stackpole+Electronics/view-part/?ref=eda"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(sheetname "/DC-DC_Converters/")
		(sheetfile "DC-DC_Converters.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -0.76 0)
			(size 0.9 0.97)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 99 "Net-(U3-PC{slash}NC)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd rect
			(at 0.76 0)
			(size 0.9 0.97)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 98 "Net-(R7-Pad2)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:CAPC1608X95N"
		(layer "B.Cu")
		(at 248.71605 72.64195)
		(property "Reference" "C7"
			(at 2.0922 0.4 0)
			(layer "B.SilkS")
		)
		(property "Value" "C_0603"
			(at 1.51 -1.07 0)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "SMD 0603 MLCC capacitor, Alternate KiCad Library"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/DC-DC_Converters/")
		(sheetfile "DC-DC_Converters.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -0.763 0)
			(size 0.95 0.98)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 303 "/GNDREF")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd rect
			(at 0.763 0)
			(size 0.95 0.98)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 4 "/DC_POS.5V")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:CAPC1608X90"
		(layer "B.Cu")
		(at 244.55905 192.79195)
		(descr "<b>CAPACITOR</b>")
		(property "Reference" "C41"
			(at 2.4992 0 0)
			(layer "B.SilkS")
		)
		(property "Value" "0.1uF"
			(at 1.56646 -1.20613 0)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "SMD 0603 MLCC capacitor, Alternate KiCad Library"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/Digital Systems/")
		(sheetfile "Digital_Systems.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -0.85 0)
			(size 1.1 1)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 35 "/Digital Systems/3.3V+")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd rect
			(at 0.85 0)
			(size 1.1 1)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 303 "/GNDREF")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:CAPC1608X90"
		(layer "B.Cu")
		(at 244.45905 183.29195)
		(descr "<b>CAPACITOR</b>")
		(property "Reference" "C46"
			(at 2.8492 0 0)
			(layer "B.SilkS")
		)
		(property "Value" "0.1uF"
			(at 1.56646 -1.20613 0)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "SMD 0603 MLCC capacitor, Alternate KiCad Library"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/Digital Systems/")
		(sheetfile "Digital_Systems.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -0.85 0)
			(size 1.1 1)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 35 "/Digital Systems/3.3V+")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd rect
			(at 0.85 0)
			(size 1.1 1)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 303 "/GNDREF")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:RESC1508X55N"
		(layer "B.Cu")
		(at 85.73905 204.86195 180)
		(property "Reference" "R4"
			(at -0.21 1.07 0)
			(layer "B.SilkS")
		)
		(property "Value" "0 Ohm"
			(at 1.54 -1.07 0)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MF" "Stackpole Electronics Inc"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description_1" "0 Ohms Jumper 0.1W, 1/10W Chip Resistor 0603 (1608 Metric) Automotive AEC-Q200 Thick Film"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Package" "1508 Stackpole"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Price" "None"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "SnapEDA_Link" "https://www.snapeda.com/parts/RMCF0603ZT0R00/Stackpole+Electronics/view-part/?ref=snap"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MP" "RMCF0603ZT0R00"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Purchase-URL" "https://www.snapeda.com/api/url_track_click_mouser/?unipart_id=3968849&manufacturer=Stackpole Electronics Inc&part_name=RMCF0603ZT0R00&search_term=rmcf0603zt0r00"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Availability" "In Stock"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Check_prices" "https://www.snapeda.com/parts/RMCF0603ZT0R00/Stackpole+Electronics/view-part/?ref=eda"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(sheetname "/DC-DC_Converters/")
		(sheetfile "DC-DC_Converters.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -0.76 0 180)
			(size 0.9 0.97)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 94 "Net-(U3-+S)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd rect
			(at 0.76 0 180)
			(size 0.9 0.97)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 5 "/DC_POS.12V")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "EPS_Footprints:CAP_NTF_55_2.8T_NIP"
		(layer "B.Cu")
		(at 174.96845 211.93925 90)
		(tags "KTF500B106M55NHT00 ")
		(property "Reference" "C2"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "KTF500B106M55NHT00"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Datasheet" "KTF500B106M55NHT00"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "CAP_NTF_55_2.8T_NIP CAP_NTF_55_2.8T_NIP-M CAP_NTF_55_2.8T_NIP-L")
		(sheetname "/DC-DC_Converters/")
		(sheetfile "DC-DC_Converters.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
		)
		(pad "1" smd rect
			(at -2.5273 0 90)
			(size 1.7526 5.4102)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 2 "Net-(C2-Pad1)")
			(pintype "unspecified")
		)
		(pad "2" smd rect
			(at 2.5273 0 90)
			(size 1.7526 5.4102)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 303 "/GNDREF")
			(pintype "unspecified")
		)
		(zone
			(net 0)
			(net_name "")
			(layer "B.Cu")
			(hatch full 0.508)
			(connect_pads
				(clearance 0)
			)
			(min_thickness 0.254)
			(filled_areas_thickness no)
			(keepout
				(tracks not_allowed)
				(vias not_allowed)
				(pads allowed)
				(copperpour not_allowed)
				(footprints allowed)
			)
			(placement
				(enabled no)
				(sheetname "")
			)
			(fill
				(thermal_gap 0.508)
				(thermal_bridge_width 0.508)
			)
			(polygon
				(pts
					(xy 177.62275 213.53945) (xy 177.62275 210.33905) (xy 172.31415 210.33905) (xy 172.31415 213.53945)
				)
			)
		)
		(embedded_fonts no)
	)
	(gr_rect
		(start 25.60825 26.89195)
		(end 307.25825 266.04195)
		(fill no)
		(layer "Edge.Cuts")
	)
	(zone
		(net 64)
		(net_name "/LCL_5.6A4")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 41)
		(connect_pads yes
			(clearance 0.5)
		)
		(min_thickness 0.5)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 266.60905 37.79195) (xy 283.60905 37.79195) (xy 283.35905 46.29195) (xy 289.10905 46.29195)
				(xy 289.10905 48.04195) (xy 285.10905 48.04195) (xy 285.10905 52.79195) (xy 278.85905 52.79195)
				(xy 278.85905 46.04195) (xy 266.60905 46.04195)
			)
		)
	)
	(zone
		(net 53)
		(net_name "/LCL_12.3A2")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 41)
		(connect_pads yes
			(clearance 0.5)
		)
		(min_thickness 0.5)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 107.10905 37.29195) (xy 124.10905 37.29195) (xy 123.85905 45.79195) (xy 129.60905 45.79195)
				(xy 129.60905 47.79195) (xy 126.10905 47.79195) (xy 126.10905 52.29195) (xy 119.35905 52.29195)
				(xy 119.35905 45.54195) (xy 107.10905 45.54195)
			)
		)
	)
	(zone
		(net 4)
		(net_name "/DC_POS.5V")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 63)
		(connect_pads yes
			(clearance 0.5)
		)
		(min_thickness 0.5)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 296.35905 48.54195) (xy 296.35905 52.54195) (xy 292.85905 52.54195) (xy 292.89105 48.54195)
			)
		)
	)
	(zone
		(net 32)
		(net_name "/LCL_9_and_3-3/9V_2A_LCL_1/OPAMP_Minus")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 73)
		(connect_pads yes
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 52.80825 231.79195) (xy 55.80825 231.79195) (xy 55.80825 233.79195) (xy 52.80825 233.79195)
			)
		)
	)
	(zone
		(net 59)
		(net_name "/LCL_5.6A3")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 41)
		(connect_pads yes
			(clearance 0.5)
		)
		(min_thickness 0.5)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 236.10905 38.04195) (xy 253.10905 38.04195) (xy 252.85905 46.54195) (xy 258.60905 46.54195)
				(xy 258.60905 48.29195) (xy 254.60905 48.29195) (xy 254.60905 53.04195) (xy 248.35905 53.04195)
				(xy 248.35905 46.29195) (xy 236.10905 46.29195)
			)
		)
	)
	(zone
		(net 16)
		(net_name "/LCL_12V/12V_3A_LCL_1/OPAMP_Minus")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 40)
		(connect_pads yes
			(clearance 0.5)
		)
		(min_thickness 0.5)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 139.10905 46.500536) (xy 151.060976 46.500536) (xy 151.060976 55.500536) (xy 158.60905 55.500536)
				(xy 158.60905 48.500536) (xy 162.35905 48.500536) (xy 162.35905 57.250536) (xy 152.810976 57.433435)
				(xy 151.85905 61.750536) (xy 139.10905 61.608258)
			)
		)
	)
	(zone
		(net 5)
		(net_name "/DC_POS.12V")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 22)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.5)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 51.60905 193.29195) (xy 55.85905 193.29195) (xy 55.85905 188.04195) (xy 51.60905 188.04195)
			)
		)
	)
	(zone
		(net 48)
		(net_name "/LCL_12.12A4")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 35)
		(connect_pads yes
			(clearance 0.5)
		)
		(min_thickness 0.5)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 37.10905 130.54195) (xy 47.10905 130.54195) (xy 47.10905 119.54195) (xy 45.60905 119.54195)
				(xy 45.60905 112.54195) (xy 37.10905 112.54195)
			)
		)
	)
	(zone
		(net 57)
		(net_name "/LCL_12.5A2")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 41)
		(connect_pads yes
			(clearance 0.5)
		)
		(min_thickness 0.5)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 41.35905 36.24195) (xy 58.353168 36.24195) (xy 58.10905 44.54195) (xy 63.85905 44.54195) (xy 63.85905 46.54195)
				(xy 60.35905 46.54195) (xy 60.35905 51.04195) (xy 53.60905 51.04195) (xy 53.60905 44.29195) (xy 41.35905 44.29195)
			)
		)
	)
	(zone
		(net 19)
		(net_name "/LCL_12V/12V_5A_LCL_1/OPAMP_Minus")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 40)
		(connect_pads yes
			(clearance 0.5)
		)
		(min_thickness 0.5)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 75.10905 45.6647) (xy 86.85905 45.6647) (xy 86.85905 54.6647) (xy 94.35905 54.6647) (xy 94.35905 47.6647)
				(xy 97.60905 47.6647) (xy 97.60905 56.9147) (xy 88.35905 56.9147) (xy 86.10905 60.9147) (xy 75.10905 60.79195)
			)
		)
	)
	(zone
		(net 11)
		(net_name "/LCL_12V/12V_12A_LCL_3/OPAMP_Minus")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 23)
		(connect_pads yes
			(clearance 0.5)
		)
		(min_thickness 0.5)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 50.95855 129.69245) (xy 60.45855 129.69245) (xy 60.45855 141.44245) (xy 62.20855 143.19245)
				(xy 62.20855 147.19245) (xy 61.95855 147.19245) (xy 61.95855 148.94245) (xy 63.45855 148.94245)
				(xy 63.45855 154.94245) (xy 46.95855 154.94245) (xy 46.95855 141.69245) (xy 57.20855 141.69245)
				(xy 57.20855 133.19245) (xy 50.95855 133.19245)
			)
		)
	)
	(zone
		(net 32)
		(net_name "/LCL_9_and_3-3/9V_2A_LCL_1/OPAMP_Minus")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 72)
		(connect_pads yes
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 47.30825 231.79195) (xy 51.55825 231.79195) (xy 51.55825 234.04195) (xy 47.30825 234.04195)
			)
		)
	)
	(zone
		(net 5)
		(net_name "/DC_POS.12V")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 42)
		(connect_pads yes
			(clearance 0.5)
		)
		(min_thickness 0.5)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 169.85905 52.79195) (xy 169.85905 48.54195) (xy 165.60905 48.54195) (xy 165.60905 52.79195)
			)
		)
	)
	(zone
		(net 30)
		(net_name "/LCL_5V/5V_6A_LCL_4/OPAMP_Minus")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 40)
		(connect_pads yes
			(clearance 0.5)
		)
		(min_thickness 0.5)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 266.35905 46.29195) (xy 278.310976 46.29195) (xy 278.310976 55.29195) (xy 286.35905 55.29195)
				(xy 286.35905 48.79195) (xy 289.60905 48.79195) (xy 289.60905 57.04195) (xy 280.060976 57.224849)
				(xy 276.85905 62.649672) (xy 266.35905 62.64967)
			)
		)
	)
	(zone
		(net 47)
		(net_name "/LCL_12.12A3")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 26)
		(connect_pads yes
			(clearance 0.5)
		)
		(min_thickness 0.5)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 37.45855 145.69245) (xy 46.45855 145.69245) (xy 46.45855 141.19245) (xy 54.20855 141.19245)
				(xy 54.20855 133.44245) (xy 50.45855 133.44245) (xy 50.45855 129.69245) (xy 47.45855 129.69245)
				(xy 47.45855 134.69245) (xy 36.70855 134.69245) (xy 36.95855 145.69245)
			)
		)
	)
	(zone
		(net 4)
		(net_name "/DC_POS.5V")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 63)
		(connect_pads yes
			(clearance 0.5)
		)
		(min_thickness 0.5)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 204.35905 48.79195) (xy 204.35905 52.79195) (xy 200.85905 52.79195) (xy 200.89105 48.79195)
			)
		)
	)
	(zone
		(net 5)
		(net_name "/DC_POS.12V")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 42)
		(connect_pads yes
			(clearance 0.5)
		)
		(min_thickness 0.5)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 105.35905 52.29195) (xy 105.35905 48.04195) (xy 101.10905 48.04195) (xy 101.10905 52.29195)
			)
		)
	)
	(zone
		(net 54)
		(net_name "/LCL_12.5A1")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 41)
		(connect_pads yes
			(clearance 0.5)
		)
		(min_thickness 0.5)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 74.85905 37.04195) (xy 91.85905 37.04195) (xy 91.60905 45.54195) (xy 97.35905 45.54195) (xy 97.35905 47.54195)
				(xy 93.85905 47.54195) (xy 93.85905 52.04195) (xy 87.10905 52.04195) (xy 87.10905 45.29195) (xy 74.85905 45.29195)
			)
		)
	)
	(zone
		(net 26)
		(net_name "/LCL_5V/5V_6A_LCL_1/OPAMP_Minus")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 40)
		(connect_pads yes
			(clearance 0.5)
		)
		(min_thickness 0.5)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 174.10905 46.434228) (xy 186.060976 46.434228) (xy 186.060976 55.434228) (xy 193.60905 55.434228)
				(xy 193.60905 48.434228) (xy 197.35905 48.434228) (xy 197.35905 57.184228) (xy 187.810976 57.367127)
				(xy 184.60905 62.79195) (xy 174.10905 62.791948)
			)
		)
	)
	(zone
		(net 72)
		(net_name "/DC_POS.3.3V")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 74)
		(connect_pads yes
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 155.30825 244.29195) (xy 155.30825 248.29195) (xy 153.05825 248.29195) (xy 153.05825 244.29195)
			)
		)
	)
	(zone
		(net 69)
		(net_name "/LCL_MIXED.3.3V1.5A")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 52)
		(connect_pads yes
			(clearance 0.5)
		)
		(min_thickness 0.5)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 174.85905 248.79195) (xy 174.85905 256.94195) (xy 155.60905 256.94195) (xy 155.60905 248.79195)
			)
		)
	)
	(zone
		(net 50)
		(net_name "/LCL_12.3A1")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 41)
		(connect_pads yes
			(clearance 0.5)
		)
		(min_thickness 0.5)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 139.35905 37.79195) (xy 156.35905 37.79195) (xy 156.10905 46.29195) (xy 161.85905 46.29195)
				(xy 161.85905 48.29195) (xy 158.35905 48.29195) (xy 158.35905 52.79195) (xy 151.60905 52.79195)
				(xy 151.60905 46.04195) (xy 139.35905 46.04195)
			)
		)
	)
	(zone
		(net 4)
		(net_name "/DC_POS.5V")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 63)
		(connect_pads yes
			(clearance 0.5)
		)
		(min_thickness 0.5)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 265.60905 48.79195) (xy 265.60905 52.79195) (xy 262.10905 52.79195) (xy 262.14105 48.79195)
			)
		)
	)
	(zone
		(net 63)
		(net_name "/LCL_5.6A2")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 41)
		(connect_pads yes
			(clearance 0.5)
		)
		(min_thickness 0.5)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 205.35905 37.79195) (xy 222.35905 37.79195) (xy 222.10905 46.29195) (xy 227.85905 46.29195)
				(xy 227.85905 48.04195) (xy 223.85905 48.04195) (xy 223.85905 52.79195) (xy 217.60905 52.79195)
				(xy 217.60905 46.04195) (xy 205.35905 46.04195)
			)
		)
	)
	(zone
		(net 5)
		(net_name "/DC_POS.12V")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 42)
		(connect_pads yes
			(clearance 0.5)
		)
		(min_thickness 0.5)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 137.85905 52.29195) (xy 137.85905 48.04195) (xy 133.60905 48.04195) (xy 133.60905 52.29195)
			)
		)
	)
	(zone
		(net 43)
		(net_name "/LCL_12.12A1")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 26)
		(connect_pads yes
			(clearance 0.5)
		)
		(min_thickness 0.5)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 37.60905 211.54195) (xy 46.60905 211.54195) (xy 46.60905 207.04195) (xy 54.35905 207.04195)
				(xy 54.35905 199.29195) (xy 50.60905 199.29195) (xy 50.60905 195.54195) (xy 47.60905 195.54195)
				(xy 47.60905 200.54195) (xy 36.85905 200.54195) (xy 37.10905 211.54195)
			)
		)
	)
	(zone
		(net 4)
		(net_name "/DC_POS.5V")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 63)
		(connect_pads yes
			(clearance 0.5)
		)
		(min_thickness 0.5)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 234.85905 48.54195) (xy 234.85905 52.54195) (xy 231.35905 52.54195) (xy 231.39105 48.54195)
			)
		)
	)
	(zone
		(net 32)
		(net_name "/LCL_9_and_3-3/9V_2A_LCL_1/OPAMP_Minus")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 20)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.5)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 60.30825 248.04195) (xy 52.85905 248.04195) (xy 52.85905 252.79195) (xy 60.35905 253.79195)
			)
		)
	)
	(zone
		(net 45)
		(net_name "/LCL_12.12A2")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 27)
		(connect_pads yes
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 36.85905 196.54195) (xy 47.10905 196.54195) (xy 47.10905 194.79195) (xy 51.10905 194.79195)
				(xy 51.10905 187.04195) (xy 45.85905 187.04195) (xy 45.85905 179.79195) (xy 36.85905 179.79195)
			)
		)
	)
	(zone
		(net 10)
		(net_name "/LCL_12V/12V_12A_LCL_2/OPAMP_Minus")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 29)
		(connect_pads yes
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 37.10905 179.29195) (xy 36.85905 179.29195) (xy 36.85905 172.29195) (xy 58.35905 172.54195)
				(xy 58.35905 186.79195) (xy 46.10905 186.54195) (xy 46.35905 179.54195)
			)
		)
	)
	(zone
		(net 5)
		(net_name "/DC_POS.12V")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 22)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.5)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 51.45855 127.44245) (xy 55.70855 127.44245) (xy 55.70855 122.19245) (xy 51.45855 122.19245)
			)
		)
	)
	(zone
		(net 5)
		(net_name "/DC_POS.12V")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 42)
		(connect_pads yes
			(clearance 0.5)
		)
		(min_thickness 0.5)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 71.60905 51.54195) (xy 71.60905 47.29195) (xy 67.35905 47.29195) (xy 67.35905 51.54195)
			)
		)
	)
	(zone
		(net 5)
		(net_name "/DC_POS.12V")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 22)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.5)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 37.10905 102.54195) (xy 41.35905 102.54195) (xy 41.35905 97.79195) (xy 37.10905 97.79195)
			)
		)
	)
	(zone
		(net 5)
		(net_name "/DC_POS.12V")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 22)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.5)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 37.60905 170.04195) (xy 41.60905 170.04195) (xy 41.60905 165.29195) (xy 37.60905 165.29195)
			)
		)
	)
	(zone
		(net 303)
		(net_name "/GNDREF")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 75)
		(connect_pads yes
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 43.80825 236.29195) (xy 42.05825 236.29195) (xy 42.05825 237.54195) (xy 43.80825 237.54195)
			)
		)
	)
	(zone
		(net 13)
		(net_name "/LCL_12V/12V_12A_LCL_4/OPAMP_Minus")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 36)
		(connect_pads yes
			(clearance 0.5)
		)
		(min_thickness 0.5)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 37.10905 104.54195) (xy 58.60905 104.54195) (xy 58.60905 119.04195) (xy 46.60905 119.04195)
				(xy 46.60905 112.04195) (xy 37.10905 112.04195)
			)
		)
	)
	(zone
		(net 22)
		(net_name "/LCL_12V/12V_5A_LCL_2/OPAMP_Minus")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 40)
		(connect_pads yes
			(clearance 0.5)
		)
		(min_thickness 0.5)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 41.35905 44.79195) (xy 53.10905 44.79195) (xy 53.10905 53.79195) (xy 60.60905 53.79195) (xy 60.60905 46.79195)
				(xy 63.85905 46.79195) (xy 63.85905 56.04195) (xy 54.60905 56.04195) (xy 52.35905 60.04195) (xy 41.35905 59.9192)
			)
		)
	)
	(zone
		(net 27)
		(net_name "/LCL_5V/5V_6A_LCL_2/OPAMP_Minus")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 40)
		(connect_pads yes
			(clearance 0.5)
		)
		(min_thickness 0.5)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 204.85905 46.184228) (xy 216.810976 46.184228) (xy 216.810976 55.184228) (xy 224.35905 55.184228)
				(xy 224.35905 48.684228) (xy 228.10905 48.684228) (xy 228.10905 56.934228) (xy 218.560976 57.117127)
				(xy 215.35905 62.54195) (xy 204.85905 62.541948)
			)
		)
	)
	(zone
		(net 72)
		(net_name "/DC_POS.3.3V")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 66)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 186.35905 222.79195) (xy 191.10905 222.79195) (xy 191.10905 226.29195) (xy 186.35905 226.29195)
			)
		)
	)
	(zone
		(net 24)
		(net_name "/LCL_5V/5V_6A_LCL_3/OPAMP_Minus")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 40)
		(connect_pads yes
			(clearance 0.5)
		)
		(min_thickness 0.5)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 235.407124 46.54195) (xy 247.35905 46.54195) (xy 247.35905 55.54195) (xy 255.407124 55.54195)
				(xy 255.407124 49.04195) (xy 258.657124 49.04195) (xy 258.657124 57.29195) (xy 249.10905 57.474849)
				(xy 245.907124 62.899672) (xy 235.407124 62.89967)
			)
		)
	)
	(zone
		(net 6)
		(net_name "/DC_POS.9V")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 71)
		(connect_pads yes
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 51.30825 227.54195) (xy 46.80825 227.62705) (xy 46.80825 225.04195) (xy 51.30825 225.04195)
			)
		)
	)
	(zone
		(net 7)
		(net_name "/LCL_12V/12V_12A_LCL_1/OPAMP_Minus")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 23)
		(connect_pads yes
			(clearance 0.5)
		)
		(min_thickness 0.5)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 51.10905 195.54195) (xy 60.60905 195.54195) (xy 60.60905 207.29195) (xy 62.35905 209.04195)
				(xy 62.35905 213.04195) (xy 62.10905 213.04195) (xy 62.10905 214.79195) (xy 63.60905 214.79195)
				(xy 63.60905 220.79195) (xy 47.10905 220.79195) (xy 47.10905 207.54195) (xy 57.35905 207.54195)
				(xy 57.35905 199.04195) (xy 51.10905 199.04195)
			)
		)
	)
	(zone
		(net 61)
		(net_name "/LCL_5.6A1")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 41)
		(connect_pads yes
			(clearance 0.5)
		)
		(min_thickness 0.5)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 174.10905 37.79195) (xy 191.10905 37.79195) (xy 190.85905 46.29195) (xy 196.60905 46.29195)
				(xy 196.60905 48.29195) (xy 193.10905 48.29195) (xy 193.10905 52.79195) (xy 186.35905 52.79195)
				(xy 186.35905 46.04195) (xy 174.10905 46.04195)
			)
		)
	)
	(zone
		(net 18)
		(net_name "/LCL_12V/12V_3A_LCL_2/OPAMP_Minus")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 40)
		(connect_pads yes
			(clearance 0.5)
		)
		(min_thickness 0.5)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 107.157124 46.109051) (xy 119.10905 46.109051) (xy 119.10905 55.109051) (xy 126.657124 55.109051)
				(xy 126.657124 48.109051) (xy 130.407124 48.109051) (xy 130.407124 56.859051) (xy 120.85905 57.04195)
				(xy 119.907124 61.359051) (xy 107.157124 61.216773)
			)
		)
	)
	(zone
		(net 33)
		(net_name "/LCL_9_and_3-3/3-3V_1-5A_LCL_1/OPAMP_Minus")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 53)
		(connect_pads yes
			(clearance 0.5)
		)
		(min_thickness 0.5)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 158.60905 240.04195) (xy 163.60905 240.04195) (xy 163.60905 245.79195) (xy 173.60905 245.79195)
				(xy 177.35905 241.54195) (xy 187.60905 241.56695) (xy 187.60905 256.29195) (xy 175.60905 256.29195)
				(xy 175.60905 247.54195) (xy 158.60905 247.54195)
			)
		)
	)
	(zone
		(net 1)
		(net_name "/EPS_IN")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 11)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 190.35905 105.34195) (xy 201.95905 105.34195) (xy 201.95905 111.74195) (xy 190.35905 111.74195)
			)
		)
	)
	(zone
		(net 4)
		(net_name "/DC_POS.5V")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 60)
		(connect_pads yes
			(clearance 0.5)
		)
		(min_thickness 0.5)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 248.894765 66.79195) (xy 249.10905 81.79195) (xy 264.580512 81.79195) (xy 264.366227 66.79195)
			)
		)
	)
	(zone
		(net 303)
		(net_name "/GNDREF")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 18)
		(connect_pads yes
			(clearance 0.5)
		)
		(min_thickness 0.5)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 137.10905 232.54195) (xy 140.60905 232.54195) (xy 140.60905 225.79195) (xy 137.10905 225.79195)
			)
		)
	)
	(zone
		(net 303)
		(net_name "/GNDREF")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 4)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 212.10905 148.459694) (xy 220.90905 148.459694) (xy 220.90905 135.259694) (xy 212.10905 135.259694)
			)
		)
	)
	(zone
		(net 71)
		(net_name "Net-(U4-+Vin)")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 17)
		(connect_pads yes
			(clearance 0.5)
		)
		(min_thickness 0.5)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 135.10905 235.54195) (xy 135.10905 238.29195) (xy 130.35905 238.29195) (xy 123.85905 237.29195)
				(xy 123.85905 234.04195) (xy 126.60905 234.04195) (xy 129.85905 236.04195) (xy 133.35905 235.54195)
			)
		)
	)
	(zone
		(net 3)
		(net_name "Net-(PS1-+V_INPUT)")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 57)
		(connect_pads yes
			(clearance 0.5)
		)
		(min_thickness 0.5)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 227.35905 125.54195) (xy 265.85905 125.54195) (xy 265.85905 142.04195) (xy 247.85905 142.04195)
				(xy 247.85905 134.54195) (xy 236.10905 134.54195) (xy 227.60905 140.29195)
			)
		)
	)
	(zone
		(net 1)
		(net_name "/EPS_IN")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 9)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 190.35905 105.34195) (xy 186.80825 104.79195) (xy 178.30825 104.79195) (xy 178.30825 111.79195)
				(xy 187.15905 111.74195) (xy 190.35905 111.74195)
			)
		)
	)
	(zone
		(net 303)
		(net_name "/GNDREF")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 10)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 190.33905 160.66195) (xy 201.93905 160.66195) (xy 201.93905 167.06195) (xy 190.33905 167.06195)
			)
		)
	)
	(zone
		(net 1)
		(net_name "/EPS_IN")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 47)
		(connect_pads yes
			(clearance 0.5)
		)
		(min_thickness 0.5)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 184.35905 207.79195) (xy 189.60905 207.79195) (xy 189.60905 220.79195) (xy 184.60905 220.79195)
			)
		)
	)
	(zone
		(net 5)
		(net_name "/DC_POS.12V")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 13)
		(connect_pads yes
			(clearance 0.5)
		)
		(min_thickness 0.5)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 78.889062 104.049725) (xy 69.489062 105.249725) (xy 66.689062 105.249725) (xy 50.742862 104.649725)
				(xy 50.742862 101.049725) (xy 72.089062 83.849725) (xy 78.889062 83.849725)
			)
		)
	)
	(zone
		(net 303)
		(net_name "/GNDREF")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 56)
		(connect_pads yes
			(clearance 0.5)
		)
		(min_thickness 0.5)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 227.60905 153.04195) (xy 246.60905 147.54195) (xy 246.60905 135.29195) (xy 236.85905 135.29195)
				(xy 227.60905 142.04195)
			)
		)
	)
	(zone
		(net 303)
		(net_name "/GNDREF")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 7)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 190.35905 95.34195) (xy 186.95905 95.34195) (xy 179.00905 96.79195) (xy 179.00905 100.29195)
				(xy 186.668141 101.74195) (xy 190.35905 101.74195)
			)
		)
	)
	(zone
		(net 1)
		(net_name "/EPS_IN")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 11)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 190.33905 170.66195) (xy 201.93905 170.66195) (xy 201.93905 177.06195) (xy 190.33905 177.06195)
			)
		)
	)
	(zone
		(net 1)
		(net_name "/EPS_IN")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 5)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 210.70905 148.459694) (xy 201.70905 148.459694) (xy 201.70905 135.459694) (xy 210.70905 135.459694)
			)
		)
	)
	(zone
		(net 70)
		(net_name "Net-(U4--Vin)")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 16)
		(connect_pads yes
			(clearance 0.5)
		)
		(min_thickness 0.5)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 135.10905 238.29195) (xy 140.60905 238.29195) (xy 140.60905 233.04195) (xy 130.10905 232.79195)
				(xy 126.35905 228.79195) (xy 123.85905 228.79195) (xy 123.85905 232.04195) (xy 129.85905 235.54195)
				(xy 135.10905 235.54195)
			)
		)
	)
	(zone
		(net 303)
		(net_name "/GNDREF")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 10)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 190.35905 95.34195) (xy 201.95905 95.34195) (xy 201.95905 101.74195) (xy 190.35905 101.74195)
			)
		)
	)
	(zone
		(net 1)
		(net_name "/EPS_IN")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 9)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 190.33905 170.66195) (xy 187.13905 170.04195) (xy 178.28905 170.04195) (xy 178.308307 177.313295)
				(xy 187.13905 177.06195) (xy 190.33905 177.06195)
			)
		)
	)
	(zone
		(net 1)
		(net_name "/EPS_IN")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 19)
		(connect_pads yes
			(clearance 0.5)
		)
		(min_thickness 0.5)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 135.60905 232.54195) (xy 132.10905 232.54195) (xy 132.10905 225.79195) (xy 135.60905 225.79195)
			)
		)
	)
	(zone
		(net 1)
		(net_name "/EPS_IN")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 3)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 212.60905 120.94195) (xy 212.60905 133.54195) (xy 221.60905 133.54195) (xy 221.60905 120.94195)
			)
		)
	)
	(zone
		(net 303)
		(net_name "/GNDREF")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 59)
		(connect_pads yes
			(clearance 0.5)
		)
		(min_thickness 0.5)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 236.10905 81.79195) (xy 248.35905 81.79195) (xy 248.463621 66.54195) (xy 237.196007 66.54195)
				(xy 236.10905 81.54195)
			)
		)
	)
	(zone
		(net 2)
		(net_name "Net-(C2-Pad1)")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 48)
		(connect_pads yes
			(clearance 0.5)
		)
		(min_thickness 0.5)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 165.10905 213.54195) (xy 178.60905 213.54195) (xy 182.10905 217.29195) (xy 182.10905 222.29195)
				(xy 165.10905 222.29195)
			)
		)
	)
	(zone
		(net 303)
		(net_name "/GNDREF")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 49)
		(connect_pads yes
			(clearance 0.5)
		)
		(min_thickness 0.5)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 164.85905 210.54195) (xy 178.85905 210.54195) (xy 179.35905 213.54195) (xy 181.60905 214.04195)
				(xy 181.60905 205.79195) (xy 164.85905 205.79195)
			)
		)
	)
	(zone
		(net 1)
		(net_name "/EPS_IN")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 55)
		(connect_pads yes
			(clearance 0.5)
		)
		(min_thickness 0.5)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 226.10905 155.79195) (xy 246.35905 150.04195) (xy 255.10905 150.04195) (xy 255.10905 162.04195)
				(xy 226.10905 162.04195)
			)
		)
	)
	(zone
		(net 303)
		(net_name "/GNDREF")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 12)
		(connect_pads yes
			(clearance 0.5)
		)
		(min_thickness 0.5)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 79.13905 192.46195) (xy 79.13905 173.66195) (xy 69.53905 171.26195) (xy 50.73905 171.29195)
				(xy 50.73905 176.66195) (xy 66.78905 192.31195)
			)
		)
	)
	(zone
		(net 6)
		(net_name "/DC_POS.9V")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 15)
		(connect_pads yes
			(clearance 0.5)
		)
		(min_thickness 0.5)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 69.35905 234.29195) (xy 82.35905 234.29195) (xy 82.35905 240.54195) (xy 73.10905 240.54195)
				(xy 69.35905 236.79195)
			)
		)
	)
	(zone
		(net 5)
		(net_name "/DC_POS.12V")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 13)
		(connect_pads yes
			(clearance 0.5)
		)
		(min_thickness 0.5)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 78.93905 169.26195) (xy 69.53905 170.46195) (xy 66.73905 170.46195) (xy 50.30916 170.544457)
				(xy 50.295193 166.662943) (xy 72.13905 149.06195) (xy 78.93905 149.06195)
			)
		)
	)
	(zone
		(net 303)
		(net_name "/GNDREF")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 12)
		(connect_pads yes
			(clearance 0.5)
		)
		(min_thickness 0.5)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 79.174085 127.27971) (xy 78.95905 108.19195) (xy 69.574085 106.07971) (xy 50.774085 107.67971)
				(xy 50.774085 111.47971) (xy 66.70905 127.44195)
			)
		)
	)
	(zone
		(net 303)
		(net_name "/GNDREF")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 50)
		(connect_pads yes
			(clearance 0.5)
		)
		(min_thickness 0.5)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 184.60905 224.84655) (xy 184.60905 236.34655) (xy 178.85905 236.34655) (xy 178.85905 224.84655)
			)
		)
	)
	(zone
		(net 92)
		(net_name "Net-(U3-+On{slash}Off)")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 6)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.5)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 188.810009 157.29195) (xy 178.48905 157.29195) (xy 178.48905 161.739891) (xy 188.789368 160.225139)
			)
		)
	)
	(zone
		(net 303)
		(net_name "/GNDREF")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 7)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 190.33905 160.66195) (xy 186.93905 160.66195) (xy 178.55825 162.29195) (xy 178.48905 165.04195)
				(xy 186.648141 167.06195) (xy 190.33905 167.06195)
			)
		)
	)
	(zone
		(net 91)
		(net_name "Net-(U2-+On{slash}Off)")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 6)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.5)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 189.067021 91.792023) (xy 178.965508 91.707548) (xy 178.903647 96.347156) (xy 188.95905 94.868421)
			)
		)
	)
	(zone
		(net 303)
		(net_name "/GNDREF")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 14)
		(connect_pads yes
			(clearance 0.5)
		)
		(min_thickness 0.5)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 82.35905 225.79195) (xy 73.10905 225.79195) (xy 69.35905 229.29195) (xy 69.35905 233.29195)
				(xy 82.35905 233.29195)
			)
		)
	)
	(zone
		(net 303)
		(net_name "/GNDREF")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 2)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 211.20905 133.54195) (xy 211.20905 120.94195) (xy 202.40905 120.94195) (xy 202.40905 133.54195)
			)
		)
	)
	(zone
		(net 303)
		(net_name "/GNDREF")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 8)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 193.43905 180.54195) (xy 193.43905 187.26195) (xy 187.13905 187.26195) (xy 178.058113 187.295663)
				(xy 178.05825 180.54195) (xy 187.13905 180.54195)
			)
		)
	)
	(zone
		(net 303)
		(net_name "/GNDREF")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 8)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 193.45905 115.34195) (xy 193.45905 121.94195) (xy 187.15905 121.94195) (xy 177.80825 122.04195)
				(xy 177.61292 115.282286) (xy 187.15905 115.34195)
			)
		)
	)
	(zone
		(net 303)
		(net_name "/GNDREF")
		(layer "In1.Cu")
		(hatch edge 0.5)
		(priority 1)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 34.65825 35.99195) (xy 298.20825 35.99195) (xy 298.20825 256.64441) (xy 34.65825 257.292565)
			)
		)
	)
	(zone
		(net 43)
		(net_name "/LCL_12.12A1")
		(layer "In2.Cu")
		(hatch edge 0.5)
		(priority 25)
		(connect_pads yes
			(clearance 0.5)
		)
		(min_thickness 0.5)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 53.80825 224.79195) (xy 35.10825 224.79195) (xy 35.10825 198.04195) (xy 44.80825 198.04195)
				(xy 45.05825 195.04195) (xy 51.80825 194.930299) (xy 51.80825 200.79195) (xy 53.80825 200.79195)
			)
		)
	)
	(zone
		(net 16)
		(net_name "/LCL_12V/12V_3A_LCL_1/OPAMP_Minus")
		(layer "In2.Cu")
		(hatch edge 0.5)
		(priority 45)
		(connect_pads yes
			(clearance 0.5)
		)
		(min_thickness 0.5)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 165.55825 52.79195) (xy 153.05825 52.79195) (xy 153.05825 57.04195) (xy 145.05825 56.79195)
				(xy 145.05825 48.04195) (xy 138.55825 48.04195) (xy 138.55825 63.04195) (xy 145.30825 63.04195)
				(xy 145.30825 59.54195) (xy 165.616006 59.179312)
			)
		)
	)
	(zone
		(net 5)
		(net_name "/DC_POS.12V")
		(layer "In2.Cu")
		(hatch edge 0.5)
		(priority 37)
		(connect_pads yes
			(clearance 0.5)
		)
		(min_thickness 0.5)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 35.10825 97.99195) (xy 50.30825 97.79195) (xy 50.30825 104.54195) (xy 35.10825 104.54195)
			)
		)
	)
	(zone
		(net 72)
		(net_name "/DC_POS.3.3V")
		(layer "In2.Cu")
		(hatch edge 0.5)
		(priority 51)
		(connect_pads yes
			(clearance 0.5)
		)
		(min_thickness 0.5)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 111.30825 229.357392) (xy 185.80825 229.607392) (xy 185.80825 248.79195) (xy 111.30825 248.79195)
			)
		)
	)
	(zone
		(net 50)
		(net_name "/LCL_12.3A1")
		(layer "In2.Cu")
		(hatch edge 0.5)
		(priority 46)
		(connect_pads yes
			(clearance 0.5)
		)
		(min_thickness 0.5)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 133.690979 37.233835) (xy 165.45632 37.233835) (xy 165.30825 51.712049) (xy 152.690979 52.214608)
				(xy 152.690979 53.983835) (xy 145.940979 53.983835) (xy 145.940979 47.233835) (xy 133.690979 47.233835)
			)
		)
	)
	(zone
		(net 3)
		(net_name "Net-(PS1-+V_INPUT)")
		(layer "In2.Cu")
		(hatch edge 0.5)
		(priority 58)
		(connect_pads yes
			(clearance 0.5)
		)
		(min_thickness 0.5)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 222.05825 146.79195) (xy 222.05825 127.29195) (xy 265.63518 127.29195) (xy 265.38518 146.79195)
			)
		)
	)
	(zone
		(net 5)
		(net_name "/DC_POS.12V")
		(layer "In2.Cu")
		(hatch edge 0.5)
		(priority 44)
		(connect_pads yes
			(clearance 0.5)
		)
		(min_thickness 0.5)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 166.566677 48.29195) (xy 171.05825 48.29195) (xy 171.05825 71.29195) (xy 166.30825 71.29195)
			)
		)
	)
	(zone
		(net 45)
		(net_name "/LCL_12.12A2")
		(layer "In2.Cu")
		(hatch edge 0.5)
		(priority 30)
		(connect_pads yes
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 34.890312 197.398168) (xy 44.30825 197.29195) (xy 44.30825 194.54195) (xy 49.30825 194.54195)
				(xy 49.30825 182.79195) (xy 34.940163 182.79195)
			)
		)
	)
	(zone
		(net 27)
		(net_name "/LCL_5V/5V_6A_LCL_2/OPAMP_Minus")
		(layer "In2.Cu")
		(hatch edge 0.5)
		(priority 65)
		(connect_pads yes
			(clearance 0.5)
		)
		(min_thickness 0.5)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 204.80825 48.04195) (xy 210.80825 48.04195) (xy 210.80825 54.79195) (xy 218.80825 54.79195)
				(xy 218.80825 52.29195) (xy 230.80825 52.29195) (xy 230.80825 64.04195) (xy 209.55825 64.04195)
				(xy 204.80825 64.04195)
			)
		)
	)
	(zone
		(net 4)
		(net_name "/DC_POS.5V")
		(layer "In2.Cu")
		(hatch edge 0.5)
		(priority 62)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.5)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 262.05825 48.79195) (xy 265.80825 48.79195) (xy 265.80825 70.54195) (xy 262.05825 70.54195)
			)
		)
	)
	(zone
		(net 26)
		(net_name "/LCL_5V/5V_6A_LCL_1/OPAMP_Minus")
		(layer "In2.Cu")
		(hatch edge 0.5)
		(priority 65)
		(connect_pads yes
			(clearance 0.5)
		)
		(min_thickness 0.5)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 171.30825 48.29195) (xy 179.80825 48.29195) (xy 179.80825 55.04195) (xy 188.05825 55.04195)
				(xy 188.05825 52.79195) (xy 199.30825 52.79195) (xy 199.30825 64.29195) (xy 178.55825 64.29195)
				(xy 171.30825 64.29195)
			)
		)
	)
	(zone
		(net 7)
		(net_name "/LCL_12V/12V_12A_LCL_1/OPAMP_Minus")
		(layer "In2.Cu")
		(hatch edge 0.5)
		(priority 24)
		(connect_pads yes
			(clearance 0.5)
		)
		(min_thickness 0.5)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 52.05825 195.29195) (xy 63.55825 195.29195) (xy 63.55825 208.04195) (xy 72.55825 208.04195)
				(xy 72.55825 224.79195) (xy 54.55825 224.79195) (xy 54.55825 200.54195) (xy 52.05825 200.54195)
			)
		)
	)
	(zone
		(net 11)
		(net_name "/LCL_12V/12V_12A_LCL_3/OPAMP_Minus")
		(layer "In2.Cu")
		(hatch edge 0.5)
		(priority 33)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.5)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 51.05825 131.04195) (xy 60.55825 131.04195) (xy 60.55825 142.54195) (xy 63.55825 142.54195)
				(xy 63.55825 158.04195) (xy 47.30825 158.04195) (xy 47.30825 143.04195) (xy 54.30825 143.04195)
				(xy 54.30825 133.29195) (xy 51.05825 133.29195)
			)
		)
	)
	(zone
		(net 72)
		(net_name "/DC_POS.3.3V")
		(layer "In2.Cu")
		(hatch edge 0.5)
		(priority 67)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 185.80825 241.54195) (xy 239.05825 241.790782) (xy 239.05825 249.29195) (xy 185.55825 248.79195)
				(xy 185.30825 243.04195) (xy 185.80825 243.04195)
			)
		)
	)
	(zone
		(net 4)
		(net_name "/DC_POS.5V")
		(layer "In2.Cu")
		(hatch edge 0.5)
		(priority 62)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.5)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 200.55825 48.54195) (xy 204.30825 48.54195) (xy 204.30825 71.29195) (xy 200.55825 71.29195)
			)
		)
	)
	(zone
		(net 5)
		(net_name "/DC_POS.12V")
		(layer "In2.Cu")
		(hatch edge 0.5)
		(priority 28)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 49.55825 105.29195) (xy 49.55825 98.54195) (xy 49.80825 86.29195) (xy 63.80825 85.79195) (xy 108.30825 85.54195)
				(xy 108.05825 125.79195) (xy 108.30825 169.04195) (xy 107.55825 205.04195) (xy 64.55825 204.79195)
				(xy 64.30825 194.04195) (xy 49.80825 194.04195) (xy 49.80825 189.54195) (xy 63.55825 189.54195)
				(xy 63.55825 170.29195) (xy 35.10825 170.809223) (xy 35.10825 158.79195) (xy 55.55825 158.79195)
				(xy 64.55825 159.04195) (xy 64.80825 105.54195) (xy 51.55825 105.54195)
			)
		)
	)
	(zone
		(net 30)
		(net_name "/LCL_5V/5V_6A_LCL_4/OPAMP_Minus")
		(layer "In2.Cu")
		(hatch edge 0.5)
		(priority 65)
		(connect_pads yes
			(clearance 0.5)
		)
		(min_thickness 0.5)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 266.30825 48.04195) (xy 272.30825 48.04195) (xy 272.30825 54.79195) (xy 280.55825 54.79195)
				(xy 280.55825 52.29195) (xy 292.05825 52.29195) (xy 292.05825 64.04195) (xy 271.05825 64.04195)
				(xy 266.30825 64.04195)
			)
		)
	)
	(zone
		(net 72)
		(net_name "/DC_POS.3.3V")
		(layer "In2.Cu")
		(hatch edge 0.5)
		(priority 68)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 136.05825 228.29195) (xy 136.05825 218.29195) (xy 176.55825 218.29195) (xy 176.55825 223.29195)
				(xy 191.05825 223.29195) (xy 191.05825 229.79195) (xy 136.05825 229.79195)
			)
		)
	)
	(zone
		(net 18)
		(net_name "/LCL_12V/12V_3A_LCL_2/OPAMP_Minus")
		(layer "In2.Cu")
		(hatch edge 0.5)
		(priority 45)
		(connect_pads yes
			(clearance 0.5)
		)
		(min_thickness 0.5)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 133.557177 52.79195) (xy 121.05825 52.79195) (xy 121.05825 56.54195) (xy 113.05825 56.29195)
				(xy 113.05825 47.54195) (xy 106.55825 47.54195) (xy 106.55825 62.54195) (xy 113.30825 62.54195)
				(xy 113.30825 59.04195) (xy 133.555234 58.680397)
			)
		)
	)
	(zone
		(net 19)
		(net_name "/LCL_12V/12V_5A_LCL_1/OPAMP_Minus")
		(layer "In2.Cu")
		(hatch edge 0.5)
		(priority 45)
		(connect_pads yes
			(clearance 0.5)
		)
		(min_thickness 0.5)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 100.80825 52.54195) (xy 88.80825 52.54195) (xy 88.80825 56.29195) (xy 80.80825 56.04195) (xy 80.80825 47.29195)
				(xy 72.80825 47.29195) (xy 72.80825 62.29195) (xy 81.05825 62.29195) (xy 81.05825 58.79195) (xy 100.80825 58.79195)
			)
		)
	)
	(zone
		(net 4)
		(net_name "/DC_POS.5V")
		(layer "In2.Cu")
		(hatch edge 0.5)
		(priority 62)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.5)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 259.55825 81.54195) (xy 259.55825 70.29195) (xy 296.80825 70.29195) (xy 296.80825 81.54195)
			)
		)
	)
	(zone
		(net 1)
		(net_name "/EPS_IN")
		(layer "In2.Cu")
		(hatch edge 0.5)
		(priority 69)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 177.80825 217.29195) (xy 177.80825 222.79195) (xy 185.05825 222.79195) (xy 185.05825 217.29195)
			)
		)
	)
	(zone
		(net 5)
		(net_name "/DC_POS.12V")
		(layer "In2.Cu")
		(hatch edge 0.5)
		(priority 44)
		(connect_pads yes
			(clearance 0.5)
		)
		(min_thickness 0.5)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 101.316677 48.04195) (xy 105.80825 48.04195) (xy 105.80825 71.04195) (xy 101.05825 71.04195)
			)
		)
	)
	(zone
		(net 5)
		(net_name "/DC_POS.12V")
		(layer "In2.Cu")
		(hatch edge 0.5)
		(priority 44)
		(connect_pads yes
			(clearance 0.5)
		)
		(min_thickness 0.5)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 68.327913 47.04195) (xy 72.80825 47.04195) (xy 72.80825 71.04195) (xy 68.05825 71.04195)
			)
		)
	)
	(zone
		(net 13)
		(net_name "/LCL_12V/12V_12A_LCL_4/OPAMP_Minus")
		(layer "In2.Cu")
		(hatch edge 0.5)
		(priority 38)
		(connect_pads yes
			(clearance 0.5)
		)
		(min_thickness 0.5)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 35.10825 106.04195) (xy 57.30825 106.04195) (xy 57.80825 116.54195) (xy 63.80825 116.54195)
				(xy 63.80825 123.04195) (xy 47.30825 123.04195) (xy 47.30825 112.04195) (xy 35.10825 112.04195)
			)
		)
	)
	(zone
		(net 64)
		(net_name "/LCL_5.6A4")
		(layer "In2.Cu")
		(hatch edge 0.5)
		(priority 64)
		(connect_pads yes
			(clearance 0.5)
		)
		(min_thickness 0.5)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 260.80825 38.54195) (xy 292.30825 38.54195) (xy 292.30825 51.79195) (xy 279.80825 51.79195)
				(xy 279.80825 53.79195) (xy 273.05825 53.79195) (xy 273.05825 47.04195) (xy 260.80825 47.04195)
			)
		)
	)
	(zone
		(net 5)
		(net_name "/DC_POS.12V")
		(layer "In2.Cu")
		(hatch edge 0.5)
		(priority 43)
		(connect_pads yes
			(clearance 0.5)
		)
		(min_thickness 0.5)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 49.80825 86.29195) (xy 49.80825 70.54195) (xy 176.05825 70.79195) (xy 175.55825 86.29195)
			)
		)
	)
	(zone
		(net 63)
		(net_name "/LCL_5.6A2")
		(layer "In2.Cu")
		(hatch edge 0.5)
		(priority 64)
		(connect_pads yes
			(clearance 0.5)
		)
		(min_thickness 0.5)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 199.30825 38.79195) (xy 229.30825 38.79195) (xy 229.30825 52.04195) (xy 218.30825 52.04195)
				(xy 218.30825 54.04195) (xy 211.55825 54.04195) (xy 211.55825 47.29195) (xy 199.30825 47.29195)
			)
		)
	)
	(zone
		(net 48)
		(net_name "/LCL_12.12A4")
		(layer "In2.Cu")
		(hatch edge 0.5)
		(priority 39)
		(connect_pads yes
			(clearance 0.5)
		)
		(min_thickness 0.5)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 35.10825 112.79195) (xy 47.05825 112.79195) (xy 47.05825 123.54195) (xy 48.05825 123.54195)
				(xy 48.05825 129.79195) (xy 35.10825 129.79195)
			)
		)
	)
	(zone
		(net 5)
		(net_name "/DC_POS.12V")
		(layer "In2.Cu")
		(hatch edge 0.5)
		(priority 32)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.5)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 65.30825 123.54195) (xy 48.65775 123.54195) (xy 48.65775 128.04195) (xy 65.30825 128.04195)
			)
		)
	)
	(zone
		(net 1)
		(net_name "/EPS_IN")
		(layer "In2.Cu")
		(hatch edge 0.5)
		(priority 70)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 135.80825 217.29195) (xy 135.80825 229.29195) (xy 123.55825 229.29195) (xy 123.55825 217.29195)
			)
		)
	)
	(zone
		(net 4)
		(net_name "/DC_POS.5V")
		(layer "In2.Cu")
		(hatch edge 0.5)
		(priority 61)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.5)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 182.55825 68.093406) (xy 262.278215 67.580737) (xy 261.753456 125.04195) (xy 221.80825 125.04195)
				(xy 221.80825 91.54195) (xy 182.55825 91.54195)
			)
		)
	)
	(zone
		(net 10)
		(net_name "/LCL_12V/12V_12A_LCL_2/OPAMP_Minus")
		(layer "In2.Cu")
		(hatch edge 0.5)
		(priority 31)
		(connect_pads yes
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 35.05825 182.04195) (xy 49.80825 182.04195) (xy 49.80825 189.04195) (xy 63.05825 189.04195)
				(xy 63.05825 181.29195) (xy 56.80825 181.29195) (xy 56.80825 174.094891) (xy 35.05825 173.839009)
			)
		)
	)
	(zone
		(net 57)
		(net_name "/LCL_12.5A2")
		(layer "In2.Cu")
		(hatch edge 0.5)
		(priority 46)
		(connect_pads yes
			(clearance 0.5)
		)
		(min_thickness 0.5)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 35.55825 36.79195) (xy 67.80825 36.79195) (xy 67.80825 52.04195) (xy 54.55825 52.04195) (xy 54.55825 52.54195)
				(xy 47.80825 52.54195) (xy 47.80825 45.79195) (xy 35.55825 45.79195)
			)
		)
	)
	(zone
		(net 53)
		(net_name "/LCL_12.3A2")
		(layer "In2.Cu")
		(hatch edge 0.5)
		(priority 46)
		(connect_pads yes
			(clearance 0.5)
		)
		(min_thickness 0.5)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 101.456734 38.129792) (xy 133.206734 38.129792) (xy 133.339192 52.041739) (xy 120.456734 52.129792)
				(xy 120.456734 53.379792) (xy 113.706734 53.379792) (xy 113.706734 46.629792) (xy 101.456734 46.629792)
			)
		)
	)
	(zone
		(net 54)
		(net_name "/LCL_12.5A1")
		(layer "In2.Cu")
		(hatch edge 0.5)
		(priority 46)
		(connect_pads yes
			(clearance 0.5)
		)
		(min_thickness 0.5)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 69.05825 37.29195) (xy 100.80825 37.29195) (xy 100.80825 51.79195) (xy 88.05825 51.79195) (xy 88.05825 53.29195)
				(xy 81.30825 53.29195) (xy 81.30825 46.54195) (xy 69.05825 46.54195)
			)
		)
	)
	(zone
		(net 61)
		(net_name "/LCL_5.6A1")
		(layer "In2.Cu")
		(hatch edge 0.5)
		(priority 64)
		(connect_pads yes
			(clearance 0.5)
		)
		(min_thickness 0.5)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 168.30825 38.79195) (xy 198.30825 38.79195) (xy 198.30825 52.29195) (xy 187.30825 52.29195)
				(xy 187.30825 54.04195) (xy 180.55825 54.04195) (xy 180.55825 47.29195) (xy 168.30825 47.29195)
			)
		)
	)
	(zone
		(net 1)
		(net_name "/EPS_IN")
		(layer "In2.Cu")
		(hatch edge 0.5)
		(priority 54)
		(connect_pads yes
			(clearance 0.5)
		)
		(min_thickness 0.5)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 219.80825 163.29195) (xy 256.30825 163.29195) (xy 256.30825 148.04195) (xy 219.80825 148.29195)
			)
		)
	)
	(zone
		(net 59)
		(net_name "/LCL_5.6A3")
		(layer "In2.Cu")
		(hatch edge 0.5)
		(priority 64)
		(connect_pads yes
			(clearance 0.5)
		)
		(min_thickness 0.5)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 229.80825 38.79195) (xy 259.80825 38.79195) (xy 259.80825 52.29195) (xy 248.80825 52.29195)
				(xy 248.80825 54.04195) (xy 242.05825 54.04195) (xy 242.05825 47.29195) (xy 229.80825 47.29195)
			)
		)
	)
	(zone
		(net 4)
		(net_name "/DC_POS.5V")
		(layer "In2.Cu")
		(hatch edge 0.5)
		(priority 62)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.5)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 231.30825 48.54195) (xy 235.05825 48.54195) (xy 235.05825 70.79195) (xy 231.30825 70.79195)
			)
		)
	)
	(zone
		(net 47)
		(net_name "/LCL_12.12A3")
		(layer "In2.Cu")
		(hatch edge 0.5)
		(priority 34)
		(connect_pads yes
			(clearance 0.5)
		)
		(min_thickness 0.5)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 46.30825 156.54195) (xy 35.10825 156.54195) (xy 35.10825 130.04195) (xy 50.30825 130.04195)
				(xy 50.30825 133.54195) (xy 54.05825 133.54195) (xy 54.05825 141.04195) (xy 46.30825 141.04195)
			)
		)
	)
	(zone
		(net 1)
		(net_name "/EPS_IN")
		(layer "In2.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 220.30825 92.54195) (xy 111.45825 92.54195) (xy 111.45825 217.79195) (xy 220.30825 217.79195)
			)
		)
	)
	(zone
		(net 5)
		(net_name "/DC_POS.12V")
		(layer "In2.Cu")
		(hatch edge 0.5)
		(priority 44)
		(connect_pads yes
			(clearance 0.5)
		)
		(min_thickness 0.5)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 134.069486 47.79195) (xy 138.55825 47.79195) (xy 138.55825 71.04195) (xy 133.80825 71.04195)
			)
		)
	)
	(zone
		(net 4)
		(net_name "/DC_POS.5V")
		(layer "In2.Cu")
		(hatch edge 0.5)
		(priority 62)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.5)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 292.80825 48.54195) (xy 296.55825 48.54195) (xy 296.55825 70.79195) (xy 292.80825 70.79195)
			)
		)
	)
	(zone
		(net 24)
		(net_name "/LCL_5V/5V_6A_LCL_3/OPAMP_Minus")
		(layer "In2.Cu")
		(hatch edge 0.5)
		(priority 65)
		(connect_pads yes
			(clearance 0.5)
		)
		(min_thickness 0.5)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 235.30825 48.29195) (xy 241.55825 48.29195) (xy 241.55825 55.04195) (xy 249.55825 55.04195)
				(xy 249.55825 53.04195) (xy 261.05825 53.04195) (xy 261.05825 64.54195) (xy 240.34678 64.251154)
				(xy 240.30825 64.29195) (xy 235.30825 64.29195)
			)
		)
	)
	(zone
		(net 6)
		(net_name "/DC_POS.9V")
		(layer "In2.Cu")
		(hatch edge 0.5)
		(priority 21)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.5)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 76.80825 225.79195) (xy 35.35825 226.049403) (xy 35.35825 256.69195) (xy 77.061529 256.69195)
			)
		)
	)
	(zone
		(net 22)
		(net_name "/LCL_12V/12V_5A_LCL_2/OPAMP_Minus")
		(layer "In2.Cu")
		(hatch edge 0.5)
		(priority 45)
		(connect_pads yes
			(clearance 0.5)
		)
		(min_thickness 0.5)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 67.80825 52.54195) (xy 55.05825 52.54195) (xy 55.05825 55.04195) (xy 47.05825 55.04195) (xy 47.05825 46.29195)
				(xy 35.55825 46.29195) (xy 35.55825 61.29195) (xy 47.30825 61.29195) (xy 47.30825 57.79195) (xy 67.80825 57.54195)
			)
		)
	)
	(embedded_fonts no)
)
