(kicad_pcb
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(general
		(thickness 1.6)
		(legacy_teardrops no)
	)
	(paper "A4")
	(layers
		(0 "F.Cu" signal)
		(2 "B.Cu" signal)
		(9 "F.Adhes" user "F.Adhesive")
		(11 "B.Adhes" user "B.Adhesive")
		(13 "F.Paste" user)
		(15 "B.Paste" user)
		(5 "F.SilkS" user "F.Silkscreen")
		(7 "B.SilkS" user "B.Silkscreen")
		(1 "F.Mask" user)
		(3 "B.Mask" user)
		(17 "Dwgs.User" user "User.Drawings")
		(19 "Cmts.User" user "User.Comments")
		(21 "Eco1.User" user "User.Eco1")
		(23 "Eco2.User" user "User.Eco2")
		(25 "Edge.Cuts" user)
		(27 "Margin" user)
		(31 "F.CrtYd" user "F.Courtyard")
		(29 "B.CrtYd" user "B.Courtyard")
		(35 "F.Fab" user)
		(33 "B.Fab" user)
		(39 "User.1" user)
		(41 "User.2" user)
		(43 "User.3" user)
		(45 "User.4" user)
	)
	(setup
		(stackup
			(layer "F.SilkS"
				(type "Top Silk Screen")
			)
			(layer "F.Paste"
				(type "Top Solder Paste")
			)
			(layer "F.Mask"
				(type "Top Solder Mask")
				(color "Black")
				(thickness 0.01)
			)
			(layer "F.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "dielectric 1"
				(type "core")
				(thickness 1.51)
				(material "FR4")
				(epsilon_r 4.5)
				(loss_tangent 0.02)
			)
			(layer "B.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "B.Mask"
				(type "Bottom Solder Mask")
				(color "Black")
				(thickness 0.01)
			)
			(layer "B.Paste"
				(type "Bottom Solder Paste")
			)
			(layer "B.SilkS"
				(type "Bottom Silk Screen")
			)
			(copper_finish "None")
			(dielectric_constraints no)
		)
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(tenting front back)
		(pcbplotparams
			(layerselection 0x00000000_00000000_55555555_5755f5ff)
			(plot_on_all_layers_selection 0x00000000_00000000_00000000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 4)
			(plotframeref no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(pdf_metadata yes)
			(pdf_single_document no)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plot_black_and_white yes)
			(sketchpadsonfab no)
			(plotpadnumbers no)
			(hidednponfab no)
			(sketchdnponfab yes)
			(crossoutdnponfab yes)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 1)
			(scaleselection 1)
			(outputdirectory "")
		)
	)
	(net 0 "")
	(net 1 "GND")
	(net 2 "Net-(C1-Pad1)")
	(net 3 "Net-(C2-Pad1)")
	(net 4 "Net-(D1:1-A)")
	(net 5 "Net-(D1:2-A)")
	(net 6 "Net-(D1:3-A)")
	(net 7 "Net-(D1:4-A)")
	(net 8 "Net-(D2:1-A)")
	(net 9 "Net-(D2:2-A)")
	(net 10 "Net-(D2:3-A)")
	(net 11 "Net-(D2:4-A)")
	(net 12 "Net-(D3:1-A)")
	(net 13 "Net-(D3:2-A)")
	(net 14 "Net-(D3:3-A)")
	(net 15 "Net-(D3:4-A)")
	(net 16 "Net-(D4:1-A)")
	(net 17 "Net-(D4:2-A)")
	(net 18 "Net-(D4:3-A)")
	(net 19 "Net-(D4:4-A)")
	(net 20 "unconnected-(IC1-P3-Pad7)")
	(net 21 "unconnected-(IC1-P4-Pad8)")
	(net 22 "/SDA")
	(net 23 "/SCL")
	(net 24 "/TFTDC")
	(net 25 "/TFTRST")
	(net 26 "+3.3V")
	(net 27 "/TFTCS")
	(net 28 "/CARDCS")
	(net 29 "/MISO")
	(net 30 "/SCK")
	(net 31 "/LITE")
	(net 32 "/MOSI")
	(net 33 "/Human-Machine Interface/Keypad/COL1")
	(net 34 "/Human-Machine Interface/Keypad/COL2")
	(net 35 "/Human-Machine Interface/Keypad/COL3")
	(net 36 "/Human-Machine Interface/Keypad/COL4")
	(net 37 "/Human-Machine Interface/Keypad/ROW3")
	(net 38 "/Human-Machine Interface/TFTRST")
	(net 39 "/Human-Machine Interface/ENC_SW")
	(net 40 "/Human-Machine Interface/ENC_CLK")
	(net 41 "/Human-Machine Interface/Keypad/ROW2")
	(net 42 "/Human-Machine Interface/Keypad/ROW1")
	(net 43 "/Human-Machine Interface/Keypad/ROW4")
	(net 44 "/Human-Machine Interface/ENC_DT")
	(net 45 "/Human-Machine Interface/LITE")
	(net 46 "unconnected-(X2-Pad15)")
	(net 47 "unconnected-(X2-Pad14)")
	(net 48 "unconnected-(X2-Pad16)")
	(net 49 "unconnected-(X2-Pad12)")
	(net 50 "unconnected-(X2-Pad11)")
	(net 51 "unconnected-(X2-Pad17)")
	(net 52 "unconnected-(X2-Pad13)")
	(net 53 "unconnected-(X2-Pad18)")
	(net 54 "/Human-Machine Interface/PCF_A2")
	(net 55 "/Human-Machine Interface/PCF_A0")
	(net 56 "/Human-Machine Interface/PCF_A1")
	(net 57 "unconnected-(IC1-P1-Pad5)")
	(net 58 "Net-(JP4-C)")
	(net 59 "/Human-Machine Interface/Audio/~{SD_MODE}")
	(net 60 "/Human-Machine Interface/Audio/GAIN_SLOT")
	(net 61 "Net-(JP6-B)")
	(net 62 "Net-(U2-OUTN)")
	(net 63 "Net-(U2-OUTP)")
	(net 64 "Net-(MK1-LR)")
	(net 65 "Net-(MK1-SD)")
	(net 66 "unconnected-(U2-NC-Pad13)")
	(net 67 "unconnected-(U2-NC-Pad5)")
	(net 68 "unconnected-(U2-NC-Pad12)")
	(net 69 "unconnected-(U2-NC-Pad6)")
	(net 70 "/~{PCF_INT}")
	(net 71 "/Human-Machine Interface/BCLK")
	(net 72 "/Human-Machine Interface/~{PCF_INT}")
	(net 73 "/Human-Machine Interface/LRCLK")
	(net 74 "/Human-Machine Interface/MIC_DOUT")
	(net 75 "/Human-Machine Interface/~{AMP_SD}")
	(net 76 "/Human-Machine Interface/AMP_DIN")
	(net 77 "Net-(IC1-P0)")
	(footprint "capstone-project:434133025816"
		(layer "F.Cu")
		(at 81.146515 117.791804)
		(property "Reference" "S1"
			(at 0.115985 0.208196 0)
			(layer "F.SilkS")
		)
		(property "Value" "434133025816"
			(at 2.7768 2.7936 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/Human-Machine Interface/Keypad/")
		(sheetfile "../Projects/capstone-project/Hardware/KiCAD/system-testbed/keypad.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -2.075 -1.075)
			(size 1.05 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 12 "Net-(D3:1-A)")
			(pintype "passive")
			(solder_mask_margin 0.102)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd rect
			(at 2.075 -1.075)
			(size 1.05 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 12 "Net-(D3:1-A)")
			(pintype "passive")
			(solder_mask_margin 0.102)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "3" smd rect
			(at -2.075 1.075)
			(size 1.05 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 37 "/Human-Machine Interface/Keypad/ROW3")
			(pintype "passive")
			(solder_mask_margin 0.102)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "4" smd rect
			(at 2.075 1.075)
			(size 1.05 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 37 "/Human-Machine Interface/Keypad/ROW3")
			(pintype "passive")
			(solder_mask_margin 0.102)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "C:/Users/zackp/OneDrive/Desktop/434133025816/Download_STP_4341x30258x6+%28rev1%29.stp"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 90 -180 90)
			)
		)
	)
	(footprint "capstone-project:434133025816"
		(layer "F.Cu")
		(at 95.85 117.8)
		(property "Reference" "S11"
			(at 0.1 -0.1 0)
			(layer "F.SilkS")
		)
		(property "Value" "434133025816"
			(at 2.7768 2.7936 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/Human-Machine Interface/Keypad/")
		(sheetfile "../Projects/capstone-project/Hardware/KiCAD/system-testbed/keypad.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -2.075 -1.075)
			(size 1.05 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 14 "Net-(D3:3-A)")
			(pintype "passive")
			(solder_mask_margin 0.102)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd rect
			(at 2.075 -1.075)
			(size 1.05 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 14 "Net-(D3:3-A)")
			(pintype "passive")
			(solder_mask_margin 0.102)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "3" smd rect
			(at -2.075 1.075)
			(size 1.05 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 37 "/Human-Machine Interface/Keypad/ROW3")
			(pintype "passive")
			(solder_mask_margin 0.102)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "4" smd rect
			(at 2.075 1.075)
			(size 1.05 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 37 "/Human-Machine Interface/Keypad/ROW3")
			(pintype "passive")
			(solder_mask_margin 0.102)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "C:/Users/zackp/OneDrive/Desktop/434133025816/Download_STP_4341x30258x6+%28rev1%29.stp"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 90 -180 90)
			)
		)
	)
	(footprint "capstone-project:PEC11J9215FS0015"
		(layer "F.Cu")
		(at 113.7 115.65 90)
		(descr "PEC11J-9215F-S0015")
		(tags "Undefined or Miscellaneous")
		(property "Reference" "U1"
			(at 2.65 0.987539 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "PEC11J-9215F-S0015"
			(at 0 0.6 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" "http://www.bourns.com/docs/Product-Datasheets/PEC11J.pdf"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Rotary Encoder Mechanical 12 mm SMD Long Life Encoder"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Height" "19.5"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Part Number" "652-PEC11J9215FS0015"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Price/Stock" "https://www.mouser.co.uk/ProductDetail/Bourns/PEC11J-9215F-S0015?qs=11PymoJGorKONEyHv%252BPUyw%3D%3D"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Name" "Bourns"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Part_Number" "PEC11J-9215F-S0015"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/Human-Machine Interface/")
		(sheetfile "human-machine-interface.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 0.6 90)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole circle
			(at 0 0 90)
			(size 2.05 2.05)
			(drill 2.05)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 4.5 90)
			(size 2.69 2.69)
			(drill 2.69)
			(layers "*.Cu" "*.Mask")
		)
		(pad "A1" smd rect
			(at -2.5 7.3 90)
			(size 1.3 2.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "Net-(C1-Pad1)")
			(pinfunction "A1")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "B1" smd rect
			(at 2.5 7.3 90)
			(size 1.3 2.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 3 "Net-(C2-Pad1)")
			(pinfunction "B1")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "C1" smd rect
			(at 0 7.3 90)
			(size 1.3 2.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 26 "+3.3V")
			(pinfunction "C1")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "D1" smd rect
			(at -2.5 -7 90)
			(size 1.3 2.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "COM")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "E1" smd rect
			(at 2.5 -7 90)
			(size 1.3 2.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 39 "/Human-Machine Interface/ENC_SW")
			(pinfunction "NO")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "MP1" smd rect
			(at -6.375 0 90)
			(size 3.75 4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "MP1")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "MP2" smd rect
			(at 6.375 0 90)
			(size 3.75 4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "MP2")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "MP3" smd rect
			(at -5 -7.9 90)
			(size 2.5 3.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "MP3")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "MP4" smd rect
			(at 5 -7.9 90)
			(size 2.5 3.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "MP4")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "MP5" smd rect
			(at -5 7.9 90)
			(size 2.5 3.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "MP5")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "MP6" smd rect
			(at 5 7.9 90)
			(size 2.5 3.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "MP6")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KIPRJMOD}/capstone-project.pretty/3dmodels/PEC11J-9215F-S0015.step"
			(offset
				(xyz 0 -0.2 2.749999959)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 0 -180)
			)
		)
	)
	(footprint "LOGO"
		(layer "F.Cu")
		(at 131.2 131.1)
		(property "Reference" "G***"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "LOGO"
			(at 0.75 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr board_only exclude_from_pos_files exclude_from_bom)
		(embedded_fonts no)
	)
	(footprint "MountingHole:MountingHole_3.2mm_M3_ISO14580_Pad"
		(layer "F.Cu")
		(at 126.950188 83.099792)
		(descr "Mounting Hole 3.2mm, M3, generated by kicad-footprint-generator mountinghole.py")
		(tags "mountinghole M3 ISO14580")
		(property "Reference" "H1"
			(at 0 -3.7 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "M3"
			(at 0 3.7 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Mounting Hole with connection"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "MountingHole*Pad*")
		(sheetname "/")
		(sheetfile "HMI.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 5.5 5.5)
			(drill 3.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "1")
			(pintype "input")
			(zone_connect 2)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 123.7 87.225 90)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C4"
			(at 2.025 0.1 180)
			(layer "F.SilkS")
		)
		(property "Value" "0.1uF"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "capacitor, US symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/Human-Machine Interface/Audio/")
		(sheetfile "untitled.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 90)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 26 "+3.3V")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at 0.775 0 90)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "capstone-project:434133025816"
		(layer "F.Cu")
		(at 117.063525 99.513525)
		(property "Reference" "S13"
			(at -0.1 0.186475 0)
			(layer "F.SilkS")
		)
		(property "Value" "434133025816"
			(at 2.7768 2.7936 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/Human-Machine Interface/Keypad/")
		(sheetfile "../Projects/capstone-project/Hardware/KiCAD/system-testbed/keypad.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -2.075 -1.075)
			(size 1.05 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 7 "Net-(D1:4-A)")
			(pintype "passive")
			(solder_mask_margin 0.102)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd rect
			(at 2.075 -1.075)
			(size 1.05 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 7 "Net-(D1:4-A)")
			(pintype "passive")
			(solder_mask_margin 0.102)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "3" smd rect
			(at -2.075 1.075)
			(size 1.05 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 42 "/Human-Machine Interface/Keypad/ROW1")
			(pintype "passive")
			(solder_mask_margin 0.102)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "4" smd rect
			(at 2.075 1.075)
			(size 1.05 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 42 "/Human-Machine Interface/Keypad/ROW1")
			(pintype "passive")
			(solder_mask_margin 0.102)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "C:/Users/zackp/OneDrive/Desktop/434133025816/Download_STP_4341x30258x6+%28rev1%29.stp"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 90 -180 90)
			)
		)
	)
	(footprint "capstone-project:434133025816"
		(layer "F.Cu")
		(at 88.4834 108.5)
		(property "Reference" "S5"
			(at 0.15 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "434133025816"
			(at 2.7768 2.7936 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/Human-Machine Interface/Keypad/")
		(sheetfile "../Projects/capstone-project/Hardware/KiCAD/system-testbed/keypad.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -2.075 -1.075)
			(size 1.05 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 5 "Net-(D1:2-A)")
			(pintype "passive")
			(solder_mask_margin 0.102)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd rect
			(at 2.075 -1.075)
			(size 1.05 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 5 "Net-(D1:2-A)")
			(pintype "passive")
			(solder_mask_margin 0.102)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "3" smd rect
			(at -2.075 1.075)
			(size 1.05 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 42 "/Human-Machine Interface/Keypad/ROW1")
			(pintype "passive")
			(solder_mask_margin 0.102)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "4" smd rect
			(at 2.075 1.075)
			(size 1.05 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 42 "/Human-Machine Interface/Keypad/ROW1")
			(pintype "passive")
			(solder_mask_margin 0.102)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "C:/Users/zackp/OneDrive/Desktop/434133025816/Download_STP_4341x30258x6+%28rev1%29.stp"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 90 -180 90)
			)
		)
	)
	(footprint "capstone-project:434133025816"
		(layer "F.Cu")
		(at 104.878012 99.483471)
		(property "Reference" "S16"
			(at 0.15 0.016529 0)
			(layer "F.SilkS")
		)
		(property "Value" "434133025816"
			(at 2.7768 2.7936 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/Human-Machine Interface/Keypad/")
		(sheetfile "../Projects/capstone-project/Hardware/KiCAD/system-testbed/keypad.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -2.075 -1.075)
			(size 1.05 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 19 "Net-(D4:4-A)")
			(pintype "passive")
			(solder_mask_margin 0.102)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd rect
			(at 2.075 -1.075)
			(size 1.05 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 19 "Net-(D4:4-A)")
			(pintype "passive")
			(solder_mask_margin 0.102)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "3" smd rect
			(at -2.075 1.075)
			(size 1.05 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 43 "/Human-Machine Interface/Keypad/ROW4")
			(pintype "passive")
			(solder_mask_margin 0.102)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "4" smd rect
			(at 2.075 1.075)
			(size 1.05 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 43 "/Human-Machine Interface/Keypad/ROW4")
			(pintype "passive")
			(solder_mask_margin 0.102)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "C:/Users/zackp/OneDrive/Desktop/434133025816/Download_STP_4341x30258x6+%28rev1%29.stp"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 90 -180 90)
			)
		)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "F.Cu")
		(at 114.3 80.4)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "Vin"
			(at 1.9 0.1 0)
			(layer "F.SilkS")
		)
		(property "Value" "TestPoint"
			(at 0 1.55 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/Human-Machine Interface/")
		(sheetfile "human-machine-interface.kicad_sch")
		(attr exclude_from_pos_files)
		(pad "1" smd circle
			(at 0 0)
			(size 1 1)
			(layers "F.Cu" "F.Mask")
			(net 26 "+3.3V")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "capstone-project:434133025816"
		(layer "F.Cu")
		(at 81.1625 108.4)
		(property "Reference" "S2"
			(at 0.15 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "434133025816"
			(at 2.7768 2.7936 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/Human-Machine Interface/Keypad/")
		(sheetfile "../Projects/capstone-project/Hardware/KiCAD/system-testbed/keypad.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -2.075 -1.075)
			(size 1.05 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 4 "Net-(D1:1-A)")
			(pintype "passive")
			(solder_mask_margin 0.102)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd rect
			(at 2.075 -1.075)
			(size 1.05 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 4 "Net-(D1:1-A)")
			(pintype "passive")
			(solder_mask_margin 0.102)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "3" smd rect
			(at -2.075 1.075)
			(size 1.05 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 42 "/Human-Machine Interface/Keypad/ROW1")
			(pintype "passive")
			(solder_mask_margin 0.102)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "4" smd rect
			(at 2.075 1.075)
			(size 1.05 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 42 "/Human-Machine Interface/Keypad/ROW1")
			(pintype "passive")
			(solder_mask_margin 0.102)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "C:/Users/zackp/OneDrive/Desktop/434133025816/Download_STP_4341x30258x6+%28rev1%29.stp"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 90 -180 90)
			)
		)
	)
	(footprint "LOGO"
		(layer "F.Cu")
		(at 70.959616 131.288892)
		(property "Reference" "G***"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "LOGO"
			(at 0.75 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr board_only exclude_from_pos_files exclude_from_bom)
		(embedded_fonts no)
	)
	(footprint "capstone-project:434133025816"
		(layer "F.Cu")
		(at 95.85 113.15)
		(property "Reference" "S10"
			(at 0.1 -0.15 0)
			(layer "F.SilkS")
		)
		(property "Value" "434133025816"
			(at 2.7768 2.7936 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/Human-Machine Interface/Keypad/")
		(sheetfile "../Projects/capstone-project/Hardware/KiCAD/system-testbed/keypad.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -2.075 -1.075)
			(size 1.05 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 10 "Net-(D2:3-A)")
			(pintype "passive")
			(solder_mask_margin 0.102)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd rect
			(at 2.075 -1.075)
			(size 1.05 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 10 "Net-(D2:3-A)")
			(pintype "passive")
			(solder_mask_margin 0.102)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "3" smd rect
			(at -2.075 1.075)
			(size 1.05 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 41 "/Human-Machine Interface/Keypad/ROW2")
			(pintype "passive")
			(solder_mask_margin 0.102)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "4" smd rect
			(at 2.075 1.075)
			(size 1.05 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 41 "/Human-Machine Interface/Keypad/ROW2")
			(pintype "passive")
			(solder_mask_margin 0.102)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "C:/Users/zackp/OneDrive/Desktop/434133025816/Download_STP_4341x30258x6+%28rev1%29.stp"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 90 -180 90)
			)
		)
	)
	(footprint "Package_DFN_QFN:TQFN-16-1EP_3x3mm_P0.5mm_EP1.23x1.23mm"
		(layer "F.Cu")
		(at 130.59 123.59)
		(descr "TQFN, 16 Pin (https://pdfserv.maximintegrated.com/package_dwgs/21-0136.PDF (T1633-5), https://pdfserv.maximintegrated.com/land_patterns/90-0032.PDF), generated with kicad-footprint-generator ipc_noLead_generator.py")
		(tags "TQFN NoLead")
		(property "Reference" "U2"
			(at -1.99 2.31 0)
			(layer "F.SilkS")
		)
		(property "Value" "MAX98357A"
			(at 0 2.8 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/MAX98357A-MAX98357B.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Mono DAC with amplifier, I2S, PCM, TDM, 32-bit, 96khz, 3.2W, TQFP-16"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TQFN*3x3mm*P0.5mm*EP1.23x1.23mm*")
		(sheetname "/Human-Machine Interface/Audio/")
		(sheetfile "untitled.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "" smd roundrect
			(at -0.31 -0.31)
			(size 0.5 0.5)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "" smd roundrect
			(at -0.31 0.31)
			(size 0.5 0.5)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "" smd roundrect
			(at 0.31 -0.31)
			(size 0.5 0.5)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "" smd roundrect
			(at 0.31 0.31)
			(size 0.5 0.5)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "1" smd roundrect
			(at -1.4375 -0.75)
			(size 0.825 0.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 76 "/Human-Machine Interface/AMP_DIN")
			(pinfunction "DIN")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at -1.4375 -0.25)
			(size 0.825 0.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 60 "/Human-Machine Interface/Audio/GAIN_SLOT")
			(pinfunction "GAIN_SLOT")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "3" smd roundrect
			(at -1.4375 0.25)
			(size 0.825 0.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "4" smd roundrect
			(at -1.4375 0.75)
			(size 0.825 0.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 59 "/Human-Machine Interface/Audio/~{SD_MODE}")
			(pinfunction "~{SD_MODE}")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "5" smd roundrect
			(at -0.75 1.4375)
			(size 0.25 0.825)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 67 "unconnected-(U2-NC-Pad5)")
			(pinfunction "NC")
			(pintype "no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "6" smd roundrect
			(at -0.25 1.4375)
			(size 0.25 0.825)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 69 "unconnected-(U2-NC-Pad6)")
			(pinfunction "NC")
			(pintype "no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "7" smd roundrect
			(at 0.25 1.4375)
			(size 0.25 0.825)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 26 "+3.3V")
			(pinfunction "VDD")
			(pintype "power_in")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "8" smd roundrect
			(at 0.75 1.4375)
			(size 0.25 0.825)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 26 "+3.3V")
			(pinfunction "VDD")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "9" smd roundrect
			(at 1.4375 0.75)
			(size 0.825 0.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 63 "Net-(U2-OUTP)")
			(pinfunction "OUTP")
			(pintype "output")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "10" smd roundrect
			(at 1.4375 0.25)
			(size 0.825 0.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 62 "Net-(U2-OUTN)")
			(pinfunction "OUTN")
			(pintype "output")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "11" smd roundrect
			(at 1.4375 -0.25)
			(size 0.825 0.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "12" smd roundrect
			(at 1.4375 -0.75)
			(size 0.825 0.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 68 "unconnected-(U2-NC-Pad12)")
			(pinfunction "NC")
			(pintype "no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "13" smd roundrect
			(at 0.75 -1.4375)
			(size 0.25 0.825)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 66 "unconnected-(U2-NC-Pad13)")
			(pinfunction "NC")
			(pintype "no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "14" smd roundrect
			(at 0.25 -1.4375)
			(size 0.25 0.825)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 73 "/Human-Machine Interface/LRCLK")
			(pinfunction "LRCLK")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "15" smd roundrect
			(at -0.25 -1.4375)
			(size 0.25 0.825)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "16" smd roundrect
			(at -0.75 -1.4375)
			(size 0.25 0.825)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 71 "/Human-Machine Interface/BCLK")
			(pinfunction "BCLK")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "17" smd rect
			(at 0 0)
			(size 1.23 1.23)
			(property pad_prop_heatsink)
			(layers "F.Cu" "F.Mask")
			(net 1 "GND")
			(pinfunction "PAD")
			(pintype "unspecified")
			(zone_connect 2)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Package_DFN_QFN.3dshapes/TQFN-16-1EP_3x3mm_P0.5mm_EP1.23x1.23mm.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 130.6 118)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C7"
			(at 0.14058 1.5 0)
			(layer "F.SilkS")
		)
		(property "Value" "22pF"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/Human-Machine Interface/Audio/")
		(sheetfile "untitled.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 71 "/Human-Machine Interface/BCLK")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at 0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "F.Cu")
		(at 112.8 83.5)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TPAMP1"
			(at 3.2 0.1 0)
			(layer "F.SilkS")
		)
		(property "Value" "~"
			(at 0 1.55 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/Human-Machine Interface/Audio/")
		(sheetfile "untitled.kicad_sch")
		(attr exclude_from_pos_files)
		(pad "1" smd circle
			(at 0 0)
			(size 1 1)
			(layers "F.Cu" "F.Mask")
			(net 76 "/Human-Machine Interface/AMP_DIN")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "LOGO"
		(layer "F.Cu")
		(at 129.6 87.5)
		(property "Reference" "G***"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "LOGO"
			(at 0.75 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr board_only exclude_from_pos_files exclude_from_bom)
		(embedded_fonts no)
	)
	(footprint "capstone-project:434133025816"
		(layer "F.Cu")
		(at 111.009703 103.486475)
		(property "Reference" "S15"
			(at -0.009703 0.013525 0)
			(layer "F.SilkS")
		)
		(property "Value" "434133025816"
			(at 2.7768 2.7936 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/Human-Machine Interface/Keypad/")
		(sheetfile "../Projects/capstone-project/Hardware/KiCAD/system-testbed/keypad.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -2.075 -1.075)
			(size 1.05 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 15 "Net-(D3:4-A)")
			(pintype "passive")
			(solder_mask_margin 0.102)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd rect
			(at 2.075 -1.075)
			(size 1.05 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 15 "Net-(D3:4-A)")
			(pintype "passive")
			(solder_mask_margin 0.102)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "3" smd rect
			(at -2.075 1.075)
			(size 1.05 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 37 "/Human-Machine Interface/Keypad/ROW3")
			(pintype "passive")
			(solder_mask_margin 0.102)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "4" smd rect
			(at 2.075 1.075)
			(size 1.05 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 37 "/Human-Machine Interface/Keypad/ROW3")
			(pintype "passive")
			(solder_mask_margin 0.102)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "C:/Users/zackp/OneDrive/Desktop/434133025816/Download_STP_4341x30258x6+%28rev1%29.stp"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 90 -180 90)
			)
		)
	)
	(footprint "capstone-project:434133025816"
		(layer "F.Cu")
		(at 95.85 122.45)
		(property "Reference" "S12"
			(at 0.1 -0.05 0)
			(layer "F.SilkS")
		)
		(property "Value" "434133025816"
			(at 2.7768 2.7936 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/Human-Machine Interface/Keypad/")
		(sheetfile "../Projects/capstone-project/Hardware/KiCAD/system-testbed/keypad.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -2.075 -1.075)
			(size 1.05 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 18 "Net-(D4:3-A)")
			(pintype "passive")
			(solder_mask_margin 0.102)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd rect
			(at 2.075 -1.075)
			(size 1.05 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 18 "Net-(D4:3-A)")
			(pintype "passive")
			(solder_mask_margin 0.102)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "3" smd rect
			(at -2.075 1.075)
			(size 1.05 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 43 "/Human-Machine Interface/Keypad/ROW4")
			(pintype "passive")
			(solder_mask_margin 0.102)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "4" smd rect
			(at 2.075 1.075)
			(size 1.05 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 43 "/Human-Machine Interface/Keypad/ROW4")
			(pintype "passive")
			(solder_mask_margin 0.102)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "C:/Users/zackp/OneDrive/Desktop/434133025816/Download_STP_4341x30258x6+%28rev1%29.stp"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 90 -180 90)
			)
		)
	)
	(footprint "capstone-project:434133025816"
		(layer "F.Cu")
		(at 81.1625 113.1)
		(property "Reference" "S3"
			(at 0.15 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "434133025816"
			(at 2.7768 2.7936 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/Human-Machine Interface/Keypad/")
		(sheetfile "../Projects/capstone-project/Hardware/KiCAD/system-testbed/keypad.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -2.075 -1.075)
			(size 1.05 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 8 "Net-(D2:1-A)")
			(pintype "passive")
			(solder_mask_margin 0.102)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd rect
			(at 2.075 -1.075)
			(size 1.05 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 8 "Net-(D2:1-A)")
			(pintype "passive")
			(solder_mask_margin 0.102)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "3" smd rect
			(at -2.075 1.075)
			(size 1.05 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 41 "/Human-Machine Interface/Keypad/ROW2")
			(pintype "passive")
			(solder_mask_margin 0.102)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "4" smd rect
			(at 2.075 1.075)
			(size 1.05 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 41 "/Human-Machine Interface/Keypad/ROW2")
			(pintype "passive")
			(solder_mask_margin 0.102)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "C:/Users/zackp/OneDrive/Desktop/434133025816/Download_STP_4341x30258x6+%28rev1%29.stp"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 90 -180 90)
			)
		)
	)
	(footprint "capstone-project:434133025816"
		(layer "F.Cu")
		(at 81.146515 122.441804)
		(property "Reference" "S4"
			(at 0.15 -0.041804 0)
			(layer "F.SilkS")
		)
		(property "Value" "434133025816"
			(at 2.7768 2.7936 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/Human-Machine Interface/Keypad/")
		(sheetfile "../Projects/capstone-project/Hardware/KiCAD/system-testbed/keypad.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -2.075 -1.075)
			(size 1.05 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 16 "Net-(D4:1-A)")
			(pintype "passive")
			(solder_mask_margin 0.102)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd rect
			(at 2.075 -1.075)
			(size 1.05 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 16 "Net-(D4:1-A)")
			(pintype "passive")
			(solder_mask_margin 0.102)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "3" smd rect
			(at -2.075 1.075)
			(size 1.05 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 43 "/Human-Machine Interface/Keypad/ROW4")
			(pintype "passive")
			(solder_mask_margin 0.102)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "4" smd rect
			(at 2.075 1.075)
			(size 1.05 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 43 "/Human-Machine Interface/Keypad/ROW4")
			(pintype "passive")
			(solder_mask_margin 0.102)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "C:/Users/zackp/OneDrive/Desktop/434133025816/Download_STP_4341x30258x6+%28rev1%29.stp"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 90 -180 90)
			)
		)
	)
	(footprint "capstone-project:434133025816"
		(layer "F.Cu")
		(at 95.85 108.5)
		(property "Reference" "S9"
			(at 0.15 -0.1 0)
			(layer "F.SilkS")
		)
		(property "Value" "434133025816"
			(at 2.7768 2.7936 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/Human-Machine Interface/Keypad/")
		(sheetfile "../Projects/capstone-project/Hardware/KiCAD/system-testbed/keypad.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -2.075 -1.075)
			(size 1.05 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 6 "Net-(D1:3-A)")
			(pintype "passive")
			(solder_mask_margin 0.102)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd rect
			(at 2.075 -1.075)
			(size 1.05 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 6 "Net-(D1:3-A)")
			(pintype "passive")
			(solder_mask_margin 0.102)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "3" smd rect
			(at -2.075 1.075)
			(size 1.05 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 42 "/Human-Machine Interface/Keypad/ROW1")
			(pintype "passive")
			(solder_mask_margin 0.102)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "4" smd rect
			(at 2.075 1.075)
			(size 1.05 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 42 "/Human-Machine Interface/Keypad/ROW1")
			(pintype "passive")
			(solder_mask_margin 0.102)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "C:/Users/zackp/OneDrive/Desktop/434133025816/Download_STP_4341x30258x6+%28rev1%29.stp"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 90 -180 90)
			)
		)
	)
	(footprint "Package_SO:SSOP-24_5.3x8.2mm_P0.65mm"
		(layer "F.Cu")
		(at 90.8 95.6 -90)
		(descr "SSOP, 24 Pin (JEDEC MO-150 variation AG, 1.75mm body thickness, https://www.jedec.org/document_search?search_api_views_fulltext=MO-150, https://ww1.microchip.com/downloads/en/PackagingSpec/00000049BQ.pdf#page=398, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/ltc-legacy-ssop/ssop_24_05-08-1640.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SSOP SO")
		(property "Reference" "IC1"
			(at 0 -5.05 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "PCF8575PWR"
			(at 0 5.05 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/pcf8575.pdf"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "16 Bits Port/Expander to I2C Bus, SSOP-24"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Height" "1.2"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Name" "Texas Instruments"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Part_Number" "PCF8575PWR"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Part Number" "595-PCF8575PWR"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Price/Stock" "https://www.mouser.co.uk/ProductDetail/Texas-Instruments/PCF8575PWR?qs=wgAEGBTxy7lfNLEoaenBaA%3D%3D"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Arrow Part Number" "PCF8575PWR"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Arrow Price/Stock" "https://www.arrow.com/en/products/pcf8575pwr/texas-instruments?region=nac"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SSOP*5.3x8.2mm*P0.65mm*")
		(sheetname "/Human-Machine Interface/")
		(sheetfile "human-machine-interface.kicad_sch")
		(attr smd)
		(pad "1" smd roundrect
			(at -3.5 -3.575 270)
			(size 1.9 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 72 "/Human-Machine Interface/~{PCF_INT}")
			(pinfunction "~{INT}")
			(pintype "open_collector")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at -3.5 -2.925 270)
			(size 1.9 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 56 "/Human-Machine Interface/PCF_A1")
			(pinfunction "A1")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "3" smd roundrect
			(at -3.5 -2.275 270)
			(size 1.9 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 54 "/Human-Machine Interface/PCF_A2")
			(pinfunction "A2")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "4" smd roundrect
			(at -3.5 -1.625 270)
			(size 1.9 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 77 "Net-(IC1-P0)")
			(pinfunction "P0")
			(pintype "bidirectional")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "5" smd roundrect
			(at -3.5 -0.975 270)
			(size 1.9 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 57 "unconnected-(IC1-P1-Pad5)")
			(pinfunction "P1")
			(pintype "bidirectional+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "6" smd roundrect
			(at -3.5 -0.325 270)
			(size 1.9 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 38 "/Human-Machine Interface/TFTRST")
			(pinfunction "P2")
			(pintype "bidirectional")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "7" smd roundrect
			(at -3.5 0.325 270)
			(size 1.9 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 20 "unconnected-(IC1-P3-Pad7)")
			(pinfunction "P3")
			(pintype "bidirectional")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "8" smd roundrect
			(at -3.5 0.975 270)
			(size 1.9 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 21 "unconnected-(IC1-P4-Pad8)")
			(pinfunction "P4")
			(pintype "bidirectional")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "9" smd roundrect
			(at -3.5 1.625 270)
			(size 1.9 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 39 "/Human-Machine Interface/ENC_SW")
			(pinfunction "P5")
			(pintype "bidirectional")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "10" smd roundrect
			(at -3.5 2.275 270)
			(size 1.9 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 44 "/Human-Machine Interface/ENC_DT")
			(pinfunction "P6")
			(pintype "bidirectional")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "11" smd roundrect
			(at -3.5 2.925 270)
			(size 1.9 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 40 "/Human-Machine Interface/ENC_CLK")
			(pinfunction "P7")
			(pintype "bidirectional")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "12" smd roundrect
			(at -3.5 3.575 270)
			(size 1.9 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "13" smd roundrect
			(at 3.5 3.575 270)
			(size 1.9 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 42 "/Human-Machine Interface/Keypad/ROW1")
			(pinfunction "P10")
			(pintype "bidirectional")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "14" smd roundrect
			(at 3.5 2.925 270)
			(size 1.9 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 41 "/Human-Machine Interface/Keypad/ROW2")
			(pinfunction "P11")
			(pintype "bidirectional")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "15" smd roundrect
			(at 3.5 2.275 270)
			(size 1.9 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 37 "/Human-Machine Interface/Keypad/ROW3")
			(pinfunction "P12")
			(pintype "bidirectional")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "16" smd roundrect
			(at 3.5 1.625 270)
			(size 1.9 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 43 "/Human-Machine Interface/Keypad/ROW4")
			(pinfunction "P13")
			(pintype "bidirectional")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "17" smd roundrect
			(at 3.5 0.975 270)
			(size 1.9 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 33 "/Human-Machine Interface/Keypad/COL1")
			(pinfunction "P14")
			(pintype "bidirectional")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "18" smd roundrect
			(at 3.5 0.325 270)
			(size 1.9 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 34 "/Human-Machine Interface/Keypad/COL2")
			(pinfunction "P15")
			(pintype "bidirectional")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "19" smd roundrect
			(at 3.5 -0.325 270)
			(size 1.9 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 35 "/Human-Machine Interface/Keypad/COL3")
			(pinfunction "P16")
			(pintype "bidirectional")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "20" smd roundrect
			(at 3.5 -0.975 270)
			(size 1.9 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 36 "/Human-Machine Interface/Keypad/COL4")
			(pinfunction "P17")
			(pintype "bidirectional")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "21" smd roundrect
			(at 3.5 -1.625 270)
			(size 1.9 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 55 "/Human-Machine Interface/PCF_A0")
			(pinfunction "A0")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "22" smd roundrect
			(at 3.5 -2.275 270)
			(size 1.9 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 23 "/SCL")
			(pinfunction "SCL")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "23" smd roundrect
			(at 3.5 -2.925 270)
			(size 1.9 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 22 "/SDA")
			(pinfunction "SDA")
			(pintype "bidirectional")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "24" smd roundrect
			(at 3.5 -3.575 270)
			(size 1.9 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 26 "+3.3V")
			(pinfunction "VCC")
			(pintype "power_in")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Package_SO.3dshapes/SSOP-24_5.3x8.2mm_P0.65mm.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "capstone-project:434133025816"
		(layer "F.Cu")
		(at 88.4834 117.8)
		(property "Reference" "S7"
			(at 0.1 -0.1 0)
			(layer "F.SilkS")
		)
		(property "Value" "434133025816"
			(at 2.7768 2.7936 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/Human-Machine Interface/Keypad/")
		(sheetfile "../Projects/capstone-project/Hardware/KiCAD/system-testbed/keypad.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -2.075 -1.075)
			(size 1.05 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 13 "Net-(D3:2-A)")
			(pintype "passive")
			(solder_mask_margin 0.102)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd rect
			(at 2.075 -1.075)
			(size 1.05 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 13 "Net-(D3:2-A)")
			(pintype "passive")
			(solder_mask_margin 0.102)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "3" smd rect
			(at -2.075 1.075)
			(size 1.05 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 37 "/Human-Machine Interface/Keypad/ROW3")
			(pintype "passive")
			(solder_mask_margin 0.102)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "4" smd rect
			(at 2.075 1.075)
			(size 1.05 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 37 "/Human-Machine Interface/Keypad/ROW3")
			(pintype "passive")
			(solder_mask_margin 0.102)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "C:/Users/zackp/OneDrive/Desktop/434133025816/Download_STP_4341x30258x6+%28rev1%29.stp"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 90 -180 90)
			)
		)
	)
	(footprint "capstone-project:434133025816"
		(layer "F.Cu")
		(at 88.4834 122.45)
		(property "Reference" "S8"
			(at 0.1 -0.15 0)
			(layer "F.SilkS")
		)
		(property "Value" "434133025816"
			(at 2.7768 2.7936 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/Human-Machine Interface/Keypad/")
		(sheetfile "../Projects/capstone-project/Hardware/KiCAD/system-testbed/keypad.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -2.075 -1.075)
			(size 1.05 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 17 "Net-(D4:2-A)")
			(pintype "passive")
			(solder_mask_margin 0.102)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd rect
			(at 2.075 -1.075)
			(size 1.05 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 17 "Net-(D4:2-A)")
			(pintype "passive")
			(solder_mask_margin 0.102)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "3" smd rect
			(at -2.075 1.075)
			(size 1.05 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 43 "/Human-Machine Interface/Keypad/ROW4")
			(pintype "passive")
			(solder_mask_margin 0.102)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "4" smd rect
			(at 2.075 1.075)
			(size 1.05 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 43 "/Human-Machine Interface/Keypad/ROW4")
			(pintype "passive")
			(solder_mask_margin 0.102)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "C:/Users/zackp/OneDrive/Desktop/434133025816/Download_STP_4341x30258x6+%28rev1%29.stp"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 90 -180 90)
			)
		)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "F.Cu")
		(at 84 82.8)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP1"
			(at 0 -1.448 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 1.55 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/Human-Machine Interface/")
		(sheetfile "human-machine-interface.kicad_sch")
		(attr exclude_from_pos_files)
		(fp_text user "${REFERENCE}"
			(at 0 -1.45 0)
			(layer "F.Fab")
		)
		(pad "1" smd circle
			(at 0 0)
			(size 1 1)
			(layers "F.Cu" "F.Mask")
			(net 45 "/Human-Machine Interface/LITE")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "capstone-project:434133025816"
		(layer "F.Cu")
		(at 110.996315 95.507244)
		(property "Reference" "S14"
			(at 0.003685 0.092756 0)
			(layer "F.SilkS")
		)
		(property "Value" "434133025816"
			(at 2.7768 2.7936 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/Human-Machine Interface/Keypad/")
		(sheetfile "../Projects/capstone-project/Hardware/KiCAD/system-testbed/keypad.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -2.075 -1.075)
			(size 1.05 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 11 "Net-(D2:4-A)")
			(pintype "passive")
			(solder_mask_margin 0.102)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd rect
			(at 2.075 -1.075)
			(size 1.05 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 11 "Net-(D2:4-A)")
			(pintype "passive")
			(solder_mask_margin 0.102)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "3" smd rect
			(at -2.075 1.075)
			(size 1.05 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 41 "/Human-Machine Interface/Keypad/ROW2")
			(pintype "passive")
			(solder_mask_margin 0.102)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "4" smd rect
			(at 2.075 1.075)
			(size 1.05 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 41 "/Human-Machine Interface/Keypad/ROW2")
			(pintype "passive")
			(solder_mask_margin 0.102)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "C:/Users/zackp/OneDrive/Desktop/434133025816/Download_STP_4341x30258x6+%28rev1%29.stp"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 90 -180 90)
			)
		)
	)
	(footprint "MountingHole:MountingHole_3.2mm_M3_ISO14580_Pad"
		(layer "F.Cu")
		(at 74.763353 83.099941)
		(descr "Mounting Hole 3.2mm, M3, generated by kicad-footprint-generator mountinghole.py")
		(tags "mountinghole M3 ISO14580")
		(property "Reference" "H2"
			(at 0 -3.7 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "M3"
			(at 0 3.7 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Mounting Hole with connection"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "MountingHole*Pad*")
		(sheetname "/")
		(sheetfile "HMI.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 5.5 5.5)
			(drill 3.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "1")
			(pintype "input")
			(zone_connect 2)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
	)
	(footprint "capstone-project:434133025816"
		(layer "F.Cu")
		(at 88.4834 113.15)
		(property "Reference" "S6"
			(at 0.1 -0.05 0)
			(layer "F.SilkS")
		)
		(property "Value" "434133025816"
			(at 2.7768 2.7936 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/Human-Machine Interface/Keypad/")
		(sheetfile "../Projects/capstone-project/Hardware/KiCAD/system-testbed/keypad.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -2.075 -1.075)
			(size 1.05 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 9 "Net-(D2:2-A)")
			(pintype "passive")
			(solder_mask_margin 0.102)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd rect
			(at 2.075 -1.075)
			(size 1.05 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 9 "Net-(D2:2-A)")
			(pintype "passive")
			(solder_mask_margin 0.102)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "3" smd rect
			(at -2.075 1.075)
			(size 1.05 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 41 "/Human-Machine Interface/Keypad/ROW2")
			(pintype "passive")
			(solder_mask_margin 0.102)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "4" smd rect
			(at 2.075 1.075)
			(size 1.05 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 41 "/Human-Machine Interface/Keypad/ROW2")
			(pintype "passive")
			(solder_mask_margin 0.102)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "C:/Users/zackp/OneDrive/Desktop/434133025816/Download_STP_4341x30258x6+%28rev1%29.stp"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 90 -180 90)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 122.1 87.225 90)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C3"
			(at 2.025 0 180)
			(layer "F.SilkS")
		)
		(property "Value" "1uF"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "capacitor, US symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/Human-Machine Interface/Audio/")
		(sheetfile "untitled.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 90)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 26 "+3.3V")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at 0.775 0 90)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Diode_SMD:D_0603_1608Metric"
		(layer "B.Cu")
		(at 88.4625 117.858 180)
		(descr "Diode SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
		(tags "diode")
		(property "Reference" "D3:2"
			(at 0 1.43 0)
			(layer "B.SilkS")
		)
		(property "Value" "D"
			(at 0 -1.43 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Diode, small symbol, filled shape"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sim.Device" "D"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TO-???* *_Diode_* *SingleDiode* D_*")
		(sheetname "/Human-Machine Interface/Keypad/")
		(sheetfile "../Projects/capstone-project/Hardware/KiCAD/system-testbed/keypad.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.7875 0 180)
			(size 0.875 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 34 "/Human-Machine Interface/Keypad/COL2")
			(pinfunction "K")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at 0.7875 0 180)
			(size 0.875 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 13 "Net-(D3:2-A)")
			(pinfunction "A")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Diode_SMD.3dshapes/D_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "capstone-project:Adafruit EYESPI FPC Connector"
		(layer "B.Cu")
		(at 90.160249 82.268651)
		(descr "WR-FPC SMT ZIF Horizontal Hinge Type")
		(tags "EYESPI, FPC")
		(property "Reference" "X2"
			(at 7.874 -2.032 0)
			(layer "B.SilkS")
		)
		(property "Value" "EYESPI"
			(at 0 -4.064 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "https://www.we-online.com/components/products/datasheet/687118149022.pdf"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "WR-FPC SMT ZIF Horizontal Hinge Type"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(sheetname "/Human-Machine Interface/")
		(sheetfile "human-machine-interface.kicad_sch")
		(attr smd allow_soldermask_bridges)
		(pad "1" smd rect
			(at -4.25 3.35)
			(size 0.3 1.3)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 26 "+3.3V")
			(pintype "passive")
			(solder_mask_margin 0.102)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd rect
			(at -3.75 3.35)
			(size 0.3 1.3)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 45 "/Human-Machine Interface/LITE")
			(pintype "passive")
			(solder_mask_margin 0.102)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "3" smd rect
			(at -3.25 3.35)
			(size 0.3 1.3)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 1 "GND")
			(pintype "passive")
			(solder_mask_margin 0.102)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "4" smd rect
			(at -2.75 3.35)
			(size 0.3 1.3)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 30 "/SCK")
			(pintype "passive")
			(solder_mask_margin 0.102)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "5" smd rect
			(at -2.25 3.35)
			(size 0.3 1.3)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 32 "/MOSI")
			(pintype "passive")
			(solder_mask_margin 0.102)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "6" smd rect
			(at -1.75 3.35)
			(size 0.3 1.3)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 29 "/MISO")
			(pintype "passive")
			(solder_mask_margin 0.102)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "7" smd rect
			(at -1.25 3.35)
			(size 0.3 1.3)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 24 "/TFTDC")
			(pintype "passive")
			(solder_mask_margin 0.102)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "8" smd rect
			(at -0.75 3.35)
			(size 0.3 1.3)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 38 "/Human-Machine Interface/TFTRST")
			(pintype "passive")
			(solder_mask_margin 0.102)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "9" smd rect
			(at -0.25 3.35)
			(size 0.3 1.3)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 27 "/TFTCS")
			(pintype "passive")
			(solder_mask_margin 0.102)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "10" smd rect
			(at 0.25 3.35)
			(size 0.3 1.3)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 28 "/CARDCS")
			(pintype "passive")
			(solder_mask_margin 0.102)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "11" smd rect
			(at 0.75 3.35)
			(size 0.3 1.3)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 50 "unconnected-(X2-Pad11)")
			(pintype "passive+no_connect")
			(solder_mask_margin 0.102)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "12" smd rect
			(at 1.25 3.35)
			(size 0.3 1.3)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 49 "unconnected-(X2-Pad12)")
			(pintype "passive+no_connect")
			(solder_mask_margin 0.102)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "13" smd rect
			(at 1.75 3.35)
			(size 0.3 1.3)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 52 "unconnected-(X2-Pad13)")
			(pintype "passive+no_connect")
			(solder_mask_margin 0.102)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "14" smd rect
			(at 2.25 3.35)
			(size 0.3 1.3)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 47 "unconnected-(X2-Pad14)")
			(pintype "passive+no_connect")
			(solder_mask_margin 0.102)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "15" smd rect
			(at 2.75 3.35)
			(size 0.3 1.3)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 46 "unconnected-(X2-Pad15)")
			(pintype "passive+no_connect")
			(solder_mask_margin 0.102)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "16" smd rect
			(at 3.25 3.35)
			(size 0.3 1.3)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 48 "unconnected-(X2-Pad16)")
			(pintype "passive+no_connect")
			(solder_mask_margin 0.102)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "17" smd rect
			(at 3.75 3.35)
			(size 0.3 1.3)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 51 "unconnected-(X2-Pad17)")
			(pintype "passive+no_connect")
			(solder_mask_margin 0.102)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "18" smd rect
			(at 4.25 3.35)
			(size 0.3 1.3)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 53 "unconnected-(X2-Pad18)")
			(pintype "passive+no_connect")
			(solder_mask_margin 0.102)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "Z1" smd rect
			(at -6.05 0.6)
			(size 2 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 1 "GND")
			(pintype "passive")
			(solder_mask_margin 0.102)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "Z2" smd rect
			(at 6.05 0.6)
			(size 2 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 1 "GND")
			(pintype "passive")
			(solder_mask_margin 0.102)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KIPRJMOD}/capstone-project.pretty/3dmodels/687118149022+(rev1).step"
			(offset
				(xyz 0 0.5 1.15)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -0 -0 -0)
			)
		)
	)
	(footprint "Diode_SMD:D_0603_1608Metric"
		(layer "B.Cu")
		(at 95.8041 108.458 180)
		(descr "Diode SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
		(tags "diode")
		(property "Reference" "D1:3"
			(at -0.0459 1.4 0)
			(layer "B.SilkS")
		)
		(property "Value" "D"
			(at 0 -1.43 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Diode, small symbol, filled shape"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sim.Device" "D"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TO-???* *_Diode_* *SingleDiode* D_*")
		(sheetname "/Human-Machine Interface/Keypad/")
		(sheetfile "../Projects/capstone-project/Hardware/KiCAD/system-testbed/keypad.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.7875 0 180)
			(size 0.875 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 35 "/Human-Machine Interface/Keypad/COL3")
			(pinfunction "K")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at 0.7875 0 180)
			(size 0.875 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 6 "Net-(D1:3-A)")
			(pinfunction "A")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Diode_SMD.3dshapes/D_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Sensor_Audio:InvenSense_ICS-43434-6_3.5x2.65mm"
		(layer "B.Cu")
		(at 126.542 88.5 -90)
		(descr "TDK InvenSense MEMS I2S Microphone: https://invensense.tdk.com/products/ics-43434/")
		(tags "microphone MEMS I2S ICS-43434 TDK InvenSense")
		(property "Reference" "MK1"
			(at -0.1 -2.558 90)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "ICS-43434"
			(at 0 -2.9 90)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Datasheet" "https://www.invensense.com/wp-content/uploads/2016/02/DS-000069-ICS-43434-v1.2.pdf"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "TDK InvenSense MEMS Microphone, 24-bit I2S, 65 dBA SNR, LGA-6"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "InvenSense*ICS*43434*")
		(sheetname "/Human-Machine Interface/Audio/")
		(sheetfile "untitled.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -0.01 0)
			(unlocked yes)
			(layer "B.Fab")
		)
		(pad "" np_thru_hole circle
			(at 0 -0.71 270)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "*.Mask")
		)
		(pad "1" smd rect
			(at -0.9 1.364 270)
			(size 0.6 0.522)
			(layers "B.Cu" "B.Mask")
			(net 73 "/Human-Machine Interface/LRCLK")
			(pinfunction "WS")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd rect
			(at -0.9 0.542 270)
			(size 0.6 0.522)
			(layers "B.Cu" "B.Mask")
			(net 64 "Net-(MK1-LR)")
			(pinfunction "LR")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "3" smd custom
			(at 0.6625 -0.71 180)
			(size 0.3 0.3)
			(layers "B.Cu" "B.Mask")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(options
				(clearance outline)
				(anchor circle)
			)
			(primitives
				(gr_circle
					(center 0 0.6625)
					(end 0.6625 0.6625)
					(width 0.3)
					(fill no)
				)
			)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "4" smd rect
			(at 0.9 0.542 270)
			(size 0.6 0.522)
			(layers "B.Cu" "B.Mask")
			(net 71 "/Human-Machine Interface/BCLK")
			(pinfunction "SCK")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "5" smd rect
			(at 0.9 1.364 270)
			(size 0.6 0.522)
			(layers "B.Cu" "B.Mask")
			(net 26 "+3.3V")
			(pinfunction "VDD")
			(pintype "power_in")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "6" smd rect
			(at 0 1.364 270)
			(size 0.6 0.522)
			(layers "B.Cu" "B.Mask")
			(net 65 "Net-(MK1-SD)")
			(pinfunction "SD")
			(pintype "output")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Sensor_Audio.3dshapes/InvenSense_ICS-43434-6_3.5x2.65mm.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "capstone-project:434133025816"
		(layer "B.Cu")
		(at 80.9 88.7 -90)
		(property "Reference" "S17"
			(at -0.1 2.8064 90)
			(layer "B.SilkS")
		)
		(property "Value" "434133025816"
			(at 2.776801 -2.7936 90)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(sheetname "/Human-Machine Interface/")
		(sheetfile "human-machine-interface.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -2.075 1.075 270)
			(size 1.05 0.65)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 26 "+3.3V")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd rect
			(at 2.075 1.075 270)
			(size 1.05 0.65)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 26 "+3.3V")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "3" smd rect
			(at -2.075 -1.075 270)
			(size 1.05 0.65)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 77 "Net-(IC1-P0)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "4" smd rect
			(at 2.075 -1.075 270)
			(size 1.05 0.65)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 77 "Net-(IC1-P0)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
		(model "C:/Users/zackp/OneDrive/Desktop/434133025816/Download_STP_4341x30258x6+%28rev1%29.stp"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 90 -180 90)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "B.Cu")
		(at 117.204634 91.720446 90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R15"
			(at 0 -1.237792 90)
			(layer "B.SilkS")
		)
		(property "Value" "2k"
			(at 0 -1.43 90)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Human-Machine Interface/Audio/")
		(sheetfile "untitled.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 90)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 59 "/Human-Machine Interface/Audio/~{SD_MODE}")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at 0.825 0 90)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 75 "/Human-Machine Interface/~{AMP_SD}")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "B.Cu")
		(at 109.410845 114.135118 -90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R7"
			(at 0 -1.389155 90)
			(layer "B.SilkS")
		)
		(property "Value" "10k"
			(at 0 -1.43 90)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Human-Machine Interface/")
		(sheetfile "human-machine-interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 270)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 3 "Net-(C2-Pad1)")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at 0.825 0 270)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 26 "+3.3V")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Diode_SMD:D_0603_1608Metric"
		(layer "B.Cu")
		(at 88.4625 122.458 180)
		(descr "Diode SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
		(tags "diode")
		(property "Reference" "D4:2"
			(at 0 1.43 0)
			(layer "B.SilkS")
		)
		(property "Value" "D"
			(at 0 -1.43 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Diode, small symbol, filled shape"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sim.Device" "D"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TO-???* *_Diode_* *SingleDiode* D_*")
		(sheetname "/Human-Machine Interface/Keypad/")
		(sheetfile "../Projects/capstone-project/Hardware/KiCAD/system-testbed/keypad.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.7875 0 180)
			(size 0.875 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 34 "/Human-Machine Interface/Keypad/COL2")
			(pinfunction "K")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at 0.7875 0 180)
			(size 0.875 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 17 "Net-(D4:2-A)")
			(pinfunction "A")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Diode_SMD.3dshapes/D_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Diode_SMD:D_0603_1608Metric"
		(layer "B.Cu")
		(at 88.475 108.458 180)
		(descr "Diode SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
		(tags "diode")
		(property "Reference" "D1:2"
			(at -0.0125 1.4 0)
			(layer "B.SilkS")
		)
		(property "Value" "D"
			(at 0 -1.43 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Diode, small symbol, filled shape"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sim.Device" "D"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TO-???* *_Diode_* *SingleDiode* D_*")
		(sheetname "/Human-Machine Interface/Keypad/")
		(sheetfile "../Projects/capstone-project/Hardware/KiCAD/system-testbed/keypad.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.7875 0 180)
			(size 0.875 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 34 "/Human-Machine Interface/Keypad/COL2")
			(pinfunction "K")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at 0.7875 0 180)
			(size 0.875 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 5 "Net-(D1:2-A)")
			(pinfunction "A")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Diode_SMD.3dshapes/D_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Jumper:SolderJumper-3_P1.3mm_Open_RoundedPad1.0x1.5mm_NumberLabels"
		(layer "B.Cu")
		(at 132.9 116.9 -90)
		(descr "SMD Solder 3-pad Jumper, 1x1.5mm rounded Pads, 0.3mm gap, open, labeled with numbers")
		(tags "solder jumper open")
		(property "Reference" "JP6"
			(at 0 -1.9 90)
			(layer "B.SilkS")
		)
		(property "Value" "GAIN_{R}"
			(at 0 -1.9 90)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Solder Jumper, 3-pole, open"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SolderJumper*Open*")
		(sheetname "/Human-Machine Interface/Audio/")
		(sheetfile "untitled.kicad_sch")
		(zone_connect 1)
		(attr exclude_from_pos_files allow_soldermask_bridges)
		(fp_text user "1"
			(at -2.6 0 90)
			(layer "B.SilkS")
		)
		(fp_text user "3"
			(at 2.6 0 90)
			(layer "B.SilkS")
		)
		(pad "1" smd custom
			(at -1.3 0 270)
			(size 1 0.5)
			(layers "B.Cu" "B.Mask")
			(net 58 "Net-(JP4-C)")
			(pinfunction "A")
			(pintype "passive")
			(zone_connect 2)
			(thermal_bridge_angle 45)
			(options
				(clearance outline)
				(anchor rect)
			)
			(primitives
				(gr_circle
					(center 0 -0.25)
					(end 0.5 -0.25)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center 0 0.25)
					(end 0.5 0.25)
					(width 0)
					(fill yes)
				)
				(gr_poly
					(pts
						(xy 0.55 -0.75) (xy 0 -0.75) (xy 0 0.75) (xy 0.55 0.75)
					)
					(width 0)
					(fill yes)
				)
			)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd rect
			(at 0 0 270)
			(size 1 1.5)
			(layers "B.Cu" "B.Mask")
			(net 60 "/Human-Machine Interface/Audio/GAIN_SLOT")
			(pinfunction "C")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "3" smd custom
			(at 1.3 0 270)
			(size 1 0.5)
			(layers "B.Cu" "B.Mask")
			(net 61 "Net-(JP6-B)")
			(pinfunction "B")
			(pintype "passive")
			(zone_connect 2)
			(thermal_bridge_angle 45)
			(options
				(clearance outline)
				(anchor rect)
			)
			(primitives
				(gr_circle
					(center 0 -0.25)
					(end 0.5 -0.25)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center 0 0.25)
					(end 0.5 0.25)
					(width 0)
					(fill yes)
				)
				(gr_poly
					(pts
						(xy 0 -0.75) (xy -0.55 -0.75) (xy -0.55 0.75) (xy 0 0.75)
					)
					(width 0)
					(fill yes)
				)
			)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
	)
	(footprint "Diode_SMD:D_0603_1608Metric"
		(layer "B.Cu")
		(at 104.878012 102.761475 180)
		(descr "Diode SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
		(tags "diode")
		(property "Reference" "D4:4"
			(at 0 1.43 0)
			(layer "B.SilkS")
		)
		(property "Value" "D"
			(at 0 -1.43 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Diode, small symbol, filled shape"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sim.Device" "D"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TO-???* *_Diode_* *SingleDiode* D_*")
		(sheetname "/Human-Machine Interface/Keypad/")
		(sheetfile "../Projects/capstone-project/Hardware/KiCAD/system-testbed/keypad.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.7875 0 180)
			(size 0.875 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 36 "/Human-Machine Interface/Keypad/COL4")
			(pinfunction "K")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at 0.7875 0 180)
			(size 0.875 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 19 "Net-(D4:4-A)")
			(pinfunction "A")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Diode_SMD.3dshapes/D_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "LOGO"
		(layer "B.Cu")
		(at 101.2 123.7 180)
		(property "Reference" "G***"
			(at 0 0 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "LOGO"
			(at 0.75 0 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(attr board_only exclude_from_pos_files exclude_from_bom)
		(embedded_fonts no)
	)
	(footprint "LOGO"
		(layer "B.Cu")
		(at 74.6 130.4 180)
		(property "Reference" "G***"
			(at 0 0 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "LOGO"
			(at 0.75 0 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(attr board_only exclude_from_pos_files exclude_from_bom)
		(embedded_fonts no)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "B.Cu")
		(at 72.3 114.3 -90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R3"
			(at -0.1 -1.4 90)
			(layer "B.SilkS")
		)
		(property "Value" "10k"
			(at 0 -1.43 90)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Human-Machine Interface/")
		(sheetfile "human-machine-interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 270)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 54 "/Human-Machine Interface/PCF_A2")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at 0.825 0 270)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "B.Cu")
		(at 105.495132 113.359843)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R5"
			(at 0 1.2 0)
			(layer "B.SilkS")
		)
		(property "Value" "10k"
			(at 0 -1.43 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Human-Machine Interface/")
		(sheetfile "human-machine-interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 44 "/Human-Machine Interface/ENC_DT")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at 0.825 0)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 3 "Net-(C2-Pad1)")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "B.Cu")
		(at 107.841716 117.274005 90)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C1"
			(at -2.325995 -0.04836 90)
			(layer "B.SilkS")
		)
		(property "Value" "0.01uF"
			(at 0 -1.43 90)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "capacitor, US symbol"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/Human-Machine Interface/")
		(sheetfile "human-machine-interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 90)
			(size 0.9 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 2 "Net-(C1-Pad1)")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at 0.775 0 90)
			(size 0.9 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Jumper:SolderJumper-2_P1.3mm_Open_TrianglePad1.0x1.5mm"
		(layer "B.Cu")
		(at 69.8 114.05)
		(descr "SMD Solder Jumper, 1x1.5mm Triangular Pads, 0.3mm gap, open")
		(tags "solder jumper open")
		(property "Reference" "JP3"
			(at 0 1.8 0)
			(layer "B.SilkS")
		)
		(property "Value" "SolderJumper_2_Open"
			(at 0 -1.9 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Solder Jumper, 2-pole, open"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SolderJumper*Open*")
		(sheetname "/Human-Machine Interface/")
		(sheetfile "human-machine-interface.kicad_sch")
		(zone_connect 1)
		(attr exclude_from_pos_files exclude_from_bom allow_soldermask_bridges)
		(pad "1" smd custom
			(at -0.725 0)
			(size 0.3 0.3)
			(layers "B.Cu" "B.Mask")
			(net 26 "+3.3V")
			(pinfunction "A")
			(pintype "passive")
			(zone_connect 2)
			(thermal_bridge_angle 45)
			(options
				(clearance outline)
				(anchor rect)
			)
			(primitives
				(gr_poly
					(pts
						(xy 1 0) (xy 0.5 -0.75) (xy -0.5 -0.75) (xy -0.5 0.75) (xy 0.5 0.75)
					)
					(width 0)
					(fill yes)
				)
			)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd custom
			(at 0.725 0)
			(size 0.3 0.3)
			(layers "B.Cu" "B.Mask")
			(net 54 "/Human-Machine Interface/PCF_A2")
			(pinfunction "B")
			(pintype "passive")
			(zone_connect 2)
			(thermal_bridge_angle 45)
			(options
				(clearance outline)
				(anchor rect)
			)
			(primitives
				(gr_poly
					(pts
						(xy 0.5 -0.75) (xy -0.65 -0.75) (xy -0.15 0) (xy -0.65 0.75) (xy 0.5 0.75)
					)
					(width 0)
					(fill yes)
				)
			)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
	)
	(footprint "Diode_SMD:D_0603_1608Metric"
		(layer "B.Cu")
		(at 81.200615 113.169004 180)
		(descr "Diode SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
		(tags "diode")
		(property "Reference" "D2:1"
			(at 0 1.43 0)
			(layer "B.SilkS")
		)
		(property "Value" "D"
			(at 0 -1.43 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Diode, small symbol, filled shape"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sim.Device" "D"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TO-???* *_Diode_* *SingleDiode* D_*")
		(sheetname "/Human-Machine Interface/Keypad/")
		(sheetfile "../Projects/capstone-project/Hardware/KiCAD/system-testbed/keypad.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.7875 0 180)
			(size 0.875 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 33 "/Human-Machine Interface/Keypad/COL1")
			(pinfunction "K")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at 0.7875 0 180)
			(size 0.875 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 8 "Net-(D2:1-A)")
			(pinfunction "A")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Diode_SMD.3dshapes/D_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Diode_SMD:D_0603_1608Metric"
		(layer "B.Cu")
		(at 95.8041 113.258 180)
		(descr "Diode SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
		(tags "diode")
		(property "Reference" "D2:3"
			(at 0 1.43 0)
			(layer "B.SilkS")
		)
		(property "Value" "D"
			(at 0 -1.43 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Diode, small symbol, filled shape"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sim.Device" "D"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TO-???* *_Diode_* *SingleDiode* D_*")
		(sheetname "/Human-Machine Interface/Keypad/")
		(sheetfile "../Projects/capstone-project/Hardware/KiCAD/system-testbed/keypad.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.7875 0 180)
			(size 0.875 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 35 "/Human-Machine Interface/Keypad/COL3")
			(pinfunction "K")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at 0.7875 0 180)
			(size 0.875 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 10 "Net-(D2:3-A)")
			(pinfunction "A")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Diode_SMD.3dshapes/D_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "B.Cu")
		(at 117.2 94.825 90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R16"
			(at -0.064414 -1.233158 90)
			(layer "B.SilkS")
		)
		(property "Value" "100k"
			(at 0 -1.43 90)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Human-Machine Interface/Audio/")
		(sheetfile "untitled.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 90)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at 0.825 0 90)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 59 "/Human-Machine Interface/Audio/~{SD_MODE}")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Jumper:SolderJumper-2_P1.3mm_Open_TrianglePad1.0x1.5mm"
		(layer "B.Cu")
		(at 69.8 117.6)
		(descr "SMD Solder Jumper, 1x1.5mm Triangular Pads, 0.3mm gap, open")
		(tags "solder jumper open")
		(property "Reference" "JP2"
			(at 0 1.8 0)
			(layer "B.SilkS")
		)
		(property "Value" "SolderJumper_2_Open"
			(at 0 -1.9 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Solder Jumper, 2-pole, open"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SolderJumper*Open*")
		(sheetname "/Human-Machine Interface/")
		(sheetfile "human-machine-interface.kicad_sch")
		(zone_connect 1)
		(attr exclude_from_pos_files exclude_from_bom allow_soldermask_bridges)
		(pad "1" smd custom
			(at -0.725 0)
			(size 0.3 0.3)
			(layers "B.Cu" "B.Mask")
			(net 26 "+3.3V")
			(pinfunction "A")
			(pintype "passive")
			(zone_connect 2)
			(thermal_bridge_angle 45)
			(options
				(clearance outline)
				(anchor rect)
			)
			(primitives
				(gr_poly
					(pts
						(xy 1 0) (xy 0.5 -0.75) (xy -0.5 -0.75) (xy -0.5 0.75) (xy 0.5 0.75)
					)
					(width 0)
					(fill yes)
				)
			)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd custom
			(at 0.725 0)
			(size 0.3 0.3)
			(layers "B.Cu" "B.Mask")
			(net 56 "/Human-Machine Interface/PCF_A1")
			(pinfunction "B")
			(pintype "passive")
			(zone_connect 2)
			(thermal_bridge_angle 45)
			(options
				(clearance outline)
				(anchor rect)
			)
			(primitives
				(gr_poly
					(pts
						(xy 0.5 -0.75) (xy -0.65 -0.75) (xy -0.15 0) (xy -0.65 0.75) (xy 0.5 0.75)
					)
					(width 0)
					(fill yes)
				)
			)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "B.Cu")
		(at 121 91.5 -90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R9"
			(at -0.05 -1.3 90)
			(layer "B.SilkS")
		)
		(property "Value" "47k"
			(at -0.1 -6.988 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Human-Machine Interface/Audio/")
		(sheetfile "untitled.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 270)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 65 "Net-(MK1-SD)")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at 0.825 0 270)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "B.Cu")
		(at 120.3 88.2 180)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R10"
			(at 0.05 1.2 0)
			(layer "B.SilkS")
		)
		(property "Value" "68"
			(at 0 -1.43 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Human-Machine Interface/Audio/")
		(sheetfile "untitled.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 180)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 65 "Net-(MK1-SD)")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at 0.825 0 180)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 74 "/Human-Machine Interface/MIC_DOUT")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Jumper:SolderJumper-3_P1.3mm_Open_RoundedPad1.0x1.5mm_NumberLabels"
		(layer "B.Cu")
		(at 127.7 116.9 -90)
		(descr "SMD Solder 3-pad Jumper, 1x1.5mm rounded Pads, 0.3mm gap, open, labeled with numbers")
		(tags "solder jumper open")
		(property "Reference" "JP4"
			(at 0 1.8 90)
			(layer "B.SilkS")
		)
		(property "Value" "GAIN_{LOGIC}"
			(at 0 -1.9 90)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Solder Jumper, 3-pole, open"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SolderJumper*Open*")
		(sheetname "/Human-Machine Interface/Audio/")
		(sheetfile "untitled.kicad_sch")
		(zone_connect 1)
		(attr exclude_from_pos_files allow_soldermask_bridges)
		(fp_text user "3"
			(at 2.6 0 90)
			(layer "B.SilkS")
		)
		(fp_text user "1"
			(at -2.6 0 90)
			(layer "B.SilkS")
		)
		(pad "1" smd custom
			(at -1.3 0 270)
			(size 1 0.5)
			(layers "B.Cu" "B.Mask")
			(net 26 "+3.3V")
			(pinfunction "A")
			(pintype "passive")
			(zone_connect 2)
			(thermal_bridge_angle 45)
			(options
				(clearance outline)
				(anchor rect)
			)
			(primitives
				(gr_circle
					(center 0 -0.25)
					(end 0.5 -0.25)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center 0 0.25)
					(end 0.5 0.25)
					(width 0)
					(fill yes)
				)
				(gr_poly
					(pts
						(xy 0.55 -0.75) (xy 0 -0.75) (xy 0 0.75) (xy 0.55 0.75)
					)
					(width 0)
					(fill yes)
				)
			)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd rect
			(at 0 0 270)
			(size 1 1.5)
			(layers "B.Cu" "B.Mask")
			(net 58 "Net-(JP4-C)")
			(pinfunction "C")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "3" smd custom
			(at 1.3 0 270)
			(size 1 0.5)
			(layers "B.Cu" "B.Mask")
			(net 1 "GND")
			(pinfunction "B")
			(pintype "passive")
			(zone_connect 2)
			(thermal_bridge_angle 45)
			(options
				(clearance outline)
				(anchor rect)
			)
			(primitives
				(gr_circle
					(center 0 -0.25)
					(end 0.5 -0.25)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center 0 0.25)
					(end 0.5 0.25)
					(width 0)
					(fill yes)
				)
				(gr_poly
					(pts
						(xy 0 -0.75) (xy -0.55 -0.75) (xy -0.55 0.75) (xy 0 0.75)
					)
					(width 0)
					(fill yes)
				)
			)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
	)
	(footprint "Jumper:SolderJumper-2_P1.3mm_Open_TrianglePad1.0x1.5mm"
		(layer "B.Cu")
		(at 69.8 121.15)
		(descr "SMD Solder Jumper, 1x1.5mm Triangular Pads, 0.3mm gap, open")
		(tags "solder jumper open")
		(property "Reference" "JP1"
			(at 0 1.8 0)
			(layer "B.SilkS")
		)
		(property "Value" "SolderJumper_2_Open"
			(at 0 -1.9 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Solder Jumper, 2-pole, open"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SolderJumper*Open*")
		(sheetname "/Human-Machine Interface/")
		(sheetfile "human-machine-interface.kicad_sch")
		(zone_connect 1)
		(attr exclude_from_pos_files exclude_from_bom allow_soldermask_bridges)
		(pad "1" smd custom
			(at -0.725 0)
			(size 0.3 0.3)
			(layers "B.Cu" "B.Mask")
			(net 26 "+3.3V")
			(pinfunction "A")
			(pintype "passive")
			(zone_connect 2)
			(thermal_bridge_angle 45)
			(options
				(clearance outline)
				(anchor rect)
			)
			(primitives
				(gr_poly
					(pts
						(xy 1 0) (xy 0.5 -0.75) (xy -0.5 -0.75) (xy -0.5 0.75) (xy 0.5 0.75)
					)
					(width 0)
					(fill yes)
				)
			)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd custom
			(at 0.725 0)
			(size 0.3 0.3)
			(layers "B.Cu" "B.Mask")
			(net 55 "/Human-Machine Interface/PCF_A0")
			(pinfunction "B")
			(pintype "passive")
			(zone_connect 2)
			(thermal_bridge_angle 45)
			(options
				(clearance outline)
				(anchor rect)
			)
			(primitives
				(gr_poly
					(pts
						(xy 0.5 -0.75) (xy -0.65 -0.75) (xy -0.15 0) (xy -0.65 0.75) (xy 0.5 0.75)
					)
					(width 0)
					(fill yes)
				)
			)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
	)
	(footprint "Connector_JST:JST_EH_B2B-EH-A_1x02_P2.50mm_Vertical"
		(layer "B.Cu")
		(at 123.4 131.85 90)
		(descr "JST EH series connector, B2B-EH-A (http://www.jst-mfg.com/product/pdf/eng/eEH.pdf), generated with kicad-footprint-generator")
		(tags "connector JST EH vertical")
		(property "Reference" "LS1"
			(at 1.25 2.8 90)
			(layer "B.SilkS")
		)
		(property "Value" "Speaker"
			(at 1.15 -2.8 90)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Speaker"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(sheetname "/Human-Machine Interface/Audio/")
		(sheetfile "untitled.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 1.25 -1.5 90)
			(layer "B.Fab")
		)
		(pad "1" thru_hole roundrect
			(at 0 0 90)
			(size 1.7 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.147059)
			(net 63 "Net-(U2-OUTP)")
			(pinfunction "1")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" thru_hole oval
			(at 2.5 0 90)
			(size 1.7 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 62 "Net-(U2-OUTN)")
			(pinfunction "2")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_JST.3dshapes/JST_EH_B2B-EH-A_1x02_P2.50mm_Vertical.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "B.Cu")
		(at 130.4 116.9 -90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R12"
			(at 3 -0.05942 90)
			(layer "B.SilkS")
		)
		(property "Value" "100k 5%"
			(at 0 -1.43 90)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Human-Machine Interface/Audio/")
		(sheetfile "untitled.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 270)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 58 "Net-(JP4-C)")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at 0.825 0 270)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 61 "Net-(JP6-B)")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Diode_SMD:D_0603_1608Metric"
		(layer "B.Cu")
		(at 81.175615 122.449804 180)
		(descr "Diode SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
		(tags "diode")
		(property "Reference" "D4:1"
			(at 0 1.43 0)
			(layer "B.SilkS")
		)
		(property "Value" "D"
			(at 0 -1.43 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Diode, small symbol, filled shape"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sim.Device" "D"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TO-???* *_Diode_* *SingleDiode* D_*")
		(sheetname "/Human-Machine Interface/Keypad/")
		(sheetfile "../Projects/capstone-project/Hardware/KiCAD/system-testbed/keypad.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.7875 0 180)
			(size 0.875 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 33 "/Human-Machine Interface/Keypad/COL1")
			(pinfunction "K")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at 0.7875 0 180)
			(size 0.875 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 16 "Net-(D4:1-A)")
			(pinfunction "A")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Diode_SMD.3dshapes/D_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "B.Cu")
		(at 72.3 117.3 -90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R2"
			(at 0 -1.4 90)
			(layer "B.SilkS")
		)
		(property "Value" "10k"
			(at 0 -1.43 90)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Human-Machine Interface/")
		(sheetfile "human-machine-interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 270)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 56 "/Human-Machine Interface/PCF_A1")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at 0.825 0 270)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Diode_SMD:D_0603_1608Metric"
		(layer "B.Cu")
		(at 95.8041 122.458 180)
		(descr "Diode SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
		(tags "diode")
		(property "Reference" "D4:3"
			(at 0 1.43 0)
			(layer "B.SilkS")
		)
		(property "Value" "D"
			(at 0 -1.43 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Diode, small symbol, filled shape"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sim.Device" "D"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TO-???* *_Diode_* *SingleDiode* D_*")
		(sheetname "/Human-Machine Interface/Keypad/")
		(sheetfile "../Projects/capstone-project/Hardware/KiCAD/system-testbed/keypad.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.7875 0 180)
			(size 0.875 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 35 "/Human-Machine Interface/Keypad/COL3")
			(pinfunction "K")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at 0.7875 0 180)
			(size 0.875 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 18 "Net-(D4:3-A)")
			(pinfunction "A")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Diode_SMD.3dshapes/D_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Diode_SMD:D_0603_1608Metric"
		(layer "B.Cu")
		(at 81.200615 108.530131 180)
		(descr "Diode SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
		(tags "diode")
		(property "Reference" "D1:1"
			(at 0 1.43 0)
			(layer "B.SilkS")
		)
		(property "Value" "D"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Diode, small symbol, filled shape"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sim.Device" "D"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TO-???* *_Diode_* *SingleDiode* D_*")
		(sheetname "/Human-Machine Interface/Keypad/")
		(sheetfile "../Projects/capstone-project/Hardware/KiCAD/system-testbed/keypad.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.7875 0 180)
			(size 0.875 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 33 "/Human-Machine Interface/Keypad/COL1")
			(pinfunction "K")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at 0.7875 0 180)
			(size 0.875 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 4 "Net-(D1:1-A)")
			(pinfunction "A")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Diode_SMD.3dshapes/D_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "B.Cu")
		(at 109.406994 117.279017 -90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R6"
			(at 0 -1.293006 90)
			(layer "B.SilkS")
		)
		(property "Value" "10k"
			(at 0 -1.43 90)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Human-Machine Interface/")
		(sheetfile "human-machine-interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 270)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 26 "+3.3V")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at 0.825 0 270)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 2 "Net-(C1-Pad1)")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "LOGO"
		(layer "B.Cu")
		(at 92.5 96.7 180)
		(property "Reference" "G***"
			(at 0 0 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "LOGO"
			(at 0.75 0 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(attr board_only exclude_from_pos_files exclude_from_bom)
		(embedded_fonts no)
	)
	(footprint "Diode_SMD:D_0603_1608Metric"
		(layer "B.Cu")
		(at 111.045358 99.926773 180)
		(descr "Diode SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
		(tags "diode")
		(property "Reference" "D2:4"
			(at -0.008642 1.456774 0)
			(layer "B.SilkS")
		)
		(property "Value" "D"
			(at 0 -1.43 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Diode, small symbol, filled shape"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sim.Device" "D"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TO-???* *_Diode_* *SingleDiode* D_*")
		(sheetname "/Human-Machine Interface/Keypad/")
		(sheetfile "../Projects/capstone-project/Hardware/KiCAD/system-testbed/keypad.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.7875 0 180)
			(size 0.875 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 36 "/Human-Machine Interface/Keypad/COL4")
			(pinfunction "K")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at 0.7875 0 180)
			(size 0.875 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 11 "Net-(D2:4-A)")
			(pinfunction "A")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Diode_SMD.3dshapes/D_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Diode_SMD:D_0603_1608Metric"
		(layer "B.Cu")
		(at 95.85 117.8508 180)
		(descr "Diode SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
		(tags "diode")
		(property "Reference" "D3:3"
			(at 0 1.43 0)
			(layer "B.SilkS")
		)
		(property "Value" "D"
			(at 0 -1.43 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Diode, small symbol, filled shape"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sim.Device" "D"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TO-???* *_Diode_* *SingleDiode* D_*")
		(sheetname "/Human-Machine Interface/Keypad/")
		(sheetfile "../Projects/capstone-project/Hardware/KiCAD/system-testbed/keypad.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.7875 0 180)
			(size 0.875 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 35 "/Human-Machine Interface/Keypad/COL3")
			(pinfunction "K")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at 0.7875 0 180)
			(size 0.875 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 14 "Net-(D3:3-A)")
			(pinfunction "A")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Diode_SMD.3dshapes/D_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Diode_SMD:D_0603_1608Metric"
		(layer "B.Cu")
		(at 111.009703 104.961475 180)
		(descr "Diode SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
		(tags "diode")
		(property "Reference" "D3:4"
			(at 0 1.43 0)
			(layer "B.SilkS")
		)
		(property "Value" "D"
			(at 0.04192 -1.626189 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Diode, small symbol, filled shape"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sim.Device" "D"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TO-???* *_Diode_* *SingleDiode* D_*")
		(sheetname "/Human-Machine Interface/Keypad/")
		(sheetfile "../Projects/capstone-project/Hardware/KiCAD/system-testbed/keypad.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.7875 0 180)
			(size 0.875 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 36 "/Human-Machine Interface/Keypad/COL4")
			(pinfunction "K")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at 0.7875 0 180)
			(size 0.875 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 15 "Net-(D3:4-A)")
			(pinfunction "A")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Diode_SMD.3dshapes/D_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "B.Cu")
		(at 122.5 84 90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R8"
			(at 0 -1.3 90)
			(layer "B.SilkS")
		)
		(property "Value" "47k"
			(at 0 -1.43 90)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Human-Machine Interface/Audio/")
		(sheetfile "untitled.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 90)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 64 "Net-(MK1-LR)")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at 0.825 0 90)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "B.Cu")
		(at 72.3 120.4 90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R1"
			(at 0 1.5 90)
			(layer "B.SilkS")
		)
		(property "Value" "10k"
			(at 0 -1.43 90)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Human-Machine Interface/")
		(sheetfile "human-machine-interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 90)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 55 "/Human-Machine Interface/PCF_A0")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at 0.825 0 90)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Diode_SMD:D_0603_1608Metric"
		(layer "B.Cu")
		(at 81.188115 117.849804 180)
		(descr "Diode SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
		(tags "diode")
		(property "Reference" "D3:1"
			(at 0 1.43 0)
			(layer "B.SilkS")
		)
		(property "Value" "D"
			(at 0 -1.43 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Diode, small symbol, filled shape"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sim.Device" "D"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TO-???* *_Diode_* *SingleDiode* D_*")
		(sheetname "/Human-Machine Interface/Keypad/")
		(sheetfile "../Projects/capstone-project/Hardware/KiCAD/system-testbed/keypad.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.7875 0 180)
			(size 0.875 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 33 "/Human-Machine Interface/Keypad/COL1")
			(pinfunction "K")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at 0.7875 0 180)
			(size 0.875 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 12 "Net-(D3:1-A)")
			(pinfunction "A")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Diode_SMD.3dshapes/D_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "B.Cu")
		(at 107.839987 114.11886 -90)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C2"
			(at -2.487615 0.046631 90)
			(layer "B.SilkS")
		)
		(property "Value" "0.01uF"
			(at 0 -1.43 90)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "capacitor, US symbol"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/Human-Machine Interface/")
		(sheetfile "human-machine-interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 270)
			(size 0.9 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 3 "Net-(C2-Pad1)")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at 0.775 0 270)
			(size 0.9 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Diode_SMD:D_0603_1608Metric"
		(layer "B.Cu")
		(at 116.884703 102.761475 180)
		(descr "Diode SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
		(tags "diode")
		(property "Reference" "D1:4"
			(at 0.0433 1.6 0)
			(layer "B.SilkS")
		)
		(property "Value" "D"
			(at 0 -1.43 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Diode, small symbol, filled shape"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sim.Device" "D"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TO-???* *_Diode_* *SingleDiode* D_*")
		(sheetname "/Human-Machine Interface/Keypad/")
		(sheetfile "../Projects/capstone-project/Hardware/KiCAD/system-testbed/keypad.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.7875 0 180)
			(size 0.875 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 36 "/Human-Machine Interface/Keypad/COL4")
			(pinfunction "K")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at 0.7875 0 180)
			(size 0.875 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 7 "Net-(D1:4-A)")
			(pinfunction "A")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Diode_SMD.3dshapes/D_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "B.Cu")
		(at 105.493356 118.031245)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R4"
			(at 0 -1.191245 0)
			(layer "B.SilkS")
		)
		(property "Value" "10k"
			(at 0 -1.43 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Human-Machine Interface/")
		(sheetfile "human-machine-interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 40 "/Human-Machine Interface/ENC_CLK")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at 0.825 0)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 2 "Net-(C1-Pad1)")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "capstone-project:Adafruit EYESPI FPC Connector"
		(layer "B.Cu")
		(at 111.969254 82.268651)
		(descr "WR-FPC SMT ZIF Horizontal Hinge Type")
		(tags "EYESPI, FPC")
		(property "Reference" "X1"
			(at 7.874 -2.032 0)
			(layer "B.SilkS")
		)
		(property "Value" "EYESPI"
			(at 0 -4.064 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "https://www.we-online.com/components/products/datasheet/687118149022.pdf"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "WR-FPC SMT ZIF Horizontal Hinge Type"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "HMI.kicad_sch")
		(attr smd allow_soldermask_bridges)
		(pad "1" smd rect
			(at -4.25 3.35)
			(size 0.3 1.3)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 26 "+3.3V")
			(pintype "passive")
			(solder_mask_margin 0.102)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd rect
			(at -3.75 3.35)
			(size 0.3 1.3)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 31 "/LITE")
			(pintype "passive")
			(solder_mask_margin 0.102)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "3" smd rect
			(at -3.25 3.35)
			(size 0.3 1.3)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 1 "GND")
			(pintype "passive")
			(solder_mask_margin 0.102)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "4" smd rect
			(at -2.75 3.35)
			(size 0.3 1.3)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 30 "/SCK")
			(pintype "passive")
			(solder_mask_margin 0.102)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "5" smd rect
			(at -2.25 3.35)
			(size 0.3 1.3)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 32 "/MOSI")
			(pintype "passive")
			(solder_mask_margin 0.102)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "6" smd rect
			(at -1.75 3.35)
			(size 0.3 1.3)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 29 "/MISO")
			(pintype "passive")
			(solder_mask_margin 0.102)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "7" smd rect
			(at -1.25 3.35)
			(size 0.3 1.3)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 24 "/TFTDC")
			(pintype "passive")
			(solder_mask_margin 0.102)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "8" smd rect
			(at -0.75 3.35)
			(size 0.3 1.3)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 25 "/TFTRST")
			(pintype "passive")
			(solder_mask_margin 0.102)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "9" smd rect
			(at -0.25 3.35)
			(size 0.3 1.3)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 27 "/TFTCS")
			(pintype "passive")
			(solder_mask_margin 0.102)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "10" smd rect
			(at 0.25 3.35)
			(size 0.3 1.3)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 28 "/CARDCS")
			(pintype "passive")
			(solder_mask_margin 0.102)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "11" smd rect
			(at 0.75 3.35)
			(size 0.3 1.3)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 76 "/Human-Machine Interface/AMP_DIN")
			(pintype "passive")
			(solder_mask_margin 0.102)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "12" smd rect
			(at 1.25 3.35)
			(size 0.3 1.3)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 74 "/Human-Machine Interface/MIC_DOUT")
			(pintype "passive")
			(solder_mask_margin 0.102)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "13" smd rect
			(at 1.75 3.35)
			(size 0.3 1.3)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 23 "/SCL")
			(pintype "passive")
			(solder_mask_margin 0.102)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "14" smd rect
			(at 2.25 3.35)
			(size 0.3 1.3)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 22 "/SDA")
			(pintype "passive")
			(solder_mask_margin 0.102)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "15" smd rect
			(at 2.75 3.35)
			(size 0.3 1.3)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 70 "/~{PCF_INT}")
			(pintype "passive")
			(solder_mask_margin 0.102)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "16" smd rect
			(at 3.25 3.35)
			(size 0.3 1.3)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 75 "/Human-Machine Interface/~{AMP_SD}")
			(pintype "passive")
			(solder_mask_margin 0.102)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "17" smd rect
			(at 3.75 3.35)
			(size 0.3 1.3)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 71 "/Human-Machine Interface/BCLK")
			(pintype "passive")
			(solder_mask_margin 0.102)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "18" smd rect
			(at 4.25 3.35)
			(size 0.3 1.3)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 73 "/Human-Machine Interface/LRCLK")
			(pintype "passive")
			(solder_mask_margin 0.102)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "Z1" smd rect
			(at -6.05 0.6)
			(size 2 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 1 "GND")
			(pintype "passive")
			(solder_mask_margin 0.102)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "Z2" smd rect
			(at 6.05 0.6)
			(size 2 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 1 "GND")
			(pintype "passive")
			(solder_mask_margin 0.102)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KIPRJMOD}/capstone-project.pretty/3dmodels/687118149022+(rev1).step"
			(offset
				(xyz 0 0.5 1.15)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -0 -0 -0)
			)
		)
	)
	(footprint "Diode_SMD:D_0603_1608Metric"
		(layer "B.Cu")
		(at 88.4875 113.258 180)
		(descr "Diode SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
		(tags "diode")
		(property "Reference" "D2:2"
			(at 0 1.43 0)
			(layer "B.SilkS")
		)
		(property "Value" "D"
			(at 0 -1.43 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Diode, small symbol, filled shape"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sim.Device" "D"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TO-???* *_Diode_* *SingleDiode* D_*")
		(sheetname "/Human-Machine Interface/Keypad/")
		(sheetfile "../Projects/capstone-project/Hardware/KiCAD/system-testbed/keypad.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.7875 0 180)
			(size 0.875 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 34 "/Human-Machine Interface/Keypad/COL2")
			(pinfunction "K")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at 0.7875 0 180)
			(size 0.875 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 9 "Net-(D2:2-A)")
			(pinfunction "A")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Diode_SMD.3dshapes/D_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(gr_arc
		(start 126.950199 78.59999)
		(mid 130.132087 79.91801)
		(end 131.44999 83.099998)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 131.45002 87.589481)
		(mid 130.149475 90.742617)
		(end 127.00417 92.062053)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 84.824854 131.5899)
		(mid 86.151676 128.399121)
		(end 89.348704 127.089876)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 70.263422 83.109426)
		(end 70.263422 87.5523)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 74.763514 92.037404)
		(end 75.078086 92.037403)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 135.451443 109.417907)
		(mid 135.883033 109.612467)
		(end 136.065919 110.075605)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 79.578102 96.562257)
		(mid 78.25128 99.753036)
		(end 75.053248 101.062277)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 131.521713 105.611812)
		(end 131.521713 105.613257)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 70.5894 136.089974)
		(mid 67.398635 134.763152)
		(end 66.089394 131.614456)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 70.525268 105.562304)
		(mid 69.418257 108.297161)
		(end 66.720618 109.492007)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 131.45002 87.589481)
		(end 131.450041 83.099998)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 89.348704 127.089876)
		(end 112.881894 127.09978)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 127.021663 101.086958)
		(mid 123.830884 99.760136)
		(end 122.521643 96.562104)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 70.5894 136.089974)
		(end 80.34984 136.089974)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 70.525268 105.562297)
		(mid 71.85209 102.371518)
		(end 75.050122 101.062277)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 127.00417 92.062053)
		(end 126.996994 92.062053)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 135.451416 109.417907)
		(mid 132.716559 108.310896)
		(end 131.521713 105.613257)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 136.065919 131.55764)
		(mid 134.75659 134.730956)
		(end 131.596977 136.05765)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 74.763514 92.037404)
		(mid 71.590165 90.728084)
		(end 70.263422 87.5523)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 122.521643 96.562054)
		(mid 123.830969 93.38879)
		(end 126.996994 92.062053)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 84.824854 131.589954)
		(mid 83.498032 134.780733)
		(end 80.34984 136.089974)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 75.050122 101.062277)
		(end 75.053248 101.062277)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 127.021693 101.086958)
		(mid 130.212472 102.41378)
		(end 131.521713 105.611812)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 79.778021 78.600005)
		(end 75.078021 78.6)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 74.76335 78.6)
		(end 75.078021 78.6)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 136.065919 110.075605)
		(end 136.065919 131.55764)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 94.95 78.6)
		(end 79.778021 78.600005)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 75.078086 92.037403)
		(mid 78.268861 93.364225)
		(end 79.578102 96.562257)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 121.88 136.05765)
		(end 131.596977 136.05765)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 66.089394 110.168876)
		(end 66.089394 131.614456)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 121.88 136.05765)
		(mid 118.689202 134.730828)
		(end 117.379961 131.532796)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 126.950199 78.59999)
		(end 94.95 78.6)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 112.881894 127.09978)
		(mid 116.038185 128.393995)
		(end 117.379961 131.532252)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 66.089394 110.168876)
		(mid 66.283953 109.674957)
		(end 66.720618 109.492071)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 70.263422 83.109426)
		(mid 71.578062 79.921358)
		(end 74.76335 78.6)
		(layer "Edge.Cuts")
	)
	(gr_text "2"
		(at 84.067089 109.497902 0)
		(layer "F.SilkS" knockout)
	)
	(gr_text "OPENAIR LAB"
		(at 87.3 87.7 0)
		(layer "F.SilkS")
	)
	(gr_text "Zachary Potersnak, Eric Mutton\n 	   Fall 2025 REV-B\n      	    (HMI)"
		(at 92.5 83 0)
		(layer "F.SilkS" knockout)
	)
	(gr_text "9"
		(at 91.4 118.9 0)
		(layer "F.SilkS" knockout)
	)
	(gr_text "Rotary "
		(at 103.9 108.2 0)
		(layer "F.SilkS" knockout)
	)
	(gr_text "  Audio \nAmplifier"
		(at 126.5 116.8 0)
		(layer "F.SilkS" knockout)
	)
	(gr_text "GPIO Expander"
		(at 96.5 99.7 90)
		(layer "F.SilkS" knockout)
	)
	(gr_text "5"
		(at 84.067089 114.297902 0)
		(layer "F.SilkS" knockout)
	)
	(gr_text "Push To \n  Talk"
		(at 77.5 90 0)
		(layer "F.SilkS" knockout)
	)
	(gr_text "LITE"
		(at 82.8 81.6 0)
		(layer "F.SilkS")
	)
	(gr_text "*"
		(at 76.5 124 0)
		(layer "F.SilkS" knockout)
	)
	(gr_text "6"
		(at 91.4 114.3 0)
		(layer "F.SilkS" knockout)
	)
	(gr_text "Encoder"
		(at 116.774649 108.364467 0)
		(layer "F.SilkS" knockout)
	)
	(gr_text "4"
		(at 76.4 114.3 0)
		(layer "F.SilkS" knockout)
	)
	(gr_text "#"
		(at 91.3 123.5 0)
		(layer "F.SilkS" knockout)
	)
	(gr_text "OpenAir Lab\nProduction"
		(at 75.044213 133.588964 0)
		(layer "F.SilkS" knockout)
	)
	(gr_text "8"
		(at 84.167089 118.997902 0)
		(layer "F.SilkS" knockout)
	)
	(gr_text "Mic"
		(at 126.1 90.9 0)
		(layer "F.SilkS" knockout)
	)
	(gr_text "0"
		(at 84.067089 123.597902 0)
		(layer "F.SilkS" knockout)
	)
	(gr_text "3"
		(at 91.4 109.5 0)
		(layer "F.SilkS" knockout)
	)
	(gr_text "1"
		(at 76.5 109.5 0)
		(layer "F.SilkS" knockout)
	)
	(gr_text "7"
		(at 76.5 119.1 0)
		(layer "F.SilkS" knockout)
	)
	(zone
		(net 43)
		(net_name "/Human-Machine Interface/Keypad/ROW4")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30047)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 79.921515 123.616804) (xy 79.921515 123.416804) (xy 79.596515 123.191804) (xy 79.070515 123.516804)
				(xy 79.596515 123.841804)
			)
		)
	)
	(zone
		(net 41)
		(net_name "/Human-Machine Interface/Keypad/ROW2")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30073)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 78.2375 114.1) (xy 78.2375 114.3) (xy 78.5625 114.5) (xy 79.0885 114.175) (xy 78.5625 113.865312)
			)
		)
	)
	(zone
		(net 42)
		(net_name "/Human-Machine Interface/Keypad/ROW1")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30062)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 92.925 109.475) (xy 92.925 109.675) (xy 93.25 109.9) (xy 93.776 109.575) (xy 93.25 109.25)
			)
		)
	)
	(zone
		(net 15)
		(net_name "Net-(D3:4-A)")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30091)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 109.699348 102.517541) (xy 109.840769 102.37612) (xy 109.459703 102.108141) (xy 108.933996 102.410768)
				(xy 109.459703 102.736475)
			)
		)
	)
	(zone
		(net 43)
		(net_name "/Human-Machine Interface/Keypad/ROW4")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30043)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 97.075 123.425) (xy 97.075 123.625) (xy 97.4 123.85) (xy 97.926 123.525) (xy 97.4 123.2)
			)
		)
	)
	(zone
		(net 41)
		(net_name "/Human-Machine Interface/Keypad/ROW2")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30082)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 79.9375 114.333) (xy 79.9375 114.133) (xy 79.6125 113.885095) (xy 79.0865 114.175) (xy 79.6125 114.5)
			)
		)
	)
	(zone
		(net 37)
		(net_name "/Human-Machine Interface/Keypad/ROW3")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30031)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 85.5584 118.775) (xy 85.5584 118.975) (xy 85.8834 119.2) (xy 86.4094 118.875) (xy 85.8834 118.55)
			)
		)
	)
	(zone
		(net 7)
		(net_name "Net-(D1:4-A)")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30094)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 118.245985 98.358773) (xy 118.387405 98.500193) (xy 118.613525 98.757507) (xy 119.139232 98.437818)
				(xy 118.613525 98.113525)
			)
		)
	)
	(zone
		(net 6)
		(net_name "Net-(D1:3-A)")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30046)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 94.625 107.525) (xy 94.625 107.325) (xy 94.3 107.1) (xy 93.774 107.425) (xy 94.3 107.75)
			)
		)
	)
	(zone
		(net 11)
		(net_name "Net-(D2:4-A)")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30096)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 112.177732 94.427025) (xy 112.319153 94.568446) (xy 112.546315 94.757244) (xy 113.072022 94.431537)
				(xy 112.546315 94.147745)
			)
		)
	)
	(zone
		(net 41)
		(net_name "/Human-Machine Interface/Keypad/ROW2")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30117)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 108.821315 97.232244) (xy 109.021315 97.232244) (xy 109.246315 96.907244) (xy 108.921315 96.581244)
				(xy 108.596315 96.907244)
			)
		)
	)
	(zone
		(net 43)
		(net_name "/Human-Machine Interface/Keypad/ROW4")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30113)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 89.075 100.25) (xy 89.275 100.25) (xy 89.367388 99.988268) (xy 89.175 99.099) (xy 88.982612 99.988268)
			)
		)
	)
	(zone
		(net 33)
		(net_name "/Human-Machine Interface/Keypad/COL1")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30100)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 89.725 100.25) (xy 89.925 100.25) (xy 90.017388 99.988268) (xy 89.825 99.099) (xy 89.632612 99.988268)
			)
		)
	)
	(zone
		(net 41)
		(net_name "/Human-Machine Interface/Keypad/ROW2")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30037)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 91.4084 114.325) (xy 91.4084 114.125) (xy 91.0834 113.9) (xy 90.5574 114.225) (xy 91.0834 114.55)
			)
		)
	)
	(zone
		(net 15)
		(net_name "Net-(D3:4-A)")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30023)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 112.234703 102.311475) (xy 112.234703 102.511475) (xy 112.559703 102.736475) (xy 113.085703 102.411475)
				(xy 112.559703 102.086475)
			)
		)
	)
	(zone
		(net 9)
		(net_name "Net-(D2:2-A)")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30095)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 87.166306 112.197335) (xy 87.307726 112.055915) (xy 86.9334 111.781819) (xy 86.407693 112.074293)
				(xy 86.9334 112.4)
			)
		)
	)
	(zone
		(net 26)
		(net_name "+3.3V")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30124)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 131.24 125.565) (xy 131.44 125.565) (xy 131.465 125.3775) (xy 131.34 125.0265) (xy 131.215 125.3775)
			)
		)
	)
	(zone
		(net 43)
		(net_name "/Human-Machine Interface/Keypad/ROW4")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30054)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 101.953012 100.458471) (xy 101.953012 100.658471) (xy 102.278012 100.883471) (xy 102.804012 100.558471)
				(xy 102.278012 100.233471)
			)
		)
	)
	(zone
		(net 41)
		(net_name "/Human-Machine Interface/Keypad/ROW2")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30106)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 87.775 100.25) (xy 87.975 100.25) (xy 88.067388 99.988268) (xy 87.875 99.099) (xy 87.682612 99.988268)
			)
		)
	)
	(zone
		(net 2)
		(net_name "Net-(C1-Pad1)")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30000)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 119.15 118) (xy 119.15 118.3) (xy 119.8 118.8) (xy 121.001 118.15) (xy 119.8 117.5)
			)
		)
	)
	(zone
		(net 38)
		(net_name "/Human-Machine Interface/TFTRST")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30101)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 91.225 90.95) (xy 91.025 90.95) (xy 90.932612 91.211732) (xy 91.125 92.101) (xy 91.317388 91.211732)
			)
		)
	)
	(zone
		(net 22)
		(net_name "/SDA")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30110)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 93.625 100.25) (xy 93.825 100.25) (xy 93.917388 99.988268) (xy 93.725 99.099) (xy 93.532612 99.988268)
			)
		)
	)
	(zone
		(net 26)
		(net_name "+3.3V")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30004)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 121.403486 87.326709) (xy 121.226709 87.503486) (xy 121.625 88.207371) (xy 122.100707 88.000707)
				(xy 122.249025 87.55)
			)
		)
	)
	(zone
		(net 41)
		(net_name "/Human-Machine Interface/Keypad/ROW2")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30084)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 82.3875 114.133) (xy 82.3875 114.333) (xy 82.7125 114.5) (xy 83.2385 114.175) (xy 82.7125 113.885095)
			)
		)
	)
	(zone
		(net 26)
		(net_name "+3.3V")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30005)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 123.575 88.9) (xy 123.825 88.9) (xy 124.15 88.322886) (xy 123.7 87.999) (xy 123.25 88.322886)
			)
		)
	)
	(zone
		(net 42)
		(net_name "/Human-Machine Interface/Keypad/ROW1")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30056)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 118.288525 100.488525) (xy 118.288525 100.688525) (xy 118.613525 100.913525) (xy 119.139525 100.588525)
				(xy 118.613525 100.263525)
			)
		)
	)
	(zone
		(net 43)
		(net_name "/Human-Machine Interface/Keypad/ROW4")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30051)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 94.625 123.625) (xy 94.625 123.425) (xy 94.3 123.2) (xy 93.774 123.525) (xy 94.3 123.85)
			)
		)
	)
	(zone
		(net 59)
		(net_name "/Human-Machine Interface/Audio/~{SD_MODE}")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30120)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 128.615 124.24) (xy 128.615 124.44) (xy 128.8025 124.465) (xy 129.1535 124.34) (xy 128.8025 124.215)
			)
		)
	)
	(zone
		(net 12)
		(net_name "Net-(D3:1-A)")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30058)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 79.921515 116.816804) (xy 79.921515 116.616804) (xy 79.596515 116.391804) (xy 79.070515 116.716804)
				(xy 79.596515 117.041804)
			)
		)
	)
	(zone
		(net 71)
		(net_name "/Human-Machine Interface/BCLK")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30008)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 129.725 118.925) (xy 129.925 118.925) (xy 130.257873 118.336104) (xy 129.825 117.999) (xy 129.392127 118.336104)
			)
		)
	)
	(zone
		(net 36)
		(net_name "/Human-Machine Interface/Keypad/COL4")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30107)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 91.675 100.25) (xy 91.875 100.25) (xy 91.967388 99.988268) (xy 91.775 99.099) (xy 91.582612 99.988268)
			)
		)
	)
	(zone
		(net 42)
		(net_name "/Human-Machine Interface/Keypad/ROW1")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30011)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 94.625 109.675) (xy 94.625 109.475) (xy 94.3 109.25) (xy 93.774 109.575) (xy 94.3 109.9)
			)
		)
	)
	(zone
		(net 62)
		(net_name "Net-(U2-OUTN)")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30125)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 132.565 123.94) (xy 132.565 123.74) (xy 132.3775 123.715) (xy 132.0265 123.84) (xy 132.3775 123.965)
			)
		)
	)
	(zone
		(net 37)
		(net_name "/Human-Machine Interface/Keypad/ROW3")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30030)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 91.4084 118.975) (xy 91.4084 118.775) (xy 91.0834 118.55) (xy 90.5574 118.875) (xy 91.0834 119.2)
			)
		)
	)
	(zone
		(net 10)
		(net_name "Net-(D2:3-A)")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30090)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 94.350225 112.680524) (xy 94.350225 112.480524) (xy 94.3 112.104118) (xy 93.774 112.075) (xy 93.651645 112.4)
			)
		)
	)
	(zone
		(net 39)
		(net_name "/Human-Machine Interface/ENC_SW")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30102)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 89.075 93.25) (xy 89.275 93.25) (xy 89.367388 92.988268) (xy 89.175 92.099) (xy 88.982612 92.988268)
			)
		)
	)
	(zone
		(net 37)
		(net_name "/Human-Machine Interface/Keypad/ROW3")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30024)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 109.784703 104.661475) (xy 109.784703 104.461475) (xy 109.459703 104.236475) (xy 108.933703 104.561475)
				(xy 109.459703 104.886475)
			)
		)
	)
	(zone
		(net 14)
		(net_name "Net-(D3:3-A)")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30012)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 97.075 116.625) (xy 97.075 116.825) (xy 97.4 117.05) (xy 97.926 116.725) (xy 97.4 116.4)
			)
		)
	)
	(zone
		(net 42)
		(net_name "/Human-Machine Interface/Keypad/ROW1")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30086)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 78.2375 109.433) (xy 78.2375 109.633) (xy 78.5625 109.8) (xy 79.0885 109.475) (xy 78.5625 109.185095)
			)
		)
	)
	(zone
		(net 37)
		(net_name "/Human-Machine Interface/Keypad/ROW3")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30029)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 92.925 118.775) (xy 92.925 118.975) (xy 93.25 119.2) (xy 93.776 118.875) (xy 93.25 118.55)
			)
		)
	)
	(zone
		(net 37)
		(net_name "/Human-Machine Interface/Keypad/ROW3")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30035)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 94.625 118.975) (xy 94.625 118.775) (xy 94.3 118.55) (xy 93.774 118.875) (xy 94.3 119.2)
			)
		)
	)
	(zone
		(net 43)
		(net_name "/Human-Machine Interface/Keypad/ROW4")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30061)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 106.103012 100.458471) (xy 106.103012 100.658471) (xy 106.428012 100.883471) (xy 106.954012 100.558471)
				(xy 106.428012 100.233471)
			)
		)
	)
	(zone
		(net 5)
		(net_name "Net-(D1:2-A)")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30049)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 87.2584 107.525) (xy 87.2584 107.325) (xy 86.9334 107.1) (xy 86.4074 107.425) (xy 86.9334 107.75)
			)
		)
	)
	(zone
		(net 34)
		(net_name "/Human-Machine Interface/Keypad/COL2")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30109)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 90.375 100.25) (xy 90.575 100.25) (xy 90.667388 99.988268) (xy 90.475 99.099) (xy 90.282612 99.988268)
			)
		)
	)
	(zone
		(net 16)
		(net_name "Net-(D4:1-A)")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30022)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 82.371515 121.266804) (xy 82.371515 121.466804) (xy 82.696515 121.691804) (xy 83.222515 121.366804)
				(xy 82.696515 121.041804)
			)
		)
	)
	(zone
		(net 16)
		(net_name "Net-(D4:1-A)")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30079)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 79.845705 121.449826) (xy 79.987125 121.308406) (xy 79.596515 121.049152) (xy 79.070808 121.366097)
				(xy 79.596515 121.691804)
			)
		)
	)
	(zone
		(net 37)
		(net_name "/Human-Machine Interface/Keypad/ROW3")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30104)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 88.425 100.25) (xy 88.625 100.25) (xy 88.717388 99.988268) (xy 88.525 99.099) (xy 88.332612 99.988268)
			)
		)
	)
	(zone
		(net 42)
		(net_name "/Human-Machine Interface/Keypad/ROW1")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30087)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 82.3875 109.433) (xy 82.3875 109.633) (xy 82.7125 109.8) (xy 83.2385 109.475) (xy 82.7125 109.185095)
			)
		)
	)
	(zone
		(net 7)
		(net_name "Net-(D1:4-A)")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30071)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 115.472624 99.064045) (xy 115.614045 98.922624) (xy 115.513525 98.503905) (xy 114.987818 98.437818)
				(xy 114.853906 98.763525)
			)
		)
	)
	(zone
		(net 37)
		(net_name "/Human-Machine Interface/Keypad/ROW3")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30032)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 112.234703 104.461475) (xy 112.234703 104.661475) (xy 112.559703 104.886475) (xy 113.085703 104.561475)
				(xy 112.559703 104.236475)
			)
		)
	)
	(zone
		(net 42)
		(net_name "/Human-Machine Interface/Keypad/ROW1")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30063)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 91.4084 109.675) (xy 91.4084 109.475) (xy 91.0834 109.25) (xy 90.5574 109.575) (xy 91.0834 109.9)
			)
		)
	)
	(zone
		(net 71)
		(net_name "/Human-Machine Interface/BCLK")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30127)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 129.925 121.615) (xy 129.725 121.615) (xy 129.715 121.8025) (xy 129.84 122.1535) (xy 129.95436 121.769779)
			)
		)
	)
	(zone
		(net 10)
		(net_name "Net-(D2:3-A)")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30055)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 97.075 111.975) (xy 97.075 112.175) (xy 97.4 112.4) (xy 97.926 112.075) (xy 97.4 111.75)
			)
		)
	)
	(zone
		(net 41)
		(net_name "/Human-Machine Interface/Keypad/ROW2")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30041)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 87.2584 114.325) (xy 87.2584 114.125) (xy 86.9334 113.9) (xy 86.4074 114.225) (xy 86.9334 114.55)
			)
		)
	)
	(zone
		(net 41)
		(net_name "/Human-Machine Interface/Keypad/ROW2")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30077)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 84.0875 114.325) (xy 84.0875 114.125) (xy 83.7625 113.880344) (xy 83.2365 114.175) (xy 83.7625 114.5)
			)
		)
	)
	(zone
		(net 35)
		(net_name "/Human-Machine Interface/Keypad/COL3")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30115)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 91.025 100.25) (xy 91.225 100.25) (xy 91.317388 99.988268) (xy 91.125 99.099) (xy 90.932612 99.988268)
			)
		)
	)
	(zone
		(net 26)
		(net_name "+3.3V")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30098)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 94.515 97.95) (xy 94.235 97.95) (xy 94.182612 98.211732) (xy 94.375 99.101) (xy 94.567388 98.211732)
			)
		)
	)
	(zone
		(net 43)
		(net_name "/Human-Machine Interface/Keypad/ROW4")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30052)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 87.2584 123.625) (xy 87.2584 123.425) (xy 86.9334 123.2) (xy 86.4074 123.525) (xy 86.9334 123.85)
			)
		)
	)
	(zone
		(net 41)
		(net_name "/Human-Machine Interface/Keypad/ROW2")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30013)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 112.221315 96.482244) (xy 112.221315 96.682244) (xy 112.546315 96.907244) (xy 113.072315 96.582244)
				(xy 112.546315 96.257244)
			)
		)
	)
	(zone
		(net 42)
		(net_name "/Human-Machine Interface/Keypad/ROW1")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30018)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 87.2584 109.675) (xy 87.2584 109.475) (xy 86.9334 109.25) (xy 86.4074 109.575) (xy 86.9334 109.9)
			)
		)
	)
	(zone
		(net 42)
		(net_name "/Human-Machine Interface/Keypad/ROW1")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30116)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 87.125 100.25) (xy 87.325 100.25) (xy 87.417388 99.988268) (xy 87.225 99.099) (xy 87.032612 99.988268)
			)
		)
	)
	(zone
		(net 41)
		(net_name "/Human-Machine Interface/Keypad/ROW2")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30014)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 109.771315 96.682244) (xy 109.771315 96.482244) (xy 109.446315 96.257244) (xy 108.920315 96.582244)
				(xy 109.446315 96.907244)
			)
		)
	)
	(zone
		(net 39)
		(net_name "/Human-Machine Interface/ENC_SW")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30003)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 104.85 113.05) (xy 104.85 113.25) (xy 105.5 113.8) (xy 106.701 113.15) (xy 105.5 112.5)
			)
		)
	)
	(zone
		(net 55)
		(net_name "/Human-Machine Interface/PCF_A0")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30112)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 92.525 97.95) (xy 92.325 97.95) (xy 92.232612 98.211732) (xy 92.425 99.101) (xy 92.617388 98.211732)
			)
		)
	)
	(zone
		(net 4)
		(net_name "Net-(D1:1-A)")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30093)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 79.9375 107.516804) (xy 79.9375 107.316804) (xy 79.6125 107.054858) (xy 79.0865 107.325) (xy 79.6125 107.65)
			)
		)
	)
	(zone
		(net 4)
		(net_name "Net-(D1:1-A)")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30080)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 82.3875 107.283) (xy 82.3875 107.483) (xy 82.7125 107.65) (xy 83.2385 107.325) (xy 82.7125 107.035095)
			)
		)
	)
	(zone
		(net 37)
		(net_name "/Human-Machine Interface/Keypad/ROW3")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30068)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 84.071515 118.975) (xy 84.071515 118.775) (xy 83.746515 118.546854) (xy 83.220515 118.866804)
				(xy 83.746515 119.191804)
			)
		)
	)
	(zone
		(net 77)
		(net_name "Net-(IC1-P0)")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30097)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 92.212867 93.12071) (xy 92.354289 93.262132) (xy 92.503669 93.05) (xy 92.425707 92.099293) (xy 92.225 92.091763)
			)
		)
	)
	(zone
		(net 3)
		(net_name "Net-(C2-Pad1)")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30001)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 119.15 113) (xy 119.15 113.3) (xy 119.8 113.8) (xy 121.001 113.15) (xy 119.8 112.5)
			)
		)
	)
	(zone
		(net 17)
		(net_name "Net-(D4:2-A)")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30021)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 89.7084 121.275) (xy 89.7084 121.475) (xy 90.0334 121.7) (xy 90.5594 121.375) (xy 90.0334 121.05)
			)
		)
	)
	(zone
		(net 9)
		(net_name "Net-(D2:2-A)")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30053)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 89.7084 111.975) (xy 89.7084 112.175) (xy 90.0334 112.4) (xy 90.5594 112.075) (xy 90.0334 111.75)
			)
		)
	)
	(zone
		(net 37)
		(net_name "/Human-Machine Interface/Keypad/ROW3")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30028)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 89.7084 118.775) (xy 89.7084 118.975) (xy 90.0334 119.2) (xy 90.5594 118.875) (xy 90.0334 118.55)
			)
		)
	)
	(zone
		(net 43)
		(net_name "/Human-Machine Interface/Keypad/ROW4")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30067)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 91.4084 123.625) (xy 91.4084 123.425) (xy 91.0834 123.2) (xy 90.5574 123.525) (xy 91.0834 123.85)
			)
		)
	)
	(zone
		(net 42)
		(net_name "/Human-Machine Interface/Keypad/ROW1")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30076)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 85.5584 109.433) (xy 85.5584 109.633) (xy 85.8834 109.874435) (xy 86.4094 109.575) (xy 85.8834 109.25)
			)
		)
	)
	(zone
		(net 44)
		(net_name "/Human-Machine Interface/ENC_DT")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30111)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 88.625 90.95) (xy 88.425 90.95) (xy 88.332612 91.211732) (xy 88.525 92.101) (xy 88.717388 91.211732)
			)
		)
	)
	(zone
		(net 42)
		(net_name "/Human-Machine Interface/Keypad/ROW1")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30019)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 89.7084 109.475) (xy 89.7084 109.675) (xy 90.0334 109.9) (xy 90.5594 109.575) (xy 90.0334 109.25)
			)
		)
	)
	(zone
		(net 71)
		(net_name "/Human-Machine Interface/BCLK")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30009)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 129.925 117.075) (xy 129.725 117.075) (xy 129.392127 117.663896) (xy 129.825 118.001) (xy 130.257873 117.663896)
			)
		)
	)
	(zone
		(net 8)
		(net_name "Net-(D2:1-A)")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30083)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 82.3875 111.983) (xy 82.3875 112.183) (xy 82.7125 112.35) (xy 83.2385 112.025) (xy 82.7125 111.735095)
			)
		)
	)
	(zone
		(net 19)
		(net_name "Net-(D4:4-A)")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30119)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 106.101042 98.503714) (xy 106.242464 98.645136) (xy 106.428012 98.733471) (xy 106.953719 98.407764)
				(xy 106.428012 98.187508)
			)
		)
	)
	(zone
		(net 41)
		(net_name "/Human-Machine Interface/Keypad/ROW2")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30038)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 92.925 114.125) (xy 92.925 114.325) (xy 93.25 114.55) (xy 93.776 114.225) (xy 93.25 113.9)
			)
		)
	)
	(zone
		(net 41)
		(net_name "/Human-Machine Interface/Keypad/ROW2")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30040)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 97.075 114.125) (xy 97.075 114.325) (xy 97.4 114.55) (xy 97.926 114.225) (xy 97.4 113.9)
			)
		)
	)
	(zone
		(net 37)
		(net_name "/Human-Machine Interface/Keypad/ROW3")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30026)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 112.234703 104.461475) (xy 112.234703 104.661475) (xy 112.559703 104.886475) (xy 113.085703 104.561475)
				(xy 112.559703 104.236475)
			)
		)
	)
	(zone
		(net 37)
		(net_name "/Human-Machine Interface/Keypad/ROW3")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30074)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 98.775 119) (xy 98.775 118.8) (xy 98.45 118.565312) (xy 97.924 118.875) (xy 98.45 119.2)
			)
		)
	)
	(zone
		(net 14)
		(net_name "Net-(D3:3-A)")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30089)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 94.542395 116.824427) (xy 94.683815 116.683007) (xy 94.3 116.417534) (xy 93.774293 116.724293)
				(xy 94.3 117.05)
			)
		)
	)
	(zone
		(net 42)
		(net_name "/Human-Machine Interface/Keypad/ROW1")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30118)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 114.888525 101.238525) (xy 115.088525 101.238525) (xy 115.313525 100.913525) (xy 114.988525 100.587525)
				(xy 114.663525 100.913525)
			)
		)
	)
	(zone
		(net 43)
		(net_name "/Human-Machine Interface/Keypad/ROW4")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30064)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 84.071515 123.616804) (xy 84.071515 123.416804) (xy 83.746515 123.191804) (xy 83.220515 123.516804)
				(xy 83.746515 123.841804)
			)
		)
	)
	(zone
		(net 37)
		(net_name "/Human-Machine Interface/Keypad/ROW3")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30033)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 82.371515 118.766804) (xy 82.371515 118.966804) (xy 82.696515 119.191804) (xy 83.222515 118.866804)
				(xy 82.696515 118.541804)
			)
		)
	)
	(zone
		(net 26)
		(net_name "+3.3V")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30006)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 122.775 87.875) (xy 122.775 88.125) (xy 123.363896 88.432873) (xy 123.701 88) (xy 123.363896 87.567127)
			)
		)
	)
	(zone
		(net 70)
		(net_name "/~{PCF_INT}")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30103)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 94.475 90.95) (xy 94.275 90.95) (xy 94.182612 91.211732) (xy 94.375 92.101) (xy 94.567388 91.211732)
			)
		)
	)
	(zone
		(net 41)
		(net_name "/Human-Machine Interface/Keypad/ROW2")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30034)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 85.5584 114.125) (xy 85.5584 114.325) (xy 85.8834 114.55) (xy 86.4094 114.225) (xy 85.8834 113.9)
			)
		)
	)
	(zone
		(net 41)
		(net_name "/Human-Machine Interface/Keypad/ROW2")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30042)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 89.7084 114.125) (xy 89.7084 114.325) (xy 90.0334 114.55) (xy 90.5594 114.225) (xy 90.0334 113.9)
			)
		)
	)
	(zone
		(net 13)
		(net_name "Net-(D3:2-A)")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30066)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 89.7084 116.625) (xy 89.7084 116.825) (xy 90.0334 117.05) (xy 90.5594 116.725) (xy 90.0334 116.4)
			)
		)
	)
	(zone
		(net 12)
		(net_name "Net-(D3:1-A)")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30059)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 82.371515 116.616804) (xy 82.371515 116.816804) (xy 82.696515 117.041804) (xy 83.222515 116.716804)
				(xy 82.696515 116.391804)
			)
		)
	)
	(zone
		(net 17)
		(net_name "Net-(D4:2-A)")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30078)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 87.183682 121.455386) (xy 87.325102 121.313966) (xy 86.9334 121.055714) (xy 86.407693 121.374293)
				(xy 86.9334 121.7)
			)
		)
	)
	(zone
		(net 54)
		(net_name "/Human-Machine Interface/PCF_A2")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30099)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 92.975 93.25) (xy 93.175 93.25) (xy 93.267388 92.988268) (xy 93.075 92.099) (xy 92.882612 92.988268)
			)
		)
	)
	(zone
		(net 8)
		(net_name "Net-(D2:1-A)")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30075)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 79.9375 112.166804) (xy 79.9375 111.966804) (xy 79.6125 111.725446) (xy 79.0865 112.025) (xy 79.6125 112.35)
			)
		)
	)
	(zone
		(net 18)
		(net_name "Net-(D4:3-A)")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30020)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 97.075 121.275) (xy 97.075 121.475) (xy 97.4 121.7) (xy 97.926 121.375) (xy 97.4 121.05)
			)
		)
	)
	(zone
		(net 37)
		(net_name "/Human-Machine Interface/Keypad/ROW3")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30027)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 87.2584 118.975) (xy 87.2584 118.775) (xy 86.9334 118.55) (xy 86.4074 118.875) (xy 86.9334 119.2)
			)
		)
	)
	(zone
		(net 42)
		(net_name "/Human-Machine Interface/Keypad/ROW1")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30057)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 115.838525 100.688525) (xy 115.838525 100.488525) (xy 115.513525 100.263525) (xy 114.987525 100.588525)
				(xy 115.513525 100.913525)
			)
		)
	)
	(zone
		(net 40)
		(net_name "/Human-Machine Interface/ENC_CLK")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30105)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 87.975 90.95) (xy 87.775 90.95) (xy 87.682612 91.211732) (xy 87.875 92.101) (xy 88.067388 91.211732)
			)
		)
	)
	(zone
		(net 43)
		(net_name "/Human-Machine Interface/Keypad/ROW4")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30048)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 89.7084 123.425) (xy 89.7084 123.625) (xy 90.0334 123.85) (xy 90.5594 123.525) (xy 90.0334 123.2)
			)
		)
	)
	(zone
		(net 42)
		(net_name "/Human-Machine Interface/Keypad/ROW1")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30081)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 79.9375 109.633) (xy 79.9375 109.433) (xy 79.6125 109.185095) (xy 79.0865 109.475) (xy 79.6125 109.8)
			)
		)
	)
	(zone
		(net 43)
		(net_name "/Human-Machine Interface/Keypad/ROW4")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30065)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 92.925 123.425) (xy 92.925 123.625) (xy 93.25 123.85) (xy 93.776 123.525) (xy 93.25 123.2)
			)
		)
	)
	(zone
		(net 5)
		(net_name "Net-(D1:2-A)")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30050)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 89.7084 107.325) (xy 89.7084 107.525) (xy 90.0334 107.75) (xy 90.5594 107.425) (xy 90.0334 107.1)
			)
		)
	)
	(zone
		(net 42)
		(net_name "/Human-Machine Interface/Keypad/ROW1")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30017)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 97.075 109.475) (xy 97.075 109.675) (xy 97.4 109.9) (xy 97.926 109.575) (xy 97.4 109.25)
			)
		)
	)
	(zone
		(net 6)
		(net_name "Net-(D1:3-A)")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30045)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 97.075 107.325) (xy 97.075 107.525) (xy 97.4 107.75) (xy 97.926 107.425) (xy 97.4 107.1)
			)
		)
	)
	(zone
		(net 26)
		(net_name "+3.3V")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30002)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 122.85 115.79) (xy 122.85 115.51) (xy 122.2 115) (xy 120.999 115.65) (xy 122.2 116.3)
			)
		)
	)
	(zone
		(net 37)
		(net_name "/Human-Machine Interface/Keypad/ROW3")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30036)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 97.075 118.775) (xy 97.075 118.975) (xy 97.4 119.2) (xy 97.926 118.875) (xy 97.4 118.55)
			)
		)
	)
	(zone
		(net 37)
		(net_name "/Human-Machine Interface/Keypad/ROW3")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30025)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 79.921515 118.966804) (xy 79.921515 118.766804) (xy 79.596515 118.541804) (xy 79.070515 118.866804)
				(xy 79.596515 119.191804)
			)
		)
	)
	(zone
		(net 41)
		(net_name "/Human-Machine Interface/Keypad/ROW2")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30039)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 94.625 114.325) (xy 94.625 114.125) (xy 94.3 113.9) (xy 93.774 114.225) (xy 94.3 114.55)
			)
		)
	)
	(zone
		(net 73)
		(net_name "/Human-Machine Interface/LRCLK")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30126)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 130.94 121.615) (xy 130.74 121.615) (xy 130.715 121.8025) (xy 130.84 122.1535) (xy 130.965 121.8025)
			)
		)
	)
	(zone
		(net 41)
		(net_name "/Human-Machine Interface/Keypad/ROW2")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30015)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 98.775 114.325) (xy 98.775 114.125) (xy 98.45 113.9) (xy 97.924 114.225) (xy 98.45 114.55)
			)
		)
	)
	(zone
		(net 42)
		(net_name "/Human-Machine Interface/Keypad/ROW1")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30085)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 84.0875 109.633) (xy 84.0875 109.433) (xy 83.7625 109.185095) (xy 83.2365 109.475) (xy 83.7625 109.8)
			)
		)
	)
	(zone
		(net 19)
		(net_name "Net-(D4:4-A)")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30070)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 103.287111 99.033991) (xy 103.428532 98.89257) (xy 103.328012 98.473851) (xy 102.802305 98.407764)
				(xy 102.668393 98.733471)
			)
		)
	)
	(zone
		(net 18)
		(net_name "Net-(D4:3-A)")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30088)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 94.544983 121.468178) (xy 94.686403 121.326758) (xy 94.3 121.063649) (xy 93.774293 121.374293)
				(xy 94.3 121.7)
			)
		)
	)
	(zone
		(net 43)
		(net_name "/Human-Machine Interface/Keypad/ROW4")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30044)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 82.371515 123.416804) (xy 82.371515 123.616804) (xy 82.696515 123.841804) (xy 83.222515 123.516804)
				(xy 82.696515 123.191804)
			)
		)
	)
	(zone
		(net 43)
		(net_name "/Human-Machine Interface/Keypad/ROW4")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30060)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 103.653012 100.658471) (xy 103.653012 100.458471) (xy 103.328012 100.233471) (xy 102.802012 100.558471)
				(xy 103.328012 100.883471)
			)
		)
	)
	(zone
		(net 76)
		(net_name "/Human-Machine Interface/AMP_DIN")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30128)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 128.693033 122.751612) (xy 128.551612 122.893033) (xy 128.766849 122.952402) (xy 129.153207 122.840707)
				(xy 128.778582 122.719758)
			)
		)
	)
	(zone
		(net 23)
		(net_name "/SCL")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30108)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 92.975 100.25) (xy 93.175 100.25) (xy 93.267388 99.988268) (xy 93.075 99.099) (xy 92.882612 99.988268)
			)
		)
	)
	(zone
		(net 63)
		(net_name "Net-(U2-OUTP)")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30121)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 132.565 124.44) (xy 132.565 124.24) (xy 132.3775 124.215) (xy 132.0265 124.34) (xy 132.3775 124.465)
			)
		)
	)
	(zone
		(net 13)
		(net_name "Net-(D3:2-A)")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30092)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 87.17238 116.832671) (xy 87.3138 116.691251) (xy 86.9334 116.422667) (xy 86.407693 116.724293)
				(xy 86.9334 117.05)
			)
		)
	)
	(zone
		(net 11)
		(net_name "Net-(D2:4-A)")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30010)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 109.605414 95.057764) (xy 109.746835 94.916343) (xy 109.446315 94.414681) (xy 108.920608 94.431537)
				(xy 108.814946 94.757244)
			)
		)
	)
	(zone
		(net 42)
		(net_name "/Human-Machine Interface/Keypad/ROW1")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30072)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 98.775 109.7) (xy 98.775 109.5) (xy 98.45 109.265312) (xy 97.924 109.575) (xy 98.45 109.9)
			)
		)
	)
	(zone
		(net 42)
		(net_name "/Human-Machine Interface/Keypad/ROW1")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30016)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 118.288525 100.488525) (xy 118.288525 100.688525) (xy 118.613525 100.913525) (xy 119.139525 100.588525)
				(xy 118.613525 100.263525)
			)
		)
	)
	(zone
		(net 26)
		(net_name "+3.3V")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30123)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 130.74 125.565) (xy 130.94 125.565) (xy 130.965 125.3775) (xy 130.84 125.0265) (xy 130.715 125.3775)
			)
		)
	)
	(zone
		(net 43)
		(net_name "/Human-Machine Interface/Keypad/ROW4")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30069)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 85.5584 123.416804) (xy 85.5584 123.616804) (xy 85.8834 123.844949) (xy 86.4094 123.525) (xy 85.8834 123.2)
			)
		)
	)
	(zone
		(net 60)
		(net_name "/Human-Machine Interface/Audio/GAIN_SLOT")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30122)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 128.615 123.24) (xy 128.615 123.44) (xy 128.8025 123.465) (xy 129.1535 123.34) (xy 128.8025 123.215)
			)
		)
	)
	(zone
		(net 56)
		(net_name "/Human-Machine Interface/PCF_A1")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30114)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 93.625 93.25) (xy 93.825 93.25) (xy 93.917388 92.988268) (xy 93.725 92.099) (xy 93.532612 92.988268)
			)
		)
	)
	(zone
		(net 26)
		(net_name "+3.3V")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30007)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 123.025 88.125) (xy 123.025 87.875) (xy 122.436104 87.567127) (xy 122.099 88) (xy 122.436104 88.432873)
			)
		)
	)
	(zone
		(net 1)
		(net_name "GND")
		(layers "F.Cu" "B.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0.25)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 61.6644 73.9) (xy 142.3 74.2) (xy 142.8 142.6) (xy 60 142.25)
			)
		)
	)
	(zone
		(net 73)
		(net_name "/Human-Machine Interface/LRCLK")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30082)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 124.803156 87.083735) (xy 124.661735 87.225156) (xy 124.917 87.70811) (xy 125.178707 87.600707)
				(xy 125.24711 87.3)
			)
		)
	)
	(zone
		(net 64)
		(net_name "Net-(MK1-LR)")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30107)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 125.915148 87.032726) (xy 125.773726 87.174148) (xy 125.739 87.3) (xy 126.000707 87.600707)
				(xy 126.179792 87.3)
			)
		)
	)
	(zone
		(net 56)
		(net_name "/Human-Machine Interface/PCF_A1")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30012)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 71.489971 116.968608) (xy 71.631392 117.110029) (xy 72.435029 116.875) (xy 72.300707 116.474293)
				(xy 71.825 116.334241)
			)
		)
	)
	(zone
		(net 10)
		(net_name "Net-(D2:3-A)")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30078)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 95.091822 112.580524) (xy 94.891822 112.580524) (xy 94.64317 112.84707) (xy 95.0166 113.259)
				(xy 95.39003 112.84707)
			)
		)
	)
	(zone
		(net 3)
		(net_name "Net-(C2-Pad1)")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30062)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 107.120132 113.459843) (xy 107.120132 113.259843) (xy 106.672525 112.959843) (xy 106.319132 113.359843)
				(xy 106.672525 113.759843)
			)
		)
	)
	(zone
		(net 56)
		(net_name "/Human-Machine Interface/PCF_A1")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30052)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 73.175 116.575) (xy 73.175 116.375) (xy 72.651537 116.090224) (xy 72.299 116.475) (xy 72.651537 116.859776)
			)
		)
	)
	(zone
		(net 40)
		(net_name "/Human-Machine Interface/ENC_CLK")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30063)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 103.868356 117.931245) (xy 103.868356 118.131245) (xy 104.315963 118.431245) (xy 104.669356 118.031245)
				(xy 104.315963 117.631245)
			)
		)
	)
	(zone
		(net 2)
		(net_name "Net-(C1-Pad1)")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30043)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 110.281994 118.240545) (xy 110.281994 117.940545) (xy 109.758531 117.719241) (xy 109.405994 118.104017)
				(xy 109.758531 118.488793)
			)
		)
	)
	(zone
		(net 54)
		(net_name "/Human-Machine Interface/PCF_A2")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30109)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 71.175 114.2) (xy 71.175 114) (xy 71.025 113.938037) (xy 70.524 114.05) (xy 71.025 114.238921)
			)
		)
	)
	(zone
		(net 75)
		(net_name "/Human-Machine Interface/~{AMP_SD}")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30095)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 115.119254 86.418651) (xy 115.319254 86.418651) (xy 115.369254 86.268651) (xy 115.219254 85.617651)
				(xy 115.069254 86.268651)
			)
		)
	)
	(zone
		(net 26)
		(net_name "+3.3V")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30056)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 109.3 115.760118) (xy 109.5 115.760118) (xy 109.806053 115.315713) (xy 109.410845 114.959118)
				(xy 109.006067 115.309318)
			)
		)
	)
	(zone
		(net 30)
		(net_name "/SCK")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30094)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 87.510249 84.818651) (xy 87.310249 84.818651) (xy 87.260249 84.968651) (xy 87.410249 85.619651)
				(xy 87.560249 84.968651)
			)
		)
	)
	(zone
		(net 30)
		(net_name "/SCK")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30110)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 109.094937 86.325736) (xy 109.236358 86.467157) (xy 109.324928 86.268651) (xy 109.219961 85.617944)
				(xy 109.069254 86.268651)
			)
		)
	)
	(zone
		(net 34)
		(net_name "/Human-Machine Interface/Keypad/COL2")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30021)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 89.175 114.1705) (xy 89.375 114.1705) (xy 89.695849 113.597962) (xy 89.275 113.257) (xy 88.854151 113.597962)
			)
		)
	)
	(zone
		(net 65)
		(net_name "Net-(MK1-SD)")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30041)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 121.828553 90.293629) (xy 121.687132 90.152208) (xy 120.890173 90.275) (xy 120.999293 90.675707)
				(xy 121.475 90.857593)
			)
		)
	)
	(zone
		(net 55)
		(net_name "/Human-Machine Interface/PCF_A0")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30050)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 71.425 121.125) (xy 71.425 121.325) (xy 71.948463 121.609776) (xy 72.301 121.225) (xy 71.948463 120.840224)
			)
		)
	)
	(zone
		(net 38)
		(net_name "/Human-Machine Interface/TFTRST")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30086)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 89.310249 86.418651) (xy 89.510249 86.418651) (xy 89.560249 86.268651) (xy 89.410249 85.617651)
				(xy 89.260249 86.268651)
			)
		)
	)
	(zone
		(net 55)
		(net_name "/Human-Machine Interface/PCF_A0")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30108)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 71.175 121.325) (xy 71.175 121.125) (xy 71.025 121.056727) (xy 70.524 121.15) (xy 71.025 121.35871)
			)
		)
	)
	(zone
		(net 65)
		(net_name "Net-(MK1-SD)")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30084)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 124.656 88.4) (xy 124.656 88.6) (xy 124.917 88.761) (xy 125.179 88.5) (xy 124.917 88.239)
			)
		)
	)
	(zone
		(net 34)
		(net_name "/Human-Machine Interface/Keypad/COL2")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30025)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 89.35 121.5455) (xy 89.15 121.5455) (xy 88.829151 122.118038) (xy 89.25 122.459) (xy 89.670849 122.118038)
			)
		)
	)
	(zone
		(net 59)
		(net_name "/Human-Machine Interface/Audio/~{SD_MODE}")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30059)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 117.104634 93.345446) (xy 117.304634 93.345446) (xy 117.604634 92.897839) (xy 117.204634 92.544446)
				(xy 116.804634 92.897839)
			)
		)
	)
	(zone
		(net 8)
		(net_name "Net-(D2:1-A)")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30069)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 80.473246 112.483989) (xy 80.273246 112.483989) (xy 80.039685 112.758074) (xy 80.413115 113.170004)
				(xy 80.786545 112.758074)
			)
		)
	)
	(zone
		(net 36)
		(net_name "/Human-Machine Interface/Keypad/COL4")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30036)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 111.897203 104.048975) (xy 111.697203 104.048975) (xy 111.376354 104.621513) (xy 111.797203 104.962475)
				(xy 112.218052 104.621513)
			)
		)
	)
	(zone
		(net 28)
		(net_name "/CARDCS")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30097)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 112.119254 86.418651) (xy 112.319254 86.418651) (xy 112.369254 86.268651) (xy 112.219254 85.617651)
				(xy 112.069254 86.268651)
			)
		)
	)
	(zone
		(net 76)
		(net_name "/Human-Machine Interface/AMP_DIN")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30098)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 112.819254 84.818651) (xy 112.619254 84.818651) (xy 112.569254 84.968651) (xy 112.719254 85.619651)
				(xy 112.869254 84.968651)
			)
		)
	)
	(zone
		(net 33)
		(net_name "/Human-Machine Interface/Keypad/COL1")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30034)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 81.863115 118.762304) (xy 82.063115 118.762304) (xy 82.396464 118.189766) (xy 81.975615 117.848804)
				(xy 81.554766 118.189766)
			)
		)
	)
	(zone
		(net 35)
		(net_name "/Human-Machine Interface/Keypad/COL3")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30013)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 96.5375 114.1705) (xy 96.7375 114.1705) (xy 97.012449 113.597962) (xy 96.5916 113.257) (xy 96.170751 113.597962)
			)
		)
	)
	(zone
		(net 34)
		(net_name "/Human-Machine Interface/Keypad/COL2")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30019)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 89.3625 107.5455) (xy 89.1625 107.5455) (xy 88.841651 108.118038) (xy 89.2625 108.459) (xy 89.683349 108.118038)
			)
		)
	)
	(zone
		(net 35)
		(net_name "/Human-Machine Interface/Keypad/COL3")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30020)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 96.6916 121.5455) (xy 96.4916 121.5455) (xy 96.170751 122.118038) (xy 96.5916 122.459) (xy 97.012449 122.118038)
			)
		)
	)
	(zone
		(net 65)
		(net_name "Net-(MK1-SD)")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30045)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 121.737132 88.778553) (xy 121.878553 88.637132) (xy 121.525 87.998852) (xy 121.124293 88.199293)
				(xy 121.093576 88.675)
			)
		)
	)
	(zone
		(net 36)
		(net_name "/Human-Machine Interface/Keypad/COL4")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30040)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 105.3 103.664674) (xy 105.5 103.664674) (xy 105.991145 103.204341) (xy 105.665512 102.760475)
				(xy 105.228012 103.017725)
			)
		)
	)
	(zone
		(net 36)
		(net_name "/Human-Machine Interface/Keypad/COL4")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30037)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 111.732858 100.839273) (xy 111.932858 100.839273) (xy 112.253707 100.266735) (xy 111.832858 99.925773)
				(xy 111.412009 100.266735)
			)
		)
	)
	(zone
		(net 59)
		(net_name "/Human-Machine Interface/Audio/~{SD_MODE}")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30058)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 117.304634 93.2) (xy 117.104634 93.2) (xy 116.802045 93.646239) (xy 117.2 94.001) (xy 117.602042 93.648971)
			)
		)
	)
	(zone
		(net 35)
		(net_name "/Human-Machine Interface/Keypad/COL3")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30065)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 96.352951 107.602931) (xy 96.21153 107.744352) (xy 96.1541 108.20175) (xy 96.592307 108.458707)
				(xy 96.880305 107.996914)
			)
		)
	)
	(zone
		(net 24)
		(net_name "/TFTDC")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30104)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 88.810249 86.418651) (xy 89.010249 86.418651) (xy 89.060249 86.268651) (xy 88.910249 85.617651)
				(xy 88.760249 86.268651)
			)
		)
	)
	(zone
		(net 27)
		(net_name "/TFTCS")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30101)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 111.619254 86.418651) (xy 111.819254 86.418651) (xy 111.869254 86.268651) (xy 111.719254 85.617651)
				(xy 111.569254 86.268651)
			)
		)
	)
	(zone
		(net 22)
		(net_name "/SDA")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30106)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 114.119254 86.418651) (xy 114.319254 86.418651) (xy 114.369254 86.268651) (xy 114.219254 85.617651)
				(xy 114.069254 86.268651)
			)
		)
	)
	(zone
		(net 3)
		(net_name "Net-(C2-Pad1)")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30042)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 110.285845 113.454475) (xy 110.285845 113.154475) (xy 109.762382 112.925342) (xy 109.409845 113.310118)
				(xy 109.762382 113.694894)
			)
		)
	)
	(zone
		(net 9)
		(net_name "Net-(D2:2-A)")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30077)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 87.790915 112.580524) (xy 87.590915 112.580524) (xy 87.32657 112.84707) (xy 87.7 113.259) (xy 88.07343 112.84707)
			)
		)
	)
	(zone
		(net 36)
		(net_name "/Human-Machine Interface/Keypad/COL4")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30005)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 106.434031 102.134377) (xy 106.29261 101.992956) (xy 105.521793 102.286475) (xy 105.664805 102.762182)
				(xy 106.103012 102.942693)
			)
		)
	)
	(zone
		(net 26)
		(net_name "+3.3V")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30007)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 109.960051 115.717495) (xy 110.158041 115.519505) (xy 109.885845 114.872441) (xy 109.410138 114.959411)
				(xy 109.243322 115.360118)
			)
		)
	)
	(zone
		(net 26)
		(net_name "+3.3V")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30057)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 109.5 115.654017) (xy 109.3 115.654017) (xy 109.00391 116.103683) (xy 109.406994 116.455017)
				(xy 109.803905 116.09956)
			)
		)
	)
	(zone
		(net 54)
		(net_name "/Human-Machine Interface/PCF_A2")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30055)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 72.5 112.675) (xy 72.3 112.675) (xy 71.944746 113.092707) (xy 72.3 113.476) (xy 72.74122 113.170694)
			)
		)
	)
	(zone
		(net 14)
		(net_name "Net-(D3:3-A)")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30079)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 95.133473 117.174085) (xy 94.933473 117.174085) (xy 94.68907 117.43987) (xy 95.0625 117.8518)
				(xy 95.43593 117.43987)
			)
		)
	)
	(zone
		(net 71)
		(net_name "/Human-Machine Interface/BCLK")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30085)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 125.886156 89.872423) (xy 126.027577 90.013844) (xy 126.238313 89.7) (xy 126.000707 89.399293)
				(xy 125.739 89.7)
			)
		)
	)
	(zone
		(net 33)
		(net_name "/Human-Machine Interface/Keypad/COL1")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30035)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 82.063115 121.537304) (xy 81.863115 121.537304) (xy 81.542266 122.109842) (xy 81.963115 122.450804)
				(xy 82.383964 122.109842)
			)
		)
	)
	(zone
		(net 6)
		(net_name "Net-(D1:3-A)")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30073)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 95.097772 107.778704) (xy 94.897772 107.778704) (xy 94.64317 108.04707) (xy 95.0166 108.459)
				(xy 95.39003 108.04707)
			)
		)
	)
	(zone
		(net 7)
		(net_name "Net-(D1:4-A)")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30023)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 116.197203 101.848975) (xy 115.997203 101.848975) (xy 115.676354 102.421513) (xy 116.097203 102.762475)
				(xy 116.518052 102.421513)
			)
		)
	)
	(zone
		(net 55)
		(net_name "/Human-Machine Interface/PCF_A0")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30051)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 73.175 121.325) (xy 73.175 121.125) (xy 72.651537 120.840224) (xy 72.299 121.225) (xy 72.651537 121.609776)
			)
		)
	)
	(zone
		(net 2)
		(net_name "Net-(C1-Pad1)")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30008)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 106.916716 117.931245) (xy 106.916716 118.131245) (xy 107.505612 118.481878) (xy 107.842716 118.049005)
				(xy 107.505612 117.616132)
			)
		)
	)
	(zone
		(net 18)
		(net_name "Net-(D4:3-A)")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30070)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 95.091822 121.773597) (xy 94.891822 121.773597) (xy 94.64317 122.04707) (xy 95.0166 122.459)
				(xy 95.39003 122.04707)
			)
		)
	)
	(zone
		(net 2)
		(net_name "Net-(C1-Pad1)")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30047)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 108.531994 117.990545) (xy 108.531994 118.190545) (xy 109.055457 118.488793) (xy 109.407994 118.104017)
				(xy 109.055457 117.719241)
			)
		)
	)
	(zone
		(net 58)
		(net_name "Net-(JP4-C)")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30064)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 131.275 116) (xy 131.275 115.8) (xy 130.751537 115.690224) (xy 130.399 116.075) (xy 130.829458 116.396909)
			)
		)
	)
	(zone
		(net 34)
		(net_name "/Human-Machine Interface/Keypad/COL2")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30022)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 89.375 116.9455) (xy 89.175 116.9455) (xy 88.829151 117.518038) (xy 89.25 117.859) (xy 89.670849 117.518038)
			)
		)
	)
	(zone
		(net 70)
		(net_name "/~{PCF_INT}")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30096)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 114.619254 86.418651) (xy 114.819254 86.418651) (xy 114.869254 86.268651) (xy 114.719254 85.617651)
				(xy 114.569254 86.268651)
			)
		)
	)
	(zone
		(net 36)
		(net_name "/Human-Machine Interface/Keypad/COL4")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30004)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 116.903684 103.388573) (xy 117.045105 103.529994) (xy 117.815921 103.236475) (xy 117.67291 102.760768)
				(xy 117.234703 102.580256)
			)
		)
	)
	(zone
		(net 34)
		(net_name "/Human-Machine Interface/Keypad/COL2")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30026)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 89.175 109.3705) (xy 89.375 109.3705) (xy 89.683349 108.797962) (xy 89.2625 108.457) (xy 88.841651 108.797962)
			)
		)
	)
	(zone
		(net 33)
		(net_name "/Human-Machine Interface/Keypad/COL1")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30029)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 82.088115 107.617631) (xy 81.888115 107.617631) (xy 81.567266 108.190169) (xy 81.988115 108.531131)
				(xy 82.408964 108.190169)
			)
		)
	)
	(zone
		(net 60)
		(net_name "/Human-Machine Interface/Audio/GAIN_SLOT")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30002)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 131.65 116.8) (xy 131.65 117) (xy 132.15 117.4) (xy 132.901 116.9) (xy 132.15 116.4)
			)
		)
	)
	(zone
		(net 12)
		(net_name "Net-(D3:1-A)")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30072)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 80.473246 117.166804) (xy 80.273246 117.166804) (xy 80.027185 117.438874) (xy 80.400615 117.850804)
				(xy 80.774045 117.438874)
			)
		)
	)
	(zone
		(net 71)
		(net_name "/Human-Machine Interface/BCLK")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30090)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 115.619254 86.418651) (xy 115.819254 86.418651) (xy 115.869254 86.268651) (xy 115.719254 85.617651)
				(xy 115.569254 86.268651)
			)
		)
	)
	(zone
		(net 63)
		(net_name "Net-(U2-OUTP)")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30000)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 125.25 131.95) (xy 125.25 131.75) (xy 124.326777 131.073223) (xy 123.399 131.85) (xy 124.326777 132.626777)
			)
		)
	)
	(zone
		(net 26)
		(net_name "+3.3V")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30083)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 124.656 89.375) (xy 124.656 89.625) (xy 124.917 89.7) (xy 125.179 89.4) (xy 124.917 89.184367)
			)
		)
	)
	(zone
		(net 33)
		(net_name "/Human-Machine Interface/Keypad/COL1")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30033)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 82.088115 116.937304) (xy 81.888115 116.937304) (xy 81.554766 117.509842) (xy 81.975615 117.850804)
				(xy 82.396464 117.509842)
			)
		)
	)
	(zone
		(net 4)
		(net_name "Net-(D1:1-A)")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30075)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 80.487778 107.851726) (xy 80.287778 107.851726) (xy 80.039685 108.119201) (xy 80.413115 108.531131)
				(xy 80.786545 108.119201)
			)
		)
	)
	(zone
		(net 3)
		(net_name "Net-(C2-Pad1)")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30049)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 108.535845 113.204475) (xy 108.535845 113.404475) (xy 109.059308 113.694894) (xy 109.411845 113.310118)
				(xy 109.059308 112.925342)
			)
		)
	)
	(zone
		(net 33)
		(net_name "/Human-Machine Interface/Keypad/COL1")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30030)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 82.088115 112.256504) (xy 81.888115 112.256504) (xy 81.567266 112.829042) (xy 81.988115 113.170004)
				(xy 82.408964 112.829042)
			)
		)
	)
	(zone
		(net 3)
		(net_name "Net-(C2-Pad1)")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30011)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 108.764987 113.404475) (xy 108.764987 113.204475) (xy 108.176091 112.910987) (xy 107.838987 113.34386)
				(xy 108.176091 113.776733)
			)
		)
	)
	(zone
		(net 15)
		(net_name "Net-(D3:4-A)")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30006)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 110.984703 104.24904) (xy 110.784703 104.24904) (xy 110.067179 104.486475) (xy 110.222203 104.962475)
				(xy 110.659703 105.134281)
			)
		)
	)
	(zone
		(net 58)
		(net_name "Net-(JP4-C)")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30003)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 128.932842 116.758579) (xy 128.791421 116.617158) (xy 128.45 116.4) (xy 127.699293 116.900707)
				(xy 128.45 117.271608)
			)
		)
	)
	(zone
		(net 44)
		(net_name "/Human-Machine Interface/ENC_DT")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30038)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 104.086538 112.634828) (xy 103.945117 112.776249) (xy 104.270132 113.525528) (xy 104.670839 113.36055)
				(xy 104.760817 112.884843)
			)
		)
	)
	(zone
		(net 16)
		(net_name "Net-(D4:1-A)")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30081)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 80.464314 121.827015) (xy 80.264314 121.827015) (xy 80.014685 122.038874) (xy 80.388115 122.450804)
				(xy 80.761545 122.038874)
			)
		)
	)
	(zone
		(net 19)
		(net_name "Net-(D4:4-A)")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30015)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 104.190512 101.848975) (xy 103.990512 101.848975) (xy 103.669663 102.421513) (xy 104.090512 102.762475)
				(xy 104.511361 102.421513)
			)
		)
	)
	(zone
		(net 11)
		(net_name "Net-(D2:4-A)")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30018)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 110.357858 99.014273) (xy 110.157858 99.014273) (xy 109.837009 99.586811) (xy 110.257858 99.927773)
				(xy 110.678707 99.586811)
			)
		)
	)
	(zone
		(net 13)
		(net_name "Net-(D3:2-A)")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30076)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 87.761164 117.180035) (xy 87.561164 117.180035) (xy 87.30157 117.44707) (xy 87.675 117.859)
				(xy 88.04843 117.44707)
			)
		)
	)
	(zone
		(net 29)
		(net_name "/MISO")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30089)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 88.510249 84.818651) (xy 88.310249 84.818651) (xy 88.260249 84.968651) (xy 88.410249 85.619651)
				(xy 88.560249 84.968651)
			)
		)
	)
	(zone
		(net 23)
		(net_name "/SCL")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30105)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 113.619254 86.418651) (xy 113.819254 86.418651) (xy 113.869254 86.268651) (xy 113.719254 85.617651)
				(xy 113.569254 86.268651)
			)
		)
	)
	(zone
		(net 2)
		(net_name "Net-(C1-Pad1)")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30009)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 108.766716 118.190545) (xy 108.766716 117.990545) (xy 108.17782 117.616132) (xy 107.840716 118.049005)
				(xy 108.17782 118.481878)
			)
		)
	)
	(zone
		(net 24)
		(net_name "/TFTDC")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30103)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 110.619254 86.418651) (xy 110.819254 86.418651) (xy 110.869254 86.268651) (xy 110.719254 85.617651)
				(xy 110.569254 86.268651)
			)
		)
	)
	(zone
		(net 35)
		(net_name "/Human-Machine Interface/Keypad/COL3")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30014)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 96.4916 118.7633) (xy 96.6916 118.7633) (xy 97.058349 118.190762) (xy 96.6375 117.8498) (xy 96.216651 118.190762)
			)
		)
	)
	(zone
		(net 58)
		(net_name "Net-(JP4-C)")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30068)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 131.9 115.8) (xy 131.9 116) (xy 132.15 116.08606) (xy 132.901 115.6) (xy 132.154278 115.562807)
			)
		)
	)
	(zone
		(net 74)
		(net_name "/Human-Machine Interface/MIC_DOUT")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30093)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 113.119254 86.418651) (xy 113.319254 86.418651) (xy 113.369254 86.268651) (xy 113.219254 85.617651)
				(xy 113.069254 86.268651)
			)
		)
	)
	(zone
		(net 61)
		(net_name "Net-(JP6-B)")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30044)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 131.128575 118.3) (xy 131.128575 118.1) (xy 130.875 117.5576) (xy 130.399 117.725) (xy 130.280262 118.125)
			)
		)
	)
	(zone
		(net 35)
		(net_name "/Human-Machine Interface/Keypad/COL3")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30017)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 96.4916 109.3705) (xy 96.6916 109.3705) (xy 97.012449 108.797962) (xy 96.5916 108.457) (xy 96.170751 108.797962)
			)
		)
	)
	(zone
		(net 32)
		(net_name "/MOSI")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30091)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 109.619254 86.418651) (xy 109.819254 86.418651) (xy 109.869254 86.268651) (xy 109.719254 85.617651)
				(xy 109.569254 86.268651)
			)
		)
	)
	(zone
		(net 74)
		(net_name "/Human-Machine Interface/MIC_DOUT")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30061)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 118.675 88.1) (xy 118.675 88.3) (xy 119.122607 88.6) (xy 119.476 88.2) (xy 119.122607 87.8)
			)
		)
	)
	(zone
		(net 2)
		(net_name "Net-(C1-Pad1)")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30060)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 107.118356 118.131245) (xy 107.118356 117.931245) (xy 106.670749 117.631245) (xy 106.317356 118.031245)
				(xy 106.670749 118.431245)
			)
		)
	)
	(zone
		(net 35)
		(net_name "/Human-Machine Interface/Keypad/COL3")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30028)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 96.7375 116.9383) (xy 96.5375 116.9383) (xy 96.216651 117.510838) (xy 96.6375 117.8518) (xy 97.058349 117.510838)
			)
		)
	)
	(zone
		(net 75)
		(net_name "/Human-Machine Interface/~{AMP_SD}")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30048)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 116.329634 90.795446) (xy 116.329634 90.995446) (xy 116.853097 91.280222) (xy 117.205634 90.895446)
				(xy 116.853097 90.51067)
			)
		)
	)
	(zone
		(net 27)
		(net_name "/TFTCS")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30100)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 90.010249 84.818651) (xy 89.810249 84.818651) (xy 89.760249 84.968651) (xy 89.910249 85.619651)
				(xy 90.060249 84.968651)
			)
		)
	)
	(zone
		(net 32)
		(net_name "/MOSI")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30087)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 88.010249 84.818651) (xy 87.810249 84.818651) (xy 87.760249 84.968651) (xy 87.910249 85.619651)
				(xy 88.060249 84.968651)
			)
		)
	)
	(zone
		(net 59)
		(net_name "/Human-Machine Interface/Audio/~{SD_MODE}")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30046)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 118.075 94.1) (xy 118.075 93.9) (xy 117.551537 93.615224) (xy 117.199 94) (xy 117.551537 94.384776)
			)
		)
	)
	(zone
		(net 34)
		(net_name "/Human-Machine Interface/Keypad/COL2")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30024)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 89.15 118.7705) (xy 89.35 118.7705) (xy 89.670849 118.197962) (xy 89.25 117.857) (xy 88.829151 118.197962)
			)
		)
	)
	(zone
		(net 5)
		(net_name "Net-(D1:2-A)")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30066)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 87.779014 107.754904) (xy 87.579014 107.754904) (xy 87.31407 108.04707) (xy 87.6875 108.459)
				(xy 88.06093 108.04707)
			)
		)
	)
	(zone
		(net 54)
		(net_name "/Human-Machine Interface/PCF_A2")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30071)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 71.918198 114) (xy 71.918198 114.2) (xy 72.525072 113.875) (xy 72.301 113.475) (xy 71.825 113.675)
			)
		)
	)
	(zone
		(net 62)
		(net_name "Net-(U2-OUTN)")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30001)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 125.233667 129.45) (xy 125.233667 129.25) (xy 124.022235 128.643251) (xy 123.399 129.35) (xy 124.022235 130.056749)
			)
		)
	)
	(zone
		(net 56)
		(net_name "/Human-Machine Interface/PCF_A1")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30111)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 71.201776 117.539645) (xy 71.060355 117.398224) (xy 71.025 117.338473) (xy 70.524293 117.600707)
				(xy 71.025 117.645465)
			)
		)
	)
	(zone
		(net 28)
		(net_name "/CARDCS")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30099)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 90.510249 84.818651) (xy 90.310249 84.818651) (xy 90.260249 84.968651) (xy 90.410249 85.619651)
				(xy 90.560249 84.968651)
			)
		)
	)
	(zone
		(net 58)
		(net_name "Net-(JP4-C)")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30054)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 129.525 115.975) (xy 129.525 116.175) (xy 130.048463 116.459776) (xy 130.401 116.075) (xy 130.048463 115.690224)
			)
		)
	)
	(zone
		(net 33)
		(net_name "/Human-Machine Interface/Keypad/COL1")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30032)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 81.888115 114.081504) (xy 82.088115 114.081504) (xy 82.408964 113.508966) (xy 81.988115 113.168004)
				(xy 81.567266 113.508966)
			)
		)
	)
	(zone
		(net 33)
		(net_name "/Human-Machine Interface/Keypad/COL1")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30031)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 81.888115 109.442631) (xy 82.088115 109.442631) (xy 82.408964 108.870093) (xy 81.988115 108.529131)
				(xy 81.567266 108.870093)
			)
		)
	)
	(zone
		(net 34)
		(net_name "/Human-Machine Interface/Keypad/COL2")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30027)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 89.375 112.3455) (xy 89.175 112.3455) (xy 88.854151 112.918038) (xy 89.275 113.259) (xy 89.695849 112.918038)
			)
		)
	)
	(zone
		(net 61)
		(net_name "Net-(JP6-B)")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30080)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 131.904278 118.1) (xy 131.904278 118.3) (xy 132.221926 118.45) (xy 132.901 118.2) (xy 132.15 117.95)
			)
		)
	)
	(zone
		(net 26)
		(net_name "+3.3V")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30039)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 110.052546 115.94) (xy 110.052546 115.66) (xy 109.238962 116.054017) (xy 109.405994 116.454017)
				(xy 109.881994 116.541481)
			)
		)
	)
	(zone
		(net 29)
		(net_name "/MISO")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30088)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 110.119254 86.418651) (xy 110.319254 86.418651) (xy 110.369254 86.268651) (xy 110.219254 85.617651)
				(xy 110.069254 86.268651)
			)
		)
	)
	(zone
		(net 45)
		(net_name "/Human-Machine Interface/LITE")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30102)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 86.510249 84.818651) (xy 86.310249 84.818651) (xy 86.260249 84.968651) (xy 86.410249 85.619651)
				(xy 86.560249 84.968651)
			)
		)
	)
	(zone
		(net 26)
		(net_name "+3.3V")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30067)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 126.704278 115.46) (xy 126.704278 115.74) (xy 126.95 115.85) (xy 127.701 115.6) (xy 127.021926 115.35)
			)
		)
	)
	(zone
		(net 64)
		(net_name "Net-(MK1-LR)")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30053)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 123.375 84.925) (xy 123.375 84.725) (xy 122.851537 84.440224) (xy 122.499 84.825) (xy 122.851537 85.209776)
			)
		)
	)
	(zone
		(net 73)
		(net_name "/Human-Machine Interface/LRCLK")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30092)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 116.319254 84.818651) (xy 116.119254 84.818651) (xy 116.069254 84.968651) (xy 116.219254 85.619651)
				(xy 116.369254 84.968651)
			)
		)
	)
	(zone
		(net 3)
		(net_name "Net-(C2-Pad1)")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30010)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 106.914987 113.259843) (xy 106.914987 113.459843) (xy 107.503883 113.776733) (xy 107.840987 113.34386)
				(xy 107.503883 112.910987)
			)
		)
	)
	(zone
		(net 35)
		(net_name "/Human-Machine Interface/Keypad/COL3")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30016)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 96.6916 112.3455) (xy 96.4916 112.3455) (xy 96.170751 112.918038) (xy 96.5916 113.259) (xy 97.012449 112.918038)
			)
		)
	)
	(zone
		(net 17)
		(net_name "Net-(D4:2-A)")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30074)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 87.749263 121.779547) (xy 87.549263 121.779547) (xy 87.30157 122.04707) (xy 87.675 122.459)
				(xy 88.04843 122.04707)
			)
		)
	)
	(embedded_fonts no)
)
