(kicad_pcb
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(general
		(thickness 1.6)
		(legacy_teardrops no)
	)
	(paper "USLetter")
	(title_block
		(title "MiniNDP")
		(date "2026-08-29")
		(rev "u1M_038")
		(company "Brian K. White - b.kenyon.w@gmail.com")
		(comment 1 "github.com/bkw777/NODE_DATAPAC")
		(comment 2 "1M RAM Disk for TRS-80 Model 100 and Kyotronic KC-85")
	)
	(layers
		(0 "F.Cu" signal)
		(2 "B.Cu" signal)
		(9 "F.Adhes" user "F.Adhesive")
		(11 "B.Adhes" user "B.Adhesive")
		(13 "F.Paste" user)
		(15 "B.Paste" user)
		(5 "F.SilkS" user "F.Silkscreen")
		(7 "B.SilkS" user "B.Silkscreen")
		(1 "F.Mask" user)
		(3 "B.Mask" user)
		(17 "Dwgs.User" user "User.Drawings")
		(19 "Cmts.User" user "User.Comments")
		(21 "Eco1.User" user "User.Eco1")
		(23 "Eco2.User" user "User.Eco2")
		(25 "Edge.Cuts" user)
		(27 "Margin" user)
		(31 "F.CrtYd" user "F.Courtyard")
		(29 "B.CrtYd" user "B.Courtyard")
		(35 "F.Fab" user)
		(33 "B.Fab" user)
	)
	(setup
		(stackup
			(layer "F.SilkS"
				(type "Top Silk Screen")
			)
			(layer "F.Paste"
				(type "Top Solder Paste")
			)
			(layer "F.Mask"
				(type "Top Solder Mask")
				(thickness 0.01)
			)
			(layer "F.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "dielectric 1"
				(type "core")
				(thickness 1.51)
				(material "FR4")
				(epsilon_r 4.5)
				(loss_tangent 0.02)
			)
			(layer "B.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "B.Mask"
				(type "Bottom Solder Mask")
				(thickness 0.01)
			)
			(layer "B.Paste"
				(type "Bottom Solder Paste")
			)
			(layer "B.SilkS"
				(type "Bottom Silk Screen")
			)
			(copper_finish "ENIG")
			(dielectric_constraints no)
		)
		(pad_to_mask_clearance 0)
		(solder_mask_min_width 0.22)
		(allow_soldermask_bridges_in_footprints yes)
		(tenting front back)
		(grid_origin 150 100)
		(pcbplotparams
			(layerselection 0x00000000_00000000_55555555_f755f5ff)
			(plot_on_all_layers_selection 0x00000000_00000000_00000000_00000000)
			(disableapertmacros no)
			(usegerberextensions yes)
			(usegerberattributes no)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 6)
			(plotframeref no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(pdf_metadata yes)
			(pdf_single_document no)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plot_black_and_white yes)
			(sketchpadsonfab no)
			(plotpadnumbers no)
			(hidednponfab no)
			(sketchdnponfab yes)
			(crossoutdnponfab yes)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 0)
			(scaleselection 1)
			(outputdirectory "GERBER_${TITLE}_${REVISION}")
		)
	)
	(net 0 "")
	(net 1 "GND")
	(net 2 "/AD1")
	(net 3 "/AD3")
	(net 4 "/AD5")
	(net 5 "/AD7")
	(net 6 "/AD6")
	(net 7 "/AD4")
	(net 8 "/AD2")
	(net 9 "/AD0")
	(net 10 "VBUS")
	(net 11 "unconnected-(J1-CLK-Pad15)")
	(net 12 "unconnected-(J1-INTR-Pad17)")
	(net 13 "VMEM")
	(net 14 "unconnected-(J1-NC-Pad20)")
	(net 15 "unconnected-(J1-NC-Pad21)")
	(net 16 "unconnected-(J1-NC-Pad22)")
	(net 17 "unconnected-(J1-~{INTA}-Pad24)")
	(net 18 "unconnected-(J1-S1-Pad27)")
	(net 19 "unconnected-(J1-S0-Pad28)")
	(net 20 "+BATT")
	(net 21 "/~{RD}")
	(net 22 "unconnected-(J1-IO{slash}~{M}-Pad13)")
	(net 23 "/BUS_A10")
	(net 24 "unconnected-(J1-RESET-Pad25)")
	(net 25 "/(A)")
	(net 26 "unconnected-(J1-A13-Pad32)")
	(net 27 "/~{WR}")
	(net 28 "unconnected-(J1-A14-Pad10)")
	(net 29 "unconnected-(J1-A12-Pad9)")
	(net 30 "/BUS_A11")
	(net 31 "unconnected-(J1-A15-Pad31)")
	(net 32 "unconnected-(J1-ALE-Pad14)")
	(net 33 "/RAMRST")
	(net 34 "/BUS_A9")
	(net 35 "/BUS_A8")
	(net 36 "/BYTE")
	(net 37 "unconnected-(U1-NC-Pad8)")
	(net 38 "unconnected-(U1-NC-Pad29)")
	(net 39 "unconnected-(U1-NC-Pad30)")
	(net 40 "unconnected-(U1-NC-Pad16)")
	(net 41 "unconnected-(U1-NC-Pad7)")
	(net 42 "unconnected-(U1-NC-Pad37)")
	(net 43 "unconnected-(U1-NC-Pad15)")
	(net 44 "unconnected-(U1-NC-Pad38)")
	(net 45 "unconnected-(U2-Y5-Pad10)")
	(net 46 "unconnected-(U2-Y1-Pad14)")
	(net 47 "unconnected-(U2-Y2-Pad13)")
	(net 48 "unconnected-(U2-Y0-Pad15)")
	(net 49 "/BLOCK")
	(net 50 "unconnected-(U2-Y7-Pad7)")
	(net 51 "unconnected-(U2-Y3-Pad12)")
	(net 52 "unconnected-(U3-Q11-Pad1)")
	(net 53 "unconnected-(U3-Q10-Pad15)")
	(net 54 "/~{Y0}")
	(net 55 "/A8")
	(net 56 "/A9")
	(net 57 "/A7")
	(net 58 "/A0")
	(net 59 "/A6")
	(net 60 "/A4")
	(net 61 "/A1")
	(net 62 "/A3")
	(net 63 "/A2")
	(net 64 "/A5")
	(net 65 "/A12")
	(net 66 "/A16")
	(net 67 "/A10")
	(net 68 "/A19")
	(net 69 "/A13")
	(net 70 "/A17")
	(net 71 "/A18")
	(net 72 "/A11")
	(net 73 "/A14")
	(net 74 "/A15")
	(footprint "000_LOCAL:DIP-40_PCB"
		(layer "B.Cu")
		(at 149.999293 100.000707)
		(descr "40-lead though-hole mounted DIP package, row spacing 15.24 mm (600 mils)")
		(tags "THT DIP DIL PDIP 2.54mm 15.24mm 600mil")
		(property "Reference" "J1"
			(at 0 1.524 180)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "Model_100_System_BUS"
			(at -25.1206 5.3848 180)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Datasheet" "datasheets/TRS-80_Model_100_User_Guide.pdf"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "CONN HEADER VERT 40P 2.54MM"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "920-0172-01"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "MiniNDP_u1M.kicad_sch")
		(zone_connect 1)
		(attr through_hole)
		(fp_line
			(start -25.654 -8.128001)
			(end -25.654 2.159)
			(layer "Edge.Cuts")
		)
		(fp_line
			(start -25.654 5.207001)
			(end -25.654 8.128)
			(layer "Edge.Cuts")
		)
		(fp_line
			(start -24.638 9.144)
			(end 24.638 9.144)
			(layer "Edge.Cuts")
		)
		(fp_line
			(start 24.638001 -9.144)
			(end -24.638001 -9.144)
			(layer "Edge.Cuts")
		)
		(fp_line
			(start 25.653999 8.128)
			(end 25.654 -8.128)
			(layer "Edge.Cuts")
		)
		(fp_arc
			(start -25.654 5.207)
			(mid -25.61997 5.080003)
			(end -25.527 4.987036)
			(layer "Edge.Cuts")
		)
		(fp_arc
			(start -25.653999 -8.128)
			(mid -25.35642 -8.84642)
			(end -24.638 -9.143999)
			(layer "Edge.Cuts")
		)
		(fp_arc
			(start -25.527 2.378964)
			(mid -25.61997 2.285997)
			(end -25.654 2.159)
			(layer "Edge.Cuts")
		)
		(fp_arc
			(start -25.527 2.378964)
			(mid -24.774114 3.683)
			(end -25.527 4.987036)
			(layer "Edge.Cuts")
		)
		(fp_arc
			(start -24.638 9.144)
			(mid -25.35642 8.84642)
			(end -25.654 8.128)
			(layer "Edge.Cuts")
		)
		(fp_arc
			(start 24.638001 -9.143999)
			(mid 25.35642 -8.846419)
			(end 25.654 -8.128)
			(layer "Edge.Cuts")
		)
		(fp_arc
			(start 25.653999 8.128)
			(mid 25.35642 8.84642)
			(end 24.638 9.143999)
			(layer "Edge.Cuts")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "B.Fab")
		)
		(pad "1" thru_hole roundrect
			(at -24.13 7.62 270)
			(size 1.524 1.524)
			(drill 0.7112)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 10 "VBUS")
			(pinfunction "VCC")
			(pintype "power_out")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" thru_hole circle
			(at -21.59 7.62 270)
			(size 1.524 1.524)
			(drill 0.7112)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_out")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "3" thru_hole circle
			(at -19.05 7.62 270)
			(size 1.524 1.524)
			(drill 0.7112)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 9 "/AD0")
			(pinfunction "AD0")
			(pintype "bidirectional")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "4" thru_hole circle
			(at -16.51 7.62 270)
			(size 1.524 1.524)
			(drill 0.7112)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 8 "/AD2")
			(pinfunction "AD2")
			(pintype "bidirectional")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "5" thru_hole circle
			(at -13.97 7.62 270)
			(size 1.524 1.524)
			(drill 0.7112)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 7 "/AD4")
			(pinfunction "AD4")
			(pintype "bidirectional")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "6" thru_hole circle
			(at -11.43 7.62 270)
			(size 1.524 1.524)
			(drill 0.7112)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "/AD6")
			(pinfunction "AD6")
			(pintype "bidirectional")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "7" thru_hole circle
			(at -8.89 7.62 270)
			(size 1.524 1.524)
			(drill 0.7112)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 35 "/BUS_A8")
			(pinfunction "A8")
			(pintype "output")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "8" thru_hole circle
			(at -6.35 7.62 270)
			(size 1.524 1.524)
			(drill 0.7112)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 23 "/BUS_A10")
			(pinfunction "A10")
			(pintype "output")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "9" thru_hole circle
			(at -3.81 7.62 270)
			(size 1.524 1.524)
			(drill 0.7112)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 29 "unconnected-(J1-A12-Pad9)")
			(pinfunction "A12")
			(pintype "output+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "10" thru_hole circle
			(at -1.27 7.62 270)
			(size 1.524 1.524)
			(drill 0.7112)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 28 "unconnected-(J1-A14-Pad10)")
			(pinfunction "A14")
			(pintype "output+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "11" thru_hole circle
			(at 1.27 7.62 270)
			(size 1.524 1.524)
			(drill 0.7112)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "12" thru_hole circle
			(at 3.81 7.62 270)
			(size 1.524 1.524)
			(drill 0.7112)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 21 "/~{RD}")
			(pinfunction "~{RD}")
			(pintype "output")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "13" thru_hole circle
			(at 6.35 7.62 270)
			(size 1.524 1.524)
			(drill 0.7112)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 22 "unconnected-(J1-IO{slash}~{M}-Pad13)")
			(pinfunction "IO/~{M}")
			(pintype "output+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "14" thru_hole circle
			(at 8.89 7.62 270)
			(size 1.524 1.524)
			(drill 0.7112)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 32 "unconnected-(J1-ALE-Pad14)")
			(pinfunction "ALE")
			(pintype "output+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "15" thru_hole circle
			(at 11.43 7.62 270)
			(size 1.524 1.524)
			(drill 0.7112)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 11 "unconnected-(J1-CLK-Pad15)")
			(pinfunction "CLK")
			(pintype "output+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "16" thru_hole circle
			(at 13.97 7.62 270)
			(size 1.524 1.524)
			(drill 0.7112)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 25 "/(A)")
			(pinfunction "(A)")
			(pintype "output")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "17" thru_hole circle
			(at 16.51 7.62 270)
			(size 1.524 1.524)
			(drill 0.7112)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 12 "unconnected-(J1-INTR-Pad17)")
			(pinfunction "INTR")
			(pintype "input+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "18" thru_hole circle
			(at 19.05 7.62 270)
			(size 1.524 1.524)
			(drill 0.7112)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "19" thru_hole circle
			(at 21.59 7.62 270)
			(size 1.524 1.524)
			(drill 0.7112)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 33 "/RAMRST")
			(pinfunction "RAM_RST")
			(pintype "output")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "20" thru_hole circle
			(at 24.13 7.62 270)
			(size 1.524 1.524)
			(drill 0.7112)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 14 "unconnected-(J1-NC-Pad20)")
			(pinfunction "NC")
			(pintype "no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "21" thru_hole circle
			(at 24.13 -7.62 270)
			(size 1.524 1.524)
			(drill 0.7112)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 15 "unconnected-(J1-NC-Pad21)")
			(pinfunction "NC")
			(pintype "no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "22" thru_hole circle
			(at 21.59 -7.62 270)
			(size 1.524 1.524)
			(drill 0.7112)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 16 "unconnected-(J1-NC-Pad22)")
			(pinfunction "NC")
			(pintype "no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "23" thru_hole circle
			(at 19.05 -7.62 270)
			(size 1.524 1.524)
			(drill 0.7112)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "24" thru_hole circle
			(at 16.51 -7.62 270)
			(size 1.524 1.524)
			(drill 0.7112)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 17 "unconnected-(J1-~{INTA}-Pad24)")
			(pinfunction "~{INTA}")
			(pintype "output+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "25" thru_hole circle
			(at 13.97 -7.62 270)
			(size 1.524 1.524)
			(drill 0.7112)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 24 "unconnected-(J1-RESET-Pad25)")
			(pinfunction "RESET")
			(pintype "output+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "26" thru_hole circle
			(at 11.43 -7.62 270)
			(size 1.524 1.524)
			(drill 0.7112)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 54 "/~{Y0}")
			(pinfunction "~{Y0}")
			(pintype "output")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "27" thru_hole circle
			(at 8.89 -7.62 270)
			(size 1.524 1.524)
			(drill 0.7112)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 18 "unconnected-(J1-S1-Pad27)")
			(pinfunction "S1")
			(pintype "output+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "28" thru_hole circle
			(at 6.35 -7.62 270)
			(size 1.524 1.524)
			(drill 0.7112)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 19 "unconnected-(J1-S0-Pad28)")
			(pinfunction "S0")
			(pintype "output+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "29" thru_hole circle
			(at 3.81 -7.62 270)
			(size 1.524 1.524)
			(drill 0.7112)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 27 "/~{WR}")
			(pinfunction "~{WR}")
			(pintype "output")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "30" thru_hole circle
			(at 1.27 -7.62 270)
			(size 1.524 1.524)
			(drill 0.7112)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "31" thru_hole circle
			(at -1.27 -7.62 270)
			(size 1.524 1.524)
			(drill 0.7112)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 31 "unconnected-(J1-A15-Pad31)")
			(pinfunction "A15")
			(pintype "output+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "32" thru_hole circle
			(at -3.81 -7.62 270)
			(size 1.524 1.524)
			(drill 0.7112)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 26 "unconnected-(J1-A13-Pad32)")
			(pinfunction "A13")
			(pintype "output+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "33" thru_hole circle
			(at -6.35 -7.62 270)
			(size 1.524 1.524)
			(drill 0.7112)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 30 "/BUS_A11")
			(pinfunction "A11")
			(pintype "output")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "34" thru_hole circle
			(at -8.89 -7.62 270)
			(size 1.524 1.524)
			(drill 0.7112)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 34 "/BUS_A9")
			(pinfunction "A9")
			(pintype "output")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "35" thru_hole circle
			(at -11.43 -7.62 270)
			(size 1.524 1.524)
			(drill 0.7112)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "/AD7")
			(pinfunction "AD7")
			(pintype "bidirectional")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "36" thru_hole circle
			(at -13.97 -7.62 270)
			(size 1.524 1.524)
			(drill 0.7112)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "/AD5")
			(pinfunction "AD5")
			(pintype "bidirectional")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "37" thru_hole circle
			(at -16.51 -7.62 270)
			(size 1.524 1.524)
			(drill 0.7112)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "/AD3")
			(pinfunction "AD3")
			(pintype "bidirectional")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "38" thru_hole circle
			(at -19.05 -7.62 270)
			(size 1.524 1.524)
			(drill 0.7112)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "/AD1")
			(pinfunction "AD1")
			(pintype "bidirectional")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "39" thru_hole circle
			(at -21.59 -7.62 270)
			(size 1.524 1.524)
			(drill 0.7112)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "40" thru_hole circle
			(at -24.13 -7.62 270)
			(size 1.524 1.524)
			(drill 0.7112)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 10 "VBUS")
			(pinfunction "VCC")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KIPRJMOD}/000_LOCAL.pretty/3dshapes/pin_header_round_cut_DIP-40.step"
			(offset
				(xyz -24.13 -7.62 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
		(model "${KIPRJMOD}/000_LOCAL.pretty/3dshapes/solder_domes_DIP-40.step"
			(offset
				(xyz -24.13 -7.62 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "000_LOCAL:Keystone_3031"
		(layer "B.Cu")
		(at 170.32 100 -90)
		(property "Reference" "BT1"
			(at -3.4 3.42 45)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "Keystone_3031"
			(at 0 -4.572 90)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Datasheet" "datasheet/Keystone_3031.pdf"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Battery Retainer Coin, 10.0mm 1 Cell PC Pin"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "Keystone 3031"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "MiniNDP_u1M.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole oval
			(at -5.3 0 270)
			(size 1.4 2.4)
			(drill oval 0.8 1.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 20 "+BATT")
			(pinfunction "+")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "1" smd oval
			(at -5.3 0 270)
			(size 1.4 4)
			(layers "B.Cu" "B.Mask")
			(net 20 "+BATT")
			(pinfunction "+")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "1" thru_hole oval
			(at 5.3 0 270)
			(size 1.4 2.4)
			(drill oval 0.8 1.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 20 "+BATT")
			(pinfunction "+")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "1" smd oval
			(at 5.3 0 270)
			(size 1.4 4)
			(layers "B.Cu" "B.Mask")
			(net 20 "+BATT")
			(pinfunction "+")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd circle
			(at 0 0 270)
			(size 8 8)
			(layers "B.Cu" "B.Mask")
			(net 1 "GND")
			(pinfunction "-")
			(pintype "passive")
			(solder_mask_margin 0.2)
			(zone_connect 2)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KIPRJMOD}/000_LOCAL.pretty/3dshapes/Keystone_3031.step"
			(offset
				(xyz 0 -4 2.8)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 0 180)
			)
		)
		(model "${KIPRJMOD}/000_LOCAL.pretty/3dshapes/CR1025_blank.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
		(model "${KIPRJMOD}/000_LOCAL.pretty/000_3d/Keystone_3031_open.step"
			(hide yes)
			(offset
				(xyz 0 -4 2.8)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 0 180)
			)
		)
	)
	(footprint "000_LOCAL:R_0805"
		(layer "B.Cu")
		(at 159.55 104.45 -90)
		(descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
		(tags "resistor 0805")
		(property "Reference" "R1"
			(at -0.045 1.875 0)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "47k"
			(at 1.155 2.175 0)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Datasheet" "datasheets/sei-rmcf_rmcp.pdf"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "RES 47K OHM 1% 1/8W 0805"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MPN" "RMCF0805FT47K0"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "MiniNDP_u1M.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.949999 0 270)
			(size 0.7 1.3)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.1)
			(net 13 "VMEM")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at 0.949999 0 270)
			(size 0.7 1.3)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.1)
			(net 33 "/RAMRST")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KIPRJMOD}/000_LOCAL.pretty/3dshapes/R_0805.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "000_LOCAL:C_0805"
		(layer "B.Cu")
		(at 155.4 95.65 -90)
		(descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
		(tags "capacitor 0805")
		(property "Reference" "C1"
			(at -1.05 1.5 90)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "1u"
			(at 1.025 1.5 90)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Datasheet" "datasheets/CL21B105KAFNNNE.pdf"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "CAP CER 1UF 25V X7R 0805"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MPN" "CL21B105KAFNNNE"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "MiniNDP_u1M.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 1.5 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9 0 270)
			(size 0.8 1.25)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.1)
			(net 10 "VBUS")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at 0.9 0 270)
			(size 0.8 1.25)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.1)
			(net 1 "GND")
			(pintype "passive")
			(zone_connect 2)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KIPRJMOD}/000_LOCAL.pretty/3dshapes/C_0805.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "000_LOCAL:TSSOP-16"
		(layer "B.Cu")
		(at 130.315 96.825 180)
		(descr "TSSOP, 16 Pin (JEDEC MO-153 Var AB https://www.jedec.org/document_search?search_api_views_fulltext=MO-153), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "TSSOP SO")
		(property "Reference" "U2"
			(at -1.25 1 90)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "HC238"
			(at 1 0 90)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Datasheet" "datasheets/HC238.pdf"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "IC DECODER/DEMUX 1 X 3:8 16SO"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MPN" "74HC238PW,118"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "DIP*W7.62mm* SOIC*3.9x9.9mm*P1.27mm* TSSOP*4.4x5mm*P0.65mm*")
		(sheetname "/")
		(sheetfile "MiniNDP_u1M.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -2.9 2.275 180)
			(size 1.2 0.35)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "A0")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at -2.9 1.625 180)
			(size 1.2 0.35)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 34 "/BUS_A9")
			(pinfunction "A1")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "3" smd roundrect
			(at -2.9 0.975 180)
			(size 1.2 0.35)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 35 "/BUS_A8")
			(pinfunction "A2")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "4" smd roundrect
			(at -2.9 0.325 180)
			(size 1.2 0.35)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 54 "/~{Y0}")
			(pinfunction "~{E1}")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "5" smd roundrect
			(at -2.9 -0.325 180)
			(size 1.2 0.35)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "~{E2}")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "6" smd roundrect
			(at -2.9 -0.975 180)
			(size 1.2 0.35)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 25 "/(A)")
			(pinfunction "E3")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "7" smd roundrect
			(at -2.9 -1.625 180)
			(size 1.2 0.35)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 50 "unconnected-(U2-Y7-Pad7)")
			(pinfunction "Y7")
			(pintype "output+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "8" smd roundrect
			(at -2.9 -2.275 180)
			(size 1.2 0.35)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "9" smd roundrect
			(at 2.9 -2.275 180)
			(size 1.2 0.35)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 36 "/BYTE")
			(pinfunction "Y6")
			(pintype "output")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "10" smd roundrect
			(at 2.9 -1.625 180)
			(size 1.2 0.35)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 45 "unconnected-(U2-Y5-Pad10)")
			(pinfunction "Y5")
			(pintype "output+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "11" smd roundrect
			(at 2.9 -0.975 180)
			(size 1.2 0.35)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 49 "/BLOCK")
			(pinfunction "Y4")
			(pintype "output")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "12" smd roundrect
			(at 2.9 -0.325 180)
			(size 1.2 0.35)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 51 "unconnected-(U2-Y3-Pad12)")
			(pinfunction "Y3")
			(pintype "output+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "13" smd roundrect
			(at 2.9 0.325 180)
			(size 1.2 0.35)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 47 "unconnected-(U2-Y2-Pad13)")
			(pinfunction "Y2")
			(pintype "output+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "14" smd roundrect
			(at 2.9 0.975 180)
			(size 1.2 0.35)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 46 "unconnected-(U2-Y1-Pad14)")
			(pinfunction "Y1")
			(pintype "output+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "15" smd roundrect
			(at 2.9 1.625 180)
			(size 1.2 0.35)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 48 "unconnected-(U2-Y0-Pad15)")
			(pinfunction "Y0")
			(pintype "output+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "16" smd roundrect
			(at 2.9 2.275 180)
			(size 1.2 0.35)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 10 "VBUS")
			(pinfunction "VCC")
			(pintype "power_in")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KIPRJMOD}/000_LOCAL.pretty/3dshapes/TSSOP-16.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "000_LOCAL:Fiducial_0.5_1.0"
		(layer "B.Cu")
		(at 125.75 105.5)
		(descr "Circular Fiducial, 0.5mm bare copper, 1mm soldermask opening (Level C)")
		(tags "fiducial")
		(property "Reference" "F1"
			(at 0 1.5 180)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "Fiducial_0.5_1.0"
			(at 0 -1.5 180)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd board_only exclude_from_bom allow_missing_courtyard)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "B.Fab")
		)
		(pad "" smd circle
			(at 0 0)
			(size 0.5 0.5)
			(layers "B.Cu" "B.Mask")
			(solder_mask_margin 0.25)
			(clearance 0.25)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
	)
	(footprint "000_LOCAL:SOT-23"
		(layer "B.Cu")
		(at 162.7 104.35 180)
		(descr "SOT-23, Standard")
		(tags "SOT-23")
		(property "Reference" "DA1"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "BAV70"
			(at -2.25 -0.25 90)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Datasheet" "datasheets/BAV70.pdf"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "DIODE ARRAY GP 75V 150MA SOT23-3"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MPN" "BAV70-7-F"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SOT?23*")
		(sheetname "/")
		(sheetfile "MiniNDP_u1M.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.15 0.95 180)
			(size 0.8 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 10 "VBUS")
			(pinfunction "A")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at -1.15 -0.95 180)
			(size 0.8 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 20 "+BATT")
			(pinfunction "A")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "3" smd roundrect
			(at 1.15 0 180)
			(size 0.8 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 13 "VMEM")
			(pinfunction "K")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KIPRJMOD}/000_LOCAL.pretty/3dshapes/SOT-23.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "000_LOCAL:TSSOP-16"
		(layer "B.Cu")
		(at 130.315 103.175 180)
		(descr "TSSOP, 16 Pin (JEDEC MO-153 Var AB https://www.jedec.org/document_search?search_api_views_fulltext=MO-153), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "TSSOP SO")
		(property "Reference" "U3"
			(at -1.25 1 90)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "HC4040"
			(at 1 0 90)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Datasheet" "datasheets/4040.pdf"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "IC BINARY COUNTER 12-BIT 16SO"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MPN" "74HC4040PW,118"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "DIP?16* SO*16*")
		(sheetname "/")
		(sheetfile "MiniNDP_u1M.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -2.9 2.275 180)
			(size 1.2 0.35)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 52 "unconnected-(U3-Q11-Pad1)")
			(pinfunction "Q11")
			(pintype "output+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at -2.9 1.625 180)
			(size 1.2 0.35)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 64 "/A5")
			(pinfunction "Q5")
			(pintype "output")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "3" smd roundrect
			(at -2.9 0.975 180)
			(size 1.2 0.35)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 60 "/A4")
			(pinfunction "Q4")
			(pintype "output")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "4" smd roundrect
			(at -2.9 0.325 180)
			(size 1.2 0.35)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 59 "/A6")
			(pinfunction "Q6")
			(pintype "output")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "5" smd roundrect
			(at -2.9 -0.325 180)
			(size 1.2 0.35)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 62 "/A3")
			(pinfunction "Q3")
			(pintype "output")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "6" smd roundrect
			(at -2.9 -0.975 180)
			(size 1.2 0.35)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 63 "/A2")
			(pinfunction "Q2")
			(pintype "output")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "7" smd roundrect
			(at -2.9 -1.625 180)
			(size 1.2 0.35)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 61 "/A1")
			(pinfunction "Q1")
			(pintype "output")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "8" smd roundrect
			(at -2.9 -2.275 180)
			(size 1.2 0.35)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "VSS")
			(pintype "power_in")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "9" smd roundrect
			(at 2.9 -2.275 180)
			(size 1.2 0.35)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 58 "/A0")
			(pinfunction "Q0")
			(pintype "output")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "10" smd roundrect
			(at 2.9 -1.625 180)
			(size 1.2 0.35)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 36 "/BYTE")
			(pinfunction "CLK")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "11" smd roundrect
			(at 2.9 -0.975 180)
			(size 1.2 0.35)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 49 "/BLOCK")
			(pinfunction "Reset")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "12" smd roundrect
			(at 2.9 -0.325 180)
			(size 1.2 0.35)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 55 "/A8")
			(pinfunction "Q8")
			(pintype "output")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "13" smd roundrect
			(at 2.9 0.325 180)
			(size 1.2 0.35)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 57 "/A7")
			(pinfunction "Q7")
			(pintype "output")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "14" smd roundrect
			(at 2.9 0.975 180)
			(size 1.2 0.35)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 56 "/A9")
			(pinfunction "Q9")
			(pintype "output")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "15" smd roundrect
			(at 2.9 1.625 180)
			(size 1.2 0.35)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 53 "unconnected-(U3-Q10-Pad15)")
			(pinfunction "Q10")
			(pintype "output+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "16" smd roundrect
			(at 2.9 2.275 180)
			(size 1.2 0.35)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 10 "VBUS")
			(pinfunction "VDD")
			(pintype "power_in")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KIPRJMOD}/000_LOCAL.pretty/3dshapes/TSSOP-16.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "000_LOCAL:C_1206"
		(layer "B.Cu")
		(at 154.3 101.6 -90)
		(descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C4"
			(at -1.575 -1.875 90)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "47u"
			(at 1.125 -1.875 90)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Datasheet" "datasheets/TDK_MLCC_Cxxxx.pdf"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "CAP CER 47UF 25V X5R 1206"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MPN" "C3216X5R1E476M160DC"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "MiniNDP_u1M.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.475001 0 270)
			(size 1.15 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.217391)
			(net 13 "VMEM")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at 1.475001 0 270)
			(size 1.15 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.217391)
			(net 1 "GND")
			(pintype "passive")
			(zone_connect 2)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KIPRJMOD}/000_LOCAL.pretty/3dshapes/C_1206.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "000_LOCAL:Fiducial_0.5_1.0"
		(layer "B.Cu")
		(at 174.638 94.539)
		(descr "Circular Fiducial, 0.5mm bare copper, 1mm soldermask opening (Level C)")
		(tags "fiducial")
		(property "Reference" "F3"
			(at 0 1.5 180)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "Fiducial_0.5_1.0"
			(at 0 -1.5 180)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd board_only exclude_from_bom allow_missing_courtyard)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "B.Fab")
		)
		(pad "" smd circle
			(at 0 0)
			(size 0.5 0.5)
			(layers "B.Cu" "B.Mask")
			(solder_mask_margin 0.25)
			(clearance 0.25)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
	)
	(footprint "000_LOCAL:TSSOP-24"
		(layer "B.Cu")
		(at 160.8 98.075 180)
		(descr "TSSOP, 24 Pin (JEDEC MO-153 Var AD https://www.jedec.org/document_search?search_api_views_fulltext=MO-153), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "TSSOP SO")
		(property "Reference" "U4"
			(at -1.3 2.1 90)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "ABT841"
			(at 1 0 90)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Datasheet" "datasheets/sn54abt841.pdf"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "IC 10BIT LATCH 3-STATE 24-SOIC"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MPN" "SN74ABT841APW"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "DIP*24* *SO*24*")
		(sheetname "/")
		(sheetfile "MiniNDP_u1M.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -2.9 3.575 180)
			(size 1.2 0.35)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "OE")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at -2.9 2.925 180)
			(size 1.2 0.35)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 30 "/BUS_A11")
			(pinfunction "D0")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "3" smd roundrect
			(at -2.9 2.275 180)
			(size 1.2 0.35)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 5 "/AD7")
			(pinfunction "D1")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "4" smd roundrect
			(at -2.9 1.625 180)
			(size 1.2 0.35)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 4 "/AD5")
			(pinfunction "D2")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "5" smd roundrect
			(at -2.9 0.975 180)
			(size 1.2 0.35)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 3 "/AD3")
			(pinfunction "D3")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "6" smd roundrect
			(at -2.9 0.325 180)
			(size 1.2 0.35)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 2 "/AD1")
			(pinfunction "D4")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "7" smd roundrect
			(at -2.9 -0.325 180)
			(size 1.2 0.35)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 9 "/AD0")
			(pinfunction "D5")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "8" smd roundrect
			(at -2.9 -0.975 180)
			(size 1.2 0.35)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 8 "/AD2")
			(pinfunction "D6")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "9" smd roundrect
			(at -2.9 -1.625 180)
			(size 1.2 0.35)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 7 "/AD4")
			(pinfunction "D7")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "10" smd roundrect
			(at -2.9 -2.275 180)
			(size 1.2 0.35)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 6 "/AD6")
			(pinfunction "D8")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "11" smd roundrect
			(at -2.9 -2.924997 180)
			(size 1.2 0.35)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 23 "/BUS_A10")
			(pinfunction "D9")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "12" smd roundrect
			(at -2.9 -3.575 180)
			(size 1.2 0.35)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "13" smd roundrect
			(at 2.9 -3.575 180)
			(size 1.2 0.35)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 49 "/BLOCK")
			(pinfunction "LE")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "14" smd roundrect
			(at 2.9 -2.925 180)
			(size 1.2 0.35)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 68 "/A19")
			(pinfunction "O9")
			(pintype "tri_state")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "15" smd roundrect
			(at 2.9 -2.275 180)
			(size 1.2 0.35)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 71 "/A18")
			(pinfunction "O8")
			(pintype "tri_state")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "16" smd roundrect
			(at 2.9 -1.625 180)
			(size 1.2 0.35)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 70 "/A17")
			(pinfunction "O7")
			(pintype "tri_state")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "17" smd roundrect
			(at 2.9 -0.975 180)
			(size 1.2 0.35)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 66 "/A16")
			(pinfunction "O6")
			(pintype "tri_state")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "18" smd roundrect
			(at 2.9 -0.325 180)
			(size 1.2 0.35)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 74 "/A15")
			(pinfunction "O5")
			(pintype "tri_state")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "19" smd roundrect
			(at 2.9 0.325 180)
			(size 1.2 0.35)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 73 "/A14")
			(pinfunction "O4")
			(pintype "tri_state")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "20" smd roundrect
			(at 2.9 0.975 180)
			(size 1.2 0.35)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 69 "/A13")
			(pinfunction "O3")
			(pintype "tri_state")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "21" smd roundrect
			(at 2.9 1.625 180)
			(size 1.2 0.35)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 65 "/A12")
			(pinfunction "O2")
			(pintype "tri_state")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "22" smd roundrect
			(at 2.9 2.275 180)
			(size 1.2 0.35)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 72 "/A11")
			(pinfunction "O1")
			(pintype "tri_state")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "23" smd roundrect
			(at 2.9 2.925 180)
			(size 1.2 0.35)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 67 "/A10")
			(pinfunction "O0")
			(pintype "tri_state")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "24" smd roundrect
			(at 2.9 3.575 180)
			(size 1.2 0.35)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 10 "VBUS")
			(pinfunction "VCC")
			(pintype "power_in")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KIPRJMOD}/000_LOCAL.pretty/3dshapes/TSSOP-24.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "000_LOCAL:C_0805"
		(layer "B.Cu")
		(at 125.65 100.25 90)
		(descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
		(tags "capacitor 0805")
		(property "Reference" "C3"
			(at -2.5 0.3 0)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "1u"
			(at -0.05 0 0)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Datasheet" "datasheets/CL21B105KAFNNNE.pdf"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "CAP CER 1UF 25V X7R 0805"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MPN" "CL21B105KAFNNNE"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "MiniNDP_u1M.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 1.55 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9 0 90)
			(size 0.8 1.25)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.1)
			(net 10 "VBUS")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at 0.9 0 90)
			(size 0.8 1.25)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.1)
			(net 1 "GND")
			(pintype "passive")
			(zone_connect 2)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KIPRJMOD}/000_LOCAL.pretty/3dshapes/C_0805.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "000_LOCAL:C_0805"
		(layer "B.Cu")
		(at 125.65 95.7 -90)
		(descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
		(tags "capacitor 0805")
		(property "Reference" "C2"
			(at 2.3 0.000001 0)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "1u"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Datasheet" "datasheets/CL21B105KAFNNNE.pdf"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "CAP CER 1UF 25V X7R 0805"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MPN" "CL21B105KAFNNNE"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "MiniNDP_u1M.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -1.55 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9 0 270)
			(size 0.8 1.25)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.1)
			(net 10 "VBUS")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at 0.9 0 270)
			(size 0.8 1.25)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.1)
			(net 1 "GND")
			(pintype "passive")
			(zone_connect 2)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KIPRJMOD}/000_LOCAL.pretty/3dshapes/C_0805.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "000_LOCAL:TSOP-II-44"
		(layer "B.Cu")
		(at 143.65 100 -90)
		(descr "TSOP-II, 44 Pin (http://www.issi.com/WW/pdf/61-64C5128AL.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "TSOP-II SO")
		(property "Reference" "U1"
			(at -4.25 7.6 180)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "AS6C8008_TSOPII"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Datasheet" "datasheets/AS6C8008.pdf"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "IC SRAM 1Mx8 PARALLEL 5v TSOP-II-44"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MPN" "AS6C8008-55ZIN"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SSOP*11.305x20.495mm*P1.27mm*")
		(sheetname "/")
		(sheetfile "MiniNDP_u1M.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -5.6 8.4 270)
			(size 1 0.5)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 64 "/A5")
			(pinfunction "A4")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at -5.6 7.6 270)
			(size 1 0.5)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 56 "/A9")
			(pinfunction "A3")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "3" smd roundrect
			(at -5.6 6.8 270)
			(size 1 0.5)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 57 "/A7")
			(pinfunction "A2")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "4" smd roundrect
			(at -5.6 6 270)
			(size 1 0.5)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 55 "/A8")
			(pinfunction "A1")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "5" smd roundrect
			(at -5.6 5.2 270)
			(size 1 0.5)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 58 "/A0")
			(pinfunction "A0")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "6" smd roundrect
			(at -5.6 4.4 270)
			(size 1 0.5)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 33 "/RAMRST")
			(pinfunction "~{CE1}")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "7" smd roundrect
			(at -5.6 3.6 270)
			(size 1 0.5)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 41 "unconnected-(U1-NC-Pad7)")
			(pinfunction "NC")
			(pintype "passive+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "8" smd roundrect
			(at -5.6 2.8 270)
			(size 1 0.5)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 37 "unconnected-(U1-NC-Pad8)")
			(pinfunction "NC")
			(pintype "passive+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "9" smd roundrect
			(at -5.6 2 270)
			(size 1 0.5)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 2 "/AD1")
			(pinfunction "Q0")
			(pintype "tri_state")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "10" smd roundrect
			(at -5.6 1.2 270)
			(size 1 0.5)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 3 "/AD3")
			(pinfunction "Q1")
			(pintype "tri_state")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "11" smd roundrect
			(at -5.6 0.4 270)
			(size 1 0.5)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 13 "VMEM")
			(pinfunction "VCC")
			(pintype "power_in")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "12" smd roundrect
			(at -5.6 -0.4 270)
			(size 1 0.5)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(zone_connect 2)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "13" smd roundrect
			(at -5.6 -1.2 270)
			(size 1 0.5)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 4 "/AD5")
			(pinfunction "Q2")
			(pintype "tri_state")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "14" smd roundrect
			(at -5.6 -2 270)
			(size 1 0.5)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 5 "/AD7")
			(pinfunction "Q3")
			(pintype "tri_state")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "15" smd roundrect
			(at -5.6 -2.8 270)
			(size 1 0.5)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 43 "unconnected-(U1-NC-Pad15)")
			(pinfunction "NC")
			(pintype "passive+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "16" smd roundrect
			(at -5.6 -3.6 270)
			(size 1 0.5)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 40 "unconnected-(U1-NC-Pad16)")
			(pinfunction "NC")
			(pintype "passive+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "17" smd roundrect
			(at -5.6 -4.4 270)
			(size 1 0.5)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 27 "/~{WR}")
			(pinfunction "~{WE}")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "18" smd roundrect
			(at -5.6 -5.2 270)
			(size 1 0.5)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 73 "/A14")
			(pinfunction "A19")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "19" smd roundrect
			(at -5.6 -6 270)
			(size 1 0.5)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 69 "/A13")
			(pinfunction "A18")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "20" smd roundrect
			(at -5.6 -6.8 270)
			(size 1 0.5)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 65 "/A12")
			(pinfunction "A17")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "21" smd roundrect
			(at -5.6 -7.6 270)
			(size 1 0.5)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 72 "/A11")
			(pinfunction "A16")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "22" smd roundrect
			(at -5.6 -8.4 270)
			(size 1 0.5)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 67 "/A10")
			(pinfunction "A15")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "23" smd roundrect
			(at 5.6 -8.4 270)
			(size 1 0.5)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 68 "/A19")
			(pinfunction "A14")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "24" smd roundrect
			(at 5.6 -7.6 270)
			(size 1 0.5)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 71 "/A18")
			(pinfunction "A13")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "25" smd roundrect
			(at 5.6 -6.8 270)
			(size 1 0.5)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 70 "/A17")
			(pinfunction "A12")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "26" smd roundrect
			(at 5.6 -6 270)
			(size 1 0.5)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 66 "/A16")
			(pinfunction "A11")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "27" smd roundrect
			(at 5.6 -5.2 270)
			(size 1 0.5)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 74 "/A15")
			(pinfunction "A10")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "28" smd roundrect
			(at 5.6 -4.4 270)
			(size 1 0.5)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 60 "/A4")
			(pinfunction "A9")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "29" smd roundrect
			(at 5.6 -3.6 270)
			(size 1 0.5)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 38 "unconnected-(U1-NC-Pad29)")
			(pinfunction "NC")
			(pintype "passive+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "30" smd roundrect
			(at 5.6 -2.8 270)
			(size 1 0.5)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 39 "unconnected-(U1-NC-Pad30)")
			(pinfunction "NC")
			(pintype "passive+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "31" smd roundrect
			(at 5.6 -2 270)
			(size 1 0.5)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 6 "/AD6")
			(pinfunction "Q4")
			(pintype "tri_state")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "32" smd roundrect
			(at 5.6 -1.2 270)
			(size 1 0.5)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 7 "/AD4")
			(pinfunction "Q5")
			(pintype "tri_state")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "33" smd roundrect
			(at 5.6 -0.4 270)
			(size 1 0.5)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 13 "VMEM")
			(pinfunction "VCC")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "34" smd roundrect
			(at 5.6 0.4 270)
			(size 1 0.5)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "passive")
			(zone_connect 2)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "35" smd roundrect
			(at 5.6 1.2 270)
			(size 1 0.5)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 8 "/AD2")
			(pinfunction "Q6")
			(pintype "tri_state")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "36" smd roundrect
			(at 5.6 2 270)
			(size 1 0.5)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 9 "/AD0")
			(pinfunction "Q7")
			(pintype "tri_state")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "37" smd roundrect
			(at 5.6 2.8 270)
			(size 1 0.5)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 42 "unconnected-(U1-NC-Pad37)")
			(pinfunction "NC")
			(pintype "passive+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "38" smd roundrect
			(at 5.6 3.6 270)
			(size 1 0.5)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 44 "unconnected-(U1-NC-Pad38)")
			(pinfunction "NC")
			(pintype "passive+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "39" smd roundrect
			(at 5.6 4.4 270)
			(size 1 0.5)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 59 "/A6")
			(pinfunction "A8")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "40" smd roundrect
			(at 5.6 5.2 270)
			(size 1 0.5)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 36 "/BYTE")
			(pinfunction "CE2")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "41" smd roundrect
			(at 5.6 6 270)
			(size 1 0.5)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 21 "/~{RD}")
			(pinfunction "~{OE}")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "42" smd roundrect
			(at 5.6 6.8 270)
			(size 1 0.5)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 62 "/A3")
			(pinfunction "A7")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "43" smd roundrect
			(at 5.6 7.6 270)
			(size 1 0.5)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 63 "/A2")
			(pinfunction "A6")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "44" smd roundrect
			(at 5.6 8.4 270)
			(size 1 0.5)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 61 "/A1")
			(pinfunction "A5")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KIPRJMOD}/000_LOCAL.pretty/3dshapes/TSOP-II-44_10.16x18.41mm_P0.8mm.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "000_LOCAL:Fiducial_0.5_1.0"
		(layer "B.Cu")
		(at 174.638 105.461)
		(descr "Circular Fiducial, 0.5mm bare copper, 1mm soldermask opening (Level C)")
		(tags "fiducial")
		(property "Reference" "F2"
			(at 0 1.5 180)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "Fiducial_0.5_1.0"
			(at 0 -1.5 180)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd board_only exclude_from_bom allow_missing_courtyard)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "B.Fab")
		)
		(pad "" smd circle
			(at 0 0)
			(size 0.5 0.5)
			(layers "B.Cu" "B.Mask")
			(solder_mask_margin 0.25)
			(clearance 0.25)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
	)
	(gr_text "${COMMENT1}\n${REVISION} - 1M RAM Disk for\nTRS-80 Model 100, Kyotronic KC-85\n"
		(at 146.825 95.555 0)
		(layer "F.SilkS")
	)
	(gr_text "Battery: CR1025"
		(at 174.13 100 90)
		(layer "F.SilkS")
	)
	(gr_text "${TITLE}"
		(at 127.14 95.809 0)
		(layer "F.SilkS")
	)
	(gr_text "Select Bank 0/1/2/3  : P=129 / 133 / 137 / 141\nSelect Block N 0-255 : OUT P,N\nRead / Write Data D  : D=INP(131) / OUT 131,D\nread/write 1024 times per block"
		(at 128.664 102.286 0)
		(layer "F.SilkS")
	)
	(gr_text "use ENIG copper finish\nfor gold battery terminal"
		(at 176.035 89.713 0)
		(layer "Eco2.User")
	)
	(zone
		(net 54)
		(net_name "/~{Y0}")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30039)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 135.145196 96.5) (xy 135.065664 96.495332) (xy 135.005069 96.482658) (xy 134.902813 96.434439)
				(xy 134.821184 96.391714) (xy 134.698773 96.354804) (xy 134.649 96.6) (xy 134.698773 96.845196)
				(xy 134.835415 96.801905) (xy 134.902813 96.765561) (xy 134.997709 96.719647) (xy 135.060872 96.705319)
				(xy 135.145196 96.7)
			)
		)
	)
	(zone
		(net 60)
		(net_name "/A4")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30053)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 146.755393 102.450122) (xy 146.812619 102.456371) (xy 146.853961 102.471502) (xy 146.901346 102.517943)
				(xy 146.932662 102.57878) (xy 146.992133 102.688893) (xy 147.200999 102.550023) (xy 147.248773 102.304804)
				(xy 147.241687 102.303394) (xy 147.004404 102.261513) (xy 146.760184 102.250181)
			)
		)
	)
	(zone
		(net 23)
		(net_name "/BUS_A10")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30048)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 157.955485 104.504978) (xy 158.018805 104.456992) (xy 158.073215 104.426881) (xy 158.177548 104.395493)
				(xy 158.270026 104.370227) (xy 158.388893 104.307867) (xy 158.25076 104.099351) (xy 158.042133 103.961107)
				(xy 157.978211 104.084594) (xy 157.958531 104.146834) (xy 157.921433 104.243802) (xy 157.884847 104.294967)
				(xy 157.825595 104.352897)
			)
		)
	)
	(zone
		(net 6)
		(net_name "/AD6")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30027)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 159.620554 102.470867) (xy 159.680092 102.41793) (xy 159.731901 102.384045) (xy 159.838304 102.345835)
				(xy 159.926235 102.318326) (xy 160.038893 102.257867) (xy 159.900707 102.049293) (xy 159.692133 101.911107)
				(xy 159.626123 102.038338) (xy 159.604164 102.111697) (xy 159.569529 102.211264) (xy 159.534998 102.266059)
				(xy 159.479133 102.329446)
			)
		)
	)
	(zone
		(net 3)
		(net_name "/AD3")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30010)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 134.627282 93.377274) (xy 134.523469 93.266455) (xy 134.445199 93.167422) (xy 134.394192 93.086999)
				(xy 134.357219 93.010478) (xy 134.314328 92.858613) (xy 134.291867 92.655871) (xy 134.273893 92.467307)
				(xy 134.236651 92.232048) (xy 133.488586 92.38) (xy 133.340634 93.128065) (xy 133.639152 93.172212)
				(xy 133.764457 93.183281) (xy 133.948608 93.202638) (xy 134.031837 93.219695) (xy 134.11338 93.246336)
				(xy 134.196395 93.286058) (xy 134.284041 93.34236) (xy 134.379476 93.41874) (xy 134.48586 93.518696)
			)
		)
	)
	(zone
		(net 58)
		(net_name "/A0")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30028)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 138.170554 100.920867) (xy 138.230092 100.86793) (xy 138.281901 100.834045) (xy 138.388304 100.795835)
				(xy 138.476235 100.768326) (xy 138.588893 100.707867) (xy 138.450707 100.499293) (xy 138.242133 100.361107)
				(xy 138.176123 100.488338) (xy 138.154164 100.561697) (xy 138.119529 100.661264) (xy 138.084998 100.716059)
				(xy 138.029133 100.779446)
			)
		)
	)
	(zone
		(net 5)
		(net_name "/AD7")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30070)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 161.958641 95.628575) (xy 161.998087 95.667) (xy 162.021466 95.702682) (xy 162.039374 95.77316)
				(xy 162.040699 95.785669) (xy 162.052271 95.854677) (xy 162.092133 95.938893) (xy 162.300773 95.800634)
				(xy 162.348773 95.554804) (xy 162.250143 95.541815) (xy 162.173664 95.528732) (xy 162.08552 95.473973)
			)
		)
	)
	(zone
		(net 36)
		(net_name "/BYTE")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30035)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 135.004804 103.65) (xy 135.084336 103.654668) (xy 135.144931 103.667342) (xy 135.247187 103.715561)
				(xy 135.328815 103.758285) (xy 135.451227 103.795196) (xy 135.501 103.55) (xy 135.451227 103.304804)
				(xy 135.314585 103.348094) (xy 135.247186 103.384439) (xy 135.15229 103.430353) (xy 135.089128 103.444681)
				(xy 135.004804 103.45)
			)
		)
	)
	(zone
		(net 10)
		(net_name "VBUS")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30020)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 158.59954 98.66674) (xy 158.704426 98.636088) (xy 158.785755 98.62159) (xy 158.901442 98.617341)
				(xy 159.008469 98.615058) (xy 159.158527 98.594236) (xy 159.100947 98.29968) (xy 158.933329 98.050559)
				(xy 158.872292 98.091541) (xy 158.695265 98.201524) (xy 158.471192 98.287891)
			)
		)
	)
	(zone
		(net 8)
		(net_name "/AD2")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30045)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 142.747704 104.084516) (xy 142.679319 104.134673) (xy 142.621624 104.166147) (xy 142.523563 104.198376)
				(xy 142.431234 104.227198) (xy 142.311107 104.292133) (xy 142.449227 104.500634) (xy 142.657867 104.638893)
				(xy 142.720085 104.517567) (xy 142.74072 104.448104) (xy 142.776715 104.348627) (xy 142.813749 104.296891)
				(xy 142.874582 104.239118)
			)
		)
	)
	(zone
		(net 55)
		(net_name "/A8")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30062)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 137.639173 100.420591) (xy 137.710141 100.264319) (xy 137.775792 100.158999) (xy 137.792616 100.134608)
				(xy 137.857867 100.038893) (xy 137.650382 99.899077) (xy 137.404804 99.948773) (xy 137.44483 100.080051)
				(xy 137.4535 100.101107) (xy 137.473629 100.153324) (xy 137.484202 100.205111) (xy 137.479648 100.265633)
				(xy 137.454398 100.344055)
			)
		)
	)
	(zone
		(net 9)
		(net_name "/AD0")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30006)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 131.94586 106.482718) (xy 131.835041 106.58653) (xy 131.736008 106.664801) (xy 131.655585 106.715808)
				(xy 131.579064 106.752781) (xy 131.427199 106.795671) (xy 131.224458 106.818133) (xy 131.035894 106.836106)
				(xy 130.800634 106.873349) (xy 130.948586 107.621414) (xy 131.696651 107.769366) (xy 131.740798 107.470847)
				(xy 131.751867 107.345543) (xy 131.771224 107.161391) (xy 131.788281 107.078162) (xy 131.814922 106.996619)
				(xy 131.854644 106.913604) (xy 131.910946 106.825959) (xy 131.987326 106.730523) (xy 132.087282 106.62414)
			)
		)
	)
	(zone
		(net 4)
		(net_name "/AD5")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30069)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 144.36919 95.665884) (xy 144.507712 95.691303) (xy 144.599432 95.733526) (xy 144.666572 95.777849)
				(xy 144.711107 95.807867) (xy 144.850991 95.60013) (xy 144.801227 95.354804) (xy 144.676517 95.395273)
				(xy 144.623482 95.423412) (xy 144.532723 95.463997) (xy 144.47384 95.47212) (xy 144.395286 95.467595)
			)
		)
	)
	(zone
		(net 9)
		(net_name "/AD0")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30064)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 158.624108 101.03323) (xy 158.678005 101.007677) (xy 158.722884 100.99761) (xy 158.792168 101.009171)
				(xy 158.845239 101.035115) (xy 158.912319 101.067998) (xy 159.001227 101.095196) (xy 159.050866 100.849501)
				(xy 158.911107 100.642133) (xy 158.784518 100.721438) (xy 158.694053 100.768987) (xy 158.693065 100.769481)
				(xy 158.524113 100.860022)
			)
		)
	)
	(zone
		(net 8)
		(net_name "/AD2")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30029)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 159.620554 101.270867) (xy 159.680092 101.21793) (xy 159.731901 101.184045) (xy 159.838304 101.145835)
				(xy 159.926235 101.118326) (xy 160.038893 101.057867) (xy 159.900707 100.849293) (xy 159.692133 100.711107)
				(xy 159.626123 100.838338) (xy 159.604164 100.911697) (xy 159.569529 101.011264) (xy 159.534998 101.066059)
				(xy 159.479133 101.129446)
			)
		)
	)
	(zone
		(net 2)
		(net_name "/AD1")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30031)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 141.120867 95.879446) (xy 141.06793 95.819908) (xy 141.034045 95.768098) (xy 140.995835 95.661696)
				(xy 140.968326 95.573765) (xy 140.907867 95.461107) (xy 140.699293 95.599293) (xy 140.561107 95.807867)
				(xy 140.688338 95.873876) (xy 140.761696 95.895835) (xy 140.861264 95.930471) (xy 140.916059 95.965002)
				(xy 140.979446 96.020867)
			)
		)
	)
	(zone
		(net 2)
		(net_name "/AD1")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30011)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 132.087282 93.377274) (xy 131.983469 93.266455) (xy 131.905199 93.167422) (xy 131.854192 93.086999)
				(xy 131.817219 93.010478) (xy 131.774328 92.858613) (xy 131.751867 92.655871) (xy 131.733893 92.467307)
				(xy 131.696651 92.232048) (xy 130.948586 92.38) (xy 130.800634 93.128065) (xy 131.099152 93.172212)
				(xy 131.224457 93.183281) (xy 131.408608 93.202638) (xy 131.491837 93.219695) (xy 131.57338 93.246336)
				(xy 131.656395 93.286058) (xy 131.744041 93.34236) (xy 131.839476 93.41874) (xy 131.94586 93.518696)
			)
		)
	)
	(zone
		(net 10)
		(net_name "VBUS")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30015)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 125.8 96.144236) (xy 125.804683 96.045767) (xy 125.817462 95.970899) (xy 125.864814 95.846106)
				(xy 125.905763 95.749634) (xy 125.944236 95.608527) (xy 125.65 95.549) (xy 125.355764 95.608527)
				(xy 125.395392 95.847582) (xy 125.400271 96.05028) (xy 125.4 96.144236)
			)
		)
	)
	(zone
		(net 21)
		(net_name "/~{RD}")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30040)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 138.145196 104.65) (xy 138.065664 104.645332) (xy 138.005069 104.632658) (xy 137.902813 104.584439)
				(xy 137.821184 104.541714) (xy 137.698773 104.504804) (xy 137.649 104.75) (xy 137.698773 104.995196)
				(xy 137.835415 104.951905) (xy 137.902813 104.915561) (xy 137.997709 104.869647) (xy 138.060872 104.855319)
				(xy 138.145196 104.85)
			)
		)
	)
	(zone
		(net 5)
		(net_name "/AD7")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30047)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 145.95198 94.841246) (xy 145.878591 94.888928) (xy 145.817777 94.918344) (xy 145.728794 94.945851)
				(xy 145.634592 94.975113) (xy 145.511107 95.042133) (xy 145.649192 95.250587) (xy 145.857867 95.388893)
				(xy 145.916239 95.273249) (xy 145.935805 95.203584) (xy 145.949376 95.153453) (xy 145.970404 95.105322)
				(xy 146.007566 95.056187) (xy 146.069542 95.003045)
			)
		)
	)
	(zone
		(net 49)
		(net_name "/BLOCK")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30021)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 129.094236 97.7) (xy 129.011011 97.695292) (xy 128.945486 97.682338) (xy 128.84669 97.637978)
				(xy 128.80659 97.611952) (xy 128.708336 97.5538) (xy 128.642594 97.527548) (xy 128.558527 97.505764)
				(xy 128.499 97.8) (xy 128.558527 98.094236) (xy 128.639399 98.073493) (xy 128.703273 98.048581)
				(xy 128.80659 97.988048) (xy 128.859116 97.954617) (xy 128.918223 97.926536) (xy 128.993425 97.9072)
				(xy 129.094236 97.9)
			)
		)
	)
	(zone
		(net 20)
		(net_name "+BATT")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30004)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 170.52 96.1) (xy 170.540468 95.929398) (xy 170.568587 95.823549) (xy 170.609218 95.715348) (xy 170.654635 95.624987)
				(xy 170.709943 95.541646) (xy 170.762984 95.481279) (xy 170.823035 95.430647) (xy 170.87953 95.397032)
				(xy 170.941261 95.373399) (xy 171.02 95.360273) (xy 170.32 94.699) (xy 169.62 95.360273) (xy 169.734679 95.385609)
				(xy 169.838903 95.447211) (xy 169.934685 95.547738) (xy 170.019643 95.690837) (xy 170.08572 95.872334)
				(xy 170.118698 96.061845) (xy 170.12 96.1)
			)
		)
	)
	(zone
		(net 3)
		(net_name "/AD3")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30024)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 142.029133 94.970554) (xy 142.082069 95.030092) (xy 142.115954 95.081901) (xy 142.154164 95.188303)
				(xy 142.181674 95.276234) (xy 142.242133 95.388893) (xy 142.450707 95.250707) (xy 142.588893 95.042133)
				(xy 142.461662 94.976123) (xy 142.388303 94.954164) (xy 142.288735 94.919529) (xy 142.233941 94.884998)
				(xy 142.170554 94.829133)
			)
		)
	)
	(zone
		(net 57)
		(net_name "/A7")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30041)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 136.95 99.895196) (xy 136.954668 99.815664) (xy 136.967342 99.755069) (xy 137.015561 99.652813)
				(xy 137.058285 99.571184) (xy 137.095196 99.448773) (xy 136.85 99.399) (xy 136.604804 99.448773)
				(xy 136.648094 99.585415) (xy 136.684439 99.652813) (xy 136.730353 99.747709) (xy 136.744681 99.810872)
				(xy 136.75 99.895196)
			)
		)
	)
	(zone
		(net 7)
		(net_name "/AD4")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30055)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 158.660414 102.281755) (xy 158.703859 102.247023) (xy 158.742628 102.229397) (xy 158.807103 102.229919)
				(xy 158.872235 102.253345) (xy 159.001227 102.295196) (xy 159.050723 102.04931) (xy 158.911107 101.842133)
				(xy 158.802229 101.913541) (xy 158.674295 102.001655) (xy 158.522361 102.137045)
			)
		)
	)
	(zone
		(net 8)
		(net_name "/AD2")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30036)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 141.954804 104.6) (xy 142.034336 104.604668) (xy 142.094931 104.617342) (xy 142.197187 104.665561)
				(xy 142.278815 104.708285) (xy 142.401227 104.745196) (xy 142.451 104.5) (xy 142.401227 104.254804)
				(xy 142.264585 104.298094) (xy 142.197186 104.334439) (xy 142.10229 104.380353) (xy 142.039128 104.394681)
				(xy 141.954804 104.4)
			)
		)
	)
	(zone
		(net 64)
		(net_name "/A5")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30051)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 134.806027 100.752577) (xy 134.752757 100.801107) (xy 134.705571 100.831733) (xy 134.616774 100.861529)
				(xy 134.602268 100.864597) (xy 134.517815 100.886967) (xy 134.411107 100.942133) (xy 134.549307 101.150719)
				(xy 134.757867 101.288893) (xy 134.795981 101.223776) (xy 134.819202 101.168499) (xy 134.838751 101.09682)
				(xy 134.868447 101.003148) (xy 134.899357 100.951303) (xy 134.950023 100.891373)
			)
		)
	)
	(zone
		(net 6)
		(net_name "/AD6")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30066)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 146.115479 104.927246) (xy 146.025108 104.851445) (xy 145.971367 104.790217) (xy 145.925725 104.718824)
				(xy 145.857867 104.611107) (xy 145.649207 104.749392) (xy 145.601227 104.995196) (xy 145.740975 105.008939)
				(xy 145.766393 105.008864) (xy 145.869932 105.017969) (xy 145.925843 105.040926) (xy 145.993727 105.085917)
			)
		)
	)
	(zone
		(net 30)
		(net_name "/BUS_A11")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30072)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 162.425923 94.997624) (xy 162.465685 95.035646) (xy 162.485122 95.069759) (xy 162.494984 95.127078)
				(xy 162.504804 95.198773) (xy 162.750781 95.150623) (xy 162.798773 94.904804) (xy 162.697217 94.894893)
				(xy 162.629908 94.887184) (xy 162.55062 94.841257)
			)
		)
	)
	(zone
		(net 23)
		(net_name "/BUS_A10")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30007)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 144.64586 106.482718) (xy 144.535041 106.58653) (xy 144.436008 106.664801) (xy 144.355585 106.715808)
				(xy 144.279064 106.752781) (xy 144.127199 106.795671) (xy 143.924458 106.818133) (xy 143.735894 106.836106)
				(xy 143.500634 106.873349) (xy 143.648586 107.621414) (xy 144.396651 107.769366) (xy 144.440798 107.470847)
				(xy 144.451867 107.345543) (xy 144.471224 107.161391) (xy 144.488281 107.078162) (xy 144.514922 106.996619)
				(xy 144.554644 106.913604) (xy 144.610946 106.825959) (xy 144.687326 106.730523) (xy 144.787282 106.62414)
			)
		)
	)
	(zone
		(net 33)
		(net_name "/RAMRST")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30032)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 140.420867 96.279446) (xy 140.36793 96.219908) (xy 140.334045 96.168098) (xy 140.295835 96.061696)
				(xy 140.268326 95.973765) (xy 140.207867 95.861107) (xy 139.999293 95.999293) (xy 139.861107 96.207867)
				(xy 139.988338 96.273876) (xy 140.061696 96.295835) (xy 140.161264 96.330471) (xy 140.216059 96.365002)
				(xy 140.279446 96.420867)
			)
		)
	)
	(zone
		(net 4)
		(net_name "/AD5")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30058)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 145.299216 95.735848) (xy 145.238122 95.718735) (xy 145.195368 95.695908) (xy 145.148379 95.640289)
				(xy 145.123762 95.587392) (xy 145.057867 95.461107) (xy 144.84902 95.599805) (xy 144.801227 95.845196)
				(xy 145.030652 95.888587) (xy 145.260193 95.932003)
			)
		)
	)
	(zone
		(net 5)
		(net_name "/AD7")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30056)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 145.227229 95.101825) (xy 145.278494 95.107873) (xy 145.315113 95.12256) (xy 145.354624 95.167468)
				(xy 145.37886 95.238077) (xy 145.401628 95.309922) (xy 145.442133 95.388893) (xy 145.650999 95.250023)
				(xy 145.698773 95.004804) (xy 145.51593 94.954943) (xy 145.500836 94.949653) (xy 145.393203 94.917661)
				(xy 145.231971 94.901882)
			)
		)
	)
	(zone
		(net 49)
		(net_name "/BLOCK")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30023)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 128.45 98.356346) (xy 128.454804 98.290591) (xy 128.468433 98.240079) (xy 128.513501 98.174289)
				(xy 128.582936 98.122731) (xy 128.66471 98.063074) (xy 128.749441 97.966671) (xy 128.5 97.799) (xy 128.205764 97.858527)
				(xy 128.244778 98.089834) (xy 128.250061 98.298286) (xy 128.25 98.356346)
			)
		)
	)
	(zone
		(net 8)
		(net_name "/AD2")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30003)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 134.61434 106.644238) (xy 134.526759 106.724912) (xy 134.445184 106.786425) (xy 134.373204 106.828612)
				(xy 134.304319 106.85787) (xy 134.170334 106.885092) (xy 134.014549 106.880191) (xy 133.918852 106.868277)
				(xy 133.665118 106.844759) (xy 133.513736 106.848964) (xy 133.340634 106.873349) (xy 133.488586 107.621414)
				(xy 134.122873 108.044052) (xy 134.199018 107.921631) (xy 134.257601 107.810715) (xy 134.339784 107.602502)
				(xy 134.384574 107.439447) (xy 134.425402 107.290868) (xy 134.486057 107.140136) (xy 134.588768 106.975612)
				(xy 134.755762 106.78566)
			)
		)
	)
	(zone
		(net 20)
		(net_name "+BATT")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30005)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 170.12 103.9) (xy 170.099532 104.070602) (xy 170.071413 104.176451) (xy 170.030782 104.284652)
				(xy 169.985365 104.375013) (xy 169.930057 104.458354) (xy 169.877016 104.51872) (xy 169.816965 104.569352)
				(xy 169.76047 104.602967) (xy 169.698739 104.626601) (xy 169.62 104.639726) (xy 170.32 105.301)
				(xy 171.02 104.639726) (xy 170.905321 104.61439) (xy 170.801098 104.552789) (xy 170.705315 104.452262)
				(xy 170.620357 104.309163) (xy 170.55428 104.127666) (xy 170.521302 103.938156) (xy 170.52 103.9)
			)
		)
	)
	(zone
		(net 55)
		(net_name "/A8")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30030)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 129.279446 103.079133) (xy 129.219908 103.132069) (xy 129.168098 103.165954) (xy 129.061697 103.204164)
				(xy 128.973765 103.231674) (xy 128.861107 103.292133) (xy 128.999293 103.500707) (xy 129.207867 103.638893)
				(xy 129.273876 103.511662) (xy 129.295835 103.438304) (xy 129.33047 103.338736) (xy 129.365002 103.283941)
				(xy 129.420867 103.220554)
			)
		)
	)
	(zone
		(net 4)
		(net_name "/AD5")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30012)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 137.167282 93.377274) (xy 137.063469 93.266455) (xy 136.985199 93.167422) (xy 136.934192 93.086999)
				(xy 136.897219 93.010478) (xy 136.854328 92.858613) (xy 136.831867 92.655871) (xy 136.813893 92.467307)
				(xy 136.776651 92.232048) (xy 136.028586 92.38) (xy 135.880634 93.128065) (xy 136.179152 93.172212)
				(xy 136.304457 93.183281) (xy 136.488608 93.202638) (xy 136.571837 93.219695) (xy 136.65338 93.246336)
				(xy 136.736395 93.286058) (xy 136.824041 93.34236) (xy 136.919476 93.41874) (xy 137.02586 93.518696)
			)
		)
	)
	(zone
		(net 10)
		(net_name "VBUS")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30000)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 125.85 93.860808) (xy 125.854892 93.734587) (xy 125.869138 93.62806) (xy 125.890098 93.544306)
				(xy 125.918006 93.472304) (xy 125.99368 93.352385) (xy 126.112103 93.23107) (xy 126.15271 93.194352)
				(xy 126.31911 93.035239) (xy 126.40944 92.931626) (xy 126.502873 92.804052) (xy 125.869293 92.379707)
				(xy 125.121935 92.529366) (xy 125.200569 92.839092) (xy 125.302612 93.108822) (xy 125.360013 93.252404)
				(xy 125.406859 93.408168) (xy 125.438428 93.602255) (xy 125.45 93.860808)
			)
		)
	)
	(zone
		(net 7)
		(net_name "/AD4")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30008)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 137.02586 106.482718) (xy 136.915041 106.58653) (xy 136.816008 106.664801) (xy 136.735585 106.715808)
				(xy 136.659064 106.752781) (xy 136.507199 106.795671) (xy 136.304458 106.818133) (xy 136.115894 106.836106)
				(xy 135.880634 106.873349) (xy 136.028586 107.621414) (xy 136.776651 107.769366) (xy 136.820798 107.470847)
				(xy 136.831867 107.345543) (xy 136.851224 107.161391) (xy 136.868281 107.078162) (xy 136.894922 106.996619)
				(xy 136.934644 106.913604) (xy 136.990946 106.825959) (xy 137.067326 106.730523) (xy 137.167282 106.62414)
			)
		)
	)
	(zone
		(net 6)
		(net_name "/AD6")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30060)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 145.305043 105.103848) (xy 145.37064 105.056275) (xy 145.425039 105.029597) (xy 145.516789 105.013462)
				(xy 145.541773 105.012322) (xy 145.698773 104.995196) (xy 145.650773 104.749366) (xy 145.442133 104.611107)
				(xy 145.365931 104.733624) (xy 145.298791 104.834804) (xy 145.178162 104.949247)
			)
		)
	)
	(zone
		(net 10)
		(net_name "VBUS")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30017)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 161.75 101.355764) (xy 161.745239 101.490957) (xy 161.731909 101.585989) (xy 161.706099 101.686303)
				(xy 161.655764 101.891473) (xy 161.95 101.951) (xy 162.244236 101.891473) (xy 162.193901 101.686305)
				(xy 162.161972 101.552049) (xy 162.15 101.355764)
			)
		)
	)
	(zone
		(net 10)
		(net_name "VBUS")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30019)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 126.212718 100.759183) (xy 126.080189 100.510292) (xy 125.947994 100.305831) (xy 125.899441 100.233329)
				(xy 125.649546 100.39911) (xy 125.483329 100.649441) (xy 125.625304 100.728171) (xy 125.645045 100.737208)
				(xy 125.704239 100.76585) (xy 125.756149 100.801236) (xy 125.805326 100.855504) (xy 125.856322 100.94079)
			)
		)
	)
	(zone
		(net 2)
		(net_name "/AD1")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30057)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 140.250689 95.464257) (xy 140.311818 95.481378) (xy 140.354595 95.504212) (xy 140.401615 95.559843)
				(xy 140.42625 95.612718) (xy 140.492133 95.738893) (xy 140.70098 95.600195) (xy 140.748773 95.354804)
				(xy 140.519312 95.311468) (xy 140.289714 95.268102)
			)
		)
	)
	(zone
		(net 30)
		(net_name "/BUS_A11")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30002)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 144.043659 93.753185) (xy 143.985777 93.676583) (xy 143.945068 93.605834) (xy 143.921583 93.545533)
				(xy 143.910023 93.488739) (xy 143.917529 93.384973) (xy 143.963109 93.277605) (xy 144.060619 93.139847)
				(xy 144.095024 93.096723) (xy 144.183775 92.983007) (xy 144.2702 92.854286) (xy 144.344443 92.704944)
				(xy 144.396651 92.529366) (xy 143.648651 92.379941) (xy 143.015713 92.804052) (xy 143.192639 93.060146)
				(xy 143.329901 93.240714) (xy 143.546105 93.488808) (xy 143.89045 93.881743)
			)
		)
	)
	(zone
		(net 25)
		(net_name "/(A)")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30046)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 134.60404 97.553435) (xy 134.513247 97.563018) (xy 134.442564 97.562325) (xy 134.35759 97.551183)
				(xy 134.252337 97.539405) (xy 134.101227 97.554804) (xy 134.149012 97.800153) (xy 134.288893 98.007867)
				(xy 134.38681 97.923882) (xy 134.427688 97.874096) (xy 134.46137 97.833018) (xy 134.500722 97.798089)
				(xy 134.555342 97.770402) (xy 134.634831 97.751049)
			)
		)
	)
	(zone
		(net 60)
		(net_name "/A4")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30042)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 138.695196 102.25) (xy 138.615664 102.245332) (xy 138.555069 102.232658) (xy 138.452813 102.184439)
				(xy 138.371184 102.141714) (xy 138.248773 102.104804) (xy 138.199 102.35) (xy 138.248773 102.595196)
				(xy 138.385415 102.551905) (xy 138.452813 102.515561) (xy 138.547709 102.469647) (xy 138.610872 102.455319)
				(xy 138.695196 102.45)
			)
		)
	)
	(zone
		(net 21)
		(net_name "/~{RD}")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30037)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 153.314097 104.5) (xy 153.393629 104.504668) (xy 153.454224 104.517342) (xy 153.55648 104.565561)
				(xy 153.638108 104.608285) (xy 153.76052 104.645196) (xy 153.810293 104.4) (xy 153.76052 104.154804)
				(xy 153.623878 104.198094) (xy 153.556479 104.234439) (xy 153.461583 104.280353) (xy 153.398421 104.294681)
				(xy 153.314097 104.3)
			)
		)
	)
	(zone
		(net 56)
		(net_name "/A9")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30043)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 129.495196 101.65) (xy 129.415664 101.645332) (xy 129.355069 101.632658) (xy 129.252813 101.584439)
				(xy 129.171184 101.541714) (xy 129.048773 101.504804) (xy 128.999 101.75) (xy 129.048773 101.995196)
				(xy 129.185415 101.951905) (xy 129.252813 101.915561) (xy 129.347709 101.869647) (xy 129.410872 101.855319)
				(xy 129.495196 101.85)
			)
		)
	)
	(zone
		(net 57)
		(net_name "/A7")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30059)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 129.410286 102.268102) (xy 129.180691 102.311467) (xy 128.951227 102.354804) (xy 128.99902 102.600195)
				(xy 129.207867 102.738893) (xy 129.273749 102.612719) (xy 129.297855 102.560813) (xy 129.328059 102.51904)
				(xy 129.374998 102.486991) (xy 129.449311 102.464257)
			)
		)
	)
	(zone
		(net 9)
		(net_name "/AD0")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30038)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 141.154804 103.8) (xy 141.234336 103.804668) (xy 141.294931 103.817342) (xy 141.397187 103.865561)
				(xy 141.478815 103.908285) (xy 141.601227 103.945196) (xy 141.651 103.7) (xy 141.601227 103.454804)
				(xy 141.464585 103.498094) (xy 141.397186 103.534439) (xy 141.30229 103.580353) (xy 141.239128 103.594681)
				(xy 141.154804 103.6)
			)
		)
	)
	(zone
		(net 25)
		(net_name "/(A)")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30025)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 155.929133 101.970554) (xy 155.982069 102.030092) (xy 156.015954 102.081901) (xy 156.054164 102.188303)
				(xy 156.081674 102.276234) (xy 156.142133 102.388893) (xy 156.350707 102.250707) (xy 156.488893 102.042133)
				(xy 156.361662 101.976123) (xy 156.288303 101.954164) (xy 156.188735 101.919529) (xy 156.133941 101.884998)
				(xy 156.070554 101.829133)
			)
		)
	)
	(zone
		(net 7)
		(net_name "/AD4")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30050)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 144.566227 104.863466) (xy 144.636707 104.813121) (xy 144.695285 104.781866) (xy 144.783222 104.751808)
				(xy 144.872221 104.722009) (xy 144.988893 104.657867) (xy 144.850781 104.449377) (xy 144.642133 104.311107)
				(xy 144.585206 104.425084) (xy 144.565634 104.502874) (xy 144.535121 104.601314) (xy 144.500366 104.651787)
				(xy 144.441528 104.707103)
			)
		)
	)
	(zone
		(net 56)
		(net_name "/A9")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30063)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 136.089783 100.42038) (xy 136.120244 100.323307) (xy 136.166877 100.191704) (xy 136.257867 100.038893)
				(xy 136.050309 99.899049) (xy 135.804804 99.948773) (xy 135.844153 100.067757) (xy 135.873703 100.122937)
				(xy 135.899 100.170398) (xy 135.91536 100.219967) (xy 135.91736 100.27993) (xy 135.899575 100.35857)
			)
		)
	)
	(zone
		(net 4)
		(net_name "/AD5")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30067)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 162.309205 96.541609) (xy 162.388269 96.561927) (xy 162.445862 96.585112) (xy 162.505212 96.618403)
				(xy 162.5819 96.659647) (xy 162.701227 96.695196) (xy 162.75098 96.450195) (xy 162.701227 96.204804)
				(xy 162.604871 96.240659) (xy 162.539293 96.290387) (xy 162.504121 96.319242) (xy 162.465026 96.341093)
				(xy 162.415299 96.351357) (xy 162.34823 96.345454)
			)
		)
	)
	(zone
		(net 33)
		(net_name "/RAMRST")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30033)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 162.55 104.904803) (xy 162.545332 104.984335) (xy 162.532658 105.04493) (xy 162.484439 105.147185)
				(xy 162.441714 105.228814) (xy 162.404804 105.351226) (xy 162.65 105.400999) (xy 162.895196 105.351226)
				(xy 162.851905 105.214583) (xy 162.815561 105.147186) (xy 162.769647 105.05229) (xy 162.755319 104.989127)
				(xy 162.75 104.904803)
			)
		)
	)
	(zone
		(net 54)
		(net_name "/~{Y0}")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30054)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 158.610191 99.449823) (xy 158.854215 99.438526) (xy 159.090946 99.396753) (xy 159.098773 99.395196)
				(xy 159.050999 99.149977) (xy 158.842133 99.011107) (xy 158.782659 99.121246) (xy 158.756507 99.173635)
				(xy 158.725123 99.213559) (xy 158.678201 99.239485) (xy 158.605435 99.249881)
			)
		)
	)
	(zone
		(net 10)
		(net_name "VBUS")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30001)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 126 106.096707) (xy 125.980301 106.243642) (xy 125.914241 106.426058) (xy 125.864072 106.519715)
				(xy 125.803003 106.611026) (xy 125.736421 106.691832) (xy 125.660862 106.76614) (xy 125.585098 106.825895)
				(xy 125.502403 106.877008) (xy 125.421713 106.914506) (xy 125.335634 106.942446) (xy 125.23287 106.960954)
				(xy 125.869293 107.621707) (xy 126.602291 107.093905) (xy 126.542336 107.037053) (xy 126.48828 106.930987)
				(xy 126.442464 106.756138) (xy 126.411126 106.495218) (xy 126.4 106.096707)
			)
		)
	)
	(zone
		(net 3)
		(net_name "/AD3")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30068)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 161.807317 96.948738) (xy 161.929781 97.058297) (xy 162.004495 97.125135) (xy 162.092133 97.238893)
				(xy 162.300707 97.100707) (xy 162.348773 96.854804) (xy 162.23795 96.849076) (xy 162.160279 96.862885)
				(xy 162.108688 96.872851) (xy 162.059068 96.872715) (xy 162.007169 96.853773) (xy 161.948738 96.807317)
			)
		)
	)
	(zone
		(net 9)
		(net_name "/AD0")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30049)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 141.949024 103.301989) (xy 141.884107 103.347854) (xy 141.828631 103.376322) (xy 141.726121 103.404824)
				(xy 141.632104 103.429143) (xy 141.511107 103.492133) (xy 141.649219 103.700623) (xy 141.857867 103.838893)
				(xy 141.920351 103.717738) (xy 141.93908 103.65886) (xy 141.976508 103.563128) (xy 142.013554 103.513647)
				(xy 142.073729 103.45835)
			)
		)
	)
	(zone
		(net 10)
		(net_name "VBUS")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30014)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 159.727046 98.488155) (xy 159.563572 98.321402) (xy 159.536099 98.289108) (xy 159.436049 98.18075)
				(xy 159.266671 98.050559) (xy 159.099259 98.29933) (xy 158.933329 98.549441) (xy 159.00656 98.592866)
				(xy 159.070168 98.620877) (xy 159.189485 98.651525) (xy 159.311503 98.685167) (xy 159.379734 98.722482)
				(xy 159.458703 98.784788)
			)
		)
	)
	(zone
		(net 3)
		(net_name "/AD3")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30071)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 142.778827 95.41024) (xy 142.737124 95.36958) (xy 142.716581 95.333557) (xy 142.705605 95.273325)
				(xy 142.695196 95.201227) (xy 142.449227 95.249366) (xy 142.401227 95.495196) (xy 142.500887 95.506204)
				(xy 142.570733 95.515784) (xy 142.651946 95.564841)
			)
		)
	)
	(zone
		(net 6)
		(net_name "/AD6")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30009)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 139.56586 106.482718) (xy 139.455041 106.58653) (xy 139.356008 106.664801) (xy 139.275585 106.715808)
				(xy 139.199064 106.752781) (xy 139.047199 106.795671) (xy 138.844458 106.818133) (xy 138.655894 106.836106)
				(xy 138.420634 106.873349) (xy 138.568586 107.621414) (xy 139.316651 107.769366) (xy 139.360798 107.470847)
				(xy 139.371867 107.345543) (xy 139.391224 107.161391) (xy 139.408281 107.078162) (xy 139.434922 106.996619)
				(xy 139.474644 106.913604) (xy 139.530946 106.825959) (xy 139.607326 106.730523) (xy 139.707282 106.62414)
			)
		)
	)
	(zone
		(net 10)
		(net_name "VBUS")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30016)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 125.4 99.805764) (xy 125.400271 99.89972) (xy 125.395392 100.102418) (xy 125.355764 100.341473)
				(xy 125.65 100.401) (xy 125.944236 100.341473) (xy 125.894901 100.171982) (xy 125.864814 100.103893)
				(xy 125.819151 99.985772) (xy 125.805156 99.90856) (xy 125.8 99.805764)
			)
		)
	)
	(zone
		(net 49)
		(net_name "/BLOCK")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30034)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 128.25 103.654804) (xy 128.245332 103.734336) (xy 128.232658 103.794931) (xy 128.184439 103.897186)
				(xy 128.141714 103.978815) (xy 128.104804 104.101227) (xy 128.35 104.151) (xy 128.595196 104.101227)
				(xy 128.551905 103.964584) (xy 128.515561 103.897187) (xy 128.469647 103.802291) (xy 128.455319 103.739128)
				(xy 128.45 103.654804)
			)
		)
	)
	(zone
		(net 2)
		(net_name "/AD1")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30052)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 160.06643 97.507937) (xy 160.114008 97.545428) (xy 160.144841 97.581883) (xy 160.172418 97.6535)
				(xy 160.178633 97.699393) (xy 160.19351 97.785531) (xy 160.211565 97.834626) (xy 160.242133 97.888893)
				(xy 160.450831 97.750555) (xy 160.588893 97.542133) (xy 160.506667 97.492547) (xy 160.441755 97.462606)
				(xy 160.383214 97.441886) (xy 160.295319 97.408719) (xy 160.17754 97.341643)
			)
		)
	)
	(zone
		(net 36)
		(net_name "/BYTE")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30022)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 130.494236 103.45) (xy 130.411011 103.445292) (xy 130.345486 103.432338) (xy 130.24669 103.387978)
				(xy 130.20659 103.361952) (xy 130.108336 103.3038) (xy 130.042594 103.277548) (xy 129.958527 103.255764)
				(xy 129.899 103.55) (xy 129.958527 103.844236) (xy 130.039399 103.823493) (xy 130.103273 103.798581)
				(xy 130.20659 103.738048) (xy 130.259116 103.704617) (xy 130.318223 103.676536) (xy 130.393425 103.6572)
				(xy 130.494236 103.65)
			)
		)
	)
	(zone
		(net 49)
		(net_name "/BLOCK")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30026)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 156.529133 101.370554) (xy 156.582069 101.430092) (xy 156.615954 101.481901) (xy 156.654164 101.588303)
				(xy 156.681674 101.676234) (xy 156.742133 101.788893) (xy 156.950707 101.650707) (xy 157.088893 101.442133)
				(xy 156.961662 101.376123) (xy 156.888303 101.354164) (xy 156.788735 101.319529) (xy 156.733941 101.284998)
				(xy 156.670554 101.229133)
			)
		)
	)
	(zone
		(net 58)
		(net_name "/A0")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30061)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 128.810143 105.289738) (xy 128.742557 105.306025) (xy 128.688958 105.308782) (xy 128.608687 105.287272)
				(xy 128.570058 105.268097) (xy 128.498289 105.234158) (xy 128.398773 105.204804) (xy 128.349047 105.4503)
				(xy 128.488893 105.657867) (xy 128.660066 105.553635) (xy 128.831849 105.492554) (xy 128.870264 105.480487)
			)
		)
	)
	(zone
		(net 64)
		(net_name "/A5")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30044)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 135.35 99.895196) (xy 135.354668 99.815664) (xy 135.367342 99.755069) (xy 135.415561 99.652813)
				(xy 135.458285 99.571184) (xy 135.495196 99.448773) (xy 135.25 99.399) (xy 135.004804 99.448773)
				(xy 135.048094 99.585415) (xy 135.084439 99.652813) (xy 135.130353 99.747709) (xy 135.144681 99.810872)
				(xy 135.15 99.895196)
			)
		)
	)
	(zone
		(net 10)
		(net_name "VBUS")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30018)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 125.45 94.955764) (xy 125.445239 95.090957) (xy 125.431909 95.185989) (xy 125.406099 95.286303)
				(xy 125.355764 95.491473) (xy 125.65 95.551) (xy 125.944236 95.491473) (xy 125.893901 95.286305)
				(xy 125.861972 95.152049) (xy 125.85 94.955764)
			)
		)
	)
	(zone
		(net 5)
		(net_name "/AD7")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30013)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 139.645284 93.275667) (xy 139.554882 93.224096) (xy 139.48372 93.171704) (xy 139.433793 93.122841)
				(xy 139.396322 93.072465) (xy 139.352306 92.966547) (xy 139.337281 92.83342) (xy 139.340734 92.691242)
				(xy 139.344297 92.481581) (xy 139.336412 92.362282) (xy 139.316651 92.232048) (xy 138.568402 92.380254)
				(xy 138.420634 93.128065) (xy 138.771748 93.190479) (xy 138.954609 93.222339) (xy 139.118852 93.263932)
				(xy 139.305228 93.334646) (xy 139.55449 93.453869)
			)
		)
	)
	(zone
		(net 7)
		(net_name "/AD4")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30065)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 145.222397 104.074431) (xy 145.030622 104.137995) (xy 144.93923 104.171) (xy 144.801227 104.204804)
				(xy 144.849035 104.450258) (xy 145.057867 104.588893) (xy 145.108044 104.486097) (xy 145.124796 104.42763)
				(xy 145.140053 104.375389) (xy 145.163331 104.33117) (xy 145.204681 104.295178) (xy 145.274153 104.267617)
			)
		)
	)
	(zone
		(net 1)
		(net_name "GND")
		(layers "F.Cu" "B.Cu")
		(hatch edge 0.508)
		(connect_pads
			(clearance 0.2)
		)
		(min_thickness 0.2)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.2)
			(thermal_bridge_width 0.3)
			(smoothing fillet)
			(radius 0.2)
		)
		(polygon
			(pts
				(xy 124.346 109.144) (xy 175.654 109.144) (xy 175.654 90.856) (xy 124.346 90.856)
			)
		)
	)
	(zone
		(net 73)
		(net_name "/A14")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30110)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 157.195095 97.950001) (xy 157.334478 97.90097) (xy 157.520148 97.879763) (xy 157.753302 97.895316)
				(xy 157.910667 97.925) (xy 157.900866 97.749501) (xy 157.3 97.663076) (xy 157.28231 97.696832) (xy 157.220855 97.731091)
				(xy 157.158024 97.753298) (xy 157.095101 97.776793)
			)
		)
	)
	(zone
		(net 59)
		(net_name "/A6")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30054)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 139.094414 104.877507) (xy 139.10255 104.977327) (xy 139.098907 105.036455) (xy 139.085863 105.093146)
				(xy 139.065876 105.13335) (xy 139.035626 105.164008) (xy 139.009515 105.177165) (xy 139.250239 105.60097)
				(xy 139.464671 105.138532) (xy 139.406579 105.11064) (xy 139.3552 105.044709) (xy 139.311069 104.932365)
				(xy 139.288601 104.829643)
			)
		)
	)
	(zone
		(net 30)
		(net_name "/BUS_A11")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30070)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 162.925 95.3) (xy 162.991579 95.290878) (xy 163.104554 95.278745) (xy 163.153453 95.290592)
				(xy 163.1875 95.325) (xy 163.701 95.15) (xy 163.1875 94.975) (xy 163.149436 95.011332) (xy 163.085856 95.021559)
				(xy 162.991579 95.009122) (xy 162.925 95)
			)
		)
	)
	(zone
		(net 5)
		(net_name "/AD7")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30097)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 162.795196 95.7) (xy 162.715664 95.695332) (xy 162.655069 95.682658) (xy 162.552813 95.634439)
				(xy 162.471184 95.591714) (xy 162.348773 95.554804) (xy 162.299 95.8) (xy 162.348773 96.045196)
				(xy 162.485415 96.001905) (xy 162.552813 95.965561) (xy 162.647709 95.919647) (xy 162.710872 95.905319)
				(xy 162.795196 95.9)
			)
		)
	)
	(zone
		(net 8)
		(net_name "/AD2")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30098)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 142.55 104.995196) (xy 142.554668 104.915664) (xy 142.567342 104.855069) (xy 142.615561 104.752813)
				(xy 142.658285 104.671184) (xy 142.695196 104.548773) (xy 142.45 104.499) (xy 142.204804 104.548773)
				(xy 142.248094 104.685415) (xy 142.284439 104.752813) (xy 142.330353 104.847709) (xy 142.344681 104.910872)
				(xy 142.35 104.995196)
			)
		)
	)
	(zone
		(net 65)
		(net_name "/A12")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30111)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 157.195095 96.649979) (xy 157.334473 96.600952) (xy 157.520136 96.57975) (xy 157.753285 96.595308)
				(xy 157.910666 96.625) (xy 157.900866 96.449501) (xy 157.3 96.363059) (xy 157.28231 96.396813) (xy 157.220854 96.431072)
				(xy 157.158024 96.453277) (xy 157.095101 96.476771)
			)
		)
	)
	(zone
		(net 49)
		(net_name "/BLOCK")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30071)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 157.125 101.8) (xy 157.191579 101.790878) (xy 157.304554 101.778745) (xy 157.353453 101.790592)
				(xy 157.3875 101.825) (xy 157.901 101.65) (xy 157.3875 101.475) (xy 157.349436 101.511332) (xy 157.285856 101.521559)
				(xy 157.191579 101.509122) (xy 157.125 101.5)
			)
		)
	)
	(zone
		(net 9)
		(net_name "/AD0")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30099)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 141.75 104.195196) (xy 141.754668 104.115664) (xy 141.767342 104.055069) (xy 141.815561 103.952813)
				(xy 141.858285 103.871184) (xy 141.895196 103.748773) (xy 141.65 103.699) (xy 141.404804 103.748773)
				(xy 141.448094 103.885415) (xy 141.484439 103.952813) (xy 141.530353 104.047709) (xy 141.544681 104.110872)
				(xy 141.55 104.195196)
			)
		)
	)
	(zone
		(net 33)
		(net_name "/RAMRST")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30085)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 163.070867 105.679445) (xy 163.01793 105.619907) (xy 162.984045 105.568097) (xy 162.945835 105.461695)
				(xy 162.918326 105.373764) (xy 162.857867 105.261106) (xy 162.649293 105.399292) (xy 162.511107 105.607866)
				(xy 162.638338 105.673875) (xy 162.711696 105.695834) (xy 162.811264 105.73047) (xy 162.866059 105.765001)
				(xy 162.929446 105.820866)
			)
		)
	)
	(zone
		(net 10)
		(net_name "VBUS")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30024)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 162.467096 102.884293) (xy 162.391796 102.8049) (xy 162.344467 102.741177) (xy 162.298592 102.656679)
				(xy 162.199441 102.483329) (xy 161.949282 102.649305) (xy 161.783329 102.899441) (xy 161.956142 103.001246)
				(xy 162.058734 103.061179) (xy 162.188956 103.171759)
			)
		)
	)
	(zone
		(net 36)
		(net_name "/BYTE")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30030)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 129.550523 104.040898) (xy 129.612701 103.985378) (xy 129.668194 103.948205) (xy 129.76942 103.909712)
				(xy 129.816178 103.899761) (xy 129.926774 103.871405) (xy 129.991823 103.843481) (xy 130.066671 103.799441)
				(xy 129.900707 103.549293) (xy 129.650559 103.383329) (xy 129.608042 103.455181) (xy 129.580491 103.517962)
				(xy 129.550238 103.633822) (xy 129.536736 103.694603) (xy 129.514797 103.756254) (xy 129.475294 103.823102)
				(xy 129.409102 103.899477)
			)
		)
	)
	(zone
		(net 35)
		(net_name "/BUS_A8")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30138)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 132.459186 95.971383) (xy 132.478808 95.968582) (xy 132.587512 95.962086) (xy 132.637616 95.97781)
				(xy 132.669015 96.018339) (xy 133.215984 95.849827) (xy 132.654301 95.691492) (xy 132.626087 95.73201)
				(xy 132.563011 95.758207) (xy 132.461082 95.771179) (xy 132.424456 95.774423)
			)
		)
	)
	(zone
		(net 59)
		(net_name "/A6")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30112)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 133.99 102.75) (xy 133.964647 102.750501) (xy 133.846363 102.744476) (xy 133.793301 102.723834)
				(xy 133.760985 102.681661) (xy 133.214 102.85) (xy 133.760985 103.018339) (xy 133.793029 102.976351)
				(xy 133.855788 102.953755) (xy 133.964648 102.949499) (xy 133.99 102.95)
			)
		)
	)
	(zone
		(net 49)
		(net_name "/BLOCK")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30059)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 127.854804 104.3) (xy 127.958667 104.304661) (xy 128.032958 104.317289) (xy 128.114687 104.343006)
				(xy 128.191788 104.368504) (xy 128.301227 104.395196) (xy 128.351 104.15) (xy 128.301227 103.904804)
				(xy 128.126279 103.952912) (xy 128.114686 103.956994) (xy 128.010461 103.987679) (xy 127.854804 104)
			)
		)
	)
	(zone
		(net 3)
		(net_name "/AD3")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30087)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 142.35 94.754804) (xy 142.345332 94.834336) (xy 142.332658 94.894931) (xy 142.284439 94.997186)
				(xy 142.241714 95.078815) (xy 142.204804 95.201227) (xy 142.45 95.251) (xy 142.695196 95.201227)
				(xy 142.651905 95.064584) (xy 142.615561 94.997187) (xy 142.569647 94.902291) (xy 142.555319 94.839128)
				(xy 142.55 94.754804)
			)
		)
	)
	(zone
		(net 10)
		(net_name "VBUS")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30072)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 126.64 101.05) (xy 126.706579 101.040878) (xy 126.819554 101.028745) (xy 126.868453 101.040592)
				(xy 126.9025 101.075) (xy 127.416 100.9) (xy 126.9025 100.725) (xy 126.864436 100.761332) (xy 126.800856 100.771559)
				(xy 126.706579 100.759122) (xy 126.64 100.75)
			)
		)
	)
	(zone
		(net 20)
		(net_name "+BATT")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30001)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 168.43345 105.5) (xy 168.686221 105.520569) (xy 168.839089 105.548472) (xy 168.998427 105.588792)
				(xy 169.143376 105.636398) (xy 169.284575 105.694943) (xy 169.39923 105.754033) (xy 169.505287 105.821636)
				(xy 169.58712 105.886368) (xy 169.659006 105.957634) (xy 169.683437 105.98655) (xy 170.321 105.3)
				(xy 169.683437 104.61345) (xy 169.561779 104.735178) (xy 169.393441 104.849256) (xy 169.174782 104.951723)
				(xy 168.910147 105.034997) (xy 168.623898 105.087737) (xy 168.43345 105.1)
			)
		)
	)
	(zone
		(net 2)
		(net_name "/AD1")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30107)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 141.075907 95.332673) (xy 141.033093 95.36872) (xy 140.993991 95.388738) (xy 140.925877 95.394175)
				(xy 140.857559 95.375682) (xy 140.767228 95.351903) (xy 140.71326 95.348095) (xy 140.651227 95.354804)
				(xy 140.699293 95.600707) (xy 140.838893 95.807867) (xy 140.980742 95.70663) (xy 141.069607 95.626116)
				(xy 141.114812 95.57931) (xy 141.217327 95.474093)
			)
		)
	)
	(zone
		(net 7)
		(net_name "/AD4")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30082)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 159.329446 101.629133) (xy 159.269908 101.682069) (xy 159.218098 101.715954) (xy 159.111697 101.754164)
				(xy 159.023765 101.781674) (xy 158.911107 101.842133) (xy 159.049293 102.050707) (xy 159.257867 102.188893)
				(xy 159.323876 102.061662) (xy 159.345835 101.988304) (xy 159.38047 101.888736) (xy 159.415002 101.833941)
				(xy 159.470867 101.770554)
			)
		)
	)
	(zone
		(net 55)
		(net_name "/A8")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30088)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 137.55 99.404804) (xy 137.545332 99.484336) (xy 137.532658 99.544931) (xy 137.484439 99.647186)
				(xy 137.441714 99.728815) (xy 137.404804 99.851227) (xy 137.65 99.901) (xy 137.895196 99.851227)
				(xy 137.851905 99.714584) (xy 137.815561 99.647187) (xy 137.769647 99.552291) (xy 137.755319 99.489128)
				(xy 137.75 99.404804)
			)
		)
	)
	(zone
		(net 9)
		(net_name "/AD0")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30083)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 159.329446 100.429133) (xy 159.269908 100.482069) (xy 159.218098 100.515954) (xy 159.111697 100.554164)
				(xy 159.023765 100.581674) (xy 158.911107 100.642133) (xy 159.049293 100.850707) (xy 159.257867 100.988893)
				(xy 159.323876 100.861662) (xy 159.345835 100.788304) (xy 159.38047 100.688736) (xy 159.415002 100.633941)
				(xy 159.470867 100.570554)
			)
		)
	)
	(zone
		(net 71)
		(net_name "/A18")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30130)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 157.14189 100.450575) (xy 157.16384 100.449942) (xy 157.273306 100.45537) (xy 157.322973 100.475922)
				(xy 157.354015 100.518339) (xy 157.900987 100.349844) (xy 157.354015 100.181661) (xy 157.322124 100.222947)
				(xy 157.25741 100.246784) (xy 157.136542 100.253213) (xy 157.110596 100.253039)
			)
		)
	)
	(zone
		(net 13)
		(net_name "VMEM")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30021)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 161.423976 103.941134) (xy 161.380147 103.890512) (xy 161.353891 103.844984) (xy 161.338837 103.76638)
				(xy 161.345599 103.695968) (xy 161.354208 103.606236) (xy 161.344236 103.491473) (xy 161.049293 103.549293)
				(xy 160.800559 103.716671) (xy 160.917453 103.915344) (xy 160.926971 103.93385) (xy 161.00128 104.062725)
				(xy 161.057683 104.134875) (xy 161.141134 104.223976)
			)
		)
	)
	(zone
		(net 5)
		(net_name "/AD7")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30089)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 145.55 94.754804) (xy 145.545332 94.834336) (xy 145.532658 94.894931) (xy 145.484439 94.997186)
				(xy 145.441714 95.078815) (xy 145.404804 95.201227) (xy 145.65 95.251) (xy 145.895196 95.201227)
				(xy 145.851905 95.064584) (xy 145.815561 94.997187) (xy 145.769647 94.902291) (xy 145.755319 94.839128)
				(xy 145.75 94.754804)
			)
		)
	)
	(zone
		(net 13)
		(net_name "VMEM")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30003)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 152.825 100.3) (xy 152.929518 100.302404) (xy 153.056331 100.314229) (xy 153.189856 100.342398)
				(xy 153.314507 100.393832) (xy 153.369719 100.431315) (xy 153.416474 100.477596) (xy 153.447561 100.523705)
				(xy 153.470073 100.577146) (xy 153.482098 100.632706) (xy 154.301 100.124999) (xy 153.65 99.549999)
				(xy 153.5905 99.618557) (xy 153.495848 99.669087) (xy 153.354638 99.701554) (xy 153.152169 99.71193)
				(xy 152.959362 99.704982) (xy 152.825 99.7)
			)
		)
	)
	(zone
		(net 4)
		(net_name "/AD5")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30073)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 162.925 96.6) (xy 162.991579 96.590878) (xy 163.104554 96.578745) (xy 163.153453 96.590592)
				(xy 163.1875 96.625) (xy 163.701 96.45) (xy 163.1875 96.275) (xy 163.149436 96.311332) (xy 163.085856 96.321559)
				(xy 162.991579 96.309122) (xy 162.925 96.3)
			)
		)
	)
	(zone
		(net 8)
		(net_name "/AD2")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30120)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 162.925 99.15) (xy 162.950352 99.149499) (xy 163.068637 99.155524) (xy 163.121699 99.176166)
				(xy 163.154015 99.218339) (xy 163.701 99.05) (xy 163.154015 98.881661) (xy 163.121972 98.923649)
				(xy 163.059213 98.946245) (xy 162.950353 98.950501) (xy 162.925 98.95)
			)
		)
	)
	(zone
		(net 68)
		(net_name "/A19")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30041)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 151.95 104.85) (xy 151.943116 104.947519) (xy 151.914925 105.061161) (xy 151.888731 105.112881)
				(xy 151.852577 105.153702) (xy 151.809515 105.177165) (xy 152.05 105.601) (xy 152.290485 105.177165)
				(xy 152.232121 105.139485) (xy 152.187323 105.066762) (xy 152.157717 104.95329) (xy 152.15 104.85)
			)
		)
	)
	(zone
		(net 58)
		(net_name "/A0")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30033)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 138.55 95.15) (xy 138.556884 95.052484) (xy 138.585074 94.938844) (xy 138.611267 94.887123)
				(xy 138.647421 94.8463) (xy 138.690485 94.822835) (xy 138.45 94.399) (xy 138.209515 94.822835) (xy 138.26788 94.860515)
				(xy 138.312677 94.933239) (xy 138.342283 95.04671) (xy 138.35 95.15)
			)
		)
	)
	(zone
		(net 73)
		(net_name "/A14")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30062)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 149.023371 95.126631) (xy 149.011608 94.985264) (xy 149.022369 94.907252) (xy 149.055413 94.845661)
				(xy 149.090485 94.822835) (xy 148.849805 94.39902) (xy 148.64609 94.869721) (xy 148.705786 94.895544)
				(xy 148.758441 94.958644) (xy 148.803854 95.066497) (xy 148.827215 95.165649)
			)
		)
	)
	(zone
		(net 25)
		(net_name "/(A)")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30074)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 133.99 97.65) (xy 133.923421 97.659122) (xy 133.810446 97.671255) (xy 133.761547 97.659408)
				(xy 133.7275 97.625) (xy 133.214 97.8) (xy 133.7275 97.975) (xy 133.765564 97.938668) (xy 133.829144 97.928441)
				(xy 133.923421 97.940878) (xy 133.99 97.95)
			)
		)
	)
	(zone
		(net 33)
		(net_name "/RAMRST")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30108)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 162.203241 105.65) (xy 162.402994 105.661037) (xy 162.52509 105.667757) (xy 162.698773 105.645195)
				(xy 162.651 105.399999) (xy 162.511107 105.192132) (xy 162.432139 105.264427) (xy 162.385174 105.336787)
				(xy 162.357829 105.38128) (xy 162.324421 105.417219) (xy 162.275906 105.441245) (xy 162.203241 105.45)
			)
		)
	)
	(zone
		(net 70)
		(net_name "/A17")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30042)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 150.35 104.85) (xy 150.343116 104.947519) (xy 150.314925 105.061161) (xy 150.288731 105.112881)
				(xy 150.252577 105.153702) (xy 150.209515 105.177165) (xy 150.45 105.601) (xy 150.690485 105.177165)
				(xy 150.632121 105.139485) (xy 150.587323 105.066762) (xy 150.557717 104.95329) (xy 150.55 104.85)
			)
		)
	)
	(zone
		(net 4)
		(net_name "/AD5")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30056)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 163.245196 96.3) (xy 163.141334 96.295339) (xy 163.067044 96.282711) (xy 162.985313 96.256994)
				(xy 162.908213 96.231495) (xy 162.798773 96.204804) (xy 162.749 96.45) (xy 162.798773 96.695196)
				(xy 162.973722 96.647087) (xy 162.985312 96.643007) (xy 163.089538 96.612321) (xy 163.245196 96.6)
			)
		)
	)
	(zone
		(net 21)
		(net_name "/~{RD}")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30006)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 153.709293 106.111349) (xy 153.704339 106.263116) (xy 153.689658 106.388487) (xy 153.668857 106.481422)
				(xy 153.640893 106.561674) (xy 153.563836 106.699387) (xy 153.436359 106.858629) (xy 153.315733 107.004673)
				(xy 153.175713 107.197362) (xy 153.809293 107.621707) (xy 154.442873 107.197362) (xy 154.263006 106.955061)
				(xy 154.182227 106.85863) (xy 154.065701 106.714728) (xy 154.01891 106.643815) (xy 153.980089 106.567318)
				(xy 153.949476 106.48053) (xy 153.927312 106.378744) (xy 153.913838 106.257253) (xy 153.909293 106.111349)
			)
		)
	)
	(zone
		(net 27)
		(net_name "/~{WR}")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30009)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 152.849016 93.428737) (xy 153.0442 93.334878) (xy 153.19764 93.273446) (xy 153.413084 93.217089)
				(xy 153.575861 93.191828) (xy 153.957952 93.128065) (xy 153.810183 92.380253) (xy 153.061935 92.232048)
				(xy 153.037209 92.442486) (xy 153.043153 92.687437) (xy 153.0485 92.854825) (xy 153.041269 92.929808)
				(xy 153.022505 93.00008) (xy 152.988514 93.066466) (xy 152.935598 93.129789) (xy 152.860063 93.190872)
				(xy 152.758212 93.250539)
			)
		)
	)
	(zone
		(net 56)
		(net_name "/A9")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30139)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 128.156312 102.066557) (xy 128.141239 102.06931) (xy 128.087272 102.078052) (xy 128.026144 102.080241)
				(xy 127.969129 102.065886) (xy 127.9275 102.025) (xy 127.414049 102.200309) (xy 127.991171 102.346679)
				(xy 128.015185 102.307237) (xy 128.07588 102.279329) (xy 128.179031 102.26194) (xy 128.218121 102.256765)
			)
		)
	)
	(zone
		(net 49)
		(net_name "/BLOCK")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30025)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 127.905764 97.95) (xy 128.004232 97.954683) (xy 128.079101 97.967462) (xy 128.203893 98.014814)
				(xy 128.300365 98.055763) (xy 128.441473 98.094236) (xy 128.501 97.8) (xy 128.441473 97.505764)
				(xy 128.271983 97.555098) (xy 128.203892 97.585186) (xy 128.085772 97.630849) (xy 128.00856 97.644844)
				(xy 127.905764 97.65)
			)
		)
	)
	(zone
		(net 65)
		(net_name "/A12")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30064)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 150.641188 95.11057) (xy 150.625033 95.004632) (xy 150.623882 94.941371) (xy 150.632044 94.879129)
				(xy 150.648747 94.831811) (xy 150.676675 94.792957) (xy 150.7 94.775) (xy 150.449778 94.399026)
				(xy 150.259094 94.87841) (xy 150.319308 94.902101) (xy 150.373485 94.963013) (xy 150.42181 95.068213)
				(xy 150.446204 95.155074)
			)
		)
	)
	(zone
		(net 10)
		(net_name "VBUS")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30010)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 126.675 100.75) (xy 126.385305 100.764381) (xy 125.98733 100.783282) (xy 125.787433 100.776738)
				(xy 125.600972 100.75) (xy 125.649 101.15) (xy 126.275 101.409168) (xy 126.279803 101.351469) (xy 126.293422 101.299281)
				(xy 126.345728 101.20669) (xy 126.43074 101.129915) (xy 126.545509 101.07368) (xy 126.668882 101.05007)
				(xy 126.675 101.05)
			)
		)
	)
	(zone
		(net 36)
		(net_name "/BYTE")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30029)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 129.8 102.955764) (xy 129.795292 103.038989) (xy 129.782338 103.104514) (xy 129.737978 103.20331)
				(xy 129.711952 103.243409) (xy 129.6538 103.341663) (xy 129.627548 103.407406) (xy 129.605764 103.491473)
				(xy 129.9 103.551) (xy 130.194236 103.491473) (xy 130.173493 103.410601) (xy 130.148581 103.346727)
				(xy 130.088048 103.243409) (xy 130.054617 103.190883) (xy 130.026536 103.131776) (xy 130.0072 103.056574)
				(xy 130 102.955764)
			)
		)
	)
	(zone
		(net 55)
		(net_name "/A8")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30034)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 137.75 95.15) (xy 137.756884 95.052484) (xy 137.785074 94.938844) (xy 137.811267 94.887123)
				(xy 137.847421 94.8463) (xy 137.890485 94.822835) (xy 137.65 94.399) (xy 137.409515 94.822835) (xy 137.46788 94.860515)
				(xy 137.512677 94.933239) (xy 137.542283 95.04671) (xy 137.55 95.15)
			)
		)
	)
	(zone
		(net 33)
		(net_name "/RAMRST")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30063)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 139.417573 95.111341) (xy 139.404385 95.027002) (xy 139.409665 94.925294) (xy 139.425112 94.880846)
				(xy 139.452198 94.845011) (xy 139.490485 94.822835) (xy 139.249691 94.399049) (xy 139.04448 94.868645)
				(xy 139.099856 94.894794) (xy 139.152057 94.960908) (xy 139.201105 95.077576) (xy 139.227365 95.173151)
			)
		)
	)
	(zone
		(net 6)
		(net_name "/AD6")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30121)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 162.925 100.45) (xy 162.950352 100.449499) (xy 163.068637 100.455524) (xy 163.121699 100.476166)
				(xy 163.154015 100.518339) (xy 163.701 100.35) (xy 163.154015 100.181661) (xy 163.121972 100.223649)
				(xy 163.059213 100.246245) (xy 162.950353 100.250501) (xy 162.925 100.25)
			)
		)
	)
	(zone
		(net 34)
		(net_name "/BUS_A9")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30140)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 133.945175 95.100936) (xy 133.927108 95.101453) (xy 133.8329 95.095403) (xy 133.789527 95.074467)
				(xy 133.760985 95.031661) (xy 133.214026 95.200222) (xy 133.760985 95.368339) (xy 133.793216 95.325748)
				(xy 133.856574 95.301908) (xy 133.966736 95.295793) (xy 133.989679 95.29592)
			)
		)
	)
	(zone
		(net 20)
		(net_name "+BATT")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30000)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 167.63345 105.5) (xy 167.886221 105.520569) (xy 168.039089 105.548472) (xy 168.198427 105.588792)
				(xy 168.343376 105.636398) (xy 168.484575 105.694943) (xy 168.59923 105.754033) (xy 168.705287 105.821636)
				(xy 168.78712 105.886368) (xy 168.859006 105.957634) (xy 168.883437 105.98655) (xy 170.321 105.3)
				(xy 168.883437 104.61345) (xy 168.761779 104.735178) (xy 168.593441 104.849256) (xy 168.374782 104.951723)
				(xy 168.110147 105.034997) (xy 167.823898 105.087737) (xy 167.63345 105.1)
			)
		)
	)
	(zone
		(net 7)
		(net_name "/AD4")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30100)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 144.95 104.945196) (xy 144.954668 104.865664) (xy 144.967342 104.805069) (xy 145.015561 104.702813)
				(xy 145.058285 104.621184) (xy 145.095196 104.498773) (xy 144.85 104.449) (xy 144.604804 104.498773)
				(xy 144.648094 104.635415) (xy 144.684439 104.702813) (xy 144.730353 104.797709) (xy 144.744681 104.860872)
				(xy 144.75 104.945196)
			)
		)
	)
	(zone
		(net 25)
		(net_name "/(A)")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30005)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 162.831304 106.62414) (xy 162.935116 106.734959) (xy 163.013387 106.833991) (xy 163.064394 106.914414)
				(xy 163.101367 106.990935) (xy 163.144257 107.1428) (xy 163.166719 107.345541) (xy 163.184692 107.534106)
				(xy 163.221935 107.769366) (xy 163.97 107.621414) (xy 164.117952 106.873349) (xy 163.819433 106.829201)
				(xy 163.694127 106.818133) (xy 163.509976 106.798775) (xy 163.426748 106.781718) (xy 163.345205 106.755077)
				(xy 163.26219 106.715355) (xy 163.174544 106.659054) (xy 163.079109 106.582674) (xy 162.972726 106.482718)
			)
		)
	)
	(zone
		(net 7)
		(net_name "/AD4")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30043)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 144.75 104.85) (xy 144.743116 104.947519) (xy 144.714925 105.061161) (xy 144.688731 105.112881)
				(xy 144.652577 105.153702) (xy 144.609515 105.177165) (xy 144.85 105.601) (xy 145.090485 105.177165)
				(xy 145.032121 105.139485) (xy 144.987323 105.066762) (xy 144.957717 104.95329) (xy 144.95 104.85)
			)
		)
	)
	(zone
		(net 69)
		(net_name "/A13")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30109)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 157.193803 97.293508) (xy 157.336547 97.246056) (xy 157.525587 97.227168) (xy 157.761684 97.245798)
				(xy 157.9097 97.275) (xy 157.900866 97.099501) (xy 157.300922 97.007862) (xy 157.282967 97.041852)
				(xy 157.221555 97.075654) (xy 157.155829 97.098107) (xy 157.093809 97.120301)
			)
		)
	)
	(zone
		(net 74)
		(net_name "/A15")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30132)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 157.215603 98.583927) (xy 157.340873 98.538194) (xy 157.508735 98.520762) (xy 157.731479 98.539237)
				(xy 157.909027 98.575) (xy 157.900725 98.399312) (xy 157.300168 98.311651) (xy 157.282341 98.344335)
				(xy 157.216848 98.382636) (xy 157.147542 98.410028) (xy 157.077976 98.438812)
			)
		)
	)
	(zone
		(net 57)
		(net_name "/A7")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30035)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 136.95 95.15) (xy 136.956884 95.052484) (xy 136.985074 94.938844) (xy 137.011267 94.887123)
				(xy 137.047421 94.8463) (xy 137.090485 94.822835) (xy 136.85 94.399) (xy 136.609515 94.822835) (xy 136.66788 94.860515)
				(xy 136.712677 94.933239) (xy 136.742283 95.04671) (xy 136.75 95.15)
			)
		)
	)
	(zone
		(net 2)
		(net_name "/AD1")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30101)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 160.945196 97.65) (xy 160.865664 97.645332) (xy 160.805069 97.632658) (xy 160.702813 97.584439)
				(xy 160.621184 97.541714) (xy 160.498773 97.504804) (xy 160.449 97.75) (xy 160.498773 97.995196)
				(xy 160.635415 97.951905) (xy 160.702813 97.915561) (xy 160.797709 97.869647) (xy 160.860872 97.855319)
				(xy 160.945196 97.85)
			)
		)
	)
	(zone
		(net 25)
		(net_name "/(A)")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30060)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 133.654804 97.95) (xy 133.758667 97.954661) (xy 133.832958 97.967289) (xy 133.914687 97.993006)
				(xy 133.991788 98.018504) (xy 134.101227 98.045196) (xy 134.151 97.8) (xy 134.101227 97.554804)
				(xy 133.926279 97.602912) (xy 133.914686 97.606994) (xy 133.810461 97.637679) (xy 133.654804 97.65)
			)
		)
	)
	(zone
		(net 13)
		(net_name "VMEM")
		(layer "B.Cu")
		(name "$teardrop_track$")
		(hatch none 0.1)
		(priority 30017)
		(attr
			(teardrop
				(type track_end)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 143 98.604764) (xy 143.000271 98.69872) (xy 142.995392 98.901418) (xy 142.955764 99.140473)
				(xy 143.25 99.2) (xy 143.544236 99.140473) (xy 143.504608 98.90142) (xy 143.499729 98.698727) (xy 143.5 98.604764)
			)
		)
	)
	(zone
		(net 13)
		(net_name "VMEM")
		(layer "B.Cu")
		(name "$teardrop_track$")
		(hatch none 0.1)
		(priority 30018)
		(attr
			(teardrop
				(type track_end)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 144.3 101.394236) (xy 144.299729 101.300273) (xy 144.304608 101.09758) (xy 144.344236 100.858527)
				(xy 144.05 100.799) (xy 143.755764 100.858527) (xy 143.795392 101.097582) (xy 143.800271 101.30028)
				(xy 143.8 101.394236)
			)
		)
	)
	(zone
		(net 49)
		(net_name "/BLOCK")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30075)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 128.19 97.65) (xy 128.123421 97.659122) (xy 128.010446 97.671255) (xy 127.961547 97.659408)
				(xy 127.9275 97.625) (xy 127.414 97.8) (xy 127.9275 97.975) (xy 127.965564 97.938668) (xy 128.029144 97.928441)
				(xy 128.123421 97.940878) (xy 128.19 97.95)
			)
		)
	)
	(zone
		(net 30)
		(net_name "/BUS_A11")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30057)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 163.245196 95) (xy 163.141334 94.995339) (xy 163.067044 94.982711) (xy 162.985313 94.956994)
				(xy 162.908213 94.931495) (xy 162.798773 94.904804) (xy 162.749 95.15) (xy 162.798773 95.395196)
				(xy 162.973722 95.347087) (xy 162.985312 95.343007) (xy 163.089538 95.312321) (xy 163.245196 95.3)
			)
		)
	)
	(zone
		(net 49)
		(net_name "/BLOCK")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30076)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 128.19 104) (xy 128.123421 104.009122) (xy 128.010446 104.021255) (xy 127.961547 104.009408)
				(xy 127.9275 103.975) (xy 127.414 104.15) (xy 127.9275 104.325) (xy 127.965564 104.288668) (xy 128.029144 104.278441)
				(xy 128.123421 104.290878) (xy 128.19 104.3)
			)
		)
	)
	(zone
		(net 55)
		(net_name "/A8")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30096)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 128.504804 103.6) (xy 128.584336 103.604668) (xy 128.644931 103.617342) (xy 128.747187 103.665561)
				(xy 128.828815 103.708285) (xy 128.951227 103.745196) (xy 129.001 103.5) (xy 128.951227 103.254804)
				(xy 128.814585 103.298094) (xy 128.747186 103.334439) (xy 128.65229 103.380353) (xy 128.589128 103.394681)
				(xy 128.504804 103.4)
			)
		)
	)
	(zone
		(net 67)
		(net_name "/A10")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30122)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 157.125 95.25) (xy 157.150352 95.249499) (xy 157.268637 95.255524) (xy 157.321699 95.276166)
				(xy 157.354015 95.318339) (xy 157.901 95.15) (xy 157.354015 94.981661) (xy 157.321972 95.023649)
				(xy 157.259213 95.046245) (xy 157.150353 95.050501) (xy 157.125 95.05)
			)
		)
	)
	(zone
		(net 60)
		(net_name "/A4")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30044)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 147.95 104.85) (xy 147.943116 104.947519) (xy 147.914925 105.061161) (xy 147.888731 105.112881)
				(xy 147.852577 105.153702) (xy 147.809515 105.177165) (xy 148.05 105.601) (xy 148.290485 105.177165)
				(xy 148.232121 105.139485) (xy 148.187323 105.066762) (xy 148.157717 104.95329) (xy 148.15 104.85)
			)
		)
	)
	(zone
		(net 6)
		(net_name "/AD6")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30136)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 160.289586 101.818245) (xy 160.246141 101.852977) (xy 160.207372 101.870603) (xy 160.142896 101.87008)
				(xy 160.077765 101.846655) (xy 159.948773 101.804804) (xy 159.899277 102.05069) (xy 160.038893 102.257867)
				(xy 160.147775 102.186456) (xy 160.275705 102.098343) (xy 160.427639 101.962955)
			)
		)
	)
	(zone
		(net 9)
		(net_name "/AD0")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30123)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 162.925 98.5) (xy 162.950352 98.499499) (xy 163.068637 98.505524) (xy 163.121699 98.526166)
				(xy 163.154015 98.568339) (xy 163.701 98.4) (xy 163.154015 98.231661) (xy 163.121972 98.273649)
				(xy 163.059213 98.296245) (xy 162.950353 98.300501) (xy 162.925 98.3)
			)
		)
	)
	(zone
		(net 66)
		(net_name "/A16")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30045)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 149.55 104.85) (xy 149.543116 104.947519) (xy 149.514925 105.061161) (xy 149.488731 105.112881)
				(xy 149.452577 105.153702) (xy 149.409515 105.177165) (xy 149.65 105.601) (xy 149.890485 105.177165)
				(xy 149.832121 105.139485) (xy 149.787323 105.066762) (xy 149.757717 104.95329) (xy 149.75 104.85)
			)
		)
	)
	(zone
		(net 58)
		(net_name "/A0")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30061)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 127.854804 105.6) (xy 127.958667 105.604661) (xy 128.032958 105.617289) (xy 128.114687 105.643006)
				(xy 128.191788 105.668504) (xy 128.301227 105.695196) (xy 128.351 105.45) (xy 128.301227 105.204804)
				(xy 128.126279 105.252912) (xy 128.114686 105.256994) (xy 128.010461 105.287679) (xy 127.854804 105.3)
			)
		)
	)
	(zone
		(net 54)
		(net_name "/~{Y0}")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30135)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 159.449147 98.91072) (xy 159.397749 98.945459) (xy 159.353591 98.962507) (xy 159.282841 98.960577)
				(xy 159.22237 98.941093) (xy 159.098773 98.904804) (xy 159.049219 99.150623) (xy 159.188893 99.357867)
				(xy 159.349115 99.246617) (xy 159.462358 99.157105) (xy 159.573844 99.067084)
			)
		)
	)
	(zone
		(net 36)
		(net_name "/BYTE")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30113)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 128.19 104.7) (xy 128.164647 104.700501) (xy 128.046363 104.694476) (xy 127.993301 104.673834)
				(xy 127.960985 104.631661) (xy 127.414 104.8) (xy 127.960985 104.968339) (xy 127.993029 104.926351)
				(xy 128.055788 104.903755) (xy 128.164648 104.899499) (xy 128.19 104.9)
			)
		)
	)
	(zone
		(net 6)
		(net_name "/AD6")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30102)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 145.75 105.245196) (xy 145.754668 105.165664) (xy 145.767342 105.105069) (xy 145.815561 105.002813)
				(xy 145.858285 104.921184) (xy 145.895196 104.798773) (xy 145.65 104.749) (xy 145.404804 104.798773)
				(xy 145.448094 104.935415) (xy 145.484439 105.002813) (xy 145.530353 105.097709) (xy 145.544681 105.160872)
				(xy 145.55 105.245196)
			)
		)
	)
	(zone
		(net 25)
		(net_name "/(A)")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30086)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 156.770867 102.529446) (xy 156.71793 102.469908) (xy 156.684045 102.418098) (xy 156.645835 102.311696)
				(xy 156.618326 102.223765) (xy 156.557867 102.111107) (xy 156.349293 102.249293) (xy 156.211107 102.457867)
				(xy 156.338338 102.523876) (xy 156.411696 102.545835) (xy 156.511264 102.580471) (xy 156.566059 102.615002)
				(xy 156.629446 102.670867)
			)
		)
	)
	(zone
		(net 13)
		(net_name "VMEM")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30028)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 160.455764 103.65) (xy 160.538989 103.654708) (xy 160.604514 103.667662) (xy 160.70331 103.712022)
				(xy 160.743409 103.738048) (xy 160.841663 103.7962) (xy 160.907406 103.822452) (xy 160.991473 103.844236)
				(xy 161.051 103.55) (xy 160.991473 103.255764) (xy 160.910601 103.276507) (xy 160.846727 103.301418)
				(xy 160.743409 103.361952) (xy 160.690883 103.395383) (xy 160.631776 103.423464) (xy 160.556574 103.4428)
				(xy 160.455764 103.45)
			)
		)
	)
	(zone
		(net 58)
		(net_name "/A0")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30090)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 138.35 100.004804) (xy 138.345332 100.084336) (xy 138.332658 100.144931) (xy 138.284439 100.247186)
				(xy 138.241714 100.328815) (xy 138.204804 100.451227) (xy 138.45 100.501) (xy 138.695196 100.451227)
				(xy 138.651905 100.314584) (xy 138.615561 100.247187) (xy 138.569647 100.152291) (xy 138.555319 100.089128)
				(xy 138.55 100.004804)
			)
		)
	)
	(zone
		(net 67)
		(net_name "/A10")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30032)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 152.510875 94.969454) (xy 152.423116 94.853445) (xy 152.381364 94.772913) (xy 152.346082 94.682395)
				(xy 152.319704 94.586225) (xy 152.303104 94.484201) (xy 152.3 94.330229) (xy 152.049293 94.399293)
				(xy 152.061848 94.9) (xy 152.122649 94.907245) (xy 152.205084 94.955022) (xy 152.34197 95.082682)
				(xy 152.369454 95.110875)
			)
		)
	)
	(zone
		(net 27)
		(net_name "/~{WR}")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30069)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 148.116373 93.61252) (xy 148.092977 93.656947) (xy 148.001085 93.816692) (xy 147.946273 93.880143)
				(xy 147.917957 93.899365) (xy 147.88953 93.907055) (xy 148.049293 94.400707) (xy 148.3 94.025) (xy 148.268314 94.002585)
				(xy 148.245932 93.975667) (xy 148.223895 93.908229) (xy 148.231531 93.822339) (xy 148.257794 93.753941)
			)
		)
	)
	(zone
		(net 36)
		(net_name "/BYTE")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30103)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 135.995196 103.45) (xy 135.915664 103.445332) (xy 135.855069 103.432658) (xy 135.752813 103.384439)
				(xy 135.671184 103.341714) (xy 135.548773 103.304804) (xy 135.499 103.55) (xy 135.548773 103.795196)
				(xy 135.685415 103.751905) (xy 135.752813 103.715561) (xy 135.847709 103.669647) (xy 135.910872 103.655319)
				(xy 135.995196 103.65)
			)
		)
	)
	(zone
		(net 10)
		(net_name "VBUS")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30077)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 157.125 94.65) (xy 157.191579 94.640878) (xy 157.304554 94.628745) (xy 157.353453 94.640592)
				(xy 157.3875 94.675) (xy 157.901 94.5) (xy 157.3875 94.325) (xy 157.349436 94.361332) (xy 157.285856 94.371559)
				(xy 157.191579 94.359122) (xy 157.125 94.35)
			)
		)
	)
	(zone
		(net 3)
		(net_name "/AD3")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30104)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 162.795196 97) (xy 162.715664 96.995332) (xy 162.655069 96.982658) (xy 162.552813 96.934439)
				(xy 162.471184 96.891714) (xy 162.348773 96.854804) (xy 162.299 97.1) (xy 162.348773 97.345196)
				(xy 162.485415 97.301905) (xy 162.552813 97.265561) (xy 162.647709 97.219647) (xy 162.710872 97.205319)
				(xy 162.795196 97.2)
			)
		)
	)
	(zone
		(net 60)
		(net_name "/A4")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30080)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 147.605194 102.874173) (xy 147.560417 102.794423) (xy 147.533134 102.729153) (xy 147.509649 102.644949)
				(xy 147.479718 102.543947) (xy 147.407867 102.411107) (xy 147.199468 102.549154) (xy 147.061107 102.757867)
				(xy 147.177285 102.816907) (xy 147.240032 102.836008) (xy 147.291138 102.851487) (xy 147.338947 102.874561)
				(xy 147.386254 102.914503) (xy 147.435853 102.980582)
			)
		)
	)
	(zone
		(net 57)
		(net_name "/A7")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30091)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 136.75 98.904804) (xy 136.745332 98.984336) (xy 136.732658 99.044931) (xy 136.684439 99.147186)
				(xy 136.641714 99.228815) (xy 136.604804 99.351227) (xy 136.85 99.401) (xy 137.095196 99.351227)
				(xy 137.051905 99.214584) (xy 137.015561 99.147187) (xy 136.969647 99.052291) (xy 136.955319 98.989128)
				(xy 136.95 98.904804)
			)
		)
	)
	(zone
		(net 33)
		(net_name "/RAMRST")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30016)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 160.55 105.45) (xy 160.444329 105.430052) (xy 160.380284 105.402636) (xy 160.31854 105.363612)
				(xy 160.272115 105.321495) (xy 160.234649 105.27111) (xy 160.212917 105.2235) (xy 160.201374 105.170337)
				(xy 160.2 105.143644) (xy 159.549 105.399999) (xy 160.156788 105.744671) (xy 160.184213 105.705472)
				(xy 160.254248 105.674477) (xy 160.388296 105.654185) (xy 160.542115 105.649997) (xy 160.55 105.65)
			)
		)
	)
	(zone
		(net 4)
		(net_name "/AD5")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30036)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 144.95 95.15) (xy 144.956884 95.052484) (xy 144.985074 94.938844) (xy 145.011267 94.887123)
				(xy 145.047421 94.8463) (xy 145.090485 94.822835) (xy 144.85 94.399) (xy 144.609515 94.822835) (xy 144.66788 94.860515)
				(xy 144.712677 94.933239) (xy 144.742283 95.04671) (xy 144.75 95.15)
			)
		)
	)
	(zone
		(net 13)
		(net_name "VMEM")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30015)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 160.55 103.45) (xy 160.431879 103.429651) (xy 160.361674 103.402299) (xy 160.29498 103.363078)
				(xy 160.249475 103.323557) (xy 160.214031 103.27631) (xy 160.195266 103.232898) (xy 160.186919 103.184381)
				(xy 160.186792 103.181422) (xy 159.549 103.500001) (xy 160.156788 103.844673) (xy 160.18469 103.780521)
				(xy 160.24975 103.72518) (xy 160.360061 103.679027) (xy 160.50774 103.651874) (xy 160.55 103.65)
			)
		)
	)
	(zone
		(net 9)
		(net_name "/AD0")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30046)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 141.55 104.85) (xy 141.543116 104.947519) (xy 141.514925 105.061161) (xy 141.488731 105.112881)
				(xy 141.452577 105.153702) (xy 141.409515 105.177165) (xy 141.65 105.601) (xy 141.890485 105.177165)
				(xy 141.832121 105.139485) (xy 141.787323 105.066762) (xy 141.757717 104.95329) (xy 141.75 104.85)
			)
		)
	)
	(zone
		(net 56)
		(net_name "/A9")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30092)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 135.95 99.404804) (xy 135.945332 99.484336) (xy 135.932658 99.544931) (xy 135.884439 99.647186)
				(xy 135.841714 99.728815) (xy 135.804804 99.851227) (xy 136.05 99.901) (xy 136.295196 99.851227)
				(xy 136.251905 99.714584) (xy 136.215561 99.647187) (xy 136.169647 99.552291) (xy 136.155319 99.489128)
				(xy 136.15 99.404804)
			)
		)
	)
	(zone
		(net 57)
		(net_name "/A7")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30137)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 128.589853 102.932046) (xy 128.819503 102.888579) (xy 129.048773 102.845196) (xy 129.00098 102.599805)
				(xy 128.792133 102.461107) (xy 128.726232 102.587434) (xy 128.702171 102.63933) (xy 128.672003 102.681104)
				(xy 128.625096 102.713158) (xy 128.550819 102.735893)
			)
		)
	)
	(zone
		(net 72)
		(net_name "/A11")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30145)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 157.125 95.95) (xy 157.185584 95.945336) (xy 157.30154 95.939552) (xy 157.352258 95.949324)
				(xy 157.3875 95.975) (xy 157.901 95.8) (xy 157.31789 95.662208) (xy 157.310491 95.690321) (xy 157.295497 95.711712)
				(xy 157.244248 95.739619) (xy 157.159783 95.749978) (xy 157.134213 95.750037) (xy 157.125 95.75)
			)
		)
	)
	(zone
		(net 61)
		(net_name "/A1")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30055)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 134.71199 105.150734) (xy 134.803336 105.213654) (xy 134.896245 105.327442) (xy 134.935748 105.399977)
				(xy 134.967395 105.480374) (xy 134.988339 105.562084) (xy 134.999034 105.648298) (xy 135 105.695763)
				(xy 135.250723 105.60069) (xy 135.136679 105.1) (xy 135.089454 105.108959) (xy 135.00807 105.085669)
				(xy 134.904893 105.034274) (xy 134.850008 105.005991)
			)
		)
	)
	(zone
		(net 69)
		(net_name "/A13")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30053)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 149.832537 95.124276) (xy 149.818975 95.017248) (xy 149.827071 94.890068) (xy 149.844039 94.838986)
				(xy 149.872288 94.796945) (xy 149.9 94.775) (xy 149.649793 94.399022) (xy 149.452229 94.873823)
				(xy 149.511573 94.898616) (xy 149.564847 94.96103) (xy 149.61203 95.068896) (xy 149.636908 95.165858)
			)
		)
	)
	(zone
		(net 6)
		(net_name "/AD6")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30047)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 145.55 104.85) (xy 145.543116 104.947519) (xy 145.514925 105.061161) (xy 145.488731 105.112881)
				(xy 145.452577 105.153702) (xy 145.409515 105.177165) (xy 145.65 105.601) (xy 145.890485 105.177165)
				(xy 145.832121 105.139485) (xy 145.787323 105.066762) (xy 145.757717 104.95329) (xy 145.75 104.85)
			)
		)
	)
	(zone
		(net 13)
		(net_name "VMEM")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30022)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 160.922066 103.932378) (xy 160.983813 104.00475) (xy 161.053064 104.084654) (xy 161.115998 104.172804)
				(xy 161.154385 104.26414) (xy 161.158679 104.309424) (xy 161.15 104.353607) (xy 161.550382 104.350923)
				(xy 161.683572 104.05) (xy 161.572381 104.03404) (xy 161.474432 103.984075) (xy 161.383273 103.899298)
				(xy 161.312472 103.807809) (xy 161.291622 103.779318)
			)
		)
	)
	(zone
		(net 5)
		(net_name "/AD7")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30124)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 162.925 95.9) (xy 162.950352 95.899499) (xy 163.068637 95.905524) (xy 163.121699 95.926166)
				(xy 163.154015 95.968339) (xy 163.701 95.8) (xy 163.154015 95.631661) (xy 163.121972 95.673649)
				(xy 163.059213 95.696245) (xy 162.950353 95.700501) (xy 162.925 95.7)
			)
		)
	)
	(zone
		(net 54)
		(net_name "/~{Y0}")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30002)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 161.35 93.877376) (xy 161.354887 93.755066) (xy 161.369094 93.65122) (xy 161.390139 93.56866)
				(xy 161.418145 93.497634) (xy 161.493709 93.380421) (xy 161.608534 93.268232) (xy 161.674717 93.213522)
				(xy 161.861183 93.049789) (xy 161.961036 92.940777) (xy 162.062873 92.804052) (xy 161.429293 92.379707)
				(xy 160.681935 92.529366) (xy 160.714023 92.66651) (xy 160.750679 92.784084) (xy 160.839438 92.985045)
				(xy 160.938163 93.150522) (xy 161.018746 93.284019) (xy 161.086289 93.433656) (xy 161.132728 93.62344)
				(xy 161.15 93.877376)
			)
		)
	)
	(zone
		(net 64)
		(net_name "/A5")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30134)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 133.954339 101.45152) (xy 133.936445 101.452003) (xy 133.836634 101.445831) (xy 133.790677 101.424741)
				(xy 133.760985 101.381661) (xy 133.214035 101.550258) (xy 133.760985 101.718339) (xy 133.79295 101.676844)
				(xy 133.85821 101.652232) (xy 133.982725 101.64466) (xy 134.006093 101.644706)
			)
		)
	)
	(zone
		(net 66)
		(net_name "/A16")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30144)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 157.146968 99.197712) (xy 157.166532 99.193396) (xy 157.286897 99.176388) (xy 157.345583 99.187333)
				(xy 157.369377 99.202181) (xy 157.3875 99.225) (xy 157.900965 99.049741) (xy 157.317488 98.91281)
				(xy 157.295159 98.951464) (xy 157.235576 98.979601) (xy 157.137409 98.997927) (xy 157.095082 99.00456)
			)
		)
	)
	(zone
		(net 36)
		(net_name "/BYTE")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30065)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 138.344052 104.916053) (xy 138.340114 104.989448) (xy 138.317116 105.073973) (xy 138.291935 105.117843)
				(xy 138.255634 105.153923) (xy 138.209515 105.177165) (xy 138.450156 105.600987) (xy 138.690485 105.177165)
				(xy 138.627361 105.138086) (xy 138.579853 105.066279) (xy 138.549136 104.959297) (xy 138.541588 104.884767)
			)
		)
	)
	(zone
		(net 10)
		(net_name "VBUS")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30011)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 156.425 94.35) (xy 156.135305 94.364381) (xy 155.73733 94.383282) (xy 155.537433 94.376738)
				(xy 155.350972 94.35) (xy 155.399 94.75) (xy 156.025 95.009168) (xy 156.029803 94.951469) (xy 156.043422 94.899281)
				(xy 156.095728 94.80669) (xy 156.18074 94.729915) (xy 156.295509 94.67368) (xy 156.418882 94.65007)
				(xy 156.425 94.65)
			)
		)
	)
	(zone
		(net 68)
		(net_name "/A19")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30125)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 157.125 101.1) (xy 157.150352 101.099499) (xy 157.268637 101.105524) (xy 157.321699 101.126166)
				(xy 157.354015 101.168339) (xy 157.901 101) (xy 157.354015 100.831661) (xy 157.321972 100.873649)
				(xy 157.259213 100.896245) (xy 157.150353 100.900501) (xy 157.125 100.9)
			)
		)
	)
	(zone
		(net 3)
		(net_name "/AD3")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30037)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 142.55 95.15) (xy 142.556884 95.052484) (xy 142.585074 94.938844) (xy 142.611267 94.887123)
				(xy 142.647421 94.8463) (xy 142.690485 94.822835) (xy 142.45 94.399) (xy 142.209515 94.822835) (xy 142.26788 94.860515)
				(xy 142.312677 94.933239) (xy 142.342283 95.04671) (xy 142.35 95.15)
			)
		)
	)
	(zone
		(net 63)
		(net_name "/A2")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30114)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 133.99 104.05) (xy 133.964647 104.050501) (xy 133.846363 104.044476) (xy 133.793301 104.023834)
				(xy 133.760985 103.981661) (xy 133.214 104.15) (xy 133.760985 104.318339) (xy 133.793029 104.276351)
				(xy 133.855788 104.253755) (xy 133.964648 104.249499) (xy 133.99 104.25)
			)
		)
	)
	(zone
		(net 58)
		(net_name "/A0")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30078)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 128.19 105.3) (xy 128.123421 105.309122) (xy 128.010446 105.321255) (xy 127.961547 105.309408)
				(xy 127.9275 105.275) (xy 127.414 105.45) (xy 127.9275 105.625) (xy 127.965564 105.588668) (xy 128.029144 105.578441)
				(xy 128.123421 105.590878) (xy 128.19 105.6)
			)
		)
	)
	(zone
		(net 62)
		(net_name "/A3")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30052)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 136.714902 104.891905) (xy 136.720607 104.962208) (xy 136.712063 105.047194) (xy 136.69481 105.098693)
				(xy 136.665352 105.142336) (xy 136.609515 105.177165) (xy 136.850382 105.600923) (xy 137.075027 105.15403)
				(xy 137.019655 105.122188) (xy 136.968635 105.049438) (xy 136.923276 104.925212) (xy 136.899677 104.815369)
			)
		)
	)
	(zone
		(net 5)
		(net_name "/AD7")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30038)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 145.75 95.15) (xy 145.756884 95.052484) (xy 145.785074 94.938844) (xy 145.811267 94.887123)
				(xy 145.847421 94.8463) (xy 145.890485 94.822835) (xy 145.65 94.399) (xy 145.409515 94.822835) (xy 145.46788 94.860515)
				(xy 145.512677 94.933239) (xy 145.542283 95.04671) (xy 145.55 95.15)
			)
		)
	)
	(zone
		(net 7)
		(net_name "/AD4")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30126)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 162.925 99.8) (xy 162.950352 99.799499) (xy 163.068637 99.805524) (xy 163.121699 99.826166)
				(xy 163.154015 99.868339) (xy 163.701 99.7) (xy 163.154015 99.531661) (xy 163.121972 99.573649)
				(xy 163.059213 99.596245) (xy 162.950353 99.600501) (xy 162.925 99.6)
			)
		)
	)
	(zone
		(net 49)
		(net_name "/BLOCK")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30058)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 157.445196 101.5) (xy 157.341334 101.495339) (xy 157.267044 101.482711) (xy 157.185313 101.456994)
				(xy 157.108213 101.431495) (xy 156.998773 101.404804) (xy 156.949 101.65) (xy 156.998773 101.895196)
				(xy 157.173722 101.847087) (xy 157.185312 101.843007) (xy 157.289538 101.812321) (xy 157.445196 101.8)
			)
		)
	)
	(zone
		(net 64)
		(net_name "/A5")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30093)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 135.15 98.904804) (xy 135.145332 98.984336) (xy 135.132658 99.044931) (xy 135.084439 99.147186)
				(xy 135.041714 99.228815) (xy 135.004804 99.351227) (xy 135.25 99.401) (xy 135.495196 99.351227)
				(xy 135.451905 99.214584) (xy 135.415561 99.147187) (xy 135.369647 99.052291) (xy 135.355319 98.989128)
				(xy 135.35 98.904804)
			)
		)
	)
	(zone
		(net 71)
		(net_name "/A18")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30048)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 151.15 104.85) (xy 151.143116 104.947519) (xy 151.114925 105.061161) (xy 151.088731 105.112881)
				(xy 151.052577 105.153702) (xy 151.009515 105.177165) (xy 151.25 105.601) (xy 151.490485 105.177165)
				(xy 151.432121 105.139485) (xy 151.387323 105.066762) (xy 151.357717 104.95329) (xy 151.35 104.85)
			)
		)
	)
	(zone
		(net 21)
		(net_name "/~{RD}")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30049)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 137.55 104.85) (xy 137.543116 104.947519) (xy 137.514925 105.061161) (xy 137.488731 105.112881)
				(xy 137.452577 105.153702) (xy 137.409515 105.177165) (xy 137.65 105.601) (xy 137.890485 105.177165)
				(xy 137.832121 105.139485) (xy 137.787323 105.066762) (xy 137.757717 104.95329) (xy 137.75 104.85)
			)
		)
	)
	(zone
		(net 33)
		(net_name "/RAMRST")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30004)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 170.461804 106.674455) (xy 170.558391 106.729193) (xy 170.635215 106.784547) (xy 170.689807 106.835928)
				(xy 170.731599 106.888774) (xy 170.783026 106.998952) (xy 170.805316 107.135043) (xy 170.807773 107.3041)
				(xy 170.810768 107.516751) (xy 170.821052 107.637583) (xy 170.841935 107.769366) (xy 171.590183 107.621161)
				(xy 171.737952 106.873349) (xy 171.502705 106.827818) (xy 171.25504 106.778352) (xy 171.057553 106.724289)
				(xy 170.845118 106.639101) (xy 170.552604 106.496257)
			)
		)
	)
	(zone
		(net 56)
		(net_name "/A9")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30141)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 128.633334 102.069425) (xy 128.694637 102.03077) (xy 128.746224 102.009779) (xy 128.833229 102.001481)
				(xy 128.865306 102.003613) (xy 128.944382 102.006786) (xy 129.048773 101.995196) (xy 129.000808 101.749413)
				(xy 128.792133 101.611107) (xy 128.770873 101.643005) (xy 128.666154 101.785508) (xy 128.515772 101.907625)
			)
		)
	)
	(zone
		(net 70)
		(net_name "/A17")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30131)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 157.14189 99.800575) (xy 157.16384 99.799942) (xy 157.273306 99.80537) (xy 157.322973 99.825922)
				(xy 157.354015 99.868339) (xy 157.900987 99.699844) (xy 157.354015 99.531661) (xy 157.322124 99.572947)
				(xy 157.25741 99.596784) (xy 157.136542 99.603213) (xy 157.110596 99.603039)
			)
		)
	)
	(zone
		(net 10)
		(net_name "VBUS")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30066)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 158.734739 94.406257) (xy 158.646579 94.402501) (xy 158.537004 94.398087) (xy 158.496837 94.384039)
				(xy 158.477778 94.355726) (xy 157.8991 94.499567) (xy 157.902322 94.675) (xy 158.110172 94.633263)
				(xy 158.311134 94.628473) (xy 158.513603 94.656204) (xy 158.604575 94.676546)
			)
		)
	)
	(zone
		(net 10)
		(net_name "VBUS")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30026)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 158.9 97.705764) (xy 158.895239 97.840957) (xy 158.881909 97.935989) (xy 158.856099 98.036303)
				(xy 158.805764 98.241473) (xy 159.1 98.301) (xy 159.394236 98.241473) (xy 159.373493 98.160601)
				(xy 159.348581 98.096727) (xy 159.288048 97.993409) (xy 159.254617 97.940883) (xy 159.226536 97.881776)
				(xy 159.2072 97.806574) (xy 159.2 97.705764)
			)
		)
	)
	(zone
		(net 61)
		(net_name "/A1")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30115)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 133.99 104.7) (xy 133.964647 104.700501) (xy 133.846363 104.694476) (xy 133.793301 104.673834)
				(xy 133.760985 104.631661) (xy 133.214 104.8) (xy 133.760985 104.968339) (xy 133.793029 104.926351)
				(xy 133.855788 104.903755) (xy 133.964648 104.899499) (xy 133.99 104.9)
			)
		)
	)
	(zone
		(net 57)
		(net_name "/A7")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30116)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 128.19 102.75) (xy 128.164647 102.750501) (xy 128.046363 102.744476) (xy 127.993301 102.723834)
				(xy 127.960985 102.681661) (xy 127.414 102.85) (xy 127.960985 103.018339) (xy 127.993029 102.976351)
				(xy 128.055788 102.953755) (xy 128.164648 102.949499) (xy 128.19 102.95)
			)
		)
	)
	(zone
		(net 34)
		(net_name "/BUS_A9")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30008)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 140.149032 93.428767) (xy 140.344252 93.33489) (xy 140.497713 93.27345) (xy 140.713171 93.217089)
				(xy 140.875931 93.191825) (xy 141.257952 93.128065) (xy 141.110183 92.380253) (xy 140.361935 92.232048)
				(xy 140.33721 92.442481) (xy 140.34316 92.687461) (xy 140.348513 92.854852) (xy 140.341283 92.929835)
				(xy 140.322521 93.000108) (xy 140.288531 93.066495) (xy 140.235616 93.129818) (xy 140.160081 93.190902)
				(xy 140.05823 93.250569)
			)
		)
	)
	(zone
		(net 54)
		(net_name "/~{Y0}")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30142)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 134.176023 96.6) (xy 134.242593 96.604808) (xy 134.291936 96.618462) (xy 134.35648 96.663309)
				(xy 134.387097 96.696271) (xy 134.437599 96.749334) (xy 134.511107 96.807867) (xy 134.651 96.6)
				(xy 134.601227 96.354804) (xy 134.560942 96.362846) (xy 134.379179 96.394221) (xy 134.176023 96.4)
			)
		)
	)
	(zone
		(net 64)
		(net_name "/A5")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30147)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 134.295065 101.528884) (xy 134.374766 101.487949) (xy 134.437481 101.464185) (xy 134.486066 101.450213)
				(xy 134.57319 101.421934) (xy 134.688893 101.357867) (xy 134.550866 101.149501) (xy 134.342133 101.011107)
				(xy 134.301495 101.101529) (xy 134.291471 101.186271) (xy 134.287952 101.232308) (xy 134.276276 101.275237)
				(xy 134.248099 101.316034) (xy 134.195073 101.355676)
			)
		)
	)
	(zone
		(net 10)
		(net_name "VBUS")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30027)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 163.22281 103.599973) (xy 163.281366 103.595556) (xy 163.356114 103.58966) (xy 163.432812 103.59483)
				(xy 163.499095 103.623619) (xy 163.524466 103.650794) (xy 163.542597 103.688582) (xy 163.850999 103.400016)
				(xy 163.542597 103.111418) (xy 163.526314 103.14661) (xy 163.504006 103.172704) (xy 163.442923 103.203286)
				(xy 163.352136 103.210043) (xy 163.286692 103.204451) (xy 163.229292 103.200027)
			)
		)
	)
	(zone
		(net 62)
		(net_name "/A3")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30117)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 133.99 103.4) (xy 133.964647 103.400501) (xy 133.846363 103.394476) (xy 133.793301 103.373834)
				(xy 133.760985 103.331661) (xy 133.214 103.5) (xy 133.760985 103.668339) (xy 133.793029 103.626351)
				(xy 133.855788 103.603755) (xy 133.964648 103.599499) (xy 133.99 103.6)
			)
		)
	)
	(zone
		(net 23)
		(net_name "/BUS_A10")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30127)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 162.925 101.099997) (xy 162.950352 101.099496) (xy 163.068637 101.105521) (xy 163.121699 101.126163)
				(xy 163.154015 101.168336) (xy 163.701 100.999997) (xy 163.154015 100.831658) (xy 163.121972 100.873646)
				(xy 163.059213 100.896242) (xy 162.950353 100.900498) (xy 162.925 100.899997)
			)
		)
	)
	(zone
		(net 2)
		(net_name "/AD1")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30031)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 141.490635 95.174748) (xy 141.536747 95.076658) (xy 141.610561 94.970707) (xy 141.654153 94.931297)
				(xy 141.702417 94.906225) (xy 141.7444 94.9) (xy 141.650499 94.399134) (xy 141.4 94.359304) (xy 141.416279 94.55552)
				(xy 141.39823 94.772793) (xy 141.345717 94.994617) (xy 141.317428 95.074754)
			)
		)
	)
	(zone
		(net 3)
		(net_name "/AD3")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30128)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 162.925 97.2) (xy 162.950352 97.199499) (xy 163.068637 97.205524) (xy 163.121699 97.226166)
				(xy 163.154015 97.268339) (xy 163.701 97.1) (xy 163.154015 96.931661) (xy 163.121972 96.973649)
				(xy 163.059213 96.996245) (xy 162.950353 97.000501) (xy 162.925 97)
			)
		)
	)
	(zone
		(net 10)
		(net_name "VBUS")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30013)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 125.35 100.4) (xy 125.360114 100.479047) (xy 125.373015 100.568875) (xy 125.370917 100.656738)
				(xy 125.358641 100.693951) (xy 125.33589 100.723494) (xy 125.300423 100.742975) (xy 125.25 100.75)
				(xy 125.65 101.151) (xy 126.05 100.75) (xy 126.007454 100.74522) (xy 125.975252 100.731763) (xy 125.938132 100.687031)
				(xy 125.925025 100.61324) (xy 125.939886 100.479047) (xy 125.95 100.4)
			)
		)
	)
	(zone
		(net 4)
		(net_name "/AD5")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30094)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 144.75 95.104804) (xy 144.745332 95.184336) (xy 144.732658 95.244931) (xy 144.684439 95.347186)
				(xy 144.641714 95.428815) (xy 144.604804 95.551227) (xy 144.85 95.601) (xy 145.095196 95.551227)
				(xy 145.051905 95.414584) (xy 145.015561 95.347187) (xy 144.969647 95.252291) (xy 144.955319 95.189128)
				(xy 144.95 95.104804)
			)
		)
	)
	(zone
		(net 56)
		(net_name "/A9")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30039)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 136.15 95.15) (xy 136.156884 95.052484) (xy 136.185074 94.938844) (xy 136.211267 94.887123)
				(xy 136.247421 94.8463) (xy 136.290485 94.822835) (xy 136.05 94.399) (xy 135.809515 94.822835) (xy 135.86788 94.860515)
				(xy 135.912677 94.933239) (xy 135.942283 95.04671) (xy 135.95 95.15)
			)
		)
	)
	(zone
		(net 10)
		(net_name "VBUS")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30014)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 125.95 95.55) (xy 125.939886 95.470953) (xy 125.926985 95.381125) (xy 125.929083 95.293262)
				(xy 125.941359 95.256049) (xy 125.96411 95.226506) (xy 125.999577 95.207025) (xy 126.05 95.2) (xy 125.65 94.799)
				(xy 125.25 95.2) (xy 125.292546 95.20478) (xy 125.324748 95.218237) (xy 125.361868 95.262969) (xy 125.374975 95.33676)
				(xy 125.360114 95.470953) (xy 125.35 95.55)
			)
		)
	)
	(zone
		(net 35)
		(net_name "/BUS_A8")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30007)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 140.056816 106.749433) (xy 140.144448 106.799593) (xy 140.21306 106.850656) (xy 140.260856 106.898368)
				(xy 140.296351 106.947608) (xy 140.336945 107.05155) (xy 140.348539 107.18333) (xy 140.342851 107.313731)
				(xy 140.336066 107.521693) (xy 140.342756 107.640083) (xy 140.361935 107.769366) (xy 141.110183 107.621161)
				(xy 141.257952 106.873349) (xy 140.877349 106.809575) (xy 140.712057 106.783682) (xy 140.55803 106.746923)
				(xy 140.381229 106.681905) (xy 140.147616 106.571235)
			)
		)
	)
	(zone
		(net 2)
		(net_name "/AD1")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30129)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 162.925 97.85) (xy 162.950352 97.849499) (xy 163.068637 97.855524) (xy 163.121699 97.876166)
				(xy 163.154015 97.918339) (xy 163.701 97.75) (xy 163.154015 97.581661) (xy 163.121972 97.623649)
				(xy 163.059213 97.646245) (xy 162.950353 97.650501) (xy 162.925 97.65)
			)
		)
	)
	(zone
		(net 74)
		(net_name "/A15")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30050)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 148.75 104.85) (xy 148.743116 104.947519) (xy 148.714925 105.061161) (xy 148.688731 105.112881)
				(xy 148.652577 105.153702) (xy 148.609515 105.177165) (xy 148.85 105.601) (xy 149.090485 105.177165)
				(xy 149.032121 105.139485) (xy 148.987323 105.066762) (xy 148.957717 104.95329) (xy 148.95 104.85)
			)
		)
	)
	(zone
		(net 10)
		(net_name "VBUS")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30079)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 126.64 94.7) (xy 126.706579 94.690878) (xy 126.819554 94.678745) (xy 126.868453 94.690592) (xy 126.9025 94.725)
				(xy 127.416 94.55) (xy 126.9025 94.375) (xy 126.864436 94.411332) (xy 126.800856 94.421559) (xy 126.706579 94.409122)
				(xy 126.64 94.4)
			)
		)
	)
	(zone
		(net 64)
		(net_name "/A5")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30040)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 135.35 95.15) (xy 135.356884 95.052484) (xy 135.385074 94.938844) (xy 135.411267 94.887123)
				(xy 135.447421 94.8463) (xy 135.490485 94.822835) (xy 135.25 94.399) (xy 135.009515 94.822835) (xy 135.06788 94.860515)
				(xy 135.112677 94.933239) (xy 135.142283 95.04671) (xy 135.15 95.15)
			)
		)
	)
	(zone
		(net 63)
		(net_name "/A2")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30068)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 135.872275 104.930098) (xy 135.888583 104.988724) (xy 135.892904 105.062289) (xy 135.883419 105.106418)
				(xy 135.860717 105.144631) (xy 135.809515 105.177165) (xy 136.050623 105.600781) (xy 136.237121 105.11906)
				(xy 136.18667 105.095977) (xy 136.129945 105.027788) (xy 136.065071 104.897848) (xy 136.036201 104.824997)
				(xy 136.02864 104.805401)
			)
		)
	)
	(zone
		(net 10)
		(net_name "VBUS")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30012)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 126.675 94.4) (xy 126.385305 94.414381) (xy 125.98733 94.433282) (xy 125.787433 94.426738) (xy 125.600972 94.4)
				(xy 125.649 94.8) (xy 126.275 95.059168) (xy 126.279803 95.001469) (xy 126.293422 94.949281) (xy 126.345728 94.85669)
				(xy 126.43074 94.779915) (xy 126.545509 94.72368) (xy 126.668882 94.70007) (xy 126.675 94.7)
			)
		)
	)
	(zone
		(net 20)
		(net_name "+BATT")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30023)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 164.55 105.1) (xy 164.47837 105.104357) (xy 164.384522 105.110306) (xy 164.288395 105.105224)
				(xy 164.207014 105.076475) (xy 164.177173 105.049275) (xy 164.157403 105.011418) (xy 163.849 105.3)
				(xy 164.157403 105.588582) (xy 164.172508 105.557152) (xy 164.19444 105.532861) (xy 164.26013 105.500743)
				(xy 164.365059 105.489424) (xy 164.47837 105.495643) (xy 164.55 105.5)
			)
		)
	)
	(zone
		(net 72)
		(net_name "/A11")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30067)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 151.462613 95.0841) (xy 151.44044 95.005435) (xy 151.431988 94.90752) (xy 151.440224 94.855794)
				(xy 151.461549 94.810388) (xy 151.5 94.775) (xy 151.2495 94.399134) (xy 151.080514 94.891151) (xy 151.134355 94.911524)
				(xy 151.191258 94.973615) (xy 151.252868 95.090668) (xy 151.287211 95.178175) (xy 151.289408 95.184099)
			)
		)
	)
	(zone
		(net 60)
		(net_name "/A4")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30143)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 137.726023 102.35) (xy 137.792593 102.354808) (xy 137.841936 102.368462) (xy 137.90648 102.413309)
				(xy 137.937097 102.446271) (xy 137.987599 102.499334) (xy 138.061107 102.557867) (xy 138.201 102.35)
				(xy 138.151227 102.104804) (xy 138.110942 102.112846) (xy 137.929179 102.144221) (xy 137.726023 102.15)
			)
		)
	)
	(zone
		(net 33)
		(net_name "/RAMRST")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30081)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 139.579133 95.720554) (xy 139.632069 95.780092) (xy 139.665954 95.831901) (xy 139.704164 95.938303)
				(xy 139.731674 96.026234) (xy 139.792133 96.138893) (xy 140.000707 96.000707) (xy 140.138893 95.792133)
				(xy 140.011662 95.726123) (xy 139.938303 95.704164) (xy 139.838735 95.669529) (xy 139.783941 95.634998)
				(xy 139.720554 95.579133)
			)
		)
	)
	(zone
		(net 55)
		(net_name "/A8")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30118)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 128.19 103.4) (xy 128.164647 103.400501) (xy 128.046363 103.394476) (xy 127.993301 103.373834)
				(xy 127.960985 103.331661) (xy 127.414 103.5) (xy 127.960985 103.668339) (xy 127.993029 103.626351)
				(xy 128.055788 103.603755) (xy 128.164648 103.599499) (xy 128.19 103.6)
			)
		)
	)
	(zone
		(net 60)
		(net_name "/A4")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30146)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 133.99 102.15) (xy 133.980787 102.150037) (xy 133.929008 102.148946) (xy 133.870549 102.13956)
				(xy 133.821289 102.113456) (xy 133.805072 102.091501) (xy 133.797109 102.062208) (xy 133.214 102.2)
				(xy 133.7275 102.375) (xy 133.768451 102.347331) (xy 133.846891 102.338968) (xy 133.929416 102.345336)
				(xy 133.99 102.35)
			)
		)
	)
	(zone
		(net 13)
		(net_name "VMEM")
		(layer "B.Cu")
		(name "$teardrop_track$")
		(hatch none 0.1)
		(priority 30019)
		(attr
			(teardrop
				(type track_end)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 144.3 101.394236) (xy 144.299729 101.300273) (xy 144.304608 101.09758) (xy 144.344236 100.858527)
				(xy 144.05 100.799) (xy 143.755764 100.858527) (xy 143.795392 101.097582) (xy 143.800271 101.30028)
				(xy 143.8 101.394236)
			)
		)
	)
	(zone
		(net 23)
		(net_name "/BUS_A10")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30095)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 158.15 103.604804) (xy 158.145332 103.684336) (xy 158.132658 103.744931) (xy 158.084439 103.847186)
				(xy 158.041714 103.928815) (xy 158.004804 104.051227) (xy 158.25 104.101) (xy 158.495196 104.051227)
				(xy 158.451905 103.914584) (xy 158.415561 103.847187) (xy 158.369647 103.752291) (xy 158.355319 103.689128)
				(xy 158.35 103.604804)
			)
		)
	)
	(zone
		(net 21)
		(net_name "/~{RD}")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30105)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 153.909293 104.895196) (xy 153.913961 104.815664) (xy 153.926635 104.755069) (xy 153.974854 104.652813)
				(xy 154.017578 104.571184) (xy 154.054489 104.448773) (xy 153.809293 104.399) (xy 153.564097 104.448773)
				(xy 153.607387 104.585415) (xy 153.643732 104.652813) (xy 153.689646 104.747709) (xy 153.703974 104.810872)
				(xy 153.709293 104.895196)
			)
		)
	)
	(zone
		(net 21)
		(net_name "/~{RD}")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30106)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 137.75 105.245196) (xy 137.754668 105.165664) (xy 137.767342 105.105069) (xy 137.815561 105.002813)
				(xy 137.858285 104.921184) (xy 137.895196 104.798773) (xy 137.65 104.749) (xy 137.404804 104.798773)
				(xy 137.448094 104.935415) (xy 137.484439 105.002813) (xy 137.530353 105.097709) (xy 137.544681 105.160872)
				(xy 137.55 105.245196)
			)
		)
	)
	(zone
		(net 36)
		(net_name "/BYTE")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30133)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 128.200368 99.003124) (xy 128.174439 99.00327) (xy 128.050085 98.99558) (xy 127.994411 98.974222)
				(xy 127.974077 98.956038) (xy 127.960985 98.931661) (xy 127.414011 99.099858) (xy 127.960985 99.268339)
				(xy 127.993374 99.224949) (xy 128.053941 99.203185) (xy 128.149891 99.200401) (xy 128.171908 99.201088)
			)
		)
	)
	(zone
		(net 8)
		(net_name "/AD2")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30051)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 142.35 104.85) (xy 142.343116 104.947519) (xy 142.314925 105.061161) (xy 142.288731 105.112881)
				(xy 142.252577 105.153702) (xy 142.209515 105.177165) (xy 142.45 105.601) (xy 142.690485 105.177165)
				(xy 142.632121 105.139485) (xy 142.587323 105.066762) (xy 142.557717 104.95329) (xy 142.55 104.85)
			)
		)
	)
	(zone
		(net 13)
		(net_name "VMEM")
		(layer "B.Cu")
		(name "$teardrop_track$")
		(hatch none 0.1)
		(priority 30020)
		(attr
			(teardrop
				(type track_end)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 143 98.604764) (xy 143.000271 98.69872) (xy 142.995392 98.901418) (xy 142.955764 99.140473)
				(xy 143.25 99.2) (xy 143.544236 99.140473) (xy 143.504608 98.90142) (xy 143.499729 98.698727) (xy 143.5 98.604764)
			)
		)
	)
	(zone
		(net 54)
		(net_name "/~{Y0}")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30119)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 133.99 96.4) (xy 133.964647 96.400501) (xy 133.846363 96.394476) (xy 133.793301 96.373834) (xy 133.760985 96.331661)
				(xy 133.214 96.5) (xy 133.760985 96.668339) (xy 133.793029 96.626351) (xy 133.855788 96.603755)
				(xy 133.964648 96.599499) (xy 133.99 96.6)
			)
		)
	)
	(zone
		(net 8)
		(net_name "/AD2")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30084)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 160.179446 100.429133) (xy 160.119908 100.482069) (xy 160.068098 100.515954) (xy 159.961697 100.554164)
				(xy 159.873765 100.581674) (xy 159.761107 100.642133) (xy 159.899293 100.850707) (xy 160.107867 100.988893)
				(xy 160.173876 100.861662) (xy 160.195835 100.788304) (xy 160.23047 100.688736) (xy 160.265002 100.633941)
				(xy 160.320867 100.570554)
			)
		)
	)
	(embedded_fonts yes)
	(embedded_files
		(file
			(name "ProggyVector.ttf")
			(type font)
		)
	)
)
