(kicad_pcb
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(general
		(thickness 1.6)
		(legacy_teardrops no)
	)
	(paper "A4")
	(layers
		(0 "F.Cu" signal)
		(2 "B.Cu" signal)
		(9 "F.Adhes" user "F.Adhesive")
		(11 "B.Adhes" user "B.Adhesive")
		(13 "F.Paste" user)
		(15 "B.Paste" user)
		(5 "F.SilkS" user "F.Silkscreen")
		(7 "B.SilkS" user "B.Silkscreen")
		(1 "F.Mask" user)
		(3 "B.Mask" user)
		(17 "Dwgs.User" user "User.Drawings")
		(19 "Cmts.User" user "User.Comments")
		(21 "Eco1.User" user "User.Eco1")
		(23 "Eco2.User" user "User.Eco2")
		(25 "Edge.Cuts" user)
		(27 "Margin" user)
		(31 "F.CrtYd" user "F.Courtyard")
		(29 "B.CrtYd" user "B.Courtyard")
		(35 "F.Fab" user)
		(33 "B.Fab" user)
		(39 "User.1" user)
		(41 "User.2" user)
		(43 "User.3" user)
		(45 "User.4" user)
	)
	(setup
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(tenting front back)
		(pcbplotparams
			(layerselection 0x00000000_00000000_55555555_5755f5ff)
			(plot_on_all_layers_selection 0x00000000_00000000_00000000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 4)
			(plotframeref no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(pdf_metadata yes)
			(pdf_single_document no)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plot_black_and_white yes)
			(sketchpadsonfab no)
			(plotpadnumbers no)
			(hidednponfab no)
			(sketchdnponfab yes)
			(crossoutdnponfab yes)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 1)
			(scaleselection 1)
			(outputdirectory "")
		)
	)
	(net 0 "")
	(net 1 "/DS1")
	(net 2 "Net-(DS1-A)")
	(net 3 "/DS2")
	(net 4 "Net-(DS2-A)")
	(net 5 "Net-(DS3-A)")
	(net 6 "/DS3")
	(net 7 "/IN_USE")
	(net 8 "/DISK_CHG")
	(net 9 "/WRITE_GATE")
	(net 10 "GND")
	(net 11 "/DS0")
	(net 12 "/+5")
	(net 13 "/READY")
	(net 14 "/DIR")
	(net 15 "/STEP")
	(net 16 "/WRITE_DATA")
	(net 17 "/WRITE_PROT")
	(net 18 "/INDEX")
	(net 19 "/TRACK_00")
	(net 20 "/DISK_CHG_RST")
	(net 21 "/READ_DATA")
	(net 22 "/MOTOR_ON")
	(net 23 "/HEAD_SEL")
	(net 24 "/4_RSRVD")
	(net 25 "unconnected-(EMU1-Pin_1-Pad1)")
	(net 26 "unconnected-(EMU1-Pin_3-Pad3)")
	(net 27 "unconnected-(EMU1-Pin_5-Pad5)")
	(net 28 "unconnected-(HP1-Pin_6-Pad6)")
	(net 29 "unconnected-(HP1-Pin_2-Pad2)")
	(net 30 "unconnected-(HP1-Pin_28-Pad28)")
	(net 31 "unconnected-(HP1-Pin_26-Pad26)")
	(net 32 "unconnected-(HP1-Pin_4-Pad4)")
	(net 33 "unconnected-(HP1-Pin_24-Pad24)")
	(net 34 "unconnected-(HP1-Pin_30-Pad30)")
	(footprint "Jumper:SolderJumper-2_P1.3mm_Open_TrianglePad1.0x1.5mm"
		(layer "F.Cu")
		(at 150.2 69.6 180)
		(descr "SMD Solder Jumper, 1x1.5mm Triangular Pads, 0.3mm gap, open")
		(tags "solder jumper open")
		(property "Reference" "DS3"
			(at 0.2 1.6 0)
			(layer "F.SilkS")
		)
		(property "Value" "~"
			(at 0 1.9 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Solder Jumper, 2-pole, open"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SolderJumper*Open*")
		(sheetname "/")
		(sheetfile "hp_floppadapter.kicad_sch")
		(zone_connect 1)
		(attr exclude_from_pos_files exclude_from_bom allow_soldermask_bridges)
		(pad "1" smd custom
			(at -0.725 0 180)
			(size 0.3 0.3)
			(layers "F.Cu" "F.Mask")
			(net 5 "Net-(DS3-A)")
			(pinfunction "A")
			(pintype "passive")
			(zone_connect 2)
			(thermal_bridge_angle 45)
			(options
				(clearance outline)
				(anchor rect)
			)
			(primitives
				(gr_poly
					(pts
						(xy 1 0) (xy 0.5 0.75) (xy -0.5 0.75) (xy -0.5 -0.75) (xy 0.5 -0.75)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "2" smd custom
			(at 0.725 0 180)
			(size 0.3 0.3)
			(layers "F.Cu" "F.Mask")
			(net 6 "/DS3")
			(pinfunction "B")
			(pintype "passive")
			(zone_connect 2)
			(thermal_bridge_angle 45)
			(options
				(clearance outline)
				(anchor rect)
			)
			(primitives
				(gr_poly
					(pts
						(xy 0.5 0.75) (xy -0.65 0.75) (xy -0.15 0) (xy -0.65 -0.75) (xy 0.5 -0.75)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(embedded_fonts no)
	)
	(footprint "Jumper:SolderJumper-2_P1.3mm_Open_TrianglePad1.0x1.5mm"
		(layer "F.Cu")
		(at 150.2 76.8)
		(descr "SMD Solder Jumper, 1x1.5mm Triangular Pads, 0.3mm gap, open")
		(tags "solder jumper open")
		(property "Reference" "DS2"
			(at 2.8 0.2 180)
			(layer "F.SilkS")
		)
		(property "Value" "~"
			(at 0 1.9 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Solder Jumper, 2-pole, open"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SolderJumper*Open*")
		(sheetname "/")
		(sheetfile "hp_floppadapter.kicad_sch")
		(zone_connect 1)
		(attr exclude_from_pos_files exclude_from_bom allow_soldermask_bridges)
		(pad "1" smd custom
			(at -0.725 0)
			(size 0.3 0.3)
			(layers "F.Cu" "F.Mask")
			(net 4 "Net-(DS2-A)")
			(pinfunction "A")
			(pintype "passive")
			(zone_connect 2)
			(thermal_bridge_angle 45)
			(options
				(clearance outline)
				(anchor rect)
			)
			(primitives
				(gr_poly
					(pts
						(xy 1 0) (xy 0.5 0.75) (xy -0.5 0.75) (xy -0.5 -0.75) (xy 0.5 -0.75)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "2" smd custom
			(at 0.725 0)
			(size 0.3 0.3)
			(layers "F.Cu" "F.Mask")
			(net 3 "/DS2")
			(pinfunction "B")
			(pintype "passive")
			(zone_connect 2)
			(thermal_bridge_angle 45)
			(options
				(clearance outline)
				(anchor rect)
			)
			(primitives
				(gr_poly
					(pts
						(xy 0.5 0.75) (xy -0.65 0.75) (xy -0.15 0) (xy -0.65 -0.75) (xy 0.5 -0.75)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(embedded_fonts no)
	)
	(footprint "Jumper:SolderJumper-2_P1.3mm_Open_TrianglePad1.0x1.5mm"
		(layer "F.Cu")
		(at 150.2 74.2)
		(descr "SMD Solder Jumper, 1x1.5mm Triangular Pads, 0.3mm gap, open")
		(tags "solder jumper open")
		(property "Reference" "DS1"
			(at -0.2 -1.8 180)
			(layer "F.SilkS")
		)
		(property "Value" "~"
			(at 0 1.9 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Solder Jumper, 2-pole, open"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SolderJumper*Open*")
		(sheetname "/")
		(sheetfile "hp_floppadapter.kicad_sch")
		(zone_connect 1)
		(attr exclude_from_pos_files exclude_from_bom allow_soldermask_bridges)
		(pad "1" smd custom
			(at -0.725 0)
			(size 0.3 0.3)
			(layers "F.Cu" "F.Mask")
			(net 2 "Net-(DS1-A)")
			(pinfunction "A")
			(pintype "passive")
			(zone_connect 2)
			(thermal_bridge_angle 45)
			(options
				(clearance outline)
				(anchor rect)
			)
			(primitives
				(gr_poly
					(pts
						(xy 1 0) (xy 0.5 0.75) (xy -0.5 0.75) (xy -0.5 -0.75) (xy 0.5 -0.75)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "2" smd custom
			(at 0.725 0)
			(size 0.3 0.3)
			(layers "F.Cu" "F.Mask")
			(net 1 "/DS1")
			(pinfunction "B")
			(pintype "passive")
			(zone_connect 2)
			(thermal_bridge_angle 45)
			(options
				(clearance outline)
				(anchor rect)
			)
			(primitives
				(gr_poly
					(pts
						(xy 0.5 0.75) (xy -0.65 0.75) (xy -0.15 0) (xy -0.65 -0.75) (xy 0.5 -0.75)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(embedded_fonts no)
	)
	(footprint "Connector_PinHeader_2.54mm:PinHeader_1x01_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 154 69.4)
		(descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x01 2.54mm single row")
		(property "Reference" "J4"
			(at 0 -2.38 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "GND"
			(at 0 2.38 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x01, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "/")
		(sheetfile "hp_floppadapter.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 10 "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Jumper:SolderJumper-2_P1.3mm_Bridged2Bar_RoundedPad1.0x1.5mm"
		(layer "F.Cu")
		(at 150.2 65)
		(descr "SMD Solder Jumper, 1x1.5mm, rounded Pads, 0.3mm gap, bridged with 2 copper strips")
		(tags "net tie solder jumper bridged")
		(property "Reference" "JP1"
			(at 0 -1.8 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "DISK_CHG_RST"
			(at 0 1.9 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Solder Jumper, 2-pole, closed/bridged"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SolderJumper*Bridged*")
		(sheetname "/")
		(sheetfile "hp_floppadapter.kicad_sch")
		(zone_connect 1)
		(attr exclude_from_pos_files exclude_from_bom allow_soldermask_bridges)
		(net_tie_pad_groups "1, 2")
		(pad "1" smd custom
			(at -0.65 0)
			(size 1 0.5)
			(layers "F.Cu" "F.Mask")
			(net 24 "/4_RSRVD")
			(pinfunction "A")
			(pintype "passive")
			(zone_connect 2)
			(thermal_bridge_angle 45)
			(options
				(clearance outline)
				(anchor rect)
			)
			(primitives
				(gr_circle
					(center 0 0.25)
					(end 0.5 0.25)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center 0 -0.25)
					(end 0.5 -0.25)
					(width 0)
					(fill yes)
				)
				(gr_poly
					(pts
						(xy 0.5 0.75) (xy 0 0.75) (xy 0 -0.75) (xy 0.5 -0.75)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "2" smd custom
			(at 0.65 0)
			(size 1 0.5)
			(layers "F.Cu" "F.Mask")
			(net 20 "/DISK_CHG_RST")
			(pinfunction "B")
			(pintype "passive")
			(zone_connect 2)
			(thermal_bridge_angle 45)
			(options
				(clearance outline)
				(anchor rect)
			)
			(primitives
				(gr_circle
					(center 0 0.25)
					(end 0.5 0.25)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center 0 -0.25)
					(end 0.5 -0.25)
					(width 0)
					(fill yes)
				)
				(gr_poly
					(pts
						(xy 0 0.75) (xy -0.5 0.75) (xy -0.5 -0.75) (xy 0 -0.75)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(embedded_fonts no)
	)
	(footprint "Connector_PinSocket_2.54mm:PinSocket_2x17_P2.54mm_Horizontal"
		(layer "F.Cu")
		(at 146.625 63.85)
		(descr "Through hole angled socket strip, 2x17, 2.54mm pitch, 8.51mm socket length, double cols (from Kicad 4.0.7), script generated")
		(tags "Through hole angled socket strip THT 2x17 2.54mm double row")
		(property "Reference" "EMU1"
			(at 3.375 -1.05 0)
			(layer "F.SilkS")
		)
		(property "Value" "GOTEK_STD"
			(at -5.65 43.41 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, double row, 02x17, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_2x??_*")
		(sheetname "/")
		(sheetfile "hp_floppadapter.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at -8.315 20.32 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 25 "unconnected-(EMU1-Pin_1-Pad1)")
			(pinfunction "Pin_1")
			(pintype "passive+no_connect")
		)
		(pad "2" thru_hole circle
			(at -2.54 0)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 8 "/DISK_CHG")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole circle
			(at 0 2.54)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 26 "unconnected-(EMU1-Pin_3-Pad3)")
			(pinfunction "Pin_3")
			(pintype "passive+no_connect")
		)
		(pad "4" thru_hole circle
			(at -2.54 2.54)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 24 "/4_RSRVD")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(pad "5" thru_hole circle
			(at 0 5.08)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 27 "unconnected-(EMU1-Pin_5-Pad5)")
			(pinfunction "Pin_5")
			(pintype "passive+no_connect")
		)
		(pad "6" thru_hole circle
			(at -2.54 5.08)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "Net-(DS3-A)")
			(pinfunction "Pin_6")
			(pintype "passive")
		)
		(pad "7" thru_hole circle
			(at 0 7.62)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 10 "GND")
			(pinfunction "Pin_7")
			(pintype "passive")
		)
		(pad "8" thru_hole circle
			(at -2.54 7.62)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 18 "/INDEX")
			(pinfunction "Pin_8")
			(pintype "passive")
		)
		(pad "9" thru_hole circle
			(at 0 10.16)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 10 "GND")
			(pinfunction "Pin_9")
			(pintype "passive")
		)
		(pad "10" thru_hole circle
			(at -2.54 10.16)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 11 "/DS0")
			(pinfunction "Pin_10")
			(pintype "passive")
		)
		(pad "11" thru_hole circle
			(at 0 12.7)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 10 "GND")
			(pinfunction "Pin_11")
			(pintype "passive")
		)
		(pad "12" thru_hole circle
			(at -2.54 12.7)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "Net-(DS1-A)")
			(pinfunction "Pin_12")
			(pintype "passive")
		)
		(pad "13" thru_hole circle
			(at 0 15.24)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 10 "GND")
			(pinfunction "Pin_13")
			(pintype "passive")
		)
		(pad "14" thru_hole circle
			(at -2.54 15.24)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "Net-(DS2-A)")
			(pinfunction "Pin_14")
			(pintype "passive")
		)
		(pad "15" thru_hole circle
			(at 0 17.78)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 10 "GND")
			(pinfunction "Pin_15")
			(pintype "passive")
		)
		(pad "16" thru_hole circle
			(at -2.54 17.78)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 22 "/MOTOR_ON")
			(pinfunction "Pin_16")
			(pintype "passive")
		)
		(pad "17" thru_hole circle
			(at 0 20.32)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 10 "GND")
			(pinfunction "Pin_17")
			(pintype "passive")
		)
		(pad "18" thru_hole circle
			(at -2.54 20.32)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 14 "/DIR")
			(pinfunction "Pin_18")
			(pintype "passive")
		)
		(pad "19" thru_hole circle
			(at 0 22.86)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 10 "GND")
			(pinfunction "Pin_19")
			(pintype "passive")
		)
		(pad "20" thru_hole circle
			(at -2.54 22.86)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 15 "/STEP")
			(pinfunction "Pin_20")
			(pintype "passive")
		)
		(pad "21" thru_hole circle
			(at 0 25.4)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 10 "GND")
			(pinfunction "Pin_21")
			(pintype "passive")
		)
		(pad "22" thru_hole circle
			(at -2.54 25.4)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 16 "/WRITE_DATA")
			(pinfunction "Pin_22")
			(pintype "passive")
		)
		(pad "23" thru_hole circle
			(at 0 27.94)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 10 "GND")
			(pinfunction "Pin_23")
			(pintype "passive")
		)
		(pad "24" thru_hole circle
			(at -2.54 27.94)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 9 "/WRITE_GATE")
			(pinfunction "Pin_24")
			(pintype "passive")
		)
		(pad "25" thru_hole circle
			(at 0 30.48)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 10 "GND")
			(pinfunction "Pin_25")
			(pintype "passive")
		)
		(pad "26" thru_hole circle
			(at -2.54 30.48)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 19 "/TRACK_00")
			(pinfunction "Pin_26")
			(pintype "passive")
		)
		(pad "27" thru_hole circle
			(at 0 33.02)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 10 "GND")
			(pinfunction "Pin_27")
			(pintype "passive")
		)
		(pad "28" thru_hole circle
			(at -2.54 33.02)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 17 "/WRITE_PROT")
			(pinfunction "Pin_28")
			(pintype "passive")
		)
		(pad "29" thru_hole circle
			(at 0 35.56)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 10 "GND")
			(pinfunction "Pin_29")
			(pintype "passive")
		)
		(pad "30" thru_hole circle
			(at -2.54 35.56)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 21 "/READ_DATA")
			(pinfunction "Pin_30")
			(pintype "passive")
		)
		(pad "31" thru_hole circle
			(at 0 38.1)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 10 "GND")
			(pinfunction "Pin_31")
			(pintype "passive")
		)
		(pad "32" thru_hole circle
			(at -2.54 38.1)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 23 "/HEAD_SEL")
			(pinfunction "Pin_32")
			(pintype "passive")
		)
		(pad "33" thru_hole circle
			(at 0 40.64)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 10 "GND")
			(pinfunction "Pin_33")
			(pintype "passive")
		)
		(pad "34" thru_hole circle
			(at -2.54 40.64)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 13 "/READY")
			(pinfunction "Pin_34")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_2x17_P2.54mm_Horizontal.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_PinHeader_2.54mm:PinHeader_1x01_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 154 73.4)
		(descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x01 2.54mm single row")
		(property "Reference" "J3"
			(at 2.5 -1 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "+5"
			(at 0 2.38 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x01, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "/")
		(sheetfile "hp_floppadapter.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 12 "/+5")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_PinHeader_2.54mm:PinHeader_1x01_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 154 65.6 -90)
		(descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x01 2.54mm single row")
		(property "Reference" "J5"
			(at 0 -2.38 270)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "DISK_CHG_RST"
			(at 0 2.38 270)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x01, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "/")
		(sheetfile "hp_floppadapter.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 20 "/DISK_CHG_RST")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_IDC:IDC-Header_2x17_P2.54mm_Horizontal"
		(layer "B.Cu")
		(at 151.2 120.52)
		(descr "Through hole IDC box header, 2x17, 2.54mm pitch, DIN 41651 / IEC 60603-13, double rows, https://docs.google.com/spreadsheets/d/16SsEcesNF15N3Lb4niX7dcUr-NY5_MFPQhobNuNppn4/edit#gid=0")
		(tags "Through hole horizontal IDC box header THT 2x17 2.54mm double row")
		(property "Reference" "HP1"
			(at -4.6 -0.52 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "HP_SHROUD"
			(at 6.215 -46.74 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, double row, 02x17, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_2x??_*")
		(sheetname "/")
		(sheetfile "hp_floppadapter.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 8.83 -20.32 90)
			(layer "B.Fab")
		)
		(pad "1" thru_hole roundrect
			(at 0 0)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.147059)
			(net 13 "/READY")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 2.54 0)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 29 "unconnected-(HP1-Pin_2-Pad2)")
			(pinfunction "Pin_2")
			(pintype "passive+no_connect")
		)
		(pad "3" thru_hole circle
			(at 0 -2.54)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 23 "/HEAD_SEL")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole circle
			(at 2.54 -2.54)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 32 "unconnected-(HP1-Pin_4-Pad4)")
			(pinfunction "Pin_4")
			(pintype "passive+no_connect")
		)
		(pad "5" thru_hole circle
			(at 0 -5.08)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 21 "/READ_DATA")
			(pinfunction "Pin_5")
			(pintype "passive")
		)
		(pad "6" thru_hole circle
			(at 2.54 -5.08)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 28 "unconnected-(HP1-Pin_6-Pad6)")
			(pinfunction "Pin_6")
			(pintype "passive+no_connect")
		)
		(pad "7" thru_hole circle
			(at 0 -7.62)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 17 "/WRITE_PROT")
			(pinfunction "Pin_7")
			(pintype "passive")
		)
		(pad "8" thru_hole circle
			(at 2.54 -7.62)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 10 "GND")
			(pinfunction "Pin_8")
			(pintype "passive")
		)
		(pad "9" thru_hole circle
			(at 0 -10.16)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 19 "/TRACK_00")
			(pinfunction "Pin_9")
			(pintype "passive")
		)
		(pad "10" thru_hole circle
			(at 2.54 -10.16)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 10 "GND")
			(pinfunction "Pin_10")
			(pintype "passive")
		)
		(pad "11" thru_hole circle
			(at 0 -12.7)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 9 "/WRITE_GATE")
			(pinfunction "Pin_11")
			(pintype "passive")
		)
		(pad "12" thru_hole circle
			(at 2.54 -12.7)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 10 "GND")
			(pinfunction "Pin_12")
			(pintype "passive")
		)
		(pad "13" thru_hole circle
			(at 0 -15.24)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 16 "/WRITE_DATA")
			(pinfunction "Pin_13")
			(pintype "passive")
		)
		(pad "14" thru_hole circle
			(at 2.54 -15.24)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 10 "GND")
			(pinfunction "Pin_14")
			(pintype "passive")
		)
		(pad "15" thru_hole circle
			(at 0 -17.78)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 15 "/STEP")
			(pinfunction "Pin_15")
			(pintype "passive")
		)
		(pad "16" thru_hole circle
			(at 2.54 -17.78)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 10 "GND")
			(pinfunction "Pin_16")
			(pintype "passive")
		)
		(pad "17" thru_hole circle
			(at 0 -20.32)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 14 "/DIR")
			(pinfunction "Pin_17")
			(pintype "passive")
		)
		(pad "18" thru_hole circle
			(at 2.54 -20.32)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 10 "GND")
			(pinfunction "Pin_18")
			(pintype "passive")
		)
		(pad "19" thru_hole circle
			(at 0 -22.86)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 22 "/MOTOR_ON")
			(pinfunction "Pin_19")
			(pintype "passive")
		)
		(pad "20" thru_hole circle
			(at 2.54 -22.86)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 10 "GND")
			(pinfunction "Pin_20")
			(pintype "passive")
		)
		(pad "21" thru_hole circle
			(at 0 -25.4)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "/DS2")
			(pinfunction "Pin_21")
			(pintype "passive")
		)
		(pad "22" thru_hole circle
			(at 2.54 -25.4)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 10 "GND")
			(pinfunction "Pin_22")
			(pintype "passive")
		)
		(pad "23" thru_hole circle
			(at 0 -27.94)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "/DS1")
			(pinfunction "Pin_23")
			(pintype "passive")
		)
		(pad "24" thru_hole circle
			(at 2.54 -27.94)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 33 "unconnected-(HP1-Pin_24-Pad24)")
			(pinfunction "Pin_24")
			(pintype "passive+no_connect")
		)
		(pad "25" thru_hole circle
			(at 0 -30.48)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 11 "/DS0")
			(pinfunction "Pin_25")
			(pintype "passive")
		)
		(pad "26" thru_hole circle
			(at 2.54 -30.48)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 31 "unconnected-(HP1-Pin_26-Pad26)")
			(pinfunction "Pin_26")
			(pintype "passive+no_connect")
		)
		(pad "27" thru_hole circle
			(at 0 -33.02)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 18 "/INDEX")
			(pinfunction "Pin_27")
			(pintype "passive")
		)
		(pad "28" thru_hole circle
			(at 2.54 -33.02)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 30 "unconnected-(HP1-Pin_28-Pad28)")
			(pinfunction "Pin_28")
			(pintype "passive+no_connect")
		)
		(pad "29" thru_hole circle
			(at 0 -35.56)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "/DS3")
			(pinfunction "Pin_29")
			(pintype "passive")
		)
		(pad "30" thru_hole circle
			(at 2.54 -35.56)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 34 "unconnected-(HP1-Pin_30-Pad30)")
			(pinfunction "Pin_30")
			(pintype "passive+no_connect")
		)
		(pad "31" thru_hole circle
			(at 0 -38.1)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 7 "/IN_USE")
			(pinfunction "Pin_31")
			(pintype "passive")
		)
		(pad "32" thru_hole circle
			(at 2.54 -38.1)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 12 "/+5")
			(pinfunction "Pin_32")
			(pintype "passive")
		)
		(pad "33" thru_hole circle
			(at 0 -40.64)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 8 "/DISK_CHG")
			(pinfunction "Pin_33")
			(pintype "passive")
		)
		(pad "34" thru_hole circle
			(at 2.54 -40.64)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 20 "/DISK_CHG_RST")
			(pinfunction "Pin_34")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_IDC.3dshapes/IDC-Header_2x17_P2.54mm_Horizontal.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(gr_poly
		(pts
			(xy 142.4 106.7) (xy 148.2 122.1) (xy 155.7 122.1) (xy 155.7 62) (xy 142.4 62)
		)
		(fill no)
		(layer "Edge.Cuts")
	)
	(gr_text "DCR"
		(at 148.4 67.4 0)
		(layer "F.SilkS")
	)
	(gr_text "GND"
		(at 152.8 70 0)
		(layer "B.SilkS")
	)
	(gr_text "+5"
		(at 152.8 73.8 0)
		(layer "B.SilkS")
	)
	(gr_text "DCR"
		(at 152.8 66.2 0)
		(layer "B.SilkS")
	)
	(gr_text "34"
		(at 149.2 117.8 90)
		(layer "B.SilkS")
	)
	(gr_text "HP#1"
		(at 155 77.6 0)
		(layer "B.SilkS")
	)
	(embedded_fonts no)
)
