(kicad_pcb (version 20211014) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A")
  (title_block
    (title "Beetje 32U4 Blok")
    (date "2018-08-10")
    (rev "0.0")
    (company "www.MakersBox.us")
    (comment 1 "648.ken@gmail.com")
  )
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
  )
  (setup
    (pad_to_mask_clearance 0)
    (pcbplotparams
      (layerselection 0x00010f0_ffffffff)
      (disableapertmacros false)
      (usegerberextensions true)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile false)
      (svguseinch false)
      (svgprecision 6)
      (excludeedgelayer true)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "gerbers/")
    )
  )
  (net 0 "")
  (net 1 "GND")
  (net 2 "/D4")
  (net 3 "Net-(A1-Pad1)")
  (net 4 "/D8")
  (net 5 "/D13")
  (net 6 "/D12")
  (net 7 "/D10")
  (net 8 "/D9")
  (net 9 "/D7")
  (net 10 "+3V3")
  (net 11 "/A3")
  (net 12 "/A5")
  (net 13 "/SCK")
  (net 14 "/MOSI")
  (net 15 "/MISO")
  (net 16 "Net-(A2-Pad1)")
  (net 17 "Net-(C1-Pad2)")
  (net 18 "Net-(C15-Pad2)")
  (net 19 "/~{RESET}")
  (net 20 "/D+")
  (net 21 "/D-")
  (net 22 "Net-(D2-Pad1)")
  (net 23 "+5V")
  (net 24 "Net-(D11-Pad1)")
  (net 25 "Net-(D13-Pad1)")
  (net 26 "/SWCLK")
  (net 27 "/SWDIO")
  (net 28 "Net-(L1-Pad2)")
  (net 29 "Net-(R8-Pad1)")
  (net 30 "VBUS")
  (net 31 "/QSPI_CS")
  (net 32 "/SCL")
  (net 33 "/DS_DATA")
  (net 34 "/DS_CLK")
  (net 35 "/D11")
  (net 36 "/A1")
  (net 37 "/A2")
  (net 38 "/A4")
  (net 39 "/SDA")
  (net 40 "unconnected-(P1-Pad1)")
  (net 41 "unconnected-(P2-Pad1)")
  (net 42 "unconnected-(P3-Pad1)")
  (net 43 "unconnected-(P4-Pad1)")
  (net 44 "unconnected-(P5-Pad1)")
  (net 45 "unconnected-(P6-Pad1)")
  (net 46 "/UDP0")
  (net 47 "/AREF")
  (net 48 "/01")
  (net 49 "/02")
  (net 50 "/03")
  (net 51 "/04")
  (net 52 "/05")
  (net 53 "/06")
  (net 54 "/07")
  (net 55 "/08")
  (net 56 "/09")
  (net 57 "/10")
  (net 58 "/11")
  (net 59 "/12")
  (net 60 "/13")
  (net 61 "/14")
  (net 62 "/15")
  (net 63 "/16")
  (net 64 "/24")
  (net 65 "/23")
  (net 66 "/22")
  (net 67 "/21")
  (net 68 "/20")
  (net 69 "/19")
  (net 70 "/18")
  (net 71 "/17")
  (net 72 "/25")
  (net 73 "/26")
  (net 74 "/27")
  (net 75 "/28")
  (net 76 "/29")
  (net 77 "/30")
  (net 78 "/31")
  (net 79 "/32")
  (net 80 "/40")
  (net 81 "/39")
  (net 82 "/38")
  (net 83 "/37")
  (net 84 "/36")
  (net 85 "/35")
  (net 86 "/34")
  (net 87 "/33")
  (net 88 "/UDP1")
  (net 89 "/UDP2")
  (net 90 "/UDP3")
  (net 91 "/UDP4")
  (net 92 "/UDP5")
  (net 93 "unconnected-(RGB1-Pad5)")
  (net 94 "unconnected-(U2-Pad10)")
  (net 95 "/UDPI")
  (net 96 "unconnected-(U2-Pad12)")
  (net 97 "unconnected-(U2-Pad15)")
  (net 98 "unconnected-(U2-Pad16)")
  (net 99 "unconnected-(U2-Pad17)")
  (net 100 "unconnected-(U2-Pad18)")
  (net 101 "unconnected-(U3-Pad10)")
  (net 102 "unconnected-(U3-Pad12)")
  (net 103 "unconnected-(U3-Pad15)")
  (net 104 "unconnected-(U3-Pad16)")
  (net 105 "unconnected-(U3-Pad18)")
  (net 106 "unconnected-(U4-Pad20)")
  (net 107 "unconnected-(U4-Pad17)")
  (net 108 "unconnected-(U4-Pad16)")
  (net 109 "unconnected-(U4-Pad15)")
  (net 110 "unconnected-(U4-Pad12)")
  (net 111 "unconnected-(U4-Pad10)")
  (net 112 "unconnected-(U4-Pad5)")
  (net 113 "unconnected-(U4-Pad2)")
  (net 114 "unconnected-(U4-Pad1)")
  (net 115 "unconnected-(U5-Pad10)")
  (net 116 "unconnected-(U5-Pad12)")
  (net 117 "unconnected-(U5-Pad15)")
  (net 118 "unconnected-(U5-Pad16)")
  (net 119 "unconnected-(U5-Pad17)")
  (net 120 "unconnected-(U5-Pad18)")
  (net 121 "unconnected-(U6-Pad18)")
  (net 122 "unconnected-(U6-Pad16)")
  (net 123 "unconnected-(U6-Pad15)")
  (net 124 "unconnected-(U6-Pad12)")
  (net 125 "unconnected-(U6-Pad10)")
  (net 126 "unconnected-(U7-Pad1)")
  (net 127 "unconnected-(U7-Pad2)")
  (net 128 "unconnected-(U7-Pad5)")
  (net 129 "unconnected-(U7-Pad10)")
  (net 130 "unconnected-(U7-Pad12)")
  (net 131 "unconnected-(U7-Pad15)")
  (net 132 "unconnected-(U7-Pad16)")
  (net 133 "unconnected-(U7-Pad17)")
  (net 134 "unconnected-(U7-Pad20)")
  (net 135 "unconnected-(RGB1-Pad6)")
  (net 136 "/D3")
  (net 137 "/RX_D0")
  (net 138 "/TX_D1")
  (net 139 "/D2")
  (net 140 "/A0{slash}D5")
  (net 141 "unconnected-(U1-Pad4)")
  (net 142 "/QSPI_DATA_0")
  (net 143 "/QSPI_DATA_1")
  (net 144 "/QSPI_DATA_2")
  (net 145 "/QSPI_DATA_3")
  (net 146 "/QSPI_SCK")
  (net 147 "unconnected-(U9-Pad39)")
  (net 148 "unconnected-(J1-Pad4)")
  (footprint "footprints:M3mount" (layer "F.Cu")
    (tedit 636FC1C2)
    (at 110.49 80.01)
    (descr "Single banana socket, footprint - 6mm drill")
    (tags "banana socket")
    (property "Sheetfile" "Board RPB30 SAM51 SeeSaw.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "P1" (at 0 -5.08) (layer "F.SilkS") hide)
    (fp_text value "M3" (at 0 5.08) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0) (size 5 5) (drill 3.4) (layers *.Cu *.Mask)
      (net 40 "unconnected-(P1-Pad1)") (pinfunction "Pin_1") (pintype "passive+no_connect"))
  )
  (footprint "footprints:M25standoff" locked (layer "F.Cu")
    (tedit 636FF644)
    (at 168 87.75)
    (descr "Single banana socket, footprint - 6mm drill")
    (tags "banana socket")
    (property "Sheetfile" "Board RPB30 SAM51 SeeSaw.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "P5" (at 0 -5.08) (layer "F.SilkS") hide)
    (fp_text value "Standoff" (at 0 5.08) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0) (size 6 6) (drill 3.7) (layers *.Cu *.Mask)
      (net 44 "unconnected-(P5-Pad1)") (pinfunction "Pin_1") (pintype "passive+no_connect"))
    (model "${KIPRJMOD}/3D/standoff9774027151R (rev1).stp"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model "${KIPRJMOD}/3D/99607A263_Stainless Steel Flared-Collar Knurled-Head Thumb Screw.STEP"
      (offset (xyz 0 0 4))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "footprints:M3mount" (layer "F.Cu")
    (tedit 636FC1C2)
    (at 167.64 80.01)
    (descr "Single banana socket, footprint - 6mm drill")
    (tags "banana socket")
    (property "Sheetfile" "Board RPB30 SAM51 SeeSaw.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "P2" (at 0 -3.3) (layer "F.SilkS") hide)
    (fp_text value "M3" (at 0.1 3.5) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0) (size 5 5) (drill 3.4) (layers *.Cu *.Mask)
      (net 41 "unconnected-(P2-Pad1)") (pinfunction "Pin_1") (pintype "passive+no_connect"))
  )
  (footprint "footprints:M3mount" (layer "F.Cu")
    (tedit 636FC1C2)
    (at 167.64 131)
    (descr "Single banana socket, footprint - 6mm drill")
    (tags "banana socket")
    (property "Sheetfile" "Board RPB30 SAM51 SeeSaw.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "P4" (at 0 -3.3) (layer "F.SilkS") hide)
    (fp_text value "M3" (at 0.1 3.5) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0) (size 5 5) (drill 3.4) (layers *.Cu *.Mask)
      (net 43 "unconnected-(P4-Pad1)") (pinfunction "Pin_1") (pintype "passive+no_connect"))
  )
  (footprint "footprints:M25standoff" locked (layer "F.Cu")
    (tedit 636FF644)
    (at 168 110)
    (descr "Single banana socket, footprint - 6mm drill")
    (tags "banana socket")
    (property "Sheetfile" "Board RPB30 SAM51 SeeSaw.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "P6" (at 0 -5.08) (layer "F.SilkS") hide)
    (fp_text value "Standoff" (at 0 5.08) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0) (size 6 6) (drill 3.7) (layers *.Cu *.Mask)
      (net 45 "unconnected-(P6-Pad1)") (pinfunction "Pin_1") (pintype "passive+no_connect"))
    (model "${KIPRJMOD}/3D/standoff9774027151R (rev1).stp"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model "${KIPRJMOD}/3D/M2_5X6MM.step"
      (offset (xyz 0 0 6))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "footprints:SAMTEC_MEC8-113-TOP-BOTTOM" locked (layer "F.Cu")
    (tedit 63786631)
    (at 119 110 90)
    (property "Sheetfile" "Board RPB30 SAM51 SeeSaw.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "X2" (at -0.5 0 180) (layer "F.SilkS"))
    (fp_text value "MEC8-113" (at 8.21 6.135 90) (layer "F.Fab"))
    (pad "" np_thru_hole circle locked (at 7.6 0 90) (size 1.65 1.65) (drill 1.65) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle locked (at -7.6 0 90) (size 1.65 1.65) (drill 1.65) (layers *.Cu *.Mask))
    (pad "1" smd rect locked (at -6.4 4 90) (size 0.5 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 67 "/21") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" smd rect locked (at -5.6 4 90) (size 0.5 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 66 "/22") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" smd rect locked (at -4.8 4 90) (size 0.5 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 65 "/23") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" smd rect locked (at -4 4 90) (size 0.5 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 64 "/24") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" smd rect locked (at -3.2 4 90) (size 0.5 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 72 "/25") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" smd rect locked (at -2.4 4 90) (size 0.5 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 73 "/26") (pinfunction "Pin_6") (pintype "passive"))
    (pad "7" smd rect locked (at 1.6 4 90) (size 0.5 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 74 "/27") (pinfunction "Pin_7") (pintype "passive"))
    (pad "8" smd rect locked (at 2.4 4 90) (size 0.5 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 75 "/28") (pinfunction "Pin_8") (pintype "passive"))
    (pad "9" smd rect locked (at 3.2 4 90) (size 0.5 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 76 "/29") (pinfunction "Pin_9") (pintype "passive"))
    (pad "10" smd rect locked (at 4 4 90) (size 0.5 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 77 "/30") (pinfunction "Pin_10") (pintype "passive"))
    (pad "11" smd rect locked (at 4.8 4 90) (size 0.5 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 36 "/A1") (pinfunction "Pin_11") (pintype "passive"))
    (pad "12" smd rect locked (at 5.6 4 90) (size 0.5 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 11 "/A3") (pinfunction "Pin_12") (pintype "passive"))
    (pad "13" smd rect locked (at 6.4 4 90) (size 0.5 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 30 "VBUS") (pinfunction "Pin_13") (pintype "passive"))
    (pad "14" smd rect locked (at -6.4 -4 90) (size 0.5 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 78 "/31") (pinfunction "Pin_14") (pintype "passive"))
    (pad "15" smd rect locked (at -5.6 -4 90) (size 0.5 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 79 "/32") (pinfunction "Pin_15") (pintype "passive"))
    (pad "16" smd rect locked (at -4.8 -4 90) (size 0.5 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 87 "/33") (pinfunction "Pin_16") (pintype "passive"))
    (pad "17" smd rect locked (at -4 -4 90) (size 0.5 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 86 "/34") (pinfunction "Pin_17") (pintype "passive"))
    (pad "18" smd rect locked (at -3.2 -4 90) (size 0.5 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 85 "/35") (pinfunction "Pin_18") (pintype "passive"))
    (pad "19" smd rect locked (at -2.4 -4 90) (size 0.5 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 84 "/36") (pinfunction "Pin_19") (pintype "passive"))
    (pad "20" smd rect locked (at 1.6 -4 90) (size 0.5 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 83 "/37") (pinfunction "Pin_20") (pintype "passive"))
    (pad "21" smd rect locked (at 2.4 -4 90) (size 0.5 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 82 "/38") (pinfunction "Pin_21") (pintype "passive"))
    (pad "22" smd rect locked (at 3.2 -4 90) (size 0.5 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 81 "/39") (pinfunction "Pin_22") (pintype "passive"))
    (pad "23" smd rect locked (at 4 -4 90) (size 0.5 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 80 "/40") (pinfunction "Pin_23") (pintype "passive"))
    (pad "24" smd rect locked (at 4.8 -4 90) (size 0.5 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 32 "/SCL") (pinfunction "Pin_24") (pintype "passive"))
    (pad "25" smd rect locked (at 5.6 -4 90) (size 0.5 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 39 "/SDA") (pinfunction "Pin_25") (pintype "passive"))
    (pad "26" smd rect locked (at 6.4 -4 90) (size 0.5 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "Pin_26") (pintype "passive"))
    (model "${KIPRJMOD}/3D/mec8-113-02-l-d-ra1.stp"
      (offset (xyz -8 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (footprint "footprints:SAMTEC_MEC8-113-TOP-BOTTOM" locked (layer "F.Cu")
    (tedit 63786631)
    (at 119 87.75 90)
    (property "Sheetfile" "Board RPB30 SAM51 SeeSaw.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "X1" (at -0.4 2.15 180) (layer "F.SilkS"))
    (fp_text value "MEC8-113" (at 8.21 6.135 90) (layer "F.Fab"))
    (pad "" np_thru_hole circle locked (at 7.6 0 90) (size 1.65 1.65) (drill 1.65) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle locked (at -7.6 0 90) (size 1.65 1.65) (drill 1.65) (layers *.Cu *.Mask))
    (pad "1" smd rect locked (at -6.4 4 90) (size 0.5 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 48 "/01") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" smd rect locked (at -5.6 4 90) (size 0.5 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 49 "/02") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" smd rect locked (at -4.8 4 90) (size 0.5 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 50 "/03") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" smd rect locked (at -4 4 90) (size 0.5 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 51 "/04") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" smd rect locked (at -3.2 4 90) (size 0.5 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 52 "/05") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" smd rect locked (at -2.4 4 90) (size 0.5 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 53 "/06") (pinfunction "Pin_6") (pintype "passive"))
    (pad "7" smd rect locked (at 1.6 4 90) (size 0.5 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 54 "/07") (pinfunction "Pin_7") (pintype "passive"))
    (pad "8" smd rect locked (at 2.4 4 90) (size 0.5 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 55 "/08") (pinfunction "Pin_8") (pintype "passive"))
    (pad "9" smd rect locked (at 3.2 4 90) (size 0.5 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 56 "/09") (pinfunction "Pin_9") (pintype "passive"))
    (pad "10" smd rect locked (at 4 4 90) (size 0.5 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 57 "/10") (pinfunction "Pin_10") (pintype "passive"))
    (pad "11" smd rect locked (at 4.8 4 90) (size 0.5 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 140 "/A0{slash}D5") (pinfunction "Pin_11") (pintype "passive"))
    (pad "12" smd rect locked (at 5.6 4 90) (size 0.5 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 37 "/A2") (pinfunction "Pin_12") (pintype "passive"))
    (pad "13" smd rect locked (at 6.4 4 90) (size 0.5 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 30 "VBUS") (pinfunction "Pin_13") (pintype "passive"))
    (pad "14" smd rect locked (at -6.4 -4 90) (size 0.5 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 58 "/11") (pinfunction "Pin_14") (pintype "passive"))
    (pad "15" smd rect locked (at -5.6 -4 90) (size 0.5 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 59 "/12") (pinfunction "Pin_15") (pintype "passive"))
    (pad "16" smd rect locked (at -4.8 -4 90) (size 0.5 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 60 "/13") (pinfunction "Pin_16") (pintype "passive"))
    (pad "17" smd rect locked (at -4 -4 90) (size 0.5 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 61 "/14") (pinfunction "Pin_17") (pintype "passive"))
    (pad "18" smd rect locked (at -3.2 -4 90) (size 0.5 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 62 "/15") (pinfunction "Pin_18") (pintype "passive"))
    (pad "19" smd rect locked (at -2.4 -4 90) (size 0.5 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 63 "/16") (pinfunction "Pin_19") (pintype "passive"))
    (pad "20" smd rect locked (at 1.6 -4 90) (size 0.5 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 71 "/17") (pinfunction "Pin_20") (pintype "passive"))
    (pad "21" smd rect locked (at 2.4 -4 90) (size 0.5 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 70 "/18") (pinfunction "Pin_21") (pintype "passive"))
    (pad "22" smd rect locked (at 3.2 -4 90) (size 0.5 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 69 "/19") (pinfunction "Pin_22") (pintype "passive"))
    (pad "23" smd rect locked (at 4 -4 90) (size 0.5 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 68 "/20") (pinfunction "Pin_23") (pintype "passive"))
    (pad "24" smd rect locked (at 4.8 -4 90) (size 0.5 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 32 "/SCL") (pinfunction "Pin_24") (pintype "passive"))
    (pad "25" smd rect locked (at 5.6 -4 90) (size 0.5 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 39 "/SDA") (pinfunction "Pin_25") (pintype "passive"))
    (pad "26" smd rect locked (at 6.4 -4 90) (size 0.5 2) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "Pin_26") (pintype "passive"))
    (model "${KIPRJMOD}/3D/mec8-113-02-l-d-ra1.stp"
      (offset (xyz -8 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (footprint "footprints:M3mount" (layer "F.Cu")
    (tedit 636FC1C2)
    (at 110.49 131)
    (descr "Single banana socket, footprint - 6mm drill")
    (tags "banana socket")
    (property "Sheetfile" "Board RPB30 SAM51 SeeSaw.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "P3" (at 0 -3.3) (layer "F.SilkS") hide)
    (fp_text value "M3" (at 0.1 3.5) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole circle locked (at 0 0) (size 5 5) (drill 3.4) (layers *.Cu *.Mask)
      (net 42 "unconnected-(P3-Pad1)") (pinfunction "Pin_1") (pintype "passive+no_connect"))
  )
  (footprint "Connector_Molex:Molex_PicoBlade_53048-0310_1x03_P1.25mm_Horizontal" (layer "F.Cu")
    (tedit 5B783024)
    (at 148.85 126.5 -90)
    (descr "Molex PicoBlade Connector System, 53048-0310, 3 Pins per row (http://www.molex.com/pdm_docs/sd/530480210_sd.pdf), generated with kicad-footprint-generator")
    (tags "connector Molex PicoBlade top entry")
    (property "Sheetfile" "Board RPB30 SAM51 SeeSaw.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J4" (at 1.25 3.8 90) (layer "F.SilkS") hide)
    (fp_text value "UDPI" (at -2.35 0.8 180) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 1.25 3.75 90) (layer "F.Fab"))
    (pad "1" thru_hole roundrect (at 0 0 270) (size 0.8 1.3) (drill 0.5) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 10 "+3V3") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 1.25 0 270) (size 0.8 1.3) (drill 0.5) (layers *.Cu *.Mask)
      (net 95 "/UDPI") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 2.5 0 270) (size 0.8 1.3) (drill 0.5) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "Pin_3") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_Molex.3dshapes/Molex_PicoBlade_53048-0310_1x03_P1.25mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "footprints:R_0603" (layer "F.Cu")
    (tedit 636FC042)
    (at 135.89 97.282 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (property "Sheetfile" "Board RPB30 SAM51 SeeSaw.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R2" (at 1.905 0 90) (layer "Dwgs.User"))
    (fp_text value "100" (at 2.032 0 90) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd rect locked (at -0.75 0 90) (size 0.5 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 88 "/UDP1") (pintype "passive"))
    (pad "2" smd rect locked (at 0.75 0 90) (size 0.5 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 95 "/UDPI") (pintype "passive"))
    (model "${KIPRJMOD}/3D/R_0603_1608Metric.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "footprints:R_0603" (layer "F.Cu")
    (tedit 636FC042)
    (at 135.89 82.55 -90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (property "Sheetfile" "Board RPB30 SAM51 SeeSaw.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R3" (at 1.905 0 90) (layer "Dwgs.User"))
    (fp_text value "100" (at -1.905 0 90) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd rect locked (at -0.75 0 270) (size 0.5 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 89 "/UDP2") (pintype "passive"))
    (pad "2" smd rect locked (at 0.75 0 270) (size 0.5 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 95 "/UDPI") (pintype "passive"))
    (model "${KIPRJMOD}/3D/R_0603_1608Metric.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "footprints:R_0603" (layer "F.Cu")
    (tedit 636FC042)
    (at 135.89 112.268 -90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (property "Sheetfile" "Board RPB30 SAM51 SeeSaw.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R4" (at 1.905 0 90) (layer "Dwgs.User"))
    (fp_text value "100" (at -1.905 0 90) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd rect locked (at -0.75 0 270) (size 0.5 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 90 "/UDP3") (pintype "passive"))
    (pad "2" smd rect locked (at 0.75 0 270) (size 0.5 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 95 "/UDPI") (pintype "passive"))
    (model "${KIPRJMOD}/3D/R_0603_1608Metric.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "footprints:R_0603" (layer "F.Cu")
    (tedit 636FC042)
    (at 135.89 118.072 -90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (property "Sheetfile" "Board RPB30 SAM51 SeeSaw.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R5" (at 1.905 0 90) (layer "Dwgs.User"))
    (fp_text value "100" (at -1.905 0 90) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd rect locked (at -0.75 0 270) (size 0.5 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 91 "/UDP4") (pintype "passive"))
    (pad "2" smd rect locked (at 0.75 0 270) (size 0.5 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 95 "/UDPI") (pintype "passive"))
    (model "${KIPRJMOD}/3D/R_0603_1608Metric.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "footprints:R_0603" (layer "F.Cu")
    (tedit 636FC042)
    (at 135.89 89.724 -90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (property "Sheetfile" "Board RPB30 SAM51 SeeSaw.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R1" (at 1.905 0 90) (layer "Dwgs.User"))
    (fp_text value "100" (at -1.905 0 90) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd rect locked (at -0.75 0 270) (size 0.5 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 46 "/UDP0") (pintype "passive"))
    (pad "2" smd rect locked (at 0.75 0 270) (size 0.5 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 95 "/UDPI") (pintype "passive"))
    (model "${KIPRJMOD}/3D/R_0603_1608Metric.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "footprints:R_0603" (layer "F.Cu")
    (tedit 636FC042)
    (at 135.89 104.636 -90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (property "Sheetfile" "Board RPB30 SAM51 SeeSaw.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R6" (at 1.905 0 90) (layer "Dwgs.User"))
    (fp_text value "100" (at -1.905 0 90) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd rect locked (at -0.75 0 270) (size 0.5 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 92 "/UDP5") (pintype "passive"))
    (pad "2" smd rect locked (at 0.75 0 270) (size 0.5 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 95 "/UDPI") (pintype "passive"))
    (model "${KIPRJMOD}/3D/R_0603_1608Metric.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "footprints:R_0603" (layer "F.Cu")
    (tedit 636FC042)
    (at 136.5 123.55)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (property "Sheetfile" "Board RPB30 SAM51 SeeSaw.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R7" (at 1.905 0) (layer "Dwgs.User"))
    (fp_text value "10K" (at -2.45 0.05) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect locked (at -0.75 0) (size 0.5 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 10 "+3V3") (pintype "passive"))
    (pad "2" smd rect locked (at 0.75 0) (size 0.5 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 95 "/UDPI") (pintype "passive"))
    (model "${KIPRJMOD}/3D/R_0603_1608Metric.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "footprints:AR_logo_18mm" (layer "F.Cu")
    (tedit 63780F59)
    (at 143 90.25)
    (property "Sheetfile" "Board RPB30 SAM51 SeeSaw.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "ARLogo1" (at 0 0) (layer "F.SilkS") hide)
    (fp_text value "SYM_Arrow_Large" (at 0.75 0) (layer "Dwgs.User"))
  )
  (footprint "Package_DFN_QFN:VQFN-20-1EP_3x3mm_P0.4mm_EP1.7x1.7mm" (layer "F.Cu")
    (tedit 5DC5F6A8)
    (at 132 111.5 -90)
    (descr "VQFN, 20 Pin (http://ww1.microchip.com/downloads/en/DeviceDoc/20%20Lead%20VQFN%203x3x0_9mm_1_7EP%20U2B%20C04-21496a.pdf), generated with kicad-footprint-generator ipc_noLead_generator.py")
    (tags "VQFN NoLead")
    (property "Sheetfile" "Board RPB30 SAM51 SeeSaw.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "U5" (at 0 -2.8 -90) (layer "F.SilkS"))
    (fp_text value "ATtiny816-M" (at 0 2.8 -90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 -90) (layer "F.Fab"))
    (pad "" smd roundrect (at -0.425 -0.425 270) (size 0.69 0.69) (layers "F.Paste") (roundrect_rratio 0.25))
    (pad "" smd roundrect (at -0.425 0.425 270) (size 0.69 0.69) (layers "F.Paste") (roundrect_rratio 0.25))
    (pad "" smd roundrect (at 0.425 -0.425 270) (size 0.69 0.69) (layers "F.Paste") (roundrect_rratio 0.25))
    (pad "" smd roundrect (at 0.425 0.425 270) (size 0.69 0.69) (layers "F.Paste") (roundrect_rratio 0.25))
    (pad "1" smd custom (at -1.45 -0.8 270) (size 0.143431 0.143431) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 74 "/27") (pinfunction "PA2") (pintype "bidirectional")
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_poly (pts
            (xy 0.35 0.000711)
            (xy 0.35 0.05)
            (xy -0.35 0.05)
            (xy -0.35 -0.05)
            (xy 0.299289 -0.05)
          ) (width 0.1) (fill yes))
      ))
    (pad "2" smd roundrect (at -1.45 -0.4 270) (size 0.8 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 73 "/26") (pinfunction "PA3") (pintype "bidirectional"))
    (pad "3" smd roundrect (at -1.45 0 270) (size 0.8 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "4" smd roundrect (at -1.45 0.4 270) (size 0.8 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 10 "+3V3") (pinfunction "VCC") (pintype "power_in"))
    (pad "5" smd custom (at -1.45 0.8 270) (size 0.143431 0.143431) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 72 "/25") (pinfunction "PA4") (pintype "bidirectional")
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_poly (pts
            (xy 0.35 -0.000711)
            (xy 0.299289 0.05)
            (xy -0.35 0.05)
            (xy -0.35 -0.05)
            (xy 0.35 -0.05)
          ) (width 0.1) (fill yes))
      ))
    (pad "6" smd custom (at -0.8 1.45 270) (size 0.143431 0.143431) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 64 "/24") (pinfunction "PA5") (pintype "bidirectional")
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_poly (pts
            (xy 0.05 0.35)
            (xy -0.05 0.35)
            (xy -0.05 -0.299289)
            (xy 0.000711 -0.35)
            (xy 0.05 -0.35)
          ) (width 0.1) (fill yes))
      ))
    (pad "7" smd roundrect (at -0.4 1.45 270) (size 0.2 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 65 "/23") (pinfunction "PA6") (pintype "bidirectional"))
    (pad "8" smd roundrect (at 0 1.45 270) (size 0.2 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 66 "/22") (pinfunction "PA7") (pintype "bidirectional"))
    (pad "9" smd roundrect (at 0.4 1.45 270) (size 0.2 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 67 "/21") (pinfunction "PB5") (pintype "bidirectional"))
    (pad "10" smd custom (at 0.8 1.45 270) (size 0.143431 0.143431) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 115 "unconnected-(U5-Pad10)") (pinfunction "PB4") (pintype "bidirectional+no_connect")
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_poly (pts
            (xy 0.05 -0.299289)
            (xy 0.05 0.35)
            (xy -0.05 0.35)
            (xy -0.05 -0.35)
            (xy -0.000711 -0.35)
          ) (width 0.1) (fill yes))
      ))
    (pad "11" smd custom (at 1.45 0.8 270) (size 0.143431 0.143431) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 8 "/D9") (pinfunction "PB3") (pintype "bidirectional")
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_poly (pts
            (xy 0.35 0.05)
            (xy -0.299289 0.05)
            (xy -0.35 -0.000711)
            (xy -0.35 -0.05)
            (xy 0.35 -0.05)
          ) (width 0.1) (fill yes))
      ))
    (pad "12" smd roundrect (at 1.45 0.4 270) (size 0.8 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 116 "unconnected-(U5-Pad12)") (pinfunction "PB2") (pintype "bidirectional+no_connect"))
    (pad "13" smd roundrect (at 1.45 0 270) (size 0.8 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 39 "/SDA") (pinfunction "PB1") (pintype "bidirectional"))
    (pad "14" smd roundrect (at 1.45 -0.4 270) (size 0.8 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 32 "/SCL") (pinfunction "PB0") (pintype "bidirectional"))
    (pad "15" smd custom (at 1.45 -0.8 270) (size 0.143431 0.143431) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 117 "unconnected-(U5-Pad15)") (pinfunction "PC0") (pintype "bidirectional+no_connect")
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_poly (pts
            (xy 0.35 0.05)
            (xy -0.35 0.05)
            (xy -0.35 0.000711)
            (xy -0.299289 -0.05)
            (xy 0.35 -0.05)
          ) (width 0.1) (fill yes))
      ))
    (pad "16" smd custom (at 0.8 -1.45 270) (size 0.143431 0.143431) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 118 "unconnected-(U5-Pad16)") (pinfunction "PC1") (pintype "bidirectional+no_connect")
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_poly (pts
            (xy 0.05 0.299289)
            (xy -0.000711 0.35)
            (xy -0.05 0.35)
            (xy -0.05 -0.35)
            (xy 0.05 -0.35)
          ) (width 0.1) (fill yes))
      ))
    (pad "17" smd roundrect (at 0.4 -1.45 270) (size 0.2 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 119 "unconnected-(U5-Pad17)") (pinfunction "PC2") (pintype "bidirectional+no_connect"))
    (pad "18" smd roundrect (at 0 -1.45 270) (size 0.2 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 120 "unconnected-(U5-Pad18)") (pinfunction "PC3") (pintype "bidirectional+no_connect"))
    (pad "19" smd roundrect (at -0.4 -1.45 270) (size 0.2 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 90 "/UDP3") (pinfunction "~{RESET}/PA0") (pintype "bidirectional"))
    (pad "20" smd custom (at -0.8 -1.45 270) (size 0.143431 0.143431) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 75 "/28") (pinfunction "PA1") (pintype "bidirectional")
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_poly (pts
            (xy 0.05 0.35)
            (xy 0.000711 0.35)
            (xy -0.05 0.299289)
            (xy -0.05 -0.35)
            (xy 0.05 -0.35)
          ) (width 0.1) (fill yes))
      ))
    (pad "21" smd rect (at 0 0 270) (size 1.7 1.7) (layers "F.Cu" "F.Mask")
      (net 1 "GND") (pinfunction "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Package_DFN_QFN.3dshapes/VQFN-20-1EP_3x3mm_P0.4mm_EP1.7x1.7mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_DFN_QFN:VQFN-20-1EP_3x3mm_P0.4mm_EP1.7x1.7mm" (layer "F.Cu")
    (tedit 5DC5F6A8)
    (at 132 104 -90)
    (descr "VQFN, 20 Pin (http://ww1.microchip.com/downloads/en/DeviceDoc/20%20Lead%20VQFN%203x3x0_9mm_1_7EP%20U2B%20C04-21496a.pdf), generated with kicad-footprint-generator ipc_noLead_generator.py")
    (tags "VQFN NoLead")
    (property "Sheetfile" "Board RPB30 SAM51 SeeSaw.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "U7" (at 0 -2.8 -90) (layer "F.SilkS"))
    (fp_text value "ATtiny816-M" (at 0 2.8 -90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 -90) (layer "F.Fab"))
    (pad "" smd roundrect (at 0.425 -0.425 270) (size 0.69 0.69) (layers "F.Paste") (roundrect_rratio 0.25))
    (pad "" smd roundrect (at 0.425 0.425 270) (size 0.69 0.69) (layers "F.Paste") (roundrect_rratio 0.25))
    (pad "" smd roundrect (at -0.425 -0.425 270) (size 0.69 0.69) (layers "F.Paste") (roundrect_rratio 0.25))
    (pad "" smd roundrect (at -0.425 0.425 270) (size 0.69 0.69) (layers "F.Paste") (roundrect_rratio 0.25))
    (pad "1" smd custom (at -1.45 -0.8 270) (size 0.143431 0.143431) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 126 "unconnected-(U7-Pad1)") (pinfunction "PA2") (pintype "bidirectional")
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_poly (pts
            (xy 0.35 0.000711)
            (xy 0.35 0.05)
            (xy -0.35 0.05)
            (xy -0.35 -0.05)
            (xy 0.299289 -0.05)
          ) (width 0.1) (fill yes))
      ))
    (pad "2" smd roundrect (at -1.45 -0.4 270) (size 0.8 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 127 "unconnected-(U7-Pad2)") (pinfunction "PA3") (pintype "bidirectional"))
    (pad "3" smd roundrect (at -1.45 0 270) (size 0.8 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "4" smd roundrect (at -1.45 0.4 270) (size 0.8 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 10 "+3V3") (pinfunction "VCC") (pintype "power_in"))
    (pad "5" smd custom (at -1.45 0.8 270) (size 0.143431 0.143431) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 128 "unconnected-(U7-Pad5)") (pinfunction "PA4") (pintype "bidirectional")
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_poly (pts
            (xy 0.35 -0.000711)
            (xy 0.299289 0.05)
            (xy -0.35 0.05)
            (xy -0.35 -0.05)
            (xy 0.35 -0.05)
          ) (width 0.1) (fill yes))
      ))
    (pad "6" smd custom (at -0.8 1.45 270) (size 0.143431 0.143431) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 80 "/40") (pinfunction "PA5") (pintype "bidirectional")
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_poly (pts
            (xy 0.05 0.35)
            (xy -0.05 0.35)
            (xy -0.05 -0.299289)
            (xy 0.000711 -0.35)
            (xy 0.05 -0.35)
          ) (width 0.1) (fill yes))
      ))
    (pad "7" smd roundrect (at -0.4 1.45 270) (size 0.2 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 81 "/39") (pinfunction "PA6") (pintype "bidirectional"))
    (pad "8" smd roundrect (at 0 1.45 270) (size 0.2 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 82 "/38") (pinfunction "PA7") (pintype "bidirectional"))
    (pad "9" smd roundrect (at 0.4 1.45 270) (size 0.2 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 83 "/37") (pinfunction "PB5") (pintype "bidirectional"))
    (pad "10" smd custom (at 0.8 1.45 270) (size 0.143431 0.143431) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 129 "unconnected-(U7-Pad10)") (pinfunction "PB4") (pintype "bidirectional+no_connect")
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_poly (pts
            (xy 0.05 -0.299289)
            (xy 0.05 0.35)
            (xy -0.05 0.35)
            (xy -0.05 -0.35)
            (xy -0.000711 -0.35)
          ) (width 0.1) (fill yes))
      ))
    (pad "11" smd custom (at 1.45 0.8 270) (size 0.143431 0.143431) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 9 "/D7") (pinfunction "PB3") (pintype "bidirectional")
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_poly (pts
            (xy 0.35 0.05)
            (xy -0.299289 0.05)
            (xy -0.35 -0.000711)
            (xy -0.35 -0.05)
            (xy 0.35 -0.05)
          ) (width 0.1) (fill yes))
      ))
    (pad "12" smd roundrect (at 1.45 0.4 270) (size 0.8 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 130 "unconnected-(U7-Pad12)") (pinfunction "PB2") (pintype "bidirectional+no_connect"))
    (pad "13" smd roundrect (at 1.45 0 270) (size 0.8 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 39 "/SDA") (pinfunction "PB1") (pintype "bidirectional"))
    (pad "14" smd roundrect (at 1.45 -0.4 270) (size 0.8 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 32 "/SCL") (pinfunction "PB0") (pintype "bidirectional"))
    (pad "15" smd custom (at 1.45 -0.8 270) (size 0.143431 0.143431) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 131 "unconnected-(U7-Pad15)") (pinfunction "PC0") (pintype "bidirectional+no_connect")
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_poly (pts
            (xy 0.35 0.05)
            (xy -0.35 0.05)
            (xy -0.35 0.000711)
            (xy -0.299289 -0.05)
            (xy 0.35 -0.05)
          ) (width 0.1) (fill yes))
      ))
    (pad "16" smd custom (at 0.8 -1.45 270) (size 0.143431 0.143431) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 132 "unconnected-(U7-Pad16)") (pinfunction "PC1") (pintype "bidirectional+no_connect")
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_poly (pts
            (xy 0.05 0.299289)
            (xy -0.000711 0.35)
            (xy -0.05 0.35)
            (xy -0.05 -0.35)
            (xy 0.05 -0.35)
          ) (width 0.1) (fill yes))
      ))
    (pad "17" smd roundrect (at 0.4 -1.45 270) (size 0.2 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 133 "unconnected-(U7-Pad17)") (pinfunction "PC2") (pintype "bidirectional+no_connect"))
    (pad "18" smd roundrect (at 0 -1.45 270) (size 0.2 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pinfunction "PC3") (pintype "bidirectional"))
    (pad "19" smd roundrect (at -0.4 -1.45 270) (size 0.2 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 92 "/UDP5") (pinfunction "~{RESET}/PA0") (pintype "bidirectional"))
    (pad "20" smd custom (at -0.8 -1.45 270) (size 0.143431 0.143431) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 134 "unconnected-(U7-Pad20)") (pinfunction "PA1") (pintype "bidirectional")
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_poly (pts
            (xy 0.05 0.35)
            (xy 0.000711 0.35)
            (xy -0.05 0.299289)
            (xy -0.05 -0.35)
            (xy 0.05 -0.35)
          ) (width 0.1) (fill yes))
      ))
    (pad "21" smd rect (at 0 0 270) (size 1.7 1.7) (layers "F.Cu" "F.Mask")
      (net 1 "GND") (pinfunction "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Package_DFN_QFN.3dshapes/VQFN-20-1EP_3x3mm_P0.4mm_EP1.7x1.7mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "footprints:C_0603" (layer "F.Cu")
    (tedit 59958EE7)
    (at 131.75 86.25)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (property "Sheetfile" "Board RPB30 SAM51 SeeSaw.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C2" (at 0 -1.5) (layer "F.Fab"))
    (fp_text value "0.1uF" (at 0.076 -1.16) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect (at -0.75 0) (size 0.8 0.75) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 10 "+3V3") (pintype "passive"))
    (pad "2" smd rect (at 0.75 0) (size 0.8 0.75) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pintype "passive"))
    (model "Capacitors_SMD.3dshapes/C_0603.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "footprints:C_0603" (layer "F.Cu")
    (tedit 59958EE7)
    (at 131.75 101.25)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (property "Sheetfile" "Board RPB30 SAM51 SeeSaw.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C7" (at 0 -1.5) (layer "F.Fab"))
    (fp_text value "0.1uF" (at 0 -1.174) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect (at -0.75 0) (size 0.8 0.75) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 10 "+3V3") (pintype "passive"))
    (pad "2" smd rect (at 0.75 0) (size 0.8 0.75) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pintype "passive"))
    (model "Capacitors_SMD.3dshapes/C_0603.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "footprints:C_0603" (layer "F.Cu")
    (tedit 59958EE7)
    (at 131.7 116.2)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (property "Sheetfile" "Board RPB30 SAM51 SeeSaw.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C6" (at 0 -1.5) (layer "F.Fab"))
    (fp_text value "0.1uF" (at 0.35 -1.138) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect (at -0.75 0) (size 0.8 0.75) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 10 "+3V3") (pintype "passive"))
    (pad "2" smd rect (at 0.75 0) (size 0.8 0.75) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pintype "passive"))
    (model "Capacitors_SMD.3dshapes/C_0603.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "footprints:C_0603" (layer "F.Cu")
    (tedit 59958EE7)
    (at 131.75 108.7)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (property "Sheetfile" "Board RPB30 SAM51 SeeSaw.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C5" (at 0 -1.5) (layer "F.Fab"))
    (fp_text value "0.1uF" (at 0.35 -1.258) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect (at -0.75 0) (size 0.8 0.75) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 10 "+3V3") (pintype "passive"))
    (pad "2" smd rect (at 0.75 0) (size 0.8 0.75) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pintype "passive"))
    (model "Capacitors_SMD.3dshapes/C_0603.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_DFN_QFN:VQFN-20-1EP_3x3mm_P0.4mm_EP1.7x1.7mm" (layer "F.Cu")
    (tedit 5DC5F6A8)
    (at 132 96.5 -90)
    (descr "VQFN, 20 Pin (http://ww1.microchip.com/downloads/en/DeviceDoc/20%20Lead%20VQFN%203x3x0_9mm_1_7EP%20U2B%20C04-21496a.pdf), generated with kicad-footprint-generator ipc_noLead_generator.py")
    (tags "VQFN NoLead")
    (property "Sheetfile" "Board RPB30 SAM51 SeeSaw.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "U3" (at 0 -2.8 -90) (layer "F.SilkS"))
    (fp_text value "ATtiny816-M" (at 0 2.8 -90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 -90) (layer "F.Fab"))
    (pad "" smd roundrect (at 0.425 -0.425 270) (size 0.69 0.69) (layers "F.Paste") (roundrect_rratio 0.25))
    (pad "" smd roundrect (at -0.425 0.425 270) (size 0.69 0.69) (layers "F.Paste") (roundrect_rratio 0.25))
    (pad "" smd roundrect (at 0.425 0.425 270) (size 0.69 0.69) (layers "F.Paste") (roundrect_rratio 0.25))
    (pad "" smd roundrect (at -0.425 -0.425 270) (size 0.69 0.69) (layers "F.Paste") (roundrect_rratio 0.25))
    (pad "1" smd custom (at -1.45 -0.8 270) (size 0.143431 0.143431) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 62 "/15") (pinfunction "PA2") (pintype "bidirectional")
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_poly (pts
            (xy 0.35 0.000711)
            (xy 0.35 0.05)
            (xy -0.35 0.05)
            (xy -0.35 -0.05)
            (xy 0.299289 -0.05)
          ) (width 0.1) (fill yes))
      ))
    (pad "2" smd roundrect (at -1.45 -0.4 270) (size 0.8 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 61 "/14") (pinfunction "PA3") (pintype "bidirectional"))
    (pad "3" smd roundrect (at -1.45 0 270) (size 0.8 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "4" smd roundrect (at -1.45 0.4 270) (size 0.8 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 10 "+3V3") (pinfunction "VCC") (pintype "power_in"))
    (pad "5" smd custom (at -1.45 0.8 270) (size 0.143431 0.143431) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 60 "/13") (pinfunction "PA4") (pintype "bidirectional")
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_poly (pts
            (xy 0.35 -0.000711)
            (xy 0.299289 0.05)
            (xy -0.35 0.05)
            (xy -0.35 -0.05)
            (xy 0.35 -0.05)
          ) (width 0.1) (fill yes))
      ))
    (pad "6" smd custom (at -0.8 1.45 270) (size 0.143431 0.143431) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 59 "/12") (pinfunction "PA5") (pintype "bidirectional")
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_poly (pts
            (xy 0.05 0.35)
            (xy -0.05 0.35)
            (xy -0.05 -0.299289)
            (xy 0.000711 -0.35)
            (xy 0.05 -0.35)
          ) (width 0.1) (fill yes))
      ))
    (pad "7" smd roundrect (at -0.4 1.45 270) (size 0.2 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 58 "/11") (pinfunction "PA6") (pintype "bidirectional"))
    (pad "8" smd roundrect (at 0 1.45 270) (size 0.2 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 57 "/10") (pinfunction "PA7") (pintype "bidirectional"))
    (pad "9" smd roundrect (at 0.4 1.45 270) (size 0.2 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 56 "/09") (pinfunction "PB5") (pintype "bidirectional"))
    (pad "10" smd custom (at 0.8 1.45 270) (size 0.143431 0.143431) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 101 "unconnected-(U3-Pad10)") (pinfunction "PB4") (pintype "bidirectional+no_connect")
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_poly (pts
            (xy 0.05 -0.299289)
            (xy 0.05 0.35)
            (xy -0.05 0.35)
            (xy -0.05 -0.35)
            (xy -0.000711 -0.35)
          ) (width 0.1) (fill yes))
      ))
    (pad "11" smd custom (at 1.45 0.8 270) (size 0.143431 0.143431) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 14 "/MOSI") (pinfunction "PB3") (pintype "bidirectional")
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_poly (pts
            (xy 0.35 0.05)
            (xy -0.299289 0.05)
            (xy -0.35 -0.000711)
            (xy -0.35 -0.05)
            (xy 0.35 -0.05)
          ) (width 0.1) (fill yes))
      ))
    (pad "12" smd roundrect (at 1.45 0.4 270) (size 0.8 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 102 "unconnected-(U3-Pad12)") (pinfunction "PB2") (pintype "bidirectional+no_connect"))
    (pad "13" smd roundrect (at 1.45 0 270) (size 0.8 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 39 "/SDA") (pinfunction "PB1") (pintype "bidirectional"))
    (pad "14" smd roundrect (at 1.45 -0.4 270) (size 0.8 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 32 "/SCL") (pinfunction "PB0") (pintype "bidirectional"))
    (pad "15" smd custom (at 1.45 -0.8 270) (size 0.143431 0.143431) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 103 "unconnected-(U3-Pad15)") (pinfunction "PC0") (pintype "bidirectional+no_connect")
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_poly (pts
            (xy 0.35 0.05)
            (xy -0.35 0.05)
            (xy -0.35 0.000711)
            (xy -0.299289 -0.05)
            (xy 0.35 -0.05)
          ) (width 0.1) (fill yes))
      ))
    (pad "16" smd custom (at 0.8 -1.45 270) (size 0.143431 0.143431) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 104 "unconnected-(U3-Pad16)") (pinfunction "PC1") (pintype "bidirectional+no_connect")
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_poly (pts
            (xy 0.05 0.299289)
            (xy -0.000711 0.35)
            (xy -0.05 0.35)
            (xy -0.05 -0.35)
            (xy 0.05 -0.35)
          ) (width 0.1) (fill yes))
      ))
    (pad "17" smd roundrect (at 0.4 -1.45 270) (size 0.2 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pinfunction "PC2") (pintype "bidirectional"))
    (pad "18" smd roundrect (at 0 -1.45 270) (size 0.2 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 105 "unconnected-(U3-Pad18)") (pinfunction "PC3") (pintype "bidirectional"))
    (pad "19" smd roundrect (at -0.4 -1.45 270) (size 0.2 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 88 "/UDP1") (pinfunction "~{RESET}/PA0") (pintype "bidirectional"))
    (pad "20" smd custom (at -0.8 -1.45 270) (size 0.143431 0.143431) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 63 "/16") (pinfunction "PA1") (pintype "bidirectional")
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_poly (pts
            (xy 0.05 0.35)
            (xy 0.000711 0.35)
            (xy -0.05 0.299289)
            (xy -0.05 -0.35)
            (xy 0.05 -0.35)
          ) (width 0.1) (fill yes))
      ))
    (pad "21" smd rect (at 0 0 270) (size 1.7 1.7) (layers "F.Cu" "F.Mask")
      (net 1 "GND") (pinfunction "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Package_DFN_QFN.3dshapes/VQFN-20-1EP_3x3mm_P0.4mm_EP1.7x1.7mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_DFN_QFN:VQFN-20-1EP_3x3mm_P0.4mm_EP1.7x1.7mm" (layer "F.Cu")
    (tedit 5DC5F6A8)
    (at 132 89 -90)
    (descr "VQFN, 20 Pin (http://ww1.microchip.com/downloads/en/DeviceDoc/20%20Lead%20VQFN%203x3x0_9mm_1_7EP%20U2B%20C04-21496a.pdf), generated with kicad-footprint-generator ipc_noLead_generator.py")
    (tags "VQFN NoLead")
    (property "Sheetfile" "Board RPB30 SAM51 SeeSaw.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "U2" (at 0 -2.8 -90) (layer "F.SilkS"))
    (fp_text value "ATtiny816-M" (at 0 2.8 -90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 -90) (layer "F.Fab"))
    (pad "" smd roundrect (at 0.425 0.425 270) (size 0.69 0.69) (layers "F.Paste") (roundrect_rratio 0.25))
    (pad "" smd roundrect (at 0.425 -0.425 270) (size 0.69 0.69) (layers "F.Paste") (roundrect_rratio 0.25))
    (pad "" smd roundrect (at -0.425 -0.425 270) (size 0.69 0.69) (layers "F.Paste") (roundrect_rratio 0.25))
    (pad "" smd roundrect (at -0.425 0.425 270) (size 0.69 0.69) (layers "F.Paste") (roundrect_rratio 0.25))
    (pad "1" smd custom (at -1.45 -0.8 270) (size 0.143431 0.143431) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 54 "/07") (pinfunction "PA2") (pintype "bidirectional")
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_poly (pts
            (xy 0.35 0.000711)
            (xy 0.35 0.05)
            (xy -0.35 0.05)
            (xy -0.35 -0.05)
            (xy 0.299289 -0.05)
          ) (width 0.1) (fill yes))
      ))
    (pad "2" smd roundrect (at -1.45 -0.4 270) (size 0.8 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 53 "/06") (pinfunction "PA3") (pintype "bidirectional"))
    (pad "3" smd roundrect (at -1.45 0 270) (size 0.8 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "4" smd roundrect (at -1.45 0.4 270) (size 0.8 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 10 "+3V3") (pinfunction "VCC") (pintype "power_in"))
    (pad "5" smd custom (at -1.45 0.8 270) (size 0.143431 0.143431) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 52 "/05") (pinfunction "PA4") (pintype "bidirectional")
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_poly (pts
            (xy 0.35 -0.000711)
            (xy 0.299289 0.05)
            (xy -0.35 0.05)
            (xy -0.35 -0.05)
            (xy 0.35 -0.05)
          ) (width 0.1) (fill yes))
      ))
    (pad "6" smd custom (at -0.8 1.45 270) (size 0.143431 0.143431) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 51 "/04") (pinfunction "PA5") (pintype "bidirectional")
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_poly (pts
            (xy 0.05 0.35)
            (xy -0.05 0.35)
            (xy -0.05 -0.299289)
            (xy 0.000711 -0.35)
            (xy 0.05 -0.35)
          ) (width 0.1) (fill yes))
      ))
    (pad "7" smd roundrect (at -0.4 1.45 270) (size 0.2 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 50 "/03") (pinfunction "PA6") (pintype "bidirectional"))
    (pad "8" smd roundrect (at 0 1.45 270) (size 0.2 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 49 "/02") (pinfunction "PA7") (pintype "bidirectional"))
    (pad "9" smd roundrect (at 0.4 1.45 270) (size 0.2 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 48 "/01") (pinfunction "PB5") (pintype "bidirectional"))
    (pad "10" smd custom (at 0.8 1.45 270) (size 0.143431 0.143431) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 94 "unconnected-(U2-Pad10)") (pinfunction "PB4") (pintype "bidirectional+no_connect")
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_poly (pts
            (xy 0.05 -0.299289)
            (xy 0.05 0.35)
            (xy -0.05 0.35)
            (xy -0.05 -0.35)
            (xy -0.000711 -0.35)
          ) (width 0.1) (fill yes))
      ))
    (pad "11" smd custom (at 1.45 0.8 270) (size 0.143431 0.143431) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 13 "/SCK") (pinfunction "PB3") (pintype "bidirectional")
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_poly (pts
            (xy 0.35 0.05)
            (xy -0.299289 0.05)
            (xy -0.35 -0.000711)
            (xy -0.35 -0.05)
            (xy 0.35 -0.05)
          ) (width 0.1) (fill yes))
      ))
    (pad "12" smd roundrect (at 1.45 0.4 270) (size 0.8 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 96 "unconnected-(U2-Pad12)") (pinfunction "PB2") (pintype "bidirectional+no_connect"))
    (pad "13" smd roundrect (at 1.45 0 270) (size 0.8 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 39 "/SDA") (pinfunction "PB1") (pintype "bidirectional"))
    (pad "14" smd roundrect (at 1.45 -0.4 270) (size 0.8 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 32 "/SCL") (pinfunction "PB0") (pintype "bidirectional"))
    (pad "15" smd custom (at 1.45 -0.8 270) (size 0.143431 0.143431) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 97 "unconnected-(U2-Pad15)") (pinfunction "PC0") (pintype "bidirectional+no_connect")
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_poly (pts
            (xy 0.35 0.05)
            (xy -0.35 0.05)
            (xy -0.35 0.000711)
            (xy -0.299289 -0.05)
            (xy 0.35 -0.05)
          ) (width 0.1) (fill yes))
      ))
    (pad "16" smd custom (at 0.8 -1.45 270) (size 0.143431 0.143431) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 98 "unconnected-(U2-Pad16)") (pinfunction "PC1") (pintype "bidirectional+no_connect")
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_poly (pts
            (xy 0.05 0.299289)
            (xy -0.000711 0.35)
            (xy -0.05 0.35)
            (xy -0.05 -0.35)
            (xy 0.05 -0.35)
          ) (width 0.1) (fill yes))
      ))
    (pad "17" smd roundrect (at 0.4 -1.45 270) (size 0.2 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 99 "unconnected-(U2-Pad17)") (pinfunction "PC2") (pintype "bidirectional"))
    (pad "18" smd roundrect (at 0 -1.45 270) (size 0.2 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 100 "unconnected-(U2-Pad18)") (pinfunction "PC3") (pintype "bidirectional"))
    (pad "19" smd roundrect (at -0.4 -1.45 270) (size 0.2 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 46 "/UDP0") (pinfunction "~{RESET}/PA0") (pintype "bidirectional"))
    (pad "20" smd custom (at -0.8 -1.45 270) (size 0.143431 0.143431) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 55 "/08") (pinfunction "PA1") (pintype "bidirectional")
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_poly (pts
            (xy 0.05 0.35)
            (xy 0.000711 0.35)
            (xy -0.05 0.299289)
            (xy -0.05 -0.35)
            (xy 0.05 -0.35)
          ) (width 0.1) (fill yes))
      ))
    (pad "21" smd rect (at 0 0 270) (size 1.7 1.7) (layers "F.Cu" "F.Mask")
      (net 1 "GND") (pinfunction "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Package_DFN_QFN.3dshapes/VQFN-20-1EP_3x3mm_P0.4mm_EP1.7x1.7mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "footprints:MEC8-113-CARD_2outline" locked (layer "F.Cu")
    (tedit 637EA855)
    (at 116.459 120 90)
    (property "Sheetfile" "Board RPB30 SAM51 SeeSaw.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "CardOutline1" (at 4.375 -1.25 90) (layer "F.Fab"))
    (fp_text value "SYM_Arrow_Large" (at 10.9 -1 90) (layer "F.Fab"))
  )
  (footprint "footprints:MEC8-113-CARD_2outline" locked (layer "F.Cu")
    (tedit 637EA855)
    (at 116.5 97.75 90)
    (property "Sheetfile" "Board RPB30 SAM51 SeeSaw.kicad_sch")
    (property "Sheetname" "")
    (clearance 0.1016)
    (attr through_hole)
    (fp_text reference "CardOutline2" (at 4.375 -1.25 90) (layer "F.Fab"))
    (fp_text value "SYM_Arrow_Large" (at 10.9 -1 90) (layer "F.Fab"))
  )
  (footprint "footprints:PinHeader_1x04_P2.54mm_Vertical" locked (layer "F.Cu")
    (tedit 63CC6AF2)
    (at 156 124.25)
    (descr "Through hole straight pin header, 1x04, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x04 2.54mm single row")
    (property "Sheetfile" "Board RPB30 SAM51 SeeSaw.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J3" (at 0 -2.33) (layer "F.Fab"))
    (fp_text value "I2C" (at -0.022 9.294) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 3.81 90) (layer "F.Fab"))
    (pad "1" thru_hole rect locked (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval locked (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 10 "+3V3") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval locked (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 32 "/SCL") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval locked (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 39 "/SDA") (pinfunction "Pin_4") (pintype "passive"))
    (model "${KIPRJMOD}/3D/OLED_0.91_128x32.stp"
      (offset (xyz -17.5 -3.75 2.5))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (footprint "footprints:C_0603" (layer "F.Cu")
    (tedit 59958EE7)
    (at 131.75 93.75)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (property "Sheetfile" "Board RPB30 SAM51 SeeSaw.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C3" (at 0 -1.5) (layer "F.Fab"))
    (fp_text value "0.1uF" (at 0 -1.294) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect (at -0.75 0) (size 0.8 0.75) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 10 "+3V3") (pintype "passive"))
    (pad "2" smd rect (at 0.75 0) (size 0.8 0.75) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pintype "passive"))
    (model "Capacitors_SMD.3dshapes/C_0603.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_DFN_QFN:VQFN-20-1EP_3x3mm_P0.4mm_EP1.7x1.7mm" (layer "F.Cu")
    (tedit 5DC5F6A8)
    (at 132 81.575 -90)
    (descr "VQFN, 20 Pin (http://ww1.microchip.com/downloads/en/DeviceDoc/20%20Lead%20VQFN%203x3x0_9mm_1_7EP%20U2B%20C04-21496a.pdf), generated with kicad-footprint-generator ipc_noLead_generator.py")
    (tags "VQFN NoLead")
    (property "Sheetfile" "Board RPB30 SAM51 SeeSaw.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "U4" (at 0 -2.8 -90) (layer "F.SilkS"))
    (fp_text value "ATtiny816-M" (at 0 2.8 -90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 -90) (layer "F.Fab"))
    (pad "" smd roundrect (at -0.425 0.425 270) (size 0.69 0.69) (layers "F.Paste") (roundrect_rratio 0.25))
    (pad "" smd roundrect (at -0.425 -0.425 270) (size 0.69 0.69) (layers "F.Paste") (roundrect_rratio 0.25))
    (pad "" smd roundrect (at 0.425 -0.425 270) (size 0.69 0.69) (layers "F.Paste") (roundrect_rratio 0.25))
    (pad "" smd roundrect (at 0.425 0.425 270) (size 0.69 0.69) (layers "F.Paste") (roundrect_rratio 0.25))
    (pad "1" smd custom (at -1.45 -0.8 270) (size 0.143431 0.143431) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 114 "unconnected-(U4-Pad1)") (pinfunction "PA2") (pintype "bidirectional")
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_poly (pts
            (xy 0.35 0.000711)
            (xy 0.35 0.05)
            (xy -0.35 0.05)
            (xy -0.35 -0.05)
            (xy 0.299289 -0.05)
          ) (width 0.1) (fill yes))
      ))
    (pad "2" smd roundrect (at -1.45 -0.4 270) (size 0.8 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 113 "unconnected-(U4-Pad2)") (pinfunction "PA3") (pintype "bidirectional"))
    (pad "3" smd roundrect (at -1.45 0 270) (size 0.8 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "4" smd roundrect (at -1.45 0.4 270) (size 0.8 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 10 "+3V3") (pinfunction "VCC") (pintype "power_in"))
    (pad "5" smd custom (at -1.45 0.8 270) (size 0.143431 0.143431) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 112 "unconnected-(U4-Pad5)") (pinfunction "PA4") (pintype "bidirectional")
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_poly (pts
            (xy 0.35 -0.000711)
            (xy 0.299289 0.05)
            (xy -0.35 0.05)
            (xy -0.35 -0.05)
            (xy 0.35 -0.05)
          ) (width 0.1) (fill yes))
      ))
    (pad "6" smd custom (at -0.8 1.45 270) (size 0.143431 0.143431) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 68 "/20") (pinfunction "PA5") (pintype "bidirectional")
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_poly (pts
            (xy 0.05 0.35)
            (xy -0.05 0.35)
            (xy -0.05 -0.299289)
            (xy 0.000711 -0.35)
            (xy 0.05 -0.35)
          ) (width 0.1) (fill yes))
      ))
    (pad "7" smd roundrect (at -0.4 1.45 270) (size 0.2 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 69 "/19") (pinfunction "PA6") (pintype "bidirectional"))
    (pad "8" smd roundrect (at 0 1.45 270) (size 0.2 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 70 "/18") (pinfunction "PA7") (pintype "bidirectional"))
    (pad "9" smd roundrect (at 0.4 1.45 270) (size 0.2 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 71 "/17") (pinfunction "PB5") (pintype "bidirectional"))
    (pad "10" smd custom (at 0.8 1.45 270) (size 0.143431 0.143431) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 111 "unconnected-(U4-Pad10)") (pinfunction "PB4") (pintype "bidirectional+no_connect")
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_poly (pts
            (xy 0.05 -0.299289)
            (xy 0.05 0.35)
            (xy -0.05 0.35)
            (xy -0.05 -0.35)
            (xy -0.000711 -0.35)
          ) (width 0.1) (fill yes))
      ))
    (pad "11" smd custom (at 1.45 0.8 270) (size 0.143431 0.143431) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 15 "/MISO") (pinfunction "PB3") (pintype "bidirectional")
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_poly (pts
            (xy 0.35 0.05)
            (xy -0.299289 0.05)
            (xy -0.35 -0.000711)
            (xy -0.35 -0.05)
            (xy 0.35 -0.05)
          ) (width 0.1) (fill yes))
      ))
    (pad "12" smd roundrect (at 1.45 0.4 270) (size 0.8 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 110 "unconnected-(U4-Pad12)") (pinfunction "PB2") (pintype "bidirectional+no_connect"))
    (pad "13" smd roundrect (at 1.45 0 270) (size 0.8 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 39 "/SDA") (pinfunction "PB1") (pintype "bidirectional"))
    (pad "14" smd roundrect (at 1.45 -0.4 270) (size 0.8 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 32 "/SCL") (pinfunction "PB0") (pintype "bidirectional"))
    (pad "15" smd custom (at 1.45 -0.8 270) (size 0.143431 0.143431) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 109 "unconnected-(U4-Pad15)") (pinfunction "PC0") (pintype "bidirectional+no_connect")
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_poly (pts
            (xy 0.35 0.05)
            (xy -0.35 0.05)
            (xy -0.35 0.000711)
            (xy -0.299289 -0.05)
            (xy 0.35 -0.05)
          ) (width 0.1) (fill yes))
      ))
    (pad "16" smd custom (at 0.8 -1.45 270) (size 0.143431 0.143431) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 108 "unconnected-(U4-Pad16)") (pinfunction "PC1") (pintype "bidirectional+no_connect")
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_poly (pts
            (xy 0.05 0.299289)
            (xy -0.000711 0.35)
            (xy -0.05 0.35)
            (xy -0.05 -0.35)
            (xy 0.05 -0.35)
          ) (width 0.1) (fill yes))
      ))
    (pad "17" smd roundrect (at 0.4 -1.45 270) (size 0.2 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 107 "unconnected-(U4-Pad17)") (pinfunction "PC2") (pintype "bidirectional+no_connect"))
    (pad "18" smd roundrect (at 0 -1.45 270) (size 0.2 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pinfunction "PC3") (pintype "bidirectional"))
    (pad "19" smd roundrect (at -0.4 -1.45 270) (size 0.2 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 89 "/UDP2") (pinfunction "~{RESET}/PA0") (pintype "bidirectional"))
    (pad "20" smd custom (at -0.8 -1.45 270) (size 0.143431 0.143431) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 106 "unconnected-(U4-Pad20)") (pinfunction "PA1") (pintype "bidirectional")
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_poly (pts
            (xy 0.05 0.35)
            (xy 0.000711 0.35)
            (xy -0.05 0.299289)
            (xy -0.05 -0.35)
            (xy 0.05 -0.35)
          ) (width 0.1) (fill yes))
      ))
    (pad "21" smd rect (at 0 0 270) (size 1.7 1.7) (layers "F.Cu" "F.Mask")
      (net 1 "GND") (pinfunction "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Package_DFN_QFN.3dshapes/VQFN-20-1EP_3x3mm_P0.4mm_EP1.7x1.7mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_DFN_QFN:VQFN-20-1EP_3x3mm_P0.4mm_EP1.7x1.7mm" (layer "F.Cu")
    (tedit 5DC5F6A8)
    (at 132 119 -90)
    (descr "VQFN, 20 Pin (http://ww1.microchip.com/downloads/en/DeviceDoc/20%20Lead%20VQFN%203x3x0_9mm_1_7EP%20U2B%20C04-21496a.pdf), generated with kicad-footprint-generator ipc_noLead_generator.py")
    (tags "VQFN NoLead")
    (property "Sheetfile" "Board RPB30 SAM51 SeeSaw.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "U6" (at 0 -2.8 -90) (layer "F.SilkS"))
    (fp_text value "ATtiny816-M" (at 0 2.8 -90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 -90) (layer "F.Fab"))
    (pad "" smd roundrect (at -0.425 0.425 270) (size 0.69 0.69) (layers "F.Paste") (roundrect_rratio 0.25))
    (pad "" smd roundrect (at 0.425 0.425 270) (size 0.69 0.69) (layers "F.Paste") (roundrect_rratio 0.25))
    (pad "" smd roundrect (at -0.425 -0.425 270) (size 0.69 0.69) (layers "F.Paste") (roundrect_rratio 0.25))
    (pad "" smd roundrect (at 0.425 -0.425 270) (size 0.69 0.69) (layers "F.Paste") (roundrect_rratio 0.25))
    (pad "1" smd custom (at -1.45 -0.8 270) (size 0.143431 0.143431) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 85 "/35") (pinfunction "PA2") (pintype "bidirectional")
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_poly (pts
            (xy 0.35 0.000711)
            (xy 0.35 0.05)
            (xy -0.35 0.05)
            (xy -0.35 -0.05)
            (xy 0.299289 -0.05)
          ) (width 0.1) (fill yes))
      ))
    (pad "2" smd roundrect (at -1.45 -0.4 270) (size 0.8 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 86 "/34") (pinfunction "PA3") (pintype "bidirectional"))
    (pad "3" smd roundrect (at -1.45 0 270) (size 0.8 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "4" smd roundrect (at -1.45 0.4 270) (size 0.8 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 10 "+3V3") (pinfunction "VCC") (pintype "power_in"))
    (pad "5" smd custom (at -1.45 0.8 270) (size 0.143431 0.143431) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 87 "/33") (pinfunction "PA4") (pintype "bidirectional")
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_poly (pts
            (xy 0.35 -0.000711)
            (xy 0.299289 0.05)
            (xy -0.35 0.05)
            (xy -0.35 -0.05)
            (xy 0.35 -0.05)
          ) (width 0.1) (fill yes))
      ))
    (pad "6" smd custom (at -0.8 1.45 270) (size 0.143431 0.143431) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 79 "/32") (pinfunction "PA5") (pintype "bidirectional")
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_poly (pts
            (xy 0.05 0.35)
            (xy -0.05 0.35)
            (xy -0.05 -0.299289)
            (xy 0.000711 -0.35)
            (xy 0.05 -0.35)
          ) (width 0.1) (fill yes))
      ))
    (pad "7" smd roundrect (at -0.4 1.45 270) (size 0.2 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 78 "/31") (pinfunction "PA6") (pintype "bidirectional"))
    (pad "8" smd roundrect (at 0 1.45 270) (size 0.2 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 77 "/30") (pinfunction "PA7") (pintype "bidirectional"))
    (pad "9" smd roundrect (at 0.4 1.45 270) (size 0.2 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 76 "/29") (pinfunction "PB5") (pintype "bidirectional"))
    (pad "10" smd custom (at 0.8 1.45 270) (size 0.143431 0.143431) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 125 "unconnected-(U6-Pad10)") (pinfunction "PB4") (pintype "bidirectional+no_connect")
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_poly (pts
            (xy 0.05 -0.299289)
            (xy 0.05 0.35)
            (xy -0.05 0.35)
            (xy -0.05 -0.35)
            (xy -0.000711 -0.35)
          ) (width 0.1) (fill yes))
      ))
    (pad "11" smd custom (at 1.45 0.8 270) (size 0.143431 0.143431) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 4 "/D8") (pinfunction "PB3") (pintype "bidirectional")
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_poly (pts
            (xy 0.35 0.05)
            (xy -0.299289 0.05)
            (xy -0.35 -0.000711)
            (xy -0.35 -0.05)
            (xy 0.35 -0.05)
          ) (width 0.1) (fill yes))
      ))
    (pad "12" smd roundrect (at 1.45 0.4 270) (size 0.8 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 124 "unconnected-(U6-Pad12)") (pinfunction "PB2") (pintype "bidirectional+no_connect"))
    (pad "13" smd roundrect (at 1.45 0 270) (size 0.8 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 39 "/SDA") (pinfunction "PB1") (pintype "bidirectional"))
    (pad "14" smd roundrect (at 1.45 -0.4 270) (size 0.8 0.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 32 "/SCL") (pinfunction "PB0") (pintype "bidirectional"))
    (pad "15" smd custom (at 1.45 -0.8 270) (size 0.143431 0.143431) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 123 "unconnected-(U6-Pad15)") (pinfunction "PC0") (pintype "bidirectional+no_connect")
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_poly (pts
            (xy 0.35 0.05)
            (xy -0.35 0.05)
            (xy -0.35 0.000711)
            (xy -0.299289 -0.05)
            (xy 0.35 -0.05)
          ) (width 0.1) (fill yes))
      ))
    (pad "16" smd custom (at 0.8 -1.45 270) (size 0.143431 0.143431) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 122 "unconnected-(U6-Pad16)") (pinfunction "PC1") (pintype "bidirectional+no_connect")
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_poly (pts
            (xy 0.05 0.299289)
            (xy -0.000711 0.35)
            (xy -0.05 0.35)
            (xy -0.05 -0.35)
            (xy 0.05 -0.35)
          ) (width 0.1) (fill yes))
      ))
    (pad "17" smd roundrect (at 0.4 -1.45 270) (size 0.2 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pinfunction "PC2") (pintype "bidirectional"))
    (pad "18" smd roundrect (at 0 -1.45 270) (size 0.2 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 121 "unconnected-(U6-Pad18)") (pinfunction "PC3") (pintype "bidirectional+no_connect"))
    (pad "19" smd roundrect (at -0.4 -1.45 270) (size 0.2 0.8) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 91 "/UDP4") (pinfunction "~{RESET}/PA0") (pintype "bidirectional"))
    (pad "20" smd custom (at -0.8 -1.45 270) (size 0.143431 0.143431) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 84 "/36") (pinfunction "PA1") (pintype "bidirectional")
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_poly (pts
            (xy 0.05 0.35)
            (xy 0.000711 0.35)
            (xy -0.05 0.299289)
            (xy -0.05 -0.35)
            (xy 0.05 -0.35)
          ) (width 0.1) (fill yes))
      ))
    (pad "21" smd rect (at 0 0 270) (size 1.7 1.7) (layers "F.Cu" "F.Mask")
      (net 1 "GND") (pinfunction "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Package_DFN_QFN.3dshapes/VQFN-20-1EP_3x3mm_P0.4mm_EP1.7x1.7mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "footprints:C_0603" (layer "F.Cu")
    (tedit 59958EE7)
    (at 131.75 78.75)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (property "Sheetfile" "Board RPB30 SAM51 SeeSaw.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C4" (at 0 -1.5) (layer "F.Fab"))
    (fp_text value "0.1uF" (at 0 -1.28) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect (at -0.75 0) (size 0.8 0.75) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 10 "+3V3") (pintype "passive"))
    (pad "2" smd rect (at 0.75 0) (size 0.8 0.75) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pintype "passive"))
    (model "Capacitors_SMD.3dshapes/C_0603.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "footprints:C_0603" (layer "F.Cu")
    (tedit 59958EE7)
    (at 113.5 123.5 90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (property "Sheetfile" "Board RPB30 SAM51 SeeSaw.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C10" (at 0 -1.5 90) (layer "F.Fab"))
    (fp_text value "1uF" (at 0 1.5 90) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd rect (at -0.75 0 90) (size 0.8 0.75) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pintype "passive"))
    (pad "2" smd rect (at 0.75 0 90) (size 0.8 0.75) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 10 "+3V3") (pintype "passive"))
    (model "${KIPRJMOD}/3D/C_0603_1608Metric.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "footprints:C_0603" (layer "F.Cu")
    (tedit 59958EE7)
    (at 127.75 123.5 -90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (property "Sheetfile" "Board RPB30 SAM51 SeeSaw.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C12" (at 0 -1.5 90) (layer "F.Fab"))
    (fp_text value "1uF" (at 0 1.5 90) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd rect (at -0.75 0 270) (size 0.8 0.75) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pintype "passive"))
    (pad "2" smd rect (at 0.75 0 270) (size 0.8 0.75) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 10 "+3V3") (pintype "passive"))
    (model "${KIPRJMOD}/3D/C_0603_1608Metric.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "footprints:R_0603" (layer "F.Cu")
    (tedit 636FC042)
    (at 151.25 87 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (property "Sheetfile" "Board RPB30 SAM51 SeeSaw.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R14" (at 1.905 0) (layer "Dwgs.User"))
    (fp_text value "100K" (at -3.05 0.05) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect locked (at -0.75 0 180) (size 0.5 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 10 "+3V3") (pintype "passive"))
    (pad "2" smd rect locked (at 0.75 0 180) (size 0.5 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 31 "/QSPI_CS") (pintype "passive"))
    (model "${KIPRJMOD}/3D/R_0603_1608Metric.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "footprints:TestPoint_Pad_D0.6mm" (layer "F.Cu")
    (tedit 5A0F774F)
    (at 156 97.05)
    (descr "SMD pad as test Point, diameter 1.0mm")
    (tags "test point SMD pad")
    (property "Sheetfile" "Board RPB30 SAM51 SeeSaw.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "TP5" (at 0 -1.448) (layer "User.1") hide)
    (fp_text value "D2" (at 1 0) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 -1.45) (layer "F.Fab") hide)
    (pad "1" smd circle (at 0 0) (size 0.6 0.6) (layers "F.Cu" "F.Mask")
      (net 139 "/D2") (pinfunction "1") (pintype "passive"))
  )
  (footprint "footprints:LED_0603" (layer "F.Cu")
    (tedit 636FBDBF)
    (at 168.402 122.428)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (property "Sheetfile" "Board RPB30 SAM51 SeeSaw.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "D11" (at 2.032 0) (layer "F.SilkS") hide)
    (fp_text value "D11" (at -2.286 0 -90 unlocked) (layer "F.SilkS"))
    (pad "1" smd rect locked (at -0.8 0 180) (size 0.8 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 24 "Net-(D11-Pad1)") (pinfunction "K") (pintype "passive"))
    (pad "2" smd rect locked (at 0.8 0 180) (size 0.8 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 35 "/D11") (pinfunction "A") (pintype "passive"))
    (model "${KIPRJMOD}/3D/LED_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "footprints:TestPoint_Pad_D0.6mm" (layer "F.Cu")
    (tedit 5A0F774F)
    (at 145 100.35)
    (descr "SMD pad as test Point, diameter 1.0mm")
    (tags "test point SMD pad")
    (property "Sheetfile" "Board RPB30 SAM51 SeeSaw.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "TP3" (at 0 -1.448) (layer "User.1") hide)
    (fp_text value "D1" (at -0.85 0) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 -1.45) (layer "F.Fab") hide)
    (pad "1" smd circle (at 0 0) (size 0.6 0.6) (layers "F.Cu" "F.Mask")
      (net 138 "/TX_D1") (pinfunction "1") (pintype "passive"))
  )
  (footprint "footprints:SOT-23-5" (layer "F.Cu")
    (tedit 58CE4E7E)
    (at 110.5 120.75 -90)
    (descr "5-pin SOT23 package")
    (tags "SOT-23-5")
    (property "Sheetfile" "Board RPB30 SAM51 SeeSaw.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "U1" (at 0.15 -0.2 180) (layer "F.SilkS"))
    (fp_text value "AP2127K" (at 0 2.9 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect locked (at -1.1 -0.95 270) (size 1.06 0.65) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 17 "Net-(C1-Pad2)") (pinfunction "VIN") (pintype "power_in"))
    (pad "2" smd rect locked (at -1.1 0 270) (size 1.06 0.65) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "3" smd rect locked (at -1.1 0.95 270) (size 1.06 0.65) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 29 "Net-(R8-Pad1)") (pinfunction "EN") (pintype "input"))
    (pad "4" smd rect locked (at 1.1 0.95 270) (size 1.06 0.65) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 141 "unconnected-(U1-Pad4)") (pinfunction "NC") (pintype "no_connect"))
    (pad "5" smd rect locked (at 1.1 -0.95 270) (size 1.06 0.65) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 10 "+3V3") (pinfunction "VOUT") (pintype "power_out"))
    (model "${KISYS3DMOD}/TO_SOT_Packages_SMD.3dshapes/SOT-23-5.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "footprints:R_0603" (layer "F.Cu")
    (tedit 636FC042)
    (at 110 85.25)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (property "Sheetfile" "Board RPB30 SAM51 SeeSaw.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R9" (at 1.905 0 180) (layer "Dwgs.User"))
    (fp_text value "1K" (at -1.905 0 180) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 180) (layer "F.Fab"))
    (pad "1" smd rect locked (at -0.75 0) (size 0.5 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 22 "Net-(D2-Pad1)") (pintype "passive"))
    (pad "2" smd rect locked (at 0.75 0) (size 0.5 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pintype "passive"))
    (model "${KIPRJMOD}/3D/R_0603_1608Metric.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "footprints:SK9822_ADA" (layer "F.Cu")
    (tedit 0)
    (at 110 109.75 -90)
    (tags "2343 ")
    (property "Sheetfile" "Board RPB30 SAM51 SeeSaw.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "RGB1" (at 0 0 unlocked) (layer "F.SilkS"))
    (fp_text value "DOTSTAR" (at -3.959 -0.109 unlocked) (layer "F.SilkS"))
    (fp_text user "*" (at -2.6416 -3.390701 90) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0 -90 unlocked) (layer "F.Fab"))
    (fp_text user "*" (at -1.8796 -2.641401 90) (layer "F.Fab"))
    (pad "1" smd rect (at -2.3876 -1.599999 270) (size 1.3462 1.0414) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 33 "/DS_DATA") (pinfunction "SDI") (pintype "input"))
    (pad "2" smd rect (at -2.3876 0 270) (size 1.3462 1.0414) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 34 "/DS_CLK") (pinfunction "CKI") (pintype "input"))
    (pad "3" smd rect (at -2.3876 1.599999 270) (size 1.3462 1.0414) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "GND") (pintype "power_out"))
    (pad "4" smd rect (at 2.3876 1.599999 270) (size 1.3462 1.0414) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 10 "+3V3") (pinfunction "VCC") (pintype "power_in"))
    (pad "5" smd rect (at 2.3876 0 270) (size 1.3462 1.0414) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 93 "unconnected-(RGB1-Pad5)") (pinfunction "CKO") (pintype "output+no_connect"))
    (pad "6" smd rect (at 2.3876 -1.599999 270) (size 1.3462 1.0414) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 135 "unconnected-(RGB1-Pad6)") (pinfunction "SDO") (pintype "output+no_connect"))
  )
  (footprint "footprints:C_0805" (layer "F.Cu")
    (tedit 636FC0BD)
    (at 110.75 115)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (property "Sheetfile" "Board RPB30 SAM51 SeeSaw.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C1" (at 0.05 0.05) (layer "F.SilkS") hide)
    (fp_text value "10uF" (at 0.2 -1.45) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 -1.5) (layer "F.Fab"))
    (pad "1" smd rect locked (at -1 0) (size 1 1.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pintype "passive"))
    (pad "2" smd rect locked (at 1 0) (size 1 1.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 17 "Net-(C1-Pad2)") (pintype "passive"))
    (model "${KIPRJMOD}/3D/C_0805_2012Metric.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "footprints:C_0603" (layer "F.Cu")
    (tedit 59958EE7)
    (at 113.5 120.384 -90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (property "Sheetfile" "Board RPB30 SAM51 SeeSaw.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C11" (at 0 -1.5 90) (layer "F.Fab"))
    (fp_text value "0.1uF" (at -0.184 -1.5 90) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd rect (at -0.75 0 270) (size 0.8 0.75) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pintype "passive"))
    (pad "2" smd rect (at 0.75 0 270) (size 0.8 0.75) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 10 "+3V3") (pintype "passive"))
    (model "${KIPRJMOD}/3D/C_0603_1608Metric.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "footprints:R_0603" (layer "F.Cu")
    (tedit 636FC042)
    (at 133.5 123.5 -90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (property "Sheetfile" "Board RPB30 SAM51 SeeSaw.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R28" (at 1.905 0 90) (layer "Dwgs.User"))
    (fp_text value "4K7" (at -1.8 -4.6 180) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd rect locked (at -0.75 0 270) (size 0.5 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 32 "/SCL") (pintype "passive"))
    (pad "2" smd rect locked (at 0.75 0 270) (size 0.5 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 10 "+3V3") (pintype "passive"))
    (model "${KIPRJMOD}/3D/R_0603_1608Metric.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "footprints:LED_0603" (layer "F.Cu")
    (tedit 636FBDBF)
    (at 110 87)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (property "Sheetfile" "Board RPB30 SAM51 SeeSaw.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "D2" (at 2.032 0) (layer "F.SilkS") hide)
    (fp_text value "PWR" (at 0 1.45 unlocked) (layer "F.SilkS"))
    (pad "1" smd rect locked (at -0.8 0 180) (size 0.8 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 22 "Net-(D2-Pad1)") (pinfunction "K") (pintype "passive"))
    (pad "2" smd rect locked (at 0.8 0 180) (size 0.8 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 23 "+5V") (pinfunction "A") (pintype "passive"))
    (model "${KIPRJMOD}/3D/LED_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "footprints:C_0603" (layer "F.Cu")
    (tedit 59958EE7)
    (at 148.987 108.839 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (property "Sheetfile" "Board RPB30 SAM51 SeeSaw.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C15" (at 0 -1.5) (layer "F.Fab"))
    (fp_text value "4.7uF" (at -3.613 -0.111) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect (at -0.75 0 180) (size 0.8 0.75) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pintype "passive"))
    (pad "2" smd rect (at 0.75 0 180) (size 0.8 0.75) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 18 "Net-(C15-Pad2)") (pintype "passive"))
    (model "${KIPRJMOD}/3D/C_0603_1608Metric.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "footprints:TestPoint_Pad_D0.6mm" (layer "F.Cu")
    (tedit 5A0F774F)
    (at 145 99.55)
    (descr "SMD pad as test Point, diameter 1.0mm")
    (tags "test point SMD pad")
    (property "Sheetfile" "Board RPB30 SAM51 SeeSaw.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "TP2" (at 0 -1.448) (layer "User.1") hide)
    (fp_text value "D0" (at -0.9 0.05) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 -1.45) (layer "F.Fab") hide)
    (pad "1" smd circle (at 0 0) (size 0.6 0.6) (layers "F.Cu" "F.Mask")
      (net 137 "/RX_D0") (pinfunction "1") (pintype "passive"))
  )
  (footprint "footprints:USB_Micro-B_Molex-105017-0001" (layer "F.Cu")
    (tedit 636FBEAD)
    (at 109.22 100.33 -90)
    (descr "http://www.molex.com/pdm_docs/sd/1050170001_sd.pdf")
    (tags "Micro-USB SMD Typ-B")
    (property "Sheetfile" "Board RPB30 SAM51 SeeSaw.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "J1" (at -0.13 -1.13 90) (layer "F.SilkS"))
    (fp_text value "USB" (at 0.3 3.45 90) (layer "F.Fab"))
    (fp_text user "PCB Edge" (at 0 1.8 90) (layer "Dwgs.User"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd rect locked (at -1.3 -2.35 270) (size 0.4 1.35) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 23 "+5V") (pinfunction "VBUS") (pintype "power_in"))
    (pad "2" smd rect locked (at -0.65 -2.35 270) (size 0.4 1.35) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 21 "/D-") (pinfunction "D-") (pintype "passive"))
    (pad "3" smd rect locked (at 0 -2.35 270) (size 0.4 1.35) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 20 "/D+") (pinfunction "D+") (pintype "passive"))
    (pad "4" smd rect locked (at 0.65 -2.35 270) (size 0.4 1.35) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 148 "unconnected-(J1-Pad4)") (pinfunction "ID") (pintype "passive"))
    (pad "5" smd rect locked (at 1.3 -2.35 270) (size 0.4 1.35) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "6" thru_hole circle locked (at -2.5 -2.35 270) (size 1.45 1.45) (drill 0.85) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "Shield") (pintype "passive"))
    (pad "6" thru_hole oval locked (at -3.5 0.35 90) (size 1.2 1.9) (drill oval 0.6 1.3) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "Shield") (pintype "passive"))
    (pad "6" thru_hole circle locked (at 2.5 -2.35 270) (size 1.45 1.45) (drill 0.85) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "Shield") (pintype "passive"))
    (pad "6" thru_hole oval locked (at 3.5 0.35 270) (size 1.2 1.9) (drill oval 0.6 1.3) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "Shield") (pintype "passive"))
    (pad "6" smd rect locked (at -1 0.35 270) (size 1.5 1.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "Shield") (pintype "passive"))
    (pad "6" smd rect locked (at 1 0.35 270) (size 1.5 1.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "Shield") (pintype "passive"))
    (pad "6" smd rect locked (at 2.9 0.35 270) (size 1.2 1.9) (layers "F.Cu" "F.Mask")
      (net 1 "GND") (pinfunction "Shield") (pintype "passive"))
    (pad "6" smd rect locked (at -2.9 0.35 270) (size 1.2 1.9) (layers "F.Cu" "F.Mask")
      (net 1 "GND") (pinfunction "Shield") (pintype "passive"))
    (model "${KIPRJMOD}/3D/USB_micro_105017-0001.stp"
      (offset (xyz 0 0 1.2))
      (scale (xyz 1 1 1))
      (rotate (xyz -90 0 0))
    )
  )
  (footprint "footprints:TestPoint_Pad_D0.6mm" (layer "F.Cu")
    (tedit 5A0F774F)
    (at 156 98.1)
    (descr "SMD pad as test Point, diameter 1.0mm")
    (tags "test point SMD pad")
    (property "Sheetfile" "Board RPB30 SAM51 SeeSaw.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "TP4" (at 0 -1.448) (layer "User.1") hide)
    (fp_text value "A5" (at 1 0.1) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 -1.45) (layer "F.Fab") hide)
    (pad "1" smd circle (at 0 0) (size 0.6 0.6) (layers "F.Cu" "F.Mask")
      (net 12 "/A5") (pinfunction "1") (pintype "passive"))
  )
  (footprint "footprints:SOP-8_3.9x4.9mm_P1.27mm" (layer "F.Cu")
    (tedit 5D9F72B1)
    (at 150.75 91.75)
    (descr "SOP, 8 Pin (http://www.macronix.com/Lists/Datasheet/Attachments/7534/MX25R3235F,%20Wide%20Range,%2032Mb,%20v1.6.pdf#page=79), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOP SO")
    (property "Footprint_1" "")
    (property "MPN" "GD25Q16CTIGR")
    (property "Sheetfile" "Board RPB30 SAM51 SeeSaw.kicad_sch")
    (property "Sheetname" "")
    (property "Value_1" "GD25x16")
    (attr smd)
    (fp_text reference "U11" (at 0 0) (layer "F.Fab"))
    (fp_text value "GD25x16" (at 0 3.4) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2.625 -1.905) (size 1.65 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 31 "/QSPI_CS") (pinfunction "SSEL") (pintype "bidirectional"))
    (pad "2" smd roundrect (at -2.625 -0.635) (size 1.65 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 143 "/QSPI_DATA_1") (pinfunction "MISO") (pintype "bidirectional"))
    (pad "3" smd roundrect (at -2.625 0.635) (size 1.65 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 144 "/QSPI_DATA_2") (pinfunction "WP#/IO2") (pintype "bidirectional"))
    (pad "4" smd roundrect (at -2.625 1.905) (size 1.65 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pinfunction "VSS") (pintype "bidirectional"))
    (pad "5" smd roundrect (at 2.625 1.905) (size 1.65 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 142 "/QSPI_DATA_0") (pinfunction "MOSI") (pintype "bidirectional"))
    (pad "6" smd roundrect (at 2.625 0.635) (size 1.65 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 146 "/QSPI_SCK") (pinfunction "SCK") (pintype "bidirectional"))
    (pad "7" smd roundrect (at 2.625 -0.635) (size 1.65 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 145 "/QSPI_DATA_3") (pinfunction "HOLD#/IO3") (pintype "bidirectional"))
    (pad "8" smd roundrect (at 2.625 -1.905) (size 1.65 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 10 "+3V3") (pinfunction "VCC") (pintype "bidirectional"))
    (model "${KICAD6_3DMODEL_DIR}/Package_SO.3dshapes/SOIC-8_3.9x4.9mm_P1.27mm.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "footprints:TestPoint_Pad_D0.6mm" (layer "F.Cu")
    (tedit 5A0F774F)
    (at 145 98.1)
    (descr "SMD pad as test Point, diameter 1.0mm")
    (tags "test point SMD pad")
    (property "Sheetfile" "Board RPB30 SAM51 SeeSaw.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "TP6" (at 0 -1.448) (layer "User.1") hide)
    (fp_text value "A0/D5" (at -1.8 -0.25) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 -1.45) (layer "F.Fab") hide)
    (pad "1" smd circle (at 0 0) (size 0.6 0.6) (layers "F.Cu" "F.Mask")
      (net 140 "/A0{slash}D5") (pinfunction "1") (pintype "passive"))
  )
  (footprint "footprints:TestPoint_Pad_D0.6mm" (layer "F.Cu")
    (tedit 5A0F774F)
    (at 144.25 106.5)
    (descr "SMD pad as test Point, diameter 1.0mm")
    (tags "test point SMD pad")
    (property "Sheetfile" "Board RPB30 SAM51 SeeSaw.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "TP1" (at 0 -1.448) (layer "User.1") hide)
    (fp_text value "3V3" (at -1.15 0.05) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 -1.45) (layer "F.Fab") hide)
    (pad "1" smd circle (at 0 0) (size 0.6 0.6) (layers "F.Cu" "F.Mask")
      (net 10 "+3V3") (pinfunction "1") (pintype "passive"))
  )
  (footprint "footprints:C_0805" (layer "F.Cu")
    (tedit 636FC0BD)
    (at 110.5 124 180)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (property "Sheetfile" "Board RPB30 SAM51 SeeSaw.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C9" (at 0 -1.5) (layer "F.SilkS"))
    (fp_text value "10uF" (at 0 1.75) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -1.5) (layer "F.Fab"))
    (pad "1" smd rect locked (at -1 0 180) (size 1 1.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pintype "passive"))
    (pad "2" smd rect locked (at 1 0 180) (size 1 1.25) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 10 "+3V3") (pintype "passive"))
    (model "${KIPRJMOD}/3D/C_0805_2012Metric.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "footprints:Digiroy" (layer "F.Cu")
    (tedit 0)
    (at 137.25 96.75 180)
    (attr board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "G***" (at 0 0) (layer "B.SilkS") hide)
    (fp_text value "LOGO" (at 0.75 0) (layer "B.SilkS") hide)
  )
  (footprint "footprints:R_0603" (layer "F.Cu")
    (tedit 636FC042)
    (at 122.5 128.954 90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (property "Sheetfile" "Board RPB30 SAM51 SeeSaw.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R13" (at 1.905 0 90) (layer "Dwgs.User"))
    (fp_text value "0" (at -1.905 0 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd rect locked (at -0.75 0 90) (size 0.5 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 30 "VBUS") (pintype "passive"))
    (pad "2" smd rect locked (at 0.75 0 90) (size 0.5 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 10 "+3V3") (pintype "passive"))
    (model "${KIPRJMOD}/3D/R_0603_1608Metric.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "footprints:Jumper" (layer "F.Cu")
    (tedit 5B6DD72B)
    (at 136.7 125.82)
    (property "Sheetfile" "Board RPB30 SAM51 SeeSaw.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "A1" (at 1.6 0.03) (layer "F.SilkS"))
    (fp_text value "Jumper" (at 0 1.25) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -1.2) (layer "F.Fab"))
    (pad "1" smd rect locked (at -0.3 0) (size 0.4 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "Net-(A1-Pad1)") (pinfunction "A") (pintype "passive"))
    (pad "2" smd rect locked (at 0.3 0) (size 0.4 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 10 "+3V3") (pinfunction "B") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0402.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "footprints:L_0805_2012Metric" (layer "F.Cu")
    (tedit 5F68FEF0)
    (at 149.9405 110.95)
    (descr "Inductor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 80, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "inductor")
    (property "Sheetfile" "Board RPB30 SAM51 SeeSaw.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "L1" (at -2.5905 -0.1154) (layer "F.SilkS") hide)
    (fp_text value "10uH" (at 3.1595 0.0346) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.0625 0) (size 0.875 1.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 18 "Net-(C15-Pad2)") (pinfunction "1") (pintype "passive"))
    (pad "2" smd roundrect (at 1.0625 0) (size 0.875 1.2) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 28 "Net-(L1-Pad2)") (pinfunction "2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "footprints:R_0603" (layer "F.Cu")
    (tedit 636FC042)
    (at 110.5 117.5)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (property "Sheetfile" "Board RPB30 SAM51 SeeSaw.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R8" (at 1.905 0 180) (layer "Dwgs.User"))
    (fp_text value "100K" (at 2.9 0.15 180) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0 180) (layer "F.Fab"))
    (pad "1" smd rect locked (at -0.75 0) (size 0.5 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 29 "Net-(R8-Pad1)") (pintype "passive"))
    (pad "2" smd rect locked (at 0.75 0) (size 0.5 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 17 "Net-(C1-Pad2)") (pintype "passive"))
    (model "${KIPRJMOD}/3D/R_0603_1608Metric.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "footprints:R_0603" (layer "F.Cu")
    (tedit 636FC042)
    (at 165.5 124.4)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (property "Sheetfile" "Board RPB30 SAM51 SeeSaw.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R10" (at 1.905 0 180) (layer "Dwgs.User"))
    (fp_text value "1K" (at -1.905 0 180) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 180) (layer "F.Fab"))
    (pad "1" smd rect locked (at -0.75 0) (size 0.5 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pintype "passive"))
    (pad "2" smd rect locked (at 0.75 0) (size 0.5 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 25 "Net-(D13-Pad1)") (pintype "passive"))
    (model "${KIPRJMOD}/3D/R_0603_1608Metric.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "footprints:R_0603" (layer "F.Cu")
    (tedit 636FC042)
    (at 131.5 123.5 -90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (property "Sheetfile" "Board RPB30 SAM51 SeeSaw.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R27" (at 1.905 0 90) (layer "Dwgs.User"))
    (fp_text value "4K7" (at -1.905 0 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd rect locked (at -0.75 0 270) (size 0.5 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 39 "/SDA") (pintype "passive"))
    (pad "2" smd rect locked (at 0.75 0 270) (size 0.5 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 10 "+3V3") (pintype "passive"))
    (model "${KIPRJMOD}/3D/R_0603_1608Metric.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "footprints:C_0603" (layer "F.Cu")
    (tedit 59958EE7)
    (at 156.21 104.001 -90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (property "Sheetfile" "Board RPB30 SAM51 SeeSaw.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C14" (at 0 -1.5 90) (layer "F.Fab"))
    (fp_text value "1uF" (at -0.001 -1.04 90) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd rect (at -0.75 0 270) (size 0.8 0.75) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 10 "+3V3") (pintype "passive"))
    (pad "2" smd rect (at 0.75 0 270) (size 0.8 0.75) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 47 "/AREF") (pintype "passive"))
    (model "${KIPRJMOD}/3D/C_0603_1608Metric.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "footprints:R_0805_HandSoldering" (layer "F.Cu")
    (tedit 636FC06B)
    (at 109 92.376 -90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (property "Sheetfile" "Board RPB30 SAM51 SeeSaw.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "F1" (at -3.81 0 90) (layer "F.SilkS") hide)
    (fp_text value "Polyfuse" (at 0.124 -1.55 90) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd rect locked (at -1.35 0 270) (size 1.5 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 23 "+5V") (pintype "passive"))
    (pad "2" smd rect locked (at 1.35 0 270) (size 1.5 1.3) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 17 "Net-(C1-Pad2)") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model "${KIPRJMOD}/3D/R_0805_2012Metric.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "footprints:R_0603" (layer "F.Cu")
    (tedit 636FC042)
    (at 136.5 129.5 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (property "Sheetfile" "Board RPB30 SAM51 SeeSaw.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R17" (at 1.905 0) (layer "Dwgs.User"))
    (fp_text value "10K" (at -2.5 0) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect locked (at -0.75 0 180) (size 0.5 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pintype "passive"))
    (pad "2" smd rect locked (at 0.75 0 180) (size 0.5 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 16 "Net-(A2-Pad1)") (pintype "passive"))
    (model "${KIPRJMOD}/3D/R_0603_1608Metric.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "footprints:QFN-48-1EP_7x7mm_P0.5mm_EP5.15x5.15mm" (layer "F.Cu")
    (tedit 5DC5F6A5)
    (at 150.5204 103.2002 180)
    (descr "QFN, 48 Pin (http://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/ltc-legacy-qfn/QFN_48_05-08-1704.pdf), generated with kicad-footprint-generator ipc_noLead_generator.py")
    (tags "QFN NoLead")
    (property "Sheetfile" "Board RPB30 SAM51 SeeSaw.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "U9" (at 0 -4.82) (layer "F.Fab"))
    (fp_text value "ATSAMD51G" (at -0.1016 5.1562) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "" smd roundrect (at -1.935 1.935 180) (size 1.04 1.04) (layers "F.Paste") (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at 1.935 0.645 180) (size 1.04 1.04) (layers "F.Paste") (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at -0.645 -1.935 180) (size 1.04 1.04) (layers "F.Paste") (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at 0.645 -0.645 180) (size 1.04 1.04) (layers "F.Paste") (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at -0.645 1.935 180) (size 1.04 1.04) (layers "F.Paste") (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at 0.645 -1.935 180) (size 1.04 1.04) (layers "F.Paste") (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at -1.935 0.645 180) (size 1.04 1.04) (layers "F.Paste") (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at 1.935 -0.645 180) (size 1.04 1.04) (layers "F.Paste") (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at 1.935 -1.935 180) (size 1.04 1.04) (layers "F.Paste") (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at -1.935 -1.935 180) (size 1.04 1.04) (layers "F.Paste") (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at 0.645 0.645 180) (size 1.04 1.04) (layers "F.Paste") (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at -0.645 0.645 180) (size 1.04 1.04) (layers "F.Paste") (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at 1.935 1.935 180) (size 1.04 1.04) (layers "F.Paste") (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at -0.645 -0.645 180) (size 1.04 1.04) (layers "F.Paste") (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at 0.645 1.935 180) (size 1.04 1.04) (layers "F.Paste") (roundrect_rratio 0.240385))
    (pad "" smd roundrect (at -1.935 -0.645 180) (size 1.04 1.04) (layers "F.Paste") (roundrect_rratio 0.240385))
    (pad "1" smd roundrect (at -3.4375 -2.75 180) (size 0.875 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 14 "/MOSI") (pinfunction "PA00") (pintype "bidirectional"))
    (pad "2" smd roundrect (at -3.4375 -2.25 180) (size 0.875 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 13 "/SCK") (pinfunction "PA01") (pintype "bidirectional"))
    (pad "3" smd roundrect (at -3.4375 -1.75 180) (size 0.875 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 140 "/A0{slash}D5") (pinfunction "PA02") (pintype "bidirectional"))
    (pad "4" smd roundrect (at -3.4375 -1.25 180) (size 0.875 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 47 "/AREF") (pinfunction "PA03") (pintype "bidirectional"))
    (pad "5" smd roundrect (at -3.4375 -0.75 180) (size 0.875 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pinfunction "GNDANA") (pintype "power_in"))
    (pad "6" smd roundrect (at -3.4375 -0.25 180) (size 0.875 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 10 "+3V3") (pinfunction "VDDANA") (pintype "power_in"))
    (pad "7" smd roundrect (at -3.4375 0.25 180) (size 0.875 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 37 "/A2") (pinfunction "PB08") (pintype "bidirectional"))
    (pad "8" smd roundrect (at -3.4375 0.75 180) (size 0.875 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 11 "/A3") (pinfunction "PB09") (pintype "bidirectional"))
    (pad "9" smd roundrect (at -3.4375 1.25 180) (size 0.875 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 38 "/A4") (pinfunction "PA04") (pintype "bidirectional"))
    (pad "10" smd roundrect (at -3.4375 1.75 180) (size 0.875 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 36 "/A1") (pinfunction "PA05") (pintype "bidirectional"))
    (pad "11" smd roundrect (at -3.4375 2.25 180) (size 0.875 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 12 "/A5") (pinfunction "PA06") (pintype "bidirectional"))
    (pad "12" smd roundrect (at -3.4375 2.75 180) (size 0.875 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 139 "/D2") (pinfunction "PA07") (pintype "bidirectional"))
    (pad "13" smd roundrect (at -2.75 3.4375 180) (size 0.25 0.875) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 142 "/QSPI_DATA_0") (pinfunction "PA08") (pintype "bidirectional"))
    (pad "14" smd roundrect (at -2.25 3.4375 180) (size 0.25 0.875) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 143 "/QSPI_DATA_1") (pinfunction "PA09") (pintype "bidirectional"))
    (pad "15" smd roundrect (at -1.75 3.4375 180) (size 0.25 0.875) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 144 "/QSPI_DATA_2") (pinfunction "PA10") (pintype "bidirectional"))
    (pad "16" smd roundrect (at -1.25 3.4375 180) (size 0.25 0.875) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 145 "/QSPI_DATA_3") (pinfunction "PA11") (pintype "bidirectional"))
    (pad "17" smd roundrect (at -0.75 3.4375 180) (size 0.25 0.875) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 10 "+3V3") (pinfunction "VDDIO") (pintype "power_in"))
    (pad "18" smd roundrect (at -0.25 3.4375 180) (size 0.25 0.875) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "19" smd roundrect (at 0.25 3.4375 180) (size 0.25 0.875) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 146 "/QSPI_SCK") (pinfunction "PB10") (pintype "bidirectional"))
    (pad "20" smd roundrect (at 0.75 3.4375 180) (size 0.25 0.875) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 31 "/QSPI_CS") (pinfunction "PB11") (pintype "bidirectional"))
    (pad "21" smd roundrect (at 1.25 3.4375 180) (size 0.25 0.875) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 39 "/SDA") (pinfunction "PA12") (pintype "bidirectional"))
    (pad "22" smd roundrect (at 1.75 3.4375 180) (size 0.25 0.875) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 32 "/SCL") (pinfunction "PA13") (pintype "bidirectional"))
    (pad "23" smd roundrect (at 2.25 3.4375 180) (size 0.25 0.875) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "/D4") (pinfunction "PA14") (pintype "bidirectional"))
    (pad "24" smd roundrect (at 2.75 3.4375 180) (size 0.25 0.875) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 140 "/A0{slash}D5") (pinfunction "PA15") (pintype "bidirectional"))
    (pad "25" smd roundrect (at 3.4375 2.75 180) (size 0.875 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 137 "/RX_D0") (pinfunction "PA16") (pintype "bidirectional"))
    (pad "26" smd roundrect (at 3.4375 2.25 180) (size 0.875 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 138 "/TX_D1") (pinfunction "PA17") (pintype "bidirectional"))
    (pad "27" smd roundrect (at 3.4375 1.75 180) (size 0.875 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 9 "/D7") (pinfunction "PA18") (pintype "bidirectional"))
    (pad "28" smd roundrect (at 3.4375 1.25 180) (size 0.875 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 8 "/D9") (pinfunction "PA19") (pintype "bidirectional"))
    (pad "29" smd roundrect (at 3.4375 0.75 180) (size 0.875 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 7 "/D10") (pinfunction "PA20") (pintype "bidirectional"))
    (pad "30" smd roundrect (at 3.4375 0.25 180) (size 0.875 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 35 "/D11") (pinfunction "PA21") (pintype "bidirectional"))
    (pad "31" smd roundrect (at 3.4375 -0.25 180) (size 0.875 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "/D13") (pinfunction "PA22") (pintype "bidirectional"))
    (pad "32" smd roundrect (at 3.4375 -0.75 180) (size 0.875 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 6 "/D12") (pinfunction "PA23") (pintype "bidirectional"))
    (pad "33" smd roundrect (at 3.4375 -1.25 180) (size 0.875 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 21 "/D-") (pinfunction "PA24") (pintype "bidirectional"))
    (pad "34" smd roundrect (at 3.4375 -1.75 180) (size 0.875 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 20 "/D+") (pinfunction "PA25") (pintype "bidirectional"))
    (pad "35" smd roundrect (at 3.4375 -2.25 180) (size 0.875 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "36" smd roundrect (at 3.4375 -2.75 180) (size 0.875 0.25) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 10 "+3V3") (pinfunction "VDDIO") (pintype "power_in"))
    (pad "37" smd roundrect (at 2.75 -3.4375 180) (size 0.25 0.875) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 136 "/D3") (pinfunction "PB22") (pintype "bidirectional"))
    (pad "38" smd roundrect (at 2.25 -3.4375 180) (size 0.25 0.875) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 15 "/MISO") (pinfunction "PB23") (pintype "bidirectional"))
    (pad "39" smd roundrect (at 1.75 -3.4375 180) (size 0.25 0.875) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 147 "unconnected-(U9-Pad39)") (pinfunction "PA27") (pintype "bidirectional+no_connect"))
    (pad "40" smd roundrect (at 1.25 -3.4375 180) (size 0.25 0.875) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 19 "/~{RESET}") (pinfunction "~{RESET}") (pintype "input"))
    (pad "41" smd roundrect (at 0.75 -3.4375 180) (size 0.25 0.875) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 18 "Net-(C15-Pad2)") (pinfunction "VDDCORE") (pintype "power_in"))
    (pad "42" smd roundrect (at 0.25 -3.4375 180) (size 0.25 0.875) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "43" smd roundrect (at -0.25 -3.4375 180) (size 0.25 0.875) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 28 "Net-(L1-Pad2)") (pinfunction "VSW") (pintype "power_out"))
    (pad "44" smd roundrect (at -0.75 -3.4375 180) (size 0.25 0.875) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 10 "+3V3") (pinfunction "VDDIO") (pintype "power_in"))
    (pad "45" smd roundrect (at -1.25 -3.4375 180) (size 0.25 0.875) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 26 "/SWCLK") (pinfunction "PA30") (pintype "bidirectional"))
    (pad "46" smd roundrect (at -1.75 -3.4375 180) (size 0.25 0.875) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 27 "/SWDIO") (pinfunction "PA31") (pintype "bidirectional"))
    (pad "47" smd roundrect (at -2.25 -3.4375 180) (size 0.25 0.875) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 34 "/DS_CLK") (pinfunction "PB02") (pintype "bidirectional"))
    (pad "48" smd roundrect (at -2.75 -3.4375 180) (size 0.25 0.875) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 33 "/DS_DATA") (pinfunction "PB03") (pintype "bidirectional"))
    (pad "49" smd rect (at 0 0 180) (size 5.15 5.15) (layers "F.Cu" "F.Mask")
      (net 1 "GND") (pinfunction "EP") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Package_DFN_QFN.3dshapes/QFN-48-1EP_7x7mm_P0.5mm_EP5.15x5.15mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "footprints:LED_0603" (layer "F.Cu")
    (tedit 636FBDBF)
    (at 168.364 124.36)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (property "Sheetfile" "Board RPB30 SAM51 SeeSaw.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "D13" (at 2.032 0) (layer "F.SilkS") hide)
    (fp_text value "D13" (at -2.286 0 -90 unlocked) (layer "F.SilkS"))
    (pad "1" smd rect locked (at -0.8 0 180) (size 0.8 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 25 "Net-(D13-Pad1)") (pinfunction "K") (pintype "passive"))
    (pad "2" smd rect locked (at 0.8 0 180) (size 0.8 0.8) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 5 "/D13") (pinfunction "A") (pintype "passive"))
    (model "${KIPRJMOD}/3D/LED_0603_1608Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "footprints:SW_TS10-63-26-BE-250-SMT-TR" (layer "F.Cu")
    (tedit 63700F76)
    (at 162 129 -90)
    (property "Sheetfile" "Board RPB30 SAM51 SeeSaw.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "SW1" (at 0.15 0 -90) (layer "F.SilkS"))
    (fp_text value "D3" (at 5.05 0 180) (layer "F.SilkS"))
    (pad "1" smd rect locked (at -3.25 0 270) (size 1.5 1.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 136 "/D3") (pinfunction "1") (pintype "passive"))
    (pad "2" smd rect locked (at 3.25 0 270) (size 1.5 1.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "2") (pintype "passive"))
  )
  (footprint "footprints:R_2512_6332Metric" (layer "F.Cu")
    (tedit 5F68FEEE)
    (at 122.5 129.25 90)
    (descr "Resistor SMD 2512 (6332 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "Board RPB30 SAM51 SeeSaw.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R15" (at 0 -2.62 90) (layer "F.Fab"))
    (fp_text value "0.1" (at 0 2.62 90) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2.9625 0 90) (size 1.225 3.35) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.204082)
      (net 30 "VBUS") (pintype "passive"))
    (pad "2" smd roundrect (at 2.9625 0 90) (size 1.225 3.35) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.204082)
      (net 10 "+3V3") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_2512_6332Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "footprints:C_0603" (layer "F.Cu")
    (tedit 59958EE7)
    (at 129.75 123.5 -90)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (property "Sheetfile" "Board RPB30 SAM51 SeeSaw.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "C13" (at 0 -1.5 90) (layer "F.Fab"))
    (fp_text value "0.1uF" (at -1.85 4.9 180) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd rect (at -0.75 0 270) (size 0.8 0.75) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pintype "passive"))
    (pad "2" smd rect (at 0.75 0 270) (size 0.8 0.75) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 10 "+3V3") (pintype "passive"))
    (model "${KIPRJMOD}/3D/C_0603_1608Metric.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "footprints:SOIC-8_3.9x4.9mm_P1.27mm" (layer "F.Cu")
    (tedit 5D9F72B1)
    (at 130.374 128.234 180)
    (descr "SOIC, 8 Pin (JEDEC MS-012AA, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_narrow-r/r_8.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOIC SO")
    (property "Sheetfile" "Board RPB30 SAM51 SeeSaw.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "U10" (at 0 0) (layer "F.Fab"))
    (fp_text value "INA219AxD" (at -0.376 -3.316) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2.475 -1.905 180) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 16 "Net-(A2-Pad1)") (pinfunction "A1") (pintype "input"))
    (pad "2" smd roundrect (at -2.475 -0.635 180) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "Net-(A1-Pad1)") (pinfunction "A0") (pintype "input"))
    (pad "3" smd roundrect (at -2.475 0.635 180) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 39 "/SDA") (pinfunction "SDA") (pintype "bidirectional"))
    (pad "4" smd roundrect (at -2.475 1.905 180) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 32 "/SCL") (pinfunction "SCL") (pintype "input"))
    (pad "5" smd roundrect (at 2.475 1.905 180) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 10 "+3V3") (pinfunction "VS") (pintype "power_in"))
    (pad "6" smd roundrect (at 2.475 0.635 180) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "GND") (pinfunction "GND") (pintype "power_in"))
    (pad "7" smd roundrect (at 2.475 -0.635 180) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 30 "VBUS") (pinfunction "IN-") (pintype "input"))
    (pad "8" smd roundrect (at 2.475 -1.905 180) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 10 "+3V3") (pinfunction "IN+") (pintype "input"))
    (model "${KICAD6_3DMODEL_DIR}/Package_SO.3dshapes/SOIC-8_3.9x4.9mm_P1.27mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "footprints:R_0603" (layer "F.Cu")
    (tedit 636FC042)
    (at 155.6 116.55 -90)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (property "Sheetfile" "Board RPB30 SAM51 SeeSaw.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R12" (at 1.905 0 90) (layer "Dwgs.User"))
    (fp_text value "1K" (at 2 -0.05 90) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd rect locked (at -0.75 0 270) (size 0.5 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 10 "+3V3") (pintype "passive"))
    (pad "2" smd rect locked (at 0.75 0 270) (size 0.5 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 26 "/SWCLK") (pintype "passive"))
    (model "${KIPRJMOD}/3D/R_0603_1608Metric.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "footprints:TestPoint_Pad_D0.6mm" (layer "F.Cu")
    (tedit 5A0F774F)
    (at 144.25 105.55)
    (descr "SMD pad as test Point, diameter 1.0mm")
    (tags "test point SMD pad")
    (property "Sheetfile" "Board RPB30 SAM51 SeeSaw.kicad_sch")
    (property "Sheetname" "")
    (attr exclude_from_pos_files)
    (fp_text reference "TP7" (at 0 -1.448) (layer "User.1") hide)
    (fp_text value "GND" (at -1.2 0.05) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 -1.45) (layer "F.Fab") hide)
    (pad "1" smd circle (at 0 0) (size 0.6 0.6) (layers "F.Cu" "F.Mask")
      (net 1 "GND") (pinfunction "1") (pintype "passive"))
  )
  (footprint "footprints:Jumper" (layer "F.Cu")
    (tedit 5B6DD72B)
    (at 136.75 131.25)
    (property "Sheetfile" "Board RPB30 SAM51 SeeSaw.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "A2" (at 1.6 -0.1) (layer "F.SilkS"))
    (fp_text value "Jumper" (at 0 1.25) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -1.2) (layer "F.Fab"))
    (pad "1" smd rect locked (at -0.3 0) (size 0.4 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 16 "Net-(A2-Pad1)") (pinfunction "A") (pintype "passive"))
    (pad "2" smd rect locked (at 0.3 0) (size 0.4 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 10 "+3V3") (pinfunction "B") (pintype "passive"))
    (model "${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0402.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "footprints:R_0603" (layer "F.Cu")
    (tedit 636FC042)
    (at 136.5 127.5 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (property "Sheetfile" "Board RPB30 SAM51 SeeSaw.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R16" (at 1.905 0) (layer "Dwgs.User"))
    (fp_text value "10K" (at -2.45 0) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect locked (at -0.75 0 180) (size 0.5 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pintype "passive"))
    (pad "2" smd rect locked (at 0.75 0 180) (size 0.5 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 3 "Net-(A1-Pad1)") (pintype "passive"))
    (model "${KIPRJMOD}/3D/R_0603_1608Metric.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Connector_Molex:Molex_PicoBlade_53048-0410_1x04_P1.25mm_Horizontal" (layer "F.Cu")
    (tedit 5B783024)
    (at 148.85 114.8 -90)
    (descr "Molex PicoBlade Connector System, 53048-0410, 4 Pins per row (http://www.molex.com/pdm_docs/sd/530480210_sd.pdf), generated with kicad-footprint-generator")
    (tags "connector Molex PicoBlade top entry")
    (property "Sheetfile" "Board RPB30 SAM51 SeeSaw.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "J2" (at 1.95 2.45 90) (layer "F.SilkS") hide)
    (fp_text value "SWD" (at -2.45 1.1 180) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 1.88 3.75 90) (layer "F.Fab"))
    (pad "1" thru_hole roundrect (at 0 0 270) (size 0.8 1.3) (drill 0.5) (layers *.Cu *.Mask) (roundrect_rratio 0.25)
      (net 10 "+3V3") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 1.25 0 270) (size 0.8 1.3) (drill 0.5) (layers *.Cu *.Mask)
      (net 26 "/SWCLK") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 2.5 0 270) (size 0.8 1.3) (drill 0.5) (layers *.Cu *.Mask)
      (net 27 "/SWDIO") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 3.75 0 270) (size 0.8 1.3) (drill 0.5) (layers *.Cu *.Mask)
      (net 1 "GND") (pinfunction "Pin_4") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_Molex.3dshapes/Molex_PicoBlade_53048-0410_1x04_P1.25mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "footprints:SW_TS10-63-26-BE-250-SMT-TR" (layer "F.Cu")
    (tedit 63700F76)
    (at 116 129 -90)
    (property "Sheetfile" "Board RPB30 SAM51 SeeSaw.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "SW2" (at 0.05 0.05 -90) (layer "F.SilkS"))
    (fp_text value "D4" (at 5 -0.05 180) (layer "F.SilkS"))
    (pad "1" smd rect locked (at -3.25 0 270) (size 1.5 1.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "/D4") (pinfunction "1") (pintype "passive"))
    (pad "2" smd rect locked (at 3.25 0 270) (size 1.5 1.4) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pinfunction "2") (pintype "passive"))
  )
  (footprint "footprints:R_0603" (layer "F.Cu")
    (tedit 636FC042)
    (at 165.5 122.4)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (property "Sheetfile" "Board RPB30 SAM51 SeeSaw.kicad_sch")
    (property "Sheetname" "")
    (attr smd)
    (fp_text reference "R11" (at 1.905 0 180) (layer "Dwgs.User"))
    (fp_text value "1K" (at -1.905 0 180) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 180) (layer "F.Fab"))
    (pad "1" smd rect locked (at -0.75 0) (size 0.5 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "GND") (pintype "passive"))
    (pad "2" smd rect locked (at 0.75 0) (size 0.5 0.9) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 24 "Net-(D11-Pad1)") (pintype "passive"))
    (model "${KIPRJMOD}/3D/R_0603_1608Metric.step"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_line (start 110.49 135) (end 167.64 135) (layer "Edge.Cuts") (width 0.15))
  (gr_line (start 167.64 76.2) (end 110.49 76.2) (layer "Edge.Cuts") (width 0.15))
  (gr_line (start 171.45 80.01) (end 171.45 123.19) (layer "Edge.Cuts") (width 0.15))
  (gr_line (start 106.68 123.19) (end 106.68 131.19) (layer "Edge.Cuts") (width 0.15))
  (gr_line (start 171.45 123.19) (end 171.45 131.19) (layer "Edge.Cuts") (width 0.15))
  (gr_arc (start 106.68 80.01) (mid 107.795923 77.315923) (end 110.49 76.2) (layer "Edge.Cuts") (width 0.15))
  (gr_arc (start 171.45 131.19) (mid 170.334077 133.884077) (end 167.64 135) (layer "Edge.Cuts") (width 0.15))
  (gr_arc (start 110.49 135) (mid 107.795923 133.884077) (end 106.68 131.19) (layer "Edge.Cuts") (width 0.15))
  (gr_arc (start 167.64 76.2) (mid 170.334077 77.315923) (end 171.45 80.01) (layer "Edge.Cuts") (width 0.15))
  (gr_line (start 106.68 123.19) (end 106.68 80.01) (layer "Edge.Cuts") (width 0.15))
  (gr_text "Rapid Prototyping Board" (at 139.7 103.14) (layer "B.SilkS"))
  (gr_text "ken.olsen@agilityrobotics.com" (at 138.684 132.588) (layer "B.SilkS"))
  (gr_text "3V3\nUDPI\nGND" (at 147.95 127.8) (layer "B.SilkS"))
  (gr_text "(SAM51D / Attiny 816)" (at 139.954 107.442) (layer "B.SilkS"))
  (gr_text "3V3\nSWCLK\nSWDIO\nGND" (at 147.95 116.7) (layer "B.SilkS"))
  (gr_text "Rev 3.0\nNov 2025" (at 122.75 131.75) (layer "B.SilkS"))
  (gr_text "I2C 0x3C = SSD1306 OLED\nI2C 0x40 = INA219A\nI2C 0x49 = SeeSaw U2\nI2C 0x4A = SeeSaw U3\nI2C 0x4B = SeeSaw U4\nI2C 0x4C = SeeSaw U5\nI2C 0x4D = SeeSaw U6\nI2C 0x4E = SeeSaw U7\n" (at 141.2 117.3) (layer "B.SilkS"))
  (gr_text "M3" (at 163.7 83.95) (layer "F.SilkS"))
  (gr_text "Rapid \nPrototyping\nBoard" (at 139.35 82.6) (layer "F.SilkS"))
  (gr_text "SDA SCL VCC GND" (at 158.75 128 90) (layer "F.SilkS"))
  (gr_text "I2C OLED Display" (at 140.55 132.95) (layer "F.SilkS"))
  (gr_text "3V3\nUDPI\nGND" (at 150.4 127.85) (layer "F.SilkS"))
  (gr_text "3V3\nSWCLK\nSWDIO\nGND" (at 150.5 116.65) (layer "F.SilkS"))
  (gr_text "M2.5" (at 163.75 92.05) (layer "F.SilkS"))
  (gr_text "v 3.0" (at 150.25 85.25) (layer "F.SilkS"))
  (gr_text "Keep It\nSimple\nStupid" (at 190 93.2) (layer "B.Mask"))
  (dimension (type aligned) (layer "Dwgs.User")
    (pts (xy 134.6 85.4) (xy 134.6 82.6))
    (height 2.4)
    (gr_text "2.8000 mm" (at 135.85 84 90) (layer "Dwgs.User"))
    (format (units 2) (units_format 1) (precision 4))
    (style (thickness 0.15) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0) keep_text_aligned)
  )
  (dimension (type aligned) (layer "Dwgs.User")
    (pts (xy 110.49 135) (xy 110.49 76.2))
    (height -12.49)
    (gr_text "58.8000 mm" (at 96.85 105.6 90) (layer "Dwgs.User"))
    (format (units 2) (units_format 1) (precision 4))
    (style (thickness 0.15) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0) keep_text_aligned)
  )
  (dimension (type aligned) (layer "Dwgs.User")
    (pts (xy 171.45 131.19) (xy 106.68 131.19))
    (height -7.81)
    (gr_text "64.7700 mm" (at 139.065 137.85) (layer "Dwgs.User"))
    (format (units 2) (units_format 1) (precision 4))
    (style (thickness 0.15) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0) keep_text_aligned)
  )
  (zone (net 1) (net_name "GND") (layer "F.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0.35))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 171.958 137)
        (xy 105.8 137.1)
        (xy 106.1 74.2)
        (xy 172.2 74.3)
      )
    )
  )
  (zone (net 1) (net_name "GND") (layer "B.Cu") (hatch edge 0.508)
    (connect_pads (clearance 0.35))
    (min_thickness 0.254) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 172.466 137)
        (xy 105.664 137)
        (xy 105.8 74.4)
        (xy 172.8 74.3)
      )
    )
  )
)
