(kicad_pcb
	(version 20260206)
	(generator "pcbnew")
	(generator_version "10.0")
	(general
		(thickness 1.6)
		(legacy_teardrops no)
	)
	(paper "A4")
	(layers
		(0 "F.Cu" signal)
		(2 "B.Cu" signal)
		(9 "F.Adhes" user "F.Adhesive")
		(11 "B.Adhes" user "B.Adhesive")
		(13 "F.Paste" user)
		(15 "B.Paste" user)
		(5 "F.SilkS" user "F.Silkscreen")
		(7 "B.SilkS" user "B.Silkscreen")
		(1 "F.Mask" user)
		(3 "B.Mask" user)
		(17 "Dwgs.User" user "User.Drawings")
		(19 "Cmts.User" user "User.Comments")
		(21 "Eco1.User" user "User.Eco1")
		(23 "Eco2.User" user "User.Eco2")
		(25 "Edge.Cuts" user)
		(27 "Margin" user)
		(31 "F.CrtYd" user "F.Courtyard")
		(29 "B.CrtYd" user "B.Courtyard")
		(35 "F.Fab" user)
		(33 "B.Fab" user)
		(39 "User.1" user)
		(41 "User.2" user)
		(43 "User.3" user)
		(45 "User.4" user)
		(47 "User.5" user)
		(49 "User.6" user)
		(51 "User.7" user)
		(53 "User.8" user)
		(55 "User.9" user)
	)
	(setup
		(stackup
			(layer "F.SilkS"
				(type "Top Silk Screen")
			)
			(layer "F.Paste"
				(type "Top Solder Paste")
			)
			(layer "F.Mask"
				(type "Top Solder Mask")
				(thickness 0.01)
			)
			(layer "F.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "dielectric 1"
				(type "core")
				(thickness 1.51)
				(material "FR4")
				(epsilon_r 4.5)
				(loss_tangent 0.02)
			)
			(layer "B.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "B.Mask"
				(type "Bottom Solder Mask")
				(thickness 0.01)
			)
			(layer "B.Paste"
				(type "Bottom Solder Paste")
			)
			(layer "B.SilkS"
				(type "Bottom Silk Screen")
			)
			(copper_finish "None")
			(dielectric_constraints no)
		)
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(tenting
			(front yes)
			(back yes)
		)
		(covering
			(front no)
			(back no)
		)
		(plugging
			(front no)
			(back no)
		)
		(capping no)
		(filling no)
		(grid_origin 130 75)
		(pcbplotparams
			(layerselection 0x00000000_00000000_55555555_5755f5ff)
			(plot_on_all_layers_selection 0x00000000_00000000_00000000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12)
			(dashed_line_gap_ratio 3)
			(svgprecision 4)
			(plotframeref no)
			(mode 1)
			(useauxorigin no)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(pdf_metadata yes)
			(pdf_single_document no)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plot_black_and_white yes)
			(sketchpadsonfab no)
			(plotpadnumbers no)
			(hidednponfab no)
			(sketchdnponfab yes)
			(crossoutdnponfab yes)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 1)
			(scaleselection 1)
			(outputdirectory "")
		)
	)
	(footprint "Library:H315305"
		(layer "F.Cu")
		(uuid "0457a396-79ed-467f-9429-1888feb9d2a9")
		(at 133.38 84.82)
		(descr "H3153-05-2")
		(tags "Connector")
		(property "Reference" "D7"
			(at 0 -2.5 0)
			(layer "F.SilkS")
			(uuid "e1b74876-b140-4f7e-a72b-c4b9b4f1e01e")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.254)
				)
			)
		)
		(property "Value" "Conn_01x01_Socket"
			(at -0.5 -3 0)
			(layer "F.SilkS")
			(hide yes)
			(uuid "11ad2043-fd8e-419e-b437-8263da3cae32")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.254)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "2c4bee0b-2006-4853-bfa3-438f29ba7ddb")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "48125a14-06ca-4dea-94d3-d7da2f4e8f42")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Manufacturer" "Harwin"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
			(uuid "ca7410ff-6a8c-4344-802d-a9e3019a11e4")
			(effects
				(font
					(size 1 1)
					(thickness 0.1)
				)
			)
		)
		(property "MPN" "H3153-05"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
			(uuid "92d7224d-0f4d-4bac-8f9d-d8285f68f32f")
			(effects
				(font
					(size 1 1)
					(thickness 0.1)
				)
			)
		)
		(property "Supplier" "Mouser"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
			(uuid "7fca2f31-fecc-4edb-b3da-0a50b669b8d6")
			(effects
				(font
					(size 1 1)
					(thickness 0.1)
				)
			)
		)
		(property "Supplier Part Number" "855-H3153-05"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
			(uuid "dc3fed4c-05e6-4ace-8845-7df1206f022d")
			(effects
				(font
					(size 1 1)
					(thickness 0.1)
				)
			)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(path "/96cb6185-2322-493c-8987-4c405f77646b")
		(sheetname "Root")
		(sheetfile "PMT1inchBase.kicad_sch")
		(attr through_hole)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_line
			(start -1.2 0)
			(end -1.2 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "11cfc00f-64a6-4c7e-9c24-66266aa0a7d0")
		)
		(fp_line
			(start 1.2 0)
			(end 1.2 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "f4d37573-2137-4e58-b69c-9951a2191bb5")
		)
		(fp_arc
			(start -1.2 0)
			(mid 0 -1.2)
			(end 1.2 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "1ad046bd-cec7-443d-a5a8-ff9f73ebb187")
		)
		(fp_arc
			(start 1.2 0)
			(mid 0 1.2)
			(end -1.2 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "e8a98d5f-7f0d-40ce-99d4-1c8b85366223")
		)
		(fp_line
			(start -1.2 -1.2)
			(end 1.2 -1.2)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "565f8f46-4da4-4bbc-b5b9-09ff581b6e65")
		)
		(fp_line
			(start -1.2 1.2)
			(end -1.2 -1.2)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "7756aa01-a4f8-443b-a054-9cf739704f90")
		)
		(fp_line
			(start 1.2 -1.2)
			(end 1.2 1.2)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "e78897a0-aa37-4300-b41d-6c0b85e506b9")
		)
		(fp_line
			(start 1.2 1.2)
			(end -1.2 1.2)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "7a312c70-77f0-4b48-b95d-3a25dd977487")
		)
		(fp_line
			(start -1.2 0)
			(end -1.2 0)
			(stroke
				(width 0.2)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "d1016431-87ac-4ad1-84e6-e64fc124ede7")
		)
		(fp_line
			(start 1.2 0)
			(end 1.2 0)
			(stroke
				(width 0.2)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "420d7abf-e7e6-4613-b3a8-cfedc856ae72")
		)
		(fp_arc
			(start -1.2 0)
			(mid 0 -1.2)
			(end 1.2 0)
			(stroke
				(width 0.2)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "35356e6f-83aa-4329-9f5f-fd3c29c9c7ca")
		)
		(fp_arc
			(start 1.2 0)
			(mid 0 1.2)
			(end -1.2 0)
			(stroke
				(width 0.2)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "50100848-e6ea-472a-9958-89379b28addc")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "9f140e2e-ac63-4371-aaba-61576236fa9b")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.254)
				)
			)
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1.65 1.65)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "Net-(D7-Pin_1)")
			(pinfunction "Pin_1")
			(pintype "passive")
			(uuid "36ba8457-6e43-4d2e-8166-821430550c2e")
		)
		(embedded_fonts no)
		(model "${KIPRJMOD}/3dmodels/H3153-05.stp"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -0 -90 -0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder"
		(layer "F.Cu")
		(uuid "07ee32a8-778a-4c9f-8ec9-b678a50f6e3b")
		(at 139.6375 76.5)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "capacitor handsolder")
		(property "Reference" "C3"
			(at 0 -1.43 0)
			(layer "F.SilkS")
			(uuid "165d3bfe-0868-4caa-8d9c-730215818edc")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "10 nF"
			(at 0 1.43 0)
			(layer "F.Fab")
			(uuid "ddd17998-9d4d-47f2-a807-a2135ab48355")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "bdd55b5c-328a-4346-8a73-d6db9123bd5d")
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "c3665666-4362-4ab3-95d2-8b025321089e")
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
			(uuid "0f17835c-fecf-44cf-b672-9e5a1570d091")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Manufacturer" "TDK"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "06bc31a6-3e2a-4088-8053-942e9d0802bb")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "MPN" "CGA3E1C0G2A103J080AC"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "5aee5528-d5f2-4cbb-b5a2-74d2d131ba4e")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Supplier Part Number" "810-CGA3E1C0G2A103J080AC"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "267101c7-8445-4238-b29a-5f5c10566996")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/539bfd15-af33-4680-86df-40d4e35e1472")
		(sheetname "Root")
		(sheetfile "PMT1inchBase.kicad_sch")
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_line
			(start -0.146267 -0.51)
			(end 0.146267 -0.51)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "4a084b56-95fc-44be-a8cf-929dd0ec298f")
		)
		(fp_line
			(start -0.146267 0.51)
			(end 0.146267 0.51)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "d5a3aaab-9a37-46ea-8787-49038f379d55")
		)
		(fp_rect
			(start -1.65 -0.73)
			(end 1.65 0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(fill no)
			(layer "F.CrtYd")
			(uuid "12500e8f-fca3-49ce-8216-46595324a19c")
		)
		(fp_rect
			(start -0.8 -0.4)
			(end 0.8 0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill no)
			(layer "F.Fab")
			(uuid "c6ecc1d8-2565-40d5-a8fd-23a45b73ae0e")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "cf54930b-0aae-4cb0-9b5b-fac14bc37ca8")
			(effects
				(font
					(size 0.4 0.4)
					(thickness 0.06)
				)
			)
		)
		(pad "1" smd roundrect
			(at -0.8625 0)
			(size 1.075 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "Net-(D9-Pin_1)")
			(pintype "passive")
			(uuid "d83b5730-41a5-4de5-b7ea-f3cfbc483d39")
		)
		(pad "2" smd roundrect
			(at 0.8625 0)
			(size 1.075 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "Net-(D10-Pin_1)")
			(pintype "passive")
			(uuid "05b18666-b6e1-4543-a3b3-0e7f5b5034ec")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(uuid "0d23a197-7f88-4a49-8807-bf9d4fd66e74")
		(at 144 82)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "resistor handsolder")
		(property "Reference" "R12"
			(at 0 -1.65 0)
			(layer "F.SilkS")
			(uuid "3d1de545-0c89-44c7-80fc-f2247b832ac1")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "2.49M"
			(at 0 1.65 0)
			(layer "F.Fab")
			(uuid "49dfeca6-53e9-40b7-b6b3-85efb233515e")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "97475187-c420-432b-838c-4da9c28adbbd")
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "6bba8f61-aa4b-4cd3-b098-8384c2a99ba8")
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
			(uuid "76f07162-826b-4974-a9f1-a9f334a569e0")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Manufacturer" "KOA Speer"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "021ecfb6-c7f6-4a6c-96b0-c7456d9b200d")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "MPN" "RS73G2ARTTD2494B"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "11967060-0786-4f18-adc1-03d9174dbdae")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Supplier Part Number" "660-RS73G2ARTTD2494B"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "fde409c4-1407-4534-80ad-86dc7812ab63")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/48e48cc5-e764-49b1-90ef-e1b7b3d5a236")
		(sheetname "Root")
		(sheetfile "PMT1inchBase.kicad_sch")
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_line
			(start -0.227064 -0.735)
			(end 0.227064 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "4e67993e-f68a-429e-828b-a1aef4a71ac1")
		)
		(fp_line
			(start -0.227064 0.735)
			(end 0.227064 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "f8fb33dd-c664-4850-9b57-df0126986a47")
		)
		(fp_rect
			(start -1.85 -0.95)
			(end 1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(fill no)
			(layer "F.CrtYd")
			(uuid "c6675c3c-ad14-4624-a203-4f9748f2eb07")
		)
		(fp_rect
			(start -1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill no)
			(layer "F.Fab")
			(uuid "b74cb068-bf3b-4937-b3a7-53d321ce3fdb")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "bcc531a0-bb1f-4b01-a0d7-0ac8931bf8cc")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net "Net-(D10-Pin_1)")
			(pintype "passive")
			(uuid "66f1aed2-0b04-49a1-a0c1-6b15ce2baced")
		)
		(pad "2" smd roundrect
			(at 1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net "Net-(GND1-Pin_1)")
			(pintype "passive")
			(uuid "73601792-9907-46ba-a5f9-33daad7cc233")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(uuid "0f30b412-0e2d-4398-954d-36487132e540")
		(at 147 79 -90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "resistor handsolder")
		(property "Reference" "RL1"
			(at 0 -1.65 270)
			(layer "F.SilkS")
			(uuid "b6d3b0e9-0588-4d08-a147-d023b4594df7")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "100K"
			(at 0 1.65 270)
			(layer "F.Fab")
			(uuid "11ee39e7-85c9-4273-b745-5c49813396ff")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
			(uuid "a868c0ff-2a5c-4bc9-b668-db187898af3a")
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Description" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
			(uuid "c3973657-5ed0-4fe4-8ed0-371ef219432a")
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 270)
			(layer "F.SilkS")
			(hide yes)
			(uuid "7d6e0f62-bac0-47e3-8bbb-a559a346e2e8")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Manufacturer" "TE Connectivity / Holsworthy"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "cc7aa36d-87ef-4e93-b871-fbc0e8bec7a1")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "MPN" "RQ73C2A100KBTDF"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "501df998-5d2d-4ad2-94a5-706a8aa6a3c7")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Supplier Part Number" "279-RQ73C2A100KBTDF"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "1cb39de3-ae5f-4734-9c07-99913b531024")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/37f89e61-be7c-4947-a3ae-2b73f0aef71e")
		(sheetname "Root")
		(sheetfile "PMT1inchBase.kicad_sch")
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_line
			(start -0.227064 0.735)
			(end 0.227064 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "982f08a2-762d-4be3-a60a-d73628089a0d")
		)
		(fp_line
			(start -0.227064 -0.735)
			(end 0.227064 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "33a0281f-d758-43bd-a8e8-c299e242d149")
		)
		(fp_rect
			(start -1.85 -0.95)
			(end 1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(fill no)
			(layer "F.CrtYd")
			(uuid "5cd3e884-9023-4be9-a651-99bbc4392dd4")
		)
		(fp_rect
			(start -1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill no)
			(layer "F.Fab")
			(uuid "ce5bb8e3-2bb5-4f1f-89a0-3294b5374ce4")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 270)
			(layer "F.Fab")
			(uuid "6d3d3d85-bd53-44cb-882f-2da2c159d6dd")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1 0 270)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net "Net-(SIG1-Pin_1)")
			(pintype "passive")
			(uuid "2e707287-9768-475f-ae7d-4c004647343c")
		)
		(pad "2" smd roundrect
			(at 1 0 270)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net "Net-(GND1-Pin_1)")
			(pintype "passive")
			(uuid "98f68cfe-becf-4b3b-bd71-7fe2abe8edce")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Library:H850405"
		(layer "F.Cu")
		(uuid "12ffd4e7-5807-43d9-811b-8073bef012b5")
		(at 122.5 70)
		(descr "H8504-05-1")
		(tags "Connector")
		(property "Reference" "HV1"
			(at 0 0 0)
			(layer "F.SilkS")
			(uuid "312f887f-9ced-46ef-9d9e-479b5fda29d4")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.254)
				)
			)
		)
		(property "Value" "Conn_01x01_Socket"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
			(uuid "050d06e6-4dc2-418c-ad2c-4a08c5d5b8b6")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.254)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "6d71ec03-0096-400f-bfcd-6e26d39c2b73")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "d5c8a29e-f361-42e2-aa41-6328b3d088dd")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(path "/d9fd39f2-e4f9-475b-ab1e-eb9a189a110b")
		(sheetname "Root")
		(sheetfile "PMT1inchBase.kicad_sch")
		(attr through_hole)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_line
			(start -2 0)
			(end -2 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "ad4f80d8-5747-4d9b-ae45-76d7fababb1b")
		)
		(fp_line
			(start 2 0)
			(end 2 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "732e979b-765f-43b8-9345-b21cf5081af5")
		)
		(fp_arc
			(start -2 0)
			(mid 0 -2)
			(end 2 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "dc1dc546-f130-4d4e-a082-ff75f1e0b12c")
		)
		(fp_arc
			(start 2 0)
			(mid 0 2)
			(end -2 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "15d5cb8e-6562-467f-94d8-1b88b9074be4")
		)
		(fp_line
			(start -3 -3)
			(end 3 -3)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "0b9d12a3-3455-430b-bad7-3d5d91e2beac")
		)
		(fp_line
			(start -3 3)
			(end -3 -3)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "de358081-a947-431b-a795-f10e9967aa33")
		)
		(fp_line
			(start 3 -3)
			(end 3 3)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "6345c569-a481-4bdd-9479-e6ee0d57d628")
		)
		(fp_line
			(start 3 3)
			(end -3 3)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "96a3f828-3396-4073-a477-4363d584b9bb")
		)
		(fp_line
			(start -2 0)
			(end -2 0)
			(stroke
				(width 0.2)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "78086f71-bc37-4c60-ae07-cf6dab26fcb9")
		)
		(fp_line
			(start 2 0)
			(end 2 0)
			(stroke
				(width 0.2)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "62bb6193-ed54-40e7-846f-07fe5eec0dc1")
		)
		(fp_arc
			(start -2 0)
			(mid 0 -2)
			(end 2 0)
			(stroke
				(width 0.2)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "121ab90c-8e6c-48d0-ac03-8b098057f3aa")
		)
		(fp_arc
			(start 2 0)
			(mid 0 2)
			(end -2 0)
			(stroke
				(width 0.2)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "bf778a83-2a9a-4495-b168-90419979780f")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "cec62cb1-ad79-417a-9dac-ea5eca5e6ca7")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.254)
				)
			)
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 3.015 3.015)
			(drill 2.01)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "Net-(HV1-Pin_1)")
			(pinfunction "Pin_1")
			(pintype "passive")
			(uuid "5f841bff-efe9-48dc-b1eb-1703393d9dfd")
		)
		(embedded_fonts no)
		(model "H8504-05.stp"
			(offset
				(xyz 0 0 0.8999999626)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 90 -180 0)
			)
		)
	)
	(footprint "Library:H315305"
		(layer "F.Cu")
		(uuid "2f6adad6-e29d-497a-a9fb-a47f1eb81d18")
		(at 138.46 64.5)
		(descr "H3153-05-2")
		(tags "Connector")
		(property "Reference" "K1"
			(at 0 -2.5 0)
			(layer "F.SilkS")
			(uuid "8e6e2f14-40fb-48dd-bf6c-eb216b58027c")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.254)
				)
			)
		)
		(property "Value" "Conn_01x01_Socket"
			(at -0.5 -3 0)
			(layer "F.SilkS")
			(hide yes)
			(uuid "c1631d55-07b1-40e5-b51d-f161dcf17bc9")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.254)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "4e9f8afe-36f8-4f62-92a1-dc9a4bd45559")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "c151f507-6434-41ad-b109-af5f9cb45b2e")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Manufacturer" "Harwin"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
			(uuid "0dc96976-deb8-43f3-bc08-dcd84c96ad66")
			(effects
				(font
					(size 1 1)
					(thickness 0.1)
				)
			)
		)
		(property "MPN" "H3153-05"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
			(uuid "395676a9-c4d1-4d51-998c-e7625f8a3344")
			(effects
				(font
					(size 1 1)
					(thickness 0.1)
				)
			)
		)
		(property "Supplier" "Mouser"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
			(uuid "8d8a9c36-46aa-4ade-8ed7-969d77f16dd7")
			(effects
				(font
					(size 1 1)
					(thickness 0.1)
				)
			)
		)
		(property "Supplier Part Number" "855-H3153-05"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
			(uuid "5bdba91c-94c7-47c8-8e48-11ecdd8ff302")
			(effects
				(font
					(size 1 1)
					(thickness 0.1)
				)
			)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(path "/1a1bff47-01da-4bed-ac2d-c77cbeb44eb9")
		(sheetname "Root")
		(sheetfile "PMT1inchBase.kicad_sch")
		(attr through_hole)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_line
			(start -1.2 0)
			(end -1.2 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "9ea66d29-03ce-4925-882e-1f098062b23e")
		)
		(fp_line
			(start 1.2 0)
			(end 1.2 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "4c1b3930-dcda-4ebf-8d26-4e7dd29b6d28")
		)
		(fp_arc
			(start -1.2 0)
			(mid 0 -1.2)
			(end 1.2 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "574e2065-6ec4-45ab-80c0-e571a4d7c323")
		)
		(fp_arc
			(start 1.2 0)
			(mid 0 1.2)
			(end -1.2 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "c7e50148-5301-434d-aa81-23364ec49eb4")
		)
		(fp_line
			(start -1.2 -1.2)
			(end 1.2 -1.2)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "4601ebdf-32f9-426c-a7e4-b7e4b220db47")
		)
		(fp_line
			(start -1.2 1.2)
			(end -1.2 -1.2)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "313ed92d-6897-489a-8141-068c2b69770a")
		)
		(fp_line
			(start 1.2 -1.2)
			(end 1.2 1.2)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "92ab5b59-bdf1-4047-8cec-deb1bd6bbb57")
		)
		(fp_line
			(start 1.2 1.2)
			(end -1.2 1.2)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "c9faa78c-0434-4286-bb3b-63db70d640be")
		)
		(fp_line
			(start -1.2 0)
			(end -1.2 0)
			(stroke
				(width 0.2)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "70823fec-9fee-46de-8b70-88d2428697f6")
		)
		(fp_line
			(start 1.2 0)
			(end 1.2 0)
			(stroke
				(width 0.2)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "2e1fec76-b295-4b07-98d5-72fd5e7c5a3e")
		)
		(fp_arc
			(start -1.2 0)
			(mid 0 -1.2)
			(end 1.2 0)
			(stroke
				(width 0.2)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "cbed1cc3-2159-4557-9734-ae4bd384bd0b")
		)
		(fp_arc
			(start 1.2 0)
			(mid 0 1.2)
			(end -1.2 0)
			(stroke
				(width 0.2)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "204c66bf-814c-42a9-9b3e-526835103df0")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "67e5d82f-78f7-4a20-9fca-4a265b30aece")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.254)
				)
			)
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1.65 1.65)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "Net-(HV1-Pin_1)")
			(pinfunction "Pin_1")
			(pintype "passive")
			(uuid "0b3e0e87-37f4-4535-a14c-8476a18d9e22")
		)
		(embedded_fonts no)
		(model "${KIPRJMOD}/3dmodels/H3153-05.stp"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -0 -90 -0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder"
		(layer "F.Cu")
		(uuid "330fa7d5-78cd-4a98-9d21-411d7f4832a7")
		(at 134.8625 78.7)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "capacitor handsolder")
		(property "Reference" "C1"
			(at 0 -1.43 0)
			(layer "F.SilkS")
			(uuid "94bfd5d8-3b59-4fee-91d3-ef4040090449")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "10 nF"
			(at 0 1.43 0)
			(layer "F.Fab")
			(uuid "c4a4e941-0d6c-4456-90d6-aa27abd42c9f")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "55ec043d-0be3-4cf8-a022-701897a2221a")
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "bdb309c2-3bbe-478a-b075-8b90a44280ff")
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
			(uuid "b522f9b5-f2df-4d0f-851b-c4f3bf635447")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Manufacturer" "TDK"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "5d0e7bf1-7bb0-4626-9cf0-e60d73920582")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "MPN" "CGA3E1C0G2A103J080AC"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "59f71fdf-e147-479e-977e-be2314dcbff6")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Supplier Part Number" "810-CGA3E1C0G2A103J080AC"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "8072d6ff-895a-4bd2-b943-e1fd70c92a91")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/b9ea74fe-a470-4f7b-b715-4eef452bc421")
		(sheetname "Root")
		(sheetfile "PMT1inchBase.kicad_sch")
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_line
			(start -0.146267 -0.51)
			(end 0.146267 -0.51)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "bf5ddfba-5d8b-4fb0-b1ff-8bd8c378bcba")
		)
		(fp_line
			(start -0.146267 0.51)
			(end 0.146267 0.51)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "da6636b1-3ed3-4b5a-b43b-3b7663390027")
		)
		(fp_rect
			(start -1.65 -0.73)
			(end 1.65 0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(fill no)
			(layer "F.CrtYd")
			(uuid "55016bfd-c003-4516-873f-ef1caab07686")
		)
		(fp_rect
			(start -0.8 -0.4)
			(end 0.8 0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill no)
			(layer "F.Fab")
			(uuid "853654c6-db7d-48c3-b48d-3de310ddad8b")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "7e73bf0e-5358-4264-b2ef-8cffbbc955e9")
			(effects
				(font
					(size 0.4 0.4)
					(thickness 0.06)
				)
			)
		)
		(pad "1" smd roundrect
			(at -0.8625 0)
			(size 1.075 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "Net-(D7-Pin_1)")
			(pintype "passive")
			(uuid "96c721ff-5d6f-446e-8953-d74a2ff9c211")
		)
		(pad "2" smd roundrect
			(at 0.8625 0)
			(size 1.075 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "Net-(D8-Pin_1)")
			(pintype "passive")
			(uuid "6e70bd77-f7bf-4f65-87ef-21c0ed49e6cc")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(uuid "3399b9ac-f320-49b4-b1f6-ca34915bfd4b")
		(at 141 62)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "resistor handsolder")
		(property "Reference" "R1"
			(at 0 -1.65 0)
			(layer "F.SilkS")
			(uuid "d6d4847c-a0fa-47b6-8294-a6d13de42fc4")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "2.49M"
			(at 0 1.65 0)
			(layer "F.Fab")
			(uuid "66be6fd8-cdd6-4273-98e7-d5489617bdb4")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "a78f26ce-ae91-4015-bee6-dc7031f7716e")
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "6ada6992-d94e-4568-8cc9-b5095a1b0485")
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
			(uuid "59373d1a-ffbe-4cd0-be5c-7b50376bc74f")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Manufacturer" "KOA Speer"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "98d840b5-d7dd-4543-92a4-9cd044dba909")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "MPN" "RS73G2ARTTD2494B"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "80cbdb4b-7977-4156-88d4-85700b2d9eb7")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Supplier Part Number" "660-RS73G2ARTTD2494B"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "9f6fd5af-740a-4ee9-9246-769339c6455c")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/13f3ebe3-3547-4fed-a8be-4c86e4038d94")
		(sheetname "Root")
		(sheetfile "PMT1inchBase.kicad_sch")
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_line
			(start -0.227064 -0.735)
			(end 0.227064 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "e782ec76-7d2a-4c68-ae4f-3233a9f1fef8")
		)
		(fp_line
			(start -0.227064 0.735)
			(end 0.227064 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "afbc8585-b468-4517-b386-aa1fb621be7e")
		)
		(fp_rect
			(start -1.85 -0.95)
			(end 1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(fill no)
			(layer "F.CrtYd")
			(uuid "34b75a64-f049-457b-8a44-d5e676708ca2")
		)
		(fp_rect
			(start -1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill no)
			(layer "F.Fab")
			(uuid "34129f5d-ee9a-4481-ba39-793161c1655c")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "ca3af8da-8e77-4935-9632-b9291f857436")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net "Net-(HV1-Pin_1)")
			(pintype "passive")
			(uuid "a1fd6bcb-60bc-4867-8082-6613919078bd")
		)
		(pad "2" smd roundrect
			(at 1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net "Net-(G1-Pin_1)")
			(pintype "passive")
			(uuid "c4f948b0-d313-46e5-a641-b65b34b39200")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder"
		(layer "F.Cu")
		(uuid "43f0e904-812d-4105-82a2-faf0fa8dd65f")
		(at 137.5 79.3625 -90)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "capacitor handsolder")
		(property "Reference" "C2"
			(at 0 -1.43 270)
			(layer "F.SilkS")
			(uuid "39fd0eb9-f54e-43c0-ba37-3b0725eb73be")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "10 nF"
			(at 0 1.43 270)
			(layer "F.Fab")
			(uuid "8fb9be5f-13c0-4e88-95cb-1027fcf58c7a")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
			(uuid "b3580bba-2ec4-4077-bff3-af1d019b33ed")
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Description" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
			(uuid "3d06e94b-9d1a-4be7-92d4-0ca274ef418e")
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 270)
			(layer "F.SilkS")
			(hide yes)
			(uuid "461cc084-6dd3-421a-8f83-dae08d679eaf")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Manufacturer" "TDK"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "7b9abdec-5033-43dd-8c92-02076581cfcc")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "MPN" "CGA3E1C0G2A103J080AC"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "e8a78cc0-97c0-4dcf-ade1-d964bf846a2c")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Supplier Part Number" "810-CGA3E1C0G2A103J080AC"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "a88d0f9c-af82-4fd2-b46c-12dc9f84006b")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/5643de0d-1c7e-4319-a55e-7547d488e969")
		(sheetname "Root")
		(sheetfile "PMT1inchBase.kicad_sch")
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_line
			(start -0.146267 0.51)
			(end 0.146267 0.51)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "f4694940-7a01-46d6-b61a-6c64ae598be6")
		)
		(fp_line
			(start -0.146267 -0.51)
			(end 0.146267 -0.51)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "86d2ce73-f8ff-467b-9002-c017a9ba840b")
		)
		(fp_rect
			(start -1.65 -0.73)
			(end 1.65 0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(fill no)
			(layer "F.CrtYd")
			(uuid "30bd61c0-04f1-4968-904b-aa3e41460e2e")
		)
		(fp_rect
			(start -0.8 -0.4)
			(end 0.8 0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill no)
			(layer "F.Fab")
			(uuid "c2ea2e9b-b283-4fcd-b9b2-d9041ecf57bb")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 270)
			(layer "F.Fab")
			(uuid "5c6246f2-e7c2-423d-beb1-afc0dec793c6")
			(effects
				(font
					(size 0.4 0.4)
					(thickness 0.06)
				)
			)
		)
		(pad "1" smd roundrect
			(at -0.8625 0 270)
			(size 1.075 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "Net-(D8-Pin_1)")
			(pintype "passive")
			(uuid "7a422338-6948-48db-9472-0b298c608ee8")
		)
		(pad "2" smd roundrect
			(at 0.8625 0 270)
			(size 1.075 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "Net-(D9-Pin_1)")
			(pintype "passive")
			(uuid "73a5aa90-b905-48ff-8ba9-6a4e1d0cc4b9")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Library:H315305"
		(layer "F.Cu")
		(uuid "45c429fd-96c7-4fa7-9371-9ea51b72130a")
		(at 130.82 84.82)
		(descr "H3153-05-2")
		(tags "Connector")
		(property "Reference" "D6"
			(at 0 -2.5 0)
			(layer "F.SilkS")
			(uuid "60d36758-67a9-4d09-b4f4-e83915fd1cb0")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.254)
				)
			)
		)
		(property "Value" "Conn_01x01_Socket"
			(at -0.5 -3 0)
			(layer "F.SilkS")
			(hide yes)
			(uuid "ebef9c8d-24d0-4733-a83b-c78526ef1d2c")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.254)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "6eef6116-5aea-4e06-950e-2440030502f4")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "7305bc0a-f0ce-4b5d-8368-593c05948fd2")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Manufacturer" "Harwin"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
			(uuid "9fe1b621-6e41-4a35-b511-54846cc9f682")
			(effects
				(font
					(size 1 1)
					(thickness 0.1)
				)
			)
		)
		(property "MPN" "H3153-05"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
			(uuid "38675d2e-2d80-464c-8b13-bc12f34fdb14")
			(effects
				(font
					(size 1 1)
					(thickness 0.1)
				)
			)
		)
		(property "Supplier" "Mouser"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
			(uuid "bb8e5bf7-fb8c-41e4-8557-bfe7fe920ac2")
			(effects
				(font
					(size 1 1)
					(thickness 0.1)
				)
			)
		)
		(property "Supplier Part Number" "855-H3153-05"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
			(uuid "13e5c45d-6a83-44aa-8510-bf914508aaf9")
			(effects
				(font
					(size 1 1)
					(thickness 0.1)
				)
			)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(path "/11b67a44-b4b5-4e69-8655-3809b238dbef")
		(sheetname "Root")
		(sheetfile "PMT1inchBase.kicad_sch")
		(attr through_hole)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_line
			(start -1.2 0)
			(end -1.2 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "8c5054e6-d880-4dea-9d66-0d8a99af3b1f")
		)
		(fp_line
			(start 1.2 0)
			(end 1.2 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "884d777a-046b-4562-8e28-a63e883f191d")
		)
		(fp_arc
			(start -1.2 0)
			(mid 0 -1.2)
			(end 1.2 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "9e85d85f-86f6-44ce-bcae-09f18628c2af")
		)
		(fp_arc
			(start 1.2 0)
			(mid 0 1.2)
			(end -1.2 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "4629d2b3-8991-4703-87f8-5e9e85271cd3")
		)
		(fp_line
			(start -1.2 -1.2)
			(end 1.2 -1.2)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "495e895c-fe0b-4eef-a565-b20920f1b08c")
		)
		(fp_line
			(start -1.2 1.2)
			(end -1.2 -1.2)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "bc96e335-e72c-443b-9d64-dfa826f06094")
		)
		(fp_line
			(start 1.2 -1.2)
			(end 1.2 1.2)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "58839c00-6010-4cb5-bc08-c0d6a3589261")
		)
		(fp_line
			(start 1.2 1.2)
			(end -1.2 1.2)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "0dc3d14e-83c8-4d24-accf-aa99ef76151b")
		)
		(fp_line
			(start -1.2 0)
			(end -1.2 0)
			(stroke
				(width 0.2)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "0515d507-ceac-462f-b33a-f4cf4d558a28")
		)
		(fp_line
			(start 1.2 0)
			(end 1.2 0)
			(stroke
				(width 0.2)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "ed17765f-34ef-447e-9e9a-8b52d035697d")
		)
		(fp_arc
			(start -1.2 0)
			(mid 0 -1.2)
			(end 1.2 0)
			(stroke
				(width 0.2)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "374d53ec-517b-4048-ae84-f26b0982e92c")
		)
		(fp_arc
			(start 1.2 0)
			(mid 0 1.2)
			(end -1.2 0)
			(stroke
				(width 0.2)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "019a5371-a407-4d39-921b-b6f0d22911f8")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "9f4bf598-6696-46ec-951c-79e9179d9212")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.254)
				)
			)
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1.65 1.65)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "Net-(D6-Pin_1)")
			(pinfunction "Pin_1")
			(pintype "passive")
			(uuid "cbe423d1-a90a-4c46-b0cd-c2cced1dcb08")
		)
		(embedded_fonts no)
		(model "${KIPRJMOD}/3dmodels/H3153-05.stp"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -0 -90 -0)
			)
		)
	)
	(footprint "Library:H315305"
		(layer "F.Cu")
		(uuid "479226db-c0a8-41df-98dd-95bfff6ee324")
		(at 135.92 64.5)
		(descr "H3153-05-2")
		(tags "Connector")
		(property "Reference" "D1"
			(at 0 -2.5 0)
			(layer "F.SilkS")
			(uuid "06d84915-4677-484f-ba3b-2df6b4a59c8c")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.254)
				)
			)
		)
		(property "Value" "Conn_01x01_Socket"
			(at -0.5 -3 0)
			(layer "F.SilkS")
			(hide yes)
			(uuid "7b8eff60-4df7-42b9-a48e-8d430a516d38")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.254)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "b37dc93a-b6b7-441e-99e3-16204c8a1d97")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "45d608fe-6a77-4c37-b2aa-50fbe781c3df")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Manufacturer" "Harwin"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
			(uuid "9ea8e10e-1568-498e-b8c4-ce340372380b")
			(effects
				(font
					(size 1 1)
					(thickness 0.1)
				)
			)
		)
		(property "MPN" "H3153-05"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
			(uuid "774078e2-d5e8-41ac-99a6-f427a1c7aad0")
			(effects
				(font
					(size 1 1)
					(thickness 0.1)
				)
			)
		)
		(property "Supplier" "Mouser"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
			(uuid "07febff5-d867-4677-b4ff-e51d11c8d23b")
			(effects
				(font
					(size 1 1)
					(thickness 0.1)
				)
			)
		)
		(property "Supplier Part Number" "855-H3153-05"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
			(uuid "66db0a3f-163c-4855-bd6e-4474074a0159")
			(effects
				(font
					(size 1 1)
					(thickness 0.1)
				)
			)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(path "/e3838803-9671-47c9-9c47-f357686f4efd")
		(sheetname "Root")
		(sheetfile "PMT1inchBase.kicad_sch")
		(attr through_hole)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_line
			(start -1.2 0)
			(end -1.2 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "c91afdf6-51b6-49e7-84af-edac96a15758")
		)
		(fp_line
			(start 1.2 0)
			(end 1.2 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "5dc67345-e735-482e-bc25-101a0c53c2b6")
		)
		(fp_arc
			(start -1.2 0)
			(mid 0 -1.2)
			(end 1.2 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "20de5bef-eff5-4eb8-aea3-a2b65955e7a4")
		)
		(fp_arc
			(start 1.2 0)
			(mid 0 1.2)
			(end -1.2 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "05b6792b-5c1d-4ac4-9558-f094240f8266")
		)
		(fp_line
			(start -1.2 -1.2)
			(end 1.2 -1.2)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "1005741d-bc84-496e-9d33-58ac684d8ecb")
		)
		(fp_line
			(start -1.2 1.2)
			(end -1.2 -1.2)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "dd9adbe3-e774-40fe-858a-fb96934af05a")
		)
		(fp_line
			(start 1.2 -1.2)
			(end 1.2 1.2)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "2ac8f7f5-a686-4cc3-8898-324bd81d95d3")
		)
		(fp_line
			(start 1.2 1.2)
			(end -1.2 1.2)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "6d898727-fb31-4c7e-abf1-f66376a27764")
		)
		(fp_line
			(start -1.2 0)
			(end -1.2 0)
			(stroke
				(width 0.2)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "2f92be10-0d83-4c54-9af7-31e2b46a2d2b")
		)
		(fp_line
			(start 1.2 0)
			(end 1.2 0)
			(stroke
				(width 0.2)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "066a990a-0ada-4b72-a462-54c95a962433")
		)
		(fp_arc
			(start -1.2 0)
			(mid 0 -1.2)
			(end 1.2 0)
			(stroke
				(width 0.2)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "43d5b8e1-45e9-40bb-9922-f93e2fbdac0d")
		)
		(fp_arc
			(start 1.2 0)
			(mid 0 1.2)
			(end -1.2 0)
			(stroke
				(width 0.2)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "b6b81368-8b72-45e0-8126-946a4f1fd6a1")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "fb8728ff-a495-463e-bd8d-f9d355c0409b")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.254)
				)
			)
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1.65 1.65)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "Net-(D1-Pin_1)")
			(pinfunction "Pin_1")
			(pintype "passive")
			(uuid "f90c2aa6-b7e3-4b6b-8559-53e3bfb8d3c1")
		)
		(embedded_fonts no)
		(model "${KIPRJMOD}/3dmodels/H3153-05.stp"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -0 -90 -0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(uuid "500db8c5-1cf2-480c-81be-38cb92b062f8")
		(at 134.5 80.5)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "resistor handsolder")
		(property "Reference" "R9"
			(at 0 -1.65 0)
			(layer "F.SilkS")
			(uuid "555af8c1-0749-41ab-b8b1-5821291394ba")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "4.99M"
			(at 0 1.65 0)
			(layer "F.Fab")
			(uuid "134d31ef-74f7-40c5-be79-e54d5604a19c")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "73935e59-d43d-4550-966a-76cea3428d0a")
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "fc08a913-2d55-4e51-a173-c167c5a469f4")
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
			(uuid "959e6f1f-dc65-4621-8098-0288c1419826")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Manufacturer" "KOA Speer"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "1cbf7318-2099-4984-80f9-13ca2d1d36d2")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "MPN" "RS73F2ATTD4994D"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "332ffab6-69c9-4834-8a1d-de499eb5e54b")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Supplier Part Number" "660-RS73F2ATTD4994D"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "06ca8d78-8411-4444-ad18-616d6d7138c4")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/babaf992-a90e-438c-a823-039d80e46f94")
		(sheetname "Root")
		(sheetfile "PMT1inchBase.kicad_sch")
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_line
			(start -0.227064 -0.735)
			(end 0.227064 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "87307b9c-1220-4b51-b1e7-4847a188874c")
		)
		(fp_line
			(start -0.227064 0.735)
			(end 0.227064 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "1d1adf7a-dc6c-418c-a00f-151acefd3afe")
		)
		(fp_rect
			(start -1.85 -0.95)
			(end 1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(fill no)
			(layer "F.CrtYd")
			(uuid "10fe9e18-9bbb-4612-a1d8-d87bee1e5887")
		)
		(fp_rect
			(start -1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill no)
			(layer "F.Fab")
			(uuid "3d6a6693-c86c-4ef6-bf33-aefa6aeef7be")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "a685a385-b246-4185-905c-c53f40e5636b")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net "Net-(D7-Pin_1)")
			(pintype "passive")
			(uuid "93af776d-71e4-4be7-ae8a-b191c524da7f")
		)
		(pad "2" smd roundrect
			(at 1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net "Net-(D8-Pin_1)")
			(pintype "passive")
			(uuid "8169269f-aa90-4243-a0be-9f765e99e3d4")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Library:H315305"
		(layer "F.Cu")
		(uuid "512da8f4-2126-4e7d-99a9-ff1e99845b7f")
		(at 141 84.82)
		(descr "H3153-05-2")
		(tags "Connector")
		(property "Reference" "D10"
			(at 0 -2.5 0)
			(layer "F.SilkS")
			(uuid "e62ab2fa-0aea-4064-8ac5-9834f6378c25")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.254)
				)
			)
		)
		(property "Value" "Conn_01x01_Socket"
			(at -0.5 -3 0)
			(layer "F.SilkS")
			(hide yes)
			(uuid "5173e08c-1e2b-4763-a985-f94f230f8fe7")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.254)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "f73ef78a-b871-486f-9e28-e7970c872866")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "6d5f29b3-a136-493d-8d26-cf9ef51665da")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Manufacturer" "Harwin"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
			(uuid "7bfc7a36-335a-42ef-8fce-cd09b95bf663")
			(effects
				(font
					(size 1 1)
					(thickness 0.1)
				)
			)
		)
		(property "MPN" "H3153-05"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
			(uuid "41e5e333-49a9-4ed0-921d-6340ffb0b8bc")
			(effects
				(font
					(size 1 1)
					(thickness 0.1)
				)
			)
		)
		(property "Supplier" "Mouser"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
			(uuid "43819427-30cb-4c0c-a6fb-67e3568ecda7")
			(effects
				(font
					(size 1 1)
					(thickness 0.1)
				)
			)
		)
		(property "Supplier Part Number" "855-H3153-05"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
			(uuid "c36d9b65-89fb-45eb-86e3-da98f8b5645d")
			(effects
				(font
					(size 1 1)
					(thickness 0.1)
				)
			)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(path "/730aa034-5bc1-44f5-a77d-b7af6d89708a")
		(sheetname "Root")
		(sheetfile "PMT1inchBase.kicad_sch")
		(attr through_hole)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_line
			(start -1.2 0)
			(end -1.2 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "a61b683c-8891-4f69-9f49-189a2c74d7b9")
		)
		(fp_line
			(start 1.2 0)
			(end 1.2 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "607a04c5-e3c7-44fa-b39c-1d72e8bba0de")
		)
		(fp_arc
			(start -1.2 0)
			(mid 0 -1.2)
			(end 1.2 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "e83518e1-155a-4f2b-8abb-c595b3e2d854")
		)
		(fp_arc
			(start 1.2 0)
			(mid 0 1.2)
			(end -1.2 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "c30ab076-7ce7-489e-83b9-aa35734067ac")
		)
		(fp_line
			(start -1.2 -1.2)
			(end 1.2 -1.2)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "2266f73c-40a8-441f-9eff-28ab00edc92f")
		)
		(fp_line
			(start -1.2 1.2)
			(end -1.2 -1.2)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "02e8ec2e-0aaa-4b27-b287-e5fc7f1aff6b")
		)
		(fp_line
			(start 1.2 -1.2)
			(end 1.2 1.2)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "e58feedf-651f-4cc9-8daa-912dbf3e2c4e")
		)
		(fp_line
			(start 1.2 1.2)
			(end -1.2 1.2)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "cb6fb28e-2a8f-49d8-a9d4-dad4d53973d5")
		)
		(fp_line
			(start -1.2 0)
			(end -1.2 0)
			(stroke
				(width 0.2)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "b028bbc1-7563-45c2-b415-6382cee87528")
		)
		(fp_line
			(start 1.2 0)
			(end 1.2 0)
			(stroke
				(width 0.2)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "59e8f686-b38e-4043-a284-c36d9e0492d1")
		)
		(fp_arc
			(start -1.2 0)
			(mid 0 -1.2)
			(end 1.2 0)
			(stroke
				(width 0.2)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "d5dea257-d6ab-4e91-b817-ecbafb883e71")
		)
		(fp_arc
			(start 1.2 0)
			(mid 0 1.2)
			(end -1.2 0)
			(stroke
				(width 0.2)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "8cda6ad8-b99e-485c-9c4c-10813ea89841")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "51428147-6436-406c-8632-9f33f716a69c")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.254)
				)
			)
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1.65 1.65)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "Net-(D10-Pin_1)")
			(pinfunction "Pin_1")
			(pintype "passive")
			(uuid "910e0c17-d016-4881-9e44-29fffba7a25f")
		)
		(embedded_fonts no)
		(model "${KIPRJMOD}/3dmodels/H3153-05.stp"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -0 -90 -0)
			)
		)
	)
	(footprint "Library:H315305"
		(layer "F.Cu")
		(uuid "63b923ce-171b-491c-bcdd-d69167bba0ef")
		(at 138.46 84.82)
		(descr "H3153-05-2")
		(tags "Connector")
		(property "Reference" "D9"
			(at 0 -2.5 0)
			(layer "F.SilkS")
			(uuid "e6d5f70c-858a-43a0-b23f-97738ce04d01")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.254)
				)
			)
		)
		(property "Value" "Conn_01x01_Socket"
			(at -0.5 -3 0)
			(layer "F.SilkS")
			(hide yes)
			(uuid "58e35e9a-0788-49d5-a439-4938c9b4b597")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.254)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "0f71c8f5-ed5d-4b1d-82dd-4eff165b7ddf")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "7986f505-b8c2-4e59-8b78-65cdaeef36f4")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Manufacturer" "Harwin"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
			(uuid "eb0b9605-206f-49cd-beb6-90a2330cd729")
			(effects
				(font
					(size 1 1)
					(thickness 0.1)
				)
			)
		)
		(property "MPN" "H3153-05"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
			(uuid "7c40ec3d-391b-4cb0-b8e7-204bb5f1921b")
			(effects
				(font
					(size 1 1)
					(thickness 0.1)
				)
			)
		)
		(property "Supplier" "Mouser"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
			(uuid "3b4b8685-724d-4c66-ba8f-c2dfaae3e2d6")
			(effects
				(font
					(size 1 1)
					(thickness 0.1)
				)
			)
		)
		(property "Supplier Part Number" "855-H3153-05"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
			(uuid "41c3778c-ea67-4524-b338-98dbe5414019")
			(effects
				(font
					(size 1 1)
					(thickness 0.1)
				)
			)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(path "/4fec1c5d-dc85-4965-a669-5b733834cfc9")
		(sheetname "Root")
		(sheetfile "PMT1inchBase.kicad_sch")
		(attr through_hole)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_line
			(start -1.2 0)
			(end -1.2 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "596f526c-d14b-4193-93cc-bedb8d3e639d")
		)
		(fp_line
			(start 1.2 0)
			(end 1.2 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "22b6d0ef-fb5c-472f-8339-9df56dd96516")
		)
		(fp_arc
			(start -1.2 0)
			(mid 0 -1.2)
			(end 1.2 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "5ae52d72-bcf1-4a6d-b1dd-e1001a44787a")
		)
		(fp_arc
			(start 1.2 0)
			(mid 0 1.2)
			(end -1.2 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "18fc8d66-d368-47ae-b46a-509dc19020a1")
		)
		(fp_line
			(start -1.2 -1.2)
			(end 1.2 -1.2)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "77f30897-2df7-4acb-a938-047255ed12e0")
		)
		(fp_line
			(start -1.2 1.2)
			(end -1.2 -1.2)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "6750b200-7e61-40d1-8d0a-9e17f353b2cf")
		)
		(fp_line
			(start 1.2 -1.2)
			(end 1.2 1.2)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "8c5429ae-9078-4af0-8fe4-823b60497525")
		)
		(fp_line
			(start 1.2 1.2)
			(end -1.2 1.2)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "cd0ee5b4-4639-41a5-8004-d5530fbfbed0")
		)
		(fp_line
			(start -1.2 0)
			(end -1.2 0)
			(stroke
				(width 0.2)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "b132377b-c1be-46e4-a804-669f09ab9b7c")
		)
		(fp_line
			(start 1.2 0)
			(end 1.2 0)
			(stroke
				(width 0.2)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "629509ff-7862-4d5e-aa87-a77ef4dcc242")
		)
		(fp_arc
			(start -1.2 0)
			(mid 0 -1.2)
			(end 1.2 0)
			(stroke
				(width 0.2)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "2368058f-b6d5-4c8c-8218-bc43a987d4af")
		)
		(fp_arc
			(start 1.2 0)
			(mid 0 1.2)
			(end -1.2 0)
			(stroke
				(width 0.2)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "b3754450-588d-4835-bef9-49b5b14a884d")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "18dce3d1-472a-4c00-aedc-941af810ec14")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.254)
				)
			)
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1.65 1.65)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "Net-(D9-Pin_1)")
			(pinfunction "Pin_1")
			(pintype "passive")
			(uuid "0f930bbe-9a83-4836-a737-f2fa15764c2c")
		)
		(embedded_fonts no)
		(model "${KIPRJMOD}/3dmodels/H3153-05.stp"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -0 -90 -0)
			)
		)
	)
	(footprint "Library:H850405"
		(layer "F.Cu")
		(uuid "6584612c-8d9d-4647-b5eb-fca1280712ff")
		(at 144.5 73)
		(descr "H8504-05-1")
		(tags "Connector")
		(property "Reference" "SIG1"
			(at 0 0 0)
			(layer "F.SilkS")
			(uuid "f5ccc58b-f432-4bdc-950a-30b3ee210264")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.254)
				)
			)
		)
		(property "Value" "Conn_01x01_Socket"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
			(uuid "5ba2e941-bc5b-45ed-92ba-00ff3d129e21")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.254)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "855c9708-d900-4864-acf0-0091c8af8a2a")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "5dfba56e-683d-448d-a659-950ca0f4db64")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(path "/41086488-f662-4563-be0d-431f96f11c84")
		(sheetname "Root")
		(sheetfile "PMT1inchBase.kicad_sch")
		(attr through_hole)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_line
			(start -2 0)
			(end -2 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "8f8b01a9-d74c-4917-8e99-8d7971c0efcb")
		)
		(fp_line
			(start 2 0)
			(end 2 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "46ed83be-a247-49e2-a4a6-9c6a165b8458")
		)
		(fp_arc
			(start -2 0)
			(mid 0 -2)
			(end 2 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "e6870273-c4d8-4940-941c-4cf5ce641963")
		)
		(fp_arc
			(start 2 0)
			(mid 0 2)
			(end -2 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "cfdec1bf-ac9c-4b1c-a7d4-9e736b747f7e")
		)
		(fp_line
			(start -3 -3)
			(end 3 -3)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "a90ab0a1-39ad-42b2-988f-b8a1ea3c2709")
		)
		(fp_line
			(start -3 3)
			(end -3 -3)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "739c5b0e-9802-4c38-a80c-de6834030e98")
		)
		(fp_line
			(start 3 -3)
			(end 3 3)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "d8431b86-7a4c-4ef8-9ed7-b1f027b5e89c")
		)
		(fp_line
			(start 3 3)
			(end -3 3)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "9a3d1b7f-6ffb-4d3d-901e-4484b25508bf")
		)
		(fp_line
			(start -2 0)
			(end -2 0)
			(stroke
				(width 0.2)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "aab66bfa-593f-48f8-9dfe-850e0fc80802")
		)
		(fp_line
			(start 2 0)
			(end 2 0)
			(stroke
				(width 0.2)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "47ea6bd0-32c7-427c-863b-21b712b9d133")
		)
		(fp_arc
			(start -2 0)
			(mid 0 -2)
			(end 2 0)
			(stroke
				(width 0.2)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "83b526de-bba6-484a-9bcf-ba665d025729")
		)
		(fp_arc
			(start 2 0)
			(mid 0 2)
			(end -2 0)
			(stroke
				(width 0.2)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "5b28baee-236b-42be-83b8-008758e2d0cf")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "3996938e-32b0-4a06-8852-f7952096f994")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.254)
				)
			)
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 3.015 3.015)
			(drill 2.01)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "Net-(SIG1-Pin_1)")
			(pinfunction "Pin_1")
			(pintype "passive")
			(uuid "c61ed44c-b8bf-4cb7-9fa7-4ceed8aa3675")
		)
		(embedded_fonts no)
		(model "H8504-05.stp"
			(offset
				(xyz 0 0 0.8999999626)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 90 -180 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(uuid "7c256387-79b9-4c70-b0b0-8d97cf0a456c")
		(at 137.5 67 180)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "resistor handsolder")
		(property "Reference" "R2"
			(at 0 -1.65 180)
			(layer "F.SilkS")
			(uuid "eb6daaeb-7a99-4f86-b1c7-55d5445bc5ff")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "7.5M"
			(at 0 1.65 180)
			(layer "F.Fab")
			(uuid "c630d978-0cc6-4754-8723-cac117170c2a")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
			(uuid "ea6538c6-bb7c-48bf-86b2-f56082d0617e")
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
			(uuid "30c304d4-3ba2-483c-b783-5d90cdf881de")
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 180)
			(layer "F.SilkS")
			(hide yes)
			(uuid "65022c79-79c9-45a6-bdf6-b2a68ba6914f")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Manufacturer" "Vishay"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "4e762ebe-5c87-4c31-ba91-5c6261ea1c54")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "MPN" "CRCW08057M50FKEA"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "2cd5656c-5d79-4293-b429-0955b3b28892")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Supplier Part Number" "71-CRCW08057M50FKEA"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "21cd9160-223c-4e83-9d7c-f8477c34bd80")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/bab11e10-fbf3-4e90-bfe6-da2bc01233fc")
		(sheetname "Root")
		(sheetfile "PMT1inchBase.kicad_sch")
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_line
			(start -0.227064 0.735)
			(end 0.227064 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "808c88d2-bd9c-4089-a431-be6813485819")
		)
		(fp_line
			(start -0.227064 -0.735)
			(end 0.227064 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "0659864f-c85b-4293-a86b-14043acf0577")
		)
		(fp_rect
			(start -1.85 -0.95)
			(end 1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(fill no)
			(layer "F.CrtYd")
			(uuid "304a66cd-3f2c-407b-acdf-467d975fdc58")
		)
		(fp_rect
			(start -1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill no)
			(layer "F.Fab")
			(uuid "c90e3a87-4ce1-4414-a2b6-07b34a9f2fd4")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "F.Fab")
			(uuid "27f47f9c-3aed-4891-8a11-e132264eae3c")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1 0 180)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net "Net-(G1-Pin_1)")
			(pintype "passive")
			(uuid "b89695d0-2659-4666-bd14-66c853e4a6ef")
		)
		(pad "2" smd roundrect
			(at 1 0 180)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net "Net-(D1-Pin_1)")
			(pintype "passive")
			(uuid "23a76c91-9d6c-43e2-abd0-6ba3f9a961a0")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Library:H315305"
		(layer "F.Cu")
		(uuid "7c940ce2-5d51-44f2-9d7e-cf87c59ba566")
		(at 133.38 64.5)
		(descr "H3153-05-2")
		(tags "Connector")
		(property "Reference" "D2"
			(at 0 -2.5 0)
			(layer "F.SilkS")
			(uuid "aec1dfd0-ab8c-4e5f-bf00-af9f42e18649")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.254)
				)
			)
		)
		(property "Value" "Conn_01x01_Socket"
			(at -0.5 -3 0)
			(layer "F.SilkS")
			(hide yes)
			(uuid "c49b8f80-3367-4d35-a17f-c084e1379e67")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.254)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "427ffc91-f43f-4c47-8b89-23d6e6bc466e")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "bad06896-74f0-45fa-bc60-6da7855b3ee9")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Manufacturer" "Harwin"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
			(uuid "c0027c39-1fcd-4a5b-9011-4f778c5fd400")
			(effects
				(font
					(size 1 1)
					(thickness 0.1)
				)
			)
		)
		(property "MPN" "H3153-05"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
			(uuid "dbeaf6df-2648-4010-85c5-8cdd2db87981")
			(effects
				(font
					(size 1 1)
					(thickness 0.1)
				)
			)
		)
		(property "Supplier" "Mouser"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
			(uuid "f9d82991-0d7a-4ffb-b2be-31835e2273d1")
			(effects
				(font
					(size 1 1)
					(thickness 0.1)
				)
			)
		)
		(property "Supplier Part Number" "855-H3153-05"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
			(uuid "5efd2df0-6864-43fe-a4cf-f063a464dfdb")
			(effects
				(font
					(size 1 1)
					(thickness 0.1)
				)
			)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(path "/cbe27321-2d27-4eff-a958-0be476564643")
		(sheetname "Root")
		(sheetfile "PMT1inchBase.kicad_sch")
		(attr through_hole)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_line
			(start -1.2 0)
			(end -1.2 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "2e5ebf12-7f75-4181-b321-6dee5590a7ce")
		)
		(fp_line
			(start 1.2 0)
			(end 1.2 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "ac862f70-8a3b-4631-8f81-bc93caea1ddf")
		)
		(fp_arc
			(start -1.2 0)
			(mid 0 -1.2)
			(end 1.2 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "59a42d10-cc32-466c-a028-d5cf98f9e75e")
		)
		(fp_arc
			(start 1.2 0)
			(mid 0 1.2)
			(end -1.2 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "38eb1f00-8d5c-4db2-9200-56daf57b9f08")
		)
		(fp_line
			(start -1.2 -1.2)
			(end 1.2 -1.2)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "d7e450be-b596-41e3-8e7b-a4d473736b48")
		)
		(fp_line
			(start -1.2 1.2)
			(end -1.2 -1.2)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "c6741e13-506f-4ab3-a4a3-39383034e120")
		)
		(fp_line
			(start 1.2 -1.2)
			(end 1.2 1.2)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "431139fb-7285-4b54-a122-dafa7c8c67de")
		)
		(fp_line
			(start 1.2 1.2)
			(end -1.2 1.2)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "b093e797-e7a7-45ed-a703-a911128b8a8a")
		)
		(fp_line
			(start -1.2 0)
			(end -1.2 0)
			(stroke
				(width 0.2)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "bbfbce38-59e2-4c0c-9ae0-b5bfb3d57d79")
		)
		(fp_line
			(start 1.2 0)
			(end 1.2 0)
			(stroke
				(width 0.2)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "bcc6124b-6e05-4691-a45d-096f38d939c4")
		)
		(fp_arc
			(start -1.2 0)
			(mid 0 -1.2)
			(end 1.2 0)
			(stroke
				(width 0.2)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "36ebeb93-2674-43ec-b60a-ba8a13e7190a")
		)
		(fp_arc
			(start 1.2 0)
			(mid 0 1.2)
			(end -1.2 0)
			(stroke
				(width 0.2)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "489b39da-d32e-4bf4-96fb-96a0293ce427")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "2630da92-9453-4b0d-ba5f-c9a71e8258c7")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.254)
				)
			)
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1.65 1.65)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "Net-(D2-Pin_1)")
			(pinfunction "Pin_1")
			(pintype "passive")
			(uuid "e87cd4be-d52b-443e-b529-7746cd54b5a4")
		)
		(embedded_fonts no)
		(model "${KIPRJMOD}/3dmodels/H3153-05.stp"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -0 -90 -0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(uuid "828388bb-d366-4eaa-9191-2390f7ba379f")
		(at 128.5 75.5 -90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "resistor handsolder")
		(property "Reference" "R6"
			(at 0 -1.65 270)
			(layer "F.SilkS")
			(uuid "8fdf1f41-7346-4ff0-8f83-762b41ba1f4e")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "4.99M"
			(at 0 1.65 270)
			(layer "F.Fab")
			(uuid "bb7e77a8-c67d-4797-a880-361a6a9b9cba")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
			(uuid "2133e4f9-9d0a-44e3-af3b-0fe4c6765e02")
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Description" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
			(uuid "215bc9f8-4e1a-49dd-9afd-2ac7e072cc61")
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 270)
			(layer "F.SilkS")
			(hide yes)
			(uuid "8bc6e804-b78b-40d1-81ea-257de00c9983")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Manufacturer" "KOA Speer"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "d172cb11-105d-46c4-aa35-79696c3ca718")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "MPN" "RS73F2ATTD4994D"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "4ed864d7-06e8-4600-97e9-489673c1144d")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Supplier Part Number" "660-RS73F2ATTD4994D "
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "d2134559-5e95-4125-9812-e24feb880502")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/94940bfe-e6a4-4400-a90c-d2d84ad61b55")
		(sheetname "Root")
		(sheetfile "PMT1inchBase.kicad_sch")
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_line
			(start -0.227064 0.735)
			(end 0.227064 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "c11ab13b-a299-49dd-9dc4-fb5f276815bc")
		)
		(fp_line
			(start -0.227064 -0.735)
			(end 0.227064 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "13b60033-95be-4419-b007-bc83bfa682bf")
		)
		(fp_rect
			(start -1.85 -0.95)
			(end 1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(fill no)
			(layer "F.CrtYd")
			(uuid "cee3235f-5ea3-4458-89fe-b7fc908ff30d")
		)
		(fp_rect
			(start -1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill no)
			(layer "F.Fab")
			(uuid "b46dde5f-df6e-45ed-afec-2b4b8cfaf44a")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 270)
			(layer "F.Fab")
			(uuid "57738a80-f19c-474c-ae9d-1ac8b062b29a")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1 0 270)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net "Net-(D4-Pin_1)")
			(pintype "passive")
			(uuid "f99c1339-638a-47ce-9d98-d403e3a3e465")
		)
		(pad "2" smd roundrect
			(at 1 0 270)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net "Net-(D5-Pin_1)")
			(pintype "passive")
			(uuid "4c914595-f661-456d-a941-e3c7227ebd12")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(uuid "8d34a14b-3878-415b-8132-5fb45a67f673")
		(at 140.5 80)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "resistor handsolder")
		(property "Reference" "R11"
			(at 0 -1.65 0)
			(layer "F.SilkS")
			(uuid "537f9616-c32b-4c60-8066-a47c93f45db2")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "4.99M"
			(at 0 1.65 0)
			(layer "F.Fab")
			(uuid "28a3c3be-253a-4008-b05b-fc1463b17ac9")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "6732d88a-449e-4b25-8596-214d3de6bb7e")
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "eb30ba71-4277-4fb3-8091-3e5b0568f9b5")
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
			(uuid "a0e37599-ad36-42dc-a90d-0c868a00b098")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Manufacturer" "KOA Speer"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "db03e3fd-b260-445f-b4c0-d0615c9eb46e")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "MPN" "RS73F2ATTD4994D"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "777d9317-f2d3-41bf-b210-5a75bf392e4c")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Supplier Part Number" "660-RS73F2ATTD4994D"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "ea80772f-8320-4d04-9ca0-34faa0073fc6")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/283f64c8-debd-43dd-b6fc-c33669afce1a")
		(sheetname "Root")
		(sheetfile "PMT1inchBase.kicad_sch")
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_line
			(start -0.227064 -0.735)
			(end 0.227064 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "ff195a92-6e6c-498d-bc37-e74b75a4c5c2")
		)
		(fp_line
			(start -0.227064 0.735)
			(end 0.227064 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "1aaaf39d-bc9e-490f-b544-5a8e1892189e")
		)
		(fp_rect
			(start -1.85 -0.95)
			(end 1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(fill no)
			(layer "F.CrtYd")
			(uuid "f4cbd448-43e7-4060-9cfe-37bb4a523762")
		)
		(fp_rect
			(start -1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill no)
			(layer "F.Fab")
			(uuid "aeacbedc-3305-43ba-8ff3-ad98f6973926")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "c36cc860-1158-490a-9be5-a2c22c19efe8")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net "Net-(D9-Pin_1)")
			(pintype "passive")
			(uuid "8bb609a5-7dca-42d9-90df-6bd4256fb15a")
		)
		(pad "2" smd roundrect
			(at 1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net "Net-(D10-Pin_1)")
			(pintype "passive")
			(uuid "05324b66-863a-41bb-bb13-fc18d9394770")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Library:H315305"
		(layer "F.Cu")
		(uuid "9e476455-ad1f-43ea-b66e-4644062c216e")
		(at 130.84 64.5)
		(descr "H3153-05-2")
		(tags "Connector")
		(property "Reference" "D3"
			(at 0 -2.5 0)
			(layer "F.SilkS")
			(uuid "adeb3f90-6ea1-4ab7-aff9-9e827f2419ca")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.254)
				)
			)
		)
		(property "Value" "Conn_01x01_Socket"
			(at -0.5 -3 0)
			(layer "F.SilkS")
			(hide yes)
			(uuid "dbc12d2d-4047-4c6f-b37f-6a3ede93afbb")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.254)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "3cde9972-65fd-4359-acc4-02fd7eea9f10")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "4e5af675-23b6-49a1-8c09-c291d635176f")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Manufacturer" "Harwin"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
			(uuid "62d24a7f-491a-497f-9ec7-65066bbedc5d")
			(effects
				(font
					(size 1 1)
					(thickness 0.1)
				)
			)
		)
		(property "MPN" "H3153-05"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
			(uuid "c1a68c48-6358-4138-84ed-1e7e51d0733b")
			(effects
				(font
					(size 1 1)
					(thickness 0.1)
				)
			)
		)
		(property "Supplier" "Mouser"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
			(uuid "6a1714aa-f2c1-4574-b7ea-fa4e0df39d1e")
			(effects
				(font
					(size 1 1)
					(thickness 0.1)
				)
			)
		)
		(property "Supplier Part Number" "855-H3153-05"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
			(uuid "659c127a-b3e3-4a42-b407-cb87f223083d")
			(effects
				(font
					(size 1 1)
					(thickness 0.1)
				)
			)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(path "/ea23de88-11dc-41ee-a283-6fceba076af3")
		(sheetname "Root")
		(sheetfile "PMT1inchBase.kicad_sch")
		(attr through_hole)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_line
			(start -1.2 0)
			(end -1.2 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "65fa9a69-3a78-4812-837b-5c1d255c130c")
		)
		(fp_line
			(start 1.2 0)
			(end 1.2 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "7fadac12-ed6f-4e75-a87a-090c4435114f")
		)
		(fp_arc
			(start -1.2 0)
			(mid 0 -1.2)
			(end 1.2 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "12944758-899e-48e0-9a6e-9f3751afc47c")
		)
		(fp_arc
			(start 1.2 0)
			(mid 0 1.2)
			(end -1.2 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "c7546a97-d54d-457d-a09f-66b3fa9dafd8")
		)
		(fp_line
			(start -1.2 -1.2)
			(end 1.2 -1.2)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "cf48694e-41af-4c59-a39a-a42f3b223d18")
		)
		(fp_line
			(start -1.2 1.2)
			(end -1.2 -1.2)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "462e7ccd-55f4-4617-bb1c-e0a27fb66583")
		)
		(fp_line
			(start 1.2 -1.2)
			(end 1.2 1.2)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "40420ec5-921e-4938-908b-9dc6cfd9dce5")
		)
		(fp_line
			(start 1.2 1.2)
			(end -1.2 1.2)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "925ba62e-e872-4076-b366-a2a98f0faf21")
		)
		(fp_line
			(start -1.2 0)
			(end -1.2 0)
			(stroke
				(width 0.2)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "cfdb6bd7-4d2e-44ef-9928-939a3486e801")
		)
		(fp_line
			(start 1.2 0)
			(end 1.2 0)
			(stroke
				(width 0.2)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "0bcdf5d6-3dff-495e-86fb-c4207668d4da")
		)
		(fp_arc
			(start -1.2 0)
			(mid 0 -1.2)
			(end 1.2 0)
			(stroke
				(width 0.2)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "803f4b78-a6e9-47e4-8dc6-d283be0cfaab")
		)
		(fp_arc
			(start 1.2 0)
			(mid 0 1.2)
			(end -1.2 0)
			(stroke
				(width 0.2)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "0be2ff27-533c-42c5-bf4e-7b619ff5d8f5")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "29612662-1c11-481c-b71e-454321cabf3a")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.254)
				)
			)
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1.65 1.65)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "Net-(D3-Pin_1)")
			(pinfunction "Pin_1")
			(pintype "passive")
			(uuid "28b2281e-c3f6-4fad-987f-52838d8d295c")
		)
		(embedded_fonts no)
		(model "${KIPRJMOD}/3dmodels/H3153-05.stp"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -0 -90 -0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(uuid "a1cf54c9-9dd8-481a-a909-30ea6a7c0193")
		(at 128.5 80)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "resistor handsolder")
		(property "Reference" "R7"
			(at 0 -1.65 0)
			(layer "F.SilkS")
			(uuid "cba553b0-305f-4611-93e4-75f51c2e6c8a")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "4.99M"
			(at 0 1.65 0)
			(layer "F.Fab")
			(uuid "69af156c-bebb-478e-b785-780aedcd8e36")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "93002963-3e64-4b22-a46d-7bce7cd1ec1f")
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "07b5cec7-7786-4429-a15b-5d1c2df6a6d1")
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
			(uuid "3ea7dbab-c429-4acb-89f6-df965deb1291")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Manufacturer" "KOA Speer"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "9d8876ac-ff45-427f-b235-caa8bdb431a5")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "MPN" "RS73F2ATTD4994D"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "5694687f-5430-4821-a557-5f0deeb4d61a")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Supplier Part Number" "660-RS73F2ATTD4994D"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "6c85751f-4b92-4575-9a58-c18b8e17e912")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/1c61e928-adf3-4404-927b-1babba86af58")
		(sheetname "Root")
		(sheetfile "PMT1inchBase.kicad_sch")
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_line
			(start -0.227064 -0.735)
			(end 0.227064 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "5c5be177-2ca7-49de-ad1e-4293715901a6")
		)
		(fp_line
			(start -0.227064 0.735)
			(end 0.227064 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "5d7d2b89-d15e-4880-8396-ec8a29b2f2ba")
		)
		(fp_rect
			(start -1.85 -0.95)
			(end 1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(fill no)
			(layer "F.CrtYd")
			(uuid "010cdbbd-1870-4dc8-b8a4-ea664b132e05")
		)
		(fp_rect
			(start -1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill no)
			(layer "F.Fab")
			(uuid "7171b480-163c-48de-a470-daa22043a9e1")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "a83be5f3-e98a-41c9-9931-4ecaa973aa9c")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net "Net-(D5-Pin_1)")
			(pintype "passive")
			(uuid "a37a387c-fdfc-4acb-b5cd-96c62a2ad4ec")
		)
		(pad "2" smd roundrect
			(at 1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net "Net-(D6-Pin_1)")
			(pintype "passive")
			(uuid "49d05d09-0ab6-4753-a2dc-09f0258b1678")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(uuid "a6c02288-7e5f-41da-8749-4258db491562")
		(at 132 82.5)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "resistor handsolder")
		(property "Reference" "R8"
			(at 0 -1.65 0)
			(layer "F.SilkS")
			(uuid "1e4e90b9-0839-4585-915a-8c59bda9214f")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "4.99M"
			(at 0 1.65 0)
			(layer "F.Fab")
			(uuid "ca26b0bf-bfa3-4e6c-8af4-60048ad0fe0d")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "4f8019ad-26ec-4738-ac80-94436399ffb5")
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "838bf302-ec14-4021-be4d-0406704830fd")
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
			(uuid "087d5580-fe56-4efc-99fe-257f4fdc3983")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Manufacturer" "KOA Speer"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "ef045fce-084d-44e0-a0d4-9205684f3a2e")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "MPN" "RS73F2ATTD4994D"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "e7356929-3ed5-446f-a901-378eeb699f93")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Supplier Part Number" "660-RS73F2ATTD4994D"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "118e46bc-0066-4fb3-b1b6-b49669af4799")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/f4e97c31-c648-4916-9d29-dff22ef79eae")
		(sheetname "Root")
		(sheetfile "PMT1inchBase.kicad_sch")
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_line
			(start -0.227064 -0.735)
			(end 0.227064 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "3fb9a98a-7461-4ce8-ab57-bf6a62ab8054")
		)
		(fp_line
			(start -0.227064 0.735)
			(end 0.227064 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "2e532287-6eb3-44ce-9e79-5089fddc09b6")
		)
		(fp_rect
			(start -1.85 -0.95)
			(end 1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(fill no)
			(layer "F.CrtYd")
			(uuid "7cc03b0d-06e3-4882-9e3a-226256a54740")
		)
		(fp_rect
			(start -1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill no)
			(layer "F.Fab")
			(uuid "97d75a07-598e-44d2-be23-9c46a254cb91")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "e9b11817-0da1-4550-8af1-4679fb02997e")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net "Net-(D6-Pin_1)")
			(pintype "passive")
			(uuid "353c0def-a55d-4510-a169-1ed2d5356b19")
		)
		(pad "2" smd roundrect
			(at 1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net "Net-(D7-Pin_1)")
			(pintype "passive")
			(uuid "aef713c6-ba0e-4191-97d0-99e924eac3ea")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Library:H315305"
		(layer "F.Cu")
		(uuid "ab0a4eee-125d-4d8e-a1d7-6f489bc3b6b7")
		(at 128.3 64.5)
		(descr "H3153-05-2")
		(tags "Connector")
		(property "Reference" "D4"
			(at 0 -2.5 0)
			(layer "F.SilkS")
			(uuid "41502667-aca3-41f1-9aca-f94a85bab5e0")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.254)
				)
			)
		)
		(property "Value" "Conn_01x01_Socket"
			(at -0.5 -3 0)
			(layer "F.SilkS")
			(hide yes)
			(uuid "7b41478f-20bd-4e1c-a254-3ae5a28c2bfe")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.254)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "f34506c3-44a5-466c-a923-3482ecd7653c")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "980aeb03-b798-47bb-a05e-5b13052e7aed")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Manufacturer" "Harwin"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
			(uuid "18e18b82-16c5-4a62-a2e2-7524e5430c5f")
			(effects
				(font
					(size 1 1)
					(thickness 0.1)
				)
			)
		)
		(property "MPN" "H3153-05"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
			(uuid "a63f3cd7-0c4f-4601-a331-5ca9ce10bcfe")
			(effects
				(font
					(size 1 1)
					(thickness 0.1)
				)
			)
		)
		(property "Supplier" "Mouser"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
			(uuid "53ff9995-cdde-4399-96c3-01a20468a04d")
			(effects
				(font
					(size 1 1)
					(thickness 0.1)
				)
			)
		)
		(property "Supplier Part Number" "855-H3153-05"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
			(uuid "2453e469-b99b-4b8a-bf8a-c1b8eeb23be8")
			(effects
				(font
					(size 1 1)
					(thickness 0.1)
				)
			)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(path "/6beafa5b-fc46-4af0-b0c4-6553a4c40023")
		(sheetname "Root")
		(sheetfile "PMT1inchBase.kicad_sch")
		(attr through_hole)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_line
			(start -1.2 0)
			(end -1.2 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "4192ff34-915a-4966-bd3a-eed79bf50093")
		)
		(fp_line
			(start 1.2 0)
			(end 1.2 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "59cc4c41-77de-4dc1-b049-f741fccc22f2")
		)
		(fp_arc
			(start -1.2 0)
			(mid 0 -1.2)
			(end 1.2 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "d99af3d1-eff9-4106-bb9d-dce208bea4a8")
		)
		(fp_arc
			(start 1.2 0)
			(mid 0 1.2)
			(end -1.2 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "1a043af8-2785-4f23-870e-e7b0ef657ec0")
		)
		(fp_line
			(start -1.2 -1.2)
			(end 1.2 -1.2)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "062de9aa-f695-4b9a-91fe-387b8d2d3e53")
		)
		(fp_line
			(start -1.2 1.2)
			(end -1.2 -1.2)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "e3e65aa9-7dec-4e55-99a9-3d1b0817e89c")
		)
		(fp_line
			(start 1.2 -1.2)
			(end 1.2 1.2)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "2ed10d1d-8d19-407c-925b-0d6211664e21")
		)
		(fp_line
			(start 1.2 1.2)
			(end -1.2 1.2)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "1b7d4717-09dd-48d2-902a-112a5f1474ed")
		)
		(fp_line
			(start -1.2 0)
			(end -1.2 0)
			(stroke
				(width 0.2)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "efd02f16-d8bc-48bb-a6c8-d0bbf8691f78")
		)
		(fp_line
			(start 1.2 0)
			(end 1.2 0)
			(stroke
				(width 0.2)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "21510ca2-7060-43bf-a5e7-0ff961b9e2cf")
		)
		(fp_arc
			(start -1.2 0)
			(mid 0 -1.2)
			(end 1.2 0)
			(stroke
				(width 0.2)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "73edbe3a-99a3-4b44-a987-26805f97c695")
		)
		(fp_arc
			(start 1.2 0)
			(mid 0 1.2)
			(end -1.2 0)
			(stroke
				(width 0.2)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "5aba54a0-f7ec-4b81-a8c1-b2481916c99f")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "9f2631c4-7b07-4fc9-81dd-b50ba2e7068a")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.254)
				)
			)
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1.65 1.65)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "Net-(D4-Pin_1)")
			(pinfunction "Pin_1")
			(pintype "passive")
			(uuid "bf4c512b-827f-4496-897a-99307f2a287c")
		)
		(embedded_fonts no)
		(model "${KIPRJMOD}/3dmodels/H3153-05.stp"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -0 -90 -0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(uuid "c0913f8b-485d-4539-b9c0-9102d1fc9f99")
		(at 132 67 180)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "resistor handsolder")
		(property "Reference" "R4"
			(at 0 -1.65 180)
			(layer "F.SilkS")
			(uuid "73f1beab-eac2-4592-b985-3f7bce43599d")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "4.99M"
			(at 0 1.65 180)
			(layer "F.Fab")
			(uuid "d5d05864-f2c1-48d0-90a1-748835deb1b8")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
			(uuid "e81638ff-ce56-438f-a314-3eabe5cf9789")
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
			(uuid "b97b8217-5e46-43ed-aa65-171b5e7b7234")
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 180)
			(layer "F.SilkS")
			(hide yes)
			(uuid "fd99304d-94e6-4590-9d59-8d85c2c7073a")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Manufacturer" "KOA Speer"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "ef9cb90c-338e-40dc-8490-805dd16ee3db")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "MPN" "RS73F2ATTD4994D"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "7a6c2229-5818-4f77-bd49-8c4d15b544e2")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Supplier Part Number" "660-RS73F2ATTD4994D"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "7dac7516-8bab-43f7-a08b-799781c25e98")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/ac4d8d84-6c21-4546-a1ce-0000f8d99a54")
		(sheetname "Root")
		(sheetfile "PMT1inchBase.kicad_sch")
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_line
			(start -0.227064 0.735)
			(end 0.227064 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "be2de551-8eb4-4169-a65d-c9c8823da8df")
		)
		(fp_line
			(start -0.227064 -0.735)
			(end 0.227064 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "ce28ea2f-df39-420d-8a41-6b820a035252")
		)
		(fp_rect
			(start -1.85 -0.95)
			(end 1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(fill no)
			(layer "F.CrtYd")
			(uuid "99e9e35e-a5b6-4c9c-bb83-5e226c56c3f4")
		)
		(fp_rect
			(start -1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill no)
			(layer "F.Fab")
			(uuid "671a7e20-2b8d-4033-8d7a-946d6a6601af")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "F.Fab")
			(uuid "3a296877-696d-4590-86af-f54025aec849")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1 0 180)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net "Net-(D2-Pin_1)")
			(pintype "passive")
			(uuid "ffc9a0b2-c8c3-49fe-b6e1-a9b1c2faffd4")
		)
		(pad "2" smd roundrect
			(at 1 0 180)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net "Net-(D3-Pin_1)")
			(pintype "passive")
			(uuid "2860b3a5-4a43-45aa-ab6a-e931ad630f3f")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Library:H315305"
		(layer "F.Cu")
		(uuid "c1041cee-e846-4f68-880f-0012ee5f4d04")
		(at 128.3 84.82)
		(descr "H3153-05-2")
		(tags "Connector")
		(property "Reference" "D5"
			(at 0 -2.5 0)
			(layer "F.SilkS")
			(uuid "be057e55-165b-451e-87e4-ec2f45f36461")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.254)
				)
			)
		)
		(property "Value" "Conn_01x01_Socket"
			(at -0.5 -3 0)
			(layer "F.SilkS")
			(hide yes)
			(uuid "6ba167b2-6c8b-4dbd-88cc-fa9fcdbcbe3f")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.254)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "51b0a1c0-5ce2-440c-89ea-4fee48ed51c8")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "36322964-f555-4f6b-bab9-7956172c757c")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Manufacturer" "Harwin"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
			(uuid "41314877-b009-403d-bf89-8ea14749070b")
			(effects
				(font
					(size 1 1)
					(thickness 0.1)
				)
			)
		)
		(property "MPN" "H3153-05"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
			(uuid "613cecad-db85-40bd-a06f-ea67a4d1860d")
			(effects
				(font
					(size 1 1)
					(thickness 0.1)
				)
			)
		)
		(property "Supplier" "Mouser"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
			(uuid "f08f2827-2c1d-4f1d-8efd-2503f26e6dd9")
			(effects
				(font
					(size 1 1)
					(thickness 0.1)
				)
			)
		)
		(property "Supplier Part Number" "855-H3153-05"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
			(uuid "b07d604d-a5f8-47fc-9f04-7414b32938f1")
			(effects
				(font
					(size 1 1)
					(thickness 0.1)
				)
			)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(path "/d6c90582-ce08-4c8b-aca5-acf368fa0ced")
		(sheetname "Root")
		(sheetfile "PMT1inchBase.kicad_sch")
		(attr through_hole)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_line
			(start -1.2 0)
			(end -1.2 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "3543c09c-5267-41dd-b367-71b45a1b9a9b")
		)
		(fp_line
			(start 1.2 0)
			(end 1.2 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "dc06f7b7-bfe5-4803-b659-6bfcc6808128")
		)
		(fp_arc
			(start -1.2 0)
			(mid 0 -1.2)
			(end 1.2 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "635e82c3-d8e0-41db-b534-273dd0a1d2d4")
		)
		(fp_arc
			(start 1.2 0)
			(mid 0 1.2)
			(end -1.2 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "451dc703-4f45-4d77-9ca7-1426a357204d")
		)
		(fp_line
			(start -1.2 -1.2)
			(end 1.2 -1.2)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "3ca923ac-fe84-4ec5-b472-26172b45eb34")
		)
		(fp_line
			(start -1.2 1.2)
			(end -1.2 -1.2)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "36094a5d-64fe-4a40-9df6-f51b8be63538")
		)
		(fp_line
			(start 1.2 -1.2)
			(end 1.2 1.2)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "9463efa5-326e-4ccd-b273-c153c3a978d7")
		)
		(fp_line
			(start 1.2 1.2)
			(end -1.2 1.2)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "b164a645-081c-4260-87aa-ef9f82685da8")
		)
		(fp_line
			(start -1.2 0)
			(end -1.2 0)
			(stroke
				(width 0.2)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "e7620fc0-01c9-44a7-97ec-8cd06c9ad858")
		)
		(fp_line
			(start 1.2 0)
			(end 1.2 0)
			(stroke
				(width 0.2)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "abd3f929-1710-4103-82fe-3a39bc84c418")
		)
		(fp_arc
			(start -1.2 0)
			(mid 0 -1.2)
			(end 1.2 0)
			(stroke
				(width 0.2)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "0d8966a9-acfc-4f8f-9b3d-18ed5e8ba93b")
		)
		(fp_arc
			(start 1.2 0)
			(mid 0 1.2)
			(end -1.2 0)
			(stroke
				(width 0.2)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "23659d2d-a772-46a8-bb6b-458a9337d87d")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "7dfb4342-98c3-498d-a7cb-1c5b5e95481e")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.254)
				)
			)
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1.65 1.65)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "Net-(D5-Pin_1)")
			(pinfunction "Pin_1")
			(pintype "passive")
			(uuid "7aab1ad7-aec7-4728-88a3-f0b1cbc5b7e5")
		)
		(embedded_fonts no)
		(model "${KIPRJMOD}/3dmodels/H3153-05.stp"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -0 -90 -0)
			)
		)
	)
	(footprint "Library:H318505"
		(layer "F.Cu")
		(uuid "c937d4cb-a0d7-450e-ace9-8c08d067cddc")
		(at 122.5 79.5)
		(descr "H3185-05-2")
		(tags "Connector")
		(property "Reference" "GND1"
			(at 0 0 0)
			(layer "F.SilkS")
			(uuid "4b681e00-1895-40cd-bb21-a16a3ef5ac42")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.254)
				)
			)
		)
		(property "Value" "Conn_01x01_Socket"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
			(uuid "b569bb65-fc88-4d71-b612-29783dcd1c2d")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.254)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "395cb8d5-e527-419e-bb70-e74565fce7ad")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "5c5cd775-3c6f-4a63-8fd8-8fa6707cda34")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(path "/9a5d070a-1016-4239-8a3f-b2658be56196")
		(sheetname "Root")
		(sheetfile "PMT1inchBase.kicad_sch")
		(attr through_hole)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_line
			(start -2 0)
			(end -2 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "bcd553a9-f605-49fa-b770-250fb5cac0f9")
		)
		(fp_line
			(start 2 0)
			(end 2 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "7be2fbaf-8e00-4497-9c69-7c68235f9a45")
		)
		(fp_arc
			(start -2 0)
			(mid 0 -2)
			(end 2 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "6f090fa5-c26d-4978-957f-427f7e52258f")
		)
		(fp_arc
			(start 2 0)
			(mid 0 2)
			(end -2 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "3c3479cf-1e67-409d-a7d0-c748f4305c3f")
		)
		(fp_line
			(start -3 -3)
			(end 3 -3)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "affaaebb-0dfa-40d1-b59b-c901597c4099")
		)
		(fp_line
			(start -3 3)
			(end -3 -3)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "416f2990-418c-4453-b2f7-b1ae46ca4ee1")
		)
		(fp_line
			(start 3 -3)
			(end 3 3)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "669ed705-ce68-4fb2-bc8b-99157f4378f2")
		)
		(fp_line
			(start 3 3)
			(end -3 3)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "42dcb107-9137-4d94-8626-2cd56f4bcd60")
		)
		(fp_line
			(start -2 0)
			(end -2 0)
			(stroke
				(width 0.2)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "f7a9b098-e0c5-4405-a14d-c7dfc3de0d99")
		)
		(fp_line
			(start 2 0)
			(end 2 0)
			(stroke
				(width 0.2)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "5e0c3bb2-4e9a-44cb-b7ba-12be34e80ba9")
		)
		(fp_arc
			(start -2 0)
			(mid 0 -2)
			(end 2 0)
			(stroke
				(width 0.2)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "71176d46-1a75-4faf-bff6-79b1525803fb")
		)
		(fp_arc
			(start 2 0)
			(mid 0 2)
			(end -2 0)
			(stroke
				(width 0.2)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "404d1f5d-ced5-4645-87d3-08e65f0f25e1")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "603af761-cbf8-408d-beb3-83c1bda89917")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.254)
				)
			)
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 3.435 3.435)
			(drill 2.29)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "Net-(GND1-Pin_1)")
			(pinfunction "Pin_1")
			(pintype "passive")
			(uuid "836b06d5-9a73-41f9-958a-ec0a4fddb831")
		)
		(embedded_fonts no)
		(model "H3185-05.stp"
			(offset
				(xyz 0 0 0.8999999626)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 -90 0)
			)
		)
	)
	(footprint "Library:H315305"
		(layer "F.Cu")
		(uuid "d28f7bc5-f286-4798-971f-74ccd261ed86")
		(at 143.54 64.5)
		(descr "H3153-05-2")
		(tags "Connector")
		(property "Reference" "G1"
			(at 0 -2.5 0)
			(layer "F.SilkS")
			(uuid "b2eb87fc-2163-4827-9eb1-81eef10dd0ba")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.254)
				)
			)
		)
		(property "Value" "Conn_01x01_Socket"
			(at -0.5 -3 0)
			(layer "F.SilkS")
			(hide yes)
			(uuid "2bc1ac35-16a7-45b7-9ddb-9d2050c89d90")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.254)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "c360fd9b-e951-4fb5-9f5a-b1a36ebaf271")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "b3c39524-eae6-43a3-8780-73e05290d326")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Manufacturer" "Harwin"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
			(uuid "8d13b453-a717-4b35-afc5-5e9a46655c73")
			(effects
				(font
					(size 1 1)
					(thickness 0.1)
				)
			)
		)
		(property "MPN" "H3153-05"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
			(uuid "7e31d78a-17f4-4a66-bd15-296d00247d62")
			(effects
				(font
					(size 1 1)
					(thickness 0.1)
				)
			)
		)
		(property "Supplier" "Mouser"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
			(uuid "70c69243-5fcb-4702-85e3-8879dc28b9e8")
			(effects
				(font
					(size 1 1)
					(thickness 0.1)
				)
			)
		)
		(property "Supplier Part Number" "855-H3153-05"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
			(uuid "e28c25b8-92b9-43b9-ae67-837b1c602b0e")
			(effects
				(font
					(size 1 1)
					(thickness 0.1)
				)
			)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(path "/533e33c2-bce0-47b2-9077-ec5b307b4908")
		(sheetname "Root")
		(sheetfile "PMT1inchBase.kicad_sch")
		(attr through_hole)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_line
			(start -1.2 0)
			(end -1.2 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "c255f76e-0f29-43f6-92d0-678bb33f3a02")
		)
		(fp_line
			(start 1.2 0)
			(end 1.2 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "f7f6b9ab-3c3c-45bf-a959-bd73359d3b42")
		)
		(fp_arc
			(start -1.2 0)
			(mid 0 -1.2)
			(end 1.2 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "73d9e843-bcac-4855-b36c-abd798b0edc9")
		)
		(fp_arc
			(start 1.2 0)
			(mid 0 1.2)
			(end -1.2 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "3b9866a2-98f2-45e0-8e81-ef6aaba14f9d")
		)
		(fp_line
			(start -1.2 -1.2)
			(end 1.2 -1.2)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "9244871e-cd85-4a0e-9ed7-3988d19adc37")
		)
		(fp_line
			(start -1.2 1.2)
			(end -1.2 -1.2)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "9817e5a9-8e92-4665-a842-15032dcc61d1")
		)
		(fp_line
			(start 1.2 -1.2)
			(end 1.2 1.2)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "c0fab4fb-cb5f-4028-9bdf-d5599cb05ae0")
		)
		(fp_line
			(start 1.2 1.2)
			(end -1.2 1.2)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "216acc67-d1fa-4fa5-9baa-7d745a1572ad")
		)
		(fp_line
			(start -1.2 0)
			(end -1.2 0)
			(stroke
				(width 0.2)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "a120aebc-c8e0-4a24-a23d-110a770fb124")
		)
		(fp_line
			(start 1.2 0)
			(end 1.2 0)
			(stroke
				(width 0.2)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "87199e15-f15d-4dae-bcf8-fccfdd1f4d9d")
		)
		(fp_arc
			(start -1.2 0)
			(mid 0 -1.2)
			(end 1.2 0)
			(stroke
				(width 0.2)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "801a99ef-b0b0-402f-9266-591d26600d38")
		)
		(fp_arc
			(start 1.2 0)
			(mid 0 1.2)
			(end -1.2 0)
			(stroke
				(width 0.2)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "1c8655b9-cdd0-46bb-a241-30a082921db8")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "79d921f0-ba2c-4fdd-b506-3b3148d8363f")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.254)
				)
			)
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1.65 1.65)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "Net-(G1-Pin_1)")
			(pinfunction "Pin_1")
			(pintype "passive")
			(uuid "08a2438f-d227-4dea-97d8-6b733d7e5dbe")
		)
		(embedded_fonts no)
		(model "${KIPRJMOD}/3dmodels/H3153-05.stp"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -0 -90 -0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder"
		(layer "F.Cu")
		(uuid "d7ebb4c3-3ac1-47d6-a3d0-268df589fce7")
		(at 144.6375 85)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "capacitor handsolder")
		(property "Reference" "C4"
			(at 0 -1.43 0)
			(layer "F.SilkS")
			(uuid "dc912d6d-6279-4efd-aeea-3c3d5bdce457")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "10 nF"
			(at 0 1.43 0)
			(layer "F.Fab")
			(uuid "d8d10921-dd43-4ac6-b6f8-12b1ee3ada11")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "27108c1a-75b6-49a3-9993-1762d737707f")
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "ab9b15db-8794-4921-a2e2-1b9dbc873e46")
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
			(uuid "0e0d5cb1-20fb-418f-ade1-0e1043e97fe8")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Manufacturer" "TDK"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "1eda9044-7085-4649-b5af-c1a8c6e5412c")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "MPN" "CGA3E1C0G2A103J080AC"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "0a1a876b-5502-4b61-b4a1-d4cf1f685202")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Supplier Part Number" "810-CGA3E1C0G2A103J080AC"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "cf81e2bd-f495-47ab-a3df-d5833fa00f88")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/8efc1bc8-e413-4364-b8a5-1b8c97688ee1")
		(sheetname "Root")
		(sheetfile "PMT1inchBase.kicad_sch")
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_line
			(start -0.146267 -0.51)
			(end 0.146267 -0.51)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "7985844a-15c6-40cb-bd1e-908a824f8f57")
		)
		(fp_line
			(start -0.146267 0.51)
			(end 0.146267 0.51)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "2e046a7a-5177-490e-a3b0-f4b209ec5057")
		)
		(fp_rect
			(start -1.65 -0.73)
			(end 1.65 0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(fill no)
			(layer "F.CrtYd")
			(uuid "66950c51-654d-4fdf-9b16-1c9f941a7eac")
		)
		(fp_rect
			(start -0.8 -0.4)
			(end 0.8 0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill no)
			(layer "F.Fab")
			(uuid "52821619-7a56-4671-b9c0-b201669c62aa")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "4e1b3897-0ef5-484d-868d-540eaedc2159")
			(effects
				(font
					(size 0.4 0.4)
					(thickness 0.06)
				)
			)
		)
		(pad "1" smd roundrect
			(at -0.8625 0)
			(size 1.075 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "Net-(D10-Pin_1)")
			(pintype "passive")
			(uuid "90fa4180-327e-416b-b0d1-f02197d8f764")
		)
		(pad "2" smd roundrect
			(at 0.8625 0)
			(size 1.075 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "Net-(GND1-Pin_1)")
			(pintype "passive")
			(uuid "72458a57-26dc-4065-90c4-11a981f83ca5")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(uuid "e45a4689-0ad5-4c7d-8b0e-d996c4b9928c")
		(at 129 69 180)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "resistor handsolder")
		(property "Reference" "R5"
			(at 0 -1.65 180)
			(layer "F.SilkS")
			(uuid "f6255db6-ef8b-4c64-bd8e-54cc9fff3b58")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "4.99M"
			(at 0 1.65 180)
			(layer "F.Fab")
			(uuid "074e2647-158e-4d63-bcb7-cfd064311798")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
			(uuid "7879b0f8-5aab-4e11-8a94-167245521026")
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
			(uuid "6f82388e-8056-4be2-958f-0fcfcd4ec353")
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 180)
			(layer "F.SilkS")
			(hide yes)
			(uuid "7224c4bf-12f1-4ee1-bd61-e7c7d91dc0a7")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Manufacturer" "KOA Speer"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "6762d57c-eb3f-4582-83ce-3469d4ed3fdb")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "MPN" "RS73F2ATTD4994D"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "b6b155b9-a224-4b75-bdae-9f87deb8f99c")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Supplier Part Number" "660-RS73F2ATTD4994D"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "bd2e2de8-9253-4a54-a816-91fe0fbb1472")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/aee7630e-c9bb-41e9-a75d-f5f143f07849")
		(sheetname "Root")
		(sheetfile "PMT1inchBase.kicad_sch")
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_line
			(start -0.227064 0.735)
			(end 0.227064 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "bde1baf5-c23d-49c5-84b0-49106b46a3c7")
		)
		(fp_line
			(start -0.227064 -0.735)
			(end 0.227064 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "6efc5e96-a46c-4f2e-92f8-72fdb07b79c6")
		)
		(fp_rect
			(start -1.85 -0.95)
			(end 1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(fill no)
			(layer "F.CrtYd")
			(uuid "a5b4f3d0-21a5-4a2c-bfbf-a59528cd8720")
		)
		(fp_rect
			(start -1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill no)
			(layer "F.Fab")
			(uuid "cf04ef16-0433-4a6c-9e29-f4a3e5f79b29")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "F.Fab")
			(uuid "91bce176-7841-4f29-a3fa-f745ed5fbd65")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1 0 180)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net "Net-(D3-Pin_1)")
			(pintype "passive")
			(uuid "5ff3d3d4-a70c-4ed0-9adb-4c203c6cc8a3")
		)
		(pad "2" smd roundrect
			(at 1 0 180)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net "Net-(D4-Pin_1)")
			(pintype "passive")
			(uuid "c551b9b0-db21-4bb7-bd29-7151015cee7d")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(uuid "e92446fb-0b02-432b-88cc-47f2f11b4276")
		(at 134.5 69 180)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "resistor handsolder")
		(property "Reference" "R3"
			(at 0 -1.65 180)
			(layer "F.SilkS")
			(uuid "f154e81d-965b-47c4-945f-9a86a9a9b07a")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "10M"
			(at 0 1.65 180)
			(layer "F.Fab")
			(uuid "aa269be6-ec6f-4781-af2b-67aa9fe5ad75")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
			(uuid "895b03cd-023d-4a52-81b0-103485ad8ed8")
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
			(uuid "a3c40c2e-6f04-407e-911d-3049df22285c")
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 180)
			(layer "F.SilkS")
			(hide yes)
			(uuid "3aff9743-a685-436b-ae2f-b6d5827ce0f0")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Manufacturer" "KOA Speer"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "7443ca35-d23e-488d-9236-08b3b276c7a0")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "MPN" "HV732ATTD1005F"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "fa5c3065-438c-4fea-912a-26c451a9cb25")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Supplier Part Number" "660-HV732ATTD1005F"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "33b4d010-c33d-4470-995d-55567ef73eea")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/e8496908-8e6d-407b-8b78-70acb2e43fea")
		(sheetname "Root")
		(sheetfile "PMT1inchBase.kicad_sch")
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_line
			(start -0.227064 0.735)
			(end 0.227064 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "0d434041-0d6e-457f-9b3c-5ead3d8f64a0")
		)
		(fp_line
			(start -0.227064 -0.735)
			(end 0.227064 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "f286afd9-196d-4449-8ee0-c08e46b53a85")
		)
		(fp_rect
			(start -1.85 -0.95)
			(end 1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(fill no)
			(layer "F.CrtYd")
			(uuid "f8bbe186-bb0d-4ff2-88c1-32f02fafe6bd")
		)
		(fp_rect
			(start -1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill no)
			(layer "F.Fab")
			(uuid "3622b84e-872e-4d16-8875-56883f058094")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "F.Fab")
			(uuid "3bdd6cf9-852d-4993-83fb-66aa8ea32b15")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1 0 180)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net "Net-(D1-Pin_1)")
			(pintype "passive")
			(uuid "3ae1db4f-f5f2-4fc4-ae9d-c1c71c5b464d")
		)
		(pad "2" smd roundrect
			(at 1 0 180)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net "Net-(D2-Pin_1)")
			(pintype "passive")
			(uuid "d3244e0c-41a4-4c83-a62d-42dab0b8d500")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Library:H315305"
		(layer "F.Cu")
		(uuid "e963fc9d-38c6-4b3e-a06c-396ff4cd066b")
		(at 135.92 84.82)
		(descr "H3153-05-2")
		(tags "Connector")
		(property "Reference" "D8"
			(at 0 -2.5 0)
			(layer "F.SilkS")
			(uuid "25526b95-9cc1-45ef-ad9a-08dcaab2059d")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.254)
				)
			)
		)
		(property "Value" "Conn_01x01_Socket"
			(at -0.5 -3 0)
			(layer "F.SilkS")
			(hide yes)
			(uuid "52b2d452-b1d5-4885-a97f-fa5d8086258e")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.254)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "9147c1f0-1e9c-4df3-80e6-ee2ec3f41a81")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "c041c051-c75c-4086-b01e-7c0bde496385")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Manufacturer" "Harwin"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
			(uuid "f6ea8b4a-57c1-4efb-8c69-ee1fe7fa2774")
			(effects
				(font
					(size 1 1)
					(thickness 0.1)
				)
			)
		)
		(property "MPN" "H3153-05"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
			(uuid "9af8e5f2-5d08-40a7-90d2-3e2041821509")
			(effects
				(font
					(size 1 1)
					(thickness 0.1)
				)
			)
		)
		(property "Supplier" "Mouser"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
			(uuid "4b1b76ee-2ab5-4b70-a396-6baecc0c42bc")
			(effects
				(font
					(size 1 1)
					(thickness 0.1)
				)
			)
		)
		(property "Supplier Part Number" "855-H3153-05"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
			(uuid "982d82c3-e6a2-48c5-afa8-720d6504e6e2")
			(effects
				(font
					(size 1 1)
					(thickness 0.1)
				)
			)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(path "/fab9b507-48ea-48a1-9418-0ab3ffec8c00")
		(sheetname "Root")
		(sheetfile "PMT1inchBase.kicad_sch")
		(attr through_hole)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_line
			(start -1.2 0)
			(end -1.2 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "a1fee91e-ec82-4b97-ab7b-8a83424a9d65")
		)
		(fp_line
			(start 1.2 0)
			(end 1.2 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "0d353335-a9e2-49ae-b29f-f1f6ee4030e9")
		)
		(fp_arc
			(start -1.2 0)
			(mid 0 -1.2)
			(end 1.2 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "01624396-2183-4990-9925-a710e0f0b675")
		)
		(fp_arc
			(start 1.2 0)
			(mid 0 1.2)
			(end -1.2 0)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "66eaf27c-9eb0-45ef-98e2-0d3dacbde7a2")
		)
		(fp_line
			(start -1.2 -1.2)
			(end 1.2 -1.2)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "97a35876-1e87-4a35-9208-43122a32c0c6")
		)
		(fp_line
			(start -1.2 1.2)
			(end -1.2 -1.2)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "33d6fa0c-d9b1-4364-9537-4f5ce42eac2e")
		)
		(fp_line
			(start 1.2 -1.2)
			(end 1.2 1.2)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "d4cc9d5a-26d3-4a75-9a8b-48141abdea85")
		)
		(fp_line
			(start 1.2 1.2)
			(end -1.2 1.2)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "292c8a1b-3f8b-4834-85cd-b0c09514880e")
		)
		(fp_line
			(start -1.2 0)
			(end -1.2 0)
			(stroke
				(width 0.2)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "4c79b053-558a-4e65-a2b6-bb0899f3981c")
		)
		(fp_line
			(start 1.2 0)
			(end 1.2 0)
			(stroke
				(width 0.2)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "32cfd62e-6f8a-41cc-a0ec-c82c675799f4")
		)
		(fp_arc
			(start -1.2 0)
			(mid 0 -1.2)
			(end 1.2 0)
			(stroke
				(width 0.2)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "c72f9607-3b97-483c-994e-d41a13288e2d")
		)
		(fp_arc
			(start 1.2 0)
			(mid 0 1.2)
			(end -1.2 0)
			(stroke
				(width 0.2)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "6991fec9-91c2-473a-998c-c4d9b8ca2aaa")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "03f57c5a-c6c7-41d2-a681-709c4d4a2c30")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.254)
				)
			)
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1.65 1.65)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "Net-(D8-Pin_1)")
			(pinfunction "Pin_1")
			(pintype "passive")
			(uuid "2778b34a-5685-42ed-8e0d-0b6aeb339463")
		)
		(embedded_fonts no)
		(model "${KIPRJMOD}/3dmodels/H3153-05.stp"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -0 -90 -0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(uuid "f4ac0283-aebb-46c0-99ee-02c23db20470")
		(at 137 82.5)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "resistor handsolder")
		(property "Reference" "R10"
			(at 0 -1.65 0)
			(layer "F.SilkS")
			(uuid "cbe706e0-f80b-443f-9375-d1086c9b513f")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "4.99M"
			(at 0 1.65 0)
			(layer "F.Fab")
			(uuid "5d07dbfd-4017-4b0b-b0d3-352ccf71c0a2")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "cd49a006-7164-4ab8-9739-66427de3673f")
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "d03774aa-c013-4b64-a64c-f573d5958205")
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
			(uuid "5e64ebce-3959-4bf9-9f24-a86df704b471")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Manufacturer" "KOA Speer"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "e83a4f3d-0eb4-49e9-8396-2ed8fae8f938")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "MPN" "RS73F2ATTD4994D"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "2686de3b-e312-46df-8950-1301bb34e9ff")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Supplier Part Number" "660-RS73F2ATTD4994D"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "bef8c49f-e028-45f4-8311-aa0e332769c8")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/86e5b172-0c14-4f47-97c3-0221298183f6")
		(sheetname "Root")
		(sheetfile "PMT1inchBase.kicad_sch")
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_line
			(start -0.227064 -0.735)
			(end 0.227064 -0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "57bd40fc-6d48-4403-aa74-da242d407292")
		)
		(fp_line
			(start -0.227064 0.735)
			(end 0.227064 0.735)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "732691a1-5988-47fa-b39c-cb5690f6d3ff")
		)
		(fp_rect
			(start -1.85 -0.95)
			(end 1.85 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(fill no)
			(layer "F.CrtYd")
			(uuid "0c6eb399-bd51-4e45-932c-d0e9c08d807b")
		)
		(fp_rect
			(start -1 -0.625)
			(end 1 0.625)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill no)
			(layer "F.Fab")
			(uuid "5854bd58-74a4-42d9-9f01-e2d753cfaefd")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "0ba94e1b-5262-4326-8374-5922974d2d8c")
			(effects
				(font
					(size 0.5 0.5)
					(thickness 0.08)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net "Net-(D8-Pin_1)")
			(pintype "passive")
			(uuid "05cbe113-8a5e-4e85-aebe-fef169d48d66")
		)
		(pad "2" smd roundrect
			(at 1 0)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net "Net-(D9-Pin_1)")
			(pintype "passive")
			(uuid "9318b744-40da-4240-b8a4-3a7db61d4c72")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(gr_rect
		(start 118.5 57)
		(end 150.5 91.5)
		(stroke
			(width 0.05)
			(type default)
		)
		(fill no)
		(layer "Edge.Cuts")
		(uuid "36f32aa5-28f5-466e-be5f-5bd2b86aa5b8")
	)
	(gr_circle
		(center 133.38 74.66)
		(end 136.38 74.66)
		(stroke
			(width 0.05)
			(type default)
		)
		(fill no)
		(layer "Edge.Cuts")
		(uuid "0f2cfe45-7446-4be6-8032-1815aa446a11")
	)
	(segment
		(start 133 82.5)
		(end 133 84.44)
		(width 0.5)
		(layer "F.Cu")
		(net "Net-(D7-Pin_1)")
		(uuid "4b5e236d-0e70-4461-b634-c44deab656fc")
	)
	(segment
		(start 133 84.44)
		(end 133.38 84.82)
		(width 0.5)
		(layer "F.Cu")
		(net "Net-(D7-Pin_1)")
		(uuid "65c84d24-ebdb-4e96-86c0-90f0a668d0ca")
	)
	(segment
		(start 133.38 80.62)
		(end 133.5 80.5)
		(width 0.5)
		(layer "F.Cu")
		(net "Net-(D7-Pin_1)")
		(uuid "7b54e28a-3173-4d80-a937-21d00a931056")
	)
	(segment
		(start 133.5 80.5)
		(end 133.5 79.2)
		(width 0.5)
		(layer "F.Cu")
		(net "Net-(D7-Pin_1)")
		(uuid "9770d761-cf2c-4b6d-abcf-3b6f18856fa3")
	)
	(segment
		(start 133.5 79.2)
		(end 134 78.7)
		(width 0.5)
		(layer "F.Cu")
		(net "Net-(D7-Pin_1)")
		(uuid "a1ea29b9-2564-4ce6-ab07-916991886df7")
	)
	(segment
		(start 133.38 84.82)
		(end 133.38 80.62)
		(width 0.5)
		(layer "F.Cu")
		(net "Net-(D7-Pin_1)")
		(uuid "cd93e888-3864-448f-9e49-98376e7212e0")
	)
	(segment
		(start 138 82.5)
		(end 138 80.725)
		(width 0.5)
		(layer "F.Cu")
		(net "Net-(D9-Pin_1)")
		(uuid "0fa61e33-03bf-40a9-8d08-4cdff65a1d18")
	)
	(segment
		(start 138 80.725)
		(end 137.5 80.225)
		(width 0.5)
		(layer "F.Cu")
		(net "Net-(D9-Pin_1)")
		(uuid "10614e6b-7eef-43af-8941-18bedbadfc16")
	)
	(segment
		(start 137.5 80.225)
		(end 139.275 80.225)
		(width 0.5)
		(layer "F.Cu")
		(net "Net-(D9-Pin_1)")
		(uuid "3cbbc64e-9538-4a53-b1c3-42339625acd5")
	)
	(segment
		(start 138.775 76.5)
		(end 138.775 79.275)
		(width 0.5)
		(layer "F.Cu")
		(net "Net-(D9-Pin_1)")
		(uuid "6b6d1ddd-abf0-475c-8e56-3ba5298fde2f")
	)
	(segment
		(start 138.46 82.96)
		(end 138 82.5)
		(width 0.5)
		(layer "F.Cu")
		(net "Net-(D9-Pin_1)")
		(uuid "6fefb93a-52e4-463e-82bc-c62a2bda0d53")
	)
	(segment
		(start 138.775 79.275)
		(end 139.5 80)
		(width 0.5)
		(layer "F.Cu")
		(net "Net-(D9-Pin_1)")
		(uuid "8438a4ed-5c3e-4d51-b97a-c96d75766b25")
	)
	(segment
		(start 138.46 84.82)
		(end 138.46 82.96)
		(width 0.5)
		(layer "F.Cu")
		(net "Net-(D9-Pin_1)")
		(uuid "851f1f06-4c79-4cdb-81b7-80d7a5f25bac")
	)
	(segment
		(start 139.275 80.225)
		(end 139.5 80)
		(width 0.5)
		(layer "F.Cu")
		(net "Net-(D9-Pin_1)")
		(uuid "8ff7de8d-81fc-4ce4-b448-e66eb1c63e5f")
	)
	(segment
		(start 141.5 80)
		(end 141.5 80.5)
		(width 0.5)
		(layer "F.Cu")
		(net "Net-(D10-Pin_1)")
		(uuid "3198b311-9dab-4b38-8c3b-a72377a66649")
	)
	(segment
		(start 141.5 76.629124)
		(end 141.5 80)
		(width 0.5)
		(layer "F.Cu")
		(net "Net-(D10-Pin_1)")
		(uuid "377f355e-c2cb-47d9-8b0e-7001a81006c9")
	)
	(segment
		(start 143.775 85)
		(end 141.18 85)
		(width 0.5)
		(layer "F.Cu")
		(net "Net-(D10-Pin_1)")
		(uuid "3b708eea-e302-40e6-83ea-0ecda4b39369")
	)
	(segment
		(start 141.370876 76.5)
		(end 140.5 76.5)
		(width 0.5)
		(layer "F.Cu")
		(net "Net-(D10-Pin_1)")
		(uuid "401eb0b1-5afc-4eab-8da4-7475a5c10fb1")
	)
	(segment
		(start 141.5 76.629124)
		(end 141.370876 76.5)
		(width 0.5)
		(layer "F.Cu")
		(net "Net-(D10-Pin_1)")
		(uuid "45bbbddb-2422-4fdf-8519-9882206cf0f0")
	)
	(segment
		(start 143 84.225)
		(end 143.775 85)
		(width 0.5)
		(layer "F.Cu")
		(net "Net-(D10-Pin_1)")
		(uuid "505af83b-374d-473e-aa7f-05748d8f1f9f")
	)
	(segment
		(start 141.18 85)
		(end 141 84.82)
		(width 0.5)
		(layer "F.Cu")
		(net "Net-(D10-Pin_1)")
		(uuid "55061bb6-db4e-463a-8791-7ba5239b0b08")
	)
	(segment
		(start 141.5 80.5)
		(end 143 82)
		(width 0.5)
		(layer "F.Cu")
		(net "Net-(D10-Pin_1)")
		(uuid "8ee0b57e-160b-40c7-bf78-4fcc1b2f8804")
	)
	(segment
		(start 143 82)
		(end 143 84.225)
		(width 0.5)
		(layer "F.Cu")
		(net "Net-(D10-Pin_1)")
		(uuid "c42a158f-8462-418a-890c-b799b6ed1d45")
	)
	(segment
		(start 145.5 85)
		(end 145.5 82.5)
		(width 0.5)
		(layer "F.Cu")
		(net "Net-(GND1-Pin_1)")
		(uuid "260a61fb-2f01-4ff1-afd0-25ce667041ff")
	)
	(segment
		(start 145.5 82.5)
		(end 145 82)
		(width 0.5)
		(layer "F.Cu")
		(net "Net-(GND1-Pin_1)")
		(uuid "2ae01c4b-02ce-48e2-8f02-b99cd593dc6a")
	)
	(segment
		(start 145 82)
		(end 147 80)
		(width 0.5)
		(layer "F.Cu")
		(net "Net-(GND1-Pin_1)")
		(uuid "4755542b-5141-440c-ae7e-367f03df4e78")
	)
	(segment
		(start 147 88)
		(end 145.25 89.75)
		(width 0.65)
		(layer "F.Cu")
		(net "Net-(GND1-Pin_1)")
		(uuid "4f3ed83c-8385-45ea-be1c-b9c674b643a9")
	)
	(segment
		(start 122.5 87.25)
		(end 122.5 79.5)
		(width 0.65)
		(layer "F.Cu")
		(net "Net-(GND1-Pin_1)")
		(uuid "73d21cfd-f6a4-49be-a3cb-4c9427931bca")
	)
	(segment
		(start 125 89.75)
		(end 122.5 87.25)
		(width 0.65)
		(layer "F.Cu")
		(net "Net-(GND1-Pin_1)")
		(uuid "b297b9f6-0c1a-4c45-8faf-fe98cfe1ff33")
	)
	(segment
		(start 147 80)
		(end 147 88)
		(width 0.65)
		(layer "F.Cu")
		(net "Net-(GND1-Pin_1)")
		(uuid "dc0d4039-4eba-4b55-be52-43c5a114b2e4")
	)
	(segment
		(start 145.25 89.75)
		(end 125 89.75)
		(width 0.65)
		(layer "F.Cu")
		(net "Net-(GND1-Pin_1)")
		(uuid "f6a2c04c-3292-47c1-9298-37787ae8efef")
	)
	(segment
		(start 144.5 75.5)
		(end 147 78)
		(width 0.5)
		(layer "F.Cu")
		(net "Net-(SIG1-Pin_1)")
		(uuid "71a9e539-23d1-44f9-b1db-863028a60efa")
	)
	(segment
		(start 144.5 73)
		(end 144.5 75.5)
		(width 0.5)
		(layer "F.Cu")
		(net "Net-(SIG1-Pin_1)")
		(uuid "eee87d8c-49aa-4caf-b30a-7cb3f4639de9")
	)
	(segment
		(start 125.5 59)
		(end 122.5 62)
		(width 0.5)
		(layer "F.Cu")
		(net "Net-(HV1-Pin_1)")
		(uuid "36a4244b-1c86-4b87-b40a-0729f80cd21c")
	)
	(segment
		(start 122.5 62)
		(end 122.5 70)
		(width 0.5)
		(layer "F.Cu")
		(net "Net-(HV1-Pin_1)")
		(uuid "641fe7db-82b5-4824-bca6-37e4ffd1d78f")
	)
	(segment
		(start 140 62)
		(end 140 59)
		(width 0.5)
		(layer "F.Cu")
		(net "Net-(HV1-Pin_1)")
		(uuid "a3a1d501-76e3-414f-8e8d-bcbc2e0da96a")
	)
	(segment
		(start 138.5 62)
		(end 140 62)
		(width 0.5)
		(layer "F.Cu")
		(net "Net-(HV1-Pin_1)")
		(uuid "b1a3e420-4317-4976-84cf-a02617536b91")
	)
	(segment
		(start 125.5 59)
		(end 140 59)
		(width 0.5)
		(layer "F.Cu")
		(net "Net-(HV1-Pin_1)")
		(uuid "c30b7c4b-0d69-4d64-a5de-89ed9351126e")
	)
	(segment
		(start 138.46 64.5)
		(end 138.46 62.04)
		(width 0.5)
		(layer "F.Cu")
		(net "Net-(HV1-Pin_1)")
		(uuid "e574719c-c459-4fe0-af31-9517c117272e")
	)
	(segment
		(start 138.46 62.04)
		(end 138.5 62)
		(width 0.5)
		(layer "F.Cu")
		(net "Net-(HV1-Pin_1)")
		(uuid "f37db04e-09fa-4960-b775-d5514b673eb2")
	)
	(segment
		(start 135.5 80.5)
		(end 135.5 82)
		(width 0.5)
		(layer "F.Cu")
		(net "Net-(D8-Pin_1)")
		(uuid "127e1ed4-bc3c-4364-abcf-d838f53cdf41")
	)
	(segment
		(start 135.725 78.6)
		(end 135.725 80.275)
		(width 0.5)
		(layer "F.Cu")
		(net "Net-(D8-Pin_1)")
		(uuid "52390c61-1643-459c-b3c1-93f0958848e2")
	)
	(segment
		(start 135.725 80.275)
		(end 135.5 80.5)
		(width 0.5)
		(layer "F.Cu")
		(net "Net-(D8-Pin_1)")
		(uuid "5c50f013-be15-4e25-837d-84431b4201cd")
	)
	(segment
		(start 136 82.5)
		(end 136 84.74)
		(width 0.5)
		(layer "F.Cu")
		(net "Net-(D8-Pin_1)")
		(uuid "8b6e075d-abaf-4d5b-945e-055fa3f50eee")
	)
	(segment
		(start 136 84.74)
		(end 135.92 84.82)
		(width 0.5)
		(layer "F.Cu")
		(net "Net-(D8-Pin_1)")
		(uuid "8da6f22d-dd13-4d16-951b-944cd870ba1f")
	)
	(segment
		(start 135.725 78.5)
		(end 137.5 78.5)
		(width 0.5)
		(layer "F.Cu")
		(net "Net-(D8-Pin_1)")
		(uuid "8dfb85a0-a8af-4888-8e41-4459f5609e5d")
	)
	(segment
		(start 135.5 82)
		(end 136 82.5)
		(width 0.5)
		(layer "F.Cu")
		(net "Net-(D8-Pin_1)")
		(uuid "95a55565-92b0-4641-a6fa-be58e4404497")
	)
	(segment
		(start 142 62)
		(end 142 62.96)
		(width 0.5)
		(layer "F.Cu")
		(net "Net-(G1-Pin_1)")
		(uuid "00be4194-3cce-4fc6-bdde-865befffdd8b")
	)
	(segment
		(start 142 62.96)
		(end 143.54 64.5)
		(width 0.5)
		(layer "F.Cu")
		(net "Net-(G1-Pin_1)")
		(uuid "3163c2a0-1aef-4f20-9350-d4f6bbb40127")
	)
	(segment
		(start 141.04 67)
		(end 138.5 67)
		(width 0.5)
		(layer "F.Cu")
		(net "Net-(G1-Pin_1)")
		(uuid "54dc29c6-01f5-4e55-b5ae-6f89f958b8ea")
	)
	(segment
		(start 143.54 64.5)
		(end 141.04 67)
		(width 0.5)
		(layer "F.Cu")
		(net "Net-(G1-Pin_1)")
		(uuid "e4bf5085-77cd-4e71-a41c-f7b5f918cff6")
	)
	(segment
		(start 130.82 84.82)
		(end 130.82 82.68)
		(width 0.5)
		(layer "F.Cu")
		(net "Net-(D6-Pin_1)")
		(uuid "6d68406d-a55d-45b0-a976-891afd7adf8b")
	)
	(segment
		(start 130.82 82.68)
		(end 131 82.5)
		(width 0.5)
		(layer "F.Cu")
		(net "Net-(D6-Pin_1)")
		(uuid "c020b18a-8f03-4b0a-84fe-62a4eef27408")
	)
	(segment
		(start 129.5 81)
		(end 131 82.5)
		(width 0.5)
		(layer "F.Cu")
		(net "Net-(D6-Pin_1)")
		(uuid "dab7bebb-4d39-4f9b-83e4-fa18a8334f59")
	)
	(segment
		(start 129.5 80)
		(end 129.5 81)
		(width 0.5)
		(layer "F.Cu")
		(net "Net-(D6-Pin_1)")
		(uuid "fdfe4255-bd0a-48ca-b497-96aa1130fd4b")
	)
	(segment
		(start 135.92 66.42)
		(end 136.5 67)
		(width 0.5)
		(layer "F.Cu")
		(net "Net-(D1-Pin_1)")
		(uuid "1c14071f-29e8-470d-a058-75bb8749152c")
	)
	(segment
		(start 136.5 67)
		(end 136.5 68)
		(width 0.5)
		(layer "F.Cu")
		(net "Net-(D1-Pin_1)")
		(uuid "59177473-556c-4a87-b777-dd4bcbc1ba08")
	)
	(segment
		(start 135.92 64.5)
		(end 135.92 66.42)
		(width 0.5)
		(layer "F.Cu")
		(net "Net-(D1-Pin_1)")
		(uuid "b14ddb77-72f4-4519-b38b-630f9c69e1c0")
	)
	(segment
		(start 136.5 68)
		(end 135.5 69)
		(width 0.5)
		(layer "F.Cu")
		(net "Net-(D1-Pin_1)")
		(uuid "eb79eb8e-2c63-4652-b358-5ca89b6ebb33")
	)
	(segment
		(start 133.5 69)
		(end 133.5 67.5)
		(width 0.5)
		(layer "F.Cu")
		(net "Net-(D2-Pin_1)")
		(uuid "3e405c29-4919-4730-95cc-45b99e590a9f")
	)
	(segment
		(start 133 64.88)
		(end 133.38 64.5)
		(width 0.5)
		(layer "F.Cu")
		(net "Net-(D2-Pin_1)")
		(uuid "6dd6060f-c5d0-41ce-a3a6-effd0194151c")
	)
	(segment
		(start 133.5 67.5)
		(end 133 67)
		(width 0.5)
		(layer "F.Cu")
		(net "Net-(D2-Pin_1)")
		(uuid "d8c0528a-daaa-495a-811d-d951e45be115")
	)
	(segment
		(start 133 67)
		(end 133 64.88)
		(width 0.5)
		(layer "F.Cu")
		(net "Net-(D2-Pin_1)")
		(uuid "fd29edf5-e3e1-49a0-b763-2f1dfe885077")
	)
	(segment
		(start 128.5 73.5)
		(end 128.5 74.5)
		(width 0.5)
		(layer "F.Cu")
		(net "Net-(D4-Pin_1)")
		(uuid "0d1ae28a-0561-4188-912e-207d6b7de295")
	)
	(segment
		(start 128.3 64.5)
		(end 128.3 68.7)
		(width 0.5)
		(layer "F.Cu")
		(net "Net-(D4-Pin_1)")
		(uuid "3a9a05c0-3603-4b5e-8b82-23a450fecd0b")
	)
	(segment
		(start 128 69)
		(end 128 73)
		(width 0.5)
		(layer "F.Cu")
		(net "Net-(D4-Pin_1)")
		(uuid "47839216-d0a2-4730-83b4-49ae7cad0bc3")
	)
	(segment
		(start 128.3 68.7)
		(end 128 69)
		(width 0.5)
		(layer "F.Cu")
		(net "Net-(D4-Pin_1)")
		(uuid "ab75dff3-dddd-43dc-a974-b62a8d57fdbc")
	)
	(segment
		(start 128 73)
		(end 128.5 73.5)
		(width 0.5)
		(layer "F.Cu")
		(net "Net-(D4-Pin_1)")
		(uuid "faef3bef-1d83-4fe8-b68a-60db9936a211")
	)
	(segment
		(start 127.5 77.5)
		(end 128.5 76.5)
		(width 0.5)
		(layer "F.Cu")
		(net "Net-(D5-Pin_1)")
		(uuid "131f73d7-b9cc-4341-9874-648d1d4ae76f")
	)
	(segment
		(start 127.5 80)
		(end 127.5 77.5)
		(width 0.5)
		(layer "F.Cu")
		(net "Net-(D5-Pin_1)")
		(uuid "320147ab-6c43-4d0a-8de5-80ef1df86321")
	)
	(segment
		(start 127.5 84.02)
		(end 128.3 84.82)
		(width 0.5)
		(layer "F.Cu")
		(net "Net-(D5-Pin_1)")
		(uuid "3565cb02-eca2-433c-bab4-a3f64a21d68e")
	)
	(segment
		(start 127.5 80)
		(end 127.5 84.02)
		(width 0.5)
		(layer "F.Cu")
		(net "Net-(D5-Pin_1)")
		(uuid "76a4cb03-48b6-427f-83a1-4d17aa8d0cc8")
	)
	(segment
		(start 131 68)
		(end 130 69)
		(width 0.5)
		(layer "F.Cu")
		(net "Net-(D3-Pin_1)")
		(uuid "282e241b-104e-4f9e-abab-1b370723465a")
	)
	(segment
		(start 130.84 66.84)
		(end 131 67)
		(width 0.5)
		(layer "F.Cu")
		(net "Net-(D3-Pin_1)")
		(uuid "3b198e46-fed1-4729-a9dd-8e49a4b5fcc6")
	)
	(segment
		(start 131 67)
		(end 131 68)
		(width 0.5)
		(layer "F.Cu")
		(net "Net-(D3-Pin_1)")
		(uuid "544d0070-35f1-4052-b94f-4965c09a9ade")
	)
	(segment
		(start 130.84 64.5)
		(end 130.84 66.84)
		(width 0.5)
		(layer "F.Cu")
		(net "Net-(D3-Pin_1)")
		(uuid "599eb96e-b308-41b4-857f-dd17cc58d495")
	)
	(embedded_fonts no)
)
