(kicad_pcb
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(general
		(thickness 1.6)
		(legacy_teardrops no)
	)
	(paper "A4")
	(layers
		(0 "F.Cu" signal)
		(2 "B.Cu" signal)
		(9 "F.Adhes" user "F.Adhesive")
		(11 "B.Adhes" user "B.Adhesive")
		(13 "F.Paste" user)
		(15 "B.Paste" user)
		(5 "F.SilkS" user "F.Silkscreen")
		(7 "B.SilkS" user "B.Silkscreen")
		(1 "F.Mask" user)
		(3 "B.Mask" user)
		(17 "Dwgs.User" user "User.Drawings")
		(19 "Cmts.User" user "User.Comments")
		(21 "Eco1.User" user "User.Eco1")
		(23 "Eco2.User" user "User.Eco2")
		(25 "Edge.Cuts" user)
		(27 "Margin" user)
		(31 "F.CrtYd" user "F.Courtyard")
		(29 "B.CrtYd" user "B.Courtyard")
		(35 "F.Fab" user)
		(33 "B.Fab" user)
		(39 "User.1" user)
		(41 "User.2" user)
		(43 "User.3" user)
		(45 "User.4" user)
	)
	(setup
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(tenting front back)
		(pcbplotparams
			(layerselection 0x00000000_00000000_55555555_5755f5ff)
			(plot_on_all_layers_selection 0x00000000_00000000_00000000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 4)
			(plotframeref no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(pdf_metadata yes)
			(pdf_single_document no)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plot_black_and_white yes)
			(sketchpadsonfab no)
			(plotpadnumbers no)
			(hidednponfab no)
			(sketchdnponfab yes)
			(crossoutdnponfab yes)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 0)
			(scaleselection 1)
			(outputdirectory "")
		)
	)
	(net 0 "")
	(net 1 "+5V")
	(net 2 "Net-(Q1-E)")
	(net 3 "Net-(Q2-E)")
	(net 4 "Net-(Q3-E)")
	(net 5 "Net-(Q4-E)")
	(net 6 "Net-(Q5-E)")
	(net 7 "Net-(Q6-E)")
	(net 8 "Net-(Q7-E)")
	(net 9 "Net-(Q8-E)")
	(net 10 "Net-(Q9-E)")
	(net 11 "Net-(Q10-E)")
	(net 12 "GND")
	(net 13 "pin0")
	(net 14 "pin1")
	(net 15 "pin2")
	(net 16 "pin3")
	(net 17 "pin4")
	(net 18 "pin5")
	(net 19 "pin6")
	(net 20 "pin7")
	(net 21 "pin8")
	(net 22 "pin9")
	(net 23 "pin20U1")
	(net 24 "left")
	(net 25 "right")
	(footprint "Laser_Harp_PCB:dumber"
		(layer "F.Cu")
		(at 154.736 117.179)
		(property "Reference" "G***"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "LOGO"
			(at 0.75 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr board_only exclude_from_pos_files exclude_from_bom)
		(embedded_fonts no)
	)
	(footprint "Connector_PinHeader_2.54mm:PinHeader_2x10_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 139.042 45.847)
		(descr "Through hole straight pin header, 2x10, 2.54mm pitch, double rows")
		(tags "Through hole pin header THT 2x10 2.54mm double row")
		(property "Reference" "Laser"
			(at 1.27 -2.38 0)
			(layer "F.SilkS")
		)
		(property "Value" "PinHeader_2x10_P2.54mm_Vertical"
			(at 1.27 25.24 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 1.27 11.43 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "+5V")
		)
		(pad "2" thru_hole circle
			(at 2.54 0)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 12 "GND")
		)
		(pad "3" thru_hole circle
			(at 0 2.54)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "+5V")
		)
		(pad "4" thru_hole circle
			(at 2.54 2.54)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 12 "GND")
		)
		(pad "5" thru_hole circle
			(at 0 5.08)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "+5V")
		)
		(pad "6" thru_hole circle
			(at 2.54 5.08)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 12 "GND")
		)
		(pad "7" thru_hole circle
			(at 0 7.62)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "+5V")
		)
		(pad "8" thru_hole circle
			(at 2.54 7.62)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 12 "GND")
		)
		(pad "9" thru_hole circle
			(at 0 10.16)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "+5V")
		)
		(pad "10" thru_hole circle
			(at 2.54 10.16)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 12 "GND")
		)
		(pad "11" thru_hole circle
			(at 0 12.7)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "+5V")
		)
		(pad "12" thru_hole circle
			(at 2.54 12.7)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 12 "GND")
		)
		(pad "13" thru_hole circle
			(at 0 15.24)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "+5V")
		)
		(pad "14" thru_hole circle
			(at 2.54 15.24)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 12 "GND")
		)
		(pad "15" thru_hole circle
			(at 0 17.78)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "+5V")
		)
		(pad "16" thru_hole circle
			(at 2.54 17.78)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 12 "GND")
		)
		(pad "17" thru_hole circle
			(at 0 20.32)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "+5V")
		)
		(pad "18" thru_hole circle
			(at 2.54 20.32)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 12 "GND")
		)
		(pad "19" thru_hole circle
			(at 0 22.86)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "+5V")
		)
		(pad "20" thru_hole circle
			(at 2.54 22.86)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 12 "GND")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x10_P2.54mm_Vertical.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Laser_Harp_PCB:ts dumb"
		(layer "F.Cu")
		(at 142.29 116.163)
		(property "Reference" "G***"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "LOGO"
			(at 0.75 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr board_only exclude_from_pos_files exclude_from_bom)
		(embedded_fonts no)
	)
	(footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal"
		(layer "F.Cu")
		(at 157.582 74.847 -90)
		(descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
		(property "Reference" "R1"
			(at 4 -2.5 90)
			(layer "F.SilkS")
		)
		(property "Value" "330"
			(at 3.81 2.37 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "Laser_Harp_PCB.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 3.81 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "Net-(Q1-E)")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 7.62 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 12 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_PinHeader_2.54mm:PinHeader_2x01_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 147.857 45.847 180)
		(descr "Through hole straight pin header, 2x01, 2.54mm pitch, double rows")
		(tags "Through hole pin header THT 2x01 2.54mm double row")
		(property "Reference" "GND+5V"
			(at 1.46 2.5 0)
			(layer "F.SilkS")
		)
		(property "Value" "PinHeader_2x01_P2.54mm_Vertical"
			(at 4.04 3 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(pad "1" thru_hole rect
			(at 0 0 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "+5V")
		)
		(pad "2" thru_hole circle
			(at 2.54 0 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 12 "GND")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x01_P2.54mm_Vertical.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_PinHeader_2.54mm:PinHeader_2x10_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 151.582 45.847)
		(descr "Through hole straight pin header, 2x10, 2.54mm pitch, double rows")
		(tags "Through hole pin header THT 2x10 2.54mm double row")
		(property "Reference" "Photo"
			(at 1.27 -2.38 0)
			(layer "F.SilkS")
		)
		(property "Value" "PinHeader_2x10_P2.54mm_Vertical"
			(at 1.27 25.24 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 1.27 11.43 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "+5V")
		)
		(pad "2" thru_hole circle
			(at 2.54 0)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "Net-(Q1-E)")
		)
		(pad "3" thru_hole circle
			(at 0 2.54)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "+5V")
		)
		(pad "4" thru_hole circle
			(at 2.54 2.54)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "Net-(Q2-E)")
		)
		(pad "5" thru_hole circle
			(at 0 5.08)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "+5V")
		)
		(pad "6" thru_hole circle
			(at 2.54 5.08)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "Net-(Q3-E)")
		)
		(pad "7" thru_hole circle
			(at 0 7.62)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "+5V")
		)
		(pad "8" thru_hole circle
			(at 2.54 7.62)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "Net-(Q4-E)")
		)
		(pad "9" thru_hole circle
			(at 0 10.16)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "+5V")
		)
		(pad "10" thru_hole circle
			(at 2.54 10.16)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "Net-(Q5-E)")
		)
		(pad "11" thru_hole circle
			(at 0 12.7)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "+5V")
		)
		(pad "12" thru_hole circle
			(at 2.54 12.7)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 7 "Net-(Q6-E)")
		)
		(pad "13" thru_hole circle
			(at 0 15.24)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "+5V")
		)
		(pad "14" thru_hole circle
			(at 2.54 15.24)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 8 "Net-(Q7-E)")
		)
		(pad "15" thru_hole circle
			(at 0 17.78)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "+5V")
		)
		(pad "16" thru_hole circle
			(at 2.54 17.78)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 9 "Net-(Q8-E)")
		)
		(pad "17" thru_hole circle
			(at 0 20.32)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "+5V")
		)
		(pad "18" thru_hole circle
			(at 2.54 20.32)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 10 "Net-(Q9-E)")
		)
		(pad "19" thru_hole circle
			(at 0 22.86)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "+5V")
		)
		(pad "20" thru_hole circle
			(at 2.54 22.86)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 11 "Net-(Q10-E)")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x10_P2.54mm_Vertical.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal"
		(layer "F.Cu")
		(at 157.582 87.847 -90)
		(descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
		(property "Reference" "R6"
			(at 3.81 -2.37 90)
			(layer "F.SilkS")
		)
		(property "Value" "330"
			(at 3.81 2.37 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "Laser_Harp_PCB.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 3.81 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 7 "Net-(Q6-E)")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 7.62 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 12 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal"
		(layer "F.Cu")
		(at 139.082 74.847 -90)
		(descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
		(property "Reference" "R5"
			(at 3.81 -2.37 90)
			(layer "F.SilkS")
		)
		(property "Value" "330"
			(at 3.81 2.37 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "Laser_Harp_PCB.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 3.81 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "Net-(Q5-E)")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 7.62 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 12 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Module:Adafruit_Feather"
		(layer "F.Cu")
		(at 162.762 49.867)
		(descr "Common footprint for the Adafruit Feather series of boards, https://learn.adafruit.com/adafruit-feather/feather-specification")
		(tags "Adafruit Feather")
		(property "Reference" "U1"
			(at 10.16 -7.62 0)
			(layer "F.SilkS")
		)
		(property "Value" "Adafruit_Feather"
			(at 10.16 45.72 180)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(clearance 0.2)
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 10.16 19.05 270)
			(layer "F.Fab")
		)
		(pad "1" thru_hole roundrect
			(at 0 0)
			(size 2.6 1.6)
			(drill 1
				(offset 0.3 0)
			)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.15625)
		)
		(pad "2" thru_hole oval
			(at 0 2.54)
			(size 2.6 1.6)
			(drill 1
				(offset 0.3 0)
			)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "3" thru_hole oval
			(at 0 5.08)
			(size 2.6 1.6)
			(drill 1
				(offset 0.3 0)
			)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "4" thru_hole oval
			(at 0 7.62)
			(size 2.6 1.6)
			(drill 1
				(offset 0.3 0)
			)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 12 "GND")
		)
		(pad "5" thru_hole oval
			(at 0 10.16)
			(size 2.6 1.6)
			(drill 1
				(offset 0.3 0)
			)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "Net-(Q5-E)")
		)
		(pad "6" thru_hole oval
			(at 0 12.7)
			(size 2.6 1.6)
			(drill 1
				(offset 0.3 0)
			)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "Net-(Q4-E)")
		)
		(pad "7" thru_hole oval
			(at 0 15.24)
			(size 2.6 1.6)
			(drill 1
				(offset 0.3 0)
			)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "Net-(Q3-E)")
		)
		(pad "8" thru_hole oval
			(at 0 17.78)
			(size 2.6 1.6)
			(drill 1
				(offset 0.3 0)
			)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "Net-(Q2-E)")
		)
		(pad "9" thru_hole oval
			(at 0 20.32)
			(size 2.6 1.6)
			(drill 1
				(offset 0.3 0)
			)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "Net-(Q1-E)")
		)
		(pad "10" thru_hole oval
			(at 0 22.86)
			(size 2.6 1.6)
			(drill 1
				(offset 0.3 0)
			)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "11" thru_hole oval
			(at 0 25.4)
			(size 2.6 1.6)
			(drill 1
				(offset 0.3 0)
			)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "12" thru_hole oval
			(at 0 27.94)
			(size 2.6 1.6)
			(drill 1
				(offset 0.3 0)
			)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "13" thru_hole oval
			(at 0 30.48)
			(size 2.6 1.6)
			(drill 1
				(offset 0.3 0)
			)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "14" thru_hole oval
			(at 0 33.02)
			(size 2.6 1.6)
			(drill 1
				(offset 0.3 0)
			)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "15" thru_hole oval
			(at 0 35.56)
			(size 2.6 1.6)
			(drill 1
				(offset 0.3 0)
			)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "16" thru_hole oval
			(at 0 38.1)
			(size 2.6 1.6)
			(drill 1
				(offset 0.3 0)
			)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "17" thru_hole oval
			(at 20.32 38.1 180)
			(size 2.6 1.6)
			(drill 1
				(offset 0.3 0)
			)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "18" thru_hole oval
			(at 20.32 35.56 180)
			(size 2.6 1.6)
			(drill 1
				(offset 0.3 0)
			)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "19" thru_hole oval
			(at 20.32 33.02 180)
			(size 2.6 1.6)
			(drill 1
				(offset 0.3 0)
			)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "20" thru_hole oval
			(at 20.32 30.48 180)
			(size 2.6 1.6)
			(drill 1
				(offset 0.3 0)
			)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 23 "pin20U1")
		)
		(pad "21" thru_hole oval
			(at 20.32 27.94 180)
			(size 2.6 1.6)
			(drill 1
				(offset 0.3 0)
			)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 13 "pin0")
		)
		(pad "22" thru_hole oval
			(at 20.32 25.4 180)
			(size 2.6 1.6)
			(drill 1
				(offset 0.3 0)
			)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 14 "pin1")
		)
		(pad "23" thru_hole oval
			(at 20.32 22.86 180)
			(size 2.6 1.6)
			(drill 1
				(offset 0.3 0)
			)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 15 "pin2")
		)
		(pad "24" thru_hole oval
			(at 20.32 20.32 180)
			(size 2.6 1.6)
			(drill 1
				(offset 0.3 0)
			)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 16 "pin3")
		)
		(pad "25" thru_hole oval
			(at 20.32 17.78 180)
			(size 2.6 1.6)
			(drill 1
				(offset 0.3 0)
			)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 17 "pin4")
		)
		(pad "26" thru_hole oval
			(at 20.32 15.24 180)
			(size 2.6 1.6)
			(drill 1
				(offset 0.3 0)
			)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "27" thru_hole oval
			(at 20.32 12.7 180)
			(size 2.6 1.6)
			(drill 1
				(offset 0.3 0)
			)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "28" thru_hole oval
			(at 20.32 10.16 180)
			(size 2.6 1.6)
			(drill 1
				(offset 0.3 0)
			)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "+5V")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Module.3dshapes/Adafruit_Feather.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal"
		(layer "F.Cu")
		(at 143.582 87.847 -90)
		(descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
		(property "Reference" "R9"
			(at 3.81 -2.37 90)
			(layer "F.SilkS")
		)
		(property "Value" "330"
			(at 3.81 2.37 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "Laser_Harp_PCB.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 3.81 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 10 "Net-(Q9-E)")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 7.62 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 12 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal"
		(layer "F.Cu")
		(at 148.082 74.847 -90)
		(descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
		(property "Reference" "R3"
			(at 3.81 -2.37 90)
			(layer "F.SilkS")
		)
		(property "Value" "330"
			(at 3.81 2.37 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "Laser_Harp_PCB.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 3.81 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "Net-(Q3-E)")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 7.62 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 12 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Module:Adafruit_Feather"
		(layer "F.Cu")
		(at 207.122 98.847 -90)
		(descr "Common footprint for the Adafruit Feather series of boards, https://learn.adafruit.com/adafruit-feather/feather-specification")
		(tags "Adafruit Feather")
		(property "Reference" "U3"
			(at 10.16 -7.62 90)
			(layer "F.SilkS")
		)
		(property "Value" "Adafruit_Feather"
			(at 10.16 45.72 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(clearance 0.2)
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 10.16 21.59 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole roundrect
			(at 0 2.54 270)
			(size 2.6 1.6)
			(drill 1
				(offset 0.3 0)
			)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.15625)
			(net 13 "pin0")
		)
		(pad "2" thru_hole oval
			(at 0 5.08 270)
			(size 2.6 1.6)
			(drill 1
				(offset 0.3 0)
			)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 14 "pin1")
		)
		(pad "3" thru_hole oval
			(at 0 7.62 270)
			(size 2.6 1.6)
			(drill 1
				(offset 0.3 0)
			)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 15 "pin2")
		)
		(pad "4" thru_hole oval
			(at 0 10.16 270)
			(size 2.6 1.6)
			(drill 1
				(offset 0.3 0)
			)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 16 "pin3")
		)
		(pad "5" thru_hole oval
			(at 0 12.7 270)
			(size 2.6 1.6)
			(drill 1
				(offset 0.3 0)
			)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 17 "pin4")
		)
		(pad "6" thru_hole oval
			(at 0 15.24 270)
			(size 2.6 1.6)
			(drill 1
				(offset 0.3 0)
			)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 18 "pin5")
		)
		(pad "7" thru_hole oval
			(at 0 17.78 270)
			(size 2.6 1.6)
			(drill 1
				(offset 0.3 0)
			)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 19 "pin6")
		)
		(pad "8" thru_hole oval
			(at 0 20.32 270)
			(size 2.6 1.6)
			(drill 1
				(offset 0.3 0)
			)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 20 "pin7")
		)
		(pad "9" thru_hole oval
			(at 0 22.86 270)
			(size 2.6 1.6)
			(drill 1
				(offset 0.3 0)
			)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 21 "pin8")
		)
		(pad "10" thru_hole oval
			(at 0 25.4 270)
			(size 2.6 1.6)
			(drill 1
				(offset 0.3 0)
			)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 22 "pin9")
		)
		(pad "11" thru_hole oval
			(at 0 27.94 270)
			(size 2.6 1.6)
			(drill 1
				(offset 0.3 0)
			)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "12" thru_hole oval
			(at 0 30.48 270)
			(size 2.6 1.6)
			(drill 1
				(offset 0.3 0)
			)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "13" thru_hole oval
			(at 0 33.02 270)
			(size 2.6 1.6)
			(drill 1
				(offset 0.3 0)
			)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "15" thru_hole oval
			(at 22.86 33.02 270)
			(size 2.6 1.6)
			(drill 1
				(offset -0.3 0)
			)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "16" thru_hole oval
			(at 22.86 30.48 270)
			(size 2.6 1.6)
			(drill 1
				(offset -0.3 0)
			)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 24 "left")
		)
		(pad "17" thru_hole oval
			(at 22.86 27.94 90)
			(size 2.6 1.6)
			(drill 1
				(offset 0.3 0)
			)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 25 "right")
		)
		(pad "18" thru_hole oval
			(at 22.86 25.4 90)
			(size 2.6 1.6)
			(drill 1
				(offset 0.3 0)
			)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 12 "GND")
		)
		(pad "19" thru_hole oval
			(at 22.86 22.86 90)
			(size 2.6 1.6)
			(drill 1
				(offset 0.3 0)
			)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "20" thru_hole oval
			(at 22.86 20.32 90)
			(size 2.6 1.6)
			(drill 1
				(offset 0.3 0)
			)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "21" thru_hole oval
			(at 22.86 17.78 90)
			(size 2.6 1.6)
			(drill 1
				(offset 0.3 0)
			)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "22" thru_hole oval
			(at 22.86 15.24 90)
			(size 2.6 1.6)
			(drill 1
				(offset 0.3 0)
			)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "23" thru_hole oval
			(at 22.86 12.7 90)
			(size 2.6 1.6)
			(drill 1
				(offset 0.3 0)
			)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "24" thru_hole oval
			(at 22.86 10.16 90)
			(size 2.6 1.6)
			(drill 1
				(offset 0.3 0)
			)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "25" thru_hole oval
			(at 22.86 7.62 90)
			(size 2.6 1.6)
			(drill 1
				(offset 0.3 0)
			)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "26" thru_hole oval
			(at 22.86 5.08 90)
			(size 2.6 1.6)
			(drill 1
				(offset 0.3 0)
			)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "27" thru_hole oval
			(at 22.86 2.54 90)
			(size 2.6 1.6)
			(drill 1
				(offset 0.3 0)
			)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 12 "GND")
		)
		(pad "28" thru_hole oval
			(at 22.86 0 90)
			(size 2.6 1.6)
			(drill 1
				(offset 0.3 0)
			)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "+5V")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Module.3dshapes/Adafruit_Feather.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal"
		(layer "F.Cu")
		(at 148.082 87.847 -90)
		(descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
		(property "Reference" "R8"
			(at 3.81 -2.37 90)
			(layer "F.SilkS")
		)
		(property "Value" "330"
			(at 3.81 2.37 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "Laser_Harp_PCB.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 3.81 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 9 "Net-(Q8-E)")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 7.62 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 12 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Module:Adafruit_Feather"
		(layer "F.Cu")
		(at 190.582 49.847)
		(descr "Common footprint for the Adafruit Feather series of boards, https://learn.adafruit.com/adafruit-feather/feather-specification")
		(tags "Adafruit Feather")
		(property "Reference" "U2"
			(at 10.16 -7.62 0)
			(layer "F.SilkS")
		)
		(property "Value" "Adafruit_Feather"
			(at 10.16 45.72 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(clearance 0.2)
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 10.16 19.05 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole roundrect
			(at 0 0)
			(size 2.6 1.6)
			(drill 1
				(offset 0.3 0)
			)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.15625)
		)
		(pad "2" thru_hole oval
			(at 0 2.54)
			(size 2.6 1.6)
			(drill 1
				(offset 0.3 0)
			)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "3" thru_hole oval
			(at 0 5.08)
			(size 2.6 1.6)
			(drill 1
				(offset 0.3 0)
			)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "4" thru_hole oval
			(at 0 7.62)
			(size 2.6 1.6)
			(drill 1
				(offset 0.3 0)
			)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 12 "GND")
		)
		(pad "5" thru_hole oval
			(at 0 10.16)
			(size 2.6 1.6)
			(drill 1
				(offset 0.3 0)
			)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 11 "Net-(Q10-E)")
		)
		(pad "6" thru_hole oval
			(at 0 12.7)
			(size 2.6 1.6)
			(drill 1
				(offset 0.3 0)
			)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 10 "Net-(Q9-E)")
		)
		(pad "7" thru_hole oval
			(at 0 15.24)
			(size 2.6 1.6)
			(drill 1
				(offset 0.3 0)
			)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 9 "Net-(Q8-E)")
		)
		(pad "8" thru_hole oval
			(at 0 17.78)
			(size 2.6 1.6)
			(drill 1
				(offset 0.3 0)
			)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 8 "Net-(Q7-E)")
		)
		(pad "9" thru_hole oval
			(at 0 20.32)
			(size 2.6 1.6)
			(drill 1
				(offset 0.3 0)
			)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 7 "Net-(Q6-E)")
		)
		(pad "10" thru_hole oval
			(at 0 22.86)
			(size 2.6 1.6)
			(drill 1
				(offset 0.3 0)
			)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "11" thru_hole oval
			(at 0 25.4)
			(size 2.6 1.6)
			(drill 1
				(offset 0.3 0)
			)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "12" thru_hole oval
			(at 0 27.94)
			(size 2.6 1.6)
			(drill 1
				(offset 0.3 0)
			)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "13" thru_hole oval
			(at 0 30.48)
			(size 2.6 1.6)
			(drill 1
				(offset 0.3 0)
			)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "14" thru_hole oval
			(at 0 33.02)
			(size 2.6 1.6)
			(drill 1
				(offset 0.3 0)
			)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "15" thru_hole oval
			(at 0 35.56)
			(size 2.6 1.6)
			(drill 1
				(offset 0.3 0)
			)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "16" thru_hole oval
			(at 0 38.1)
			(size 2.6 1.6)
			(drill 1
				(offset 0.3 0)
			)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "17" thru_hole oval
			(at 20.32 38.1 180)
			(size 2.6 1.6)
			(drill 1
				(offset 0.3 0)
			)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "18" thru_hole oval
			(at 20.32 35.56 180)
			(size 2.6 1.6)
			(drill 1
				(offset 0.3 0)
			)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "19" thru_hole oval
			(at 20.32 33.02 180)
			(size 2.6 1.6)
			(drill 1
				(offset 0.3 0)
			)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "20" thru_hole oval
			(at 20.32 30.48 180)
			(size 2.6 1.6)
			(drill 1
				(offset 0.3 0)
			)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "21" thru_hole oval
			(at 20.32 27.94 180)
			(size 2.6 1.6)
			(drill 1
				(offset 0.3 0)
			)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 18 "pin5")
		)
		(pad "22" thru_hole oval
			(at 20.32 25.4 180)
			(size 2.6 1.6)
			(drill 1
				(offset 0.3 0)
			)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 19 "pin6")
		)
		(pad "23" thru_hole oval
			(at 20.32 22.86 180)
			(size 2.6 1.6)
			(drill 1
				(offset 0.3 0)
			)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 20 "pin7")
		)
		(pad "24" thru_hole oval
			(at 20.32 20.32 180)
			(size 2.6 1.6)
			(drill 1
				(offset 0.3 0)
			)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 21 "pin8")
		)
		(pad "25" thru_hole oval
			(at 20.32 17.78 180)
			(size 2.6 1.6)
			(drill 1
				(offset 0.3 0)
			)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 22 "pin9")
		)
		(pad "26" thru_hole oval
			(at 20.32 15.24 180)
			(size 2.6 1.6)
			(drill 1
				(offset 0.3 0)
			)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "27" thru_hole oval
			(at 20.32 12.7 180)
			(size 2.6 1.6)
			(drill 1
				(offset 0.3 0)
			)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "28" thru_hole oval
			(at 20.32 10.16 180)
			(size 2.6 1.6)
			(drill 1
				(offset 0.3 0)
			)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "+5V")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Module.3dshapes/Adafruit_Feather.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal"
		(layer "F.Cu")
		(at 152.582 74.847 -90)
		(descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
		(property "Reference" "R2"
			(at 3.98 -2.67 90)
			(layer "F.SilkS")
		)
		(property "Value" "330"
			(at 3.81 2.37 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "Laser_Harp_PCB.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 3.81 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "Net-(Q2-E)")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 7.62 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 12 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal"
		(layer "F.Cu")
		(at 152.582 87.847 -90)
		(descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
		(property "Reference" "R7"
			(at 3.81 -2.37 90)
			(layer "F.SilkS")
		)
		(property "Value" "330"
			(at 3.81 2.37 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "Laser_Harp_PCB.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 3.81 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 8 "Net-(Q7-E)")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 7.62 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 12 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal"
		(layer "F.Cu")
		(at 143.582 74.847 -90)
		(descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
		(property "Reference" "R4"
			(at 3.81 -2.37 90)
			(layer "F.SilkS")
		)
		(property "Value" "330"
			(at 3.81 2.37 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "Laser_Harp_PCB.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 3.81 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "Net-(Q4-E)")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 7.62 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 12 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 150.582 101.347)
		(descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x03 2.54mm single row")
		(property "Reference" "Speaker"
			(at 0 -2.38 0)
			(layer "F.SilkS")
		)
		(property "Value" "PinHeader_1x03_P2.54mm_Vertical"
			(at 0 7.46 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 2.54 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 12 "GND")
		)
		(pad "2" thru_hole circle
			(at 0 2.54)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 25 "right")
		)
		(pad "3" thru_hole circle
			(at 0 5.08)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 24 "left")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal"
		(layer "F.Cu")
		(at 139.082 87.847 -90)
		(descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
		(property "Reference" "R10"
			(at 3.81 -2.37 90)
			(layer "F.SilkS")
		)
		(property "Value" "330"
			(at 3.81 2.37 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "Laser_Harp_PCB.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 3.81 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 11 "Net-(Q10-E)")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 7.62 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 12 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 143.082 101.307)
		(descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x03 2.54mm single row")
		(property "Reference" "Relay"
			(at 0 -2.38 0)
			(layer "F.SilkS")
		)
		(property "Value" "PinHeader_1x03_P2.54mm_Vertical"
			(at 0 7.46 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 2.54 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 23 "pin20U1")
		)
		(pad "2" thru_hole circle
			(at 0 2.54)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "+5V")
		)
		(pad "3" thru_hole circle
			(at 0 5.08)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 12 "GND")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(gr_circle
		(center 135.1 125.15)
		(end 136.6 125.15)
		(fill no)
		(layer "Edge.Cuts")
	)
	(gr_circle
		(center 135.1 42.1)
		(end 136.6 42.1)
		(fill no)
		(layer "Edge.Cuts")
	)
	(gr_circle
		(center 215.45 125.15)
		(end 213.95 125.15)
		(fill no)
		(layer "Edge.Cuts")
	)
	(gr_circle
		(center 215.45 42.1)
		(end 213.95 42.1)
		(fill no)
		(layer "Edge.Cuts")
	)
	(gr_rect
		(start 132.5 39.5)
		(end 218.059 127.762)
		(fill no)
		(layer "Edge.Cuts")
	)
	(gr_text "330"
		(at 148.767 79.968 90)
		(layer "F.SilkS")
	)
	(gr_text "330"
		(at 158.292 79.968 90)
		(layer "F.SilkS")
	)
	(gr_text "330"
		(at 139.75 79.968 90)
		(layer "F.SilkS")
	)
	(gr_text "330"
		(at 144.195 93.049 90)
		(layer "F.SilkS")
	)
	(gr_text "330"
		(at 153.212 79.968 90)
		(layer "F.SilkS")
	)
	(gr_text "SOUND BOARD"
		(at 210.87 115.147 90)
		(layer "F.SilkS")
	)
	(gr_text "ADAFRUIT ESP32"
		(at 166.801 46.694 0)
		(layer "F.SilkS")
	)
	(gr_text "330"
		(at 153.212 93.049 90)
		(layer "F.SilkS")
	)
	(gr_text "ADAFRUIT ESP32"
		(at 194.614 46.694 0)
		(layer "F.SilkS")
	)
	(gr_text "330"
		(at 148.767 93.049 90)
		(layer "F.SilkS")
	)
	(gr_text "330"
		(at 144.195 79.968 90)
		(layer "F.SilkS")
	)
	(gr_text "330"
		(at 139.732 93.047 90)
		(layer "F.SilkS")
	)
	(gr_text "330"
		(at 158.292 93.049 90)
		(layer "F.SilkS")
	)
	(embedded_fonts no)
)
