(kicad_pcb
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(general
		(thickness 1.6)
		(legacy_teardrops no)
	)
	(paper "A4")
	(layers
		(0 "F.Cu" signal)
		(2 "B.Cu" signal)
		(9 "F.Adhes" user "F.Adhesive")
		(11 "B.Adhes" user "B.Adhesive")
		(13 "F.Paste" user)
		(15 "B.Paste" user)
		(5 "F.SilkS" user "F.Silkscreen")
		(7 "B.SilkS" user "B.Silkscreen")
		(1 "F.Mask" user)
		(3 "B.Mask" user)
		(17 "Dwgs.User" user "User.Drawings")
		(19 "Cmts.User" user "User.Comments")
		(21 "Eco1.User" user "User.Eco1")
		(23 "Eco2.User" user "User.Eco2")
		(25 "Edge.Cuts" user)
		(27 "Margin" user)
		(31 "F.CrtYd" user "F.Courtyard")
		(29 "B.CrtYd" user "B.Courtyard")
		(35 "F.Fab" user)
		(33 "B.Fab" user)
		(39 "User.1" user)
		(41 "User.2" user)
		(43 "User.3" user)
		(45 "User.4" user)
	)
	(setup
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(tenting front back)
		(pcbplotparams
			(layerselection 0x00000000_00000000_55555555_5755f5ff)
			(plot_on_all_layers_selection 0x00000000_00000000_00000000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 4)
			(plotframeref no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(pdf_metadata yes)
			(pdf_single_document no)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plot_black_and_white yes)
			(sketchpadsonfab no)
			(plotpadnumbers no)
			(hidednponfab no)
			(sketchdnponfab yes)
			(crossoutdnponfab yes)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 1)
			(scaleselection 1)
			(outputdirectory "")
		)
	)
	(net 0 "")
	(net 1 "GND")
	(net 2 "VIN")
	(net 3 "Net-(U1-BST)")
	(net 4 "VOUT")
	(net 5 "Net-(U1-EN)")
	(net 6 "Net-(U1-FB)")
	(net 7 "Net-(U1-PG)")
	(net 8 "Net-(U1-SS)")
	(net 9 "/SW")
	(net 10 "Net-(C6-Pad1)")
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 109 59.775 90)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C4"
			(at 2.05 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "22nf"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "capacitor, small US symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "C0603C223J3RACTU"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "eval-MP2338GTL.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 90)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 8 "Net-(U1-SS)")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at 0.775 0 90)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 111.25 59.775 90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R2"
			(at 2.05 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "49.9k"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, small US symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "AC0603FR-1349K9L"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "eval-MP2338GTL.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 90)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 5 "Net-(U1-EN)")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at 0.825 0 90)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 113.5 59.775 -90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R1"
			(at -2.025 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "180k"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, small US symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" " RC0603FR-10180KL"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "eval-MP2338GTL.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 270)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "VIN")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at 0.825 0 270)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 5 "Net-(U1-EN)")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 106.75 65.1)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R5"
			(at -2.375 0 180)
			(layer "F.SilkS")
		)
		(property "Value" "40.2k"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, small US symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" " RC0603FR-1340K2L"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "eval-MP2338GTL.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 10 "Net-(C6-Pad1)")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at 0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "project:691137710002"
		(layer "F.Cu")
		(at 122.785 79.425)
		(property "Reference" "J2"
			(at -4.185 -4.625 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Screw_Terminal_01x02"
			(at 4.12 5.365 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic screw terminal, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "691137710002"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TerminalBlock*:*")
		(sheetname "/")
		(sheetfile "eval-MP2338GTL.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole circle
			(at -2.5 0)
			(size 1.95 1.95)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" thru_hole circle
			(at 2.5 0)
			(size 1.95 1.95)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "VOUT")
			(pinfunction "Pin_2")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
		(model "${KIPRJMOD}/3dmodels/691137710002.step"
			(offset
				(xyz -5 -4 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 -0 90)
			)
		)
	)
	(footprint "MountingHole:MountingHole_2.7mm_M2.5_DIN965_Pad"
		(layer "F.Cu")
		(at 131.9 53.1)
		(descr "Mounting Hole 2.7mm, M2.5, generated by kicad-footprint-generator mountinghole.py")
		(tags "mountinghole M2.5 DIN965")
		(property "Reference" "H3"
			(at 0 -3.3 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "MountingHole"
			(at 0 3.3 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Mounting Hole without connection"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "MountingHole*")
		(sheetname "/")
		(sheetfile "eval-MP2338GTL.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 4.7 4.7)
			(drill 2.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(zone_connect 2)
		)
		(embedded_fonts no)
	)
	(footprint "MountingHole:MountingHole_2.7mm_M2.5_DIN965_Pad"
		(layer "F.Cu")
		(at 102.6 81.8)
		(descr "Mounting Hole 2.7mm, M2.5, generated by kicad-footprint-generator mountinghole.py")
		(tags "mountinghole M2.5 DIN965")
		(property "Reference" "H2"
			(at 0 -3.3 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "MountingHole"
			(at 0 3.3 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Mounting Hole without connection"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "MountingHole*")
		(sheetname "/")
		(sheetfile "eval-MP2338GTL.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 4.7 4.7)
			(drill 2.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(zone_connect 2)
		)
		(embedded_fonts no)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "F.Cu")
		(at 111.775 70.475)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C2"
			(at 1.625 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "10uf"
			(at 0 1.68 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "capacitor, small US symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "GRM21BR61H106KE43L"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "eval-MP2338GTL.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "VIN")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at 0.95 0)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 106.75 62.85 180)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R4"
			(at 2.4 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "10k"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, small US symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "RC0603FR-0710KL "
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "eval-MP2338GTL.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 180)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 6 "Net-(U1-FB)")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at 0.825 0 180)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 10 "Net-(C6-Pad1)")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "F.Cu")
		(at 111.775 67.725)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C3"
			(at 1.625 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "0.1uf"
			(at 0 1.68 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "capacitor, small US symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "CC0805MRX7R9BB104"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "eval-MP2338GTL.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "VIN")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at 0.95 0)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 106.75 59.775 90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R6"
			(at 2.025 0 180)
			(layer "F.SilkS")
		)
		(property "Value" "360k"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, small US symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "RC0603FR-07360KL "
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "eval-MP2338GTL.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 90)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 10 "Net-(C6-Pad1)")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at 0.825 0 90)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 4 "VOUT")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "F.Cu")
		(at 122.75 72 180)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C7"
			(at -1.65 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "22uf"
			(at 0 1.68 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "capacitor, small US symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "C2012X7S1A226MT000E"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "eval-MP2338GTL.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0 180)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 4 "VOUT")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at 0.95 0 180)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "F.Cu")
		(at 114.725 64.225 -90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C5"
			(at -2.1 0 180)
			(layer "F.SilkS")
		)
		(property "Value" "0.1uf"
			(at 0 1.68 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "capacitor, small US symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "CC0805MRX7R9BB104"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "eval-MP2338GTL.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0 270)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 3 "Net-(U1-BST)")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at 0.95 0 270)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 9 "/SW")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "F.Cu")
		(at 111.775 73.225)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C1"
			(at 1.625 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "10uf"
			(at 0 1.68 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "capacitor, small US symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "GRM21BR61H106KE43L"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "eval-MP2338GTL.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "VIN")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at 0.95 0)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 106.75 67.35 180)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R3"
			(at 2.375 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "100k"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, small US symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "RC0603FR-07100KL "
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "eval-MP2338GTL.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 180)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 7 "Net-(U1-PG)")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at 0.825 0 180)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 4 "VOUT")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 104.5 59.775 90)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C6"
			(at 2.025 0 180)
			(layer "F.SilkS")
		)
		(property "Value" "470pf"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "capacitor, small US symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "885012206081"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "eval-MP2338GTL.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 90)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 10 "Net-(C6-Pad1)")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at 0.775 0 90)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 4 "VOUT")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "project:WE-HCI_7050"
		(layer "F.Cu")
		(at 121.225 65.175)
		(property "Reference" "L1"
			(at 0.05 -4.7564 0)
			(layer "F.SilkS")
		)
		(property "Value" "6.5uH"
			(at 2.1604 4.3536 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Inductor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "744314650"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Choke_* *Coil* Inductor_* L_*")
		(sheetname "/")
		(sheetfile "eval-MP2338GTL.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -2.55 0)
			(size 2.7 2.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 9 "/SW")
			(pinfunction "1")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd rect
			(at 2.55 0)
			(size 2.7 2.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 4 "VOUT")
			(pinfunction "2")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
		(model "${KIPRJMOD}/3dmodels/WE-HCI_7050.step"
			(offset
				(xyz 0 0 1.5)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -0 -0 -90)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "F.Cu")
		(at 122.75 74.25 180)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C8"
			(at -1.65 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "22uf"
			(at 0 1.68 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "capacitor, small US symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "C2012X7S1A226MT000E"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "eval-MP2338GTL.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0 180)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 4 "VOUT")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at 0.95 0 180)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MountingHole:MountingHole_2.7mm_M2.5_DIN965_Pad"
		(layer "F.Cu")
		(at 131.9 81.8)
		(descr "Mounting Hole 2.7mm, M2.5, generated by kicad-footprint-generator mountinghole.py")
		(tags "mountinghole M2.5 DIN965")
		(property "Reference" "H4"
			(at 0 -3.3 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "MountingHole"
			(at 0 3.3 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Mounting Hole without connection"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "MountingHole*")
		(sheetname "/")
		(sheetfile "eval-MP2338GTL.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 4.7 4.7)
			(drill 2.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(zone_connect 2)
		)
		(embedded_fonts no)
	)
	(footprint "Package_TO_SOT_SMD:SOT-583-8"
		(layer "F.Cu")
		(at 111.435 65.075 90)
		(descr "https://www.ti.com/lit/ds/symlink/tps62933.pdf")
		(tags "SOT-583-8")
		(property "Reference" "U1"
			(at 2.075 -0.035 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "MP2338GTL-P"
			(at 0 2.8 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" " MP2338GTL-P"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "eval-MP2338GTL.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.74 -0.75 90)
			(size 0.67 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.1666666667)
			(net 7 "Net-(U1-PG)")
			(pinfunction "PG")
			(pintype "output")
			(thermal_bridge_angle 45)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at -0.74 -0.25 90)
			(size 0.67 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.1666666667)
			(net 2 "VIN")
			(pinfunction "VIN")
			(pintype "power_in")
			(thermal_bridge_angle 45)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "3" smd roundrect
			(at -0.74 0.25 90)
			(size 0.67 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.1666666667)
			(net 9 "/SW")
			(pinfunction "SW")
			(pintype "power_out")
			(thermal_bridge_angle 45)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "4" smd roundrect
			(at -0.74 0.75 90)
			(size 0.67 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.1666666667)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(thermal_bridge_angle 45)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "5" smd roundrect
			(at 0.74 0.75 90)
			(size 0.67 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.1666666667)
			(net 3 "Net-(U1-BST)")
			(pinfunction "BST")
			(pintype "input")
			(thermal_bridge_angle 45)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "6" smd roundrect
			(at 0.74 0.25 90)
			(size 0.67 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.1666666667)
			(net 5 "Net-(U1-EN)")
			(pinfunction "EN")
			(pintype "input")
			(thermal_bridge_angle 45)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "7" smd roundrect
			(at 0.74 -0.25 90)
			(size 0.67 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.1666666667)
			(net 8 "Net-(U1-SS)")
			(pinfunction "SS")
			(pintype "input")
			(thermal_bridge_angle 45)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "8" smd roundrect
			(at 0.74 -0.75 90)
			(size 0.67 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.1666666667)
			(net 6 "Net-(U1-FB)")
			(pinfunction "FB")
			(pintype "input")
			(thermal_bridge_angle 45)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-583-8.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "project:691137710002"
		(layer "F.Cu")
		(at 111.785 79.425)
		(property "Reference" "J1"
			(at -4.185 -4.625 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Screw_Terminal_01x02"
			(at 4.12 5.365 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic screw terminal, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "691137710002"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TerminalBlock*:*")
		(sheetname "/")
		(sheetfile "eval-MP2338GTL.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole circle
			(at -2.5 0)
			(size 1.95 1.95)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "VIN")
			(pinfunction "Pin_1")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" thru_hole circle
			(at 2.5 0)
			(size 1.95 1.95)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_2")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
		(model "${KIPRJMOD}/3dmodels/691137710002.step"
			(offset
				(xyz -5 -4 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 -0 90)
			)
		)
	)
	(footprint "MountingHole:MountingHole_2.7mm_M2.5_DIN965_Pad"
		(layer "F.Cu")
		(at 102.6 53.1)
		(descr "Mounting Hole 2.7mm, M2.5, generated by kicad-footprint-generator mountinghole.py")
		(tags "mountinghole M2.5 DIN965")
		(property "Reference" "H1"
			(at 0 -3.3 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "MountingHole"
			(at 0 3.3 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Mounting Hole without connection"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "MountingHole*")
		(sheetname "/")
		(sheetfile "eval-MP2338GTL.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 4.7 4.7)
			(drill 2.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(zone_connect 2)
		)
		(embedded_fonts no)
	)
	(gr_rect
		(start 99.5 50)
		(end 135 85)
		(fill no)
		(layer "Edge.Cuts")
	)
	(gr_text "+"
		(at 103.5 76 0)
		(layer "F.SilkS" knockout)
	)
	(gr_text "VIN"
		(at 103.5 73.75 0)
		(layer "F.SilkS")
	)
	(gr_text "+"
		(at 131 76 0)
		(layer "F.SilkS" knockout)
	)
	(gr_text "GND"
		(at 117.3 75.6 0)
		(layer "F.SilkS" knockout)
	)
	(gr_text "sndsgd/eval-MP2338GTL\nrev1"
		(at 117.2 54.25 0)
		(layer "F.SilkS")
	)
	(gr_text "VOUT"
		(at 131 73.71 0)
		(layer "F.SilkS")
	)
	(zone
		(net 3)
		(net_name "Net-(U1-BST)")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30022)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 112.266317 63.925104) (xy 112.124896 63.783683) (xy 112.041512 64.026816) (xy 112.184293 64.335707)
				(xy 112.331194 64.030866)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layer "F.Cu")
		(hatch edge 0.5)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(keepout
			(tracks allowed)
			(vias allowed)
			(pads allowed)
			(copperpour not_allowed)
			(footprints allowed)
		)
		(placement
			(enabled no)
			(sheetname "/")
		)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.75)
		)
		(polygon
			(pts
				(xy 112.35 69.75) (xy 112 69.75) (xy 112 71.2) (xy 112.35 71.2)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layer "F.Cu")
		(hatch edge 0.5)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(keepout
			(tracks allowed)
			(vias allowed)
			(pads allowed)
			(copperpour not_allowed)
			(footprints allowed)
		)
		(placement
			(enabled no)
			(sheetname "/")
		)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.75)
		)
		(polygon
			(pts
				(xy 110.325 70.125) (xy 110.125 70.125) (xy 110.125 70.875) (xy 110.325 70.875)
			)
		)
	)
	(zone
		(net 2)
		(net_name "VIN")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 1)
		(connect_pads thru_hole_only
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0)
			(thermal_bridge_width 0.75)
		)
		(polygon
			(pts
				(xy 111.035 65.48) (xy 111.035 66.175) (xy 108.375 68.925) (xy 108.375 81.475) (xy 111.525 81.475)
				(xy 111.525 66.625) (xy 111.335056 66.275103) (xy 111.334879 65.48)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layer "F.Cu")
		(hatch edge 0.5)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(keepout
			(tracks allowed)
			(vias allowed)
			(pads allowed)
			(copperpour not_allowed)
			(footprints allowed)
		)
		(placement
			(enabled no)
			(sheetname "/")
		)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.75)
		)
		(polygon
			(pts
				(xy 121.3 73.875) (xy 121.1 73.875) (xy 121.1 74.625) (xy 121.3 74.625)
			)
		)
	)
	(zone
		(net 9)
		(net_name "/SW")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 6)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 111.535 66.15) (xy 111.535 65.175) (xy 111.595 65.025) (xy 111.730001 64.912499) (xy 111.875 64.875)
				(xy 112.7 64.875) (xy 113 64.575) (xy 113.3 64.475) (xy 115.425 64.475) (xy 117.125 63.6) (xy 120.455974 63.6)
				(xy 120.48363 66.725) (xy 115.495231 66.725) (xy 113.951645 66.19375) (xy 112.775 65.275) (xy 112.075 65.275)
				(xy 111.825 65.525) (xy 111.835 66.15)
			)
		)
	)
	(zone
		(net 3)
		(net_name "Net-(U1-BST)")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30000)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 113.5 63.175) (xy 113.5 63.375) (xy 114.154329 63.75597) (xy 114.726 63.275) (xy 114.154329 62.79403)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layer "F.Cu")
		(hatch edge 0.5)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(keepout
			(tracks allowed)
			(vias allowed)
			(pads allowed)
			(copperpour not_allowed)
			(footprints allowed)
		)
		(placement
			(enabled no)
			(sheetname "/")
		)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.75)
		)
		(polygon
			(pts
				(xy 118.325 66.275) (xy 118.325 66.475) (xy 119.075 66.475) (xy 119.075 66.275)
			)
		)
	)
	(zone
		(net 5)
		(net_name "Net-(U1-EN)")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30018)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 113.181802 61.226776) (xy 113.323224 61.368198) (xy 113.783377 60.998333) (xy 113.500707 60.599293)
				(xy 113.040224 60.876537)
			)
		)
	)
	(zone
		(net 1)
		(net_name "GND")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 2)
		(connect_pads thru_hole_only
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.75)
		)
		(polygon
			(pts
				(xy 112.035 65.48) (xy 112.035 66.075) (xy 112.025 66.282143) (xy 112.025 81.425) (xy 122.282034 81.425)
				(xy 122.3 69.9) (xy 117.7 69.9) (xy 112.185 65.48)
			)
		)
	)
	(zone
		(net 8)
		(net_name "Net-(U1-SS)")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30020)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 111.285 63.85) (xy 111.085 63.85) (xy 111.038806 64.030866) (xy 111.185 64.336) (xy 111.331194 64.030866)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layer "F.Cu")
		(hatch edge 0.5)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(keepout
			(tracks allowed)
			(vias allowed)
			(pads allowed)
			(copperpour not_allowed)
			(footprints allowed)
		)
		(placement
			(enabled no)
			(sheetname "/")
		)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.75)
		)
		(polygon
			(pts
				(xy 112.35 72.5) (xy 112 72.5) (xy 112 73.95) (xy 112.35 73.95)
			)
		)
	)
	(zone
		(net 5)
		(net_name "Net-(U1-EN)")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30009)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 112.125 60.7) (xy 112.125 60.5) (xy 111.601537 60.215224) (xy 111.249 60.6) (xy 111.601537 60.984776)
			)
		)
	)
	(zone
		(net 2)
		(net_name "VIN")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30017)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 113.6 58.15) (xy 113.4 58.15) (xy 113.1 58.597606) (xy 113.5 58.951) (xy 113.9 58.597606)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layer "F.Cu")
		(hatch edge 0.5)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(keepout
			(tracks allowed)
			(vias allowed)
			(pads allowed)
			(copperpour not_allowed)
			(footprints allowed)
		)
		(placement
			(enabled no)
			(sheetname "/")
		)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.75)
		)
		(polygon
			(pts
				(xy 113.425 72.875) (xy 113.225 72.875) (xy 113.225 73.625) (xy 113.425 73.625)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layer "F.Cu")
		(hatch edge 0.5)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(keepout
			(tracks allowed)
			(vias allowed)
			(pads allowed)
			(copperpour not_allowed)
			(footprints allowed)
		)
		(placement
			(enabled no)
			(sheetname "/")
		)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.75)
		)
		(polygon
			(pts
				(xy 124.4 73.875) (xy 124.2 73.875) (xy 124.2 74.625) (xy 124.4 74.625)
			)
		)
	)
	(zone
		(net 4)
		(net_name "VOUT")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30003)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 105.425 59.05) (xy 105.425 58.85) (xy 104.836104 58.567127) (xy 104.499 59) (xy 104.836787 59.432416)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layer "F.Cu")
		(hatch edge 0.5)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(keepout
			(tracks allowed)
			(vias allowed)
			(pads allowed)
			(copperpour not_allowed)
			(footprints allowed)
		)
		(placement
			(enabled no)
			(sheetname "/")
		)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.75)
		)
		(polygon
			(pts
				(xy 113.425 70.125) (xy 113.225 70.125) (xy 113.225 70.875) (xy 113.425 70.875)
			)
		)
	)
	(zone
		(net 10)
		(net_name "Net-(C6-Pad1)")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30012)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 105.825 63.725) (xy 106.025 63.725) (xy 106.309776 63.201537) (xy 105.925 62.849) (xy 105.540224 63.201537)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layer "F.Cu")
		(hatch edge 0.5)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(keepout
			(tracks allowed)
			(vias allowed)
			(pads allowed)
			(copperpour not_allowed)
			(footprints allowed)
		)
		(placement
			(enabled no)
			(sheetname "/")
		)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.75)
		)
		(polygon
			(pts
				(xy 120.025 65.525) (xy 120.225 65.525) (xy 120.225 64.775) (xy 120.025 64.775)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layer "F.Cu")
		(hatch edge 0.5)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(keepout
			(tracks allowed)
			(vias allowed)
			(pads allowed)
			(copperpour not_allowed)
			(footprints allowed)
		)
		(placement
			(enabled no)
			(sheetname "/")
		)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.75)
		)
		(polygon
			(pts
				(xy 112.86 79.25) (xy 112.86 79.6) (xy 116.085 79.6) (xy 116.085 79.25)
			)
		)
	)
	(zone
		(net 10)
		(net_name "Net-(C6-Pad1)")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30014)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 106.65 61.4) (xy 106.85 61.4) (xy 107.15 60.952393) (xy 106.75 60.599) (xy 106.35 60.952393)
			)
		)
	)
	(zone
		(net 10)
		(net_name "Net-(C6-Pad1)")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30005)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 106.453553 62.162868) (xy 106.312132 62.021447) (xy 105.744456 62.375) (xy 105.924293 62.850707)
				(xy 106.325 62.961043)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layer "F.Cu")
		(hatch edge 0.5)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(keepout
			(tracks allowed)
			(vias allowed)
			(pads allowed)
			(copperpour not_allowed)
			(footprints allowed)
		)
		(placement
			(enabled no)
			(sheetname "/")
		)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.75)
		)
		(polygon
			(pts
				(xy 121.3 71.625) (xy 121.1 71.625) (xy 121.1 72.375) (xy 121.3 72.375)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layer "F.Cu")
		(hatch edge 0.5)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(keepout
			(tracks allowed)
			(vias allowed)
			(pads allowed)
			(copperpour not_allowed)
			(footprints allowed)
		)
		(placement
			(enabled no)
			(sheetname "/")
		)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.75)
		)
		(polygon
			(pts
				(xy 113.425 67.375) (xy 113.225 67.375) (xy 113.225 68.125) (xy 113.425 68.125)
			)
		)
	)
	(zone
		(net 4)
		(net_name "VOUT")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30016)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 106.85 58.15) (xy 106.65 58.15) (xy 106.35 58.597606) (xy 106.75 58.951) (xy 107.15 58.597606)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layer "F.Cu")
		(hatch edge 0.5)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(keepout
			(tracks allowed)
			(vias allowed)
			(pads allowed)
			(copperpour not_allowed)
			(footprints allowed)
		)
		(placement
			(enabled no)
			(sheetname "/")
		)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.75)
		)
		(polygon
			(pts
				(xy 111.55 67) (xy 111.2 67) (xy 111.2 68.45) (xy 111.55 68.45)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layer "F.Cu")
		(hatch edge 0.5)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(keepout
			(tracks allowed)
			(vias allowed)
			(pads allowed)
			(copperpour not_allowed)
			(footprints allowed)
		)
		(placement
			(enabled no)
			(sheetname "/")
		)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.75)
		)
		(polygon
			(pts
				(xy 112.35 67) (xy 112 67) (xy 112 68.45) (xy 112.35 68.45)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layer "F.Cu")
		(hatch edge 0.5)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(keepout
			(tracks allowed)
			(vias allowed)
			(pads allowed)
			(copperpour not_allowed)
			(footprints allowed)
		)
		(placement
			(enabled no)
			(sheetname "/")
		)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.75)
		)
		(polygon
			(pts
				(xy 110.325 72.85) (xy 110.125 72.85) (xy 110.125 73.6) (xy 110.325 73.6)
			)
		)
	)
	(zone
		(net 7)
		(net_name "Net-(U1-PG)")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30015)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 108.375 67.45) (xy 108.375 67.25) (xy 107.927393 66.95) (xy 107.574 67.35) (xy 107.927393 67.75)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layer "F.Cu")
		(hatch edge 0.5)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(keepout
			(tracks allowed)
			(vias allowed)
			(pads allowed)
			(copperpour not_allowed)
			(footprints allowed)
		)
		(placement
			(enabled no)
			(sheetname "/")
		)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.75)
		)
		(polygon
			(pts
				(xy 123.425 63.875) (xy 123.425 64.075) (xy 124.175 64.075) (xy 124.175 63.875)
			)
		)
	)
	(zone
		(net 5)
		(net_name "Net-(U1-EN)")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30008)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 112.625 60.5) (xy 112.625 60.7) (xy 113.148463 60.984776) (xy 113.501 60.6) (xy 113.148463 60.215224)
			)
		)
	)
	(zone
		(net 10)
		(net_name "Net-(C6-Pad1)")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30011)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 106.025 64.225) (xy 105.825 64.225) (xy 105.540224 64.748463) (xy 105.925 65.101) (xy 106.309776 64.748463)
			)
		)
	)
	(zone
		(net 4)
		(net_name "VOUT")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30007)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 105.875 58.85) (xy 105.875 59.05) (xy 106.398463 59.334776) (xy 106.751 58.95) (xy 106.398463 58.565224)
			)
		)
	)
	(zone
		(net 5)
		(net_name "Net-(U1-EN)")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30021)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 111.785 63.85) (xy 111.585 63.85) (xy 111.538806 64.030866) (xy 111.685 64.336) (xy 111.831194 64.030866)
			)
		)
	)
	(zone
		(net 8)
		(net_name "Net-(U1-SS)")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30001)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 109.560044 61.376465) (xy 109.701465 61.235044) (xy 109.475 60.416953) (xy 108.999293 60.549293)
				(xy 108.789344 61)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layer "F.Cu")
		(hatch edge 0.5)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(keepout
			(tracks allowed)
			(vias allowed)
			(pads allowed)
			(copperpour not_allowed)
			(footprints allowed)
		)
		(placement
			(enabled no)
			(sheetname "/")
		)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.75)
		)
		(polygon
			(pts
				(xy 122.225 65.525) (xy 122.425 65.525) (xy 122.425 64.775) (xy 122.225 64.775)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layer "F.Cu")
		(hatch edge 0.5)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(keepout
			(tracks allowed)
			(vias allowed)
			(pads allowed)
			(copperpour not_allowed)
			(footprints allowed)
		)
		(placement
			(enabled no)
			(sheetname "/")
		)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.75)
		)
		(polygon
			(pts
				(xy 125.325 64.775) (xy 125.125 64.775) (xy 125.125 65.525) (xy 125.325 65.525)
			)
		)
	)
	(zone
		(net 4)
		(net_name "VOUT")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30004)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 105.341406 66.624985) (xy 105.199985 66.766406) (xy 105.525 67.515685) (xy 105.925707 67.350707)
				(xy 106.015685 66.875)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layer "F.Cu")
		(hatch edge 0.5)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(keepout
			(tracks allowed)
			(vias allowed)
			(pads allowed)
			(copperpour not_allowed)
			(footprints allowed)
		)
		(placement
			(enabled no)
			(sheetname "/")
		)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.75)
		)
		(polygon
			(pts
				(xy 111.2 71.2) (xy 111.55 71.2) (xy 111.55 69.75) (xy 111.2 69.75)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layer "F.Cu")
		(hatch edge 0.5)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(keepout
			(tracks allowed)
			(vias allowed)
			(pads allowed)
			(copperpour not_allowed)
			(footprints allowed)
		)
		(placement
			(enabled no)
			(sheetname "/")
		)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.75)
		)
		(polygon
			(pts
				(xy 124.175 66.475) (xy 124.175 66.275) (xy 123.425 66.275) (xy 123.425 66.475)
			)
		)
	)
	(zone
		(net 10)
		(net_name "Net-(C6-Pad1)")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30002)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 105.425 60.7) (xy 105.425 60.5) (xy 104.836787 60.117583) (xy 104.499 60.55) (xy 104.836104 60.982873)
			)
		)
	)
	(zone
		(net 4)
		(net_name "VOUT")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30006)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 103.555546 59.053033) (xy 103.696967 59.194454) (xy 104.163896 59.432873) (xy 104.500707 58.999293)
				(xy 104.090901 58.615901)
			)
		)
	)
	(zone
		(net 6)
		(net_name "Net-(U1-FB)")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30013)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 108.375 62.95) (xy 108.375 62.75) (xy 107.927393 62.45) (xy 107.574 62.85) (xy 107.927393 63.25)
			)
		)
	)
	(zone
		(net 1)
		(net_name "GND")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 6)
		(connect_pads
			(clearance 0.25)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 110.835 65.455) (xy 110.685 65.79) (xy 107.825 68.65) (xy 107.825 85.45) (xy 98.975 85.45) (xy 98.975 49.704899)
				(xy 138.701416 49.573051) (xy 138.765695 85.35) (xy 128.25 85.35) (xy 128.25 62.75) (xy 115.75 62.775)
				(xy 111.4 64.7)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layer "F.Cu")
		(hatch edge 0.5)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(keepout
			(tracks allowed)
			(vias allowed)
			(pads allowed)
			(copperpour not_allowed)
			(footprints allowed)
		)
		(placement
			(enabled no)
			(sheetname "/")
		)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.75)
		)
		(polygon
			(pts
				(xy 114.635 77.825) (xy 113.96 77.825) (xy 113.96 81.05) (xy 114.635 81.05)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layer "F.Cu")
		(hatch edge 0.5)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(keepout
			(tracks allowed)
			(vias allowed)
			(pads allowed)
			(copperpour not_allowed)
			(footprints allowed)
		)
		(placement
			(enabled no)
			(sheetname "/")
		)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.75)
		)
		(polygon
			(pts
				(xy 110.325 67.375) (xy 110.125 67.375) (xy 110.125 68.125) (xy 110.325 68.125)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layer "F.Cu")
		(hatch edge 0.5)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(keepout
			(tracks allowed)
			(vias allowed)
			(pads allowed)
			(copperpour not_allowed)
			(footprints allowed)
		)
		(placement
			(enabled no)
			(sheetname "/")
		)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.75)
		)
		(polygon
			(pts
				(xy 111.55 72.5) (xy 111.2 72.5) (xy 111.2 73.95) (xy 111.55 73.95)
			)
		)
	)
	(zone
		(net 10)
		(net_name "Net-(C6-Pad1)")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30010)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 105.875 60.5) (xy 105.875 60.7) (xy 106.398463 60.984776) (xy 106.751 60.6) (xy 106.398463 60.215224)
			)
		)
	)
	(zone
		(net 4)
		(net_name "VOUT")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 4)
		(connect_pads thru_hole_only
			(clearance 0)
		)
		(min_thickness 0.1)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.75)
		)
		(polygon
			(pts
				(xy 123.2 68) (xy 121.9 66.7) (xy 121.9 63.525) (xy 126.4 63.525) (xy 126.4 74.633333) (xy 127.4 75.9)
				(xy 127.39853 81.425) (xy 123.2 81.425)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layer "F.Cu")
		(hatch edge 0.5)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(keepout
			(tracks allowed)
			(vias allowed)
			(pads allowed)
			(copperpour not_allowed)
			(footprints allowed)
		)
		(placement
			(enabled no)
			(sheetname "/")
		)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.75)
		)
		(polygon
			(pts
				(xy 124.4 71.625) (xy 124.2 71.625) (xy 124.2 72.375) (xy 124.4 72.375)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layer "F.Cu")
		(hatch edge 0.5)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(keepout
			(tracks allowed)
			(vias allowed)
			(pads allowed)
			(copperpour not_allowed)
			(footprints allowed)
		)
		(placement
			(enabled no)
			(sheetname "/")
		)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.75)
		)
		(polygon
			(pts
				(xy 119.075 64.075) (xy 119.075 63.875) (xy 118.325 63.875) (xy 118.325 64.075)
			)
		)
	)
	(zone
		(net 6)
		(net_name "Net-(U1-FB)")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30019)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 110.523282 63.831861) (xy 110.381861 63.973282) (xy 110.535 64.372197) (xy 110.685707 64.335707)
				(xy 110.67536 64)
			)
		)
	)
	(zone
		(net 7)
		(net_name "Net-(U1-PG)")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30023)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 110.358224 66.000355) (xy 110.499645 66.141776) (xy 110.565926 66.146206) (xy 110.685707 65.814293)
				(xy 110.535 65.752868)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layer "F.Cu")
		(hatch edge 0.5)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(keepout
			(tracks allowed)
			(vias allowed)
			(pads allowed)
			(copperpour not_allowed)
			(footprints allowed)
		)
		(placement
			(enabled no)
			(sheetname "/")
		)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.75)
		)
		(polygon
			(pts
				(xy 117.125 65.525) (xy 117.325 65.525) (xy 117.325 64.775) (xy 117.125 64.775)
			)
		)
	)
	(zone
		(net 1)
		(net_name "GND")
		(layer "B.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 97 46.8) (xy 143 46.8) (xy 143 93) (xy 97 93)
			)
		)
	)
	(embedded_fonts no)
)
