(kicad_pcb
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(general
		(thickness 1.6)
		(legacy_teardrops no)
	)
	(paper "A5")
	(layers
		(0 "F.Cu" signal)
		(2 "B.Cu" signal)
		(9 "F.Adhes" user "F.Adhesive")
		(11 "B.Adhes" user "B.Adhesive")
		(13 "F.Paste" user)
		(15 "B.Paste" user)
		(5 "F.SilkS" user "F.Silkscreen")
		(7 "B.SilkS" user "B.Silkscreen")
		(1 "F.Mask" user)
		(3 "B.Mask" user)
		(17 "Dwgs.User" user "User.Drawings")
		(19 "Cmts.User" user "User.Comments")
		(21 "Eco1.User" user "User.Eco1")
		(23 "Eco2.User" user "User.Eco2")
		(25 "Edge.Cuts" user)
		(27 "Margin" user)
		(31 "F.CrtYd" user "F.Courtyard")
		(29 "B.CrtYd" user "B.Courtyard")
		(35 "F.Fab" user)
		(33 "B.Fab" user)
	)
	(setup
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(tenting front back)
		(aux_axis_origin 111.798 70.702)
		(grid_origin 231.648 144.78)
		(pcbplotparams
			(layerselection 0x00000000_00000000_55555555_575555ff)
			(plot_on_all_layers_selection 0x00000000_00000000_00000000_00000000)
			(disableapertmacros no)
			(usegerberextensions yes)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 4)
			(plotframeref no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(pdf_metadata yes)
			(pdf_single_document no)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plot_black_and_white yes)
			(sketchpadsonfab no)
			(plotpadnumbers no)
			(hidednponfab no)
			(sketchdnponfab yes)
			(crossoutdnponfab yes)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 0)
			(scaleselection 1)
			(outputdirectory "D:/Retro/Apple II/Elektronikk/Kempston-adapter/Gerber")
		)
	)
	(net 0 "")
	(net 1 "+5V")
	(net 2 "Net-(C1-Pad2)")
	(net 3 "Net-(C2-Pad2)")
	(net 4 "UP")
	(net 5 "DOWN")
	(net 6 "LEFT")
	(net 7 "RIGHT")
	(net 8 "PADDLE_B")
	(net 9 "TRIGGER")
	(net 10 "GND")
	(net 11 "PADDLE_A")
	(net 12 "BUT_1")
	(net 13 "GAME2")
	(net 14 "GAME0")
	(net 15 "BUT_2")
	(net 16 "BUT_0")
	(net 17 "GAME1")
	(net 18 "GAME3")
	(net 19 "Net-(Q1-C)")
	(net 20 "Net-(Q1-B)")
	(net 21 "Net-(Q2-C)")
	(net 22 "Net-(Q2-B)")
	(net 23 "Net-(Q3-C)")
	(net 24 "Net-(Q3-B)")
	(net 25 "Net-(Q4-C)")
	(net 26 "Net-(Q4-B)")
	(net 27 "Net-(Q5-B)")
	(net 28 "Net-(Q6-B)")
	(footprint "Capacitor_THT:C_Disc_D3.0mm_W1.6mm_P2.50mm"
		(layer "F.Cu")
		(at 88.557 47.873)
		(descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=3.0*1.6mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
		(tags "C Disc series Radial pin pitch 2.50mm  diameter 3.0mm width 1.6mm Capacitor")
		(property "Reference" "C1"
			(at 1.25 -2.05 0)
			(layer "F.SilkS")
		)
		(property "Value" "C_Small"
			(at 1.25 2.05 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "AppleJoy.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 1.25 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "+5V")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 2.5 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "Net-(C1-Pad2)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D3.0mm_W1.6mm_P2.50mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal"
		(layer "F.Cu")
		(at 100.749 58.287 -90)
		(descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.167W length 3.6mm diameter 1.6mm")
		(property "Reference" "R12"
			(at 3.803 -0.04 270)
			(layer "F.SilkS")
		)
		(property "Value" "560"
			(at 3.81 1.92 270)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "AppleJoy.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 3.81 0 270)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 270)
			(size 1.4 1.4)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 10 "GND")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 7.62 0 270)
			(size 1.4 1.4)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 16 "BUT_0")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal"
		(layer "F.Cu")
		(at 95.542 54.985 180)
		(descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.167W length 3.6mm diameter 1.6mm")
		(property "Reference" "R2"
			(at 3.762 -0.056 180)
			(layer "F.SilkS")
		)
		(property "Value" "1k"
			(at 3.81 1.92 180)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "AppleJoy.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 3.81 0 180)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 180)
			(size 1.4 1.4)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 17 "GAME1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 7.62 0 180)
			(size 1.4 1.4)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 19 "Net-(Q1-C)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal"
		(layer "F.Cu")
		(at 91.097 50.921)
		(descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.167W length 3.6mm diameter 1.6mm")
		(property "Reference" "R1"
			(at 3.821 0.029 0)
			(layer "F.SilkS")
		)
		(property "Value" "1k"
			(at 3.81 1.92 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "AppleJoy.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 3.81 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1.4 1.4)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "Net-(C1-Pad2)")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 7.62 0)
			(size 1.4 1.4)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 17 "GAME1")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_THT:TO-92_Inline_Wide"
		(layer "F.Cu")
		(at 96.938 65.78 90)
		(descr "TO-92 leads in-line, wide, drill 0.75mm (see NXP sot054_po.pdf)")
		(tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
		(property "Reference" "Q2"
			(at 2.54 1.85 90)
			(layer "F.SilkS")
		)
		(property "Value" "BC558"
			(at 2.54 2.79 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "-0.2A Ic, -40V Vce, Small Signal PNP Transistor, TO-92"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "AppleJoy.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 2.54 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 90)
			(size 1.5 1.5)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 17 "GAME1")
			(pinfunction "E")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 2.54 0 90)
			(size 1.5 1.5)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 22 "Net-(Q2-B)")
			(pinfunction "B")
			(pintype "input")
		)
		(pad "3" thru_hole circle
			(at 5.08 0 90)
			(size 1.5 1.5)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 21 "Net-(Q2-C)")
			(pinfunction "C")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_THT.3dshapes/TO-92_Inline_Wide.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_THT:CP_Radial_D5.0mm_P2.00mm"
		(layer "F.Cu")
		(at 100.72 54.512)
		(descr "CP, Radial series, Radial, pin pitch=2.00mm, , diameter=5mm, Electrolytic Capacitor")
		(tags "CP Radial series Radial pin pitch 2.00mm  diameter 5mm Electrolytic Capacitor")
		(property "Reference" "C3"
			(at 4.688 -1.232 0)
			(layer "F.SilkS")
		)
		(property "Value" "1uF"
			(at 1 3.75 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Polarized capacitor, small US symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "AppleJoy.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 1 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "+5V")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 2 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 10 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/CP_Radial_D5.0mm_P2.00mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal"
		(layer "F.Cu")
		(at 105.448 50.54)
		(descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.167W length 3.6mm diameter 1.6mm")
		(property "Reference" "R9"
			(at 3.8 -0.03 0)
			(layer "F.SilkS")
		)
		(property "Value" "1k"
			(at 3.81 1.92 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "AppleJoy.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 3.81 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1.4 1.4)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "Net-(C2-Pad2)")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 7.62 0)
			(size 1.4 1.4)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 14 "GAME0")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal"
		(layer "F.Cu")
		(at 105.267 57.271)
		(descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.167W length 3.6mm diameter 1.6mm")
		(property "Reference" "R5"
			(at 3.797 0.058 0)
			(layer "F.SilkS")
		)
		(property "Value" "10k"
			(at 3.81 1.92 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "AppleJoy.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 3.81 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1.4 1.4)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 10 "GND")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 7.62 0)
			(size 1.4 1.4)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 23 "Net-(Q3-C)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal"
		(layer "F.Cu")
		(at 111.925 60.573 -90)
		(descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.167W length 3.6mm diameter 1.6mm")
		(property "Reference" "R10"
			(at 3.787 -0.093 270)
			(layer "F.SilkS")
		)
		(property "Value" "1k"
			(at 3.81 1.92 270)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "AppleJoy.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 3.81 0 270)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 270)
			(size 1.4 1.4)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 26 "Net-(Q4-B)")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 7.62 0 270)
			(size 1.4 1.4)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "LEFT")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal"
		(layer "F.Cu")
		(at 87.795 75.909 90)
		(descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.167W length 3.6mm diameter 1.6mm")
		(property "Reference" "R11"
			(at 3.81 -0.097 90)
			(layer "F.SilkS")
		)
		(property "Value" "1k"
			(at 3.81 1.92 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "AppleJoy.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 3.81 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 90)
			(size 1.4 1.4)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 27 "Net-(Q5-B)")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 7.62 0 90)
			(size 1.4 1.4)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 9 "TRIGGER")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal"
		(layer "F.Cu")
		(at 107.861 55.112)
		(descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.167W length 3.6mm diameter 1.6mm")
		(property "Reference" "R7"
			(at 3.797 0.058 0)
			(layer "F.SilkS")
		)
		(property "Value" "1k"
			(at 3.81 1.92 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "AppleJoy.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 3.81 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1.4 1.4)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 14 "GAME0")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 7.62 0)
			(size 1.4 1.4)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 25 "Net-(Q4-C)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal"
		(layer "F.Cu")
		(at 93.891 60.573 -90)
		(descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.167W length 3.6mm diameter 1.6mm")
		(property "Reference" "R6"
			(at 3.807 -0.007 270)
			(layer "F.SilkS")
		)
		(property "Value" "1k"
			(at 3.81 1.92 270)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "AppleJoy.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 3.81 0 270)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 270)
			(size 1.4 1.4)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 22 "Net-(Q2-B)")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 7.62 0 270)
			(size 1.4 1.4)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "DOWN")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_THT:TO-92_Inline_Wide"
		(layer "F.Cu")
		(at 111.798 75.78 90)
		(descr "TO-92 leads in-line, wide, drill 0.75mm (see NXP sot054_po.pdf)")
		(tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
		(property "Reference" "Q6"
			(at 2.54 1.85 90)
			(layer "F.SilkS")
		)
		(property "Value" "BC558"
			(at 2.54 2.79 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "-0.2A Ic, -40V Vce, Small Signal PNP Transistor, TO-92"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "AppleJoy.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 2.54 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 90)
			(size 1.5 1.5)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "+5V")
			(pinfunction "E")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 2.54 0 90)
			(size 1.5 1.5)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 28 "Net-(Q6-B)")
			(pinfunction "B")
			(pintype "input")
		)
		(pad "3" thru_hole circle
			(at 5.08 0 90)
			(size 1.5 1.5)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 12 "BUT_1")
			(pinfunction "C")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_THT.3dshapes/TO-92_Inline_Wide.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal"
		(layer "F.Cu")
		(at 102.908 58.287 -90)
		(descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.167W length 3.6mm diameter 1.6mm")
		(property "Reference" "R13"
			(at 3.803 -0.04 270)
			(layer "F.SilkS")
		)
		(property "Value" "560"
			(at 3.81 1.92 270)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "AppleJoy.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 3.81 0 270)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 270)
			(size 1.4 1.4)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 10 "GND")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 7.62 0 270)
			(size 1.4 1.4)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 12 "BUT_1")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_THT:C_Disc_D3.0mm_W1.6mm_P2.50mm"
		(layer "F.Cu")
		(at 114.933 48 180)
		(descr "C, Disc series, Radial, pin pitch=2.50mm, , diameter*width=3.0*1.6mm^2, Capacitor, http://www.vishay.com/docs/45233/krseries.pdf")
		(tags "C Disc series Radial pin pitch 2.50mm  diameter 3.0mm width 1.6mm Capacitor")
		(property "Reference" "C2"
			(at 1.25 -2.05 180)
			(layer "F.SilkS")
		)
		(property "Value" "C_Small"
			(at 1.25 2.05 180)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "AppleJoy.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 1.25 0 180)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "+5V")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 2.5 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "Net-(C2-Pad2)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D3.0mm_W1.6mm_P2.50mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal"
		(layer "F.Cu")
		(at 109.766 60.573 -90)
		(descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.167W length 3.6mm diameter 1.6mm")
		(property "Reference" "R8"
			(at 3.817 -0.102 270)
			(layer "F.SilkS")
		)
		(property "Value" "1k"
			(at 3.81 1.92 270)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "AppleJoy.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 3.81 0 270)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 270)
			(size 1.4 1.4)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 24 "Net-(Q3-B)")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 7.62 0 270)
			(size 1.4 1.4)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 7 "RIGHT")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal"
		(layer "F.Cu")
		(at 91.732 60.573 -90)
		(descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.167W length 3.6mm diameter 1.6mm")
		(property "Reference" "R3"
			(at 3.807 -0.007 270)
			(layer "F.SilkS")
		)
		(property "Value" "1k"
			(at 3.81 1.92 270)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "AppleJoy.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 3.81 0 270)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 270)
			(size 1.4 1.4)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 20 "Net-(Q1-B)")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 7.62 0 270)
			(size 1.4 1.4)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "UP")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal"
		(layer "F.Cu")
		(at 115.608 75.909 90)
		(descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.167W length 3.6mm diameter 1.6mm")
		(property "Reference" "R14"
			(at 3.799 0.09 90)
			(layer "F.SilkS")
		)
		(property "Value" "1k"
			(at 3.81 1.92 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "AppleJoy.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 3.81 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 90)
			(size 1.4 1.4)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 28 "Net-(Q6-B)")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 7.62 0 90)
			(size 1.4 1.4)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 11 "PADDLE_A")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_THT:TO-92_Inline_Wide"
		(layer "F.Cu")
		(at 114.973 65.78 90)
		(descr "TO-92 leads in-line, wide, drill 0.75mm (see NXP sot054_po.pdf)")
		(tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
		(property "Reference" "Q4"
			(at 2.54 1.85 90)
			(layer "F.SilkS")
		)
		(property "Value" "BC558"
			(at 2.54 2.79 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "-0.2A Ic, -40V Vce, Small Signal PNP Transistor, TO-92"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "AppleJoy.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 2.54 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 90)
			(size 1.5 1.5)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "+5V")
			(pinfunction "E")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 2.54 0 90)
			(size 1.5 1.5)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 26 "Net-(Q4-B)")
			(pinfunction "B")
			(pintype "input")
		)
		(pad "3" thru_hole circle
			(at 5.08 0 90)
			(size 1.5 1.5)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 25 "Net-(Q4-C)")
			(pinfunction "C")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_THT.3dshapes/TO-92_Inline_Wide.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_THT:TO-92_Inline_Wide"
		(layer "F.Cu")
		(at 87.918 65.79 90)
		(descr "TO-92 leads in-line, wide, drill 0.75mm (see NXP sot054_po.pdf)")
		(tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
		(property "Reference" "Q1"
			(at 2.54 1.85 90)
			(layer "F.SilkS")
		)
		(property "Value" "BC558"
			(at 2.54 2.79 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "-0.2A Ic, -40V Vce, Small Signal PNP Transistor, TO-92"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "AppleJoy.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 2.54 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 90)
			(size 1.5 1.5)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "+5V")
			(pinfunction "E")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 2.54 0 90)
			(size 1.5 1.5)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 20 "Net-(Q1-B)")
			(pinfunction "B")
			(pintype "input")
		)
		(pad "3" thru_hole circle
			(at 5.08 0 90)
			(size 1.5 1.5)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 19 "Net-(Q1-C)")
			(pinfunction "C")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_THT.3dshapes/TO-92_Inline_Wide.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_Dsub:DSUB-9_Male_EdgeMount_P2.77mm"
		(layer "F.Cu")
		(at 101.712 76.492)
		(descr "9-pin D-Sub connector, solder-cups edge-mounted, male, x-pin-pitch 2.77mm, distance of mounting holes 25mm, see https://disti-assets.s3.amazonaws.com/tonar/files/datasheets/16730.pdf")
		(tags "9-pin D-Sub connector edge mount solder cup male x-pin-pitch 2.77mm mounting holes distance 25mm")
		(property "Reference" "J1"
			(at -7.784 -0.142 0)
			(layer "F.SilkS")
		)
		(property "Value" "Atari"
			(at 0 16.69 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "9-pin male plug pin D-SUB connector"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "AppleJoy.kicad_sch")
		(attr smd)
		(fp_text user "PCB edge"
			(at -10.425 1.323333 0)
			(layer "Dwgs.User")
		)
		(fp_text user "${REFERENCE}"
			(at 0 3.39 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -5.54 0)
			(size 1.846667 3.48)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 4 "UP")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -2.77 0)
			(size 1.846667 3.48)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 5 "DOWN")
			(pinfunction "2")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at 0 0)
			(size 1.846667 3.48)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 6 "LEFT")
			(pinfunction "3")
			(pintype "passive")
		)
		(pad "4" smd rect
			(at 2.77 0)
			(size 1.846667 3.48)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 7 "RIGHT")
			(pinfunction "4")
			(pintype "passive")
		)
		(pad "5" smd rect
			(at 5.54 0)
			(size 1.846667 3.48)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 8 "PADDLE_B")
			(pinfunction "5")
			(pintype "passive")
		)
		(pad "6" smd rect
			(at -4.155 0)
			(size 1.846667 3.48)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 9 "TRIGGER")
			(pinfunction "6")
			(pintype "passive")
		)
		(pad "7" smd rect
			(at -1.385 0)
			(size 1.846667 3.48)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 1 "+5V")
			(pinfunction "7")
			(pintype "passive")
		)
		(pad "8" smd rect
			(at 1.385 0)
			(size 1.846667 3.48)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 10 "GND")
			(pinfunction "8")
			(pintype "passive")
		)
		(pad "9" smd rect
			(at 4.155 0)
			(size 1.846667 3.48)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 11 "PADDLE_A")
			(pinfunction "9")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Connector_Dsub.3dshapes/DSUB-9_Male_EdgeMount_P2.77mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_THT:TO-92_Inline_Wide"
		(layer "F.Cu")
		(at 90.838 75.78 90)
		(descr "TO-92 leads in-line, wide, drill 0.75mm (see NXP sot054_po.pdf)")
		(tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
		(property "Reference" "Q5"
			(at 2.54 1.85 90)
			(layer "F.SilkS")
		)
		(property "Value" "BC558"
			(at 2.54 2.79 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "-0.2A Ic, -40V Vce, Small Signal PNP Transistor, TO-92"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "AppleJoy.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 2.54 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 90)
			(size 1.5 1.5)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "+5V")
			(pinfunction "E")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 2.54 0 90)
			(size 1.5 1.5)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 27 "Net-(Q5-B)")
			(pinfunction "B")
			(pintype "input")
		)
		(pad "3" thru_hole circle
			(at 5.08 0 90)
			(size 1.5 1.5)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 16 "BUT_0")
			(pinfunction "C")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_THT.3dshapes/TO-92_Inline_Wide.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_THT:TO-92_Inline_Wide"
		(layer "F.Cu")
		(at 105.958 65.78 90)
		(descr "TO-92 leads in-line, wide, drill 0.75mm (see NXP sot054_po.pdf)")
		(tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
		(property "Reference" "Q3"
			(at 2.54 1.85 90)
			(layer "F.SilkS")
		)
		(property "Value" "BC558"
			(at 2.54 2.79 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "-0.2A Ic, -40V Vce, Small Signal PNP Transistor, TO-92"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "AppleJoy.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 2.54 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 90)
			(size 1.5 1.5)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 14 "GAME0")
			(pinfunction "E")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 2.54 0 90)
			(size 1.5 1.5)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 24 "Net-(Q3-B)")
			(pinfunction "B")
			(pintype "input")
		)
		(pad "3" thru_hole circle
			(at 5.08 0 90)
			(size 1.5 1.5)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 23 "Net-(Q3-C)")
			(pinfunction "C")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_THT.3dshapes/TO-92_Inline_Wide.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal"
		(layer "F.Cu")
		(at 98.39 57.144 180)
		(descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.167W length 3.6mm diameter 1.6mm")
		(property "Reference" "R4"
			(at 3.762 -0.056 180)
			(layer "F.SilkS")
		)
		(property "Value" "10k"
			(at 3.81 1.92 180)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "AppleJoy.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 3.81 0 180)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 180)
			(size 1.4 1.4)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 10 "GND")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 7.62 0 180)
			(size 1.4 1.4)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 21 "Net-(Q2-C)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Potentiometer_THT:Potentiometer_Runtron_RM-065_Vertical"
		(layer "B.Cu")
		(at 110.03 48 -90)
		(descr "Potentiometer, vertical, Trimmer, RM-065 https://components101.com/sites/default/files/component_datasheet/Preset%20Potentiometer%20%28Trimpot%29.pdf")
		(tags "Potentiometer Trimmer RM-065")
		(property "Reference" "RV2"
			(at 4.5 -4.5 90)
			(layer "B.SilkS")
		)
		(property "Value" "100k"
			(at 2.6 -7.4 90)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Trim-potentiometer, US symbol"
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "AppleJoy.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 2.5 -2.5 90)
			(layer "B.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 270)
			(size 1.56 1.56)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "+5V")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 2.5 -5 270)
			(size 1.56 1.56)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 14 "GAME0")
			(pinfunction "2")
			(pintype "passive")
		)
		(pad "3" thru_hole circle
			(at 5 0 270)
			(size 1.56 1.56)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 10 "GND")
			(pinfunction "3")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Potentiometer_THT.3dshapes/Potentiometer_Runtron_RM-065_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Potentiometer_THT:Potentiometer_Runtron_RM-065_Vertical"
		(layer "B.Cu")
		(at 93.41 52.921 90)
		(descr "Potentiometer, vertical, Trimmer, RM-065 https://components101.com/sites/default/files/component_datasheet/Preset%20Potentiometer%20%28Trimpot%29.pdf")
		(tags "Potentiometer Trimmer RM-065")
		(property "Reference" "RV1"
			(at 0.351 -3.722 270)
			(layer "B.SilkS")
		)
		(property "Value" "100k"
			(at 2.6 -7.4 270)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Trim-potentiometer, US symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "AppleJoy.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 2.5 -2.5 270)
			(layer "B.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 90)
			(size 1.56 1.56)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 10 "GND")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 2.5 -5 90)
			(size 1.56 1.56)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 17 "GAME1")
			(pinfunction "2")
			(pintype "passive")
		)
		(pad "3" thru_hole circle
			(at 5 0 90)
			(size 1.56 1.56)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "+5V")
			(pinfunction "3")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Potentiometer_THT.3dshapes/Potentiometer_Runtron_RM-065_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_Dsub:DSUB-9_Male_EdgeMount_P2.77mm"
		(layer "B.Cu")
		(at 101.735 47.482)
		(descr "9-pin D-Sub connector, solder-cups edge-mounted, male, x-pin-pitch 2.77mm, distance of mounting holes 25mm, see https://disti-assets.s3.amazonaws.com/tonar/files/datasheets/16730.pdf")
		(tags "9-pin D-Sub connector edge mount solder cup male x-pin-pitch 2.77mm mounting holes distance 25mm")
		(property "Reference" "J2"
			(at -7.597 -1.202 0)
			(layer "B.SilkS")
		)
		(property "Value" "Apple"
			(at 0 -16.69 0)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "9-pin male plug pin D-SUB connector"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "AppleJoy.kicad_sch")
		(attr smd)
		(fp_text user "PCB edge"
			(at -10.425 -1.323333 0)
			(layer "Dwgs.User")
		)
		(fp_text user "${REFERENCE}"
			(at 0 -3.39 0)
			(layer "B.Fab")
		)
		(pad "1" smd rect
			(at -5.54 0)
			(size 1.846667 3.48)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 12 "BUT_1")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -2.77 0)
			(size 1.846667 3.48)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 1 "+5V")
			(pinfunction "2")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at 0 0)
			(size 1.846667 3.48)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 10 "GND")
			(pinfunction "3")
			(pintype "passive")
		)
		(pad "4" smd rect
			(at 2.77 0)
			(size 1.846667 3.48)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 13 "GAME2")
			(pinfunction "4")
			(pintype "passive")
		)
		(pad "5" smd rect
			(at 5.54 0)
			(size 1.846667 3.48)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 14 "GAME0")
			(pinfunction "5")
			(pintype "passive")
		)
		(pad "6" smd rect
			(at -4.155 0)
			(size 1.846667 3.48)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 15 "BUT_2")
			(pinfunction "6")
			(pintype "passive")
		)
		(pad "7" smd rect
			(at -1.385 0)
			(size 1.846667 3.48)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 16 "BUT_0")
			(pinfunction "7")
			(pintype "passive")
		)
		(pad "8" smd rect
			(at 1.385 0)
			(size 1.846667 3.48)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 17 "GAME1")
			(pinfunction "8")
			(pintype "passive")
		)
		(pad "9" smd rect
			(at 4.155 0)
			(size 1.846667 3.48)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 18 "GAME3")
			(pinfunction "9")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Connector_Dsub.3dshapes/DSUB-9_Male_EdgeMount_P2.77mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(gr_line
		(start 85.212 47.492)
		(end 85.212 76.492)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 85.212 47.492)
		(mid 85.797786 46.077786)
		(end 87.212 45.492)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 87.212 78.492)
		(mid 85.797786 77.906214)
		(end 85.212 76.492)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 87.212 78.492)
		(end 116.212 78.492)
		(layer "Edge.Cuts")
	)
	(gr_circle
		(center 101.712 70.492)
		(end 103.363 70.492)
		(fill no)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 116.212 45.492)
		(end 87.212 45.492)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 116.212 45.492)
		(mid 117.626214 46.077786)
		(end 118.212 47.492)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 118.212 76.492)
		(mid 117.626214 77.906214)
		(end 116.212 78.492)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 118.212 76.492)
		(end 118.212 47.492)
		(layer "Edge.Cuts")
	)
	(gr_text "Original design by Tor Arne Hustvedt 2021"
		(at 86.128 63.33 90)
		(layer "B.SilkS")
	)
	(gr_text "Revised layout by Chris RYU 2023"
		(at 89.788 54.02 90)
		(layer "B.SilkS")
	)
	(gr_text "Apple"
		(at 103.908 50.92 0)
		(layer "B.SilkS")
	)
	(gr_text "Joystick/Gamepad"
		(at 108.338 73.79 0)
		(layer "B.SilkS")
	)
	(gr_text "Apple II joystick adaptor"
		(at 117.259 63.367 90)
		(layer "B.SilkS")
	)
	(dimension
		(type aligned)
		(layer "Dwgs.User")
		(pts
			(xy 250 156) (xy 217 156)
		)
		(height -7.068)
		(format
			(prefix "")
			(suffix "")
			(units 2)
			(units_format 1)
			(precision 4)
		)
		(style
			(thickness 0.15)
			(arrow_length 1.27)
			(text_position_mode 0)
			(arrow_direction outward)
			(extension_height 0.58642)
			(extension_offset 0)
			(keep_text_aligned yes)
		)
		(gr_text "33.0000 mm"
			(at 233.5 161.918 0)
			(layer "Dwgs.User")
		)
	)
	(dimension
		(type aligned)
		(layer "Dwgs.User")
		(pts
			(xy 219 158) (xy 219 125)
		)
		(height -7.418)
		(format
			(prefix "")
			(suffix "")
			(units 2)
			(units_format 1)
			(precision 4)
		)
		(style
			(thickness 0.15)
			(arrow_length 1.27)
			(text_position_mode 0)
			(arrow_direction outward)
			(extension_height 0.58642)
			(extension_offset 0)
			(keep_text_aligned yes)
		)
		(gr_text "33.0000 mm"
			(at 210.432 141.5 90)
			(layer "Dwgs.User")
		)
	)
	(zone
		(net 10)
		(net_name "GND")
		(layers "F.Cu" "B.Cu")
		(hatch edge 0.508)
		(connect_pads
			(clearance 0.508)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.508)
			(thermal_bridge_width 0.508)
		)
		(polygon
			(pts
				(xy 118.148 78.48) (xy 85.255 78.48) (xy 85.1915 45.587) (xy 118.0845 45.587)
			)
		)
	)
	(embedded_fonts no)
)
