(kicad_pcb
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(general
		(thickness 1.6)
		(legacy_teardrops no)
	)
	(paper "B")
	(layers
		(0 "F.Cu" signal)
		(4 "In1.Cu" signal)
		(6 "In2.Cu" signal)
		(8 "In3.Cu" signal)
		(10 "In4.Cu" signal)
		(2 "B.Cu" signal)
		(9 "F.Adhes" user "F.Adhesive")
		(11 "B.Adhes" user "B.Adhesive")
		(13 "F.Paste" user)
		(15 "B.Paste" user)
		(5 "F.SilkS" user "F.Silkscreen")
		(7 "B.SilkS" user "B.Silkscreen")
		(1 "F.Mask" user)
		(3 "B.Mask" user)
		(17 "Dwgs.User" user "User.Drawings")
		(19 "Cmts.User" user "User.Comments")
		(21 "Eco1.User" user "User.Eco1")
		(23 "Eco2.User" user "User.Eco2")
		(25 "Edge.Cuts" user)
		(27 "Margin" user)
		(31 "F.CrtYd" user "F.Courtyard")
		(29 "B.CrtYd" user "B.Courtyard")
		(35 "F.Fab" user)
		(33 "B.Fab" user)
		(39 "User.1" user)
		(41 "User.2" user)
		(43 "User.3" user)
		(45 "User.4" user)
	)
	(setup
		(stackup
			(layer "F.SilkS"
				(type "Top Silk Screen")
			)
			(layer "F.Paste"
				(type "Top Solder Paste")
			)
			(layer "F.Mask"
				(type "Top Solder Mask")
				(thickness 0.01)
			)
			(layer "F.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "dielectric 1"
				(type "prepreg")
				(thickness 0.1)
				(material "FR4")
				(epsilon_r 4.5)
				(loss_tangent 0.02)
			)
			(layer "In1.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "dielectric 2"
				(type "core")
				(thickness 0.535)
				(material "FR4")
				(epsilon_r 4.5)
				(loss_tangent 0.02)
			)
			(layer "In2.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "dielectric 3"
				(type "prepreg")
				(thickness 0.1)
				(material "FR4")
				(epsilon_r 4.5)
				(loss_tangent 0.02)
			)
			(layer "In3.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "dielectric 4"
				(type "core")
				(thickness 0.535)
				(material "FR4")
				(epsilon_r 4.5)
				(loss_tangent 0.02)
			)
			(layer "In4.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "dielectric 5"
				(type "prepreg")
				(thickness 0.1)
				(material "FR4")
				(epsilon_r 4.5)
				(loss_tangent 0.02)
			)
			(layer "B.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "B.Mask"
				(type "Bottom Solder Mask")
				(thickness 0.01)
			)
			(layer "B.Paste"
				(type "Bottom Solder Paste")
			)
			(layer "B.SilkS"
				(type "Bottom Silk Screen")
			)
			(copper_finish "None")
			(dielectric_constraints no)
		)
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(tenting front back)
		(pcbplotparams
			(layerselection 0x00000000_00000000_55555555_f755f5ff)
			(plot_on_all_layers_selection 0x00000000_00000000_00000000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 4)
			(plotframeref no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(pdf_metadata yes)
			(pdf_single_document no)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plot_black_and_white yes)
			(plotinvisibletext no)
			(sketchpadsonfab no)
			(plotpadnumbers no)
			(hidednponfab no)
			(sketchdnponfab yes)
			(crossoutdnponfab yes)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 0)
			(scaleselection 1)
			(outputdirectory "Gerbers/")
		)
	)
	(net 0 "")
	(net 1 "/12Vpower/48V_RTN_DISA")
	(net 2 "/48Vpower/VF48P0_BRD")
	(net 3 "/VFF48P0_M1")
	(net 4 "/48Vpower/VF48P0_DISA")
	(net 5 "/12Vpower/VFFF48P0_PS11")
	(net 6 "/12Vpower/VBU0P0_11_21")
	(net 7 "/VB12P6_GD")
	(net 8 "/VB0P0_GD")
	(net 9 "/12Vpower/VFF48P0_DISA")
	(net 10 "Net-(C24-Pad2)")
	(net 11 "/12Vpower/VBU12P6_11_21")
	(net 12 "/BankPower1/VBU96P0")
	(net 13 "/VB96P0B1")
	(net 14 "/BankPower1/VBU0P0")
	(net 15 "/VB0P0B1")
	(net 16 "/BankPower1/VBU24P0")
	(net 17 "/VB24N0B1")
	(net 18 "/12Vpower/C50P_VB12P6_GD_EN_L")
	(net 19 "/BankPower4/VBU96P0")
	(net 20 "Net-(D1-K)")
	(net 21 "Net-(D2-K)")
	(net 22 "Net-(SW2-B)")
	(net 23 "Net-(U2-FB)")
	(net 24 "Net-(U2-EN)")
	(net 25 "/VB96P0B4")
	(net 26 "/VB0P0B4")
	(net 27 "Net-(SW3-B)")
	(net 28 "/VB24N0B4")
	(net 29 "unconnected-(U2-NC-Pad6)")
	(net 30 "unconnected-(U2-DNC-Pad5)")
	(net 31 "unconnected-(U2-SW-Pad4)")
	(net 32 "unconnected-(U2-NC-Pad3)")
	(net 33 "unconnected-(U2-PGOOD-Pad12)")
	(net 34 "unconnected-(U2-NC-Pad13)")
	(net 35 "unconnected-(U2-V5V-Pad11)")
	(net 36 "/15Vaux/VP15P0")
	(net 37 "Net-(C42-Pad2)")
	(net 38 "Net-(J1-VB24N0_FB3)")
	(net 39 "Net-(J1-LF_FB4)")
	(net 40 "Net-(J1-VB96P0_FB1)")
	(net 41 "Net-(J1-VB24N0_FB1)")
	(net 42 "Net-(J1-LF_FB1)")
	(net 43 "Net-(J1-LF_FB3)")
	(net 44 "Net-(J1-VB96P0_FB2)")
	(net 45 "Net-(J1-VB96P0_FB3)")
	(net 46 "Net-(J1-VB24N0_FB2)")
	(net 47 "Net-(J1-VB96P0_FB4)")
	(net 48 "Net-(J1-VB24N0_FB4)")
	(net 49 "Net-(J1-LF_FB2)")
	(net 50 "/VB96P0B2")
	(net 51 "/BankPower4/VBU0P0")
	(net 52 "/VB0P0B2")
	(net 53 "/BankPower4/VBU24P0")
	(net 54 "/VB24N0B2")
	(net 55 "/BankPower2/VBU0P0")
	(net 56 "/BankPower2/VBU24P0")
	(net 57 "/BankPower2/VBU96P0")
	(net 58 "/VB96P0B3")
	(net 59 "/VB0P0B3")
	(net 60 "/VB24N0B3")
	(net 61 "/BankPower3/VBU0P0")
	(net 62 "/BankPower3/VBU24P0")
	(net 63 "/BankPower3/VBU96P0")
	(net 64 "/V48P0")
	(net 65 "Net-(D5-A)")
	(net 66 "Net-(D6-A)")
	(net 67 "Net-(D7-K)")
	(net 68 "Net-(D9-K)")
	(net 69 "/BankPower1/ENABLE")
	(net 70 "/BankPower4/ENABLE")
	(net 71 "/BankPower2/ENABLE")
	(net 72 "/BankPower3/ENABLE")
	(net 73 "Net-(SW4-B)")
	(net 74 "Net-(SW1-B)")
	(net 75 "Net-(D11-K)")
	(net 76 "/48V_RTN_M1")
	(net 77 "/48V_RTN")
	(net 78 "Net-(C60-Pad2)")
	(net 79 "Net-(C78-Pad2)")
	(net 80 "Net-(D3-A)")
	(net 81 "Net-(D4-A)")
	(net 82 "Net-(D8-K)")
	(net 83 "Net-(D10-K)")
	(net 84 "Net-(J5-Pin_1)")
	(net 85 "Net-(J1-VB12P6)")
	(footprint "CustomLibraries:MillMax-Socket-0364-0-15-15-13-27-10-0"
		(layer "F.Cu")
		(at 148.984898 93.980813)
		(descr "0364-0-15-15-13-27-10-0-2")
		(tags "Connector")
		(property "Reference" "J13"
			(at 4.5974 1.6764 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "0364-0-15-15-13-27-10-0"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" "kicad-embed://Mill Max catalog-0364-0-15-15-13-27-10-0.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "CN/CONTACT SKT .048 TO .064 PIN 30UIN GOLD CONTACT//10UIN GOLD BODY"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DigikeyPN" "ED90089-ND"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "TPN" "699-882-00 "
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "/BankPower2/")
		(sheetfile "BankPower.kicad_sch")
		(attr through_hole exclude_from_pos_files)
		(embedded_fonts no)
		(model "C:/InstalledPrograms/KiCADV5/KiCad/CustomLibraries/LIB_0364-0-15-15-13-27-10-0/0364-0-15-15-13-27-10-0/3D/0364-0-15-15-13-27-10-0.stp"
			(offset
				(xyz 0 0 0.635)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -0 -90 -0)
			)
		)
	)
	(footprint "CustomLibraries:MillMax-Socket-0327-0-15-15-34-27-10-0_NO-SILK"
		(layer "F.Cu")
		(at 220.3814 206.4455)
		(descr "0364-0-15-15-13-27-10-0-2")
		(tags "Connector")
		(property "Reference" "J6"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "0327-0-15-15-34-27-10-0"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" "kicad-embed://Mill Max catalog-0364-0-15-15-13-27-10-0.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "CN/CONTACT SKT .032 TO .046 PIN 30UIN GOLD CONTACT//10UIN GOLD BODY"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DigikeyPN" "ED90081-ND"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "TPN" "699-881-00 "
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "/12Vpower/")
		(sheetfile "12Vpower.kicad_sch")
		(attr through_hole exclude_from_pos_files)
		(embedded_fonts no)
		(model "C:/InstalledPrograms/KiCADV5/KiCad/CustomLibraries/LIB_0364-0-15-15-13-27-10-0/0364-0-15-15-13-27-10-0/3D/0364-0-15-15-13-27-10-0.stp"
			(offset
				(xyz 0 0 0.635)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -0 -90 -0)
			)
		)
	)
	(footprint "MountingHole:MountingHole_3.5mm"
		(layer "F.Cu")
		(at 241.151388 37.508237)
		(descr "Mounting Hole 3.5mm, no annular")
		(tags "mounting hole 3.5mm no annular")
		(property "Reference" "H1"
			(at 0 -4.5 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "MountingHole"
			(at 0 4.5 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Mounting Hole without connection"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "MountingHole*")
		(sheetname "/")
		(sheetfile "BenchPowerBoardNewCMchoke.kicad_sch")
		(clearance 3.81)
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 3.5 3.5)
			(drill 3.5)
			(layers "*.Cu" "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "CustomLibraries:Amphenol_power_conn-Receptacle"
		(layer "F.Cu")
		(at 92.798178 211.329438)
		(property "Reference" "J1"
			(at -28.9 -10.475 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "~"
			(at -27.455 -13.1 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 -18.2 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "CUSTOM/CN, 14POS POWER SOCKET DWR 3MM RADSOCK"
			(at 0 -18.2 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "TPN" "694-989-00"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MFGPN" "AMPHENOL CORP  10179038-S014LF"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "BenchPowerBoardNewCMchoke.kicad_sch")
		(attr through_hole)
		(fp_text user "GND"
			(at 18.73 11.03 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "A"
			(at 31 -4 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "C"
			(at 30.56 5.33 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "B"
			(at 31 0.6 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "B1+"
			(at -21.43 -9.61 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "B2+"
			(at -11.14 -9.61 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "B4+"
			(at 8.712919 -9.483928 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "12V"
			(at 23.397594 -9.61 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "B3+"
			(at -1.61 -9.61 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "${REFERENCE}"
			(at -0.015 -12.93 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole circle
			(at -25.25 0 180)
			(size 3.302 3.302)
			(drill 3.4)
			(layers "F&B.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 25.25 -5.5 180)
			(size 3.302 3.302)
			(drill 3.4)
			(layers "F&B.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 25.25 0 180)
			(size 3.302 3.302)
			(drill 3.4)
			(layers "F&B.Cu" "*.Mask")
		)
		(pad "A1" thru_hole circle
			(at 20 -4.5 180)
			(size 4.064 4.064)
			(drill 3.175)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 85 "Net-(J1-VB12P6)")
			(pinfunction "VB12P6")
			(pintype "passive")
		)
		(pad "A2" thru_hole circle
			(at 10 -4.5 180)
			(size 4.064 4.064)
			(drill 3.175)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 47 "Net-(J1-VB96P0_FB4)")
			(pinfunction "VB96P0_FB4")
			(pintype "passive")
		)
		(pad "A3" thru_hole circle
			(at 0 -4.5 180)
			(size 4.064 4.064)
			(drill 3.175)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 45 "Net-(J1-VB96P0_FB3)")
			(pinfunction "VB96P0_FB3")
			(pintype "passive")
		)
		(pad "A4" thru_hole circle
			(at -10 -4.5 180)
			(size 4.064 4.064)
			(drill 3.175)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 44 "Net-(J1-VB96P0_FB2)")
			(pinfunction "VB96P0_FB2")
			(pintype "passive")
		)
		(pad "A5" thru_hole circle
			(at -20 -4.5 180)
			(size 4.064 4.064)
			(drill 3.175)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 40 "Net-(J1-VB96P0_FB1)")
			(pinfunction "VB96P0_FB1")
			(pintype "passive")
		)
		(pad "B2" thru_hole circle
			(at 15 0 180)
			(size 4.064 4.064)
			(drill 3.175)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 39 "Net-(J1-LF_FB4)")
			(pinfunction "LF_FB4")
			(pintype "passive")
		)
		(pad "B3" thru_hole circle
			(at 5 0 180)
			(size 4.064 4.064)
			(drill 3.175)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 43 "Net-(J1-LF_FB3)")
			(pinfunction "LF_FB3")
			(pintype "passive")
		)
		(pad "B4" thru_hole circle
			(at -5 0 180)
			(size 4.064 4.064)
			(drill 3.175)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 49 "Net-(J1-LF_FB2)")
			(pinfunction "LF_FB2")
			(pintype "passive")
		)
		(pad "B5" thru_hole circle
			(at -15 0 180)
			(size 4.064 4.064)
			(drill 3.175)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 42 "Net-(J1-LF_FB1)")
			(pinfunction "LF_FB1")
			(pintype "passive")
		)
		(pad "C1" thru_hole circle
			(at 20 4.5 180)
			(size 4.064 4.064)
			(drill 3.175)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 8 "/VB0P0_GD")
			(pinfunction "BRDGND")
			(pintype "passive")
		)
		(pad "C2" thru_hole circle
			(at 10 4.5 180)
			(size 4.064 4.064)
			(drill 3.175)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 48 "Net-(J1-VB24N0_FB4)")
			(pinfunction "VB24N0_FB4")
			(pintype "passive")
		)
		(pad "C3" thru_hole circle
			(at 0 4.5 270)
			(size 4.064 4.064)
			(drill 3.175)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 38 "Net-(J1-VB24N0_FB3)")
			(pinfunction "VB24N0_FB3")
			(pintype "passive")
		)
		(pad "C4" thru_hole circle
			(at -10 4.5 180)
			(size 4.064 4.064)
			(drill 3.175)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 46 "Net-(J1-VB24N0_FB2)")
			(pinfunction "VB24N0_FB2")
			(pintype "passive")
		)
		(pad "C5" thru_hole circle
			(at -20 4.5 180)
			(size 4.064 4.064)
			(drill 3.175)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 41 "Net-(J1-VB24N0_FB1)")
			(pinfunction "VB24N0_FB1")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KIPRJMOD}/Components/694-989-00_14PinConn-Socket.STEP"
			(offset
				(xyz 2.38 -2.76 13)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -0 -0 -180)
			)
		)
		(model "${KIPRJMOD}/694-989-00_14PinConn-Socket.STEP"
			(offset
				(xyz 2.37999999 -2.759999992 13.00000001)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -0 -0 -180)
			)
		)
	)
	(footprint "CustomLibraries:FIL_CM5441Z101B-10"
		(layer "F.Cu")
		(at 156.593 220.4226 90)
		(descr "Common Mode Choke 100 MHZ 100R 75A 2LN 100 OHM  Laird  CM5441Z101B-10")
		(tags "Choke ")
		(property "Reference" "L1"
			(at 8.4122 -0.1206 270)
			(layer "F.SilkS")
		)
		(property "Value" "CM5441Z101B-10"
			(at 4.57 6.335 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "kicad-embed://cm5441z101b-10-datasheet.pdf"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Common Mode Choke 100 MHZ 100R 75A 2LN 100 OHM"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "STANDARD" "100 MHZ 100R 75A"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MAXIMUM_PACKAGE_HEIGHT" "10.77 mm"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER" "Laird"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DigikeyPN" "240-2489-ND"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "TPN" "626-010-00"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/12Vpower/")
		(sheetfile "12Vpower.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole oval
			(at -3.175 2.64 90)
			(size 4.58 2.29)
			(drill oval 3.56 1.52)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 11 "/12Vpower/VBU12P6_11_21")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" thru_hole oval
			(at 3.175 2.64 90)
			(size 4.58 2.29)
			(drill oval 3.56 1.52)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "/12Vpower/VBU0P0_11_21")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "3" thru_hole oval
			(at 3.175 -2.64 90)
			(size 4.58 2.29)
			(drill oval 3.56 1.52)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 8 "/VB0P0_GD")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "4" thru_hole oval
			(at -3.175 -2.64 90)
			(size 4.58 2.29)
			(drill oval 3.56 1.52)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 7 "/VB12P6_GD")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
		(model "C:/InstalledPrograms/KiCADV5/KiCad/CustomLibraries/CM5441Z101B_10/CM5441Z101B-10.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 -0 -0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_Elec_10x10.2"
		(layer "F.Cu")
		(at 121.200755 179.050863 180)
		(descr "SMD capacitor, aluminum electrolytic nonpolar, 10.0x10.2mm")
		(tags "capacitor electrolyic nonpolar")
		(property "Reference" "C69"
			(at 7.0358 -3.0504 0)
			(layer "F.SilkS")
		)
		(property "Value" "120uF/63V/10x10"
			(at 0 6.2 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "CAP, ALUMINUM POLYMER 120UF 20% 63V RADIAL"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DigikeyPN" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "TPN" "701-721-00"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MFGPN" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "CP_*")
		(sheetname "/BankPower4/")
		(sheetfile "BankPower.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -4.4 0 180)
			(size 4.6 2.1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.119048)
			(net 78 "Net-(C60-Pad2)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 4.4 0 180)
			(size 4.6 2.1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.119048)
			(net 26 "/VB0P0B4")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_Elec_10x10.2.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "CustomLibraries:MillMax-Socket-0364-0-15-15-13-27-10-0"
		(layer "F.Cu")
		(at 169.5814 221.6855)
		(descr "0364-0-15-15-13-27-10-0-2")
		(tags "Connector")
		(property "Reference" "J2"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "0364-0-15-15-13-27-10-0"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" "kicad-embed://Mill Max catalog-0364-0-15-15-13-27-10-0.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "CN/CONTACT SKT .048 TO .064 PIN 30UIN GOLD CONTACT//10UIN GOLD BODY"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DigikeyPN" "ED90089-ND"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "TPN" "699-882-00 "
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "/12Vpower/")
		(sheetfile "12Vpower.kicad_sch")
		(attr through_hole exclude_from_pos_files)
		(embedded_fonts no)
		(model "C:/InstalledPrograms/KiCADV5/KiCad/CustomLibraries/LIB_0364-0-15-15-13-27-10-0/0364-0-15-15-13-27-10-0/3D/0364-0-15-15-13-27-10-0.stp"
			(offset
				(xyz 0 0 0.635)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -0 -90 -0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_Elec_10x10.2"
		(layer "F.Cu")
		(at 121.200755 136.939883 180)
		(descr "SMD capacitor, aluminum electrolytic nonpolar, 10.0x10.2mm")
		(tags "capacitor electrolyic nonpolar")
		(property "Reference" "C87"
			(at 7.0358 -3.0504 0)
			(layer "F.SilkS")
		)
		(property "Value" "120uF/63V/10x10"
			(at 0 6.2 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "CAP, ALUMINUM POLYMER 120UF 20% 63V RADIAL"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DigikeyPN" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "TPN" "701-721-00"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MFGPN" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "CP_*")
		(sheetname "/BankPower3/")
		(sheetfile "BankPower.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -4.4 0 180)
			(size 4.6 2.1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.119048)
			(net 79 "Net-(C78-Pad2)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 4.4 0 180)
			(size 4.6 2.1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.119048)
			(net 59 "/VB0P0B3")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_Elec_10x10.2.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "CustomLibraries:MillMax-Socket-0327-0-15-15-34-27-10-0_NO-SILK"
		(layer "F.Cu")
		(at 207.627155 172.613063)
		(descr "0364-0-15-15-13-27-10-0-2")
		(tags "Connector")
		(property "Reference" "J26"
			(at -4.826 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "0327-0-15-15-34-27-10-0"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" "kicad-embed://Mill Max catalog-0364-0-15-15-13-27-10-0.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "CN/CONTACT SKT .032 TO .046 PIN 30UIN GOLD CONTACT//10UIN GOLD BODY"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DigikeyPN" "ED90081-ND"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "TPN" "699-881-00 "
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "/BankPower4/")
		(sheetfile "BankPower.kicad_sch")
		(attr through_hole exclude_from_pos_files)
		(embedded_fonts no)
		(model "C:/InstalledPrograms/KiCADV5/KiCad/CustomLibraries/LIB_0364-0-15-15-13-27-10-0/0364-0-15-15-13-27-10-0/3D/0364-0-15-15-13-27-10-0.stp"
			(offset
				(xyz 0 0 0.635)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -0 -90 -0)
			)
		)
	)
	(footprint "CustomLibraries:MillMax-Socket-0327-0-15-15-34-27-10-0_NO-SILK"
		(layer "F.Cu")
		(at 207.627155 145.894483)
		(descr "0364-0-15-15-13-27-10-0-2")
		(tags "Connector")
		(property "Reference" "J29"
			(at -3.0226 2.413 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "0327-0-15-15-34-27-10-0"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" "kicad-embed://Mill Max catalog-0364-0-15-15-13-27-10-0.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "CN/CONTACT SKT .032 TO .046 PIN 30UIN GOLD CONTACT//10UIN GOLD BODY"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DigikeyPN" "ED90081-ND"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "TPN" "699-881-00 "
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "/BankPower3/")
		(sheetfile "BankPower.kicad_sch")
		(attr through_hole exclude_from_pos_files)
		(embedded_fonts no)
		(model "C:/InstalledPrograms/KiCADV5/KiCad/CustomLibraries/LIB_0364-0-15-15-13-27-10-0/0364-0-15-15-13-27-10-0/3D/0364-0-15-15-13-27-10-0.stp"
			(offset
				(xyz 0 0 0.635)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -0 -90 -0)
			)
		)
	)
	(footprint "CustomLibraries:CM4440Z111R10"
		(layer "F.Cu")
		(at 136.407871 39.554498 180)
		(descr "CM4440Z111R-10-2")
		(tags "Inductor")
		(property "Reference" "FL2"
			(at 1.1736 -7.534 0)
			(layer "F.SilkS")
		)
		(property "Value" "CM4440Z111R_10"
			(at 0 0.213 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" "kicad-embed://cm4440z111r-10-datasheet.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "COMMON MODE CHOKES TRIPLE 110OHM 100MHZ 20A 0.001OHM DCR"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DigikeyPN" "240-CM4440Z111R-10CT-ND"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "TPN" "693-673-00"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "L* L_CommonMode*")
		(sheetname "/BankPower1/")
		(sheetfile "BankPower.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0.213 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -2.54 3.435 180)
			(size 2.03 5.08)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 12 "/BankPower1/VBU96P0")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 0 3.435 180)
			(size 2.03 5.08)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 14 "/BankPower1/VBU0P0")
			(pinfunction "2")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at 2.54 3.435 180)
			(size 2.03 5.08)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 16 "/BankPower1/VBU24P0")
			(pinfunction "3")
			(pintype "passive")
		)
		(pad "4" smd rect
			(at 2.54 -3.435 180)
			(size 2.03 5.08)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 17 "/VB24N0B1")
			(pinfunction "4")
			(pintype "passive")
		)
		(pad "5" smd rect
			(at 0 -3.435 180)
			(size 2.03 5.08)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 15 "/VB0P0B1")
			(pinfunction "5")
			(pintype "passive")
		)
		(pad "6" smd rect
			(at -2.54 -3.435 180)
			(size 2.03 5.08)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 13 "/VB96P0B1")
			(pinfunction "6")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "CM4440Z111R-10.stp"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
		(model "C:/InstalledPrograms/KiCADV5/KiCad/CustomLibraries/LIB_CM4440Z111R-10/CM4440Z111R-10/3D/CM4440Z111R-10.stp"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -0 -0 -0)
			)
		)
	)
	(footprint "CustomLibraries:MillMax-Socket-0327-0-15-15-34-27-10-0_NO-SILK"
		(layer "F.Cu")
		(at 207.404898 104.902813)
		(descr "0364-0-15-15-13-27-10-0-2")
		(tags "Connector")
		(property "Reference" "J8"
			(at -3.0226 2.413 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "0327-0-15-15-34-27-10-0"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" "kicad-embed://Mill Max catalog-0364-0-15-15-13-27-10-0.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "CN/CONTACT SKT .032 TO .046 PIN 30UIN GOLD CONTACT//10UIN GOLD BODY"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DigikeyPN" "ED90081-ND"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "TPN" "699-881-00 "
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "/BankPower2/")
		(sheetfile "BankPower.kicad_sch")
		(attr through_hole exclude_from_pos_files)
		(embedded_fonts no)
		(model "C:/InstalledPrograms/KiCADV5/KiCad/CustomLibraries/LIB_0364-0-15-15-13-27-10-0/0364-0-15-15-13-27-10-0/3D/0364-0-15-15-13-27-10-0.stp"
			(offset
				(xyz 0 0 0.635)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -0 -90 -0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1206_3216Metric_Pad1.33x1.80mm_HandSolder"
		(layer "F.Cu")
		(at 262.299553 99.054635)
		(descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C14"
			(at 0.270307 2.252407 0)
			(layer "F.SilkS")
		)
		(property "Value" "4.7UF/100VDC/1206"
			(at 0 1.85 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "CAP, CERAMIC 4.7UF 10% 100V X7S 1206"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MFGPN" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DigikeyPN" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "TPN" "698-396-00"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/15Vaux/")
		(sheetfile "15Vaux.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.5625 0)
			(size 1.325 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.188679)
			(net 3 "/VFF48P0_M1")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.5625 0)
			(size 1.325 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.188679)
			(net 76 "/48V_RTN_M1")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "LED_SMD:LED_0603_1608Metric_Pad1.05x0.95mm_HandSolder"
		(layer "F.Cu")
		(at 140.772752 71.930153 90)
		(descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
		(tags "LED handsolder")
		(property "Reference" "D10"
			(at -0.058351 -1.826939 90)
			(layer "F.SilkS")
		)
		(property "Value" "LED"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Light emitting diode"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DigikeyPN" "350-2035-1-ND"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MFGPN" "DIALIGHT CO  598-8070-107F"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "LED* LED_SMD:* LED_THT:*")
		(sheetname "/")
		(sheetfile "BenchPowerBoardNewCMchoke.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.875 0 90)
			(size 1.05 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 83 "Net-(D10-K)")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.875 0 90)
			(size 1.05 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 13 "/VB96P0B1")
			(pinfunction "A")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "CustomLibraries:MillMax-Socket-0364-0-15-15-13-27-10-0"
		(layer "F.Cu")
		(at 149.207155 169.463463)
		(descr "0364-0-15-15-13-27-10-0-2")
		(tags "Connector")
		(property "Reference" "J31"
			(at 1.07188 -3.4798 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "0364-0-15-15-13-27-10-0"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" "kicad-embed://Mill Max catalog-0364-0-15-15-13-27-10-0.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "CN/CONTACT SKT .048 TO .064 PIN 30UIN GOLD CONTACT//10UIN GOLD BODY"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DigikeyPN" "ED90089-ND"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "TPN" "699-882-00 "
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "/BankPower4/")
		(sheetfile "BankPower.kicad_sch")
		(attr through_hole exclude_from_pos_files)
		(embedded_fonts no)
		(model "C:/InstalledPrograms/KiCADV5/KiCad/CustomLibraries/LIB_0364-0-15-15-13-27-10-0/0364-0-15-15-13-27-10-0/3D/0364-0-15-15-13-27-10-0.stp"
			(offset
				(xyz 0 0 0.635)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -0 -90 -0)
			)
		)
	)
	(footprint "Fuse:Fuse_Littelfuse-NANO2-451_453"
		(layer "F.Cu")
		(at 236.2342 223.9556 180)
		(descr "Littelfuse NANO2 https://www.littelfuse.com/~/media/electronics/datasheets/fuses/littelfuse_fuse_451_453_datasheet.pdf.pdf")
		(tags "Fuse Nano2")
		(property "Reference" "F1"
			(at -0.641307 2.954511 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "10A"
			(at 0 2.7 180)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "451/453 Series Very Fast-Acting Fuse"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "TPN" "522-946-10"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DigikeyPN" "F2591CT-ND"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MFGPN" "0451010.MRL"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*Fuse*")
		(sheetname "/12Vpower/")
		(sheetfile "12Vpower.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -2.455 0 180)
			(size 1.96 3.15)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 9 "/12Vpower/VFF48P0_DISA")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 2.455 0 180)
			(size 1.96 3.15)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 5 "/12Vpower/VFFF48P0_PS11")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Fuse.3dshapes/Fuse_Littelfuse-NANO2-451_453.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "CustomLibraries:MillMax-Socket-0364-0-15-15-13-27-10-0"
		(layer "F.Cu")
		(at 149.207155 184.703463 180)
		(descr "0364-0-15-15-13-27-10-0-2")
		(tags "Connector")
		(property "Reference" "J23"
			(at -3.8862 2.0066 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "0364-0-15-15-13-27-10-0"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" "kicad-embed://Mill Max catalog-0364-0-15-15-13-27-10-0.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "CN/CONTACT SKT .048 TO .064 PIN 30UIN GOLD CONTACT//10UIN GOLD BODY"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DigikeyPN" "ED90089-ND"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "TPN" "699-882-00 "
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "/BankPower4/")
		(sheetfile "BankPower.kicad_sch")
		(attr through_hole exclude_from_pos_files)
		(embedded_fonts no)
		(model "C:/InstalledPrograms/KiCADV5/KiCad/CustomLibraries/LIB_0364-0-15-15-13-27-10-0/0364-0-15-15-13-27-10-0/3D/0364-0-15-15-13-27-10-0.stp"
			(offset
				(xyz 0 0 0.635)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -0 -90 -0)
			)
		)
	)
	(footprint "CustomLibraries:MillMax-Socket-0364-0-15-15-13-27-10-0"
		(layer "F.Cu")
		(at 149.207155 142.592483 180)
		(descr "0364-0-15-15-13-27-10-0-2")
		(tags "Connector")
		(property "Reference" "J30"
			(at -3.8862 2.0066 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "0364-0-15-15-13-27-10-0"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" "kicad-embed://Mill Max catalog-0364-0-15-15-13-27-10-0.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "CN/CONTACT SKT .048 TO .064 PIN 30UIN GOLD CONTACT//10UIN GOLD BODY"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DigikeyPN" "ED90089-ND"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "TPN" "699-882-00 "
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "/BankPower3/")
		(sheetfile "BankPower.kicad_sch")
		(attr through_hole exclude_from_pos_files)
		(embedded_fonts no)
		(model "C:/InstalledPrograms/KiCADV5/KiCad/CustomLibraries/LIB_0364-0-15-15-13-27-10-0/0364-0-15-15-13-27-10-0/3D/0364-0-15-15-13-27-10-0.stp"
			(offset
				(xyz 0 0 0.635)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -0 -90 -0)
			)
		)
	)
	(footprint "CustomLibraries:MillMax-Socket-0364-0-15-15-13-27-10-0"
		(layer "F.Cu")
		(at 148.984898 86.360813)
		(descr "0364-0-15-15-13-27-10-0-2")
		(tags "Connector")
		(property "Reference" "J17"
			(at 1.07188 -3.4798 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "0364-0-15-15-13-27-10-0"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" "kicad-embed://Mill Max catalog-0364-0-15-15-13-27-10-0.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "CN/CONTACT SKT .048 TO .064 PIN 30UIN GOLD CONTACT//10UIN GOLD BODY"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DigikeyPN" "ED90089-ND"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "TPN" "699-882-00 "
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "/BankPower2/")
		(sheetfile "BankPower.kicad_sch")
		(attr through_hole exclude_from_pos_files)
		(embedded_fonts no)
		(model "C:/InstalledPrograms/KiCADV5/KiCad/CustomLibraries/LIB_0364-0-15-15-13-27-10-0/0364-0-15-15-13-27-10-0/3D/0364-0-15-15-13-27-10-0.stp"
			(offset
				(xyz 0 0 0.635)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -0 -90 -0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_Elec_10x10.2"
		(layer "F.Cu")
		(at 122.504471 53.597098 180)
		(descr "SMD capacitor, aluminum electrolytic nonpolar, 10.0x10.2mm")
		(tags "capacitor electrolyic nonpolar")
		(property "Reference" "C51"
			(at 7.0358 -3.0504 0)
			(layer "F.SilkS")
		)
		(property "Value" "120uF/63V/10x10"
			(at 0 6.2 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "CAP, ALUMINUM POLYMER 120UF 20% 63V RADIAL"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DigikeyPN" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "TPN" "701-721-00"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MFGPN" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "CP_*")
		(sheetname "/BankPower1/")
		(sheetfile "BankPower.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -4.4 0 180)
			(size 4.6 2.1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.119048)
			(net 37 "Net-(C42-Pad2)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 4.4 0 180)
			(size 4.6 2.1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.119048)
			(net 15 "/VB0P0B1")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_Elec_10x10.2.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "CustomLibraries:MillMax-Socket-0327-0-15-15-34-27-10-0_NO-SILK"
		(layer "F.Cu")
		(at 169.5814 214.0655)
		(descr "0364-0-15-15-13-27-10-0-2")
		(tags "Connector")
		(property "Reference" "J5"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "0327-0-15-15-34-27-10-0"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" "kicad-embed://Mill Max catalog-0364-0-15-15-13-27-10-0.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "CN/CONTACT SKT .032 TO .046 PIN 30UIN GOLD CONTACT//10UIN GOLD BODY"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DigikeyPN" "ED90081-ND"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "TPN" "699-881-00 "
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "/12Vpower/")
		(sheetfile "12Vpower.kicad_sch")
		(attr through_hole exclude_from_pos_files)
		(embedded_fonts no)
		(model "C:/InstalledPrograms/KiCADV5/KiCad/CustomLibraries/LIB_0364-0-15-15-13-27-10-0/0364-0-15-15-13-27-10-0/3D/0364-0-15-15-13-27-10-0.stp"
			(offset
				(xyz 0 0 0.635)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -0 -90 -0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 218.119231 130.871546 -90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R28"
			(at 3.257765 0.226876 90)
			(layer "F.SilkS")
		)
		(property "Value" "2k"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "TPN" "636-702-00"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/BankPower3/")
		(sheetfile "BankPower.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 270)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 36 "/15Vaux/VP15P0")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0 270)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 27 "Net-(SW3-B)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "LED_SMD:LED_0603_1608Metric_Pad1.05x0.95mm_HandSolder"
		(layer "F.Cu")
		(at 140.822709 197.118337 90)
		(descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
		(tags "LED handsolder")
		(property "Reference" "D7"
			(at 0 -1.43 90)
			(layer "F.SilkS")
		)
		(property "Value" "LED"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Light emitting diode"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DigikeyPN" "350-2035-1-ND"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MFGPN" "DIALIGHT CO  598-8070-107F"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "LED* LED_SMD:* LED_THT:*")
		(sheetname "/")
		(sheetfile "BenchPowerBoardNewCMchoke.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.875 0 90)
			(size 1.05 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 67 "Net-(D7-K)")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.875 0 90)
			(size 1.05 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 25 "/VB96P0B4")
			(pinfunction "A")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_Elec_10x10.2"
		(layer "F.Cu")
		(at 120.978498 95.948213 180)
		(descr "SMD capacitor, aluminum electrolytic nonpolar, 10.0x10.2mm")
		(tags "capacitor electrolyic nonpolar")
		(property "Reference" "C31"
			(at 7.0358 -3.0504 0)
			(layer "F.SilkS")
		)
		(property "Value" "120uF/63V/10x10"
			(at 0 6.2 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "CAP, ALUMINUM POLYMER 120UF 20% 63V RADIAL"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DigikeyPN" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "TPN" "701-721-00"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MFGPN" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "CP_*")
		(sheetname "/BankPower2/")
		(sheetfile "BankPower.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -4.4 0 180)
			(size 4.6 2.1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.119048)
			(net 10 "Net-(C24-Pad2)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 4.4 0 180)
			(size 4.6 2.1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.119048)
			(net 52 "/VB0P0B2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_Elec_10x10.2.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "LED_SMD:LED_0603_1608Metric_Pad1.05x0.95mm_HandSolder"
		(layer "F.Cu")
		(at 124.381606 75.401019 180)
		(descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
		(tags "LED handsolder")
		(property "Reference" "D5"
			(at -2.87883 -0.180131 0)
			(layer "F.SilkS")
		)
		(property "Value" "LED"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Light emitting diode"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DigikeyPN" "350-2035-1-ND"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MFGPN" "DIALIGHT CO  598-8070-107F"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "LED* LED_SMD:* LED_THT:*")
		(sheetname "/")
		(sheetfile "BenchPowerBoardNewCMchoke.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.875 0 180)
			(size 1.05 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 54 "/VB24N0B2")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.875 0 180)
			(size 1.05 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 65 "Net-(D5-A)")
			(pinfunction "A")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "CustomLibraries:RDA0015A-MFG"
		(layer "F.Cu")
		(at 256.641397 97.80017 -90)
		(tags "TPSM5601R5HRDAR ")
		(property "Reference" "U2"
			(at -4.854119 -0.066548 270)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "TPSM5601R5HRDAR"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "TPSM5601R5HRDAR"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "TPN" "682-341-00"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DigikeyPN" "296-TPSM5601R5HRDARCT-ND"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "RDA0015A-MFG")
		(sheetname "/15Vaux/")
		(sheetfile "15Vaux.kicad_sch")
		(fp_text user "${REFERENCE}"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -2.000001 -2.145 270)
			(size 1.4 0.499999)
			(layers "F.Cu" "F.Mask")
			(net 3 "/VFF48P0_M1")
			(pinfunction "VIN")
			(pintype "power_in")
		)
		(pad "2" smd rect
			(at -2.35 -1.17 270)
			(size 0.700001 0.349999)
			(layers "F.Cu" "F.Mask")
			(net 24 "Net-(U2-EN)")
			(pinfunction "EN")
			(pintype "input")
		)
		(pad "3" smd rect
			(at -2.35 -0.519999 270)
			(size 0.700001 0.349999)
			(layers "F.Cu" "F.Mask")
			(net 32 "unconnected-(U2-NC-Pad3)")
			(pinfunction "NC")
			(pintype "unspecified")
		)
		(pad "4" smd rect
			(at -2.35 0.13 270)
			(size 0.700001 0.349999)
			(layers "F.Cu" "F.Mask")
			(net 31 "unconnected-(U2-SW-Pad4)")
			(pinfunction "SW")
			(pintype "power_in")
		)
		(pad "5" smd rect
			(at -2.35 0.780001 270)
			(size 0.700001 0.349999)
			(layers "F.Cu" "F.Mask")
			(net 30 "unconnected-(U2-DNC-Pad5)")
			(pinfunction "DNC")
			(pintype "unspecified")
		)
		(pad "6" smd rect
			(at -2.35 1.430002 270)
			(size 0.700001 0.349999)
			(layers "F.Cu" "F.Mask")
			(net 29 "unconnected-(U2-NC-Pad6)")
			(pinfunction "NC")
			(pintype "unspecified")
		)
		(pad "7" smd rect
			(at -2.000001 2.154999 270)
			(size 1.4 0.499999)
			(layers "F.Cu" "F.Mask")
			(net 36 "/15Vaux/VP15P0")
			(pinfunction "VOUT")
			(pintype "unspecified")
		)
		(pad "8" smd rect
			(at 2.000001 2.154999 270)
			(size 1.4 0.499999)
			(layers "F.Cu" "F.Mask")
			(net 36 "/15Vaux/VP15P0")
			(pinfunction "VOUT")
			(pintype "unspecified")
		)
		(pad "9" smd rect
			(at 2.35 1.43 270)
			(size 0.700001 0.349999)
			(layers "F.Cu" "F.Mask")
			(net 23 "Net-(U2-FB)")
			(pinfunction "FB")
			(pintype "input")
		)
		(pad "10" smd rect
			(at 2.35 0.780001 270)
			(size 0.700001 0.349999)
			(layers "F.Cu" "F.Mask")
			(net 76 "/48V_RTN_M1")
			(pinfunction "AGND")
			(pintype "power_in")
		)
		(pad "11" smd rect
			(at 2.35 0.13 270)
			(size 0.700001 0.349999)
			(layers "F.Cu" "F.Mask")
			(net 35 "unconnected-(U2-V5V-Pad11)")
			(pinfunction "V5V")
			(pintype "power_in")
		)
		(pad "12" smd rect
			(at 2.35 -0.519999 270)
			(size 0.700001 0.349999)
			(layers "F.Cu" "F.Mask")
			(net 33 "unconnected-(U2-PGOOD-Pad12)")
			(pinfunction "PGOOD")
			(pintype "open_collector")
		)
		(pad "13" smd rect
			(at 2.35 -1.17 270)
			(size 0.700001 0.349999)
			(layers "F.Cu" "F.Mask")
			(net 34 "unconnected-(U2-NC-Pad13)")
			(pinfunction "NC")
			(pintype "unspecified")
		)
		(pad "14" smd rect
			(at 2.000001 -2.145 270)
			(size 1.4 0.499999)
			(layers "F.Cu" "F.Mask")
			(net 3 "/VFF48P0_M1")
			(pinfunction "VIN")
			(pintype "power_in")
		)
		(pad "15" thru_hole circle
			(at -1.000001 -1.000001 270)
			(size 0.499999 0.499999)
			(drill 0.2032)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 76 "/48V_RTN_M1")
			(pinfunction "PGND")
			(pintype "power_in")
		)
		(pad "15" thru_hole circle
			(at -1.000001 0 270)
			(size 0.499999 0.499999)
			(drill 0.2032)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 76 "/48V_RTN_M1")
			(pinfunction "PGND")
			(pintype "power_in")
		)
		(pad "15" thru_hole circle
			(at -1.000001 1.000001 270)
			(size 0.499999 0.499999)
			(drill 0.2032)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 76 "/48V_RTN_M1")
			(pinfunction "PGND")
			(pintype "power_in")
		)
		(pad "15" thru_hole circle
			(at 0 -2.000001 270)
			(size 0.499999 0.499999)
			(drill 0.2032)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 76 "/48V_RTN_M1")
			(pinfunction "PGND")
			(pintype "power_in")
		)
		(pad "15" thru_hole circle
			(at 0 -1.000001 270)
			(size 0.499999 0.499999)
			(drill 0.2032)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 76 "/48V_RTN_M1")
			(pinfunction "PGND")
			(pintype "power_in")
		)
		(pad "15" smd circle
			(at 0 0 270)
			(size 2.250001 2.250001)
			(layers "F.Cu" "F.Mask")
			(net 76 "/48V_RTN_M1")
			(pinfunction "PGND")
			(pintype "power_in")
		)
		(pad "15" thru_hole circle
			(at 0 1.000001 270)
			(size 0.499999 0.499999)
			(drill 0.2032)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 76 "/48V_RTN_M1")
			(pinfunction "PGND")
			(pintype "power_in")
		)
		(pad "15" thru_hole circle
			(at 0 2.000001 270)
			(size 0.499999 0.499999)
			(drill 0.2032)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 76 "/48V_RTN_M1")
			(pinfunction "PGND")
			(pintype "power_in")
		)
		(pad "15" thru_hole circle
			(at 1.000001 -1.000001 270)
			(size 0.499999 0.499999)
			(drill 0.2032)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 76 "/48V_RTN_M1")
			(pinfunction "PGND")
			(pintype "power_in")
		)
		(pad "15" thru_hole circle
			(at 1.000001 0 270)
			(size 0.499999 0.499999)
			(drill 0.2032)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 76 "/48V_RTN_M1")
			(pinfunction "PGND")
			(pintype "power_in")
		)
		(pad "15" thru_hole circle
			(at 1.000001 1.000001 270)
			(size 0.499999 0.499999)
			(drill 0.2032)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 76 "/48V_RTN_M1")
			(pinfunction "PGND")
			(pintype "power_in")
		)
		(pad "24" thru_hole circle
			(at 0.0254 0 270)
			(size 0.499999 0.499999)
			(drill 0.2032)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(embedded_fonts no)
		(model "C:/InstalledPrograms/KiCADV5/KiCad/CustomLibraries/TPSM5601R5HRDAR/RDA0015A.stp"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -0 -0 -0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_Elec_10x10.2"
		(layer "F.Cu")
		(at 121.097555 147.928083 180)
		(descr "SMD capacitor, aluminum electrolytic nonpolar, 10.0x10.2mm")
		(tags "capacitor electrolyic nonpolar")
		(property "Reference" "C85"
			(at 7.1882 -3.1012 0)
			(layer "F.SilkS")
		)
		(property "Value" "120uF/63V/10x10"
			(at 0 6.2 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "CAP, ALUMINUM POLYMER 120UF 20% 63V RADIAL"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DigikeyPN" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "TPN" "701-721-00"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MFGPN" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "CP_*")
		(sheetname "/BankPower3/")
		(sheetfile "BankPower.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -4.4 0 180)
			(size 4.6 2.1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.119048)
			(net 79 "Net-(C78-Pad2)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 4.4 0 180)
			(size 4.6 2.1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.119048)
			(net 59 "/VB0P0B3")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_Elec_10x10.2.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "LED_SMD:LED_0603_1608Metric_Pad1.05x0.95mm_HandSolder"
		(layer "F.Cu")
		(at 124.433471 33.096498 180)
		(descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
		(tags "LED handsolder")
		(property "Reference" "D6"
			(at -3.048 -0.16 0)
			(layer "F.SilkS")
		)
		(property "Value" "LED"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Light emitting diode"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DigikeyPN" "350-2035-1-ND"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MFGPN" "DIALIGHT CO  598-8070-107F"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "LED* LED_SMD:* LED_THT:*")
		(sheetname "/")
		(sheetfile "BenchPowerBoardNewCMchoke.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.875 0 180)
			(size 1.05 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 17 "/VB24N0B1")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.875 0 180)
			(size 1.05 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 66 "Net-(D6-A)")
			(pinfunction "A")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "CustomLibraries:MillMax-Socket-0327-0-15-15-34-27-10-0_NO-SILK"
		(layer "F.Cu")
		(at 207.404898 81.890413)
		(descr "0364-0-15-15-13-27-10-0-2")
		(tags "Connector")
		(property "Reference" "J11"
			(at -5.6896 -0.7874 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "0327-0-15-15-34-27-10-0"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" "kicad-embed://Mill Max catalog-0364-0-15-15-13-27-10-0.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "CN/CONTACT SKT .032 TO .046 PIN 30UIN GOLD CONTACT//10UIN GOLD BODY"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DigikeyPN" "ED90081-ND"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "TPN" "699-881-00 "
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "/BankPower2/")
		(sheetfile "BankPower.kicad_sch")
		(attr through_hole exclude_from_pos_files)
		(embedded_fonts no)
		(model "C:/InstalledPrograms/KiCADV5/KiCad/CustomLibraries/LIB_0364-0-15-15-13-27-10-0/0364-0-15-15-13-27-10-0/3D/0364-0-15-15-13-27-10-0.stp"
			(offset
				(xyz 0 0 0.635)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -0 -90 -0)
			)
		)
	)
	(footprint "CustomLibraries:MillMax-Socket-0327-0-15-15-34-27-10-0_NO-SILK"
		(layer "F.Cu")
		(at 208.930871 54.931698)
		(descr "0364-0-15-15-13-27-10-0-2")
		(tags "Connector")
		(property "Reference" "J21"
			(at -3.937 -0.2839 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "0327-0-15-15-34-27-10-0"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" "kicad-embed://Mill Max catalog-0364-0-15-15-13-27-10-0.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "CN/CONTACT SKT .032 TO .046 PIN 30UIN GOLD CONTACT//10UIN GOLD BODY"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DigikeyPN" "ED90081-ND"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "TPN" "699-881-00 "
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "/BankPower1/")
		(sheetfile "BankPower.kicad_sch")
		(attr through_hole exclude_from_pos_files)
		(embedded_fonts no)
		(model "C:/InstalledPrograms/KiCADV5/KiCad/CustomLibraries/LIB_0364-0-15-15-13-27-10-0/0364-0-15-15-13-27-10-0/3D/0364-0-15-15-13-27-10-0.stp"
			(offset
				(xyz 0 0 0.635)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -0 -90 -0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1206_3216Metric_Pad1.33x1.80mm_HandSolder"
		(layer "F.Cu")
		(at 262.294377 96.666332)
		(descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C11"
			(at 0.82874 -1.970332 0)
			(layer "F.SilkS")
		)
		(property "Value" "4.7UF/100VDC/1206"
			(at 0 1.85 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "CAP, CERAMIC 4.7UF 10% 100V X7S 1206"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MFGPN" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DigikeyPN" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "TPN" "698-396-00"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/15Vaux/")
		(sheetfile "15Vaux.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.5625 0)
			(size 1.325 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.188679)
			(net 3 "/VFF48P0_M1")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.5625 0)
			(size 1.325 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.188679)
			(net 76 "/48V_RTN_M1")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_Elec_10x10.2"
		(layer "F.Cu")
		(at 135.144098 95.953413 180)
		(descr "SMD capacitor, aluminum electrolytic nonpolar, 10.0x10.2mm")
		(tags "capacitor electrolyic nonpolar")
		(property "Reference" "C28"
			(at 6.9088 -3.6854 0)
			(layer "F.SilkS")
		)
		(property "Value" "120uF/63V/10x10"
			(at 0 6.2 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "CAP, ALUMINUM POLYMER 120UF 20% 63V RADIAL"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DigikeyPN" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "TPN" "701-721-00"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MFGPN" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "CP_*")
		(sheetname "/BankPower2/")
		(sheetfile "BankPower.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -4.4 0 180)
			(size 4.6 2.1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.119048)
			(net 50 "/VB96P0B2")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 4.4 0 180)
			(size 4.6 2.1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.119048)
			(net 10 "Net-(C24-Pad2)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_Elec_10x10.2.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_Elec_10x10.2"
		(layer "F.Cu")
		(at 145.0437 220.723 90)
		(descr "SMD capacitor, aluminum electrolytic nonpolar, 10.0x10.2mm")
		(tags "capacitor electrolyic nonpolar")
		(property "Reference" "C8"
			(at 6.997492 3.231402 90)
			(layer "F.SilkS")
		)
		(property "Value" "390uF/25V/10x10"
			(at 0 6.2 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "390UF 25V 20% ALUM ELECT"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DigikeyPN" "493-4544-1-ND"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "TPN" "131-516-13"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "CP_*")
		(sheetname "/12Vpower/")
		(sheetfile "12Vpower.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -4.4 0 90)
			(size 4.6 2.1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.119048)
			(net 7 "/VB12P6_GD")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 4.4 0 90)
			(size 4.6 2.1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.119048)
			(net 8 "/VB0P0_GD")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_Elec_10x10.2.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 219.722417 41.60119 -90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R22"
			(at 3.109157 -0.064025 90)
			(layer "F.SilkS")
		)
		(property "Value" "2k"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "TPN" "636-702-00"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/BankPower1/")
		(sheetfile "BankPower.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 270)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 36 "/15Vaux/VP15P0")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0 270)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 74 "Net-(SW1-B)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 218.400383 167.099288 -90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R25"
			(at 3.53495 -0.064025 90)
			(layer "F.SilkS")
		)
		(property "Value" "2k"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "TPN" "636-702-00"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/BankPower4/")
		(sheetfile "BankPower.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 270)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 36 "/15Vaux/VP15P0")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0 270)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 73 "Net-(SW4-B)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_Elec_10x10.2"
		(layer "F.Cu")
		(at 136.670071 53.602298 180)
		(descr "SMD capacitor, aluminum electrolytic nonpolar, 10.0x10.2mm")
		(tags "capacitor electrolyic nonpolar")
		(property "Reference" "C46"
			(at 6.9088 -3.6854 0)
			(layer "F.SilkS")
		)
		(property "Value" "120uF/63V/10x10"
			(at 0 6.2 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "CAP, ALUMINUM POLYMER 120UF 20% 63V RADIAL"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DigikeyPN" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "TPN" "701-721-00"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MFGPN" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "CP_*")
		(sheetname "/BankPower1/")
		(sheetfile "BankPower.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -4.4 0 180)
			(size 4.6 2.1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.119048)
			(net 13 "/VB96P0B1")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 4.4 0 180)
			(size 4.6 2.1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.119048)
			(net 37 "Net-(C42-Pad2)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_Elec_10x10.2.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "CustomLibraries:FUSC10030X305N"
		(layer "F.Cu")
		(at 247.433155 164.591177 -90)
		(property "Reference" "F3"
			(at 0.968393 3.020713 180)
			(layer "F.SilkS")
		)
		(property "Value" "0456030.ER"
			(at 3.195 3.465 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "FUSE 30A 125V FAST NANO2 SMD"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MAXIMUM_PACKAGE_HEIGHT" "3.05mm"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "CREATOR" "ANA"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "STANDARD" "IPC 7351B"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTREV" "GD. 08/24/21"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "VERIFIER" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER" "Littelfuse"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DigikeyPN" "F3345CT-ND"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "TPN" "603-301-00"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/48Vpower/")
		(sheetfile "48Vpower.kicad_sch")
		(attr smd)
		(pad "1" smd roundrect
			(at -4.365 0 270)
			(size 2.16 3.16)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.125)
			(net 64 "/V48P0")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd roundrect
			(at 4.365 0 270)
			(size 2.16 3.16)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.125)
			(net 4 "/48Vpower/VF48P0_DISA")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
		(model "C:/InstalledPrograms/KiCADV5/KiCad/CustomLibraries/0456030_ER/0456030.ER.step"
			(offset
				(xyz 0 -1.5748 1.524)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -0 -0 -0)
			)
		)
	)
	(footprint "LED_SMD:LED_0603_1608Metric_Pad1.05x0.95mm_HandSolder"
		(layer "F.Cu")
		(at 126.187053 226.843311)
		(descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
		(tags "LED handsolder")
		(property "Reference" "D1"
			(at -0.3372 1.5672 0)
			(layer "F.SilkS")
		)
		(property "Value" "LED"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "DIODES, GREEN, 2.4V, 40MCD,0603, 0.025AMPS, LIGHT EMITTING"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DigikeyPN" "350-2035-1-ND"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "TPN" "702-390-01"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MFGPN" "DIALIGHT CO  598-8070-107F"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "LED* LED_SMD:* LED_THT:*")
		(sheetname "/")
		(sheetfile "BenchPowerBoardNewCMchoke.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.875 0)
			(size 1.05 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 20 "Net-(D1-K)")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.875 0)
			(size 1.05 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 7 "/VB12P6_GD")
			(pinfunction "A")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "CustomLibraries:MillMax-Socket-0364-0-15-15-13-27-10-0"
		(layer "F.Cu")
		(at 169.5814 206.4455)
		(descr "0364-0-15-15-13-27-10-0-2")
		(tags "Connector")
		(property "Reference" "J7"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "0364-0-15-15-13-27-10-0"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" "kicad-embed://Mill Max catalog-0364-0-15-15-13-27-10-0.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "CN/CONTACT SKT .048 TO .064 PIN 30UIN GOLD CONTACT//10UIN GOLD BODY"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DigikeyPN" "ED90089-ND"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "TPN" "699-882-00 "
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "/12Vpower/")
		(sheetfile "12Vpower.kicad_sch")
		(attr through_hole exclude_from_pos_files)
		(embedded_fonts no)
		(model "C:/InstalledPrograms/KiCADV5/KiCad/CustomLibraries/LIB_0364-0-15-15-13-27-10-0/0364-0-15-15-13-27-10-0/3D/0364-0-15-15-13-27-10-0.stp"
			(offset
				(xyz 0 0 0.635)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -0 -90 -0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "F.Cu")
		(at 120.940262 116.535568 180)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R5"
			(at 2.921 -0.126 0)
			(layer "F.SilkS")
		)
		(property "Value" "22k"
			(at 0 1.65 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DigikeyPN" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "BenchPowerBoardNewCMchoke.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 180)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net 81 "Net-(D4-A)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 180)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net 59 "/VB0P0B3")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_Elec_10x10.2"
		(layer "F.Cu")
		(at 135.366355 179.056063 180)
		(descr "SMD capacitor, aluminum electrolytic nonpolar, 10.0x10.2mm")
		(tags "capacitor electrolyic nonpolar")
		(property "Reference" "C64"
			(at 6.9088 -3.6854 0)
			(layer "F.SilkS")
		)
		(property "Value" "120uF/63V/10x10"
			(at 0 6.2 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "CAP, ALUMINUM POLYMER 120UF 20% 63V RADIAL"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DigikeyPN" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "TPN" "701-721-00"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MFGPN" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "CP_*")
		(sheetname "/BankPower4/")
		(sheetfile "BankPower.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -4.4 0 180)
			(size 4.6 2.1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.119048)
			(net 25 "/VB96P0B4")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 4.4 0 180)
			(size 4.6 2.1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.119048)
			(net 78 "Net-(C60-Pad2)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_Elec_10x10.2.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MountingHole:MountingHole_3.5mm"
		(layer "F.Cu")
		(at 181.264227 115.145568)
		(descr "Mounting Hole 3.5mm, no annular")
		(tags "mounting hole 3.5mm no annular")
		(property "Reference" "H3"
			(at 0 -4.5 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "MountingHole"
			(at 0 4.5 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Mounting Hole without connection"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "MountingHole*")
		(sheetname "/")
		(sheetfile "BenchPowerBoardNewCMchoke.kicad_sch")
		(clearance 3.81)
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 3.5 3.5)
			(drill 3.5)
			(layers "*.Cu" "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "LED_SMD:LED_0603_1608Metric_Pad1.05x0.95mm_HandSolder"
		(layer "F.Cu")
		(at 140.680787 113.766566 90)
		(descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
		(tags "LED handsolder")
		(property "Reference" "D9"
			(at -0.303858 -1.524421 90)
			(layer "F.SilkS")
		)
		(property "Value" "LED"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Light emitting diode"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DigikeyPN" "350-2035-1-ND"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MFGPN" "DIALIGHT CO  598-8070-107F"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "LED* LED_SMD:* LED_THT:*")
		(sheetname "/")
		(sheetfile "BenchPowerBoardNewCMchoke.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.875 0 90)
			(size 1.05 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 68 "Net-(D9-K)")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.875 0 90)
			(size 1.05 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 50 "/VB96P0B2")
			(pinfunction "A")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_Elec_10x10.2"
		(layer "F.Cu")
		(at 121.587555 165.236513)
		(descr "SMD capacitor, aluminum electrolytic nonpolar, 10.0x10.2mm")
		(tags "capacitor electrolyic nonpolar")
		(property "Reference" "C72"
			(at 0.0508 6.246 0)
			(layer "F.SilkS")
		)
		(property "Value" "330uF/35V/10x10"
			(at 0 6.2 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "CAP, ALUMINUM POLYMER 330UF 20% 35V RADIAL"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DigikeyPN" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "TPN" "698-622-00"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MFGPN" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "CP_*")
		(sheetname "/BankPower4/")
		(sheetfile "BankPower.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -4.4 0)
			(size 4.6 2.1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.119048)
			(net 26 "/VB0P0B4")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 4.4 0)
			(size 4.6 2.1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.119048)
			(net 28 "/VB24N0B4")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_Elec_10x10.2.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "LED_SMD:LED_0603_1608Metric_Pad1.05x0.95mm_HandSolder"
		(layer "F.Cu")
		(at 140.168023 155.256608 90)
		(descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
		(tags "LED handsolder")
		(property "Reference" "D8"
			(at -0.293362 -1.458683 90)
			(layer "F.SilkS")
		)
		(property "Value" "LED"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Light emitting diode"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DigikeyPN" "350-2035-1-ND"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MFGPN" "DIALIGHT CO  598-8070-107F"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "LED* LED_SMD:* LED_THT:*")
		(sheetname "/")
		(sheetfile "BenchPowerBoardNewCMchoke.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.875 0 90)
			(size 1.05 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 82 "Net-(D8-K)")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.875 0 90)
			(size 1.05 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 58 "/VB96P0B3")
			(pinfunction "A")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "CustomLibraries:CS2600"
		(layer "F.Cu")
		(at 179.466871 52.315498 180)
		(property "Reference" "PS1"
			(at -39.016157 17.906623 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "CS2600"
			(at 0 1 180)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "kicad-embed://CS2600 Datasheet.pdf"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "DCDC/ CUSTOM ISOLATED FIXED RATIO 53V INPUT/98V OUTPUT"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "TPN" "680-436-00"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MFGPN" "CS2600"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/BankPower1/")
		(sheetfile "BankPower.kicad_sch")
		(attr exclude_from_pos_files)
		(fp_text user "Vstart"
			(at -33.643693 3.953824 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "EN"
			(at -34.387706 -3.804855 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "GND"
			(at 35.728515 11.193459 270)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "Vout-"
			(at 35.985733 4.378349 270)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "Vin-"
			(at -34.97565 12.522307 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "Vin+"
			(at -32.92892 -8.386835 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "Vou+"
			(at 35.715573 -5.040542 270)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "${REFERENCE}"
			(at 0 2.5 180)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at -29.464 -10.2362 180)
			(size 5.08 5.08)
			(drill 1.651)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "/VFF48P0_M1")
			(pinfunction "Vin+")
			(pintype "input")
		)
		(pad "2" thru_hole circle
			(at -29.464 -2.6162 180)
			(size 5.08 5.08)
			(drill 1.651)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 69 "/BankPower1/ENABLE")
			(pinfunction "ON/OFF")
			(pintype "input")
		)
		(pad "3" thru_hole circle
			(at -29.464 5.1562 180)
			(size 5.08 5.08)
			(drill 1.651)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 36 "/15Vaux/VP15P0")
			(pinfunction "VSTART")
			(pintype "input")
		)
		(pad "4" thru_hole circle
			(at -29.464 12.7762 180)
			(size 5.08 5.08)
			(drill 1.651)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 76 "/48V_RTN_M1")
			(pinfunction "Vin-")
			(pintype "input")
		)
		(pad "5" thru_hole circle
			(at 28.956 8.3058 180)
			(size 5.08 5.08)
			(drill 2.54)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 14 "/BankPower1/VBU0P0")
			(pinfunction "GND")
			(pintype "input")
		)
		(pad "6" thru_hole circle
			(at 28.956 0.6858 180)
			(size 5.08 5.08)
			(drill 2.54)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 16 "/BankPower1/VBU24P0")
			(pinfunction "Vout-")
			(pintype "input")
		)
		(pad "7" thru_hole circle
			(at 28.956 -6.9342 180)
			(size 5.08 5.08)
			(drill 2.54)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 12 "/BankPower1/VBU96P0")
			(pinfunction "Vout+")
			(pintype "input")
		)
		(embedded_fonts no)
	)
	(footprint "CustomLibraries:MillMax-Socket-0327-0-15-15-34-27-10-0_NO-SILK"
		(layer "F.Cu")
		(at 207.627155 164.993063)
		(descr "0364-0-15-15-13-27-10-0-2")
		(tags "Connector")
		(property "Reference" "J25"
			(at -5.6896 -0.7874 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "0327-0-15-15-34-27-10-0"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" "kicad-embed://Mill Max catalog-0364-0-15-15-13-27-10-0.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "CN/CONTACT SKT .032 TO .046 PIN 30UIN GOLD CONTACT//10UIN GOLD BODY"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DigikeyPN" "ED90081-ND"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "TPN" "699-881-00 "
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "/BankPower4/")
		(sheetfile "BankPower.kicad_sch")
		(attr through_hole exclude_from_pos_files)
		(embedded_fonts no)
		(model "C:/InstalledPrograms/KiCADV5/KiCad/CustomLibraries/LIB_0364-0-15-15-13-27-10-0/0364-0-15-15-13-27-10-0/3D/0364-0-15-15-13-27-10-0.stp"
			(offset
				(xyz 0 0 0.635)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -0 -90 -0)
			)
		)
	)
	(footprint "CustomLibraries:MillMax-Socket-0327-0-15-15-34-27-10-0_NO-SILK"
		(layer "F.Cu")
		(at 208.930871 47.159298)
		(descr "0364-0-15-15-13-27-10-0-2")
		(tags "Connector")
		(property "Reference" "J19"
			(at -4.826 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "0327-0-15-15-34-27-10-0"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" "kicad-embed://Mill Max catalog-0364-0-15-15-13-27-10-0.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "CN/CONTACT SKT .032 TO .046 PIN 30UIN GOLD CONTACT//10UIN GOLD BODY"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DigikeyPN" "ED90081-ND"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "TPN" "699-881-00 "
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "/BankPower1/")
		(sheetfile "BankPower.kicad_sch")
		(attr through_hole exclude_from_pos_files)
		(embedded_fonts no)
		(model "C:/InstalledPrograms/KiCADV5/KiCad/CustomLibraries/LIB_0364-0-15-15-13-27-10-0/0364-0-15-15-13-27-10-0/3D/0364-0-15-15-13-27-10-0.stp"
			(offset
				(xyz 0 0 0.635)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -0 -90 -0)
			)
		)
	)
	(footprint "CustomLibraries:EBE4120x030xxx"
		(layer "F.Cu")
		(at 194.9814 214.0655 180)
		(property "Reference" "PS5"
			(at 37.236208 10.564625 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "EBE4120N030N76"
			(at 0 1 180)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "\"C:\\Documentation\\Dragon\\Grogu\\ProtoBoards\\GroguModulePowerBoard\\Components\\EBE4120x030xxx.pdf\""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "DC-DC CONVERTER, 40-60VIN, 12.6VOUT, 40A. 480W, 1/8 BR"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "TPN" "636-038-00"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DigikeyPN" "2392-EBE4120N030N76-ND"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/12Vpower/")
		(sheetfile "12Vpower.kicad_sch")
		(attr exclude_from_pos_files)
		(fp_text user "EN"
			(at -33.278942 -2.001213 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "+Vout"
			(at 33.084466 -3.435571 270)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "-Vin"
			(at -30.520486 6.646245 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "Trim"
			(at 33.057885 3.364383 270)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "-Vout"
			(at 33.283378 14.248616 270)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "+Vin"
			(at -30.420432 -9.56135 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "${REFERENCE}"
			(at 0 2.5 180)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at -25.4 -7.62 180)
			(size 5.08 5.08)
			(drill 1.651)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "/12Vpower/VFFF48P0_PS11")
			(pinfunction "+INPUT")
			(pintype "input")
		)
		(pad "2" thru_hole circle
			(at -25.4 0 180)
			(size 5.08 5.08)
			(drill 1.651)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 18 "/12Vpower/C50P_VB12P6_GD_EN_L")
			(pinfunction "ON/OFF")
			(pintype "input")
		)
		(pad "3" thru_hole circle
			(at -25.4 7.62 180)
			(size 5.08 5.08)
			(drill 1.651)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "/12Vpower/48V_RTN_DISA")
			(pinfunction "-INPUT")
			(pintype "input")
		)
		(pad "4" thru_hole circle
			(at 25.4 7.62 180)
			(size 5.08 5.08)
			(drill 2.54)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "/12Vpower/VBU0P0_11_21")
			(pinfunction "_OUTPUT")
			(pintype "output")
		)
		(pad "6" thru_hole circle
			(at 25.4 0 180)
			(size 5.08 5.08)
			(drill 1.651)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 84 "Net-(J5-Pin_1)")
			(pinfunction "TRIM")
			(pintype "input")
		)
		(pad "8" thru_hole circle
			(at 25.4 -7.62 180)
			(size 5.08 5.08)
			(drill 2.54)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 11 "/12Vpower/VBU12P6_11_21")
			(pinfunction "+OUTPUT")
			(pintype "output")
		)
		(embedded_fonts no)
	)
	(footprint "Capacitor_SMD:C_Elec_10x10.2"
		(layer "F.Cu")
		(at 220.664293 149.946716 -90)
		(descr "SMD capacitor, aluminum electrolytic nonpolar, 10.0x10.2mm")
		(tags "capacitor electrolyic nonpolar")
		(property "Reference" "C79"
			(at 0 -6.2 90)
			(layer "F.SilkS")
		)
		(property "Value" "120uF/63V/10x10"
			(at 0 6.2 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "CAP, ALUMINUM POLYMER 120UF 20% 63V RADIAL"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DigikeyPN" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "TPN" "701-721-00"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MFGPN" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "CP_*")
		(sheetname "/BankPower3/")
		(sheetfile "BankPower.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 270)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -4.4 0 270)
			(size 4.6 2.1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.119048)
			(net 3 "/VFF48P0_M1")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 4.4 0 270)
			(size 4.6 2.1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.119048)
			(net 76 "/48V_RTN_M1")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_Elec_10x10.2.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_Elec_10x10.2"
		(layer "F.Cu")
		(at 220.572257 190.931591 -90)
		(descr "SMD capacitor, aluminum electrolytic nonpolar, 10.0x10.2mm")
		(tags "capacitor electrolyic nonpolar")
		(property "Reference" "C61"
			(at 0 -6.2 90)
			(layer "F.SilkS")
		)
		(property "Value" "120uF/63V/10x10"
			(at 0 6.2 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "CAP, ALUMINUM POLYMER 120UF 20% 63V RADIAL"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DigikeyPN" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "TPN" "701-721-00"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MFGPN" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "CP_*")
		(sheetname "/BankPower4/")
		(sheetfile "BankPower.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 270)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -4.4 0 270)
			(size 4.6 2.1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.119048)
			(net 3 "/VFF48P0_M1")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 4.4 0 270)
			(size 4.6 2.1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.119048)
			(net 76 "/48V_RTN_M1")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_Elec_10x10.2.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "CustomLibraries:MillMax-Socket-0364-0-15-15-13-27-10-0"
		(layer "F.Cu")
		(at 150.510871 59.249698 180)
		(descr "0364-0-15-15-13-27-10-0-2")
		(tags "Connector")
		(property "Reference" "J16"
			(at -3.8862 2.0066 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "0364-0-15-15-13-27-10-0"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" "kicad-embed://Mill Max catalog-0364-0-15-15-13-27-10-0.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "CN/CONTACT SKT .048 TO .064 PIN 30UIN GOLD CONTACT//10UIN GOLD BODY"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DigikeyPN" "ED90089-ND"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "TPN" "699-882-00 "
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "/BankPower1/")
		(sheetfile "BankPower.kicad_sch")
		(attr through_hole exclude_from_pos_files)
		(embedded_fonts no)
		(model "C:/InstalledPrograms/KiCADV5/KiCad/CustomLibraries/LIB_0364-0-15-15-13-27-10-0/0364-0-15-15-13-27-10-0/3D/0364-0-15-15-13-27-10-0.stp"
			(offset
				(xyz 0 0 0.635)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -0 -90 -0)
			)
		)
	)
	(footprint "CustomLibraries:MillMax-Socket-0364-0-15-15-13-27-10-0"
		(layer "F.Cu")
		(at 150.510871 44.009698)
		(descr "0364-0-15-15-13-27-10-0-2")
		(tags "Connector")
		(property "Reference" "J24"
			(at 1.07188 -3.4798 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "0364-0-15-15-13-27-10-0"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" "kicad-embed://Mill Max catalog-0364-0-15-15-13-27-10-0.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "CN/CONTACT SKT .048 TO .064 PIN 30UIN GOLD CONTACT//10UIN GOLD BODY"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DigikeyPN" "ED90089-ND"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "TPN" "699-882-00 "
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "/BankPower1/")
		(sheetfile "BankPower.kicad_sch")
		(attr through_hole exclude_from_pos_files)
		(embedded_fonts no)
		(model "C:/InstalledPrograms/KiCADV5/KiCad/CustomLibraries/LIB_0364-0-15-15-13-27-10-0/0364-0-15-15-13-27-10-0/3D/0364-0-15-15-13-27-10-0.stp"
			(offset
				(xyz 0 0 0.635)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -0 -90 -0)
			)
		)
	)
	(footprint "CustomLibraries:MillMax-Socket-0327-0-15-15-34-27-10-0_NO-SILK"
		(layer "F.Cu")
		(at 208.930871 39.539298)
		(descr "0364-0-15-15-13-27-10-0-2")
		(tags "Connector")
		(property "Reference" "J18"
			(at -5.6896 -0.7874 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "0327-0-15-15-34-27-10-0"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" "kicad-embed://Mill Max catalog-0364-0-15-15-13-27-10-0.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "CN/CONTACT SKT .032 TO .046 PIN 30UIN GOLD CONTACT//10UIN GOLD BODY"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DigikeyPN" "ED90081-ND"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "TPN" "699-881-00 "
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "/BankPower1/")
		(sheetfile "BankPower.kicad_sch")
		(attr through_hole exclude_from_pos_files)
		(embedded_fonts no)
		(model "C:/InstalledPrograms/KiCADV5/KiCad/CustomLibraries/LIB_0364-0-15-15-13-27-10-0/0364-0-15-15-13-27-10-0/3D/0364-0-15-15-13-27-10-0.stp"
			(offset
				(xyz 0 0 0.635)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -0 -90 -0)
			)
		)
	)
	(footprint "CustomLibraries:MillMax-Socket-0364-0-15-15-13-27-10-0"
		(layer "F.Cu")
		(at 149.207155 177.083463)
		(descr "0364-0-15-15-13-27-10-0-2")
		(tags "Connector")
		(property "Reference" "J27"
			(at 4.5974 1.6764 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "0364-0-15-15-13-27-10-0"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" "kicad-embed://Mill Max catalog-0364-0-15-15-13-27-10-0.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "CN/CONTACT SKT .048 TO .064 PIN 30UIN GOLD CONTACT//10UIN GOLD BODY"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DigikeyPN" "ED90089-ND"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "TPN" "699-882-00 "
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "/BankPower4/")
		(sheetfile "BankPower.kicad_sch")
		(attr through_hole exclude_from_pos_files)
		(embedded_fonts no)
		(model "C:/InstalledPrograms/KiCADV5/KiCad/CustomLibraries/LIB_0364-0-15-15-13-27-10-0/0364-0-15-15-13-27-10-0/3D/0364-0-15-15-13-27-10-0.stp"
			(offset
				(xyz 0 0 0.635)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -0 -90 -0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 256.011989 106.626846)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R11"
			(at 0 -1.43 0)
			(layer "F.SilkS")
		)
		(property "Value" "12.7k"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DigikeyPN" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "BenchPowerBoardNewCMchoke.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 75 "Net-(D11-K)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 76 "/48V_RTN_M1")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_Elec_10x10.2"
		(layer "F.Cu")
		(at 135.366355 136.945083 180)
		(descr "SMD capacitor, aluminum electrolytic nonpolar, 10.0x10.2mm")
		(tags "capacitor electrolyic nonpolar")
		(property "Reference" "C78"
			(at 6.9088 -3.6854 0)
			(layer "F.SilkS")
		)
		(property "Value" "120uF/63V/10x10"
			(at 0 6.2 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "CAP, ALUMINUM POLYMER 120UF 20% 63V RADIAL"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DigikeyPN" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "TPN" "701-721-00"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MFGPN" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "CP_*")
		(sheetname "/BankPower3/")
		(sheetfile "BankPower.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -4.4 0 180)
			(size 4.6 2.1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.119048)
			(net 58 "/VB96P0B3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 4.4 0 180)
			(size 4.6 2.1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.119048)
			(net 79 "Net-(C78-Pad2)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_Elec_10x10.2.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "CustomLibraries:MillMax-Socket-0327-0-15-15-34-27-10-0_NO-SILK"
		(layer "F.Cu")
		(at 207.627155 188.005463)
		(descr "0364-0-15-15-13-27-10-0-2")
		(tags "Connector")
		(property "Reference" "J22"
			(at -3.0226 2.413 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "0327-0-15-15-34-27-10-0"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" "kicad-embed://Mill Max catalog-0364-0-15-15-13-27-10-0.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "CN/CONTACT SKT .032 TO .046 PIN 30UIN GOLD CONTACT//10UIN GOLD BODY"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DigikeyPN" "ED90081-ND"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "TPN" "699-881-00 "
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "/BankPower4/")
		(sheetfile "BankPower.kicad_sch")
		(attr through_hole exclude_from_pos_files)
		(embedded_fonts no)
		(model "C:/InstalledPrograms/KiCADV5/KiCad/CustomLibraries/LIB_0364-0-15-15-13-27-10-0/0364-0-15-15-13-27-10-0/3D/0364-0-15-15-13-27-10-0.stp"
			(offset
				(xyz 0 0 0.635)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -0 -90 -0)
			)
		)
	)
	(footprint "MountingHole:MountingHole_3.5mm"
		(layer "F.Cu")
		(at 261.537387 221.323549)
		(descr "Mounting Hole 3.5mm, no annular")
		(tags "mounting hole 3.5mm no annular")
		(property "Reference" "H4"
			(at 0 -4.5 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "MountingHole"
			(at 0 4.5 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Mounting Hole without connection"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "MountingHole*")
		(sheetname "/")
		(sheetfile "BenchPowerBoardNewCMchoke.kicad_sch")
		(clearance 3.81)
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 3.5 3.5)
			(drill 3.5)
			(layers "*.Cu" "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "CustomLibraries:CM4440Z111R10"
		(layer "F.Cu")
		(at 134.881898 81.905613 180)
		(descr "CM4440Z111R-10-2")
		(tags "Inductor")
		(property "Reference" "FL1"
			(at 1.1736 -7.534 0)
			(layer "F.SilkS")
		)
		(property "Value" "CM4440Z111R_10"
			(at 0 0.213 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" "kicad-embed://cm4440z111r-10-datasheet.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "COMMON MODE CHOKES TRIPLE 110OHM 100MHZ 20A 0.001OHM DCR"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DigikeyPN" "240-CM4440Z111R-10CT-ND"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "TPN" "693-673-00"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "L* L_CommonMode*")
		(sheetname "/BankPower2/")
		(sheetfile "BankPower.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0.213 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -2.54 3.435 180)
			(size 2.03 5.08)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 57 "/BankPower2/VBU96P0")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 0 3.435 180)
			(size 2.03 5.08)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 55 "/BankPower2/VBU0P0")
			(pinfunction "2")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at 2.54 3.435 180)
			(size 2.03 5.08)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 56 "/BankPower2/VBU24P0")
			(pinfunction "3")
			(pintype "passive")
		)
		(pad "4" smd rect
			(at 2.54 -3.435 180)
			(size 2.03 5.08)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 54 "/VB24N0B2")
			(pinfunction "4")
			(pintype "passive")
		)
		(pad "5" smd rect
			(at 0 -3.435 180)
			(size 2.03 5.08)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 52 "/VB0P0B2")
			(pinfunction "5")
			(pintype "passive")
		)
		(pad "6" smd rect
			(at -2.54 -3.435 180)
			(size 2.03 5.08)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 50 "/VB96P0B2")
			(pinfunction "6")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "CM4440Z111R-10.stp"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
		(model "C:/InstalledPrograms/KiCADV5/KiCad/CustomLibraries/LIB_CM4440Z111R-10/CM4440Z111R-10/3D/CM4440Z111R-10.stp"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -0 -0 -0)
			)
		)
	)
	(footprint "CustomLibraries:MillMax-Socket-0364-0-15-15-13-27-10-0"
		(layer "F.Cu")
		(at 149.207155 127.352483)
		(descr "0364-0-15-15-13-27-10-0-2")
		(tags "Connector")
		(property "Reference" "J36"
			(at 1.07188 -3.4798 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "0364-0-15-15-13-27-10-0"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" "kicad-embed://Mill Max catalog-0364-0-15-15-13-27-10-0.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "CN/CONTACT SKT .048 TO .064 PIN 30UIN GOLD CONTACT//10UIN GOLD BODY"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DigikeyPN" "ED90089-ND"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "TPN" "699-882-00 "
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "/BankPower3/")
		(sheetfile "BankPower.kicad_sch")
		(attr through_hole exclude_from_pos_files)
		(embedded_fonts no)
		(model "C:/InstalledPrograms/KiCADV5/KiCad/CustomLibraries/LIB_0364-0-15-15-13-27-10-0/0364-0-15-15-13-27-10-0/3D/0364-0-15-15-13-27-10-0.stp"
			(offset
				(xyz 0 0 0.635)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -0 -90 -0)
			)
		)
	)
	(footprint "CustomLibraries:MPT-02-6.30-XX-X-V"
		(layer "F.Cu")
		(at 254.691286 149.87196 180)
		(descr "VERTICAL POWER TERMINAL.")
		(property "Reference" "U1"
			(at 11.71077 -1.869244 0)
			(layer "F.SilkS")
		)
		(property "Value" "MPT-02-6.30-XX-X-V"
			(at 8.39218 8.027085 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://mm.digikey.com/Volume0/opasdata/d220001/medias/docus/6129/mpt-xx-6.30-xx-x-v-xx-mkt.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "SAMTEC  5.00 mm PowerStrip™/30 A Dual Blade Terminal Strip"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MFGPN" "MPT-02-6.30-03-L-V"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Digikey" "SAM12731-ND"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "BenchPowerBoardNewCMchoke.kicad_sch")
		(attr through_hole)
		(pad "" np_thru_hole circle
			(at -6.31 -2.15 180)
			(size 1.19 1.19)
			(drill 1.19)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 6.31 -2.15 180)
			(size 1.19 1.19)
			(drill 1.19)
			(layers "*.Cu" "*.Mask")
		)
		(pad "P1-1" thru_hole circle
			(at 3.44 2.54 180)
			(size 1.5 1.5)
			(drill 1.04)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 64 "/V48P0")
			(pinfunction "1")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "P1-2" thru_hole circle
			(at 3.44 0 180)
			(size 1.5 1.5)
			(drill 1.04)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 64 "/V48P0")
			(pinfunction "2")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "P1-3" thru_hole circle
			(at 3.44 -2.54 180)
			(size 1.5 1.5)
			(drill 1.04)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 64 "/V48P0")
			(pinfunction "3")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "P1-4" thru_hole circle
			(at 1.56 2.54 180)
			(size 1.5 1.5)
			(drill 1.04)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 64 "/V48P0")
			(pinfunction "4")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "P1-5" thru_hole circle
			(at 1.56 0 180)
			(size 1.5 1.5)
			(drill 1.04)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 64 "/V48P0")
			(pinfunction "5")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "P1-6" thru_hole circle
			(at 1.56 -2.54 180)
			(size 1.5 1.5)
			(drill 1.04)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 64 "/V48P0")
			(pinfunction "6")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "P2-1" thru_hole circle
			(at -1.56 2.54 180)
			(size 1.5 1.5)
			(drill 1.04)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 77 "/48V_RTN")
			(pinfunction "7")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "P2-2" thru_hole circle
			(at -1.56 0 180)
			(size 1.5 1.5)
			(drill 1.04)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 77 "/48V_RTN")
			(pinfunction "8")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "P2-3" thru_hole circle
			(at -1.56 -2.54 180)
			(size 1.5 1.5)
			(drill 1.04)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 77 "/48V_RTN")
			(pinfunction "9")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "P2-4" thru_hole circle
			(at -3.44 2.54 180)
			(size 1.5 1.5)
			(drill 1.04)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 77 "/48V_RTN")
			(pinfunction "10")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "P2-5" thru_hole circle
			(at -3.44 0 180)
			(size 1.5 1.5)
			(drill 1.04)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 77 "/48V_RTN")
			(pinfunction "11")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "P2-6" thru_hole circle
			(at -3.44 -2.54 180)
			(size 1.5 1.5)
			(drill 1.04)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 77 "/48V_RTN")
			(pinfunction "12")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
		(model "C:/InstalledPrograms/KiCADV5/KiCad/CustomLibraries/MPT_02_6_30_03_L_V/MPT-02-6.30-XX-X-V.step"
			(offset
				(xyz 0 6.2484 10.16)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -0 -0 -0)
			)
		)
	)
	(footprint "CustomLibraries:ToggleSwitch-TE-2267078-1"
		(layer "F.Cu")
		(at 225.925417 45.264557 90)
		(property "Reference" "SW1"
			(at -7.043121 0.107439 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "TE CONNECTIVITY 	2267078-1"
			(at 0 1 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Single Pole Single Throw (SPST) switch"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DigikeyPN" "450-2110-ND"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MFGPN" "2267078-1"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "TPN" "666-036-12"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Field8" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/BankPower1/")
		(sheetfile "BankPower.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 2.5 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at -2.54 0 90)
			(size 2.54 2.54)
			(drill 1.0922)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 69 "/BankPower1/ENABLE")
			(pinfunction "A")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 2.54 0 90)
			(size 2.54 2.54)
			(drill 1.0922)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 74 "Net-(SW1-B)")
			(pinfunction "B")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "C:/InstalledPrograms/KiCADV5/KiCad/Custom3DModels/ENG_CVM_CVM_2267078-1_A1.3d_stp/c-2267078-1-a1-3d.stp"
			(offset
				(xyz 0 0 21.59)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -0 -0 -90)
			)
		)
	)
	(footprint "LED_SMD:LED_0603_1608Metric_Pad1.05x0.95mm_HandSolder"
		(layer "F.Cu")
		(at 124.55718 158.519711 180)
		(descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
		(tags "LED handsolder")
		(property "Reference" "D3"
			(at -0.382854 2.01804 0)
			(layer "F.SilkS")
		)
		(property "Value" "LED"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Light emitting diode"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DigikeyPN" "350-2035-1-ND"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MFGPN" "DIALIGHT CO  598-8070-107F"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "LED* LED_SMD:* LED_THT:*")
		(sheetname "/")
		(sheetfile "BenchPowerBoardNewCMchoke.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.875 0 180)
			(size 1.05 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 28 "/VB24N0B4")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.875 0 180)
			(size 1.05 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 80 "Net-(D3-A)")
			(pinfunction "A")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_Elec_10x10.2"
		(layer "F.Cu")
		(at 245.096413 213.327372 90)
		(descr "SMD capacitor, aluminum electrolytic nonpolar, 10.0x10.2mm")
		(tags "capacitor electrolyic nonpolar")
		(property "Reference" "C22"
			(at -0.967625 6.679442 90)
			(layer "F.SilkS")
		)
		(property "Value" "100uF/63V"
			(at 0 6.2 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Polarized capacitor, US symbol"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DigikeyPN" "493-6185-1-ND"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "TPN" "131-516-00"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "CP_*")
		(sheetname "/48Vpower/")
		(sheetfile "48Vpower.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -4.4 0 90)
			(size 4.6 2.1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.119048)
			(net 9 "/12Vpower/VFF48P0_DISA")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 4.4 0 90)
			(size 4.6 2.1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.119048)
			(net 1 "/12Vpower/48V_RTN_DISA")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_Elec_10x10.2.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "CustomLibraries:CM4440Z111R10"
		(layer "F.Cu")
		(at 135.104155 122.897283 180)
		(descr "CM4440Z111R-10-2")
		(tags "Inductor")
		(property "Reference" "FL4"
			(at 1.1736 -7.534 0)
			(layer "F.SilkS")
		)
		(property "Value" "CM4440Z111R_10"
			(at 0 0.213 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" "kicad-embed://cm4440z111r-10-datasheet.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "COMMON MODE CHOKES TRIPLE 110OHM 100MHZ 20A 0.001OHM DCR"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DigikeyPN" "240-CM4440Z111R-10CT-ND"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "TPN" "693-673-00"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "L* L_CommonMode*")
		(sheetname "/BankPower3/")
		(sheetfile "BankPower.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0.213 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -2.54 3.435 180)
			(size 2.03 5.08)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 63 "/BankPower3/VBU96P0")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 0 3.435 180)
			(size 2.03 5.08)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 61 "/BankPower3/VBU0P0")
			(pinfunction "2")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at 2.54 3.435 180)
			(size 2.03 5.08)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 62 "/BankPower3/VBU24P0")
			(pinfunction "3")
			(pintype "passive")
		)
		(pad "4" smd rect
			(at 2.54 -3.435 180)
			(size 2.03 5.08)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 60 "/VB24N0B3")
			(pinfunction "4")
			(pintype "passive")
		)
		(pad "5" smd rect
			(at 0 -3.435 180)
			(size 2.03 5.08)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 59 "/VB0P0B3")
			(pinfunction "5")
			(pintype "passive")
		)
		(pad "6" smd rect
			(at -2.54 -3.435 180)
			(size 2.03 5.08)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 58 "/VB96P0B3")
			(pinfunction "6")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "CM4440Z111R-10.stp"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
		(model "C:/InstalledPrograms/KiCADV5/KiCad/CustomLibraries/LIB_CM4440Z111R-10/CM4440Z111R-10/3D/CM4440Z111R-10.stp"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -0 -0 -0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "F.Cu")
		(at 120.666271 33.128698 180)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R9"
			(at 3.2932 -0.126 0)
			(layer "F.SilkS")
		)
		(property "Value" "22k"
			(at 0 1.65 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DigikeyPN" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "BenchPowerBoardNewCMchoke.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 180)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net 66 "Net-(D6-A)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 180)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net 15 "/VB0P0B1")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_Elec_10x10.2"
		(layer "F.Cu")
		(at 230.202008 120.679064 -90)
		(descr "SMD capacitor, aluminum electrolytic nonpolar, 10.0x10.2mm")
		(tags "capacitor electrolyic nonpolar")
		(property "Reference" "C19"
			(at -6.657297 -4.800225 0)
			(layer "F.SilkS")
		)
		(property "Value" "100uF/63V"
			(at 0 6.2 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Polarized capacitor, US symbol"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DigikeyPN" "493-6185-1-ND"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "TPN" "131-516-00"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "CP_*")
		(sheetname "/48Vpower/")
		(sheetfile "48Vpower.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -4.4 0 270)
			(size 4.6 2.1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.119048)
			(net 3 "/VFF48P0_M1")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 4.4 0 270)
			(size 4.6 2.1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.119048)
			(net 76 "/48V_RTN_M1")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_Elec_10x10.2.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "F.Cu")
		(at 251.517601 97.205454 180)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C16"
			(at 3.372213 -0.032066 0)
			(layer "F.SilkS")
		)
		(property "Value" "4.7uF/25V/0805"
			(at 0 1.68 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "CAP 4.7UF 10% 25V 0805 X7R"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DigikeyPN" "399-C0805C475K3RACTUCT-ND"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "TPN" "111-815-05"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MFGPN" "KEMET ELECTRONICS CORP  C0805C475K3RACTU"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/15Vaux/")
		(sheetfile "15Vaux.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.0375 0 180)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 36 "/15Vaux/VP15P0")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.0375 0 180)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 76 "/48V_RTN_M1")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_Elec_10x10.2"
		(layer "F.Cu")
		(at 136.664071 64.603298 180)
		(descr "SMD capacitor, aluminum electrolytic nonpolar, 10.0x10.2mm")
		(tags "capacitor electrolyic nonpolar")
		(property "Reference" "C42"
			(at 7.112 -3.66 0)
			(layer "F.SilkS")
		)
		(property "Value" "120uF/63V/10x10"
			(at 0 6.2 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "CAP, ALUMINUM POLYMER 120UF 20% 63V RADIAL"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DigikeyPN" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "TPN" "701-721-00"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MFGPN" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "CP_*")
		(sheetname "/BankPower1/")
		(sheetfile "BankPower.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -4.4 0 180)
			(size 4.6 2.1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.119048)
			(net 13 "/VB96P0B1")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 4.4 0 180)
			(size 4.6 2.1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.119048)
			(net 37 "Net-(C42-Pad2)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_Elec_10x10.2.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_Elec_10x10.2"
		(layer "F.Cu")
		(at 221.283471 66.375751 -90)
		(descr "SMD capacitor, aluminum electrolytic nonpolar, 10.0x10.2mm")
		(tags "capacitor electrolyic nonpolar")
		(property "Reference" "C43"
			(at 0 -6.2 90)
			(layer "F.SilkS")
		)
		(property "Value" "120uF/63V/10x10"
			(at 0 6.2 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "CAP, ALUMINUM POLYMER 120UF 20% 63V RADIAL"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DigikeyPN" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "TPN" "701-721-00"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MFGPN" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "CP_*")
		(sheetname "/BankPower1/")
		(sheetfile "BankPower.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -4.4 0 270)
			(size 4.6 2.1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.119048)
			(net 3 "/VFF48P0_M1")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 4.4 0 270)
			(size 4.6 2.1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.119048)
			(net 76 "/48V_RTN_M1")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_Elec_10x10.2.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_Elec_10x10.2"
		(layer "F.Cu")
		(at 121.587555 123.125533)
		(descr "SMD capacitor, aluminum electrolytic nonpolar, 10.0x10.2mm")
		(tags "capacitor electrolyic nonpolar")
		(property "Reference" "C90"
			(at 0.0508 6.246 0)
			(layer "F.SilkS")
		)
		(property "Value" "330uF/35V/10x10"
			(at 0 6.2 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "CAP, ALUMINUM POLYMER 330UF 20% 35V RADIAL"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DigikeyPN" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "TPN" "698-622-00"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MFGPN" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "CP_*")
		(sheetname "/BankPower3/")
		(sheetfile "BankPower.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -4.4 0)
			(size 4.6 2.1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.119048)
			(net 59 "/VB0P0B3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 4.4 0)
			(size 4.6 2.1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.119048)
			(net 60 "/VB24N0B3")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_Elec_10x10.2.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_Elec_10x10.2"
		(layer "F.Cu")
		(at 135.360355 190.057063 180)
		(descr "SMD capacitor, aluminum electrolytic nonpolar, 10.0x10.2mm")
		(tags "capacitor electrolyic nonpolar")
		(property "Reference" "C60"
			(at 7.112 -3.66 0)
			(layer "F.SilkS")
		)
		(property "Value" "120uF/63V/10x10"
			(at 0 6.2 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "CAP, ALUMINUM POLYMER 120UF 20% 63V RADIAL"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DigikeyPN" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "TPN" "701-721-00"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MFGPN" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "CP_*")
		(sheetname "/BankPower4/")
		(sheetfile "BankPower.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -4.4 0 180)
			(size 4.6 2.1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.119048)
			(net 25 "/VB96P0B4")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 4.4 0 180)
			(size 4.6 2.1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.119048)
			(net 78 "Net-(C60-Pad2)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_Elec_10x10.2.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "F.Cu")
		(at 120.99814 158.557111 180)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R3"
			(at 3.143801 -0.16261 0)
			(layer "F.SilkS")
		)
		(property "Value" "22k"
			(at 0 1.65 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DigikeyPN" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "BenchPowerBoardNewCMchoke.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 180)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net 80 "Net-(D3-A)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 180)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net 26 "/VB0P0B4")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "CustomLibraries:FUSC10030X305N"
		(layer "F.Cu")
		(at 253.466646 140.214749)
		(property "Reference" "F2"
			(at -0.10369 -2.917702 0)
			(layer "F.SilkS")
		)
		(property "Value" "0456030.ER"
			(at 3.195 3.465 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "FUSE 30A 125V FAST NANO2 SMD"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MAXIMUM_PACKAGE_HEIGHT" "3.05mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "CREATOR" "ANA"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "STANDARD" "IPC 7351B"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTREV" "GD. 08/24/21"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "VERIFIER" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER" "Littelfuse"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DigikeyPN" "F3345CT-ND"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "TPN" "603-301-00"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/48Vpower/")
		(sheetfile "48Vpower.kicad_sch")
		(attr smd)
		(pad "1" smd roundrect
			(at -4.365 0)
			(size 2.16 3.16)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.125)
			(net 64 "/V48P0")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd roundrect
			(at 4.365 0)
			(size 2.16 3.16)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.125)
			(net 2 "/48Vpower/VF48P0_BRD")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
		(model "C:/InstalledPrograms/KiCADV5/KiCad/CustomLibraries/0456030_ER/0456030.ER.step"
			(offset
				(xyz 0 -1.5748 1.524)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -0 -0 -0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "F.Cu")
		(at 119.277206 75.593219 180)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R7"
			(at 3.159668 -0.138942 0)
			(layer "F.SilkS")
		)
		(property "Value" "22k"
			(at 0 1.65 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DigikeyPN" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "BenchPowerBoardNewCMchoke.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 180)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net 65 "Net-(D5-A)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 180)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net 52 "/VB0P0B2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "LED_SMD:LED_0603_1608Metric_Pad1.05x0.95mm_HandSolder"
		(layer "F.Cu")
		(at 251.859174 106.618561 180)
		(descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
		(tags "LED handsolder")
		(property "Reference" "D11"
			(at 0 -1.43 0)
			(layer "F.SilkS")
		)
		(property "Value" "LED"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "DIODES, GREEN, 2.4V, 40MCD,0603, 0.025AMPS, LIGHT EMITTING"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DigikeyPN" "350-2035-1-ND"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MFGPN" "DIALIGHT CO  598-8070-107F"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "TPN" "702-390-01"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "LED* LED_SMD:* LED_THT:*")
		(sheetname "/")
		(sheetfile "BenchPowerBoardNewCMchoke.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.875 0 180)
			(size 1.05 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 75 "Net-(D11-K)")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.875 0 180)
			(size 1.05 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 36 "/15Vaux/VP15P0")
			(pinfunction "A")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "CustomLibraries:MillMax-Socket-0327-0-15-15-34-27-10-0_NO-SILK"
		(layer "F.Cu")
		(at 207.627155 138.274483)
		(descr "0364-0-15-15-13-27-10-0-2")
		(tags "Connector")
		(property "Reference" "J35"
			(at -3.937 -0.2839 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "0327-0-15-15-34-27-10-0"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" "kicad-embed://Mill Max catalog-0364-0-15-15-13-27-10-0.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "CN/CONTACT SKT .032 TO .046 PIN 30UIN GOLD CONTACT//10UIN GOLD BODY"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DigikeyPN" "ED90081-ND"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "TPN" "699-881-00 "
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "/BankPower3/")
		(sheetfile "BankPower.kicad_sch")
		(attr through_hole exclude_from_pos_files)
		(embedded_fonts no)
		(model "C:/InstalledPrograms/KiCADV5/KiCad/CustomLibraries/LIB_0364-0-15-15-13-27-10-0/0364-0-15-15-13-27-10-0/3D/0364-0-15-15-13-27-10-0.stp"
			(offset
				(xyz 0 0 0.635)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -0 -90 -0)
			)
		)
	)
	(footprint "CustomLibraries:MillMax-Socket-0327-0-15-15-34-27-10-0_NO-SILK"
		(layer "F.Cu")
		(at 208.930871 62.551698)
		(descr "0364-0-15-15-13-27-10-0-2")
		(tags "Connector")
		(property "Reference" "J15"
			(at -3.0226 2.413 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "0327-0-15-15-34-27-10-0"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" "kicad-embed://Mill Max catalog-0364-0-15-15-13-27-10-0.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "CN/CONTACT SKT .032 TO .046 PIN 30UIN GOLD CONTACT//10UIN GOLD BODY"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DigikeyPN" "ED90081-ND"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "TPN" "699-881-00 "
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "/BankPower1/")
		(sheetfile "BankPower.kicad_sch")
		(attr through_hole exclude_from_pos_files)
		(embedded_fonts no)
		(model "C:/InstalledPrograms/KiCADV5/KiCad/CustomLibraries/LIB_0364-0-15-15-13-27-10-0/0364-0-15-15-13-27-10-0/3D/0364-0-15-15-13-27-10-0.stp"
			(offset
				(xyz 0 0 0.635)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -0 -90 -0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_Elec_10x10.2"
		(layer "F.Cu")
		(at 121.097555 190.039063 180)
		(descr "SMD capacitor, aluminum electrolytic nonpolar, 10.0x10.2mm")
		(tags "capacitor electrolyic nonpolar")
		(property "Reference" "C67"
			(at 7.1882 -3.1012 0)
			(layer "F.SilkS")
		)
		(property "Value" "120uF/63V/10x10"
			(at 0 6.2 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "CAP, ALUMINUM POLYMER 120UF 20% 63V RADIAL"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DigikeyPN" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "TPN" "701-721-00"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MFGPN" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "CP_*")
		(sheetname "/BankPower4/")
		(sheetfile "BankPower.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -4.4 0 180)
			(size 4.6 2.1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.119048)
			(net 78 "Net-(C60-Pad2)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 4.4 0 180)
			(size 4.6 2.1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.119048)
			(net 26 "/VB0P0B4")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_Elec_10x10.2.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_Elec_10x10.2"
		(layer "F.Cu")
		(at 120.875298 106.936413 180)
		(descr "SMD capacitor, aluminum electrolytic nonpolar, 10.0x10.2mm")
		(tags "capacitor electrolyic nonpolar")
		(property "Reference" "C33"
			(at 7.1882 -3.1012 0)
			(layer "F.SilkS")
		)
		(property "Value" "120uF/63V/10x10"
			(at 0 6.2 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "CAP, ALUMINUM POLYMER 120UF 20% 63V RADIAL"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DigikeyPN" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "TPN" "701-721-00"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MFGPN" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "CP_*")
		(sheetname "/BankPower2/")
		(sheetfile "BankPower.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -4.4 0 180)
			(size 4.6 2.1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.119048)
			(net 10 "Net-(C24-Pad2)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 4.4 0 180)
			(size 4.6 2.1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.119048)
			(net 52 "/VB0P0B2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_Elec_10x10.2.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MountingHole:MountingHole_3.5mm"
		(layer "F.Cu")
		(at 88.689722 38.224087)
		(descr "Mounting Hole 3.5mm, no annular")
		(tags "mounting hole 3.5mm no annular")
		(property "Reference" "H2"
			(at 0 -4.5 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "MountingHole"
			(at 0 4.5 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Mounting Hole without connection"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "MountingHole*")
		(sheetname "/")
		(sheetfile "BenchPowerBoardNewCMchoke.kicad_sch")
		(clearance 3.81)
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 3.5 3.5)
			(drill 3.5)
			(layers "*.Cu" "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 259.941105 93.386025 180)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R13"
			(at -0.07512 1.589852 0)
			(layer "F.SilkS")
		)
		(property "Value" "0"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "RES 14K 1% 100PPM 0.1W 0603"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "TPN" "636-000-00"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/15Vaux/")
		(sheetfile "15Vaux.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 180)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 3 "/VFF48P0_M1")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0 180)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 24 "Net-(U2-EN)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "CustomLibraries:CS2600"
		(layer "F.Cu")
		(at 178.163155 135.658283 180)
		(property "Reference" "PS3"
			(at -39.038554 16.54519 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "CS2600"
			(at 0 1 180)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "kicad-embed://CS2600 Datasheet.pdf"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "DCDC/ CUSTOM ISOLATED FIXED RATIO 53V INPUT/98V OUTPUT"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "TPN" "680-436-00"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MFGPN" "CS2600"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/BankPower3/")
		(sheetfile "BankPower.kicad_sch")
		(attr exclude_from_pos_files)
		(fp_text user "Vin-"
			(at -35.076965 11.445486 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "Vou+"
			(at 35.841029 -5.898806 270)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "Vout-"
			(at 35.390353 4.083225 270)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "Vin+"
			(at -33.134452 -9.040025 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "Vstart"
			(at -34.922261 6.76975 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "EN"
			(at -34.475968 -3.209219 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "GND"
			(at 35.420987 11.335009 270)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "${REFERENCE}"
			(at 0 2.5 180)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at -29.464 -10.2362 180)
			(size 5.08 5.08)
			(drill 1.651)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "/VFF48P0_M1")
			(pinfunction "Vin+")
			(pintype "input")
		)
		(pad "2" thru_hole circle
			(at -29.464 -2.6162 180)
			(size 5.08 5.08)
			(drill 1.651)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 72 "/BankPower3/ENABLE")
			(pinfunction "ON/OFF")
			(pintype "input")
		)
		(pad "3" thru_hole circle
			(at -29.464 5.1562 180)
			(size 5.08 5.08)
			(drill 1.651)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 36 "/15Vaux/VP15P0")
			(pinfunction "VSTART")
			(pintype "input")
		)
		(pad "4" thru_hole circle
			(at -29.464 12.7762 180)
			(size 5.08 5.08)
			(drill 1.651)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 76 "/48V_RTN_M1")
			(pinfunction "Vin-")
			(pintype "input")
		)
		(pad "5" thru_hole circle
			(at 28.956 8.3058 180)
			(size 5.08 5.08)
			(drill 2.54)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 61 "/BankPower3/VBU0P0")
			(pinfunction "GND")
			(pintype "input")
		)
		(pad "6" thru_hole circle
			(at 28.956 0.6858 180)
			(size 5.08 5.08)
			(drill 2.54)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 62 "/BankPower3/VBU24P0")
			(pinfunction "Vout-")
			(pintype "input")
		)
		(pad "7" thru_hole circle
			(at 28.956 -6.9342 180)
			(size 5.08 5.08)
			(drill 2.54)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 63 "/BankPower3/VBU96P0")
			(pinfunction "Vout+")
			(pintype "input")
		)
		(embedded_fonts no)
	)
	(footprint "CustomLibraries:CS2600"
		(layer "F.Cu")
		(at 178.163155 177.769263 180)
		(property "Reference" "PS4"
			(at -39.56333 17.054859 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "CS2600"
			(at 0 1 180)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "kicad-embed://CS2600 Datasheet.pdf"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "DCDC/ CUSTOM ISOLATED FIXED RATIO 53V INPUT/98V OUTPUT"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "TPN" "680-436-00"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MFGPN" "CS2600"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/BankPower4/")
		(sheetfile "BankPower.kicad_sch")
		(attr exclude_from_pos_files)
		(fp_text user "Vstart"
			(at -34.10505 2.964201 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "GND"
			(at 35.208091 11.335009 270)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "Vout-"
			(at 35.177457 4.083225 270)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "Vin+"
			(at -33.563963 -7.836404 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "Vin-"
			(at -33.911765 12.722867 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "EN"
			(at -34.774011 -2.229881 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "Vou+"
			(at 35.486201 -4.976253 270)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "${REFERENCE}"
			(at 0 2.5 180)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at -29.464 -10.2362 180)
			(size 5.08 5.08)
			(drill 1.651)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "/VFF48P0_M1")
			(pinfunction "Vin+")
			(pintype "input")
		)
		(pad "2" thru_hole circle
			(at -29.464 -2.6162 180)
			(size 5.08 5.08)
			(drill 1.651)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 70 "/BankPower4/ENABLE")
			(pinfunction "ON/OFF")
			(pintype "input")
		)
		(pad "3" thru_hole circle
			(at -29.464 5.1562 180)
			(size 5.08 5.08)
			(drill 1.651)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 36 "/15Vaux/VP15P0")
			(pinfunction "VSTART")
			(pintype "input")
		)
		(pad "4" thru_hole circle
			(at -29.464 12.7762 180)
			(size 5.08 5.08)
			(drill 1.651)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 76 "/48V_RTN_M1")
			(pinfunction "Vin-")
			(pintype "input")
		)
		(pad "5" thru_hole circle
			(at 28.956 8.3058 180)
			(size 5.08 5.08)
			(drill 2.54)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 51 "/BankPower4/VBU0P0")
			(pinfunction "GND")
			(pintype "input")
		)
		(pad "6" thru_hole circle
			(at 28.956 0.6858 180)
			(size 5.08 5.08)
			(drill 2.54)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 53 "/BankPower4/VBU24P0")
			(pinfunction "Vout-")
			(pintype "input")
		)
		(pad "7" thru_hole circle
			(at 28.956 -6.9342 180)
			(size 5.08 5.08)
			(drill 2.54)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 19 "/BankPower4/VBU96P0")
			(pinfunction "Vout+")
			(pintype "input")
		)
		(embedded_fonts no)
	)
	(footprint "CustomLibraries:MillMax-Socket-0327-0-15-15-34-27-10-0_NO-SILK"
		(layer "F.Cu")
		(at 207.404898 97.282813)
		(descr "0364-0-15-15-13-27-10-0-2")
		(tags "Connector")
		(property "Reference" "J14"
			(at -3.937 -0.2839 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "0327-0-15-15-34-27-10-0"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" "kicad-embed://Mill Max catalog-0364-0-15-15-13-27-10-0.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "CN/CONTACT SKT .032 TO .046 PIN 30UIN GOLD CONTACT//10UIN GOLD BODY"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DigikeyPN" "ED90081-ND"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "TPN" "699-881-00 "
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "/BankPower2/")
		(sheetfile "BankPower.kicad_sch")
		(attr through_hole exclude_from_pos_files)
		(embedded_fonts no)
		(model "C:/InstalledPrograms/KiCADV5/KiCad/CustomLibraries/LIB_0364-0-15-15-13-27-10-0/0364-0-15-15-13-27-10-0/3D/0364-0-15-15-13-27-10-0.stp"
			(offset
				(xyz 0 0 0.635)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -0 -90 -0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_Elec_10x10.2"
		(layer "F.Cu")
		(at 233.5972 213.454 90)
		(descr "SMD capacitor, aluminum electrolytic nonpolar, 10.0x10.2mm")
		(tags "capacitor electrolyic nonpolar")
		(property "Reference" "C9"
			(at -6.604 -2.5932 90)
			(layer "F.SilkS")
		)
		(property "Value" "120uF/63V/10x10"
			(at 0 6.2 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "CAP, ALUMINUM POLYMER 120UF 20% 63V RADIAL"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DigikeyPN" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "TPN" "701-721-00"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MFGPN" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "CP_*")
		(sheetname "/12Vpower/")
		(sheetfile "12Vpower.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -4.4 0 90)
			(size 4.6 2.1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.119048)
			(net 5 "/12Vpower/VFFF48P0_PS11")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 4.4 0 90)
			(size 4.6 2.1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.119048)
			(net 1 "/12Vpower/48V_RTN_DISA")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_Elec_10x10.2.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_Elec_10x10.2"
		(layer "F.Cu")
		(at 219.58026 107.564483 -90)
		(descr "SMD capacitor, aluminum electrolytic nonpolar, 10.0x10.2mm")
		(tags "capacitor electrolyic nonpolar")
		(property "Reference" "C25"
			(at 0 -6.2 90)
			(layer "F.SilkS")
		)
		(property "Value" "120uF/63V/10x10"
			(at 0 6.2 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "CAP, ALUMINUM POLYMER 120UF 20% 63V RADIAL"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DigikeyPN" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "TPN" "701-721-00"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MFGPN" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "CP_*")
		(sheetname "/BankPower2/")
		(sheetfile "BankPower.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 270)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -4.4 0 270)
			(size 4.6 2.1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.119048)
			(net 3 "/VFF48P0_M1")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 4.4 0 270)
			(size 4.6 2.1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.119048)
			(net 76 "/48V_RTN_M1")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_Elec_10x10.2.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_Elec_10x10.2"
		(layer "F.Cu")
		(at 121.365298 82.133863)
		(descr "SMD capacitor, aluminum electrolytic nonpolar, 10.0x10.2mm")
		(tags "capacitor electrolyic nonpolar")
		(property "Reference" "C36"
			(at 0.0508 6.246 0)
			(layer "F.SilkS")
		)
		(property "Value" "330uF/35V/10x10"
			(at 0 6.2 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "CAP, ALUMINUM POLYMER 330UF 20% 35V RADIAL"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DigikeyPN" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "TPN" "698-622-00"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MFGPN" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "CP_*")
		(sheetname "/BankPower2/")
		(sheetfile "BankPower.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -4.4 0)
			(size 4.6 2.1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.119048)
			(net 52 "/VB0P0B2")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 4.4 0)
			(size 4.6 2.1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.119048)
			(net 54 "/VB24N0B2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_Elec_10x10.2.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "LED_SMD:LED_0603_1608Metric_Pad1.05x0.95mm_HandSolder"
		(layer "F.Cu")
		(at 256.556765 158.976812 180)
		(descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
		(tags "LED handsolder")
		(property "Reference" "D2"
			(at 3.264178 0.438357 0)
			(layer "F.SilkS")
		)
		(property "Value" "LED"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Light emitting diode"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DigikeyPN" "350-2035-1-ND"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MFGPN" "DIALIGHT CO  598-8070-107F"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "LED* LED_SMD:* LED_THT:*")
		(sheetname "/")
		(sheetfile "BenchPowerBoardNewCMchoke.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.875 0 180)
			(size 1.05 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 21 "Net-(D2-K)")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.875 0 180)
			(size 1.05 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 64 "/V48P0")
			(pinfunction "A")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_Elec_10x10.2"
		(layer "F.Cu")
		(at 122.891271 39.782748)
		(descr "SMD capacitor, aluminum electrolytic nonpolar, 10.0x10.2mm")
		(tags "capacitor electrolyic nonpolar")
		(property "Reference" "C54"
			(at 0.0508 6.246 0)
			(layer "F.SilkS")
		)
		(property "Value" "330uF/35V/10x10"
			(at 0 6.2 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "CAP, ALUMINUM POLYMER 330UF 20% 35V RADIAL"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DigikeyPN" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "TPN" "698-622-00"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MFGPN" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "CP_*")
		(sheetname "/BankPower1/")
		(sheetfile "BankPower.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -4.4 0)
			(size 4.6 2.1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.119048)
			(net 15 "/VB0P0B1")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 4.4 0)
			(size 4.6 2.1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.119048)
			(net 17 "/VB24N0B1")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_Elec_10x10.2.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "CustomLibraries:ToggleSwitch-TE-2267078-1"
		(layer "F.Cu")
		(at 224.621701 170.718322 90)
		(property "Reference" "SW4"
			(at -6.903812 -0.04348 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "TE CONNECTIVITY 	2267078-1"
			(at 0 1 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Single Pole Single Throw (SPST) switch"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DigikeyPN" "450-2110-ND"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MFGPN" "2267078-1"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "TPN" "666-036-12"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Field8" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/BankPower4/")
		(sheetfile "BankPower.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 2.5 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at -2.54 0 90)
			(size 2.54 2.54)
			(drill 1.0922)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 70 "/BankPower4/ENABLE")
			(pinfunction "A")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 2.54 0 90)
			(size 2.54 2.54)
			(drill 1.0922)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 73 "Net-(SW4-B)")
			(pinfunction "B")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "C:/InstalledPrograms/KiCADV5/KiCad/Custom3DModels/ENG_CVM_CVM_2267078-1_A1.3d_stp/c-2267078-1-a1-3d.stp"
			(offset
				(xyz 0 0 21.59)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -0 -0 -90)
			)
		)
	)
	(footprint "CustomLibraries:ToggleSwitch-TE-2267078-1"
		(layer "F.Cu")
		(at 224.385149 134.521145 90)
		(property "Reference" "SW3"
			(at -6.741284 0.142266 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "TE CONNECTIVITY 	2267078-1"
			(at 0 1 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Single Pole Single Throw (SPST) switch"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DigikeyPN" "450-2110-ND"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MFGPN" "2267078-1"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "TPN" "666-036-12"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Field8" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/BankPower3/")
		(sheetfile "BankPower.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 2.5 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at -2.54 0 90)
			(size 2.54 2.54)
			(drill 1.0922)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 72 "/BankPower3/ENABLE")
			(pinfunction "A")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 2.54 0 90)
			(size 2.54 2.54)
			(drill 1.0922)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 27 "Net-(SW3-B)")
			(pinfunction "B")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "C:/InstalledPrograms/KiCADV5/KiCad/Custom3DModels/ENG_CVM_CVM_2267078-1_A1.3d_stp/c-2267078-1-a1-3d.stp"
			(offset
				(xyz 0 0 21.59)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -0 -0 -90)
			)
		)
	)
	(footprint "MountingHole:MountingHole_3.5mm"
		(layer "F.Cu")
		(at 64.59336 224.999259)
		(descr "Mounting Hole 3.5mm, no annular")
		(tags "mounting hole 3.5mm no annular")
		(property "Reference" "H6"
			(at 0 -4.5 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "MountingHole"
			(at 0 4.5 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Mounting Hole without connection"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "MountingHole*")
		(sheetname "/")
		(sheetfile "BenchPowerBoardNewCMchoke.kicad_sch")
		(clearance 3.81)
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 3.5 3.5)
			(drill 3.5)
			(layers "*.Cu" "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "Capacitor_SMD:C_Elec_10x10.2"
		(layer "F.Cu")
		(at 133.9498 220.5588 90)
		(descr "SMD capacitor, aluminum electrolytic nonpolar, 10.0x10.2mm")
		(tags "capacitor electrolyic nonpolar")
		(property "Reference" "C2"
			(at -0.031083 -6.12035 90)
			(layer "F.SilkS")
		)
		(property "Value" "390uF/25V/10x10"
			(at 0 6.2 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "390UF 25V 20% ALUM ELECT"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DigikeyPN" "493-4544-1-ND"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "TPN" "131-516-13"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "CP_*")
		(sheetname "/12Vpower/")
		(sheetfile "12Vpower.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -4.4 0 90)
			(size 4.6 2.1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.119048)
			(net 7 "/VB12P6_GD")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 4.4 0 90)
			(size 4.6 2.1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.119048)
			(net 8 "/VB0P0_GD")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_Elec_10x10.2.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "CustomLibraries:MillMax-Socket-0327-0-15-15-34-27-10-0_NO-SILK"
		(layer "F.Cu")
		(at 220.3814 221.6855)
		(descr "0364-0-15-15-13-27-10-0-2")
		(tags "Connector")
		(property "Reference" "J3"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "0327-0-15-15-34-27-10-0"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" "kicad-embed://Mill Max catalog-0364-0-15-15-13-27-10-0.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "CN/CONTACT SKT .032 TO .046 PIN 30UIN GOLD CONTACT//10UIN GOLD BODY"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DigikeyPN" "ED90081-ND"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "TPN" "699-881-00 "
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "/12Vpower/")
		(sheetfile "12Vpower.kicad_sch")
		(attr through_hole exclude_from_pos_files)
		(embedded_fonts no)
		(model "C:/InstalledPrograms/KiCADV5/KiCad/CustomLibraries/LIB_0364-0-15-15-13-27-10-0/0364-0-15-15-13-27-10-0/3D/0364-0-15-15-13-27-10-0.stp"
			(offset
				(xyz 0 0 0.635)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -0 -90 -0)
			)
		)
	)
	(footprint "MountingHole:MountingHole_3.5mm"
		(layer "F.Cu")
		(at 132.870254 204.915274)
		(descr "Mounting Hole 3.5mm, no annular")
		(tags "mounting hole 3.5mm no annular")
		(property "Reference" "H5"
			(at 0 -4.5 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "MountingHole"
			(at 0 4.5 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Mounting Hole without connection"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "MountingHole*")
		(sheetname "/")
		(sheetfile "BenchPowerBoardNewCMchoke.kicad_sch")
		(clearance 3.81)
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 3.5 3.5)
			(drill 3.5)
			(layers "*.Cu" "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "Capacitor_SMD:C_Elec_10x10.2"
		(layer "F.Cu")
		(at 135.138098 106.954413 180)
		(descr "SMD capacitor, aluminum electrolytic nonpolar, 10.0x10.2mm")
		(tags "capacitor electrolyic nonpolar")
		(property "Reference" "C24"
			(at 7.112 -3.66 0)
			(layer "F.SilkS")
		)
		(property "Value" "120uF/63V/10x10"
			(at 0 6.2 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "CAP, ALUMINUM POLYMER 120UF 20% 63V RADIAL"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DigikeyPN" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "TPN" "701-721-00"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MFGPN" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "CP_*")
		(sheetname "/BankPower2/")
		(sheetfile "BankPower.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -4.4 0 180)
			(size 4.6 2.1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.119048)
			(net 50 "/VB96P0B2")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 4.4 0 180)
			(size 4.6 2.1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.119048)
			(net 10 "Net-(C24-Pad2)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_Elec_10x10.2.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "CustomLibraries:MillMax-Socket-0327-0-15-15-34-27-10-0_NO-SILK"
		(layer "F.Cu")
		(at 207.627155 130.502083)
		(descr "0364-0-15-15-13-27-10-0-2")
		(tags "Connector")
		(property "Reference" "J33"
			(at -4.826 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "0327-0-15-15-34-27-10-0"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" "kicad-embed://Mill Max catalog-0364-0-15-15-13-27-10-0.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "CN/CONTACT SKT .032 TO .046 PIN 30UIN GOLD CONTACT//10UIN GOLD BODY"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DigikeyPN" "ED90081-ND"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "TPN" "699-881-00 "
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "/BankPower3/")
		(sheetfile "BankPower.kicad_sch")
		(attr through_hole exclude_from_pos_files)
		(embedded_fonts no)
		(model "C:/InstalledPrograms/KiCADV5/KiCad/CustomLibraries/LIB_0364-0-15-15-13-27-10-0/0364-0-15-15-13-27-10-0/3D/0364-0-15-15-13-27-10-0.stp"
			(offset
				(xyz 0 0 0.635)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -0 -90 -0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "F.Cu")
		(at 251.501032 99.324526 180)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C12"
			(at 3.4036 0.1488 0)
			(layer "F.SilkS")
		)
		(property "Value" "4.7uF/25V/0805"
			(at 0 1.68 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "CAP 4.7UF 10% 25V 0805 X7R"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DigikeyPN" "399-C0805C475K3RACTUCT-ND"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "TPN" "111-815-05"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MFGPN" "KEMET ELECTRONICS CORP  C0805C475K3RACTU"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/15Vaux/")
		(sheetfile "15Vaux.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.0375 0 180)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 36 "/15Vaux/VP15P0")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.0375 0 180)
			(size 1.175 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.212766)
			(net 76 "/48V_RTN_M1")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 218.138333 84.000034 -90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R19"
			(at 3.015778 0.042424 90)
			(layer "F.SilkS")
		)
		(property "Value" "2k"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "TPN" "636-702-00"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/BankPower2/")
		(sheetfile "BankPower.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 270)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 36 "/15Vaux/VP15P0")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0 270)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 22 "Net-(SW2-B)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "CustomLibraries:MillMax-Socket-0364-0-15-15-13-27-10-0"
		(layer "F.Cu")
		(at 150.510871 51.629698)
		(descr "0364-0-15-15-13-27-10-0-2")
		(tags "Connector")
		(property "Reference" "J20"
			(at 4.5974 1.6764 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "0364-0-15-15-13-27-10-0"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" "kicad-embed://Mill Max catalog-0364-0-15-15-13-27-10-0.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "CN/CONTACT SKT .048 TO .064 PIN 30UIN GOLD CONTACT//10UIN GOLD BODY"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DigikeyPN" "ED90089-ND"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "TPN" "699-882-00 "
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "/BankPower1/")
		(sheetfile "BankPower.kicad_sch")
		(attr through_hole exclude_from_pos_files)
		(embedded_fonts no)
		(model "C:/InstalledPrograms/KiCADV5/KiCad/CustomLibraries/LIB_0364-0-15-15-13-27-10-0/0364-0-15-15-13-27-10-0/3D/0364-0-15-15-13-27-10-0.stp"
			(offset
				(xyz 0 0 0.635)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -0 -90 -0)
			)
		)
	)
	(footprint "CustomLibraries:CM4440Z111R10"
		(layer "F.Cu")
		(at 135.104155 165.008263 180)
		(descr "CM4440Z111R-10-2")
		(tags "Inductor")
		(property "Reference" "FL3"
			(at 1.1736 -7.534 0)
			(layer "F.SilkS")
		)
		(property "Value" "CM4440Z111R_10"
			(at 0 0.213 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" "kicad-embed://cm4440z111r-10-datasheet.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "COMMON MODE CHOKES TRIPLE 110OHM 100MHZ 20A 0.001OHM DCR"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DigikeyPN" "240-CM4440Z111R-10CT-ND"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "TPN" "693-673-00"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "L* L_CommonMode*")
		(sheetname "/BankPower4/")
		(sheetfile "BankPower.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0.213 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -2.54 3.435 180)
			(size 2.03 5.08)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 19 "/BankPower4/VBU96P0")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 0 3.435 180)
			(size 2.03 5.08)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 51 "/BankPower4/VBU0P0")
			(pinfunction "2")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at 2.54 3.435 180)
			(size 2.03 5.08)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 53 "/BankPower4/VBU24P0")
			(pinfunction "3")
			(pintype "passive")
		)
		(pad "4" smd rect
			(at 2.54 -3.435 180)
			(size 2.03 5.08)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 28 "/VB24N0B4")
			(pinfunction "4")
			(pintype "passive")
		)
		(pad "5" smd rect
			(at 0 -3.435 180)
			(size 2.03 5.08)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 26 "/VB0P0B4")
			(pinfunction "5")
			(pintype "passive")
		)
		(pad "6" smd rect
			(at -2.54 -3.435 180)
			(size 2.03 5.08)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 25 "/VB96P0B4")
			(pinfunction "6")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "CM4440Z111R-10.stp"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
		(model "C:/InstalledPrograms/KiCADV5/KiCad/CustomLibraries/LIB_CM4440Z111R-10/CM4440Z111R-10/3D/CM4440Z111R-10.stp"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -0 -0 -0)
			)
		)
	)
	(footprint "CustomLibraries:ToggleSwitch-TE-2267078-1"
		(layer "F.Cu")
		(at 224.399444 87.615672 90)
		(property "Reference" "SW2"
			(at -6.927029 -0.020262 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "TE CONNECTIVITY 	2267078-1"
			(at 0 1 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Single Pole Single Throw (SPST) switch"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DigikeyPN" "450-2110-ND"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MFGPN" "2267078-1"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "TPN" "666-036-12"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Field8" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/BankPower2/")
		(sheetfile "BankPower.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 2.5 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at -2.54 0 90)
			(size 2.54 2.54)
			(drill 1.0922)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 71 "/BankPower2/ENABLE")
			(pinfunction "A")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 2.54 0 90)
			(size 2.54 2.54)
			(drill 1.0922)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 22 "Net-(SW2-B)")
			(pinfunction "B")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "C:/InstalledPrograms/KiCADV5/KiCad/Custom3DModels/ENG_CVM_CVM_2267078-1_A1.3d_stp/c-2267078-1-a1-3d.stp"
			(offset
				(xyz 0 0 21.59)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -0 -0 -90)
			)
		)
	)
	(footprint "Capacitor_SMD:C_Elec_10x10.2"
		(layer "F.Cu")
		(at 122.401271 64.585298 180)
		(descr "SMD capacitor, aluminum electrolytic nonpolar, 10.0x10.2mm")
		(tags "capacitor electrolyic nonpolar")
		(property "Reference" "C49"
			(at 7.1882 -3.1012 0)
			(layer "F.SilkS")
		)
		(property "Value" "120uF/63V/10x10"
			(at 0 6.2 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "CAP, ALUMINUM POLYMER 120UF 20% 63V RADIAL"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DigikeyPN" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "TPN" "701-721-00"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MFGPN" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "CP_*")
		(sheetname "/BankPower1/")
		(sheetfile "BankPower.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -4.4 0 180)
			(size 4.6 2.1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.119048)
			(net 37 "Net-(C42-Pad2)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 4.4 0 180)
			(size 4.6 2.1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.119048)
			(net 15 "/VB0P0B1")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_Elec_10x10.2.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 256.15062 101.802939)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R14"
			(at 2.9464 0.1194 0)
			(layer "F.SilkS")
		)
		(property "Value" "1k"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "RES 1K 1% 0.1W 100PPM 0603"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "TPN" "636-700-00"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DigikeyPN" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/15Vaux/")
		(sheetfile "15Vaux.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 23 "Net-(U2-FB)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 76 "/48V_RTN_M1")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "CustomLibraries:MillMax-Socket-0364-0-15-15-13-27-10-0"
		(layer "F.Cu")
		(at 148.984898 101.600813 180)
		(descr "0364-0-15-15-13-27-10-0-2")
		(tags "Connector")
		(property "Reference" "J9"
			(at -3.8862 2.0066 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "0364-0-15-15-13-27-10-0"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" "kicad-embed://Mill Max catalog-0364-0-15-15-13-27-10-0.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "CN/CONTACT SKT .048 TO .064 PIN 30UIN GOLD CONTACT//10UIN GOLD BODY"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DigikeyPN" "ED90089-ND"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "TPN" "699-882-00 "
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "/BankPower2/")
		(sheetfile "BankPower.kicad_sch")
		(attr through_hole exclude_from_pos_files)
		(embedded_fonts no)
		(model "C:/InstalledPrograms/KiCADV5/KiCad/CustomLibraries/LIB_0364-0-15-15-13-27-10-0/0364-0-15-15-13-27-10-0/3D/0364-0-15-15-13-27-10-0.stp"
			(offset
				(xyz 0 0 0.635)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -0 -90 -0)
			)
		)
	)
	(footprint "CustomLibraries:MillMax-Socket-0327-0-15-15-34-27-10-0_NO-SILK"
		(layer "F.Cu")
		(at 207.404898 89.510413)
		(descr "0364-0-15-15-13-27-10-0-2")
		(tags "Connector")
		(property "Reference" "J12"
			(at -4.826 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "0327-0-15-15-34-27-10-0"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" "kicad-embed://Mill Max catalog-0364-0-15-15-13-27-10-0.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "CN/CONTACT SKT .032 TO .046 PIN 30UIN GOLD CONTACT//10UIN GOLD BODY"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DigikeyPN" "ED90081-ND"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "TPN" "699-881-00 "
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "/BankPower2/")
		(sheetfile "BankPower.kicad_sch")
		(attr through_hole exclude_from_pos_files)
		(embedded_fonts no)
		(model "C:/InstalledPrograms/KiCADV5/KiCad/CustomLibraries/LIB_0364-0-15-15-13-27-10-0/0364-0-15-15-13-27-10-0/3D/0364-0-15-15-13-27-10-0.stp"
			(offset
				(xyz 0 0 0.635)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -0 -90 -0)
			)
		)
	)
	(footprint "CustomLibraries:MillMax-Socket-0327-0-15-15-34-27-10-0_NO-SILK"
		(layer "F.Cu")
		(at 207.627155 180.385463)
		(descr "0364-0-15-15-13-27-10-0-2")
		(tags "Connector")
		(property "Reference" "J28"
			(at -3.937 -0.2839 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "0327-0-15-15-34-27-10-0"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" "kicad-embed://Mill Max catalog-0364-0-15-15-13-27-10-0.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "CN/CONTACT SKT .032 TO .046 PIN 30UIN GOLD CONTACT//10UIN GOLD BODY"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DigikeyPN" "ED90081-ND"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "TPN" "699-881-00 "
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "/BankPower4/")
		(sheetfile "BankPower.kicad_sch")
		(attr through_hole exclude_from_pos_files)
		(embedded_fonts no)
		(model "C:/InstalledPrograms/KiCADV5/KiCad/CustomLibraries/LIB_0364-0-15-15-13-27-10-0/0364-0-15-15-13-27-10-0/3D/0364-0-15-15-13-27-10-0.stp"
			(offset
				(xyz 0 0 0.635)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -0 -90 -0)
			)
		)
	)
	(footprint "CustomLibraries:CS2600"
		(layer "F.Cu")
		(at 177.940898 94.666613 180)
		(property "Reference" "PS2"
			(at -39.980555 16.247264 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "CS2600"
			(at 0 1 180)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "kicad-embed://CS2600 Datasheet.pdf"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "DCDC/ CUSTOM ISOLATED FIXED RATIO 53V INPUT/98V OUTPUT"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "TPN" "680-436-00"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MFGPN" "CS2600"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/BankPower2/")
		(sheetfile "BankPower.kicad_sch")
		(attr exclude_from_pos_files)
		(fp_text user "Vin+"
			(at -32.600749 -7.582917 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "Vout-"
			(at 35.968464 4.083225 270)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "Vin-"
			(at -35.036669 12.456644 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "Vou+"
			(at 36.24383 -4.059137 270)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "Vstart"
			(at -33.577396 4.137689 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "GND"
			(at 34.9008 11.2526 270)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "EN"
			(at -33.488326 -3.077687 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "${REFERENCE}"
			(at 0 2.5 180)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at -29.464 -10.2362 180)
			(size 5.08 5.08)
			(drill 1.651)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "/VFF48P0_M1")
			(pinfunction "Vin+")
			(pintype "input")
		)
		(pad "2" thru_hole circle
			(at -29.464 -2.6162 180)
			(size 5.08 5.08)
			(drill 1.651)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 71 "/BankPower2/ENABLE")
			(pinfunction "ON/OFF")
			(pintype "input")
		)
		(pad "3" thru_hole circle
			(at -29.464 5.1562 180)
			(size 5.08 5.08)
			(drill 1.651)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 36 "/15Vaux/VP15P0")
			(pinfunction "VSTART")
			(pintype "input")
		)
		(pad "4" thru_hole circle
			(at -29.464 12.7762 180)
			(size 5.08 5.08)
			(drill 1.651)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 76 "/48V_RTN_M1")
			(pinfunction "Vin-")
			(pintype "input")
		)
		(pad "5" thru_hole circle
			(at 28.956 8.3058 180)
			(size 5.08 5.08)
			(drill 2.54)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 55 "/BankPower2/VBU0P0")
			(pinfunction "GND")
			(pintype "input")
		)
		(pad "6" thru_hole circle
			(at 28.956 0.6858 180)
			(size 5.08 5.08)
			(drill 2.54)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 56 "/BankPower2/VBU24P0")
			(pinfunction "Vout-")
			(pintype "input")
		)
		(pad "7" thru_hole circle
			(at 28.956 -6.9342 180)
			(size 5.08 5.08)
			(drill 2.54)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 57 "/BankPower2/VBU96P0")
			(pinfunction "Vout+")
			(pintype "input")
		)
		(embedded_fonts no)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 253.07858 101.800481)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R12"
			(at -0.005584 1.477876 0)
			(layer "F.SilkS")
		)
		(property "Value" "14k"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "RES 14K 1% 100PPM 0.1W 0603"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "TPN" "636-702-81"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DigikeyPN" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/15Vaux/")
		(sheetfile "15Vaux.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 36 "/15Vaux/VP15P0")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 23 "Net-(U2-FB)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "CustomLibraries:MillMax-Socket-0327-0-15-15-34-27-10-0_NO-SILK"
		(layer "F.Cu")
		(at 220.3814 214.0655)
		(descr "0364-0-15-15-13-27-10-0-2")
		(tags "Connector")
		(property "Reference" "J4"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "0327-0-15-15-34-27-10-0"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" "kicad-embed://Mill Max catalog-0364-0-15-15-13-27-10-0.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "CN/CONTACT SKT .032 TO .046 PIN 30UIN GOLD CONTACT//10UIN GOLD BODY"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DigikeyPN" "ED90081-ND"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "TPN" "699-881-00 "
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "/12Vpower/")
		(sheetfile "12Vpower.kicad_sch")
		(attr through_hole exclude_from_pos_files)
		(embedded_fonts no)
		(model "C:/InstalledPrograms/KiCADV5/KiCad/CustomLibraries/LIB_0364-0-15-15-13-27-10-0/0364-0-15-15-13-27-10-0/3D/0364-0-15-15-13-27-10-0.stp"
			(offset
				(xyz 0 0 0.635)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -0 -90 -0)
			)
		)
	)
	(footprint "CustomLibraries:ToggleSwitch-TE-2267078-1"
		(layer "F.Cu")
		(at 232.410197 199.087959 -90)
		(property "Reference" "SW5"
			(at 6.433424 -4.882775 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "TE CONNECTIVITY 	2267078-1"
			(at 0 1 270)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Single Pole Single Throw (SPST) switch"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DigikeyPN" "450-2110-ND"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MFGPN" "2267078-1"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "TPN" "666-036-12"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Field8" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/12Vpower/")
		(sheetfile "12Vpower.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 2.5 270)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at -2.54 0 270)
			(size 2.54 2.54)
			(drill 1.0922)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 18 "/12Vpower/C50P_VB12P6_GD_EN_L")
			(pinfunction "A")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 2.54 0 270)
			(size 2.54 2.54)
			(drill 1.0922)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "/12Vpower/48V_RTN_DISA")
			(pinfunction "B")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "C:/InstalledPrograms/KiCADV5/KiCad/Custom3DModels/ENG_CVM_CVM_2267078-1_A1.3d_stp/c-2267078-1-a1-3d.stp"
			(offset
				(xyz 0 0 21.59)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -0 -0 -90)
			)
		)
	)
	(footprint "CustomLibraries:eSGCTO-277_GAS"
		(layer "F.Cu")
		(at 253.493586 162.612072 180)
		(tags "GSGC1060S ")
		(property "Reference" "D12"
			(at -5.528416 -1.175956 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "GSGC151BS"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "DIODE SCHOTTKY 100V 8A TO277"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DigikeyPN" "4786-GSGC151BSCT-ND"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MFGPN" "Good-Ark Semiconductor  GSGC151BS"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TO-???* *_Diode_* *SingleDiode* D_*")
		(sheetname "/48Vpower/")
		(sheetfile "48Vpower.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -2.7559 -0.930001 180)
			(size 1.0922 0.9906)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 77 "/48V_RTN")
			(pinfunction "A")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -2.7559 0.930001 180)
			(size 1.0922 0.9906)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 77 "/48V_RTN")
			(pinfunction "A")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at 1.1049 0 180)
			(size 4.3942 3.302)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 64 "/V48P0")
			(pinfunction "K")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "C:/InstalledPrograms/KiCADV5/KiCad/CustomLibraries/ul_GSGC1060S/eSGC_TO-277__GAS.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -0 -0 -0)
			)
		)
	)
	(footprint "CustomLibraries:XF2506-HOCMC-1200milRound"
		(layer "F.Cu")
		(at 252.888812 185.995455 180)
		(property "Reference" "L3"
			(at 15.143837 1.424257 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "XF2506-HOCMC"
			(at 0 1 180)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "\"C:\\Documentation\\Dragon\\Grogu\\ProtoBoards\\GroguModulePowerBoard\\Components\\XF2506-VOCMC.pdf\""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "IND COMMON MODE CHOKE 250UH 0.0025 OHM DCR"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "TPN" "681-329-00"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MFGPN" "XFMRS  XF2506-HOCMC"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Choke_* *Coil* Inductor_* L_*")
		(sheetname "/48Vpower/")
		(sheetfile "48Vpower.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 2.5 180)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at -6.751066 8.045679 180)
			(size 5.715 5.715)
			(drill 3.175)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 77 "/48V_RTN")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at -6.02422 -8.603463 180)
			(size 5.715 5.715)
			(drill 3.175)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "/12Vpower/48V_RTN_DISA")
			(pinfunction "2")
			(pintype "passive")
		)
		(pad "3" thru_hole circle
			(at 6.02422 -8.603463 180)
			(size 5.715 5.715)
			(drill 3.175)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 9 "/12Vpower/VFF48P0_DISA")
			(pinfunction "3")
			(pintype "passive")
		)
		(pad "4" thru_hole circle
			(at 6.751066 8.045679 180)
			(size 5.715 5.715)
			(drill 3.175)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "/48Vpower/VF48P0_DISA")
			(pinfunction "4")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "Capacitor_SMD:C_Elec_10x10.2"
		(layer "F.Cu")
		(at 135.360355 147.946083 180)
		(descr "SMD capacitor, aluminum electrolytic nonpolar, 10.0x10.2mm")
		(tags "capacitor electrolyic nonpolar")
		(property "Reference" "C82"
			(at 7.112 -3.66 0)
			(layer "F.SilkS")
		)
		(property "Value" "120uF/63V/10x10"
			(at 0 6.2 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "CAP, ALUMINUM POLYMER 120UF 20% 63V RADIAL"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DigikeyPN" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "TPN" "701-721-00"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MFGPN" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "CP_*")
		(sheetname "/BankPower3/")
		(sheetfile "BankPower.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -4.4 0 180)
			(size 4.6 2.1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.119048)
			(net 58 "/VB96P0B3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 4.4 0 180)
			(size 4.6 2.1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.119048)
			(net 79 "Net-(C78-Pad2)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_Elec_10x10.2.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "CustomLibraries:XF2506A-VOCMC-CN-12x18.0mm"
		(layer "F.Cu")
		(at 252.131232 120.66394 -90)
		(descr "CUSTOM COMMON MODE CHOKE 250UH 21 ADC 0.0025 OHMS")
		(tags "choke")
		(property "Reference" "L2"
			(at -3.73 -12.27 270)
			(layer "F.SilkS")
		)
		(property "Value" "XF2506A-VOCMC-CN"
			(at 0 11.77 270)
			(layer "F.Fab")
		)
		(property "Datasheet" "\"C:\\Documentation\\Dragon\\Grogu\\ProtoBoards\\GroguModulePowerBoard\\Components\\XF2506-VOCMC.pdf\""
			(at -5.02 -8.63 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "CUSTOM COMMON MODE CHOKE 250UH 21 ADC 0.0025 OHMS"
			(at -5.02 -8.63 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "TPN" "522-008-10"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MFGPN" "XFMRS  XF2506A-VOCMC-CN"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Choke_* *Coil* Inductor_* L_*")
		(sheetname "/48Vpower/")
		(sheetfile "48Vpower.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 0 270)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at -4.7625 -7.9375 270)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 77 "/48V_RTN")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "1" thru_hole rect
			(at -4.7625 -6.35 270)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 77 "/48V_RTN")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 4.7625 -7.9375 270)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "/48Vpower/VF48P0_BRD")
			(pinfunction "2")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 4.7625 -6.35 270)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "/48Vpower/VF48P0_BRD")
			(pinfunction "2")
			(pintype "passive")
		)
		(pad "3" thru_hole circle
			(at -4.7625 6.35 270)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 76 "/48V_RTN_M1")
			(pinfunction "3")
			(pintype "passive")
		)
		(pad "3" thru_hole circle
			(at -4.7625 7.9375 270)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 76 "/48V_RTN_M1")
			(pinfunction "3")
			(pintype "passive")
		)
		(pad "4" thru_hole circle
			(at 4.7625 6.35 270)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "/VFF48P0_M1")
			(pinfunction "4")
			(pintype "passive")
		)
		(pad "4" thru_hole circle
			(at 4.7625 7.9375 270)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "/VFF48P0_M1")
			(pinfunction "4")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Inductor_THT.3dshapes/Choke_Schaffner_RN212-04-12.5x18.0mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "CustomLibraries:MillMax-Socket-0327-0-15-15-34-27-10-0_NO-SILK"
		(layer "F.Cu")
		(at 207.627155 122.882083)
		(descr "0364-0-15-15-13-27-10-0-2")
		(tags "Connector")
		(property "Reference" "J32"
			(at -5.6896 -0.7874 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "0327-0-15-15-34-27-10-0"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" "kicad-embed://Mill Max catalog-0364-0-15-15-13-27-10-0.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "CN/CONTACT SKT .032 TO .046 PIN 30UIN GOLD CONTACT//10UIN GOLD BODY"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DigikeyPN" "ED90081-ND"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "TPN" "699-881-00 "
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "/BankPower3/")
		(sheetfile "BankPower.kicad_sch")
		(attr through_hole exclude_from_pos_files)
		(embedded_fonts no)
		(model "C:/InstalledPrograms/KiCADV5/KiCad/CustomLibraries/LIB_0364-0-15-15-13-27-10-0/0364-0-15-15-13-27-10-0/3D/0364-0-15-15-13-27-10-0.stp"
			(offset
				(xyz 0 0 0.635)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -0 -90 -0)
			)
		)
	)
	(footprint "CustomLibraries:MillMax-Socket-0364-0-15-15-13-27-10-0"
		(layer "F.Cu")
		(at 149.207155 134.972483)
		(descr "0364-0-15-15-13-27-10-0-2")
		(tags "Connector")
		(property "Reference" "J34"
			(at 4.5974 1.6764 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "0364-0-15-15-13-27-10-0"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" "kicad-embed://Mill Max catalog-0364-0-15-15-13-27-10-0.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "CN/CONTACT SKT .048 TO .064 PIN 30UIN GOLD CONTACT//10UIN GOLD BODY"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DigikeyPN" "ED90089-ND"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "TPN" "699-882-00 "
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "/BankPower3/")
		(sheetfile "BankPower.kicad_sch")
		(attr through_hole exclude_from_pos_files)
		(embedded_fonts no)
		(model "C:/InstalledPrograms/KiCADV5/KiCad/CustomLibraries/LIB_0364-0-15-15-13-27-10-0/0364-0-15-15-13-27-10-0/3D/0364-0-15-15-13-27-10-0.stp"
			(offset
				(xyz 0 0 0.635)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -0 -90 -0)
			)
		)
	)
	(footprint "LED_SMD:LED_0603_1608Metric_Pad1.05x0.95mm_HandSolder"
		(layer "F.Cu")
		(at 124.602707 116.385567 180)
		(descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
		(tags "LED handsolder")
		(property "Reference" "D4"
			(at -0.405652 1.747606 0)
			(layer "F.SilkS")
		)
		(property "Value" "LED"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Light emitting diode"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DigikeyPN" "350-2035-1-ND"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MFGPN" "DIALIGHT CO  598-8070-107F"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "LED* LED_SMD:* LED_THT:*")
		(sheetname "/")
		(sheetfile "BenchPowerBoardNewCMchoke.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.875 0 180)
			(size 1.05 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 60 "/VB24N0B3")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.875 0 180)
			(size 1.05 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 81 "Net-(D4-A)")
			(pinfunction "A")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "B.Cu")
		(at 229.820788 47.843694 180)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R30"
			(at 0 1.43 0)
			(layer "B.SilkS")
		)
		(property "Value" "1k"
			(at 0 -1.43 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "TPN" "636-700-00"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/BankPower1/")
		(sheetfile "BankPower.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 180)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 76 "/48V_RTN_M1")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0 180)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 69 "/BankPower1/ENABLE")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1206_3216Metric_Pad1.33x1.80mm_HandSolder"
		(layer "B.Cu")
		(at 155.850271 61.765648)
		(descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C48"
			(at 3.9624 -0.03425 0)
			(layer "B.SilkS")
		)
		(property "Value" "0.1uF/200V/1206"
			(at 0 -1.85 0)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "CAP CER 0.1UF 10% 200V X7R 1206"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "DigikeyPN" "399-12986-1-ND"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "TPN" "693-921-00"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MFGPN" "KEMET ELECTRONICS CORP  C1206X104K2RACAUTO"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/BankPower1/")
		(sheetfile "BankPower.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.5625 0)
			(size 1.325 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.188679)
			(net 12 "/BankPower1/VBU96P0")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.5625 0)
			(size 1.325 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.188679)
			(net 14 "/BankPower1/VBU0P0")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1210_3225Metric_Pad1.33x2.70mm_HandSolder"
		(layer "B.Cu")
		(at 177.978355 177.132463 180)
		(descr "Capacitor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C71"
			(at 0 2.3 0)
			(layer "B.SilkS")
		)
		(property "Value" "22nF/1000V/1210"
			(at 0 -2.3 0)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "CAP, CERAMIC 0.022UF 5% 1KV NP0 1210"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MFGPN" "MURATA ELECTRONICS NO AMERICA  GRM32E5C3A223JWAAK "
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "DigikeyPN" "490-GRM32E5C3A223JWAAKCT-ND"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "TPN" "693-678-00"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/BankPower4/")
		(sheetfile "BankPower.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.5625 0 180)
			(size 1.325 2.7)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.188679)
			(net 76 "/48V_RTN_M1")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.5625 0 180)
			(size 1.325 2.7)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.188679)
			(net 53 "/BankPower4/VBU24P0")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1210_3225Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1206_3216Metric_Pad1.33x1.80mm_HandSolder"
		(layer "B.Cu")
		(at 155.274955 129.479733 180)
		(descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C92"
			(at -3.8608 0.0466 0)
			(layer "B.SilkS")
		)
		(property "Value" "10uF/35V/1206"
			(at 0 -1.85 0)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "CAP, 10UF 20% 35V X7R FLEX 1206"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "DigikeyPN" "445-172484-1-ND"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "TPN" "634-905-00"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MFGPN" "TDK CORP  CGA5L1X7R1V106M160AE"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/BankPower3/")
		(sheetfile "BankPower.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.5625 0 180)
			(size 1.325 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.188679)
			(net 61 "/BankPower3/VBU0P0")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.5625 0 180)
			(size 1.325 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.188679)
			(net 62 "/BankPower3/VBU24P0")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "B.Cu")
		(at 122.465271 59.263498 180)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R21"
			(at 0 1.65 0)
			(layer "B.SilkS")
		)
		(property "Value" "75k"
			(at 0 -1.65 0)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "DigiketPN" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/BankPower1/")
		(sheetfile "BankPower.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 180)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902)
			(net 37 "Net-(C42-Pad2)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 180)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902)
			(net 15 "/VB0P0B1")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1210_3225Metric_Pad1.33x2.70mm_HandSolder"
		(layer "B.Cu")
		(at 177.978355 127.276483 180)
		(descr "Capacitor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C88"
			(at 0 2.3 0)
			(layer "B.SilkS")
		)
		(property "Value" "22nF/1000V/1210"
			(at 0 -2.3 0)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "CAP, CERAMIC 0.022UF 5% 1KV NP0 1210"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MFGPN" "MURATA ELECTRONICS NO AMERICA  GRM32E5C3A223JWAAK "
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "DigikeyPN" "490-GRM32E5C3A223JWAAKCT-ND"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "TPN" "693-678-00"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/BankPower3/")
		(sheetfile "BankPower.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.5625 0 180)
			(size 1.325 2.7)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.188679)
			(net 76 "/48V_RTN_M1")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.5625 0 180)
			(size 1.325 2.7)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.188679)
			(net 61 "/BankPower3/VBU0P0")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1210_3225Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1206_3216Metric_Pad1.33x1.80mm_HandSolder"
		(layer "B.Cu")
		(at 155.278355 131.857483 180)
		(descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C93"
			(at -4.6736 -0.2328 0)
			(layer "B.SilkS")
		)
		(property "Value" "10uF/35V/1206"
			(at 0 -1.85 0)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "CAP, 10UF 20% 35V X7R FLEX 1206"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "DigikeyPN" "445-172484-1-ND"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "TPN" "634-905-00"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MFGPN" "TDK CORP  CGA5L1X7R1V106M160AE"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/BankPower3/")
		(sheetfile "BankPower.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.5625 0 180)
			(size 1.325 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.188679)
			(net 61 "/BankPower3/VBU0P0")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.5625 0 180)
			(size 1.325 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.188679)
			(net 62 "/BankPower3/VBU24P0")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "B.Cu")
		(at 120.939298 101.614613 180)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R18"
			(at 0 1.65 0)
			(layer "B.SilkS")
		)
		(property "Value" "75k"
			(at 0 -1.65 0)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/BankPower2/")
		(sheetfile "BankPower.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 180)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902)
			(net 10 "Net-(C24-Pad2)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 180)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902)
			(net 52 "/VB0P0B2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "B.Cu")
		(at 136.544071 59.260498 180)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R20"
			(at 0 1.65 0)
			(layer "B.SilkS")
		)
		(property "Value" "75k"
			(at 0 -1.65 0)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "DigiketPN" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/BankPower1/")
		(sheetfile "BankPower.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 180)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902)
			(net 13 "/VB96P0B1")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 180)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902)
			(net 37 "Net-(C42-Pad2)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1206_3216Metric_Pad1.33x1.80mm_HandSolder"
		(layer "B.Cu")
		(at 182.06145 213.980992 90)
		(descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C3"
			(at 3.6576 -0.182 90)
			(layer "B.SilkS")
		)
		(property "Value" "10uF/35V/1206"
			(at 0 -1.85 90)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "CAP, 10UF 20% 35V X7R FLEX 1206"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "DigikeyPN" "445-172484-1-ND"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "TPN" "634-905-00"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MFGPN" "TDK CORP  CGA5L1X7R1V106M160AE"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/12Vpower/")
		(sheetfile "12Vpower.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.5625 0 90)
			(size 1.325 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.188679)
			(net 11 "/12Vpower/VBU12P6_11_21")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.5625 0 90)
			(size 1.325 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.188679)
			(net 6 "/12Vpower/VBU0P0_11_21")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "B.Cu")
		(at 194.9666 220.2406 180)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C1"
			(at 0 1.68 180)
			(layer "B.SilkS")
		)
		(property "Value" "470nF/100V/0805"
			(at 0 -1.68 180)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "CAP CER 0.47UF 100V X7R 0805"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "TPN" "111-169-03"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MFGPN" "08051C474KAZ2A"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "DigikeyPN" "478-KGF21KR72A474KUCT-ND"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/12Vpower/")
		(sheetfile "12Vpower.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.0375 0 180)
			(size 1.175 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.212766)
			(net 5 "/12Vpower/VFFF48P0_PS11")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.0375 0 180)
			(size 1.175 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.212766)
			(net 6 "/12Vpower/VBU0P0_11_21")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1206_3216Metric_Pad1.33x1.80mm_HandSolder"
		(layer "B.Cu")
		(at 156.582071 48.514698 180)
		(descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C57"
			(at -4.6736 -0.2328 0)
			(layer "B.SilkS")
		)
		(property "Value" "10uF/35V/1206"
			(at 0 -1.85 0)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "CAP, 10UF 20% 35V X7R FLEX 1206"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "DigikeyPN" "445-172484-1-ND"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "TPN" "634-905-00"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MFGPN" "TDK CORP  CGA5L1X7R1V106M160AE"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/BankPower1/")
		(sheetfile "BankPower.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.5625 0 180)
			(size 1.325 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.188679)
			(net 14 "/BankPower1/VBU0P0")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.5625 0 180)
			(size 1.325 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.188679)
			(net 16 "/BankPower1/VBU24P0")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "B.Cu")
		(at 135.240355 142.603283 180)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R26"
			(at 0 1.65 0)
			(layer "B.SilkS")
		)
		(property "Value" "75k"
			(at 0 -1.65 0)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "DigiketPN" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/BankPower3/")
		(sheetfile "BankPower.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 180)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902)
			(net 58 "/VB96P0B3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 180)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902)
			(net 79 "Net-(C78-Pad2)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "B.Cu")
		(at 228.418366 90.118524 180)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R29"
			(at 0 1.43 0)
			(layer "B.SilkS")
		)
		(property "Value" "1k"
			(at 0 -1.43 0)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "TPN" "636-700-00"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/BankPower2/")
		(sheetfile "BankPower.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 180)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 76 "/48V_RTN_M1")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0 180)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 71 "/BankPower2/ENABLE")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1206_3216Metric_Pad1.33x1.80mm_HandSolder"
		(layer "B.Cu")
		(at 154.546555 187.219413)
		(descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C68"
			(at 3.9624 -0.03425 0)
			(layer "B.SilkS")
		)
		(property "Value" "0.1uF/200V/1206"
			(at 0 -1.85 0)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "CAP CER 0.1UF 10% 200V X7R 1206"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "DigikeyPN" "399-12986-1-ND"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "TPN" "693-921-00"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MFGPN" "KEMET ELECTRONICS CORP  C1206X104K2RACAUTO"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/BankPower4/")
		(sheetfile "BankPower.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.5625 0)
			(size 1.325 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.188679)
			(net 19 "/BankPower4/VBU96P0")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.5625 0)
			(size 1.325 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.188679)
			(net 51 "/BankPower4/VBU0P0")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "B.Cu")
		(at 121.161555 184.717263 180)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R24"
			(at 0 1.65 0)
			(layer "B.SilkS")
		)
		(property "Value" "75k"
			(at 0 -1.65 0)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/BankPower4/")
		(sheetfile "BankPower.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 180)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902)
			(net 78 "Net-(C60-Pad2)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 180)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902)
			(net 26 "/VB0P0B4")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "B.Cu")
		(at 245.649471 121.036643 90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C18"
			(at 0 1.68 90)
			(layer "B.SilkS")
		)
		(property "Value" "10nF/100V"
			(at 0 -1.68 90)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MFGPN" "C0805C103K1RAC"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "DigikeyPN" "399-C0805C103K1RAC7025CT-ND"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "TPN" "111-123-04"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/48Vpower/")
		(sheetfile "48Vpower.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.0375 0 90)
			(size 1.175 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.212766)
			(net 3 "/VFF48P0_M1")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.0375 0 90)
			(size 1.175 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.212766)
			(net 76 "/48V_RTN_M1")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1210_3225Metric_Pad1.33x2.70mm_HandSolder"
		(layer "B.Cu")
		(at 177.756098 86.284813 180)
		(descr "Capacitor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C34"
			(at 0 2.3 0)
			(layer "B.SilkS")
		)
		(property "Value" "22nF/1000V/1210"
			(at 0 -2.3 0)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "CAP, CERAMIC 0.022UF 5% 1KV NP0 1210"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MFGPN" "MURATA ELECTRONICS NO AMERICA  GRM32E5C3A223JWAAK "
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "DigikeyPN" "490-GRM32E5C3A223JWAAKCT-ND"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "TPN" "693-678-00"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/BankPower2/")
		(sheetfile "BankPower.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.5625 0 180)
			(size 1.325 2.7)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.188679)
			(net 76 "/48V_RTN_M1")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.5625 0 180)
			(size 1.325 2.7)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.188679)
			(net 55 "/BankPower2/VBU0P0")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1210_3225Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1206_3216Metric_Pad1.33x1.80mm_HandSolder"
		(layer "B.Cu")
		(at 154.324298 104.116763)
		(descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C30"
			(at 3.9624 -0.03425 0)
			(layer "B.SilkS")
		)
		(property "Value" "0.1uF/200V/1206"
			(at 0 -1.85 0)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "CAP CER 0.1UF 10% 200V X7R 1206"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "DigikeyPN" "399-12986-1-ND"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "TPN" "693-921-00"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MFGPN" "KEMET ELECTRONICS CORP  C1206X104K2RACAUTO"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/BankPower2/")
		(sheetfile "BankPower.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.5625 0)
			(size 1.325 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.188679)
			(net 57 "/BankPower2/VBU96P0")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.5625 0)
			(size 1.325 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.188679)
			(net 55 "/BankPower2/VBU0P0")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "B.Cu")
		(at 228.313169 173.284039 180)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R31"
			(at 0 1.43 0)
			(layer "B.SilkS")
		)
		(property "Value" "1k"
			(at 0 -1.43 0)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "TPN" "636-700-00"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/BankPower4/")
		(sheetfile "BankPower.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 180)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 76 "/48V_RTN_M1")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0 180)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 70 "/BankPower4/ENABLE")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "B.Cu")
		(at 135.018098 101.611613 180)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R17"
			(at 0 1.65 0)
			(layer "B.SilkS")
		)
		(property "Value" "75k"
			(at 0 -1.65 0)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/BankPower2/")
		(sheetfile "BankPower.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 180)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902)
			(net 50 "/VB96P0B2")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 180)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902)
			(net 10 "Net-(C24-Pad2)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1210_3225Metric_Pad1.33x2.70mm_HandSolder"
		(layer "B.Cu")
		(at 179.282071 59.187498 180)
		(descr "Capacitor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C41"
			(at 0 2.3 0)
			(layer "B.SilkS")
		)
		(property "Value" "22nF/1000V/1210"
			(at 0 -2.3 0)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "CAP, CERAMIC 0.022UF 5% 1KV NP0 1210"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MFGPN" "MURATA ELECTRONICS NO AMERICA  GRM32E5C3A223JWAAK "
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "DigikeyPN" "490-GRM32E5C3A223JWAAKCT-ND"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "TPN" "693-678-00"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/BankPower1/")
		(sheetfile "BankPower.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.5625 0 180)
			(size 1.325 2.7)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.188679)
			(net 76 "/48V_RTN_M1")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.5625 0 180)
			(size 1.325 2.7)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.188679)
			(net 12 "/BankPower1/VBU96P0")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1210_3225Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1206_3216Metric_Pad1.33x1.80mm_HandSolder"
		(layer "B.Cu")
		(at 155.278355 173.968463 180)
		(descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C76"
			(at -4.6736 -0.2328 0)
			(layer "B.SilkS")
		)
		(property "Value" "10uF/35V/1206"
			(at 0 -1.85 0)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "CAP, 10UF 20% 35V X7R FLEX 1206"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "DigikeyPN" "445-172484-1-ND"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "TPN" "634-905-00"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MFGPN" "TDK CORP  CGA5L1X7R1V106M160AE"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/BankPower4/")
		(sheetfile "BankPower.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.5625 0 180)
			(size 1.325 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.188679)
			(net 51 "/BankPower4/VBU0P0")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.5625 0 180)
			(size 1.325 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.188679)
			(net 53 "/BankPower4/VBU24P0")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1210_3225Metric_Pad1.33x2.70mm_HandSolder"
		(layer "B.Cu")
		(at 177.756098 101.538613 180)
		(descr "Capacitor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C23"
			(at 0 2.3 0)
			(layer "B.SilkS")
		)
		(property "Value" "22nF/1000V/1210"
			(at 0 -2.3 0)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "CAP, CERAMIC 0.022UF 5% 1KV NP0 1210"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MFGPN" "MURATA ELECTRONICS NO AMERICA  GRM32E5C3A223JWAAK "
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "DigikeyPN" "490-GRM32E5C3A223JWAAKCT-ND"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "TPN" "693-678-00"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/BankPower2/")
		(sheetfile "BankPower.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.5625 0 180)
			(size 1.325 2.7)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.188679)
			(net 76 "/48V_RTN_M1")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.5625 0 180)
			(size 1.325 2.7)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.188679)
			(net 57 "/BankPower2/VBU96P0")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1210_3225Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "B.Cu")
		(at 200.965344 188.187927 180)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C62"
			(at 0 1.68 0)
			(layer "B.SilkS")
		)
		(property "Value" "470nF/100V/0805"
			(at 0 -1.68 0)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "CAP CER 0.47UF 100V X7R 0805"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MFGPN" "08051C474KAZ2A"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "DigikeyPN" "478-KGF21KR72A474KUCT-ND"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "TPN" "111-169-03"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/BankPower4/")
		(sheetfile "BankPower.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.0375 0 180)
			(size 1.175 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.212766)
			(net 3 "/VFF48P0_M1")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.0375 0 180)
			(size 1.175 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.212766)
			(net 76 "/48V_RTN_M1")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1206_3216Metric_Pad1.33x1.80mm_HandSolder"
		(layer "B.Cu")
		(at 154.334498 101.780163)
		(descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C32"
			(at 4.1148 0.11815 0)
			(layer "B.SilkS")
		)
		(property "Value" "0.1uF/200V/1206"
			(at 0 -1.85 0)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "CAP CER 0.1UF 10% 200V X7R 1206"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "DigikeyPN" "399-12986-1-ND"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "TPN" "693-921-00"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MFGPN" "KEMET ELECTRONICS CORP  C1206X104K2RACAUTO"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/BankPower2/")
		(sheetfile "BankPower.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.5625 0)
			(size 1.325 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.188679)
			(net 57 "/BankPower2/VBU96P0")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.5625 0)
			(size 1.325 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.188679)
			(net 55 "/BankPower2/VBU0P0")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "B.Cu")
		(at 194.6641 206.201 180)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C10"
			(at 0 1.68 0)
			(layer "B.SilkS")
		)
		(property "Value" "470nF/100V/0805"
			(at 0 -1.68 0)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "CAP CER 0.47UF 100V X7R 0805"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MFGPN" "08051C474KAZ2A"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "DigikeyPN" "478-KGF21KR72A474KUCT-ND"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "TPN" "111-169-03"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/12Vpower/")
		(sheetfile "12Vpower.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.0375 0 180)
			(size 1.175 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.212766)
			(net 1 "/12Vpower/48V_RTN_DISA")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.0375 0 180)
			(size 1.175 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.212766)
			(net 6 "/12Vpower/VBU0P0_11_21")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_1206_3216Metric"
		(layer "B.Cu")
		(at 254.012001 181.854787)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R16"
			(at -0.018257 -2.027486 0)
			(layer "B.SilkS")
		)
		(property "Value" "100k"
			(at 0 -1.82 0)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "TPN" "654-510-00"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/48Vpower/")
		(sheetfile "48Vpower.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.4625 0)
			(size 1.125 1.75)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.222222)
			(net 4 "/48Vpower/VF48P0_DISA")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.4625 0)
			(size 1.125 1.75)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.222222)
			(net 77 "/48V_RTN")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "B.Cu")
		(at 255.781479 92.171198)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C15"
			(at -0.11207 -1.888752 0)
			(layer "B.SilkS")
		)
		(property "Value" "4.7uF/25V/0805"
			(at 0 -1.68 0)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "CAP 4.7UF 10% 25V 0805 X7R"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "DigikeyPN" "399-C0805C475K3RACTUCT-ND"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "TPN" "111-815-05"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MFGPN" "KEMET ELECTRONICS CORP  C0805C475K3RACTU"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/15Vaux/")
		(sheetfile "15Vaux.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.0375 0)
			(size 1.175 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.212766)
			(net 36 "/15Vaux/VP15P0")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.0375 0)
			(size 1.175 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.212766)
			(net 76 "/48V_RTN_M1")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "B.Cu")
		(at 121.161555 142.606283 180)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R27"
			(at 0 1.65 0)
			(layer "B.SilkS")
		)
		(property "Value" "75k"
			(at 0 -1.65 0)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "DigikeyPN" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/BankPower3/")
		(sheetfile "BankPower.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 180)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902)
			(net 79 "Net-(C78-Pad2)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 180)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902)
			(net 59 "/VB0P0B3")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1210_3225Metric_Pad1.33x2.70mm_HandSolder"
		(layer "B.Cu")
		(at 179.282071 43.933698 180)
		(descr "Capacitor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C52"
			(at 0 2.3 0)
			(layer "B.SilkS")
		)
		(property "Value" "22nF/1000V/1210"
			(at 0 -2.3 0)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "CAP, CERAMIC 0.022UF 5% 1KV NP0 1210"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MFGPN" "MURATA ELECTRONICS NO AMERICA  GRM32E5C3A223JWAAK "
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "DigikeyPN" "490-GRM32E5C3A223JWAAKCT-ND"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "TPN" "693-678-00"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/BankPower1/")
		(sheetfile "BankPower.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.5625 0 180)
			(size 1.325 2.7)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.188679)
			(net 76 "/48V_RTN_M1")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.5625 0 180)
			(size 1.325 2.7)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.188679)
			(net 14 "/BankPower1/VBU0P0")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1210_3225Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "B.Cu")
		(at 260.99963 158.888128)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R2"
			(at 3.332869 0.431707 180)
			(layer "B.SilkS")
		)
		(property "Value" "50K"
			(at 0 -1.65 180)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "BenchPowerBoardNewCMchoke.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902)
			(net 21 "Net-(D2-K)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902)
			(net 77 "/48V_RTN")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1206_3216Metric_Pad1.33x1.80mm_HandSolder"
		(layer "B.Cu")
		(at 155.274955 134.191533 180)
		(descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C94"
			(at -3.9878 -0.1566 0)
			(layer "B.SilkS")
		)
		(property "Value" "10uF/35V/1206"
			(at 0 -1.85 0)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "CAP, 10UF 20% 35V X7R FLEX 1206"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "DigikeyPN" "445-172484-1-ND"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "TPN" "634-905-00"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MFGPN" "TDK CORP  CGA5L1X7R1V106M160AE"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/BankPower3/")
		(sheetfile "BankPower.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.5625 0 180)
			(size 1.325 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.188679)
			(net 61 "/BankPower3/VBU0P0")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.5625 0 180)
			(size 1.325 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.188679)
			(net 62 "/BankPower3/VBU24P0")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1206_3216Metric_Pad1.33x1.80mm_HandSolder"
		(layer "B.Cu")
		(at 147.677348 107.998413 -90)
		(descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C29"
			(at 4.0386 0.11815 90)
			(layer "B.SilkS")
		)
		(property "Value" "0.1uF/200V/1206"
			(at 0 -1.85 90)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "CAP CER 0.1UF 10% 200V X7R 1206"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "DigikeyPN" "399-12986-1-ND"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "TPN" "693-921-00"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MFGPN" "KEMET ELECTRONICS CORP  C1206X104K2RACAUTO"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/BankPower2/")
		(sheetfile "BankPower.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.5625 0 270)
			(size 1.325 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.188679)
			(net 57 "/BankPower2/VBU96P0")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.5625 0 270)
			(size 1.325 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.188679)
			(net 55 "/BankPower2/VBU0P0")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "B.Cu")
		(at 200.579471 104.267194 180)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C26"
			(at 0 1.68 0)
			(layer "B.SilkS")
		)
		(property "Value" "470nF/100V/0805"
			(at 0 -1.68 0)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "CAP CER 0.47UF 100V X7R 0805"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MFGPN" "08051C474KAZ2A"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "DigikeyPN" "478-KGF21KR72A474KUCT-ND"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "TPN" "111-169-03"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/BankPower2/")
		(sheetfile "BankPower.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.0375 0 180)
			(size 1.175 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.212766)
			(net 3 "/VFF48P0_M1")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.0375 0 180)
			(size 1.175 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.212766)
			(net 76 "/48V_RTN_M1")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1210_3225Metric_Pad1.33x2.70mm_HandSolder"
		(layer "B.Cu")
		(at 177.978355 135.021483 180)
		(descr "Capacitor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C89"
			(at 0 2.3 0)
			(layer "B.SilkS")
		)
		(property "Value" "22nF/1000V/1210"
			(at 0 -2.3 0)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "CAP, CERAMIC 0.022UF 5% 1KV NP0 1210"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MFGPN" "MURATA ELECTRONICS NO AMERICA  GRM32E5C3A223JWAAK "
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "DigikeyPN" "490-GRM32E5C3A223JWAAKCT-ND"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "TPN" "693-678-00"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/BankPower3/")
		(sheetfile "BankPower.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.5625 0 180)
			(size 1.325 2.7)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.188679)
			(net 76 "/48V_RTN_M1")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.5625 0 180)
			(size 1.325 2.7)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.188679)
			(net 62 "/BankPower3/VBU24P0")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1210_3225Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1206_3216Metric_Pad1.33x1.80mm_HandSolder"
		(layer "B.Cu")
		(at 156.578671 46.136948 180)
		(descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C55"
			(at -3.8608 0.0466 0)
			(layer "B.SilkS")
		)
		(property "Value" "10uF/35V/1206"
			(at 0 -1.85 0)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "CAP, 10UF 20% 35V X7R FLEX 1206"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "DigikeyPN" "445-172484-1-ND"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "TPN" "634-905-00"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MFGPN" "TDK CORP  CGA5L1X7R1V106M160AE"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/BankPower1/")
		(sheetfile "BankPower.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.5625 0 180)
			(size 1.325 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.188679)
			(net 14 "/BankPower1/VBU0P0")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.5625 0 180)
			(size 1.325 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.188679)
			(net 16 "/BankPower1/VBU24P0")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1206_3216Metric_Pad1.33x1.80mm_HandSolder"
		(layer "B.Cu")
		(at 150.030148 108.008213 -90)
		(descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C27"
			(at 4.064 0.16895 90)
			(layer "B.SilkS")
		)
		(property "Value" "0.1uF/200V/1206"
			(at 0 -1.85 90)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "CAP CER 0.1UF 10% 200V X7R 1206"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "DigikeyPN" "399-12986-1-ND"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "TPN" "693-921-00"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MFGPN" "KEMET ELECTRONICS CORP  C1206X104K2RACAUTO"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/BankPower2/")
		(sheetfile "BankPower.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.5625 0 270)
			(size 1.325 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.188679)
			(net 57 "/BankPower2/VBU96P0")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.5625 0 270)
			(size 1.325 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.188679)
			(net 55 "/BankPower2/VBU0P0")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "B.Cu")
		(at 133.929018 220.361708 90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R1"
			(at 0 1.43 90)
			(layer "B.SilkS")
		)
		(property "Value" "12.7k"
			(at 0 -1.43 90)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "DigikeyPN" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "BenchPowerBoardNewCMchoke.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 90)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 20 "Net-(D1-K)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0 90)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 8 "/VB0P0_GD")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1206_3216Metric_Pad1.33x1.80mm_HandSolder"
		(layer "B.Cu")
		(at 155.052698 88.488063 180)
		(descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C38"
			(at -3.8608 0.0466 0)
			(layer "B.SilkS")
		)
		(property "Value" "10uF/35V/1206"
			(at 0 -1.85 0)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "CAP, 10UF 20% 35V X7R FLEX 1206"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "DigikeyPN" "445-172484-1-ND"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "TPN" "634-905-00"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MFGPN" "TDK CORP  CGA5L1X7R1V106M160AE"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/BankPower2/")
		(sheetfile "BankPower.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.5625 0 180)
			(size 1.325 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.188679)
			(net 55 "/BankPower2/VBU0P0")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.5625 0 180)
			(size 1.325 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.188679)
			(net 56 "/BankPower2/VBU24P0")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1206_3216Metric_Pad1.33x1.80mm_HandSolder"
		(layer "B.Cu")
		(at 156.578671 50.848748 180)
		(descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C58"
			(at -3.9878 -0.1566 0)
			(layer "B.SilkS")
		)
		(property "Value" "10uF/35V/1206"
			(at 0 -1.85 0)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "CAP, 10UF 20% 35V X7R FLEX 1206"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "DigikeyPN" "445-172484-1-ND"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "TPN" "634-905-00"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MFGPN" "TDK CORP  CGA5L1X7R1V106M160AE"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/BankPower1/")
		(sheetfile "BankPower.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.5625 0 180)
			(size 1.325 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.188679)
			(net 14 "/BankPower1/VBU0P0")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.5625 0 180)
			(size 1.325 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.188679)
			(net 16 "/BankPower1/VBU24P0")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "B.Cu")
		(at 259.015397 120.545027 90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C17"
			(at 0.145782 1.918991 90)
			(layer "B.SilkS")
		)
		(property "Value" "10nF/100V"
			(at 0 -1.68 90)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "TPN" "111-123-04"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MFGPN" "C0805C103K1RAC"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "DigikeyPN" "399-C0805C103K1RAC7025CT-ND"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/48Vpower/")
		(sheetfile "48Vpower.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.0375 0 90)
			(size 1.175 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.212766)
			(net 2 "/48Vpower/VF48P0_BRD")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.0375 0 90)
			(size 1.175 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.212766)
			(net 77 "/48V_RTN")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1206_3216Metric_Pad1.33x1.80mm_HandSolder"
		(layer "B.Cu")
		(at 179.6002 213.985792 90)
		(descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C4"
			(at 3.7846 -0.1312 90)
			(layer "B.SilkS")
		)
		(property "Value" "10uF/35V/1206"
			(at 0 -1.85 90)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "CAP, 10UF 20% 35V X7R FLEX 1206"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "DigikeyPN" "445-172484-1-ND"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "TPN" "634-905-00"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MFGPN" "TDK CORP  CGA5L1X7R1V106M160AE"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/12Vpower/")
		(sheetfile "12Vpower.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.5625 0 90)
			(size 1.325 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.188679)
			(net 11 "/12Vpower/VBU12P6_11_21")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.5625 0 90)
			(size 1.325 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.188679)
			(net 6 "/12Vpower/VBU0P0_11_21")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "B.Cu")
		(at 202.050905 61.868357 180)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C44"
			(at 0 1.68 0)
			(layer "B.SilkS")
		)
		(property "Value" "470nF/100V/0805"
			(at 0 -1.68 0)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "CAP CER 0.47UF 100V X7R 0805"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MFGPN" "08051C474KAZ2A"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "DigikeyPN" "478-KGF21KR72A474KUCT-ND"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "TPN" "111-169-03"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/BankPower1/")
		(sheetfile "BankPower.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.0375 0 180)
			(size 1.175 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.212766)
			(net 3 "/VFF48P0_M1")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.0375 0 180)
			(size 1.175 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.212766)
			(net 76 "/48V_RTN_M1")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "B.Cu")
		(at 134.3957 154.749342 180)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R6"
			(at 2.811008 0.086736 0)
			(layer "B.SilkS")
		)
		(property "Value" "100k"
			(at 0 -1.65 0)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "BenchPowerBoardNewCMchoke.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 180)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902)
			(net 82 "Net-(D8-K)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 180)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902)
			(net 59 "/VB0P0B3")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "B.Cu")
		(at 255.799079 94.315998)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C13"
			(at -3.388161 -0.249061 0)
			(layer "B.SilkS")
		)
		(property "Value" "4.7uF/25V/0805"
			(at 0 -1.68 0)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "CAP 4.7UF 10% 25V 0805 X7R"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "DigikeyPN" "399-C0805C475K3RACTUCT-ND"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "TPN" "111-815-05"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MFGPN" "KEMET ELECTRONICS CORP  C0805C475K3RACTU"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/15Vaux/")
		(sheetfile "15Vaux.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.0375 0)
			(size 1.175 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.212766)
			(net 36 "/15Vaux/VP15P0")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.0375 0)
			(size 1.175 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.212766)
			(net 76 "/48V_RTN_M1")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1210_3225Metric_Pad1.33x2.70mm_HandSolder"
		(layer "B.Cu")
		(at 177.978355 169.387463 180)
		(descr "Capacitor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C70"
			(at 0 2.3 0)
			(layer "B.SilkS")
		)
		(property "Value" "22nF/1000V/1210"
			(at 0 -2.3 0)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "CAP, CERAMIC 0.022UF 5% 1KV NP0 1210"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MFGPN" "MURATA ELECTRONICS NO AMERICA  GRM32E5C3A223JWAAK "
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "DigikeyPN" "490-GRM32E5C3A223JWAAKCT-ND"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "TPN" "693-678-00"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/BankPower4/")
		(sheetfile "BankPower.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.5625 0 180)
			(size 1.325 2.7)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.188679)
			(net 76 "/48V_RTN_M1")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.5625 0 180)
			(size 1.325 2.7)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.188679)
			(net 51 "/BankPower4/VBU0P0")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1210_3225Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1206_3216Metric_Pad1.33x1.80mm_HandSolder"
		(layer "B.Cu")
		(at 154.556755 142.771833)
		(descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C83"
			(at 4.1148 0.11815 0)
			(layer "B.SilkS")
		)
		(property "Value" "0.1uF/200V/1206"
			(at 0 -1.85 0)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "CAP CER 0.1UF 10% 200V X7R 1206"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "DigikeyPN" "399-12986-1-ND"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "TPN" "693-921-00"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MFGPN" "KEMET ELECTRONICS CORP  C1206X104K2RACAUTO"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/BankPower3/")
		(sheetfile "BankPower.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.5625 0)
			(size 1.325 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.188679)
			(net 63 "/BankPower3/VBU96P0")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.5625 0)
			(size 1.325 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.188679)
			(net 61 "/BankPower3/VBU0P0")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1206_3216Metric_Pad1.33x1.80mm_HandSolder"
		(layer "B.Cu")
		(at 154.546555 145.108433)
		(descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C81"
			(at 3.9624 -0.03425 0)
			(layer "B.SilkS")
		)
		(property "Value" "0.1uF/200V/1206"
			(at 0 -1.85 0)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "CAP CER 0.1UF 10% 200V X7R 1206"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "DigikeyPN" "399-12986-1-ND"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "TPN" "693-921-00"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MFGPN" "KEMET ELECTRONICS CORP  C1206X104K2RACAUTO"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/BankPower3/")
		(sheetfile "BankPower.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.5625 0)
			(size 1.325 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.188679)
			(net 63 "/BankPower3/VBU96P0")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.5625 0)
			(size 1.325 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.188679)
			(net 61 "/BankPower3/VBU0P0")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1206_3216Metric_Pad1.33x1.80mm_HandSolder"
		(layer "B.Cu")
		(at 155.278355 127.106933 180)
		(descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C91"
			(at -3.9878 -0.1566 0)
			(layer "B.SilkS")
		)
		(property "Value" "10uF/35V/1206"
			(at 0 -1.85 0)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "CAP, 10UF 20% 35V X7R FLEX 1206"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "DigikeyPN" "445-172484-1-ND"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "TPN" "634-905-00"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MFGPN" "TDK CORP  CGA5L1X7R1V106M160AE"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/BankPower3/")
		(sheetfile "BankPower.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.5625 0 180)
			(size 1.325 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.188679)
			(net 61 "/BankPower3/VBU0P0")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.5625 0 180)
			(size 1.325 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.188679)
			(net 62 "/BankPower3/VBU24P0")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1206_3216Metric_Pad1.33x1.80mm_HandSolder"
		(layer "B.Cu")
		(at 155.860471 59.429048)
		(descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C45"
			(at 4.1148 0.11815 0)
			(layer "B.SilkS")
		)
		(property "Value" "0.1uF/200V/1206"
			(at 0 -1.85 0)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "CAP CER 0.1UF 10% 200V X7R 1206"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "DigikeyPN" "399-12986-1-ND"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "TPN" "693-921-00"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MFGPN" "KEMET ELECTRONICS CORP  C1206X104K2RACAUTO"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/BankPower1/")
		(sheetfile "BankPower.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.5625 0)
			(size 1.325 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.188679)
			(net 12 "/BankPower1/VBU96P0")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.5625 0)
			(size 1.325 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.188679)
			(net 14 "/BankPower1/VBU0P0")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1206_3216Metric_Pad1.33x1.80mm_HandSolder"
		(layer "B.Cu")
		(at 155.056098 90.865813 180)
		(descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C37"
			(at -4.6736 -0.2328 0)
			(layer "B.SilkS")
		)
		(property "Value" "10uF/35V/1206"
			(at 0 -1.85 0)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "CAP, 10UF 20% 35V X7R FLEX 1206"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "DigikeyPN" "445-172484-1-ND"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "TPN" "634-905-00"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MFGPN" "TDK CORP  CGA5L1X7R1V106M160AE"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/BankPower2/")
		(sheetfile "BankPower.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.5625 0 180)
			(size 1.325 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.188679)
			(net 55 "/BankPower2/VBU0P0")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.5625 0 180)
			(size 1.325 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.188679)
			(net 56 "/BankPower2/VBU24P0")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1206_3216Metric_Pad1.33x1.80mm_HandSolder"
		(layer "B.Cu")
		(at 154.556755 184.882813)
		(descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C65"
			(at 4.1148 0.11815 0)
			(layer "B.SilkS")
		)
		(property "Value" "0.1uF/200V/1206"
			(at 0 -1.85 0)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "CAP CER 0.1UF 10% 200V X7R 1206"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "DigikeyPN" "399-12986-1-ND"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "TPN" "693-921-00"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MFGPN" "KEMET ELECTRONICS CORP  C1206X104K2RACAUTO"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/BankPower4/")
		(sheetfile "BankPower.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.5625 0)
			(size 1.325 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.188679)
			(net 19 "/BankPower4/VBU96P0")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.5625 0)
			(size 1.325 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.188679)
			(net 51 "/BankPower4/VBU0P0")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1210_3225Metric_Pad1.33x2.70mm_HandSolder"
		(layer "B.Cu")
		(at 177.978355 184.641263 180)
		(descr "Capacitor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C59"
			(at 0 2.3 0)
			(layer "B.SilkS")
		)
		(property "Value" "22nF/1000V/1210"
			(at 0 -2.3 0)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "CAP, CERAMIC 0.022UF 5% 1KV NP0 1210"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MFGPN" "MURATA ELECTRONICS NO AMERICA  GRM32E5C3A223JWAAK "
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "DigikeyPN" "490-GRM32E5C3A223JWAAKCT-ND"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "TPN" "693-678-00"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/BankPower4/")
		(sheetfile "BankPower.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.5625 0 180)
			(size 1.325 2.7)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.188679)
			(net 76 "/48V_RTN_M1")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.5625 0 180)
			(size 1.325 2.7)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.188679)
			(net 19 "/BankPower4/VBU96P0")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1210_3225Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1206_3216Metric_Pad1.33x1.80mm_HandSolder"
		(layer "B.Cu")
		(at 155.274955 171.590713 180)
		(descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C73"
			(at -3.8608 0.0466 0)
			(layer "B.SilkS")
		)
		(property "Value" "10uF/35V/1206"
			(at 0 -1.85 0)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "CAP, 10UF 20% 35V X7R FLEX 1206"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "DigikeyPN" "445-172484-1-ND"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "TPN" "634-905-00"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MFGPN" "TDK CORP  CGA5L1X7R1V106M160AE"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/BankPower4/")
		(sheetfile "BankPower.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.5625 0 180)
			(size 1.325 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.188679)
			(net 51 "/BankPower4/VBU0P0")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.5625 0 180)
			(size 1.325 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.188679)
			(net 53 "/BankPower4/VBU24P0")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "B.Cu")
		(at 200.863083 146.097398 180)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C80"
			(at 0 1.68 0)
			(layer "B.SilkS")
		)
		(property "Value" "470nF/100V/0805"
			(at 0 -1.68 0)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "CAP CER 0.47UF 100V X7R 0805"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MFGPN" "08051C474KAZ2A"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "DigikeyPN" "478-KGF21KR72A474KUCT-ND"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "TPN" "111-169-03"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/BankPower3/")
		(sheetfile "BankPower.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.0375 0 180)
			(size 1.175 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.212766)
			(net 3 "/VFF48P0_M1")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.0375 0 180)
			(size 1.175 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.212766)
			(net 76 "/48V_RTN_M1")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_1206_3216Metric"
		(layer "B.Cu")
		(at 256.468847 120.67268 90)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R15"
			(at -0.11265 -2.199756 90)
			(layer "B.SilkS")
		)
		(property "Value" "100k"
			(at 0 -1.82 90)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "TPN" "654-510-00"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/48Vpower/")
		(sheetfile "48Vpower.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.4625 0 90)
			(size 1.125 1.75)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.222222)
			(net 2 "/48Vpower/VF48P0_BRD")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.4625 0 90)
			(size 1.125 1.75)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.222222)
			(net 77 "/48V_RTN")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1210_3225Metric_Pad1.33x2.70mm_HandSolder"
		(layer "B.Cu")
		(at 177.978355 142.530283 180)
		(descr "Capacitor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C77"
			(at 0 2.3 0)
			(layer "B.SilkS")
		)
		(property "Value" "22nF/1000V/1210"
			(at 0 -2.3 0)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "CAP, CERAMIC 0.022UF 5% 1KV NP0 1210"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MFGPN" "MURATA ELECTRONICS NO AMERICA  GRM32E5C3A223JWAAK "
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "DigikeyPN" "490-GRM32E5C3A223JWAAKCT-ND"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "TPN" "693-678-00"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/BankPower3/")
		(sheetfile "BankPower.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.5625 0 180)
			(size 1.325 2.7)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.188679)
			(net 76 "/48V_RTN_M1")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.5625 0 180)
			(size 1.325 2.7)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.188679)
			(net 63 "/BankPower3/VBU96P0")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1210_3225Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1206_3216Metric_Pad1.33x1.80mm_HandSolder"
		(layer "B.Cu")
		(at 174.7188 213.998792 90)
		(descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C7"
			(at 3.7846 -0.055 90)
			(layer "B.SilkS")
		)
		(property "Value" "10uF/35V/1206"
			(at 0 -1.85 90)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "CAP, 10UF 20% 35V X7R FLEX 1206"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "DigikeyPN" "445-172484-1-ND"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "TPN" "634-905-00"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MFGPN" "TDK CORP  CGA5L1X7R1V106M160AE"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/12Vpower/")
		(sheetfile "12Vpower.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.5625 0 90)
			(size 1.325 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.188679)
			(net 11 "/12Vpower/VBU12P6_11_21")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.5625 0 90)
			(size 1.325 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.188679)
			(net 6 "/12Vpower/VBU0P0_11_21")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "B.Cu")
		(at 215.3252 213.8475 90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C5"
			(at 0 1.68 270)
			(layer "B.SilkS")
		)
		(property "Value" "470nF/100V/0805"
			(at 0 -1.68 270)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "CAP CER 0.47UF 100V X7R 0805"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MFGPN" "08051C474KAZ2A"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "DigikeyPN" "478-KGF21KR72A474KUCT-ND"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "TPN" "111-169-03"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/12Vpower/")
		(sheetfile "12Vpower.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 270)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.0375 0 90)
			(size 1.175 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.212766)
			(net 5 "/12Vpower/VFFF48P0_PS11")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.0375 0 90)
			(size 1.175 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.212766)
			(net 1 "/12Vpower/48V_RTN_DISA")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1206_3216Metric_Pad1.33x1.80mm_HandSolder"
		(layer "B.Cu")
		(at 156.582071 43.764148 180)
		(descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C56"
			(at -3.9878 -0.1566 0)
			(layer "B.SilkS")
		)
		(property "Value" "10uF/35V/1206"
			(at 0 -1.85 0)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "CAP, 10UF 20% 35V X7R FLEX 1206"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "DigikeyPN" "445-172484-1-ND"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "TPN" "634-905-00"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MFGPN" "TDK CORP  CGA5L1X7R1V106M160AE"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/BankPower1/")
		(sheetfile "BankPower.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.5625 0 180)
			(size 1.325 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.188679)
			(net 14 "/BankPower1/VBU0P0")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.5625 0 180)
			(size 1.325 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.188679)
			(net 16 "/BankPower1/VBU24P0")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1206_3216Metric_Pad1.33x1.80mm_HandSolder"
		(layer "B.Cu")
		(at 155.052698 93.199863 180)
		(descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C40"
			(at -3.9878 -0.1566 0)
			(layer "B.SilkS")
		)
		(property "Value" "10uF/35V/1206"
			(at 0 -1.85 0)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "CAP, 10UF 20% 35V X7R FLEX 1206"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "DigikeyPN" "445-172484-1-ND"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "TPN" "634-905-00"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MFGPN" "TDK CORP  CGA5L1X7R1V106M160AE"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/BankPower2/")
		(sheetfile "BankPower.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.5625 0 180)
			(size 1.325 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.188679)
			(net 55 "/BankPower2/VBU0P0")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.5625 0 180)
			(size 1.325 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.188679)
			(net 56 "/BankPower2/VBU24P0")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "B.Cu")
		(at 134.053071 71.412698 180)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R10"
			(at 3.778384 -0.220202 180)
			(layer "B.SilkS")
		)
		(property "Value" "100k"
			(at 0 -1.65 180)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "DigiketPN" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "BenchPowerBoardNewCMchoke.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 180)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902)
			(net 83 "Net-(D10-K)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 180)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902)
			(net 15 "/VB0P0B1")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1206_3216Metric_Pad1.33x1.80mm_HandSolder"
		(layer "B.Cu")
		(at 150.252405 191.110863 -90)
		(descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C63"
			(at 4.064 0.16895 90)
			(layer "B.SilkS")
		)
		(property "Value" "0.1uF/200V/1206"
			(at 0 -1.85 90)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "CAP CER 0.1UF 10% 200V X7R 1206"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "DigikeyPN" "399-12986-1-ND"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "TPN" "693-921-00"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MFGPN" "KEMET ELECTRONICS CORP  C1206X104K2RACAUTO"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/BankPower4/")
		(sheetfile "BankPower.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 270)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.5625 0 270)
			(size 1.325 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.188679)
			(net 19 "/BankPower4/VBU96P0")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.5625 0 270)
			(size 1.325 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.188679)
			(net 51 "/BankPower4/VBU0P0")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1206_3216Metric_Pad1.33x1.80mm_HandSolder"
		(layer "B.Cu")
		(at 147.899605 148.990083 -90)
		(descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C86"
			(at 4.0386 0.11815 90)
			(layer "B.SilkS")
		)
		(property "Value" "0.1uF/200V/1206"
			(at 0 -1.85 90)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "CAP CER 0.1UF 10% 200V X7R 1206"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "DigikeyPN" "399-12986-1-ND"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "TPN" "693-921-00"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MFGPN" "KEMET ELECTRONICS CORP  C1206X104K2RACAUTO"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/BankPower3/")
		(sheetfile "BankPower.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.5625 0 270)
			(size 1.325 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.188679)
			(net 63 "/BankPower3/VBU96P0")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.5625 0 270)
			(size 1.325 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.188679)
			(net 61 "/BankPower3/VBU0P0")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "B.Cu")
		(at 134.324379 196.808709 180)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R4"
			(at 3.345242 0.115419 0)
			(layer "B.SilkS")
		)
		(property "Value" "100k"
			(at 0 -1.65 0)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "BenchPowerBoardNewCMchoke.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 180)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902)
			(net 67 "Net-(D7-K)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 180)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902)
			(net 26 "/VB0P0B4")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "B.Cu")
		(at 245.192113 213.087857 90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C21"
			(at 0 1.68 90)
			(layer "B.SilkS")
		)
		(property "Value" "10nF/100V"
			(at 0 -1.68 90)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MFGPN" "C0805C103K1RAC"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "DigikeyPN" "399-C0805C103K1RAC7025CT-ND"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "TPN" "111-123-04"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/48Vpower/")
		(sheetfile "48Vpower.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.0375 0 90)
			(size 1.175 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.212766)
			(net 9 "/12Vpower/VFF48P0_DISA")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.0375 0 90)
			(size 1.175 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.212766)
			(net 1 "/12Vpower/48V_RTN_DISA")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1206_3216Metric_Pad1.33x1.80mm_HandSolder"
		(layer "B.Cu")
		(at 147.899605 191.101063 -90)
		(descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C66"
			(at 4.0386 0.11815 90)
			(layer "B.SilkS")
		)
		(property "Value" "0.1uF/200V/1206"
			(at 0 -1.85 90)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "CAP CER 0.1UF 10% 200V X7R 1206"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "DigikeyPN" "399-12986-1-ND"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "TPN" "693-921-00"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MFGPN" "KEMET ELECTRONICS CORP  C1206X104K2RACAUTO"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/BankPower4/")
		(sheetfile "BankPower.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.5625 0 270)
			(size 1.325 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.188679)
			(net 19 "/BankPower4/VBU96P0")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.5625 0 270)
			(size 1.325 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.188679)
			(net 51 "/BankPower4/VBU0P0")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1206_3216Metric_Pad1.33x1.80mm_HandSolder"
		(layer "B.Cu")
		(at 149.203321 65.647298 -90)
		(descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C47"
			(at 4.0386 0.11815 90)
			(layer "B.SilkS")
		)
		(property "Value" "0.1uF/200V/1206"
			(at 0 -1.85 90)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "CAP CER 0.1UF 10% 200V X7R 1206"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "DigikeyPN" "399-12986-1-ND"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "TPN" "693-921-00"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MFGPN" "KEMET ELECTRONICS CORP  C1206X104K2RACAUTO"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/BankPower1/")
		(sheetfile "BankPower.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.5625 0 270)
			(size 1.325 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.188679)
			(net 12 "/BankPower1/VBU96P0")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.5625 0 270)
			(size 1.325 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.188679)
			(net 14 "/BankPower1/VBU0P0")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1210_3225Metric_Pad1.33x2.70mm_HandSolder"
		(layer "B.Cu")
		(at 179.282071 51.678698 180)
		(descr "Capacitor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C53"
			(at 0 2.3 0)
			(layer "B.SilkS")
		)
		(property "Value" "22nF/1000V/1210"
			(at 0 -2.3 0)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "CAP, CERAMIC 0.022UF 5% 1KV NP0 1210"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MFGPN" "MURATA ELECTRONICS NO AMERICA  GRM32E5C3A223JWAAK "
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "DigikeyPN" "490-GRM32E5C3A223JWAAKCT-ND"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "TPN" "693-678-00"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/BankPower1/")
		(sheetfile "BankPower.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.5625 0 180)
			(size 1.325 2.7)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.188679)
			(net 76 "/48V_RTN_M1")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.5625 0 180)
			(size 1.325 2.7)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.188679)
			(net 16 "/BankPower1/VBU24P0")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1210_3225Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1206_3216Metric_Pad1.33x1.80mm_HandSolder"
		(layer "B.Cu")
		(at 151.556121 65.657098 -90)
		(descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C50"
			(at 4.064 0.16895 90)
			(layer "B.SilkS")
		)
		(property "Value" "0.1uF/200V/1206"
			(at 0 -1.85 90)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "CAP CER 0.1UF 10% 200V X7R 1206"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "DigikeyPN" "399-12986-1-ND"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "TPN" "693-921-00"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MFGPN" "KEMET ELECTRONICS CORP  C1206X104K2RACAUTO"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/BankPower1/")
		(sheetfile "BankPower.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.5625 0 270)
			(size 1.325 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.188679)
			(net 12 "/BankPower1/VBU96P0")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.5625 0 270)
			(size 1.325 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.188679)
			(net 14 "/BankPower1/VBU0P0")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1210_3225Metric_Pad1.33x2.70mm_HandSolder"
		(layer "B.Cu")
		(at 177.756098 94.029813 180)
		(descr "Capacitor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C35"
			(at 0 2.3 0)
			(layer "B.SilkS")
		)
		(property "Value" "22nF/1000V/1210"
			(at 0 -2.3 0)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "CAP, CERAMIC 0.022UF 5% 1KV NP0 1210"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MFGPN" "MURATA ELECTRONICS NO AMERICA  GRM32E5C3A223JWAAK "
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "DigikeyPN" "490-GRM32E5C3A223JWAAKCT-ND"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "TPN" "693-678-00"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/BankPower2/")
		(sheetfile "BankPower.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.5625 0 180)
			(size 1.325 2.7)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.188679)
			(net 76 "/48V_RTN_M1")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.5625 0 180)
			(size 1.325 2.7)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.188679)
			(net 56 "/BankPower2/VBU24P0")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1210_3225Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1206_3216Metric_Pad1.33x1.80mm_HandSolder"
		(layer "B.Cu")
		(at 150.252405 148.999883 -90)
		(descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C84"
			(at 4.064 0.16895 90)
			(layer "B.SilkS")
		)
		(property "Value" "0.1uF/200V/1206"
			(at 0 -1.85 90)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "CAP CER 0.1UF 10% 200V X7R 1206"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "DigikeyPN" "399-12986-1-ND"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "TPN" "693-921-00"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MFGPN" "KEMET ELECTRONICS CORP  C1206X104K2RACAUTO"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/BankPower3/")
		(sheetfile "BankPower.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 270)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.5625 0 270)
			(size 1.325 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.188679)
			(net 63 "/BankPower3/VBU96P0")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.5625 0 270)
			(size 1.325 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.188679)
			(net 61 "/BankPower3/VBU0P0")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "B.Cu")
		(at 135.330646 113.765295 180)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R8"
			(at 3.048 -0.001 0)
			(layer "B.SilkS")
		)
		(property "Value" "100k"
			(at 0 -1.65 0)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "BenchPowerBoardNewCMchoke.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 180)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902)
			(net 68 "Net-(D9-K)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 180)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902)
			(net 52 "/VB0P0B2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "B.Cu")
		(at 135.240355 184.714263 180)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R23"
			(at 0 1.65 0)
			(layer "B.SilkS")
		)
		(property "Value" "75k"
			(at 0 -1.65 0)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/BankPower4/")
		(sheetfile "BankPower.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 180)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902)
			(net 25 "/VB96P0B4")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 180)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902)
			(net 78 "Net-(C60-Pad2)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1206_3216Metric_Pad1.33x1.80mm_HandSolder"
		(layer "B.Cu")
		(at 155.278355 169.217913 180)
		(descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C74"
			(at -3.9878 -0.1566 0)
			(layer "B.SilkS")
		)
		(property "Value" "10uF/35V/1206"
			(at 0 -1.85 0)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "CAP, 10UF 20% 35V X7R FLEX 1206"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "DigikeyPN" "445-172484-1-ND"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "TPN" "634-905-00"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MFGPN" "TDK CORP  CGA5L1X7R1V106M160AE"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/BankPower4/")
		(sheetfile "BankPower.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.5625 0 180)
			(size 1.325 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.188679)
			(net 51 "/BankPower4/VBU0P0")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.5625 0 180)
			(size 1.325 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.188679)
			(net 53 "/BankPower4/VBU24P0")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1206_3216Metric_Pad1.33x1.80mm_HandSolder"
		(layer "B.Cu")
		(at 177.16895 213.980992 90)
		(descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C6"
			(at 3.7592 -0.1566 90)
			(layer "B.SilkS")
		)
		(property "Value" "10uF/35V/1206"
			(at 0 -1.85 90)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "CAP, 10UF 20% 35V X7R FLEX 1206"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "DigikeyPN" "445-172484-1-ND"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "TPN" "634-905-00"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MFGPN" "TDK CORP  CGA5L1X7R1V106M160AE"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/12Vpower/")
		(sheetfile "12Vpower.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.5625 0 90)
			(size 1.325 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.188679)
			(net 11 "/12Vpower/VBU12P6_11_21")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.5625 0 90)
			(size 1.325 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.188679)
			(net 6 "/12Vpower/VBU0P0_11_21")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1206_3216Metric_Pad1.33x1.80mm_HandSolder"
		(layer "B.Cu")
		(at 155.056098 86.115263 180)
		(descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C39"
			(at -3.9878 -0.1566 0)
			(layer "B.SilkS")
		)
		(property "Value" "10uF/35V/1206"
			(at 0 -1.85 0)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "CAP, 10UF 20% 35V X7R FLEX 1206"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MFGPN" "TDK CORP  CGA5L1X7R1V106M160AE"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "DigikeyPN" "445-172484-1-ND"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "TPN" "634-905-00"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/BankPower2/")
		(sheetfile "BankPower.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.5625 0 180)
			(size 1.325 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.188679)
			(net 55 "/BankPower2/VBU0P0")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.5625 0 180)
			(size 1.325 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.188679)
			(net 56 "/BankPower2/VBU24P0")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1206_3216Metric_Pad1.33x1.80mm_HandSolder"
		(layer "B.Cu")
		(at 155.274955 176.302513 180)
		(descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C75"
			(at -3.9878 -0.1566 0)
			(layer "B.SilkS")
		)
		(property "Value" "10uF/35V/1206"
			(at 0 -1.85 0)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "CAP, 10UF 20% 35V X7R FLEX 1206"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "DigikeyPN" "445-172484-1-ND"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "TPN" "634-905-00"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MFGPN" "TDK CORP  CGA5L1X7R1V106M160AE"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/BankPower4/")
		(sheetfile "BankPower.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.5625 0 180)
			(size 1.325 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.188679)
			(net 51 "/BankPower4/VBU0P0")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.5625 0 180)
			(size 1.325 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.188679)
			(net 53 "/BankPower4/VBU24P0")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder"
		(layer "B.Cu")
		(at 253.839909 184.443612)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C20"
			(at 3.668533 0.523527 0)
			(layer "B.SilkS")
		)
		(property "Value" "10nF/100V"
			(at 0 -1.68 0)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "TPN" "111-123-04"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MFGPN" "C0805C103K1RAC"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "DigikeyPN" "399-C0805C103K1RAC7025CT-ND"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/48Vpower/")
		(sheetfile "48Vpower.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.0375 0)
			(size 1.175 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.212766)
			(net 4 "/48Vpower/VF48P0_DISA")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.0375 0)
			(size 1.175 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.212766)
			(net 77 "/48V_RTN")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "B.Cu")
		(at 228.04883 137.064594 180)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R32"
			(at 0 1.43 0)
			(layer "B.SilkS")
		)
		(property "Value" "1k"
			(at 0 -1.43 0)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "TPN" "636-700-00"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/BankPower3/")
		(sheetfile "BankPower.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 180)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 76 "/48V_RTN_M1")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0 180)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 72 "/BankPower3/ENABLE")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(gr_line
		(start 60.8084 30.999512)
		(end 269.571 30.999512)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 59.792789 32.004729)
		(end 60.808453 30.998831)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 269.571 230.383911)
		(end 270.587 229.367911)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 270.587 229.367911)
		(end 270.51 32.004)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 59.7924 229.367911)
		(end 60.8084 230.383911)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 269.571 30.999512)
		(end 270.51 32.004)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 60.8084 230.383911)
		(end 269.571 230.383911)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 59.7924 229.367911)
		(end 59.7924 32.004)
		(layer "Edge.Cuts")
	)
	(gr_text "Bench Power Board"
		(at 69.50709 148.524671 90)
		(layer "F.SilkS")
	)
	(gr_text "B2G"
		(at 85.384378 189.819921 0)
		(layer "F.SilkS")
	)
	(gr_text "B4-"
		(at 102.622682 195.451481 0)
		(layer "F.SilkS")
	)
	(gr_text "MF, KMc 11/2025"
		(at 114.744604 47.84193 0)
		(layer "F.SilkS")
	)
	(gr_text "B1+"
		(at 64.14026 188.266627 0)
		(layer "F.SilkS")
	)
	(gr_text "B3-"
		(at 92.602113 195.885565 0)
		(layer "F.SilkS")
	)
	(gr_text "B2+"
		(at 77.194892 186.237259 0)
		(layer "F.SilkS")
	)
	(gr_text "ON\n\n\nOFF"
		(at 230.595314 49.208958 0)
		(layer "F.SilkS")
	)
	(gr_text "B4G"
		(at 107.202273 182.564658 0)
		(layer "F.SilkS")
	)
	(gr_text "B3+"
		(at 91.497989 182.812211 0)
		(layer "F.SilkS")
	)
	(gr_text "B3G"
		(at 97.319805 189.565415 0)
		(layer "F.SilkS")
	)
	(gr_text "B1G"
		(at 71.848518 192.28634 0)
		(layer "F.SilkS")
	)
	(gr_text "ON\n\n\nOFF"
		(at 229.09298 138.491142 0)
		(layer "F.SilkS")
	)
	(gr_text "B4+"
		(at 110.169466 195.928446 0)
		(layer "F.SilkS")
	)
	(gr_text "ON\n\n\nOFF"
		(at 229.526873 91.777255 0)
		(layer "F.SilkS")
	)
	(gr_text "ON\n\n\nOFF"
		(at 236.786213 203.180186 0)
		(layer "F.SilkS")
	)
	(gr_text "B1-"
		(at 60.823244 195.508853 0)
		(layer "F.SilkS")
	)
	(gr_text "ON\n\n\nOFF"
		(at 229.211248 174.736336 0)
		(layer "F.SilkS")
	)
	(gr_text "B2-"
		(at 77.424085 195.349547 0)
		(layer "F.SilkS")
	)
	(zone
		(net 25)
		(net_name "/VB96P0B4")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 27)
		(connect_pads yes
			(clearance 0.508)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 110.309363 196.290913) (xy 115.357473 196.284235) (xy 115.364066 198.176603) (xy 110.309363 198.18328)
			)
		)
	)
	(zone
		(net 17)
		(net_name "/VB24N0B1")
		(layer "F.Cu")
		(hatch edge 0.508)
		(priority 20)
		(connect_pads thru_hole_only
			(clearance 0.508)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.254)
			(thermal_bridge_width 0.762)
		)
		(polygon
			(pts
				(xy 60.884165 195.681601) (xy 65.804111 195.655637) (xy 65.804111 197.6093) (xy 60.898338 197.6093)
			)
		)
	)
	(zone
		(net 28)
		(net_name "/VB24N0B4")
		(layer "F.Cu")
		(hatch edge 0.508)
		(priority 4)
		(connect_pads thru_hole_only
			(clearance 0.508)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.254)
			(thermal_bridge_width 0.762)
			(smoothing fillet)
			(radius 0.508)
		)
		(polygon
			(pts
				(xy 123.062155 163.714063) (xy 129.107355 163.688663) (xy 133.812481 166.095937) (xy 133.850937 171.05678)
				(xy 123.10475 171.08299)
			)
		)
	)
	(zone
		(net 59)
		(net_name "/VB0P0B3")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 51)
		(connect_pads yes
			(clearance 0.508)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 96.619912 189.982491) (xy 101.546535 189.975974) (xy 101.553212 191.892387) (xy 96.619912 191.898904)
			)
		)
	)
	(zone
		(net 54)
		(net_name "/VB24N0B2")
		(layer "F.Cu")
		(hatch edge 0.508)
		(priority 4)
		(connect_pads thru_hole_only
			(clearance 0.508)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.254)
			(thermal_bridge_width 0.762)
			(smoothing fillet)
			(radius 0.508)
		)
		(polygon
			(pts
				(xy 122.839898 80.611413) (xy 128.885098 80.586013) (xy 133.590224 82.993287) (xy 133.62868 87.95413)
				(xy 122.882493 87.98034)
			)
		)
	)
	(zone
		(net 38)
		(net_name "Net-(J1-VB24N0_FB3)")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 51)
		(connect_pads yes
			(clearance 0.508)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 91.929835 198.497582) (xy 96.957913 198.507598) (xy 96.957913 200.337203) (xy 91.915156 200.347229)
			)
		)
	)
	(zone
		(net 28)
		(net_name "/VB24N0B4")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 26)
		(connect_pads yes
			(clearance 0.508)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 102.061112 195.720939) (xy 107.107766 195.714263) (xy 107.115743 198.003875) (xy 102.061112 198.010551)
			)
		)
	)
	(zone
		(net 26)
		(net_name "/VB0P0B4")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 26)
		(connect_pads yes
			(clearance 0.508)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 106.957102 183.242449) (xy 112.005212 183.235771) (xy 112.011889 185.152184) (xy 106.957102 185.158861)
			)
		)
	)
	(zone
		(net 9)
		(net_name "/12Vpower/VFF48P0_DISA")
		(layer "F.Cu")
		(hatch edge 0.508)
		(priority 35)
		(connect_pads thru_hole_only
			(clearance 0.508)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.254)
			(thermal_bridge_width 0.762)
			(smoothing fillet)
			(radius 2.54)
		)
		(polygon
			(pts
				(xy 237.471094 214.900236) (xy 247.339746 214.900236) (xy 247.339746 221.947624) (xy 242.545394 226.741976)
				(xy 237.43019 226.741976)
			)
		)
	)
	(zone
		(net 45)
		(net_name "Net-(J1-VB96P0_FB3)")
		(layer "F.Cu")
		(hatch edge 0.508)
		(priority 26)
		(connect_pads thru_hole_only
			(clearance 0.508)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.254)
			(thermal_bridge_width 0.762)
		)
		(polygon
			(pts
				(xy 96.152095 187.840106) (xy 91.105374 187.846782) (xy 91.097308 185.531741) (xy 96.152095 185.525064)
			)
		)
	)
	(zone
		(net 44)
		(net_name "Net-(J1-VB96P0_FB2)")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 26)
		(connect_pads yes
			(clearance 0.508)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 81.437901 191.25422) (xy 76.391096 191.260896) (xy 76.383445 189.064795) (xy 81.437901 189.058118)
			)
		)
	)
	(zone
		(net 43)
		(net_name "Net-(J1-LF_FB3)")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 51)
		(connect_pads yes
			(clearance 0.508)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 96.561321 192.311498) (xy 101.536519 192.321409) (xy 101.536519 193.880858) (xy 96.548788 193.890774)
			)
		)
	)
	(zone
		(net 49)
		(net_name "Net-(J1-LF_FB2)")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 27)
		(connect_pads yes
			(clearance 0.508)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 84.968323 192.776218) (xy 89.988279 192.786218) (xy 89.988279 194.996955) (xy 84.95062 195.00697)
			)
		)
	)
	(zone
		(net 39)
		(net_name "Net-(J1-LF_FB4)")
		(layer "F.Cu")
		(hatch edge 0.508)
		(priority 27)
		(connect_pads thru_hole_only
			(clearance 0.508)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.254)
			(thermal_bridge_width 0.762)
		)
		(polygon
			(pts
				(xy 106.967118 185.57119) (xy 111.995196 185.581206) (xy 111.995196 187.685012) (xy 106.950262 187.695042)
			)
		)
	)
	(zone
		(net 40)
		(net_name "Net-(J1-VB96P0_FB1)")
		(layer "F.Cu")
		(hatch edge 0.508)
		(priority 20)
		(connect_pads yes
			(clearance 0.508)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.254)
			(thermal_bridge_width 0.762)
		)
		(polygon
			(pts
				(xy 63.690677 191.436863) (xy 68.725149 191.458036) (xy 68.725149 192.957027) (xy 63.696908 192.963257)
			)
		)
	)
	(zone
		(net 42)
		(net_name "Net-(J1-LF_FB1)")
		(layer "F.Cu")
		(hatch edge 0.508)
		(priority 23)
		(connect_pads yes
			(clearance 0.508)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.254)
			(thermal_bridge_width 0.762)
		)
		(polygon
			(pts
				(xy 71.880337 194.637151) (xy 76.118258 194.641718) (xy 76.118258 196.37519) (xy 71.872523 196.37976)
			)
		)
	)
	(zone
		(net 48)
		(net_name "Net-(J1-VB24N0_FB4)")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 26)
		(connect_pads yes
			(clearance 0.508)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 102.059182 198.317532) (xy 107.099206 198.313652) (xy 107.099206 200.49001) (xy 102.060046 200.496115)
			)
		)
	)
	(zone
		(net 50)
		(net_name "/VB96P0B2")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 26)
		(connect_pads yes
			(clearance 0.508)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 81.427057 188.655328) (xy 76.399807 188.645313) (xy 76.399807 186.571147) (xy 81.443677 186.56112)
			)
		)
	)
	(zone
		(net 13)
		(net_name "/VB96P0B1")
		(layer "F.Cu")
		(hatch edge 0.508)
		(priority 19)
		(connect_pads thru_hole_only
			(clearance 0.508)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.254)
			(thermal_bridge_width 0.762)
		)
		(polygon
			(pts
				(xy 63.860936 188.98154) (xy 68.795238 188.98154) (xy 68.804583 191.028154) (xy 63.870282 191.037499)
			)
		)
	)
	(zone
		(net 41)
		(net_name "Net-(J1-VB24N0_FB1)")
		(layer "F.Cu")
		(hatch edge 0.508)
		(priority 20)
		(connect_pads thru_hole_only
			(clearance 0.508)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.254)
			(thermal_bridge_width 0.762)
		)
		(polygon
			(pts
				(xy 60.903587 198.069295) (xy 65.815565 198.065442) (xy 65.822063 200.215799) (xy 60.903587 200.223507)
			)
		)
	)
	(zone
		(net 17)
		(net_name "/VB24N0B1")
		(layer "F.Cu")
		(hatch edge 0.508)
		(priority 4)
		(connect_pads thru_hole_only
			(clearance 0.508)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.254)
			(thermal_bridge_width 0.762)
			(smoothing fillet)
			(radius 0.508)
		)
		(polygon
			(pts
				(xy 124.365871 38.260298) (xy 130.411071 38.234898) (xy 135.116197 40.642172) (xy 135.154653 45.603015)
				(xy 124.408466 45.629225)
			)
		)
	)
	(zone
		(net 58)
		(net_name "/VB96P0B3")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 27)
		(connect_pads yes
			(clearance 0.508)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 96.142079 185.112735) (xy 91.114001 185.102719) (xy 91.114001 183.05425) (xy 96.158496 183.04422)
			)
		)
	)
	(zone
		(net 15)
		(net_name "/VB0P0B1")
		(layer "F.Cu")
		(hatch edge 0.508)
		(priority 24)
		(connect_pads yes
			(clearance 0.508)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.254)
			(thermal_bridge_width 0.762)
		)
		(polygon
			(pts
				(xy 71.890572 194.165585) (xy 76.157197 194.187466) (xy 76.157197 192.432674) (xy 71.890572 192.454555)
			)
		)
	)
	(zone
		(net 6)
		(net_name "/12Vpower/VBU0P0_11_21")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 47)
		(connect_pads thru_hole_only
			(clearance 0.508)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.254)
			(thermal_bridge_width 0.762)
			(smoothing fillet)
			(radius 1.27)
		)
		(polygon
			(pts
				(xy 157.161828 220.022005) (xy 162.9774 220.022005) (xy 163.122865 219.87654) (xy 163.122865 213.104949)
				(xy 165.624384 210.60343) (xy 173.973143 210.60343) (xy 173.973143 205.19474) (xy 171.742058 202.963655)
				(xy 163.258083 202.963655) (xy 157.173307 209.048431) (xy 157.11606 209.048431) (xy 157.11606 219.976237)
			)
		)
	)
	(zone
		(net 11)
		(net_name "/12Vpower/VBU12P6_11_21")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 46)
		(connect_pads thru_hole_only
			(clearance 0.508)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.254)
			(thermal_bridge_width 0.762)
			(smoothing fillet)
			(radius 1.27)
		)
		(polygon
			(pts
				(xy 157.201839 220.686418) (xy 163.991991 220.686418) (xy 166.696399 217.98201) (xy 166.696399 217.835674)
				(xy 173.840376 217.835674) (xy 173.953057 217.948355) (xy 173.953057 227.0195) (xy 173.689957 227.2826)
				(xy 157.208656 227.2826) (xy 157.201839 227.275783)
			)
		)
	)
	(zone
		(net 54)
		(net_name "/VB24N0B2")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 26)
		(connect_pads yes
			(clearance 0.508)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 77.215778 195.518871) (xy 82.262593 195.512195) (xy 82.270565 197.800212) (xy 77.215778 197.806889)
			)
		)
	)
	(zone
		(net 3)
		(net_name "/VFF48P0_M1")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 32)
		(connect_pads thru_hole_only
			(clearance 0.508)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.254)
			(thermal_bridge_width 0.508)
			(smoothing fillet)
			(radius 1.27)
		)
		(polygon
			(pts
				(xy 261.804779 112.844108) (xy 251.903111 112.883844) (xy 249.248999 117.272055) (xy 249.307244 128.074469)
				(xy 238.06102 128.074469) (xy 232.350475 120.957221) (xy 228.371634 120.937325) (xy 228.371634 115.517941)
				(xy 228.30772 109.669876) (xy 255.816588 109.657848) (xy 258.338155 107.289388) (xy 258.338155 101.160587)
				(xy 258.328701 101.151133) (xy 258.328701 92.365785) (xy 261.682049 92.365785)
			)
		)
	)
	(zone
		(net 47)
		(net_name "Net-(J1-VB96P0_FB4)")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 27)
		(connect_pads yes
			(clearance 0.508)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 110.320422 198.488258) (xy 115.347457 198.498272) (xy 115.347457 200.813852) (xy 110.301886 200.823883)
			)
		)
	)
	(zone
		(net 52)
		(net_name "/VB0P0B2")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 51)
		(connect_pads yes
			(clearance 0.508)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 84.950185 190.080334) (xy 89.997016 190.073658) (xy 90.004972 192.357196) (xy 84.950185 192.363873)
			)
		)
	)
	(zone
		(net 46)
		(net_name "Net-(J1-VB24N0_FB2)")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 27)
		(connect_pads yes
			(clearance 0.508)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 77.225794 198.219218) (xy 82.253872 198.229234) (xy 82.253872 199.916508) (xy 77.212244 199.926531)
			)
		)
	)
	(zone
		(net 36)
		(net_name "/15Vaux/VP15P0")
		(layer "F.Cu")
		(hatch edge 0.508)
		(priority 33)
		(connect_pads thru_hole_only
			(clearance 0.508)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.254)
			(thermal_bridge_width 0.762)
			(smoothing chamfer)
			(radius 0.508)
		)
		(polygon
			(pts
				(xy 255.474618 96.5804) (xy 255.490212 91.892928) (xy 248.016003 91.863992) (xy 245.853119 91.844807)
				(xy 245.855887 108.251358) (xy 252.492627 108.231841) (xy 252.500207 103.169101) (xy 255.211397 100.862515)
			)
		)
	)
	(zone
		(net 60)
		(net_name "/VB24N0B3")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 51)
		(connect_pads yes
			(clearance 0.508)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 91.919819 196.168841) (xy 96.967929 196.162163) (xy 96.974606 198.078576) (xy 91.919819 198.085253)
			)
		)
	)
	(zone
		(net 3)
		(net_name "/VFF48P0_M1")
		(layers "F.Cu" "B.Cu")
		(hatch edge 0.508)
		(priority 10)
		(connect_pads thru_hole_only
			(clearance 0.508)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.254)
			(thermal_bridge_width 0.762)
			(smoothing fillet)
			(radius 0.254)
		)
		(polygon
			(pts
				(xy 201.203676 140.76628) (xy 223.110452 140.796748) (xy 223.110452 149.781083) (xy 201.175852 149.781083)
			)
		)
	)
	(zone
		(net 3)
		(net_name "/VFF48P0_M1")
		(layers "F.Cu" "B.Cu")
		(hatch edge 0.508)
		(priority 10)
		(connect_pads thru_hole_only
			(clearance 0.508)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.254)
			(thermal_bridge_width 0.762)
			(smoothing fillet)
			(radius 0.254)
		)
		(polygon
			(pts
				(xy 200.981419 99.77461) (xy 222.765323 99.804908) (xy 222.765323 108.789413) (xy 200.953595 108.789413)
			)
		)
	)
	(zone
		(net 52)
		(net_name "/VB0P0B2")
		(layers "F.Cu" "B.Cu")
		(hatch edge 0.508)
		(priority 3)
		(connect_pads thru_hole_only
			(clearance 0.508)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.254)
			(thermal_bridge_width 0.762)
			(smoothing fillet)
			(radius 0.508)
		)
		(polygon
			(pts
				(xy 113.375499 90.186228) (xy 113.291457 109.140499) (xy 120.124057 109.140499) (xy 120.124057 93.189299)
				(xy 135.922857 93.189299) (xy 135.955857 82.810099) (xy 133.916257 82.810099) (xy 133.820128 90.232198)
			)
		)
	)
	(zone
		(net 58)
		(net_name "/VB96P0B3")
		(layers "F.Cu" "B.Cu")
		(hatch edge 0.508)
		(priority 7)
		(connect_pads thru_hole_only
			(clearance 0.508)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.254)
			(thermal_bridge_width 0.762)
			(smoothing fillet)
			(radius 0.508)
		)
		(polygon
			(pts
				(xy 136.582555 123.847683) (xy 142.043555 123.847683) (xy 142.043555 149.196883) (xy 136.582555 149.196883)
			)
		)
	)
	(zone
		(net 59)
		(net_name "/VB0P0B3")
		(layers "F.Cu" "B.Cu")
		(hatch edge 0.508)
		(priority 3)
		(connect_pads thru_hole_only
			(clearance 0.508)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.254)
			(thermal_bridge_width 0.762)
			(smoothing fillet)
			(radius 0.508)
		)
		(polygon
			(pts
				(xy 113.56407 119.146283) (xy 113.56407 149.601127) (xy 120.39667 149.601127) (xy 120.39667 134.15861)
				(xy 136.19547 134.15861) (xy 136.22847 123.77941) (xy 134.18887 123.77941) (xy 134.11267 129.66281)
				(xy 120.39667 129.68821) (xy 120.39667 119.14721)
			)
		)
	)
	(zone
		(net 3)
		(net_name "/VFF48P0_M1")
		(layers "F.Cu" "B.Cu")
		(hatch edge 0.508)
		(priority 10)
		(connect_pads thru_hole_only
			(clearance 0.508)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.254)
			(thermal_bridge_width 0.762)
			(smoothing fillet)
			(radius 0.254)
		)
		(polygon
			(pts
				(xy 202.507392 57.423495) (xy 224.421939 57.453973) (xy 224.421939 66.438298) (xy 202.479568 66.438298)
			)
		)
	)
	(zone
		(net 15)
		(net_name "/VB0P0B1")
		(layers "F.Cu" "B.Cu")
		(hatch edge 0.508)
		(priority 3)
		(connect_pads thru_hole_only
			(clearance 0.508)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.254)
			(thermal_bridge_width 0.762)
			(smoothing fillet)
			(radius 0.508)
		)
		(polygon
			(pts
				(xy 114.8726 49.190608) (xy 114.840871 66.835298) (xy 121.673471 66.835298) (xy 121.673471 51.461508)
				(xy 137.470435 51.461508) (xy 137.505271 40.504898) (xy 135.465671 40.504898) (xy 135.354254 49.107471)
			)
		)
	)
	(zone
		(net 50)
		(net_name "/VB96P0B2")
		(layers "F.Cu" "B.Cu")
		(hatch edge 0.508)
		(priority 7)
		(connect_pads thru_hole_only
			(clearance 0.508)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.254)
			(thermal_bridge_width 0.762)
			(smoothing fillet)
			(radius 0.508)
		)
		(polygon
			(pts
				(xy 136.360298 82.856013) (xy 141.821298 82.856013) (xy 141.821298 108.205213) (xy 136.360298 108.205213)
			)
		)
	)
	(zone
		(net 3)
		(net_name "/VFF48P0_M1")
		(layers "F.Cu" "B.Cu")
		(hatch edge 0.508)
		(priority 10)
		(connect_pads thru_hole_only
			(clearance 0.508)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.254)
			(thermal_bridge_width 0.762)
			(smoothing fillet)
			(radius 0.254)
		)
		(polygon
			(pts
				(xy 201.203676 182.87726) (xy 223.041426 182.907632) (xy 223.041426 191.892063) (xy 201.175852 191.892063)
			)
		)
	)
	(zone
		(net 13)
		(net_name "/VB96P0B1")
		(layers "F.Cu" "B.Cu")
		(hatch edge 0.508)
		(priority 7)
		(connect_pads thru_hole_only
			(clearance 0.508)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.254)
			(thermal_bridge_width 0.762)
			(smoothing fillet)
			(radius 0.508)
		)
		(polygon
			(pts
				(xy 137.886271 40.504898) (xy 143.347271 40.504898) (xy 143.347271 65.854098) (xy 137.886271 65.854098)
			)
		)
	)
	(zone
		(net 25)
		(net_name "/VB96P0B4")
		(layers "F.Cu" "B.Cu")
		(hatch edge 0.508)
		(priority 7)
		(connect_pads thru_hole_only
			(clearance 0.508)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.254)
			(thermal_bridge_width 0.762)
			(smoothing fillet)
			(radius 0.508)
		)
		(polygon
			(pts
				(xy 136.582555 165.958663) (xy 142.043555 165.958663) (xy 142.043555 191.307863) (xy 136.582555 191.307863)
			)
		)
	)
	(zone
		(net 45)
		(net_name "Net-(J1-VB96P0_FB3)")
		(layers "F.Cu" "B.Cu" "In1.Cu")
		(hatch edge 0.508)
		(priority 50)
		(connect_pads thru_hole_only
			(clearance 0.381)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.127)
			(thermal_bridge_width 0.762)
			(smoothing fillet)
			(radius 1.016)
		)
		(polygon
			(pts
				(xy 89.958397 185.525064) (xy 89.958397 189.512356) (xy 90.262274 190.991012) (xy 90.257067 195.304079)
				(xy 90.241066 197.217396) (xy 90.237126 198.374074) (xy 90.204774 207.87199) (xy 91.718734 209.38595)
				(xy 94.826217 209.332948) (xy 100.118661 204.040504) (xy 100.118661 197.062292) (xy 98.409473 194.301204)
				(xy 98.409473 185.529924) (xy 98.410943 185.528454) (xy 98.407553 185.525064)
			)
		)
	)
	(zone
		(net 2)
		(net_name "/48Vpower/VF48P0_BRD")
		(layers "F.Cu" "B.Cu" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu")
		(hatch edge 0.508)
		(priority 38)
		(connect_pads thru_hole_only
			(clearance 0.508)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.254)
			(thermal_bridge_width 0.762)
			(smoothing chamfer)
			(radius 0.762)
		)
		(polygon
			(pts
				(xy 254.153962 120.983174) (xy 260.051867 120.983174) (xy 262.324788 123.256095) (xy 262.324788 143.15196)
				(xy 254.086685 143.15196)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layers "F.Cu" "B.Cu" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu")
		(name "thieving")
		(hatch edge 0.508)
		(connect_pads no
			(clearance 5.08)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(fill yes
			(mode hatch)
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 9.999999)
			(hatch_thickness 0.508)
			(hatch_gap 5.08)
			(hatch_orientation 0)
			(hatch_smoothing_level 3)
			(hatch_smoothing_value 1)
			(hatch_border_algorithm hatch_thickness)
			(hatch_min_hole_area 0.3)
		)
		(polygon
			(pts
				(xy 277.999677 27.572626) (xy 277.999677 231.655233) (xy 51.292628 233.046075) (xy 50.950905 27.572626)
			)
		)
	)
	(zone
		(net 37)
		(net_name "Net-(C42-Pad2)")
		(layers "F.Cu" "B.Cu" "In2.Cu")
		(hatch edge 0.508)
		(priority 5)
		(connect_pads thru_hole_only
			(clearance 0.508)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.254)
			(thermal_bridge_width 0.762)
			(smoothing fillet)
			(radius 0.508)
		)
		(polygon
			(pts
				(xy 122.773271 52.138098) (xy 136.743271 52.138098) (xy 136.743271 66.362098) (xy 122.773271 66.362098)
			)
		)
	)
	(zone
		(net 10)
		(net_name "Net-(C24-Pad2)")
		(layers "F.Cu" "B.Cu" "In2.Cu")
		(hatch edge 0.508)
		(priority 5)
		(connect_pads thru_hole_only
			(clearance 0.508)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.254)
			(thermal_bridge_width 0.762)
			(smoothing fillet)
			(radius 0.508)
		)
		(polygon
			(pts
				(xy 121.247298 94.489213) (xy 135.217298 94.489213) (xy 135.217298 108.713213) (xy 121.247298 108.713213)
			)
		)
	)
	(zone
		(net 78)
		(net_name "Net-(C60-Pad2)")
		(layers "F.Cu" "B.Cu" "In2.Cu")
		(hatch edge 0.508)
		(priority 5)
		(connect_pads thru_hole_only
			(clearance 0.508)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.254)
			(thermal_bridge_width 0.762)
			(smoothing fillet)
			(radius 0.508)
		)
		(polygon
			(pts
				(xy 121.469555 177.591863) (xy 135.439555 177.591863) (xy 135.439555 191.905959) (xy 121.469555 191.905959)
			)
		)
	)
	(zone
		(net 79)
		(net_name "Net-(C78-Pad2)")
		(layers "F.Cu" "B.Cu" "In2.Cu")
		(hatch edge 0.508)
		(priority 5)
		(connect_pads thru_hole_only
			(clearance 0.508)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.254)
			(thermal_bridge_width 0.762)
			(smoothing fillet)
			(radius 0.508)
		)
		(polygon
			(pts
				(xy 121.469555 135.480883) (xy 135.439555 135.480883) (xy 135.439555 149.704883) (xy 121.469555 149.704883)
			)
		)
	)
	(zone
		(net 8)
		(net_name "/VB0P0_GD")
		(layers "F.Cu" "B.Cu" "In4.Cu")
		(hatch edge 0.508)
		(priority 30)
		(connect_pads thru_hole_only
			(clearance 0.508)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.127)
			(thermal_bridge_width 0.762)
			(smoothing fillet)
			(radius 1.27)
		)
		(polygon
			(pts
				(xy 110.48834 211.57966) (xy 156.008646 211.61296) (xy 156.050618 220.049438) (xy 110.530228 220.082738)
			)
		)
	)
	(zone
		(net 13)
		(net_name "/VB96P0B1")
		(layers "F.Cu" "In1.Cu")
		(hatch edge 0.508)
		(priority 2)
		(connect_pads thru_hole_only
			(clearance 0.508)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.254)
			(thermal_bridge_width 0.762)
			(smoothing fillet)
			(radius 2.54)
		)
		(polygon
			(pts
				(xy 143.906871 52.373204) (xy 138.296712 52.3394) (xy 138.262909 62.450125) (xy 68.192258 62.489692)
				(xy 53.115539 72.467721) (xy 53.048376 190.936928) (xy 71.323283 190.926527) (xy 71.323271 82.398585)
				(xy 82.790546 73.943768) (xy 143.971782 73.943009)
			)
		)
	)
	(zone
		(net 7)
		(net_name "/VB12P6_GD")
		(layers "F.Cu" "In1.Cu")
		(hatch edge 0.508)
		(priority 31)
		(connect_pads thru_hole_only
			(clearance 0.508)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.254)
			(thermal_bridge_width 0.762)
			(smoothing chamfer)
			(radius 0.508)
		)
		(polygon
			(pts
				(xy 123.874086 217.437229) (xy 123.874086 228.3073) (xy 156.180201 228.342762) (xy 156.180201 220.736792)
				(xy 133.172846 220.783461) (xy 130.326798 217.435351)
			)
		)
	)
	(zone
		(net 46)
		(net_name "Net-(J1-VB24N0_FB2)")
		(layers "F.Cu" "In1.Cu")
		(hatch edge 0.508)
		(priority 14)
		(connect_pads thru_hole_only
			(clearance 0.381)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.127)
			(thermal_bridge_width 0.762)
			(smoothing chamfer)
			(radius 0.508)
		)
		(polygon
			(pts
				(xy 77.186972 198.21914) (xy 77.21375 207.44089) (xy 80.249016 209.167119) (xy 80.245132 217.482989)
				(xy 80.899931 218.644473) (xy 85.335039 218.603663) (xy 85.351997 215.474678) (xy 83.166959 208.368255)
				(xy 83.087597 198.230895)
			)
		)
	)
	(zone
		(net 50)
		(net_name "/VB96P0B2")
		(layers "F.Cu" "In1.Cu")
		(hatch edge 0.5)
		(priority 26)
		(connect_pads yes
			(clearance 0.508)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(smoothing chamfer)
			(radius 0.508)
		)
		(polygon
			(pts
				(xy 87.765675 105.13556) (xy 141.831351 105.230393) (xy 141.831351 114.594187) (xy 99.76002 114.585073)
				(xy 82.107321 125.888993) (xy 81.881534 188.527952) (xy 76.496251 188.5296) (xy 73.044255 182.036037)
				(xy 73.35114 114.298004)
			)
		)
	)
	(zone
		(net 1)
		(net_name "/12Vpower/48V_RTN_DISA")
		(layers "F.Cu" "In1.Cu")
		(hatch edge 0.508)
		(priority 37)
		(connect_pads thru_hole_only
			(clearance 0.508)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.254)
			(thermal_bridge_width 0.762)
			(smoothing fillet)
			(radius 2.54)
		)
		(polygon
			(pts
				(xy 216.484753 203.215311) (xy 240.770499 203.292607) (xy 252.473909 198.840994) (xy 252.43312 190.886201)
				(xy 263.244494 190.8333) (xy 263.222149 200.876092) (xy 251.809902 212.656476) (xy 216.497068 212.703991)
			)
		)
	)
	(zone
		(net 85)
		(net_name "Net-(J1-VB12P6)")
		(layers "F.Cu" "In1.Cu")
		(hatch edge 0.508)
		(priority 32)
		(connect_pads thru_hole_only
			(clearance 0.508)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.254)
			(thermal_bridge_width 0.762)
			(smoothing fillet)
			(radius 0.508)
		)
		(polygon
			(pts
				(xy 123.874086 210.631824) (xy 115.163521 203.048985) (xy 108.960349 203.077909) (xy 108.960349 208.397703)
				(xy 110.469024 209.334681) (xy 110.469024 213.417968) (xy 109.098225 214.48786) (xy 109.130473 228.275652)
				(xy 123.874086 228.3073)
			)
		)
	)
	(zone
		(net 5)
		(net_name "/12Vpower/VFFF48P0_PS11")
		(layers "F.Cu" "In1.Cu")
		(hatch edge 0.508)
		(priority 30)
		(connect_pads thru_hole_only
			(clearance 0.508)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.254)
			(thermal_bridge_width 0.762)
			(smoothing chamfer)
			(radius 0.508)
		)
		(polygon
			(pts
				(xy 217.319522 217.711307) (xy 227.967879 217.745111) (xy 230.8043 214.29541) (xy 236.249935 214.263564)
				(xy 236.249935 227.717382) (xy 217.38713 227.751187)
			)
		)
	)
	(zone
		(net 25)
		(net_name "/VB96P0B4")
		(layers "F.Cu" "In1.Cu")
		(hatch edge 0.508)
		(priority 42)
		(connect_pads thru_hole_only
			(clearance 0.508)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.254)
			(thermal_bridge_width 0.762)
			(smoothing fillet)
			(radius 1.27)
		)
		(polygon
			(pts
				(xy 136.567137 188.501438) (xy 142.144848 188.501438) (xy 142.144848 198.135786) (xy 142.043555 198.237079)
				(xy 110.339117 198.237079) (xy 110.309363 198.207325) (xy 110.309363 192.862194) (xy 110.816428 192.355129)
				(xy 136.569502 192.35768)
			)
		)
	)
	(zone
		(net 48)
		(net_name "Net-(J1-VB24N0_FB4)")
		(layers "F.Cu" "In1.Cu")
		(hatch edge 0.5)
		(priority 56)
		(connect_pads thru_hole_only
			(clearance 0.381)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.254)
			(thermal_bridge_width 0.508)
			(smoothing fillet)
			(radius 0.508)
		)
		(polygon
			(pts
				(xy 107.453099 218.657296) (xy 107.099206 198.47755) (xy 102.059247 198.48143) (xy 102.025866 198.481731)
				(xy 99.973176 216.509254) (xy 101.056898 218.657296)
			)
		)
	)
	(zone
		(net 40)
		(net_name "Net-(J1-VB96P0_FB1)")
		(layers "F.Cu" "In1.Cu")
		(hatch edge 0.508)
		(priority 19)
		(connect_pads thru_hole_only
			(clearance 0.508)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.127)
			(thermal_bridge_width 0.762)
			(smoothing chamfer)
			(radius 0.508)
		)
		(polygon
			(pts
				(xy 63.474511 191.045911) (xy 70.243059 191.065724) (xy 75.238412 197.477275) (xy 75.238412 209.309964)
				(xy 67.280008 209.313341)
			)
		)
	)
	(zone
		(net 58)
		(net_name "/VB96P0B3")
		(layers "F.Cu" "In1.Cu")
		(hatch edge 0.5)
		(priority 41)
		(connect_pads thru_hole_only
			(clearance 0.508)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.254)
			(thermal_bridge_width 0.762)
			(smoothing fillet)
			(radius 1.27)
		)
		(polygon
			(pts
				(xy 136.588314 145.825883) (xy 142.326624 145.868563) (xy 142.326624 157.220273) (xy 142.149616 157.397281)
				(xy 103.450395 157.401973) (xy 97.413142 165.280587) (xy 97.402261 185.10207) (xy 90.051911 185.086672)
				(xy 87.896928 182.931689) (xy 87.826228 158.972951) (xy 95.445248 150.479365) (xy 136.600066 150.479365)
			)
		)
	)
	(zone
		(net 26)
		(net_name "/VB0P0B4")
		(layers "F.Cu" "In1.Cu")
		(hatch edge 0.508)
		(priority 3)
		(connect_pads thru_hole_only
			(clearance 0.508)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.254)
			(thermal_bridge_width 0.762)
			(smoothing fillet)
			(radius 0.508)
		)
		(polygon
			(pts
				(xy 110.878107 161.317) (xy 106.951342 165.953421) (xy 106.957102 185.158861) (xy 112.011889 185.152184)
				(xy 112.019317 191.79809) (xy 120.375157 191.789189) (xy 120.375157 176.297108) (xy 136.173957 176.297108)
				(xy 136.206957 165.917908) (xy 134.167357 165.917908) (xy 134.091157 171.801308) (xy 120.375157 171.826708)
				(xy 120.375157 161.285708)
			)
		)
	)
	(zone
		(net 4)
		(net_name "/48Vpower/VF48P0_DISA")
		(layers "F.Cu" "In1.Cu" "In2.Cu")
		(hatch edge 0.508)
		(priority 37)
		(connect_pads thru_hole_only
			(clearance 0.508)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.254)
			(thermal_bridge_width 0.762)
			(smoothing fillet)
			(radius 2.54)
		)
		(polygon
			(pts
				(xy 244.390181 166.982393) (xy 254.33737 166.91479) (xy 254.326527 181.976669) (xy 241.56534 182.020575)
				(xy 241.627697 169.424416)
			)
		)
	)
	(zone
		(net 77)
		(net_name "/48V_RTN")
		(layers "F.Cu" "In1.Cu" "In2.Cu" "In3.Cu")
		(hatch edge 0.508)
		(priority 36)
		(connect_pads thru_hole_only
			(clearance 0.508)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.254)
			(thermal_bridge_width 0.762)
			(smoothing fillet)
			(radius 2.54)
		)
		(polygon
			(pts
				(xy 254.143463 113.358564) (xy 274.106528 113.328469) (xy 274.106528 174.271112) (xy 265.367698 183.009942)
				(xy 255.344912 182.974787) (xy 255.406269 155.898188) (xy 254.06912 154.647623) (xy 254.06912 146.699473)
			)
		)
	)
	(zone
		(net 64)
		(net_name "/V48P0")
		(layers "F.Cu" "In1.Cu" "In3.Cu")
		(hatch edge 0.508)
		(priority 37)
		(connect_pads thru_hole_only
			(clearance 0.508)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.254)
			(thermal_bridge_width 0.762)
			(smoothing chamfer)
			(radius 0.762)
		)
		(polygon
			(pts
				(xy 244.687465 137.152564) (xy 254.464952 137.152564) (xy 254.496492 137.184104) (xy 254.496492 164.044767)
				(xy 253.999717 164.541542) (xy 246.843066 164.541542) (xy 244.687465 162.385941)
			)
		)
	)
	(zone
		(net 60)
		(net_name "/VB24N0B3")
		(layers "F.Cu" "In3.Cu")
		(hatch edge 0.508)
		(priority 4)
		(connect_pads thru_hole_only
			(clearance 0.508)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.254)
			(thermal_bridge_width 0.762)
			(smoothing fillet)
			(radius 0.508)
		)
		(polygon
			(pts
				(xy 123.062155 121.603083) (xy 129.107355 121.577683) (xy 133.812481 123.984957) (xy 133.850937 128.9458)
				(xy 123.10475 128.97201)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layer "F.Mask")
		(hatch edge 0.508)
		(priority 32)
		(connect_pads thru_hole_only
			(clearance 0.508)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.762)
			(thermal_bridge_width 0.254)
			(smoothing fillet)
			(radius 0.508)
		)
		(polygon
			(pts
				(xy 121.466002 220.629625) (xy 126.690115 220.629625) (xy 126.852644 220.792154) (xy 126.852644 224.739262)
				(xy 121.419565 224.739262) (xy 121.419565 220.676062)
			)
		)
	)
	(zone
		(net 14)
		(net_name "/BankPower1/VBU0P0")
		(layer "B.Cu")
		(hatch edge 0.508)
		(priority 1)
		(connect_pads thru_hole_only
			(clearance 0.508)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.254)
			(thermal_bridge_width 0.762)
			(smoothing fillet)
			(radius 0.508)
		)
		(polygon
			(pts
				(xy 178.061471 32.469098) (xy 135.059271 32.367498) (xy 135.059271 39.225498) (xy 144.406471 39.250898)
				(xy 144.381071 69.842698) (xy 160.529059 69.842698) (xy 160.579859 65.743098) (xy 178.290071 65.743098)
			)
		)
	)
	(zone
		(net 77)
		(net_name "/48V_RTN")
		(layer "B.Cu")
		(hatch edge 0.508)
		(priority 36)
		(connect_pads thru_hole_only
			(clearance 0.508)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.254)
			(thermal_bridge_width 0.762)
			(smoothing fillet)
			(radius 2.54)
		)
		(polygon
			(pts
				(xy 254.547485 145.713278) (xy 254.509352 185.687403) (xy 271.058098 185.676799) (xy 271.22274 145.676505)
			)
		)
	)
	(zone
		(net 61)
		(net_name "/BankPower3/VBU0P0")
		(layer "B.Cu")
		(hatch edge 0.508)
		(priority 1)
		(connect_pads thru_hole_only
			(clearance 0.508)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.254)
			(thermal_bridge_width 0.762)
			(smoothing fillet)
			(radius 0.508)
		)
		(polygon
			(pts
				(xy 176.757755 115.811883) (xy 133.755555 115.710283) (xy 133.755555 122.568283) (xy 143.102755 122.593683)
				(xy 143.077355 153.185483) (xy 159.225343 153.185483) (xy 159.276143 149.085883) (xy 176.986355 149.085883)
			)
		)
	)
	(zone
		(net 1)
		(net_name "/12Vpower/48V_RTN_DISA")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 25)
		(connect_pads thru_hole_only
			(clearance 0.508)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.254)
			(thermal_bridge_width 0.762)
			(smoothing chamfer)
			(radius 0.508)
		)
		(polygon
			(pts
				(xy 194.828491 201.1115) (xy 225.7154 201.1115) (xy 225.77478 213.804658) (xy 210.145809 213.858925)
				(xy 208.213064 216.097506) (xy 195.096952 216.373026)
			)
		)
	)
	(zone
		(net 51)
		(net_name "/BankPower4/VBU0P0")
		(layer "B.Cu")
		(hatch edge 0.508)
		(priority 1)
		(connect_pads thru_hole_only
			(clearance 0.508)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.254)
			(thermal_bridge_width 0.762)
			(smoothing fillet)
			(radius 0.508)
		)
		(polygon
			(pts
				(xy 176.757755 157.922863) (xy 133.755555 157.821263) (xy 133.755555 164.679263) (xy 143.102755 164.704663)
				(xy 143.077355 195.296463) (xy 160.262522 195.296463) (xy 160.313322 191.196863) (xy 176.986355 191.196863)
			)
		)
	)
	(zone
		(net 4)
		(net_name "/48Vpower/VF48P0_DISA")
		(layer "B.Cu")
		(hatch edge 0.508)
		(priority 40)
		(connect_pads thru_hole_only
			(clearance 0.508)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.254)
			(thermal_bridge_width 0.762)
			(smoothing fillet)
			(radius 2.54)
		)
		(polygon
			(pts
				(xy 253.337167 174.505508) (xy 253.340319 174.50866) (xy 253.340319 186.867465) (xy 246.740608 186.867465)
				(xy 242.462687 182.589544) (xy 242.474224 174.505508)
			)
		)
	)
	(zone
		(net 77)
		(net_name "/48V_RTN")
		(layer "B.Cu")
		(hatch edge 0.508)
		(priority 39)
		(connect_pads thru_hole_only
			(clearance 0.508)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.254)
			(thermal_bridge_width 0.508)
			(smoothing fillet)
			(radius 2.54)
		)
		(polygon
			(pts
				(xy 254.563899 114.127445) (xy 259.681825 114.127445) (xy 261.251721 115.697341) (xy 261.251721 120.181254)
				(xy 255.250985 120.181254) (xy 254.563899 119.494168)
			)
		)
	)
	(zone
		(net 55)
		(net_name "/BankPower2/VBU0P0")
		(layer "B.Cu")
		(hatch edge 0.508)
		(priority 1)
		(connect_pads thru_hole_only
			(clearance 0.508)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.254)
			(thermal_bridge_width 0.762)
			(smoothing fillet)
			(radius 0.508)
		)
		(polygon
			(pts
				(xy 176.535498 74.820213) (xy 133.533298 74.718613) (xy 133.533298 81.576613) (xy 142.880498 81.602013)
				(xy 142.855098 112.193813) (xy 159.003086 112.193813) (xy 159.053886 108.094213) (xy 176.764098 108.094213)
			)
		)
	)
	(zone
		(net 5)
		(net_name "/12Vpower/VFFF48P0_PS11")
		(layer "B.Cu")
		(hatch edge 0.508)
		(priority 28)
		(connect_pads thru_hole_only
			(clearance 0.508)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.254)
			(thermal_bridge_width 0.762)
			(smoothing chamfer)
			(radius 0.508)
		)
		(polygon
			(pts
				(xy 195.024557 215.446471) (xy 205.110494 215.422341) (xy 208.4898 214.178756) (xy 225.077611 214.178756)
				(xy 225.111415 226.348308) (xy 195.059383 226.382112)
			)
		)
	)
	(zone
		(net 16)
		(net_name "/BankPower1/VBU24P0")
		(layers "B.Cu" "In1.Cu")
		(hatch edge 0.508)
		(priority 2)
		(connect_pads thru_hole_only
			(clearance 0.508)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.254)
			(thermal_bridge_width 0.762)
			(smoothing fillet)
			(radius 0.254)
		)
		(polygon
			(pts
				(xy 178.881871 50.055298) (xy 162.625871 50.055298) (xy 156.471471 50.055298) (xy 156.471471 42.730698)
				(xy 154.185471 42.730698) (xy 154.1336 48.269077) (xy 146.006671 48.267898) (xy 146.006671 55.202098)
				(xy 165.648471 55.211498) (xy 178.881871 55.211498)
			)
		)
	)
	(zone
		(net 49)
		(net_name "Net-(J1-LF_FB2)")
		(layers "B.Cu" "In1.Cu")
		(hatch edge 0.508)
		(priority 48)
		(connect_pads thru_hole_only
			(clearance 0.508)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.127)
			(thermal_bridge_width 0.762)
			(smoothing fillet)
			(radius 1.016)
		)
		(polygon
			(pts
				(xy 89.988279 192.786218) (xy 89.988279 198.100081) (xy 88.872029 198.520618) (xy 88.872029 208.33327)
				(xy 90.641038 211.067193) (xy 89.858877 213.550973) (xy 87.163233 214.596128) (xy 84.964077 212.396972)
				(xy 84.964077 206.085307) (xy 84.080912 205.202142) (xy 84.08141 192.771692)
			)
		)
	)
	(zone
		(net 53)
		(net_name "/BankPower4/VBU24P0")
		(layers "B.Cu" "In1.Cu")
		(hatch edge 0.508)
		(priority 2)
		(connect_pads thru_hole_only
			(clearance 0.508)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.254)
			(thermal_bridge_width 0.762)
			(smoothing fillet)
			(radius 0.254)
		)
		(polygon
			(pts
				(xy 177.578155 175.509063) (xy 161.322155 175.509063) (xy 155.167755 175.509063) (xy 155.167755 168.184463)
				(xy 152.881755 168.184463) (xy 152.829884 173.722842) (xy 144.702955 173.721663) (xy 144.702955 180.655863)
				(xy 164.344755 180.665263) (xy 177.578155 180.665263)
			)
		)
	)
	(zone
		(net 63)
		(net_name "/BankPower3/VBU96P0")
		(layers "B.Cu" "In1.Cu")
		(hatch edge 0.508)
		(priority 1)
		(connect_pads thru_hole_only
			(clearance 0.508)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.254)
			(thermal_bridge_width 0.762)
			(smoothing fillet)
			(radius 0.254)
		)
		(polygon
			(pts
				(xy 144.761355 139.113083) (xy 177.070155 139.113083) (xy 177.070155 148.434883) (xy 144.761355 148.434883)
			)
		)
	)
	(zone
		(net 57)
		(net_name "/BankPower2/VBU96P0")
		(layers "B.Cu" "In1.Cu")
		(hatch edge 0.508)
		(priority 1)
		(connect_pads thru_hole_only
			(clearance 0.508)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.254)
			(thermal_bridge_width 0.762)
			(smoothing fillet)
			(radius 0.254)
		)
		(polygon
			(pts
				(xy 144.539098 98.121413) (xy 176.847898 98.121413) (xy 176.847898 107.443213) (xy 144.539098 107.443213)
			)
		)
	)
	(zone
		(net 62)
		(net_name "/BankPower3/VBU24P0")
		(layers "B.Cu" "In1.Cu")
		(hatch edge 0.508)
		(priority 2)
		(connect_pads thru_hole_only
			(clearance 0.508)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.254)
			(thermal_bridge_width 0.762)
			(smoothing fillet)
			(radius 0.254)
		)
		(polygon
			(pts
				(xy 177.578155 133.398083) (xy 161.322155 133.398083) (xy 155.167755 133.398083) (xy 155.167755 126.073483)
				(xy 152.881755 126.073483) (xy 152.829884 131.611862) (xy 144.702955 131.610683) (xy 144.702955 138.544883)
				(xy 164.344755 138.554283) (xy 177.578155 138.554283)
			)
		)
	)
	(zone
		(net 56)
		(net_name "/BankPower2/VBU24P0")
		(layers "B.Cu" "In1.Cu")
		(hatch edge 0.508)
		(priority 2)
		(connect_pads thru_hole_only
			(clearance 0.508)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.254)
			(thermal_bridge_width 0.762)
			(smoothing fillet)
			(radius 0.254)
		)
		(polygon
			(pts
				(xy 177.355898 92.406413) (xy 161.099898 92.406413) (xy 154.945498 92.406413) (xy 154.945498 85.081813)
				(xy 152.659498 85.081813) (xy 152.607627 90.620192) (xy 144.480698 90.619013) (xy 144.480698 97.553213)
				(xy 164.122498 97.562613) (xy 177.355898 97.562613)
			)
		)
	)
	(zone
		(net 12)
		(net_name "/BankPower1/VBU96P0")
		(layers "B.Cu" "In1.Cu")
		(hatch edge 0.508)
		(priority 1)
		(connect_pads thru_hole_only
			(clearance 0.508)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.254)
			(thermal_bridge_width 0.762)
			(smoothing fillet)
			(radius 0.254)
		)
		(polygon
			(pts
				(xy 146.065071 55.770298) (xy 178.373871 55.770298) (xy 178.373871 65.092098) (xy 146.065071 65.092098)
			)
		)
	)
	(zone
		(net 19)
		(net_name "/BankPower4/VBU96P0")
		(layers "B.Cu" "In1.Cu")
		(hatch edge 0.508)
		(priority 1)
		(connect_pads thru_hole_only
			(clearance 0.508)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.254)
			(thermal_bridge_width 0.762)
			(smoothing fillet)
			(radius 0.254)
		)
		(polygon
			(pts
				(xy 144.761355 181.224063) (xy 177.070155 181.224063) (xy 177.070155 190.545863) (xy 144.761355 190.545863)
			)
		)
	)
	(zone
		(net 42)
		(net_name "Net-(J1-LF_FB1)")
		(layers "B.Cu" "In4.Cu")
		(hatch edge 0.508)
		(priority 22)
		(connect_pads thru_hole_only
			(clearance 0.381)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.127)
			(thermal_bridge_width 0.762)
			(smoothing fillet)
			(radius 0.508)
		)
		(polygon
			(pts
				(xy 70.11054 211.281057) (xy 69.092771 209.492035) (xy 69.150066 194.550624) (xy 76.616169 194.617212)
				(xy 76.616169 199.171705) (xy 76.763045 207.758466) (xy 79.944069 209.779351) (xy 79.951918 213.869534)
				(xy 74.465686 213.858793)
			)
		)
	)
	(zone
		(net 28)
		(net_name "/VB24N0B4")
		(layers "B.Cu" "In4.Cu")
		(hatch edge 0.508)
		(priority 52)
		(connect_pads thru_hole_only
			(clearance 0.508)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.254)
			(thermal_bridge_width 0.762)
			(smoothing fillet)
			(radius 1.016)
		)
		(polygon
			(pts
				(xy 128.373093 163.688663) (xy 111.652213 163.725639) (xy 103.996683 169.081706) (xy 104.018096 191.64298)
				(xy 101.738435 193.982217) (xy 101.731757 197.819694) (xy 107.80293 197.887955) (xy 112.959766 193.630017)
				(xy 112.928268 176.23338) (xy 115.812874 173.62201) (xy 133.831724 173.656063) (xy 133.812481 166.095937)
			)
		)
	)
	(zone
		(net 47)
		(net_name "Net-(J1-VB96P0_FB4)")
		(layers "B.Cu" "In4.Cu")
		(hatch edge 0.5)
		(priority 57)
		(connect_pads thru_hole_only
			(clearance 0.508)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.127)
			(thermal_bridge_width 0.508)
			(smoothing fillet)
			(radius 0.508)
		)
		(polygon
			(pts
				(xy 102.377984 209.845358) (xy 109.661745 209.808184) (xy 109.661745 204) (xy 116 204) (xy 116 198.5)
				(xy 109 198.5) (xy 100.791918 204.293941) (xy 100.791918 209.081069)
			)
		)
	)
	(zone
		(net 76)
		(net_name "/48V_RTN_M1")
		(layers "B.Cu" "In4.Cu")
		(hatch edge 0.508)
		(priority 9)
		(connect_pads thru_hole_only
			(clearance 0.508)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.254)
			(thermal_bridge_width 0.762)
			(smoothing chamfer)
			(radius 0.508)
		)
		(polygon
			(pts
				(xy 264.486875 35.831298) (xy 214.187871 35.831298) (xy 180.405871 35.831298) (xy 180.405871 79.868774)
				(xy 238.547952 79.868774) (xy 238.657015 106.588531) (xy 264.486876 106.657046)
			)
		)
	)
	(zone
		(net 54)
		(net_name "/VB24N0B2")
		(layers "B.Cu" "In4.Cu")
		(hatch edge 0.508)
		(priority 43)
		(connect_pads thru_hole_only
			(clearance 0.508)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.254)
			(thermal_bridge_width 0.762)
			(smoothing fillet)
			(radius 0.508)
		)
		(polygon
			(pts
				(xy 130.269614 79.672677) (xy 85.837148 79.672677) (xy 73.270242 88.601386) (xy 73.190734 189.985388)
				(xy 77.217135 193.473845) (xy 77.217135 197.66798) (xy 83.91931 197.648413) (xy 83.91931 110.0143)
				(xy 103.177248 90.428662) (xy 133.627069 90.428662) (xy 133.645083 83.241066)
			)
		)
	)
	(zone
		(net 6)
		(net_name "/12Vpower/VBU0P0_11_21")
		(layers "B.Cu" "In4.Cu")
		(hatch edge 0.5)
		(priority 16)
		(connect_pads thru_hole_only
			(clearance 0.508)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.254)
			(thermal_bridge_width 0.762)
			(smoothing fillet)
			(radius 0.508)
		)
		(polygon
			(pts
				(xy 194.139522 202.997904) (xy 194.156424 226.309609) (xy 183.326364 226.360313) (xy 183.366426 214.221548)
				(xy 182.523118 213.37824) (xy 167.617283 213.251562) (xy 163.122865 216.694092) (xy 163.130724 220.022005)
				(xy 157.161828 220.022005) (xy 157.191874 202.971207)
			)
		)
	)
	(zone
		(net 11)
		(net_name "/12Vpower/VBU12P6_11_21")
		(layers "B.Cu" "In4.Cu")
		(hatch edge 0.5)
		(priority 17)
		(connect_pads thru_hole_only
			(clearance 0.508)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.254)
			(thermal_bridge_width 0.762)
			(smoothing fillet)
			(radius 1.27)
		)
		(polygon
			(pts
				(xy 157.201839 220.686418) (xy 163.991991 220.726836) (xy 169.79517 214.694153) (xy 184.005969 214.725874)
				(xy 184.039773 228.081281) (xy 157.097738 228.115085)
			)
		)
	)
	(zone
		(net 76)
		(net_name "/48V_RTN_M1")
		(layers "B.Cu" "In4.Cu")
		(hatch edge 0.508)
		(priority 9)
		(connect_pads yes
			(clearance 0.508)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.254)
			(thermal_bridge_width 0.762)
			(smoothing fillet)
			(radius 2.54)
		)
		(polygon
			(pts
				(xy 241.175272 161.285063) (xy 212.884155 161.285063) (xy 179.102155 161.285063) (xy 179.102155 197.581663)
				(xy 241.175272 197.581663)
			)
		)
	)
	(zone
		(net 17)
		(net_name "/VB24N0B1")
		(layers "B.Cu" "In4.Cu")
		(hatch edge 0.508)
		(priority 13)
		(connect_pads thru_hole_only
			(clearance 0.508)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.254)
			(thermal_bridge_width 0.762)
			(smoothing chamfer)
			(radius 0.508)
		)
		(polygon
			(pts
				(xy 134.839208 49.166869) (xy 134.839208 38.980503) (xy 130.382871 37.862144) (xy 67.34337 37.91236)
				(xy 50.640539 52.41094) (xy 50.687855 197.645768) (xy 71.353939 197.675688) (xy 71.350534 193.303947)
				(xy 71.284791 82.202203) (xy 117.553778 49.097865)
			)
		)
	)
	(zone
		(net 76)
		(net_name "/48V_RTN_M1")
		(layers "B.Cu" "In4.Cu")
		(hatch edge 0.508)
		(priority 9)
		(connect_pads thru_hole_only
			(clearance 0.508)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.254)
			(thermal_bridge_width 0.762)
			(smoothing chamfer)
			(radius 0.762)
		)
		(polygon
			(pts
				(xy 243.58285 119.174083) (xy 212.884155 119.174083) (xy 179.102155 119.174083) (xy 179.102155 162.583697)
				(xy 243.58285 162.583697)
			)
		)
	)
	(zone
		(net 76)
		(net_name "/48V_RTN_M1")
		(layers "B.Cu" "In4.Cu")
		(hatch edge 0.508)
		(priority 9)
		(connect_pads thru_hole_only
			(clearance 0.508)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.254)
			(thermal_bridge_width 0.762)
			(smoothing fillet)
			(radius 2.54)
		)
		(polygon
			(pts
				(xy 247.435604 78.182413) (xy 212.661898 78.182413) (xy 178.879898 78.182413) (xy 178.879898 120.598743)
				(xy 247.435604 120.598743)
			)
		)
	)
	(zone
		(net 46)
		(net_name "Net-(J1-VB24N0_FB2)")
		(layers "B.Cu" "In4.Cu")
		(hatch edge 0.508)
		(priority 14)
		(connect_pads thru_hole_only
			(clearance 0.381)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.127)
			(thermal_bridge_width 0.762)
			(smoothing fillet)
			(radius 0.508)
		)
		(polygon
			(pts
				(xy 77.183938 198.204768) (xy 77.210716 207.426518) (xy 80.222242 209.351376) (xy 80.209004 216.710549)
				(xy 81.205019 218.477289) (xy 85.839205 218.483642) (xy 85.8162 203.990049) (xy 83.108523 201.277014)
				(xy 83.084563 198.216523)
			)
		)
	)
	(zone
		(net 16)
		(net_name "/BankPower1/VBU24P0")
		(layers "In1.Cu" "In2.Cu")
		(hatch edge 0.508)
		(priority 6)
		(connect_pads thru_hole_only
			(clearance 0.508)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.254)
			(thermal_bridge_width 0.762)
			(smoothing fillet)
			(radius 0.508)
		)
		(polygon
			(pts
				(xy 132.849471 30.801534) (xy 152.482129 30.801534) (xy 155.999117 42.740777) (xy 156.065071 55.125898)
				(xy 135.338671 55.150312) (xy 135.338671 40.628607) (xy 132.849471 40.624105)
			)
		)
	)
	(zone
		(net 62)
		(net_name "/BankPower3/VBU24P0")
		(layers "In1.Cu" "In2.Cu")
		(hatch edge 0.508)
		(priority 6)
		(connect_pads thru_hole_only
			(clearance 0.508)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.254)
			(thermal_bridge_width 0.762)
			(smoothing fillet)
			(radius 0.508)
		)
		(polygon
			(pts
				(xy 131.545755 115.981316) (xy 151.719545 115.981316) (xy 154.695401 126.083562) (xy 154.761355 138.468683)
				(xy 134.034955 138.493097) (xy 134.034955 123.971392) (xy 131.545755 123.96689)
			)
		)
	)
	(zone
		(net 3)
		(net_name "/VFF48P0_M1")
		(layers "In1.Cu" "In2.Cu")
		(hatch edge 0.508)
		(priority 34)
		(connect_pads thru_hole_only
			(clearance 0.508)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.254)
			(thermal_bridge_width 0.762)
			(smoothing fillet)
			(radius 2.54)
		)
		(polygon
			(pts
				(xy 202.762216 192.101139) (xy 234.72137 192.073911) (xy 234.72137 171.048413) (xy 237.862738 168.919997)
				(xy 237.673581 57.514283) (xy 203.083915 57.564033)
			)
		)
	)
	(zone
		(net 56)
		(net_name "/BankPower2/VBU24P0")
		(layers "In1.Cu" "In2.Cu")
		(hatch edge 0.508)
		(priority 6)
		(connect_pads thru_hole_only
			(clearance 0.508)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.254)
			(thermal_bridge_width 0.762)
			(smoothing fillet)
			(radius 0.508)
		)
		(polygon
			(pts
				(xy 130.244895 74.597009) (xy 151.381627 74.597009) (xy 154.473144 85.091892) (xy 154.539098 97.477013)
				(xy 133.812698 97.501427) (xy 133.812698 90.874491) (xy 130.244895 90.868039)
			)
		)
	)
	(zone
		(net 53)
		(net_name "/BankPower4/VBU24P0")
		(layers "In1.Cu" "In2.Cu")
		(hatch edge 0.508)
		(priority 6)
		(connect_pads thru_hole_only
			(clearance 0.508)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.254)
			(thermal_bridge_width 0.762)
			(smoothing fillet)
			(radius 0.508)
		)
		(polygon
			(pts
				(xy 131.545755 158.060529) (xy 151.710187 158.060529) (xy 154.695401 168.194542) (xy 154.761355 180.579663)
				(xy 134.034955 180.604077) (xy 134.034955 166.082372) (xy 131.545755 166.07787)
			)
		)
	)
	(zone
		(net 52)
		(net_name "/VB0P0B2")
		(layers "In2.Cu" "In3.Cu")
		(hatch edge 0.5)
		(priority 10)
		(connect_pads yes
			(clearance 0.508)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(smoothing fillet)
			(radius 1.27)
		)
		(polygon
			(pts
				(xy 84.800832 192.477427) (xy 90.880721 192.481786) (xy 91.035137 124.48259) (xy 100.803091 114.741061)
				(xy 120.143238 114.710702) (xy 119.616218 80.718064) (xy 89.16575 80.731208) (xy 73.926652 93.280201)
				(xy 73.928687 171.738283)
			)
		)
	)
	(zone
		(net 39)
		(net_name "Net-(J1-LF_FB4)")
		(layers "In2.Cu" "In3.Cu")
		(hatch edge 0.508)
		(priority 55)
		(connect_pads thru_hole_only
			(clearance 0.381)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.254)
			(thermal_bridge_width 0.762)
			(smoothing fillet)
			(radius 0.508)
		)
		(polygon
			(pts
				(xy 105.102919 214) (xy 110.268476 214.013063) (xy 110.634822 211.352217) (xy 110.041242 204.392702)
				(xy 111.978701 202.9714) (xy 111.978701 185.5) (xy 105.102919 185.5)
			)
		)
	)
	(zone
		(net 44)
		(net_name "Net-(J1-VB96P0_FB2)")
		(layers "In2.Cu" "In3.Cu")
		(hatch edge 0.508)
		(priority 44)
		(connect_pads thru_hole_only
			(clearance 0.381)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.254)
			(thermal_bridge_width 0.762)
			(smoothing fillet)
			(radius 1.27)
		)
		(polygon
			(pts
				(xy 76.383114 188.969947) (xy 81.495017 188.969947) (xy 83.610326 191.085256) (xy 83.610326 192.336016)
				(xy 87.362604 196.088294) (xy 87.362604 206.650876) (xy 84.532654 209.480826) (xy 81.323385 209.480826)
				(xy 80.103831 208.591568) (xy 80.103831 200.89732) (xy 81.370292 199.489804) (xy 81.394357 196.978394)
				(xy 76.376908 191.421572)
			)
		)
	)
	(zone
		(net 59)
		(net_name "/VB0P0B3")
		(layers "In2.Cu" "In3.Cu")
		(hatch edge 0.508)
		(priority 51)
		(connect_pads thru_hole_only
			(clearance 0.508)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.254)
			(thermal_bridge_width 0.762)
			(smoothing fillet)
			(radius 1.016)
		)
		(polygon
			(pts
				(xy 120.024057 119.297029) (xy 103.03649 119.297029) (xy 93.929007 128.404512) (xy 93.929007 190.041136)
				(xy 95.746453 191.858582) (xy 101.609567 191.858582) (xy 102.772255 190.695894) (xy 102.772255 160.566372)
				(xy 110.150544 153.188083) (xy 120.087125 153.188083) (xy 120.087125 119.360097)
			)
		)
	)
	(zone
		(net 41)
		(net_name "Net-(J1-VB24N0_FB1)")
		(layers "In2.Cu" "In3.Cu")
		(hatch edge 0.508)
		(priority 15)
		(connect_pads yes
			(clearance 0.508)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.254)
			(thermal_bridge_width 0.762)
			(smoothing fillet)
			(radius 1.27)
		)
		(polygon
			(pts
				(xy 60.415918 198.027973) (xy 68.201795 198.031702) (xy 71.396302 210.911144) (xy 75.114776 214.866248)
				(xy 75.081516 218.333943) (xy 60.404283 218.366044)
			)
		)
	)
	(zone
		(net 43)
		(net_name "Net-(J1-LF_FB3)")
		(layers "In2.Cu" "In3.Cu")
		(hatch edge 0.5)
		(priority 54)
		(connect_pads
			(clearance 0.508)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 100.5 201) (xy 101.5 199.5) (xy 101.5 192.5) (xy 96.5 192.5) (xy 96.5 195) (xy 97.5 196) (xy 97.5 201)
			)
		)
	)
	(zone
		(net 43)
		(net_name "Net-(J1-LF_FB3)")
		(layers "In2.Cu" "In3.Cu")
		(hatch edge 0.5)
		(priority 53)
		(connect_pads thru_hole_only
			(clearance 0.381)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.254)
			(thermal_bridge_width 0.762)
			(smoothing fillet)
			(radius 0.508)
		)
		(polygon
			(pts
				(xy 100.5 201) (xy 100.56629 210.56629) (xy 100.5 214) (xy 95.201112 214) (xy 95.201112 201)
			)
		)
	)
	(zone
		(net 15)
		(net_name "/VB0P0B1")
		(layers "In2.Cu" "In3.Cu")
		(hatch edge 0.508)
		(priority 11)
		(connect_pads thru_hole_only
			(clearance 0.508)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.254)
			(thermal_bridge_width 0.762)
			(smoothing fillet)
			(radius 0.508)
		)
		(polygon
			(pts
				(xy 120.902469 37.807597) (xy 78.706398 37.888277) (xy 56.816489 53.31264) (xy 57.149339 194.19961)
				(xy 76.235512 194.20513) (xy 76.211643 192.578431) (xy 71.32439 183.350506) (xy 71.324419 87.42989)
				(xy 89.121533 74.269809) (xy 120.967468 74.373652)
			)
		)
	)
	(zone
		(net 38)
		(net_name "Net-(J1-VB24N0_FB3)")
		(layers "In2.Cu" "In3.Cu" "In4.Cu")
		(hatch edge 0.508)
		(priority 49)
		(connect_pads thru_hole_only
			(clearance 0.381)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.127)
			(thermal_bridge_width 0.762)
			(smoothing fillet)
			(radius 0.508)
		)
		(polygon
			(pts
				(xy 96.957913 198.507598) (xy 89.067793 198.520976) (xy 89.138345 218.628157) (xy 90.385353 218.5)
				(xy 90.389049 218.5) (xy 91.577277 218.526102) (xy 94.180206 218.526102) (xy 96.939549 215.766759)
				(xy 96.939549 206.039698) (xy 96.957913 206.021334)
			)
		)
	)
	(zone
		(net 9)
		(net_name "/12Vpower/VFF48P0_DISA")
		(layers "In3.Cu" "In4.Cu")
		(hatch edge 0.508)
		(priority 29)
		(connect_pads thru_hole_only
			(clearance 0.508)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.254)
			(thermal_bridge_width 0.762)
			(smoothing fillet)
			(radius 2.54)
		)
		(polygon
			(pts
				(xy 238.61008 227.580511) (xy 252.050853 227.580511) (xy 252.050853 194.361885) (xy 249.379455 191.022718)
				(xy 242.615171 191.005165) (xy 242.6166 200.775274) (xy 237.605015 218.329669) (xy 237.608596 225.632524)
			)
		)
	)
	(zone
		(net 63)
		(net_name "/BankPower3/VBU96P0")
		(layers "In3.Cu" "In4.Cu")
		(hatch edge 0.508)
		(priority 8)
		(connect_pads thru_hole_only
			(clearance 0.508)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.254)
			(thermal_bridge_width 0.762)
			(smoothing fillet)
			(radius 0.508)
		)
		(polygon
			(pts
				(xy 141.61312 136.506652) (xy 135.755255 134.085361) (xy 135.693753 116.928343) (xy 145.401829 116.941682)
				(xy 145.357926 138.212583) (xy 153.76531 138.190632) (xy 153.76531 148.112663) (xy 141.604238 148.134614)
			)
		)
	)
	(zone
		(net 12)
		(net_name "/BankPower1/VBU96P0")
		(layers "In3.Cu" "In4.Cu")
		(hatch edge 0.508)
		(priority 8)
		(connect_pads thru_hole_only
			(clearance 0.508)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.254)
			(thermal_bridge_width 0.762)
			(smoothing fillet)
			(radius 0.508)
		)
		(polygon
			(pts
				(xy 142.916836 53.163867) (xy 137.058971 50.742576) (xy 136.997469 33.585558) (xy 146.705545 33.598897)
				(xy 146.661642 54.869798) (xy 155.069026 54.847847) (xy 155.069026 64.769878) (xy 142.907954 64.791829)
			)
		)
	)
	(zone
		(net 19)
		(net_name "/BankPower4/VBU96P0")
		(layers "In3.Cu" "In4.Cu")
		(hatch edge 0.508)
		(priority 8)
		(connect_pads thru_hole_only
			(clearance 0.508)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.254)
			(thermal_bridge_width 0.762)
			(smoothing fillet)
			(radius 0.508)
		)
		(polygon
			(pts
				(xy 141.61312 178.617632) (xy 135.755255 176.196341) (xy 135.693753 159.039323) (xy 145.401829 159.052662)
				(xy 145.357926 180.323563) (xy 153.76531 180.301612) (xy 153.76531 190.223643) (xy 141.604238 190.245594)
			)
		)
	)
	(zone
		(net 57)
		(net_name "/BankPower2/VBU96P0")
		(layers "In3.Cu" "In4.Cu")
		(hatch edge 0.508)
		(priority 8)
		(connect_pads thru_hole_only
			(clearance 0.508)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.254)
			(thermal_bridge_width 0.762)
			(smoothing fillet)
			(radius 0.508)
		)
		(polygon
			(pts
				(xy 141.390863 95.514982) (xy 135.532998 93.093691) (xy 135.471496 75.936673) (xy 145.179572 75.950012)
				(xy 145.135669 97.220913) (xy 153.543053 97.198962) (xy 153.543053 107.120993) (xy 141.381981 107.142944)
			)
		)
	)
	(zone
		(net 61)
		(net_name "/BankPower3/VBU0P0")
		(layer "In4.Cu")
		(hatch edge 0.5)
		(priority 21)
		(connect_pads
			(clearance 0.508)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 144.898718 148.786519) (xy 155.63103 148.764014) (xy 155.613005 125.578656) (xy 160.270456 125.589738)
				(xy 160.270456 153.077093) (xy 144.898718 153.090935)
			)
		)
	)
	(zone
		(net 14)
		(net_name "/BankPower1/VBU0P0")
		(layer "In4.Cu")
		(hatch edge 0.5)
		(priority 21)
		(connect_pads
			(clearance 0.508)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 146.202434 65.443734) (xy 156.934746 65.421229) (xy 156.916721 42.235871) (xy 161.574172 42.246953)
				(xy 161.574172 69.734308) (xy 146.202434 69.74815)
			)
		)
	)
	(zone
		(net 60)
		(net_name "/VB24N0B3")
		(layer "In4.Cu")
		(hatch edge 0.508)
		(priority 45)
		(connect_pads thru_hole_only
			(clearance 0.508)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.254)
			(thermal_bridge_width 0.762)
			(smoothing fillet)
			(radius 1.27)
		)
		(polygon
			(pts
				(xy 133.850937 131.787489) (xy 133.850937 123.984957) (xy 131.443663 121.577683) (xy 97.35254 121.663843)
				(xy 86.454926 131.580672) (xy 86.394589 188.487059) (xy 90.734966 190.884038) (xy 90.734966 198.073088)
				(xy 97.313199 198.081273) (xy 97.290662 189.337225) (xy 98.658919 186.970925) (xy 98.645191 140.67913)
				(xy 107.536832 131.787489)
			)
		)
	)
	(zone
		(net 61)
		(net_name "/BankPower3/VBU0P0")
		(layer "In4.Cu")
		(hatch edge 0.5)
		(priority 21)
		(connect_pads
			(clearance 0.508)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 144.898718 148.786519) (xy 155.63103 148.764014) (xy 155.613005 125.578656) (xy 160.270456 125.589738)
				(xy 160.270456 153.077093) (xy 144.898718 153.090935)
			)
		)
	)
	(zone
		(net 55)
		(net_name "/BankPower2/VBU0P0")
		(layer "In4.Cu")
		(hatch edge 0.5)
		(priority 21)
		(connect_pads
			(clearance 0.508)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 144.676461 107.794849) (xy 155.408773 107.772344) (xy 155.390748 84.586986) (xy 160.048199 84.598068)
				(xy 160.048199 112.085423) (xy 144.676461 112.099265)
			)
		)
	)
	(zone
		(net 51)
		(net_name "/BankPower4/VBU0P0")
		(layer "In4.Cu")
		(hatch edge 0.5)
		(priority 21)
		(connect_pads
			(clearance 0.508)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 144.898718 190.897499) (xy 155.63103 190.874994) (xy 155.613005 167.689636) (xy 160.270456 167.700718)
				(xy 160.270456 195.188073) (xy 144.898718 195.201915)
			)
		)
	)
	(embedded_fonts no)
)
