(kicad_pcb (version 20221018) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )
  (setup
    (pad_to_mask_clearance 0)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (plot_on_all_layers_selection 0x0000000_00000000)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (dashed_line_dash_ratio 12.000000)
      (dashed_line_gap_ratio 3.000000)
      (svgprecision 4)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory "")
    )
  )
  (net 0 "")
  (net 1 "+12V")
  (net 2 "GND")
  (net 3 "-12V")
  (net 4 "Net-(D1-COM)")
  (net 5 "Net-(D2-COM)")
  (net 6 "/FACE")
  (net 7 "Net-(J1-Pin_1)")
  (net 8 "Net-(J1-Pin_10)")
  (net 9 "Net-(U1A-+)")
  (net 10 "Net-(D3-K)")
  (net 11 "Net-(D4-K)")
  (net 12 "Net-(D4-A)")
  (net 13 "Net-(D5-K)")
  (net 14 "Net-(D5-A)")
  (net 15 "/GATE_IN'")
  (net 16 "unconnected-(J2-PadTN)")
  (net 17 "/GATE_OUT'")
  (net 18 "unconnected-(J3-PadTN)")
  (net 19 "/SLEW_OUT'")
  (net 20 "unconnected-(J4-PadTN)")
  (net 21 "Net-(Q1A-C1)")
  (net 22 "Net-(Q2-D)")
  (net 23 "Net-(Q3-D)")
  (net 24 "Net-(R6-Pad1)")
  (net 25 "Net-(U1A--)")
  (net 26 "Net-(R10-Pad1)")
  (net 27 "Net-(U1B--)")
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (at 124.17 90.624)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "gate-delay.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R9" (at 0 -1.65) (layer "F.SilkS"))
    (fp_text value "22K" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 2 "GND") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 25 "Net-(U1A--)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (at 147.792 91.386)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "gate-delay.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R2" (at -2.794 0) (layer "F.SilkS"))
    (fp_text value "10" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 4 "Net-(D1-COM)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 7 "Net-(J1-Pin_1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Eurorack:AudioJack2_Tayda_A-2566" (layer "F.Cu")
    (at 115.534 84.528 180)
    (property "PartNum" "A-2566")
    (property "Sheetfile" "gate-delay.kicad_sch")
    (property "Sheetname" "")
    (property "Vendor" "Tayda")
    (property "ki_description" "Audio Jack, 2 Poles (Mono / TS), Switched T Pole (Normalling)")
    (property "ki_keywords" "audio jack receptacle mono headphones phone TS connector")
    (attr through_hole)
    (fp_text reference "J3" (at 5.6896 -4.445 270 unlocked) (layer "F.SilkS"))
    (fp_text value "gate_out" (at 0 1 180 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2.5 180 unlocked) (layer "F.Fab"))
    (pad "S" thru_hole oval (at -4.7 0.6 180) (size 2.25 3.75) (drill oval 1.45 2.95) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pintype "passive"))
    (pad "S" thru_hole oval (at 4.7 0.6 180) (size 2.25 2.7) (drill oval 1.45 1.9) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pintype "passive"))
    (pad "T" thru_hole oval (at 0 -4.8 180) (size 3.5 1.5) (drill oval 2.7 0.7) (layers "*.Cu" "*.Mask")
      (net 17 "/GATE_OUT'") (pintype "passive"))
    (pad "TN" thru_hole oval (at 0 3.3 180) (size 3.5 1.5) (drill oval 2.7 0.7) (layers "*.Cu" "*.Mask")
      (net 18 "unconnected-(J3-PadTN)") (pintype "passive+no_connect"))
    (model "./models3d/A-2566.wrl"
      (offset (xyz 0 -0.15 11.5))
      (scale (xyz 0.385 0.385 0.385))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Eurorack:AudioJack2_Tayda_A-2566" (layer "F.Cu")
    (at 103.342 84.528 180)
    (property "PartNum" "A-2566")
    (property "Sheetfile" "gate-delay.kicad_sch")
    (property "Sheetname" "")
    (property "Vendor" "Tayda")
    (property "ki_description" "Audio Jack, 2 Poles (Mono / TS), Switched T Pole (Normalling)")
    (property "ki_keywords" "audio jack receptacle mono headphones phone TS connector")
    (attr through_hole)
    (fp_text reference "J2" (at 5.6642 -4.4704 270 unlocked) (layer "F.SilkS"))
    (fp_text value "gate_in" (at 0 1 180 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2.5 180 unlocked) (layer "F.Fab"))
    (pad "S" thru_hole oval (at -4.7 0.6 180) (size 2.25 3.75) (drill oval 1.45 2.95) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pintype "passive"))
    (pad "S" thru_hole oval (at 4.7 0.6 180) (size 2.25 2.7) (drill oval 1.45 1.9) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pintype "passive"))
    (pad "T" thru_hole oval (at 0 -4.8 180) (size 3.5 1.5) (drill oval 2.7 0.7) (layers "*.Cu" "*.Mask")
      (net 15 "/GATE_IN'") (pintype "passive"))
    (pad "TN" thru_hole oval (at 0 3.3 180) (size 3.5 1.5) (drill oval 2.7 0.7) (layers "*.Cu" "*.Mask")
      (net 16 "unconnected-(J2-PadTN)") (pintype "passive+no_connect"))
    (model "./models3d/A-2566.wrl"
      (offset (xyz 0 -0.15 11.5))
      (scale (xyz 0.385 0.385 0.385))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (at 136.0064 83.258)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "gate-delay.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R3" (at 0 -1.65) (layer "F.SilkS"))
    (fp_text value "1K" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 15 "/GATE_IN'") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 10 "Net-(D3-K)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (at 139.918 96.9994)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "gate-delay.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R7" (at -0.0508 1.6256) (layer "F.SilkS"))
    (fp_text value "1K" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 24 "Net-(R6-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 23 "Net-(Q3-D)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-23" (layer "F.Cu")
    (at 146.776 85.544 -90)
    (descr "SOT, 3 Pin (https://www.jedec.org/system/files/docs/to-236h.pdf variant AB), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOT TO_SOT_SMD")
    (property "PartNum" "863-BAT54SLT1G")
    (property "Sheetfile" "gate-delay.kicad_sch")
    (property "Sheetname" "")
    (property "Vendor" "Mouser")
    (property "ki_description" "Vr 30V, If 200mA, Dual schottky barrier diode, in series, SOT-323")
    (property "ki_keywords" "schottky diode")
    (attr smd)
    (fp_text reference "D2" (at -1.2414 -2.6268 90) (layer "F.SilkS"))
    (fp_text value "BAT54S" (at 0 2.4 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9375 -0.95 270) (size 1.475 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "-12V") (pinfunction "A") (pintype "passive"))
    (pad "2" smd roundrect (at -0.9375 0.95 270) (size 1.475 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "+12V") (pinfunction "K") (pintype "passive"))
    (pad "3" smd roundrect (at 0.9375 0 270) (size 1.475 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 5 "Net-(D2-COM)") (pinfunction "COM") (pintype "passive"))
    (model "${KICAD7_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_SMD:C_0805_2012Metric" (layer "F.Cu")
    (at 130.266 96.212 90)
    (descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
    (tags "capacitor")
    (property "Sheetfile" "gate-delay.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr smd)
    (fp_text reference "C4" (at -2.7432 0.508 90) (layer "F.SilkS"))
    (fp_text value "100n" (at 0 1.68 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.95 0 90) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "+12V") (pintype "passive"))
    (pad "2" smd roundrect (at 0.95 0 90) (size 1 1.45) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "-12V") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Eurorack:Mech-MountingHole" (layer "F.Cu")
    (at 101.534 107.2805)
    (property "Sheetfile" "gate-delay.kicad_sch")
    (property "Sheetname" "")
    (property "exclude_from_bom" "")
    (property "ki_description" "Mounting Hole with connection")
    (property "ki_keywords" "mounting hole")
    (attr through_hole exclude_from_bom)
    (fp_text reference "H1" (at 0 -2.54 unlocked) (layer "F.Fab"))
    (fp_text value "mount0" (at 0 2.54 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole oval (at 0 0 90) (size 3.5 7.8) (drill oval 3.2 7.5) (layers "*.Cu" "*.Mask")
      (net 6 "/FACE") (pinfunction "1") (pintype "output"))
  )
  (footprint "Eurorack:AudioJack2_Tayda_A-2566" (layer "F.Cu")
    (at 103.342 95.704 180)
    (property "PartNum" "A-2566")
    (property "Sheetfile" "gate-delay.kicad_sch")
    (property "Sheetname" "")
    (property "Vendor" "Tayda")
    (property "ki_description" "Audio Jack, 2 Poles (Mono / TS), Switched T Pole (Normalling)")
    (property "ki_keywords" "audio jack receptacle mono headphones phone TS connector")
    (attr through_hole)
    (fp_text reference "J4" (at 5.6642 -4.4704 270 unlocked) (layer "F.SilkS"))
    (fp_text value "slew_out" (at 0 1 180 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2.5 180 unlocked) (layer "F.Fab"))
    (pad "S" thru_hole oval (at -4.7 0.6 180) (size 2.25 3.75) (drill oval 1.45 2.95) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pintype "passive"))
    (pad "S" thru_hole oval (at 4.7 0.6 180) (size 2.25 2.7) (drill oval 1.45 1.9) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pintype "passive"))
    (pad "T" thru_hole oval (at 0 -4.8 180) (size 3.5 1.5) (drill oval 2.7 0.7) (layers "*.Cu" "*.Mask")
      (net 19 "/SLEW_OUT'") (pintype "passive"))
    (pad "TN" thru_hole oval (at 0 3.3 180) (size 3.5 1.5) (drill oval 2.7 0.7) (layers "*.Cu" "*.Mask")
      (net 20 "unconnected-(J4-PadTN)") (pintype "passive+no_connect"))
    (model "./models3d/A-2566.wrl"
      (offset (xyz 0 -0.15 11.5))
      (scale (xyz 0.385 0.385 0.385))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Eurorack:Mech-AudioJack-Hole-Output-CV" (layer "F.Cu")
    (at 103.342 129.4565)
    (property "Sheetfile" "gate-delay.kicad_sch")
    (property "Sheetname" "")
    (property "exclude_from_bom" "")
    (property "ki_description" "Mounting Hole with connection")
    (property "ki_keywords" "mounting hole")
    (attr through_hole exclude_from_bom)
    (fp_text reference "H7" (at 0.4 0.1 unlocked) (layer "F.Fab"))
    (fp_text value "slew" (at 0.058 6.1215 unlocked) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 7.7 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 90) (size 8 8) (drill 6.4) (layers "*.Cu" "*.Mask")
      (net 6 "/FACE") (pinfunction "1") (pintype "input"))
    (model "./models3d/A-2566.wrl"
      (offset (xyz 0 0 -1.5))
      (scale (xyz 0.385 0.385 0.385))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LED_THT:LED_D3.0mm" (layer "F.Cu")
    (at 114.259 95.704)
    (descr "LED, diameter 3.0mm, 2 pins")
    (tags "LED diameter 3.0mm 2 pins")
    (property "Sheetfile" "gate-delay.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Light emitting diode")
    (property "ki_keywords" "LED diode")
    (attr through_hole)
    (fp_text reference "D5" (at 1.27 -2.96) (layer "F.SilkS"))
    (fp_text value "LED_GREEN" (at 1.27 2.96) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.8 1.8) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 13 "Net-(D5-K)") (pinfunction "K") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.54 0) (size 1.8 1.8) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 14 "Net-(D5-A)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/LED_THT.3dshapes/LED_D3.0mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (at 147.792 88.846)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "gate-delay.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R1" (at -2.794 0) (layer "F.SilkS"))
    (fp_text value "10" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 5 "Net-(D2-COM)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 8 "Net-(J1-Pin_10)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_TO_SOT_SMD:SOT-23" (layer "F.Cu")
    (at 146.776 94.688 -90)
    (descr "SOT, 3 Pin (https://www.jedec.org/system/files/docs/to-236h.pdf variant AB), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOT TO_SOT_SMD")
    (property "PartNum" "863-BAT54SLT1G")
    (property "Sheetfile" "gate-delay.kicad_sch")
    (property "Sheetname" "")
    (property "Vendor" "Mouser")
    (property "ki_description" "Vr 30V, If 200mA, Dual schottky barrier diode, in series, SOT-323")
    (property "ki_keywords" "schottky diode")
    (attr smd)
    (fp_text reference "D1" (at -1.1652 -2.576 90) (layer "F.SilkS"))
    (fp_text value "BAT54S" (at 0 2.4 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9375 -0.95 270) (size 1.475 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "-12V") (pinfunction "A") (pintype "passive"))
    (pad "2" smd roundrect (at -0.9375 0.95 270) (size 1.475 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "+12V") (pinfunction "K") (pintype "passive"))
    (pad "3" smd roundrect (at 0.9375 0 270) (size 1.475 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 4 "Net-(D1-COM)") (pinfunction "COM") (pintype "passive"))
    (model "${KICAD7_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Eurorack:Mech-MountingHole" (layer "F.Cu")
    (at 152.3 140.79)
    (property "Sheetfile" "gate-delay.kicad_sch")
    (property "Sheetname" "")
    (property "exclude_from_bom" "")
    (property "ki_description" "Mounting Hole with connection")
    (property "ki_keywords" "mounting hole")
    (attr through_hole exclude_from_bom)
    (fp_text reference "H4" (at 0 -2.54 unlocked) (layer "F.Fab"))
    (fp_text value "mount1" (at 0 2.54 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole oval (at 0 0 90) (size 3.5 7.8) (drill oval 3.2 7.5) (layers "*.Cu" "*.Mask")
      (net 6 "/FACE") (pinfunction "1") (pintype "input"))
  )
  (footprint "Package_TO_SOT_SMD:SOT-23" (layer "F.Cu")
    (at 139.918 93.4942 90)
    (descr "SOT, 3 Pin (https://www.jedec.org/system/files/docs/to-236h.pdf variant AB), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOT TO_SOT_SMD")
    (property "PartNum" "863-MMBF170LT1G")
    (property "Sheetfile" "gate-delay.kicad_sch")
    (property "Sheetname" "")
    (property "Vendor" "Mouser")
    (property "ki_description" "0.5A Id, 60V Vds, N-Channel MOSFET, SOT-23")
    (property "ki_keywords" "N-Channel MOSFET")
    (attr smd)
    (fp_text reference "Q3" (at 1.2446 2.7432 180) (layer "F.SilkS"))
    (fp_text value "MMBF170" (at 0 2.4 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9375 -0.95 90) (size 1.475 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 21 "Net-(Q1A-C1)") (pinfunction "G") (pintype "input"))
    (pad "2" smd roundrect (at -0.9375 0.95 90) (size 1.475 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pinfunction "S") (pintype "passive"))
    (pad "3" smd roundrect (at 0.9375 0 90) (size 1.475 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 23 "Net-(Q3-D)") (pinfunction "D") (pintype "passive"))
    (model "${KICAD7_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Eurorack:Mech-LED-Hole-3mm-Bezel" (layer "F.Cu")
    (at 115.534 129.319)
    (property "Sheetfile" "gate-delay.kicad_sch")
    (property "Sheetname" "")
    (property "exclude_from_bom" "")
    (property "ki_description" "Mounting Hole with connection")
    (property "ki_keywords" "mounting hole")
    (attr through_hole exclude_from_bom)
    (fp_text reference "H9" (at 0 -3.81 unlocked) (layer "F.SilkS") hide)
    (fp_text value "led" (at 0 3.81 unlocked) (layer "F.Fab") hide)
    (fp_text user "${REFERENCE}" (at 0 5.08 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 6.65 6.65) (drill 6.2) (layers "*.Cu" "*.Mask")
      (net 6 "/FACE") (pinfunction "1") (pintype "output"))
  )
  (footprint "Diode_SMD:D_SOD-323_HandSoldering" (layer "F.Cu")
    (at 129.25 85.7218 -90)
    (descr "SOD-323")
    (tags "SOD-323")
    (property "Sheetfile" "gate-delay.kicad_sch")
    (property "Sheetname" "")
    (property "Sim.Device" "D")
    (property "Sim.Pins" "1=K 2=A")
    (property "ki_description" "Diode")
    (property "ki_keywords" "diode")
    (attr smd)
    (fp_text reference "D4" (at -0.127 1.6764 90) (layer "F.SilkS"))
    (fp_text value "1N4148" (at 0.1 1.9 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -1.85 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.25 0 270) (size 1 1) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 11 "Net-(D4-K)") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect (at 1.25 0 270) (size 1 1) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 12 "Net-(D4-A)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SOD-323.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (at 109.6158 99.1838 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "gate-delay.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R14" (at -0.0508 1.778 90) (layer "F.SilkS"))
    (fp_text value "1K" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 19 "/SLEW_OUT'") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 27 "Net-(U1B--)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Diode_SMD:D_SOD-323_HandSoldering" (layer "F.Cu")
    (at 138.4448 85.9504)
    (descr "SOD-323")
    (tags "SOD-323")
    (property "Sheetfile" "gate-delay.kicad_sch")
    (property "Sheetname" "")
    (property "Sim.Device" "D")
    (property "Sim.Pins" "1=K 2=A")
    (property "ki_description" "Diode")
    (property "ki_keywords" "diode")
    (attr smd)
    (fp_text reference "D3" (at -2.8092 0.2286 90) (layer "F.SilkS"))
    (fp_text value "1N4148" (at 0.1 1.9) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 -1.85) (layer "F.Fab"))
    (pad "1" smd roundrect (at -1.25 0) (size 1 1) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 10 "Net-(D3-K)") (pinfunction "K") (pintype "passive"))
    (pad "2" smd roundrect (at 1.25 0) (size 1 1) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 2 "GND") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SOD-323.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (at 128.234 81.988)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "gate-delay.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R10" (at 0 -1.65) (layer "F.SilkS"))
    (fp_text value "1K" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 26 "Net-(R10-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 11 "Net-(D4-K)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Eurorack:Mech-MountingHole" (layer "F.Cu")
    (at 152.3 107.14)
    (property "Sheetfile" "gate-delay.kicad_sch")
    (property "Sheetname" "")
    (property "exclude_from_bom" "")
    (property "ki_description" "Mounting Hole with connection")
    (property "ki_keywords" "mounting hole")
    (attr through_hole exclude_from_bom)
    (fp_text reference "H2" (at 0 -2.54 unlocked) (layer "F.Fab"))
    (fp_text value "mount1" (at 0 2.54 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole oval (at 0 0 90) (size 3.5 7.8) (drill oval 3.2 7.5) (layers "*.Cu" "*.Mask")
      (net 6 "/FACE") (pinfunction "1") (pintype "input"))
  )
  (footprint "Package_TO_SOT_SMD:SOT-23" (layer "F.Cu")
    (at 136.1221 93.4688 -90)
    (descr "SOT, 3 Pin (https://www.jedec.org/system/files/docs/to-236h.pdf variant AB), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOT TO_SOT_SMD")
    (property "PartNum" "512-BSS84")
    (property "Sheetfile" "gate-delay.kicad_sch")
    (property "Sheetname" "")
    (property "Vendor" "Mouser")
    (property "ki_description" "-0.13A Id, -50V Vds, P-Channel MOSFET, SOT-23")
    (property "ki_keywords" "P-Channel MOSFET")
    (attr smd)
    (fp_text reference "Q2" (at -1.0922 2.7432 -180) (layer "F.SilkS"))
    (fp_text value "BSS84" (at 0 2.4 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9375 -0.95 270) (size 1.475 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 21 "Net-(Q1A-C1)") (pinfunction "G") (pintype "input"))
    (pad "2" smd roundrect (at -0.9375 0.95 270) (size 1.475 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "+12V") (pinfunction "S") (pintype "passive"))
    (pad "3" smd roundrect (at 0.9375 0 270) (size 1.475 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 22 "Net-(Q2-D)") (pinfunction "D") (pintype "passive"))
    (model "${KICAD7_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (at 111.978 94.18 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "gate-delay.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R12" (at 0 -1.65 90) (layer "F.SilkS"))
    (fp_text value "1K" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 13 "Net-(D5-K)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (at 128.234 90.624)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "gate-delay.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R8" (at 0 -1.65) (layer "F.SilkS"))
    (fp_text value "110K" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 25 "Net-(U1A--)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 1 "+12V") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_SO:TSOP-6_1.65x3.05mm_P0.95mm" (layer "F.Cu")
    (at 137.5152 89.3286 -90)
    (descr "TSOP-6 package (comparable to TSOT-23), https://www.vishay.com/docs/71200/71200.pdf")
    (tags "Jedec MO-193C TSOP-6L")
    (property "PartNum" "771-BCM847DS135")
    (property "Sheetfile" "gate-delay.kicad_sch")
    (property "Sheetname" "")
    (property "Vendor" "Mouser")
    (property "ki_description" "Dual NPN transistor, 6 pin package")
    (property "ki_keywords" "transistor NPN")
    (attr smd)
    (fp_text reference "Q1" (at -1.143 -2.5044 90) (layer "F.SilkS"))
    (fp_text value "BCM847" (at 0 2.5 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd rect (at -1.16 -0.95 270) (size 0.7 0.51) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 2 "GND") (pinfunction "E1") (pintype "passive"))
    (pad "2" smd rect (at -1.16 0 270) (size 0.7 0.51) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 10 "Net-(D3-K)") (pinfunction "B1") (pintype "input"))
    (pad "3" smd rect (at -1.16 0.95 270) (size 0.7 0.51) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 1 "+12V") (pinfunction "C2") (pintype "passive"))
    (pad "4" smd rect (at 1.16 0.95 270) (size 0.7 0.51) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 14 "Net-(D5-A)") (pinfunction "E2") (pintype "passive"))
    (pad "5" smd rect (at 1.16 0 270) (size 0.7 0.51) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 11 "Net-(D4-K)") (pinfunction "B2") (pintype "input"))
    (pad "6" smd rect (at 1.16 -0.95 270) (size 0.7 0.51) (layers "F.Cu" "F.Paste" "F.Mask")
      (net 21 "Net-(Q1A-C1)") (pinfunction "C1") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Package_SO.3dshapes/TSOP-6_1.65x3.05mm_P0.95mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm" (layer "F.Cu")
    (at 125.694 96.212 -90)
    (descr "SOIC, 8 Pin (JEDEC MS-012AA, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_narrow-r/r_8.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "SOIC SO")
    (property "PartNum" "771-BCM847DS135")
    (property "Sheetfile" "gate-delay.kicad_sch")
    (property "Sheetname" "")
    (property "Vendor" "Mouser")
    (property "ki_description" "Dual Low-Noise JFET-Input Operational Amplifiers, DIP-8/SOIC-8")
    (property "ki_keywords" "dual opamp")
    (attr smd)
    (fp_text reference "U1" (at -2.6416 -3.8862 -180) (layer "F.SilkS"))
    (fp_text value "TL072" (at 0 3.4 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -2.475 -1.905 270) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 12 "Net-(D4-A)") (pintype "output"))
    (pad "2" smd roundrect (at -2.475 -0.635 270) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 25 "Net-(U1A--)") (pinfunction "-") (pintype "input"))
    (pad "3" smd roundrect (at -2.475 0.635 270) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 9 "Net-(U1A-+)") (pinfunction "+") (pintype "input"))
    (pad "4" smd roundrect (at -2.475 1.905 270) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 3 "-12V") (pinfunction "V-") (pintype "power_in"))
    (pad "5" smd roundrect (at 2.475 1.905 270) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 9 "Net-(U1A-+)") (pinfunction "+") (pintype "input"))
    (pad "6" smd roundrect (at 2.475 0.635 270) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 27 "Net-(U1B--)") (pinfunction "-") (pintype "input"))
    (pad "7" smd roundrect (at 2.475 -0.635 270) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 27 "Net-(U1B--)") (pintype "output"))
    (pad "8" smd roundrect (at 2.475 -1.905 270) (size 1.95 0.6) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25)
      (net 1 "+12V") (pinfunction "V+") (pintype "power_in"))
    (model "${KICAD7_3DMODEL_DIR}/Package_SO.3dshapes/SOIC-8_3.9x4.9mm_P1.27mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Eurorack:Mech-Potentiometer-Hole_level_90deg" (layer "F.Cu")
    (at 148.806 123.731)
    (property "Sheetfile" "gate-delay.kicad_sch")
    (property "Sheetname" "")
    (property "exclude_from_bom" "")
    (property "ki_description" "Mounting Hole with connection")
    (property "ki_keywords" "mounting hole")
    (attr through_hole exclude_from_bom)
    (fp_text reference "H8" (at 0 -9.906 unlocked) (layer "F.Fab"))
    (fp_text value "delay" (at 0 11.43 unlocked) (layer "F.SilkS"))
    (fp_text user "10" (at 6.35 6.35 unlocked) (layer "F.SilkS"))
    (fp_text user "0" (at -5.08 6.35 unlocked) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 7.62 unlocked) (layer "F.Fab"))
    (pad "" thru_hole oval (at 0 -7.8) (size 3.3 1.5) (drill oval 3.1 1.3) (layers "*.Cu" "*.Mask"))
    (pad "1" thru_hole circle (at 0 0) (size 12 12) (drill 7.5) (layers "*.Cu" "*.Mask")
      (net 6 "/FACE") (pinfunction "1") (pintype "input"))
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (at 141.6452 89.3286 -90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "gate-delay.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R5" (at 0 -1.65 90) (layer "F.SilkS"))
    (fp_text value "22K" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 1 "+12V") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 270) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 21 "Net-(Q1A-C1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (at 139.9688 83.258)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "gate-delay.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R4" (at 0 -1.65) (layer "F.SilkS"))
    (fp_text value "22K" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 10 "Net-(D3-K)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Eurorack:Mech-MountingHole" (layer "F.Cu")
    (at 102 140.79)
    (property "Sheetfile" "gate-delay.kicad_sch")
    (property "Sheetname" "")
    (property "exclude_from_bom" "")
    (property "ki_description" "Mounting Hole with connection")
    (property "ki_keywords" "mounting hole")
    (attr through_hole exclude_from_bom)
    (fp_text reference "H3" (at 0 -2.54 unlocked) (layer "F.Fab"))
    (fp_text value "mount1" (at 0 2.54 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole oval (at 0 0 90) (size 3.5 7.8) (drill oval 3.2 7.5) (layers "*.Cu" "*.Mask")
      (net 6 "/FACE") (pinfunction "1") (pintype "input"))
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (at 124.17 86.56 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "gate-delay.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R13" (at 0 -1.65 90) (layer "F.SilkS"))
    (fp_text value "1K" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 17 "/GATE_OUT'") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 26 "Net-(R10-Pad1)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Eurorack:Mech-AudioJack-Hole-Output-Gate" (layer "F.Cu")
    (at 115.534 118.2805)
    (property "Sheetfile" "gate-delay.kicad_sch")
    (property "Sheetname" "")
    (property "exclude_from_bom" "")
    (property "ki_description" "Mounting Hole with connection")
    (property "ki_keywords" "mounting hole")
    (attr through_hole exclude_from_bom)
    (fp_text reference "H6" (at 0.4 0.1 unlocked) (layer "F.Fab"))
    (fp_text value "output" (at -0.025 -6.6 unlocked) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 7.7 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 90) (size 8 8) (drill 6.4) (layers "*.Cu" "*.Mask")
      (net 6 "/FACE") (pinfunction "1") (pintype "input"))
    (model "./models3d/A-2566.wrl"
      (offset (xyz 0 0 -1.5))
      (scale (xyz 0.385 0.385 0.385))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Eurorack:Potentiometer_RV16AF-41-15R1" (layer "F.Cu")
    (at 148.806 90.116 -90)
    (descr "Alpha 16mm Potentiometer Single -- Tayda Electronics ")
    (property "Sheetfile" "gate-delay.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Potentiometer")
    (property "ki_keywords" "resistor variable")
    (attr through_hole)
    (fp_text reference "RV1" (at -8.2804 -5.2598 -90 unlocked) (layer "F.SilkS"))
    (fp_text value "A1M" (at 0 4.826 -90 unlocked) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 6.604 -90 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole circle (at -5 16 270) (size 2.2 2.2) (drill 1.2) (layers "*.Cu" "*.Mask")
      (net 24 "Net-(R6-Pad1)") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle (at 0 16 270) (size 2.2 2.2) (drill 1.2) (layers "*.Cu" "*.Mask")
      (net 9 "Net-(U1A-+)") (pinfunction "2") (pintype "passive"))
    (pad "3" thru_hole circle (at 5 16 270) (size 2.2 2.2) (drill 1.2) (layers "*.Cu" "*.Mask")
      (net 9 "Net-(U1A-+)") (pinfunction "3") (pintype "passive"))
  )
  (footprint "Eurorack:Mech-AudioJack-Hole-Input-Gate" (layer "F.Cu")
    (at 103.342 118.143)
    (property "Sheetfile" "gate-delay.kicad_sch")
    (property "Sheetname" "")
    (property "exclude_from_bom" "")
    (property "ki_description" "Mounting Hole with connection")
    (property "ki_keywords" "mounting hole")
    (attr through_hole exclude_from_bom)
    (fp_text reference "H5" (at 0.4 0.1 unlocked) (layer "F.Fab"))
    (fp_text value "input" (at -0.025 -6.6 unlocked) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 7.7 unlocked) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 90) (size 8 8) (drill 6.4) (layers "*.Cu" "*.Mask")
      (net 6 "/FACE") (pinfunction "1") (pintype "input"))
    (model "./models3d/A-2566.wrl"
      (offset (xyz 0 0 -1.5))
      (scale (xyz 0.385 0.385 0.385))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (at 124.17 81.48 90)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "gate-delay.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R11" (at 0 -1.65 90) (layer "F.SilkS"))
    (fp_text value "10K" (at 0 1.65 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0 90) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 26 "Net-(R10-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 90) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Resistor_SMD:R_0805_2012Metric" (layer "F.Cu")
    (at 136.1334 96.9994 180)
    (descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
    (tags "resistor")
    (property "Sheetfile" "gate-delay.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (attr smd)
    (fp_text reference "R6" (at 0 -1.65) (layer "F.SilkS"))
    (fp_text value "1K" (at 0 1.65) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" smd roundrect (at -0.9125 0 180) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 24 "Net-(R6-Pad1)") (pintype "passive"))
    (pad "2" smd roundrect (at 0.9125 0 180) (size 1.025 1.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.243902)
      (net 22 "Net-(Q2-D)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Eurorack:PinHeader_2x05_P2.54mm_Vertical" (layer "B.Cu")
    (at 151.094 95.196)
    (descr "Through hole straight pin header, 2x05, 2.54mm pitch, double rows")
    (tags "Through hole pin header THT 2x05 2.54mm double row")
    (property "PartNum" "A-2939")
    (property "Sheetfile" "gate-delay.kicad_sch")
    (property "Sheetname" "")
    (property "Vendor" "Tayda")
    (property "ki_description" "Generic connector, double row, 02x05, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)")
    (property "ki_keywords" "connector")
    (attr through_hole)
    (fp_text reference "J1" (at -4.572 -1.524) (layer "B.SilkS"))
    (fp_text value "Conn_02x05_Odd_Even" (at 1.2446 -16.2052) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 1.27 -5.08 90) (layer "B.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 7 "Net-(J1-Pin_1)") (pinfunction "Pin_1") (pintype "passive"))
    (pad "2" thru_hole oval (at 2.54 0) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 7 "Net-(J1-Pin_1)") (pinfunction "Pin_2") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 -2.54) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "Pin_3") (pintype "passive"))
    (pad "4" thru_hole oval (at 2.54 -2.54) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "Pin_4") (pintype "passive"))
    (pad "5" thru_hole oval (at 0 -5.08) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "Pin_5") (pintype "passive"))
    (pad "6" thru_hole oval (at 2.54 -5.08) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "Pin_6") (pintype "passive"))
    (pad "7" thru_hole oval (at 0 -7.62) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "Pin_7") (pintype "passive"))
    (pad "8" thru_hole oval (at 2.54 -7.62) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "Pin_8") (pintype "passive"))
    (pad "9" thru_hole oval (at 0 -10.16) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 8 "Net-(J1-Pin_10)") (pinfunction "Pin_9") (pintype "passive"))
    (pad "10" thru_hole oval (at 2.54 -10.16) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 8 "Net-(J1-Pin_10)") (pinfunction "Pin_10") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x05_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:CP_Radial_D5.0mm_P2.50mm" (layer "B.Cu")
    (at 143.284888 97.736)
    (descr "CP, Radial series, Radial, pin pitch=2.50mm, , diameter=5mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.50mm  diameter 5mm Electrolytic Capacitor")
    (property "Sheetfile" "gate-delay.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Polarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr through_hole)
    (fp_text reference "C1" (at -0.572888 -3.302 90) (layer "B.SilkS"))
    (fp_text value "22u 50V" (at 1.25 -3.75) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 1.25 0) (layer "B.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 1 "+12V") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.5 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/CP_Radial_D5.0mm_P2.50mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:CP_Radial_D5.0mm_P2.50mm" (layer "B.Cu")
    (at 145.695113 82.242 180)
    (descr "CP, Radial series, Radial, pin pitch=2.50mm, , diameter=5mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.50mm  diameter 5mm Electrolytic Capacitor")
    (property "Sheetfile" "gate-delay.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Polarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr through_hole)
    (fp_text reference "C2" (at 2.983113 -3.556 90) (layer "B.SilkS"))
    (fp_text value "22u 50V" (at 1.25 -3.75) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 1.25 0) (layer "B.Fab"))
    (pad "1" thru_hole rect (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.5 0 180) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 3 "-12V") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/CP_Radial_D5.0mm_P2.50mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "Capacitor_THT:C_Rect_L7.2mm_W5.5mm_P5.00mm_FKS2_FKP2_MKS2_MKP2" (layer "B.Cu")
    (at 121.0966 93.4834 -90)
    (descr "C, Rect series, Radial, pin pitch=5.00mm, , length*width=7.2*5.5mm^2, Capacitor, http://www.wima.com/EN/WIMA_FKS_2.pdf")
    (tags "C Rect series Radial pin pitch 5.00mm  length 7.2mm width 5.5mm Capacitor")
    (property "Sheetfile" "gate-delay.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr through_hole)
    (fp_text reference "C3" (at -2.0974 0.3302 -180) (layer "B.SilkS"))
    (fp_text value "1u box" (at 2.5 -4 90) (layer "B.Fab"))
    (fp_text user "${REFERENCE}" (at 2.5 0 90) (layer "B.Fab"))
    (pad "1" thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 9 "Net-(U1A-+)") (pintype "passive"))
    (pad "2" thru_hole circle (at 5 0 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Rect_L7.2mm_W5.5mm_P5.00mm_FKS2_FKP2_MKS2_MKP2.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_rect (start 96.7 79.1) (end 157.3 101.6)
    (fill none) (layer "Edge.Cuts"))
  (gr_rect (start 96.7 104.14) (end 157.3 143.79)
    (fill none) (layer "Edge.Cuts"))
  (gr_text "POWER" (at 146.014 90.116 -90) (layer "B.SilkS"))
  (gr_text "thismatters/gate-delay/v0" (at 131.028 80.718) (layer "B.SilkS"))
  (gr_text "gate delay" (at 127.2032 142.5194) (layer "F.SilkS"))
  (gr_text "thismatters/gate-delay/v0" (at 97.05 125.418 -90) (layer "F.SilkS"))
  (zone (net 2) (net_name "GND") (layers "F&B.Cu") (hatch edge 0.5)
    (connect_pads (clearance 0.5))
    (min_thickness 0.25) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy 157.698 78.432)
        (xy 96.23 78.432)
        (xy 96.23 101.8)
        (xy 157.698 101.8)
      )
    )
  )
  (zone (net 6) (net_name "/FACE") (layers "F&B.Cu") (hatch edge 0.5)
    (priority 1)
    (connect_pads (clearance 0.5))
    (min_thickness 0.25) (filled_areas_thickness no)
    (fill yes (thermal_gap 0.5) (thermal_bridge_width 0.5))
    (polygon
      (pts
        (xy 95.78 103.574)
        (xy 157.756 103.574)
        (xy 157.756 144.722)
        (xy 95.78 144.722)
      )
    )
  )
)
