(kicad_pcb
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(general
		(thickness 1.6)
		(legacy_teardrops no)
	)
	(paper "A4")
	(layers
		(0 "F.Cu" signal)
		(2 "B.Cu" signal)
		(9 "F.Adhes" user "F.Adhesive")
		(11 "B.Adhes" user "B.Adhesive")
		(13 "F.Paste" user)
		(15 "B.Paste" user)
		(5 "F.SilkS" user "F.Silkscreen")
		(7 "B.SilkS" user "B.Silkscreen")
		(1 "F.Mask" user)
		(3 "B.Mask" user)
		(17 "Dwgs.User" user "User.Drawings")
		(19 "Cmts.User" user "User.Comments")
		(21 "Eco1.User" user "User.Eco1")
		(23 "Eco2.User" user "User.Eco2")
		(25 "Edge.Cuts" user)
		(27 "Margin" user)
		(31 "F.CrtYd" user "F.Courtyard")
		(29 "B.CrtYd" user "B.Courtyard")
		(35 "F.Fab" user)
		(33 "B.Fab" user)
		(39 "User.1" user)
		(41 "User.2" user)
		(43 "User.3" user)
		(45 "User.4" user)
	)
	(setup
		(stackup
			(layer "F.SilkS"
				(type "Top Silk Screen")
			)
			(layer "F.Paste"
				(type "Top Solder Paste")
			)
			(layer "F.Mask"
				(type "Top Solder Mask")
				(thickness 0.01)
			)
			(layer "F.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "dielectric 1"
				(type "core")
				(thickness 1.51)
				(material "FR4")
				(epsilon_r 4.5)
				(loss_tangent 0.02)
			)
			(layer "B.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "B.Mask"
				(type "Bottom Solder Mask")
				(thickness 0.01)
			)
			(layer "B.Paste"
				(type "Bottom Solder Paste")
			)
			(layer "B.SilkS"
				(type "Bottom Silk Screen")
			)
			(copper_finish "None")
			(dielectric_constraints no)
		)
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(tenting front back)
		(pcbplotparams
			(layerselection 0x00000000_00000000_55555555_5755f5ff)
			(plot_on_all_layers_selection 0x00000000_00000000_00000000_02000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 4)
			(plotframeref no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(pdf_metadata yes)
			(pdf_single_document yes)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plot_black_and_white no)
			(sketchpadsonfab no)
			(plotpadnumbers no)
			(hidednponfab no)
			(sketchdnponfab yes)
			(crossoutdnponfab yes)
			(subtractmaskfromsilk no)
			(outputformat 4)
			(mirror no)
			(drillshape 0)
			(scaleselection 1)
			(outputdirectory "../../StrikeSense_Updated PCB Files_3.16/Updated StrikeSense_PCB Files_3.16/")
		)
	)
	(net 0 "")
	(net 1 "Net-(SW+1-Pin_1)")
	(net 2 "Net-(D1-A)")
	(net 3 "Net-(D1-K)")
	(net 4 "Net-(J1-Pin_8)")
	(net 5 "GND")
	(net 6 "/DATA_LA")
	(net 7 "Net-(J1-Pin_10)")
	(net 8 "/DATA_T")
	(net 9 "+3.3V")
	(net 10 "Net-(J1-Pin_9)")
	(net 11 "/DATA_LL")
	(net 12 "Net-(J1-Pin_7)")
	(net 13 "+5V")
	(net 14 "/DATA_RA")
	(net 15 "/DATA_RL")
	(net 16 "Net-(J3-Pin_10)")
	(net 17 "Net-(J3-Pin_4)")
	(net 18 "Net-(J3-Pin_6)")
	(net 19 "Net-(J3-Pin_8)")
	(net 20 "Net-(J3-Pin_7)")
	(net 21 "Net-(J3-Pin_5)")
	(net 22 "Net-(J3-Pin_9)")
	(net 23 "Net-(LED1-A)")
	(net 24 "Net-(U2-SDI{slash}SD1)")
	(net 25 "Net-(U2-SDO{slash}SD0)")
	(net 26 "Net-(U2-IO15)")
	(net 27 "Net-(U2-SCS{slash}CMD)")
	(net 28 "Net-(U1-S0)")
	(net 29 "Net-(U1-S1)")
	(net 30 "Net-(U1-S2)")
	(net 31 "Net-(U1-COM)")
	(net 32 "Net-(U1-S3)")
	(net 33 "unconnected-(U2-SENSOR_VN-Pad5)")
	(net 34 "unconnected-(U2-NC-Pad32)")
	(net 35 "unconnected-(U2-IO14-Pad13)")
	(net 36 "unconnected-(U2-TXD0{slash}IO1-Pad35)")
	(net 37 "unconnected-(U2-SENSOR_VP-Pad4)")
	(net 38 "unconnected-(U2-IO27-Pad12)")
	(net 39 "Net-(U2-GND-Pad1)")
	(net 40 "Net-(U2-IO12)")
	(net 41 "/PSPSRA1")
	(net 42 "/PSRL1")
	(net 43 "/PS_T")
	(net 44 "/PSRL2")
	(net 45 "/PSRA2")
	(footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal"
		(layer "F.Cu")
		(at 120.25 60.75)
		(descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
		(property "Reference" "R19"
			(at 3.81 -2.37 0)
			(layer "F.SilkS")
		)
		(property "Value" "330"
			(at 28.5 -2.5 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "StrikeSense_PCB.kicad_sch")
		(attr through_hole)
		(fp_text user "D_Ex1"
			(at 3.81 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 17 "Net-(J3-Pin_4)")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 7.62 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 26 "Net-(U2-IO15)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_BarrelJack:BarrelJack_Horizontal"
		(layer "F.Cu")
		(at 141.351 42.926 180)
		(descr "DC Barrel Jack")
		(tags "Power Jack")
		(property "Reference" "Battery1"
			(at -8.75 6 0)
			(layer "F.SilkS")
		)
		(property "Value" "Barrel_Jack"
			(at -6.2 -5.5 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "DC Barrel Jack"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "BarrelJack*")
		(sheetname "/")
		(sheetfile "StrikeSense_PCB.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at -3 -2.95 0)
			(layer "F.Fab")
		)
		(pad "GND" thru_hole roundrect
			(at -6 0 180)
			(size 3 3.5)
			(drill oval 1 3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 5 "GND")
			(zone_connect 2)
			(thermal_gap 0)
		)
		(pad "GND" thru_hole roundrect
			(at -3 4.7 180)
			(size 3.5 3.5)
			(drill oval 3 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
		)
		(pad "V+" thru_hole rect
			(at 0 0 180)
			(size 3.5 3.5)
			(drill oval 1 3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "Net-(SW+1-Pin_1)")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_BarrelJack.3dshapes/BarrelJack_Horizontal.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal"
		(layer "F.Cu")
		(at 134.19 104.5)
		(descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
		(property "Reference" "R11"
			(at -2.364 -0.106 0)
			(layer "F.SilkS")
		)
		(property "Value" "1000"
			(at 3.81 2.37 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "StrikeSense_PCB.kicad_sch")
		(attr through_hole)
		(fp_text user "PS_Ex2"
			(at 3.81 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 19 "Net-(J3-Pin_8)")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 7.62 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "GND")
			(pintype "passive")
			(zone_connect 2)
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "capstoneespslot:ESP32 DevKit V4"
		(layer "F.Cu")
		(at 168.2 137.3)
		(property "Reference" "U2"
			(at 14.7 -17.47 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "ESP32-WROOM-32"
			(at 14.73 -15.97 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.espressif.com/sites/default/files/documentation/esp32-wroom-32_datasheet_en.pdf"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "RF Module, ESP32-D0WDQ6 SoC, Wi-Fi 802.11b/g/n, Bluetooth, BLE, 32-bit, 2.7-3.6V, onboard antenna, SMD"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "ESP32?WROOM?32*")
		(sheetname "/")
		(sheetfile "StrikeSense_PCB.kicad_sch")
		(attr smd)
		(pad "0" thru_hole circle
			(at 26.7 -13.99)
			(size 1.4 1.4)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "2" thru_hole circle
			(at 26.7 -11.45)
			(size 1.4 1.4)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(pinfunction "VDD")
			(pintype "power_in")
		)
		(pad "3v3" thru_hole circle
			(at 1.3 -46.97)
			(size 1.4 1.4)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 9 "+3.3V")
		)
		(pad "4" thru_hole circle
			(at 26.7 -16.53)
			(size 1.4 1.4)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 37 "unconnected-(U2-SENSOR_VP-Pad4)")
			(pinfunction "SENSOR_VP")
			(pintype "input")
		)
		(pad "5" thru_hole circle
			(at 26.7 -24.11)
			(size 1.4 1.4)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 33 "unconnected-(U2-SENSOR_VN-Pad5)")
			(pinfunction "SENSOR_VN")
			(pintype "input")
		)
		(pad "5V" thru_hole circle
			(at 1.3 -1.29)
			(size 1.4 1.4)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "12" thru_hole circle
			(at 1.3 -16.53)
			(size 1.4 1.4)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 38 "unconnected-(U2-IO27-Pad12)")
			(pinfunction "IO27")
			(pintype "bidirectional")
		)
		(pad "13" thru_hole circle
			(at 1.3 -11.45)
			(size 1.4 1.4)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 35 "unconnected-(U2-IO14-Pad13)")
			(pinfunction "IO14")
			(pintype "bidirectional")
		)
		(pad "14" thru_hole circle
			(at 1.3 -19.07)
			(size 1.4 1.4)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 40 "Net-(U2-IO12)")
			(pinfunction "IO12")
			(pintype "bidirectional")
		)
		(pad "15" thru_hole circle
			(at 26.7 -8.91)
			(size 1.4 1.4)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 39 "Net-(U2-GND-Pad1)")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "16" thru_hole circle
			(at 26.7 -19.07)
			(size 1.4 1.4)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 11 "/DATA_LL")
			(pinfunction "IO13")
			(pintype "bidirectional")
		)
		(pad "17" thru_hole circle
			(at 26.7 -21.61)
			(size 1.4 1.4)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "/DATA_LA")
			(pinfunction "SHD/SD2")
			(pintype "bidirectional")
		)
		(pad "18" thru_hole circle
			(at 26.7 -26.65)
			(size 1.4 1.4)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 8 "/DATA_T")
			(pinfunction "SWP/SD3")
			(pintype "bidirectional")
		)
		(pad "19" thru_hole circle
			(at 26.7 -29.19)
			(size 1.4 1.4)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 27 "Net-(U2-SCS{slash}CMD)")
			(pinfunction "SCS/CMD")
			(pintype "bidirectional")
		)
		(pad "21" thru_hole circle
			(at 26.7 -34.27)
			(size 1.4 1.4)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 25 "Net-(U2-SDO{slash}SD0)")
			(pinfunction "SDO/SD0")
			(pintype "bidirectional")
		)
		(pad "22" thru_hole circle
			(at 26.7 -41.89)
			(size 1.4 1.4)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 24 "Net-(U2-SDI{slash}SD1)")
			(pinfunction "SDI/SD1")
			(pintype "bidirectional")
		)
		(pad "23" thru_hole circle
			(at 26.7 -44.43)
			(size 1.4 1.4)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 26 "Net-(U2-IO15)")
			(pinfunction "IO15")
			(pintype "bidirectional")
		)
		(pad "25" thru_hole circle
			(at 1.3 -26.65)
			(size 1.4 1.4)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 30 "Net-(U1-S2)")
			(pinfunction "IO0")
			(pintype "bidirectional")
		)
		(pad "26" thru_hole circle
			(at 1.3 -24.15)
			(size 1.4 1.4)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 29 "Net-(U1-S1)")
			(pinfunction "IO4")
			(pintype "bidirectional")
		)
		(pad "27" thru_hole circle
			(at 1.3 -21.61)
			(size 1.4 1.4)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 28 "Net-(U1-S0)")
			(pinfunction "IO16")
			(pintype "bidirectional")
		)
		(pad "32" thru_hole circle
			(at 1.3 -31.73)
			(size 1.4 1.4)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 34 "unconnected-(U2-NC-Pad32)")
			(pinfunction "NC")
			(pintype "no_connect")
		)
		(pad "33" thru_hole circle
			(at 1.3 -29.19)
			(size 1.4 1.4)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 32 "Net-(U1-S3)")
			(pinfunction "IO21")
			(pintype "bidirectional")
		)
		(pad "34" thru_hole circle
			(at 1.3 -36.81)
			(size 1.4 1.4)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 31 "Net-(U1-COM)")
			(pinfunction "RXD0/IO3")
			(pintype "bidirectional")
		)
		(pad "35" thru_hole circle
			(at 1.3 -34.27)
			(size 1.4 1.4)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 36 "unconnected-(U2-TXD0{slash}IO1-Pad35)")
			(pinfunction "TXD0/IO1")
			(pintype "bidirectional")
		)
		(pad "CLK" thru_hole circle
			(at 26.7 -1.29)
			(size 1.4 1.4)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "CMD" thru_hole circle
			(at 1.3 -3.83)
			(size 1.4 1.4)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "D0" thru_hole circle
			(at 26.7 -3.83)
			(size 1.4 1.4)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "D1" thru_hole circle
			(at 26.7 -6.37)
			(size 1.4 1.4)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "D2" thru_hole circle
			(at 1.3 -8.91)
			(size 1.4 1.4)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "D3" thru_hole circle
			(at 1.3 -6.37)
			(size 1.4 1.4)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "EN" thru_hole circle
			(at 1.3 -44.43)
			(size 1.4 1.4)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "GND" thru_hole circle
			(at 1.3 -13.99)
			(size 1.4 1.4)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "GND")
			(zone_connect 2)
		)
		(pad "GND" thru_hole rect
			(at 26.7 -46.97)
			(size 1.4 1.4)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "GND")
			(zone_connect 2)
		)
		(pad "GND" thru_hole circle
			(at 26.7 -31.73)
			(size 1.4 1.4)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "GND")
			(zone_connect 2)
		)
		(pad "RX" thru_hole circle
			(at 26.7 -36.81)
			(size 1.4 1.4)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "TX" thru_hole circle
			(at 26.7 -39.35)
			(size 1.4 1.4)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "VN" thru_hole circle
			(at 1.3 -39.35)
			(size 1.4 1.4)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "VP" thru_hole circle
			(at 1.3 -41.89)
			(size 1.4 1.4)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(embedded_fonts no)
	)
	(footprint "MountingHole:MountingHole_3.2mm_M3_ISO14580"
		(layer "F.Cu")
		(at 205.105 145.415)
		(descr "Mounting Hole 3.2mm, M3, no annular, generated by kicad-footprint-generator mountinghole.py")
		(tags "mountinghole M3 ISO14580")
		(property "Reference" "REF**"
			(at 0 -3.7 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "MountingHole_3.2mm_M3_ISO14580"
			(at 0 3.7 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 3.2 3.2)
			(drill 3.2)
			(layers "*.Cu" "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal"
		(layer "F.Cu")
		(at 200 129.159)
		(descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
		(property "Reference" "R2"
			(at 9.677 0.08 0)
			(layer "F.SilkS")
		)
		(property "Value" "1000"
			(at 3.81 2.37 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "StrikeSense_PCB.kicad_sch")
		(attr through_hole)
		(fp_text user "PSRA1"
			(at 3.81 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "GND")
			(pintype "passive")
			(zone_connect 2)
		)
		(pad "2" thru_hole circle
			(at 7.62 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 41 "/PSPSRA1")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal"
		(layer "F.Cu")
		(at 200.152 111.125)
		(descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
		(property "Reference" "R17"
			(at 3.683 -2.413 0)
			(layer "F.SilkS")
		)
		(property "Value" "330"
			(at 28.5 -2.5 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "StrikeSense_PCB.kicad_sch")
		(attr through_hole)
		(fp_text user "DataRA"
			(at 3.81 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 24 "Net-(U2-SDI{slash}SD1)")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 7.62 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 14 "/DATA_RA")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal"
		(layer "F.Cu")
		(at 132.44 127.25)
		(descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
		(property "Reference" "R6"
			(at -2.392 0.004 0)
			(layer "F.SilkS")
		)
		(property "Value" "1000"
			(at 3.81 2.37 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "StrikeSense_PCB.kicad_sch")
		(attr through_hole)
		(fp_text user "PSLA1"
			(at 3.81 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 12 "Net-(J1-Pin_7)")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 7.62 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal"
		(layer "F.Cu")
		(at 134.25 101)
		(descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
		(property "Reference" "R10"
			(at -2.424 0.092 0)
			(layer "F.SilkS")
		)
		(property "Value" "1000"
			(at 3.81 2.37 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "StrikeSense_PCB.kicad_sch")
		(attr through_hole)
		(fp_text user "PS_Ex1"
			(at 3.81 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 20 "Net-(J3-Pin_7)")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 7.62 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "GND")
			(pintype "passive")
			(zone_connect 2)
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal"
		(layer "F.Cu")
		(at 200 136.525)
		(descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
		(property "Reference" "R4"
			(at 9.8 -0.625 0)
			(layer "F.SilkS")
		)
		(property "Value" "1000"
			(at 3.81 2.37 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "StrikeSense_PCB.kicad_sch")
		(attr through_hole)
		(fp_text user "PSRL1"
			(at 3.81 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "GND")
			(pintype "passive")
			(zone_connect 2)
		)
		(pad "2" thru_hole circle
			(at 7.62 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 42 "/PSRL1")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal"
		(layer "F.Cu")
		(at 200 132.842)
		(descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
		(property "Reference" "R3"
			(at 9.677 0.508 0)
			(layer "F.SilkS")
		)
		(property "Value" "1000"
			(at 3.81 2.37 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "StrikeSense_PCB.kicad_sch")
		(attr through_hole)
		(fp_text user "PSRA2"
			(at 3.81 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "GND")
			(pintype "passive")
			(zone_connect 2)
		)
		(pad "2" thru_hole circle
			(at 7.62 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 45 "/PSRA2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal"
		(layer "F.Cu")
		(at 120.25 65.75)
		(descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
		(property "Reference" "R20"
			(at 3.81 -2.37 0)
			(layer "F.SilkS")
		)
		(property "Value" "330"
			(at 28.5 -2.5 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "StrikeSense_PCB.kicad_sch")
		(attr through_hole)
		(fp_text user "D_Ex2"
			(at 3.81 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 21 "Net-(J3-Pin_5)")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 7.62 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 27 "Net-(U2-SCS{slash}CMD)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal"
		(layer "F.Cu")
		(at 147.19 92.2)
		(descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
		(property "Reference" "R22"
			(at 3.81 -2.37 0)
			(layer "F.SilkS")
		)
		(property "Value" "330"
			(at 3.81 2.37 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "StrikeSense_PCB.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 3.81 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 9 "+3.3V")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 7.62 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 23 "Net-(LED1-A)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal"
		(layer "F.Cu")
		(at 120.25 70.75)
		(descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
		(property "Reference" "R21"
			(at 3.81 -2.37 0)
			(layer "F.SilkS")
		)
		(property "Value" "330"
			(at 28.5 -2.5 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "StrikeSense_PCB.kicad_sch")
		(attr through_hole)
		(fp_text user "D_Ex3"
			(at 3.81 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 18 "Net-(J3-Pin_6)")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 7.62 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 40 "Net-(U2-IO12)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal"
		(layer "F.Cu")
		(at 120.5 114.5)
		(descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
		(property "Reference" "R14"
			(at 10.564 0.054 0)
			(layer "F.SilkS")
		)
		(property "Value" "330"
			(at 28.5 -2.5 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "StrikeSense_PCB.kicad_sch")
		(attr through_hole)
		(fp_text user "Data_T"
			(at 3.81 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 8 "/DATA_T")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 7.62 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 8 "/DATA_T")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal"
		(layer "F.Cu")
		(at 132.44 135.5)
		(descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
		(property "Reference" "R8"
			(at -2.392 0.136 0)
			(layer "F.SilkS")
		)
		(property "Value" "1000"
			(at 3.81 2.37 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "StrikeSense_PCB.kicad_sch")
		(attr through_hole)
		(fp_text user "PSLL1"
			(at 3.81 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 10 "Net-(J1-Pin_9)")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 7.62 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MountingHole:MountingHole_3.2mm_M3_ISO14580"
		(layer "F.Cu")
		(at 205.105 92.583)
		(descr "Mounting Hole 3.2mm, M3, no annular, generated by kicad-footprint-generator mountinghole.py")
		(tags "mountinghole M3 ISO14580")
		(property "Reference" "REF**"
			(at 0 -3.7 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "MountingHole_3.2mm_M3_ISO14580"
			(at 0 3.7 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 3.2 3.2)
			(drill 3.2)
			(layers "*.Cu" "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "MountingHole:MountingHole_3.2mm_M3_ISO14580"
		(layer "F.Cu")
		(at 110 145.75)
		(descr "Mounting Hole 3.2mm, M3, no annular, generated by kicad-footprint-generator mountinghole.py")
		(tags "mountinghole M3 ISO14580")
		(property "Reference" "REF**"
			(at 0 -3.7 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "MountingHole_3.2mm_M3_ISO14580"
			(at 0 3.7 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 3.2 3.2)
			(drill 3.2)
			(layers "*.Cu" "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "Multiplexer_CD74HC4067M:Untitled"
		(layer "F.Cu")
		(at 154 120)
		(property "Reference" "U1"
			(at 4.5 -18 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "CD74HC4067M"
			(at 3.5 -16 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/cd74hc4067.pdf"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "High-Speed CMOS Logic 16-Channel Analog Multiplexer/Demultiplexer, SOIC-24"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SOIC*W*7.5x15.4mm*P1.27mm*")
		(sheetname "/")
		(sheetfile "StrikeSense_PCB.kicad_sch")
		(attr smd)
		(fp_text user "GND"
			(at 3 11 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "VCC"
			(at 3 8.5 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(pad "1" thru_hole circle
			(at -7.62 -17.78)
			(size 1.4 1.4)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 20 "Net-(J3-Pin_7)")
			(pinfunction "COM")
			(pintype "passive")
		)
		(pad "1" thru_hole circle
			(at 7.62 -7.62)
			(size 1.4 1.4)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 31 "Net-(U1-COM)")
			(pinfunction "COM")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at -7.62 -15.24)
			(size 1.4 1.4)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 19 "Net-(J3-Pin_8)")
			(pinfunction "I7")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 7.62 -5.08)
			(size 1.4 1.4)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 32 "Net-(U1-S3)")
			(pinfunction "I7")
			(pintype "passive")
		)
		(pad "3" thru_hole circle
			(at -7.62 -12.7)
			(size 1.4 1.4)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 22 "Net-(J3-Pin_9)")
			(pinfunction "I6")
			(pintype "passive")
		)
		(pad "3" thru_hole circle
			(at 7.62 -2.54)
			(size 1.4 1.4)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 30 "Net-(U1-S2)")
			(pinfunction "I6")
			(pintype "passive")
		)
		(pad "4" thru_hole circle
			(at -7.593572 -10.165714)
			(size 1.4 1.4)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 16 "Net-(J3-Pin_10)")
			(pinfunction "I5")
			(pintype "passive")
		)
		(pad "4" thru_hole circle
			(at 7.646428 -0.005714)
			(size 1.4 1.4)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 29 "Net-(U1-S1)")
			(pinfunction "I5")
			(pintype "passive")
		)
		(pad "5" thru_hole circle
			(at -7.62 -7.62)
			(size 1.4 1.4)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(pinfunction "I4")
			(pintype "passive")
		)
		(pad "5" thru_hole circle
			(at 7.62 2.54)
			(size 1.4 1.4)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 28 "Net-(U1-S0)")
			(pinfunction "I4")
			(pintype "passive")
		)
		(pad "6" thru_hole circle
			(at -7.62 -5.08)
			(size 1.4 1.4)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(pinfunction "I3")
			(pintype "passive")
		)
		(pad "6" thru_hole circle
			(at 7.62 5.08)
			(size 1.4 1.4)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "GND")
			(pinfunction "I3")
			(pintype "passive")
			(zone_connect 2)
		)
		(pad "7" thru_hole circle
			(at -7.62 -2.54)
			(size 1.4 1.4)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(pinfunction "I2")
			(pintype "passive")
		)
		(pad "7" thru_hole circle
			(at 7.62 7.62)
			(size 1.4 1.4)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 9 "+3.3V")
			(pinfunction "I2")
			(pintype "passive")
		)
		(pad "8" thru_hole circle
			(at -7.62 0)
			(size 1.4 1.4)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 43 "/PS_T")
			(pinfunction "I1")
			(pintype "passive")
		)
		(pad "8" thru_hole rect
			(at 7.62 10.16)
			(size 1.4 1.4)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "GND")
			(pinfunction "I1")
			(pintype "passive")
			(zone_connect 2)
		)
		(pad "9" thru_hole circle
			(at -7.62 2.54)
			(size 1.4 1.4)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 41 "/PSPSRA1")
			(pinfunction "I0")
			(pintype "passive")
		)
		(pad "10" thru_hole circle
			(at -7.62 5.08)
			(size 1.4 1.4)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 45 "/PSRA2")
			(pinfunction "S0")
			(pintype "input")
		)
		(pad "11" thru_hole circle
			(at -7.62 7.62)
			(size 1.4 1.4)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 42 "/PSRL1")
			(pinfunction "S1")
			(pintype "input")
		)
		(pad "12" thru_hole circle
			(at -7.593572 10.154286)
			(size 1.4 1.4)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 44 "/PSRL2")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "13" thru_hole circle
			(at -7.62 12.7)
			(size 1.4 1.4)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 12 "Net-(J1-Pin_7)")
			(pinfunction "S3")
			(pintype "input")
		)
		(pad "14" thru_hole circle
			(at -7.62 15.24)
			(size 1.4 1.4)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "Net-(J1-Pin_8)")
			(pinfunction "S2")
			(pintype "input")
		)
		(pad "15" thru_hole circle
			(at -7.62 17.78)
			(size 1.4 1.4)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 10 "Net-(J1-Pin_9)")
			(pinfunction "~{E}")
			(pintype "input")
		)
		(pad "16" thru_hole circle
			(at -7.62 20.32)
			(size 1.4 1.4)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 7 "Net-(J1-Pin_10)")
			(pinfunction "I15")
			(pintype "passive")
		)
		(zone
			(net 0)
			(net_name "")
			(layer "F.SilkS")
			(hatch edge 0.5)
			(connect_pads
				(clearance 0)
			)
			(min_thickness 0.25)
			(filled_areas_thickness no)
			(keepout
				(tracks allowed)
				(vias allowed)
				(pads not_allowed)
				(copperpour allowed)
				(footprints not_allowed)
			)
			(placement
				(enabled no)
				(sheetname "")
			)
			(fill
				(thermal_gap 0.5)
				(thermal_bridge_width 0.5)
			)
			(polygon
				(pts
					(xy 144 100) (xy 164 100) (xy 164 142.86) (xy 144 142.86)
				)
			)
		)
		(embedded_fonts no)
	)
	(footprint "MountingHole:MountingHole_3.2mm_M3_ISO14580"
		(layer "F.Cu")
		(at 109.982 29.718)
		(descr "Mounting Hole 3.2mm, M3, no annular, generated by kicad-footprint-generator mountinghole.py")
		(tags "mountinghole M3 ISO14580")
		(property "Reference" "REF**"
			(at 0 -3.7 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "MountingHole_3.2mm_M3_ISO14580"
			(at 0 3.7 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 3.2 3.2)
			(drill 3.2)
			(layers "*.Cu" "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal"
		(layer "F.Cu")
		(at 200 125.603)
		(descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
		(property "Reference" "R1"
			(at 9.677 -0.635 0)
			(layer "F.SilkS")
		)
		(property "Value" "1000"
			(at 3.81 2.37 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "StrikeSense_PCB.kicad_sch")
		(attr through_hole)
		(fp_text user "PS_T"
			(at 3.81 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "GND")
			(pintype "passive")
			(zone_connect 2)
		)
		(pad "2" thru_hole circle
			(at 7.62 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 43 "/PS_T")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_THTPad_D2.0mm_Drill1.0mm"
		(layer "F.Cu")
		(at 130.3 32)
		(descr "THT pad as test Point, diameter 2.0mm, hole diameter 1.0mm")
		(tags "test point THT pad")
		(property "Reference" "SW-1"
			(at 0.5 -2.25 0)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_01x01"
			(at 21.717 -8.636 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x01, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "/")
		(sheetfile "StrikeSense_PCB.kicad_sch")
		(attr exclude_from_pos_files)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.5 1.5)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "Net-(D1-A)")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "TerminalBlock_Phoenix:TerminalBlock_Phoenix_MKDS-1,5-10-5.08_1x10_P5.08mm_Horizontal"
		(layer "F.Cu")
		(at 218 141.986 90)
		(descr "Terminal Block Phoenix MKDS-1,5-10-5.08, 10 pins, pitch 5.08mm, size 50.8x9.8mm, drill diameter 1.3mm, pad diameter 2.6mm, http://www.farnell.com/datasheets/100425.pdf, script-generated using https://gitlab.com/kicad/libraries/kicad-footprint-generator/-/tree/master/scripts/TerminalBlock_Phoenix")
		(tags "THT Terminal Block Phoenix MKDS-1,5-10-5.08 pitch 5.08mm size 50.8x9.8mm drill 1.3mm pad 2.6mm")
		(property "Reference" "J2"
			(at 50.038 -0.254 180)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_01x10"
			(at 22.86 5.72 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x10, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "/")
		(sheetfile "StrikeSense_PCB.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 22.86 3.2 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 90)
			(size 2.6 2.6)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 44 "/PSRL2")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 5.08 0 90)
			(size 2.6 2.6)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 42 "/PSRL1")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole circle
			(at 10.16 0 90)
			(size 2.6 2.6)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 45 "/PSRA2")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole circle
			(at 15.24 0 90)
			(size 2.6 2.6)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 41 "/PSPSRA1")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(pad "5" thru_hole circle
			(at 20.32 0 90)
			(size 2.6 2.6)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 43 "/PS_T")
			(pinfunction "Pin_5")
			(pintype "passive")
		)
		(pad "6" thru_hole circle
			(at 25.4 0 90)
			(size 2.6 2.6)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 15 "/DATA_RL")
			(pinfunction "Pin_6")
			(pintype "passive")
		)
		(pad "7" thru_hole circle
			(at 30.48 0 90)
			(size 2.6 2.6)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 14 "/DATA_RA")
			(pinfunction "Pin_7")
			(pintype "passive")
		)
		(pad "8" thru_hole circle
			(at 35.56 0 90)
			(size 2.6 2.6)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 9 "+3.3V")
			(pinfunction "Pin_8")
			(pintype "passive")
		)
		(pad "9" thru_hole rect
			(at 40.64 0 90)
			(size 2.6 2.6)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "GND")
			(pinfunction "Pin_9")
			(pintype "passive")
			(zone_connect 2)
		)
		(pad "10" thru_hole circle
			(at 45.72 0 90)
			(size 2.6 2.6)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 13 "+5V")
			(pinfunction "Pin_10")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/TerminalBlock_Phoenix.3dshapes/TerminalBlock_Phoenix_MKDS-1,5-10-5.08_1x10_P5.08mm_Horizontal.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_THTPad_D2.0mm_Drill1.0mm"
		(layer "F.Cu")
		(at 136.028 32.004)
		(descr "THT pad as test Point, diameter 2.0mm, hole diameter 1.0mm")
		(tags "test point THT pad")
		(property "Reference" "SW+1"
			(at 0 -2.25 0)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_01x01"
			(at 18 -0.5 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x01, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "/")
		(sheetfile "StrikeSense_PCB.kicad_sch")
		(attr exclude_from_pos_files)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "Net-(SW+1-Pin_1)")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "TerminalBlock_Phoenix:TerminalBlock_Phoenix_MKDS-1,5-10-5.08_1x10_P5.08mm_Horizontal"
		(layer "F.Cu")
		(at 111.506 93.25 -90)
		(descr "Terminal Block Phoenix MKDS-1,5-10-5.08, 10 pins, pitch 5.08mm, size 50.8x9.8mm, drill diameter 1.3mm, pad diameter 2.6mm, http://www.farnell.com/datasheets/100425.pdf, script-generated using https://gitlab.com/kicad/libraries/kicad-footprint-generator/-/tree/master/scripts/TerminalBlock_Phoenix")
		(tags "THT Terminal Block Phoenix MKDS-1,5-10-5.08 pitch 5.08mm size 50.8x9.8mm drill 1.3mm pad 2.6mm")
		(property "Reference" "J1"
			(at -3.969 -0.28 0)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_01x10"
			(at 25.06 -4 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x10, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "/")
		(sheetfile "StrikeSense_PCB.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 22.86 3.2 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 270)
			(size 2.6 2.6)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 13 "+5V")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole rect
			(at 5.08 0 270)
			(size 2.6 2.6)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "GND")
			(pinfunction "Pin_2")
			(pintype "passive")
			(zone_connect 2)
		)
		(pad "3" thru_hole circle
			(at 10.16 0 270)
			(size 2.6 2.6)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 9 "+3.3V")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole circle
			(at 15.24 0 270)
			(size 2.6 2.6)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 8 "/DATA_T")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(pad "5" thru_hole circle
			(at 20.32 0 270)
			(size 2.6 2.6)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "/DATA_LA")
			(pinfunction "Pin_5")
			(pintype "passive")
		)
		(pad "6" thru_hole circle
			(at 25.4 0 270)
			(size 2.6 2.6)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 11 "/DATA_LL")
			(pinfunction "Pin_6")
			(pintype "passive")
		)
		(pad "7" thru_hole circle
			(at 30.48 0 270)
			(size 2.6 2.6)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 12 "Net-(J1-Pin_7)")
			(pinfunction "Pin_7")
			(pintype "passive")
		)
		(pad "8" thru_hole circle
			(at 35.56 0 270)
			(size 2.6 2.6)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "Net-(J1-Pin_8)")
			(pinfunction "Pin_8")
			(pintype "passive")
		)
		(pad "9" thru_hole circle
			(at 40.64 0 270)
			(size 2.6 2.6)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 10 "Net-(J1-Pin_9)")
			(pinfunction "Pin_9")
			(pintype "passive")
		)
		(pad "10" thru_hole circle
			(at 45.72 0 270)
			(size 2.6 2.6)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 7 "Net-(J1-Pin_10)")
			(pinfunction "Pin_10")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/TerminalBlock_Phoenix.3dshapes/TerminalBlock_Phoenix_MKDS-1,5-10-5.08_1x10_P5.08mm_Horizontal.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal"
		(layer "F.Cu")
		(at 134.19 111.5)
		(descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
		(property "Reference" "R13"
			(at -2.364 0.006 0)
			(layer "F.SilkS")
		)
		(property "Value" "1000"
			(at 3.81 2.37 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "StrikeSense_PCB.kicad_sch")
		(attr through_hole)
		(fp_text user "PS_Ex4"
			(at 3.81 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 16 "Net-(J3-Pin_10)")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 7.62 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "GND")
			(pintype "passive")
			(zone_connect 2)
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MountingHole:MountingHole_3.2mm_M3_ISO14580"
		(layer "F.Cu")
		(at 152.273 29.718)
		(descr "Mounting Hole 3.2mm, M3, no annular, generated by kicad-footprint-generator mountinghole.py")
		(tags "mountinghole M3 ISO14580")
		(property "Reference" "REF**"
			(at 0 -3.7 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "MountingHole_3.2mm_M3_ISO14580"
			(at 0 3.7 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 3.2 3.2)
			(drill 3.2)
			(layers "*.Cu" "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "capstoneespslot:BuckConverter3v3"
		(layer "F.Cu")
		(at 155.956 68.92 180)
		(property "Reference" "U3"
			(at 4.2 -8.6 270)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "XL1509-3.3"
			(at 5.7 -8.6 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://datasheet.lcsc.com/lcsc/1809050422_XLSEMI-XL1509-5-0E1_C61063.pdf"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Buck DC/DC Converter, 2A, 3.3V Output Voltage, 4.5-40V Input Voltage"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SOIC*3.9x4.9mm*P1.27mm*")
		(sheetname "/")
		(sheetfile "StrikeSense_PCB.kicad_sch")
		(attr smd)
		(pad "IN+" thru_hole circle
			(at 10.185 -1.08 180)
			(size 1.4 1.4)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "Net-(D1-K)")
		)
		(pad "IN-" thru_hole rect
			(at 1.015 -1.08 180)
			(size 1.4 1.4)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "GND")
			(zone_connect 2)
		)
		(pad "OUT+" thru_hole circle
			(at 10.185 -16.32 180)
			(size 1.4 1.4)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 9 "+3.3V")
		)
		(pad "OUT-" thru_hole circle
			(at 1.015 -16.32 180)
			(size 1.4 1.4)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "GND")
			(zone_connect 2)
		)
		(embedded_fonts no)
	)
	(footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal"
		(layer "F.Cu")
		(at 132.69 139.25)
		(descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
		(property "Reference" "R9"
			(at -2.388 -0.058 0)
			(layer "F.SilkS")
		)
		(property "Value" "1000"
			(at 3.81 2.37 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "StrikeSense_PCB.kicad_sch")
		(attr through_hole)
		(fp_text user "PSLL2"
			(at 3.81 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 7 "Net-(J1-Pin_10)")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 7.62 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal"
		(layer "F.Cu")
		(at 132.44 131.25)
		(descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
		(property "Reference" "R7"
			(at -2.392 0.068 0)
			(layer "F.SilkS")
		)
		(property "Value" "1000"
			(at 3.81 2.37 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "StrikeSense_PCB.kicad_sch")
		(attr through_hole)
		(fp_text user "PSLA2"
			(at 3.81 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "Net-(J1-Pin_8)")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 7.62 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Diode_THT:D_DO-201_P15.24mm_Horizontal"
		(layer "F.Cu")
		(at 125.476 48.895 90)
		(descr "Diode, DO-201 series, Axial, Horizontal, pin pitch=15.24mm, length*diameter=9.53*5.21mm^2, http://www.diodes.com/_files/packages/DO-201.pdf")
		(tags "Diode DO-201 series Axial Horizontal pin pitch 15.24mm  length 9.53mm diameter 5.21mm")
		(property "Reference" "D1"
			(at 8.001 4.064 90)
			(layer "F.SilkS")
		)
		(property "Value" "1N5400"
			(at 4.5 4.25 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "http://www.vishay.com/docs/88516/1n5400.pdf"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "50V 3A General Purpose Rectifier Diode, DO-201AD"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Device" "D"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "D*DO?201AD*")
		(sheetname "/")
		(sheetfile "StrikeSense_PCB.kicad_sch")
		(attr through_hole)
		(fp_text user "K"
			(at 0 -2.3 90)
			(layer "F.SilkS")
		)
		(fp_text user "${REFERENCE}"
			(at 7.62 0 90)
			(layer "F.Fab")
		)
		(fp_text user "K"
			(at 0 -2.3 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole roundrect
			(at 0 0 90)
			(size 2.6 2.6)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.096154)
			(net 3 "Net-(D1-K)")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 15.24 0 90)
			(size 2.6 2.6)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "Net-(D1-A)")
			(pinfunction "A")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Diode_THT.3dshapes/D_DO-201_P15.24mm_Horizontal.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal"
		(layer "F.Cu")
		(at 200 140.208)
		(descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
		(property "Reference" "R5"
			(at 9.677 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "1000"
			(at 3.81 2.37 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "StrikeSense_PCB.kicad_sch")
		(attr through_hole)
		(fp_text user "PSRL2"
			(at 3.81 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "GND")
			(pintype "passive")
			(zone_connect 2)
		)
		(pad "2" thru_hole circle
			(at 7.62 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 44 "/PSRL2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal"
		(layer "F.Cu")
		(at 134.19 108)
		(descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
		(property "Reference" "R12"
			(at -2.618 -0.05 0)
			(layer "F.SilkS")
		)
		(property "Value" "1000"
			(at 3.81 2.37 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "StrikeSense_PCB.kicad_sch")
		(attr through_hole)
		(fp_text user "PS_Ex3"
			(at 3.81 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 22 "Net-(J3-Pin_9)")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 7.62 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "GND")
			(pintype "passive")
			(zone_connect 2)
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TerminalBlock_Phoenix:TerminalBlock_Phoenix_MKDS-1,5-10-5.08_1x10_P5.08mm_Horizontal"
		(layer "F.Cu")
		(at 111.506 38.25 -90)
		(descr "Terminal Block Phoenix MKDS-1,5-10-5.08, 10 pins, pitch 5.08mm, size 50.8x9.8mm, drill diameter 1.3mm, pad diameter 2.6mm, http://www.farnell.com/datasheets/100425.pdf, script-generated using https://gitlab.com/kicad/libraries/kicad-footprint-generator/-/tree/master/scripts/TerminalBlock_Phoenix")
		(tags "THT Terminal Block Phoenix MKDS-1,5-10-5.08 pitch 5.08mm size 50.8x9.8mm drill 1.3mm pad 2.6mm")
		(property "Reference" "J3"
			(at 16.106 -4.09 90)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_01x10"
			(at 22.86 5.72 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x10, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "/")
		(sheetfile "StrikeSense_PCB.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 22.86 3.2 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 270)
			(size 2.6 2.6)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 13 "+5V")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole rect
			(at 5.08 0 270)
			(size 2.6 2.6)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "GND")
			(pinfunction "Pin_2")
			(pintype "passive")
			(zone_connect 2)
		)
		(pad "3" thru_hole circle
			(at 10.16 0 270)
			(size 2.6 2.6)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 9 "+3.3V")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole circle
			(at 15.24 0 270)
			(size 2.6 2.6)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 17 "Net-(J3-Pin_4)")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(pad "5" thru_hole circle
			(at 20.32 0 270)
			(size 2.6 2.6)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 21 "Net-(J3-Pin_5)")
			(pinfunction "Pin_5")
			(pintype "passive")
		)
		(pad "6" thru_hole circle
			(at 25.4 0 270)
			(size 2.6 2.6)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 18 "Net-(J3-Pin_6)")
			(pinfunction "Pin_6")
			(pintype "passive")
		)
		(pad "7" thru_hole circle
			(at 30.48 0 270)
			(size 2.6 2.6)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 20 "Net-(J3-Pin_7)")
			(pinfunction "Pin_7")
			(pintype "passive")
		)
		(pad "8" thru_hole circle
			(at 35.56 0 270)
			(size 2.6 2.6)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 19 "Net-(J3-Pin_8)")
			(pinfunction "Pin_8")
			(pintype "passive")
		)
		(pad "9" thru_hole circle
			(at 40.64 0 270)
			(size 2.6 2.6)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 22 "Net-(J3-Pin_9)")
			(pinfunction "Pin_9")
			(pintype "passive")
		)
		(pad "10" thru_hole circle
			(at 45.72 0 270)
			(size 2.6 2.6)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 16 "Net-(J3-Pin_10)")
			(pinfunction "Pin_10")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/TerminalBlock_Phoenix.3dshapes/TerminalBlock_Phoenix_MKDS-1,5-10-5.08_1x10_P5.08mm_Horizontal.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal"
		(layer "F.Cu")
		(at 120.5 124.5)
		(descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
		(property "Reference" "R16"
			(at 10.31 -0.04 0)
			(layer "F.SilkS")
		)
		(property "Value" "330"
			(at 28.5 -2.5 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "StrikeSense_PCB.kicad_sch")
		(attr through_hole)
		(fp_text user "Data_LL"
			(at 3.81 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 11 "/DATA_LL")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 7.62 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 11 "/DATA_LL")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "capstoneespslot:BuckConverter5v"
		(layer "F.Cu")
		(at 143.764 68.8125 180)
		(property "Reference" "U4"
			(at 4.1 -8.7 270)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "XL1509-5.0"
			(at 5.6 -8.7 270)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://datasheet.lcsc.com/lcsc/1809050422_XLSEMI-XL1509-5-0E1_C61063.pdf"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Buck DC/DC Converter, 2A, 5V Output Voltage, 7-40V Input Voltage"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SOIC*3.9x4.9mm*P1.27mm*")
		(sheetname "/")
		(sheetfile "StrikeSense_PCB.kicad_sch")
		(attr smd)
		(pad "IN+" thru_hole circle
			(at 9.88 -1.588 180)
			(size 1.4 1.4)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "Net-(D1-K)")
		)
		(pad "IN-" thru_hole rect
			(at 1.32 -1.588 180)
			(size 1.4 1.4)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "GND")
			(zone_connect 2)
		)
		(pad "OUT+" thru_hole circle
			(at 9.88 -15.812 180)
			(size 1.4 1.4)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 13 "+5V")
		)
		(pad "OUT-" thru_hole circle
			(at 1.32 -15.812 180)
			(size 1.4 1.4)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "GND")
			(zone_connect 2)
		)
		(embedded_fonts no)
	)
	(footprint "LED_THT:LED_D3.0mm"
		(layer "F.Cu")
		(at 160.9 92.075 180)
		(descr "LED, diameter 3.0mm, 2 pins, generated by kicad-footprint-generator")
		(tags "LED")
		(property "Reference" "LED1"
			(at -1.7 2.675 0)
			(layer "F.SilkS")
		)
		(property "Value" "LED"
			(at 1.27 2.96 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Light emitting diode"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "LED* LED_SMD:* LED_THT:*")
		(sheetname "/")
		(sheetfile "StrikeSense_PCB.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 1.27 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 180)
			(size 1.8 1.8)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "GND")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 2.54 0 180)
			(size 1.8 1.8)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 23 "Net-(LED1-A)")
			(pinfunction "A")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/LED_THT.3dshapes/LED_D3.0mm.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal"
		(layer "F.Cu")
		(at 120.5 119.5)
		(descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
		(property "Reference" "R15"
			(at 10.564 -0.12 0)
			(layer "F.SilkS")
		)
		(property "Value" "330"
			(at 28.5 -2.5 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "StrikeSense_PCB.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 3.81 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "/DATA_LA")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 7.62 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "/DATA_LA")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal"
		(layer "F.Cu")
		(at 200.152 115.443)
		(descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
		(property "Reference" "R18"
			(at 3.683 2.413 0)
			(layer "F.SilkS")
		)
		(property "Value" "330"
			(at 28.5 -2.5 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "StrikeSense_PCB.kicad_sch")
		(attr through_hole)
		(fp_text user "DataRL"
			(at 3.81 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 25 "Net-(U2-SDO{slash}SD0)")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 7.62 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 15 "/DATA_RL")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(gr_arc
		(start 224.155 147.447)
		(mid 223.708631 148.524631)
		(end 222.631 148.971)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 222.631 148.971)
		(end 106.807 148.971)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 155.448 25.019)
		(mid 156.525631 25.465369)
		(end 156.972 26.543)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 106.807 148.971)
		(mid 105.729369 148.524631)
		(end 105.283 147.447)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 157.607 88.519)
		(mid 157.157987 88.333013)
		(end 156.972 87.884)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 105.283 26.67)
		(end 105.283 147.447)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 156.972 87.884)
		(end 156.972 26.543)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 155.448 25.019)
		(end 106.934 25.019)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 157.607 88.519)
		(end 222.631 88.519)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 105.283 26.67)
		(mid 105.766567 25.502567)
		(end 106.934 25.019)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 222.631 88.519)
		(mid 223.708631 88.965369)
		(end 224.155 90.043)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 224.155 90.043)
		(end 224.155 147.447)
		(layer "Edge.Cuts")
	)
	(gr_text "J17"
		(at 209.554 127.38 0)
		(layer "F.SilkS")
	)
	(gr_text "J3"
		(at 117.475 104.013 0)
		(layer "F.SilkS")
	)
	(gr_text "J29"
		(at 117.221 79.629 0)
		(layer "F.SilkS")
	)
	(gr_text "SIG"
		(at 157.5 112.75 0)
		(layer "F.SilkS")
	)
	(gr_text "J4"
		(at 117.475 108.966 0)
		(layer "F.SilkS")
	)
	(gr_text "J22"
		(at 117.221 44.069 0)
		(layer "F.SilkS")
	)
	(gr_text "S0"
		(at 157.5 123.25 0)
		(layer "F.SilkS")
	)
	(gr_text "J15"
		(at 209.808 116.712 0)
		(layer "F.SilkS")
	)
	(gr_text "J27"
		(at 117.475 69.215 0)
		(layer "F.SilkS")
	)
	(gr_text "J5"
		(at 117.348 114.046 0)
		(layer "F.SilkS")
	)
	(gr_text "EN"
		(at 157.5 125.75 0)
		(layer "F.SilkS")
	)
	(gr_text "J6"
		(at 117.348 118.872 0)
		(layer "F.SilkS")
	)
	(gr_text "J14"
		(at 209.681 112.267 0)
		(layer "F.SilkS")
	)
	(gr_text "J23"
		(at 117.475 49.022 0)
		(layer "F.SilkS")
	)
	(gr_text "J21"
		(at 117.221 38.989 0)
		(layer "F.SilkS")
	)
	(gr_text "J25"
		(at 117.348 59.055 0)
		(layer "F.SilkS")
	)
	(gr_text "J13"
		(at 209.554 106.806 0)
		(layer "F.SilkS")
	)
	(gr_text "J11"
		(at 209.3 96.9 0)
		(layer "F.SilkS")
	)
	(gr_text "J8"
		(at 117.094 129.794 0)
		(layer "F.SilkS")
	)
	(gr_text "J1"
		(at 117.348 93.853 0)
		(layer "F.SilkS")
	)
	(gr_text "S2"
		(at 157.5 118.25 0)
		(layer "F.SilkS")
	)
	(gr_text "S1\n"
		(at 157.5 120.25 0)
		(layer "F.SilkS")
	)
	(gr_text "J30"
		(at 117.221 84.455 0)
		(layer "F.SilkS")
	)
	(gr_text "J2"
		(at 117.221 99.06 0)
		(layer "F.SilkS")
	)
	(gr_text "J18"
		(at 209.808 132.333 0)
		(layer "F.SilkS")
	)
	(gr_text "J7"
		(at 117.348 125.476 0)
		(layer "F.SilkS")
	)
	(gr_text "J24"
		(at 117.348 54.229 0)
		(layer "F.SilkS")
	)
	(gr_text "J16"
		(at 209.8 122.173 0)
		(layer "F.SilkS")
	)
	(gr_text "J28"
		(at 117.221 74.549 0)
		(layer "F.SilkS")
	)
	(gr_text "Strike Sense\nE-Shido \nSmart Sensing Suit"
		(at 145.288 61.849 0)
		(layer "F.SilkS")
	)
	(gr_text "J26"
		(at 117.348 64.008 0)
		(layer "F.SilkS")
	)
	(gr_text "S3\n"
		(at 157.5 115.25 0)
		(layer "F.SilkS")
	)
	(gr_text "J9"
		(at 117.348 134.747 0)
		(layer "F.SilkS")
	)
	(gr_text "J20"
		(at 209.554 143.001 0)
		(layer "F.SilkS")
	)
	(gr_text "J10"
		(at 117.221 139.827 0)
		(layer "F.SilkS")
	)
	(gr_text "J12"
		(at 209.427 101.599 0)
		(layer "F.SilkS")
	)
	(gr_text "J19"
		(at 209.6 137.8 0)
		(layer "F.SilkS")
	)
	(zone
		(net 5)
		(net_name "GND")
		(layer "F.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 169.7 59.6) (xy 169.9 21.9) (xy 97.2 21.9) (xy 98.3 154.4) (xy 232.7 153.4) (xy 234 92.5) (xy 169.7 59.5)
				(xy 192.5 47.9)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layers "F.Cu" "B.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(keepout
			(tracks not_allowed)
			(vias not_allowed)
			(pads not_allowed)
			(copperpour not_allowed)
			(footprints allowed)
		)
		(placement
			(enabled no)
			(sheetname "")
		)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 172.23 80.08) (xy 172.2 93) (xy 192.2 93) (xy 192.23 80.08)
			)
		)
	)
	(zone
		(net 5)
		(net_name "GND")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 1)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 175.8 21.2) (xy 94.9 20.6) (xy 98.3 158.7) (xy 236.8 156.3) (xy 238.8 86.9) (xy 176.1 21.2)
			)
		)
	)
	(embedded_fonts no)
)
