(kicad_pcb
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(general
		(thickness 1.6)
		(legacy_teardrops no)
	)
	(paper "A4")
	(layers
		(0 "F.Cu" signal)
		(2 "B.Cu" signal)
		(9 "F.Adhes" user "F.Adhesive")
		(11 "B.Adhes" user "B.Adhesive")
		(13 "F.Paste" user)
		(15 "B.Paste" user)
		(5 "F.SilkS" user "F.Silkscreen")
		(7 "B.SilkS" user "B.Silkscreen")
		(1 "F.Mask" user)
		(3 "B.Mask" user)
		(17 "Dwgs.User" user "User.Drawings")
		(19 "Cmts.User" user "User.Comments")
		(21 "Eco1.User" user "User.Eco1")
		(23 "Eco2.User" user "User.Eco2")
		(25 "Edge.Cuts" user)
		(27 "Margin" user)
		(31 "F.CrtYd" user "F.Courtyard")
		(29 "B.CrtYd" user "B.Courtyard")
		(35 "F.Fab" user)
		(33 "B.Fab" user)
		(39 "User.1" user)
		(41 "User.2" user)
		(43 "User.3" user)
		(45 "User.4" user)
	)
	(setup
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(tenting front back)
		(pcbplotparams
			(layerselection 0x00000000_00000000_55555555_5755f5ff)
			(plot_on_all_layers_selection 0x00000000_00000000_00000000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 4)
			(plotframeref no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(pdf_metadata yes)
			(pdf_single_document no)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plot_black_and_white yes)
			(sketchpadsonfab no)
			(plotpadnumbers no)
			(hidednponfab no)
			(sketchdnponfab yes)
			(crossoutdnponfab yes)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 1)
			(scaleselection 1)
			(outputdirectory "")
		)
	)
	(net 0 "")
	(net 1 "+5V")
	(net 2 "GND")
	(net 3 "Net-(D1-DIN)")
	(net 4 "Net-(D1-DOUT)")
	(net 5 "Net-(D2-DOUT)")
	(net 6 "unconnected-(D3-DOUT-Pad1)")
	(footprint "Seeed Studio XIAO Series Library:LED_D89.0mm-4_RGB"
		(layer "F.Cu")
		(at 153.344612 94.560242 180)
		(descr "LED, RGB, diameter 5.0mm, 4 pins, https://www.kingbright.com/attachments/file/psearch/000/00/00/L-154A4SUREQBFZGEW(Ver.13A).pdf, generated by kicad-footprint-generator")
		(tags "LED")
		(property "Reference" "D2"
			(at 1.905 -3.96 180)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "8mm APA106"
			(at 1.905 3.96 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "RGB LED with integrated controller"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "LED*WS2812*PLCC*5.0x5.0mm*P3.2mm*")
		(sheetname "/")
		(sheetfile "three_light_head.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 1.905 0 180)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 180)
			(size 1.07 1.8)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "Net-(D2-DOUT)")
			(pinfunction "DOUT")
			(pintype "output")
		)
		(pad "2" thru_hole oval
			(at 1.27 0 180)
			(size 1.07 1.8)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "3" thru_hole oval
			(at 2.54 0 180)
			(size 1.07 1.8)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "+5V")
			(pinfunction "V+")
			(pintype "power_in")
		)
		(pad "4" thru_hole oval
			(at 3.81 0 180)
			(size 1.07 1.8)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "Net-(D1-DOUT)")
			(pinfunction "DIN")
			(pintype "input")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/LED_THT.3dshapes/LED_D5.0mm-4_RGB.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_Wire:SolderWire-0.127sqmm_1x03_P3.7mm_D0.48mm_OD1mm"
		(layer "F.Cu")
		(at 147.762727 109)
		(descr "Soldered wire connection, for 3 times 0.127 mm² wires, basic insulation, conductor diameter 0.48mm, outer diameter 1mm, size source Multi-Contact FLEXI-E/HK 0.127 (https://www.staubli.com/content/dam/ecs/catalogs-brochures/TM/CAB-Main-11014119-en.pdf#page=9), bend radius 3 times outer diameter, generated with kicad-footprint-generator")
		(tags "connector wire 0.127sqmm")
		(property "Reference" "J1"
			(at 3.7 -2.05 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Conn_01x03_Pin"
			(at 3.7 2.05 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x03, script generated"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "/")
		(sheetfile "three_light_head.kicad_sch")
		(attr exclude_from_pos_files)
		(fp_text user "${REFERENCE}"
			(at 3.7 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole roundrect
			(at 0.936 0)
			(size 1.7 1.7)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.147059)
			(net 3 "Net-(D1-DIN)")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 3.7 0)
			(size 1.7 1.7)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "+5V")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole circle
			(at 6.479069 0)
			(size 1.7 1.7)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_Wire.3dshapes/SolderWire-0.127sqmm_1x03_P3.7mm_D0.48mm_OD1mm.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Seeed Studio XIAO Series Library:LED_D89.0mm-4_RGB"
		(layer "F.Cu")
		(at 153.344612 85.47 180)
		(descr "LED, RGB, diameter 5.0mm, 4 pins, https://www.kingbright.com/attachments/file/psearch/000/00/00/L-154A4SUREQBFZGEW(Ver.13A).pdf, generated by kicad-footprint-generator")
		(tags "LED")
		(property "Reference" "D3"
			(at 1.905 -3.96 180)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "8mm APA106"
			(at 1.905 3.96 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "RGB LED with integrated controller"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "LED*WS2812*PLCC*5.0x5.0mm*P3.2mm*")
		(sheetname "/")
		(sheetfile "three_light_head.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 1.905 0 180)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 180)
			(size 1.07 1.8)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "unconnected-(D3-DOUT-Pad1)")
			(pinfunction "DOUT")
			(pintype "output+no_connect")
		)
		(pad "2" thru_hole oval
			(at 1.27 0 180)
			(size 1.07 1.8)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "3" thru_hole oval
			(at 2.54 0 180)
			(size 1.07 1.8)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "+5V")
			(pinfunction "V+")
			(pintype "power_in")
		)
		(pad "4" thru_hole oval
			(at 3.81 0 180)
			(size 1.07 1.8)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "Net-(D2-DOUT)")
			(pinfunction "DIN")
			(pintype "input")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/LED_THT.3dshapes/LED_D5.0mm-4_RGB.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Seeed Studio XIAO Series Library:LED_D89.0mm-4_RGB"
		(layer "F.Cu")
		(at 153.344612 103.5 180)
		(descr "LED, RGB, diameter 5.0mm, 4 pins, https://www.kingbright.com/attachments/file/psearch/000/00/00/L-154A4SUREQBFZGEW(Ver.13A).pdf, generated by kicad-footprint-generator")
		(tags "LED")
		(property "Reference" "D1"
			(at 1.905 -3.96 180)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "8mm APA106"
			(at 1.905 3.96 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "RGB LED with integrated controller"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "LED*WS2812*PLCC*5.0x5.0mm*P3.2mm*")
		(sheetname "/")
		(sheetfile "three_light_head.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 1.905 0 180)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 180)
			(size 1.07 1.8)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "Net-(D1-DOUT)")
			(pinfunction "DOUT")
			(pintype "output")
		)
		(pad "2" thru_hole oval
			(at 1.27 0 180)
			(size 1.07 1.8)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "3" thru_hole oval
			(at 2.54 0 180)
			(size 1.07 1.8)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "+5V")
			(pinfunction "V+")
			(pintype "power_in")
		)
		(pad "4" thru_hole oval
			(at 3.81 0 180)
			(size 1.07 1.8)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "Net-(D1-DIN)")
			(pinfunction "DIN")
			(pintype "input")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/LED_THT.3dshapes/LED_D5.0mm-4_RGB.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Symbol:OSHW-Symbol_6.7x6mm_SilkScreen"
		(layer "B.Cu")
		(at 151.342816 89.969534 90)
		(descr "Open Source Hardware Symbol")
		(tags "Logo Symbol OSHW")
		(property "Reference" "REF**"
			(at 0 0 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "OSHW-Symbol_6.7x6mm_SilkScreen"
			(at 0.75 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom allow_missing_courtyard)
		(embedded_fonts no)
	)
	(gr_rect
		(start 146.87829 81)
		(end 155.87829 111)
		(fill no)
		(layer "Edge.Cuts")
	)
	(gr_text "Din"
		(at 147.5 111 0)
		(layer "F.SilkS")
	)
	(gr_text "5v"
		(at 150.5 111 0)
		(layer "F.SilkS")
	)
	(gr_text "Gnd"
		(at 152.754342 111.01234 0)
		(layer "F.SilkS")
	)
	(gr_text "Version \n  2.0"
		(at 150 101.5 270)
		(layer "B.SilkS")
	)
	(gr_text "Eric Timberlake - January 2026"
		(at 147.298857 106.145371 270)
		(layer "B.SilkS")
	)
	(gr_text "APA106 8mm Signal Head"
		(at 154.5 105 270)
		(layer "B.SilkS")
	)
	(gr_text "5V"
		(at 152.5 111 0)
		(layer "B.SilkS")
	)
	(gr_text "Gnd"
		(at 155.785678 110.972454 0)
		(layer "B.SilkS")
	)
	(gr_text "Din"
		(at 150 111 0)
		(layer "B.SilkS")
	)
	(dimension
		(type orthogonal)
		(layer "User.4")
		(pts
			(xy 149.595 103.53) (xy 149.19 94.53)
		)
		(height -4.5)
		(orientation 1)
		(format
			(prefix "")
			(suffix "")
			(units 3)
			(units_format 0)
			(precision 4)
			(suppress_zeroes yes)
		)
		(style
			(thickness 0.1)
			(arrow_length 1.27)
			(text_position_mode 0)
			(arrow_direction outward)
			(extension_height 0.58642)
			(extension_offset 0.5)
			(keep_text_aligned yes)
		)
		(gr_text "9"
			(at 143.945 99.03 90)
			(layer "User.4")
		)
	)
	(dimension
		(type orthogonal)
		(layer "User.4")
		(pts
			(xy 146.87829 81) (xy 155.87829 81)
		)
		(height -4.5)
		(orientation 0)
		(format
			(prefix "")
			(suffix "")
			(units 3)
			(units_format 0)
			(precision 4)
			(suppress_zeroes yes)
		)
		(style
			(thickness 0.1)
			(arrow_length 1.27)
			(text_position_mode 0)
			(arrow_direction outward)
			(extension_height 0.58642)
			(extension_offset 0.5)
			(keep_text_aligned yes)
		)
		(gr_text "9"
			(at 151.37829 75.35 0)
			(layer "User.4")
		)
	)
	(dimension
		(type orthogonal)
		(layer "User.4")
		(pts
			(xy 155.87829 81) (xy 155.87829 111)
		)
		(height 4.62171)
		(orientation 1)
		(format
			(prefix "")
			(suffix "")
			(units 3)
			(units_format 0)
			(precision 4)
			(suppress_zeroes yes)
		)
		(style
			(thickness 0.1)
			(arrow_length 1.27)
			(text_position_mode 0)
			(arrow_direction outward)
			(extension_height 0.58642)
			(extension_offset 0.5)
			(keep_text_aligned yes)
		)
		(gr_text "30"
			(at 159.35 96 90)
			(layer "User.4")
		)
	)
	(dimension
		(type orthogonal)
		(layer "User.4")
		(pts
			(xy 149 94.5) (xy 149.034612 85.5)
		)
		(height -3.905)
		(orientation 1)
		(format
			(prefix "")
			(suffix "")
			(units 3)
			(units_format 0)
			(precision 4)
			(suppress_zeroes yes)
		)
		(style
			(thickness 0.1)
			(arrow_length 1.27)
			(text_position_mode 0)
			(arrow_direction outward)
			(extension_height 0.58642)
			(extension_offset 0.5)
			(keep_text_aligned yes)
		)
		(gr_text "9"
			(at 143.945 90 90)
			(layer "User.4")
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "F.Cu")
		(name "ground")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 146 80) (xy 146 111.5) (xy 157 111.5) (xy 157 80)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "B.Cu")
		(name "ground")
		(hatch edge 0.5)
		(priority 1)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 143.275947 80.300654) (xy 143.275947 112.128888) (xy 158.730849 112.128888) (xy 158.730849 80.300654)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layer "Edge.Cuts")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(keepout
			(tracks not_allowed)
			(vias not_allowed)
			(pads not_allowed)
			(copperpour allowed)
			(footprints allowed)
		)
		(placement
			(enabled no)
			(sheetname "/")
		)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 145.254583 113.137629) (xy 156.68594 113.137629) (xy 156.68594 77.813604) (xy 145.254583 77.813604)
			)
		)
	)
	(embedded_fonts no)
)
