(kicad_pcb
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(general
		(thickness 1.6)
		(legacy_teardrops no)
	)
	(paper "A4")
	(layers
		(0 "F.Cu" signal)
		(4 "In1.Cu" signal)
		(6 "In2.Cu" signal)
		(2 "B.Cu" signal)
		(9 "F.Adhes" user "F.Adhesive")
		(11 "B.Adhes" user "B.Adhesive")
		(13 "F.Paste" user)
		(15 "B.Paste" user)
		(5 "F.SilkS" user "F.Silkscreen")
		(7 "B.SilkS" user "B.Silkscreen")
		(1 "F.Mask" user)
		(3 "B.Mask" user)
		(17 "Dwgs.User" user "User.Drawings")
		(19 "Cmts.User" user "User.Comments")
		(21 "Eco1.User" user "User.Eco1")
		(23 "Eco2.User" user "User.Eco2")
		(25 "Edge.Cuts" user)
		(27 "Margin" user)
		(31 "F.CrtYd" user "F.Courtyard")
		(29 "B.CrtYd" user "B.Courtyard")
		(35 "F.Fab" user)
		(33 "B.Fab" user)
		(39 "User.1" user)
		(41 "User.2" user)
		(43 "User.3" user)
		(45 "User.4" user)
		(47 "User.5" user)
		(49 "User.6" user)
		(51 "User.7" user)
		(53 "User.8" user)
		(55 "User.9" user)
	)
	(setup
		(stackup
			(layer "F.SilkS"
				(type "Top Silk Screen")
			)
			(layer "F.Paste"
				(type "Top Solder Paste")
			)
			(layer "F.Mask"
				(type "Top Solder Mask")
				(thickness 0.01)
			)
			(layer "F.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "dielectric 1"
				(type "prepreg")
				(thickness 0.1)
				(material "FR4")
				(epsilon_r 4.5)
				(loss_tangent 0.02)
			)
			(layer "In1.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "dielectric 2"
				(type "core")
				(thickness 1.24)
				(material "FR4")
				(epsilon_r 4.5)
				(loss_tangent 0.02)
			)
			(layer "In2.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "dielectric 3"
				(type "prepreg")
				(thickness 0.1)
				(material "FR4")
				(epsilon_r 4.5)
				(loss_tangent 0.02)
			)
			(layer "B.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "B.Mask"
				(type "Bottom Solder Mask")
				(thickness 0.01)
			)
			(layer "B.Paste"
				(type "Bottom Solder Paste")
			)
			(layer "B.SilkS"
				(type "Bottom Silk Screen")
			)
			(copper_finish "None")
			(dielectric_constraints no)
		)
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(tenting front back)
		(pcbplotparams
			(layerselection 0x00000000_00000000_55555555_5755f5ff)
			(plot_on_all_layers_selection 0x00000000_00000000_00000000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 4)
			(plotframeref no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(pdf_metadata yes)
			(pdf_single_document no)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plot_black_and_white yes)
			(sketchpadsonfab no)
			(plotpadnumbers no)
			(hidednponfab no)
			(sketchdnponfab yes)
			(crossoutdnponfab yes)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 0)
			(scaleselection 1)
			(outputdirectory "gerbers/")
		)
	)
	(property "ADDRESS1" "13500 SW 72nd Ave STE 100")
	(property "ADDRESS2" "Portland, OR  97223")
	(property "ADDRESS3" "217.391.3724")
	(property "ADDRESS4" "http://www.opalkelly.com")
	(property "DOCUMENTNUMBER" "xxx")
	(property "ORGANIZATION" "Opal Kelly")
	(property "PAGESETUP" "Record=PageOptions¦CenterHorizontal=True¦CenterVertical=True¦PrintScale=0.52¦XCorrection=1.00¦YCorrection=1.00¦PrintKind=0¦BorderSize=5000000¦LeftOffset=0¦BottomOffset=0¦Orientation=2¦PaperLength=1000¦PaperWidth=1000¦Scale=100¦PaperSource=7¦PrintQuality=-4¦MediaType=1¦DitherType=10¦PaperKind=Letter¦PrintScaleMode=1")
	(property "SHEETTOTAL" "1")
	(net 0 "")
	(net 1 "/szg_interface/R_GA")
	(net 2 "GND")
	(net 3 "+3.3V")
	(net 4 "Net-(D1-A)")
	(net 5 "/szg_interface/MCU_SDA_MOSI")
	(net 6 "/szg_interface/MCU_MISO")
	(net 7 "/szg_interface/MCU_RESET_B")
	(net 8 "/szg_interface/MCU_SCL_USCK")
	(net 9 "/szg_interface/S6_D2N")
	(net 10 "/szg_interface/S20")
	(net 11 "/szg_interface/S24")
	(net 12 "/szg_interface/S5_D3P")
	(net 13 "/szg_interface/P2C_CLKN")
	(net 14 "/szg_interface/S7_D3N")
	(net 15 "/szg_interface/S14_D6N")
	(net 16 "/szg_interface/S21")
	(net 17 "/szg_interface/C2P_CLKN")
	(net 18 "/szg_interface/S17")
	(net 19 "/szg_interface/S27")
	(net 20 "/szg_interface/S22")
	(net 21 "/szg_interface/S10_D4N")
	(net 22 "/szg_interface/C2P_CLKP")
	(net 23 "/szg_interface/S19")
	(net 24 "/szg_interface/S25")
	(net 25 "/szg_interface/S8_D4P")
	(net 26 "/szg_interface/S18")
	(net 27 "/szg_interface/S16")
	(net 28 "/szg_interface/S13_D7P")
	(net 29 "/szg_interface/S9_D5P")
	(net 30 "/szg_interface/RSVD_38")
	(net 31 "/szg_interface/RSVD_37")
	(net 32 "/szg_interface/S26")
	(net 33 "VIO")
	(net 34 "/szg_interface/S23")
	(net 35 "/szg_interface/P2C_CLKP")
	(net 36 "/szg_interface/S11_D5N")
	(net 37 "/szg_interface/S15_D7N")
	(net 38 "/szg_interface/S12_D6P")
	(net 39 "unconnected-(MH1-Pad1)")
	(net 40 "unconnected-(MH2-Pad1)")
	(net 41 "unconnected-(MH3-Pad1)")
	(net 42 "unconnected-(MH4-Pad1)")
	(net 43 "+5V")
	(net 44 "/lvds_interface/MISO1")
	(net 45 "/lvds_interface/MOSI1")
	(net 46 "/lvds_interface/SCLK")
	(net 47 "/lvds_interface/CS")
	(net 48 "/lvds_interface/MOSI2")
	(net 49 "/lvds_interface/MISO2")
	(net 50 "/lvds_interface1/MOSI1")
	(net 51 "/lvds_interface1/CS")
	(net 52 "/lvds_interface1/MOSI2")
	(net 53 "/lvds_interface1/MISO1")
	(net 54 "/lvds_interface1/SCLK")
	(net 55 "/lvds_interface1/MISO2")
	(net 56 "/lvds_interface2/MISO1")
	(net 57 "/lvds_interface2/MOSI2")
	(net 58 "/lvds_interface2/CS")
	(net 59 "/lvds_interface2/MOSI1")
	(net 60 "/lvds_interface2/SCLK")
	(net 61 "/lvds_interface2/MISO2")
	(net 62 "/lvds_interface3/MOSI1")
	(net 63 "/lvds_interface3/MOSI2")
	(net 64 "/lvds_interface3/SCLK")
	(net 65 "/lvds_interface3/MISO1")
	(net 66 "/lvds_interface3/CS")
	(net 67 "/lvds_interface3/MISO2")
	(net 68 "unconnected-(MH5-Pad1)")
	(net 69 "unconnected-(MH6-Pad1)")
	(net 70 "/szg_interface/S3_D1N")
	(net 71 "/szg_interface/S0_D0P")
	(net 72 "/szg_interface/S1_D1P")
	(net 73 "/szg_interface/S4_D2P")
	(net 74 "/szg_interface/S2_D0N")
	(net 75 "unconnected-(U1-PA2-Pad3)")
	(net 76 "unconnected-(U1-PA1-Pad4)")
	(net 77 "unconnected-(U1-PA7-Pad15)")
	(net 78 "unconnected-(U1-XTAL2{slash}PB1-Pad12)")
	(net 79 "unconnected-(U1-NC-Pad10)")
	(net 80 "unconnected-(U1-PA3-Pad2)")
	(net 81 "unconnected-(U1-NC-Pad6)")
	(net 82 "unconnected-(U1-NC-Pad19)")
	(net 83 "unconnected-(U1-XTAL1{slash}PB0-Pad11)")
	(net 84 "unconnected-(U1-NC-Pad17)")
	(net 85 "unconnected-(U1-PB2-Pad14)")
	(net 86 "unconnected-(U1-NC-Pad7)")
	(net 87 "unconnected-(U1-NC-Pad18)")
	(net 88 "/lvds_interface/MOSI1_N")
	(net 89 "/lvds_interface/SCLK_N")
	(net 90 "/lvds_interface/MISO2_P")
	(net 91 "/lvds_interface/SCLK_P")
	(net 92 "/lvds_interface/MOSI2_P")
	(net 93 "/lvds_interface/CS_P")
	(net 94 "/lvds_interface/MOSI2_N")
	(net 95 "/lvds_interface/MISO1_N")
	(net 96 "/lvds_interface/MOSI1_P")
	(net 97 "/lvds_interface/MISO1_P")
	(net 98 "/lvds_interface/CS_N")
	(net 99 "/lvds_interface/MISO2_N")
	(net 100 "/lvds_interface1/SCLK_N")
	(net 101 "/lvds_interface1/CS_N")
	(net 102 "/lvds_interface1/MISO1_N")
	(net 103 "/lvds_interface1/MOSI2_N")
	(net 104 "/lvds_interface1/MISO2_P")
	(net 105 "/lvds_interface1/MISO2_N")
	(net 106 "/lvds_interface1/MOSI2_P")
	(net 107 "/lvds_interface1/CS_P")
	(net 108 "/lvds_interface1/MOSI1_N")
	(net 109 "/lvds_interface1/MISO1_P")
	(net 110 "/lvds_interface1/SCLK_P")
	(net 111 "/lvds_interface1/MOSI1_P")
	(net 112 "/lvds_interface2/MISO2_N")
	(net 113 "/lvds_interface2/CS_N")
	(net 114 "/lvds_interface2/MISO1_N")
	(net 115 "/lvds_interface2/MOSI1_N")
	(net 116 "/lvds_interface2/MISO2_P")
	(net 117 "/lvds_interface2/MOSI1_P")
	(net 118 "/lvds_interface2/MOSI2_N")
	(net 119 "/lvds_interface2/SCLK_P")
	(net 120 "/lvds_interface2/MOSI2_P")
	(net 121 "/lvds_interface2/SCLK_N")
	(net 122 "/lvds_interface2/MISO1_P")
	(net 123 "/lvds_interface2/CS_P")
	(net 124 "/lvds_interface3/MOSI1_N")
	(net 125 "/lvds_interface3/MISO2_N")
	(net 126 "/lvds_interface3/MOSI2_N")
	(net 127 "/lvds_interface3/CS_N")
	(net 128 "/lvds_interface3/MOSI2_P")
	(net 129 "/lvds_interface3/MISO1_N")
	(net 130 "/lvds_interface3/MOSI1_P")
	(net 131 "/lvds_interface3/MISO1_P")
	(net 132 "/lvds_interface3/SCLK_N")
	(net 133 "/lvds_interface3/CS_P")
	(net 134 "/lvds_interface3/SCLK_P")
	(net 135 "/lvds_interface3/MISO2_P")
	(net 136 "Net-(U13-VREF)")
	(net 137 "Net-(U13-SS)")
	(net 138 "-5V")
	(net 139 "Net-(JP1-C)")
	(net 140 "unconnected-(U13-N.C.-Pad4)")
	(net 141 "unconnected-(U13-CC-Pad8)")
	(net 142 "unconnected-(U13-N.C.-Pad5)")
	(net 143 "unconnected-(U13-N.C.-Pad6)")
	(net 144 "unconnected-(J7-Pin_2-Pad2)")
	(net 145 "Net-(J7-Pin_9)")
	(net 146 "unconnected-(J7-Pin_7-Pad7)")
	(net 147 "Net-(D3-K)")
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 135.52 123.2 180)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C7"
			(at 0 1.099999 0)
			(layer "F.Fab")
		)
		(property "Value" "0.1uF"
			(at 0 1.16 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Ceramic capacitor"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "CREATED_ON" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DATE" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DESCRIPTION" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ID" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "INVENTORY_PRICE" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTTYPE" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ROHS" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/lvds_interface/")
		(sheetfile "lvds-interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 180)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 43 "+5V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 180)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 142.9 106.9125 90)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C11"
			(at 1.7125 0.4 180)
			(layer "F.Fab")
		)
		(property "Value" "0.1uF"
			(at 0 1.16 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Ceramic capacitor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "CREATED_ON" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DATE" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DESCRIPTION" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ID" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "INVENTORY_PRICE" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTTYPE" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ROHS" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/lvds_interface1/")
		(sheetfile "lvds-interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 90)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 3 "+3.3V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 90)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 139.18 103.6925)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C10"
			(at 2.42 0 0)
			(layer "F.Fab")
		)
		(property "Value" "0.001uF"
			(at 0 1.16 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Ceramic capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "CREATED_ON" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DATE" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DESCRIPTION" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ID" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "INVENTORY_PRICE" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTTYPE" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ROHS" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/lvds_interface1/")
		(sheetfile "lvds-interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 3 "+3.3V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_SMD:SOT-23-5"
		(layer "F.Cu")
		(at 161.8 106.1)
		(descr "SOT, 5 Pin (JEDEC MO-178 Var AA https://www.jedec.org/document_search?search_api_views_fulltext=MO-178), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOT TO_SOT_SMD")
		(property "Reference" "U9"
			(at 0 2.5 0)
			(layer "F.Fab")
		)
		(property "Value" "SN65LVDT2DBV"
			(at 0 2.4 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/sn65lvdt2.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "High-Speed Differential Line Receiver, 110 Ω Terminated, 630Mbps, SOT-23-5"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "CREATED_ON" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DATE" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DESCRIPTION" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ID" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "INVENTORY_PRICE" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTTYPE" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ROHS" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer" "Texas Instruments"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SOT?23*")
		(sheetname "/lvds_interface3/")
		(sheetfile "lvds-interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.1375 -0.95)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 3 "+3.3V")
			(pinfunction "V_{CC}")
			(pintype "power_in")
		)
		(pad "2" smd roundrect
			(at -1.1375 0)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "3" smd roundrect
			(at -1.1375 0.95)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 135 "/lvds_interface3/MISO2_P")
			(pinfunction "A")
			(pintype "input")
		)
		(pad "4" smd roundrect
			(at 1.1375 0.95)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 125 "/lvds_interface3/MISO2_N")
			(pinfunction "B")
			(pintype "input")
		)
		(pad "5" smd roundrect
			(at 1.1375 -0.95)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 67 "/lvds_interface3/MISO2")
			(pinfunction "R")
			(pintype "output")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 145.5 106.9125 90)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C9"
			(at 0 1.2 90)
			(layer "F.Fab")
		)
		(property "Value" "0.001uF"
			(at 0 1.16 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Ceramic capacitor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "CREATED_ON" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DATE" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DESCRIPTION" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ID" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "INVENTORY_PRICE" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTTYPE" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ROHS" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/lvds_interface1/")
		(sheetfile "lvds-interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 90)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 3 "+3.3V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 90)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 156.62 123.2 180)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C25"
			(at 0 1.2 0)
			(layer "F.Fab")
		)
		(property "Value" "0.1uF"
			(at 0 1.16 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Ceramic capacitor"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "CREATED_ON" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DATE" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DESCRIPTION" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ID" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "INVENTORY_PRICE" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTTYPE" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ROHS" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/lvds_interface3/")
		(sheetfile "lvds-interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 180)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 43 "+5V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 180)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "LED_SMD:LED_0402_1005Metric"
		(layer "F.Cu")
		(at 159.7 67.6 180)
		(descr "LED SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
		(tags "LED")
		(property "Reference" "D1"
			(at 0 -1.17 0)
			(layer "F.Fab")
		)
		(property "Value" "LED"
			(at 0 1.17 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Light emitting diode"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "CREATED_ON" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DATE" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DESCRIPTION" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ID" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "INVENTORY_PRICE" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTTYPE" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ROHS" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "LED* LED_SMD:* LED_THT:*")
		(sheetname "/")
		(sheetfile "szg-adapter.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.485 0 180)
			(size 0.59 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.485 0 180)
			(size 0.59 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 4 "Net-(D1-A)")
			(pinfunction "A")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 149 128.5 90)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C20"
			(at 0 -1.16 90)
			(layer "F.Fab")
		)
		(property "Value" "0.1uF"
			(at 0 1.16 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Ceramic capacitor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "CREATED_ON" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DATE" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DESCRIPTION" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ID" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "INVENTORY_PRICE" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTTYPE" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ROHS" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/lvds_interface2/")
		(sheetfile "lvds-interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 90)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 90)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 138 "-5V")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Inductor_SMD:L_0603_1608Metric"
		(layer "F.Cu")
		(at 166.052501 95.85 180)
		(descr "Inductor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
		(tags "inductor")
		(property "Reference" "L1"
			(at 0 -1.43 0)
			(layer "F.Fab")
		)
		(property "Value" "10uH"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Inductor, small symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "CREATED_ON" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DATE" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DESCRIPTION" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ID" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "INVENTORY_PRICE" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTTYPE" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ROHS" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Choke_* *Coil* Inductor_* L_*")
		(sheetname "/power-management/")
		(sheetfile "power.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.787501 0 180)
			(size 0.875 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.787501 0 180)
			(size 0.875 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 147 "Net-(D3-K)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_SO:TSSOP-24_4.4x7.8mm_P0.65mm"
		(layer "F.Cu")
		(at 131.7 92.8875 -90)
		(descr "TSSOP, 24 Pin (JEDEC MO-153 variation AD, 1.00mm body thickness, https://www.jedec.org/document_search?search_api_views_fulltext=MO-153), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "TSSOP SO")
		(property "Reference" "U11"
			(at 0 -4.85 90)
			(layer "F.Fab")
		)
		(property "Value" "SN74LVC8T245"
			(at 0 4.85 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/sn74lvc8t245.pdf"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "8-Bit Dual-Supply Bus Transceiver With Configurable Voltage Translation and 3-State Outputs"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "CREATED_ON" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DATE" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DESCRIPTION" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ID" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "INVENTORY_PRICE" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTTYPE" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ROHS" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer" "Texas Instruments"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SSOP*5.3x8.2mm* SSOP*3.9x8.7mm* TSSOP*4.4x7.8mm* TVSOP*4.4x5.0mm* Texas*VQFN*RHL*")
		(sheetname "/voltage_translation1/")
		(sheetfile "voltage_translation.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -2.8625 -3.575 270)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 33 "VIO")
			(pinfunction "V_{CCA}")
			(pintype "power_in")
		)
		(pad "2" smd roundrect
			(at -2.8625 -2.925 270)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 33 "VIO")
			(pinfunction "DIR")
			(pintype "input")
		)
		(pad "3" smd roundrect
			(at -2.8625 -2.275 270)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 14 "/szg_interface/S7_D3N")
			(pinfunction "A1")
			(pintype "bidirectional")
		)
		(pad "4" smd roundrect
			(at -2.8625 -1.625 270)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 9 "/szg_interface/S6_D2N")
			(pinfunction "A2")
			(pintype "bidirectional")
		)
		(pad "5" smd roundrect
			(at -2.8625 -0.975 270)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 12 "/szg_interface/S5_D3P")
			(pinfunction "A3")
			(pintype "bidirectional")
		)
		(pad "6" smd roundrect
			(at -2.8625 -0.325 270)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 73 "/szg_interface/S4_D2P")
			(pinfunction "A4")
			(pintype "bidirectional")
		)
		(pad "7" smd roundrect
			(at -2.8625 0.325 270)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 70 "/szg_interface/S3_D1N")
			(pinfunction "A5")
			(pintype "bidirectional")
		)
		(pad "8" smd roundrect
			(at -2.8625 0.975 270)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 74 "/szg_interface/S2_D0N")
			(pinfunction "A6")
			(pintype "bidirectional")
		)
		(pad "9" smd roundrect
			(at -2.8625 1.625 270)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 72 "/szg_interface/S1_D1P")
			(pinfunction "A7")
			(pintype "bidirectional")
		)
		(pad "10" smd roundrect
			(at -2.8625 2.275 270)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 71 "/szg_interface/S0_D0P")
			(pinfunction "A8")
			(pintype "bidirectional")
		)
		(pad "11" smd roundrect
			(at -2.8625 2.925 270)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "12" smd roundrect
			(at -2.8625 3.575 270)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "13" smd roundrect
			(at 2.8625 3.575 270)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "14" smd roundrect
			(at 2.8625 2.925 270)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 47 "/lvds_interface/CS")
			(pinfunction "B8")
			(pintype "bidirectional")
		)
		(pad "15" smd roundrect
			(at 2.8625 2.275 270)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 48 "/lvds_interface/MOSI2")
			(pinfunction "B7")
			(pintype "bidirectional")
		)
		(pad "16" smd roundrect
			(at 2.8625 1.625 270)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 46 "/lvds_interface/SCLK")
			(pinfunction "B6")
			(pintype "bidirectional")
		)
		(pad "17" smd roundrect
			(at 2.8625 0.975 270)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 45 "/lvds_interface/MOSI1")
			(pinfunction "B5")
			(pintype "bidirectional")
		)
		(pad "18" smd roundrect
			(at 2.8625 0.325 270)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 51 "/lvds_interface1/CS")
			(pinfunction "B4")
			(pintype "bidirectional")
		)
		(pad "19" smd roundrect
			(at 2.8625 -0.325 270)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 52 "/lvds_interface1/MOSI2")
			(pinfunction "B3")
			(pintype "bidirectional")
		)
		(pad "20" smd roundrect
			(at 2.8625 -0.975 270)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 54 "/lvds_interface1/SCLK")
			(pinfunction "B2")
			(pintype "bidirectional")
		)
		(pad "21" smd roundrect
			(at 2.8625 -1.625 270)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 50 "/lvds_interface1/MOSI1")
			(pinfunction "B1")
			(pintype "bidirectional")
		)
		(pad "22" smd roundrect
			(at 2.8625 -2.275 270)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "~{OE}")
			(pintype "input")
		)
		(pad "23" smd roundrect
			(at 2.8625 -2.925 270)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 3 "+3.3V")
			(pinfunction "V_{CCB}")
			(pintype "power_in")
		)
		(pad "24" smd roundrect
			(at 2.8625 -3.575 270)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 3 "+3.3V")
			(pinfunction "V_{CCB}")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Package_SO.3dshapes/TSSOP-24_4.4x7.8mm_P0.65mm.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 156.6 89.4875 -90)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C27"
			(at 0 -1.16 90)
			(layer "F.Fab")
		)
		(property "Value" "0.1uF"
			(at 0 1.16 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Ceramic capacitor"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "CREATED_ON" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DATE" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DESCRIPTION" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ID" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "INVENTORY_PRICE" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTTYPE" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ROHS" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/voltage_translation/")
		(sheetfile "voltage_translation.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 270)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 270)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 33 "VIO")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 136.6 89.4875 -90)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C29"
			(at 0 -1.16 90)
			(layer "F.Fab")
		)
		(property "Value" "0.1uF"
			(at 0 1.16 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Ceramic capacitor"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "CREATED_ON" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DATE" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DESCRIPTION" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ID" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "INVENTORY_PRICE" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTTYPE" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ROHS" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/voltage_translation1/")
		(sheetfile "voltage_translation.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 270)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 270)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 33 "VIO")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "F.Cu")
		(at 169.065 96.499999 -90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C35"
			(at 0 -1.679999 90)
			(layer "F.Fab")
		)
		(property "Value" "33uF"
			(at 0 1.679999 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Ceramic capacitor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "CREATED_ON" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DATE" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DESCRIPTION" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ID" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "INVENTORY_PRICE" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTTYPE" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ROHS" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/power-management/")
		(sheetfile "power.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.949999 0 270)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 43 "+5V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.949999 0 270)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_SO:TSSOP-20_4.4x6.5mm_P0.65mm"
		(layer "F.Cu")
		(at 133.5 112.1 -90)
		(descr "TSSOP, 20 Pin (JEDEC MO-153 Var AC https://www.jedec.org/document_search?search_api_views_fulltext=MO-153), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "TSSOP SO")
		(property "Reference" "U2"
			(at 0 -4.2 90)
			(layer "F.Fab")
		)
		(property "Value" "SN65LVDT41"
			(at 0 4.2 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Multi-channel transceivers for SPI over LVDS"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "CREATED_ON" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DATE" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DESCRIPTION" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ID" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "INVENTORY_PRICE" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTTYPE" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ROHS" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer" "Texas Instruments"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/lvds_interface/")
		(sheetfile "lvds-interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -2.8625 -2.925 270)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 45 "/lvds_interface/MOSI1")
			(pinfunction "1D")
			(pintype "input")
		)
		(pad "2" smd roundrect
			(at -2.8625 -2.275 270)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "3" smd roundrect
			(at -2.8625 -1.625 270)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 46 "/lvds_interface/SCLK")
			(pinfunction "2D")
			(pintype "input")
		)
		(pad "4" smd roundrect
			(at -2.8625 -0.975 270)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 3 "+3.3V")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(pad "5" smd roundrect
			(at -2.8625 -0.325 270)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 48 "/lvds_interface/MOSI2")
			(pinfunction "3D")
			(pintype "input")
		)
		(pad "6" smd roundrect
			(at -2.8625 0.325 270)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "7" smd roundrect
			(at -2.8625 0.975 270)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 47 "/lvds_interface/CS")
			(pinfunction "4D")
			(pintype "input")
		)
		(pad "8" smd roundrect
			(at -2.8625 1.625 270)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 3 "+3.3V")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(pad "9" smd roundrect
			(at -2.8625 2.275 270)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 44 "/lvds_interface/MISO1")
			(pinfunction "5R")
			(pintype "output")
		)
		(pad "10" smd roundrect
			(at -2.8625 2.925 270)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "11" smd roundrect
			(at 2.8625 2.925 270)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 95 "/lvds_interface/MISO1_N")
			(pinfunction "5B")
			(pintype "output")
		)
		(pad "12" smd roundrect
			(at 2.8625 2.275 270)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 97 "/lvds_interface/MISO1_P")
			(pinfunction "5A")
			(pintype "output")
		)
		(pad "13" smd roundrect
			(at 2.8625 1.625 270)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 98 "/lvds_interface/CS_N")
			(pinfunction "4Z")
			(pintype "output")
		)
		(pad "14" smd roundrect
			(at 2.8625 0.975 270)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 93 "/lvds_interface/CS_P")
			(pinfunction "4Y")
			(pintype "output")
		)
		(pad "15" smd roundrect
			(at 2.8625 0.325 270)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 94 "/lvds_interface/MOSI2_N")
			(pinfunction "3Z")
			(pintype "output")
		)
		(pad "16" smd roundrect
			(at 2.8625 -0.325 270)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 92 "/lvds_interface/MOSI2_P")
			(pinfunction "3Y")
			(pintype "output")
		)
		(pad "17" smd roundrect
			(at 2.8625 -0.975 270)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 89 "/lvds_interface/SCLK_N")
			(pinfunction "2Z")
			(pintype "output")
		)
		(pad "18" smd roundrect
			(at 2.8625 -1.625 270)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 91 "/lvds_interface/SCLK_P")
			(pinfunction "2Y")
			(pintype "output")
		)
		(pad "19" smd roundrect
			(at 2.8625 -2.275 270)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 88 "/lvds_interface/MOSI1_N")
			(pinfunction "1Z")
			(pintype "output")
		)
		(pad "20" smd roundrect
			(at 2.8625 -2.925 270)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 96 "/lvds_interface/MOSI1_P")
			(pinfunction "1Y")
			(pintype "output")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Package_SO.3dshapes/TSSOP-20_4.4x6.5mm_P0.65mm.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 137.12 103.7 180)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C12"
			(at 2.42 -0.0925 0)
			(layer "F.Fab")
		)
		(property "Value" "0.1uF"
			(at 0 1.16 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Ceramic capacitor"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "CREATED_ON" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DATE" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DESCRIPTION" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ID" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "INVENTORY_PRICE" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTTYPE" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ROHS" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/lvds_interface1/")
		(sheetfile "lvds-interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 180)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 3 "+3.3V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 180)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 156.5 106.9 90)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C15"
			(at 0.2 1.2 90)
			(layer "F.Fab")
		)
		(property "Value" "0.001uF"
			(at 0 1.16 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Ceramic capacitor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "CREATED_ON" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DATE" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DESCRIPTION" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ID" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "INVENTORY_PRICE" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTTYPE" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ROHS" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/lvds_interface2/")
		(sheetfile "lvds-interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 90)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 3 "+3.3V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 90)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 161.18 102.6)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C24"
			(at 2.32 -0.1 0)
			(layer "F.Fab")
		)
		(property "Value" "0.1uF"
			(at 0 1.16 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Ceramic capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "CREATED_ON" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DATE" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DESCRIPTION" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ID" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "INVENTORY_PRICE" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTTYPE" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ROHS" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/lvds_interface3/")
		(sheetfile "lvds-interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 3 "+3.3V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 168.245 82.15)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C33"
			(at -2.345 0.05 0)
			(layer "F.Fab")
		)
		(property "Value" "0.1uF"
			(at 0 1.16 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Ceramic capacitor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "CREATED_ON" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DATE" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DESCRIPTION" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ID" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "INVENTORY_PRICE" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTTYPE" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ROHS" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/power-management/")
		(sheetfile "power.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 43 "+5V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_THTPad_D3.0mm_Drill1.5mm"
		(layer "F.Cu")
		(at 160.2 79 -90)
		(descr "THT pad as test Point, diameter 3.0mm, hole diameter 1.5mm")
		(tags "test point THT pad")
		(property "Reference" "TP5"
			(at 0 -2.398 90)
			(layer "F.Fab")
		)
		(property "Value" "VIO"
			(at 0 2.55 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Test point, plated through-hole, 65/100mil"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "CREATED_ON" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DATE" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DESCRIPTION" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ID" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "INVENTORY_PRICE" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTTYPE" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ROHS" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*TP-PTH-65/100*")
		(sheetname "/power-management/")
		(sheetfile "power.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 -2.4 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 270)
			(size 3 3)
			(drill 1.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 138 "-5V")
			(pinfunction "PIN")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "Diode_SMD:D_SOD-323F"
		(layer "F.Cu")
		(at 162.765 95.85 180)
		(descr "SOD-323F http://www.nxp.com/documents/outline_drawing/SOD323F.pdf")
		(tags "SOD-323F")
		(property "Reference" "D3"
			(at 0 -1.85 0)
			(layer "F.Fab")
		)
		(property "Value" "B5817"
			(at 0.1 1.9 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Schottky diode"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "CREATED_ON" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DATE" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DESCRIPTION" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ID" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "INVENTORY_PRICE" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTTYPE" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ROHS" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TO-???* *_Diode_* *SingleDiode* D_*")
		(sheetname "/power-management/")
		(sheetfile "power.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -1.85 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.1 0 180)
			(size 0.5 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 147 "Net-(D3-K)")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.1 0 180)
			(size 0.5 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 138 "-5V")
			(pinfunction "A")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SOD-323F.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MountingHole:MountingHole_3.2mm_M3_Pad"
		(layer "F.Cu")
		(at 131.4 77.8)
		(descr "Mounting Hole 3.2mm, M3")
		(tags "mounting hole 3.2mm m3")
		(property "Reference" "MH4"
			(at 0 -4.2 0)
			(layer "F.Fab")
		)
		(property "Value" "MTG"
			(at 0 4.2 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Mounting hole"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "CREATED_ON" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DATE" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DESCRIPTION" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ID" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "INVENTORY_PRICE" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTTYPE" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ROHS" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*MTG-3.2/6.5-PTH*")
		(sheetname "/szg_interface/")
		(sheetfile "szg-interface.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 6.4 6.4)
			(drill 3.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 42 "unconnected-(MH4-Pad1)")
			(pinfunction "1")
			(pintype "passive+no_connect")
		)
		(embedded_fonts no)
	)
	(footprint "Package_TO_SOT_SMD:SOT-23-5"
		(layer "F.Cu")
		(at 128.8 106.1)
		(descr "SOT, 5 Pin (JEDEC MO-178 Var AA https://www.jedec.org/document_search?search_api_views_fulltext=MO-178), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOT TO_SOT_SMD")
		(property "Reference" "U3"
			(at 0 2.5 0)
			(layer "F.Fab")
		)
		(property "Value" "SN65LVDT2DBV"
			(at 0 2.4 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/sn65lvdt2.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "High-Speed Differential Line Receiver, 110 Ω Terminated, 630Mbps, SOT-23-5"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "CREATED_ON" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DATE" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DESCRIPTION" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ID" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "INVENTORY_PRICE" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTTYPE" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ROHS" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer" "Texas Instruments"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SOT?23*")
		(sheetname "/lvds_interface/")
		(sheetfile "lvds-interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.1375 -0.95)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 3 "+3.3V")
			(pinfunction "V_{CC}")
			(pintype "power_in")
		)
		(pad "2" smd roundrect
			(at -1.1375 0)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "3" smd roundrect
			(at -1.1375 0.95)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 90 "/lvds_interface/MISO2_P")
			(pinfunction "A")
			(pintype "input")
		)
		(pad "4" smd roundrect
			(at 1.1375 0.95)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 99 "/lvds_interface/MISO2_N")
			(pinfunction "B")
			(pintype "input")
		)
		(pad "5" smd roundrect
			(at 1.1375 -0.95)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 49 "/lvds_interface/MISO2")
			(pinfunction "R")
			(pintype "output")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 149.62 123.2 180)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C19"
			(at 0 1.2 0)
			(layer "F.Fab")
		)
		(property "Value" "0.1uF"
			(at 0 1.16 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Ceramic capacitor"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "CREATED_ON" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DATE" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DESCRIPTION" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ID" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "INVENTORY_PRICE" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTTYPE" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ROHS" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/lvds_interface2/")
		(sheetfile "lvds-interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 180)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 43 "+5V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 180)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 146.5 96.2875 -90)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C32"
			(at 0 -1.16 90)
			(layer "F.Fab")
		)
		(property "Value" "0.1uF"
			(at 0 1.16 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Ceramic capacitor"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "CREATED_ON" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DATE" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DESCRIPTION" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ID" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "INVENTORY_PRICE" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTTYPE" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ROHS" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/voltage_translation2/")
		(sheetfile "voltage_translation.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 270)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 3 "+3.3V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 270)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 136.5 96.2875 -90)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C30"
			(at 0 -1.16 90)
			(layer "F.Fab")
		)
		(property "Value" "0.1uF"
			(at 0 1.16 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Ceramic capacitor"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "CREATED_ON" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DATE" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DESCRIPTION" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ID" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "INVENTORY_PRICE" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTTYPE" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ROHS" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/voltage_translation1/")
		(sheetfile "voltage_translation.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 270)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 3 "+3.3V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 270)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 150.18 103.7)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C16"
			(at 2.32 0 0)
			(layer "F.Fab")
		)
		(property "Value" "0.001uF"
			(at 0 1.16 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Ceramic capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "CREATED_ON" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DATE" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DESCRIPTION" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ID" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "INVENTORY_PRICE" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTTYPE" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ROHS" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/lvds_interface2/")
		(sheetfile "lvds-interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 3 "+3.3V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "lvds-conn:A79633"
		(layer "F.Cu")
		(at 138.5 125.2)
		(property "Reference" "J3"
			(at 0 1.7004 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_02x08_Row_Letter_First"
			(at 0 3.2004 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at -0.0508 2.159 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, double row, 02x08, row letter first pin numbering scheme (pin number consists of a letter for the row and a number for the pin index in this row. a1, ..., aN; b1, ..., bN), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at -0.0508 2.159 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "CREATED_ON" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DATE" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DESCRIPTION" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ID" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "INVENTORY_PRICE" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTTYPE" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ROHS" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_2x??_*")
		(sheetname "/lvds_interface/")
		(sheetfile "lvds-interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 4.7004 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "a1" smd rect
			(at -2.2098 -0.635)
			(size 0.381 1.016)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 43 "+5V")
			(pinfunction "Pin_a1")
			(pintype "passive")
		)
		(pad "a2" smd rect
			(at -1.5748 -0.635)
			(size 0.381 1.016)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 90 "/lvds_interface/MISO2_P")
			(pinfunction "Pin_a2")
			(pintype "passive")
		)
		(pad "a3" smd rect
			(at -0.9398 -0.635)
			(size 0.381 1.016)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 99 "/lvds_interface/MISO2_N")
			(pinfunction "Pin_a3")
			(pintype "passive")
		)
		(pad "a4" smd rect
			(at -0.3048 -0.635)
			(size 0.381 1.016)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 92 "/lvds_interface/MOSI2_P")
			(pinfunction "Pin_a4")
			(pintype "passive")
		)
		(pad "a5" smd rect
			(at 0.3302 -0.635)
			(size 0.381 1.016)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 94 "/lvds_interface/MOSI2_N")
			(pinfunction "Pin_a5")
			(pintype "passive")
		)
		(pad "a6" smd rect
			(at 0.9652 -0.635)
			(size 0.381 1.016)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 93 "/lvds_interface/CS_P")
			(pinfunction "Pin_a6")
			(pintype "passive")
		)
		(pad "a7" smd rect
			(at 1.6002 -0.635)
			(size 0.381 1.016)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 98 "/lvds_interface/CS_N")
			(pinfunction "Pin_a7")
			(pintype "passive")
		)
		(pad "a8" smd rect
			(at 2.2352 -0.635)
			(size 0.381 1.016)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "GND")
			(pinfunction "Pin_a8")
			(pintype "passive")
		)
		(pad "b1" smd rect
			(at -2.2098 0.508)
			(size 0.381 0.762)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 138 "-5V")
			(pinfunction "Pin_b1")
			(pintype "passive")
		)
		(pad "b2" smd rect
			(at -1.5748 0.508)
			(size 0.381 0.762)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 89 "/lvds_interface/SCLK_N")
			(pinfunction "Pin_b2")
			(pintype "passive")
		)
		(pad "b3" smd rect
			(at -0.9398 0.508)
			(size 0.381 0.762)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 91 "/lvds_interface/SCLK_P")
			(pinfunction "Pin_b3")
			(pintype "passive")
		)
		(pad "b4" smd rect
			(at -0.3048 0.508)
			(size 0.381 0.762)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 88 "/lvds_interface/MOSI1_N")
			(pinfunction "Pin_b4")
			(pintype "passive")
		)
		(pad "b5" smd rect
			(at 0.3302 0.508)
			(size 0.381 0.762)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 96 "/lvds_interface/MOSI1_P")
			(pinfunction "Pin_b5")
			(pintype "passive")
		)
		(pad "b6" smd rect
			(at 0.9652 0.508)
			(size 0.381 0.762)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 95 "/lvds_interface/MISO1_N")
			(pinfunction "Pin_b6")
			(pintype "passive")
		)
		(pad "b7" smd rect
			(at 1.6002 0.508)
			(size 0.381 0.762)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 97 "/lvds_interface/MISO1_P")
			(pinfunction "Pin_b7")
			(pintype "passive")
		)
		(pad "b8" smd rect
			(at 2.2352 0.508)
			(size 0.381 0.762)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 3 "+3.3V")
			(pinfunction "Pin_b8")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 128.18 103.7)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C4"
			(at 1.92 0 0)
			(layer "F.Fab")
		)
		(property "Value" "0.001uF"
			(at 0 1.16 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Ceramic capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "CREATED_ON" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DATE" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DESCRIPTION" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ID" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "INVENTORY_PRICE" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTTYPE" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ROHS" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/lvds_interface/")
		(sheetfile "lvds-interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 3 "+3.3V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 142.52 123.2 180)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C13"
			(at 0 1.2 0)
			(layer "F.Fab")
		)
		(property "Value" "0.1uF"
			(at 0 1.16 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Ceramic capacitor"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "CREATED_ON" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DATE" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DESCRIPTION" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ID" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "INVENTORY_PRICE" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTTYPE" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ROHS" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/lvds_interface1/")
		(sheetfile "lvds-interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 180)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 43 "+5V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 180)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "lvds-conn:A79633"
		(layer "F.Cu")
		(at 145.5 125.2)
		(property "Reference" "J4"
			(at 0 1.7004 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_02x08_Row_Letter_First"
			(at 0 3.2004 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at -0.0508 2.159 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, double row, 02x08, row letter first pin numbering scheme (pin number consists of a letter for the row and a number for the pin index in this row. a1, ..., aN; b1, ..., bN), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at -0.0508 2.159 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "CREATED_ON" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DATE" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DESCRIPTION" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ID" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "INVENTORY_PRICE" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTTYPE" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ROHS" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_2x??_*")
		(sheetname "/lvds_interface1/")
		(sheetfile "lvds-interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 4.7004 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "a1" smd rect
			(at -2.2098 -0.635)
			(size 0.381 1.016)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 43 "+5V")
			(pinfunction "Pin_a1")
			(pintype "passive")
		)
		(pad "a2" smd rect
			(at -1.5748 -0.635)
			(size 0.381 1.016)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 104 "/lvds_interface1/MISO2_P")
			(pinfunction "Pin_a2")
			(pintype "passive")
		)
		(pad "a3" smd rect
			(at -0.9398 -0.635)
			(size 0.381 1.016)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 105 "/lvds_interface1/MISO2_N")
			(pinfunction "Pin_a3")
			(pintype "passive")
		)
		(pad "a4" smd rect
			(at -0.3048 -0.635)
			(size 0.381 1.016)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 106 "/lvds_interface1/MOSI2_P")
			(pinfunction "Pin_a4")
			(pintype "passive")
		)
		(pad "a5" smd rect
			(at 0.3302 -0.635)
			(size 0.381 1.016)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 103 "/lvds_interface1/MOSI2_N")
			(pinfunction "Pin_a5")
			(pintype "passive")
		)
		(pad "a6" smd rect
			(at 0.9652 -0.635)
			(size 0.381 1.016)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 107 "/lvds_interface1/CS_P")
			(pinfunction "Pin_a6")
			(pintype "passive")
		)
		(pad "a7" smd rect
			(at 1.6002 -0.635)
			(size 0.381 1.016)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 101 "/lvds_interface1/CS_N")
			(pinfunction "Pin_a7")
			(pintype "passive")
		)
		(pad "a8" smd rect
			(at 2.2352 -0.635)
			(size 0.381 1.016)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "GND")
			(pinfunction "Pin_a8")
			(pintype "passive")
		)
		(pad "b1" smd rect
			(at -2.2098 0.508)
			(size 0.381 0.762)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 138 "-5V")
			(pinfunction "Pin_b1")
			(pintype "passive")
		)
		(pad "b2" smd rect
			(at -1.5748 0.508)
			(size 0.381 0.762)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 100 "/lvds_interface1/SCLK_N")
			(pinfunction "Pin_b2")
			(pintype "passive")
		)
		(pad "b3" smd rect
			(at -0.9398 0.508)
			(size 0.381 0.762)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 110 "/lvds_interface1/SCLK_P")
			(pinfunction "Pin_b3")
			(pintype "passive")
		)
		(pad "b4" smd rect
			(at -0.3048 0.508)
			(size 0.381 0.762)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 108 "/lvds_interface1/MOSI1_N")
			(pinfunction "Pin_b4")
			(pintype "passive")
		)
		(pad "b5" smd rect
			(at 0.3302 0.508)
			(size 0.381 0.762)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 111 "/lvds_interface1/MOSI1_P")
			(pinfunction "Pin_b5")
			(pintype "passive")
		)
		(pad "b6" smd rect
			(at 0.9652 0.508)
			(size 0.381 0.762)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 102 "/lvds_interface1/MISO1_N")
			(pinfunction "Pin_b6")
			(pintype "passive")
		)
		(pad "b7" smd rect
			(at 1.6002 0.508)
			(size 0.381 0.762)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 109 "/lvds_interface1/MISO1_P")
			(pinfunction "Pin_b7")
			(pintype "passive")
		)
		(pad "b8" smd rect
			(at 2.2352 0.508)
			(size 0.381 0.762)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 3 "+3.3V")
			(pinfunction "Pin_b8")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "Package_SO:SOIC-16W_7.5x10.3mm_P1.27mm"
		(layer "F.Cu")
		(at 164.565 88.75 -90)
		(descr "SOIC, 16 Pin (JEDEC MS-013AA, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_wide-rw/rw_16.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOIC SO")
		(property "Reference" "U13"
			(at 0 -6.1 90)
			(layer "F.Fab")
		)
		(property "Value" "MAX739EWE"
			(at 0 6.1 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Buck-Boost Switching Regulator IC Negative Fixed -5V 1 Output 300mA 16-SOIC (0.295\", 7.50mm Width)"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer" "Analog Devices Inc./Maxim Integrated"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "CREATED_ON" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DATE" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DESCRIPTION" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ID" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "INVENTORY_PRICE" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTTYPE" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ROHS" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/power-management/")
		(sheetfile "power.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -4.65 -4.445 270)
			(size 2.05 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 43 "+5V")
			(pinfunction "V+")
			(pintype "power_in")
		)
		(pad "2" smd roundrect
			(at -4.65 -3.175 270)
			(size 2.05 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 43 "+5V")
			(pinfunction "nSHDN")
			(pintype "input")
		)
		(pad "3" smd roundrect
			(at -4.65 -1.905 270)
			(size 2.05 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 136 "Net-(U13-VREF)")
			(pinfunction "VREF")
			(pintype "power_in")
		)
		(pad "4" smd roundrect
			(at -4.65 -0.635 270)
			(size 2.05 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 140 "unconnected-(U13-N.C.-Pad4)")
			(pinfunction "N.C.")
			(pintype "no_connect")
		)
		(pad "5" smd roundrect
			(at -4.65 0.635 270)
			(size 2.05 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 142 "unconnected-(U13-N.C.-Pad5)")
			(pinfunction "N.C.")
			(pintype "no_connect")
		)
		(pad "6" smd roundrect
			(at -4.65 1.905 270)
			(size 2.05 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 143 "unconnected-(U13-N.C.-Pad6)")
			(pinfunction "N.C.")
			(pintype "no_connect")
		)
		(pad "7" smd roundrect
			(at -4.65 3.175 270)
			(size 2.05 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 137 "Net-(U13-SS)")
			(pinfunction "SS")
			(pintype "bidirectional")
		)
		(pad "8" smd roundrect
			(at -4.65 4.445 270)
			(size 2.05 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 141 "unconnected-(U13-CC-Pad8)")
			(pinfunction "CC")
			(pintype "input+no_connect")
		)
		(pad "9" smd roundrect
			(at 4.65 4.445 270)
			(size 2.05 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 138 "-5V")
			(pinfunction "Vout")
			(pintype "power_out")
		)
		(pad "10" smd roundrect
			(at 4.65 3.175 270)
			(size 2.05 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 139 "Net-(JP1-C)")
			(pinfunction "DRV-")
			(pintype "input")
		)
		(pad "11" smd roundrect
			(at 4.65 1.905 270)
			(size 2.05 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "12" smd roundrect
			(at 4.65 0.635 270)
			(size 2.05 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 147 "Net-(D3-K)")
			(pinfunction "LX")
			(pintype "power_out")
		)
		(pad "13" smd roundrect
			(at 4.65 -0.635 270)
			(size 2.05 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 147 "Net-(D3-K)")
			(pinfunction "LX")
			(pintype "power_out")
		)
		(pad "14" smd roundrect
			(at 4.65 -1.905 270)
			(size 2.05 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 147 "Net-(D3-K)")
			(pinfunction "LX")
			(pintype "power_out")
		)
		(pad "15" smd roundrect
			(at 4.65 -3.175 270)
			(size 2.05 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 43 "+5V")
			(pinfunction "V+")
			(pintype "power_in")
		)
		(pad "16" smd roundrect
			(at 4.65 -4.445 270)
			(size 2.05 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 43 "+5V")
			(pinfunction "V+")
			(pintype "power_in")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Package_SO.3dshapes/SOIC-16W_7.5x10.3mm_P1.27mm.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_SO:TSSOP-20_4.4x6.5mm_P0.65mm"
		(layer "F.Cu")
		(at 155.5 112.1 -90)
		(descr "TSSOP, 20 Pin (JEDEC MO-153 Var AC https://www.jedec.org/document_search?search_api_views_fulltext=MO-153), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "TSSOP SO")
		(property "Reference" "U6"
			(at 0 -4.2 90)
			(layer "F.Fab")
		)
		(property "Value" "SN65LVDT41"
			(at 0 4.2 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Multi-channel transceivers for SPI over LVDS"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "CREATED_ON" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DATE" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DESCRIPTION" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ID" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "INVENTORY_PRICE" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTTYPE" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ROHS" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer" "Texas Instruments"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/lvds_interface2/")
		(sheetfile "lvds-interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -2.8625 -2.925 270)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 59 "/lvds_interface2/MOSI1")
			(pinfunction "1D")
			(pintype "input")
		)
		(pad "2" smd roundrect
			(at -2.8625 -2.275 270)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "3" smd roundrect
			(at -2.8625 -1.625 270)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 60 "/lvds_interface2/SCLK")
			(pinfunction "2D")
			(pintype "input")
		)
		(pad "4" smd roundrect
			(at -2.8625 -0.975 270)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 3 "+3.3V")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(pad "5" smd roundrect
			(at -2.8625 -0.325 270)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 57 "/lvds_interface2/MOSI2")
			(pinfunction "3D")
			(pintype "input")
		)
		(pad "6" smd roundrect
			(at -2.8625 0.325 270)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "7" smd roundrect
			(at -2.8625 0.975 270)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 58 "/lvds_interface2/CS")
			(pinfunction "4D")
			(pintype "input")
		)
		(pad "8" smd roundrect
			(at -2.8625 1.625 270)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 3 "+3.3V")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(pad "9" smd roundrect
			(at -2.8625 2.275 270)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 56 "/lvds_interface2/MISO1")
			(pinfunction "5R")
			(pintype "output")
		)
		(pad "10" smd roundrect
			(at -2.8625 2.925 270)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "11" smd roundrect
			(at 2.8625 2.925 270)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 114 "/lvds_interface2/MISO1_N")
			(pinfunction "5B")
			(pintype "output")
		)
		(pad "12" smd roundrect
			(at 2.8625 2.275 270)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 122 "/lvds_interface2/MISO1_P")
			(pinfunction "5A")
			(pintype "output")
		)
		(pad "13" smd roundrect
			(at 2.8625 1.625 270)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 113 "/lvds_interface2/CS_N")
			(pinfunction "4Z")
			(pintype "output")
		)
		(pad "14" smd roundrect
			(at 2.8625 0.975 270)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 123 "/lvds_interface2/CS_P")
			(pinfunction "4Y")
			(pintype "output")
		)
		(pad "15" smd roundrect
			(at 2.8625 0.325 270)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 118 "/lvds_interface2/MOSI2_N")
			(pinfunction "3Z")
			(pintype "output")
		)
		(pad "16" smd roundrect
			(at 2.8625 -0.325 270)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 120 "/lvds_interface2/MOSI2_P")
			(pinfunction "3Y")
			(pintype "output")
		)
		(pad "17" smd roundrect
			(at 2.8625 -0.975 270)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 121 "/lvds_interface2/SCLK_N")
			(pinfunction "2Z")
			(pintype "output")
		)
		(pad "18" smd roundrect
			(at 2.8625 -1.625 270)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 119 "/lvds_interface2/SCLK_P")
			(pinfunction "2Y")
			(pintype "output")
		)
		(pad "19" smd roundrect
			(at 2.8625 -2.275 270)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 115 "/lvds_interface2/MOSI1_N")
			(pinfunction "1Z")
			(pintype "output")
		)
		(pad "20" smd roundrect
			(at 2.8625 -2.925 270)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 117 "/lvds_interface2/MOSI1_P")
			(pinfunction "1Y")
			(pintype "output")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Package_SO.3dshapes/TSSOP-20_4.4x6.5mm_P0.65mm.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "lvds-conn:A79633"
		(layer "F.Cu")
		(at 159.5 125.2)
		(property "Reference" "J6"
			(at 0 1.7004 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_02x08_Row_Letter_First"
			(at 0 3.2004 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at -0.0508 2.159 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, double row, 02x08, row letter first pin numbering scheme (pin number consists of a letter for the row and a number for the pin index in this row. a1, ..., aN; b1, ..., bN), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at -0.0508 2.159 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "CREATED_ON" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DATE" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DESCRIPTION" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ID" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "INVENTORY_PRICE" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTTYPE" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ROHS" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_2x??_*")
		(sheetname "/lvds_interface3/")
		(sheetfile "lvds-interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 4.7004 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "a1" smd rect
			(at -2.2098 -0.635)
			(size 0.381 1.016)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 43 "+5V")
			(pinfunction "Pin_a1")
			(pintype "passive")
		)
		(pad "a2" smd rect
			(at -1.5748 -0.635)
			(size 0.381 1.016)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 135 "/lvds_interface3/MISO2_P")
			(pinfunction "Pin_a2")
			(pintype "passive")
		)
		(pad "a3" smd rect
			(at -0.9398 -0.635)
			(size 0.381 1.016)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 125 "/lvds_interface3/MISO2_N")
			(pinfunction "Pin_a3")
			(pintype "passive")
		)
		(pad "a4" smd rect
			(at -0.3048 -0.635)
			(size 0.381 1.016)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 128 "/lvds_interface3/MOSI2_P")
			(pinfunction "Pin_a4")
			(pintype "passive")
		)
		(pad "a5" smd rect
			(at 0.3302 -0.635)
			(size 0.381 1.016)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 126 "/lvds_interface3/MOSI2_N")
			(pinfunction "Pin_a5")
			(pintype "passive")
		)
		(pad "a6" smd rect
			(at 0.9652 -0.635)
			(size 0.381 1.016)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 133 "/lvds_interface3/CS_P")
			(pinfunction "Pin_a6")
			(pintype "passive")
		)
		(pad "a7" smd rect
			(at 1.6002 -0.635)
			(size 0.381 1.016)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 127 "/lvds_interface3/CS_N")
			(pinfunction "Pin_a7")
			(pintype "passive")
		)
		(pad "a8" smd rect
			(at 2.2352 -0.635)
			(size 0.381 1.016)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "GND")
			(pinfunction "Pin_a8")
			(pintype "passive")
		)
		(pad "b1" smd rect
			(at -2.2098 0.508)
			(size 0.381 0.762)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 138 "-5V")
			(pinfunction "Pin_b1")
			(pintype "passive")
		)
		(pad "b2" smd rect
			(at -1.5748 0.508)
			(size 0.381 0.762)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 132 "/lvds_interface3/SCLK_N")
			(pinfunction "Pin_b2")
			(pintype "passive")
		)
		(pad "b3" smd rect
			(at -0.9398 0.508)
			(size 0.381 0.762)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 134 "/lvds_interface3/SCLK_P")
			(pinfunction "Pin_b3")
			(pintype "passive")
		)
		(pad "b4" smd rect
			(at -0.3048 0.508)
			(size 0.381 0.762)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 124 "/lvds_interface3/MOSI1_N")
			(pinfunction "Pin_b4")
			(pintype "passive")
		)
		(pad "b5" smd rect
			(at 0.3302 0.508)
			(size 0.381 0.762)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 130 "/lvds_interface3/MOSI1_P")
			(pinfunction "Pin_b5")
			(pintype "passive")
		)
		(pad "b6" smd rect
			(at 0.9652 0.508)
			(size 0.381 0.762)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 129 "/lvds_interface3/MISO1_N")
			(pinfunction "Pin_b6")
			(pintype "passive")
		)
		(pad "b7" smd rect
			(at 1.6002 0.508)
			(size 0.381 0.762)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 131 "/lvds_interface3/MISO1_P")
			(pinfunction "Pin_b7")
			(pintype "passive")
		)
		(pad "b8" smd rect
			(at 2.2352 0.508)
			(size 0.381 0.762)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 3 "+3.3V")
			(pinfunction "Pin_b8")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "lvds-conn:A79633"
		(layer "F.Cu")
		(at 152.5 125.2)
		(property "Reference" "J5"
			(at 0 1.7004 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_02x08_Row_Letter_First"
			(at 0 3.2004 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at -0.0508 2.159 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, double row, 02x08, row letter first pin numbering scheme (pin number consists of a letter for the row and a number for the pin index in this row. a1, ..., aN; b1, ..., bN), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at -0.0508 2.159 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "CREATED_ON" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DATE" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DESCRIPTION" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ID" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "INVENTORY_PRICE" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTTYPE" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ROHS" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_2x??_*")
		(sheetname "/lvds_interface2/")
		(sheetfile "lvds-interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 4.7004 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "a1" smd rect
			(at -2.2098 -0.635)
			(size 0.381 1.016)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 43 "+5V")
			(pinfunction "Pin_a1")
			(pintype "passive")
		)
		(pad "a2" smd rect
			(at -1.5748 -0.635)
			(size 0.381 1.016)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 116 "/lvds_interface2/MISO2_P")
			(pinfunction "Pin_a2")
			(pintype "passive")
		)
		(pad "a3" smd rect
			(at -0.9398 -0.635)
			(size 0.381 1.016)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 112 "/lvds_interface2/MISO2_N")
			(pinfunction "Pin_a3")
			(pintype "passive")
		)
		(pad "a4" smd rect
			(at -0.3048 -0.635)
			(size 0.381 1.016)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 120 "/lvds_interface2/MOSI2_P")
			(pinfunction "Pin_a4")
			(pintype "passive")
		)
		(pad "a5" smd rect
			(at 0.3302 -0.635)
			(size 0.381 1.016)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 118 "/lvds_interface2/MOSI2_N")
			(pinfunction "Pin_a5")
			(pintype "passive")
		)
		(pad "a6" smd rect
			(at 0.9652 -0.635)
			(size 0.381 1.016)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 123 "/lvds_interface2/CS_P")
			(pinfunction "Pin_a6")
			(pintype "passive")
		)
		(pad "a7" smd rect
			(at 1.6002 -0.635)
			(size 0.381 1.016)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 113 "/lvds_interface2/CS_N")
			(pinfunction "Pin_a7")
			(pintype "passive")
		)
		(pad "a8" smd rect
			(at 2.2352 -0.635)
			(size 0.381 1.016)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "GND")
			(pinfunction "Pin_a8")
			(pintype "passive")
		)
		(pad "b1" smd rect
			(at -2.2098 0.508)
			(size 0.381 0.762)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 138 "-5V")
			(pinfunction "Pin_b1")
			(pintype "passive")
		)
		(pad "b2" smd rect
			(at -1.5748 0.508)
			(size 0.381 0.762)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 121 "/lvds_interface2/SCLK_N")
			(pinfunction "Pin_b2")
			(pintype "passive")
		)
		(pad "b3" smd rect
			(at -0.9398 0.508)
			(size 0.381 0.762)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 119 "/lvds_interface2/SCLK_P")
			(pinfunction "Pin_b3")
			(pintype "passive")
		)
		(pad "b4" smd rect
			(at -0.3048 0.508)
			(size 0.381 0.762)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 115 "/lvds_interface2/MOSI1_N")
			(pinfunction "Pin_b4")
			(pintype "passive")
		)
		(pad "b5" smd rect
			(at 0.3302 0.508)
			(size 0.381 0.762)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 117 "/lvds_interface2/MOSI1_P")
			(pinfunction "Pin_b5")
			(pintype "passive")
		)
		(pad "b6" smd rect
			(at 0.9652 0.508)
			(size 0.381 0.762)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 114 "/lvds_interface2/MISO1_N")
			(pinfunction "Pin_b6")
			(pintype "passive")
		)
		(pad "b7" smd rect
			(at 1.6002 0.508)
			(size 0.381 0.762)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 122 "/lvds_interface2/MISO1_P")
			(pinfunction "Pin_b7")
			(pintype "passive")
		)
		(pad "b8" smd rect
			(at 2.2352 0.508)
			(size 0.381 0.762)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 3 "+3.3V")
			(pinfunction "Pin_b8")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "Package_SO:TSSOP-20_4.4x6.5mm_P0.65mm"
		(layer "F.Cu")
		(at 144.5 112.1 -90)
		(descr "TSSOP, 20 Pin (JEDEC MO-153 Var AC https://www.jedec.org/document_search?search_api_views_fulltext=MO-153), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "TSSOP SO")
		(property "Reference" "U4"
			(at 0 -4.2 90)
			(layer "F.Fab")
		)
		(property "Value" "SN65LVDT41"
			(at 0 4.2 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Multi-channel transceivers for SPI over LVDS"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "CREATED_ON" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DATE" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DESCRIPTION" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ID" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "INVENTORY_PRICE" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTTYPE" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ROHS" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer" "Texas Instruments"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/lvds_interface1/")
		(sheetfile "lvds-interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -2.8625 -2.925 270)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 50 "/lvds_interface1/MOSI1")
			(pinfunction "1D")
			(pintype "input")
		)
		(pad "2" smd roundrect
			(at -2.8625 -2.275 270)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "3" smd roundrect
			(at -2.8625 -1.625 270)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 54 "/lvds_interface1/SCLK")
			(pinfunction "2D")
			(pintype "input")
		)
		(pad "4" smd roundrect
			(at -2.8625 -0.975 270)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 3 "+3.3V")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(pad "5" smd roundrect
			(at -2.8625 -0.325 270)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 52 "/lvds_interface1/MOSI2")
			(pinfunction "3D")
			(pintype "input")
		)
		(pad "6" smd roundrect
			(at -2.8625 0.325 270)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "7" smd roundrect
			(at -2.8625 0.975 270)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 51 "/lvds_interface1/CS")
			(pinfunction "4D")
			(pintype "input")
		)
		(pad "8" smd roundrect
			(at -2.8625 1.625 270)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 3 "+3.3V")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(pad "9" smd roundrect
			(at -2.8625 2.275 270)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 53 "/lvds_interface1/MISO1")
			(pinfunction "5R")
			(pintype "output")
		)
		(pad "10" smd roundrect
			(at -2.8625 2.925 270)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "11" smd roundrect
			(at 2.8625 2.925 270)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 102 "/lvds_interface1/MISO1_N")
			(pinfunction "5B")
			(pintype "output")
		)
		(pad "12" smd roundrect
			(at 2.8625 2.275 270)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 109 "/lvds_interface1/MISO1_P")
			(pinfunction "5A")
			(pintype "output")
		)
		(pad "13" smd roundrect
			(at 2.8625 1.625 270)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 101 "/lvds_interface1/CS_N")
			(pinfunction "4Z")
			(pintype "output")
		)
		(pad "14" smd roundrect
			(at 2.8625 0.975 270)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 107 "/lvds_interface1/CS_P")
			(pinfunction "4Y")
			(pintype "output")
		)
		(pad "15" smd roundrect
			(at 2.8625 0.325 270)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 103 "/lvds_interface1/MOSI2_N")
			(pinfunction "3Z")
			(pintype "output")
		)
		(pad "16" smd roundrect
			(at 2.8625 -0.325 270)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 106 "/lvds_interface1/MOSI2_P")
			(pinfunction "3Y")
			(pintype "output")
		)
		(pad "17" smd roundrect
			(at 2.8625 -0.975 270)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 100 "/lvds_interface1/SCLK_N")
			(pinfunction "2Z")
			(pintype "output")
		)
		(pad "18" smd roundrect
			(at 2.8625 -1.625 270)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 110 "/lvds_interface1/SCLK_P")
			(pinfunction "2Y")
			(pintype "output")
		)
		(pad "19" smd roundrect
			(at 2.8625 -2.275 270)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 108 "/lvds_interface1/MOSI1_N")
			(pinfunction "1Z")
			(pintype "output")
		)
		(pad "20" smd roundrect
			(at 2.8625 -2.925 270)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 111 "/lvds_interface1/MOSI1_P")
			(pinfunction "1Y")
			(pintype "output")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Package_SO.3dshapes/TSSOP-20_4.4x6.5mm_P0.65mm.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 160.885 82.15)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C36"
			(at 0 -1.16 0)
			(layer "F.Fab")
		)
		(property "Value" "0.1uF"
			(at 0 1.16 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Ceramic capacitor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "CREATED_ON" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DATE" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DESCRIPTION" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ID" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "INVENTORY_PRICE" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTTYPE" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ROHS" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/power-management/")
		(sheetfile "power.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 137 "Net-(U13-SS)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 146.6 89.5875 -90)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C31"
			(at 0 -1.16 90)
			(layer "F.Fab")
		)
		(property "Value" "0.1uF"
			(at 0 1.16 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Ceramic capacitor"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "CREATED_ON" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DATE" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DESCRIPTION" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ID" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "INVENTORY_PRICE" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTTYPE" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ROHS" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/voltage_translation2/")
		(sheetfile "voltage_translation.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 270)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 270)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 33 "VIO")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_THTPad_D3.0mm_Drill1.5mm"
		(layer "F.Cu")
		(at 136.5 64.1)
		(descr "THT pad as test Point, diameter 3.0mm, hole diameter 1.5mm")
		(tags "test point THT pad")
		(property "Reference" "TP2"
			(at 0 -2.398 0)
			(layer "F.Fab")
		)
		(property "Value" "+5V"
			(at 0 2.55 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Test point, plated through-hole, 65/100mil"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "CREATED_ON" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DATE" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DESCRIPTION" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ID" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "INVENTORY_PRICE" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTTYPE" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ROHS" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*TP-PTH-65/100*")
		(sheetname "/szg_interface/")
		(sheetfile "szg-interface.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 -2.4 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 3 3)
			(drill 1.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 43 "+5V")
			(pinfunction "PIN")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "F.Cu")
		(at 159.965 96.499999 90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C37"
			(at -1.250001 -1.7 90)
			(layer "F.Fab")
		)
		(property "Value" "33uF"
			(at 0 1.679999 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Ceramic capacitor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "CREATED_ON" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DATE" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DESCRIPTION" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ID" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "INVENTORY_PRICE" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTTYPE" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ROHS" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/power-management/")
		(sheetfile "power.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.949999 0 90)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.949999 0 90)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 138 "-5V")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MountingHole:MountingHole_3.2mm_M3_Pad"
		(layer "F.Cu")
		(at 166.4 77.8)
		(descr "Mounting Hole 3.2mm, M3")
		(tags "mounting hole 3.2mm m3")
		(property "Reference" "MH3"
			(at 0 -4.2 0)
			(layer "F.Fab")
		)
		(property "Value" "MTG"
			(at 0 4.2 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Mounting hole"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "CREATED_ON" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DATE" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DESCRIPTION" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ID" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "INVENTORY_PRICE" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTTYPE" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ROHS" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*MTG-3.2/6.5-PTH*")
		(sheetname "/szg_interface/")
		(sheetfile "szg-interface.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 6.4 6.4)
			(drill 3.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 41 "unconnected-(MH3-Pad1)")
			(pinfunction "1")
			(pintype "passive+no_connect")
		)
		(embedded_fonts no)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 134.5 106.9 90)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C3"
			(at 0 1.2 90)
			(layer "F.Fab")
		)
		(property "Value" "0.001uF"
			(at 0 1.16 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Ceramic capacitor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "CREATED_ON" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DATE" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DESCRIPTION" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ID" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "INVENTORY_PRICE" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTTYPE" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ROHS" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/lvds_interface/")
		(sheetfile "lvds-interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 90)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 3 "+3.3V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 90)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 164.9 106.92 90)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C23"
			(at 1.72 0.4 180)
			(layer "F.Fab")
		)
		(property "Value" "0.1uF"
			(at 0 1.16 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Ceramic capacitor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "CREATED_ON" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DATE" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DESCRIPTION" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ID" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "INVENTORY_PRICE" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTTYPE" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ROHS" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/lvds_interface3/")
		(sheetfile "lvds-interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 90)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 3 "+3.3V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 90)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MountingHole:MountingHole_3.2mm_M3_Pad"
		(layer "F.Cu")
		(at 165.9 67.8)
		(descr "Mounting Hole 3.2mm, M3")
		(tags "mounting hole 3.2mm m3")
		(property "Reference" "MH1"
			(at 0 -4.2 0)
			(layer "F.Fab")
		)
		(property "Value" "MTG"
			(at 0 4.2 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Mounting hole"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "CREATED_ON" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DATE" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DESCRIPTION" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ID" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "INVENTORY_PRICE" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTTYPE" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ROHS" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*MTG-3.2/6.5-PTH*")
		(sheetname "/szg_interface/")
		(sheetfile "szg-interface.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 6.4 6.4)
			(drill 3.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 39 "unconnected-(MH1-Pad1)")
			(pinfunction "1")
			(pintype "passive+no_connect")
		)
		(embedded_fonts no)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 153.9 106.9 90)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C17"
			(at 1.7 0.4 180)
			(layer "F.Fab")
		)
		(property "Value" "0.1uF"
			(at 0 1.16 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Ceramic capacitor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "CREATED_ON" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DATE" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DESCRIPTION" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ID" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "INVENTORY_PRICE" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTTYPE" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ROHS" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/lvds_interface2/")
		(sheetfile "lvds-interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 90)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 3 "+3.3V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 90)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 142 128.5 90)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C14"
			(at 0 -1.16 90)
			(layer "F.Fab")
		)
		(property "Value" "0.1uF"
			(at 0 1.16 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Ceramic capacitor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "CREATED_ON" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DATE" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DESCRIPTION" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ID" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "INVENTORY_PRICE" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTTYPE" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ROHS" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/lvds_interface1/")
		(sheetfile "lvds-interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 90)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 90)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 138 "-5V")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 148.02 103.7 180)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C18"
			(at 2.32 -0.1 0)
			(layer "F.Fab")
		)
		(property "Value" "0.1uF"
			(at 0 1.16 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Ceramic capacitor"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "CREATED_ON" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DATE" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DESCRIPTION" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ID" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "INVENTORY_PRICE" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTTYPE" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ROHS" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/lvds_interface2/")
		(sheetfile "lvds-interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 180)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 3 "+3.3V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 180)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 135 128.5 90)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C8"
			(at 0 -1.16 90)
			(layer "F.Fab")
		)
		(property "Value" "0.1uF"
			(at 0 1.16 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Ceramic capacitor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "CREATED_ON" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DATE" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DESCRIPTION" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ID" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "INVENTORY_PRICE" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTTYPE" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ROHS" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/lvds_interface/")
		(sheetfile "lvds-interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 90)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 90)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 138 "-5V")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 156.6 96.1875 -90)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C28"
			(at 0 -1.16 90)
			(layer "F.Fab")
		)
		(property "Value" "0.1uF"
			(at 0 1.16 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Ceramic capacitor"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "CREATED_ON" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DATE" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DESCRIPTION" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ID" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "INVENTORY_PRICE" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTTYPE" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ROHS" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/voltage_translation/")
		(sheetfile "voltage_translation.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 270)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 3 "+3.3V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 270)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 131.9 106.92 90)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C5"
			(at 1.72 0 180)
			(layer "F.Fab")
		)
		(property "Value" "0.1uF"
			(at 0 1.16 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Ceramic capacitor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "CREATED_ON" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DATE" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DESCRIPTION" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ID" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "INVENTORY_PRICE" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTTYPE" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ROHS" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/lvds_interface/")
		(sheetfile "lvds-interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 90)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 3 "+3.3V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 90)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "lvds-conn:iacoma"
		(layer "F.Cu")
		(at 148.9 69.65)
		(property "Reference" "G***"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "LOGO"
			(at 0.75 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr board_only exclude_from_pos_files exclude_from_bom)
		(embedded_fonts no)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 161.18 103.7)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C22"
			(at 2.32 0 0)
			(layer "F.Fab")
		)
		(property "Value" "0.001uF"
			(at 0 1.16 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Ceramic capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "CREATED_ON" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DATE" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DESCRIPTION" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ID" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "INVENTORY_PRICE" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTTYPE" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ROHS" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/lvds_interface3/")
		(sheetfile "lvds-interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 3 "+3.3V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_THTPad_D3.0mm_Drill1.5mm"
		(layer "F.Cu")
		(at 128.9 72.7 180)
		(descr "THT pad as test Point, diameter 3.0mm, hole diameter 1.5mm")
		(tags "test point THT pad")
		(property "Reference" "TP4"
			(at -3.2 0 0)
			(layer "F.Fab")
		)
		(property "Value" "GND"
			(at 0 2.55 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Test point, plated through-hole, 65/100mil"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "CREATED_ON" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DATE" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DESCRIPTION" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ID" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "INVENTORY_PRICE" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTTYPE" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ROHS" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*TP-PTH-65/100*")
		(sheetname "/szg_interface/")
		(sheetfile "szg-interface.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 -2.4 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 180)
			(size 3 3)
			(drill 1.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "PIN")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "MountingHole:MountingHole_3.2mm_M3_Pad"
		(layer "F.Cu")
		(at 166.4 125.8)
		(descr "Mounting Hole 3.2mm, M3")
		(tags "mounting hole 3.2mm m3")
		(property "Reference" "MH5"
			(at 0 -4.2 0)
			(layer "F.Fab")
		)
		(property "Value" "MTG"
			(at 0 4.2 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Mounting hole"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "CREATED_ON" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DATE" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DESCRIPTION" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ID" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "INVENTORY_PRICE" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTTYPE" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ROHS" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*MTG-3.2/6.5-PTH*")
		(sheetname "/szg_interface/")
		(sheetfile "szg-interface.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 6.4 6.4)
			(drill 3.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 68 "unconnected-(MH5-Pad1)")
			(pinfunction "1")
			(pintype "passive+no_connect")
		)
		(embedded_fonts no)
	)
	(footprint "Package_SO:TSSOP-20_4.4x6.5mm_P0.65mm"
		(layer "F.Cu")
		(at 166.5 112.1 -90)
		(descr "TSSOP, 20 Pin (JEDEC MO-153 Var AC https://www.jedec.org/document_search?search_api_views_fulltext=MO-153), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "TSSOP SO")
		(property "Reference" "U8"
			(at 0 -4.2 90)
			(layer "F.Fab")
		)
		(property "Value" "SN65LVDT41"
			(at 0 4.2 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Multi-channel transceivers for SPI over LVDS"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "CREATED_ON" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DATE" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DESCRIPTION" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ID" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "INVENTORY_PRICE" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTTYPE" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ROHS" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer" "Texas Instruments"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/lvds_interface3/")
		(sheetfile "lvds-interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -2.8625 -2.925 270)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 62 "/lvds_interface3/MOSI1")
			(pinfunction "1D")
			(pintype "input")
		)
		(pad "2" smd roundrect
			(at -2.8625 -2.275 270)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "3" smd roundrect
			(at -2.8625 -1.625 270)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 64 "/lvds_interface3/SCLK")
			(pinfunction "2D")
			(pintype "input")
		)
		(pad "4" smd roundrect
			(at -2.8625 -0.975 270)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 3 "+3.3V")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(pad "5" smd roundrect
			(at -2.8625 -0.325 270)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 63 "/lvds_interface3/MOSI2")
			(pinfunction "3D")
			(pintype "input")
		)
		(pad "6" smd roundrect
			(at -2.8625 0.325 270)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "7" smd roundrect
			(at -2.8625 0.975 270)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 66 "/lvds_interface3/CS")
			(pinfunction "4D")
			(pintype "input")
		)
		(pad "8" smd roundrect
			(at -2.8625 1.625 270)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 3 "+3.3V")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(pad "9" smd roundrect
			(at -2.8625 2.275 270)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 65 "/lvds_interface3/MISO1")
			(pinfunction "5R")
			(pintype "output")
		)
		(pad "10" smd roundrect
			(at -2.8625 2.925 270)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "11" smd roundrect
			(at 2.8625 2.925 270)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 129 "/lvds_interface3/MISO1_N")
			(pinfunction "5B")
			(pintype "output")
		)
		(pad "12" smd roundrect
			(at 2.8625 2.275 270)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 131 "/lvds_interface3/MISO1_P")
			(pinfunction "5A")
			(pintype "output")
		)
		(pad "13" smd roundrect
			(at 2.8625 1.625 270)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 127 "/lvds_interface3/CS_N")
			(pinfunction "4Z")
			(pintype "output")
		)
		(pad "14" smd roundrect
			(at 2.8625 0.975 270)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 133 "/lvds_interface3/CS_P")
			(pinfunction "4Y")
			(pintype "output")
		)
		(pad "15" smd roundrect
			(at 2.8625 0.325 270)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 126 "/lvds_interface3/MOSI2_N")
			(pinfunction "3Z")
			(pintype "output")
		)
		(pad "16" smd roundrect
			(at 2.8625 -0.325 270)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 128 "/lvds_interface3/MOSI2_P")
			(pinfunction "3Y")
			(pintype "output")
		)
		(pad "17" smd roundrect
			(at 2.8625 -0.975 270)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 132 "/lvds_interface3/SCLK_N")
			(pinfunction "2Z")
			(pintype "output")
		)
		(pad "18" smd roundrect
			(at 2.8625 -1.625 270)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 134 "/lvds_interface3/SCLK_P")
			(pinfunction "2Y")
			(pintype "output")
		)
		(pad "19" smd roundrect
			(at 2.8625 -2.275 270)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 124 "/lvds_interface3/MOSI1_N")
			(pinfunction "1Z")
			(pintype "output")
		)
		(pad "20" smd roundrect
			(at 2.8625 -2.925 270)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 130 "/lvds_interface3/MOSI1_P")
			(pinfunction "1Y")
			(pintype "output")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Package_SO.3dshapes/TSSOP-20_4.4x6.5mm_P0.65mm.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_THTPad_D3.0mm_Drill1.5mm"
		(layer "F.Cu")
		(at 157.7 74.7 180)
		(descr "THT pad as test Point, diameter 3.0mm, hole diameter 1.5mm")
		(tags "test point THT pad")
		(property "Reference" "TP3"
			(at 0 -2.5 0)
			(layer "F.Fab")
		)
		(property "Value" "VIO"
			(at 0 2.55 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Test point, plated through-hole, 65/100mil"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "CREATED_ON" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DATE" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DESCRIPTION" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ID" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "INVENTORY_PRICE" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTTYPE" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ROHS" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*TP-PTH-65/100*")
		(sheetname "/szg_interface/")
		(sheetfile "szg-interface.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 -2.4 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 180)
			(size 3 3)
			(drill 1.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 33 "VIO")
			(pinfunction "PIN")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 159.7 66.4 180)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R3"
			(at 0 1.2 0)
			(layer "F.Fab")
		)
		(property "Value" "60R"
			(at 0 1.17 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, small US symbol"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "CREATED_ON" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DATE" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DESCRIPTION" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ID" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "INVENTORY_PRICE" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTTYPE" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ROHS" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "szg-adapter.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 180)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 3 "+3.3V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 180)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 4 "Net-(D1-A)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 167.5 106.92 90)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C21"
			(at 0.22 1.2 90)
			(layer "F.Fab")
		)
		(property "Value" "0.001uF"
			(at 0 1.16 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Ceramic capacitor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "CREATED_ON" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DATE" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DESCRIPTION" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ID" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "INVENTORY_PRICE" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTTYPE" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ROHS" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/lvds_interface3/")
		(sheetfile "lvds-interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 90)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 3 "+3.3V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 90)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 128.18 102.6)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C6"
			(at 0 -1.16 0)
			(layer "F.Fab")
		)
		(property "Value" "0.1uF"
			(at 0 1.16 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Ceramic capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "CREATED_ON" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DATE" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DESCRIPTION" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ID" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "INVENTORY_PRICE" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTTYPE" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ROHS" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/lvds_interface/")
		(sheetfile "lvds-interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 3 "+3.3V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MountingHole:MountingHole_3.2mm_M3_Pad"
		(layer "F.Cu")
		(at 131.9 67.8)
		(descr "Mounting Hole 3.2mm, M3")
		(tags "mounting hole 3.2mm m3")
		(property "Reference" "MH2"
			(at 0 -4.2 0)
			(layer "F.Fab")
		)
		(property "Value" "MTG"
			(at 0 4.2 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Mounting hole"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "CREATED_ON" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DATE" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DESCRIPTION" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ID" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "INVENTORY_PRICE" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTTYPE" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ROHS" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*MTG-3.2/6.5-PTH*")
		(sheetname "/szg_interface/")
		(sheetfile "szg-interface.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 6.4 6.4)
			(drill 3.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 40 "unconnected-(MH2-Pad1)")
			(pinfunction "1")
			(pintype "passive+no_connect")
		)
		(embedded_fonts no)
	)
	(footprint "Package_SO:TSSOP-24_4.4x7.8mm_P0.65mm"
		(layer "F.Cu")
		(at 141.7 92.8875 -90)
		(descr "TSSOP, 24 Pin (JEDEC MO-153 variation AD, 1.00mm body thickness, https://www.jedec.org/document_search?search_api_views_fulltext=MO-153), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "TSSOP SO")
		(property "Reference" "U12"
			(at 0 -4.85 90)
			(layer "F.Fab")
		)
		(property "Value" "SN74LVC8T245"
			(at 0 4.85 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/sn74lvc8t245.pdf"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "8-Bit Dual-Supply Bus Transceiver With Configurable Voltage Translation and 3-State Outputs"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "CREATED_ON" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DATE" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DESCRIPTION" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ID" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "INVENTORY_PRICE" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTTYPE" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ROHS" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer" "Texas Instruments"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SSOP*5.3x8.2mm* SSOP*3.9x8.7mm* TSSOP*4.4x7.8mm* TVSOP*4.4x5.0mm* Texas*VQFN*RHL*")
		(sheetname "/voltage_translation2/")
		(sheetfile "voltage_translation.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -2.8625 -3.575 270)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 33 "VIO")
			(pinfunction "V_{CCA}")
			(pintype "power_in")
		)
		(pad "2" smd roundrect
			(at -2.8625 -2.925 270)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "DIR")
			(pintype "input")
		)
		(pad "3" smd roundrect
			(at -2.8625 -2.275 270)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 37 "/szg_interface/S15_D7N")
			(pinfunction "A1")
			(pintype "bidirectional")
		)
		(pad "4" smd roundrect
			(at -2.8625 -1.625 270)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 15 "/szg_interface/S14_D6N")
			(pinfunction "A2")
			(pintype "bidirectional")
		)
		(pad "5" smd roundrect
			(at -2.8625 -0.975 270)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 28 "/szg_interface/S13_D7P")
			(pinfunction "A3")
			(pintype "bidirectional")
		)
		(pad "6" smd roundrect
			(at -2.8625 -0.325 270)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 38 "/szg_interface/S12_D6P")
			(pinfunction "A4")
			(pintype "bidirectional")
		)
		(pad "7" smd roundrect
			(at -2.8625 0.325 270)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 36 "/szg_interface/S11_D5N")
			(pinfunction "A5")
			(pintype "bidirectional")
		)
		(pad "8" smd roundrect
			(at -2.8625 0.975 270)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 21 "/szg_interface/S10_D4N")
			(pinfunction "A6")
			(pintype "bidirectional")
		)
		(pad "9" smd roundrect
			(at -2.8625 1.625 270)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 29 "/szg_interface/S9_D5P")
			(pinfunction "A7")
			(pintype "bidirectional")
		)
		(pad "10" smd roundrect
			(at -2.8625 2.275 270)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 25 "/szg_interface/S8_D4P")
			(pinfunction "A8")
			(pintype "bidirectional")
		)
		(pad "11" smd roundrect
			(at -2.8625 2.925 270)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "12" smd roundrect
			(at -2.8625 3.575 270)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "13" smd roundrect
			(at 2.8625 3.575 270)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "14" smd roundrect
			(at 2.8625 2.925 270)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 49 "/lvds_interface/MISO2")
			(pinfunction "B8")
			(pintype "bidirectional")
		)
		(pad "15" smd roundrect
			(at 2.8625 2.275 270)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 44 "/lvds_interface/MISO1")
			(pinfunction "B7")
			(pintype "bidirectional")
		)
		(pad "16" smd roundrect
			(at 2.8625 1.625 270)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 55 "/lvds_interface1/MISO2")
			(pinfunction "B6")
			(pintype "bidirectional")
		)
		(pad "17" smd roundrect
			(at 2.8625 0.975 270)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 53 "/lvds_interface1/MISO1")
			(pinfunction "B5")
			(pintype "bidirectional")
		)
		(pad "18" smd roundrect
			(at 2.8625 0.325 270)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 61 "/lvds_interface2/MISO2")
			(pinfunction "B4")
			(pintype "bidirectional")
		)
		(pad "19" smd roundrect
			(at 2.8625 -0.325 270)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 56 "/lvds_interface2/MISO1")
			(pinfunction "B3")
			(pintype "bidirectional")
		)
		(pad "20" smd roundrect
			(at 2.8625 -0.975 270)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 67 "/lvds_interface3/MISO2")
			(pinfunction "B2")
			(pintype "bidirectional")
		)
		(pad "21" smd roundrect
			(at 2.8625 -1.625 270)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 65 "/lvds_interface3/MISO1")
			(pinfunction "B1")
			(pintype "bidirectional")
		)
		(pad "22" smd roundrect
			(at 2.8625 -2.275 270)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "~{OE}")
			(pintype "input")
		)
		(pad "23" smd roundrect
			(at 2.8625 -2.925 270)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 3 "+3.3V")
			(pinfunction "V_{CCB}")
			(pintype "power_in")
		)
		(pad "24" smd roundrect
			(at 2.8625 -3.575 270)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 3 "+3.3V")
			(pinfunction "V_{CCB}")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Package_SO.3dshapes/TSSOP-24_4.4x7.8mm_P0.65mm.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 156 128.5 90)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C26"
			(at 0 -1.16 90)
			(layer "F.Fab")
		)
		(property "Value" "0.1uF"
			(at 0 1.16 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Ceramic capacitor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "CREATED_ON" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DATE" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DESCRIPTION" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ID" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "INVENTORY_PRICE" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTTYPE" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ROHS" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/lvds_interface3/")
		(sheetfile "lvds-interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 90)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 90)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 138 "-5V")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_SMD:SOT-23-5"
		(layer "F.Cu")
		(at 150.8 106.1)
		(descr "SOT, 5 Pin (JEDEC MO-178 Var AA https://www.jedec.org/document_search?search_api_views_fulltext=MO-178), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOT TO_SOT_SMD")
		(property "Reference" "U7"
			(at 0 2.5 0)
			(layer "F.Fab")
		)
		(property "Value" "SN65LVDT2DBV"
			(at 0 2.4 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/sn65lvdt2.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "High-Speed Differential Line Receiver, 110 Ω Terminated, 630Mbps, SOT-23-5"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "CREATED_ON" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DATE" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DESCRIPTION" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ID" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "INVENTORY_PRICE" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTTYPE" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ROHS" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer" "Texas Instruments"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SOT?23*")
		(sheetname "/lvds_interface2/")
		(sheetfile "lvds-interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.1375 -0.95)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 3 "+3.3V")
			(pinfunction "V_{CC}")
			(pintype "power_in")
		)
		(pad "2" smd roundrect
			(at -1.1375 0)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "3" smd roundrect
			(at -1.1375 0.95)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 116 "/lvds_interface2/MISO2_P")
			(pinfunction "A")
			(pintype "input")
		)
		(pad "4" smd roundrect
			(at 1.1375 0.95)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 112 "/lvds_interface2/MISO2_N")
			(pinfunction "B")
			(pintype "input")
		)
		(pad "5" smd roundrect
			(at 1.1375 -0.95)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 61 "/lvds_interface2/MISO2")
			(pinfunction "R")
			(pintype "output")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_THTPad_D3.0mm_Drill1.5mm"
		(layer "F.Cu")
		(at 161.7 72.3)
		(descr "THT pad as test Point, diameter 3.0mm, hole diameter 1.5mm")
		(tags "test point THT pad")
		(property "Reference" "TP1"
			(at 0 -2.398 0)
			(layer "F.Fab")
		)
		(property "Value" "+3.3V"
			(at 0 2.55 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Test point, plated through-hole, 65/100mil"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "CREATED_ON" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DATE" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DESCRIPTION" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ID" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "INVENTORY_PRICE" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTTYPE" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ROHS" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*TP-PTH-65/100*")
		(sheetname "/szg_interface/")
		(sheetfile "szg-interface.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 -2.4 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 3 3)
			(drill 1.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "+3.3V")
			(pinfunction "PIN")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "Connector_PinHeader_1.27mm:PinHeader_2x05_P1.27mm_Vertical_SMD"
		(layer "F.Cu")
		(at 139.4 77.9 -90)
		(descr "surface-mounted straight pin header, 2x05, 1.27mm pitch, double rows")
		(tags "Surface mounted pin header SMD 2x05 1.27mm double row")
		(property "Reference" "J7"
			(at -4.2 -4.2 90)
			(layer "F.Fab")
		)
		(property "Value" "3220-10-0300-00"
			(at 0 4.285001 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://www.cnctech.us/pdfs/3220-XX-0300-00_.pdf"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Connector Header Surface Mount 10 position 0.050\" (1.27mm); Shrouded with partial opening on one side. Many equivalent parts also exist, such as the \"SWD 0.05\" Pitch Connector - 10 Pin SMT Box Header\" from Adafruit."
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "CREATED_ON" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DATE" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DESCRIPTION" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ID" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "INVENTORY_PRICE" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTTYPE" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ROHS" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer" "CNC Tech"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_2x??_*")
		(sheetname "/szg_interface/")
		(sheetfile "szg-interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.95 -2.54 270)
			(size 2.4 0.74)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 3 "+3.3V")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.95 -2.54 270)
			(size 2.4 0.74)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 144 "unconnected-(J7-Pin_2-Pad2)")
			(pinfunction "Pin_2")
			(pintype "passive+no_connect")
		)
		(pad "3" smd rect
			(at -1.95 -1.27 270)
			(size 2.4 0.74)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "GND")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" smd rect
			(at 1.95 -1.27 270)
			(size 2.4 0.74)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 8 "/szg_interface/MCU_SCL_USCK")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(pad "5" smd rect
			(at -1.95 0 270)
			(size 2.4 0.74)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "GND")
			(pinfunction "Pin_5")
			(pintype "passive")
		)
		(pad "6" smd rect
			(at 1.95 0 270)
			(size 2.4 0.74)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 6 "/szg_interface/MCU_MISO")
			(pinfunction "Pin_6")
			(pintype "passive")
		)
		(pad "7" smd rect
			(at -1.95 1.27 270)
			(size 2.4 0.74)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 146 "unconnected-(J7-Pin_7-Pad7)")
			(pinfunction "Pin_7")
			(pintype "passive+no_connect")
		)
		(pad "8" smd rect
			(at 1.95 1.27 270)
			(size 2.4 0.74)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 5 "/szg_interface/MCU_SDA_MOSI")
			(pinfunction "Pin_8")
			(pintype "passive")
		)
		(pad "9" smd rect
			(at -1.95 2.54 270)
			(size 2.4 0.74)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 145 "Net-(J7-Pin_9)")
			(pinfunction "Pin_9")
			(pintype "passive")
		)
		(pad "10" smd rect
			(at 1.95 2.54 270)
			(size 2.4 0.74)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 7 "/szg_interface/MCU_RESET_B")
			(pinfunction "Pin_10")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_PinHeader_1.27mm.3dshapes/PinHeader_2x05_P1.27mm_Vertical_SMD.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_SMD:SOT-23-5"
		(layer "F.Cu")
		(at 139.8 106.1)
		(descr "SOT, 5 Pin (JEDEC MO-178 Var AA https://www.jedec.org/document_search?search_api_views_fulltext=MO-178), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOT TO_SOT_SMD")
		(property "Reference" "U5"
			(at 0 2.4925 0)
			(layer "F.Fab")
		)
		(property "Value" "SN65LVDT2DBV"
			(at 0 2.4 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/sn65lvdt2.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "High-Speed Differential Line Receiver, 110 Ω Terminated, 630Mbps, SOT-23-5"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "CREATED_ON" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DATE" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DESCRIPTION" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ID" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "INVENTORY_PRICE" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTTYPE" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ROHS" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer" "Texas Instruments"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SOT?23*")
		(sheetname "/lvds_interface1/")
		(sheetfile "lvds-interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.1375 -0.95)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 3 "+3.3V")
			(pinfunction "V_{CC}")
			(pintype "power_in")
		)
		(pad "2" smd roundrect
			(at -1.1375 0)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "3" smd roundrect
			(at -1.1375 0.95)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 104 "/lvds_interface1/MISO2_P")
			(pinfunction "A")
			(pintype "input")
		)
		(pad "4" smd roundrect
			(at 1.1375 0.95)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 105 "/lvds_interface1/MISO2_N")
			(pinfunction "B")
			(pintype "input")
		)
		(pad "5" smd roundrect
			(at 1.1375 -0.95)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 55 "/lvds_interface1/MISO2")
			(pinfunction "R")
			(pintype "output")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MountingHole:MountingHole_3.2mm_M3_Pad"
		(layer "F.Cu")
		(at 131.4 125.8)
		(descr "Mounting Hole 3.2mm, M3")
		(tags "mounting hole 3.2mm m3")
		(property "Reference" "MH6"
			(at 0 -4.2 0)
			(layer "F.Fab")
		)
		(property "Value" "MTG"
			(at 0 4.2 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Mounting hole"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "CREATED_ON" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DATE" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DESCRIPTION" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ID" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "INVENTORY_PRICE" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTTYPE" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ROHS" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*MTG-3.2/6.5-PTH*")
		(sheetname "/szg_interface/")
		(sheetfile "szg-interface.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 6.4 6.4)
			(drill 3.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 69 "unconnected-(MH6-Pad1)")
			(pinfunction "1")
			(pintype "passive+no_connect")
		)
		(embedded_fonts no)
	)
	(footprint "Package_SO:TSSOP-24_4.4x7.8mm_P0.65mm"
		(layer "F.Cu")
		(at 151.8 92.875 -90)
		(descr "TSSOP, 24 Pin (JEDEC MO-153 variation AD, 1.00mm body thickness, https://www.jedec.org/document_search?search_api_views_fulltext=MO-153), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "TSSOP SO")
		(property "Reference" "U10"
			(at 0 -4.85 90)
			(layer "F.Fab")
		)
		(property "Value" "SN74LVC8T245"
			(at 0 4.85 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/sn74lvc8t245.pdf"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "8-Bit Dual-Supply Bus Transceiver With Configurable Voltage Translation and 3-State Outputs"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "CREATED_ON" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DATE" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DESCRIPTION" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ID" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "INVENTORY_PRICE" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTTYPE" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "ROHS" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer" "Texas Instruments"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SSOP*5.3x8.2mm* SSOP*3.9x8.7mm* TSSOP*4.4x7.8mm* TVSOP*4.4x5.0mm* Texas*VQFN*RHL*")
		(sheetname "/voltage_translation/")
		(sheetfile "voltage_translation.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -2.8625 -3.575 270)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 33 "VIO")
			(pinfunction "V_{CCA}")
			(pintype "power_in")
		)
		(pad "2" smd roundrect
			(at -2.8625 -2.925 270)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 33 "VIO")
			(pinfunction "DIR")
			(pintype "input")
		)
		(pad "3" smd roundrect
			(at -2.8625 -2.275 270)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 34 "/szg_interface/S23")
			(pinfunction "A1")
			(pintype "bidirectional")
		)
		(pad "4" smd roundrect
			(at -2.8625 -1.625 270)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 20 "/szg_interface/S22")
			(pinfunction "A2")
			(pintype "bidirectional")
		)
		(pad "5" smd roundrect
			(at -2.8625 -0.975 270)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 16 "/szg_interface/S21")
			(pinfunction "A3")
			(pintype "bidirectional")
		)
		(pad "6" smd roundrect
			(at -2.8625 -0.325 270)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 10 "/szg_interface/S20")
			(pinfunction "A4")
			(pintype "bidirectional")
		)
		(pad "7" smd roundrect
			(at -2.8625 0.325 270)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 23 "/szg_interface/S19")
			(pinfunction "A5")
			(pintype "bidirectional")
		)
		(pad "8" smd roundrect
			(at -2.8625 0.975 270)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 26 "/szg_interface/S18")
			(pinfunction "A6")
			(pintype "bidirectional")
		)
		(pad "9" smd roundrect
			(at -2.8625 1.625 270)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 18 "/szg_interface/S17")
			(pinfunction "A7")
			(pintype "bidirectional")
		)
		(pad "10" smd roundrect
			(at -2.8625 2.275 270)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 27 "/szg_interface/S16")
			(pinfunction "A8")
			(pintype "bidirectional")
		)
		(pad "11" smd roundrect
			(at -2.8625 2.925 270)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "12" smd roundrect
			(at -2.8625 3.575 270)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "13" smd roundrect
			(at 2.8625 3.575 270)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "14" smd roundrect
			(at 2.8625 2.925 270)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 58 "/lvds_interface2/CS")
			(pinfunction "B8")
			(pintype "bidirectional")
		)
		(pad "15" smd roundrect
			(at 2.8625 2.275 270)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 57 "/lvds_interface2/MOSI2")
			(pinfunction "B7")
			(pintype "bidirectional")
		)
		(pad "16" smd roundrect
			(at 2.8625 1.625 270)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 60 "/lvds_interface2/SCLK")
			(pinfunction "B6")
			(pintype "bidirectional")
		)
		(pad "17" smd roundrect
			(at 2.8625 0.975 270)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 59 "/lvds_interface2/MOSI1")
			(pinfunction "B5")
			(pintype "bidirectional")
		)
		(pad "18" smd roundrect
			(at 2.8625 0.325 270)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 66 "/lvds_interface3/CS")
			(pinfunction "B4")
			(pintype "bidirectional")
		)
		(pad "19" smd roundrect
			(at 2.8625 -0.325 270)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 63 "/lvds_interface3/MOSI2")
			(pinfunction "B3")
			(pintype "bidirectional")
		)
		(pad "20" smd roundrect
			(at 2.8625 -0.975 270)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 64 "/lvds_interface3/SCLK")
			(pinfunction "B2")
			(pintype "bidirectional")
		)
		(pad "21" smd roundrect
			(at 2.8625 -1.625 270)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 62 "/lvds_interface3/MOSI1")
			(pinfunction "B1")
			(pintype "bidirectional")
		)
		(pad "22" smd roundrect
			(at 2.8625 -2.275 270)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "~{OE}")
			(pintype "input")
		)
		(pad "23" smd roundrect
			(at 2.8625 -2.925 270)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 3 "+3.3V")
			(pinfunction "V_{CCB}")
			(pintype "power_in")
		)
		(pad "24" smd roundrect
			(at 2.8625 -3.575 270)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 3 "+3.3V")
			(pinfunction "V_{CCB}")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Package_SO.3dshapes/TSSOP-24_4.4x7.8mm_P0.65mm.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "B.Cu")
		(at 165.515001 84.05 180)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C34"
			(at 0 -1.6 0)
			(layer "B.SilkS")
		)
		(property "Value" "3.3uF"
			(at 0 -1.679999 0)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Ceramic capacitor"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "CREATED_ON" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "DATE" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "DESCRIPTION" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "ID" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "INVENTORY_PRICE" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "PARTTYPE" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "ROHS" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/power-management/")
		(sheetfile "power.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.949999 0 180)
			(size 1 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 136 "Net-(U13-VREF)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.949999 0 180)
			(size 1 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Jumper:SolderJumper-3_P1.3mm_Bridged12_RoundedPad1.0x1.5mm_NumberLabels"
		(layer "B.Cu")
		(at 161.4 93.5)
		(descr "SMD Solder 3-pad Jumper, 1x1.5mm rounded Pads, 0.3mm gap, pads 1-2 bridged with 1 copper strip, labeled with numbers")
		(tags "net tie solder jumper bridged")
		(property "Reference" "JP1"
			(at 0 1.8 0)
			(layer "B.SilkS")
		)
		(property "Value" "SolderJumper_3_Bridged12"
			(at 0 -1.9 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "3-pole Solder Jumper, pins 1+2 closed/bridged"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "CREATED_ON" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "DATE" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "DESCRIPTION" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "ID" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "INVENTORY_PRICE" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "PARTTYPE" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "ROHS" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SolderJumper*Bridged12*")
		(sheetname "/power-management/")
		(sheetfile "power.kicad_sch")
		(zone_connect 1)
		(attr exclude_from_pos_files exclude_from_bom allow_soldermask_bridges)
		(net_tie_pad_groups "1, 2")
		(fp_text user "3"
			(at 2.600001 0 0)
			(layer "B.SilkS")
		)
		(fp_text user "1"
			(at -2.600001 0 0)
			(layer "B.SilkS")
		)
		(pad "1" smd custom
			(at -1.3 0)
			(size 1 0.5)
			(layers "B.Cu" "B.Mask")
			(net 138 "-5V")
			(pinfunction "A")
			(pintype "passive")
			(zone_connect 2)
			(thermal_bridge_angle 45)
			(options
				(clearance outline)
				(anchor rect)
			)
			(primitives
				(gr_poly
					(pts
						(xy 0.55 -0.75) (xy 0 -0.75) (xy 0 0.75) (xy 0.55 0.75)
					)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center 0 -0.25)
					(end 0.5 -0.25)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center 0 0.25)
					(end 0.5 0.25)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "2" smd rect
			(at 0 0)
			(size 1 1.5)
			(layers "B.Cu" "B.Mask")
			(net 139 "Net-(JP1-C)")
			(pinfunction "C")
			(pintype "passive")
		)
		(pad "3" smd custom
			(at 1.3 0)
			(size 1 0.5)
			(layers "B.Cu" "B.Mask")
			(net 2 "GND")
			(pinfunction "B")
			(pintype "passive")
			(zone_connect 2)
			(thermal_bridge_angle 45)
			(options
				(clearance outline)
				(anchor rect)
			)
			(primitives
				(gr_circle
					(center 0 -0.25)
					(end 0.5 -0.25)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center 0 0.25)
					(end 0.5 0.25)
					(width 0)
					(fill yes)
				)
				(gr_poly
					(pts
						(xy 0 -0.75) (xy -0.55 -0.75) (xy -0.55 0.75) (xy 0 0.75)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(embedded_fonts no)
	)
	(footprint "Jumper:SolderJumper-2_P1.3mm_Open_RoundedPad1.0x1.5mm"
		(layer "B.Cu")
		(at 132.550001 72.9 180)
		(descr "SMD Solder Jumper, 1x1.5mm, rounded Pads, 0.3mm gap, open")
		(tags "solder jumper open")
		(property "Reference" "JP2"
			(at 0 1.8 0)
			(layer "B.Fab")
		)
		(property "Value" "SolderJumper_2_Open"
			(at 0 -1.9 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Solder Jumper, 2-pole, open"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "CREATED_ON" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "DATE" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "DESCRIPTION" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "ID" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "INVENTORY_PRICE" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "PARTTYPE" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "ROHS" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SolderJumper*Open*")
		(sheetname "/szg_interface/")
		(sheetfile "szg-interface.kicad_sch")
		(zone_connect 1)
		(attr exclude_from_pos_files exclude_from_bom allow_soldermask_bridges)
		(pad "1" smd custom
			(at -0.649999 0 180)
			(size 1 0.5)
			(layers "B.Cu" "B.Mask")
			(net 145 "Net-(J7-Pin_9)")
			(pinfunction "A")
			(pintype "passive")
			(zone_connect 2)
			(thermal_bridge_angle 45)
			(options
				(clearance outline)
				(anchor rect)
			)
			(primitives
				(gr_circle
					(center 0 -0.25)
					(end 0.5 -0.25)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center 0 0.25)
					(end 0.5 0.25)
					(width 0)
					(fill yes)
				)
				(gr_poly
					(pts
						(xy 0.5 -0.75) (xy 0 -0.75) (xy 0 0.75) (xy 0.5 0.75)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "2" smd custom
			(at 0.649999 0 180)
			(size 1 0.5)
			(layers "B.Cu" "B.Mask")
			(net 2 "GND")
			(pinfunction "B")
			(pintype "passive")
			(zone_connect 2)
			(thermal_bridge_angle 45)
			(options
				(clearance outline)
				(anchor rect)
			)
			(primitives
				(gr_circle
					(center 0 -0.25)
					(end 0.5 -0.25)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center 0 0.25)
					(end 0.5 0.25)
					(width 0)
					(fill yes)
				)
				(gr_poly
					(pts
						(xy 0 -0.75) (xy -0.5 -0.75) (xy -0.5 0.75) (xy 0 0.75)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(embedded_fonts no)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "B.Cu")
		(at 140.91 73.1)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R1"
			(at 1.99 0 0)
			(layer "B.Fab")
		)
		(property "Value" "10k"
			(at 0 -1.17 0)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Thick-film resistor"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "REVISION" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "DESCRIPTION 2" "SM-0402, 1%, 1/16W"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MANUFACTURER" "Vishay"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MANUFACTURER_PN" "CRCW040210K0FKED"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "PARTNUMBER" "001521"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "VALUEFLOAT" "10000"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "ALTIUM_VALUE" "10.0 k"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "TOLERANCE (%)" "1"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "UPDATED_ON" "3/21/2017 2:29:49 PM"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "X_LIFECYCLE_STATUS" "Production"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "CREATED_ON" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "DATE" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "DESCRIPTION" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "ID" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "INVENTORY_PRICE" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "PARTTYPE" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "ROHS" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*RESC1005X06N*")
		(sheetname "/szg_interface/")
		(sheetfile "szg-interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0)
			(size 0.54 0.64)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 1 "/szg_interface/R_GA")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0)
			(size 0.54 0.64)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 3 "+3.3V")
			(pinfunction "2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Mezzanine Connector:SAMTEC_QTE-020-01-X-D-A"
		(layer "B.Cu")
		(at 148.9 67.8)
		(property "Reference" "J1"
			(at 0 1.3 0)
			(layer "B.Fab")
		)
		(property "Value" "QTE-020-01-F-D-A"
			(at 4.355 -5.135 0)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "0.8mm hi-speed, high-density header (female)"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "REVISION" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "DATE" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "PARTNUMBER" "000973"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "CREATED_ON" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "DESCRIPTION" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "ID" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "INVENTORY_PRICE" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MANUFACTURER" "Samtec"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MANUFACTURER_PN" "QTE-020-01-F-D-A"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "PARTTYPE" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "ROHS" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "UPDATED_ON" "2/26/2018 2:13:14 PM"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer" "Samtec"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*QTE-020-01-X-D-A-L*")
		(sheetname "/szg_interface/")
		(sheetfile "szg-interface.kicad_sch")
		(attr smd)
		(pad "" np_thru_hole circle
			(at -9.24 2.04)
			(size 1.02 1.02)
			(drill 1.02)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 9.24 2.04)
			(size 1.02 1.02)
			(drill 1.02)
			(layers "*.Cu" "*.Mask")
		)
		(pad "0" smd rect
			(at -8.445 0)
			(size 2.54 0.64)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 2 "GND")
			(pinfunction "0")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "0" smd rect
			(at -3.175 0)
			(size 4.7 0.64)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 2 "GND")
			(pinfunction "0")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "0" smd rect
			(at 3.175 0)
			(size 4.7 0.64)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 2 "GND")
			(pinfunction "0")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "0" smd rect
			(at 8.445 0)
			(size 2.54 0.64)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 2 "GND")
			(pinfunction "0")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "1" smd rect
			(at -7.6 3.09)
			(size 0.46 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 8 "/szg_interface/MCU_SCL_USCK")
			(pinfunction "1")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd rect
			(at -7.6 -3.09)
			(size 0.46 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 43 "+5V")
			(pinfunction "2")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "3" smd rect
			(at -6.8 3.09)
			(size 0.46 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 5 "/szg_interface/MCU_SDA_MOSI")
			(pinfunction "3")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "4" smd rect
			(at -6.8 -3.09)
			(size 0.46 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 1 "/szg_interface/R_GA")
			(pinfunction "4")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "5" smd rect
			(at -6 3.09)
			(size 0.46 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 71 "/szg_interface/S0_D0P")
			(pinfunction "5")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "6" smd rect
			(at -6 -3.09)
			(size 0.46 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 72 "/szg_interface/S1_D1P")
			(pinfunction "6")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "7" smd rect
			(at -5.2 3.09)
			(size 0.46 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 74 "/szg_interface/S2_D0N")
			(pinfunction "7")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "8" smd rect
			(at -5.2 -3.09)
			(size 0.46 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 70 "/szg_interface/S3_D1N")
			(pinfunction "8")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "9" smd rect
			(at -4.4 3.09)
			(size 0.46 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 73 "/szg_interface/S4_D2P")
			(pinfunction "9")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "10" smd rect
			(at -4.4 -3.09)
			(size 0.46 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 12 "/szg_interface/S5_D3P")
			(pinfunction "10")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "11" smd rect
			(at -3.6 3.09)
			(size 0.46 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 9 "/szg_interface/S6_D2N")
			(pinfunction "11")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "12" smd rect
			(at -3.6 -3.09)
			(size 0.46 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 14 "/szg_interface/S7_D3N")
			(pinfunction "12")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "13" smd rect
			(at -2.8 3.09)
			(size 0.46 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 25 "/szg_interface/S8_D4P")
			(pinfunction "13")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "14" smd rect
			(at -2.8 -3.09)
			(size 0.46 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 29 "/szg_interface/S9_D5P")
			(pinfunction "14")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "15" smd rect
			(at -2 3.09)
			(size 0.46 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 21 "/szg_interface/S10_D4N")
			(pinfunction "15")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "16" smd rect
			(at -2 -3.09)
			(size 0.46 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 36 "/szg_interface/S11_D5N")
			(pinfunction "16")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "17" smd rect
			(at -1.2 3.09)
			(size 0.46 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 38 "/szg_interface/S12_D6P")
			(pinfunction "17")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "18" smd rect
			(at -1.2 -3.09)
			(size 0.46 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 28 "/szg_interface/S13_D7P")
			(pinfunction "18")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "19" smd rect
			(at -0.4 3.09)
			(size 0.46 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 15 "/szg_interface/S14_D6N")
			(pinfunction "19")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "20" smd rect
			(at -0.4 -3.09)
			(size 0.46 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 37 "/szg_interface/S15_D7N")
			(pinfunction "20")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "21" smd rect
			(at 0.4 3.09)
			(size 0.46 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 27 "/szg_interface/S16")
			(pinfunction "21")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "22" smd rect
			(at 0.4 -3.09)
			(size 0.46 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 18 "/szg_interface/S17")
			(pinfunction "22")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "23" smd rect
			(at 1.2 3.09)
			(size 0.46 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 26 "/szg_interface/S18")
			(pinfunction "23")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "24" smd rect
			(at 1.2 -3.09)
			(size 0.46 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 23 "/szg_interface/S19")
			(pinfunction "24")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "25" smd rect
			(at 2 3.09)
			(size 0.46 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 10 "/szg_interface/S20")
			(pinfunction "25")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "26" smd rect
			(at 2 -3.09)
			(size 0.46 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 16 "/szg_interface/S21")
			(pinfunction "26")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "27" smd rect
			(at 2.8 3.09)
			(size 0.46 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 20 "/szg_interface/S22")
			(pinfunction "27")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "28" smd rect
			(at 2.8 -3.09)
			(size 0.46 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 34 "/szg_interface/S23")
			(pinfunction "28")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "29" smd rect
			(at 3.6 3.09)
			(size 0.46 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 11 "/szg_interface/S24")
			(pinfunction "29")
			(pintype "passive+no_connect")
			(solder_mask_margin 0.102)
		)
		(pad "30" smd rect
			(at 3.6 -3.09)
			(size 0.46 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 24 "/szg_interface/S25")
			(pinfunction "30")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "31" smd rect
			(at 4.4 3.09)
			(size 0.46 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 32 "/szg_interface/S26")
			(pinfunction "31")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "32" smd rect
			(at 4.4 -3.09)
			(size 0.46 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 19 "/szg_interface/S27")
			(pinfunction "32")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "33" smd rect
			(at 5.2 3.09)
			(size 0.46 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 35 "/szg_interface/P2C_CLKP")
			(pinfunction "33")
			(pintype "passive+no_connect")
			(solder_mask_margin 0.102)
		)
		(pad "34" smd rect
			(at 5.2 -3.09)
			(size 0.46 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 22 "/szg_interface/C2P_CLKP")
			(pinfunction "34")
			(pintype "passive+no_connect")
			(solder_mask_margin 0.102)
		)
		(pad "35" smd rect
			(at 6 3.09)
			(size 0.46 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 13 "/szg_interface/P2C_CLKN")
			(pinfunction "35")
			(pintype "passive+no_connect")
			(solder_mask_margin 0.102)
		)
		(pad "36" smd rect
			(at 6 -3.09)
			(size 0.46 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 17 "/szg_interface/C2P_CLKN")
			(pinfunction "36")
			(pintype "passive+no_connect")
			(solder_mask_margin 0.102)
		)
		(pad "37" smd rect
			(at 6.8 3.09)
			(size 0.46 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 31 "/szg_interface/RSVD_37")
			(pinfunction "37")
			(pintype "passive+no_connect")
			(solder_mask_margin 0.102)
		)
		(pad "38" smd rect
			(at 6.8 -3.09)
			(size 0.46 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 30 "/szg_interface/RSVD_38")
			(pinfunction "38")
			(pintype "passive+no_connect")
			(solder_mask_margin 0.102)
		)
		(pad "39" smd rect
			(at 7.6 3.09)
			(size 0.46 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 33 "VIO")
			(pinfunction "39")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "40" smd rect
			(at 7.6 -3.09)
			(size 0.46 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 3 "+3.3V")
			(pinfunction "40")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
	)
	(footprint "Package_DFN_QFN:QFN-20-1EP_4x4mm_P0.5mm_EP2.6x2.6mm"
		(layer "B.Cu")
		(at 139.4 77.925 -90)
		(descr "QFN, 20 Pin (http://ww1.microchip.com/downloads/en/DeviceDoc/doc2535.pdf#page=164), generated with kicad-footprint-generator ipc_noLead_generator.py")
		(tags "QFN NoLead")
		(property "Reference" "U1"
			(at 0 3.3 90)
			(layer "B.Fab")
		)
		(property "Value" "ATtiny44A-M"
			(at 0 -3.3 90)
			(layer "B.Fab")
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/doc8183.pdf"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "20MHz, 4kB Flash, 256B SRAM, 256B EEPROM, debugWIRE, QFN-20"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "CREATED_ON" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "DATE" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "DESCRIPTION" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "ID" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "INVENTORY_PRICE" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "PARTTYPE" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "ROHS" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer" "Microchip Technology"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "QFN*1EP*4x4mm*P0.5mm*")
		(sheetname "/szg_interface/")
		(sheetfile "szg-interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "" smd roundrect
			(at -0.65 -0.65 270)
			(size 1.05 1.05)
			(layers "B.Paste")
			(roundrect_rratio 0.238095)
		)
		(pad "" smd roundrect
			(at -0.65 0.65 270)
			(size 1.05 1.05)
			(layers "B.Paste")
			(roundrect_rratio 0.238095)
		)
		(pad "" smd roundrect
			(at 0.65 -0.65 270)
			(size 1.05 1.05)
			(layers "B.Paste")
			(roundrect_rratio 0.238095)
		)
		(pad "" smd roundrect
			(at 0.65 0.65 270)
			(size 1.05 1.05)
			(layers "B.Paste")
			(roundrect_rratio 0.238095)
		)
		(pad "1" smd roundrect
			(at -1.925 1 270)
			(size 0.85 0.25)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 8 "/szg_interface/MCU_SCL_USCK")
			(pinfunction "PA4")
			(pintype "bidirectional")
		)
		(pad "2" smd roundrect
			(at -1.925 0.5 270)
			(size 0.85 0.25)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 80 "unconnected-(U1-PA3-Pad2)")
			(pinfunction "PA3")
			(pintype "bidirectional+no_connect")
		)
		(pad "3" smd roundrect
			(at -1.925 0 270)
			(size 0.85 0.25)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 75 "unconnected-(U1-PA2-Pad3)")
			(pinfunction "PA2")
			(pintype "bidirectional+no_connect")
		)
		(pad "4" smd roundrect
			(at -1.925 -0.5 270)
			(size 0.85 0.25)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 76 "unconnected-(U1-PA1-Pad4)")
			(pinfunction "PA1")
			(pintype "bidirectional+no_connect")
		)
		(pad "5" smd roundrect
			(at -1.925 -1 270)
			(size 0.85 0.25)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 1 "/szg_interface/R_GA")
			(pinfunction "AREF/PA0")
			(pintype "bidirectional")
		)
		(pad "6" smd roundrect
			(at -1 -1.925 270)
			(size 0.25 0.85)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 81 "unconnected-(U1-NC-Pad6)")
			(pinfunction "NC")
			(pintype "no_connect")
		)
		(pad "7" smd roundrect
			(at -0.5 -1.925 270)
			(size 0.25 0.85)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 86 "unconnected-(U1-NC-Pad7)")
			(pinfunction "NC")
			(pintype "no_connect")
		)
		(pad "8" smd roundrect
			(at 0 -1.925 270)
			(size 0.25 0.85)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "9" smd roundrect
			(at 0.5 -1.925 270)
			(size 0.25 0.85)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 3 "+3.3V")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(pad "10" smd roundrect
			(at 1 -1.925 270)
			(size 0.25 0.85)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 79 "unconnected-(U1-NC-Pad10)")
			(pinfunction "NC")
			(pintype "no_connect")
		)
		(pad "11" smd roundrect
			(at 1.925 -1 270)
			(size 0.85 0.25)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 83 "unconnected-(U1-XTAL1{slash}PB0-Pad11)")
			(pinfunction "XTAL1/PB0")
			(pintype "bidirectional+no_connect")
		)
		(pad "12" smd roundrect
			(at 1.925 -0.5 270)
			(size 0.85 0.25)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 78 "unconnected-(U1-XTAL2{slash}PB1-Pad12)")
			(pinfunction "XTAL2/PB1")
			(pintype "bidirectional+no_connect")
		)
		(pad "13" smd roundrect
			(at 1.925 0 270)
			(size 0.85 0.25)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 7 "/szg_interface/MCU_RESET_B")
			(pinfunction "~{RESET}/PB3")
			(pintype "bidirectional")
		)
		(pad "14" smd roundrect
			(at 1.925 0.5 270)
			(size 0.85 0.25)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 85 "unconnected-(U1-PB2-Pad14)")
			(pinfunction "PB2")
			(pintype "bidirectional+no_connect")
		)
		(pad "15" smd roundrect
			(at 1.925 1 270)
			(size 0.85 0.25)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 77 "unconnected-(U1-PA7-Pad15)")
			(pinfunction "PA7")
			(pintype "bidirectional+no_connect")
		)
		(pad "16" smd roundrect
			(at 1 1.925 270)
			(size 0.25 0.85)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 5 "/szg_interface/MCU_SDA_MOSI")
			(pinfunction "PA6")
			(pintype "bidirectional")
		)
		(pad "17" smd roundrect
			(at 0.5 1.925 270)
			(size 0.25 0.85)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 84 "unconnected-(U1-NC-Pad17)")
			(pinfunction "NC")
			(pintype "no_connect")
		)
		(pad "18" smd roundrect
			(at 0 1.925 270)
			(size 0.25 0.85)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 87 "unconnected-(U1-NC-Pad18)")
			(pinfunction "NC")
			(pintype "no_connect")
		)
		(pad "19" smd roundrect
			(at -0.5 1.925 270)
			(size 0.25 0.85)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 82 "unconnected-(U1-NC-Pad19)")
			(pinfunction "NC")
			(pintype "no_connect")
		)
		(pad "20" smd roundrect
			(at -1 1.925 270)
			(size 0.25 0.85)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 6 "/szg_interface/MCU_MISO")
			(pinfunction "PA5")
			(pintype "bidirectional")
		)
		(pad "21" smd rect
			(at 0 0 270)
			(size 2.6 2.6)
			(property pad_prop_heatsink)
			(layers "B.Cu" "B.Mask")
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "passive")
			(zone_connect 2)
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Package_DFN_QFN.3dshapes/QFN-20-1EP_4x4mm_P0.5mm_EP2.6x2.6mm.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "B.Cu")
		(at 140.9 74.5 180)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C2"
			(at -2 0 0)
			(layer "B.Fab")
		)
		(property "Value" "0.1uF"
			(at 0 -1.16 0)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Ceramic capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "REVISION" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "DESCRIPTION 2" "SM-0402, 10%, 10v"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MANUFACTURER" "Kemet"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MANUFACTURER_PN" "C0402C104K8PACTU"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "PARTNUMBER" "000070"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "VALUEFLOAT" "1E-7"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "ALTIUM_VALUE" "0.1 u"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "TOLERANCE (%)" "10"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "UPDATED_ON" "5/15/2017 4:50:04 PM"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "CREATED_ON" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "DATE" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "DESCRIPTION" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "ID" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "INVENTORY_PRICE" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "PARTTYPE" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "ROHS" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*CAPC1005X06N*")
		(sheetname "/szg_interface/")
		(sheetfile "szg-interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 180)
			(size 0.56 0.62)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 180)
			(size 0.56 0.62)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 1 "/szg_interface/R_GA")
			(pinfunction "2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "B.Cu")
		(at 139.89 81.3)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R2"
			(at 0 1.17 0)
			(layer "B.Fab")
		)
		(property "Value" "10k"
			(at 0 -1.17 0)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Thick-film resistor"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "REVISION" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "DESCRIPTION 2" "SM-0402, 1%, 1/16W"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MANUFACTURER" "Vishay"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MANUFACTURER_PN" "CRCW040210K0FKED"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "PARTNUMBER" "001521"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "VALUEFLOAT" "10000"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "ALTIUM_VALUE" "10.0 k"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "TOLERANCE (%)" "1"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "UPDATED_ON" "3/21/2017 2:29:49 PM"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "X_LIFECYCLE_STATUS" "Production"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "CREATED_ON" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "DATE" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "DESCRIPTION" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "ID" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "INVENTORY_PRICE" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "PARTTYPE" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "ROHS" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*RESC1005X06N*")
		(sheetname "/szg_interface/")
		(sheetfile "szg-interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0)
			(size 0.54 0.64)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 7 "/szg_interface/MCU_RESET_B")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0)
			(size 0.54 0.64)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 3 "+3.3V")
			(pinfunction "2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "B.Cu")
		(at 142.9 78.1 -90)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C1"
			(at 0 -1.3 90)
			(layer "B.Fab")
		)
		(property "Value" "0.1uF"
			(at 0 -1.16 90)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Ceramic capacitor"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "REVISION" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "DESCRIPTION 2" "SM-0402, 10%, 10v"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MANUFACTURER" "Kemet"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MANUFACTURER_PN" "C0402C104K8PACTU"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "PARTNUMBER" "000070"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "VALUEFLOAT" "1E-7"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "ALTIUM_VALUE" "0.1 u"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "TOLERANCE (%)" "10"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "UPDATED_ON" "11/17/2016 12:16:56 PM"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "CREATED_ON" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "DATE" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "DESCRIPTION" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "ID" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "INVENTORY_PRICE" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "PARTTYPE" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "ROHS" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*CAPC1005X06N*")
		(sheetname "/szg_interface/")
		(sheetfile "szg-interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 270)
			(size 0.56 0.62)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 270)
			(size 0.56 0.62)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 3 "+3.3V")
			(pinfunction "2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(gr_line
		(start 126.4 130.8)
		(end 171.4 130.8)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 171.4 60.8)
		(end 126.4 60.8)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 171.4 60.8)
		(end 171.4 130.8)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 126.4 60.8)
		(end 126.4 130.8)
		(layer "Edge.Cuts")
	)
	(gr_text "v2"
		(at 154.7 71.6 0)
		(layer "F.SilkS")
	)
	(gr_text "3"
		(at 151.9 123.4 0)
		(layer "F.SilkS")
	)
	(gr_text "4"
		(at 158.85 123.4 0)
		(layer "F.SilkS")
	)
	(gr_text "1"
		(at 137.9 123.4 0)
		(layer "F.SilkS")
	)
	(gr_text "2"
		(at 144.9 123.4 0)
		(layer "F.SilkS")
	)
	(zone
		(net 2)
		(net_name "GND")
		(layers "F.Cu" "B.Cu")
		(hatch edge 0.5)
		(priority 2)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 171.4 60.8) (xy 171.4 130.8) (xy 126.4 130.8) (xy 126.4 60.8)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layers "F.Cu" "B.Cu" "In1.Cu" "In2.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(keepout
			(tracks allowed)
			(vias allowed)
			(pads not_allowed)
			(copperpour not_allowed)
			(footprints allowed)
		)
		(placement
			(enabled no)
			(sheetname "")
		)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 168.4 92) (xy 160.7 92) (xy 160.7 85.5) (xy 168.4 85.5)
			)
		)
	)
	(zone
		(net 3)
		(net_name "+3.3V")
		(layer "In1.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 126.4 60.8) (xy 171.4 60.8) (xy 171.4 130.8) (xy 126.4 130.8)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "In2.Cu")
		(hatch edge 0.5)
		(priority 1)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 126.4 60.8) (xy 171.4 60.8) (xy 171.4 130.8) (xy 126.4 130.8)
			)
		)
	)
	(embedded_fonts no)
)
