(kicad_pcb
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(general
		(thickness 1.6)
		(legacy_teardrops no)
	)
	(paper "A4")
	(layers
		(0 "F.Cu" signal)
		(2 "B.Cu" signal)
		(9 "F.Adhes" user "F.Adhesive")
		(11 "B.Adhes" user "B.Adhesive")
		(13 "F.Paste" user)
		(15 "B.Paste" user)
		(5 "F.SilkS" user "F.Silkscreen")
		(7 "B.SilkS" user "B.Silkscreen")
		(1 "F.Mask" user)
		(3 "B.Mask" user)
		(17 "Dwgs.User" user "User.Drawings")
		(19 "Cmts.User" user "User.Comments")
		(21 "Eco1.User" user "User.Eco1")
		(23 "Eco2.User" user "User.Eco2")
		(25 "Edge.Cuts" user)
		(27 "Margin" user)
		(31 "F.CrtYd" user "F.Courtyard")
		(29 "B.CrtYd" user "B.Courtyard")
		(35 "F.Fab" user)
		(33 "B.Fab" user)
		(39 "User.1" user)
		(41 "User.2" user)
		(43 "User.3" user)
		(45 "User.4" user)
	)
	(setup
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(tenting front back)
		(pcbplotparams
			(layerselection 0x00000000_00000000_55555555_5755f5ff)
			(plot_on_all_layers_selection 0x00000000_00000000_00000000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 4)
			(plotframeref no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(pdf_metadata yes)
			(pdf_single_document no)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plot_black_and_white yes)
			(sketchpadsonfab no)
			(plotpadnumbers no)
			(hidednponfab no)
			(sketchdnponfab yes)
			(crossoutdnponfab yes)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 1)
			(scaleselection 1)
			(outputdirectory "")
		)
	)
	(net 0 "")
	(net 1 "/CAN0_H")
	(net 2 "GND")
	(net 3 "/CAN0_L")
	(net 4 "/CAN1_L")
	(net 5 "/CAN1_H")
	(net 6 "/CAN2_L")
	(net 7 "/CAN2_H")
	(net 8 "/CAN3_H")
	(net 9 "/CAN3_L")
	(net 10 "unconnected-(J5-Pin_2-Pad2)")
	(net 11 "unconnected-(J5-Pin_1-Pad1)")
	(net 12 "unconnected-(J6-Pin_2-Pad2)")
	(net 13 "unconnected-(J6-Pin_1-Pad1)")
	(net 14 "unconnected-(J7-Pin_2-Pad2)")
	(net 15 "unconnected-(J7-Pin_1-Pad1)")
	(net 16 "unconnected-(J8-Pin_1-Pad1)")
	(net 17 "unconnected-(J8-Pin_2-Pad2)")
	(net 18 "Net-(LED1-K)")
	(net 19 "Net-(LED1-A)")
	(net 20 "Net-(LED2-K)")
	(net 21 "Net-(LED3-K)")
	(net 22 "Net-(LED5-A)")
	(net 23 "Net-(LED5-K)")
	(net 24 "Net-(LED6-K)")
	(net 25 "Net-(LED7-K)")
	(net 26 "Net-(LED9-A)")
	(net 27 "Net-(LED10-A)")
	(net 28 "Net-(LED10-K)")
	(net 29 "Net-(LED11-K)")
	(net 30 "Net-(LED13-A)")
	(net 31 "Net-(LED13-K)")
	(net 32 "Net-(LED14-K)")
	(net 33 "Net-(LED15-K)")
	(net 34 "CAN0_+12V")
	(net 35 "CAN1_+12V")
	(net 36 "CAN2_+12V")
	(net 37 "CAN3_+12V")
	(footprint "PCM_LED_SMD_AKL:LED_0603_1608Metric"
		(layer "F.Cu")
		(at 107.505 99.75 -90)
		(descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
		(tags "LED")
		(property "Reference" "LED3"
			(at 0 -1.83 90)
			(layer "F.SilkS")
		)
		(property "Value" "LED_0603_Yellow"
			(at 0 1.43 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.mouser.com/datasheet/3/281/1/LTST_C190KSKT.pdf"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Yellow SMD LED, 0603, Alternate KiCad Library"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "LED* LED_SMD:* LED_THT:*")
		(sheetname "/")
		(sheetfile "RAD_Compute_CAN_Breakout.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -0.75 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.7875 0 270)
			(size 0.875 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 21 "Net-(LED3-K)")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.7875 0 270)
			(size 0.875 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 20 "Net-(LED2-K)")
			(pinfunction "A")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "PCM_Resistor_SMD_AKL:R_0603_1608Metric"
		(layer "F.Cu")
		(at 138.665 95.64 -90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), Alternate KiCad Library")
		(tags "resistor")
		(property "Reference" "R2"
			(at 0 -1.5 90)
			(layer "F.SilkS")
		)
		(property "Value" "120"
			(at 0 1.43 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "SMD 0603 Chip Resistor, US Symbol, Alternate KiCad Library"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "RAD_Compute_CAN_Breakout.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 270)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 35 "CAN1_+12V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0 270)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 22 "Net-(LED5-A)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "PCM_LED_SMD_AKL:LED_0603_1608Metric"
		(layer "F.Cu")
		(at 149.385 99.75 -90)
		(descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
		(tags "LED")
		(property "Reference" "LED11"
			(at 0 -1.83 90)
			(layer "F.SilkS")
		)
		(property "Value" "LED_0603_Yellow"
			(at 0 1.43 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.mouser.com/datasheet/3/281/1/LTST_C190KSKT.pdf"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Yellow SMD LED, 0603, Alternate KiCad Library"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "LED* LED_SMD:* LED_THT:*")
		(sheetname "/")
		(sheetfile "RAD_Compute_CAN_Breakout.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -0.75 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.7875 0 270)
			(size 0.875 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 29 "Net-(LED11-K)")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.7875 0 270)
			(size 0.875 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 28 "Net-(LED10-K)")
			(pinfunction "A")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "PCM_Resistor_SMD_AKL:R_0603_1608Metric"
		(layer "F.Cu")
		(at 180.545 95.64 -90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), Alternate KiCad Library")
		(tags "resistor")
		(property "Reference" "R4"
			(at 0 -1.5 90)
			(layer "F.SilkS")
		)
		(property "Value" "120"
			(at 0 1.43 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "SMD 0603 Chip Resistor, US Symbol, Alternate KiCad Library"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "RAD_Compute_CAN_Breakout.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 270)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 37 "CAN3_+12V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0 270)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 30 "Net-(LED13-A)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "PCM_LED_SMD_AKL:LED_0603_1608Metric"
		(layer "F.Cu")
		(at 128.445 99.75 -90)
		(descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
		(tags "LED")
		(property "Reference" "LED7"
			(at 0 -1.83 90)
			(layer "F.SilkS")
		)
		(property "Value" "LED_0603_Yellow"
			(at 0 1.43 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.mouser.com/datasheet/3/281/1/LTST_C190KSKT.pdf"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Yellow SMD LED, 0603, Alternate KiCad Library"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "LED* LED_SMD:* LED_THT:*")
		(sheetname "/")
		(sheetfile "RAD_Compute_CAN_Breakout.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -0.75 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.7875 0 270)
			(size 0.875 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 25 "Net-(LED7-K)")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.7875 0 270)
			(size 0.875 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 24 "Net-(LED6-K)")
			(pinfunction "A")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Library:Molex_Nano-Fit_105312-xx04_2x02_P2.50mm_Vertical"
		(layer "F.Cu")
		(at 134.695 99.48 -90)
		(descr "Molex Nano-Fit Power Connectors, 105310-xx04, 2 Pins per row (http://www.molex.com/pdm_docs/sd/1053101208_sd.pdf), generated with kicad-footprint-generator")
		(tags "connector Molex Nano-Fit side entry")
		(property "Reference" "J2"
			(at 1.25 -2.92 270)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_02x02_Odd_Even"
			(at 1.25 5.42 270)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, double row, 02x02, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_2x??_*")
		(sheetname "/")
		(sheetfile "RAD_Compute_CAN_Breakout.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 3.54 1.25 0)
			(layer "F.Fab")
		)
		(pad "" thru_hole circle
			(at 0.29 -2.17 270)
			(size 2 2)
			(drill 1.6)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "" thru_hole circle
			(at 0.29 4.67 270)
			(size 2 2)
			(drill 1.6)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "1" thru_hole custom
			(at 0 0 270)
			(size 1.417157 1.417157)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 35 "CAN1_+12V")
			(pinfunction "Pin_1")
			(pintype "passive")
			(thermal_bridge_angle 90)
			(options
				(clearance outline)
				(anchor circle)
			)
			(primitives
				(gr_poly
					(pts
						(xy 0.6 0.6) (xy -0.2 0.6) (xy -0.6 0.2) (xy -0.6 -0.6) (xy 0.6 -0.6)
					)
					(width 0.5)
					(fill yes)
				)
			)
		)
		(pad "2" thru_hole circle
			(at 0 2.5 270)
			(size 1.7 1.7)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "/CAN1_H")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole circle
			(at 2.5 0 270)
			(size 1.7 1.7)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole circle
			(at 2.5 2.5 270)
			(size 1.7 1.7)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "/CAN1_L")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KIPRJMOD}/Library.pretty/105312-2204/3D/105312-2204.stp"
			(offset
				(xyz 1.25 -1.25 4.8)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -0 -0 -90)
			)
		)
	)
	(footprint "Library:Molex_Nano-Fit_105312-xx04_2x02_P2.50mm_Vertical"
		(layer "F.Cu")
		(at 155.635 99.48 -90)
		(descr "Molex Nano-Fit Power Connectors, 105310-xx04, 2 Pins per row (http://www.molex.com/pdm_docs/sd/1053101208_sd.pdf), generated with kicad-footprint-generator")
		(tags "connector Molex Nano-Fit side entry")
		(property "Reference" "J3"
			(at 1.25 -2.92 90)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_02x02_Odd_Even"
			(at 1.25 5.42 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, double row, 02x02, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_2x??_*")
		(sheetname "/")
		(sheetfile "RAD_Compute_CAN_Breakout.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 3.54 1.25 0)
			(layer "F.Fab")
		)
		(pad "" thru_hole circle
			(at 0.29 -2.17 270)
			(size 2 2)
			(drill 1.6)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "" thru_hole circle
			(at 0.29 4.67 270)
			(size 2 2)
			(drill 1.6)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "1" thru_hole custom
			(at 0 0 270)
			(size 1.417157 1.417157)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 36 "CAN2_+12V")
			(pinfunction "Pin_1")
			(pintype "passive")
			(thermal_bridge_angle 90)
			(options
				(clearance outline)
				(anchor circle)
			)
			(primitives
				(gr_poly
					(pts
						(xy 0.6 0.6) (xy -0.2 0.6) (xy -0.6 0.2) (xy -0.6 -0.6) (xy 0.6 -0.6)
					)
					(width 0.5)
					(fill yes)
				)
			)
		)
		(pad "2" thru_hole circle
			(at 0 2.5 270)
			(size 1.7 1.7)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 7 "/CAN2_H")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole circle
			(at 2.5 0 270)
			(size 1.7 1.7)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole circle
			(at 2.5 2.5 270)
			(size 1.7 1.7)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "/CAN2_L")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KIPRJMOD}/Library.pretty/105312-2204/3D/105312-2204.stp"
			(offset
				(xyz 1.25 -1.25 4.8)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -0 -0 -90)
			)
		)
	)
	(footprint "PCM_LED_SMD_AKL:LED_0603_1608Metric"
		(layer "F.Cu")
		(at 154.385 95.25 180)
		(descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
		(tags "LED")
		(property "Reference" "LED12"
			(at 0 -1.83 0)
			(layer "F.SilkS")
		)
		(property "Value" "LED_0603_Yellow"
			(at 0 1.43 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.mouser.com/datasheet/3/281/1/LTST_C190KSKT.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Yellow SMD LED, 0603, Alternate KiCad Library"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "LED* LED_SMD:* LED_THT:*")
		(sheetname "/")
		(sheetfile "RAD_Compute_CAN_Breakout.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -0.75 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.7875 0 180)
			(size 0.875 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.7875 0 180)
			(size 0.875 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 29 "Net-(LED11-K)")
			(pinfunction "A")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Library:Molex_Nano-Fit_105312-xx04_2x02_P2.50mm_Vertical"
		(layer "F.Cu")
		(at 176.575 99.48 -90)
		(descr "Molex Nano-Fit Power Connectors, 105310-xx04, 2 Pins per row (http://www.molex.com/pdm_docs/sd/1053101208_sd.pdf), generated with kicad-footprint-generator")
		(tags "connector Molex Nano-Fit side entry")
		(property "Reference" "J4"
			(at 1.25 -2.92 90)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_02x02_Odd_Even"
			(at 1.25 5.42 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, double row, 02x02, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_2x??_*")
		(sheetname "/")
		(sheetfile "RAD_Compute_CAN_Breakout.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 3.54 1.25 0)
			(layer "F.Fab")
		)
		(pad "" thru_hole circle
			(at 0.29 -2.17 270)
			(size 2 2)
			(drill 1.6)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "" thru_hole circle
			(at 0.29 4.67 270)
			(size 2 2)
			(drill 1.6)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "1" thru_hole custom
			(at 0 0 270)
			(size 1.417157 1.417157)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 37 "CAN3_+12V")
			(pinfunction "Pin_1")
			(pintype "passive")
			(thermal_bridge_angle 90)
			(options
				(clearance outline)
				(anchor circle)
			)
			(primitives
				(gr_poly
					(pts
						(xy 0.6 0.6) (xy -0.2 0.6) (xy -0.6 0.2) (xy -0.6 -0.6) (xy 0.6 -0.6)
					)
					(width 0.5)
					(fill yes)
				)
			)
		)
		(pad "2" thru_hole circle
			(at 0 2.5 270)
			(size 1.7 1.7)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 8 "/CAN3_H")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole circle
			(at 2.5 0 270)
			(size 1.7 1.7)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole circle
			(at 2.5 2.5 270)
			(size 1.7 1.7)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 9 "/CAN3_L")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KIPRJMOD}/Library.pretty/105312-2204/3D/105312-2204.stp"
			(offset
				(xyz 1.25 -1.25 4.8)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -0 -0 -90)
			)
		)
	)
	(footprint "PCM_LED_SMD_AKL:LED_0603_1608Metric"
		(layer "F.Cu")
		(at 138.445 99.75 90)
		(descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
		(tags "LED")
		(property "Reference" "LED5"
			(at 0 -1.83 90)
			(layer "F.SilkS")
		)
		(property "Value" "LED_0603_Yellow"
			(at 0 1.43 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.mouser.com/datasheet/3/281/1/LTST_C190KSKT.pdf"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Yellow SMD LED, 0603, Alternate KiCad Library"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "LED* LED_SMD:* LED_THT:*")
		(sheetname "/")
		(sheetfile "RAD_Compute_CAN_Breakout.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -0.75 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.7875 0 90)
			(size 0.875 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 23 "Net-(LED5-K)")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.7875 0 90)
			(size 0.875 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 22 "Net-(LED5-A)")
			(pinfunction "A")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "PCM_Resistor_SMD_AKL:R_0603_1608Metric"
		(layer "F.Cu")
		(at 117.725 95.64 -90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), Alternate KiCad Library")
		(tags "resistor")
		(property "Reference" "R1"
			(at 0 -1.5 90)
			(layer "F.SilkS")
		)
		(property "Value" "120"
			(at 0 1.43 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "SMD 0603 Chip Resistor, US Symbol, Alternate KiCad Library"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "RAD_Compute_CAN_Breakout.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 270)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 34 "CAN0_+12V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0 270)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 19 "Net-(LED1-A)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "PCM_LED_SMD_AKL:LED_0603_1608Metric"
		(layer "F.Cu")
		(at 133.445 104.5)
		(descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
		(tags "LED")
		(property "Reference" "LED6"
			(at 0 -1.83 0)
			(layer "F.SilkS")
		)
		(property "Value" "LED_0603_Yellow"
			(at 0 1.43 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.mouser.com/datasheet/3/281/1/LTST_C190KSKT.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Yellow SMD LED, 0603, Alternate KiCad Library"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "LED* LED_SMD:* LED_THT:*")
		(sheetname "/")
		(sheetfile "RAD_Compute_CAN_Breakout.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -0.75 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.7875 0)
			(size 0.875 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 24 "Net-(LED6-K)")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.7875 0)
			(size 0.875 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 23 "Net-(LED5-K)")
			(pinfunction "A")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "PCM_LED_SMD_AKL:LED_0603_1608Metric"
		(layer "F.Cu")
		(at 154.385 104.5)
		(descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
		(tags "LED")
		(property "Reference" "LED10"
			(at 0 -1.83 0)
			(layer "F.SilkS")
		)
		(property "Value" "LED_0603_Yellow"
			(at 0 1.43 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.mouser.com/datasheet/3/281/1/LTST_C190KSKT.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Yellow SMD LED, 0603, Alternate KiCad Library"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "LED* LED_SMD:* LED_THT:*")
		(sheetname "/")
		(sheetfile "RAD_Compute_CAN_Breakout.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -0.75 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.7875 0)
			(size 0.875 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 28 "Net-(LED10-K)")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.7875 0)
			(size 0.875 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 27 "Net-(LED10-A)")
			(pinfunction "A")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "PCM_LED_SMD_AKL:LED_0603_1608Metric"
		(layer "F.Cu")
		(at 180.325 99.75 90)
		(descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
		(tags "LED")
		(property "Reference" "LED13"
			(at 0 -1.83 90)
			(layer "F.SilkS")
		)
		(property "Value" "LED_0603_Yellow"
			(at 0 1.43 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.mouser.com/datasheet/3/281/1/LTST_C190KSKT.pdf"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Yellow SMD LED, 0603, Alternate KiCad Library"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "LED* LED_SMD:* LED_THT:*")
		(sheetname "/")
		(sheetfile "RAD_Compute_CAN_Breakout.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -0.75 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.7875 0 90)
			(size 0.875 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 31 "Net-(LED13-K)")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.7875 0 90)
			(size 0.875 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 30 "Net-(LED13-A)")
			(pinfunction "A")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Library:Molex_Nano-Fit_105312-xx04_2x02_P2.50mm_Vertical"
		(layer "F.Cu")
		(at 113.755 99.48 -90)
		(descr "Molex Nano-Fit Power Connectors, 105310-xx04, 2 Pins per row (http://www.molex.com/pdm_docs/sd/1053101208_sd.pdf), generated with kicad-footprint-generator")
		(tags "connector Molex Nano-Fit side entry")
		(property "Reference" "J1"
			(at 1.25 -2.92 90)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_02x02_Odd_Even"
			(at 1.25 5.42 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, double row, 02x02, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_2x??_*")
		(sheetname "/")
		(sheetfile "RAD_Compute_CAN_Breakout.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 3.54 1.25 0)
			(layer "F.Fab")
		)
		(pad "" thru_hole circle
			(at 0.29 -2.17 270)
			(size 2 2)
			(drill 1.6)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "" thru_hole circle
			(at 0.29 4.67 270)
			(size 2 2)
			(drill 1.6)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "1" thru_hole custom
			(at 0 0 270)
			(size 1.417157 1.417157)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 34 "CAN0_+12V")
			(pinfunction "Pin_1")
			(pintype "passive")
			(thermal_bridge_angle 90)
			(options
				(clearance outline)
				(anchor circle)
			)
			(primitives
				(gr_poly
					(pts
						(xy 0.6 0.6) (xy -0.2 0.6) (xy -0.6 0.2) (xy -0.6 -0.6) (xy 0.6 -0.6)
					)
					(width 0.5)
					(fill yes)
				)
			)
		)
		(pad "2" thru_hole circle
			(at 0 2.5 270)
			(size 1.7 1.7)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "/CAN0_H")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole circle
			(at 2.5 0 270)
			(size 1.7 1.7)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole circle
			(at 2.5 2.5 270)
			(size 1.7 1.7)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "/CAN0_L")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KIPRJMOD}/Library.pretty/105312-2204/3D/105312-2204.stp"
			(offset
				(xyz 1.25 -1.25 4.8)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -0 -0 -90)
			)
		)
	)
	(footprint "PCM_LED_SMD_AKL:LED_0603_1608Metric"
		(layer "F.Cu")
		(at 117.505 99.75 90)
		(descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
		(tags "LED")
		(property "Reference" "LED1"
			(at 0 2 90)
			(layer "F.SilkS")
		)
		(property "Value" "LED_0603_Yellow"
			(at 0 1.43 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.mouser.com/datasheet/3/281/1/LTST_C190KSKT.pdf"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Yellow SMD LED, 0603, Alternate KiCad Library"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "LED* LED_SMD:* LED_THT:*")
		(sheetname "/")
		(sheetfile "RAD_Compute_CAN_Breakout.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -0.75 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.7875 0 90)
			(size 0.875 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 18 "Net-(LED1-K)")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.7875 0 90)
			(size 0.875 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 19 "Net-(LED1-A)")
			(pinfunction "A")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "PCM_LED_SMD_AKL:LED_0603_1608Metric"
		(layer "F.Cu")
		(at 175.325 104.5)
		(descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
		(tags "LED")
		(property "Reference" "LED14"
			(at 0 -1.83 0)
			(layer "F.SilkS")
		)
		(property "Value" "LED_0603_Yellow"
			(at 0 1.43 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.mouser.com/datasheet/3/281/1/LTST_C190KSKT.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Yellow SMD LED, 0603, Alternate KiCad Library"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "LED* LED_SMD:* LED_THT:*")
		(sheetname "/")
		(sheetfile "RAD_Compute_CAN_Breakout.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -0.75 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.7875 0)
			(size 0.875 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 32 "Net-(LED14-K)")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.7875 0)
			(size 0.875 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 31 "Net-(LED13-K)")
			(pinfunction "A")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "PCM_LED_SMD_AKL:LED_0603_1608Metric"
		(layer "F.Cu")
		(at 159.385 99.75 90)
		(descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
		(tags "LED")
		(property "Reference" "LED9"
			(at 0 -1.83 90)
			(layer "F.SilkS")
		)
		(property "Value" "LED_0603_Yellow"
			(at 0 1.43 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.mouser.com/datasheet/3/281/1/LTST_C190KSKT.pdf"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Yellow SMD LED, 0603, Alternate KiCad Library"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "LED* LED_SMD:* LED_THT:*")
		(sheetname "/")
		(sheetfile "RAD_Compute_CAN_Breakout.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -0.75 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.7875 0 90)
			(size 0.875 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 27 "Net-(LED10-A)")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.7875 0 90)
			(size 0.875 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 26 "Net-(LED9-A)")
			(pinfunction "A")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "PCM_Resistor_SMD_AKL:R_0603_1608Metric"
		(layer "F.Cu")
		(at 159.605 95.64 -90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), Alternate KiCad Library")
		(tags "resistor")
		(property "Reference" "R3"
			(at 0 -1.5 90)
			(layer "F.SilkS")
		)
		(property "Value" "120"
			(at 0 1.43 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "SMD 0603 Chip Resistor, US Symbol, Alternate KiCad Library"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "RAD_Compute_CAN_Breakout.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 270)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 36 "CAN2_+12V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0 270)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 26 "Net-(LED9-A)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "PCM_LED_SMD_AKL:LED_0603_1608Metric"
		(layer "F.Cu")
		(at 175.325 95.25 180)
		(descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
		(tags "LED")
		(property "Reference" "LED16"
			(at 0 -1.83 0)
			(layer "F.SilkS")
		)
		(property "Value" "LED_0603_Yellow"
			(at 0 1.43 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.mouser.com/datasheet/3/281/1/LTST_C190KSKT.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Yellow SMD LED, 0603, Alternate KiCad Library"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "LED* LED_SMD:* LED_THT:*")
		(sheetname "/")
		(sheetfile "RAD_Compute_CAN_Breakout.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -0.75 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.7875 0 180)
			(size 0.875 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.7875 0 180)
			(size 0.875 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 33 "Net-(LED15-K)")
			(pinfunction "A")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "PCM_LED_SMD_AKL:LED_0603_1608Metric"
		(layer "F.Cu")
		(at 133.445 95.25 180)
		(descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
		(tags "LED")
		(property "Reference" "LED8"
			(at 0 -1.83 0)
			(layer "F.SilkS")
		)
		(property "Value" "LED_0603_Yellow"
			(at 0 1.43 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.mouser.com/datasheet/3/281/1/LTST_C190KSKT.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Yellow SMD LED, 0603, Alternate KiCad Library"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "LED* LED_SMD:* LED_THT:*")
		(sheetname "/")
		(sheetfile "RAD_Compute_CAN_Breakout.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -0.75 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.7875 0 180)
			(size 0.875 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.7875 0 180)
			(size 0.875 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 25 "Net-(LED7-K)")
			(pinfunction "A")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "PCM_LED_SMD_AKL:LED_0603_1608Metric"
		(layer "F.Cu")
		(at 112.505 95.25 180)
		(descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
		(tags "LED")
		(property "Reference" "LED4"
			(at 0 -1.83 0)
			(layer "F.SilkS")
		)
		(property "Value" "LED_0603_Yellow"
			(at 0 1.43 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.mouser.com/datasheet/3/281/1/LTST_C190KSKT.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Yellow SMD LED, 0603, Alternate KiCad Library"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "LED* LED_SMD:* LED_THT:*")
		(sheetname "/")
		(sheetfile "RAD_Compute_CAN_Breakout.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -0.75 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.7875 0 180)
			(size 0.875 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.7875 0 180)
			(size 0.875 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 21 "Net-(LED3-K)")
			(pinfunction "A")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "PCM_LED_SMD_AKL:LED_0603_1608Metric"
		(layer "F.Cu")
		(at 112.505 104.5)
		(descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
		(tags "LED")
		(property "Reference" "LED2"
			(at 0 -1.83 0)
			(layer "F.SilkS")
		)
		(property "Value" "LED_0603_Yellow"
			(at 0 1.43 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.mouser.com/datasheet/3/281/1/LTST_C190KSKT.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Yellow SMD LED, 0603, Alternate KiCad Library"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "LED* LED_SMD:* LED_THT:*")
		(sheetname "/")
		(sheetfile "RAD_Compute_CAN_Breakout.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -0.75 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.7875 0)
			(size 0.875 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 20 "Net-(LED2-K)")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.7875 0)
			(size 0.875 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 18 "Net-(LED1-K)")
			(pinfunction "A")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "PCM_LED_SMD_AKL:LED_0603_1608Metric"
		(layer "F.Cu")
		(at 170.325 99.75 -90)
		(descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
		(tags "LED")
		(property "Reference" "LED15"
			(at 0 -1.83 90)
			(layer "F.SilkS")
		)
		(property "Value" "LED_0603_Yellow"
			(at 0 1.43 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.mouser.com/datasheet/3/281/1/LTST_C190KSKT.pdf"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Yellow SMD LED, 0603, Alternate KiCad Library"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "LED* LED_SMD:* LED_THT:*")
		(sheetname "/")
		(sheetfile "RAD_Compute_CAN_Breakout.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -0.75 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.7875 0 270)
			(size 0.875 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 33 "Net-(LED15-K)")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.7875 0 270)
			(size 0.875 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 32 "Net-(LED14-K)")
			(pinfunction "A")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_JST:JST_SUR_SM05B-SURS-TF_1x05-1MP_P0.80mm_Horizontal"
		(layer "B.Cu")
		(at 175.325 96)
		(descr "JST SUR series connector, SM05B-SURS-TF (http://www.jst-mfg.com/product/pdf/eng/eSUR.pdf), generated with kicad-footprint-generator")
		(tags "connector JST SUR horizontal")
		(property "Reference" "J8"
			(at 0 2.85 0)
			(layer "B.SilkS")
		)
		(property "Value" "Conn_01x05_Pin"
			(at 0 -2.85 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x05, script generated"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "/")
		(sheetfile "RAD_Compute_CAN_Breakout.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.6 1.15)
			(size 0.5 1)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 16 "unconnected-(J8-Pin_1-Pad1)")
			(pinfunction "Pin_1")
			(pintype "passive+no_connect")
		)
		(pad "2" smd roundrect
			(at -0.8 1.15)
			(size 0.5 1)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 17 "unconnected-(J8-Pin_2-Pad2)")
			(pinfunction "Pin_2")
			(pintype "passive+no_connect")
		)
		(pad "3" smd roundrect
			(at 0 1.15)
			(size 0.5 1)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" smd roundrect
			(at 0.8 1.15)
			(size 0.5 1)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 8 "/CAN3_H")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(pad "5" smd roundrect
			(at 1.6 1.15)
			(size 0.5 1)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 9 "/CAN3_L")
			(pinfunction "Pin_5")
			(pintype "passive")
		)
		(pad "MP" smd roundrect
			(at -2.9 -0.8)
			(size 1.2 1.7)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.208333)
		)
		(pad "MP" smd roundrect
			(at 2.9 -0.8)
			(size 1.2 1.7)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.208333)
		)
		(embedded_fonts no)
		(model "${KIPRJMOD}/Library.pretty/BM05B-SURS-TF/3D/BM05B-SURS-TF.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -0 -0 -180)
			)
		)
	)
	(footprint "Connector_JST:JST_SUR_SM05B-SURS-TF_1x05-1MP_P0.80mm_Horizontal"
		(layer "B.Cu")
		(at 112.505 96)
		(descr "JST SUR series connector, SM05B-SURS-TF (http://www.jst-mfg.com/product/pdf/eng/eSUR.pdf), generated with kicad-footprint-generator")
		(tags "connector JST SUR horizontal")
		(property "Reference" "J5"
			(at 0 2.85 0)
			(layer "B.SilkS")
		)
		(property "Value" "Conn_01x05_Pin"
			(at 0 -2.85 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x05, script generated"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "/")
		(sheetfile "RAD_Compute_CAN_Breakout.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.6 1.15)
			(size 0.5 1)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 11 "unconnected-(J5-Pin_1-Pad1)")
			(pinfunction "Pin_1")
			(pintype "passive+no_connect")
		)
		(pad "2" smd roundrect
			(at -0.8 1.15)
			(size 0.5 1)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 10 "unconnected-(J5-Pin_2-Pad2)")
			(pinfunction "Pin_2")
			(pintype "passive+no_connect")
		)
		(pad "3" smd roundrect
			(at 0 1.15)
			(size 0.5 1)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" smd roundrect
			(at 0.8 1.15)
			(size 0.5 1)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 1 "/CAN0_H")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(pad "5" smd roundrect
			(at 1.6 1.15)
			(size 0.5 1)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 3 "/CAN0_L")
			(pinfunction "Pin_5")
			(pintype "passive")
		)
		(pad "MP" smd roundrect
			(at -2.9 -0.8)
			(size 1.2 1.7)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.208333)
		)
		(pad "MP" smd roundrect
			(at 2.9 -0.8)
			(size 1.2 1.7)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.208333)
		)
		(embedded_fonts no)
		(model "${KIPRJMOD}/Library.pretty/BM05B-SURS-TF/3D/BM05B-SURS-TF.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -0 -0 -180)
			)
		)
	)
	(footprint "Connector_JST:JST_SUR_SM05B-SURS-TF_1x05-1MP_P0.80mm_Horizontal"
		(layer "B.Cu")
		(at 133.445 96)
		(descr "JST SUR series connector, SM05B-SURS-TF (http://www.jst-mfg.com/product/pdf/eng/eSUR.pdf), generated with kicad-footprint-generator")
		(tags "connector JST SUR horizontal")
		(property "Reference" "J6"
			(at 0 2.85 0)
			(layer "B.SilkS")
		)
		(property "Value" "Conn_01x05_Pin"
			(at 0 -2.85 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x05, script generated"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "/")
		(sheetfile "RAD_Compute_CAN_Breakout.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.6 1.15)
			(size 0.5 1)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 13 "unconnected-(J6-Pin_1-Pad1)")
			(pinfunction "Pin_1")
			(pintype "passive+no_connect")
		)
		(pad "2" smd roundrect
			(at -0.8 1.15)
			(size 0.5 1)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 12 "unconnected-(J6-Pin_2-Pad2)")
			(pinfunction "Pin_2")
			(pintype "passive+no_connect")
		)
		(pad "3" smd roundrect
			(at 0 1.15)
			(size 0.5 1)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" smd roundrect
			(at 0.8 1.15)
			(size 0.5 1)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 5 "/CAN1_H")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(pad "5" smd roundrect
			(at 1.6 1.15)
			(size 0.5 1)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 4 "/CAN1_L")
			(pinfunction "Pin_5")
			(pintype "passive")
		)
		(pad "MP" smd roundrect
			(at -2.9 -0.8)
			(size 1.2 1.7)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.208333)
		)
		(pad "MP" smd roundrect
			(at 2.9 -0.8)
			(size 1.2 1.7)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.208333)
		)
		(embedded_fonts no)
		(model "${KIPRJMOD}/Library.pretty/BM05B-SURS-TF/3D/BM05B-SURS-TF.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -0 -0 -180)
			)
		)
	)
	(footprint "Connector_JST:JST_SUR_SM05B-SURS-TF_1x05-1MP_P0.80mm_Horizontal"
		(layer "B.Cu")
		(at 154.385 96)
		(descr "JST SUR series connector, SM05B-SURS-TF (http://www.jst-mfg.com/product/pdf/eng/eSUR.pdf), generated with kicad-footprint-generator")
		(tags "connector JST SUR horizontal")
		(property "Reference" "J7"
			(at 0 2.85 0)
			(layer "B.SilkS")
		)
		(property "Value" "Conn_01x05_Pin"
			(at 0 -2.85 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x05, script generated"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "/")
		(sheetfile "RAD_Compute_CAN_Breakout.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.6 1.15)
			(size 0.5 1)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 15 "unconnected-(J7-Pin_1-Pad1)")
			(pinfunction "Pin_1")
			(pintype "passive+no_connect")
		)
		(pad "2" smd roundrect
			(at -0.8 1.15)
			(size 0.5 1)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 14 "unconnected-(J7-Pin_2-Pad2)")
			(pinfunction "Pin_2")
			(pintype "passive+no_connect")
		)
		(pad "3" smd roundrect
			(at 0 1.15)
			(size 0.5 1)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" smd roundrect
			(at 0.8 1.15)
			(size 0.5 1)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 7 "/CAN2_H")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(pad "5" smd roundrect
			(at 1.6 1.15)
			(size 0.5 1)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 6 "/CAN2_L")
			(pinfunction "Pin_5")
			(pintype "passive")
		)
		(pad "MP" smd roundrect
			(at -2.9 -0.8)
			(size 1.2 1.7)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.208333)
		)
		(pad "MP" smd roundrect
			(at 2.9 -0.8)
			(size 1.2 1.7)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.208333)
		)
		(embedded_fonts no)
		(model "${KIPRJMOD}/Library.pretty/BM05B-SURS-TF/3D/BM05B-SURS-TF.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -0 -0 -180)
			)
		)
	)
	(gr_line
		(start 188.39 94)
		(end 99.44 94)
		(layer "Edge.Cuts")
	)
	(gr_circle
		(center 184.84 98.76)
		(end 186.19 98.76)
		(fill no)
		(layer "Edge.Cuts")
	)
	(gr_circle
		(center 102.84 98.76)
		(end 104.19 98.76)
		(fill no)
		(layer "Edge.Cuts")
	)
	(gr_circle
		(center 143.84 98.76)
		(end 145.19 98.76)
		(fill no)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 99.44 105)
		(end 188.39 105)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 99.44 94)
		(end 99.44 105)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 188.39 105)
		(end 188.39 94)
		(layer "Edge.Cuts")
	)
	(zone
		(net 2)
		(net_name "GND")
		(layers "F.Cu" "B.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0.25)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 99.44 94) (xy 188.39 94) (xy 188.39 105) (xy 99.43 105.01)
			)
		)
	)
	(embedded_fonts no)
)
