(kicad_pcb
	(version 20260206)
	(generator "pcbnew")
	(generator_version "10.0")
	(general
		(thickness 1.6)
		(legacy_teardrops no)
	)
	(paper "A4")
	(layers
		(0 "F.Cu" signal)
		(2 "B.Cu" signal)
		(9 "F.Adhes" user "F.Adhesive")
		(11 "B.Adhes" user "B.Adhesive")
		(13 "F.Paste" user)
		(15 "B.Paste" user)
		(5 "F.SilkS" user "F.Silkscreen")
		(7 "B.SilkS" user "B.Silkscreen")
		(1 "F.Mask" user)
		(3 "B.Mask" user)
		(17 "Dwgs.User" user "User.Drawings")
		(19 "Cmts.User" user "User.Comments")
		(21 "Eco1.User" user "User.Eco1")
		(23 "Eco2.User" user "User.Eco2")
		(25 "Edge.Cuts" user)
		(27 "Margin" user)
		(31 "F.CrtYd" user "F.Courtyard")
		(29 "B.CrtYd" user "B.Courtyard")
		(35 "F.Fab" user)
		(33 "B.Fab" user)
		(39 "User.1" user)
		(41 "User.2" user)
		(43 "User.3" user)
		(45 "User.4" user)
	)
	(setup
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(tenting
			(front yes)
			(back yes)
		)
		(covering
			(front no)
			(back no)
		)
		(plugging
			(front no)
			(back no)
		)
		(capping no)
		(filling no)
		(pcbplotparams
			(layerselection 0x00000000_00000000_55555555_5755f5ff)
			(plot_on_all_layers_selection 0x00000000_00000000_00000000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12)
			(dashed_line_gap_ratio 3)
			(svgprecision 4)
			(plotframeref no)
			(mode 1)
			(useauxorigin no)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(pdf_metadata yes)
			(pdf_single_document no)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plot_black_and_white yes)
			(sketchpadsonfab no)
			(plotpadnumbers no)
			(hidednponfab no)
			(sketchdnponfab yes)
			(crossoutdnponfab yes)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 1)
			(scaleselection 1)
			(outputdirectory "")
		)
	)
	(footprint "AAA:Diode"
		(layer "F.Cu")
		(at 118.11 76.2)
		(property "Reference" "D3"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "~"
			(at 0 -1.524 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "breadboard power.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "A" "K")
			)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(pad "A" thru_hole circle
			(at -2.54 0)
			(size 1.75 1.75)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "Net-(D3-PadA)")
			(pintype "passive")
		)
		(pad "K" thru_hole circle
			(at 2.54 0)
			(size 1.75 1.75)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "Net-(J1-Pin_1)")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "Capacitor_THT:CP_Radial_D4.0mm_P2.00mm"
		(layer "F.Cu")
		(at 154.94 81.28 180)
		(descr "CP, Radial series, Radial, pin pitch=2.00mm, diameter=4mm, height=7mm, Electrolytic Capacitor")
		(tags "CP Radial series Radial pin pitch 2.00mm diameter 4mm height 7mm Electrolytic Capacitor")
		(property "Reference" "C1"
			(at -1.449801 -2.54 0)
			(layer "F.SilkS")
		)
		(property "Value" "C_Polarized"
			(at 1 3.25 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Polarized capacitor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "capacitor/THT/other"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property ki_fp_filters "CP_*")
		(sheetname "/")
		(sheetfile "breadboard power.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1" "2")
			)
		)
		(attr through_hole)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 1 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole roundrect
			(at 0 0 180)
			(size 1.2 1.2)
			(drill 0.6)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.208333)
			(net "+12V")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 2 0 180)
			(size 1.2 1.2)
			(drill 0.6)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Capacitor_THT.3dshapes/CP_Radial_D4.0mm_P2.00mm.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "AAA:Diode"
		(layer "F.Cu")
		(at 118.11 83.82)
		(property "Reference" "D4"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "~"
			(at 0 -1.524 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "breadboard power.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "A" "K")
			)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(pad "A" thru_hole circle
			(at -2.54 0)
			(size 1.75 1.75)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "Net-(D3-PadA)")
			(pintype "passive")
		)
		(pad "K" thru_hole circle
			(at 2.54 0)
			(size 1.75 1.75)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "Net-(J1-Pin_10)")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "Capacitor_THT:CP_Radial_D4.0mm_P2.00mm"
		(layer "F.Cu")
		(at 108.68 81.28 180)
		(descr "CP, Radial series, Radial, pin pitch=2.00mm, diameter=4mm, height=7mm, Electrolytic Capacitor")
		(tags "CP Radial series Radial pin pitch 2.00mm diameter 4mm height 7mm Electrolytic Capacitor")
		(property "Reference" "C2"
			(at -1.449801 -2.54 0)
			(layer "F.SilkS")
		)
		(property "Value" "C_Polarized"
			(at 1 3.25 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Polarized capacitor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "capacitor/THT/other"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property ki_fp_filters "CP_*")
		(sheetname "/")
		(sheetfile "breadboard power.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1" "2")
			)
		)
		(attr through_hole)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 1 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole roundrect
			(at 0 0 180)
			(size 1.2 1.2)
			(drill 0.6)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.208333)
			(net "GND")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 2 0 180)
			(size 1.2 1.2)
			(drill 0.6)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "-12V")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Capacitor_THT.3dshapes/CP_Radial_D4.0mm_P2.00mm.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal"
		(layer "F.Cu")
		(at 123.19 86.36)
		(descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
		(property "Reference" "R3"
			(at 3.81 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "R_US"
			(at 3.81 2.37 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "resistor/THT"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "breadboard power.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1" "2")
			)
		)
		(attr through_hole)
		(duplicate_pad_numbers_are_jumpers no)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "Net-(D1-PadK)")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 7.62 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "Net-(U1-VI)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 148.59 78.74)
		(descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x03 2.54mm single row")
		(property "Reference" "J2"
			(at 0 -2.38 0)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_01x03"
			(at 0 7.46 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x03, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "connector/pin_header_socket"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "/")
		(sheetfile "breadboard power.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1" "2" "3")
			)
		)
		(attr through_hole)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 2.54 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "+5V")
			(pinfunction "Pin_1_1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 0 2.54)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "Net-(J2-Pin_2)")
			(pinfunction "Pin_2_2")
			(pintype "passive")
		)
		(pad "3" thru_hole circle
			(at 0 5.08)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "GND")
			(pinfunction "Pin_3_3")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "AAA:Diode"
		(layer "F.Cu")
		(at 125.73 76.2)
		(property "Reference" "D1"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "~"
			(at 0 -1.524 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "breadboard power.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "A" "K")
			)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(pad "A" thru_hole circle
			(at -2.54 0)
			(size 1.75 1.75)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "Net-(J1-Pin_1)")
			(pintype "passive")
		)
		(pad "K" thru_hole circle
			(at 2.54 0)
			(size 1.75 1.75)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "Net-(D1-PadK)")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "Connector_PinHeader_2.54mm:PinHeader_2x05_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 127 78.74 -90)
		(descr "Through hole straight pin header, 2x05, 2.54mm pitch, double rows")
		(tags "Through hole pin header THT 2x05 2.54mm double row")
		(property "Reference" "J1"
			(at 1.27 -2.38 90)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_02x05_Odd_Even"
			(at 1.27 12.54 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, double row, 02x05, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "connector/pin_header_socket"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_2x??_*")
		(sheetname "/")
		(sheetfile "breadboard power.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1" "3" "5" "7" "9" "2" "4" "6" "8" "10")
			)
		)
		(attr through_hole)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 1.27 5.08 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "Net-(J1-Pin_1)")
			(pinfunction "Pin_1_1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 2.54 0 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "Net-(J1-Pin_1)")
			(pinfunction "Pin_2_2")
			(pintype "passive")
		)
		(pad "3" thru_hole circle
			(at 0 2.54 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "GND")
			(pinfunction "Pin_3_3")
			(pintype "passive")
		)
		(pad "4" thru_hole circle
			(at 2.54 2.54 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "GND")
			(pinfunction "Pin_4_4")
			(pintype "passive")
		)
		(pad "5" thru_hole circle
			(at 0 5.08 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "GND")
			(pinfunction "Pin_5_5")
			(pintype "passive")
		)
		(pad "6" thru_hole circle
			(at 2.54 5.08 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "GND")
			(pinfunction "Pin_6_6")
			(pintype "passive")
		)
		(pad "7" thru_hole circle
			(at 0 7.62 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "GND")
			(pinfunction "Pin_7_7")
			(pintype "passive")
		)
		(pad "8" thru_hole circle
			(at 2.54 7.62 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "GND")
			(pinfunction "Pin_8_8")
			(pintype "passive")
		)
		(pad "9" thru_hole circle
			(at 0 10.16 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "Net-(J1-Pin_10)")
			(pinfunction "Pin_9_9")
			(pintype "passive")
		)
		(pad "10" thru_hole circle
			(at 2.54 10.16 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "Net-(J1-Pin_10)")
			(pinfunction "Pin_10_10")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x05_P2.54mm_Vertical.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "AAA:Diode"
		(layer "F.Cu")
		(at 125.73 83.82)
		(property "Reference" "D2"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "~"
			(at 0 -1.524 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "breadboard power.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "A" "K")
			)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(pad "A" thru_hole circle
			(at -2.54 0)
			(size 1.75 1.75)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "Net-(J1-Pin_10)")
			(pintype "passive")
		)
		(pad "K" thru_hole circle
			(at 2.54 0)
			(size 1.75 1.75)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "Net-(D1-PadK)")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "Capacitor_THT:CP_Radial_D4.0mm_P2.00mm"
		(layer "F.Cu")
		(at 135.89 77.47 180)
		(descr "CP, Radial series, Radial, pin pitch=2.00mm, diameter=4mm, height=7mm, Electrolytic Capacitor")
		(tags "CP Radial series Radial pin pitch 2.00mm diameter 4mm height 7mm Electrolytic Capacitor")
		(property "Reference" "C3"
			(at -1.449801 -2.54 0)
			(layer "F.SilkS")
		)
		(property "Value" "C_Polarized"
			(at 1 3.25 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Polarized capacitor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "capacitor/THT/other"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property ki_fp_filters "CP_*")
		(sheetname "/")
		(sheetfile "breadboard power.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1" "2")
			)
		)
		(attr through_hole)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 1 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole roundrect
			(at 0 0 180)
			(size 1.2 1.2)
			(drill 0.6)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.208333)
			(net "Net-(U1-VI)")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 2 0 180)
			(size 1.2 1.2)
			(drill 0.6)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Capacitor_THT.3dshapes/CP_Radial_D4.0mm_P2.00mm.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal"
		(layer "F.Cu")
		(at 130.81 76.2 -90)
		(descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
		(property "Reference" "R1"
			(at 3.81 0 90)
			(layer "F.SilkS")
		)
		(property "Value" "R_US"
			(at 3.81 2.37 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "resistor/THT"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "breadboard power.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1" "2")
			)
		)
		(attr through_hole)
		(duplicate_pad_numbers_are_jumpers no)
		(pad "1" thru_hole circle
			(at 0 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "Net-(D1-PadK)")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 7.62 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "+12V")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_THT:TO-92_Inline"
		(layer "F.Cu")
		(at 140.97 83.82 180)
		(descr "TO-92 leads in-line, narrow, oval pads, drill 0.75mm (see NXP sot054_po.pdf)")
		(tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
		(property "Reference" "U1"
			(at 1.27 -3.384904 0)
			(layer "F.SilkS")
		)
		(property "Value" "LM4931"
			(at 1.27 2.79 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm2931-n.pdf"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "100mA Low drop-out regulator, Fixed Output 5V, TO-92"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TO?92*")
		(sheetname "/")
		(sheetfile "breadboard power.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "3" "2" "1")
			)
		)
		(attr through_hole)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 1.27 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 180)
			(size 1.05 1.5)
			(drill 0.75)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "+5V")
			(pinfunction "VO_1")
			(pintype "power_out")
		)
		(pad "2" thru_hole oval
			(at 1.27 0 180)
			(size 1.05 1.5)
			(drill 0.75)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "GND")
			(pinfunction "GND_2")
			(pintype "power_in")
		)
		(pad "3" thru_hole oval
			(at 2.54 0 180)
			(size 1.05 1.5)
			(drill 0.75)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "Net-(U1-VI)")
			(pinfunction "VI_3")
			(pintype "power_in")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Package_TO_SOT_THT.3dshapes/TO-92_Inline.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_THT:CP_Radial_D4.0mm_P2.00mm"
		(layer "F.Cu")
		(at 144.78 77.47 180)
		(descr "CP, Radial series, Radial, pin pitch=2.00mm, diameter=4mm, height=7mm, Electrolytic Capacitor")
		(tags "CP Radial series Radial pin pitch 2.00mm diameter 4mm height 7mm Electrolytic Capacitor")
		(property "Reference" "C4"
			(at -1.449801 -2.54 0)
			(layer "F.SilkS")
		)
		(property "Value" "C_Polarized"
			(at 1 3.25 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Polarized capacitor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "capacitor/THT/other"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property ki_fp_filters "CP_*")
		(sheetname "/")
		(sheetfile "breadboard power.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1" "2")
			)
		)
		(attr through_hole)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 1 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole roundrect
			(at 0 0 180)
			(size 1.2 1.2)
			(drill 0.6)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.208333)
			(net "+5V")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 2 0 180)
			(size 1.2 1.2)
			(drill 0.6)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Capacitor_THT.3dshapes/CP_Radial_D4.0mm_P2.00mm.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal"
		(layer "F.Cu")
		(at 113.03 76.2 -90)
		(descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=7.62mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 7.62mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
		(property "Reference" "R2"
			(at 3.81 0 90)
			(layer "F.SilkS")
		)
		(property "Value" "R_US"
			(at 3.81 2.37 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "resistor/THT"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "breadboard power.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1" "2")
			)
		)
		(attr through_hole)
		(duplicate_pad_numbers_are_jumpers no)
		(pad "1" thru_hole circle
			(at 0 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "Net-(D3-PadA)")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 7.62 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "-12V")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical"
		(layer "B.Cu")
		(at 154.94 86.36 90)
		(descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x02 2.54mm single row")
		(property "Reference" "J3"
			(at 0 -5.08 90)
			(layer "B.SilkS")
		)
		(property "Value" "Conn_01x02"
			(at 0 -4.92 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "connector/pin_header_socket"
			(at 0 0 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "/")
		(sheetfile "breadboard power.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1" "2")
			)
		)
		(attr through_hole)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 -1.27 0)
			(layer "B.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "+12V")
			(pinfunction "Pin_1_1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 0 -2.54 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "Net-(J2-Pin_2)")
			(pinfunction "Pin_2_2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical"
		(layer "B.Cu")
		(at 109.22 86.36 90)
		(descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x02 2.54mm single row")
		(property "Reference" "J6"
			(at 0 2.38 90)
			(layer "B.SilkS")
		)
		(property "Value" "Conn_01x02"
			(at 0 -4.92 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "connector/pin_header_socket"
			(at 0 0 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "/")
		(sheetfile "breadboard power.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1" "2")
			)
		)
		(attr through_hole)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 -1.27 0)
			(layer "B.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "GND")
			(pinfunction "Pin_1_1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 0 -2.54 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "-12V")
			(pinfunction "Pin_2_2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical"
		(layer "B.Cu")
		(at 154.94 76.2 90)
		(descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x02 2.54mm single row")
		(property "Reference" "J4"
			(at 0 -5.08 90)
			(layer "B.SilkS")
		)
		(property "Value" "Conn_01x02"
			(at 0 -4.92 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "connector/pin_header_socket"
			(at 0 0 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "/")
		(sheetfile "breadboard power.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1" "2")
			)
		)
		(attr through_hole)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 -1.27 0)
			(layer "B.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "+12V")
			(pinfunction "Pin_1_1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 0 -2.54 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "Net-(J2-Pin_2)")
			(pinfunction "Pin_2_2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical"
		(layer "B.Cu")
		(at 109.22 76.2 90)
		(descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x02 2.54mm single row")
		(property "Reference" "J5"
			(at 0 2.38 90)
			(layer "B.SilkS")
		)
		(property "Value" "Conn_01x02"
			(at 0 -4.92 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "connector/pin_header_socket"
			(at 0 0 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "/")
		(sheetfile "breadboard power.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1" "2")
			)
		)
		(attr through_hole)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 -1.27 0)
			(layer "B.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "GND")
			(pinfunction "Pin_1_1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 0 -2.54 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "-12V")
			(pinfunction "Pin_2_2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(gr_line
		(start 105.41 74.93)
		(end 105.41 87.63)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 156.21 74.93)
		(end 105.41 74.93)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 156.21 74.93)
		(end 156.21 87.63)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 156.21 87.63)
		(end 105.41 87.63)
		(layer "Edge.Cuts")
	)
	(embedded_fonts no)
)
