(kicad_pcb
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(general
		(thickness 1.6)
		(legacy_teardrops no)
	)
	(paper "A4")
	(layers
		(0 "F.Cu" signal)
		(2 "B.Cu" signal)
		(9 "F.Adhes" user "F.Adhesive")
		(11 "B.Adhes" user "B.Adhesive")
		(13 "F.Paste" user)
		(15 "B.Paste" user)
		(5 "F.SilkS" user "F.Silkscreen")
		(7 "B.SilkS" user "B.Silkscreen")
		(1 "F.Mask" user)
		(3 "B.Mask" user)
		(17 "Dwgs.User" user "User.Drawings")
		(19 "Cmts.User" user "User.Comments")
		(21 "Eco1.User" user "User.Eco1")
		(23 "Eco2.User" user "User.Eco2")
		(25 "Edge.Cuts" user)
		(27 "Margin" user)
		(31 "F.CrtYd" user "F.Courtyard")
		(29 "B.CrtYd" user "B.Courtyard")
		(35 "F.Fab" user)
		(33 "B.Fab" user)
		(39 "User.1" user)
		(41 "User.2" user)
		(43 "User.3" user)
		(45 "User.4" user)
	)
	(setup
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(tenting front back)
		(pcbplotparams
			(layerselection 0x00000000_00000000_55555555_5755f5ff)
			(plot_on_all_layers_selection 0x00000000_00000000_00000000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 4)
			(plotframeref no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(pdf_metadata yes)
			(pdf_single_document no)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plot_black_and_white yes)
			(sketchpadsonfab no)
			(plotpadnumbers no)
			(hidednponfab no)
			(sketchdnponfab yes)
			(crossoutdnponfab yes)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 0)
			(scaleselection 1)
			(outputdirectory "gerber")
		)
	)
	(net 0 "")
	(net 1 "GND")
	(net 2 "+5V")
	(net 3 "/CANL")
	(net 4 "/CANH")
	(net 5 "Net-(J1-Pin_1)")
	(net 6 "Net-(J2-Pin_2)")
	(net 7 "+24V")
	(net 8 "+3.3V")
	(net 9 "Net-(J2-Pin_3)")
	(net 10 "unconnected-(U3-NC-Pad4)")
	(net 11 "unconnected-(U1-VREF-Pad5)")
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 145.5 102 -90)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C4"
			(at 0 -3 270)
			(layer "F.SilkS")
		)
		(property "Value" "1uF"
			(at 0 1.16 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "can-splitter.kicad_sch")
		(attr smd dnp)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 270)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 8 "+3.3V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 270)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_JST:JST_PH_S4B-PH-K_1x04_P2.00mm_Horizontal"
		(layer "F.Cu")
		(at 146 93 180)
		(descr "JST PH series connector, S4B-PH-K (http://www.jst-mfg.com/product/pdf/eng/ePH.pdf), generated with kicad-footprint-generator")
		(tags "connector JST PH horizontal")
		(property "Reference" "J2"
			(at 9 5 0)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_01x04"
			(at 3 7.45 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x04, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "/")
		(sheetfile "can-splitter.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 3 2.5 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole roundrect
			(at 0 0 180)
			(size 1.2 1.75)
			(drill 0.75)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.208333)
			(net 1 "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 2 0 180)
			(size 1.2 1.75)
			(drill 0.75)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "Net-(J2-Pin_2)")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 4 0 180)
			(size 1.2 1.75)
			(drill 0.75)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 9 "Net-(J2-Pin_3)")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole oval
			(at 6 0 180)
			(size 1.2 1.75)
			(drill 0.75)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "+5V")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_JST.3dshapes/JST_PH_S4B-PH-K_1x04_P2.00mm_Horizontal.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Jumper:SolderJumper-2_P1.3mm_Open_TrianglePad1.0x1.5mm"
		(layer "F.Cu")
		(at 153.725 101.5)
		(descr "SMD Solder Jumper, 1x1.5mm Triangular Pads, 0.3mm gap, open")
		(tags "solder jumper open")
		(property "Reference" "J1"
			(at 2.5 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_01x02"
			(at 0 1.9 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "/")
		(sheetfile "can-splitter.kicad_sch")
		(zone_connect 1)
		(attr exclude_from_pos_files allow_soldermask_bridges)
		(pad "1" smd custom
			(at -0.725 0)
			(size 0.3 0.3)
			(layers "F.Cu" "F.Mask")
			(net 5 "Net-(J1-Pin_1)")
			(pinfunction "Pin_1")
			(pintype "passive")
			(zone_connect 2)
			(thermal_bridge_angle 45)
			(options
				(clearance outline)
				(anchor rect)
			)
			(primitives
				(gr_poly
					(pts
						(xy 1 0) (xy 0.5 0.75) (xy -0.5 0.75) (xy -0.5 -0.75) (xy 0.5 -0.75)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "2" smd custom
			(at 0.725 0)
			(size 0.3 0.3)
			(layers "F.Cu" "F.Mask")
			(net 3 "/CANL")
			(pinfunction "Pin_2")
			(pintype "passive")
			(zone_connect 2)
			(thermal_bridge_angle 45)
			(options
				(clearance outline)
				(anchor rect)
			)
			(primitives
				(gr_poly
					(pts
						(xy 0.5 0.75) (xy -0.65 0.75) (xy -0.15 0) (xy -0.65 -0.75) (xy 0.5 -0.75)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(embedded_fonts no)
	)
	(footprint "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
		(layer "F.Cu")
		(at 145.5 98)
		(descr "SOIC, 8 Pin (JEDEC MS-012AA, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_narrow-r/r_8.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOIC SO")
		(property "Reference" "U1"
			(at 0 -3.4 0)
			(layer "F.SilkS")
		)
		(property "Value" "SN65HVD1050D"
			(at 0 3.4 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/sn65hvd1050.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "CAN Bus Transceiver, EMC optimised, 5.0V, 1Mbps, SOIC-8"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Vendor" "https://www.digikey.com/en/products/detail/texas-instruments/SN65HVD1050DR/1574460"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SOIC*3.9x4.9mm*P1.27mm*")
		(sheetname "/")
		(sheetfile "can-splitter.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -2.475 -1.905)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 9 "Net-(J2-Pin_3)")
			(pinfunction "TXD")
			(pintype "input")
		)
		(pad "2" smd roundrect
			(at -2.475 -0.635)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "3" smd roundrect
			(at -2.475 0.635)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "+5V")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(pad "4" smd roundrect
			(at -2.475 1.905)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 6 "Net-(J2-Pin_2)")
			(pinfunction "RXD")
			(pintype "output")
		)
		(pad "5" smd roundrect
			(at 2.475 1.905)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 11 "unconnected-(U1-VREF-Pad5)")
			(pinfunction "VREF")
			(pintype "passive+no_connect")
		)
		(pad "6" smd roundrect
			(at 2.475 0.635)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 3 "/CANL")
			(pinfunction "CANL")
			(pintype "bidirectional")
		)
		(pad "7" smd roundrect
			(at 2.475 -0.635)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 4 "/CANH")
			(pinfunction "CANH")
			(pintype "bidirectional")
		)
		(pad "8" smd roundrect
			(at 2.475 -1.905)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "S")
			(pintype "input")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Package_SO.3dshapes/SOIC-8_3.9x4.9mm_P1.27mm.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MountingHole:MountingHole_3.2mm_M3_ISO7380"
		(layer "F.Cu")
		(at 165 89.5)
		(descr "Mounting Hole 3.2mm, M3, no annular, generated by kicad-footprint-generator mountinghole.py")
		(tags "mountinghole M3 ISO7380")
		(property "Reference" "H1"
			(at 0 -3.8 0)
			(layer "F.SilkS")
		)
		(property "Value" "MountingHole"
			(at 0 3.8 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Mounting Hole without connection"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "MountingHole*")
		(sheetname "/")
		(sheetfile "can-splitter.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 3.2 3.2)
			(drill 3.2)
			(layers "*.Cu" "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "MountingHole:MountingHole_3.2mm_M3_ISO7380"
		(layer "F.Cu")
		(at 132.5 89.5)
		(descr "Mounting Hole 3.2mm, M3, no annular, generated by kicad-footprint-generator mountinghole.py")
		(tags "mountinghole M3 ISO7380")
		(property "Reference" "H2"
			(at 0 -3.8 0)
			(layer "F.SilkS")
		)
		(property "Value" "MountingHole"
			(at 0 3.8 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Mounting Hole without connection"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "MountingHole*")
		(sheetname "/")
		(sheetfile "can-splitter.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 3.2 3.2)
			(drill 3.2)
			(layers "*.Cu" "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "Package_TO_SOT_SMD:SOT-353_SC-70-5"
		(layer "F.Cu")
		(at 143 102.35)
		(descr "SOT, 5 Pin (https://home.jeita.or.jp/tsc/std-pdf/ED-7500A.pdf#page=171, JEDEC MO-203, variant AA, https://www.jedec.org/document_search?search_api_views_fulltext=MO-203), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOT TO_SOT_SMD SC-88A SOT-353 SC-70-5")
		(property "Reference" "U3"
			(at -2 -1.95 0)
			(layer "F.SilkS")
		)
		(property "Value" "MIC5365-3.3YC5"
			(at 0 1.95 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/aemDocuments/documents/APID/ProductDocuments/DataSheets/MIC5365-6-High-Performance-Single-150mA-LDO-DS20006605A.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "150mA Low-dropout Voltage Regulator, Vout 3.3V, Vin up to 5.5V, SC-70-5"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SOT*353*SC*70*")
		(sheetname "/")
		(sheetfile "can-splitter.kicad_sch")
		(attr smd dnp)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.8875 -0.65)
			(size 1.325 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "+5V")
			(pinfunction "VIN")
			(pintype "power_in")
		)
		(pad "2" smd roundrect
			(at -0.8875 0)
			(size 1.325 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "3" smd roundrect
			(at -0.8875 0.65)
			(size 1.325 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "+5V")
			(pinfunction "EN")
			(pintype "input")
		)
		(pad "4" smd roundrect
			(at 0.8875 0.65)
			(size 1.325 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 10 "unconnected-(U3-NC-Pad4)")
			(pinfunction "NC")
			(pintype "no_connect")
		)
		(pad "5" smd roundrect
			(at 0.8875 -0.65)
			(size 1.325 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 8 "+3.3V")
			(pinfunction "VOUT")
			(pintype "power_out")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-353_SC-70-5.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 147 102 -90)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C2"
			(at 0 -3 90)
			(layer "F.SilkS")
		)
		(property "Value" "0.1uF"
			(at 0 1.16 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "can-splitter.kicad_sch")
		(attr smd dnp)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 270)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 8 "+3.3V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 270)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 151 98 -90)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R1"
			(at 2 0 270)
			(layer "F.SilkS")
		)
		(property "Value" "R"
			(at 0 1.17 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "can-splitter.kicad_sch")
		(attr smd dnp)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 270)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 4 "/CANH")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 270)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 5 "Net-(J1-Pin_1)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_SMD:SOT-23-3"
		(layer "F.Cu")
		(at 154.8625 98)
		(descr "SOT, 3 Pin (JEDEC MO-178 inferred 3-pin variant https://www.jedec.org/document_search?search_api_views_fulltext=MO-178), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOT TO_SOT_SMD")
		(property "Reference" "D1"
			(at 0 -2.4 0)
			(layer "F.SilkS")
		)
		(property "Value" "DESD2CAN2SOQ"
			(at 0 2.4 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/esdal.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "CAN BUS ESD PROTECTION DIODE, SOT23"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SOT?23*")
		(sheetname "/")
		(sheetfile "can-splitter.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.1375 -0.95)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 4 "/CANH")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at -1.1375 0.95)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 3 "/CANL")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "3" smd roundrect
			(at 1.1375 0)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "A")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23-3.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_Molex:Molex_Micro-Fit_3.0_43650-0200_1x02_P3.00mm_Horizontal"
		(layer "F.Cu")
		(at 152.5 93.32)
		(descr "Molex Micro-Fit 3.0 Connector System, 43650-0200 (compatible alternatives: 43650-0201, 43650-0202), 2 Pins per row (https://www.molex.com/pdm_docs/sd/436500300_sd.pdf), generated with kicad-footprint-generator")
		(tags "connector Molex Micro-Fit_3.0 horizontal")
		(property "Reference" "J5"
			(at 7.5 -5.82 0)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_01x02"
			(at 1.5 3.22 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "/")
		(sheetfile "can-splitter.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 1.5 -8.22 0)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole circle
			(at 1.5 -4.32)
			(size 3 3)
			(drill 3)
			(layers "*.Cu" "*.Mask")
		)
		(pad "1" thru_hole roundrect
			(at 0 0)
			(size 1.5 2.02)
			(drill 1.02)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.166667)
			(net 7 "+24V")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 3 0)
			(size 1.5 2.02)
			(drill 1.02)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_Molex.3dshapes/Molex_Micro-Fit_3.0_43650-0200_1x02_P3.00mm_Horizontal.step"
			(offset
				(xyz 1.5 8.9 0.6)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -0 -0 -180)
			)
		)
	)
	(footprint "Connector_Molex:Molex_Micro-Fit_3.0_43045-0400_2x02_P3.00mm_Horizontal"
		(layer "F.Cu")
		(at 161.18 97 -90)
		(descr "Molex Micro-Fit 3.0 Connector System, 43045-0400 (alternative finishes: 43045-040x), 2 Pins per row (https://www.molex.com/pdm_docs/sd/430450201_sd.pdf), generated with kicad-footprint-generator")
		(tags "connector Molex Micro-Fit_3.0 horizontal")
		(property "Reference" "J3"
			(at -4.5 -5.5 180)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_02x02_Odd_Even"
			(at 2.32 10.7 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, double row, 02x02, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_2x??_*")
		(sheetname "/")
		(sheetfile "can-splitter.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 1.5 -8.22 90)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole circle
			(at 1.5 -4.32 270)
			(size 3 3)
			(drill 3)
			(layers "*.Cu" "*.Mask")
		)
		(pad "1" thru_hole roundrect
			(at 0 0 270)
			(size 1.5 1.5)
			(drill 1.02)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.166667)
			(net 7 "+24V")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 3 0 270)
			(size 1.5 1.5)
			(drill 1.02)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole circle
			(at 0 3 270)
			(size 1.5 1.5)
			(drill 1.02)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "/CANH")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole circle
			(at 3 3 270)
			(size 1.5 1.5)
			(drill 1.02)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "/CANL")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_Molex.3dshapes/Molex_Micro-Fit_3.0_43045-0400_2x02_P3.00mm_Horizontal.step"
			(offset
				(xyz 1.5 3.9 4)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 -0 -180)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 140.5 102 -90)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C3"
			(at 0 1.5 90)
			(layer "F.SilkS")
		)
		(property "Value" "1uF"
			(at 0 1.16 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "can-splitter.kicad_sch")
		(attr smd dnp)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 270)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "+5V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 270)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_Molex:Molex_Micro-Fit_3.0_43045-0400_2x02_P3.00mm_Horizontal"
		(layer "F.Cu")
		(at 136.32 100 90)
		(descr "Molex Micro-Fit 3.0 Connector System, 43045-0400 (alternative finishes: 43045-040x), 2 Pins per row (https://www.molex.com/pdm_docs/sd/430450201_sd.pdf), generated with kicad-footprint-generator")
		(tags "connector Molex Micro-Fit_3.0 horizontal")
		(property "Reference" "J4"
			(at 7.5 -5 180)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_02x02_Odd_Even"
			(at 1.5 5.7 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, double row, 02x02, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_2x??_*")
		(sheetname "/")
		(sheetfile "can-splitter.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 1.5 -8.22 90)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole circle
			(at 1.5 -4.32 90)
			(size 3 3)
			(drill 3)
			(layers "*.Cu" "*.Mask")
		)
		(pad "1" thru_hole roundrect
			(at 0 0 90)
			(size 1.5 1.5)
			(drill 1.02)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.166667)
			(net 7 "+24V")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 3 0 90)
			(size 1.5 1.5)
			(drill 1.02)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole circle
			(at 0 3 90)
			(size 1.5 1.5)
			(drill 1.02)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "/CANH")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole circle
			(at 3 3 90)
			(size 1.5 1.5)
			(drill 1.02)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "/CANL")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_Molex.3dshapes/Molex_Micro-Fit_3.0_43045-0400_2x02_P3.00mm_Horizontal.step"
			(offset
				(xyz 1.5 3.95 4)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 -0 -180)
			)
		)
	)
	(gr_rect
		(start 129.5 86.5)
		(end 168 104)
		(fill no)
		(layer "Edge.Cuts")
	)
	(dimension
		(type orthogonal)
		(layer "Dwgs.User")
		(pts
			(xy 129.5 86.5) (xy 129.5 104)
		)
		(height -5.5)
		(orientation 1)
		(format
			(prefix "")
			(suffix "")
			(units 3)
			(units_format 0)
			(precision 4)
			(suppress_zeroes yes)
		)
		(style
			(thickness 0.2)
			(arrow_length 1.27)
			(text_position_mode 0)
			(arrow_direction outward)
			(extension_height 0.58642)
			(extension_offset 0.5)
			(keep_text_aligned yes)
		)
		(gr_text "17.5"
			(at 122.2 95.25 90)
			(layer "Dwgs.User")
		)
	)
	(dimension
		(type orthogonal)
		(layer "Dwgs.User")
		(pts
			(xy 129.5 86.5) (xy 168 86.5)
		)
		(height -4)
		(orientation 0)
		(format
			(prefix "")
			(suffix "")
			(units 3)
			(units_format 0)
			(precision 4)
			(suppress_zeroes yes)
		)
		(style
			(thickness 0.2)
			(arrow_length 1.27)
			(text_position_mode 0)
			(arrow_direction outward)
			(extension_height 0.58642)
			(extension_offset 0.5)
			(keep_text_aligned yes)
		)
		(gr_text "38.5"
			(at 148.75 80.7 0)
			(layer "Dwgs.User")
		)
	)
	(zone
		(net 7)
		(net_name "+24V")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 1)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.2)
			(thermal_bridge_width 0.6)
		)
		(polygon
			(pts
				(xy 133.5 101.5) (xy 137 101.5) (xy 137 98.5) (xy 135.5 98.5) (xy 135.5 91.5) (xy 151 91.5) (xy 151 95)
				(xy 154 95) (xy 154 92) (xy 159.5 92) (xy 159.5 98.5) (xy 162.585 98.5) (xy 162.5 89.5) (xy 133.5 89.5)
			)
		)
	)
	(zone
		(net 1)
		(net_name "GND")
		(layer "B.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.2)
			(thermal_bridge_width 0.6)
		)
		(polygon
			(pts
				(xy 129.5 86.5) (xy 168 86.5) (xy 168 104) (xy 129.5 104)
			)
		)
	)
	(embedded_fonts no)
)
