(kicad_pcb
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(general
		(thickness 1.6)
		(legacy_teardrops no)
	)
	(paper "A4")
	(layers
		(0 "F.Cu" signal)
		(2 "B.Cu" signal)
		(9 "F.Adhes" user "F.Adhesive")
		(11 "B.Adhes" user "B.Adhesive")
		(13 "F.Paste" user)
		(15 "B.Paste" user)
		(5 "F.SilkS" user "F.Silkscreen")
		(7 "B.SilkS" user "B.Silkscreen")
		(1 "F.Mask" user)
		(3 "B.Mask" user)
		(17 "Dwgs.User" user "User.Drawings")
		(19 "Cmts.User" user "User.Comments")
		(21 "Eco1.User" user "User.Eco1")
		(23 "Eco2.User" user "User.Eco2")
		(25 "Edge.Cuts" user)
		(27 "Margin" user)
		(31 "F.CrtYd" user "F.Courtyard")
		(29 "B.CrtYd" user "B.Courtyard")
		(35 "F.Fab" user)
		(33 "B.Fab" user)
		(39 "User.1" user)
		(41 "User.2" user)
		(43 "User.3" user)
		(45 "User.4" user)
	)
	(setup
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(tenting front back)
		(aux_axis_origin 72.1 50)
		(grid_origin 72.1 50)
		(pcbplotparams
			(layerselection 0x00000000_00000000_55555555_5755557f)
			(plot_on_all_layers_selection 0x00000000_00000000_00000000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 4)
			(plotframeref no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(pdf_metadata yes)
			(pdf_single_document no)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plot_black_and_white yes)
			(sketchpadsonfab no)
			(plotpadnumbers no)
			(hidednponfab no)
			(sketchdnponfab yes)
			(crossoutdnponfab yes)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 0)
			(scaleselection 1)
			(outputdirectory "")
		)
	)
	(net 0 "")
	(net 1 "PWM")
	(net 2 "GND")
	(net 3 "Net-(C2-Pad1)")
	(net 4 "MIC")
	(net 5 "ADC0")
	(net 6 "SP")
	(net 7 "Net-(D1-Pad2)")
	(net 8 "LED_GND")
	(net 9 "Net-(D2-Pad2)")
	(net 10 "Net-(D3-Pad2)")
	(net 11 "Net-(D4-Pad2)")
	(net 12 "+3V3")
	(net 13 "PTT_R")
	(net 14 "TX0")
	(net 15 "RX0")
	(net 16 "Net-(Q1-B)")
	(net 17 "PTT")
	(net 18 "CON")
	(net 19 "STA")
	(net 20 "CDT")
	(net 21 "unconnected-(U1-GPIO2-Pad4)")
	(net 22 "unconnected-(U1-GPIO21-Pad27)")
	(net 23 "unconnected-(U1-GPIO22-Pad29)")
	(net 24 "unconnected-(U1-GPIO19-Pad25)")
	(net 25 "RX1")
	(net 26 "unconnected-(U1-ADC_VREF-Pad35)")
	(net 27 "unconnected-(U1-VSYS-Pad39)")
	(net 28 "unconnected-(U1-GPIO27_ADC1-Pad32)_1")
	(net 29 "unconnected-(U1-GPIO3-Pad5)")
	(net 30 "unconnected-(U1-SWCLK-Pad41)")
	(net 31 "+5V")
	(net 32 "unconnected-(U1-RUN-Pad30)")
	(net 33 "unconnected-(U1-3V3_EN-Pad37)")
	(net 34 "unconnected-(U1-GPIO13-Pad17)_1")
	(net 35 "unconnected-(U1-GND-Pad8)")
	(net 36 "TX1")
	(net 37 "unconnected-(U1-AGND-Pad33)")
	(net 38 "unconnected-(U1-GPIO28_ADC2-Pad34)_1")
	(net 39 "unconnected-(U1-GND-Pad18)_1")
	(net 40 "unconnected-(U1-SWDIO-Pad43)_1")
	(net 41 "unconnected-(U1-GPIO9-Pad12)_1")
	(net 42 "unconnected-(U1-GPIO8-Pad11)")
	(net 43 "unconnected-(U1-GPIO7-Pad10)")
	(net 44 "unconnected-(U1-GPIO20-Pad26)")
	(net 45 "unconnected-(U1-GPIO6-Pad9)_1")
	(net 46 "Net-(C1-Pad1)")
	(net 47 "OPT2")
	(net 48 "OPT1")
	(net 49 "unconnected-(U1-GPIO6-Pad9)")
	(net 50 "unconnected-(U1-GPIO28_ADC2-Pad34)")
	(net 51 "unconnected-(U1-GPIO2-Pad4)_1")
	(net 52 "unconnected-(U1-GPIO7-Pad10)_1")
	(net 53 "unconnected-(U1-GND-Pad18)")
	(net 54 "unconnected-(U1-GPIO9-Pad12)")
	(net 55 "unconnected-(U1-ADC_VREF-Pad35)_1")
	(net 56 "unconnected-(U1-GPIO21-Pad27)_1")
	(net 57 "unconnected-(U1-GPIO27_ADC1-Pad32)")
	(net 58 "unconnected-(U1-GPIO3-Pad5)_1")
	(net 59 "unconnected-(U1-GPIO22-Pad29)_1")
	(net 60 "unconnected-(U1-SWCLK-Pad41)_1")
	(net 61 "unconnected-(U1-RUN-Pad30)_1")
	(net 62 "unconnected-(U1-GPIO8-Pad11)_1")
	(net 63 "unconnected-(U1-3V3_EN-Pad37)_1")
	(net 64 "unconnected-(U1-GPIO13-Pad17)")
	(net 65 "unconnected-(U1-VSYS-Pad39)_1")
	(net 66 "unconnected-(U1-GND-Pad8)_1")
	(net 67 "unconnected-(U1-AGND-Pad33)_1")
	(net 68 "unconnected-(U1-GPIO19-Pad25)_1")
	(net 69 "unconnected-(U1-SWDIO-Pad43)")
	(net 70 "OPT3")
	(footprint "LED_THT:LED_D3.0mm_Horizontal_O1.27mm_Z2.0mm"
		(layer "F.Cu")
		(at 77.18 86.83 -90)
		(descr "LED, diameter 3.0mm, horizontal offset 1.27mm, z-position of LED center 2.0mm, 2 pins, generated by kicad-footprint-generator")
		(tags "LED")
		(property "Reference" "D1"
			(at -1.83 3.08 180)
			(layer "F.SilkS")
		)
		(property "Value" "LED_3mm"
			(at 1.27 7.63 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "3mm diameter small LED"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "LED_D3.0mm_Clear LED_D3.0mm_Horizontal_O1.27mm_Z2.0mm LED_D3.0mm_Horizontal_O3.81mm_Z2.0mm LED_D3.0mm_Horizontal_O6.35mm_Z2.0mm")
		(sheetname "/")
		(sheetfile "pcb.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 1.27 3.12 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 270)
			(size 1.8 1.8)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 8 "LED_GND")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 2.54 0 270)
			(size 1.8 1.8)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 7 "Net-(D1-Pad2)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/LED_THT.3dshapes/LED_D3.0mm_Horizontal_O1.27mm_Z2.0mm.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal"
		(layer "F.Cu")
		(at 87.86 105.55)
		(descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=5.08mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 5.08mm 0.167W length 3.6mm diameter 1.6mm")
		(property "Reference" "R10"
			(at 2.54 -1.92 0)
			(layer "F.SilkS")
		)
		(property "Value" "100"
			(at 2.54 1.92 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "pcb.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 2.54 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1.4 1.4)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 46 "Net-(C1-Pad1)")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 5.08 0)
			(size 1.4 1.4)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "PWM")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MountingHole:MountingHole_3.2mm_M3_ISO14580"
		(layer "F.Cu")
		(at 77.18 116.04)
		(descr "Mounting Hole 3.2mm, M3, no annular, generated by kicad-footprint-generator mountinghole.py")
		(tags "mountinghole M3 ISO14580")
		(property "Reference" " "
			(at 0 -3.7 0)
			(layer "F.SilkS")
		)
		(property "Value" "MountingHole_3.2mm_M3_ISO14580"
			(at 25.52 -9.04 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 3.2 3.2)
			(drill 3.2)
			(layers "*.Cu" "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "Button_Switch_THT:SW_DIP_SPSTx04_Piano_CTS_Series194-4MSTN_W7.62mm_P2.54mm"
		(layer "F.Cu")
		(at 97.5 118.58 90)
		(descr "4x-dip-switch SPST CTS_Series194-4MSTN, Piano, row spacing 7.62 mm (300 mils), body size  (see https://www.ctscorp.com/wp-content/uploads/194-195.pdf)")
		(tags "DIP Switch SPST Piano 7.62mm 300mil")
		(property "Reference" "SW1"
			(at 3.81 -3.42 90)
			(layer "F.SilkS")
		)
		(property "Value" "SW_DIP_x04"
			(at 3.81 11.04 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "4x DIP Switch, Single Pole Single Throw (SPST) switch, small symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SW?DIP?x4*")
		(sheetname "/")
		(sheetfile "pcb.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 3.81 3.81 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole roundrect
			(at 0 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.15625)
			(net 2 "GND")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 0 2.54 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pintype "passive")
		)
		(pad "3" thru_hole circle
			(at 0 5.08 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pintype "passive")
		)
		(pad "4" thru_hole circle
			(at 0 7.62 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pintype "passive")
		)
		(pad "5" thru_hole circle
			(at 7.62 7.62 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 8 "LED_GND")
			(pintype "passive")
		)
		(pad "6" thru_hole circle
			(at 7.62 5.08 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 70 "OPT3")
			(pintype "passive")
		)
		(pad "7" thru_hole circle
			(at 7.62 2.54 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 47 "OPT2")
			(pintype "passive")
		)
		(pad "8" thru_hole circle
			(at 7.62 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 48 "OPT1")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Button_Switch_THT.3dshapes/SW_DIP_SPSTx04_Piano_CTS_Series194-4MSTN_W7.62mm_P2.54mm.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 90)
			)
		)
	)
	(footprint "Capacitor_THT:C_Disc_D3.0mm_W2.0mm_P2.50mm"
		(layer "F.Cu")
		(at 86.1 61.5 -90)
		(descr "C, Disc series, Radial, pin pitch=2.50mm, diameter*width=3*2mm^2, Capacitor")
		(tags "C Disc series Radial pin pitch 2.50mm diameter 3mm width 2mm Capacitor")
		(property "Reference" "C2"
			(at 4.5 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "100nF"
			(at 1.25 2.25 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "pcb.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 1.25 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "Net-(C2-Pad1)")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 2.5 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "MIC")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D3.0mm_W2.0mm_P2.50mm.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal"
		(layer "F.Cu")
		(at 119.09 80.48 -90)
		(descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=5.08mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 5.08mm 0.167W length 3.6mm diameter 1.6mm")
		(property "Reference" "R3"
			(at 7.32 -0.01 90)
			(layer "F.SilkS")
		)
		(property "Value" "10k"
			(at 2.54 1.92 270)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "pcb.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 2.54 0 270)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 270)
			(size 1.4 1.4)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "ADC0")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 5.08 0 270)
			(size 1.4 1.4)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:PJ-307"
		(layer "F.Cu")
		(at 79.72 65.24)
		(descr "https://datasheet.lcsc.com/szlcsc/Boom-Precision-Elec-PJ-307C_C16684.pdf")
		(property "Reference" "J2"
			(at 1.88 -7.24 180)
			(layer "F.SilkS")
		)
		(property "Value" "AudioJack2"
			(at -5.12 -0.24 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Audio Jack, 3 Poles (Stereo / TRS)"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Jack*")
		(sheetname "/")
		(sheetfile "pcb.kicad_sch")
		(attr through_hole)
		(pad "" np_thru_hole circle
			(at -5.5 -5)
			(size 1.2 1.2)
			(drill 0.762)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at -5.5 5)
			(size 1.2 1.2)
			(drill 0.762)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at -3 -5)
			(size 1.2 1.2)
			(drill 0.762)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at -3 5)
			(size 1.2 1.2)
			(drill 0.762)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 2 0)
			(size 1.2 1.2)
			(drill 0.762)
			(layers "*.Cu" "*.Mask")
		)
		(pad "R" thru_hole oval
			(at 2 -5)
			(size 2.5 1.8)
			(drill oval 1.7 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 14 "TX0")
			(pintype "passive")
		)
		(pad "RN" thru_hole oval
			(at 2 -2.5)
			(size 2.5 1.8)
			(drill oval 1.7 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "S" thru_hole oval
			(at -3 0 90)
			(size 2.5 1.8)
			(drill oval 1.7 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pintype "passive")
		)
		(pad "T" thru_hole oval
			(at 2 5)
			(size 2.5 1.8)
			(drill oval 1.7 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 15 "RX0")
			(pintype "passive")
		)
		(pad "TN" thru_hole oval
			(at 2 2.5)
			(size 2.5 1.8)
			(drill oval 1.7 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_Audio.3dshapes/Jack_3.5mm_CUI_SJ1-3525N_Horizontal.step"
			(offset
				(xyz -3 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 180 180 -90)
			)
		)
	)
	(footprint "Connector_Audio:Jack_3.5mm_PJ320D_Horizontal"
		(layer "F.Cu")
		(at 78.435 78.65)
		(descr "Headphones with microphone connector, 3.5mm, 4 pins (http://www.qingpu-electronics.com/en/products/WQP-PJ320D-72.html)")
		(tags "3.5mm jack mic microphone phones headphones 4pins audio plug")
		(property "Reference" "J1"
			(at -7 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "AudioJack1"
			(at -0.835 3.85 180)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Audio Jack, 4 Poles (TRRS)"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Jack*")
		(sheetname "/")
		(sheetfile "pcb.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at -0.835 0.1 90)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole circle
			(at -4.775 0)
			(size 1.5 1.5)
			(drill 1.5)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 2.225 0)
			(size 1.5 1.5)
			(drill 1.5)
			(layers "*.Cu" "*.Mask")
		)
		(pad "R1" smd rect
			(at -0.175 -3.25)
			(size 1.2 2.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 4 "MIC")
			(pintype "passive")
		)
		(pad "R2" smd rect
			(at -3.175 -3.25)
			(size 1.2 2.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 13 "PTT_R")
			(pintype "passive")
		)
		(pad "S" smd rect
			(at 4.925 3.25)
			(size 1.2 2.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "GND")
			(pintype "passive")
		)
		(pad "T" smd rect
			(at 3.825 -3.25)
			(size 1.2 2.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 6 "SP")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KIPRJMOD}/models/PJ320D.STEP"
			(offset
				(xyz -1.2 0 -11.5)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -0 -0 -0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal"
		(layer "F.Cu")
		(at 82.09 72.5 180)
		(descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=5.08mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 5.08mm 0.167W length 3.6mm diameter 1.6mm")
		(property "Reference" "R9"
			(at -2.41 0.1 180)
			(layer "F.SilkS")
		)
		(property "Value" "R"
			(at 2.54 1.92 180)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "pcb.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 2.54 0 180)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 180)
			(size 1.4 1.4)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "MIC")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 5.08 0 180)
			(size 1.4 1.4)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 13 "PTT_R")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_THT:C_Disc_D3.0mm_W2.0mm_P2.50mm"
		(layer "F.Cu")
		(at 86.6 77.5 -90)
		(descr "C, Disc series, Radial, pin pitch=2.50mm, diameter*width=3*2mm^2, Capacitor")
		(tags "C Disc series Radial pin pitch 2.50mm diameter 3mm width 2mm Capacitor")
		(property "Reference" "C1"
			(at -2 0 180)
			(layer "F.SilkS")
		)
		(property "Value" "100nF"
			(at -2.5 -0.5 180)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "pcb.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 1.25 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 46 "Net-(C1-Pad1)")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 2.5 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D3.0mm_W2.0mm_P2.50mm.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:RPi_Pico_SMD_TH"
		(layer "F.Cu")
		(at 102.58 76)
		(descr "Through hole straight pin header, 2x20, 2.54mm pitch, double rows")
		(tags "Through hole pin header THT 2x20 2.54mm double row")
		(property "Reference" "U1"
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "Pico"
			(at 0 2.159 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "pcb.kicad_sch")
		(attr through_hole)
		(fp_text user "GP4"
			(at -12.8 -11.43 45)
			(layer "F.SilkS")
		)
		(fp_text user "GP27"
			(at 13.054 -3.8 45)
			(layer "F.SilkS")
		)
		(fp_text user "VSYS"
			(at 13.2 -21.59 45)
			(layer "F.SilkS")
		)
		(fp_text user "GP19"
			(at 13.054 13.97 45)
			(layer "F.SilkS")
		)
		(fp_text user "GP2"
			(at -12.9 -16.51 45)
			(layer "F.SilkS")
		)
		(fp_text user "SWCLK"
			(at -5.7 26.2 0)
			(layer "F.SilkS")
		)
		(fp_text user "GP12"
			(at -13.2 13.97 45)
			(layer "F.SilkS")
		)
		(fp_text user "GP21"
			(at 13.054 8.9 45)
			(layer "F.SilkS")
		)
		(fp_text user "GND"
			(at -12.8 -6.35 45)
			(layer "F.SilkS")
		)
		(fp_text user "GP17"
			(at 13.054 21.59 45)
			(layer "F.SilkS")
		)
		(fp_text user "VBUS"
			(at 13.3 -24.2 45)
			(layer "F.SilkS")
		)
		(fp_text user "GP22"
			(at 13.054 3.81 45)
			(layer "F.SilkS")
		)
		(fp_text user "GP16"
			(at 13.054 24.13 45)
			(layer "F.SilkS")
		)
		(fp_text user "GND"
			(at 12.8 6.35 45)
			(layer "F.SilkS")
		)
		(fp_text user "GP13"
			(at -13.054 16.51 45)
			(layer "F.SilkS")
		)
		(fp_text user "3V3"
			(at 12.9 -13.9 45)
			(layer "F.SilkS")
		)
		(fp_text user "GP14"
			(at -13.1 21.59 45)
			(layer "F.SilkS")
		)
		(fp_text user "GP3"
			(at -12.8 -13.97 45)
			(layer "F.SilkS")
		)
		(fp_text user "GP9"
			(at -12.8 3.81 45)
			(layer "F.SilkS")
		)
		(fp_text user "GP1"
			(at -12.9 -21.6 45)
			(layer "F.SilkS")
		)
		(fp_text user "GND"
			(at 12.8 19.05 45)
			(layer "F.SilkS")
		)
		(fp_text user "GP6"
			(at -12.8 -3.81 45)
			(layer "F.SilkS")
		)
		(fp_text user "GP5"
			(at -12.8 -8.89 45)
			(layer "F.SilkS")
		)
		(fp_text user "RUN"
			(at 13 1.27 45)
			(layer "F.SilkS")
		)
		(fp_text user "GND"
			(at -12.8 19.05 45)
			(layer "F.SilkS")
		)
		(fp_text user "3V3_EN"
			(at 13.7 -17.2 45)
			(layer "F.SilkS")
		)
		(fp_text user "GP10"
			(at -13.054 8.89 45)
			(layer "F.SilkS")
		)
		(fp_text user "GP18"
			(at 13.054 16.51 45)
			(layer "F.SilkS")
		)
		(fp_text user "GP20"
			(at 13.054 11.43 45)
			(layer "F.SilkS")
		)
		(fp_text user "GP15"
			(at -13.054 24.13 45)
			(layer "F.SilkS")
		)
		(fp_text user "AGND"
			(at 13.054 -6.35 45)
			(layer "F.SilkS")
		)
		(fp_text user "GND"
			(at -12.8 -19.05 45)
			(layer "F.SilkS")
		)
		(fp_text user "GND"
			(at -12.8 6.35 45)
			(layer "F.SilkS")
		)
		(fp_text user "SWDIO"
			(at 5.6 26.2 0)
			(layer "F.SilkS")
		)
		(fp_text user "GP26"
			(at 13.054 -1.27 45)
			(layer "F.SilkS")
		)
		(fp_text user "GP0"
			(at -12.8 -24.13 45)
			(layer "F.SilkS")
		)
		(fp_text user "GP8"
			(at -12.8 1.27 45)
			(layer "F.SilkS")
		)
		(fp_text user "ADC_VREF"
			(at 14 -12.5 45)
			(layer "F.SilkS")
		)
		(fp_text user "GP7"
			(at -12.7 -1.3 45)
			(layer "F.SilkS")
		)
		(fp_text user "GP11"
			(at -13.2 11.43 45)
			(layer "F.SilkS")
		)
		(fp_text user "GND"
			(at 12.8 -19.05 45)
			(layer "F.SilkS")
		)
		(fp_text user "GP28"
			(at 13.054 -9.144 45)
			(layer "F.SilkS")
		)
		(fp_text user "Copper Keepouts shown on Dwgs layer"
			(at 0.1 -30.2 0)
			(layer "Cmts.User")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole oval
			(at -2.725 -24)
			(size 1.8 1.8)
			(drill 1.8)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole oval
			(at -2.425 -20.97)
			(size 1.5 1.5)
			(drill 1.5)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole oval
			(at 2.425 -20.97)
			(size 1.5 1.5)
			(drill 1.5)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole oval
			(at 2.725 -24)
			(size 1.8 1.8)
			(drill 1.8)
			(layers "*.Cu" "*.Mask")
		)
		(pad "1" thru_hole oval
			(at -8.89 -24.13)
			(size 1.7 1.7)
			(drill 1.02)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 14 "TX0")
			(pinfunction "GPIO0")
			(pintype "bidirectional")
		)
		(pad "1" smd rect
			(at -8.89 -24.13)
			(size 3.5 1.7)
			(drill
				(offset -0.9 0)
			)
			(layers "F.Cu" "F.Mask")
			(net 14 "TX0")
			(pinfunction "GPIO0")
			(pintype "bidirectional")
		)
		(pad "2" thru_hole oval
			(at -8.89 -21.59)
			(size 1.7 1.7)
			(drill 1.02)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 15 "RX0")
			(pinfunction "GPIO1")
			(pintype "bidirectional")
		)
		(pad "2" smd rect
			(at -8.89 -21.59)
			(size 3.5 1.7)
			(drill
				(offset -0.9 0)
			)
			(layers "F.Cu" "F.Mask")
			(net 15 "RX0")
			(pinfunction "GPIO1")
			(pintype "bidirectional")
		)
		(pad "3" thru_hole rect
			(at -8.89 -19.05)
			(size 1.7 1.7)
			(drill 1.02)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "3" smd rect
			(at -8.89 -19.05)
			(size 3.5 1.7)
			(drill
				(offset -0.9 0)
			)
			(layers "F.Cu" "F.Mask")
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "4" thru_hole oval
			(at -8.89 -16.51)
			(size 1.7 1.7)
			(drill 1.02)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 21 "unconnected-(U1-GPIO2-Pad4)")
			(pinfunction "GPIO2")
			(pintype "bidirectional+no_connect")
		)
		(pad "4" smd rect
			(at -8.89 -16.51)
			(size 3.5 1.7)
			(drill
				(offset -0.9 0)
			)
			(layers "F.Cu" "F.Mask")
			(net 51 "unconnected-(U1-GPIO2-Pad4)_1")
			(pinfunction "GPIO2")
			(pintype "bidirectional+no_connect")
		)
		(pad "5" thru_hole oval
			(at -8.89 -13.97)
			(size 1.7 1.7)
			(drill 1.02)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 58 "unconnected-(U1-GPIO3-Pad5)_1")
			(pinfunction "GPIO3")
			(pintype "bidirectional+no_connect")
		)
		(pad "5" smd rect
			(at -8.89 -13.97)
			(size 3.5 1.7)
			(drill
				(offset -0.9 0)
			)
			(layers "F.Cu" "F.Mask")
			(net 29 "unconnected-(U1-GPIO3-Pad5)")
			(pinfunction "GPIO3")
			(pintype "bidirectional+no_connect")
		)
		(pad "6" thru_hole oval
			(at -8.89 -11.43)
			(size 1.7 1.7)
			(drill 1.02)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 36 "TX1")
			(pinfunction "GPIO4")
			(pintype "bidirectional")
		)
		(pad "6" smd rect
			(at -8.89 -11.43)
			(size 3.5 1.7)
			(drill
				(offset -0.9 0)
			)
			(layers "F.Cu" "F.Mask")
			(net 36 "TX1")
			(pinfunction "GPIO4")
			(pintype "bidirectional")
		)
		(pad "7" thru_hole oval
			(at -8.89 -8.89)
			(size 1.7 1.7)
			(drill 1.02)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 25 "RX1")
			(pinfunction "GPIO5")
			(pintype "bidirectional")
		)
		(pad "7" smd rect
			(at -8.89 -8.89)
			(size 3.5 1.7)
			(drill
				(offset -0.9 0)
			)
			(layers "F.Cu" "F.Mask")
			(net 25 "RX1")
			(pinfunction "GPIO5")
			(pintype "bidirectional")
		)
		(pad "8" thru_hole rect
			(at -8.89 -6.35)
			(size 1.7 1.7)
			(drill 1.02)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 66 "unconnected-(U1-GND-Pad8)_1")
			(pinfunction "GND")
			(pintype "power_in+no_connect")
		)
		(pad "8" smd rect
			(at -8.89 -6.35)
			(size 3.5 1.7)
			(drill
				(offset -0.9 0)
			)
			(layers "F.Cu" "F.Mask")
			(net 35 "unconnected-(U1-GND-Pad8)")
			(pinfunction "GND")
			(pintype "power_in+no_connect")
		)
		(pad "9" thru_hole oval
			(at -8.89 -3.81)
			(size 1.7 1.7)
			(drill 1.02)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 45 "unconnected-(U1-GPIO6-Pad9)_1")
			(pinfunction "GPIO6")
			(pintype "bidirectional+no_connect")
		)
		(pad "9" smd rect
			(at -8.89 -3.81)
			(size 3.5 1.7)
			(drill
				(offset -0.9 0)
			)
			(layers "F.Cu" "F.Mask")
			(net 49 "unconnected-(U1-GPIO6-Pad9)")
			(pinfunction "GPIO6")
			(pintype "bidirectional+no_connect")
		)
		(pad "10" thru_hole oval
			(at -8.89 -1.27)
			(size 1.7 1.7)
			(drill 1.02)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 43 "unconnected-(U1-GPIO7-Pad10)")
			(pinfunction "GPIO7")
			(pintype "bidirectional+no_connect")
		)
		(pad "10" smd rect
			(at -8.89 -1.27)
			(size 3.5 1.7)
			(drill
				(offset -0.9 0)
			)
			(layers "F.Cu" "F.Mask")
			(net 52 "unconnected-(U1-GPIO7-Pad10)_1")
			(pinfunction "GPIO7")
			(pintype "bidirectional+no_connect")
		)
		(pad "11" thru_hole oval
			(at -8.89 1.27)
			(size 1.7 1.7)
			(drill 1.02)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 42 "unconnected-(U1-GPIO8-Pad11)")
			(pinfunction "GPIO8")
			(pintype "bidirectional+no_connect")
		)
		(pad "11" smd rect
			(at -8.89 1.27)
			(size 3.5 1.7)
			(drill
				(offset -0.9 0)
			)
			(layers "F.Cu" "F.Mask")
			(net 62 "unconnected-(U1-GPIO8-Pad11)_1")
			(pinfunction "GPIO8")
			(pintype "bidirectional+no_connect")
		)
		(pad "12" thru_hole oval
			(at -8.89 3.81)
			(size 1.7 1.7)
			(drill 1.02)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 54 "unconnected-(U1-GPIO9-Pad12)")
			(pinfunction "GPIO9")
			(pintype "bidirectional+no_connect")
		)
		(pad "12" smd rect
			(at -8.89 3.81)
			(size 3.5 1.7)
			(drill
				(offset -0.9 0)
			)
			(layers "F.Cu" "F.Mask")
			(net 41 "unconnected-(U1-GPIO9-Pad12)_1")
			(pinfunction "GPIO9")
			(pintype "bidirectional+no_connect")
		)
		(pad "13" thru_hole rect
			(at -8.89 6.35)
			(size 1.7 1.7)
			(drill 1.02)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "13" smd rect
			(at -8.89 6.35)
			(size 3.5 1.7)
			(drill
				(offset -0.9 0)
			)
			(layers "F.Cu" "F.Mask")
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "14" thru_hole oval
			(at -8.89 8.89)
			(size 1.7 1.7)
			(drill 1.02)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "PWM")
			(pinfunction "GPIO10")
			(pintype "bidirectional")
		)
		(pad "14" smd rect
			(at -8.89 8.89)
			(size 3.5 1.7)
			(drill
				(offset -0.9 0)
			)
			(layers "F.Cu" "F.Mask")
			(net 1 "PWM")
			(pinfunction "GPIO10")
			(pintype "bidirectional")
		)
		(pad "15" thru_hole oval
			(at -8.89 11.43)
			(size 1.7 1.7)
			(drill 1.02)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 17 "PTT")
			(pinfunction "GPIO11")
			(pintype "bidirectional")
		)
		(pad "15" smd rect
			(at -8.89 11.43)
			(size 3.5 1.7)
			(drill
				(offset -0.9 0)
			)
			(layers "F.Cu" "F.Mask")
			(net 17 "PTT")
			(pinfunction "GPIO11")
			(pintype "bidirectional")
		)
		(pad "16" thru_hole oval
			(at -8.89 13.97)
			(size 1.7 1.7)
			(drill 1.02)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 20 "CDT")
			(pinfunction "GPIO12")
			(pintype "bidirectional")
		)
		(pad "16" smd rect
			(at -8.89 13.97)
			(size 3.5 1.7)
			(drill
				(offset -0.9 0)
			)
			(layers "F.Cu" "F.Mask")
			(net 20 "CDT")
			(pinfunction "GPIO12")
			(pintype "bidirectional")
		)
		(pad "17" thru_hole oval
			(at -8.89 16.51)
			(size 1.7 1.7)
			(drill 1.02)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 64 "unconnected-(U1-GPIO13-Pad17)")
			(pinfunction "GPIO13")
			(pintype "bidirectional+no_connect")
		)
		(pad "17" smd rect
			(at -8.89 16.51)
			(size 3.5 1.7)
			(drill
				(offset -0.9 0)
			)
			(layers "F.Cu" "F.Mask")
			(net 34 "unconnected-(U1-GPIO13-Pad17)_1")
			(pinfunction "GPIO13")
			(pintype "bidirectional+no_connect")
		)
		(pad "18" thru_hole rect
			(at -8.89 19.05)
			(size 1.7 1.7)
			(drill 1.02)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 39 "unconnected-(U1-GND-Pad18)_1")
			(pinfunction "GND")
			(pintype "power_in+no_connect")
		)
		(pad "18" smd rect
			(at -8.89 19.05)
			(size 3.5 1.7)
			(drill
				(offset -0.9 0)
			)
			(layers "F.Cu" "F.Mask")
			(net 53 "unconnected-(U1-GND-Pad18)")
			(pinfunction "GND")
			(pintype "power_in+no_connect")
		)
		(pad "19" thru_hole oval
			(at -8.89 21.59)
			(size 1.7 1.7)
			(drill 1.02)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 18 "CON")
			(pinfunction "GPIO14")
			(pintype "bidirectional")
		)
		(pad "19" smd rect
			(at -8.89 21.59)
			(size 3.5 1.7)
			(drill
				(offset -0.9 0)
			)
			(layers "F.Cu" "F.Mask")
			(net 18 "CON")
			(pinfunction "GPIO14")
			(pintype "bidirectional")
		)
		(pad "20" thru_hole oval
			(at -8.89 24.13)
			(size 1.7 1.7)
			(drill 1.02)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 19 "STA")
			(pinfunction "GPIO15")
			(pintype "bidirectional")
		)
		(pad "20" smd rect
			(at -8.89 24.13)
			(size 3.5 1.7)
			(drill
				(offset -0.9 0)
			)
			(layers "F.Cu" "F.Mask")
			(net 19 "STA")
			(pinfunction "GPIO15")
			(pintype "bidirectional")
		)
		(pad "21" thru_hole oval
			(at 8.89 24.13)
			(size 1.7 1.7)
			(drill 1.02)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 48 "OPT1")
			(pinfunction "GPIO16")
			(pintype "bidirectional")
		)
		(pad "21" smd rect
			(at 8.89 24.13)
			(size 3.5 1.7)
			(drill
				(offset 0.9 0)
			)
			(layers "F.Cu" "F.Mask")
			(net 48 "OPT1")
			(pinfunction "GPIO16")
			(pintype "bidirectional")
		)
		(pad "22" thru_hole oval
			(at 8.89 21.59)
			(size 1.7 1.7)
			(drill 1.02)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 47 "OPT2")
			(pinfunction "GPIO17")
			(pintype "bidirectional")
		)
		(pad "22" smd rect
			(at 8.89 21.59)
			(size 3.5 1.7)
			(drill
				(offset 0.9 0)
			)
			(layers "F.Cu" "F.Mask")
			(net 47 "OPT2")
			(pinfunction "GPIO17")
			(pintype "bidirectional")
		)
		(pad "23" thru_hole rect
			(at 8.89 19.05)
			(size 1.7 1.7)
			(drill 1.02)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "23" smd rect
			(at 8.89 19.05)
			(size 3.5 1.7)
			(drill
				(offset 0.9 0)
			)
			(layers "F.Cu" "F.Mask")
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "24" thru_hole oval
			(at 8.89 16.51)
			(size 1.7 1.7)
			(drill 1.02)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 70 "OPT3")
			(pinfunction "GPIO18")
			(pintype "bidirectional")
		)
		(pad "24" smd rect
			(at 8.89 16.51)
			(size 3.5 1.7)
			(drill
				(offset 0.9 0)
			)
			(layers "F.Cu" "F.Mask")
			(net 70 "OPT3")
			(pinfunction "GPIO18")
			(pintype "bidirectional")
		)
		(pad "25" thru_hole oval
			(at 8.89 13.97)
			(size 1.7 1.7)
			(drill 1.02)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 24 "unconnected-(U1-GPIO19-Pad25)")
			(pinfunction "GPIO19")
			(pintype "bidirectional+no_connect")
		)
		(pad "25" smd rect
			(at 8.89 13.97)
			(size 3.5 1.7)
			(drill
				(offset 0.9 0)
			)
			(layers "F.Cu" "F.Mask")
			(net 68 "unconnected-(U1-GPIO19-Pad25)_1")
			(pinfunction "GPIO19")
			(pintype "bidirectional+no_connect")
		)
		(pad "26" thru_hole oval
			(at 8.89 11.43)
			(size 1.7 1.7)
			(drill 1.02)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 44 "unconnected-(U1-GPIO20-Pad26)")
			(pinfunction "GPIO20")
			(pintype "bidirectional")
		)
		(pad "26" smd rect
			(at 8.89 11.43)
			(size 3.5 1.7)
			(drill
				(offset 0.9 0)
			)
			(layers "F.Cu" "F.Mask")
			(net 44 "unconnected-(U1-GPIO20-Pad26)")
			(pinfunction "GPIO20")
			(pintype "bidirectional")
		)
		(pad "27" thru_hole oval
			(at 8.89 8.89)
			(size 1.7 1.7)
			(drill 1.02)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 22 "unconnected-(U1-GPIO21-Pad27)")
			(pinfunction "GPIO21")
			(pintype "bidirectional+no_connect")
		)
		(pad "27" smd rect
			(at 8.89 8.89)
			(size 3.5 1.7)
			(drill
				(offset 0.9 0)
			)
			(layers "F.Cu" "F.Mask")
			(net 56 "unconnected-(U1-GPIO21-Pad27)_1")
			(pinfunction "GPIO21")
			(pintype "bidirectional+no_connect")
		)
		(pad "28" thru_hole rect
			(at 8.89 6.35)
			(size 1.7 1.7)
			(drill 1.02)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "28" smd rect
			(at 8.89 6.35)
			(size 3.5 1.7)
			(drill
				(offset 0.9 0)
			)
			(layers "F.Cu" "F.Mask")
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "29" thru_hole oval
			(at 8.89 3.81)
			(size 1.7 1.7)
			(drill 1.02)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 23 "unconnected-(U1-GPIO22-Pad29)")
			(pinfunction "GPIO22")
			(pintype "bidirectional+no_connect")
		)
		(pad "29" smd rect
			(at 8.89 3.81)
			(size 3.5 1.7)
			(drill
				(offset 0.9 0)
			)
			(layers "F.Cu" "F.Mask")
			(net 59 "unconnected-(U1-GPIO22-Pad29)_1")
			(pinfunction "GPIO22")
			(pintype "bidirectional+no_connect")
		)
		(pad "30" thru_hole oval
			(at 8.89 1.27)
			(size 1.7 1.7)
			(drill 1.02)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 61 "unconnected-(U1-RUN-Pad30)_1")
			(pinfunction "RUN")
			(pintype "input+no_connect")
		)
		(pad "30" smd rect
			(at 8.89 1.27)
			(size 3.5 1.7)
			(drill
				(offset 0.9 0)
			)
			(layers "F.Cu" "F.Mask")
			(net 32 "unconnected-(U1-RUN-Pad30)")
			(pinfunction "RUN")
			(pintype "input+no_connect")
		)
		(pad "31" thru_hole oval
			(at 8.89 -1.27)
			(size 1.7 1.7)
			(drill 1.02)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "ADC0")
			(pinfunction "GPIO26_ADC0")
			(pintype "bidirectional")
		)
		(pad "31" smd rect
			(at 8.89 -1.27)
			(size 3.5 1.7)
			(drill
				(offset 0.9 0)
			)
			(layers "F.Cu" "F.Mask")
			(net 5 "ADC0")
			(pinfunction "GPIO26_ADC0")
			(pintype "bidirectional")
		)
		(pad "32" thru_hole oval
			(at 8.89 -3.81)
			(size 1.7 1.7)
			(drill 1.02)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 57 "unconnected-(U1-GPIO27_ADC1-Pad32)")
			(pinfunction "GPIO27_ADC1")
			(pintype "bidirectional+no_connect")
		)
		(pad "32" smd rect
			(at 8.89 -3.81)
			(size 3.5 1.7)
			(drill
				(offset 0.9 0)
			)
			(layers "F.Cu" "F.Mask")
			(net 28 "unconnected-(U1-GPIO27_ADC1-Pad32)_1")
			(pinfunction "GPIO27_ADC1")
			(pintype "bidirectional+no_connect")
		)
		(pad "33" thru_hole rect
			(at 8.89 -6.35)
			(size 1.7 1.7)
			(drill 1.02)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 67 "unconnected-(U1-AGND-Pad33)_1")
			(pinfunction "AGND")
			(pintype "power_in+no_connect")
		)
		(pad "33" smd rect
			(at 8.89 -6.35)
			(size 3.5 1.7)
			(drill
				(offset 0.9 0)
			)
			(layers "F.Cu" "F.Mask")
			(net 37 "unconnected-(U1-AGND-Pad33)")
			(pinfunction "AGND")
			(pintype "power_in+no_connect")
		)
		(pad "34" thru_hole oval
			(at 8.89 -8.89)
			(size 1.7 1.7)
			(drill 1.02)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 38 "unconnected-(U1-GPIO28_ADC2-Pad34)_1")
			(pinfunction "GPIO28_ADC2")
			(pintype "bidirectional+no_connect")
		)
		(pad "34" smd rect
			(at 8.89 -8.89)
			(size 3.5 1.7)
			(drill
				(offset 0.9 0)
			)
			(layers "F.Cu" "F.Mask")
			(net 50 "unconnected-(U1-GPIO28_ADC2-Pad34)")
			(pinfunction "GPIO28_ADC2")
			(pintype "bidirectional+no_connect")
		)
		(pad "35" thru_hole oval
			(at 8.89 -11.43)
			(size 1.7 1.7)
			(drill 1.02)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 55 "unconnected-(U1-ADC_VREF-Pad35)_1")
			(pinfunction "ADC_VREF")
			(pintype "power_in+no_connect")
		)
		(pad "35" smd rect
			(at 8.89 -11.43)
			(size 3.5 1.7)
			(drill
				(offset 0.9 0)
			)
			(layers "F.Cu" "F.Mask")
			(net 26 "unconnected-(U1-ADC_VREF-Pad35)")
			(pinfunction "ADC_VREF")
			(pintype "power_in+no_connect")
		)
		(pad "36" thru_hole oval
			(at 8.89 -13.97)
			(size 1.7 1.7)
			(drill 1.02)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 12 "+3V3")
			(pinfunction "3V3")
			(pintype "power_out")
		)
		(pad "36" smd rect
			(at 8.89 -13.97)
			(size 3.5 1.7)
			(drill
				(offset 0.9 0)
			)
			(layers "F.Cu" "F.Mask")
			(net 12 "+3V3")
			(pinfunction "3V3")
			(pintype "power_out")
		)
		(pad "37" thru_hole oval
			(at 8.89 -16.51)
			(size 1.7 1.7)
			(drill 1.02)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 33 "unconnected-(U1-3V3_EN-Pad37)")
			(pinfunction "3V3_EN")
			(pintype "input+no_connect")
		)
		(pad "37" smd rect
			(at 8.89 -16.51)
			(size 3.5 1.7)
			(drill
				(offset 0.9 0)
			)
			(layers "F.Cu" "F.Mask")
			(net 63 "unconnected-(U1-3V3_EN-Pad37)_1")
			(pinfunction "3V3_EN")
			(pintype "input+no_connect")
		)
		(pad "38" thru_hole rect
			(at 8.89 -19.05)
			(size 1.7 1.7)
			(drill 1.02)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "38" smd rect
			(at 8.89 -19.05)
			(size 3.5 1.7)
			(drill
				(offset 0.9 0)
			)
			(layers "F.Cu" "F.Mask")
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "39" thru_hole oval
			(at 8.89 -21.59)
			(size 1.7 1.7)
			(drill 1.02)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 27 "unconnected-(U1-VSYS-Pad39)")
			(pinfunction "VSYS")
			(pintype "power_in+no_connect")
		)
		(pad "39" smd rect
			(at 8.89 -21.59)
			(size 3.5 1.7)
			(drill
				(offset 0.9 0)
			)
			(layers "F.Cu" "F.Mask")
			(net 65 "unconnected-(U1-VSYS-Pad39)_1")
			(pinfunction "VSYS")
			(pintype "power_in+no_connect")
		)
		(pad "40" thru_hole oval
			(at 8.89 -24.13)
			(size 1.7 1.7)
			(drill 1.02)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 31 "+5V")
			(pinfunction "VBUS")
			(pintype "power_in")
		)
		(pad "40" smd rect
			(at 8.89 -24.13)
			(size 3.5 1.7)
			(drill
				(offset 0.9 0)
			)
			(layers "F.Cu" "F.Mask")
			(net 31 "+5V")
			(pinfunction "VBUS")
			(pintype "power_in")
		)
		(pad "41" thru_hole oval
			(at -2.54 23.9)
			(size 1.7 1.7)
			(drill 1.02)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 60 "unconnected-(U1-SWCLK-Pad41)_1")
			(pinfunction "SWCLK")
			(pintype "input+no_connect")
		)
		(pad "41" smd rect
			(at -2.54 23.9 90)
			(size 3.5 1.7)
			(drill
				(offset -0.9 0)
			)
			(layers "F.Cu" "F.Mask")
			(net 30 "unconnected-(U1-SWCLK-Pad41)")
			(pinfunction "SWCLK")
			(pintype "input+no_connect")
		)
		(pad "42" thru_hole rect
			(at 0 23.9)
			(size 1.7 1.7)
			(drill 1.02)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "42" smd rect
			(at 0 23.9 90)
			(size 3.5 1.7)
			(drill
				(offset -0.9 0)
			)
			(layers "F.Cu" "F.Mask")
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "43" thru_hole oval
			(at 2.54 23.9)
			(size 1.7 1.7)
			(drill 1.02)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 40 "unconnected-(U1-SWDIO-Pad43)_1")
			(pinfunction "SWDIO")
			(pintype "bidirectional+no_connect")
		)
		(pad "43" smd rect
			(at 2.54 23.9 90)
			(size 3.5 1.7)
			(drill
				(offset -0.9 0)
			)
			(layers "F.Cu" "F.Mask")
			(net 69 "unconnected-(U1-SWDIO-Pad43)")
			(pinfunction "SWDIO")
			(pintype "bidirectional+no_connect")
		)
		(embedded_fonts no)
		(model "${KIPRJMOD}/models/Raspberry Pi Pico-R3.STEP"
			(offset
				(xyz 0 0 8)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 -0 -0)
			)
		)
		(model "/home/codeman/projects/Raspberry Pi Pico-R3.STEP"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 -0 -0)
			)
		)
		(model "${KIPRJMOD}/models/SSW-120-01-G-S.stp"
			(offset
				(xyz 9 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 -0 90)
			)
		)
		(model "${KIPRJMOD}/models/SSW-120-01-G-S.stp"
			(offset
				(xyz -9 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 -0 -90)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal"
		(layer "F.Cu")
		(at 81.1 99)
		(descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=5.08mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 5.08mm 0.167W length 3.6mm diameter 1.6mm")
		(property "Reference" "R8"
			(at -1.6 0 90)
			(layer "F.SilkS")
		)
		(property "Value" "4.7K"
			(at 8 0 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "pcb.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 2.54 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1.4 1.4)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 16 "Net-(Q1-B)")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 5.08 0)
			(size 1.4 1.4)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Diode_THT:D_DO-35_SOD27_P7.62mm_Horizontal"
		(layer "F.Cu")
		(at 122.1 86.69 -90)
		(descr "Diode, DO-35_SOD27 series, Axial, Horizontal, pin pitch=7.62mm, length*diameter=4*2mm^2, http://www.diodes.com/_files/packages/DO-35.pdf")
		(tags "Diode DO-35_SOD27 series Axial Horizontal pin pitch 7.62mm  length 4mm diameter 2mm")
		(property "Reference" "D6"
			(at 3.81 2 90)
			(layer "F.SilkS")
		)
		(property "Value" "1N4148"
			(at 3.81 2.12 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/1N4148_1N4448.pdf"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "100V 0.15A standard switching diode, DO-35"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Device" "D"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "D*DO?35*")
		(sheetname "/")
		(sheetfile "pcb.kicad_sch")
		(attr through_hole)
		(fp_text user "K"
			(at 0 -1.8 90)
			(layer "F.SilkS")
		)
		(fp_text user "K"
			(at 0 -1.8 90)
			(layer "F.Fab")
		)
		(fp_text user "${REFERENCE}"
			(at 4.11 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole roundrect
			(at 0 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.15625)
			(net 5 "ADC0")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 7.62 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "A")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Diode_THT.3dshapes/D_DO-35_SOD27_P7.62mm_Horizontal.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MountingHole:MountingHole_3.2mm_M3_ISO14580"
		(layer "F.Cu")
		(at 120.36 55.08)
		(descr "Mounting Hole 3.2mm, M3, no annular, generated by kicad-footprint-generator mountinghole.py")
		(tags "mountinghole M3 ISO14580")
		(property "Reference" " "
			(at 0 -3.7 0)
			(layer "F.SilkS")
		)
		(property "Value" "MountingHole_3.2mm_M3_ISO14580"
			(at -4.76 8.92 270)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 3.2 3.2)
			(drill 3.2)
			(layers "*.Cu" "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal"
		(layer "F.Cu")
		(at 86.02 95.72 180)
		(descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=5.08mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 5.08mm 0.167W length 3.6mm diameter 1.6mm")
		(property "Reference" "R6"
			(at 6.72 -0.08 270)
			(layer "F.SilkS")
		)
		(property "Value" "1k"
			(at -2.08 0.22 180)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "pcb.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 2.54 0 180)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 180)
			(size 1.4 1.4)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 20 "CDT")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 5.08 0 180)
			(size 1.4 1.4)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 9 "Net-(D2-Pad2)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "LED_THT:LED_D3.0mm_Horizontal_O1.27mm_Z2.0mm"
		(layer "F.Cu")
		(at 77.18 93.18 -90)
		(descr "LED, diameter 3.0mm, horizontal offset 1.27mm, z-position of LED center 2.0mm, 2 pins, generated by kicad-footprint-generator")
		(tags "LED")
		(property "Reference" "D2"
			(at -1.93 3.58 180)
			(layer "F.SilkS")
		)
		(property "Value" "LED_3mm"
			(at 1.27 7.63 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "3mm diameter small LED"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "LED_D3.0mm_Clear LED_D3.0mm_Horizontal_O1.27mm_Z2.0mm LED_D3.0mm_Horizontal_O3.81mm_Z2.0mm LED_D3.0mm_Horizontal_O6.35mm_Z2.0mm")
		(sheetname "/")
		(sheetfile "pcb.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 1.27 3.12 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 270)
			(size 1.8 1.8)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 8 "LED_GND")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 2.54 0 270)
			(size 1.8 1.8)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 9 "Net-(D2-Pad2)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/LED_THT.3dshapes/LED_D3.0mm_Horizontal_O1.27mm_Z2.0mm.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_THT:C_Disc_D3.0mm_W2.0mm_P2.50mm"
		(layer "F.Cu")
		(at 83.85 86 180)
		(descr "C, Disc series, Radial, pin pitch=2.50mm, diameter*width=3*2mm^2, Capacitor")
		(tags "C Disc series Radial pin pitch 2.50mm diameter 3mm width 2mm Capacitor")
		(property "Reference" "C3"
			(at -2.25 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "100nF"
			(at -3.75 -0.5 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "pcb.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 1.25 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "ADC0")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 2.5 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "SP")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D3.0mm_W2.0mm_P2.50mm.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal"
		(layer "F.Cu")
		(at 86.09 92.5 180)
		(descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=5.08mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 5.08mm 0.167W length 3.6mm diameter 1.6mm")
		(property "Reference" "R7"
			(at 6.74 0 270)
			(layer "F.SilkS")
		)
		(property "Value" "4.7K"
			(at -3.01 0 180)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "pcb.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 2.54 0 180)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 180)
			(size 1.4 1.4)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 17 "PTT")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 5.08 0 180)
			(size 1.4 1.4)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 16 "Net-(Q1-B)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Diode_THT:D_DO-35_SOD27_P7.62mm_Horizontal"
		(layer "F.Cu")
		(at 122.6 72.86 -90)
		(descr "Diode, DO-35_SOD27 series, Axial, Horizontal, pin pitch=7.62mm, length*diameter=4*2mm^2, http://www.diodes.com/_files/packages/DO-35.pdf")
		(tags "Diode DO-35_SOD27 series Axial Horizontal pin pitch 7.62mm  length 4mm diameter 2mm")
		(property "Reference" "D5"
			(at -2.26 0 90)
			(layer "F.SilkS")
		)
		(property "Value" "1N4148"
			(at -2.36 1 180)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/1N4148_1N4448.pdf"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "100V 0.15A standard switching diode, DO-35"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Device" "D"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "D*DO?35*")
		(sheetname "/")
		(sheetfile "pcb.kicad_sch")
		(attr through_hole)
		(fp_text user "K"
			(at 0 -1.8 90)
			(layer "F.SilkS")
		)
		(fp_text user "K"
			(at 0 -1.8 90)
			(layer "F.Fab")
		)
		(fp_text user "${REFERENCE}"
			(at 4.11 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole roundrect
			(at 0 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.15625)
			(net 12 "+3V3")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 7.62 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "ADC0")
			(pinfunction "A")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Diode_THT.3dshapes/D_DO-35_SOD27_P7.62mm_Horizontal.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MountingHole:MountingHole_3.2mm_M3_ISO14580"
		(layer "F.Cu")
		(at 120.36 116.04)
		(descr "Mounting Hole 3.2mm, M3, no annular, generated by kicad-footprint-generator mountinghole.py")
		(tags "mountinghole M3 ISO14580")
		(property "Reference" "3.2mm M3"
			(at 0 -3.7 0)
			(layer "F.SilkS")
		)
		(property "Value" "MountingHole_3.2mm_M3_ISO14580"
			(at -17.76 -9.04 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 3.2 3.2)
			(drill 3.2)
			(layers "*.Cu" "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "Potentiometer_THT:Potentiometer_Runtron_RM-063_Horizontal"
		(layer "F.Cu")
		(at 83.53 52.54)
		(descr "Potentiometer, horizontal, Trimmer, RM-063 http://www.runtron.com/down/PDF%20Datasheet/Carbon%20Film%20Potentiometer/RM065%20RM063.pdf")
		(tags "Potentiometer Trimmer RM-063")
		(property "Reference" "RV1"
			(at 2.5 4.46 0)
			(layer "F.SilkS")
		)
		(property "Value" "10k"
			(at 2.4 4.5 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Trim-potentiometer, US symbol"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Potentiometer*")
		(sheetname "/")
		(sheetfile "pcb.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 2.5 0.3 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.55 1.55)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 46 "Net-(C1-Pad1)")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 2.5 2.5)
			(size 1.55 1.55)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "Net-(C2-Pad1)")
			(pinfunction "2")
			(pintype "passive")
		)
		(pad "3" thru_hole circle
			(at 5 0)
			(size 1.55 1.55)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "3")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KIPRJMOD}/models/User Library-RM-063.STEP"
			(offset
				(xyz 2.5 -0.3 -2.5)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 -0 -180)
			)
		)
	)
	(footprint "LED_THT:LED_D3.0mm_Horizontal_O1.27mm_Z2.0mm"
		(layer "F.Cu")
		(at 77.475 99.53 -90)
		(descr "LED, diameter 3.0mm, horizontal offset 1.27mm, z-position of LED center 2.0mm, 2 pins, generated by kicad-footprint-generator")
		(tags "LED")
		(property "Reference" "D3"
			(at -1.78 3.875 180)
			(layer "F.SilkS")
		)
		(property "Value" "LED_3mm"
			(at 1.27 7.63 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "3mm diameter small LED"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "LED_D3.0mm_Clear LED_D3.0mm_Horizontal_O1.27mm_Z2.0mm LED_D3.0mm_Horizontal_O3.81mm_Z2.0mm LED_D3.0mm_Horizontal_O6.35mm_Z2.0mm")
		(sheetname "/")
		(sheetfile "pcb.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 1.27 3.12 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 270)
			(size 1.8 1.8)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 8 "LED_GND")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 2.54 0 270)
			(size 1.8 1.8)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 10 "Net-(D3-Pad2)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/LED_THT.3dshapes/LED_D3.0mm_Horizontal_O1.27mm_Z2.0mm.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MountingHole:MountingHole_3.2mm_M3_ISO14580"
		(layer "F.Cu")
		(at 77.18 55.08)
		(descr "Mounting Hole 3.2mm, M3, no annular, generated by kicad-footprint-generator mountinghole.py")
		(tags "mountinghole M3 ISO14580")
		(property "Reference" "3.2mm M3"
			(at 0 -3.7 0)
			(layer "F.SilkS")
		)
		(property "Value" "MountingHole_3.2mm_M3_ISO14580"
			(at -3.98 8.92 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole circle
			(at 0 0)
			(size 3.2 3.2)
			(drill 3.2)
			(layers "*.Cu" "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal"
		(layer "F.Cu")
		(at 87.29 108.42 180)
		(descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=5.08mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 5.08mm 0.167W length 3.6mm diameter 1.6mm")
		(property "Reference" "R5"
			(at 2.54 -1.92 180)
			(layer "F.SilkS")
		)
		(property "Value" "1k"
			(at 2.54 1.92 180)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "pcb.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 2.54 0 180)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 180)
			(size 1.4 1.4)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 19 "STA")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 5.08 0 180)
			(size 1.4 1.4)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 11 "Net-(D4-Pad2)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal"
		(layer "F.Cu")
		(at 119.09 72.91 -90)
		(descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=5.08mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 5.08mm 0.167W length 3.6mm diameter 1.6mm")
		(property "Reference" "R2"
			(at -1.91 0.19 90)
			(layer "F.SilkS")
		)
		(property "Value" "10k"
			(at 2.54 1.92 270)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "pcb.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 2.54 0 270)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 270)
			(size 1.4 1.4)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 12 "+3V3")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 5.08 0 270)
			(size 1.4 1.4)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "ADC0")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "LED_THT:LED_D3.0mm_Horizontal_O1.27mm_Z2.0mm"
		(layer "F.Cu")
		(at 77.18 105.88 -90)
		(descr "LED, diameter 3.0mm, horizontal offset 1.27mm, z-position of LED center 2.0mm, 2 pins, generated by kicad-footprint-generator")
		(tags "LED")
		(property "Reference" "D4"
			(at -1.88 3.58 180)
			(layer "F.SilkS")
		)
		(property "Value" "LED_3mm"
			(at 1.27 7.63 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "3mm diameter small LED"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "LED_D3.0mm_Clear LED_D3.0mm_Horizontal_O1.27mm_Z2.0mm LED_D3.0mm_Horizontal_O3.81mm_Z2.0mm LED_D3.0mm_Horizontal_O6.35mm_Z2.0mm")
		(sheetname "/")
		(sheetfile "pcb.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 1.27 3.12 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 270)
			(size 1.8 1.8)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 8 "LED_GND")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 2.54 0 270)
			(size 1.8 1.8)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 11 "Net-(D4-Pad2)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/LED_THT.3dshapes/LED_D3.0mm_Horizontal_O1.27mm_Z2.0mm.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal"
		(layer "F.Cu")
		(at 86.02 102.07 180)
		(descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=5.08mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 5.08mm 0.167W length 3.6mm diameter 1.6mm")
		(property "Reference" "R4"
			(at 2.54 -1.92 180)
			(layer "F.SilkS")
		)
		(property "Value" "1k"
			(at -2.08 0.07 180)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "pcb.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 2.54 0 180)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 180)
			(size 1.4 1.4)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 18 "CON")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 5.08 0 180)
			(size 1.4 1.4)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 10 "Net-(D3-Pad2)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_THT:TO-92_Inline"
		(layer "F.Cu")
		(at 121.1 60.23 -90)
		(descr "TO-92 leads in-line, narrow, oval pads, drill 0.75mm (see NXP sot054_po.pdf)")
		(tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
		(property "Reference" "Q1"
			(at 5.17 -0.2 90)
			(layer "F.SilkS")
		)
		(property "Value" "2N3904"
			(at 1.27 2.79 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/2N3903-D.PDF"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "0.2A Ic, 40V Vce, Small Signal NPN Transistor, TO-92"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TO?92*")
		(sheetname "/")
		(sheetfile "pcb.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 1.27 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 270)
			(size 1.05 1.5)
			(drill 0.75)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "E")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 1.27 0 270)
			(size 1.05 1.5)
			(drill 0.75)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 16 "Net-(Q1-B)")
			(pinfunction "B")
			(pintype "input")
		)
		(pad "3" thru_hole oval
			(at 2.54 0 270)
			(size 1.05 1.5)
			(drill 0.75)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 13 "PTT_R")
			(pinfunction "C")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Package_TO_SOT_THT.3dshapes/TO-92_Inline.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal"
		(layer "F.Cu")
		(at 86.02 89.37 180)
		(descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=5.08mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 5.08mm 0.167W length 3.6mm diameter 1.6mm")
		(property "Reference" "R1"
			(at 6.67 -0.13 270)
			(layer "F.SilkS")
		)
		(property "Value" "1k"
			(at -2.08 -0.13 180)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "pcb.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 2.54 0 180)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 180)
			(size 1.4 1.4)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 17 "PTT")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 5.08 0 180)
			(size 1.4 1.4)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 7 "Net-(D1-Pad2)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(gr_arc
		(start 74.1 121.12)
		(mid 72.685786 120.534214)
		(end 72.1 119.12)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 125.44 119.12)
		(mid 124.854214 120.534214)
		(end 123.44 121.12)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 72.1 52)
		(mid 72.685786 50.585786)
		(end 74.1 50)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 74.1 50)
		(end 123.44 50)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 123.44 50)
		(mid 124.854214 50.585786)
		(end 125.44 52)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 125.44 52)
		(end 125.44 119.12)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 123.44 121.12)
		(end 74.1 121.12)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 72.1 119.12)
		(end 72.1 52)
		(layer "Edge.Cuts")
	)
	(gr_text "Rev 0.70"
		(at 83.55 119.3 0)
		(layer "F.SilkS")
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "F.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 72.1 50) (xy 125.44 50) (xy 125.44 121.12) (xy 72.1 121.12)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 1)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 72.1 50) (xy 125.44 50) (xy 125.44 121.12) (xy 72.1 121.12)
			)
		)
	)
	(embedded_fonts no)
)
