(kicad_pcb
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(general
		(thickness 1.6)
		(legacy_teardrops no)
	)
	(paper "A4")
	(layers
		(0 "F.Cu" signal)
		(31 "B.Cu" signal)
		(32 "B.Adhes" user "B.Adhesive")
		(33 "F.Adhes" user "F.Adhesive")
		(34 "B.Paste" user)
		(35 "F.Paste" user)
		(36 "B.SilkS" user "B.Silkscreen")
		(37 "F.SilkS" user "F.Silkscreen")
		(38 "B.Mask" user)
		(39 "F.Mask" user)
		(40 "Dwgs.User" user "User.Drawings")
		(41 "Cmts.User" user "User.Comments")
		(42 "Eco1.User" user "User.Eco1")
		(43 "Eco2.User" user "User.Eco2")
		(44 "Edge.Cuts" user)
		(45 "Margin" user)
		(46 "B.CrtYd" user "B.Courtyard")
		(47 "F.CrtYd" user "F.Courtyard")
		(48 "B.Fab" user)
		(49 "F.Fab" user)
		(50 "User.1" user)
		(51 "User.2" user)
		(52 "User.3" user)
		(53 "User.4" user)
		(54 "User.5" user)
		(55 "User.6" user)
		(56 "User.7" user)
		(57 "User.8" user)
		(58 "User.9" user)
	)
	(setup
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(pcbplotparams
			(layerselection 0x00010fc_ffffffff)
			(plot_on_all_layers_selection 0x0000000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 4)
			(plotframeref no)
			(viasonmask no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plotreference yes)
			(plotvalue yes)
			(plotfptext yes)
			(plotinvisibletext no)
			(sketchpadsonfab no)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 0)
			(scaleselection 1)
			(outputdirectory "HDMI_BoB-gerbers/")
		)
	)
	(net 0 "")
	(net 1 "GND")
	(footprint "Connector_HDMI:HDMI_A_Molex_208658-1001_Horizontal"
		(layer "F.Cu")
		(at 154.0668 100.2646)
		(descr "HDMI Molex Type A https://www.molex.com/pdm_docs/sd/2086581001_sd.pdf")
		(tags "HDMI Molex Type A")
		(property "Reference" "H2"
			(at 5.9352 -9.006 0)
			(layer "F.SilkS")
		)
		(property "Value" "HDMI_A_Molex_208658-1001_Horizontal"
			(at 1.715 8.706971 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "C7501808"
			(at 0 0 0)
			(unlocked yes)
			(layer "Dwgs.User")
			(hide yes)
		)
		(fp_text user "PCB Edge"
			(at 5.715 0 90)
			(layer "Dwgs.User")
		)
		(pad "1" smd rect
			(at -3.285 -4.5)
			(size 2.6 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
		)
		(pad "2" smd rect
			(at -3.285 -4)
			(size 2.6 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
		)
		(pad "3" smd rect
			(at -3.285 -3.5)
			(size 2.6 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
		)
		(pad "4" smd rect
			(at -3.285 -3)
			(size 2.6 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
		)
		(pad "5" smd rect
			(at -3.285 -2.5)
			(size 2.6 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
		)
		(pad "6" smd rect
			(at -3.285 -2)
			(size 2.6 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
		)
		(pad "7" smd rect
			(at -3.285 -1.5)
			(size 2.6 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
		)
		(pad "8" smd rect
			(at -3.285 -1)
			(size 2.6 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
		)
		(pad "9" smd rect
			(at -3.285 -0.5)
			(size 2.6 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
		)
		(pad "10" smd rect
			(at -3.285 0)
			(size 2.6 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
		)
		(pad "11" smd rect
			(at -3.285 0.5)
			(size 2.6 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
		)
		(pad "12" smd rect
			(at -3.285 1)
			(size 2.6 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
		)
		(pad "13" smd rect
			(at -3.285 1.5)
			(size 2.6 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
		)
		(pad "14" smd rect
			(at -3.285 2)
			(size 2.6 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
		)
		(pad "15" smd rect
			(at -3.285 2.5)
			(size 2.6 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
		)
		(pad "16" smd rect
			(at -3.285 3)
			(size 2.6 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
		)
		(pad "17" smd rect
			(at -3.285 3.5)
			(size 2.6 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
		)
		(pad "18" smd rect
			(at -3.285 4)
			(size 2.6 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
		)
		(pad "19" smd rect
			(at -3.285 4.5)
			(size 2.6 0.3)
			(layers "F.Cu" "F.Paste" "F.Mask")
		)
		(pad "SH" thru_hole oval
			(at -2.525 -7.25)
			(size 3.3 1.5)
			(drill oval 2.7 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
		)
		(pad "SH" thru_hole oval
			(at -2.525 7.25)
			(size 3.3 1.5)
			(drill oval 2.7 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
		)
		(pad "SH" thru_hole oval
			(at 3.435 -7.25)
			(size 2.3 1.5)
			(drill oval 1.7 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
		)
		(pad "SH" thru_hole oval
			(at 3.435 7.25)
			(size 2.3 1.5)
			(drill oval 1.7 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
		)
		(model "${KICAD6_3DMODEL_DIR}/Connector_HDMI.3dshapes/HDMI_A_Molex_208658-1001_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_PinHeader_2.54mm:PinHeader_2x10_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 139.9758 88.9726)
		(descr "Through hole straight pin header, 2x10, 2.54mm pitch, double rows")
		(tags "Through hole pin header THT 2x10 2.54mm double row")
		(property "Reference" "H1"
			(at 0.0798 -1.9014 0)
			(layer "F.SilkS")
		)
		(property "Value" "PinHeader_2x10_P2.54mm_Vertical"
			(at 1.27 25.19 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Connector_PinHeader_2.54mm:PinHeader_2x10_P2.54mm_Vertical"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 1.27 11.43 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "2" thru_hole oval
			(at 2.54 0)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
		)
		(pad "3" thru_hole oval
			(at 0 2.54)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "4" thru_hole oval
			(at 2.54 2.54)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "5" thru_hole oval
			(at 0 5.08)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
		)
		(pad "6" thru_hole oval
			(at 2.54 5.08)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "7" thru_hole oval
			(at 0 7.62)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "8" thru_hole oval
			(at 2.54 7.62)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
		)
		(pad "9" thru_hole oval
			(at 0 10.16)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "10" thru_hole oval
			(at 2.54 10.16)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "11" thru_hole oval
			(at 0 12.7)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
		)
		(pad "12" thru_hole oval
			(at 2.54 12.7)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "13" thru_hole oval
			(at 0 15.24)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "14" thru_hole oval
			(at 2.54 15.24)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "15" thru_hole oval
			(at 0 17.78)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "16" thru_hole oval
			(at 2.54 17.78)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "17" thru_hole oval
			(at 0 20.32)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
		)
		(pad "18" thru_hole oval
			(at 2.54 20.32)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "19" thru_hole oval
			(at 0 22.86)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "20" thru_hole oval
			(at 2.54 22.86)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x10_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(gr_line
		(start 161.5694 86.5124)
		(end 161.5694 114.6302)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 161.5694 114.6302)
		(end 137.3124 114.6302)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 137.3124 86.5124)
		(end 161.5694 86.5124)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 137.3124 114.6302)
		(end 137.3124 86.5124)
		(layer "Edge.Cuts")
	)
	(gr_text "2"
		(at 144.399 89.3318 0)
		(layer "F.SilkS")
	)
	(gr_text "19"
		(at 147.5958 106.7526 0)
		(layer "F.SilkS")
	)
	(gr_text "19"
		(at 137.5918 112.268 0)
		(layer "F.SilkS")
	)
	(gr_text "1"
		(at 148.3578 94.8146 0)
		(layer "F.SilkS")
	)
	(gr_text "1"
		(at 137.6172 89.3064 0)
		(layer "F.SilkS")
	)
	(gr_text "HDMI break-out\nboard by\nRalle Palaveev\n(c) 2024"
		(at 157.988 103.124 0)
		(layer "B.Mask")
	)
	(zone
		(net 1)
		(net_name "GND")
		(layers "F&B.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0.2)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 137.3124 86.5124) (xy 161.5694 86.5124) (xy 161.5658 114.6266) (xy 137.3124 114.6266)
			)
		)
	)
)
