(kicad_pcb
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(general
		(thickness 1.6)
		(legacy_teardrops no)
	)
	(paper "A4")
	(layers
		(0 "F.Cu" signal)
		(4 "In1.Cu" signal)
		(6 "In2.Cu" signal)
		(2 "B.Cu" signal)
		(9 "F.Adhes" user "F.Adhesive")
		(11 "B.Adhes" user "B.Adhesive")
		(13 "F.Paste" user)
		(15 "B.Paste" user)
		(5 "F.SilkS" user "F.Silkscreen")
		(7 "B.SilkS" user "B.Silkscreen")
		(1 "F.Mask" user)
		(3 "B.Mask" user)
		(17 "Dwgs.User" user "User.Drawings")
		(19 "Cmts.User" user "User.Comments")
		(21 "Eco1.User" user "User.Eco1")
		(23 "Eco2.User" user "User.Eco2")
		(25 "Edge.Cuts" user)
		(27 "Margin" user)
		(31 "F.CrtYd" user "F.Courtyard")
		(29 "B.CrtYd" user "B.Courtyard")
		(35 "F.Fab" user)
		(33 "B.Fab" user)
		(39 "User.1" user)
		(41 "User.2" user)
		(43 "User.3" user)
		(45 "User.4" user)
		(47 "User.5" user)
		(49 "User.6" user)
		(51 "User.7" user)
		(53 "User.8" user)
		(55 "User.9" user)
	)
	(setup
		(stackup
			(layer "F.SilkS"
				(type "Top Silk Screen")
			)
			(layer "F.Paste"
				(type "Top Solder Paste")
			)
			(layer "F.Mask"
				(type "Top Solder Mask")
				(thickness 0.01)
			)
			(layer "F.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "dielectric 1"
				(type "prepreg")
				(thickness 0.1)
				(material "FR4")
				(epsilon_r 4.5)
				(loss_tangent 0.02)
			)
			(layer "In1.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "dielectric 2"
				(type "core")
				(thickness 1.24)
				(material "FR4")
				(epsilon_r 4.5)
				(loss_tangent 0.02)
			)
			(layer "In2.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "dielectric 3"
				(type "prepreg")
				(thickness 0.1)
				(material "FR4")
				(epsilon_r 4.5)
				(loss_tangent 0.02)
			)
			(layer "B.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "B.Mask"
				(type "Bottom Solder Mask")
				(thickness 0.01)
			)
			(layer "B.Paste"
				(type "Bottom Solder Paste")
			)
			(layer "B.SilkS"
				(type "Bottom Silk Screen")
			)
			(copper_finish "None")
			(dielectric_constraints no)
		)
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(tenting front back)
		(grid_origin 86.233 87.249)
		(pcbplotparams
			(layerselection 0x00000000_00000000_55555555_5755f5ff)
			(plot_on_all_layers_selection 0x00000000_00000000_00000000_00000000)
			(disableapertmacros no)
			(usegerberextensions yes)
			(usegerberattributes no)
			(usegerberadvancedattributes no)
			(creategerberjobfile no)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 4)
			(plotframeref no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(pdf_metadata yes)
			(pdf_single_document no)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plot_black_and_white yes)
			(sketchpadsonfab no)
			(plotpadnumbers no)
			(hidednponfab no)
			(sketchdnponfab yes)
			(crossoutdnponfab yes)
			(subtractmaskfromsilk yes)
			(outputformat 1)
			(mirror no)
			(drillshape 0)
			(scaleselection 1)
			(outputdirectory "main-bd-837-8015-01-gerbers-pcbway/")
		)
	)
	(net 0 "")
	(net 1 "Net-(BT1-+)")
	(net 2 "GND")
	(net 3 "Net-(IC9-CT)")
	(net 4 "VCC2")
	(net 5 "Net-(IC10-VCC)")
	(net 6 "LRCKB")
	(net 7 "25M")
	(net 8 "CDCK")
	(net 9 "Net-(CN1-Pin_2)")
	(net 10 "Net-(CN1-Pin_3)")
	(net 11 "Net-(CN1-Pin_5)")
	(net 12 "Net-(CN1-Pin_6)")
	(net 13 "Net-(CN1-Pin_7)")
	(net 14 "Net-(CN1-Pin_8)")
	(net 15 "Net-(CN1-Pin_9)")
	(net 16 "Net-(CN1-Pin_10)")
	(net 17 "BCLK")
	(net 18 "SDATA")
	(net 19 "LRCK")
	(net 20 "DFCK")
	(net 21 "unconnected-(CN1-Pin_15-Pad15)")
	(net 22 "unconnected-(CN1-Pin_16-Pad16)")
	(net 23 "Net-(CN1-Pin_17)")
	(net 24 "SBSO")
	(net 25 "unconnected-(CN1-Pin_19-Pad19)")
	(net 26 "SCOR")
	(net 27 "WFCK")
	(net 28 "M.VCC")
	(net 29 "M.GND")
	(net 30 "Net-(CN3-Pin_19)")
	(net 31 "~{ERES}")
	(net 32 "BCLKB")
	(net 33 "DFCKB")
	(net 34 "DDATA")
	(net 35 "ATT")
	(net 36 "SHFT")
	(net 37 "LATCH")
	(net 38 "VCC")
	(net 39 "PDATA")
	(net 40 "PWCLK")
	(net 41 "PBCLK")
	(net 42 "PLRCK")
	(net 43 "SL2")
	(net 44 "SR2")
	(net 45 "12M")
	(net 46 "Net-(IC2-12M)")
	(net 47 "50M")
	(net 48 "Net-(IC2-25M)")
	(net 49 "D4")
	(net 50 "D3")
	(net 51 "D2")
	(net 52 "D1")
	(net 53 "D0")
	(net 54 "~{AS}")
	(net 55 "~{UDS}")
	(net 56 "~{LDS}")
	(net 57 "R{slash}~{W}")
	(net 58 "~{DTAK}")
	(net 59 "unconnected-(IC1-BG-Pad11)")
	(net 60 "unconnected-(IC1-NC-Pad18)")
	(net 61 "~{HALT}")
	(net 62 "~{RES}")
	(net 63 "unconnected-(IC1-VMA-Pad21)")
	(net 64 "~{VPA}")
	(net 65 "unconnected-(IC1-FC2-Pad28)")
	(net 66 "FC1")
	(net 67 "FC0")
	(net 68 "unconnected-(IC1-NC-Pad31)")
	(net 69 "A1")
	(net 70 "A2")
	(net 71 "A3")
	(net 72 "A4")
	(net 73 "A5")
	(net 74 "A6")
	(net 75 "A7")
	(net 76 "A8")
	(net 77 "A9")
	(net 78 "A10")
	(net 79 "A11")
	(net 80 "A12")
	(net 81 "A13")
	(net 82 "A14")
	(net 83 "A15")
	(net 84 "A16")
	(net 85 "A17")
	(net 86 "A18")
	(net 87 "A19")
	(net 88 "unconnected-(IC1-A20-Pad51)")
	(net 89 "unconnected-(IC1-A21-Pad53)")
	(net 90 "unconnected-(IC1-A22-Pad54)")
	(net 91 "unconnected-(IC1-A23-Pad55)")
	(net 92 "D15")
	(net 93 "D14")
	(net 94 "D13")
	(net 95 "D12")
	(net 96 "D11")
	(net 97 "D10")
	(net 98 "D9")
	(net 99 "D8")
	(net 100 "D7")
	(net 101 "D6")
	(net 102 "D5")
	(net 103 "~{BRAM}")
	(net 104 "~{BROM}")
	(net 105 "~{ROM}")
	(net 106 "~{CAS0}")
	(net 107 "~{LWR}")
	(net 108 "~{UWR}")
	(net 109 "~{ASEL}")
	(net 110 "~{CAS2}")
	(net 111 "~{FDC}")
	(net 112 "FRES")
	(net 113 "Net-(IC11-A0)")
	(net 114 "Net-(IC11-A1)")
	(net 115 "Net-(IC11-A2)")
	(net 116 "Net-(IC11-A3)")
	(net 117 "Net-(IC11-A4)")
	(net 118 "Net-(IC11-A5)")
	(net 119 "Net-(IC11-A6)")
	(net 120 "Net-(IC11-A7)")
	(net 121 "Net-(IC11-D8)")
	(net 122 "Net-(IC11-D9)")
	(net 123 "Net-(IC11-D10)")
	(net 124 "Net-(IC11-D11)")
	(net 125 "Net-(IC11-D12)")
	(net 126 "Net-(IC11-D13)")
	(net 127 "Net-(IC11-D14)")
	(net 128 "Net-(IC11-D15)")
	(net 129 "~{ERAS}")
	(net 130 "~{ECAS}")
	(net 131 "~{EOE}")
	(net 132 "~{ORAS}")
	(net 133 "~{OCAS}")
	(net 134 "~{OOE}")
	(net 135 "~{OWE}")
	(net 136 "Net-(IC12-A0)")
	(net 137 "Net-(IC12-A1)")
	(net 138 "Net-(IC12-A2)")
	(net 139 "Net-(IC12-A3)")
	(net 140 "Net-(IC12-A4)")
	(net 141 "Net-(IC12-A5)")
	(net 142 "Net-(IC12-A6)")
	(net 143 "Net-(IC12-A7)")
	(net 144 "Net-(IC12-D8)")
	(net 145 "Net-(IC12-D9)")
	(net 146 "Net-(IC12-D10)")
	(net 147 "Net-(IC12-D11)")
	(net 148 "Net-(IC12-D12)")
	(net 149 "Net-(IC12-D13)")
	(net 150 "Net-(IC12-D14)")
	(net 151 "Net-(IC12-D15)")
	(net 152 "Net-(IC2-LEDR)")
	(net 153 "Net-(IC2-LEDG)")
	(net 154 "WFCKD")
	(net 155 "SCORB")
	(net 156 "SBSOB")
	(net 157 "SDATAB")
	(net 158 "CDCKD")
	(net 159 "~{PCM}")
	(net 160 "~{DTEN}")
	(net 161 "~{WAIT}")
	(net 162 "~{HRD}")
	(net 163 "~{INT}")
	(net 164 "~{CDC}")
	(net 165 "~{COE}")
	(net 166 "C2LR")
	(net 167 "PA8")
	(net 168 "PA7")
	(net 169 "PA6")
	(net 170 "PA5")
	(net 171 "PA4")
	(net 172 "PA3")
	(net 173 "PA2")
	(net 174 "PA1")
	(net 175 "PA0")
	(net 176 "~{PRAS}")
	(net 177 "~{PCAS}")
	(net 178 "~{CUWE}")
	(net 179 "VA1")
	(net 180 "VA2")
	(net 181 "VA3")
	(net 182 "VA4")
	(net 183 "VA5")
	(net 184 "VA6")
	(net 185 "VA7")
	(net 186 "VA8")
	(net 187 "VA9")
	(net 188 "VA10")
	(net 189 "VA11")
	(net 190 "VA12")
	(net 191 "VA13")
	(net 192 "VA14")
	(net 193 "VA15")
	(net 194 "VA16")
	(net 195 "VA17")
	(net 196 "VD0")
	(net 197 "VD1")
	(net 198 "VD2")
	(net 199 "VD3")
	(net 200 "VD4")
	(net 201 "VD5")
	(net 202 "VD6")
	(net 203 "VD7")
	(net 204 "VD8")
	(net 205 "VD9")
	(net 206 "VD10")
	(net 207 "VD11")
	(net 208 "VD12")
	(net 209 "VD13")
	(net 210 "VD14")
	(net 211 "VD15")
	(net 212 "unconnected-(IC3-N.C.-Pad11)")
	(net 213 "unconnected-(IC3-N.C.-Pad20)")
	(net 214 "unconnected-(IC3-SHL-Pad29)")
	(net 215 "unconnected-(IC3-SHR-Pad30)")
	(net 216 "unconnected-(IC3-DAC7-Pad31)")
	(net 217 "unconnected-(IC3-DAC6-Pad32)")
	(net 218 "unconnected-(IC3-DAC5-Pad33)")
	(net 219 "unconnected-(IC3-DAC4-Pad34)")
	(net 220 "unconnected-(IC3-DAC3-Pad37)")
	(net 221 "unconnected-(IC3-DAC7L-Pad38)")
	(net 222 "unconnected-(IC3-DAC7R-Pad39)")
	(net 223 "unconnected-(IC3-RAMAX-Pad42)")
	(net 224 "/WD7")
	(net 225 "/WD6")
	(net 226 "/WD5")
	(net 227 "/WD4")
	(net 228 "/WD3")
	(net 229 "/WD2")
	(net 230 "/WD1")
	(net 231 "/WD0")
	(net 232 "/RA14")
	(net 233 "/RA13")
	(net 234 "/RA12")
	(net 235 "/RA11")
	(net 236 "/RA10")
	(net 237 "/RA9")
	(net 238 "/RA8")
	(net 239 "~{RAS2X}")
	(net 240 "~{CLWEX}")
	(net 241 "~{RCS1X}")
	(net 242 "Net-(IC13-~{WE})")
	(net 243 "/RA7")
	(net 244 "/RA6")
	(net 245 "/RA5")
	(net 246 "/RA4")
	(net 247 "unconnected-(IC3-XOUT-Pad71)")
	(net 248 "/RA3")
	(net 249 "/RA2")
	(net 250 "/RA1")
	(net 251 "/RA0")
	(net 252 "unconnected-(IC5-N.C.-Pad10)")
	(net 253 "unconnected-(IC6-N.C.-Pad10)")
	(net 254 "unconnected-(IC7-N.C.-Pad10)")
	(net 255 "unconnected-(IC8-N.C.-Pad10)")
	(net 256 "unconnected-(IC9-~{ALARM1}-Pad6)")
	(net 257 "unconnected-(IC9-~{ALARM2}-Pad7)")
	(net 258 "unconnected-(IC9-RESET-Pad9)")
	(net 259 "Net-(IC10-CS2)")
	(net 260 "unconnected-(IC9-VSENSE-Pad12)")
	(net 261 "~{EWE}")
	(net 262 "/RAA6")
	(net 263 "/RAA7")
	(net 264 "/RAA8")
	(net 265 "/RAA9")
	(net 266 "/RAA10")
	(net 267 "/RAA11")
	(net 268 "/RAA12")
	(net 269 "unconnected-(IC15-RA14-Pad10)")
	(net 270 "unconnected-(IC15-RA15-Pad11)")
	(net 271 "Net-(IC15-~{RWE})")
	(net 272 "Net-(IC15-~{ROE})")
	(net 273 "unconnected-(IC15-ERA-Pad15)")
	(net 274 "/CD7")
	(net 275 "/CD6")
	(net 276 "/CD5")
	(net 277 "/CD4")
	(net 278 "/CD3")
	(net 279 "/CD2")
	(net 280 "/CD1")
	(net 281 "/CD0")
	(net 282 "unconnected-(IC15-XTAL-Pad26)")
	(net 283 "unconnected-(IC15-MCK-Pad37)")
	(net 284 "unconnected-(IC15-~{STEN}-Pad60)")
	(net 285 "unconnected-(IC15-~{EOP}-Pad61)")
	(net 286 "Net-(IC15-~{RCS})")
	(net 287 "unconnected-(IC15-~{HDE}-Pad63)")
	(net 288 "/RAA0")
	(net 289 "/RAA1")
	(net 290 "/RAA2")
	(net 291 "/RAA3")
	(net 292 "/RAA4")
	(net 293 "/RAA5")
	(net 294 "unconnected-(CN2-Pin_a2-Pada2)")
	(net 295 "Net-(LD1-K)")
	(net 296 "Net-(LD1-A)")
	(net 297 "Net-(LD2-K)")
	(net 298 "Net-(LD2-A)")
	(net 299 "unconnected-(OSC1-EN-Pad1)")
	(net 300 "Net-(TR2-B)")
	(net 301 "Net-(TR1-B)")
	(net 302 "unconnected-(CN2-Pin_a27-Pada27)")
	(net 303 "unconnected-(CN2-Pin_a28-Pada28)")
	(net 304 "unconnected-(CN2-Pin_b24-Padb24)")
	(net 305 "unconnected-(CN2-Pin_b25-Padb25)")
	(net 306 "unconnected-(CN2-Pin_b27-Padb27)")
	(net 307 "unconnected-(CN2-Pin_b28-Padb28)")
	(net 308 "~{RCS2X}")
	(net 309 "~{ROE}")
	(net 310 "~{RAACS1}")
	(net 311 "BCK")
	(net 312 "~{RAACS2}")
	(net 313 "unconnected-(IC11-N.C.-Pad1)")
	(net 314 "unconnected-(IC12-N.C.-Pad1)")
	(net 315 "E")
	(net 316 "~{IPL2}")
	(net 317 "~{IPL1}")
	(net 318 "~{IPL0}")
	(net 319 "unconnected-(IC12-N.C.-Pad20)")
	(net 320 "unconnected-(IC12-N.C.-Pad31)")
	(net 321 "unconnected-(IC12-N.C.-Pad32)")
	(net 322 "unconnected-(IC12-N.C.-Pad37)")
	(net 323 "unconnected-(IC9-N.C.-Pad1)")
	(net 324 "unconnected-(IC9-N.C.-Pad15)")
	(net 325 "unconnected-(IC10-N.C.-Pad1)")
	(net 326 "unconnected-(IC11-N.C.-Pad20)")
	(net 327 "unconnected-(IC11-N.C.-Pad31)")
	(net 328 "unconnected-(IC11-N.C.-Pad32)")
	(net 329 "unconnected-(IC11-N.C.-Pad37)")
	(net 330 "unconnected-(IC17-N.C.-Pad1)")
	(net 331 "unconnected-(IC18-N.C.-Pad1)")
	(net 332 "Net-(OSC1-OUT)")
	(net 333 "~{RAS2}")
	(net 334 "~{CLWE}")
	(net 335 "unconnected-(IC16-Pad11)")
	(net 336 "unconnected-(IC19A-~{Q}-Pad6)")
	(net 337 "unconnected-(IC19B-~{Q}-Pad8)")
	(net 338 "unconnected-(IC19B-Q-Pad9)")
	(net 339 "unconnected-(IC9-VBAT1-Pad2)")
	(footprint "Oscillator:Oscillator_DIP-14"
		(layer "F.Cu")
		(at 187.6298 76.581)
		(descr "Oscillator, DIP14, http://cdn-reichelt.de/documents/datenblatt/B400/OSZI.pdf")
		(tags "oscillator")
		(property "Reference" "OSC1"
			(at 16.3576 3.9624 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "50MHz"
			(at 7.62 3.74 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Crystal Clock Oscillator, DIP14-style metal package"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "MegaCD.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 7.62 -3.81 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 299 "unconnected-(OSC1-EN-Pad1)")
			(pinfunction "EN")
			(pintype "input+no_connect")
		)
		(pad "7" thru_hole circle
			(at 15.24 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "8" thru_hole circle
			(at 15.24 -7.62)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 332 "Net-(OSC1-OUT)")
			(pinfunction "OUT")
			(pintype "output")
		)
		(pad "14" thru_hole circle
			(at 0 -7.62)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "VCC2")
			(pinfunction "Vcc")
			(pintype "power_in")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Oscillator.3dshapes/Oscillator_DIP-14.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MegaCD_Footprints:ZIP-40"
		(layer "F.Cu")
		(at 211.963 121.158 180)
		(descr "20-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
		(tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
		(property "Reference" "IC11"
			(at 6.0452 33.8582 270)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "TC511664BZ"
			(at 1.27 52.07 180)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "MegaCD.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 1.016 -2.54 180)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 180)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 313 "unconnected-(IC11-N.C.-Pad1)")
			(pinfunction "N.C.")
			(pintype "no_connect")
		)
		(pad "2" thru_hole oval
			(at 2.54 1.27 180)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 121 "Net-(IC11-D8)")
			(pinfunction "D8")
			(pintype "tri_state")
		)
		(pad "3" thru_hole oval
			(at 0 2.54 180)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 122 "Net-(IC11-D9)")
			(pinfunction "D9")
			(pintype "tri_state")
		)
		(pad "4" thru_hole oval
			(at 2.54 3.81 180)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 123 "Net-(IC11-D10)")
			(pinfunction "D10")
			(pintype "tri_state")
		)
		(pad "5" thru_hole oval
			(at 0 5.08 180)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 124 "Net-(IC11-D11)")
			(pinfunction "D11")
			(pintype "tri_state")
		)
		(pad "6" thru_hole oval
			(at 2.54 6.35 180)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 125 "Net-(IC11-D12)")
			(pinfunction "D12")
			(pintype "tri_state")
		)
		(pad "7" thru_hole oval
			(at 0 7.62 180)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 126 "Net-(IC11-D13)")
			(pinfunction "D13")
			(pintype "tri_state")
		)
		(pad "8" thru_hole oval
			(at 2.54 8.89 180)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 127 "Net-(IC11-D14)")
			(pinfunction "D14")
			(pintype "tri_state")
		)
		(pad "9" thru_hole oval
			(at 0 10.16 180)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 128 "Net-(IC11-D15)")
			(pinfunction "D15")
			(pintype "tri_state")
		)
		(pad "10" thru_hole oval
			(at 2.54 11.43 180)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "11" thru_hole oval
			(at 0 12.7 180)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 113 "Net-(IC11-A0)")
			(pinfunction "D0")
			(pintype "tri_state")
		)
		(pad "12" thru_hole oval
			(at 2.54 13.97 180)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 114 "Net-(IC11-A1)")
			(pinfunction "D1")
			(pintype "tri_state")
		)
		(pad "13" thru_hole oval
			(at 0 15.24 180)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "VCC2")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(pad "14" thru_hole oval
			(at 2.54 16.51 180)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 115 "Net-(IC11-A2)")
			(pinfunction "D2")
			(pintype "tri_state")
		)
		(pad "15" thru_hole oval
			(at 0 17.78 180)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 116 "Net-(IC11-A3)")
			(pinfunction "D3")
			(pintype "tri_state")
		)
		(pad "16" thru_hole oval
			(at 2.54 19.05 180)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 117 "Net-(IC11-A4)")
			(pinfunction "D4")
			(pintype "tri_state")
		)
		(pad "17" thru_hole oval
			(at 0 20.32 180)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 118 "Net-(IC11-A5)")
			(pinfunction "D5")
			(pintype "tri_state")
		)
		(pad "18" thru_hole oval
			(at 2.54 21.59 180)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 119 "Net-(IC11-A6)")
			(pinfunction "D6")
			(pintype "tri_state")
		)
		(pad "19" thru_hole oval
			(at 0 22.86 180)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 120 "Net-(IC11-A7)")
			(pinfunction "D7")
			(pintype "tri_state")
		)
		(pad "20" thru_hole oval
			(at 2.54 24.13 180)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 326 "unconnected-(IC11-N.C.-Pad20)")
			(pinfunction "N.C.")
			(pintype "no_connect")
		)
		(pad "21" thru_hole oval
			(at 0 25.4 180)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "VCC2")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(pad "22" thru_hole oval
			(at 2.54 26.67 180)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 261 "~{EWE}")
			(pinfunction "~{UWE}")
			(pintype "input")
		)
		(pad "23" thru_hole oval
			(at 0 27.94 180)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 261 "~{EWE}")
			(pinfunction "~{LWE}")
			(pintype "input")
		)
		(pad "24" thru_hole oval
			(at 2.54 29.21 180)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 129 "~{ERAS}")
			(pinfunction "~{RAS}")
			(pintype "input")
		)
		(pad "25" thru_hole oval
			(at 0 30.48 180)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 113 "Net-(IC11-A0)")
			(pinfunction "A0")
			(pintype "input")
		)
		(pad "26" thru_hole oval
			(at 2.54 31.75 180)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 114 "Net-(IC11-A1)")
			(pinfunction "A1")
			(pintype "input")
		)
		(pad "27" thru_hole oval
			(at 0 33.02 180)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 115 "Net-(IC11-A2)")
			(pinfunction "A2")
			(pintype "input")
		)
		(pad "28" thru_hole oval
			(at 2.54 34.29 180)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 116 "Net-(IC11-A3)")
			(pinfunction "A3")
			(pintype "input")
		)
		(pad "29" thru_hole oval
			(at 0 35.56 180)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 117 "Net-(IC11-A4)")
			(pinfunction "A4")
			(pintype "input")
		)
		(pad "30" thru_hole oval
			(at 2.54 36.83 180)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "VCC2")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(pad "31" thru_hole oval
			(at 0 38.1 180)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 327 "unconnected-(IC11-N.C.-Pad31)")
			(pinfunction "N.C.")
			(pintype "no_connect")
		)
		(pad "32" thru_hole oval
			(at 2.54 39.37 180)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 328 "unconnected-(IC11-N.C.-Pad32)")
			(pinfunction "N.C.")
			(pintype "no_connect")
		)
		(pad "33" thru_hole oval
			(at 0 40.64 180)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "34" thru_hole oval
			(at 2.54 41.91 180)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 118 "Net-(IC11-A5)")
			(pinfunction "A5")
			(pintype "input")
		)
		(pad "35" thru_hole oval
			(at 0 43.18 180)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 119 "Net-(IC11-A6)")
			(pinfunction "A6")
			(pintype "input")
		)
		(pad "36" thru_hole oval
			(at 2.54 44.45 180)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 120 "Net-(IC11-A7)")
			(pinfunction "A7")
			(pintype "input")
		)
		(pad "37" thru_hole oval
			(at 0 45.72 180)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 329 "unconnected-(IC11-N.C.-Pad37)")
			(pinfunction "N.C.")
			(pintype "no_connect")
		)
		(pad "38" thru_hole oval
			(at 2.54 46.99 180)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 131 "~{EOE}")
			(pinfunction "~{OE}")
			(pintype "input")
		)
		(pad "39" thru_hole oval
			(at 0 48.26 180)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 130 "~{ECAS}")
			(pinfunction "~{CAS}")
			(pintype "input")
		)
		(pad "40" thru_hole oval
			(at 2.54 49.53 180)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Package_DIP.3dshapes/DIP-20_W7.62mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MegaCD_Footprints:FB_P5.00mm"
		(layer "F.Cu")
		(at 176.0766 78.4606)
		(property "Reference" "FB1"
			(at -0.4864 2.54 0)
			(layer "F.SilkS")
		)
		(property "Value" "FB"
			(at 2.5 2.2 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Ferrite bead, small symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "MegaCD.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 2.5 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 45 "12M")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 5 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 46 "Net-(IC2-12M)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D4.3mm_W1.9mm_P5.00mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MegaCD_Footprints:SOIC-14W_5.3mm_P1.27mm"
		(layer "F.Cu")
		(at 201.676 59.6706 90)
		(descr "16-Lead Plastic Small Outline (SO) - Wide, 5.3 mm Body (http://www.ti.com/lit/ml/msop002a/msop002a.pdf)")
		(tags "SOIC 1.27")
		(property "Reference" "IC19"
			(at 6.356 -4.0894 180)
			(layer "F.SilkS")
		)
		(property "Value" "74AC74"
			(at 0 6.2 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Dual D Flip-flop, Set & Reset"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "MegaCD.kicad_sch")
		(attr smd)
		(fp_text user "${VALUE}"
			(at 0 -0.635 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "${REFERENCE}"
			(at 0 -0.762 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -3.55 -4.445 90)
			(size 1.5 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 4 "VCC2")
			(pinfunction "~{R}")
			(pintype "input")
		)
		(pad "2" smd rect
			(at -3.55 -3.175 90)
			(size 1.5 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 239 "~{RAS2X}")
			(pinfunction "D")
			(pintype "input")
		)
		(pad "3" smd rect
			(at -3.55 -1.905 90)
			(size 1.5 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 47 "50M")
			(pinfunction "C")
			(pintype "input")
		)
		(pad "4" smd rect
			(at -3.55 -0.635 90)
			(size 1.5 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 4 "VCC2")
			(pinfunction "~{S}")
			(pintype "input")
		)
		(pad "5" smd rect
			(at -3.55 0.635 90)
			(size 1.5 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 333 "~{RAS2}")
			(pinfunction "Q")
			(pintype "output")
		)
		(pad "6" smd rect
			(at -3.55 1.905 90)
			(size 1.5 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 336 "unconnected-(IC19A-~{Q}-Pad6)")
			(pinfunction "~{Q}")
			(pintype "output+no_connect")
		)
		(pad "7" smd rect
			(at -3.55 3.175 90)
			(size 1.5 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "8" smd rect
			(at 3.556 3.175 90)
			(size 1.5 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 337 "unconnected-(IC19B-~{Q}-Pad8)")
			(pinfunction "~{Q}")
			(pintype "output+no_connect")
		)
		(pad "9" smd rect
			(at 3.55 1.905 90)
			(size 1.5 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 338 "unconnected-(IC19B-Q-Pad9)")
			(pinfunction "Q")
			(pintype "output+no_connect")
		)
		(pad "10" smd rect
			(at 3.55 0.635 90)
			(size 1.5 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 4 "VCC2")
			(pinfunction "~{S}")
			(pintype "input")
		)
		(pad "11" smd rect
			(at 3.55 -0.635 90)
			(size 1.5 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 4 "VCC2")
			(pinfunction "C")
			(pintype "input")
		)
		(pad "12" smd rect
			(at 3.55 -1.905 90)
			(size 1.5 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 4 "VCC2")
			(pinfunction "D")
			(pintype "input")
		)
		(pad "13" smd rect
			(at 3.55 -3.175 90)
			(size 1.5 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 4 "VCC2")
			(pinfunction "~{R}")
			(pintype "input")
		)
		(pad "14" smd rect
			(at 3.55 -4.445 90)
			(size 1.5 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 4 "VCC2")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Package_SO.3dshapes/SOIC-16W_5.3x10.2mm_P1.27mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MegaCD_Footprints:FB_P5.00mm"
		(layer "F.Cu")
		(at 162.8394 118.3894 180)
		(property "Reference" "FB5"
			(at 8.2804 0.2032 180)
			(layer "F.SilkS")
		)
		(property "Value" "FB"
			(at 2.5 2.2 180)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Ferrite bead, small symbol"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "MegaCD.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 2.5 0 180)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 48 "Net-(IC2-25M)")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 5 0 180)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 7 "25M")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D4.3mm_W1.9mm_P5.00mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MegaCD_Footprints:CP_Elec_3x5.4"
		(layer "F.Cu")
		(at 177.4966 129.7178 180)
		(descr "SMD capacitor, aluminum electrolytic, Nichicon, 3.0x5.4mm")
		(tags "capacitor electrolytic")
		(property "Reference" "C12"
			(at 0.3824 2.8448 0)
			(layer "F.SilkS")
		)
		(property "Value" "10uF"
			(at 0 2.7 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Polarized capacitor"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "MegaCD.kicad_sch")
		(attr smd)
		(fp_text user "-"
			(at 1.6016 3.937 180)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "+"
			(at -5.3072 1.0668 180)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.597 0 180)
			(size 2.394 1.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.15625)
			(net 4 "VCC2")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.597 0 180)
			(size 2.394 1.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.15625)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/CP_Elec_3x5.4.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MegaCD_Footprints:CON-25P-ANGLE"
		(layer "F.Cu")
		(at 108.758 128.651)
		(descr "20-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
		(tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
		(property "Reference" "CN1"
			(at 15.2702 -5.5372 0)
			(layer "F.SilkS")
		)
		(property "Value" "CON 25P ANGLE"
			(at 19.05 2.54 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x25, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "MegaCD.kicad_sch")
		(attr through_hole)
		(fp_text user "1"
			(at -4.5926 0.4572 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "24"
			(at 28.1226 -4.2672 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "25"
			(at 30.2054 -3.048 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "2"
			(at -3.729 -1.0668 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "${REFERENCE}"
			(at 6.35 2.54 180)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 90)
			(size 1.2 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 8 "CDCK")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole roundrect
			(at 1.25 -2.54 90)
			(size 1.2 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 9 "Net-(CN1-Pin_2)")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole roundrect
			(at 2.5 0 90)
			(size 1.2 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 10 "Net-(CN1-Pin_3)")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole roundrect
			(at 3.75 -2.54 90)
			(size 1.2 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 31 "~{ERES}")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(pad "5" thru_hole roundrect
			(at 5 0 90)
			(size 1.2 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 11 "Net-(CN1-Pin_5)")
			(pinfunction "Pin_5")
			(pintype "passive")
		)
		(pad "6" thru_hole roundrect
			(at 6.25 -2.54 90)
			(size 1.2 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 12 "Net-(CN1-Pin_6)")
			(pinfunction "Pin_6")
			(pintype "passive")
		)
		(pad "7" thru_hole roundrect
			(at 7.5 0 90)
			(size 1.2 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 13 "Net-(CN1-Pin_7)")
			(pinfunction "Pin_7")
			(pintype "passive")
		)
		(pad "8" thru_hole roundrect
			(at 8.75 -2.54 90)
			(size 1.2 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 14 "Net-(CN1-Pin_8)")
			(pinfunction "Pin_8")
			(pintype "passive")
		)
		(pad "9" thru_hole roundrect
			(at 10 0 90)
			(size 1.2 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 15 "Net-(CN1-Pin_9)")
			(pinfunction "Pin_9")
			(pintype "passive")
		)
		(pad "10" thru_hole roundrect
			(at 11.25 -2.54 90)
			(size 1.2 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 16 "Net-(CN1-Pin_10)")
			(pinfunction "Pin_10")
			(pintype "passive")
		)
		(pad "11" thru_hole roundrect
			(at 12.5 0 90)
			(size 1.2 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 17 "BCLK")
			(pinfunction "Pin_11")
			(pintype "passive")
		)
		(pad "12" thru_hole roundrect
			(at 13.75 -2.54 90)
			(size 1.2 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 18 "SDATA")
			(pinfunction "Pin_12")
			(pintype "passive")
		)
		(pad "13" thru_hole roundrect
			(at 15 0 90)
			(size 1.2 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 19 "LRCK")
			(pinfunction "Pin_13")
			(pintype "passive")
		)
		(pad "14" thru_hole roundrect
			(at 16.25 -2.54 90)
			(size 1.2 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 20 "DFCK")
			(pinfunction "Pin_14")
			(pintype "passive")
		)
		(pad "15" thru_hole roundrect
			(at 17.5 0 90)
			(size 1.2 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 21 "unconnected-(CN1-Pin_15-Pad15)")
			(pinfunction "Pin_15")
			(pintype "passive+no_connect")
		)
		(pad "16" thru_hole roundrect
			(at 18.75 -2.54 90)
			(size 1.2 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 22 "unconnected-(CN1-Pin_16-Pad16)")
			(pinfunction "Pin_16")
			(pintype "passive+no_connect")
		)
		(pad "17" thru_hole roundrect
			(at 20 0 90)
			(size 1.2 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 23 "Net-(CN1-Pin_17)")
			(pinfunction "Pin_17")
			(pintype "passive")
		)
		(pad "18" thru_hole roundrect
			(at 21.25 -2.54 90)
			(size 1.2 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 24 "SBSO")
			(pinfunction "Pin_18")
			(pintype "passive")
		)
		(pad "19" thru_hole roundrect
			(at 22.5 0 90)
			(size 1.2 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 25 "unconnected-(CN1-Pin_19-Pad19)")
			(pinfunction "Pin_19")
			(pintype "passive+no_connect")
		)
		(pad "20" thru_hole roundrect
			(at 23.75 -2.54 90)
			(size 1.2 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 26 "SCOR")
			(pinfunction "Pin_20")
			(pintype "passive")
		)
		(pad "21" thru_hole roundrect
			(at 25 0 90)
			(size 1.2 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "Pin_21")
			(pintype "passive")
		)
		(pad "22" thru_hole roundrect
			(at 26.25 -2.54 90)
			(size 1.2 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 27 "WFCK")
			(pinfunction "Pin_22")
			(pintype "passive")
		)
		(pad "23" thru_hole roundrect
			(at 27.5 0 90)
			(size 1.2 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 4 "VCC2")
			(pinfunction "Pin_23")
			(pintype "passive")
		)
		(pad "24" thru_hole roundrect
			(at 28.75 -2.54 90)
			(size 1.2 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 28 "M.VCC")
			(pinfunction "Pin_24")
			(pintype "passive")
		)
		(pad "25" thru_hole roundrect
			(at 30 0 90)
			(size 1.2 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 29 "M.GND")
			(pinfunction "Pin_25")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Package_DIP.3dshapes/DIP-20_W7.62mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MegaCD_Footprints:SOIC-28Wider"
		(layer "F.Cu")
		(at 174.1932 69.6468 90)
		(descr "SOIC, 28 Pin (JEDEC MS-013AE, https://www.analog.com/media/en/package-pcb-resources/package/35833120341221rw_28.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOIC SO")
		(property "Reference" "IC10"
			(at 0.4318 -12.2174 180)
			(layer "F.SilkS")
		)
		(property "Value" "MB8464A-10L"
			(at 0 9.9 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "MegaCD.kicad_sch")
		(attr smd)
		(fp_text user "${VALUE}"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -5.715 -8.255 90)
			(size 2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 325 "unconnected-(IC10-N.C.-Pad1)")
			(pinfunction "N.C.")
			(pintype "no_connect")
		)
		(pad "2" smd roundrect
			(at -5.715 -6.985 90)
			(size 2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 81 "A13")
			(pinfunction "A12")
			(pintype "input")
		)
		(pad "3" smd roundrect
			(at -5.715 -5.715 90)
			(size 2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 76 "A8")
			(pinfunction "A7")
			(pintype "input")
		)
		(pad "4" smd roundrect
			(at -5.715 -4.445 90)
			(size 2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 75 "A7")
			(pinfunction "A6")
			(pintype "input")
		)
		(pad "5" smd roundrect
			(at -5.715 -3.175 90)
			(size 2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 74 "A6")
			(pinfunction "A5")
			(pintype "input")
		)
		(pad "6" smd roundrect
			(at -5.715 -1.905 90)
			(size 2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 73 "A5")
			(pinfunction "A4")
			(pintype "input")
		)
		(pad "7" smd roundrect
			(at -5.715 -0.635 90)
			(size 2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 72 "A4")
			(pinfunction "A3")
			(pintype "input")
		)
		(pad "8" smd roundrect
			(at -5.715 0.635 90)
			(size 2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 71 "A3")
			(pinfunction "A2")
			(pintype "input")
		)
		(pad "9" smd roundrect
			(at -5.715 1.905 90)
			(size 2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 70 "A2")
			(pinfunction "A1")
			(pintype "input")
		)
		(pad "10" smd roundrect
			(at -5.715 3.175 90)
			(size 2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 69 "A1")
			(pinfunction "A0")
			(pintype "input")
		)
		(pad "11" smd roundrect
			(at -5.715 4.445 90)
			(size 2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 53 "D0")
			(pinfunction "D0")
			(pintype "tri_state")
		)
		(pad "12" smd roundrect
			(at -5.715 5.715 90)
			(size 2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 52 "D1")
			(pinfunction "D1")
			(pintype "tri_state")
		)
		(pad "13" smd roundrect
			(at -5.715 6.985 90)
			(size 2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 51 "D2")
			(pinfunction "D2")
			(pintype "tri_state")
		)
		(pad "14" smd roundrect
			(at -5.715 8.255 90)
			(size 2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "15" smd roundrect
			(at 5.715 8.255 90)
			(size 2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 50 "D3")
			(pinfunction "D3")
			(pintype "tri_state")
		)
		(pad "16" smd roundrect
			(at 5.715 6.985 90)
			(size 2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 49 "D4")
			(pinfunction "D4")
			(pintype "tri_state")
		)
		(pad "17" smd roundrect
			(at 5.715 5.715 90)
			(size 2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 102 "D5")
			(pinfunction "D5")
			(pintype "tri_state")
		)
		(pad "18" smd roundrect
			(at 5.715 4.445 90)
			(size 2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 101 "D6")
			(pinfunction "D6")
			(pintype "tri_state")
		)
		(pad "19" smd roundrect
			(at 5.715 3.175 90)
			(size 2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 100 "D7")
			(pinfunction "D7")
			(pintype "tri_state")
		)
		(pad "20" smd roundrect
			(at 5.715 1.905 90)
			(size 2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 103 "~{BRAM}")
			(pinfunction "~{CS1}")
			(pintype "input")
		)
		(pad "21" smd roundrect
			(at 5.715 0.635 90)
			(size 2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 79 "A11")
			(pinfunction "A10")
			(pintype "input")
		)
		(pad "22" smd roundrect
			(at 5.715 -0.635 90)
			(size 2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 165 "~{COE}")
			(pinfunction "~{OE}")
			(pintype "input")
		)
		(pad "23" smd roundrect
			(at 5.715 -1.905 90)
			(size 2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 80 "A12")
			(pinfunction "A11")
			(pintype "input")
		)
		(pad "24" smd roundrect
			(at 5.715 -3.175 90)
			(size 2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 78 "A10")
			(pinfunction "A9")
			(pintype "input")
		)
		(pad "25" smd roundrect
			(at 5.715 -4.445 90)
			(size 2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 77 "A9")
			(pinfunction "A8")
			(pintype "input")
		)
		(pad "26" smd roundrect
			(at 5.715 -5.715 90)
			(size 2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 259 "Net-(IC10-CS2)")
			(pinfunction "CS2")
			(pintype "input")
		)
		(pad "27" smd roundrect
			(at 5.715 -6.985 90)
			(size 2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 334 "~{CLWE}")
			(pinfunction "~{WE}")
			(pintype "input")
		)
		(pad "28" smd roundrect
			(at 5.715 -8.255 90)
			(size 2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 5 "Net-(IC10-VCC)")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Package_SO.3dshapes/SOIC-28W_7.5x17.9mm_P1.27mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MegaCD_Footprints:ZIP-20"
		(layer "F.Cu")
		(at 119.38 117.221 90)
		(descr "20-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
		(tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
		(property "Reference" "IC7"
			(at -2.1336 10.541 180)
			(layer "F.SilkS")
		)
		(property "Value" "MB81C4256Z"
			(at 1.27 26.67 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "MegaCD.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 1.016 -2.54 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 90)
			(size 1.3 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 165 "~{COE}")
			(pinfunction "~{OE}")
			(pintype "input")
		)
		(pad "2" thru_hole roundrect
			(at 2.54 1.27 90)
			(size 1.3 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 177 "~{PCAS}")
			(pinfunction "~{CAS}")
			(pintype "input")
		)
		(pad "3" thru_hole roundrect
			(at 0 2.54 90)
			(size 1.3 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 97 "D10")
			(pinfunction "D2")
			(pintype "tri_state")
		)
		(pad "4" thru_hole roundrect
			(at 2.54 3.81 90)
			(size 1.3 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 96 "D11")
			(pinfunction "D3")
			(pintype "tri_state")
		)
		(pad "5" thru_hole roundrect
			(at 0 5.08 90)
			(size 1.3 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "VSS")
			(pintype "power_in")
		)
		(pad "6" thru_hole roundrect
			(at 2.54 6.35 90)
			(size 1.3 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 99 "D8")
			(pinfunction "D0")
			(pintype "tri_state")
		)
		(pad "7" thru_hole roundrect
			(at 0 7.62 90)
			(size 1.3 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 98 "D9")
			(pinfunction "D1")
			(pintype "tri_state")
		)
		(pad "8" thru_hole roundrect
			(at 2.54 8.89 90)
			(size 1.3 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 178 "~{CUWE}")
			(pinfunction "~{WE}")
			(pintype "input")
		)
		(pad "9" thru_hole roundrect
			(at 0 10.16 90)
			(size 1.3 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 176 "~{PRAS}")
			(pinfunction "~{RAS}")
			(pintype "input")
		)
		(pad "10" thru_hole roundrect
			(at 2.54 11.43 90)
			(size 1.3 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 254 "unconnected-(IC7-N.C.-Pad10)")
			(pinfunction "N.C.")
			(pintype "input+no_connect")
		)
		(pad "11" thru_hole roundrect
			(at 0 12.7 90)
			(size 1.3 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 175 "PA0")
			(pinfunction "A0")
			(pintype "input")
		)
		(pad "12" thru_hole roundrect
			(at 2.54 13.97 90)
			(size 1.3 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 174 "PA1")
			(pinfunction "A1")
			(pintype "input")
		)
		(pad "13" thru_hole roundrect
			(at 0 15.24 90)
			(size 1.3 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 173 "PA2")
			(pinfunction "A2")
			(pintype "input")
		)
		(pad "14" thru_hole roundrect
			(at 2.54 16.51 90)
			(size 1.3 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 172 "PA3")
			(pinfunction "A3")
			(pintype "input")
		)
		(pad "15" thru_hole roundrect
			(at 0 17.78 90)
			(size 1.3 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 4 "VCC2")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(pad "16" thru_hole roundrect
			(at 2.54 19.05 90)
			(size 1.3 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 171 "PA4")
			(pinfunction "A4")
			(pintype "input")
		)
		(pad "17" thru_hole roundrect
			(at 0 20.32 90)
			(size 1.3 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 170 "PA5")
			(pinfunction "A5")
			(pintype "input")
		)
		(pad "18" thru_hole roundrect
			(at 2.54 21.59 90)
			(size 1.3 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 169 "PA6")
			(pinfunction "A6")
			(pintype "input")
		)
		(pad "19" thru_hole roundrect
			(at 0 22.86 90)
			(size 1.3 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 168 "PA7")
			(pinfunction "A7")
			(pintype "input")
		)
		(pad "20" thru_hole roundrect
			(at 2.54 24.13 90)
			(size 1.3 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 167 "PA8")
			(pinfunction "A8")
			(pintype "input")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Package_DIP.3dshapes/DIP-20_W7.62mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MegaCD_Footprints:CP_Elec_3x5.4"
		(layer "F.Cu")
		(at 59.563 84.223 90)
		(descr "SMD capacitor, aluminum electrolytic, Nichicon, 3.0x5.4mm")
		(tags "capacitor electrolytic")
		(property "Reference" "C41"
			(at 4.3908 -1.524 270)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "10uF"
			(at 0 2.7 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Polarized capacitor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "MegaCD.kicad_sch")
		(attr smd)
		(fp_text user "-"
			(at 0.53 3.683 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "+"
			(at -4.423 3.302 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.597 0 90)
			(size 2.394 1.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.15625)
			(net 4 "VCC2")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.597 0 90)
			(size 2.394 1.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.15625)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/CP_Elec_3x5.4.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MegaCD_Footprints:FB_P5.00mm"
		(layer "F.Cu")
		(at 55.245 81.026 -90)
		(property "Reference" "FB4"
			(at -3.1242 0.508 270)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "FBA04"
			(at 2.5 2.2 270)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Ferrite bead, small symbol"
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "MegaCD.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 2.5 0 270)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "VCC2")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 5 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 30 "Net-(CN3-Pin_19)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D4.3mm_W1.9mm_P5.00mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MegaCD_Footprints:CP_Elec_3x5.4"
		(layer "F.Cu")
		(at 177.5446 123.3678 180)
		(descr "SMD capacitor, aluminum electrolytic, Nichicon, 3.0x5.4mm")
		(tags "capacitor electrolytic")
		(property "Reference" "C11"
			(at -3.0494 2.2098 180)
			(layer "F.SilkS")
		)
		(property "Value" "10uF"
			(at 0 2.7 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Polarized capacitor"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "MegaCD.kicad_sch")
		(attr smd)
		(fp_text user "+"
			(at -4.7004 -0.8128 180)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "-"
			(at 1.3956 3.9624 180)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.597 0 180)
			(size 2.394 1.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.15625)
			(net 4 "VCC2")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.597 0 180)
			(size 2.394 1.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.15625)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/CP_Elec_3x5.4.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MegaCD_Footprints:C_Radial_5mm"
		(layer "F.Cu")
		(at 56.642 123.4802 -90)
		(property "Reference" "C48"
			(at 0.0908 -4.318 270)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "100uF"
			(at 0 1 270)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Polarized capacitor"
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "MegaCD.kicad_sch")
		(attr through_hole)
		(fp_text user "+"
			(at 2.65165 -0.883883 270)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "-"
			(at -5.3 3.1 270)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "${REFERENCE}"
			(at 0 2.5 270)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" thru_hole roundrect
			(at 2.5 0 270)
			(size 1.5 1.5)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 4 "VCC2")
			(pintype "passive")
		)
		(pad "2" thru_hole roundrect
			(at -2.5 0 270)
			(size 1.5 1.5)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "MegaCD_Footprints:CP_Elec_3x5.4"
		(layer "F.Cu")
		(at 148.6154 107.4674 180)
		(descr "SMD capacitor, aluminum electrolytic, Nichicon, 3.0x5.4mm")
		(tags "capacitor electrolytic")
		(property "Reference" "C10"
			(at -2.9972 -3.3528 0)
			(layer "F.SilkS")
		)
		(property "Value" "10uF"
			(at 0 2.7 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Polarized capacitor"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "MegaCD.kicad_sch")
		(attr smd)
		(fp_text user "-"
			(at 1.76 2.75 180)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "+"
			(at -4.342 -0.508 180)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.597 0 180)
			(size 2.394 1.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.15625)
			(net 4 "VCC2")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.597 0 180)
			(size 2.394 1.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.15625)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/CP_Elec_3x5.4.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MegaCD_Footprints:CP_Elec_3x5.4"
		(layer "F.Cu")
		(at 136.7042 120.6246 180)
		(descr "SMD capacitor, aluminum electrolytic, Nichicon, 3.0x5.4mm")
		(tags "capacitor electrolytic")
		(property "Reference" "C13"
			(at 3.7352 -2.8956 0)
			(layer "F.SilkS")
		)
		(property "Value" "10uF"
			(at 0 2.7 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Polarized capacitor"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "MegaCD.kicad_sch")
		(attr smd)
		(fp_text user "+"
			(at -5.2564 1.8796 180)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "-"
			(at 3.0748 0.254 180)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.597 0 180)
			(size 2.394 1.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.15625)
			(net 4 "VCC2")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.597 0 180)
			(size 2.394 1.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.15625)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/CP_Elec_3x5.4.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MegaCD_Footprints:ZIP-40"
		(layer "F.Cu")
		(at 218.948 121.158 180)
		(descr "20-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
		(tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
		(property "Reference" "IC12"
			(at -3.5814 33.8582 270)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "TC511664BZ"
			(at 1.27 52.07 180)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "MegaCD.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 1.016 -2.54 180)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 180)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 314 "unconnected-(IC12-N.C.-Pad1)")
			(pinfunction "N.C.")
			(pintype "no_connect")
		)
		(pad "2" thru_hole oval
			(at 2.54 1.27 180)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 144 "Net-(IC12-D8)")
			(pinfunction "D8")
			(pintype "tri_state")
		)
		(pad "3" thru_hole oval
			(at 0 2.54 180)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 145 "Net-(IC12-D9)")
			(pinfunction "D9")
			(pintype "tri_state")
		)
		(pad "4" thru_hole oval
			(at 2.54 3.81 180)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 146 "Net-(IC12-D10)")
			(pinfunction "D10")
			(pintype "tri_state")
		)
		(pad "5" thru_hole oval
			(at 0 5.08 180)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 147 "Net-(IC12-D11)")
			(pinfunction "D11")
			(pintype "tri_state")
		)
		(pad "6" thru_hole oval
			(at 2.54 6.35 180)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 148 "Net-(IC12-D12)")
			(pinfunction "D12")
			(pintype "tri_state")
		)
		(pad "7" thru_hole oval
			(at 0 7.62 180)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 149 "Net-(IC12-D13)")
			(pinfunction "D13")
			(pintype "tri_state")
		)
		(pad "8" thru_hole oval
			(at 2.54 8.89 180)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 150 "Net-(IC12-D14)")
			(pinfunction "D14")
			(pintype "tri_state")
		)
		(pad "9" thru_hole oval
			(at 0 10.16 180)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 151 "Net-(IC12-D15)")
			(pinfunction "D15")
			(pintype "tri_state")
		)
		(pad "10" thru_hole oval
			(at 2.54 11.43 180)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "11" thru_hole oval
			(at 0 12.7 180)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 136 "Net-(IC12-A0)")
			(pinfunction "D0")
			(pintype "tri_state")
		)
		(pad "12" thru_hole oval
			(at 2.54 13.97 180)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 137 "Net-(IC12-A1)")
			(pinfunction "D1")
			(pintype "tri_state")
		)
		(pad "13" thru_hole oval
			(at 0 15.24 180)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "VCC2")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(pad "14" thru_hole oval
			(at 2.54 16.51 180)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 138 "Net-(IC12-A2)")
			(pinfunction "D2")
			(pintype "tri_state")
		)
		(pad "15" thru_hole oval
			(at 0 17.78 180)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 139 "Net-(IC12-A3)")
			(pinfunction "D3")
			(pintype "tri_state")
		)
		(pad "16" thru_hole oval
			(at 2.54 19.05 180)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 140 "Net-(IC12-A4)")
			(pinfunction "D4")
			(pintype "tri_state")
		)
		(pad "17" thru_hole oval
			(at 0 20.32 180)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 141 "Net-(IC12-A5)")
			(pinfunction "D5")
			(pintype "tri_state")
		)
		(pad "18" thru_hole oval
			(at 2.54 21.59 180)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 142 "Net-(IC12-A6)")
			(pinfunction "D6")
			(pintype "tri_state")
		)
		(pad "19" thru_hole oval
			(at 0 22.86 180)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 143 "Net-(IC12-A7)")
			(pinfunction "D7")
			(pintype "tri_state")
		)
		(pad "20" thru_hole oval
			(at 2.54 24.13 180)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 319 "unconnected-(IC12-N.C.-Pad20)")
			(pinfunction "N.C.")
			(pintype "no_connect")
		)
		(pad "21" thru_hole oval
			(at 0 25.4 180)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "VCC2")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(pad "22" thru_hole oval
			(at 2.54 26.67 180)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 135 "~{OWE}")
			(pinfunction "~{UWE}")
			(pintype "input")
		)
		(pad "23" thru_hole oval
			(at 0 27.94 180)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 135 "~{OWE}")
			(pinfunction "~{LWE}")
			(pintype "input")
		)
		(pad "24" thru_hole oval
			(at 2.54 29.21 180)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 132 "~{ORAS}")
			(pinfunction "~{RAS}")
			(pintype "input")
		)
		(pad "25" thru_hole oval
			(at 0 30.48 180)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 136 "Net-(IC12-A0)")
			(pinfunction "A0")
			(pintype "input")
		)
		(pad "26" thru_hole oval
			(at 2.54 31.75 180)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 137 "Net-(IC12-A1)")
			(pinfunction "A1")
			(pintype "input")
		)
		(pad "27" thru_hole oval
			(at 0 33.02 180)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 138 "Net-(IC12-A2)")
			(pinfunction "A2")
			(pintype "input")
		)
		(pad "28" thru_hole oval
			(at 2.54 34.29 180)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 139 "Net-(IC12-A3)")
			(pinfunction "A3")
			(pintype "input")
		)
		(pad "29" thru_hole oval
			(at 0 35.56 180)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 140 "Net-(IC12-A4)")
			(pinfunction "A4")
			(pintype "input")
		)
		(pad "30" thru_hole oval
			(at 2.54 36.83 180)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "VCC2")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(pad "31" thru_hole oval
			(at 0 38.1 180)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 320 "unconnected-(IC12-N.C.-Pad31)")
			(pinfunction "N.C.")
			(pintype "no_connect")
		)
		(pad "32" thru_hole oval
			(at 2.54 39.37 180)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 321 "unconnected-(IC12-N.C.-Pad32)")
			(pinfunction "N.C.")
			(pintype "no_connect")
		)
		(pad "33" thru_hole oval
			(at 0 40.64 180)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "34" thru_hole oval
			(at 2.54 41.91 180)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 141 "Net-(IC12-A5)")
			(pinfunction "A5")
			(pintype "input")
		)
		(pad "35" thru_hole oval
			(at 0 43.18 180)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 142 "Net-(IC12-A6)")
			(pinfunction "A6")
			(pintype "input")
		)
		(pad "36" thru_hole oval
			(at 2.54 44.45 180)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 143 "Net-(IC12-A7)")
			(pinfunction "A7")
			(pintype "input")
		)
		(pad "37" thru_hole oval
			(at 0 45.72 180)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 322 "unconnected-(IC12-N.C.-Pad37)")
			(pinfunction "N.C.")
			(pintype "no_connect")
		)
		(pad "38" thru_hole oval
			(at 2.54 46.99 180)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 134 "~{OOE}")
			(pinfunction "~{OE}")
			(pintype "input")
		)
		(pad "39" thru_hole oval
			(at 0 48.26 180)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 133 "~{OCAS}")
			(pinfunction "~{CAS}")
			(pintype "input")
		)
		(pad "40" thru_hole oval
			(at 2.54 49.53 180)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Package_DIP.3dshapes/DIP-20_W7.62mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MegaCD_Footprints:PQFP-80_14x20mm_P0.8mm_long_pads"
		(layer "F.Cu")
		(at 100.323 110.849 90)
		(descr "PQFP80 14x20 / QIP80E CASE 122BS (see ON Semiconductor 122BS.PDF)")
		(tags "QFP 0.8")
		(property "Reference" "IC15"
			(at -13.8396 0.896 180)
			(layer "F.SilkS")
		)
		(property "Value" "LC8951"
			(at 0 5.08 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "MegaCD.kicad_sch")
		(attr smd)
		(fp_text user "41"
			(at 11.2048 8.2112 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "25"
			(at -5.5592 15.4756 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "65"
			(at 6.836 -16.503 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "64"
			(at 10.922 -11.677 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "${VALUE}"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "40"
			(at 4.1436 14.866 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "24"
			(at -12.4172 8.7192 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "•"
			(at 10.2616 5.4102 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "80"
			(at -7.642 -17.646 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "" smd circle
			(at -9.144 -12.446)
			(size 0.75 0.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
		)
		(pad "" smd circle
			(at -9.142 12.446)
			(size 0.75 0.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
		)
		(pad "" smd circle
			(at 9.144 -12.446)
			(size 0.75 0.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
		)
		(pad "" smd circle
			(at 9.146 12.446)
			(size 0.75 0.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
		)
		(pad "1" smd rect
			(at -9.017 -9.2 90)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "GND")
			(pinfunction "VSS")
			(pintype "power_in")
		)
		(pad "2" smd rect
			(at -9.017 -8.4 90)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 262 "/RAA6")
			(pinfunction "RA6")
			(pintype "output")
		)
		(pad "3" smd rect
			(at -9.017 -7.6 90)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 263 "/RAA7")
			(pinfunction "RA7")
			(pintype "output")
		)
		(pad "4" smd rect
			(at -9.017 -6.8 90)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 264 "/RAA8")
			(pinfunction "RA8")
			(pintype "output")
		)
		(pad "5" smd rect
			(at -9.017 -6 90)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 265 "/RAA9")
			(pinfunction "RA9")
			(pintype "output")
		)
		(pad "6" smd rect
			(at -9.017 -5.2 90)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 266 "/RAA10")
			(pinfunction "RA10")
			(pintype "output")
		)
		(pad "7" smd rect
			(at -9.017 -4.4 90)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 267 "/RAA11")
			(pinfunction "RA11")
			(pintype "output")
		)
		(pad "8" smd rect
			(at -9.017 -3.6 90)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 268 "/RAA12")
			(pinfunction "RA12")
			(pintype "output")
		)
		(pad "9" smd rect
			(at -9.017 -2.8 90)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 310 "~{RAACS1}")
			(pinfunction "RA13")
			(pintype "output")
		)
		(pad "10" smd rect
			(at -9.017 -2 90)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 269 "unconnected-(IC15-RA14-Pad10)")
			(pinfunction "RA14")
			(pintype "output+no_connect")
		)
		(pad "11" smd rect
			(at -9.017 -1.2 90)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 270 "unconnected-(IC15-RA15-Pad11)")
			(pinfunction "RA15")
			(pintype "output+no_connect")
		)
		(pad "12" smd rect
			(at -9.017 -0.4 90)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 271 "Net-(IC15-~{RWE})")
			(pinfunction "~{RWE}")
			(pintype "output")
		)
		(pad "13" smd rect
			(at -9.017 0.4 90)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "GND")
			(pinfunction "VSS")
			(pintype "power_in")
		)
		(pad "14" smd rect
			(at -9.017 1.2 90)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 272 "Net-(IC15-~{ROE})")
			(pinfunction "~{ROE}")
			(pintype "output")
		)
		(pad "15" smd rect
			(at -9.017 2 90)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 273 "unconnected-(IC15-ERA-Pad15)")
			(pinfunction "ERA")
			(pintype "passive+no_connect")
		)
		(pad "16" smd rect
			(at -9.017 2.8 90)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 274 "/CD7")
			(pinfunction "IO8")
			(pintype "bidirectional")
		)
		(pad "17" smd rect
			(at -9.017 3.58 90)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 275 "/CD6")
			(pinfunction "IO7")
			(pintype "bidirectional")
		)
		(pad "18" smd rect
			(at -9.017 4.4 90)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 276 "/CD5")
			(pinfunction "IO6")
			(pintype "bidirectional")
		)
		(pad "19" smd rect
			(at -9.017 5.2 90)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 277 "/CD4")
			(pinfunction "IO5")
			(pintype "bidirectional")
		)
		(pad "20" smd rect
			(at -9.017 6 90)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 278 "/CD3")
			(pinfunction "IO4")
			(pintype "bidirectional")
		)
		(pad "21" smd rect
			(at -9.017 6.8 90)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 279 "/CD2")
			(pinfunction "IO3")
			(pintype "bidirectional")
		)
		(pad "22" smd rect
			(at -9.017 7.6 90)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 280 "/CD1")
			(pinfunction "IO2")
			(pintype "bidirectional")
		)
		(pad "23" smd rect
			(at -9.017 8.4 90)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 281 "/CD0")
			(pinfunction "IO1")
			(pintype "bidirectional")
		)
		(pad "24" smd rect
			(at -9.017 9.2 90)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "GND")
			(pinfunction "VSS")
			(pintype "power_in")
		)
		(pad "25" smd rect
			(at -6 12.065 180)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 7 "25M")
			(pinfunction "XTALCK")
			(pintype "input")
		)
		(pad "26" smd rect
			(at -5.2 12.065 180)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 282 "unconnected-(IC15-XTAL-Pad26)")
			(pinfunction "XTAL")
			(pintype "input+no_connect")
		)
		(pad "27" smd rect
			(at -4.4 12.065 180)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "GND")
			(pinfunction "TEST1")
			(pintype "passive")
		)
		(pad "28" smd rect
			(at -3.6 12.065 180)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "GND")
			(pinfunction "TEST2")
			(pintype "passive")
		)
		(pad "29" smd rect
			(at -2.8 12.065 180)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "GND")
			(pinfunction "CSEL")
			(pintype "passive")
		)
		(pad "30" smd rect
			(at -2 12.065 180)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "GND")
			(pinfunction "LMSEL")
			(pintype "passive")
		)
		(pad "31" smd rect
			(at -1.2 12.065 180)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 4 "VCC2")
			(pinfunction "VDD")
			(pintype "power_in")
		)
		(pad "32" smd rect
			(at -0.4 12.065 180)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 6 "LRCKB")
			(pinfunction "LRCK")
			(pintype "input")
		)
		(pad "33" smd rect
			(at 0.4 12.065 180)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 157 "SDATAB")
			(pinfunction "SDATA")
			(pintype "input")
		)
		(pad "34" smd rect
			(at 1.2 12.065 180)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 311 "BCK")
			(pinfunction "BCK")
			(pintype "input")
		)
		(pad "35" smd rect
			(at 2 12.065 180)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "GND")
			(pinfunction "VSS")
			(pintype "power_in")
		)
		(pad "36" smd rect
			(at 2.8 12.065 180)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 166 "C2LR")
			(pinfunction "C2PO")
			(pintype "input")
		)
		(pad "37" smd rect
			(at 3.6 12.065 180)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 283 "unconnected-(IC15-MCK-Pad37)")
			(pinfunction "MCK")
			(pintype "input+no_connect")
		)
		(pad "38" smd rect
			(at 4.4 12.065 180)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 53 "D0")
			(pinfunction "D0")
			(pintype "bidirectional")
		)
		(pad "39" smd rect
			(at 5.2 12.065 180)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 52 "D1")
			(pinfunction "D1")
			(pintype "bidirectional")
		)
		(pad "40" smd rect
			(at 6 12.065 180)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 51 "D2")
			(pinfunction "D2")
			(pintype "bidirectional")
		)
		(pad "41" smd rect
			(at 9.017 9.2 90)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "GND")
			(pinfunction "VSS")
			(pintype "power_in")
		)
		(pad "42" smd rect
			(at 9.017 8.4 90)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 50 "D3")
			(pinfunction "D3")
			(pintype "bidirectional")
		)
		(pad "43" smd rect
			(at 9.017 7.6 90)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 49 "D4")
			(pinfunction "D4")
			(pintype "bidirectional")
		)
		(pad "44" smd rect
			(at 9.017 6.8 90)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 102 "D5")
			(pinfunction "D5")
			(pintype "bidirectional")
		)
		(pad "45" smd rect
			(at 9.017 6 90)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 101 "D6")
			(pinfunction "D6")
			(pintype "bidirectional")
		)
		(pad "46" smd rect
			(at 9.017 5.2 90)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 100 "D7")
			(pinfunction "D7")
			(pintype "bidirectional")
		)
		(pad "47" smd rect
			(at 9.017 4.4 90)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 69 "A1")
			(pinfunction "RS")
			(pintype "input")
		)
		(pad "48" smd rect
			(at 9.017 3.6 90)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 165 "~{COE}")
			(pinfunction "~{RD}")
			(pintype "input")
		)
		(pad "49" smd rect
			(at 9.017 2.8 90)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 334 "~{CLWE}")
			(pinfunction "~{WR}")
			(pintype "input")
		)
		(pad "50" smd rect
			(at 9.017 2 90)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 164 "~{CDC}")
			(pinfunction "~{CS}")
			(pintype "input")
		)
		(pad "51" smd rect
			(at 9.017 1.2 90)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 163 "~{INT}")
			(pinfunction "~{INT}")
			(pintype "input")
		)
		(pad "52" smd rect
			(at 9.017 0.4 90)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "GND")
			(pinfunction "VSS")
			(pintype "power_in")
		)
		(pad "53" smd rect
			(at 9.017 -0.4 90)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 31 "~{ERES}")
			(pinfunction "~{RESET}")
			(pintype "input")
		)
		(pad "54" smd rect
			(at 9.017 -1.2 90)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "GND")
			(pinfunction "~{ENABLE}")
			(pintype "input")
		)
		(pad "55" smd rect
			(at 9.017 -2 90)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 4 "VCC2")
			(pinfunction "~{HWR}")
			(pintype "input")
		)
		(pad "56" smd rect
			(at 9.017 -2.8 90)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 162 "~{HRD}")
			(pinfunction "~{HRD}")
			(pintype "input")
		)
		(pad "57" smd rect
			(at 9.017 -3.6 90)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 4 "VCC2")
			(pinfunction "~{CMD}")
			(pintype "input")
		)
		(pad "58" smd rect
			(at 9.017 -4.4 90)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 161 "~{WAIT}")
			(pinfunction "~{WAIT}")
			(pintype "input")
		)
		(pad "59" smd rect
			(at 9.017 -5.2 90)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 160 "~{DTEN}")
			(pinfunction "~{DTEN}")
			(pintype "input")
		)
		(pad "60" smd rect
			(at 9.017 -6 90)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 284 "unconnected-(IC15-~{STEN}-Pad60)")
			(pinfunction "~{STEN}")
			(pintype "input+no_connect")
		)
		(pad "61" smd rect
			(at 9.017 -6.8 90)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 285 "unconnected-(IC15-~{EOP}-Pad61)")
			(pinfunction "~{EOP}")
			(pintype "input+no_connect")
		)
		(pad "62" smd rect
			(at 9.017 -7.6 90)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 286 "Net-(IC15-~{RCS})")
			(pinfunction "~{RCS}")
			(pintype "output")
		)
		(pad "63" smd rect
			(at 9.017 -8.4 90)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 287 "unconnected-(IC15-~{HDE}-Pad63)")
			(pinfunction "~{HDE}")
			(pintype "input+no_connect")
		)
		(pad "64" smd rect
			(at 9.017 -9.2 90)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "GND")
			(pinfunction "VSS")
			(pintype "power_in")
		)
		(pad "65" smd rect
			(at 6 -12.065 180)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 168 "PA7")
			(pinfunction "HD7")
			(pintype "bidirectional")
		)
		(pad "66" smd rect
			(at 5.2 -12.065 180)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 169 "PA6")
			(pinfunction "HD6")
			(pintype "bidirectional")
		)
		(pad "67" smd rect
			(at 4.4 -12.065 180)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 170 "PA5")
			(pinfunction "HD5")
			(pintype "bidirectional")
		)
		(pad "68" smd rect
			(at 3.6 -12.065 180)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 171 "PA4")
			(pinfunction "HD4")
			(pintype "bidirectional")
		)
		(pad "69" smd rect
			(at 2.8 -12.065 180)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 172 "PA3")
			(pinfunction "HD3")
			(pintype "bidirectional")
		)
		(pad "70" smd rect
			(at 2 -12.065 180)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 173 "PA2")
			(pinfunction "HD2")
			(pintype "bidirectional")
		)
		(pad "71" smd rect
			(at 1.2 -12.065 180)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 174 "PA1")
			(pinfunction "HD1")
			(pintype "bidirectional")
		)
		(pad "72" smd rect
			(at 0.4 -12.065 180)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 175 "PA0")
			(pinfunction "HD0")
			(pintype "bidirectional")
		)
		(pad "73" smd rect
			(at -0.4 -12.065 180)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 4 "VCC2")
			(pinfunction "VDD")
			(pintype "power_in")
		)
		(pad "74" smd rect
			(at -1.2 -12.065 180)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "GND")
			(pinfunction "SELDRQ")
			(pintype "input")
		)
		(pad "75" smd rect
			(at -2 -12.065 180)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 288 "/RAA0")
			(pinfunction "RA0")
			(pintype "output")
		)
		(pad "76" smd rect
			(at -2.8 -12.065 180)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 289 "/RAA1")
			(pinfunction "RA1")
			(pintype "output")
		)
		(pad "77" smd rect
			(at -3.6 -12.065 180)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 290 "/RAA2")
			(pinfunction "RA2")
			(pintype "output")
		)
		(pad "78" smd rect
			(at -4.4 -12.065 180)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 291 "/RAA3")
			(pinfunction "RA3")
			(pintype "output")
		)
		(pad "79" smd rect
			(at -5.2 -12.065 180)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 292 "/RAA4")
			(pinfunction "RA4")
			(pintype "output")
		)
		(pad "80" smd rect
			(at -6 -12.065 180)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 293 "/RAA5")
			(pinfunction "RA5")
			(pintype "output")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Package_QFP.3dshapes/PQFP-80_14x20mm_P0.8mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MegaCD_Footprints:CON-21P"
		(layer "F.Cu")
		(at 57.15 91.279 -90)
		(descr "20-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
		(tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
		(property "Reference" "CN3"
			(at 9.178 2.8194 270)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "CON 21P"
			(at 19.05 2.54 270)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x21, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "MegaCD.kicad_sch")
		(attr through_hole)
		(fp_text user "21"
			(at 23.3004 4.6482 270)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "1"
			(at -0.474 4.3434 270)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "2"
			(at 0.796 2.9718 270)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "20"
			(at 22.2844 3.0734 270)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "${REFERENCE}"
			(at 6.35 2.54 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole roundrect
			(at 1.25 -2.54)
			(size 1.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 30 "Net-(CN3-Pin_19)")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole roundrect
			(at 2.5 0)
			(size 1.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 31 "~{ERES}")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole roundrect
			(at 3.75 -2.54)
			(size 1.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 32 "BCLKB")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(pad "5" thru_hole roundrect
			(at 5 0)
			(size 1.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 6 "LRCKB")
			(pinfunction "Pin_5")
			(pintype "passive")
		)
		(pad "6" thru_hole roundrect
			(at 6.25 -2.54)
			(size 1.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 33 "DFCKB")
			(pinfunction "Pin_6")
			(pintype "passive")
		)
		(pad "7" thru_hole roundrect
			(at 7.5 0)
			(size 1.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 34 "DDATA")
			(pinfunction "Pin_7")
			(pintype "passive")
		)
		(pad "8" thru_hole roundrect
			(at 8.75 -2.54)
			(size 1.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 35 "ATT")
			(pinfunction "Pin_8")
			(pintype "passive")
		)
		(pad "9" thru_hole roundrect
			(at 10 0)
			(size 1.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 36 "SHFT")
			(pinfunction "Pin_9")
			(pintype "passive")
		)
		(pad "10" thru_hole roundrect
			(at 11.25 -2.54)
			(size 1.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 37 "LATCH")
			(pinfunction "Pin_10")
			(pintype "passive")
		)
		(pad "11" thru_hole roundrect
			(at 12.5 0)
			(size 1.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 38 "VCC")
			(pinfunction "Pin_11")
			(pintype "passive")
		)
		(pad "12" thru_hole roundrect
			(at 13.75 -2.54)
			(size 1.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "Pin_12")
			(pintype "passive")
		)
		(pad "13" thru_hole roundrect
			(at 15 0)
			(size 1.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 39 "PDATA")
			(pinfunction "Pin_13")
			(pintype "passive")
		)
		(pad "14" thru_hole roundrect
			(at 16.25 -2.54)
			(size 1.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 40 "PWCLK")
			(pinfunction "Pin_14")
			(pintype "passive")
		)
		(pad "15" thru_hole roundrect
			(at 17.5 0)
			(size 1.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 41 "PBCLK")
			(pinfunction "Pin_15")
			(pintype "passive")
		)
		(pad "16" thru_hole roundrect
			(at 18.75 -2.54)
			(size 1.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 42 "PLRCK")
			(pinfunction "Pin_16")
			(pintype "passive")
		)
		(pad "17" thru_hole roundrect
			(at 20 0)
			(size 1.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 43 "SL2")
			(pinfunction "Pin_17")
			(pintype "passive")
		)
		(pad "18" thru_hole roundrect
			(at 21.25 -2.54)
			(size 1.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 44 "SR2")
			(pinfunction "Pin_18")
			(pintype "passive")
		)
		(pad "19" thru_hole roundrect
			(at 22.5 0)
			(size 1.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 30 "Net-(CN3-Pin_19)")
			(pinfunction "Pin_19")
			(pintype "passive")
		)
		(pad "20" thru_hole roundrect
			(at 23.75 -2.54)
			(size 1.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 28 "M.VCC")
			(pinfunction "Pin_20")
			(pintype "passive")
		)
		(pad "21" thru_hole roundrect
			(at 25 0)
			(size 1.4 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 29 "M.GND")
			(pinfunction "Pin_21")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Package_DIP.3dshapes/DIP-20_W7.62mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MegaCD_Footprints:CP_Elec_3x5.4"
		(layer "F.Cu")
		(at 65.151 57.531 90)
		(descr "SMD capacitor, aluminum electrolytic, Nichicon, 3.0x5.4mm")
		(tags "capacitor electrolytic")
		(property "Reference" "C42"
			(at 1.0668 -3.048 270)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "10uF"
			(at 0 2.7 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Polarized capacitor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "MegaCD.kicad_sch")
		(attr smd)
		(fp_text user "+"
			(at -4.9276 -0.3556 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "-"
			(at 2.4892 2.1336 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.597 0 90)
			(size 2.394 1.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.15625)
			(net 4 "VCC2")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.597 0 90)
			(size 2.394 1.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.15625)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/CP_Elec_3x5.4.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MegaCD_Footprints:SOIC-14W_5.3mm_P1.27mm"
		(layer "F.Cu")
		(at 95.2754 66.167 90)
		(descr "16-Lead Plastic Small Outline (SO) - Wide, 5.3 mm Body (http://www.ti.com/lit/ml/msop002a/msop002a.pdf)")
		(tags "SOIC 1.27")
		(property "Reference" "IC16"
			(at 6.2992 -3.0988 180)
			(layer "F.SilkS")
		)
		(property "Value" "74HC86"
			(at 0 6.2 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Quad 2-input XOR"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "MegaCD.kicad_sch")
		(attr smd)
		(fp_text user "${VALUE}"
			(at 0 -0.6604 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "${REFERENCE}"
			(at 0 -0.762 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -3.55 -4.445 90)
			(size 1.5 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 4 "VCC2")
			(pintype "input")
		)
		(pad "2" smd rect
			(at -3.55 -3.175 90)
			(size 1.5 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 32 "BCLKB")
			(pintype "input")
		)
		(pad "3" smd rect
			(at -3.55 -1.905 90)
			(size 1.5 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 311 "BCK")
			(pintype "output")
		)
		(pad "4" smd rect
			(at -3.55 -0.635 90)
			(size 1.5 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 4 "VCC2")
			(pintype "input")
		)
		(pad "5" smd rect
			(at -3.55 0.635 90)
			(size 1.5 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 310 "~{RAACS1}")
			(pintype "input")
		)
		(pad "6" smd rect
			(at -3.55 1.905 90)
			(size 1.5 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 312 "~{RAACS2}")
			(pintype "output")
		)
		(pad "7" smd rect
			(at -3.55 3.175 90)
			(size 1.5 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "8" smd rect
			(at 3.556 3.175 90)
			(size 1.5 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 240 "~{CLWEX}")
			(pintype "output")
		)
		(pad "9" smd rect
			(at 3.55 1.905 90)
			(size 1.5 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 334 "~{CLWE}")
			(pintype "input")
		)
		(pad "10" smd rect
			(at 3.55 0.635 90)
			(size 1.5 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "GND")
			(pintype "input")
		)
		(pad "11" smd rect
			(at 3.55 -0.635 90)
			(size 1.5 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 335 "unconnected-(IC16-Pad11)")
			(pintype "output+no_connect")
		)
		(pad "12" smd rect
			(at 3.55 -1.905 90)
			(size 1.5 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 4 "VCC2")
			(pintype "input")
		)
		(pad "13" smd rect
			(at 3.55 -3.175 90)
			(size 1.5 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 4 "VCC2")
			(pintype "input")
		)
		(pad "14" smd rect
			(at 3.55 -4.445 90)
			(size 1.5 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 4 "VCC2")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Package_SO.3dshapes/SOIC-16W_5.3x10.2mm_P1.27mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MegaCD_Footprints:SOT-23-Wide"
		(layer "F.Cu")
		(at 224.155 114.046 90)
		(descr "SOT, 3 Pin (https://www.jedec.org/system/files/docs/to-236h.pdf variant AB), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOT TO_SOT_SMD")
		(property "Reference" "TR2"
			(at 3.5814 1.3208 180)
			(layer "F.SilkS")
		)
		(property "Value" "C1623"
			(at 0 2.4 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Bipolar transistor symbol for simulation only, substrate tied to the emitter"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Device" "NPN"
			(at 338.201 -110.109 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" "1=B 2=E 3=C"
			(at 338.201 -110.109 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Type" "GUMMELPOON"
			(at 338.201 -110.109 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "MegaCD.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.016 -0.95 90)
			(size 1.5 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 300 "Net-(TR2-B)")
			(pinfunction "B")
			(pintype "input")
		)
		(pad "2" smd roundrect
			(at -1.016 0.95 90)
			(size 1.5 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "E")
			(pintype "open_emitter")
		)
		(pad "3" smd roundrect
			(at 1.016 0 90)
			(size 1.5 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 295 "Net-(LD1-K)")
			(pinfunction "C")
			(pintype "open_collector")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MegaCD_Footprints:Battery_no_symbols"
		(layer "F.Cu")
		(at 208.9658 59.309)
		(descr "20-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
		(tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
		(property "Reference" "BT1"
			(at 0.4064 7.874 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "AL2032"
			(at 7.62 0 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Multiple-cell battery"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "MegaCD.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 20.32 7.62 180)
			(layer "F.Fab")
		)
		(pad "1" thru_hole oval
			(at 0 -5.08 90)
			(size 2 2)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "Net-(BT1-+)")
			(pinfunction "+")
			(pintype "passive")
		)
		(pad "1" thru_hole oval
			(at 0 5.08 90)
			(size 2 2)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "Net-(BT1-+)")
			(pinfunction "+")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 15.24 0 90)
			(size 2 2)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "-")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 17.78 0 90)
			(size 2 2)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "-")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Package_DIP.3dshapes/DIP-20_W7.62mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MegaCD_Footprints:SOIC-28Wider"
		(layer "F.Cu")
		(at 72.39 117.094 90)
		(descr "SOIC, 28 Pin (JEDEC MS-013AE, https://www.analog.com/media/en/package-pcb-resources/package/35833120341221rw_28.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOIC SO")
		(property "Reference" "IC17"
			(at -6.0198 11.2014 180)
			(layer "F.SilkS")
		)
		(property "Value" "MB8464A-90L"
			(at 0 9.9 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "MegaCD.kicad_sch")
		(attr smd)
		(fp_text user "${VALUE}"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -5.715 -8.255 90)
			(size 2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 330 "unconnected-(IC17-N.C.-Pad1)")
			(pinfunction "N.C.")
			(pintype "no_connect")
		)
		(pad "2" smd roundrect
			(at -5.715 -6.985 90)
			(size 2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 268 "/RAA12")
			(pinfunction "A12")
			(pintype "input")
		)
		(pad "3" smd roundrect
			(at -5.715 -5.715 90)
			(size 2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 263 "/RAA7")
			(pinfunction "A7")
			(pintype "input")
		)
		(pad "4" smd roundrect
			(at -5.715 -4.445 90)
			(size 2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 262 "/RAA6")
			(pinfunction "A6")
			(pintype "input")
		)
		(pad "5" smd roundrect
			(at -5.715 -3.175 90)
			(size 2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 293 "/RAA5")
			(pinfunction "A5")
			(pintype "input")
		)
		(pad "6" smd roundrect
			(at -5.715 -1.905 90)
			(size 2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 292 "/RAA4")
			(pinfunction "A4")
			(pintype "input")
		)
		(pad "7" smd roundrect
			(at -5.715 -0.635 90)
			(size 2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 291 "/RAA3")
			(pinfunction "A3")
			(pintype "input")
		)
		(pad "8" smd roundrect
			(at -5.715 0.635 90)
			(size 2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 290 "/RAA2")
			(pinfunction "A2")
			(pintype "input")
		)
		(pad "9" smd roundrect
			(at -5.715 1.905 90)
			(size 2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 289 "/RAA1")
			(pinfunction "A1")
			(pintype "input")
		)
		(pad "10" smd roundrect
			(at -5.715 3.175 90)
			(size 2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 288 "/RAA0")
			(pinfunction "A0")
			(pintype "input")
		)
		(pad "11" smd roundrect
			(at -5.715 4.445 90)
			(size 2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 281 "/CD0")
			(pinfunction "D0")
			(pintype "tri_state")
		)
		(pad "12" smd roundrect
			(at -5.715 5.715 90)
			(size 2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 280 "/CD1")
			(pinfunction "D1")
			(pintype "tri_state")
		)
		(pad "13" smd roundrect
			(at -5.715 6.985 90)
			(size 2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 279 "/CD2")
			(pinfunction "D2")
			(pintype "tri_state")
		)
		(pad "14" smd roundrect
			(at -5.715 8.255 90)
			(size 2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "15" smd roundrect
			(at 5.715 8.255 90)
			(size 2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 278 "/CD3")
			(pinfunction "D3")
			(pintype "tri_state")
		)
		(pad "16" smd roundrect
			(at 5.715 6.985 90)
			(size 2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 277 "/CD4")
			(pinfunction "D4")
			(pintype "tri_state")
		)
		(pad "17" smd roundrect
			(at 5.715 5.715 90)
			(size 2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 276 "/CD5")
			(pinfunction "D5")
			(pintype "tri_state")
		)
		(pad "18" smd roundrect
			(at 5.715 4.445 90)
			(size 2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 275 "/CD6")
			(pinfunction "D6")
			(pintype "tri_state")
		)
		(pad "19" smd roundrect
			(at 5.715 3.175 90)
			(size 2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 274 "/CD7")
			(pinfunction "D7")
			(pintype "tri_state")
		)
		(pad "20" smd roundrect
			(at 5.715 1.905 90)
			(size 2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 286 "Net-(IC15-~{RCS})")
			(pinfunction "~{CS1}")
			(pintype "input")
		)
		(pad "21" smd roundrect
			(at 5.715 0.635 90)
			(size 2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 266 "/RAA10")
			(pinfunction "A10")
			(pintype "input")
		)
		(pad "22" smd roundrect
			(at 5.715 -0.635 90)
			(size 2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 272 "Net-(IC15-~{ROE})")
			(pinfunction "~{OE}")
			(pintype "input")
		)
		(pad "23" smd roundrect
			(at 5.715 -1.905 90)
			(size 2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 267 "/RAA11")
			(pinfunction "A11")
			(pintype "input")
		)
		(pad "24" smd roundrect
			(at 5.715 -3.175 90)
			(size 2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 265 "/RAA9")
			(pinfunction "A9")
			(pintype "input")
		)
		(pad "25" smd roundrect
			(at 5.715 -4.445 90)
			(size 2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 264 "/RAA8")
			(pinfunction "A8")
			(pintype "input")
		)
		(pad "26" smd roundrect
			(at 5.715 -5.715 90)
			(size 2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 310 "~{RAACS1}")
			(pinfunction "CS2")
			(pintype "input")
		)
		(pad "27" smd roundrect
			(at 5.715 -6.985 90)
			(size 2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 271 "Net-(IC15-~{RWE})")
			(pinfunction "~{WE}")
			(pintype "input")
		)
		(pad "28" smd roundrect
			(at 5.715 -8.255 90)
			(size 2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 4 "VCC2")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Package_SO.3dshapes/SOIC-28W_7.5x17.9mm_P1.27mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MegaCD_Footprints:ZIP-20"
		(layer "F.Cu")
		(at 148.209 124.7902 90)
		(descr "20-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
		(tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
		(property "Reference" "IC6"
			(at 4.7244 -1.3716 180)
			(layer "F.SilkS")
		)
		(property "Value" "MB81C4256Z"
			(at 1.27 26.67 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "MegaCD.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 1.016 -2.54 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 90)
			(size 1.3 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 165 "~{COE}")
			(pinfunction "~{OE}")
			(pintype "input")
		)
		(pad "2" thru_hole roundrect
			(at 2.54 1.27 90)
			(size 1.3 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 177 "~{PCAS}")
			(pinfunction "~{CAS}")
			(pintype "input")
		)
		(pad "3" thru_hole roundrect
			(at 0 2.54 90)
			(size 1.3 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 101 "D6")
			(pinfunction "D2")
			(pintype "tri_state")
		)
		(pad "4" thru_hole roundrect
			(at 2.54 3.81 90)
			(size 1.3 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 100 "D7")
			(pinfunction "D3")
			(pintype "tri_state")
		)
		(pad "5" thru_hole roundrect
			(at 0 5.08 90)
			(size 1.3 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "VSS")
			(pintype "power_in")
		)
		(pad "6" thru_hole roundrect
			(at 2.54 6.35 90)
			(size 1.3 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 49 "D4")
			(pinfunction "D0")
			(pintype "tri_state")
		)
		(pad "7" thru_hole roundrect
			(at 0 7.62 90)
			(size 1.3 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 102 "D5")
			(pinfunction "D1")
			(pintype "tri_state")
		)
		(pad "8" thru_hole roundrect
			(at 2.54 8.89 90)
			(size 1.3 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 334 "~{CLWE}")
			(pinfunction "~{WE}")
			(pintype "input")
		)
		(pad "9" thru_hole roundrect
			(at 0 10.16 90)
			(size 1.3 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 176 "~{PRAS}")
			(pinfunction "~{RAS}")
			(pintype "input")
		)
		(pad "10" thru_hole roundrect
			(at 2.54 11.43 90)
			(size 1.3 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 253 "unconnected-(IC6-N.C.-Pad10)")
			(pinfunction "N.C.")
			(pintype "input+no_connect")
		)
		(pad "11" thru_hole roundrect
			(at 0 12.7 90)
			(size 1.3 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 175 "PA0")
			(pinfunction "A0")
			(pintype "input")
		)
		(pad "12" thru_hole roundrect
			(at 2.54 13.97 90)
			(size 1.3 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 174 "PA1")
			(pinfunction "A1")
			(pintype "input")
		)
		(pad "13" thru_hole roundrect
			(at 0 15.24 90)
			(size 1.3 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 173 "PA2")
			(pinfunction "A2")
			(pintype "input")
		)
		(pad "14" thru_hole roundrect
			(at 2.54 16.51 90)
			(size 1.3 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 172 "PA3")
			(pinfunction "A3")
			(pintype "input")
		)
		(pad "15" thru_hole roundrect
			(at 0 17.78 90)
			(size 1.3 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 4 "VCC2")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(pad "16" thru_hole roundrect
			(at 2.54 19.05 90)
			(size 1.3 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 171 "PA4")
			(pinfunction "A4")
			(pintype "input")
		)
		(pad "17" thru_hole roundrect
			(at 0 20.32 90)
			(size 1.3 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 170 "PA5")
			(pinfunction "A5")
			(pintype "input")
		)
		(pad "18" thru_hole roundrect
			(at 2.54 21.59 90)
			(size 1.3 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 169 "PA6")
			(pinfunction "A6")
			(pintype "input")
		)
		(pad "19" thru_hole roundrect
			(at 0 22.86 90)
			(size 1.3 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 168 "PA7")
			(pinfunction "A7")
			(pintype "input")
		)
		(pad "20" thru_hole roundrect
			(at 2.54 24.13 90)
			(size 1.3 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 167 "PA8")
			(pinfunction "A8")
			(pintype "input")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Package_DIP.3dshapes/DIP-20_W7.62mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MegaCD_Footprints:SOIC-28Wider"
		(layer "F.Cu")
		(at 73.66 68.326 90)
		(descr "SOIC, 28 Pin (JEDEC MS-013AE, https://www.analog.com/media/en/package-pcb-resources/package/35833120341221rw_28.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOIC SO")
		(property "Reference" "IC13"
			(at -2.667 -12.6746 180)
			(layer "F.SilkS")
		)
		(property "Value" "TC51832"
			(at 0 9.9 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "MegaCD.kicad_sch")
		(attr smd)
		(fp_text user "${VALUE}"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -5.715 -8.255 90)
			(size 2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 232 "/RA14")
			(pinfunction "A14")
			(pintype "input")
		)
		(pad "2" smd roundrect
			(at -5.715 -6.985 90)
			(size 2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 234 "/RA12")
			(pinfunction "A12")
			(pintype "input")
		)
		(pad "3" smd roundrect
			(at -5.715 -5.715 90)
			(size 2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 243 "/RA7")
			(pinfunction "A7")
			(pintype "input")
		)
		(pad "4" smd roundrect
			(at -5.715 -4.445 90)
			(size 2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 244 "/RA6")
			(pinfunction "A6")
			(pintype "input")
		)
		(pad "5" smd roundrect
			(at -5.715 -3.175 90)
			(size 2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 245 "/RA5")
			(pinfunction "A5")
			(pintype "input")
		)
		(pad "6" smd roundrect
			(at -5.715 -1.905 90)
			(size 2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 246 "/RA4")
			(pinfunction "A4")
			(pintype "input")
		)
		(pad "7" smd roundrect
			(at -5.715 -0.635 90)
			(size 2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 248 "/RA3")
			(pinfunction "A3")
			(pintype "input")
		)
		(pad "8" smd roundrect
			(at -5.715 0.635 90)
			(size 2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 249 "/RA2")
			(pinfunction "A2")
			(pintype "input")
		)
		(pad "9" smd roundrect
			(at -5.715 1.905 90)
			(size 2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 250 "/RA1")
			(pinfunction "A1")
			(pintype "input")
		)
		(pad "10" smd roundrect
			(at -5.715 3.175 90)
			(size 2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 251 "/RA0")
			(pinfunction "A0")
			(pintype "input")
		)
		(pad "11" smd roundrect
			(at -5.715 4.445 90)
			(size 2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 231 "/WD0")
			(pinfunction "D0")
			(pintype "tri_state")
		)
		(pad "12" smd roundrect
			(at -5.715 5.715 90)
			(size 2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 230 "/WD1")
			(pinfunction "D1")
			(pintype "tri_state")
		)
		(pad "13" smd roundrect
			(at -5.715 6.985 90)
			(size 2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 229 "/WD2")
			(pinfunction "D2")
			(pintype "tri_state")
		)
		(pad "14" smd roundrect
			(at -5.715 8.255 90)
			(size 2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "15" smd roundrect
			(at 5.715 8.255 90)
			(size 2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 228 "/WD3")
			(pinfunction "D3")
			(pintype "tri_state")
		)
		(pad "16" smd roundrect
			(at 5.715 6.985 90)
			(size 2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 227 "/WD4")
			(pinfunction "D4")
			(pintype "tri_state")
		)
		(pad "17" smd roundrect
			(at 5.715 5.715 90)
			(size 2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 226 "/WD5")
			(pinfunction "D5")
			(pintype "tri_state")
		)
		(pad "18" smd roundrect
			(at 5.715 4.445 90)
			(size 2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 225 "/WD6")
			(pinfunction "D6")
			(pintype "tri_state")
		)
		(pad "19" smd roundrect
			(at 5.715 3.175 90)
			(size 2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 224 "/WD7")
			(pinfunction "D7")
			(pintype "tri_state")
		)
		(pad "20" smd roundrect
			(at 5.715 1.905 90)
			(size 2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 241 "~{RCS1X}")
			(pinfunction "~{CE}")
			(pintype "input")
		)
		(pad "21" smd roundrect
			(at 5.715 0.635 90)
			(size 2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 236 "/RA10")
			(pinfunction "A10")
			(pintype "input")
		)
		(pad "22" smd roundrect
			(at 5.715 -0.635 90)
			(size 2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 309 "~{ROE}")
			(pinfunction "~{OE}")
			(pintype "input")
		)
		(pad "23" smd roundrect
			(at 5.715 -1.905 90)
			(size 2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 235 "/RA11")
			(pinfunction "A11")
			(pintype "input")
		)
		(pad "24" smd roundrect
			(at 5.715 -3.175 90)
			(size 2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 237 "/RA9")
			(pinfunction "A9")
			(pintype "input")
		)
		(pad "25" smd roundrect
			(at 5.715 -4.445 90)
			(size 2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 238 "/RA8")
			(pinfunction "A8")
			(pintype "input")
		)
		(pad "26" smd roundrect
			(at 5.715 -5.715 90)
			(size 2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 233 "/RA13")
			(pinfunction "A13")
			(pintype "input")
		)
		(pad "27" smd roundrect
			(at 5.715 -6.985 90)
			(size 2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 242 "Net-(IC13-~{WE})")
			(pinfunction "~{WE}")
			(pintype "input")
		)
		(pad "28" smd roundrect
			(at 5.715 -8.255 90)
			(size 2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 4 "VCC2")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Package_SO.3dshapes/SOIC-28W_7.5x17.9mm_P1.27mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MegaCD_Footprints:SOIC-28Wider"
		(layer "F.Cu")
		(at 72.39 100.711 90)
		(descr "SOIC, 28 Pin (JEDEC MS-013AE, https://www.analog.com/media/en/package-pcb-resources/package/35833120341221rw_28.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOIC SO")
		(property "Reference" "IC18"
			(at 1.016 -10.4394 270)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "MB8464A-90L"
			(at 0 9.9 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "MegaCD.kicad_sch")
		(attr smd)
		(fp_text user "${VALUE}"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -5.715 -8.255 90)
			(size 2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 331 "unconnected-(IC18-N.C.-Pad1)")
			(pinfunction "N.C.")
			(pintype "no_connect")
		)
		(pad "2" smd roundrect
			(at -5.715 -6.985 90)
			(size 2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 268 "/RAA12")
			(pinfunction "A12")
			(pintype "input")
		)
		(pad "3" smd roundrect
			(at -5.715 -5.715 90)
			(size 2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 263 "/RAA7")
			(pinfunction "A7")
			(pintype "input")
		)
		(pad "4" smd roundrect
			(at -5.715 -4.445 90)
			(size 2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 262 "/RAA6")
			(pinfunction "A6")
			(pintype "input")
		)
		(pad "5" smd roundrect
			(at -5.715 -3.175 90)
			(size 2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 293 "/RAA5")
			(pinfunction "A5")
			(pintype "input")
		)
		(pad "6" smd roundrect
			(at -5.715 -1.905 90)
			(size 2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 292 "/RAA4")
			(pinfunction "A4")
			(pintype "input")
		)
		(pad "7" smd roundrect
			(at -5.715 -0.635 90)
			(size 2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 291 "/RAA3")
			(pinfunction "A3")
			(pintype "input")
		)
		(pad "8" smd roundrect
			(at -5.715 0.635 90)
			(size 2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 290 "/RAA2")
			(pinfunction "A2")
			(pintype "input")
		)
		(pad "9" smd roundrect
			(at -5.715 1.905 90)
			(size 2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 289 "/RAA1")
			(pinfunction "A1")
			(pintype "input")
		)
		(pad "10" smd roundrect
			(at -5.715 3.175 90)
			(size 2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 288 "/RAA0")
			(pinfunction "A0")
			(pintype "input")
		)
		(pad "11" smd roundrect
			(at -5.715 4.445 90)
			(size 2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 281 "/CD0")
			(pinfunction "D0")
			(pintype "tri_state")
		)
		(pad "12" smd roundrect
			(at -5.715 5.715 90)
			(size 2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 280 "/CD1")
			(pinfunction "D1")
			(pintype "tri_state")
		)
		(pad "13" smd roundrect
			(at -5.715 6.985 90)
			(size 2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 279 "/CD2")
			(pinfunction "D2")
			(pintype "tri_state")
		)
		(pad "14" smd roundrect
			(at -5.715 8.255 90)
			(size 2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "15" smd roundrect
			(at 5.715 8.255 90)
			(size 2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 278 "/CD3")
			(pinfunction "D3")
			(pintype "tri_state")
		)
		(pad "16" smd roundrect
			(at 5.715 6.985 90)
			(size 2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 277 "/CD4")
			(pinfunction "D4")
			(pintype "tri_state")
		)
		(pad "17" smd roundrect
			(at 5.715 5.715 90)
			(size 2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 276 "/CD5")
			(pinfunction "D5")
			(pintype "tri_state")
		)
		(pad "18" smd roundrect
			(at 5.715 4.445 90)
			(size 2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 275 "/CD6")
			(pinfunction "D6")
			(pintype "tri_state")
		)
		(pad "19" smd roundrect
			(at 5.715 3.175 90)
			(size 2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 274 "/CD7")
			(pinfunction "D7")
			(pintype "tri_state")
		)
		(pad "20" smd roundrect
			(at 5.715 1.905 90)
			(size 2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 286 "Net-(IC15-~{RCS})")
			(pinfunction "~{CS1}")
			(pintype "input")
		)
		(pad "21" smd roundrect
			(at 5.715 0.635 90)
			(size 2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 266 "/RAA10")
			(pinfunction "A10")
			(pintype "input")
		)
		(pad "22" smd roundrect
			(at 5.715 -0.635 90)
			(size 2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 272 "Net-(IC15-~{ROE})")
			(pinfunction "~{OE}")
			(pintype "input")
		)
		(pad "23" smd roundrect
			(at 5.715 -1.905 90)
			(size 2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 267 "/RAA11")
			(pinfunction "A11")
			(pintype "input")
		)
		(pad "24" smd roundrect
			(at 5.715 -3.175 90)
			(size 2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 265 "/RAA9")
			(pinfunction "A9")
			(pintype "input")
		)
		(pad "25" smd roundrect
			(at 5.715 -4.445 90)
			(size 2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 264 "/RAA8")
			(pinfunction "A8")
			(pintype "input")
		)
		(pad "26" smd roundrect
			(at 5.715 -5.715 90)
			(size 2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 312 "~{RAACS2}")
			(pinfunction "CS2")
			(pintype "input")
		)
		(pad "27" smd roundrect
			(at 5.715 -6.985 90)
			(size 2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 271 "Net-(IC15-~{RWE})")
			(pinfunction "~{WE}")
			(pintype "input")
		)
		(pad "28" smd roundrect
			(at 5.715 -8.255 90)
			(size 2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 4 "VCC2")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Package_SO.3dshapes/SOIC-28W_7.5x17.9mm_P1.27mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MegaCD_Footprints:EDGE-60P"
		(layer "F.Cu")
		(at 120.65 50.8)
		(property "Reference" "CN2"
			(at -22.2504 6.5278 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "EDGE 60P"
			(at 10.16 5.08 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, double row, 02x30, row letter first pin numbering scheme (pin number consists of a letter for the row and a number for the pin index in this row. a1, ..., aN; b1, ..., bN), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "MegaCD.kicad_sch")
		(attr smd)
		(fp_text user "B1"
			(at 36 5.85 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "B30"
			(at -38.3 6.2 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "A1"
			(at 37.7 5.8 0)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(fp_text user "A30"
			(at -35.45 6.2 0)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(fp_text user "${REFERENCE}"
			(at -10.16 5.08 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "a1" smd rect
			(at 36.83 0 90)
			(size 8 1.778)
			(layers "B.Cu")
			(net 2 "GND")
			(pinfunction "Pin_a1")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "a2" smd rect
			(at 34.29 0 90)
			(size 8 1.778)
			(layers "B.Cu")
			(net 294 "unconnected-(CN2-Pin_a2-Pada2)")
			(pinfunction "Pin_a2")
			(pintype "passive+no_connect")
			(thermal_bridge_angle 45)
		)
		(pad "a3" smd rect
			(at 31.75 0 90)
			(size 8 1.778)
			(layers "B.Cu")
			(net 106 "~{CAS0}")
			(pinfunction "Pin_a3")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "a4" smd rect
			(at 29.21 0 90)
			(size 8 1.778)
			(layers "B.Cu")
			(net 196 "VD0")
			(pinfunction "Pin_a4")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "a5" smd rect
			(at 26.67 0 90)
			(size 8 1.778)
			(layers "B.Cu")
			(net 197 "VD1")
			(pinfunction "Pin_a5")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "a6" smd rect
			(at 24.13 0 90)
			(size 8 1.778)
			(layers "B.Cu")
			(net 198 "VD2")
			(pinfunction "Pin_a6")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "a7" smd rect
			(at 21.59 0 90)
			(size 8 1.778)
			(layers "B.Cu")
			(net 199 "VD3")
			(pinfunction "Pin_a7")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "a8" smd rect
			(at 19.05 0 90)
			(size 8 1.778)
			(layers "B.Cu")
			(net 200 "VD4")
			(pinfunction "Pin_a8")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "a9" smd rect
			(at 16.51 0 90)
			(size 8 1.778)
			(layers "B.Cu")
			(net 201 "VD5")
			(pinfunction "Pin_a9")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "a10" smd rect
			(at 13.97 0 90)
			(size 8 1.778)
			(layers "B.Cu")
			(net 202 "VD6")
			(pinfunction "Pin_a10")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "a11" smd rect
			(at 11.43 0 90)
			(size 8 1.778)
			(layers "B.Cu")
			(net 203 "VD7")
			(pinfunction "Pin_a11")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "a12" smd rect
			(at 8.89 0 90)
			(size 8 1.778)
			(layers "B.Cu")
			(net 2 "GND")
			(pinfunction "Pin_a12")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "a13" smd rect
			(at 6.35 0 90)
			(size 8 1.778)
			(layers "B.Cu")
			(net 204 "VD8")
			(pinfunction "Pin_a13")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "a14" smd rect
			(at 3.81 0 90)
			(size 8 1.778)
			(layers "B.Cu")
			(net 205 "VD9")
			(pinfunction "Pin_a14")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "a15" smd rect
			(at 1.27 0 90)
			(size 8 1.778)
			(layers "B.Cu")
			(net 206 "VD10")
			(pinfunction "Pin_a15")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "a16" smd rect
			(at -1.27 0 90)
			(size 8 1.778)
			(layers "B.Cu")
			(net 207 "VD11")
			(pinfunction "Pin_a16")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "a17" smd rect
			(at -3.81 0 90)
			(size 8 1.778)
			(layers "B.Cu")
			(net 208 "VD12")
			(pinfunction "Pin_a17")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "a18" smd rect
			(at -6.35 0 90)
			(size 8 1.778)
			(layers "B.Cu")
			(net 209 "VD13")
			(pinfunction "Pin_a18")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "a19" smd rect
			(at -8.89 0 90)
			(size 8 1.778)
			(layers "B.Cu")
			(net 210 "VD14")
			(pinfunction "Pin_a19")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "a20" smd rect
			(at -11.43 0 90)
			(size 8 1.778)
			(layers "B.Cu")
			(net 211 "VD15")
			(pinfunction "Pin_a20")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "a21" smd rect
			(at -13.97 0 90)
			(size 8 1.778)
			(layers "B.Cu")
			(net 105 "~{ROM}")
			(pinfunction "Pin_a21")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "a22" smd rect
			(at -16.51 0 90)
			(size 8 1.778)
			(layers "B.Cu")
			(net 109 "~{ASEL}")
			(pinfunction "Pin_a22")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "a23" smd rect
			(at -19.05 0 90)
			(size 8 1.778)
			(layers "B.Cu")
			(net 239 "~{RAS2X}")
			(pinfunction "Pin_a23")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "a24" smd rect
			(at -21.59 0 90)
			(size 8 1.778)
			(layers "B.Cu")
			(net 111 "~{FDC}")
			(pinfunction "Pin_a24")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "a25" smd rect
			(at -24.13 0 90)
			(size 8 1.778)
			(layers "B.Cu")
			(net 112 "FRES")
			(pinfunction "Pin_a25")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "a26" smd rect
			(at -26.67 0 90)
			(size 8 1.778)
			(layers "B.Cu")
			(net 38 "VCC")
			(pinfunction "Pin_a26")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "a27" smd rect
			(at -29.21 0 90)
			(size 8 1.778)
			(layers "B.Cu")
			(net 302 "unconnected-(CN2-Pin_a27-Pada27)")
			(pinfunction "Pin_a27")
			(pintype "passive+no_connect")
			(thermal_bridge_angle 45)
		)
		(pad "a28" smd rect
			(at -31.75 0 90)
			(size 8 1.778)
			(layers "B.Cu")
			(net 303 "unconnected-(CN2-Pin_a28-Pada28)")
			(pinfunction "Pin_a28")
			(pintype "passive+no_connect")
			(thermal_bridge_angle 45)
		)
		(pad "a29" smd rect
			(at -34.29 0 90)
			(size 8 1.778)
			(layers "B.Cu")
			(net 44 "SR2")
			(pinfunction "Pin_a29")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "a30" smd rect
			(at -36.83 0 90)
			(size 8 1.778)
			(layers "B.Cu")
			(net 2 "GND")
			(pinfunction "Pin_a30")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "b1" smd rect
			(at 36.83 0 90)
			(size 8 1.778)
			(layers "F.Cu")
			(net 2 "GND")
			(pinfunction "Pin_b1")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "b2" smd rect
			(at 34.29 0 90)
			(size 8 1.778)
			(layers "F.Cu")
			(net 2 "GND")
			(pinfunction "Pin_b2")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "b3" smd rect
			(at 31.75 0 90)
			(size 8 1.778)
			(layers "F.Cu")
			(net 179 "VA1")
			(pinfunction "Pin_b3")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "b4" smd rect
			(at 29.21 0 90)
			(size 8 1.778)
			(layers "F.Cu")
			(net 180 "VA2")
			(pinfunction "Pin_b4")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "b5" smd rect
			(at 26.67 0 90)
			(size 8 1.778)
			(layers "F.Cu")
			(net 181 "VA3")
			(pinfunction "Pin_b5")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "b6" smd rect
			(at 24.13 0 90)
			(size 8 1.778)
			(layers "F.Cu")
			(net 182 "VA4")
			(pinfunction "Pin_b6")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "b7" smd rect
			(at 21.59 0 90)
			(size 8 1.778)
			(layers "F.Cu")
			(net 183 "VA5")
			(pinfunction "Pin_b7")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "b8" smd rect
			(at 19.05 0 90)
			(size 8 1.778)
			(layers "F.Cu")
			(net 184 "VA6")
			(pinfunction "Pin_b8")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "b9" smd rect
			(at 16.51 0 90)
			(size 8 1.778)
			(layers "F.Cu")
			(net 185 "VA7")
			(pinfunction "Pin_b9")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "b10" smd rect
			(at 13.97 0 90)
			(size 8 1.778)
			(layers "F.Cu")
			(net 186 "VA8")
			(pinfunction "Pin_b10")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "b11" smd rect
			(at 11.43 0 90)
			(size 8 1.778)
			(layers "F.Cu")
			(net 187 "VA9")
			(pinfunction "Pin_b11")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "b12" smd rect
			(at 8.89 0 90)
			(size 8 1.778)
			(layers "F.Cu")
			(net 2 "GND")
			(pinfunction "Pin_b12")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "b13" smd rect
			(at 6.35 0 90)
			(size 8 1.778)
			(layers "F.Cu")
			(net 188 "VA10")
			(pinfunction "Pin_b13")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "b14" smd rect
			(at 3.81 0 90)
			(size 8 1.778)
			(layers "F.Cu")
			(net 189 "VA11")
			(pinfunction "Pin_b14")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "b15" smd rect
			(at 1.27 0 90)
			(size 8 1.778)
			(layers "F.Cu")
			(net 190 "VA12")
			(pinfunction "Pin_b15")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "b16" smd rect
			(at -1.27 0 90)
			(size 8 1.778)
			(layers "F.Cu")
			(net 191 "VA13")
			(pinfunction "Pin_b16")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "b17" smd rect
			(at -3.81 0 90)
			(size 8 1.778)
			(layers "F.Cu")
			(net 192 "VA14")
			(pinfunction "Pin_b17")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "b18" smd rect
			(at -6.35 0 90)
			(size 8 1.778)
			(layers "F.Cu")
			(net 193 "VA15")
			(pinfunction "Pin_b18")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "b19" smd rect
			(at -8.89 0 90)
			(size 8 1.778)
			(layers "F.Cu")
			(net 194 "VA16")
			(pinfunction "Pin_b19")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "b20" smd rect
			(at -11.43 0 90)
			(size 8 1.778)
			(layers "F.Cu")
			(net 195 "VA17")
			(pinfunction "Pin_b20")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "b21" smd rect
			(at -13.97 0 90)
			(size 8 1.778)
			(layers "F.Cu")
			(net 107 "~{LWR}")
			(pinfunction "Pin_b21")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "b22" smd rect
			(at -16.51 0 90)
			(size 8 1.778)
			(layers "F.Cu")
			(net 108 "~{UWR}")
			(pinfunction "Pin_b22")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "b23" smd rect
			(at -19.05 0 90)
			(size 8 1.778)
			(layers "F.Cu")
			(net 110 "~{CAS2}")
			(pinfunction "Pin_b23")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "b24" smd rect
			(at -21.59 0 90)
			(size 8 1.778)
			(layers "F.Cu")
			(net 304 "unconnected-(CN2-Pin_b24-Padb24)")
			(pinfunction "Pin_b24")
			(pintype "passive+no_connect")
			(thermal_bridge_angle 45)
		)
		(pad "b25" smd rect
			(at -24.13 0 90)
			(size 8 1.778)
			(layers "F.Cu")
			(net 305 "unconnected-(CN2-Pin_b25-Padb25)")
			(pinfunction "Pin_b25")
			(pintype "passive+no_connect")
			(thermal_bridge_angle 45)
		)
		(pad "b26" smd rect
			(at -26.67 0 90)
			(size 8 1.778)
			(layers "F.Cu")
			(net 38 "VCC")
			(pinfunction "Pin_b26")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "b27" smd rect
			(at -29.21 0 90)
			(size 8 1.778)
			(layers "F.Cu")
			(net 306 "unconnected-(CN2-Pin_b27-Padb27)")
			(pinfunction "Pin_b27")
			(pintype "passive+no_connect")
			(thermal_bridge_angle 45)
		)
		(pad "b28" smd rect
			(at -31.75 0 90)
			(size 8 1.778)
			(layers "F.Cu")
			(net 307 "unconnected-(CN2-Pin_b28-Padb28)")
			(pinfunction "Pin_b28")
			(pintype "passive+no_connect")
			(thermal_bridge_angle 45)
		)
		(pad "b29" smd rect
			(at -34.29 0 90)
			(size 8 1.778)
			(layers "F.Cu")
			(net 43 "SL2")
			(pinfunction "Pin_b29")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(pad "b30" smd rect
			(at -36.83 0 90)
			(size 8 1.778)
			(layers "F.Cu")
			(net 2 "GND")
			(pinfunction "Pin_b30")
			(pintype "passive")
			(thermal_bridge_angle 45)
		)
		(embedded_fonts no)
	)
	(footprint "MegaCD_Footprints:SOIC-16W_5.3x10.2mm_P1.27mm"
		(layer "F.Cu")
		(at 188.8744 59.6586 90)
		(descr "16-Lead Plastic Small Outline (SO) - Wide, 5.3 mm Body (http://www.ti.com/lit/ml/msop002a/msop002a.pdf)")
		(tags "SOIC 1.27")
		(property "Reference" "IC9"
			(at 6.7504 0.0254 180)
			(layer "F.SilkS")
		)
		(property "Value" "MB3790"
			(at 0 6.2 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "MegaCD.kicad_sch")
		(attr smd)
		(fp_text user "${VALUE}"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -3.55 -4.445 90)
			(size 1.5 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 323 "unconnected-(IC9-N.C.-Pad1)")
			(pinfunction "N.C.")
			(pintype "no_connect")
		)
		(pad "2" smd rect
			(at -3.55 -3.175 90)
			(size 1.5 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 339 "unconnected-(IC9-VBAT1-Pad2)")
			(pinfunction "VBAT1")
			(pintype "power_in+no_connect")
		)
		(pad "3" smd rect
			(at -3.55 -1.905 90)
			(size 1.5 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 5 "Net-(IC10-VCC)")
			(pinfunction "VOUT")
			(pintype "power_out")
		)
		(pad "4" smd rect
			(at -3.55 -0.635 90)
			(size 1.5 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 5 "Net-(IC10-VCC)")
			(pinfunction "VOUT")
			(pintype "power_out")
		)
		(pad "5" smd rect
			(at -3.55 0.635 90)
			(size 1.5 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "Net-(BT1-+)")
			(pinfunction "VBAT2")
			(pintype "power_in")
		)
		(pad "6" smd rect
			(at -3.55 1.905 90)
			(size 1.5 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 256 "unconnected-(IC9-~{ALARM1}-Pad6)")
			(pinfunction "~{ALARM1}")
			(pintype "output+no_connect")
		)
		(pad "7" smd rect
			(at -3.55 3.175 90)
			(size 1.5 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 257 "unconnected-(IC9-~{ALARM2}-Pad7)")
			(pinfunction "~{ALARM2}")
			(pintype "output+no_connect")
		)
		(pad "8" smd rect
			(at -3.55 4.445 90)
			(size 1.5 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "9" smd rect
			(at 3.55 4.445 90)
			(size 1.5 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 258 "unconnected-(IC9-RESET-Pad9)")
			(pinfunction "RESET")
			(pintype "input+no_connect")
		)
		(pad "10" smd rect
			(at 3.55 3.175 90)
			(size 1.5 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 259 "Net-(IC10-CS2)")
			(pinfunction "~{RESET}")
			(pintype "input")
		)
		(pad "11" smd rect
			(at 3.55 1.905 90)
			(size 1.5 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 3 "Net-(IC9-CT)")
			(pinfunction "CT")
			(pintype "passive")
		)
		(pad "12" smd rect
			(at 3.55 0.635 90)
			(size 1.5 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 260 "unconnected-(IC9-VSENSE-Pad12)")
			(pinfunction "VSENSE")
			(pintype "input+no_connect")
		)
		(pad "13" smd rect
			(at 3.55 -0.635 90)
			(size 1.5 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 4 "VCC2")
			(pinfunction "VIN")
			(pintype "power_in")
		)
		(pad "14" smd rect
			(at 3.55 -1.905 90)
			(size 1.5 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 4 "VCC2")
			(pinfunction "VIN")
			(pintype "power_in")
		)
		(pad "15" smd rect
			(at 3.55 -3.175 90)
			(size 1.5 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 324 "unconnected-(IC9-N.C.-Pad15)")
			(pinfunction "N.C.")
			(pintype "no_connect")
		)
		(pad "16" smd rect
			(at 3.55 -4.445 90)
			(size 1.5 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "GND")
			(pinfunction "CONTROL")
			(pintype "input")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Package_SO.3dshapes/SOIC-16W_5.3x10.2mm_P1.27mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MegaCD_Footprints:SOT-23-Wide"
		(layer "F.Cu")
		(at 224.155 119.761 90)
		(descr "SOT, 3 Pin (https://www.jedec.org/system/files/docs/to-236h.pdf variant AB), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOT TO_SOT_SMD")
		(property "Reference" "TR1"
			(at -3.6068 2.1844 180)
			(layer "F.SilkS")
		)
		(property "Value" "C1623"
			(at 0 2.4 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Bipolar transistor symbol for simulation only, substrate tied to the emitter"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Device" "NPN"
			(at 343.916 -104.394 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" "1=B 2=E 3=C"
			(at 343.916 -104.394 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Type" "GUMMELPOON"
			(at 343.916 -104.394 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "MegaCD.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.016 -0.95 90)
			(size 1.5 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 301 "Net-(TR1-B)")
			(pinfunction "B")
			(pintype "input")
		)
		(pad "2" smd roundrect
			(at -1.016 0.95 90)
			(size 1.5 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "E")
			(pintype "open_emitter")
		)
		(pad "3" smd roundrect
			(at 1.016 0 90)
			(size 1.5 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 297 "Net-(LD2-K)")
			(pinfunction "C")
			(pintype "open_collector")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MegaCD_Footprints:CP_Elec_3x5.4"
		(layer "F.Cu")
		(at 158.8262 102.489 90)
		(descr "SMD capacitor, aluminum electrolytic, Nichicon, 3.0x5.4mm")
		(tags "capacitor electrolytic")
		(property "Reference" "C53"
			(at -4.6736 0.1016 180)
			(layer "F.SilkS")
		)
		(property "Value" "10uF"
			(at 0 2.7 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Polarized capacitor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "MegaCD.kicad_sch")
		(attr smd)
		(fp_text user "+"
			(at -1.9812 3.81 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "-"
			(at 0.508 3.81 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.597 0 90)
			(size 2.394 1.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.15625)
			(net 4 "VCC2")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.597 0 90)
			(size 2.394 1.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.15625)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/CP_Elec_3x5.4.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MegaCD_Footprints:CP_Elec_3x5.4"
		(layer "F.Cu")
		(at 204.3938 105.1306 90)
		(descr "SMD capacitor, aluminum electrolytic, Nichicon, 3.0x5.4mm")
		(tags "capacitor electrolytic")
		(property "Reference" "C23"
			(at -8.128 1.27 270)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "10uF"
			(at 0 2.7 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Polarized capacitor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "MegaCD.kicad_sch")
		(attr smd)
		(fp_text user "-"
			(at 2.45 -1.05 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "+"
			(at -5.08 2.413 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.597 0 90)
			(size 2.394 1.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.15625)
			(net 4 "VCC2")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.597 0 90)
			(size 2.394 1.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.15625)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/CP_Elec_3x5.4.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MegaCD_Footprints:CP_Elec_3x5.4"
		(layer "F.Cu")
		(at 118.11 84.177 90)
		(descr "SMD capacitor, aluminum electrolytic, Nichicon, 3.0x5.4mm")
		(tags "capacitor electrolytic")
		(property "Reference" "C9"
			(at -3.9356 -0.4826 270)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "10uF"
			(at 0 2.7 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Polarized capacitor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "MegaCD.kicad_sch")
		(attr smd)
		(fp_text user "+"
			(at -3.6816 -1.1938 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "-"
			(at 0.5856 -1.1938 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.597 0 90)
			(size 2.394 1.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.15625)
			(net 4 "VCC2")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.597 0 90)
			(size 2.394 1.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.15625)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/CP_Elec_3x5.4.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MegaCD_Footprints:ZIP-20"
		(layer "F.Cu")
		(at 119.38 110.3122 90)
		(descr "20-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
		(tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
		(property "Reference" "IC8"
			(at 5.6896 17.0434 180)
			(layer "F.SilkS")
		)
		(property "Value" "MB81C4256Z"
			(at 1.27 26.67 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "MegaCD.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 1.016 -2.54 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 90)
			(size 1.3 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 165 "~{COE}")
			(pinfunction "~{OE}")
			(pintype "input")
		)
		(pad "2" thru_hole roundrect
			(at 2.54 1.27 90)
			(size 1.3 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 177 "~{PCAS}")
			(pinfunction "~{CAS}")
			(pintype "input")
		)
		(pad "3" thru_hole roundrect
			(at 0 2.54 90)
			(size 1.3 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 93 "D14")
			(pinfunction "D2")
			(pintype "tri_state")
		)
		(pad "4" thru_hole roundrect
			(at 2.54 3.81 90)
			(size 1.3 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 92 "D15")
			(pinfunction "D3")
			(pintype "tri_state")
		)
		(pad "5" thru_hole roundrect
			(at 0 5.08 90)
			(size 1.3 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "VSS")
			(pintype "power_in")
		)
		(pad "6" thru_hole roundrect
			(at 2.54 6.35 90)
			(size 1.3 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 95 "D12")
			(pinfunction "D0")
			(pintype "tri_state")
		)
		(pad "7" thru_hole roundrect
			(at 0 7.62 90)
			(size 1.3 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 94 "D13")
			(pinfunction "D1")
			(pintype "tri_state")
		)
		(pad "8" thru_hole roundrect
			(at 2.54 8.89 90)
			(size 1.3 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 178 "~{CUWE}")
			(pinfunction "~{WE}")
			(pintype "input")
		)
		(pad "9" thru_hole roundrect
			(at 0 10.16 90)
			(size 1.3 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 176 "~{PRAS}")
			(pinfunction "~{RAS}")
			(pintype "input")
		)
		(pad "10" thru_hole roundrect
			(at 2.54 11.43 90)
			(size 1.3 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 255 "unconnected-(IC8-N.C.-Pad10)")
			(pinfunction "N.C.")
			(pintype "input+no_connect")
		)
		(pad "11" thru_hole roundrect
			(at 0 12.7 90)
			(size 1.3 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 175 "PA0")
			(pinfunction "A0")
			(pintype "input")
		)
		(pad "12" thru_hole roundrect
			(at 2.54 13.97 90)
			(size 1.3 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 174 "PA1")
			(pinfunction "A1")
			(pintype "input")
		)
		(pad "13" thru_hole roundrect
			(at 0 15.24 90)
			(size 1.3 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 173 "PA2")
			(pinfunction "A2")
			(pintype "input")
		)
		(pad "14" thru_hole roundrect
			(at 2.54 16.51 90)
			(size 1.3 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 172 "PA3")
			(pinfunction "A3")
			(pintype "input")
		)
		(pad "15" thru_hole roundrect
			(at 0 17.78 90)
			(size 1.3 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 4 "VCC2")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(pad "16" thru_hole roundrect
			(at 2.54 19.05 90)
			(size 1.3 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 171 "PA4")
			(pinfunction "A4")
			(pintype "input")
		)
		(pad "17" thru_hole roundrect
			(at 0 20.32 90)
			(size 1.3 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 170 "PA5")
			(pinfunction "A5")
			(pintype "input")
		)
		(pad "18" thru_hole roundrect
			(at 2.54 21.59 90)
			(size 1.3 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 169 "PA6")
			(pinfunction "A6")
			(pintype "input")
		)
		(pad "19" thru_hole roundrect
			(at 0 22.86 90)
			(size 1.3 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 168 "PA7")
			(pinfunction "A7")
			(pintype "input")
		)
		(pad "20" thru_hole roundrect
			(at 2.54 24.13 90)
			(size 1.3 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 167 "PA8")
			(pinfunction "A8")
			(pintype "input")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Package_DIP.3dshapes/DIP-20_W7.62mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MegaCD_Footprints:C_Radial_5mm"
		(layer "F.Cu")
		(at 187.4882 128.016)
		(property "Reference" "C26"
			(at 3.85 -3.8 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "100uF"
			(at 0 1 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Polarized capacitor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "MegaCD.kicad_sch")
		(attr through_hole)
		(fp_text user "-"
			(at -5.0908 -0.5334 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "+"
			(at 2.65165 -0.883883 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "${REFERENCE}"
			(at 0 2.5 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" thru_hole roundrect
			(at 2.5 0)
			(size 1.5 1.5)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 4 "VCC2")
			(pintype "passive")
		)
		(pad "2" thru_hole roundrect
			(at -2.5 0)
			(size 1.5 1.5)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "MegaCD_Footprints:ZIP-20"
		(layer "F.Cu")
		(at 148.209 130.8354 90)
		(descr "20-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
		(tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
		(property "Reference" "IC5"
			(at -0.4064 -3.2004 180)
			(layer "F.SilkS")
		)
		(property "Value" "MB81C4256Z"
			(at 1.27 26.67 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "MegaCD.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 1.016 -2.54 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 90)
			(size 1.3 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 165 "~{COE}")
			(pinfunction "~{OE}")
			(pintype "input")
		)
		(pad "2" thru_hole roundrect
			(at 2.54 1.27 90)
			(size 1.3 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 177 "~{PCAS}")
			(pinfunction "~{CAS}")
			(pintype "input")
		)
		(pad "3" thru_hole roundrect
			(at 0 2.54 90)
			(size 1.3 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 51 "D2")
			(pinfunction "D2")
			(pintype "tri_state")
		)
		(pad "4" thru_hole roundrect
			(at 2.54 3.81 90)
			(size 1.3 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 50 "D3")
			(pinfunction "D3")
			(pintype "tri_state")
		)
		(pad "5" thru_hole roundrect
			(at 0 5.08 90)
			(size 1.3 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "VSS")
			(pintype "power_in")
		)
		(pad "6" thru_hole roundrect
			(at 2.54 6.35 90)
			(size 1.3 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 53 "D0")
			(pinfunction "D0")
			(pintype "tri_state")
		)
		(pad "7" thru_hole roundrect
			(at 0 7.62 90)
			(size 1.3 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 52 "D1")
			(pinfunction "D1")
			(pintype "tri_state")
		)
		(pad "8" thru_hole roundrect
			(at 2.54 8.89 90)
			(size 1.3 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 334 "~{CLWE}")
			(pinfunction "~{WE}")
			(pintype "input")
		)
		(pad "9" thru_hole roundrect
			(at 0 10.16 90)
			(size 1.3 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 176 "~{PRAS}")
			(pinfunction "~{RAS}")
			(pintype "input")
		)
		(pad "10" thru_hole roundrect
			(at 2.54 11.43 90)
			(size 1.3 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 252 "unconnected-(IC5-N.C.-Pad10)")
			(pinfunction "N.C.")
			(pintype "input+no_connect")
		)
		(pad "11" thru_hole roundrect
			(at 0 12.7 90)
			(size 1.3 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 175 "PA0")
			(pinfunction "A0")
			(pintype "input")
		)
		(pad "12" thru_hole roundrect
			(at 2.54 13.97 90)
			(size 1.3 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 174 "PA1")
			(pinfunction "A1")
			(pintype "input")
		)
		(pad "13" thru_hole roundrect
			(at 0 15.24 90)
			(size 1.3 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 173 "PA2")
			(pinfunction "A2")
			(pintype "input")
		)
		(pad "14" thru_hole roundrect
			(at 2.54 16.51 90)
			(size 1.3 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 172 "PA3")
			(pinfunction "A3")
			(pintype "input")
		)
		(pad "15" thru_hole roundrect
			(at 0 17.78 90)
			(size 1.3 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 4 "VCC2")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(pad "16" thru_hole roundrect
			(at 2.54 19.05 90)
			(size 1.3 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 171 "PA4")
			(pinfunction "A4")
			(pintype "input")
		)
		(pad "17" thru_hole roundrect
			(at 0 20.32 90)
			(size 1.3 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 170 "PA5")
			(pinfunction "A5")
			(pintype "input")
		)
		(pad "18" thru_hole roundrect
			(at 2.54 21.59 90)
			(size 1.3 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 169 "PA6")
			(pinfunction "A6")
			(pintype "input")
		)
		(pad "19" thru_hole roundrect
			(at 0 22.86 90)
			(size 1.3 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 168 "PA7")
			(pinfunction "A7")
			(pintype "input")
		)
		(pad "20" thru_hole roundrect
			(at 2.54 24.13 90)
			(size 1.3 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 167 "PA8")
			(pinfunction "A8")
			(pintype "input")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Package_DIP.3dshapes/DIP-20_W7.62mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MegaCD_Footprints:CP_Elec_3x5.4"
		(layer "F.Cu")
		(at 95.274 125.73 180)
		(descr "SMD capacitor, aluminum electrolytic, Nichicon, 3.0x5.4mm")
		(tags "capacitor electrolytic")
		(property "Reference" "C46"
			(at 5.1802 0.9398 180)
			(layer "F.SilkS")
		)
		(property "Value" "10uF"
			(at 0 2.7 180)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Polarized capacitor"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "MegaCD.kicad_sch")
		(attr smd)
		(fp_text user "-"
			(at 1.675 -0.889 180)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "+"
			(at -4.421 -0.889 180)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.597 0 180)
			(size 2.394 1.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.15625)
			(net 4 "VCC2")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.597 0 180)
			(size 2.394 1.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.15625)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/CP_Elec_3x5.4.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MegaCD_Footprints:CP_Elec_3x5.4"
		(layer "F.Cu")
		(at 210.082 126.238 180)
		(descr "SMD capacitor, aluminum electrolytic, Nichicon, 3.0x5.4mm")
		(tags "capacitor electrolytic")
		(property "Reference" "C28"
			(at 0.405 -3.556 180)
			(layer "F.SilkS")
		)
		(property "Value" "10uF"
			(at 0 2.7 180)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Polarized capacitor"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "MegaCD.kicad_sch")
		(attr smd)
		(fp_text user "+"
			(at -3.024 -1.397 180)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "-"
			(at 1.294 -1.397 180)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.597 0 180)
			(size 2.394 1.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.15625)
			(net 4 "VCC2")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.597 0 180)
			(size 2.394 1.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.15625)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/CP_Elec_3x5.4.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MegaCD_Footprints:PQFP-80_14x20mm_P0.8mm_long_pads"
		(layer "F.Cu")
		(at 100.323 85.471 90)
		(descr "PQFP80 14x20 / QIP80E CASE 122BS (see ON Semiconductor 122BS.PDF)")
		(tags "QFP 0.8")
		(property "Reference" "IC3"
			(at 12.954 -12.058 180)
			(layer "F.SilkS")
		)
		(property "Value" "315-5476A"
			(at 0 5.08 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "MegaCD.kicad_sch")
		(attr smd)
		(fp_text user "65"
			(at 6.7056 -16.8332 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "25"
			(at -7.62 15 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "80"
			(at -6.6548 -17.392 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "${VALUE}"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "24"
			(at -12.5476 8.1604 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "1"
			(at -12.3444 -11.2452 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "" smd circle
			(at -9.144 -12.446)
			(size 0.75 0.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
		)
		(pad "" smd circle
			(at -9.142 12.446)
			(size 0.75 0.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
		)
		(pad "" smd circle
			(at 9.144 -12.446)
			(size 0.75 0.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
		)
		(pad "" smd circle
			(at 9.146 12.446)
			(size 0.75 0.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
		)
		(pad "1" smd rect
			(at -9.017 -9.2 90)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 78 "A10")
			(pinfunction "A10")
			(pintype "input")
		)
		(pad "2" smd rect
			(at -9.017 -8.4 90)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 77 "A9")
			(pinfunction "A9")
			(pintype "input")
		)
		(pad "3" smd rect
			(at -9.017 -7.6 90)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 76 "A8")
			(pinfunction "A8")
			(pintype "input")
		)
		(pad "4" smd rect
			(at -9.017 -6.8 90)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 75 "A7")
			(pinfunction "A7")
			(pintype "input")
		)
		(pad "5" smd rect
			(at -9.017 -6 90)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 74 "A6")
			(pinfunction "A6")
			(pintype "input")
		)
		(pad "6" smd rect
			(at -9.017 -5.2 90)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 73 "A5")
			(pinfunction "A5")
			(pintype "input")
		)
		(pad "7" smd rect
			(at -9.017 -4.4 90)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 72 "A4")
			(pinfunction "A4")
			(pintype "input")
		)
		(pad "8" smd rect
			(at -9.017 -3.6 90)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 71 "A3")
			(pinfunction "A3")
			(pintype "input")
		)
		(pad "9" smd rect
			(at -9.017 -2.8 90)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 70 "A2")
			(pinfunction "A1")
			(pintype "input")
		)
		(pad "10" smd rect
			(at -9.017 -2 90)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 69 "A1")
			(pinfunction "A0")
			(pintype "input")
		)
		(pad "11" smd rect
			(at -9.017 -1.2 90)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 212 "unconnected-(IC3-N.C.-Pad11)")
			(pinfunction "N.C.")
			(pintype "no_connect")
		)
		(pad "12" smd rect
			(at -9.017 -0.4 90)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 4 "VCC2")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(pad "13" smd rect
			(at -9.017 0.4 90)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 165 "~{COE}")
			(pinfunction "~{RD}")
			(pintype "input")
		)
		(pad "14" smd rect
			(at -9.017 1.2 90)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 240 "~{CLWEX}")
			(pinfunction "~{WR}")
			(pintype "input")
		)
		(pad "15" smd rect
			(at -9.017 2 90)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "16" smd rect
			(at -9.017 2.8 90)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "GND")
			(pinfunction "TEST1")
			(pintype "power_in")
		)
		(pad "17" smd rect
			(at -9.017 3.58 90)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "GND")
			(pinfunction "TEST2")
			(pintype "power_in")
		)
		(pad "18" smd rect
			(at -9.017 4.4 90)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "GND")
			(pinfunction "TEST3")
			(pintype "power_in")
		)
		(pad "19" smd rect
			(at -9.017 5.2 90)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 4 "VCC2")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(pad "20" smd rect
			(at -9.017 6 90)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 213 "unconnected-(IC3-N.C.-Pad20)")
			(pinfunction "N.C.")
			(pintype "no_connect")
		)
		(pad "21" smd rect
			(at -9.017 6.8 90)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 100 "D7")
			(pinfunction "D7")
			(pintype "bidirectional")
		)
		(pad "22" smd rect
			(at -9.017 7.6 90)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 101 "D6")
			(pinfunction "D6")
			(pintype "bidirectional")
		)
		(pad "23" smd rect
			(at -9.017 8.4 90)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 102 "D5")
			(pinfunction "D5")
			(pintype "bidirectional")
		)
		(pad "24" smd rect
			(at -9.017 9.2 90)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 49 "D4")
			(pinfunction "D4")
			(pintype "bidirectional")
		)
		(pad "25" smd rect
			(at -6 12.065 180)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 50 "D3")
			(pinfunction "D3")
			(pintype "bidirectional")
		)
		(pad "26" smd rect
			(at -5.2 12.065 180)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 51 "D2")
			(pinfunction "D2")
			(pintype "bidirectional")
		)
		(pad "27" smd rect
			(at -4.4 12.065 180)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 52 "D1")
			(pinfunction "D1")
			(pintype "bidirectional")
		)
		(pad "28" smd rect
			(at -3.6 12.065 180)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 53 "D0")
			(pinfunction "D0")
			(pintype "bidirectional")
		)
		(pad "29" smd rect
			(at -2.8 12.065 180)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 214 "unconnected-(IC3-SHL-Pad29)")
			(pinfunction "SHL")
			(pintype "passive+no_connect")
		)
		(pad "30" smd rect
			(at -2 12.065 180)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 215 "unconnected-(IC3-SHR-Pad30)")
			(pinfunction "SHR")
			(pintype "passive+no_connect")
		)
		(pad "31" smd rect
			(at -1.2 12.065 180)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 216 "unconnected-(IC3-DAC7-Pad31)")
			(pinfunction "DAC7")
			(pintype "bidirectional+no_connect")
		)
		(pad "32" smd rect
			(at -0.4 12.065 180)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 217 "unconnected-(IC3-DAC6-Pad32)")
			(pinfunction "DAC6")
			(pintype "bidirectional+no_connect")
		)
		(pad "33" smd rect
			(at 0.4 12.065 180)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 218 "unconnected-(IC3-DAC5-Pad33)")
			(pinfunction "DAC5")
			(pintype "bidirectional+no_connect")
		)
		(pad "34" smd rect
			(at 1.2 12.065 180)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 219 "unconnected-(IC3-DAC4-Pad34)")
			(pinfunction "DAC4")
			(pintype "bidirectional+no_connect")
		)
		(pad "35" smd rect
			(at 2 12.065 180)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 41 "PBCLK")
			(pinfunction "BCLK")
			(pintype "input")
		)
		(pad "36" smd rect
			(at 2.8 12.065 180)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 39 "PDATA")
			(pinfunction "DATA")
			(pintype "input")
		)
		(pad "37" smd rect
			(at 3.6 12.065 180)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 220 "unconnected-(IC3-DAC3-Pad37)")
			(pinfunction "DAC3")
			(pintype "bidirectional+no_connect")
		)
		(pad "38" smd rect
			(at 4.4 12.065 180)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 221 "unconnected-(IC3-DAC7L-Pad38)")
			(pinfunction "DAC7L")
			(pintype "passive+no_connect")
		)
		(pad "39" smd rect
			(at 5.2 12.065 180)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 222 "unconnected-(IC3-DAC7R-Pad39)")
			(pinfunction "DAC7R")
			(pintype "passive+no_connect")
		)
		(pad "40" smd rect
			(at 6 12.065 180)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 42 "PLRCK")
			(pinfunction "LRCK")
			(pintype "input")
		)
		(pad "41" smd rect
			(at 9.017 9.2 90)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 40 "PWCLK")
			(pinfunction "WCLK1")
			(pintype "input")
		)
		(pad "42" smd rect
			(at 9.017 8.4 90)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 223 "unconnected-(IC3-RAMAX-Pad42)")
			(pinfunction "RAMAX")
			(pintype "output+no_connect")
		)
		(pad "43" smd rect
			(at 9.017 7.6 90)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 4 "VCC2")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(pad "44" smd rect
			(at 9.017 6.8 90)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 224 "/WD7")
			(pinfunction "RAMAD7")
			(pintype "bidirectional")
		)
		(pad "45" smd rect
			(at 9.017 6 90)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 225 "/WD6")
			(pinfunction "RAMAD6")
			(pintype "bidirectional")
		)
		(pad "46" smd rect
			(at 9.017 5.2 90)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 226 "/WD5")
			(pinfunction "RAMAD5")
			(pintype "bidirectional")
		)
		(pad "47" smd rect
			(at 9.017 4.4 90)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 227 "/WD4")
			(pinfunction "RAMAD4")
			(pintype "bidirectional")
		)
		(pad "48" smd rect
			(at 9.017 3.6 90)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 228 "/WD3")
			(pinfunction "RAMAD3")
			(pintype "bidirectional")
		)
		(pad "49" smd rect
			(at 9.017 2.8 90)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 229 "/WD2")
			(pinfunction "RAMAD2")
			(pintype "bidirectional")
		)
		(pad "50" smd rect
			(at 9.017 2 90)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 230 "/WD1")
			(pinfunction "RAMAD1")
			(pintype "bidirectional")
		)
		(pad "51" smd rect
			(at 9.017 1.2 90)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 231 "/WD0")
			(pinfunction "RAMAD0")
			(pintype "bidirectional")
		)
		(pad "52" smd rect
			(at 9.017 0.4 90)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "53" smd rect
			(at 9.017 -0.4 90)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 232 "/RA14")
			(pinfunction "RAMA14")
			(pintype "output")
		)
		(pad "54" smd rect
			(at 9.017 -1.2 90)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 233 "/RA13")
			(pinfunction "RAMA13")
			(pintype "output")
		)
		(pad "55" smd rect
			(at 9.017 -2 90)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 234 "/RA12")
			(pinfunction "RAMA12")
			(pintype "output")
		)
		(pad "56" smd rect
			(at 9.017 -2.8 90)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 235 "/RA11")
			(pinfunction "RAMA11")
			(pintype "output")
		)
		(pad "57" smd rect
			(at 9.017 -3.6 90)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 236 "/RA10")
			(pinfunction "RAMA10")
			(pintype "output")
		)
		(pad "58" smd rect
			(at 9.017 -4.4 90)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 237 "/RA9")
			(pinfunction "RAMA9")
			(pintype "output")
		)
		(pad "59" smd rect
			(at 9.017 -5.2 90)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 238 "/RA8")
			(pinfunction "RAMA8")
			(pintype "output")
		)
		(pad "60" smd rect
			(at 9.017 -6 90)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 241 "~{RCS1X}")
			(pinfunction "~{RCS1}")
			(pintype "input")
		)
		(pad "61" smd rect
			(at 9.017 -6.8 90)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 308 "~{RCS2X}")
			(pinfunction "~{RCS2}")
			(pintype "input")
		)
		(pad "62" smd rect
			(at 9.017 -7.6 90)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 309 "~{ROE}")
			(pinfunction "~{ROE}")
			(pintype "input")
		)
		(pad "63" smd rect
			(at 9.017 -8.4 90)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 242 "Net-(IC13-~{WE})")
			(pinfunction "~{RWE}")
			(pintype "input")
		)
		(pad "64" smd rect
			(at 9.017 -9.2 90)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 31 "~{ERES}")
			(pinfunction "~{RES}")
			(pintype "input")
		)
		(pad "65" smd rect
			(at 6 -12.065 180)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 243 "/RA7")
			(pinfunction "RAMA7")
			(pintype "output")
		)
		(pad "66" smd rect
			(at 5.2 -12.065 180)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 244 "/RA6")
			(pinfunction "RAMA6")
			(pintype "output")
		)
		(pad "67" smd rect
			(at 4.4 -12.065 180)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 245 "/RA5")
			(pinfunction "RAMA5")
			(pintype "output")
		)
		(pad "68" smd rect
			(at 3.6 -12.065 180)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 246 "/RA4")
			(pinfunction "RAMA4")
			(pintype "output")
		)
		(pad "69" smd rect
			(at 2.8 -12.065 180)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 4 "VCC2")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(pad "70" smd rect
			(at 2 -12.065 180)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 45 "12M")
			(pinfunction "XIN")
			(pintype "input")
		)
		(pad "71" smd rect
			(at 1.2 -12.065 180)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 247 "unconnected-(IC3-XOUT-Pad71)")
			(pinfunction "XOUT")
			(pintype "output+no_connect")
		)
		(pad "72" smd rect
			(at 0.4 -12.065 180)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "73" smd rect
			(at -0.4 -12.065 180)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 248 "/RA3")
			(pinfunction "RAMA3")
			(pintype "output")
		)
		(pad "74" smd rect
			(at -1.2 -12.065 180)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 249 "/RA2")
			(pinfunction "RAMA2")
			(pintype "output")
		)
		(pad "75" smd rect
			(at -2 -12.065 180)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 250 "/RA1")
			(pinfunction "RAMA1")
			(pintype "output")
		)
		(pad "76" smd rect
			(at -2.8 -12.065 180)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 251 "/RA0")
			(pinfunction "RAMA0")
			(pintype "output")
		)
		(pad "77" smd rect
			(at -3.6 -12.065 180)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 159 "~{PCM}")
			(pinfunction "~{CS}")
			(pintype "input")
		)
		(pad "78" smd rect
			(at -4.4 -12.065 180)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 81 "A13")
			(pinfunction "A13")
			(pintype "input")
		)
		(pad "79" smd rect
			(at -5.2 -12.065 180)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 80 "A12")
			(pinfunction "A12")
			(pintype "input")
		)
		(pad "80" smd rect
			(at -6 -12.065 180)
			(size 3.16 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 79 "A11")
			(pinfunction "A11")
			(pintype "input")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Package_QFP.3dshapes/PQFP-80_14x20mm_P0.8mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MegaCD_Footprints:PLCC-68-Longer_Pads"
		(layer "F.Cu")
		(at 137.16 89.281 90)
		(descr "PLCC, 68 pins, surface mount")
		(tags "plcc smt")
		(property "Reference" "IC1"
			(at -5.2832 -17.399 270)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "68HC000"
			(at 0 3.81 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Microprocessor, 16-bit bus"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "MegaCD.kicad_sch")
		(attr smd)
		(fp_text user "10"
			(at -14.986 -13.6906 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "43"
			(at 12.446 14.686 270)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "9"
			(at -10.5156 -15.6718 270)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "1"
			(at -0.8636 -16.5354 270)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "26"
			(at -15.5956 9.7282 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "${VALUE}"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "27"
			(at -9.8044 13.9446 270)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "" smd circle
			(at -13.462 13.462)
			(size 0.75 0.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
		)
		(pad "" smd circle
			(at 13.462 -13.462)
			(size 0.75 0.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
		)
		(pad "1" smd rect
			(at 0 -11.938 90)
			(size 0.7 2.425)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 49 "D4")
			(pinfunction "D4")
			(pintype "bidirectional")
		)
		(pad "2" smd rect
			(at -1.27 -11.938 90)
			(size 0.7 2.425)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 50 "D3")
			(pinfunction "D3")
			(pintype "bidirectional")
		)
		(pad "3" smd rect
			(at -2.54 -11.938 90)
			(size 0.7 2.425)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 51 "D2")
			(pinfunction "D2")
			(pintype "bidirectional")
		)
		(pad "4" smd rect
			(at -3.81 -11.938 90)
			(size 0.7 2.425)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 52 "D1")
			(pinfunction "D1")
			(pintype "bidirectional")
		)
		(pad "5" smd rect
			(at -5.08 -11.938 90)
			(size 0.7 2.425)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 53 "D0")
			(pinfunction "D0")
			(pintype "bidirectional")
		)
		(pad "6" smd rect
			(at -6.35 -11.938 90)
			(size 0.7 2.425)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 54 "~{AS}")
			(pinfunction "AS")
			(pintype "output")
		)
		(pad "7" smd rect
			(at -7.62 -11.938 90)
			(size 0.7 2.425)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 55 "~{UDS}")
			(pinfunction "UDS")
			(pintype "output")
		)
		(pad "8" smd rect
			(at -8.89 -11.938 90)
			(size 0.7 2.425)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 56 "~{LDS}")
			(pinfunction "LDS")
			(pintype "output")
		)
		(pad "9" smd rect
			(at -10.16 -11.938 90)
			(size 0.7 2.425)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 57 "R{slash}~{W}")
			(pinfunction "R/W")
			(pintype "output")
		)
		(pad "10" smd rect
			(at -11.938 -10.16 90)
			(size 2.425 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 58 "~{DTAK}")
			(pinfunction "DTACK")
			(pintype "input")
		)
		(pad "11" smd rect
			(at -11.938 -8.89 90)
			(size 2.425 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 59 "unconnected-(IC1-BG-Pad11)")
			(pinfunction "BG")
			(pintype "output+no_connect")
		)
		(pad "12" smd rect
			(at -11.938 -7.62 90)
			(size 2.425 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 4 "VCC2")
			(pinfunction "BGACK")
			(pintype "input")
		)
		(pad "13" smd rect
			(at -11.938 -6.35 90)
			(size 2.425 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 4 "VCC2")
			(pinfunction "BR")
			(pintype "input")
		)
		(pad "14" smd rect
			(at -11.938 -5.08 90)
			(size 2.425 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 4 "VCC2")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(pad "15" smd rect
			(at -11.938 -3.81 90)
			(size 2.425 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 45 "12M")
			(pinfunction "CLK")
			(pintype "input")
		)
		(pad "16" smd rect
			(at -11.938 -2.54 90)
			(size 2.425 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "17" smd rect
			(at -11.938 -1.27 90)
			(size 2.425 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "18" smd rect
			(at -11.938 0 90)
			(size 2.425 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 60 "unconnected-(IC1-NC-Pad18)")
			(pinfunction "NC")
			(pintype "no_connect")
		)
		(pad "19" smd rect
			(at -11.938 1.27 90)
			(size 2.425 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 61 "~{HALT}")
			(pinfunction "HALT")
			(pintype "bidirectional")
		)
		(pad "20" smd rect
			(at -11.938 2.54 90)
			(size 2.425 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 62 "~{RES}")
			(pinfunction "RESET")
			(pintype "input")
		)
		(pad "21" smd rect
			(at -11.938 3.81 90)
			(size 2.425 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 63 "unconnected-(IC1-VMA-Pad21)")
			(pinfunction "VMA")
			(pintype "output+no_connect")
		)
		(pad "22" smd rect
			(at -11.938 5.08 90)
			(size 2.425 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 315 "E")
			(pinfunction "E")
			(pintype "output")
		)
		(pad "23" smd rect
			(at -11.938 6.35 90)
			(size 2.425 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 64 "~{VPA}")
			(pinfunction "VPA")
			(pintype "input")
		)
		(pad "24" smd rect
			(at -11.938 7.62 90)
			(size 2.425 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 4 "VCC2")
			(pinfunction "BERR")
			(pintype "input")
		)
		(pad "25" smd rect
			(at -11.938 8.89 90)
			(size 2.425 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 316 "~{IPL2}")
			(pinfunction "IPL2")
			(pintype "input")
		)
		(pad "26" smd rect
			(at -11.938 10.16 90)
			(size 2.425 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 317 "~{IPL1}")
			(pinfunction "IPL1")
			(pintype "input")
		)
		(pad "27" smd rect
			(at -10.16 11.938 90)
			(size 0.7 2.425)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 318 "~{IPL0}")
			(pinfunction "IPL0")
			(pintype "input")
		)
		(pad "28" smd rect
			(at -8.89 11.938 90)
			(size 0.7 2.425)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 65 "unconnected-(IC1-FC2-Pad28)")
			(pinfunction "FC2")
			(pintype "output+no_connect")
		)
		(pad "29" smd rect
			(at -7.62 11.938 90)
			(size 0.7 2.425)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 66 "FC1")
			(pinfunction "FC1")
			(pintype "output")
		)
		(pad "30" smd rect
			(at -6.35 11.938 90)
			(size 0.7 2.425)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 67 "FC0")
			(pinfunction "FC0")
			(pintype "output")
		)
		(pad "31" smd rect
			(at -5.08 11.938 90)
			(size 0.7 2.425)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 68 "unconnected-(IC1-NC-Pad31)")
			(pinfunction "NC")
			(pintype "no_connect")
		)
		(pad "32" smd rect
			(at -3.81 11.938 90)
			(size 0.7 2.425)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 69 "A1")
			(pinfunction "A1")
			(pintype "output")
		)
		(pad "33" smd rect
			(at -2.54 11.938 90)
			(size 0.7 2.425)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 70 "A2")
			(pinfunction "A2")
			(pintype "output")
		)
		(pad "34" smd rect
			(at -1.27 11.938 90)
			(size 0.7 2.425)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 71 "A3")
			(pinfunction "A3")
			(pintype "output")
		)
		(pad "35" smd rect
			(at 0 11.938 90)
			(size 0.7 2.425)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 72 "A4")
			(pinfunction "A4")
			(pintype "output")
		)
		(pad "36" smd rect
			(at 1.27 11.938 90)
			(size 0.7 2.425)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 73 "A5")
			(pinfunction "A5")
			(pintype "output")
		)
		(pad "37" smd rect
			(at 2.54 11.938 90)
			(size 0.7 2.425)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 74 "A6")
			(pinfunction "A6")
			(pintype "output")
		)
		(pad "38" smd rect
			(at 3.81 11.938 90)
			(size 0.7 2.425)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 75 "A7")
			(pinfunction "A7")
			(pintype "output")
		)
		(pad "39" smd rect
			(at 5.08 11.938 90)
			(size 0.7 2.425)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 76 "A8")
			(pinfunction "A8")
			(pintype "output")
		)
		(pad "40" smd rect
			(at 6.35 11.938 90)
			(size 0.7 2.425)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 77 "A9")
			(pinfunction "A9")
			(pintype "output")
		)
		(pad "41" smd rect
			(at 7.62 11.938 90)
			(size 0.7 2.425)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 78 "A10")
			(pinfunction "A10")
			(pintype "output")
		)
		(pad "42" smd rect
			(at 8.89 11.938 90)
			(size 0.7 2.425)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 79 "A11")
			(pinfunction "A11")
			(pintype "output")
		)
		(pad "43" smd rect
			(at 10.16 11.938 90)
			(size 0.7 2.425)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 80 "A12")
			(pinfunction "A12")
			(pintype "output")
		)
		(pad "44" smd rect
			(at 11.938 10.16 90)
			(size 2.425 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 81 "A13")
			(pinfunction "A13")
			(pintype "output")
		)
		(pad "45" smd rect
			(at 11.938 8.89 90)
			(size 2.425 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 82 "A14")
			(pinfunction "A14")
			(pintype "output")
		)
		(pad "46" smd rect
			(at 11.938 7.62 90)
			(size 2.425 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 83 "A15")
			(pinfunction "A15")
			(pintype "output")
		)
		(pad "47" smd rect
			(at 11.938 6.35 90)
			(size 2.425 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 84 "A16")
			(pinfunction "A16")
			(pintype "output")
		)
		(pad "48" smd rect
			(at 11.938 5.08 90)
			(size 2.425 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 85 "A17")
			(pinfunction "A17")
			(pintype "output")
		)
		(pad "49" smd rect
			(at 11.938 3.81 90)
			(size 2.425 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 86 "A18")
			(pinfunction "A18")
			(pintype "output")
		)
		(pad "50" smd rect
			(at 11.938 2.54 90)
			(size 2.425 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 87 "A19")
			(pinfunction "A19")
			(pintype "output")
		)
		(pad "51" smd rect
			(at 11.938 1.27 90)
			(size 2.425 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 88 "unconnected-(IC1-A20-Pad51)")
			(pinfunction "A20")
			(pintype "output+no_connect")
		)
		(pad "52" smd rect
			(at 11.938 0 90)
			(size 2.425 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 4 "VCC2")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(pad "53" smd rect
			(at 11.938 -1.27 90)
			(size 2.425 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 89 "unconnected-(IC1-A21-Pad53)")
			(pinfunction "A21")
			(pintype "output+no_connect")
		)
		(pad "54" smd rect
			(at 11.938 -2.54 90)
			(size 2.425 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 90 "unconnected-(IC1-A22-Pad54)")
			(pinfunction "A22")
			(pintype "output+no_connect")
		)
		(pad "55" smd rect
			(at 11.938 -3.81 90)
			(size 2.425 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 91 "unconnected-(IC1-A23-Pad55)")
			(pinfunction "A23")
			(pintype "output+no_connect")
		)
		(pad "56" smd rect
			(at 11.938 -5.08 90)
			(size 2.425 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "57" smd rect
			(at 11.938 -6.35 90)
			(size 2.425 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "58" smd rect
			(at 11.938 -7.62 90)
			(size 2.425 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 92 "D15")
			(pinfunction "D15")
			(pintype "bidirectional")
		)
		(pad "59" smd rect
			(at 11.938 -8.89 90)
			(size 2.425 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 93 "D14")
			(pinfunction "D14")
			(pintype "bidirectional")
		)
		(pad "60" smd rect
			(at 11.938 -10.16 90)
			(size 2.425 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 94 "D13")
			(pinfunction "D13")
			(pintype "bidirectional")
		)
		(pad "61" smd rect
			(at 10.16 -11.938 90)
			(size 0.7 2.425)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 95 "D12")
			(pinfunction "D12")
			(pintype "bidirectional")
		)
		(pad "62" smd rect
			(at 8.89 -11.938 90)
			(size 0.7 2.425)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 96 "D11")
			(pinfunction "D11")
			(pintype "bidirectional")
		)
		(pad "63" smd rect
			(at 7.62 -11.938 90)
			(size 0.7 2.425)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 97 "D10")
			(pinfunction "D10")
			(pintype "bidirectional")
		)
		(pad "64" smd rect
			(at 6.35 -11.938 90)
			(size 0.7 2.425)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 98 "D9")
			(pinfunction "D9")
			(pintype "bidirectional")
		)
		(pad "65" smd rect
			(at 5.08 -11.938 90)
			(size 0.7 2.425)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 99 "D8")
			(pinfunction "D8")
			(pintype "bidirectional")
		)
		(pad "66" smd rect
			(at 3.81 -11.938 90)
			(size 0.7 2.425)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 100 "D7")
			(pinfunction "D7")
			(pintype "bidirectional")
		)
		(pad "67" smd rect
			(at 2.54 -11.938 90)
			(size 0.7 2.425)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 101 "D6")
			(pinfunction "D6")
			(pintype "bidirectional")
		)
		(pad "68" smd rect
			(at 1.27 -11.938 90)
			(size 0.7 2.425)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 102 "D5")
			(pinfunction "D5")
			(pintype "bidirectional")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Package_LCC.3dshapes/PLCC-68.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MegaCD_Footprints:CP_Elec_3x5.4"
		(layer "F.Cu")
		(at 217.7 126.238 180)
		(descr "SMD capacitor, aluminum electrolytic, Nichicon, 3.0x5.4mm")
		(tags "capacitor electrolytic")
		(property "Reference" "C31"
			(at 0.276 -3.556 180)
			(layer "F.SilkS")
		)
		(property "Value" "10uF"
			(at 0 2.7 180)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Polarized capacitor"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "MegaCD.kicad_sch")
		(attr smd)
		(fp_text user "-"
			(at 1.292 -1.41 180)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "+"
			(at -3.026 -1.397 180)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.597 0 180)
			(size 2.394 1.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.15625)
			(net 4 "VCC2")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.597 0 180)
			(size 2.394 1.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.15625)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/CP_Elec_3x5.4.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MegaCD_Footprints:FB_P5.00mm"
		(layer "F.Cu")
		(at 205.359 94.314 -90)
		(property "Reference" "FB2"
			(at -2.366 2.159 0)
			(layer "F.SilkS")
		)
		(property "Value" "FB"
			(at 2.5 2.2 270)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Ferrite bead, small symbol"
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "MegaCD.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 2.5 0 270)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 332 "Net-(OSC1-OUT)")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 5 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 47 "50M")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Disc_D4.3mm_W1.9mm_P5.00mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MegaCD_Footprints:DIP-40_W15.24mm_Socket"
		(layer "F.Cu")
		(at 104.14 72.644 90)
		(descr "40-lead though-hole mounted DIP package, row spacing 15.24 mm (600 mils), Socket")
		(tags "THT DIP DIL PDIP 2.54mm 15.24mm 600mil Socket")
		(property "Reference" "IC4"
			(at 6.096 53.213 180)
			(layer "F.SilkS")
		)
		(property "Value" "27C1024"
			(at 7.62 50.59 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "MegaCD.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 7.62 24.13 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "VCC2")
			(pinfunction "VPP")
			(pintype "power_in")
		)
		(pad "2" thru_hole roundrect
			(at 0 2.54 90)
			(size 1.5 1.5)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 104 "~{BROM}")
			(pinfunction "~{CE}")
			(pintype "input")
		)
		(pad "3" thru_hole roundrect
			(at 0 5.08 90)
			(size 1.5 1.5)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 211 "VD15")
			(pinfunction "D15")
			(pintype "tri_state")
		)
		(pad "4" thru_hole roundrect
			(at 0 7.62 90)
			(size 1.5 1.5)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 210 "VD14")
			(pinfunction "D14")
			(pintype "tri_state")
		)
		(pad "5" thru_hole roundrect
			(at 0 10.16 90)
			(size 1.5 1.5)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 209 "VD13")
			(pinfunction "D13")
			(pintype "tri_state")
		)
		(pad "6" thru_hole roundrect
			(at 0 12.7 90)
			(size 1.5 1.5)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 208 "VD12")
			(pinfunction "D12")
			(pintype "tri_state")
		)
		(pad "7" thru_hole roundrect
			(at 0 15.24 90)
			(size 1.5 1.5)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 207 "VD11")
			(pinfunction "D11")
			(pintype "tri_state")
		)
		(pad "8" thru_hole roundrect
			(at 0 17.78 90)
			(size 1.5 1.5)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 206 "VD10")
			(pinfunction "D10")
			(pintype "tri_state")
		)
		(pad "9" thru_hole roundrect
			(at 0 20.32 90)
			(size 1.5 1.5)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 205 "VD9")
			(pinfunction "D9")
			(pintype "tri_state")
		)
		(pad "10" thru_hole roundrect
			(at 0 22.86 90)
			(size 1.5 1.5)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 204 "VD8")
			(pinfunction "D8")
			(pintype "tri_state")
		)
		(pad "11" thru_hole roundrect
			(at 0 25.4 90)
			(size 1.5 1.5)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "12" thru_hole roundrect
			(at 0 27.94 90)
			(size 1.5 1.5)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 203 "VD7")
			(pinfunction "D7")
			(pintype "tri_state")
		)
		(pad "13" thru_hole roundrect
			(at 0 30.48 90)
			(size 1.5 1.5)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 202 "VD6")
			(pinfunction "D6")
			(pintype "tri_state")
		)
		(pad "14" thru_hole roundrect
			(at 0 33.02 90)
			(size 1.5 1.5)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 201 "VD5")
			(pinfunction "D5")
			(pintype "tri_state")
		)
		(pad "15" thru_hole roundrect
			(at 0 35.56 90)
			(size 1.5 1.5)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 200 "VD4")
			(pinfunction "D4")
			(pintype "tri_state")
		)
		(pad "16" thru_hole roundrect
			(at 0 38.1 90)
			(size 1.5 1.5)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 199 "VD3")
			(pinfunction "D3")
			(pintype "tri_state")
		)
		(pad "17" thru_hole roundrect
			(at 0 40.64 90)
			(size 1.5 1.5)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 198 "VD2")
			(pinfunction "D2")
			(pintype "tri_state")
		)
		(pad "18" thru_hole roundrect
			(at 0 43.18 90)
			(size 1.5 1.5)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 197 "VD1")
			(pinfunction "D1")
			(pintype "tri_state")
		)
		(pad "19" thru_hole roundrect
			(at 0 45.72 90)
			(size 1.5 1.5)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 196 "VD0")
			(pinfunction "D0")
			(pintype "tri_state")
		)
		(pad "20" thru_hole roundrect
			(at 0 48.26 90)
			(size 1.5 1.5)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 106 "~{CAS0}")
			(pinfunction "~{OE}")
			(pintype "input")
		)
		(pad "21" thru_hole roundrect
			(at 15.24 48.26 90)
			(size 1.5 1.5)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 179 "VA1")
			(pinfunction "A0")
			(pintype "input")
		)
		(pad "22" thru_hole roundrect
			(at 15.24 45.72 90)
			(size 1.5 1.5)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 180 "VA2")
			(pinfunction "A1")
			(pintype "input")
		)
		(pad "23" thru_hole roundrect
			(at 15.24 43.18 90)
			(size 1.5 1.5)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 181 "VA3")
			(pinfunction "A2")
			(pintype "input")
		)
		(pad "24" thru_hole roundrect
			(at 15.24 40.64 90)
			(size 1.5 1.5)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 182 "VA4")
			(pinfunction "A3")
			(pintype "input")
		)
		(pad "25" thru_hole roundrect
			(at 15.24 38.1 90)
			(size 1.5 1.5)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 183 "VA5")
			(pinfunction "A4")
			(pintype "input")
		)
		(pad "26" thru_hole roundrect
			(at 15.24 35.56 90)
			(size 1.5 1.5)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 184 "VA6")
			(pinfunction "A5")
			(pintype "input")
		)
		(pad "27" thru_hole roundrect
			(at 15.24 33.02 90)
			(size 1.5 1.5)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 185 "VA7")
			(pinfunction "A6")
			(pintype "input")
		)
		(pad "28" thru_hole roundrect
			(at 15.24 30.48 90)
			(size 1.5 1.5)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 186 "VA8")
			(pinfunction "A7")
			(pintype "input")
		)
		(pad "29" thru_hole roundrect
			(at 15.24 27.94 90)
			(size 1.5 1.5)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 187 "VA9")
			(pinfunction "A8")
			(pintype "input")
		)
		(pad "30" thru_hole roundrect
			(at 15.24 25.4 90)
			(size 1.5 1.5)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "31" thru_hole roundrect
			(at 15.24 22.86 90)
			(size 1.5 1.5)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 188 "VA10")
			(pinfunction "A9")
			(pintype "input")
		)
		(pad "32" thru_hole roundrect
			(at 15.24 20.32 90)
			(size 1.5 1.5)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 189 "VA11")
			(pinfunction "A10")
			(pintype "input")
		)
		(pad "33" thru_hole roundrect
			(at 15.24 17.78 90)
			(size 1.5 1.5)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 190 "VA12")
			(pinfunction "A11")
			(pintype "input")
		)
		(pad "34" thru_hole roundrect
			(at 15.24 15.24 90)
			(size 1.5 1.5)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 191 "VA13")
			(pinfunction "A12")
			(pintype "input")
		)
		(pad "35" thru_hole roundrect
			(at 15.24 12.7 90)
			(size 1.5 1.5)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 192 "VA14")
			(pinfunction "A13")
			(pintype "input")
		)
		(pad "36" thru_hole roundrect
			(at 15.24 10.16 90)
			(size 1.5 1.5)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 193 "VA15")
			(pinfunction "A14")
			(pintype "input")
		)
		(pad "37" thru_hole roundrect
			(at 15.24 7.62 90)
			(size 1.5 1.5)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 194 "VA16")
			(pinfunction "A15")
			(pintype "input")
		)
		(pad "38" thru_hole roundrect
			(at 15.24 5.08 90)
			(size 1.5 1.5)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "D.C.")
			(pintype "power_in")
		)
		(pad "39" thru_hole roundrect
			(at 15.24 2.54 90)
			(size 1.5 1.5)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 4 "VCC2")
			(pinfunction "~{PGM}")
			(pintype "input")
		)
		(pad "40" thru_hole roundrect
			(at 15.24 0 90)
			(size 1.5 1.5)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 4 "VCC2")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Package_DIP.3dshapes/DIP-40_W15.24mm_Socket.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MegaCD_Footprints:CP_Elec_3x5.4"
		(layer "F.Cu")
		(at 118.11 77.978 90)
		(descr "SMD capacitor, aluminum electrolytic, Nichicon, 3.0x5.4mm")
		(tags "capacitor electrolytic")
		(property "Reference" "C37"
			(at -1.905 2.921 270)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "10uF"
			(at 0 2.7 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Polarized capacitor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "MegaCD.kicad_sch")
		(attr smd)
		(fp_text user "-"
			(at 2.1082 -0.6858 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "+"
			(at -3.8354 -0.889 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.597 0 90)
			(size 2.394 1.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.15625)
			(net 4 "VCC2")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.597 0 90)
			(size 2.394 1.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.15625)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/CP_Elec_3x5.4.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MegaCD_Footprints:PQFP-208_28x28mm_P0.5mm_Wider"
		(layer "F.Cu")
		(at 183.7704 101.4764 90)
		(descr "PQFP, 208 Pin (http://www.microsemi.com/index.php?option=com_docman&task=doc_download&gid=131095), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "PQFP QFP")
		(property "Reference" "IC2"
			(at 16.3102 -19.5594 180)
			(layer "F.SilkS")
		)
		(property "Value" "315-5548"
			(at 0.025 11.6 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "MegaCD.kicad_sch")
		(attr smd)
		(fp_text user "157"
			(at 12.175 -21.0834 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "52"
			(at -19.2498 14.121 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "105"
			(at 17.75 13.5 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "1"
			(at -18.8942 -14.2762 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "${VALUE}"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "208"
			(at -13.475 -20.7786 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "104"
			(at 12.575 17.05 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "53"
			(at -15.897 18.439 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "156"
			(at 18.1 -15.4954 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "" smd circle
			(at -15.875 -15.875)
			(size 0.75 0.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
		)
		(pad "" smd circle
			(at -15.875 15.875)
			(size 0.75 0.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
		)
		(pad "" smd circle
			(at 15.853 -15.851)
			(size 0.75 0.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
		)
		(pad "" smd circle
			(at 15.853 15.875)
			(size 0.75 0.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
		)
		(pad "1" smd roundrect
			(at -15.5 -12.75 90)
			(size 1.975 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 48 "Net-(IC2-25M)")
			(pinfunction "25M")
			(pintype "output")
		)
		(pad "2" smd roundrect
			(at -15.5 -12.25 90)
			(size 1.975 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 103 "~{BRAM}")
			(pinfunction "~{BRAM}")
			(pintype "output")
		)
		(pad "3" smd roundrect
			(at -15.5 -11.75 90)
			(size 1.975 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "VSS")
			(pintype "power_in")
		)
		(pad "4" smd roundrect
			(at -15.5 -11.25 90)
			(size 1.975 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 104 "~{BROM}")
			(pinfunction "~{BROM}")
			(pintype "output")
		)
		(pad "5" smd roundrect
			(at -15.5 -10.75 90)
			(size 1.975 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 105 "~{ROM}")
			(pinfunction "~{ROM}")
			(pintype "output")
		)
		(pad "6" smd roundrect
			(at -15.5 -10.25 90)
			(size 1.975 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 106 "~{CAS0}")
			(pinfunction "~{CAS0}")
			(pintype "output")
		)
		(pad "7" smd roundrect
			(at -15.5 -9.75 90)
			(size 1.975 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 107 "~{LWR}")
			(pinfunction "~{LWR}")
			(pintype "output")
		)
		(pad "8" smd roundrect
			(at -15.5 -9.25 90)
			(size 1.975 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 108 "~{UWR}")
			(pinfunction "~{UWR}")
			(pintype "output")
		)
		(pad "9" smd roundrect
			(at -15.5 -8.75 90)
			(size 1.975 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 109 "~{ASEL}")
			(pinfunction "~{ASEL}")
			(pintype "output")
		)
		(pad "10" smd roundrect
			(at -15.5 -8.25 90)
			(size 1.975 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 4 "VCC2")
			(pinfunction "VDD")
			(pintype "power_in")
		)
		(pad "11" smd roundrect
			(at -15.5 -7.75 90)
			(size 1.975 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 333 "~{RAS2}")
			(pinfunction "~{RAS2}")
			(pintype "output")
		)
		(pad "12" smd roundrect
			(at -15.5 -7.25 90)
			(size 1.975 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 110 "~{CAS2}")
			(pinfunction "~{CAS2}")
			(pintype "output")
		)
		(pad "13" smd roundrect
			(at -15.5 -6.75 90)
			(size 1.975 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 111 "~{FDC}")
			(pinfunction "~{FDC}")
			(pintype "output")
		)
		(pad "14" smd roundrect
			(at -15.5 -6.25 90)
			(size 1.975 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 112 "FRES")
			(pinfunction "FRES")
			(pintype "output")
		)
		(pad "15" smd roundrect
			(at -15.5 -5.75 90)
			(size 1.975 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "VSS")
			(pintype "power_in")
		)
		(pad "16" smd roundrect
			(at -15.5 -5.25 90)
			(size 1.975 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 31 "~{ERES}")
			(pinfunction "~{ERES}")
			(pintype "output")
		)
		(pad "17" smd roundrect
			(at -15.5 -4.75 90)
			(size 1.975 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 113 "Net-(IC11-A0)")
			(pinfunction "EAD0")
			(pintype "input")
		)
		(pad "18" smd roundrect
			(at -15.5 -4.25 90)
			(size 1.975 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 114 "Net-(IC11-A1)")
			(pinfunction "EAD1")
			(pintype "input")
		)
		(pad "19" smd roundrect
			(at -15.5 -3.75 90)
			(size 1.975 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 115 "Net-(IC11-A2)")
			(pinfunction "EAD2")
			(pintype "input")
		)
		(pad "20" smd roundrect
			(at -15.5 -3.25 90)
			(size 1.975 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 116 "Net-(IC11-A3)")
			(pinfunction "EAD3")
			(pintype "input")
		)
		(pad "21" smd roundrect
			(at -15.5 -2.75 90)
			(size 1.975 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 117 "Net-(IC11-A4)")
			(pinfunction "EAD4")
			(pintype "input")
		)
		(pad "22" smd roundrect
			(at -15.5 -2.25 90)
			(size 1.975 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 118 "Net-(IC11-A5)")
			(pinfunction "EAD5")
			(pintype "input")
		)
		(pad "23" smd roundrect
			(at -15.5 -1.75 90)
			(size 1.975 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 119 "Net-(IC11-A6)")
			(pinfunction "EAD6")
			(pintype "input")
		)
		(pad "24" smd roundrect
			(at -15.5 -1.25 90)
			(size 1.975 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 120 "Net-(IC11-A7)")
			(pinfunction "EAD7")
			(pintype "input")
		)
		(pad "25" smd roundrect
			(at -15.5 -0.75 90)
			(size 1.975 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 121 "Net-(IC11-D8)")
			(pinfunction "ED8")
			(pintype "input")
		)
		(pad "26" smd roundrect
			(at -15.5 -0.25 90)
			(size 1.975 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "VSS")
			(pintype "power_in")
		)
		(pad "27" smd roundrect
			(at -15.5 0.25 90)
			(size 1.975 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 4 "VCC2")
			(pinfunction "VDD")
			(pintype "power_in")
		)
		(pad "28" smd roundrect
			(at -15.5 0.75 90)
			(size 1.975 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 122 "Net-(IC11-D9)")
			(pinfunction "ED9")
			(pintype "input")
		)
		(pad "29" smd roundrect
			(at -15.5 1.25 90)
			(size 1.975 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 123 "Net-(IC11-D10)")
			(pinfunction "ED10")
			(pintype "input")
		)
		(pad "30" smd roundrect
			(at -15.5 1.75 90)
			(size 1.975 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 124 "Net-(IC11-D11)")
			(pinfunction "ED11")
			(pintype "input")
		)
		(pad "31" smd roundrect
			(at -15.5 2.25 90)
			(size 1.975 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 125 "Net-(IC11-D12)")
			(pinfunction "ED12")
			(pintype "input")
		)
		(pad "32" smd roundrect
			(at -15.5 2.75 90)
			(size 1.975 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 126 "Net-(IC11-D13)")
			(pinfunction "ED13")
			(pintype "input")
		)
		(pad "33" smd roundrect
			(at -15.5 3.25 90)
			(size 1.975 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 127 "Net-(IC11-D14)")
			(pinfunction "ED14")
			(pintype "input")
		)
		(pad "34" smd roundrect
			(at -15.5 3.75 90)
			(size 1.975 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 128 "Net-(IC11-D15)")
			(pinfunction "ED15")
			(pintype "input")
		)
		(pad "35" smd roundrect
			(at -15.5 4.25 90)
			(size 1.975 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 129 "~{ERAS}")
			(pinfunction "~{ERAS}")
			(pintype "input")
		)
		(pad "36" smd roundrect
			(at -15.5 4.75 90)
			(size 1.975 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 130 "~{ECAS}")
			(pinfunction "~{ECAS}")
			(pintype "input")
		)
		(pad "37" smd roundrect
			(at -15.5 5.25 90)
			(size 1.975 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 131 "~{EOE}")
			(pinfunction "~{EOE}")
			(pintype "input")
		)
		(pad "38" smd roundrect
			(at -15.5 5.75 90)
			(size 1.975 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "VSS")
			(pintype "power_in")
		)
		(pad "39" smd roundrect
			(at -15.5 6.25 90)
			(size 1.975 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 261 "~{EWE}")
			(pinfunction "~{EWE}")
			(pintype "input")
		)
		(pad "40" smd roundrect
			(at -15.5 6.75 90)
			(size 1.975 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 132 "~{ORAS}")
			(pinfunction "~{ORAS}")
			(pintype "input")
		)
		(pad "41" smd roundrect
			(at -15.5 7.25 90)
			(size 1.975 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 133 "~{OCAS}")
			(pinfunction "~{OCAS}")
			(pintype "input")
		)
		(pad "42" smd roundrect
			(at -15.5 7.75 90)
			(size 1.975 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 134 "~{OOE}")
			(pinfunction "~{OOE}")
			(pintype "input")
		)
		(pad "43" smd roundrect
			(at -15.5 8.25 90)
			(size 1.975 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 4 "VCC2")
			(pinfunction "VDD")
			(pintype "power_in")
		)
		(pad "44" smd roundrect
			(at -15.5 8.75 90)
			(size 1.975 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 135 "~{OWE}")
			(pinfunction "~{OWE}")
			(pintype "input")
		)
		(pad "45" smd roundrect
			(at -15.5 9.25 90)
			(size 1.975 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 136 "Net-(IC12-A0)")
			(pinfunction "OAD0")
			(pintype "input")
		)
		(pad "46" smd roundrect
			(at -15.5 9.75 90)
			(size 1.975 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 137 "Net-(IC12-A1)")
			(pinfunction "OAD1")
			(pintype "input")
		)
		(pad "47" smd roundrect
			(at -15.5 10.25 90)
			(size 1.975 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 138 "Net-(IC12-A2)")
			(pinfunction "OAD2")
			(pintype "input")
		)
		(pad "48" smd roundrect
			(at -15.5 10.75 90)
			(size 1.975 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 139 "Net-(IC12-A3)")
			(pinfunction "OAD3")
			(pintype "input")
		)
		(pad "49" smd roundrect
			(at -15.5 11.25 90)
			(size 1.975 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 140 "Net-(IC12-A4)")
			(pinfunction "OAD4")
			(pintype "input")
		)
		(pad "50" smd roundrect
			(at -15.5 11.75 90)
			(size 1.975 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "VSS")
			(pintype "power_in")
		)
		(pad "51" smd roundrect
			(at -15.5 12.25 90)
			(size 1.975 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 141 "Net-(IC12-A5)")
			(pinfunction "OAD5")
			(pintype "input")
		)
		(pad "52" smd roundrect
			(at -15.5 12.75 90)
			(size 1.975 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 142 "Net-(IC12-A6)")
			(pinfunction "OAD6")
			(pintype "input")
		)
		(pad "53" smd roundrect
			(at -12.75 15.5 90)
			(size 0.3 1.975)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 143 "Net-(IC12-A7)")
			(pinfunction "OAD7")
			(pintype "input")
		)
		(pad "54" smd roundrect
			(at -12.25 15.5 90)
			(size 0.3 1.975)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 144 "Net-(IC12-D8)")
			(pinfunction "OD8")
			(pintype "input")
		)
		(pad "55" smd roundrect
			(at -11.75 15.5 90)
			(size 0.3 1.975)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 145 "Net-(IC12-D9)")
			(pinfunction "OD9")
			(pintype "input")
		)
		(pad "56" smd roundrect
			(at -11.25 15.5 90)
			(size 0.3 1.975)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 146 "Net-(IC12-D10)")
			(pinfunction "OD10")
			(pintype "input")
		)
		(pad "57" smd roundrect
			(at -10.75 15.5 90)
			(size 0.3 1.975)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 147 "Net-(IC12-D11)")
			(pinfunction "OD11")
			(pintype "input")
		)
		(pad "58" smd roundrect
			(at -10.25 15.5 90)
			(size 0.3 1.975)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 148 "Net-(IC12-D12)")
			(pinfunction "OD12")
			(pintype "input")
		)
		(pad "59" smd roundrect
			(at -9.75 15.5 90)
			(size 0.3 1.975)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 149 "Net-(IC12-D13)")
			(pinfunction "OD13")
			(pintype "input")
		)
		(pad "60" smd roundrect
			(at -9.25 15.5 90)
			(size 0.3 1.975)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "VSS")
			(pintype "power_in")
		)
		(pad "61" smd roundrect
			(at -8.75 15.5 90)
			(size 0.3 1.975)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 4 "VCC2")
			(pinfunction "VDD")
			(pintype "power_in")
		)
		(pad "62" smd roundrect
			(at -8.25 15.5 90)
			(size 0.3 1.975)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 150 "Net-(IC12-D14)")
			(pinfunction "OD14")
			(pintype "input")
		)
		(pad "63" smd roundrect
			(at -7.75 15.5 90)
			(size 0.3 1.975)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 151 "Net-(IC12-D15)")
			(pinfunction "OD15")
			(pintype "input")
		)
		(pad "64" smd roundrect
			(at -7.25 15.5 90)
			(size 0.3 1.975)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 152 "Net-(IC2-LEDR)")
			(pinfunction "LEDR")
			(pintype "output")
		)
		(pad "65" smd roundrect
			(at -6.75 15.5 90)
			(size 0.3 1.975)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 153 "Net-(IC2-LEDG)")
			(pinfunction "LEDG")
			(pintype "output")
		)
		(pad "66" smd roundrect
			(at -6.25 15.5 90)
			(size 0.3 1.975)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 37 "LATCH")
			(pinfunction "LATCH")
			(pintype "output")
		)
		(pad "67" smd roundrect
			(at -5.75 15.5 90)
			(size 0.3 1.975)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 36 "SHFT")
			(pinfunction "SHFT")
			(pintype "output")
		)
		(pad "68" smd roundrect
			(at -5.25 15.5 90)
			(size 0.3 1.975)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 35 "ATT")
			(pinfunction "AT")
			(pintype "output")
		)
		(pad "69" smd roundrect
			(at -4.75 15.5 90)
			(size 0.3 1.975)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 34 "DDATA")
			(pinfunction "DTM")
			(pintype "output")
		)
		(pad "70" smd roundrect
			(at -4.25 15.5 90)
			(size 0.3 1.975)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 154 "WFCKD")
			(pinfunction "WFCK")
			(pintype "input")
		)
		(pad "71" smd roundrect
			(at -3.75 15.5 90)
			(size 0.3 1.975)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 155 "SCORB")
			(pinfunction "SCOR")
			(pintype "input")
		)
		(pad "72" smd roundrect
			(at -3.25 15.5 90)
			(size 0.3 1.975)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "VSS")
			(pintype "power_in")
		)
		(pad "73" smd roundrect
			(at -2.75 15.5 90)
			(size 0.3 1.975)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 156 "SBSOB")
			(pinfunction "SBSO")
			(pintype "input")
		)
		(pad "74" smd roundrect
			(at -2.25 15.5 90)
			(size 0.3 1.975)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 23 "Net-(CN1-Pin_17)")
			(pinfunction "EXCK")
			(pintype "input")
		)
		(pad "75" smd roundrect
			(at -1.75 15.5 90)
			(size 0.3 1.975)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 6 "LRCKB")
			(pinfunction "LRCK")
			(pintype "input")
		)
		(pad "76" smd roundrect
			(at -1.25 15.5 90)
			(size 0.3 1.975)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 157 "SDATAB")
			(pinfunction "SDATA")
			(pintype "input")
		)
		(pad "77" smd roundrect
			(at -0.75 15.5 90)
			(size 0.3 1.975)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 16 "Net-(CN1-Pin_10)")
			(pinfunction "C2PO")
			(pintype "input")
		)
		(pad "78" smd roundrect
			(at -0.25 15.5 90)
			(size 0.3 1.975)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 15 "Net-(CN1-Pin_9)")
			(pinfunction "DB3")
			(pintype "input")
		)
		(pad "79" smd roundrect
			(at 0.25 15.5 90)
			(size 0.3 1.975)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 4 "VCC2")
			(pinfunction "VDD")
			(pintype "power_in")
		)
		(pad "80" smd roundrect
			(at 0.75 15.5 90)
			(size 0.3 1.975)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 14 "Net-(CN1-Pin_8)")
			(pinfunction "DB2")
			(pintype "input")
		)
		(pad "81" smd roundrect
			(at 1.25 15.5 90)
			(size 0.3 1.975)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 13 "Net-(CN1-Pin_7)")
			(pinfunction "DB1")
			(pintype "input")
		)
		(pad "82" smd roundrect
			(at 1.75 15.5 90)
			(size 0.3 1.975)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 12 "Net-(CN1-Pin_6)")
			(pinfunction "DB0")
			(pintype "input")
		)
		(pad "83" smd roundrect
			(at 2.25 15.5 90)
			(size 0.3 1.975)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 11 "Net-(CN1-Pin_5)")
			(pinfunction "HDCK")
			(pintype "input")
		)
		(pad "84" smd roundrect
			(at 2.75 15.5 90)
			(size 0.3 1.975)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 47 "50M")
			(pinfunction "50M")
			(pintype "output")
		)
		(pad "85" smd roundrect
			(at 3.25 15.5 90)
			(size 0.3 1.975)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "VSS")
			(pintype "power_in")
		)
		(pad "86" smd roundrect
			(at 3.75 15.5 90)
			(size 0.3 1.975)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 10 "Net-(CN1-Pin_3)")
			(pinfunction "~{IRQ}")
			(pintype "input")
		)
		(pad "87" smd roundrect
			(at 4.25 15.5 90)
			(size 0.3 1.975)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 9 "Net-(CN1-Pin_2)")
			(pinfunction "D/M")
			(pintype "input")
		)
		(pad "88" smd roundrect
			(at 4.75 15.5 90)
			(size 0.3 1.975)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 158 "CDCKD")
			(pinfunction "CDCK")
			(pintype "input")
		)
		(pad "89" smd roundrect
			(at 5.25 15.5 90)
			(size 0.3 1.975)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 159 "~{PCM}")
			(pinfunction "~{PCM}")
			(pintype "output")
		)
		(pad "90" smd roundrect
			(at 5.75 15.5 90)
			(size 0.3 1.975)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 160 "~{DTEN}")
			(pinfunction "~{DTEN}")
			(pintype "output")
		)
		(pad "91" smd roundrect
			(at 6.25 15.5 90)
			(size 0.3 1.975)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 161 "~{WAIT}")
			(pinfunction "~{WAIT}")
			(pintype "output")
		)
		(pad "92" smd roundrect
			(at 6.75 15.5 90)
			(size 0.3 1.975)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 162 "~{HRD}")
			(pinfunction "~{HRD}")
			(pintype "output")
		)
		(pad "93" smd roundrect
			(at 7.25 15.5 90)
			(size 0.3 1.975)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 163 "~{INT}")
			(pinfunction "~{INT}")
			(pintype "output")
		)
		(pad "94" smd roundrect
			(at 7.75 15.5 90)
			(size 0.3 1.975)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 164 "~{CDC}")
			(pinfunction "~{CDC}")
			(pintype "output")
		)
		(pad "95" smd roundrect
			(at 8.25 15.5 90)
			(size 0.3 1.975)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 165 "~{COE}")
			(pinfunction "~{COE}")
			(pintype "output")
		)
		(pad "96" smd roundrect
			(at 8.75 15.5 90)
			(size 0.3 1.975)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "VSS")
			(pintype "power_in")
		)
		(pad "97" smd roundrect
			(at 9.25 15.5 90)
			(size 0.3 1.975)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 4 "VCC2")
			(pinfunction "VDD")
			(pintype "power_in")
		)
		(pad "98" smd roundrect
			(at 9.75 15.5 90)
			(size 0.3 1.975)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 166 "C2LR")
			(pinfunction "C2LR")
			(pintype "output")
		)
		(pad "99" smd roundrect
			(at 10.25 15.5 90)
			(size 0.3 1.975)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 87 "A19")
			(pinfunction "A19")
			(pintype "output")
		)
		(pad "100" smd roundrect
			(at 10.75 15.5 90)
			(size 0.3 1.975)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 86 "A18")
			(pinfunction "A18")
			(pintype "output")
		)
		(pad "101" smd roundrect
			(at 11.25 15.5 90)
			(size 0.3 1.975)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 85 "A17")
			(pinfunction "A17")
			(pintype "output")
		)
		(pad "102" smd roundrect
			(at 11.75 15.5 90)
			(size 0.3 1.975)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 84 "A16")
			(pinfunction "A16")
			(pintype "output")
		)
		(pad "103" smd roundrect
			(at 12.25 15.5 90)
			(size 0.3 1.975)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 83 "A15")
			(pinfunction "A15")
			(pintype "output")
		)
		(pad "104" smd roundrect
			(at 12.75 15.5 90)
			(size 0.3 1.975)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 82 "A14")
			(pinfunction "A14")
			(pintype "output")
		)
		(pad "105" smd roundrect
			(at 15.5 12.75 90)
			(size 1.975 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 81 "A13")
			(pinfunction "A13")
			(pintype "output")
		)
		(pad "106" smd roundrect
			(at 15.5 12.25 90)
			(size 1.975 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 80 "A12")
			(pinfunction "A12")
			(pintype "output")
		)
		(pad "107" smd roundrect
			(at 15.5 11.75 90)
			(size 1.975 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "VSS")
			(pintype "power_in")
		)
		(pad "108" smd roundrect
			(at 15.5 11.25 90)
			(size 1.975 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 79 "A11")
			(pinfunction "A11")
			(pintype "output")
		)
		(pad "109" smd roundrect
			(at 15.5 10.75 90)
			(size 1.975 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 78 "A10")
			(pinfunction "A10")
			(pintype "output")
		)
		(pad "110" smd roundrect
			(at 15.5 10.25 90)
			(size 1.975 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 77 "A9")
			(pinfunction "A9")
			(pintype "output")
		)
		(pad "111" smd roundrect
			(at 15.5 9.75 90)
			(size 1.975 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 76 "A8")
			(pinfunction "A8")
			(pintype "output")
		)
		(pad "112" smd roundrect
			(at 15.5 9.25 90)
			(size 1.975 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 75 "A7")
			(pinfunction "A7")
			(pintype "output")
		)
		(pad "113" smd roundrect
			(at 15.5 8.75 90)
			(size 1.975 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 74 "A6")
			(pinfunction "A6")
			(pintype "output")
		)
		(pad "114" smd roundrect
			(at 15.5 8.25 90)
			(size 1.975 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 4 "VCC2")
			(pinfunction "VDD")
			(pintype "power_in")
		)
		(pad "115" smd roundrect
			(at 15.5 7.75 90)
			(size 1.975 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 73 "A5")
			(pinfunction "A5")
			(pintype "output")
		)
		(pad "116" smd roundrect
			(at 15.5 7.25 90)
			(size 1.975 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 72 "A4")
			(pinfunction "A4")
			(pintype "output")
		)
		(pad "117" smd roundrect
			(at 15.5 6.75 90)
			(size 1.975 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 71 "A3")
			(pinfunction "A3")
			(pintype "output")
		)
		(pad "118" smd roundrect
			(at 15.5 6.25 90)
			(size 1.975 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 70 "A2")
			(pinfunction "A2")
			(pintype "output")
		)
		(pad "119" smd roundrect
			(at 15.5 5.75 90)
			(size 1.975 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "VSS")
			(pintype "power_in")
		)
		(pad "120" smd roundrect
			(at 15.5 5.25 90)
			(size 1.975 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 69 "A1")
			(pinfunction "A1")
			(pintype "output")
		)
		(pad "121" smd roundrect
			(at 15.5 4.75 90)
			(size 1.975 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 67 "FC0")
			(pinfunction "FC0")
			(pintype "output")
		)
		(pad "122" smd roundrect
			(at 15.5 4.25 90)
			(size 1.975 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 66 "FC1")
			(pinfunction "FC1")
			(pintype "output")
		)
		(pad "123" smd roundrect
			(at 15.5 3.75 90)
			(size 1.975 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 318 "~{IPL0}")
			(pinfunction "~{IPL0}")
			(pintype "output")
		)
		(pad "124" smd roundrect
			(at 15.5 3.25 90)
			(size 1.975 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 317 "~{IPL1}")
			(pinfunction "~{IPL1}")
			(pintype "output")
		)
		(pad "125" smd roundrect
			(at 15.5 2.75 90)
			(size 1.975 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 316 "~{IPL2}")
			(pinfunction "~{IPL2}")
			(pintype "output")
		)
		(pad "126" smd roundrect
			(at 15.5 2.25 90)
			(size 1.975 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 64 "~{VPA}")
			(pinfunction "~{VPA}")
			(pintype "output")
		)
		(pad "127" smd roundrect
			(at 15.5 1.75 90)
			(size 1.975 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 62 "~{RES}")
			(pinfunction "~{RESET}")
			(pintype "output")
		)
		(pad "128" smd roundrect
			(at 15.5 1.25 90)
			(size 1.975 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 61 "~{HALT}")
			(pinfunction "~{HALT}")
			(pintype "output")
		)
		(pad "129" smd roundrect
			(at 15.5 0.75 90)
			(size 1.975 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 46 "Net-(IC2-12M)")
			(pinfunction "12M")
			(pintype "output")
		)
		(pad "130" smd roundrect
			(at 15.5 0.25 90)
			(size 1.975 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "VSS")
			(pintype "power_in")
		)
		(pad "131" smd roundrect
			(at 15.5 -0.25 90)
			(size 1.975 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 4 "VCC2")
			(pinfunction "VDD")
			(pintype "power_in")
		)
		(pad "132" smd roundrect
			(at 15.5 -0.75 90)
			(size 1.975 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 58 "~{DTAK}")
			(pinfunction "~{DTAK}")
			(pintype "output")
		)
		(pad "133" smd roundrect
			(at 15.5 -1.25 90)
			(size 1.975 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 57 "R{slash}~{W}")
			(pinfunction "R/~{W}")
			(pintype "output")
		)
		(pad "134" smd roundrect
			(at 15.5 -1.75 90)
			(size 1.975 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 56 "~{LDS}")
			(pinfunction "~{LDS}")
			(pintype "output")
		)
		(pad "135" smd roundrect
			(at 15.5 -2.25 90)
			(size 1.975 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 55 "~{UDS}")
			(pinfunction "~{UDS}")
			(pintype "output")
		)
		(pad "136" smd roundrect
			(at 15.5 -2.75 90)
			(size 1.975 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 54 "~{AS}")
			(pinfunction "~{AS}")
			(pintype "output")
		)
		(pad "137" smd roundrect
			(at 15.5 -3.25 90)
			(size 1.975 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 53 "D0")
			(pinfunction "D0")
			(pintype "bidirectional")
		)
		(pad "138" smd roundrect
			(at 15.5 -3.75 90)
			(size 1.975 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 52 "D1")
			(pinfunction "D1")
			(pintype "bidirectional")
		)
		(pad "139" smd roundrect
			(at 15.5 -4.25 90)
			(size 1.975 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 51 "D2")
			(pinfunction "D2")
			(pintype "bidirectional")
		)
		(pad "140" smd roundrect
			(at 15.5 -4.75 90)
			(size 1.975 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 50 "D3")
			(pinfunction "D3")
			(pintype "bidirectional")
		)
		(pad "141" smd roundrect
			(at 15.5 -5.25 90)
			(size 1.975 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 49 "D4")
			(pinfunction "D4")
			(pintype "bidirectional")
		)
		(pad "142" smd roundrect
			(at 15.5 -5.75 90)
			(size 1.975 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "VSS")
			(pintype "power_in")
		)
		(pad "143" smd roundrect
			(at 15.5 -6.25 90)
			(size 1.975 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 102 "D5")
			(pinfunction "D5")
			(pintype "bidirectional")
		)
		(pad "144" smd roundrect
			(at 15.5 -6.75 90)
			(size 1.975 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 101 "D6")
			(pinfunction "D6")
			(pintype "bidirectional")
		)
		(pad "145" smd roundrect
			(at 15.5 -7.25 90)
			(size 1.975 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 100 "D7")
			(pinfunction "D7")
			(pintype "bidirectional")
		)
		(pad "146" smd roundrect
			(at 15.5 -7.75 90)
			(size 1.975 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 99 "D8")
			(pinfunction "D8")
			(pintype "bidirectional")
		)
		(pad "147" smd roundrect
			(at 15.5 -8.25 90)
			(size 1.975 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 4 "VCC2")
			(pinfunction "VDD")
			(pintype "power_in")
		)
		(pad "148" smd roundrect
			(at 15.5 -8.75 90)
			(size 1.975 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 98 "D9")
			(pinfunction "D9")
			(pintype "bidirectional")
		)
		(pad "149" smd roundrect
			(at 15.5 -9.25 90)
			(size 1.975 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 97 "D10")
			(pinfunction "D10")
			(pintype "bidirectional")
		)
		(pad "150" smd roundrect
			(at 15.5 -9.75 90)
			(size 1.975 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 96 "D11")
			(pinfunction "D11")
			(pintype "bidirectional")
		)
		(pad "151" smd roundrect
			(at 15.5 -10.25 90)
			(size 1.975 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 95 "D12")
			(pinfunction "D12")
			(pintype "bidirectional")
		)
		(pad "152" smd roundrect
			(at 15.5 -10.75 90)
			(size 1.975 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 94 "D13")
			(pinfunction "D13")
			(pintype "bidirectional")
		)
		(pad "153" smd roundrect
			(at 15.5 -11.25 90)
			(size 1.975 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 93 "D14")
			(pinfunction "D14")
			(pintype "bidirectional")
		)
		(pad "154" smd roundrect
			(at 15.5 -11.75 90)
			(size 1.975 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "VSS")
			(pintype "power_in")
		)
		(pad "155" smd roundrect
			(at 15.5 -12.25 90)
			(size 1.975 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 92 "D15")
			(pinfunction "D15")
			(pintype "bidirectional")
		)
		(pad "156" smd roundrect
			(at 15.5 -12.75 90)
			(size 1.975 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 175 "PA0")
			(pinfunction "PA0")
			(pintype "power_in")
		)
		(pad "157" smd roundrect
			(at 12.75 -15.5 90)
			(size 0.3 1.975)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 174 "PA1")
			(pinfunction "PA1")
			(pintype "power_in")
		)
		(pad "158" smd roundrect
			(at 12.25 -15.5 90)
			(size 0.3 1.975)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 173 "PA2")
			(pinfunction "PA2")
			(pintype "power_in")
		)
		(pad "159" smd roundrect
			(at 11.75 -15.5 90)
			(size 0.3 1.975)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 172 "PA3")
			(pinfunction "PA3")
			(pintype "power_in")
		)
		(pad "160" smd roundrect
			(at 11.25 -15.5 90)
			(size 0.3 1.975)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 171 "PA4")
			(pinfunction "PA4")
			(pintype "power_in")
		)
		(pad "161" smd roundrect
			(at 10.75 -15.5 90)
			(size 0.3 1.975)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 170 "PA5")
			(pinfunction "PA5")
			(pintype "power_in")
		)
		(pad "162" smd roundrect
			(at 10.25 -15.5 90)
			(size 0.3 1.975)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 169 "PA6")
			(pinfunction "PA6")
			(pintype "power_in")
		)
		(pad "163" smd roundrect
			(at 9.75 -15.5 90)
			(size 0.3 1.975)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 168 "PA7")
			(pinfunction "PA7")
			(pintype "power_in")
		)
		(pad "164" smd roundrect
			(at 9.25 -15.5 90)
			(size 0.3 1.975)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "VSS")
			(pintype "power_in")
		)
		(pad "165" smd roundrect
			(at 8.75 -15.5 90)
			(size 0.3 1.975)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 4 "VCC2")
			(pinfunction "VDD")
			(pintype "power_in")
		)
		(pad "166" smd roundrect
			(at 8.25 -15.5 90)
			(size 0.3 1.975)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 167 "PA8")
			(pinfunction "PA8")
			(pintype "power_in")
		)
		(pad "167" smd roundrect
			(at 7.75 -15.5 90)
			(size 0.3 1.975)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 176 "~{PRAS}")
			(pinfunction "~{PRAS}")
			(pintype "output")
		)
		(pad "168" smd roundrect
			(at 7.25 -15.5 90)
			(size 0.3 1.975)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 177 "~{PCAS}")
			(pinfunction "~{PCAS}")
			(pintype "output")
		)
		(pad "169" smd roundrect
			(at 6.75 -15.5 90)
			(size 0.3 1.975)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 178 "~{CUWE}")
			(pinfunction "~{CUWE}")
			(pintype "output")
		)
		(pad "170" smd roundrect
			(at 6.25 -15.5 90)
			(size 0.3 1.975)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 334 "~{CLWE}")
			(pinfunction "~{CLWE}")
			(pintype "output")
		)
		(pad "171" smd roundrect
			(at 5.75 -15.5 90)
			(size 0.3 1.975)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 179 "VA1")
			(pinfunction "VA1")
			(pintype "output")
		)
		(pad "172" smd roundrect
			(at 5.25 -15.5 90)
			(size 0.3 1.975)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 180 "VA2")
			(pinfunction "VA2")
			(pintype "output")
		)
		(pad "173" smd roundrect
			(at 4.75 -15.5 90)
			(size 0.3 1.975)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 181 "VA3")
			(pinfunction "VA3")
			(pintype "output")
		)
		(pad "174" smd roundrect
			(at 4.25 -15.5 90)
			(size 0.3 1.975)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 182 "VA4")
			(pinfunction "VA4")
			(pintype "output")
		)
		(pad "175" smd roundrect
			(at 3.75 -15.5 90)
			(size 0.3 1.975)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 183 "VA5")
			(pinfunction "VA5")
			(pintype "output")
		)
		(pad "176" smd roundrect
			(at 3.25 -15.5 90)
			(size 0.3 1.975)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "VSS")
			(pintype "power_in")
		)
		(pad "177" smd roundrect
			(at 2.75 -15.5 90)
			(size 0.3 1.975)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 184 "VA6")
			(pinfunction "VA6")
			(pintype "output")
		)
		(pad "178" smd roundrect
			(at 2.25 -15.5 90)
			(size 0.3 1.975)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 185 "VA7")
			(pinfunction "VA7")
			(pintype "output")
		)
		(pad "179" smd roundrect
			(at 1.75 -15.5 90)
			(size 0.3 1.975)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 186 "VA8")
			(pinfunction "VA8")
			(pintype "output")
		)
		(pad "180" smd roundrect
			(at 1.25 -15.5 90)
			(size 0.3 1.975)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 187 "VA9")
			(pinfunction "VA9")
			(pintype "output")
		)
		(pad "181" smd roundrect
			(at 0.75 -15.5 90)
			(size 0.3 1.975)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 188 "VA10")
			(pinfunction "VA10")
			(pintype "output")
		)
		(pad "182" smd roundrect
			(at 0.25 -15.5 90)
			(size 0.3 1.975)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 189 "VA11")
			(pinfunction "VA11")
			(pintype "output")
		)
		(pad "183" smd roundrect
			(at -0.25 -15.5 90)
			(size 0.3 1.975)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 4 "VCC2")
			(pinfunction "VDD")
			(pintype "power_in")
		)
		(pad "184" smd roundrect
			(at -0.75 -15.5 90)
			(size 0.3 1.975)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 190 "VA12")
			(pinfunction "VA12")
			(pintype "output")
		)
		(pad "185" smd roundrect
			(at -1.25 -15.5 90)
			(size 0.3 1.975)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 191 "VA13")
			(pinfunction "VA13")
			(pintype "output")
		)
		(pad "186" smd roundrect
			(at -1.75 -15.5 90)
			(size 0.3 1.975)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 192 "VA14")
			(pinfunction "VA14")
			(pintype "output")
		)
		(pad "187" smd roundrect
			(at -2.25 -15.5 90)
			(size 0.3 1.975)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 193 "VA15")
			(pinfunction "VA15")
			(pintype "output")
		)
		(pad "188" smd roundrect
			(at -2.75 -15.5 90)
			(size 0.3 1.975)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 194 "VA16")
			(pinfunction "VA16")
			(pintype "output")
		)
		(pad "189" smd roundrect
			(at -3.25 -15.5 90)
			(size 0.3 1.975)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "VSS")
			(pintype "power_in")
		)
		(pad "190" smd roundrect
			(at -3.75 -15.5 90)
			(size 0.3 1.975)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 195 "VA17")
			(pinfunction "VA17")
			(pintype "output")
		)
		(pad "191" smd roundrect
			(at -4.25 -15.5 90)
			(size 0.3 1.975)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 196 "VD0")
			(pinfunction "VD0")
			(pintype "bidirectional")
		)
		(pad "192" smd roundrect
			(at -4.75 -15.5 90)
			(size 0.3 1.975)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 197 "VD1")
			(pinfunction "VD1")
			(pintype "bidirectional")
		)
		(pad "193" smd roundrect
			(at -5.25 -15.5 90)
			(size 0.3 1.975)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 198 "VD2")
			(pinfunction "VD2")
			(pintype "bidirectional")
		)
		(pad "194" smd roundrect
			(at -5.75 -15.5 90)
			(size 0.3 1.975)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 199 "VD3")
			(pinfunction "VD3")
			(pintype "bidirectional")
		)
		(pad "195" smd roundrect
			(at -6.25 -15.5 90)
			(size 0.3 1.975)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 200 "VD4")
			(pinfunction "VD4")
			(pintype "bidirectional")
		)
		(pad "196" smd roundrect
			(at -6.75 -15.5 90)
			(size 0.3 1.975)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 201 "VD5")
			(pinfunction "VD5")
			(pintype "bidirectional")
		)
		(pad "197" smd roundrect
			(at -7.25 -15.5 90)
			(size 0.3 1.975)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 202 "VD6")
			(pinfunction "VD6")
			(pintype "bidirectional")
		)
		(pad "198" smd roundrect
			(at -7.75 -15.5 90)
			(size 0.3 1.975)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 203 "VD7")
			(pinfunction "VD7")
			(pintype "bidirectional")
		)
		(pad "199" smd roundrect
			(at -8.25 -15.5 90)
			(size 0.3 1.975)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 204 "VD8")
			(pinfunction "VD8")
			(pintype "bidirectional")
		)
		(pad "200" smd roundrect
			(at -8.75 -15.5 90)
			(size 0.3 1.975)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "VSS")
			(pintype "power_in")
		)
		(pad "201" smd roundrect
			(at -9.25 -15.5 90)
			(size 0.3 1.975)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 4 "VCC2")
			(pinfunction "VDD")
			(pintype "power_in")
		)
		(pad "202" smd roundrect
			(at -9.75 -15.5 90)
			(size 0.3 1.975)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 205 "VD9")
			(pinfunction "VD9")
			(pintype "bidirectional")
		)
		(pad "203" smd roundrect
			(at -10.25 -15.5 90)
			(size 0.3 1.975)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 206 "VD10")
			(pinfunction "VD10")
			(pintype "bidirectional")
		)
		(pad "204" smd roundrect
			(at -10.75 -15.5 90)
			(size 0.3 1.975)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 207 "VD11")
			(pinfunction "VD11")
			(pintype "bidirectional")
		)
		(pad "205" smd roundrect
			(at -11.25 -15.5 90)
			(size 0.3 1.975)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 208 "VD12")
			(pinfunction "VD12")
			(pintype "bidirectional")
		)
		(pad "206" smd roundrect
			(at -11.75 -15.5 90)
			(size 0.3 1.975)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 209 "VD13")
			(pinfunction "VD13")
			(pintype "bidirectional")
		)
		(pad "207" smd roundrect
			(at -12.25 -15.5 90)
			(size 0.3 1.975)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 210 "VD14")
			(pinfunction "VD14")
			(pintype "bidirectional")
		)
		(pad "208" smd roundrect
			(at -12.75 -15.5 90)
			(size 0.3 1.975)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 211 "VD15")
			(pinfunction "VD15")
			(pintype "bidirectional")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Package_QFP.3dshapes/PQFP-208_28x28mm_P0.5mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MegaCD_Footprints:SOIC-28Wider"
		(layer "F.Cu")
		(at 72.39 84.074 90)
		(descr "SOIC, 28 Pin (JEDEC MS-013AE, https://www.analog.com/media/en/package-pcb-resources/package/35833120341221rw_28.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOIC SO")
		(property "Reference" "IC14"
			(at 7.8486 -11.049 180)
			(layer "F.SilkS")
		)
		(property "Value" "TC51832"
			(at 0 9.9 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "MegaCD.kicad_sch")
		(attr smd)
		(fp_text user "${VALUE}"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -5.715 -8.255 90)
			(size 2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 232 "/RA14")
			(pinfunction "A14")
			(pintype "input")
		)
		(pad "2" smd roundrect
			(at -5.715 -6.985 90)
			(size 2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 234 "/RA12")
			(pinfunction "A12")
			(pintype "input")
		)
		(pad "3" smd roundrect
			(at -5.715 -5.715 90)
			(size 2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 243 "/RA7")
			(pinfunction "A7")
			(pintype "input")
		)
		(pad "4" smd roundrect
			(at -5.715 -4.445 90)
			(size 2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 244 "/RA6")
			(pinfunction "A6")
			(pintype "input")
		)
		(pad "5" smd roundrect
			(at -5.715 -3.175 90)
			(size 2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 245 "/RA5")
			(pinfunction "A5")
			(pintype "input")
		)
		(pad "6" smd roundrect
			(at -5.715 -1.905 90)
			(size 2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 246 "/RA4")
			(pinfunction "A4")
			(pintype "input")
		)
		(pad "7" smd roundrect
			(at -5.715 -0.635 90)
			(size 2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 248 "/RA3")
			(pinfunction "A3")
			(pintype "input")
		)
		(pad "8" smd roundrect
			(at -5.715 0.635 90)
			(size 2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 249 "/RA2")
			(pinfunction "A2")
			(pintype "input")
		)
		(pad "9" smd roundrect
			(at -5.715 1.905 90)
			(size 2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 250 "/RA1")
			(pinfunction "A1")
			(pintype "input")
		)
		(pad "10" smd roundrect
			(at -5.715 3.175 90)
			(size 2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 251 "/RA0")
			(pinfunction "A0")
			(pintype "input")
		)
		(pad "11" smd roundrect
			(at -5.715 4.445 90)
			(size 2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 231 "/WD0")
			(pinfunction "D0")
			(pintype "tri_state")
		)
		(pad "12" smd roundrect
			(at -5.715 5.715 90)
			(size 2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 230 "/WD1")
			(pinfunction "D1")
			(pintype "tri_state")
		)
		(pad "13" smd roundrect
			(at -5.715 6.985 90)
			(size 2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 229 "/WD2")
			(pinfunction "D2")
			(pintype "tri_state")
		)
		(pad "14" smd roundrect
			(at -5.715 8.255 90)
			(size 2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "15" smd roundrect
			(at 5.715 8.255 90)
			(size 2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 228 "/WD3")
			(pinfunction "D3")
			(pintype "tri_state")
		)
		(pad "16" smd roundrect
			(at 5.715 6.985 90)
			(size 2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 227 "/WD4")
			(pinfunction "D4")
			(pintype "tri_state")
		)
		(pad "17" smd roundrect
			(at 5.715 5.715 90)
			(size 2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 226 "/WD5")
			(pinfunction "D5")
			(pintype "tri_state")
		)
		(pad "18" smd roundrect
			(at 5.715 4.445 90)
			(size 2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 225 "/WD6")
			(pinfunction "D6")
			(pintype "tri_state")
		)
		(pad "19" smd roundrect
			(at 5.715 3.175 90)
			(size 2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 224 "/WD7")
			(pinfunction "D7")
			(pintype "tri_state")
		)
		(pad "20" smd roundrect
			(at 5.715 1.905 90)
			(size 2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 308 "~{RCS2X}")
			(pinfunction "~{CE}")
			(pintype "input")
		)
		(pad "21" smd roundrect
			(at 5.715 0.635 90)
			(size 2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 236 "/RA10")
			(pinfunction "A10")
			(pintype "input")
		)
		(pad "22" smd roundrect
			(at 5.715 -0.635 90)
			(size 2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 309 "~{ROE}")
			(pinfunction "~{OE}")
			(pintype "input")
		)
		(pad "23" smd roundrect
			(at 5.715 -1.905 90)
			(size 2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 235 "/RA11")
			(pinfunction "A11")
			(pintype "input")
		)
		(pad "24" smd roundrect
			(at 5.715 -3.175 90)
			(size 2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 237 "/RA9")
			(pinfunction "A9")
			(pintype "input")
		)
		(pad "25" smd roundrect
			(at 5.715 -4.445 90)
			(size 2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 238 "/RA8")
			(pinfunction "A8")
			(pintype "input")
		)
		(pad "26" smd roundrect
			(at 5.715 -5.715 90)
			(size 2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 233 "/RA13")
			(pinfunction "A13")
			(pintype "input")
		)
		(pad "27" smd roundrect
			(at 5.715 -6.985 90)
			(size 2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 242 "Net-(IC13-~{WE})")
			(pinfunction "~{WE}")
			(pintype "input")
		)
		(pad "28" smd roundrect
			(at 5.715 -8.255 90)
			(size 2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 4 "VCC2")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Package_SO.3dshapes/SOIC-28W_7.5x17.9mm_P1.27mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MegaCD_Footprints:SMD_0805_HandSolder_Medium"
		(layer "B.Cu")
		(at 146.0246 124.0028 90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C8"
			(at 3.6068 0.5334 270)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "22nF"
			(at 0 -1.68 270)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "MegaCD.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 270)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.143 0 90)
			(size 1.3 1.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.2127658333)
			(net 4 "VCC2")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.143 0 90)
			(size 1.3 1.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.2127658333)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MegaCD_Footprints:SMD_0805_HandSolder_Medium"
		(layer "B.Cu")
		(at 202.184 59.182)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C50"
			(at 0 -2.032 0)
			(layer "B.SilkS")
		)
		(property "Value" "22nF"
			(at 0 -1.68 0)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "MegaCD.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.143 0)
			(size 1.3 1.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.2127658333)
			(net 4 "VCC2")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.143 0)
			(size 1.3 1.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.2127658333)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MegaCD_Footprints:SMD_0805_HandSolder_Medium"
		(layer "B.Cu")
		(at 225.806 123.825 90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "R5"
			(at 0 1.905 270)
			(layer "B.SilkS")
		)
		(property "Value" "160"
			(at 0 -1.68 270)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "MegaCD.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 270)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.143 0 90)
			(size 1.3 1.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.2127658333)
			(net 298 "Net-(LD2-A)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.143 0 90)
			(size 1.3 1.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.2127658333)
			(net 4 "VCC2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MegaCD_Footprints:SMD_0805_HandSolder_Medium"
		(layer "B.Cu")
		(at 94.488 61.214)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C49"
			(at -1.143 -1.905 0)
			(layer "B.SilkS")
		)
		(property "Value" "22nF"
			(at 0 -1.68 0)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "MegaCD.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.143 0)
			(size 1.3 1.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.2127658333)
			(net 4 "VCC2")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.143 0)
			(size 1.3 1.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.2127658333)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MegaCD_Footprints:Test_Point_1.5mm"
		(layer "B.Cu")
		(at 175.5902 80.5688 180)
		(property "Reference" "M57"
			(at 0 -2.0828 0)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "TestPoint"
			(at 0 -2.032 0)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "MegaCD.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -3.683 0)
			(unlocked yes)
			(layer "B.Fab")
		)
		(pad "1" smd circle
			(at 0 0 180)
			(size 1.5 1.5)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 45 "12M")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "MegaCD_Footprints:SMD_0805_HandSolder_Medium"
		(layer "B.Cu")
		(at 64.008 113.284 -90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C44"
			(at -1.651 -2.159 270)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "22nF"
			(at 0 -1.68 90)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "MegaCD.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.143 0 270)
			(size 1.3 1.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.2127658333)
			(net 4 "VCC2")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.143 0 270)
			(size 1.3 1.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.2127658333)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MegaCD_Footprints:SMD_0805_HandSolder_Medium"
		(layer "B.Cu")
		(at 171.196 120.4214)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C18"
			(at 0.762 -2.0574 180)
			(layer "B.SilkS")
		)
		(property "Value" "0"
			(at 0 -1.68 180)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "MegaCD.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.143 0)
			(size 1.3 1.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.2127658333)
			(net 177 "~{PCAS}")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.143 0)
			(size 1.3 1.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.2127658333)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MegaCD_Footprints:Test_Point_1.5mm"
		(layer "B.Cu")
		(at 135.9662 77.2414 180)
		(property "Reference" "M9"
			(at -0.3048 2.0574 0)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "TestPoint"
			(at 0 -2.032 0)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "MegaCD.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -3.683 0)
			(unlocked yes)
			(layer "B.Fab")
		)
		(pad "1" smd circle
			(at 0 0 180)
			(size 1.5 1.5)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 107 "~{LWR}")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "MegaCD_Footprints:Test_Point_1.5mm"
		(layer "B.Cu")
		(at 164.5158 86.7918 180)
		(property "Reference" "M5"
			(at 0 1.905 0)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "TestPoint"
			(at 0 -2.032 0)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "MegaCD.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -3.683 0)
			(unlocked yes)
			(layer "B.Fab")
		)
		(pad "1" smd circle
			(at 0 0 180)
			(size 1.5 1.5)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 67 "FC0")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "MegaCD_Footprints:SMD_0805_HandSolder_Medium"
		(layer "B.Cu")
		(at 147.4724 106.4514)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C21"
			(at 1.7526 -2.0574 180)
			(layer "B.SilkS")
		)
		(property "Value" "0"
			(at 0 -1.68 180)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "MegaCD.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.143 0)
			(size 1.3 1.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.2127658333)
			(net 176 "~{PRAS}")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.143 0)
			(size 1.3 1.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.2127658333)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MegaCD_Footprints:SMD_0805_HandSolder_Medium"
		(layer "B.Cu")
		(at 198.628 89.408)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "R3"
			(at -1.651 -2.032 180)
			(layer "B.SilkS")
		)
		(property "Value" "2.2K"
			(at 0 -1.68 180)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "MegaCD.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.143 0)
			(size 1.3 1.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.2127658333)
			(net 4 "VCC2")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.143 0)
			(size 1.3 1.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.2127658333)
			(net 81 "A13")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MegaCD_Footprints:SMD_0805_HandSolder_Medium"
		(layer "B.Cu")
		(at 214.1982 86.9188 -90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C29"
			(at -3.8608 0.0762 270)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "100pF"
			(at 0 -1.68 90)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "MegaCD.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.143 0 270)
			(size 1.3 1.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.2127658333)
			(net 129 "~{ERAS}")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.143 0 270)
			(size 1.3 1.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.2127658333)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MegaCD_Footprints:SMD_0805_HandSolder_Medium"
		(layer "B.Cu")
		(at 95.8596 89.2302 180)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "J2"
			(at 0 1.905 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "2TS"
			(at 0 -1.68 0)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Jumper, 2-pole, closed/bridged"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "MegaCD.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.143 0 180)
			(size 1.3 1.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.2127658333)
			(net 41 "PBCLK")
			(pinfunction "A")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.143 0 180)
			(size 1.3 1.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.2127658333)
			(net 41 "PBCLK")
			(pinfunction "B")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MegaCD_Footprints:SMD_0805_HandSolder_Medium"
		(layer "B.Cu")
		(at 177.927 128.6764 -90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C16"
			(at 3.2766 0.889 180)
			(layer "B.SilkS")
		)
		(property "Value" "0"
			(at 0 -1.68 90)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "MegaCD.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.143 0 270)
			(size 1.3 1.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.2127658333)
			(net 177 "~{PCAS}")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.143 0 270)
			(size 1.3 1.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.2127658333)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MegaCD_Footprints:SMD_0805_HandSolder_Medium"
		(layer "B.Cu")
		(at 108.2548 63.9826)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "J5"
			(at 0 1.905 180)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "~"
			(at 0 -1.68 180)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Jumper, 2-pole, closed/bridged"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "MegaCD.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.143 0)
			(size 1.3 1.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.2127658333)
			(net 107 "~{LWR}")
			(pinfunction "A")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.143 0)
			(size 1.3 1.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.2127658333)
			(net 107 "~{LWR}")
			(pinfunction "B")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MegaCD_Footprints:Test_Point_1.5mm"
		(layer "B.Cu")
		(at 141.478 97.536 180)
		(property "Reference" "M7"
			(at -0.381 -2.3114 0)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "TestPoint"
			(at 0 -2.032 0)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "MegaCD.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -3.683 0)
			(unlocked yes)
			(layer "B.Fab")
		)
		(pad "1" smd circle
			(at 0 0 180)
			(size 1.5 1.5)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 315 "E")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "MegaCD_Footprints:SMD_0805_HandSolder_Medium"
		(layer "B.Cu")
		(at 159.0802 100.457)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C52"
			(at 4.1148 -0.127 180)
			(layer "B.SilkS")
		)
		(property "Value" "22nF"
			(at 0 -1.68 180)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "MegaCD.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.143 0)
			(size 1.3 1.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.2127658333)
			(net 2 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.143 0)
			(size 1.3 1.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.2127658333)
			(net 4 "VCC2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MegaCD_Footprints:Test_Point_1.5mm"
		(layer "B.Cu")
		(at 112.649 75.311 180)
		(property "Reference" "M10"
			(at 0.127 -3.937 0)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "TestPoint"
			(at 0 -2.032 0)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "MegaCD.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -3.683 0)
			(unlocked yes)
			(layer "B.Fab")
		)
		(pad "1" smd circle
			(at 0 0 180)
			(size 1.5 1.5)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 108 "~{UWR}")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "MegaCD_Footprints:Test_Point_1.5mm"
		(layer "B.Cu")
		(at 164.465 59.8678 180)
		(property "Reference" "M192"
			(at 0 -2.0828 0)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "TestPoint"
			(at 0 -2.032 0)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "MegaCD.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -3.683 0)
			(unlocked yes)
			(layer "B.Fab")
		)
		(pad "1" smd circle
			(at 0 0 180)
			(size 1.5 1.5)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 2 "GND")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "MegaCD_Footprints:SMD_0805_HandSolder_Medium"
		(layer "B.Cu")
		(at 67.945 79.756 90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C40"
			(at 0 1.905 270)
			(layer "B.SilkS")
		)
		(property "Value" "22nF"
			(at 0 -1.68 270)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "MegaCD.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 270)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.143 0 90)
			(size 1.3 1.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.2127658333)
			(net 4 "VCC2")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.143 0 90)
			(size 1.3 1.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.2127658333)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MegaCD_Footprints:SMD_0805_HandSolder_Medium"
		(layer "B.Cu")
		(at 214.1982 91.948 90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C36"
			(at -3.937 0.1778 270)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "100pF"
			(at 0 -1.68 270)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "MegaCD.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 270)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.143 0 90)
			(size 1.3 1.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.2127658333)
			(net 261 "~{EWE}")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.143 0 90)
			(size 1.3 1.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.2127658333)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MegaCD_Footprints:SMD_0805_HandSolder_Medium"
		(layer "B.Cu")
		(at 211.963 67.183 -90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C27"
			(at 1.397 2.286 270)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "22nF"
			(at 0 -1.68 90)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "MegaCD.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.143 0 270)
			(size 1.3 1.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.2127658333)
			(net 4 "VCC2")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.143 0 270)
			(size 1.3 1.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.2127658333)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MegaCD_Footprints:SMD_0805_HandSolder_Medium"
		(layer "B.Cu")
		(at 167.132 117.3734)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C55"
			(at 0 -2.0574 180)
			(layer "B.SilkS")
		)
		(property "Value" "33pF"
			(at 0 -1.68 180)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Polarized capacitor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "MegaCD.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.143 0)
			(size 1.3 1.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.2127658333)
			(net 7 "25M")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.143 0)
			(size 1.3 1.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.2127658333)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MegaCD_Footprints:SMD_0805_HandSolder_Medium"
		(layer "B.Cu")
		(at 85.9282 85.344 -90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C56"
			(at 4.191 -1.0668 270)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "0"
			(at 0 -1.68 90)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "MegaCD.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.143 0 270)
			(size 1.3 1.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.2127658333)
			(net 45 "12M")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.143 0 270)
			(size 1.3 1.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.2127658333)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MegaCD_Footprints:SMD_0805_HandSolder_Medium"
		(layer "B.Cu")
		(at 95.504 87.0966 180)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "J3"
			(at 0 1.905 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "MH"
			(at 0 -1.68 0)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Jumper, 2-pole, closed/bridged"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "MegaCD.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.143 0 180)
			(size 1.3 1.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.2127658333)
			(net 39 "PDATA")
			(pinfunction "A")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.143 0 180)
			(size 1.3 1.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.2127658333)
			(net 39 "PDATA")
			(pinfunction "B")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MegaCD_Footprints:SOIC-20W_7.5x12.8mm_P1.27mm_narrowed"
		(layer "B.Cu")
		(at 97.7392 121.3612 90)
		(descr "SOIC, 20 Pin (JEDEC MS-013AC, https://www.analog.com/media/en/package-pcb-resources/package/233848rw_20.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOIC SO")
		(property "Reference" "IC20"
			(at 3.7846 -9.7282 180)
			(layer "B.SilkS")
		)
		(property "Value" "74HC245"
			(at 0 -7.35 90)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Octal BUS Transceivers, 3-State outputs"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "MegaCD.kicad_sch")
		(attr smd)
		(fp_text user "${VALUE}"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -3.683 5.715 90)
			(size 2.05 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "A->B")
			(pintype "input")
		)
		(pad "2" smd roundrect
			(at -3.683 4.445 90)
			(size 2.05 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 157 "SDATAB")
			(pinfunction "A0")
			(pintype "tri_state")
		)
		(pad "3" smd roundrect
			(at -3.683 3.175 90)
			(size 2.05 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 33 "DFCKB")
			(pinfunction "A1")
			(pintype "tri_state")
		)
		(pad "4" smd roundrect
			(at -3.683 1.905 90)
			(size 2.05 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 6 "LRCKB")
			(pinfunction "A2")
			(pintype "tri_state")
		)
		(pad "5" smd roundrect
			(at -3.683 0.635 90)
			(size 2.05 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 32 "BCLKB")
			(pinfunction "A3")
			(pintype "tri_state")
		)
		(pad "6" smd roundrect
			(at -3.683 -0.635 90)
			(size 2.05 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 156 "SBSOB")
			(pinfunction "A4")
			(pintype "tri_state")
		)
		(pad "7" smd roundrect
			(at -3.683 -1.905 90)
			(size 2.05 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 155 "SCORB")
			(pinfunction "A5")
			(pintype "tri_state")
		)
		(pad "8" smd roundrect
			(at -3.683 -3.175 90)
			(size 2.05 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 154 "WFCKD")
			(pinfunction "A6")
			(pintype "tri_state")
		)
		(pad "9" smd roundrect
			(at -3.683 -4.445 90)
			(size 2.05 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 158 "CDCKD")
			(pinfunction "A7")
			(pintype "tri_state")
		)
		(pad "10" smd roundrect
			(at -3.683 -5.715 90)
			(size 2.05 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "11" smd roundrect
			(at 3.683 -5.715 90)
			(size 2.05 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 8 "CDCK")
			(pinfunction "B7")
			(pintype "tri_state")
		)
		(pad "12" smd roundrect
			(at 3.683 -4.445 90)
			(size 2.05 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 27 "WFCK")
			(pinfunction "B6")
			(pintype "tri_state")
		)
		(pad "13" smd roundrect
			(at 3.683 -3.175 90)
			(size 2.05 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 26 "SCOR")
			(pinfunction "B5")
			(pintype "tri_state")
		)
		(pad "14" smd roundrect
			(at 3.683 -1.905 90)
			(size 2.05 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 24 "SBSO")
			(pinfunction "B4")
			(pintype "tri_state")
		)
		(pad "15" smd roundrect
			(at 3.683 -0.635 90)
			(size 2.05 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 17 "BCLK")
			(pinfunction "B3")
			(pintype "tri_state")
		)
		(pad "16" smd roundrect
			(at 3.683 0.635 90)
			(size 2.05 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 19 "LRCK")
			(pinfunction "B2")
			(pintype "tri_state")
		)
		(pad "17" smd roundrect
			(at 3.683 1.905 90)
			(size 2.05 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 20 "DFCK")
			(pinfunction "B1")
			(pintype "tri_state")
		)
		(pad "18" smd roundrect
			(at 3.683 3.175 90)
			(size 2.05 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 18 "SDATA")
			(pinfunction "B0")
			(pintype "tri_state")
		)
		(pad "19" smd roundrect
			(at 3.683 4.445 90)
			(size 2.05 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "CE")
			(pintype "input")
		)
		(pad "20" smd roundrect
			(at 3.683 5.715 90)
			(size 2.05 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 4 "VCC2")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Package_SO.3dshapes/SOIC-20W_7.5x12.8mm_P1.27mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MegaCD_Footprints:Test_Point_1.5mm"
		(layer "B.Cu")
		(at 154.178 91.567 180)
		(property "Reference" "M3"
			(at -0.9398 -2.286 0)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "TestPoint"
			(at 0 -2.032 0)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "MegaCD.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -3.683 0)
			(unlocked yes)
			(layer "B.Fab")
		)
		(pad "1" smd circle
			(at 0 0 180)
			(size 1.5 1.5)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 317 "~{IPL1}")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "MegaCD_Footprints:SMD_0805_HandSolder_Medium"
		(layer "B.Cu")
		(at 105.664 74.803 180)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C57"
			(at 4.064 -0.889 0)
			(layer "B.SilkS")
		)
		(property "Value" "0"
			(at 0 -1.68 0)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "MegaCD.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.143 0 180)
			(size 1.3 1.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.2127658333)
			(net 109 "~{ASEL}")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.143 0 180)
			(size 1.3 1.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.2127658333)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MegaCD_Footprints:LED"
		(layer "B.Cu")
		(at 225.6282 86.1314 90)
		(property "Reference" "LD1"
			(at -4.6228 0.4572 270)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "RED"
			(at 0 -1 270)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Light emitting diode"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "MegaCD.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 -2.5 270)
			(unlocked yes)
			(layer "B.Fab")
		)
		(pad "1" thru_hole roundrect
			(at 1.27 0 90)
			(size 1.5 1.5)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 295 "Net-(LD1-K)")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" thru_hole roundrect
			(at -1.27 0 90)
			(size 1.5 1.5)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 296 "Net-(LD1-A)")
			(pinfunction "A")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "MegaCD_Footprints:SMD_0805_HandSolder_Medium"
		(layer "B.Cu")
		(at 101.473 58.801 -90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C4"
			(at 1.651 -2.159 270)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "22nF"
			(at 0 -1.68 90)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "MegaCD.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.143 0 270)
			(size 1.3 1.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.2127658333)
			(net 4 "VCC2")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.143 0 270)
			(size 1.3 1.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.2127658333)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MegaCD_Footprints:Test_Point_1.5mm"
		(layer "B.Cu")
		(at 197.866 61.849 180)
		(property "Reference" "M0"
			(at 0 1.905 0)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "TestPoint"
			(at 0 -2.032 0)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "MegaCD.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -3.683 0)
			(unlocked yes)
			(layer "B.Fab")
		)
		(pad "1" smd circle
			(at 0 0 180)
			(size 1.5 1.5)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 259 "Net-(IC10-CS2)")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "MegaCD_Footprints:SMD_0805_HandSolder_Medium"
		(layer "B.Cu")
		(at 193.294 56.007 180)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C14"
			(at 0 1.905 0)
			(layer "B.SilkS")
		)
		(property "Value" "22nF"
			(at 0 -1.68 0)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "MegaCD.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.143 0 180)
			(size 1.3 1.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.2127658333)
			(net 4 "VCC2")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.143 0 180)
			(size 1.3 1.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.2127658333)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MegaCD_Footprints:SMD_0805_HandSolder_Medium"
		(layer "B.Cu")
		(at 135.128 102.87)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "R2"
			(at 0 -2.032 180)
			(layer "B.SilkS")
		)
		(property "Value" "4.7K"
			(at 0 -1.68 180)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "MegaCD.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.143 0)
			(size 1.3 1.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.2127658333)
			(net 4 "VCC2")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.143 0)
			(size 1.3 1.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.2127658333)
			(net 61 "~{HALT}")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MegaCD_Footprints:Test_Point_1.5mm"
		(layer "B.Cu")
		(at 103.9114 69.8754 180)
		(property "Reference" "M11"
			(at -2.6924 1.3208 0)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "TestPoint"
			(at 0 -2.032 0)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "MegaCD.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -3.683 0)
			(unlocked yes)
			(layer "B.Fab")
		)
		(pad "1" smd circle
			(at 0 0 180)
			(size 1.5 1.5)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 110 "~{CAS2}")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "MegaCD_Footprints:SMD_0805_HandSolder_Medium"
		(layer "B.Cu")
		(at 137.668 95.631 -90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "R1"
			(at -1.397 -2.159 270)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "4.7K"
			(at 0 -1.68 90)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "MegaCD.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.143 0 270)
			(size 1.3 1.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.2127658333)
			(net 4 "VCC2")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.143 0 270)
			(size 1.3 1.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.2127658333)
			(net 62 "~{RES}")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MegaCD_Footprints:SMD_0805_HandSolder_Medium"
		(layer "B.Cu")
		(at 115.697 108.6358 180)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C22"
			(at 2.159 1.9558 0)
			(layer "B.SilkS")
		)
		(property "Value" "0"
			(at 0 -1.68 0)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "MegaCD.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.143 0 180)
			(size 1.3 1.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.2127658333)
			(net 177 "~{PCAS}")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.143 0 180)
			(size 1.3 1.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.2127658333)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MegaCD_Footprints:SMD_0805_HandSolder_Medium"
		(layer "B.Cu")
		(at 87.376 112.014 -90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C43"
			(at -4.064 0.127 270)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "22nF"
			(at 0 -1.68 90)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "MegaCD.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.143 0 270)
			(size 1.3 1.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.2127658333)
			(net 4 "VCC2")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.143 0 270)
			(size 1.3 1.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.2127658333)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MegaCD_Footprints:SMD_0805_HandSolder_Medium"
		(layer "B.Cu")
		(at 104.775 97.79 -90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C58"
			(at -3.175 -2.159 270)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "0"
			(at 0 -1.68 90)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "MegaCD.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.143 0 270)
			(size 1.3 1.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.2127658333)
			(net 240 "~{CLWEX}")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.143 0 270)
			(size 1.3 1.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.2127658333)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MegaCD_Footprints:SMD_0805_HandSolder_Medium"
		(layer "B.Cu")
		(at 199.771 85.979 90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C24"
			(at 0 2.032 270)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "22nF"
			(at 0 -1.68 270)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "MegaCD.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 270)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.143 0 90)
			(size 1.3 1.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.2127658333)
			(net 4 "VCC2")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.143 0 90)
			(size 1.3 1.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.2127658333)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MegaCD_Footprints:SMD_0805_HandSolder_Medium"
		(layer "B.Cu")
		(at 115.697 114.7318 180)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C20"
			(at 3.937 1.3208 0)
			(layer "B.SilkS")
		)
		(property "Value" "0"
			(at 0 -1.68 0)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "MegaCD.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.143 0 180)
			(size 1.3 1.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.2127658333)
			(net 177 "~{PCAS}")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.143 0 180)
			(size 1.3 1.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.2127658333)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MegaCD_Footprints:SMD_0805_HandSolder_Narrow"
		(layer "B.Cu")
		(at 130.2512 118.999 180)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C19"
			(at 4.0132 -0.127 0)
			(layer "B.SilkS")
		)
		(property "Value" "0"
			(at 0 -1.68 0)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "MegaCD.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.143 0 180)
			(size 1.3 1.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.2127658333)
			(net 176 "~{PRAS}")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.143 0 180)
			(size 1.3 1.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.2127658333)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MegaCD_Footprints:SMD_0805_HandSolder_Medium"
		(layer "B.Cu")
		(at 175.387 128.6764 90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C5"
			(at -3.4036 -1.905 0)
			(layer "B.SilkS")
		)
		(property "Value" "22nF"
			(at 0 -1.68 270)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "MegaCD.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 270)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.143 0 90)
			(size 1.3 1.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.2127658333)
			(net 4 "VCC2")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.143 0 90)
			(size 1.3 1.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.2127658333)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MegaCD_Footprints:SMD_0805_HandSolder_Medium"
		(layer "B.Cu")
		(at 64.008 99.949 -90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C45"
			(at 1.651 -2.032 270)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "22nF"
			(at 0 -1.68 90)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "MegaCD.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.143 0 270)
			(size 1.3 1.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.2127658333)
			(net 4 "VCC2")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.143 0 270)
			(size 1.3 1.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.2127658333)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MegaCD_Footprints:SMD_0805_HandSolder_Medium"
		(layer "B.Cu")
		(at 198.501 114.173)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "R6"
			(at -3.81 -0.127 180)
			(layer "B.SilkS")
		)
		(property "Value" "4.7K"
			(at 0 -1.68 180)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "MegaCD.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.143 0)
			(size 1.3 1.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.2127658333)
			(net 152 "Net-(IC2-LEDR)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.143 0)
			(size 1.3 1.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.2127658333)
			(net 300 "Net-(TR2-B)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MegaCD_Footprints:SMD_0805_HandSolder_Medium"
		(layer "B.Cu")
		(at 90.043 112.014 -90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C47"
			(at -4.064 0.127 270)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "200pF"
			(at 0 -1.68 90)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Polarized capacitor"
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "MegaCD.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.143 0 270)
			(size 1.3 1.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.2127658333)
			(net 6 "LRCKB")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.143 0 270)
			(size 1.3 1.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.2127658333)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MegaCD_Footprints:SMD_0805_HandSolder_Medium"
		(layer "B.Cu")
		(at 147.4724 108.6358)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C7"
			(at 3.6576 1.0922 180)
			(layer "B.SilkS")
		)
		(property "Value" "22nF"
			(at 0 -1.68 180)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "MegaCD.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.143 0)
			(size 1.3 1.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.2127658333)
			(net 4 "VCC2")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.143 0)
			(size 1.3 1.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.2127658333)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MegaCD_Footprints:SMD_0805_HandSolder_Medium"
		(layer "B.Cu")
		(at 215.1634 67.183 -90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C30"
			(at 0 -2.0066 270)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "22nF"
			(at 0 -1.68 90)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "MegaCD.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.143 0 270)
			(size 1.3 1.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.2127658333)
			(net 4 "VCC2")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.143 0 270)
			(size 1.3 1.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.2127658333)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MegaCD_Footprints:SMD_0805_HandSolder_Medium"
		(layer "B.Cu")
		(at 176.8094 123.0884 90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C6"
			(at 3.9624 0.4826 270)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "22nF"
			(at 0 -1.68 270)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "MegaCD.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 270)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.143 0 90)
			(size 1.3 1.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.2127658333)
			(net 4 "VCC2")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.143 0 90)
			(size 1.3 1.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.2127658333)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MegaCD_Footprints:LED"
		(layer "B.Cu")
		(at 225.6282 129.1082 90)
		(property "Reference" "LD2"
			(at 0 -2.032 270)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "GREEN"
			(at 0 -1 270)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Light emitting diode"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "MegaCD.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 -2.5 270)
			(unlocked yes)
			(layer "B.Fab")
		)
		(pad "1" thru_hole roundrect
			(at 1.27 0 90)
			(size 1.5 1.5)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 297 "Net-(LD2-K)")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" thru_hole roundrect
			(at -1.27 0 90)
			(size 1.5 1.5)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.25)
			(net 298 "Net-(LD2-A)")
			(pinfunction "A")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "MegaCD_Footprints:SMD_0805_HandSolder_Medium"
		(layer "B.Cu")
		(at 131.953 88.646)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C2"
			(at 0.508 -2.159 180)
			(layer "B.SilkS")
		)
		(property "Value" "22nF"
			(at 0 -1.68 180)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "MegaCD.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.143 0)
			(size 1.3 1.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.2127658333)
			(net 4 "VCC2")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.143 0)
			(size 1.3 1.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.2127658333)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MegaCD_Footprints:SMD_0805_HandSolder_Medium"
		(layer "B.Cu")
		(at 108.3056 118.1862)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C51"
			(at -0.6096 -2.4892 180)
			(layer "B.SilkS")
		)
		(property "Value" "22nF"
			(at 0 -1.68 180)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "MegaCD.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.143 0)
			(size 1.3 1.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.2127658333)
			(net 4 "VCC2")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.143 0)
			(size 1.3 1.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.2127658333)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MegaCD_Footprints:SMD_0805_HandSolder_Medium"
		(layer "B.Cu")
		(at 180.5686 123.0884 90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C17"
			(at 4.4704 -0.8636 270)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "0"
			(at 0 -1.68 270)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "MegaCD.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 270)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.143 0 90)
			(size 1.3 1.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.2127658333)
			(net 176 "~{PRAS}")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.143 0 90)
			(size 1.3 1.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.2127658333)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MegaCD_Footprints:Test_Point_1.5mm"
		(layer "B.Cu")
		(at 160.655 86.7918 180)
		(property "Reference" "M6"
			(at 0.3048 1.905 0)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "TestPoint"
			(at 0 -2.032 0)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "MegaCD.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -3.683 0)
			(unlocked yes)
			(layer "B.Fab")
		)
		(pad "1" smd circle
			(at 0 0 180)
			(size 1.5 1.5)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 66 "FC1")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "MegaCD_Footprints:SMD_0805_HandSolder_Medium"
		(layer "B.Cu")
		(at 69.977 61.976)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C39"
			(at 0 1.905 180)
			(layer "B.SilkS")
		)
		(property "Value" "22nF"
			(at 0 -1.68 180)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "MegaCD.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.143 0)
			(size 1.3 1.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.2127658333)
			(net 4 "VCC2")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.143 0)
			(size 1.3 1.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.2127658333)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MegaCD_Footprints:Test_Point_1.5mm"
		(layer "B.Cu")
		(at 148.463 95.631 180)
		(property "Reference" "M4"
			(at -0.254 -2.1336 0)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "TestPoint"
			(at 0 -2.032 0)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "MegaCD.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -3.683 0)
			(unlocked yes)
			(layer "B.Fab")
		)
		(pad "1" smd circle
			(at 0 0 180)
			(size 1.5 1.5)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 316 "~{IPL2}")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "MegaCD_Footprints:SMD_0805_HandSolder_Medium"
		(layer "B.Cu")
		(at 88.1634 85.344 -90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C38"
			(at 4.191 -0.9906 270)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "22nF"
			(at 0 -1.68 90)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "MegaCD.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.143 0 270)
			(size 1.3 1.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.2127658333)
			(net 4 "VCC2")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.143 0 270)
			(size 1.3 1.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.2127658333)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MegaCD_Footprints:SMD_0805_HandSolder_Medium"
		(layer "B.Cu")
		(at 198.501 116.713)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "R7"
			(at -3.429 0 180)
			(layer "B.SilkS")
		)
		(property "Value" "4.7K"
			(at 0 -1.68 180)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "MegaCD.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.143 0)
			(size 1.3 1.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.2127658333)
			(net 153 "Net-(IC2-LEDG)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.143 0)
			(size 1.3 1.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.2127658333)
			(net 301 "Net-(TR1-B)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MegaCD_Footprints:SMD_0805_HandSolder_Medium"
		(layer "B.Cu")
		(at 101.981 97.79 90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "J1"
			(at 0 1.905 270)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "~"
			(at 0 -1.68 270)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Jumper, 2-pole, closed/bridged"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "MegaCD.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 270)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.143 0 90)
			(size 1.3 1.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.2127658333)
			(net 165 "~{COE}")
			(pinfunction "A")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.143 0 90)
			(size 1.3 1.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.2127658333)
			(net 165 "~{COE}")
			(pinfunction "B")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MegaCD_Footprints:SMD_0805_HandSolder_Medium"
		(layer "B.Cu")
		(at 180.467 128.6764 90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C15"
			(at 0.0254 2.159 270)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "0"
			(at 0 -1.68 270)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "MegaCD.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 270)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.143 0 90)
			(size 1.3 1.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.2127658333)
			(net 176 "~{PRAS}")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.143 0 90)
			(size 1.3 1.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.2127658333)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MegaCD_Footprints:SMD_0805_HandSolder_Medium"
		(layer "B.Cu")
		(at 169.037 65.786 90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C3"
			(at 0 1.905 270)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "22nF"
			(at 0 -1.68 270)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "MegaCD.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 270)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.143 0 90)
			(size 1.3 1.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.2127658333)
			(net 5 "Net-(IC10-VCC)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.143 0 90)
			(size 1.3 1.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.2127658333)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MegaCD_Footprints:SMD_0805_HandSolder_Medium"
		(layer "B.Cu")
		(at 221.361 86.868 90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C32"
			(at 0 1.905 270)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "100pF"
			(at 0 -1.68 270)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "MegaCD.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 270)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.143 0 90)
			(size 1.3 1.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.2127658333)
			(net 132 "~{ORAS}")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.143 0 90)
			(size 1.3 1.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.2127658333)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MegaCD_Footprints:Test_Point_1.5mm"
		(layer "B.Cu")
		(at 130.7846 79.3242 180)
		(property "Reference" "M8"
			(at -0.0254 2.1082 0)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "TestPoint"
			(at 0 -2.032 0)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "MegaCD.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -3.683 0)
			(unlocked yes)
			(layer "B.Fab")
		)
		(pad "1" smd circle
			(at 0 0 180)
			(size 1.5 1.5)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 195 "VA17")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "MegaCD_Footprints:Test_Point_1.5mm"
		(layer "B.Cu")
		(at 145.288 96.901 180)
		(property "Reference" "M1"
			(at -0.4826 -2.3368 0)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "TestPoint"
			(at 0 -2.032 0)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "MegaCD.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -3.683 0)
			(unlocked yes)
			(layer "B.Fab")
		)
		(pad "1" smd circle
			(at 0 0 180)
			(size 1.5 1.5)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 64 "~{VPA}")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "MegaCD_Footprints:SMD_0805_HandSolder_Medium"
		(layer "B.Cu")
		(at 120.7262 81.9658 180)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C54"
			(at 0 1.905 0)
			(layer "B.SilkS")
		)
		(property "Value" "0"
			(at 0 -1.68 0)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "MegaCD.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.143 0 180)
			(size 1.3 1.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.2127658333)
			(net 97 "D10")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.143 0 180)
			(size 1.3 1.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.2127658333)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MegaCD_Footprints:Test_Point_1.5mm"
		(layer "B.Cu")
		(at 155.702 89.408 180)
		(property "Reference" "M2"
			(at -0.7874 1.905 0)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "TestPoint"
			(at 0 -2.032 0)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "MegaCD.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -3.683 0)
			(unlocked yes)
			(layer "B.Fab")
		)
		(pad "1" smd circle
			(at 0 0 180)
			(size 1.5 1.5)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 318 "~{IPL0}")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "MegaCD_Footprints:SMD_0805_HandSolder_Medium"
		(layer "B.Cu")
		(at 221.488 71.6495 90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C33"
			(at 0 2.032 270)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "Not used"
			(at 0 -1.68 270)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "MegaCD.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 270)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.143 0 90)
			(size 1.3 1.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.2127658333)
			(net 133 "~{OCAS}")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.143 0 90)
			(size 1.3 1.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.2127658333)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MegaCD_Footprints:SMD_0805_HandSolder_Medium"
		(layer "B.Cu")
		(at 148.59 63.119 180)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "J4"
			(at 0 1.905 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "CAS0"
			(at 0 -1.68 0)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Jumper, 2-pole, closed/bridged"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "MegaCD.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.143 0 180)
			(size 1.3 1.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.2127658333)
			(net 106 "~{CAS0}")
			(pinfunction "A")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.143 0 180)
			(size 1.3 1.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.2127658333)
			(net 106 "~{CAS0}")
			(pinfunction "B")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MegaCD_Footprints:SMD_0805_HandSolder_Medium"
		(layer "B.Cu")
		(at 193.675 70.358)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C25"
			(at 0 -1.905 180)
			(layer "B.SilkS")
		)
		(property "Value" "22nF"
			(at 0 -1.68 180)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "MegaCD.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.143 0)
			(size 1.3 1.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.2127658333)
			(net 4 "VCC2")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.143 0)
			(size 1.3 1.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.2127658333)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MegaCD_Footprints:SMD_0805_HandSolder_Medium"
		(layer "B.Cu")
		(at 225.298 78.851 90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "R4"
			(at -0.524 2.032 270)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "360"
			(at 0 -1.68 270)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "MegaCD.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 270)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.143 0 90)
			(size 1.3 1.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.2127658333)
			(net 296 "Net-(LD1-A)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.143 0 90)
			(size 1.3 1.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.2127658333)
			(net 4 "VCC2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MegaCD_Footprints:SMD_0805_HandSolder_Medium"
		(layer "B.Cu")
		(at 193.294 60.198 180)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C1"
			(at 0 -2.032 0)
			(layer "B.SilkS")
		)
		(property "Value" "1000pF"
			(at 0 -1.68 0)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "MegaCD.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.143 0 180)
			(size 1.3 1.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.2127658333)
			(net 3 "Net-(IC9-CT)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.143 0 180)
			(size 1.3 1.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.2127658333)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MegaCD_Footprints:SMD_0805_HandSolder_Medium"
		(layer "B.Cu")
		(at 214.1982 72.2884 90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C35"
			(at -4.0386 0.1778 270)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "Not used"
			(at 0 -1.68 270)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "MegaCD.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 270)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.143 0 90)
			(size 1.3 1.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.2127658333)
			(net 130 "~{ECAS}")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.143 0 90)
			(size 1.3 1.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.2127658333)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MegaCD_Footprints:SMD_0805_HandSolder_Medium"
		(layer "B.Cu")
		(at 221.361 93.853 90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C34"
			(at 0 1.905 270)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "100pF"
			(at 0 -1.68 270)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetfile "MegaCD.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 270)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.143 0 90)
			(size 1.3 1.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.2127658333)
			(net 135 "~{OWE}")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.143 0 90)
			(size 1.3 1.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.2127658333)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(gr_line
		(start 45.72 45.72)
		(end 67.72 45.72)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 234.62 45.72)
		(end 234.62 57.72)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 234.62 57.72)
		(end 234.12 57.72)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 212.1 137.72)
		(end 212.1 136.65)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 70.22 56.72)
		(end 79.97 56.72)
		(layer "Edge.Cuts")
	)
	(gr_circle
		(center 177.5968 50.597569)
		(end 179.2968 50.597569)
		(fill no)
		(layer "Edge.Cuts")
	)
	(gr_circle
		(center 63.6524 50.5968)
		(end 65.3524 50.5968)
		(fill no)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 234.12 64.72)
		(end 234.62 64.72)
		(layer "Edge.Cuts")
	)
	(gr_circle
		(center 232.05323 124.309885)
		(end 233.20323 124.309885)
		(fill no)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 159.87 46.72)
		(end 159.87 55.22)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 81.47 46.72)
		(mid 81.762893 46.012893)
		(end 82.47 45.72)
		(layer "Edge.Cuts")
	)
	(gr_circle
		(center 232.05323 91.234515)
		(end 233.20323 91.234515)
		(fill no)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 45.72 45.72)
		(end 45.72 137.72)
		(layer "Edge.Cuts")
	)
	(gr_circle
		(center 232.05323 81.28)
		(end 233.20323 81.28)
		(fill no)
		(layer "Edge.Cuts")
	)
	(gr_circle
		(center 183.5912 50.5968)
		(end 185.1912 50.5968)
		(fill no)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 172.62 55.22)
		(end 172.62 46.72)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 234.12 64.72)
		(mid 230.62 61.22)
		(end 234.12 57.72)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 196.088 130.6068)
		(end 195.1228 130.6068)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 196.088 130.6068)
		(mid 198.193698 132.753009)
		(end 196.0626 134.874)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 173.62 45.72)
		(end 234.62 45.72)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 219.202 137.7188)
		(end 234.62 137.72)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 67.72 45.72)
		(mid 68.427107 46.012893)
		(end 68.72 46.72)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 161.37 56.72)
		(mid 160.30934 56.28066)
		(end 159.87 55.22)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 229.0064 75.4888)
		(end 229.0064 77.72)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 161.37 56.72)
		(end 171.12 56.72)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 234.62 64.72)
		(end 234.62 75.4888)
		(layer "Edge.Cuts")
	)
	(gr_circle
		(center 50.6984 132.6896)
		(end 52.7984 132.6896)
		(fill no)
		(layer "Edge.Cuts")
	)
	(gr_circle
		(center 57.658 50.5968)
		(end 59.258 50.5968)
		(fill no)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 212.1 136.65)
		(mid 215.651 133.095993)
		(end 219.202 136.65)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 234.62 77.72)
		(end 229.0064 77.72)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 196.0626 134.874)
		(end 195.0974 134.874)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 45.72 137.72)
		(end 212.1 137.72)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 234.62 77.72)
		(end 234.62 137.72)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 81.47 55.22)
		(end 81.47 46.72)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 70.22 56.72)
		(mid 69.15934 56.28066)
		(end 68.72 55.22)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 219.202 137.7188)
		(end 219.202 136.65)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 172.62 55.22)
		(mid 172.18066 56.28066)
		(end 171.12 56.72)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 229.0064 75.4888)
		(end 234.62 75.4888)
		(layer "Edge.Cuts")
	)
	(gr_circle
		(center 57.658 61.1632)
		(end 61.308 61.1632)
		(fill no)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 68.72 46.72)
		(end 68.72 55.22)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 172.62 46.72)
		(mid 172.912893 46.012893)
		(end 173.62 45.72)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 82.47 45.72)
		(end 158.87 45.72)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 195.0974 134.874)
		(mid 193.012518 132.727914)
		(end 195.1228 130.6068)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 81.47 55.22)
		(mid 81.03066 56.28066)
		(end 79.97 56.72)
		(layer "Edge.Cuts")
	)
	(gr_circle
		(center 230.5812 107.7468)
		(end 232.2812 107.7468)
		(fill no)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 158.87 45.72)
		(mid 159.577107 46.012893)
		(end 159.87 46.72)
		(layer "Edge.Cuts")
	)
	(gr_circle
		(center 232.05323 134.2644)
		(end 233.20323 134.2644)
		(fill no)
		(layer "Edge.Cuts")
	)
	(image
		(at 140.081 91.2114)
		(layer "User.1")
		(scale 4)
	)
	(image
		(at 140.1572 91.5416)
		(layer "User.2")
		(scale 4)
	)
	(gr_text "MADE IN KICAD"
		(at 220.2942 62.9666 0)
		(layer "B.Cu" knockout)
	)
	(gr_text "®EPRO  2023"
		(at 221.1578 55.2958 0)
		(layer "B.Cu" knockout)
	)
	(gr_text "171-61058-01"
		(at 219.6338 52.4002 0)
		(layer "B.Cu" knockout)
	)
	(gr_text "SEGA"
		(at 153.924 82.55 0)
		(layer "F.SilkS")
	)
	(gr_text "44"
		(at 148.1074 75.4634 0)
		(layer "F.SilkS")
	)
	(gr_text "OSC"
		(at 202.2094 81.0514 0)
		(layer "F.SilkS")
	)
	(gr_text "REPRO v1.3\nBY COSAM"
		(at 222.5294 108.8136 270)
		(layer "F.SilkS")
	)
	(gr_text "837-8015-01"
		(at 162.433 89.4334 270)
		(layer "F.SilkS")
	)
	(gr_text "MAIN BD"
		(at 152.45921 95.631 270)
		(layer "F.SilkS")
	)
	(gr_text "WayWayWay"
		(at 91.8718 131.3942 0)
		(layer "F.SilkS")
	)
	(gr_text "BT"
		(at 208.4578 67.691 0)
		(layer "F.SilkS")
	)
	(gr_text "1"
		(at 188.341 81.7118 90)
		(layer "F.SilkS")
	)
	(gr_text "MCE2 ONLY"
		(at 183.769 105.664 0)
		(layer "F.SilkS")
	)
	(gr_text "IC BD MEGA-CD"
		(at 154.6606 86.995 270)
		(layer "F.SilkS")
	)
	(gr_text "68"
		(at 120.9802 86.6902 270)
		(layer "F.SilkS")
	)
	(gr_text "RED"
		(at 229.0318 87.6554 -90)
		(layer "B.SilkS")
	)
	(gr_text "GREEN"
		(at 229.0318 131.5974 -90)
		(layer "B.SilkS")
	)
	(zone
		(net 4)
		(net_name "VCC2")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 104)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 200.7362 101.2698) (xy 200.7362 100.1522) (xy 204.1906 100.1522) (xy 205.867 101.8286) (xy 205.867 102.1334)
				(xy 202.9206 102.1334) (xy 202.057 101.2698)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 38)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 102.2858 126.2634) (xy 106.1466 126.2634) (xy 106.1466 124.1806) (xy 104.013 124.1806) (xy 102.2858 125.9078)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 55)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.25)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 90.8558 83.8962) (xy 93.5482 83.8962) (xy 98.3234 88.6206) (xy 104.1146 88.6206) (xy 104.1146 91.7194)
				(xy 96.2406 91.7194) (xy 96.2406 90.1446) (xy 94.9706 88.8746) (xy 90.8558 88.8746)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 2)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 82.4738 57.531) (xy 84.8614 57.531) (xy 84.9122 64.0334) (xy 82.8294 64.0334) (xy 82.8294 60.9854)
				(xy 66.675 60.9854) (xy 66.675 54.2798) (xy 65.6082 54.2798) (xy 65.6082 55.0418) (xy 64.5922 55.0418)
				(xy 64.5922 54.2798) (xy 63.4238 54.2798) (xy 63.4238 61.0362) (xy 63.0174 61.0362) (xy 63.0174 46.4566)
				(xy 67.8942 46.4566) (xy 67.8942 55.0418) (xy 67.945 55.4482) (xy 67.9958 55.753) (xy 68.1482 56.1594)
				(xy 68.3006 56.4134) (xy 68.453 56.6674) (xy 68.6562 56.8706) (xy 68.9102 57.0738) (xy 69.1642 57.2262)
				(xy 69.5198 57.3786) (xy 69.8754 57.4802) (xy 70.3326 57.531)
			)
		)
	)
	(zone
		(net 4)
		(net_name "VCC2")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 32)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 90.8558 80.391) (xy 96.6978 80.391) (xy 98.8822 82.5754) (xy 99.7966 82.5754) (xy 99.7966 82.2706)
				(xy 100.0506 82.0166) (xy 102.5906 82.0166) (xy 104.013 80.5942) (xy 107.1118 80.5942) (xy 107.4166 80.2894)
				(xy 107.4166 78.9686) (xy 108.585 78.9686) (xy 108.585 82.3722) (xy 108.077 82.8802) (xy 104.9782 82.8802)
				(xy 104.3686 83.4898) (xy 104.3686 84.6074) (xy 105.3846 85.6234) (xy 109.601 85.6234) (xy 109.855 85.8774)
				(xy 109.855 88.4682) (xy 108.839 89.4842) (xy 107.061 89.4842) (xy 106.6546 89.8906) (xy 106.6546 92.6846)
				(xy 105.3846 92.583) (xy 105.3846 91.5162) (xy 105.029 91.1098) (xy 105.029 88.3666) (xy 104.4702 87.8078)
				(xy 98.8314 87.8078) (xy 93.9546 82.9818) (xy 90.8558 82.9818)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 49)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.25)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 90.8558 111.7854) (xy 92.6338 111.7854) (xy 92.6338 114.0714) (xy 93.0402 114.4778) (xy 93.0402 117.4242)
				(xy 90.8558 117.4242)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 11)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.25)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 209.2706 128.143) (xy 209.2706 136.9314) (xy 220.1926 136.9314) (xy 225.5774 136.9314) (xy 225.5774 131.953)
				(xy 224.0534 131.953) (xy 224.0534 124.9426) (xy 222.5294 124.9426) (xy 222.5294 127.4826) (xy 221.869 128.143)
				(xy 214.757 128.143)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 52)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.25)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 100.9142 78.5114) (xy 100.9142 79.3242) (xy 100.5078 79.7306) (xy 99.8474 79.7306) (xy 99.3394 80.2894)
				(xy 99.3394 82.169) (xy 98.933 82.169) (xy 96.7486 79.9338) (xy 90.8558 79.9338) (xy 90.8558 79.5274)
				(xy 91.8718 78.5114)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 25)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.25)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 76.6318 91.2114) (xy 81.2546 91.2114) (xy 81.2546 93.345) (xy 76.6318 93.345)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 4)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.25)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 53.0098 69.3166) (xy 53.0098 61.0362) (xy 62.8142 61.0362) (xy 62.8142 64.8462) (xy 63.3222 64.8462)
				(xy 64.6938 66.167) (xy 64.6938 66.675) (xy 62.611 66.675) (xy 62.103 67.1322) (xy 62.103 69.6722)
				(xy 61.4426 69.6722) (xy 61.4426 70.485) (xy 60.7822 71.1454) (xy 60.7822 72.7202) (xy 59.2074 72.7202)
				(xy 58.547 73.3806) (xy 58.547 75.4634) (xy 60.4266 77.2922) (xy 60.4266 80.899) (xy 57.9374 80.899)
				(xy 57.9882 84.7598) (xy 53.3654 84.7598) (xy 53.3654 87.6554) (xy 55.245 87.6554) (xy 55.245 88.3158)
				(xy 54.3306 89.2302) (xy 53.1114 89.2302) (xy 52.705 89.6366) (xy 52.705 90.805) (xy 53.1114 91.2114)
				(xy 55.9054 91.2114) (xy 55.9054 91.9734) (xy 55.245 93.091) (xy 55.245 101.3206) (xy 46.355 101.3206)
				(xy 46.355 69.3166)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 114)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 133.5786 103.251) (xy 137.1346 103.251) (xy 137.1346 103.9114) (xy 139.319 103.9114) (xy 139.319 102.9462)
				(xy 146.7358 102.9462) (xy 147.0406 103.251) (xy 148.3614 103.251) (xy 148.3614 104.1146) (xy 148.7678 104.521)
				(xy 151.6126 104.521) (xy 151.6126 105.791) (xy 152.6794 106.807) (xy 152.6794 107.569) (xy 153.2382 108.0262)
				(xy 153.2382 108.6358) (xy 153.797 109.093) (xy 155.321 109.093) (xy 157.7086 111.4806) (xy 157.7086 112.5474)
				(xy 155.8798 112.5474) (xy 155.7274 112.6998) (xy 155.7274 114.2746) (xy 155.3718 113.8682) (xy 154.305 113.8682)
				(xy 153.8986 114.2746) (xy 153.8986 113.7158) (xy 154.4574 113.2586) (xy 154.4574 112.2426) (xy 154.2034 111.9886)
				(xy 154.0002 111.9886) (xy 153.797 111.7854) (xy 152.4254 111.7854) (xy 152.0698 112.141) (xy 152.0698 113.2586)
				(xy 151.257 114.0714) (xy 151.257 115.2906) (xy 150.9014 115.5954) (xy 150.9014 116.5606) (xy 151.1046 116.7638)
				(xy 151.1046 118.1354) (xy 150.4442 118.6434) (xy 150.241 118.7958) (xy 150.241 120.0658) (xy 149.6314 120.6754)
				(xy 148.5646 120.6754) (xy 148.0058 121.2342) (xy 148.0058 122.5042) (xy 146.7866 123.7234) (xy 146.7866 125.9078)
				(xy 147.447 126.5682) (xy 147.6502 126.5682) (xy 147.6502 128.0414) (xy 146.8882 128.0414) (xy 146.1262 128.8034)
				(xy 146.1262 129.6162) (xy 146.5834 130.0226) (xy 146.9898 130.0226) (xy 146.9898 131.4958) (xy 139.6746 131.4958)
				(xy 138.557 130.3782) (xy 138.557 129.667) (xy 139.7254 129.667) (xy 140.1826 129.2098) (xy 140.1826 126.8222)
				(xy 141.4526 126.8222) (xy 142.621 127.9906) (xy 143.8402 127.9906) (xy 143.8402 128.2954) (xy 144.1958 128.7018)
				(xy 145.1102 128.7018) (xy 145.8722 127.7874) (xy 145.8722 124.4854) (xy 146.1262 124.2314) (xy 146.1262 123.1138)
				(xy 146.3802 122.8598) (xy 146.3802 121.1326) (xy 148.209 119.3038) (xy 148.209 116.967) (xy 149.0218 116.1542)
				(xy 149.0218 115.5446) (xy 150.1902 114.5286) (xy 150.495 114.5286) (xy 150.495 114.2238) (xy 151.5618 113.157)
				(xy 151.5618 111.8362) (xy 151.3078 111.5822) (xy 151.3078 109.5502) (xy 151.765 109.093) (xy 151.765 106.807)
				(xy 151.257 106.3498) (xy 145.9738 106.3498) (xy 145.9738 105.1814) (xy 144.9578 105.1814) (xy 144.6022 104.8258)
				(xy 142.5702 104.8258) (xy 142.2146 105.1814) (xy 133.5786 105.1814)
			)
		)
	)
	(zone
		(net 4)
		(net_name "VCC2")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 1)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.25)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 138.9634 79.8322) (xy 138.9634 81.1022) (xy 140.5382 82.677) (xy 141.859 82.677) (xy 142.5194 83.3374)
				(xy 142.5194 85.6234) (xy 142.5194 87.2998) (xy 142.4686 87.3506) (xy 141.4018 87.3506) (xy 140.9446 86.8934)
				(xy 140.9446 84.8614) (xy 137.4902 81.407) (xy 137.4902 79.8322) (xy 137.541 79.7814) (xy 137.9982 79.7814)
				(xy 138.049 79.8322)
			)
		)
	)
	(zone
		(net 4)
		(net_name "VCC2")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 111)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 132.8674 106.6038) (xy 132.8674 105.4862) (xy 142.5194 105.4862) (xy 142.8242 105.1814) (xy 144.2466 105.1814)
				(xy 144.5006 105.3846) (xy 145.3134 105.3846) (xy 145.5674 105.6386) (xy 145.6182 108.331) (xy 145.9738 108.6866)
				(xy 151.3078 108.6866) (xy 151.3078 109.1438) (xy 150.9522 109.4994) (xy 150.9522 110.5662) (xy 147.5486 110.5662)
				(xy 146.9898 110.0074) (xy 145.6182 110.0074) (xy 144.653 109.0422) (xy 144.653 106.6038)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 16)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.25)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 169.3926 57.5818) (xy 161.7726 57.5818) (xy 161.7726 58.3438) (xy 165.481 62.0522) (xy 169.3926 62.0522)
				(xy 181.1782 62.0522) (xy 181.1782 46.5074) (xy 173.3042 46.5074) (xy 173.3042 55.4482) (xy 173.1518 56.0578)
				(xy 172.9994 56.3626) (xy 172.7454 56.6674) (xy 172.5422 56.8706) (xy 172.085 57.2262) (xy 171.7294 57.3786)
				(xy 171.323 57.4802) (xy 170.815 57.531) (xy 170.1546 57.5818)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 37)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 82.5246 103.8098) (xy 82.5246 107.4674) (xy 83.7946 108.7374) (xy 85.217 108.7374) (xy 85.217 106.4514)
				(xy 84.6582 105.8418) (xy 84.6582 103.8098)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 87)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 176.5046 112.9538) (xy 176.5046 112.4966) (xy 176.9618 112.0394) (xy 178.3842 112.0394) (xy 178.8922 111.5314)
				(xy 179.5018 111.5314) (xy 179.5018 112.5982) (xy 178.3334 113.7666) (xy 178.0286 113.7666) (xy 178.0286 113.3094)
				(xy 177.5714 112.8522) (xy 176.6062 112.8522)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 7)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.25)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 80.9498 131.953) (xy 101.4222 131.9022) (xy 101.4222 131.5466) (xy 103.505 129.4638) (xy 105.6894 129.4638)
				(xy 107.7722 131.5466) (xy 107.7722 132.461) (xy 137.1346 132.461) (xy 138.4046 133.731) (xy 142.4178 133.731)
				(xy 142.4178 136.9822) (xy 80.9498 137.033)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 24)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.25)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 128.905 59.817) (xy 126.6698 62.0522) (xy 126.6698 66.7766) (xy 126.6698 71.1454) (xy 127.0254 71.501)
				(xy 128.8542 71.501) (xy 129.413 71.501) (xy 128.8542 70.9422) (xy 128.8542 68.453) (xy 129.159 68.1482)
				(xy 130.5306 68.1482) (xy 130.5306 67.1322) (xy 131.0894 66.5734) (xy 131.0894 59.817)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 29)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.25)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 170.815 86.6902) (xy 173.2534 86.6902) (xy 173.2534 85.5218) (xy 171.9834 84.2518) (xy 170.815 84.2518)
			)
		)
	)
	(zone
		(net 4)
		(net_name "VCC2")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 100)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 158.115 99.3394) (xy 158.115 94.4626) (xy 157.7086 94.0562) (xy 157.7086 85.8266) (xy 156.7942 84.9122)
				(xy 156.7942 77.4954) (xy 155.8798 76.581) (xy 155.8798 72.1614) (xy 157.3022 70.6882) (xy 157.3022 66.675)
				(xy 156.8958 66.2686) (xy 153.5938 66.2686) (xy 153.5938 68.0466) (xy 155.321 68.0466) (xy 156.083 68.8086)
				(xy 156.083 69.7738) (xy 155.3718 70.485) (xy 154.5082 70.485) (xy 153.9494 71.0438) (xy 153.9494 71.9582)
				(xy 153.9494 76.8858) (xy 155.321 78.2574) (xy 155.321 86.7918) (xy 156.5402 88.011) (xy 156.5402 103.4542)
				(xy 157.5054 104.4194) (xy 158.369 104.4194) (xy 158.369 103.6066) (xy 157.607 103.6066) (xy 157.607 99.3394)
			)
		)
	)
	(zone
		(net 4)
		(net_name "VCC2")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 19)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 147.2438 69.9262) (xy 151.511 69.9262) (xy 151.511 65.8622) (xy 150.2918 64.7954) (xy 146.0246 64.7954)
				(xy 146.0246 68.8086)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 17)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 202.0062 106.1974) (xy 202.0062 110.363) (xy 203.1238 110.363) (xy 203.6318 110.363) (xy 203.1238 109.855)
				(xy 203.1238 106.1974)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 3)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.25)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 63.0174 46.4566) (xy 46.355 46.4566) (xy 46.355 69.3166) (xy 51.435 69.3166) (xy 53.0098 69.3166)
				(xy 53.0098 65.5066) (xy 53.0098 61.0362) (xy 63.0174 61.0362)
			)
		)
	)
	(zone
		(net 4)
		(net_name "VCC2")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 51)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 186.3598 57.9374) (xy 189.4078 57.9374) (xy 189.4078 60.7822) (xy 186.3598 60.7822)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 54)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 190.4746 96.647) (xy 190.4746 97.0026) (xy 191.6938 98.2218) (xy 194.5386 98.2218) (xy 195.1482 98.8314)
				(xy 197.7898 98.8314) (xy 197.7898 97.8154) (xy 193.8274 97.8154) (xy 192.659 96.647)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 5)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.25)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 55.245 101.3206) (xy 46.355 101.3206) (xy 46.355 137.033) (xy 54.6862 137.033) (xy 54.6862 127.8382)
				(xy 55.245 127.3302) (xy 55.2958 124.7902) (xy 57.8866 124.7902) (xy 59.6646 123.0122) (xy 59.6646 121.4882)
				(xy 57.8866 121.4882) (xy 57.8866 122.301) (xy 55.245 122.301) (xy 55.245 119.6594) (xy 56.1594 119.6594)
				(xy 56.1594 120.4214) (xy 57.0738 120.4214) (xy 57.0738 119.6594) (xy 57.8866 119.6594) (xy 57.8866 120.4722)
				(xy 57.1246 120.4722) (xy 57.1246 121.4882) (xy 59.6646 121.4882) (xy 59.6646 120.3198) (xy 57.3278 117.7798)
				(xy 55.245 117.7798) (xy 55.245 104.8766)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 36)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 189.0522 102.1334) (xy 189.0522 101.727) (xy 190.0682 101.727) (xy 190.373 101.4222) (xy 190.9318 101.4222)
				(xy 194.3354 104.8258) (xy 194.3354 105.2322) (xy 192.151 105.2322)
			)
		)
	)
	(zone
		(net 4)
		(net_name "VCC2")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 103)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 205.613 103.0478) (xy 205.613 107.6198) (xy 208.0006 107.6198) (xy 208.0006 104.4702) (xy 206.375 103.0478)
			)
		)
	)
	(zone
		(net 4)
		(net_name "VCC2")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 43)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.25)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 129.1082 103.251) (xy 132.8674 103.251) (xy 132.8674 106.6038) (xy 129.1082 106.6038)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 33)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 80.391 87.3506) (xy 80.391 81.9658) (xy 81.7626 81.9658) (xy 81.7626 87.3506) (xy 81.7118 87.3506)
			)
		)
	)
	(zone
		(net 4)
		(net_name "VCC2")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 46)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.25)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 114.6302 88.5698) (xy 117.5766 88.5698) (xy 117.5766 88.011) (xy 116.8146 87.249) (xy 116.8146 85.5218)
				(xy 116.5606 85.2678) (xy 116.5606 75.2602) (xy 116.3066 75.2602) (xy 115.5954 75.9714) (xy 115.5954 81.7118)
				(xy 114.6302 81.7118)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 47)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 166.6494 83.5914) (xy 169.545 83.5914) (xy 169.545 81.7118) (xy 170.307 80.9498) (xy 170.307 79.9338)
				(xy 170.1038 79.7306) (xy 168.9354 79.7306) (xy 168.4782 79.2734) (xy 166.6494 79.2734)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 12)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 233.9086 128.1938) (xy 233.9086 136.9314) (xy 225.5774 136.9314) (xy 225.5774 131.953) (xy 227.3046 131.953)
				(xy 227.3046 128.1938)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 27)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.25)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 102.9462 96.5454) (xy 106.6038 96.5454) (xy 106.9086 96.901) (xy 106.9086 98.171) (xy 106.7562 98.3742)
				(xy 105.4862 98.3742) (xy 104.8766 98.3742) (xy 103.6574 97.0534) (xy 102.9462 97.0534)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 13)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.25)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 233.9086 128.1938) (xy 227.3046 128.1938) (xy 227.3046 124.333) (xy 226.5934 123.6218) (xy 226.5934 111.2774)
				(xy 233.9086 111.2774)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 40)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.25)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 201.6506 119.2022) (xy 197.0786 119.2022) (xy 197.0786 120.4722) (xy 197.5358 120.9294) (xy 200.9394 120.9294)
				(xy 202.093735 120.9294) (xy 202.1078 120.3198) (xy 203.1238 119.3546) (xy 204.2922 119.3546) (xy 205.2574 118.3894)
				(xy 206.0194 118.3894) (xy 206.5782 117.8306) (xy 206.5782 116.8654) (xy 206.883 116.5606) (xy 206.883 109.9058)
				(xy 206.3242 109.347) (xy 205.0034 109.347) (xy 205.0034 110.3122) (xy 204.7494 110.5662) (xy 204.7494 115.3922)
				(xy 204.343 115.7986) (xy 204.343 116.3574) (xy 203.7334 116.967) (xy 201.6506 116.967)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 21)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.25)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 88.8238 58.4962) (xy 87.6554 58.4962) (xy 87.2998 58.8518) (xy 87.2998 65.2018) (xy 86.4362 65.2018)
				(xy 86.4362 70.5866) (xy 86.8934 71.0438) (xy 86.8934 73.8378) (xy 87.3506 74.295) (xy 90.7542 74.295)
				(xy 90.7542 72.4662) (xy 89.8398 72.4662) (xy 89.8398 67.6402) (xy 89.8398 66.8274) (xy 89.8398 65.5066)
				(xy 88.8238 65.5066)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 15)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 181.1782 62.0522) (xy 185.1914 62.0522) (xy 185.801 61.5442) (xy 185.801 57.7342) (xy 183.6166 57.7342)
				(xy 183.6166 54.737) (xy 206.0194 54.737) (xy 206.0194 58.039) (xy 204.1906 58.039) (xy 204.1906 61.9506)
				(xy 206.0194 61.9506) (xy 206.0194 65.3034) (xy 207.2894 66.5734) (xy 207.2894 71.5518) (xy 207.645 71.9074)
				(xy 208.9658 71.9074) (xy 208.9658 71.1962) (xy 208.3054 71.1962) (xy 208.3054 70.3326) (xy 209.1182 70.3326)
				(xy 209.1182 71.3994) (xy 209.7786 71.3994) (xy 209.7786 70.3326) (xy 210.6422 70.3326) (xy 210.6422 71.1962)
				(xy 209.931 71.1962) (xy 209.931 71.9074) (xy 213.233 71.9074) (xy 213.1822 90.7034) (xy 214.8078 90.7034)
				(xy 214.8078 72.0598) (xy 215.9762 72.0598) (xy 215.9762 71.247) (xy 214.8586 71.247) (xy 214.8586 70.3834)
				(xy 217.6018 70.3834) (xy 217.6018 71.9582) (xy 224.663 71.9582) (xy 224.663 60.6806) (xy 222.631 60.6806)
				(xy 222.631 57.8866) (xy 224.7138 57.8866) (xy 224.663 51.943) (xy 224.663 46.5074) (xy 181.1782 46.5074)
			)
		)
	)
	(zone
		(net 4)
		(net_name "VCC2")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 120)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 90.8558 63.7794) (xy 93.6498 63.7794) (xy 94.1578 64.2874) (xy 94.1578 64.9478) (xy 92.9386 64.9478)
				(xy 92.583 65.3034) (xy 90.8558 65.3034)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 42)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 177.2666 124.6886) (xy 174.625 124.6886) (xy 174.625 122.7074) (xy 175.0314 122.301) (xy 176.8094 122.301)
				(xy 177.165 121.9454) (xy 183.2102 121.9454) (xy 183.2102 120.1674) (xy 180.975 120.1674) (xy 180.213 119.4054)
				(xy 177.927 119.4054) (xy 176.5046 120.8278) (xy 176.5046 121.1834) (xy 175.9966 121.6914) (xy 175.0314 121.6914)
				(xy 174.0662 122.6566) (xy 174.0662 124.9934) (xy 174.4218 125.349) (xy 174.4218 126.0094) (xy 173.9138 126.5174)
				(xy 173.9138 127.0254) (xy 173.4058 127.5334) (xy 173.4058 128.6002) (xy 174.3202 129.5146) (xy 174.5742 129.5146)
				(xy 174.5742 128.2954) (xy 177.2666 128.2954)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 10)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.25)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 183.9722 128.4478) (xy 184.7342 128.4478) (xy 184.7342 127.2286) (xy 184.9374 127.2286) (xy 184.9374 127.4826)
				(xy 185.801 127.4826) (xy 185.801 127.2286) (xy 186.0042 127.2286) (xy 186.0042 128.4478) (xy 189.1538 128.4478)
				(xy 189.1538 126.7714) (xy 191.9986 126.7714) (xy 193.2686 128.0414) (xy 198.0438 128.0414) (xy 200.5838 130.5814)
				(xy 200.5838 136.9314) (xy 209.2706 136.9314) (xy 209.2706 128.143) (xy 206.3242 128.143) (xy 206.3242 126.619)
				(xy 207.645 126.619) (xy 207.645 125.6538) (xy 206.2734 125.6538) (xy 206.2734 124.9426) (xy 193.0146 124.9426)
				(xy 192.3034 124.2314) (xy 189.103 124.2314) (xy 188.0362 125.5522) (xy 185.3438 125.5522) (xy 184.9374 125.1458)
				(xy 184.4294 125.1458) (xy 183.9722 125.5522)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 31)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 119.4054 73.8886) (xy 121.539 73.8886) (xy 121.539 76.7842) (xy 121.0818 77.2414) (xy 121.0818 82.0166)
				(xy 121.0818 88.6714) (xy 120.3198 89.3318) (xy 120.3198 95.7834) (xy 119.3038 96.7994) (xy 117.6782 96.7994)
				(xy 116.1034 98.3742) (xy 116.1034 99.6442) (xy 111.5822 99.6442) (xy 111.5822 96.901) (xy 115.951 96.901)
				(xy 118.1354 94.7166) (xy 118.1354 88.1634) (xy 119.4054 86.8934)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 116)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.05)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 98.5266 127.5842) (xy 98.5266 124.1806) (xy 98.9838 123.7234) (xy 99.9998 123.7234) (xy 99.9998 127.0254)
				(xy 99.441 127.5842)
			)
		)
	)
	(zone
		(net 4)
		(net_name "VCC2")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 121)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 118.618 73.914) (xy 118.618 74.041) (xy 118.618 74.803) (xy 115.824 74.803) (xy 115.824 73.66)
				(xy 118.364 73.66)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 117)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.05)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 92.1258 125.5014) (xy 92.1258 127.5842) (xy 83.2866 127.5842) (xy 82.3722 126.6698) (xy 82.3722 125.5014)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 53)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 182.4482 66.7258) (xy 183.4134 65.7606) (xy 183.4134 65.0494) (xy 185.2422 65.0494) (xy 185.2422 65.7606)
				(xy 185.801 66.3194) (xy 186.8678 66.3194) (xy 187.071 66.1162) (xy 187.8838 66.1162) (xy 188.7982 65.3034)
				(xy 192.2526 65.3034) (xy 192.8622 65.3034) (xy 193.3702 65.3034) (xy 194.0306 65.3034) (xy 198.8566 65.3034)
				(xy 198.8566 66.7258) (xy 200.025 67.8942) (xy 201.5998 67.8942) (xy 201.5998 69.8754) (xy 203.581 71.8566)
				(xy 203.581 75.3618) (xy 201.6506 75.3618) (xy 201.6506 78.105) (xy 203.5302 78.105) (xy 203.5302 78.8162)
				(xy 189.1538 78.8162) (xy 189.1538 75.311) (xy 186.563 75.311) (xy 186.563 71.0946) (xy 185.801 70.3326)
				(xy 185.801 66.9798) (xy 184.6326 66.9798) (xy 184.1246 67.4878) (xy 182.4482 67.4878)
			)
		)
	)
	(zone
		(net 4)
		(net_name "VCC2")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 97)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 165.3794 109.4486) (xy 165.3794 110.0074) (xy 163.1442 110.0074) (xy 158.7246 105.5878) (xy 160.0454 105.5878)
				(xy 160.0454 104.4194) (xy 159.0802 104.4194) (xy 159.0802 103.6066) (xy 160.2486 103.6066) (xy 160.655 103.9622)
				(xy 160.655 105.791) (xy 164.3126 109.4486)
			)
		)
	)
	(zone
		(net 4)
		(net_name "VCC2")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 44)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.25)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 130.2258 94.2086) (xy 128.5494 95.885) (xy 128.5494 99.3394) (xy 132.8674 99.3394) (xy 132.8674 94.5642)
				(xy 132.2578 93.853) (xy 132.2578 94.2086)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 8)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.25)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 142.4178 133.731) (xy 171.323 133.731) (xy 171.323 136.9822) (xy 142.4178 136.9822)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 96)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 165.4302 108.2802) (xy 165.4302 108.7882) (xy 165.6334 108.9914) (xy 165.6334 109.093) (xy 164.465 109.093)
				(xy 161.0106 105.6386) (xy 161.0106 103.759) (xy 160.147 102.8954) (xy 160.147 99.949) (xy 159.5374 99.3394)
				(xy 158.4706 99.3394) (xy 158.4706 94.361) (xy 158.0642 93.9546) (xy 158.0642 85.5218) (xy 157.099 84.5566)
				(xy 157.099 77.2414) (xy 156.1846 76.327) (xy 156.083 72.4154) (xy 157.6578 70.8406) (xy 157.6578 66.6242)
				(xy 158.9278 65.3542) (xy 161.0106 65.3542) (xy 161.0106 69.1134) (xy 159.2834 70.6374) (xy 159.2834 70.993)
				(xy 159.0294 71.247) (xy 159.0294 71.5518) (xy 157.4546 73.1266) (xy 157.4546 75.057) (xy 158.2166 75.819)
				(xy 158.2166 78.5622) (xy 158.9786 79.3242) (xy 158.9786 80.137) (xy 159.3342 80.4926) (xy 159.3342 90.0938)
				(xy 160.147 90.9066) (xy 160.147 98.8314) (xy 161.5694 100.2538) (xy 161.5694 102.5398) (xy 162.6362 103.6066)
				(xy 162.687 105.537)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 30)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 127.9906 73.6346) (xy 127.9906 74.3458) (xy 128.2446 74.5998) (xy 129.2606 74.5998) (xy 130.1242 75.4634)
				(xy 132.715 75.4634) (xy 133.0706 75.1078) (xy 133.0706 74.7014) (xy 132.6642 74.295) (xy 130.8354 74.295)
				(xy 130.2258 73.6346)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 99)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 181.1274 110.7694) (xy 181.1274 111.887) (xy 183.261 111.887) (xy 183.9214 112.4966) (xy 183.9214 113.4618)
				(xy 184.4294 113.4618) (xy 184.4294 111.2266) (xy 185.0898 110.5662) (xy 185.7502 110.5662) (xy 186.2582 111.0742)
				(xy 186.2582 112.1918) (xy 187.1218 112.1918) (xy 189.4586 114.2746) (xy 189.5094 114.2746) (xy 189.5094 112.5474)
				(xy 186.817 109.855) (xy 186.817 107.7214) (xy 186.5122 107.4166) (xy 186.5122 106.6038) (xy 186.7154 106.4006)
				(xy 187.9346 106.4006) (xy 188.1886 106.6546) (xy 188.1886 107.6198) (xy 189.103 108.5342) (xy 189.103 109.601)
				(xy 192.659 113.157) (xy 193.0146 113.157) (xy 193.0146 115.3922) (xy 197.6882 115.3922) (xy 197.6882 111.0234)
				(xy 197.0278 111.0234) (xy 196.3166 111.7346) (xy 196.3166 112.2426) (xy 194.3354 112.2426) (xy 192.6082 110.5154)
				(xy 191.643 110.5154) (xy 190.881 109.7534) (xy 190.881 107.0102) (xy 189.2046 105.3338) (xy 187.7822 105.3338)
				(xy 187.7822 103.505) (xy 184.3278 103.505) (xy 184.3278 109.2454) (xy 182.7022 110.7694)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 18)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 64.6938 66.675) (xy 64.6938 69.215) (xy 64.0334 69.8754) (xy 64.0334 70.8914) (xy 63.5254 71.4502)
				(xy 63.5254 87.9602) (xy 62.2046 87.9602) (xy 62.2046 71.1454) (xy 63.1698 70.1802) (xy 63.1698 68.6054)
				(xy 64.0334 67.7418) (xy 64.0334 66.929) (xy 63.8302 66.675)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 6)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.25)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 59.6646 123.0122) (xy 57.8866 124.7902) (xy 57.8866 127.381) (xy 55.245 127.3302) (xy 54.6862 127.8382)
				(xy 54.6862 129.921) (xy 58.4962 129.921) (xy 58.4962 133.7818) (xy 54.6862 133.7818) (xy 54.6862 137.033)
				(xy 80.9498 137.033) (xy 80.9498 131.953) (xy 80.6958 131.953) (xy 74.803 126.111) (xy 65.5066 126.111)
				(xy 65.5066 126.9746) (xy 63.4746 129.0066) (xy 59.7154 129.0066)
			)
		)
	)
	(zone
		(net 4)
		(net_name "VCC2")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 48)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 196.6214 57.9374) (xy 202.9714 57.9374) (xy 202.9714 61.7982) (xy 199.7202 61.7982) (xy 199.7202 60.0202)
				(xy 199.2122 59.5122) (xy 198.3486 59.5122) (xy 197.8406 60.0202) (xy 197.8406 61.4934) (xy 196.469 61.4934)
				(xy 196.469 64.897) (xy 194.2338 64.897) (xy 194.2338 61.5442) (xy 194.0814 61.3918) (xy 193.7258 61.3918)
				(xy 192.9638 60.6298) (xy 192.9638 60.1218) (xy 191.7954 60.1218) (xy 191.0842 59.4106) (xy 192.913 59.4106)
				(xy 192.913 59.1566) (xy 194.8434 59.1566) (xy 195.3514 59.6646) (xy 196.0118 59.6646) (xy 196.6214 59.055)
			)
		)
	)
	(zone
		(net 4)
		(net_name "VCC2")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 41)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 177.7746 124.6886) (xy 177.7746 128.2954) (xy 180.5178 128.2954) (xy 180.5686 130.3782) (xy 180.0606 130.8862)
				(xy 177.7746 130.8862) (xy 177.7746 131.8006) (xy 179.6542 131.8006) (xy 181.4322 130.0226) (xy 181.4322 122.4534)
				(xy 180.5178 122.4534) (xy 180.5178 124.6886)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 23)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.25)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 102.6922 72.1614) (xy 102.6922 74.295) (xy 100.2538 74.295) (xy 99.8982 73.9394) (xy 99.8982 73.279)
				(xy 99.3902 72.771) (xy 99.3902 70.7898) (xy 99.9998 70.7898) (xy 101.3714 72.1614)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 50)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.25)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 96.5454 114.173) (xy 96.901 114.173) (xy 96.901 112.1918) (xy 98.8822 112.1918) (xy 100.1522 110.9218)
				(xy 100.3046 110.9218) (xy 101.5238 112.141) (xy 101.5238 113.2586) (xy 99.1362 113.2586) (xy 98.679 113.7158)
				(xy 98.679 115.5446) (xy 99.441 116.3066) (xy 99.6442 116.3066) (xy 100.8126 117.475) (xy 100.8126 117.6274)
				(xy 100.6094 117.4242) (xy 96.5454 117.4242)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 110)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 122.7074 118.2878) (xy 132.3594 118.2878) (xy 132.3594 119.1006) (xy 133.0198 119.761) (xy 133.5786 119.761)
				(xy 133.5786 121.9962) (xy 136.3218 121.9962) (xy 136.3218 123.063) (xy 136.0678 123.3678) (xy 133.8326 123.3678)
				(xy 132.7658 122.301) (xy 132.7658 121.539) (xy 132.3086 121.031) (xy 130.8354 121.031) (xy 130.8354 122.3518)
				(xy 131.3942 122.9106) (xy 131.953 122.9106) (xy 133.3246 124.2822) (xy 133.3246 124.7902) (xy 131.2418 124.7902)
				(xy 129.6162 123.317) (xy 129.6162 120.9294) (xy 128.2954 120.9294) (xy 128.2954 120.269) (xy 128.0922 120.015)
				(xy 125.7554 120.015) (xy 125.3998 120.3198) (xy 125.3998 121.1326) (xy 125.603 121.3866) (xy 126.1618 121.3866)
				(xy 126.1618 122.047) (xy 125.6538 122.047) (xy 125.1458 122.555) (xy 125.1458 122.3518) (xy 124.6378 121.8438)
				(xy 124.6378 120.0658) (xy 124.2314 119.6594) (xy 122.7074 119.6594)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 28)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.25)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 110.4138 96.9518) (xy 115.7986 96.9518) (xy 115.7986 98.1202) (xy 114.935 98.9838) (xy 114.935 99.6442)
				(xy 110.8202 99.6442) (xy 110.5662 99.3902) (xy 108.585 99.3902) (xy 108.585 98.171) (xy 109.8042 96.9518)
			)
		)
	)
	(zone
		(net 4)
		(net_name "VCC2")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 45)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.25)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 130.7338 86.1314) (xy 130.7338 88.3158) (xy 130.7846 88.3666) (xy 132.461 88.3666) (xy 132.969 88.9254)
				(xy 132.969 89.535) (xy 130.4798 89.535) (xy 129.6162 88.6714) (xy 129.6162 86.995) (xy 129.8702 86.741)
				(xy 129.8702 86.1314)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 34)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 100.1522 110.9218) (xy 100.6094 110.4646) (xy 100.6094 106.1974) (xy 99.5426 105.283) (xy 98.933 105.283)
				(xy 98.5774 104.9274) (xy 98.5774 104.4702) (xy 99.0854 103.9622) (xy 100.965 103.9622) (xy 100.965 104.9782)
				(xy 101.6254 105.6386) (xy 101.6254 106.6038) (xy 101.9302 106.9086) (xy 103.9114 106.9086) (xy 104.5718 106.2482)
				(xy 104.5718 104.5718) (xy 105.6386 104.5718) (xy 107.0102 105.9434) (xy 107.0102 107.9754) (xy 104.9274 110.0582)
				(xy 104.9274 111.1758) (xy 103.3526 111.1758) (xy 102.743 111.7854) (xy 102.743 113.2586) (xy 100.1522 113.2586)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 20)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.25)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 224.663 46.5074) (xy 224.663 48.0314) (xy 228.5238 48.0314) (xy 228.5238 51.943) (xy 224.663 51.943)
				(xy 224.7138 57.8866) (xy 228.2698 57.8866) (xy 228.219 60.6806) (xy 224.663 60.6806) (xy 224.663 70.2818)
				(xy 220.091 70.2818) (xy 220.091 76.2254) (xy 221.0562 77.0382) (xy 221.0562 85.0138) (xy 221.9198 85.8774)
				(xy 222.1738 85.8774) (xy 224.409 83.6422) (xy 227.2538 83.6422) (xy 227.2538 87.1982) (xy 233.9086 87.1982)
				(xy 233.9086 78.613) (xy 229.743 78.613) (xy 228.473 78.613) (xy 228.473 74.803) (xy 233.9086 74.803)
				(xy 233.9086 56.7182) (xy 233.9086 46.5074)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 22)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.25)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 98.425 64.6938) (xy 97.663 64.6938) (xy 97.663 68.1482) (xy 98.1202 68.5546) (xy 99.9998 68.5546)
				(xy 99.9998 67.2846) (xy 101.5238 65.7606) (xy 101.5238 60.071) (xy 100.3046 58.8518) (xy 96.393 58.8518)
				(xy 95.123 60.1218) (xy 95.123 60.7314) (xy 96.4438 60.7314) (xy 96.4438 60.1218) (xy 96.647 59.8678)
				(xy 97.7646 59.8678) (xy 98.0694 60.1726) (xy 98.0694 60.7314) (xy 99.3902 60.7314) (xy 99.3902 63.7286)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 107)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 201.2442 94.0054) (xy 202.565 92.6846) (xy 203.7842 92.6846) (xy 204.2414 93.091) (xy 204.2414 95.2246)
				(xy 204.597 95.5802) (xy 206.3242 95.5802) (xy 206.3242 97.4598) (xy 205.613 98.171) (xy 204.597 98.171)
				(xy 203.835 98.933) (xy 203.3778 98.933) (xy 203.3778 98.679) (xy 203.7334 98.3742) (xy 203.7334 97.5614)
				(xy 203.1746 97.0026) (xy 201.2442 97.0026)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 35)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 106.7562 117.5766) (xy 106.7562 115.951) (xy 108.331 114.5286) (xy 108.331 112.903) (xy 109.9566 112.903)
				(xy 109.9566 116.3574) (xy 109.347 116.967) (xy 109.347 117.5766)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 26)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.25)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 90.1446 99.695) (xy 90.1446 96.5962) (xy 86.0298 96.5962) (xy 86.0298 90.551) (xy 83.185 90.551)
				(xy 83.185 91.1606) (xy 84.0994 92.075) (xy 84.5566 92.075) (xy 84.8614 92.3798) (xy 84.8614 94.615)
				(xy 84.5566 94.9706) (xy 84.5566 99.695)
			)
		)
	)
	(zone
		(net 4)
		(net_name "VCC2")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 56)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 197.8406 101.727) (xy 194.2338 101.727) (xy 192.5574 100.0506) (xy 192.5574 99.8474) (xy 193.4718 99.8474)
				(xy 194.7926 101.1682) (xy 197.8406 101.1682)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 14)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.25)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 233.9086 111.2774) (xy 222.5802 111.2774) (xy 222.5802 109.2454) (xy 222.0214 108.6866) (xy 222.0214 106.3498)
				(xy 222.5802 105.791) (xy 222.5802 92.9386) (xy 224.1042 91.4146) (xy 224.1042 88.8746) (xy 227.2538 88.8746)
				(xy 227.2538 87.1982) (xy 233.9086 87.1982)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 115)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 139.8778 121.793) (xy 139.8778 123.063) (xy 140.589 123.7742) (xy 140.589 124.6378) (xy 139.7254 124.6378)
				(xy 138.2522 123.1646) (xy 138.2522 122.047) (xy 138.5062 121.793)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "F.Cu")
		(hatch edge 0.5)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.25)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 127.0254 79.5274) (xy 130.8862 79.5274) (xy 130.8862 80.899) (xy 131.2926 80.899) (xy 131.2926 81.8642)
				(xy 132.5626 81.8642) (xy 136.8806 86.1822) (xy 136.8806 87.757) (xy 135.8138 88.7222) (xy 135.8138 91.313)
				(xy 136.779 92.2782) (xy 141.859 92.2782) (xy 141.859 93.3958) (xy 140.8938 94.361) (xy 140.2842 94.361)
				(xy 139.9794 94.6658) (xy 139.9794 95.631) (xy 136.4742 99.1362) (xy 133.6802 99.1362) (xy 133.6802 95.2754)
				(xy 134.2898 94.6658) (xy 134.2898 89.3318) (xy 132.9182 87.9602) (xy 131.1402 87.9602) (xy 131.1402 85.7758)
				(xy 128.905 85.7758) (xy 127.9398 84.8106) (xy 127.0254 84.8106)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 108)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 196.0118 87.503) (xy 192.5066 87.503) (xy 192.5066 88.6206) (xy 191.135 88.6206) (xy 190.7286 88.2142)
				(xy 190.7286 87.503) (xy 189.5602 87.503) (xy 189.5602 87.6554) (xy 189.8142 87.9094) (xy 189.8142 89.4842)
				(xy 189.103 90.1954) (xy 188.8998 90.1954) (xy 185.7502 93.345) (xy 183.7182 93.345) (xy 182.8546 94.2086)
				(xy 182.8546 97.917) (xy 179.0446 101.727) (xy 179.0446 103.251) (xy 179.8066 104.013) (xy 182.9054 104.013)
				(xy 182.9054 103.0478) (xy 185.547 100.4062) (xy 185.547 95.631) (xy 186.6138 94.5642) (xy 189.865 94.5642)
				(xy 190.2206 94.9198) (xy 192.151 94.9198) (xy 192.151 92.7862) (xy 194.437 90.5002) (xy 196.0118 90.5002)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 39)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 115.951 102.7938) (xy 115.951 105.3338) (xy 114.6302 106.6546) (xy 114.6302 109.6518) (xy 115.3414 109.6518)
				(xy 115.8494 110.1598) (xy 115.8494 117.729) (xy 117.8814 117.729) (xy 117.8814 107.1626) (xy 117.2718 106.553)
				(xy 117.2718 105.029) (xy 117.7798 104.521) (xy 118.237 104.521) (xy 118.237 102.3874) (xy 117.8814 102.0318)
				(xy 116.713 102.0318)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 9)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.25)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 171.323 133.731) (xy 181.0766 133.731) (xy 183.9722 130.8354) (xy 183.9722 128.4478) (xy 184.7342 128.4478)
				(xy 184.7342 128.8542) (xy 186.0042 128.8542) (xy 186.0042 128.4478) (xy 189.1538 128.4478) (xy 189.1538 129.3114)
				(xy 190.4238 129.3114) (xy 190.4238 136.9822) (xy 171.323 136.9822)
			)
		)
	)
	(zone
		(net 4)
		(net_name "VCC2")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 123)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 142.2654 105.9434) (xy 144.2466 105.9434) (xy 145.2626 104.9274) (xy 149.2758 104.9274) (xy 149.733 104.4702)
				(xy 159.8422 104.4702) (xy 163.449 100.9142) (xy 163.449 100.711) (xy 169.9514 100.711) (xy 170.1038 100.6094)
				(xy 179.959 100.6094) (xy 182.8038 97.7646) (xy 184.023 97.7646) (xy 186.7154 95.0722) (xy 189.2554 95.0722)
				(xy 189.2554 93.7514) (xy 189.4586 93.5482) (xy 190.5254 93.5482) (xy 190.5254 92.5322) (xy 188.0362 92.5322)
				(xy 186.1566 94.4118) (xy 184.6326 94.4118) (xy 184.6326 95.3262) (xy 183.5658 96.393) (xy 182.3466 96.393)
				(xy 179.4002 99.3394) (xy 173.5074 99.3394) (xy 173.2026 99.6442) (xy 163.4998 99.6442) (xy 163.4998 99.3902)
				(xy 163.2458 99.1362) (xy 161.3154 99.1362) (xy 161.3154 101.3714) (xy 157.099 101.3714) (xy 155.2194 103.251)
				(xy 149.0726 103.251) (xy 148.4122 103.9114) (xy 142.2654 103.9114)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 148)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.25)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 151.4602 105.3846) (xy 151.4602 108.331) (xy 153.1874 108.331) (xy 153.1874 107.4166) (xy 154.4574 107.4166)
				(xy 154.9146 107.8738) (xy 163.3982 107.8738) (xy 165.4302 105.8418) (xy 165.4302 105.029) (xy 165.1254 104.7242)
				(xy 165.1254 103.8606) (xy 165.5318 103.4542) (xy 166.497 103.4542) (xy 166.9542 103.9622) (xy 167.767 103.9622)
				(xy 168.3258 103.4034) (xy 173.0502 103.4034) (xy 174.4726 101.981) (xy 180.721 101.981) (xy 183.515 99.187)
				(xy 183.9722 99.187) (xy 184.2262 98.9838) (xy 184.2262 98.5266) (xy 183.8198 98.1202) (xy 183.1086 98.1202)
				(xy 180.2638 100.965) (xy 173.9646 100.965) (xy 172.6946 102.3874) (xy 170.0022 102.3874) (xy 169.4942 101.8794)
				(xy 164.0586 101.8794) (xy 160.5534 105.3846)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 79)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 224.5614 131.6482) (xy 224.5614 131.953) (xy 228.473 131.953) (xy 228.473 135.6614) (xy 226.441 135.6614)
				(xy 226.441 136.9314) (xy 229.3366 136.9314) (xy 229.3366 131.6482)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 62)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 82.9818 98.933) (xy 82.9818 98.3234) (xy 70.485 98.3234) (xy 68.961 99.8982) (xy 65.5066 99.8982)
				(xy 65.5066 102.489) (xy 63.2714 102.489) (xy 63.2714 107.6706) (xy 79.2734 107.6706) (xy 80.3402 106.6038)
				(xy 84.1502 106.6038) (xy 84.455 106.299) (xy 84.455 104.4702) (xy 83.7946 103.759) (xy 67.9958 103.759)
				(xy 67.7926 103.5558) (xy 67.7926 102.1842) (xy 69.0118 102.1842) (xy 69.9262 101.2698) (xy 71.8566 101.2698)
				(xy 72.8218 100.3046) (xy 75.7174 100.3046) (xy 76.1238 99.8982) (xy 77.9526 99.8982) (xy 78.4606 100.4062)
				(xy 78.4606 100.7618) (xy 78.867 101.1682) (xy 81.4578 101.1682) (xy 81.4578 100.457)
			)
		)
	)
	(zone
		(net 4)
		(net_name "VCC2")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 94)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.25)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 58.4454 119.6086) (xy 58.4454 117.7798) (xy 59.055 117.7798) (xy 61.0362 115.7986) (xy 61.0362 110.0074)
				(xy 62.9158 108.1278) (xy 79.8322 108.1278) (xy 80.9498 107.0102) (xy 84.5058 107.0102) (xy 85.4202 107.0102)
				(xy 86.6902 107.0102) (xy 88.2142 108.5342) (xy 88.2142 109.4994) (xy 86.3854 109.4994) (xy 86.3854 111.0742)
				(xy 85.4202 111.0742) (xy 84.1502 109.8042) (xy 81.6102 109.8042) (xy 80.391 111.0234) (xy 68.3006 111.0234)
				(xy 66.675 112.649) (xy 65.4558 112.649) (xy 65.4558 110.7186) (xy 62.8142 110.7186) (xy 62.8142 115.8494)
				(xy 59.055 119.6086)
			)
		)
	)
	(zone
		(net 4)
		(net_name "VCC2")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 143)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.25)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 190.5254 92.5322) (xy 190.5254 93.5482) (xy 191.0334 93.5482) (xy 192.1002 94.615) (xy 192.1002 95.6818)
				(xy 192.7098 96.2914) (xy 192.7098 103.6066) (xy 199.3646 103.6066) (xy 202.4634 100.5078) (xy 202.4634 99.8474)
				(xy 202.1078 99.4918) (xy 202.1078 97.3074) (xy 202.3618 97.0534) (xy 203.2254 97.0534) (xy 203.4794 96.7994)
				(xy 203.4794 93.091) (xy 206.121 90.4494) (xy 206.121 86.233) (xy 207.2894 85.0646) (xy 208.1022 85.0646)
				(xy 208.1022 82.9818) (xy 205.5114 82.9818) (xy 204.1906 84.3026) (xy 204.1906 89.8906) (xy 202.5142 91.567)
				(xy 202.5142 95.2246) (xy 202.2094 95.5294) (xy 199.517 95.5294) (xy 199.517 91.7702) (xy 197.0278 91.7702)
				(xy 196.5198 91.2622) (xy 196.5198 88.3158) (xy 198.8058 88.3158) (xy 198.8058 86.233) (xy 196.1134 86.233)
				(xy 195.3006 87.0458) (xy 195.3006 88.8746) (xy 192.151 88.8746) (xy 192.151 86.8426) (xy 191.4398 86.1314)
				(xy 174.6758 86.1822) (xy 174.5234 86.3346) (xy 174.5234 88.0618) (xy 179.8574 88.0618) (xy 180.5686 87.249)
				(xy 183.5658 87.249) (xy 184.2262 87.9094) (xy 184.2262 88.1126) (xy 184.4802 88.3666) (xy 185.1914 88.3666)
				(xy 186.4106 87.1474) (xy 188.0362 87.1474) (xy 188.341 87.4522) (xy 189.5602 87.4522) (xy 189.8142 87.7062)
				(xy 189.8142 90.7542) (xy 193.4718 90.7542) (xy 194.7926 92.075) (xy 195.2498 92.075) (xy 195.4022 92.2274)
				(xy 195.4022 92.6846) (xy 196.9262 94.2086) (xy 196.9262 96.8502) (xy 193.8274 96.8502) (xy 193.8274 95.8342)
				(xy 193.3194 95.2754) (xy 193.3194 94.4626) (xy 191.389 92.5322)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 73)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 52.705 104.3686) (xy 46.4058 104.3686) (xy 46.355 132.1054) (xy 59.6646 132.1054) (xy 52.705 125.095)
				(xy 52.705 112.8014)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 58)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 132.969 96.647) (xy 133.2738 96.3422) (xy 134.1374 96.3422) (xy 135.255 97.4598) (xy 135.255 98.5266)
				(xy 136.0678 99.3394) (xy 136.0678 99.695) (xy 135.255 99.695) (xy 134.9248 100.0506) (xy 124.8918 100.0506)
				(xy 122.9106 98.0694) (xy 115.2652 98.0694) (xy 114.7318 98.6282) (xy 114.7318 100.7618) (xy 116.6114 102.6414)
				(xy 116.6114 104.3178) (xy 116.1034 104.8258) (xy 112.141 104.8258) (xy 110.9218 106.045) (xy 105.791 106.045)
				(xy 105.3846 105.6386) (xy 105.3846 105.283) (xy 113.8682 96.8248) (xy 124.3584 96.8248) (xy 125.0442 97.5106)
				(xy 132.715 97.5106) (xy 132.969 97.2566)
			)
		)
	)
	(zone
		(net 4)
		(net_name "VCC2")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 83)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.25)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 222.885 74.1934) (xy 222.885 69.0626) (xy 217.8558 69.0626) (xy 217.1954 68.4022) (xy 217.1954 65.2526)
				(xy 226.6442 65.2526) (xy 226.6442 74.1934)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 147)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.25)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 99.6442 74.803) (xy 99.6442 73.0758) (xy 98.2726 71.8566) (xy 96.139 71.8566) (xy 95.2754 70.993)
				(xy 87.9602 70.993) (xy 86.5886 69.6214) (xy 76.8858 69.6214) (xy 76.0222 68.7578) (xy 74.3458 68.7578)
				(xy 74.041 68.453) (xy 73.1266 68.453) (xy 72.2122 69.3674) (xy 69.2658 69.3674) (xy 68.8594 69.7738)
				(xy 67.5894 69.7738) (xy 67.2338 70.1294) (xy 65.659 70.1294) (xy 65.0494 70.739) (xy 65.0494 72.1614)
				(xy 59.563 72.1614) (xy 59.563 72.517) (xy 58.6486 73.4314) (xy 58.6486 74.549) (xy 60.325 74.549)
				(xy 60.579 74.295) (xy 61.595 74.295) (xy 62.611 73.279) (xy 66.2178 73.279) (xy 67.183 72.3138)
				(xy 83.6422 72.3138) (xy 85.1662 73.8378) (xy 86.3854 73.8378) (xy 86.8426 73.3806) (xy 89.027 73.3806)
				(xy 89.027 75.4634) (xy 66.4718 75.4634) (xy 62.3062 79.629) (xy 58.9534 79.629) (xy 58.9534 77.9018)
				(xy 54.6354 77.9018) (xy 54.6354 72.009) (xy 55.9054 70.739) (xy 61.849 70.739) (xy 62.865 69.723)
				(xy 62.865 68.8086) (xy 65.3542 66.3194) (xy 74.4474 66.3194) (xy 74.4474 66.7766) (xy 74.803 67.183)
				(xy 75.9714 67.183) (xy 76.327 66.8274) (xy 81.407 66.8274) (xy 82.8294 68.2498) (xy 84.709 68.2498)
				(xy 86.5886 66.3702) (xy 90.5002 66.3702) (xy 91.1606 67.0306) (xy 94.0054 67.0306) (xy 94.0054 67.7418)
				(xy 94.9198 68.6562) (xy 99.441 68.6562) (xy 99.441 70.9422) (xy 100.5586 72.0598) (xy 100.5586 74.803)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 146)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.25)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 112.1918 82.1182) (xy 114.173 82.1182) (xy 114.173 80.137) (xy 114.4778 79.7814) (xy 115.443 79.7814)
				(xy 115.7478 80.0862) (xy 115.7478 82.423) (xy 118.1354 82.423) (xy 118.1354 80.8482) (xy 129.3114 80.8482)
				(xy 129.3114 78.7146) (xy 113.919 78.7146) (xy 112.1918 78.7146)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 139)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.25)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 213.0806 74.7522) (xy 213.0806 83.5406) (xy 215.3666 83.5406) (xy 215.3666 83.2358) (xy 216.5858 83.2358)
				(xy 216.5858 82.8802) (xy 215.3666 82.8802) (xy 215.3666 78.1558) (xy 216.5858 78.1558) (xy 216.5858 77.7494)
				(xy 215.3666 77.7494) (xy 215.3666 75.6158) (xy 216.4842 75.6158) (xy 216.4842 75.2094) (xy 215.3666 75.2094)
				(xy 215.3666 74.7522)
			)
		)
	)
	(zone
		(net 4)
		(net_name "VCC2")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 106)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.25)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 116.8146 73.8886) (xy 116.8146 75.8698) (xy 134.3914 75.8698) (xy 134.6962 75.565) (xy 136.9314 75.565)
				(xy 137.5918 76.2254) (xy 137.5918 80.9498) (xy 139.065 80.9498) (xy 139.065 77.3938) (xy 146.1262 77.3938)
				(xy 147.3454 76.1746) (xy 151.3078 76.1746) (xy 151.765 75.7174) (xy 151.765 73.8886) (xy 144.399 73.8886)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 72)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 46.355 65.3542) (xy 51.1302 65.3542) (xy 51.1302 93.2434) (xy 52.705 94.8182) (xy 52.705 104.3686)
				(xy 46.4058 104.3686)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 132)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 196.215 117.7798) (xy 201.0918 117.7798) (xy 201.4982 117.3734) (xy 204.851 117.3734) (xy 205.2066 117.729)
				(xy 205.2066 118.3386) (xy 204.1398 119.253) (xy 202.819 119.253) (xy 202.0062 120.0658) (xy 199.263 120.0658)
				(xy 196.977 122.3518) (xy 190.9826 122.3518) (xy 189.6618 121.031) (xy 188.9506 121.031) (xy 188.6458 120.7262)
				(xy 188.6458 119.1006) (xy 191.4398 116.3066) (xy 191.4398 115.189) (xy 191.7446 114.8842) (xy 192.3034 114.8842)
				(xy 192.659 114.5286) (xy 192.659 112.8014) (xy 193.0654 112.395) (xy 195.3514 112.395) (xy 195.5546 112.5982)
				(xy 195.5546 117.1194)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 125)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 155.829 126.0094) (xy 147.3454 126.0094) (xy 147.1422 126.2126) (xy 147.1422 127.8382) (xy 147.2946 127.9906)
				(xy 147.8534 127.9906) (xy 147.8534 128.4986) (xy 148.2598 128.4986) (xy 148.2598 126.9238) (xy 150.5458 126.9238)
				(xy 150.5458 128.4986) (xy 150.9522 128.4986) (xy 150.9522 126.9238) (xy 155.6258 126.9238) (xy 155.6258 128.7018)
				(xy 156.0322 128.7018) (xy 156.0322 126.1618)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 112)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 1)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 188.341 62.4586) (xy 189.357 62.4586) (xy 190.3222 63.4238) (xy 193.675 63.4238) (xy 193.675 65.4558)
				(xy 190.2206 68.9102) (xy 189.2046 68.9102) (xy 188.7982 68.453) (xy 188.7982 67.7926) (xy 186.4106 67.7926)
				(xy 186.4106 70.1802) (xy 187.325 70.1802) (xy 188.6458 71.501) (xy 195.961 71.501) (xy 195.961 69.4182)
				(xy 195.2498 68.8086) (xy 193.6242 68.8086) (xy 193.6242 68.4022) (xy 195.0466 66.9798) (xy 199.6186 66.9798)
				(xy 201.2442 65.3542) (xy 204.851 65.3542) (xy 207.137 67.6402) (xy 207.8482 67.6402) (xy 207.8482 75.9206)
				(xy 206.5782 76.9874) (xy 206.5782 78.7654) (xy 207.7974 78.7654) (xy 207.8482 82.3722) (xy 205.2574 82.3722)
				(xy 203.7334 83.8962) (xy 203.7334 89.6874) (xy 202.057 91.3638) (xy 202.057 94.9706) (xy 199.9234 94.9706)
				(xy 199.9234 91.1098) (xy 201.041 89.9922) (xy 201.041 82.2706) (xy 202.2602 81.0514) (xy 202.2602 79.9846)
				(xy 201.6506 79.375) (xy 199.4662 79.375) (xy 199.1106 79.0194) (xy 186.1566 79.0194) (xy 186.1566 76.581)
				(xy 185.4962 75.819) (xy 185.4962 71.501) (xy 185.0898 71.0946) (xy 181.9402 71.0946) (xy 181.9402 70.5866)
				(xy 182.245 70.2818) (xy 184.023 70.2818) (xy 185.801 68.5038) (xy 185.801 66.929) (xy 187.2742 66.929)
				(xy 187.2742 63.5254)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 124)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 150.1902 119.9134) (xy 148.7678 119.9134) (xy 148.463 119.6086) (xy 148.463 118.999) (xy 150.1902 118.999)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 119)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 233.9086 136.9314) (xy 229.3366 136.9314) (xy 229.3366 131.6482) (xy 227.3046 131.6482) (xy 227.3554 64.2874)
				(xy 234.0102 64.2874)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 105)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.25)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 189.7126 94.0054) (xy 189.7126 95.0722) (xy 190.1698 95.5294) (xy 190.1698 102.2858) (xy 192.3034 102.2858)
				(xy 192.3034 96.4438) (xy 191.6938 95.8342) (xy 191.6938 94.869) (xy 190.8302 94.0054)
			)
		)
	)
	(zone
		(net 4)
		(net_name "VCC2")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 82)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.25)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 226.5426 107.7722) (xy 223.4438 107.7722) (xy 223.4438 106.299) (xy 221.361 106.299) (xy 221.361 103.1494)
				(xy 222.123 102.3874) (xy 222.123 96.901) (xy 222.8342 96.2406) (xy 222.8342 79.1718) (xy 220.345 79.1718)
				(xy 220.345 74.1934) (xy 226.6442 74.1934) (xy 226.6442 76.1238) (xy 224.1042 76.1238) (xy 224.1042 89.0778)
				(xy 226.5426 89.0778)
			)
		)
	)
	(zone
		(net 4)
		(net_name "VCC2")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 75)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 189.4586 126.7714) (xy 208.7626 126.7714) (xy 211.3026 129.3114) (xy 211.3026 129.9718) (xy 223.901 129.9718)
				(xy 223.901 127.127) (xy 224.5614 126.5682) (xy 224.5614 122.809) (xy 224.3582 122.809) (xy 222.5294 124.6378)
				(xy 214.8586 124.6378) (xy 213.9442 125.5522) (xy 211.9122 125.5522) (xy 211.3534 124.9934) (xy 190.6778 124.9934)
				(xy 189.5094 126.1618) (xy 189.4586 126.1618)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 86)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.25)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 118.745 60.6806) (xy 128.905 60.6806) (xy 131.2418 63.0174) (xy 143.2814 63.0174) (xy 145.0086 64.6938)
				(xy 160.147 64.6938) (xy 163.195 64.6938) (xy 163.195 66.421) (xy 158.7754 66.421) (xy 158.1658 65.8114)
				(xy 151.3078 65.8114) (xy 151.0538 66.0654) (xy 144.5514 66.0654) (xy 144.2974 65.8114) (xy 118.745 65.8114)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 70)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 62.7126 61.2394) (xy 67.3354 61.2394) (xy 67.3354 60.6806) (xy 72.3646 60.6806) (xy 73.025 60.0202)
				(xy 90.601713 60.0202) (xy 90.9066 59.7154) (xy 95.0722 59.7154) (xy 97.7138 59.7154) (xy 98.2218 60.2234)
				(xy 98.2218 62.2046) (xy 98.933 62.2046) (xy 100.5078 63.7794) (xy 100.5078 64.5922) (xy 106.0958 64.5922)
				(xy 106.0958 62.611) (xy 106.7562 61.9506) (xy 109.2962 61.9506) (xy 110.5154 63.1698) (xy 110.5154 65.4558)
				(xy 110.871 65.8114) (xy 118.745 65.8114) (xy 118.745 60.6806) (xy 113.7666 60.6806) (xy 111.887 58.801)
				(xy 103.4034 58.801) (xy 103.4034 60.6298) (xy 102.997 61.0362) (xy 100.3554 61.0362) (xy 100.3554 58.800903)
				(xy 100.0506 58.4962) (xy 98.3742 58.4962) (xy 97.8662 57.9882) (xy 97.8662 57.0738) (xy 91.4654 57.0738)
				(xy 91.4654 58.039) (xy 85.3694 58.039) (xy 84.8106 57.4802) (xy 70.1802 57.4802) (xy 69.5706 57.3786)
				(xy 69.1134 57.1754) (xy 68.8086 56.9722) (xy 68.5038 56.7182) (xy 68.3514 56.4642) (xy 68.0974 56.007)
				(xy 67.945 55.6006) (xy 67.8942 55.0926) (xy 67.8942 46.4566) (xy 62.7126 46.4566)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 84)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.25)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 208.5086 46.5074) (xy 208.5086 49.657) (xy 206.4258 49.657) (xy 188.7982 49.657) (xy 188.7982 54.1782)
				(xy 185.039 57.9374) (xy 185.039 61.7474) (xy 183.5658 63.2206) (xy 167.8686 63.2206) (xy 167.8686 65.151)
				(xy 165.5826 65.151) (xy 164.719 66.0146) (xy 164.719 66.421) (xy 163.195 66.421) (xy 163.195 57.5818)
				(xy 170.9166 57.5818) (xy 170.9166 58.8518) (xy 179.8574 58.8518) (xy 179.8574 56.007) (xy 186.3598 56.007)
				(xy 186.3598 46.5074) (xy 206.0702 46.5074)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 66)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 86.3854 113.3602) (xy 80.899 113.3602) (xy 80.3402 113.919) (xy 77.7494 113.919) (xy 76.835 114.8334)
				(xy 73.9902 114.8334) (xy 72.4662 115.7478) (xy 71.1454 115.7478) (xy 69.8246 116.459) (xy 67.9958 116.459)
				(xy 66.0146 117.4242) (xy 64.7954 117.4242) (xy 64.4398 117.7798) (xy 64.4398 119.5578) (xy 81.0006 119.5578)
				(xy 83.947 122.5042) (xy 86.741 122.5042) (xy 86.741 122.809) (xy 87.757 123.825) (xy 91.2622 123.825)
				(xy 91.2622 126.619) (xy 100.1014 126.619) (xy 100.1014 128.7526) (xy 99.5426 129.3114) (xy 85.5726 129.3114)
				(xy 83.8454 127.5842) (xy 66.7766 127.5842) (xy 64.4906 125.2982) (xy 59.3598 125.2982) (xy 55.8546 121.793)
				(xy 55.8546 120.269) (xy 59.1058 120.269) (xy 63.5254 115.8494) (xy 65.7098 115.8494) (xy 66.675 114.8842)
				(xy 67.691 114.8842) (xy 70.485 112.0902) (xy 81.0006 112.0902) (xy 81.3054 112.395) (xy 84.5058 112.395)
				(xy 85.1154 111.7854) (xy 86.3854 111.7854)
			)
		)
	)
	(zone
		(net 4)
		(net_name "VCC2")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 95)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.25)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 65.5574 130.4798) (xy 65.5574 131.953) (xy 74.8538 131.953) (xy 75.5142 132.6134) (xy 103.505 132.6134)
				(xy 103.505 132.1562) (xy 102.9462 132.1562) (xy 101.981 131.191) (xy 81.3054 131.191) (xy 80.5942 130.4798)
				(xy 73.9902 130.4798)
			)
		)
	)
	(zone
		(net 4)
		(net_name "VCC2")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 127)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 143.3322 133.0706) (xy 141.1478 133.0706) (xy 140.6398 132.5626) (xy 134.6454 132.5626) (xy 134.6454 132.1054)
				(xy 135.8646 130.8862) (xy 135.8646 129.8194) (xy 140.7414 129.7686) (xy 141.8082 130.8354) (xy 143.3322 130.8354)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 130)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 177.927 122.8598) (xy 177.927 120.8786) (xy 176.5554 120.8786) (xy 176.5554 120.2182) (xy 177.3682 119.4054)
				(xy 179.2986 119.4054) (xy 180.1114 120.2182) (xy 180.1114 120.8278) (xy 179.451 120.8278) (xy 179.451 122.8598)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 129)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 104.3178 124.1806) (xy 104.3178 126.873) (xy 103.3526 126.873) (xy 103.3526 129.9718) (xy 103.8606 130.4798)
				(xy 106.7054 130.4798) (xy 106.7054 128.651) (xy 106.3498 128.2954) (xy 106.3498 127.127) (xy 106.8578 126.619)
				(xy 106.8578 124.1806)
			)
		)
	)
	(zone
		(net 4)
		(net_name "VCC2")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 101)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.25)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 54.737 78.4098) (xy 54.737 79.629) (xy 56.6166 79.629) (xy 56.6166 82.1182) (xy 66.0654 82.1182)
				(xy 66.7258 81.4578) (xy 66.7258 80.3402) (xy 58.4454 80.3402) (xy 58.4454 78.4098)
			)
		)
	)
	(zone
		(net 4)
		(net_name "VCC2")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 145)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.25)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 86.487 82.5246) (xy 95.4786 82.5246) (xy 96.7994 81.2038) (xy 96.7994 79.5274) (xy 86.8934 79.5274)
				(xy 85.8774 80.5434) (xy 85.8774 81.2546) (xy 86.487 81.8642)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 71)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 46.355 46.4566) (xy 51.1556 46.4566) (xy 51.1556 61.214) (xy 52.7558 61.214) (xy 52.7558 65.3542)
				(xy 46.355 65.3542)
			)
		)
	)
	(zone
		(net 4)
		(net_name "VCC2")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 89)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.25)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 155.5242 66.421) (xy 151.8666 66.421) (xy 151.6126 66.675) (xy 144.0434 66.675) (xy 143.7894 66.421)
				(xy 110.4646 66.421) (xy 109.2962 65.2526) (xy 108.4326 65.2526) (xy 99.6442 65.2526) (xy 99.6442 64.135)
				(xy 98.4758 63.0174) (xy 95.4786 63.0174) (xy 94.7674 62.3062) (xy 92.2782 62.3062) (xy 92.2782 60.3758)
				(xy 88.2142 60.3758) (xy 88.2142 63.4238) (xy 94.0562 63.4238) (xy 95.1738 64.5414) (xy 97.0534 64.5414)
				(xy 99.695 67.183) (xy 107.569 67.183) (xy 108.9406 68.5546) (xy 112.0902 68.5546) (xy 121.9962 68.5546)
				(xy 123.2154 67.3354) (xy 134.3914 67.3354) (xy 135.1534 68.0974) (xy 142.7226 68.0974) (xy 143.0782 68.453)
				(xy 153.035 68.453) (xy 153.797 67.691) (xy 155.5242 67.691)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 122)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 132.715 105.4354) (xy 139.319 105.4354) (xy 139.319 105.6386) (xy 141.7574 105.6386) (xy 141.7574 103.8606)
				(xy 142.0622 103.5558) (xy 148.209 103.5558) (xy 148.9202 102.8446) (xy 155.067 102.8446) (xy 156.845 101.0666)
				(xy 156.845 99.8474) (xy 157.3022 99.3902) (xy 160.8582 99.3902) (xy 160.8582 98.7298) (xy 163.4998 98.7298)
				(xy 164.0078 99.2886) (xy 172.9994 99.2886) (xy 173.355 98.933) (xy 173.355 98.6282) (xy 168.3258 98.6282)
				(xy 168.3258 98.171) (xy 167.2082 97.0534) (xy 157.9118 97.0534) (xy 153.3398 101.6254) (xy 148.7678 101.6254)
				(xy 147.955 102.4382) (xy 144.4498 102.4382) (xy 144.145 102.6922) (xy 141.1986 102.6922) (xy 139.1666 104.7242)
				(xy 133.4262 104.7242)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 128)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 113.5634 107.7722) (xy 113.5634 109.6518) (xy 117.9322 109.6518) (xy 118.2878 109.855) (xy 118.2878 111.4298)
				(xy 113.1062 111.4298) (xy 111.7346 110.0582) (xy 111.7346 108.4834) (xy 113.2586 106.9594) (xy 115.0366 106.9594)
				(xy 115.3922 107.2642) (xy 115.3922 107.7722)
			)
		)
	)
	(zone
		(net 4)
		(net_name "VCC2")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 81)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.25)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 221.8182 122.0978) (xy 223.0882 122.0978) (xy 223.5454 122.555) (xy 223.901 122.555) (xy 223.901 121.1326)
				(xy 226.5426 121.1326) (xy 226.5426 107.7722) (xy 223.4438 107.7722) (xy 223.4438 109.8042) (xy 221.869 111.379)
				(xy 220.2942 111.379) (xy 220.2942 119.2022) (xy 220.599 119.507) (xy 220.599 120.8786)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 137)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 207.0354 52.4002) (xy 207.0354 54.9402) (xy 207.7466 55.6514) (xy 207.7466 61.341) (xy 202.7174 61.341)
				(xy 202.7174 60.4266) (xy 204.4954 60.4266) (xy 204.4954 58.039) (xy 202.7174 58.039) (xy 202.7174 52.4002)
			)
		)
	)
	(zone
		(net 4)
		(net_name "VCC2")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 91)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.25)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 51.5874 68.5546) (xy 61.6458 68.5546) (xy 61.6458 68.8594) (xy 61.087 69.4182) (xy 54.5846 69.4182)
				(xy 53.2638 70.739) (xy 53.2638 85.725) (xy 51.5874 85.725)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 80)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 51.1556 46.4566) (xy 51.1556 50.5968) (xy 55.0164 50.5968) (xy 55.0164 54.6862) (xy 63.0682 54.6862)
				(xy 63.0682 46.4566)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 76)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 190.9318 133.1722) (xy 190.0682 133.1722) (xy 190.0682 130.3274) (xy 192.913 127.4826) (xy 208.2038 127.4826)
				(xy 211.0994 130.3782) (xy 211.0994 136.9314) (xy 201.1934 136.9314) (xy 201.1934 131.2926) (xy 198.2978 128.397)
				(xy 193.5226 128.397) (xy 190.9318 130.9878)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 131)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 183.8706 129.3114) (xy 183.8706 126.7714) (xy 183.5658 126.7714) (xy 183.5658 126.4666) (xy 183.3118 126.2126)
				(xy 181.3814 126.1618) (xy 181.3814 129.159) (xy 181.9402 129.159) (xy 182.8038 130.175) (xy 185.7502 130.175)
				(xy 185.7502 129.3114)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 140)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.25)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 216.5858 83.2358) (xy 216.5858 82.8802) (xy 217.3478 82.8802) (xy 217.5002 82.7278) (xy 217.5002 78.1558)
				(xy 216.5858 78.1558) (xy 216.5858 77.7494) (xy 217.5002 77.7494) (xy 217.5002 75.6158) (xy 216.4842 75.6158)
				(xy 216.4842 75.2094) (xy 217.5002 75.2094) (xy 217.5002 71.6534) (xy 217.9574 71.6534) (xy 217.9574 76.7334)
				(xy 217.9574 82.9818) (xy 217.7034 83.2358)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 134)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 228.6254 63.8556) (xy 228.6254 64.5922) (xy 210.7946 64.5922) (xy 210.7946 59.9186) (xy 213.233 59.9186)
				(xy 213.233 61.9506) (xy 211.8106 61.9506) (xy 211.8106 63.8556)
			)
		)
	)
	(zone
		(net 4)
		(net_name "VCC2")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 142)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.25)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 180.0606 109.8042) (xy 180.0606 111.0742) (xy 184.1754 111.0742) (xy 184.8358 111.7346) (xy 185.8518 111.7346)
				(xy 186.3598 111.2266) (xy 186.3598 108.9914) (xy 185.547 108.1786) (xy 185.547 105.9434) (xy 183.9214 105.9434)
				(xy 182.6006 107.2134) (xy 182.6006 108.839) (xy 181.6354 109.8042)
			)
		)
	)
	(zone
		(net 4)
		(net_name "VCC2")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 63)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.25)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 63.5254 96.7486) (xy 64.389 95.885) (xy 83.5914 95.885) (xy 87.5538 95.885) (xy 91.1098 99.441)
				(xy 98.679 99.441) (xy 98.9838 99.1362) (xy 98.9838 97.7646) (xy 98.425 97.2058) (xy 98.425 94.3102)
				(xy 98.6282 94.107) (xy 100.1522 94.107) (xy 102.235 92.0242) (xy 102.235 90.7542) (xy 102.9462 90.043)
				(xy 106.5022 90.043) (xy 106.5022 90.4494) (xy 107.0102 90.9574) (xy 108.0262 90.9574) (xy 108.0262 91.821)
				(xy 108.4834 92.2782) (xy 109.2454 92.2782) (xy 109.7026 91.821) (xy 109.7026 93.8022) (xy 109.4486 94.0562)
				(xy 105.9434 94.0562) (xy 105.537 93.599) (xy 105.537 91.3638) (xy 105.2322 91.0082) (xy 104.3178 91.0082)
				(xy 104.013 91.313) (xy 104.013 94.0562) (xy 103.4542 94.0562) (xy 103.4542 95.377) (xy 100.711 95.377)
				(xy 99.8474 96.2406) (xy 99.8474 96.901) (xy 100.8126 97.8662) (xy 100.8126 100.0506) (xy 100.203 100.6602)
				(xy 90.7034 100.6602) (xy 87.2998 97.2566) (xy 81.4578 97.2566) (xy 69.6722 97.2566) (xy 68.9102 98.0186)
				(xy 65.2526 98.0186) (xy 65.2526 97.3582) (xy 63.5254 97.3582)
			)
		)
	)
	(zone
		(net 4)
		(net_name "VCC2")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 93)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.25)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 53.1114 108.7374) (xy 53.1114 124.5362) (xy 60.4774 131.953) (xy 65.5574 131.953) (xy 65.5574 130.4798)
				(xy 63.5254 130.4798) (xy 55.1942 122.1486) (xy 55.1942 119.6086) (xy 58.4454 119.6086) (xy 58.4454 117.7798)
				(xy 55.1942 117.7798) (xy 55.1942 108.7374)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 65)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 93.4974 116.4082) (xy 93.4974 116.0018) (xy 92.0242 114.5286) (xy 86.6902 114.5286) (xy 86.6902 120.523)
				(xy 88.011 120.523) (xy 88.773 121.285) (xy 92.2274 121.285) (xy 92.2274 120.1166) (xy 91.1098 118.999)
				(xy 91.1098 116.4082)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 85)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.25)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 157.861 56.1086) (xy 157.861 59.4614) (xy 158.115 59.7154) (xy 158.9786 59.7154) (xy 159.4358 60.1726)
				(xy 159.4358 62.7634) (xy 158.4198 63.7794) (xy 156.591 63.7794) (xy 155.6766 64.6938) (xy 163.195 64.6938)
				(xy 163.195 57.5818) (xy 160.7566 57.5818) (xy 158.7754 55.6006)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 61)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 126.4666 93.6498) (xy 126.4666 92.6338) (xy 125.9078 92.075) (xy 118.0846 92.075) (xy 117.6274 92.5322)
				(xy 112.395 92.5322) (xy 111.379 93.4974) (xy 111.379 95.0214) (xy 110.871 95.5294) (xy 105.8926 95.5294)
				(xy 105.8926 99.6442) (xy 105.5878 99.949) (xy 102.1842 99.949) (xy 101.1174 101.0158) (xy 90.5002 101.0158)
				(xy 86.995 97.5614) (xy 83.5406 97.5614) (xy 82.3722 97.5614) (xy 81.4578 98.4758) (xy 81.915 99.9998)
				(xy 82.931 99.9998) (xy 83.7946 100.8634) (xy 86.0298 100.8634) (xy 88.9254 103.759) (xy 94.6658 103.759)
				(xy 95.885 104.9782) (xy 100.3554 104.9782) (xy 100.8126 104.521) (xy 100.8126 103.3018) (xy 101.6762 102.4382)
				(xy 105.7402 102.4382) (xy 114.4778 93.6498)
			)
		)
	)
	(zone
		(net 4)
		(net_name "VCC2")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 98)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.25)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 208.1022 107.6706) (xy 205.6638 107.6706) (xy 205.6638 107.4674) (xy 207.5434 105.5878) (xy 208.1022 105.5878)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 136)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 208.5086 49.657) (xy 208.5086 52.4002) (xy 201.549 52.4002) (xy 201.549 49.657)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 113)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.25)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 208.1022 92.9386) (xy 206.4766 92.9386) (xy 206.4766 96.4946) (xy 208.1022 94.869)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 78)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 51.1556 61.214) (xy 63.0682 61.2394) (xy 63.0682 54.6862) (xy 51.1556 54.6862)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 141)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.25)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 198.1454 113.0554) (xy 196.9262 111.8362) (xy 196.9262 108.331) (xy 203.3778 108.331) (xy 203.3778 109.7026)
				(xy 207.3402 109.7026) (xy 207.645 109.9566) (xy 207.0354 110.6678) (xy 201.7522 110.6678) (xy 201.295 111.125)
				(xy 201.295 112.7506) (xy 200.8886 113.0554)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 118)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 159.639 91.7194) (xy 158.0642 93.2942) (xy 158.0642 93.7514) (xy 158.1658 93.853) (xy 168.6306 93.853)
				(xy 168.9354 93.5482) (xy 170.9674 93.5482) (xy 171.5262 94.107) (xy 171.5262 94.615) (xy 172.3898 94.615)
				(xy 173.101 93.9038) (xy 176.7586 93.9038) (xy 177.0126 93.6498) (xy 180.0606 93.6498) (xy 180.3146 93.9038)
				(xy 180.3146 94.7166) (xy 180.6702 95.0722) (xy 180.6702 96.4438) (xy 178.7906 98.3234) (xy 176.2506 98.3234)
				(xy 175.895 97.9678) (xy 175.895 97.0026) (xy 173.9138 97.0026) (xy 172.9486 97.9678) (xy 172.9486 98.9838)
				(xy 179.1462 98.9838) (xy 182.0926 96.0374) (xy 183.4134 96.0374) (xy 184.277 95.1738) (xy 184.277 94.4118)
				(xy 183.515 94.4118) (xy 183.1594 94.0562) (xy 181.6354 94.0562) (xy 180.7718 93.1926) (xy 168.7322 93.1926)
				(xy 167.259 91.7194)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 67)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 112.1918 116.1542) (xy 110.8202 116.1542) (xy 110.8202 117.221) (xy 111.2266 117.6274) (xy 117.983 117.6274)
				(xy 117.983 116.7638) (xy 112.8014 116.7638)
			)
		)
	)
	(zone
		(net 4)
		(net_name "VCC2")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 68)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 141.1732 131.7244) (xy 142.113 132.6642) (xy 141.1478 132.6642) (xy 140.3096 131.7244)
			)
		)
	)
	(zone
		(net 4)
		(net_name "VCC2")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 64)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 108.585 110.109) (xy 108.585 109.601) (xy 102.5906 109.601) (xy 102.3366 109.601) (xy 101.9302 109.601)
				(xy 100.3554 109.601) (xy 98.9838 110.9726) (xy 98.679 110.9726) (xy 98.171 110.9726) (xy 97.917 111.2266)
				(xy 97.917 112.0394) (xy 98.8822 113.0046) (xy 101.2698 113.0046) (xy 101.6762 113.411) (xy 102.8954 113.411)
				(xy 102.8954 111.379) (xy 103.1494 111.125) (xy 104.1654 111.125) (xy 104.4702 111.4298) (xy 107.0102 111.4298)
				(xy 107.9754 111.4298) (xy 108.4834 111.4298) (xy 108.9914 111.0742)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 77)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 209.7278 136.9314) (xy 211.4042 136.9314) (xy 226.441 136.9314) (xy 226.441 135.6614) (xy 224.5614 135.6614)
				(xy 224.5614 131.6482) (xy 222.9866 131.6482) (xy 221.7166 130.3782) (xy 209.7278 130.3782)
			)
		)
	)
	(zone
		(net 4)
		(net_name "VCC2")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 92)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.25)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 51.5874 85.725) (xy 53.2638 85.725) (xy 53.2638 87.8078) (xy 54.8894 89.4334) (xy 54.8894 103.9622)
				(xy 54.0258 103.9622) (xy 53.6702 104.3178) (xy 53.6702 105.6386) (xy 53.975 105.9434) (xy 55.1942 105.9434)
				(xy 55.1942 108.7374) (xy 53.1114 108.7374) (xy 53.1114 94.2086) (xy 51.5874 92.6846)
			)
		)
	)
	(zone
		(net 4)
		(net_name "VCC2")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 59)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 129.8702 86.741) (xy 129.6162 86.995) (xy 129.6162 88.4174) (xy 128.651 88.4174) (xy 128.2446 88.8238)
				(xy 126.873 88.8238) (xy 126.619 89.0778) (xy 126.1618 89.0778) (xy 126.1618 89.4842) (xy 126.7714 89.4842)
				(xy 127.0762 89.1794) (xy 128.397 89.1794) (xy 128.8034 88.773) (xy 129.6162 88.773) (xy 130.0226 88.773)
				(xy 130.0226 87.6046) (xy 131.445 87.6046) (xy 131.445 87.2998) (xy 132.3594 86.3854) (xy 134.6962 86.3854)
				(xy 134.9502 86.6394) (xy 142.5702 86.6394) (xy 142.5702 85.1662) (xy 142.2146 84.8614) (xy 129.8702 84.8614)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 109)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.25)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 202.6158 103.5558) (xy 204.851 103.5558) (xy 205.7654 102.6414) (xy 205.7654 101.7778) (xy 206.7814 100.8634)
				(xy 204.4954 100.8634) (xy 204.4954 101.5746) (xy 202.6158 103.4542)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 151)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 213.8426 54.1782) (xy 213.8426 53.2638) (xy 227.6348 53.2638) (xy 227.6348 54.1528)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 144)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.25)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 56.7182 82.8294) (xy 56.7182 85.8266) (xy 58.3946 87.503) (xy 60.1218 87.503) (xy 61.4426 88.8238)
				(xy 64.4906 88.8238) (xy 65.4558 89.789) (xy 65.4558 92.7862) (xy 66.167 93.4974) (xy 80.899 93.4974)
				(xy 81.8134 92.4814) (xy 84.8106 92.4814) (xy 85.1154 92.7862) (xy 85.1154 93.4466) (xy 85.6234 93.9546)
				(xy 90.2462 93.9546) (xy 91.4146 92.7862) (xy 91.4146 89.2302) (xy 93.2434 87.4014) (xy 93.2434 85.979)
				(xy 97.2566 85.979) (xy 98.425 84.8106) (xy 104.8766 84.8106) (xy 104.8766 83.2866) (xy 106.553 83.2866)
				(xy 108.9914 80.8482) (xy 109.601 80.8482) (xy 110.1598 81.407) (xy 110.1598 82.1182) (xy 112.1918 82.1182)
				(xy 112.1918 78.7146) (xy 109.855 78.7146) (xy 109.4994 78.359) (xy 109.4994 77.1398) (xy 109.1438 76.7334)
				(xy 102.489 76.7334) (xy 100.5586 74.803) (xy 99.6442 74.803) (xy 99.6442 76.9874) (xy 103.1494 76.9874)
				(xy 104.2162 78.0542) (xy 106.5022 78.0542) (xy 107.2642 78.8162) (xy 107.2642 80.3402) (xy 105.6386 81.9658)
				(xy 101.5746 81.9658) (xy 101.0666 81.407) (xy 99.7966 81.407) (xy 98.4758 80.0862) (xy 97.3582 80.0862)
				(xy 97.3582 81.5594) (xy 95.7834 83.1342) (xy 89.1794 83.1342) (xy 89.1794 87.8078) (xy 86.1822 87.8078)
				(xy 86.1822 89.4842) (xy 85.5218 90.1446) (xy 81.9658 90.1446) (xy 81.5594 89.7382) (xy 78.7146 89.7382)
				(xy 76.073 92.3798) (xy 67.3862 92.3798) (xy 66.9798 92.0242) (xy 66.9798 91.313) (xy 70.8914 87.4014)
				(xy 82.3214 87.4014) (xy 82.8802 86.8426) (xy 82.8802 84.3534) (xy 64.135 84.3534) (xy 62.611 82.8294)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 69)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 190.9318 136.9822) (xy 46.355 137.033) (xy 46.355 132.1054) (xy 59.6646 132.1054) (xy 59.8678 132.3594)
				(xy 74.2442 132.3594) (xy 74.9046 133.0198) (xy 100.8634 133.0198) (xy 101.219 133.3754) (xy 135.6614 133.3754)
				(xy 135.9662 133.0706) (xy 140.5382 133.0706) (xy 140.9446 133.477) (xy 177.8762 133.477) (xy 178.181 133.1722)
				(xy 190.9318 133.1722)
			)
		)
	)
	(zone
		(net 4)
		(net_name "VCC2")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 60)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 126.2126 89.789) (xy 126.2126 88.011) (xy 125.7046 87.503) (xy 112.2934 87.503) (xy 110.617 89.1794)
				(xy 110.617 90.3478) (xy 109.7026 91.2114) (xy 109.7026 93.8022) (xy 111.9886 91.5162) (xy 113.0554 91.5162)
				(xy 113.7666 90.805) (xy 113.7666 89.4842) (xy 114.681 88.5698) (xy 116.713 88.5698) (xy 118.0846 89.9414)
				(xy 126.0602 89.9414)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 16)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.25)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 169.3926 57.5818) (xy 169.3926 58.8518) (xy 169.9514 58.8518) (xy 170.9166 58.8518) (xy 171.4246 58.8518)
				(xy 174.2694 58.8518) (xy 177.0126 58.8518) (xy 178.435 58.8518) (xy 179.8574 58.8518) (xy 179.8574 57.1246)
				(xy 179.8574 56.6674) (xy 179.8574 56.007) (xy 186.3598 56.007) (xy 186.3598 46.5074) (xy 173.3042 46.5074)
				(xy 173.3042 55.4482) (xy 173.1518 56.0578) (xy 172.9994 56.3626) (xy 172.7454 56.6674) (xy 172.5422 56.8706)
				(xy 172.085 57.2262) (xy 171.7294 57.3786) (xy 171.323 57.4802) (xy 170.815 57.531) (xy 170.1546 57.5818)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 126)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 147.8534 127.9906) (xy 147.8534 129.7686) (xy 156.0322 129.7686) (xy 156.0322 128.7018) (xy 155.6258 128.7018)
				(xy 155.6258 129.3114) (xy 150.9522 129.3114) (xy 150.9522 128.4986) (xy 150.5458 128.4986) (xy 150.5458 129.3114)
				(xy 148.2598 129.3114) (xy 148.2598 127.9906)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 102)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.25)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 60.4266 75.5142) (xy 60.4266 79.629) (xy 66.7258 79.629) (xy 66.7258 77.089) (xy 69.3166 77.089)
				(xy 69.3166 81.8134) (xy 71.8058 81.8134) (xy 74.5998 79.0194) (xy 80.391 79.0194) (xy 83.2358 76.1746)
				(xy 95.3262 76.1746) (xy 95.9358 75.565) (xy 95.9358 74.6506) (xy 91.821 74.6506) (xy 90.7542 73.3806)
				(xy 89.027 73.3806) (xy 87.757 74.6506) (xy 66.4718 74.6506) (xy 64.2874 76.835) (xy 62.357 76.835)
				(xy 61.9506 76.4286) (xy 61.9506 75.5142)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 149)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.25)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 201.041 82.2706) (xy 199.3138 82.2706) (xy 198.9582 82.677) (xy 198.9582 83.185) (xy 194.8942 83.185)
				(xy 194.4878 83.5914) (xy 187.4266 83.5914) (xy 187.0202 83.9978) (xy 184.8358 83.9978) (xy 183.9722 83.1342)
				(xy 182.8038 83.1342) (xy 181.991 84.0486) (xy 180.7718 84.0486) (xy 180.5178 83.7946) (xy 172.4406 83.7946)
				(xy 172.085 83.439) (xy 171.323 83.439) (xy 170.815 82.931) (xy 168.8338 82.931) (xy 167.8178 81.915)
				(xy 165.0746 81.915) (xy 164.1602 82.8294) (xy 156.7434 82.8294) (xy 153.6446 86.2838) (xy 153.6446 86.8426)
				(xy 153.797 86.6902) (xy 157.0482 86.6902) (xy 159.2326 84.5058) (xy 165.9382 84.5058) (xy 167.8686 86.4362)
				(xy 171.323 86.4362) (xy 172.9486 88.0618) (xy 174.1678 88.0618) (xy 174.1678 85.9282) (xy 174.4218 85.6742)
				(xy 191.5922 85.6742) (xy 192.5066 86.5886) (xy 192.5066 88.4682) (xy 194.8942 88.4682) (xy 194.8942 86.6902)
				(xy 195.707 85.8774) (xy 198.6534 85.8774) (xy 198.6534 83.8454) (xy 201.041 83.8454)
			)
		)
	)
	(zone
		(net 4)
		(net_name "VCC2")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 90)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.25)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 88.2142 63.4238) (xy 88.2142 60.3758) (xy 74.041 60.3758) (xy 72.517 61.8998) (xy 72.517 63.2206)
				(xy 67.3354 63.2206) (xy 67.3354 61.6458) (xy 62.6618 61.6458) (xy 62.6618 62.3062) (xy 62.5602 62.865)
				(xy 62.2554 63.4746) (xy 61.8998 64.0842) (xy 61.4426 64.5922) (xy 61.087 64.897) (xy 60.7314 65.1002)
				(xy 60.1726 65.405) (xy 59.5122 65.6082) (xy 58.5978 65.7098) (xy 57.531 65.7098) (xy 51.5874 65.7098)
				(xy 51.5874 68.5546) (xy 61.6458 68.5546) (xy 61.6458 66.3702) (xy 63.3222 64.6938) (xy 80.137 64.6938)
				(xy 81.3562 63.4238)
			)
		)
	)
	(zone
		(net 4)
		(net_name "VCC2")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 57)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 128.3462 96.4692) (xy 127.762 95.885) (xy 126.3142 95.885) (xy 125.857 95.4278) (xy 115.2906 95.4278)
				(xy 114.173 96.5454) (xy 124.587 96.5454) (xy 125.2982 97.2566) (xy 127.7874 97.2566) (xy 128.3462 96.52)
			)
		)
	)
	(zone
		(net 4)
		(net_name "VCC2")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 138)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 201.7522 58.039) (xy 199.9742 58.039) (xy 199.9742 59.6138) (xy 197.4342 59.6138) (xy 196.6214 58.801)
				(xy 196.6214 54.991) (xy 190.6778 54.991) (xy 190.6778 56.5658) (xy 188.1886 59.055) (xy 188.1886 60.9346)
				(xy 181.8894 67.2338) (xy 178.7398 67.2338) (xy 174.7774 71.1962) (xy 168.1226 71.1962) (xy 167.6654 71.6534)
				(xy 163.3474 71.6534) (xy 161.3662 69.6722) (xy 157.9118 69.6722) (xy 155.9306 67.691) (xy 155.5242 67.691)
				(xy 155.5242 66.421) (xy 157.7086 66.421) (xy 158.4198 67.1322) (xy 165.735 67.1322) (xy 166.9542 68.3514)
				(xy 170.307 68.3514) (xy 170.307 63.6778) (xy 183.9214 63.6778) (xy 185.547 62.0522) (xy 185.547 58.1406)
				(xy 189.3062 54.3814) (xy 189.3062 50.1142) (xy 200.9394 50.1142) (xy 200.9394 54.1782) (xy 201.7522 54.991)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 135)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 210.7946 53.5178) (xy 209.677 52.4002) (xy 208.5086 52.4002) (xy 208.5086 50.8762) (xy 211.836 50.8762)
				(xy 211.836 53.2892) (xy 213.995 53.2892) (xy 213.995 60.2234) (xy 210.7946 60.2234)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 88)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 213.233 56.3626) (xy 213.233 61.976) (xy 229.3366 61.9506) (xy 229.3366 56.3626)
			)
		)
	)
	(zone
		(net 4)
		(net_name "VCC2")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 74)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 177.4698 133.0706) (xy 143.3322 133.0706) (xy 143.3322 130.8354) (xy 146.8882 130.8354) (xy 146.8882 131.953)
				(xy 164.6174 131.953) (xy 172.2374 131.953) (xy 172.2374 131.2418) (xy 173.0502 131.2418) (xy 173.709736 131.9022)
				(xy 174.9806 131.9022) (xy 175.590435 131.277542) (xy 179.2986 131.2926) (xy 179.5018 131.0894)
				(xy 186.563 131.0894) (xy 186.563 126.1618) (xy 189.4586 126.1618) (xy 189.4586 126.7714) (xy 192.659 126.7714)
				(xy 190.3222 129.1082) (xy 189.3062 129.1082) (xy 189.3062 132.7658) (xy 177.7746 132.7658)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 133)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 234.0102 64.2874) (xy 228.6508 64.3382) (xy 228.6508 56.6674) (xy 228.2952 56.6674) (xy 228.2952 54.1528)
				(xy 227.4824 54.1528) (xy 227.4824 51.4096) (xy 208.5086 51.4096) (xy 208.5086 46.5074) (xy 234.0102 46.5582)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "In1.Cu")
		(hatch edge 0.5)
		(priority 150)
		(connect_pads
			(clearance 0.2)
		)
		(min_thickness 0.2)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(smoothing fillet)
			(radius 0.3)
		)
		(polygon
			(pts
				(xy 46.355 46.4566) (xy 233.9086 46.5074) (xy 233.9086 136.9314) (xy 46.355 137.033)
			)
		)
	)
	(zone
		(net 4)
		(net_name "VCC2")
		(layer "In2.Cu")
		(hatch edge 0.5)
		(priority 150)
		(connect_pads
			(clearance 0.2)
		)
		(min_thickness 0.2)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(smoothing fillet)
			(radius 0.3)
		)
		(polygon
			(pts
				(xy 46.355 46.4566) (xy 233.9086 46.5074) (xy 233.9086 136.9314) (xy 46.355 137.033)
			)
		)
	)
	(embedded_fonts no)
)
