(kicad_pcb (version 20171130) (host pcbnew "(5.1.12)-1")
  (general
    (thickness 1.6)
    (drawings 33)
    (tracks 191)
    (zones 0)
    (modules 45)
    (nets 41)
  )
  (page B)
  (title_block
    (title Aspera)
    (date 2023-01-22)
    (rev 1.0)
    (comment 1 "DAQ Board")
    (comment 2 ASPERA-UA-DWG-00002_DAQ)
  )
  (layers
    (0 F.Cu signal)
    (1 In1.Cu signal)
    (2 In2.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user hide)
    (35 F.Paste user hide)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user hide)
    (47 F.CrtYd user hide)
    (48 B.Fab user hide)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.25)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.15)
    (segment_width 0.2)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 0.7 0.7)
    (mod_text_width 0.15)
    (pad_size 5.5372 5.5372)
    (pad_drill 2.4384)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 50 50)
    (grid_origin 50 50)
    (visible_elements 7FFFFF7F)
    (pcbplotparams
      (layerselection 0x10000_7fffff80)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer false)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue false)
      (plotinvisibletext false)
      (padsonsilk true)
      (subtractmaskfromsilk false)
      (outputformat 4)
      (mirror true)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "gerbers1b"))
  )
  (net 0 "")
  (net 1 GND)
  (net 2 /PCB_top_level/HVPS_TEMP+)
  (net 3 /PCB_top_level/HVPS_TEMP1-)
  (net 4 /PCB_top_level/HVPS_TEMP2-)
  (net 5 /PCB_top_level/HVPS1_Vset)
  (net 6 /PCB_top_level/HVPS1_Vmon)
  (net 7 /PCB_top_level/HVPS1_Imon)
  (net 8 /PCB_top_level/HVPS2_Vmon)
  (net 9 CHASSIS)
  (net 10 "Net-(C1-Pad1)")
  (net 11 "Net-(C2-Pad2)")
  (net 12 "Net-(C5-Pad2)")
  (net 13 "Net-(C6-Pad2)")
  (net 14 "Net-(C7-Pad2)")
  (net 15 "Net-(C8-Pad2)")
  (net 16 /PCB_top_level/+6.2V_HVPS)
  (net 17 /PCB_top_level/-6.2V_HVPS)
  (net 18 /PCB_top_level/-6.2V_IN)
  (net 19 /PCB_top_level/+6.2V_IN)
  (net 20 /PCB_top_level/HVPS1_ON_OUT_5V)
  (net 21 /PCB_top_level/HVPS_ANODE_VSTATUS)
  (net 22 "Net-(Q1-Pad1)")
  (net 23 /PCB_top_level/HVPS_LEVSET)
  (net 24 /PCB_top_level/HVPS_STRIP_CSTATUS)
  (net 25 /PCB_top_level/HVPS_MCP_VSTATUS)
  (net 26 /PCB_top_level/HVPS_EN_N)
  (net 27 /PCB_top_level/HVPS2.RTN)
  (net 28 /PCB_top_level/HVPS2_ON_OUT_5V)
  (net 29 "Net-(J6-Pad18)")
  (net 30 /PCB_top_level/HVPS2.PWR)
  (net 31 "Net-(J6-Pad14)")
  (net 32 "Net-(J6-Pad13)")
  (net 33 "Net-(J6-Pad12)")
  (net 34 "Net-(J6-Pad11)")
  (net 35 /PCB_top_level/HVPS2_Imon)
  (net 36 /PCB_top_level/HVPS2_Vset)
  (net 37 /PCB_top_level/HVPS1.RTN)
  (net 38 /PCB_top_level/HVPS1.PWR)
  (net 39 "Net-(J2-Pad14)")
  (net 40 "Net-(J2-Pad10)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /PCB_top_level/HVPS1.PWR)
    (add_net /PCB_top_level/HVPS1.RTN)
    (add_net /PCB_top_level/HVPS1_Imon)
    (add_net /PCB_top_level/HVPS1_ON_OUT_5V)
    (add_net /PCB_top_level/HVPS1_Vmon)
    (add_net /PCB_top_level/HVPS1_Vset)
    (add_net /PCB_top_level/HVPS2.PWR)
    (add_net /PCB_top_level/HVPS2.RTN)
    (add_net /PCB_top_level/HVPS2_Imon)
    (add_net /PCB_top_level/HVPS2_ON_OUT_5V)
    (add_net /PCB_top_level/HVPS2_Vmon)
    (add_net /PCB_top_level/HVPS2_Vset)
    (add_net /PCB_top_level/HVPS_ANODE_VSTATUS)
    (add_net /PCB_top_level/HVPS_EN_N)
    (add_net /PCB_top_level/HVPS_LEVSET)
    (add_net /PCB_top_level/HVPS_MCP_VSTATUS)
    (add_net /PCB_top_level/HVPS_STRIP_CSTATUS)
    (add_net /PCB_top_level/HVPS_TEMP+)
    (add_net /PCB_top_level/HVPS_TEMP1-)
    (add_net /PCB_top_level/HVPS_TEMP2-)
    (add_net CHASSIS)
    (add_net GND)
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(C2-Pad2)")
    (add_net "Net-(C5-Pad2)")
    (add_net "Net-(C6-Pad2)")
    (add_net "Net-(C7-Pad2)")
    (add_net "Net-(C8-Pad2)")
    (add_net "Net-(J2-Pad10)")
    (add_net "Net-(J2-Pad14)")
    (add_net "Net-(J6-Pad11)")
    (add_net "Net-(J6-Pad12)")
    (add_net "Net-(J6-Pad13)")
    (add_net "Net-(J6-Pad14)")
    (add_net "Net-(J6-Pad18)")
    (add_net "Net-(Q1-Pad1)")
  )
  (net_class power ""
    (clearance 0.2)
    (trace_width 0.5)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /PCB_top_level/+6.2V_HVPS)
    (add_net /PCB_top_level/+6.2V_IN)
    (add_net /PCB_top_level/-6.2V_HVPS)
    (add_net /PCB_top_level/-6.2V_IN)
  )
  (module Aspera_footprints:26ga_term_with_strain_relief (layer F.Cu) (tedit 68FA7E0A)
    (at 94.23 73.44)
    (fp_text reference TP6 (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value -6.2V (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 3.81 0) (size 1.27 1.27) (drill 1.27) (layers *.Cu))
    (pad 1 thru_hole circle (at 0 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 18 /PCB_top_level/-6.2V_IN))
  )
  (module Aspera_footprints:26ga_term_with_strain_relief (layer F.Cu) (tedit 68FA7E0A)
    (at 94.25 81.57)
    (fp_text reference TP5 (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value GND (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 3.81 0) (size 1.27 1.27) (drill 1.27) (layers *.Cu))
    (pad 1 thru_hole circle (at 0 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module Aspera_footprints:26ga_term_with_strain_relief (layer F.Cu) (tedit 68FA7E0A)
    (at 94.26 78.47)
    (fp_text reference TP4 (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value +6.2V (at 0 -0.5) (layer F.Fab) hide)
    (pad "" np_thru_hole circle (at 3.81 0) (size 1.27 1.27) (drill 1.27) (layers *.Cu))
    (pad 1 thru_hole circle (at 0 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 19 /PCB_top_level/+6.2V_IN))
  )
  (module Aspera_footprints:26ga_term_with_strain_relief (layer F.Cu) (tedit 68FA7E0A)
    (at 94.25 71.5)
    (fp_text reference TP3 (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value -6.2V (at 5.58 1.01 90) (layer F.SilkS))
    (pad "" np_thru_hole circle (at 3.81 0) (size 1.27 1.27) (drill 1.27) (layers *.Cu))
    (pad 1 thru_hole circle (at 0 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 18 /PCB_top_level/-6.2V_IN))
  )
  (module Aspera_footprints:26ga_term_with_strain_relief (layer F.Cu) (tedit 68FA7E0A)
    (at 94.25 83.5)
    (fp_text reference TP2 (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value GND (at 5.51 -1.06 90) (layer F.SilkS))
    (pad "" np_thru_hole circle (at 3.81 0) (size 1.27 1.27) (drill 1.27) (layers *.Cu))
    (pad 1 thru_hole circle (at 0 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 1 GND))
  )
  (module Aspera_footprints:26ga_term_with_strain_relief (layer F.Cu) (tedit 68FA7E0A)
    (at 94.25 76.53)
    (fp_text reference TP1 (at 0 0.5) (layer F.SilkS) hide)
    (fp_text value +6.2V (at 5.45 1.24 90) (layer F.SilkS))
    (pad "" np_thru_hole circle (at 3.81 0) (size 1.27 1.27) (drill 1.27) (layers *.Cu))
    (pad 1 thru_hole circle (at 0 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 19 /PCB_top_level/+6.2V_IN))
  )
  (module Aspera_footprints:M80-5412022 (layer F.Cu) (tedit 62DC716C)
    (at 81.3 86.3)
    (descr M80-54120YY)
    (tags Connector)
    (fp_text reference J6 (at -8.1 -2.4) (layer F.SilkS))
    (fp_text value Conn_02x10 (at 0 0) (layer F.SilkS) hide)
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 22 np_thru_hole circle (at -21.5 1) (size 2.2 0) (drill 2.2) (layers *.Cu *.Mask))
    (pad 21 np_thru_hole circle (at 3.5 1) (size 2.2 0) (drill 2.2) (layers *.Cu *.Mask))
    (pad 20 thru_hole circle (at -18 2) (size 1.15 1.15) (drill 0.65) (layers *.Cu *.Mask)
      (net 27 /PCB_top_level/HVPS2.RTN))
    (pad 19 thru_hole circle (at -16 2) (size 1.15 1.15) (drill 0.65) (layers *.Cu *.Mask)
      (net 28 /PCB_top_level/HVPS2_ON_OUT_5V))
    (pad 18 thru_hole circle (at -14 2) (size 1.15 1.15) (drill 0.65) (layers *.Cu *.Mask)
      (net 29 "Net-(J6-Pad18)"))
    (pad 17 thru_hole circle (at -12 2) (size 1.15 1.15) (drill 0.65) (layers *.Cu *.Mask)
      (net 30 /PCB_top_level/HVPS2.PWR))
    (pad 16 thru_hole circle (at -10 2) (size 1.15 1.15) (drill 0.65) (layers *.Cu *.Mask)
      (net 7 /PCB_top_level/HVPS1_Imon))
    (pad 15 thru_hole circle (at -8 2) (size 1.15 1.15) (drill 0.65) (layers *.Cu *.Mask)
      (net 5 /PCB_top_level/HVPS1_Vset))
    (pad 14 thru_hole circle (at -6 2) (size 1.15 1.15) (drill 0.65) (layers *.Cu *.Mask)
      (net 31 "Net-(J6-Pad14)"))
    (pad 13 thru_hole circle (at -4 2) (size 1.15 1.15) (drill 0.65) (layers *.Cu *.Mask)
      (net 32 "Net-(J6-Pad13)"))
    (pad 12 thru_hole circle (at -2 2) (size 1.15 1.15) (drill 0.65) (layers *.Cu *.Mask)
      (net 33 "Net-(J6-Pad12)"))
    (pad 11 thru_hole circle (at 0 2) (size 1.15 1.15) (drill 0.65) (layers *.Cu *.Mask)
      (net 34 "Net-(J6-Pad11)"))
    (pad 10 thru_hole circle (at -18 0) (size 1.15 1.15) (drill 0.65) (layers *.Cu *.Mask)
      (net 35 /PCB_top_level/HVPS2_Imon))
    (pad 9 thru_hole circle (at -16 0) (size 1.15 1.15) (drill 0.65) (layers *.Cu *.Mask)
      (net 36 /PCB_top_level/HVPS2_Vset))
    (pad 8 thru_hole circle (at -14 0) (size 1.15 1.15) (drill 0.65) (layers *.Cu *.Mask)
      (net 8 /PCB_top_level/HVPS2_Vmon))
    (pad 7 thru_hole circle (at -12 0) (size 1.15 1.15) (drill 0.65) (layers *.Cu *.Mask)
      (net 37 /PCB_top_level/HVPS1.RTN))
    (pad 6 thru_hole circle (at -10 0) (size 1.15 1.15) (drill 0.65) (layers *.Cu *.Mask)
      (net 38 /PCB_top_level/HVPS1.PWR))
    (pad 5 thru_hole circle (at -8 0) (size 1.15 1.15) (drill 0.65) (layers *.Cu *.Mask)
      (net 20 /PCB_top_level/HVPS1_ON_OUT_5V))
    (pad 4 thru_hole circle (at -6 0) (size 1.15 1.15) (drill 0.65) (layers *.Cu *.Mask)
      (net 6 /PCB_top_level/HVPS1_Vmon))
    (pad 3 thru_hole circle (at -4 0) (size 1.15 1.15) (drill 0.65) (layers *.Cu *.Mask)
      (net 3 /PCB_top_level/HVPS_TEMP1-))
    (pad 2 thru_hole circle (at -2 0) (size 1.15 1.15) (drill 0.65) (layers *.Cu *.Mask)
      (net 4 /PCB_top_level/HVPS_TEMP2-))
    (pad 1 thru_hole rect (at 0 0) (size 1.15 1.15) (drill 0.65) (layers *.Cu *.Mask)
      (net 2 /PCB_top_level/HVPS_TEMP+))
    (model ${KIPRJMOD}/../../Libraries/Solid_models/M80_5412022_ASM_cp.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Aspera_footprints:HolePlated_2-56_0.23_standoff_smallest (layer F.Cu) (tedit 68D19D03)
    (at 97.65 64)
    (descr "Mounting Hole 1/4\" pad, 2-56 hole")
    (tags "mounting hole .250 2-56")
    (zone_connect 2)
    (fp_text reference X4 (at 0 -4.2) (layer F.SilkS) hide)
    (fp_text value HOLE_CONNECT (at 0 4.2) (layer F.Fab) hide)
    (fp_text user %R (at 1.35 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 5.5372 5.5372) (drill 2.4384) (layers *.Cu *.Mask)
      (net 9 CHASSIS) (clearance 0.1524) (zone_connect 2))
  )
  (module Aspera_footprints:HolePlated_2-56_0.23_standoff_smallest (layer F.Cu) (tedit 68D19D1D)
    (at 91.3 91.25)
    (descr "Mounting Hole 1/4\" pad, 2-56 hole")
    (tags "mounting hole .250 2-56")
    (zone_connect 2)
    (fp_text reference X3 (at 0 -4.2) (layer F.SilkS) hide)
    (fp_text value HOLE_CONNECT (at 0 4.2) (layer F.Fab) hide)
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 5.5372 5.5372) (drill 2.4384) (layers *.Cu *.Mask)
      (net 9 CHASSIS) (clearance 0.1524) (zone_connect 2))
  )
  (module Aspera_footprints:HolePlated_2-56_0.23_standoff_smallest (layer F.Cu) (tedit 68D19D36)
    (at 53.25 91.25)
    (descr "Mounting Hole 1/4\" pad, 2-56 hole")
    (tags "mounting hole .250 2-56")
    (zone_connect 2)
    (fp_text reference X2 (at 0 -4.2) (layer F.SilkS) hide)
    (fp_text value HOLE_CONNECT (at 0 4.2) (layer F.Fab) hide)
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 5.5372 5.5372) (drill 2.4384) (layers *.Cu *.Mask)
      (net 9 CHASSIS) (clearance 0.1524) (zone_connect 2))
  )
  (module Aspera_footprints:HolePlated_2-56_0.23_standoff_smallest (layer F.Cu) (tedit 68D19CED)
    (at 53.2 53.2)
    (descr "Mounting Hole 1/4\" pad, 2-56 hole")
    (tags "mounting hole .250 2-56")
    (zone_connect 2)
    (fp_text reference X1 (at 0 -4.2) (layer F.SilkS) hide)
    (fp_text value HOLE_CONNECT (at 0 4.2) (layer F.Fab) hide)
    (fp_text user %R (at 0.3 0) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 5.5372 5.5372) (drill 2.4384) (layers *.Cu *.Mask)
      (net 9 CHASSIS) (clearance 0.1524) (zone_connect 2))
  )
  (module Aspera_footprints:SOIC-16W_7.5x10.3mm_Pitch1.27mm (layer F.Cu) (tedit 68CDF42A)
    (at 75.35 74.6 180)
    (descr "16-Lead Plastic Small Outline (SO) - Wide, 7.50 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U1 (at 0 -6.25) (layer F.SilkS))
    (fp_text value AD704AR-16 (at 0 6.25) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 16 smd rect (at 4.65 -4.445 180) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 7 /PCB_top_level/HVPS1_Imon))
    (pad 15 smd rect (at 4.65 -3.175 180) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(C7-Pad2)"))
    (pad 14 smd rect (at 4.65 -1.905 180) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 24 /PCB_top_level/HVPS_STRIP_CSTATUS))
    (pad 13 smd rect (at 4.65 -0.635 180) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(C2-Pad2)"))
    (pad 12 smd rect (at 4.65 0.635 180) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 25 /PCB_top_level/HVPS_MCP_VSTATUS))
    (pad 11 smd rect (at 4.65 1.905 180) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(C6-Pad2)"))
    (pad 10 smd rect (at 4.65 3.175 180) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 /PCB_top_level/HVPS2_Vmon))
    (pad 9 smd rect (at 4.65 4.445 180) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask))
    (pad 8 smd rect (at -4.65 4.445 180) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask))
    (pad 7 smd rect (at -4.65 3.175 180) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 6 /PCB_top_level/HVPS1_Vmon))
    (pad 6 smd rect (at -4.65 1.905 180) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(C5-Pad2)"))
    (pad 5 smd rect (at -4.65 0.635 180) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 21 /PCB_top_level/HVPS_ANODE_VSTATUS))
    (pad 4 smd rect (at -4.65 -0.635 180) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(C1-Pad1)"))
    (pad 3 smd rect (at -4.65 -1.905 180) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 2 smd rect (at -4.65 -3.175 180) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(C8-Pad2)"))
    (pad 1 smd rect (at -4.65 -4.445 180) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 23 /PCB_top_level/HVPS_LEVSET))
    (model ${KIPRJMOD}/../../Libraries/Solid_models/SOIC-16W_7.5x10.3mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Aspera_footprints:GUSTO_R_0603_HandSoldering (layer F.Cu) (tedit 68CDF3C9)
    (at 83.85 78.1 90)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R5 (at -2.75 0 90) (layer F.SilkS))
    (fp_text value 10K (at 0 1.55 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd rect (at 1.1 0 90) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(C8-Pad2)"))
    (pad 1 smd rect (at -1.1 0 90) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 23 /PCB_top_level/HVPS_LEVSET))
    (model ${KIPRJMOD}/../../Libraries/Solid_models/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Aspera_footprints:GUSTO_R_0603_HandSoldering (layer F.Cu) (tedit 68CDF3C9)
    (at 60.8 78.1 90)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R14 (at -3.15 -0.09 270) (layer F.SilkS))
    (fp_text value 499K (at 0 1.55 270) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd rect (at 1.1 0 90) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 24 /PCB_top_level/HVPS_STRIP_CSTATUS))
    (pad 1 smd rect (at -1.1 0 90) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model ${KIPRJMOD}/../../Libraries/Solid_models/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Aspera_footprints:GUSTO_R_0603_HandSoldering (layer F.Cu) (tedit 68CDF3C9)
    (at 66.85 74.35)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R13 (at -3 0.05) (layer F.SilkS))
    (fp_text value 499K (at 0 1.55) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd rect (at 1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 25 /PCB_top_level/HVPS_MCP_VSTATUS))
    (pad 1 smd rect (at -1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model ${KIPRJMOD}/../../Libraries/Solid_models/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Aspera_footprints:GUSTO_R_0603_HandSoldering (layer F.Cu) (tedit 68CDF3C9)
    (at 83.6 74.35 180)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R12 (at -3.25 0) (layer F.SilkS))
    (fp_text value 499K (at 0 1.55) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 21 /PCB_top_level/HVPS_ANODE_VSTATUS))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model ${KIPRJMOD}/../../Libraries/Solid_models/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Aspera_footprints:GUSTO_R_0603_HandSoldering (layer F.Cu) (tedit 68CDF3C9)
    (at 77.65 65.15 180)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R11 (at 0.25 1.15) (layer F.SilkS))
    (fp_text value 10K (at 0 1.55) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd rect (at 1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(Q1-Pad1)"))
    (pad 1 smd rect (at -1.1 0 180) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model ${KIPRJMOD}/../../Libraries/Solid_models/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Aspera_footprints:GUSTO_R_0603_HandSoldering (layer F.Cu) (tedit 68CDF3C9)
    (at 69.15 65.4 90)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R10 (at 0.05 -1.31 270) (layer F.SilkS))
    (fp_text value 10K (at 0 1.55 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd rect (at 1.1 0 90) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 16 /PCB_top_level/+6.2V_HVPS))
    (pad 1 smd rect (at -1.1 0 90) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 26 /PCB_top_level/HVPS_EN_N))
    (model ${KIPRJMOD}/../../Libraries/Solid_models/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Aspera_footprints:GUSTO_R_0603_HandSoldering (layer F.Cu) (tedit 68CDF3C9)
    (at 77.65 66.9)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R9 (at -0.25 1.2) (layer F.SilkS))
    (fp_text value 10K (at 0 1.55) (layer F.Fab) hide)
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd rect (at 1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 20 /PCB_top_level/HVPS1_ON_OUT_5V))
    (pad 1 smd rect (at -1.1 0) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(Q1-Pad1)"))
    (model ${KIPRJMOD}/../../Libraries/Solid_models/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Aspera_footprints:GUSTO_R_0603_HandSoldering (layer F.Cu) (tedit 68CDF3C9)
    (at 62.85 78.1 90)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R8 (at -2.7 0.1 90) (layer F.SilkS))
    (fp_text value 10K (at 0 1.55 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd rect (at 1.1 0 90) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(C7-Pad2)"))
    (pad 1 smd rect (at -1.1 0 90) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model ${KIPRJMOD}/../../Libraries/Solid_models/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Aspera_footprints:GUSTO_R_0603_HandSoldering (layer F.Cu) (tedit 68CDF3C9)
    (at 62.85 71.6 270)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R7 (at -2.59 -0.1 90) (layer F.SilkS))
    (fp_text value 10K (at 0 1.55 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd rect (at 1.1 0 270) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(C6-Pad2)"))
    (pad 1 smd rect (at -1.1 0 270) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model ${KIPRJMOD}/../../Libraries/Solid_models/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Aspera_footprints:GUSTO_R_0603_HandSoldering (layer F.Cu) (tedit 68CDF3C9)
    (at 87.85 71.6 270)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R6 (at -2.6 0.05 90) (layer F.SilkS))
    (fp_text value 10K (at 0 1.55 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd rect (at 1.1 0 270) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(C5-Pad2)"))
    (pad 1 smd rect (at -1.1 0 270) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (model ${KIPRJMOD}/../../Libraries/Solid_models/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Aspera_footprints:GUSTO_R_0603_HandSoldering (layer F.Cu) (tedit 68CDF3C9)
    (at 87.85 78.1 90)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R1 (at -2.75 0 90) (layer F.SilkS))
    (fp_text value 20K (at 0 1.55 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd rect (at 1.1 0 90) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(C8-Pad2)"))
    (pad 1 smd rect (at -1.1 0 90) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 5 /PCB_top_level/HVPS1_Vset))
    (model ${KIPRJMOD}/../../Libraries/Solid_models/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Aspera_footprints:GUSTO_R_0603_HandSoldering (layer F.Cu) (tedit 68CDF3C9)
    (at 66.85 78.1 270)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R4 (at 2.7 0.06 90) (layer F.SilkS))
    (fp_text value 10K (at 0 1.55 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd rect (at 1.1 0 270) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 7 /PCB_top_level/HVPS1_Imon))
    (pad 1 smd rect (at -1.1 0 270) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(C7-Pad2)"))
    (model ${KIPRJMOD}/../../Libraries/Solid_models/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Aspera_footprints:GUSTO_R_0603_HandSoldering (layer F.Cu) (tedit 68CDF3C9)
    (at 66.85 71.6 90)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R3 (at 2.59 0.03 90) (layer F.SilkS))
    (fp_text value 10K (at 0 1.55 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd rect (at 1.1 0 90) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 8 /PCB_top_level/HVPS2_Vmon))
    (pad 1 smd rect (at -1.1 0 90) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(C6-Pad2)"))
    (model ${KIPRJMOD}/../../Libraries/Solid_models/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Aspera_footprints:GUSTO_R_0603_HandSoldering (layer F.Cu) (tedit 68CDF3C9)
    (at 83.85 71.6 90)
    (descr "Resistor SMD 0603, hand soldering")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R2 (at 2.6 0.05 90) (layer F.SilkS))
    (fp_text value 10K (at 0 1.55 90) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd rect (at 1.1 0 90) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 6 /PCB_top_level/HVPS1_Vmon))
    (pad 1 smd rect (at -1.1 0 90) (size 1.2 0.9) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(C5-Pad2)"))
    (model ${KIPRJMOD}/../../Libraries/Solid_models/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Aspera_footprints:SOT-23_Handsoldering (layer F.Cu) (tedit 68CDF392)
    (at 72.9 65.9 180)
    (descr "SOT-23, Handsoldering")
    (tags SOT-23)
    (attr smd)
    (fp_text reference Q1 (at 0.4 2.1) (layer F.SilkS))
    (fp_text value BC816-25HVL (at 0 2.5) (layer F.Fab) hide)
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 3 smd rect (at 1.5 0 180) (size 1.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 26 /PCB_top_level/HVPS_EN_N))
    (pad 2 smd rect (at -1.5 0.95 180) (size 1.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -1.5 -0.95 180) (size 1.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(Q1-Pad1)"))
    (model ${KIPRJMOD}/../../Libraries/Solid_models/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Aspera_footprints:SPM7054 (layer B.Cu) (tedit 68CDF353)
    (at 88.5 64.9 180)
    (fp_text reference L4 (at -4.9 -3.4) (layer B.SilkS))
    (fp_text value 100uH (at 0 -3.1) (layer B.Fab) hide)
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at -3.05 0 180) (size 3 3.3) (layers B.Cu B.Paste B.Mask)
      (net 18 /PCB_top_level/-6.2V_IN))
    (pad 2 smd rect (at 3.05 0 180) (size 3 3.3) (layers B.Cu B.Paste B.Mask)
      (net 17 /PCB_top_level/-6.2V_HVPS))
    (model ${KIPRJMOD}/../../Libraries/Solid_models/SPM7054.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Aspera_footprints:SPM7054 (layer B.Cu) (tedit 68CDF353)
    (at 64.1 80.6 180)
    (fp_text reference L3 (at 5.03 -3.12) (layer B.SilkS))
    (fp_text value 100uH (at 0 -3.1) (layer B.Fab) hide)
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at -3.05 0 180) (size 3 3.3) (layers B.Cu B.Paste B.Mask)
      (net 19 /PCB_top_level/+6.2V_IN))
    (pad 2 smd rect (at 3.05 0 180) (size 3 3.3) (layers B.Cu B.Paste B.Mask)
      (net 16 /PCB_top_level/+6.2V_HVPS))
    (model ${KIPRJMOD}/../../Libraries/Solid_models/SPM7054.step
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Aspera_footprints:GUSTO_L_1210_HandSoldering (layer B.Cu) (tedit 68CDF2F5)
    (at 87.7 70.9 180)
    (descr "Resistor SMD 1210, hand soldering")
    (tags "resistor 1210")
    (attr smd)
    (fp_text reference L2 (at -3.54 -2.22) (layer B.SilkS))
    (fp_text value 10uH (at 0 -2.7) (layer B.Fab) hide)
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd rect (at 2 0 180) (size 2 2.5) (layers B.Cu B.Paste B.Mask)
      (net 11 "Net-(C2-Pad2)"))
    (pad 1 smd rect (at -2 0 180) (size 2 2.5) (layers B.Cu B.Paste B.Mask)
      (net 18 /PCB_top_level/-6.2V_IN))
    (model ${KIPRJMOD}/../../Libraries/Solid_models/L_1210.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Aspera_footprints:GUSTO_L_1210_HandSoldering (layer B.Cu) (tedit 68CDF2F5)
    (at 85.4 82.2 180)
    (descr "Resistor SMD 1210, hand soldering")
    (tags "resistor 1210")
    (attr smd)
    (fp_text reference L1 (at 4.21 0.54) (layer B.SilkS))
    (fp_text value 10uH (at 0 -2.7) (layer B.Fab) hide)
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd rect (at 2 0 180) (size 2 2.5) (layers B.Cu B.Paste B.Mask)
      (net 10 "Net-(C1-Pad1)"))
    (pad 1 smd rect (at -2 0 180) (size 2 2.5) (layers B.Cu B.Paste B.Mask)
      (net 19 /PCB_top_level/+6.2V_IN))
    (model ${KIPRJMOD}/../../Libraries/Solid_models/L_1210.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Aspera_footprints:M80-54016YY (layer F.Cu) (tedit 68CDF2B3)
    (at 56.8 78.4 270)
    (descr M80-54016YY)
    (tags Connector)
    (fp_text reference J2 (at -12.25 -2 90) (layer F.SilkS))
    (fp_text value "Harwin M80, 2x8" (at 0 0 90) (layer F.SilkS) hide)
    (fp_text user %R (at -8.2 3.85 90) (layer F.Fab))
    (pad 18 thru_hole circle (at -17.5 1 270) (size 3.75 3.75) (drill 2.25) (layers *.Cu *.Mask))
    (pad 17 thru_hole circle (at 3.5 1 270) (size 3.75 3.75) (drill 2.25) (layers *.Cu *.Mask))
    (pad 16 thru_hole circle (at -14 2 270) (size 1.15 1.15) (drill 0.7) (layers *.Cu *.Mask)
      (net 17 /PCB_top_level/-6.2V_HVPS))
    (pad 15 thru_hole circle (at -12 2 270) (size 1.15 1.15) (drill 0.7) (layers *.Cu *.Mask)
      (net 26 /PCB_top_level/HVPS_EN_N))
    (pad 14 thru_hole circle (at -10 2 270) (size 1.15 1.15) (drill 0.7) (layers *.Cu *.Mask)
      (net 39 "Net-(J2-Pad14)"))
    (pad 13 thru_hole circle (at -8 2 270) (size 1.15 1.15) (drill 0.7) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 12 thru_hole circle (at -6 2 270) (size 1.15 1.15) (drill 0.7) (layers *.Cu *.Mask)
      (net 24 /PCB_top_level/HVPS_STRIP_CSTATUS))
    (pad 11 thru_hole circle (at -4 2 270) (size 1.15 1.15) (drill 0.7) (layers *.Cu *.Mask)
      (net 16 /PCB_top_level/+6.2V_HVPS))
    (pad 10 thru_hole circle (at -2 2 270) (size 1.15 1.15) (drill 0.7) (layers *.Cu *.Mask)
      (net 40 "Net-(J2-Pad10)"))
    (pad 9 thru_hole circle (at 0 2 270) (size 1.15 1.15) (drill 0.7) (layers *.Cu *.Mask)
      (net 3 /PCB_top_level/HVPS_TEMP1-))
    (pad 8 thru_hole circle (at -14 0 270) (size 1.15 1.15) (drill 0.7) (layers *.Cu *.Mask)
      (net 17 /PCB_top_level/-6.2V_HVPS))
    (pad 7 thru_hole circle (at -12 0 270) (size 1.15 1.15) (drill 0.7) (layers *.Cu *.Mask)
      (net 21 /PCB_top_level/HVPS_ANODE_VSTATUS))
    (pad 6 thru_hole circle (at -10 0 270) (size 1.15 1.15) (drill 0.7) (layers *.Cu *.Mask)
      (net 23 /PCB_top_level/HVPS_LEVSET))
    (pad 5 thru_hole circle (at -8 0 270) (size 1.15 1.15) (drill 0.7) (layers *.Cu *.Mask)
      (net 1 GND))
    (pad 4 thru_hole circle (at -6 0 270) (size 1.15 1.15) (drill 0.7) (layers *.Cu *.Mask)
      (net 25 /PCB_top_level/HVPS_MCP_VSTATUS))
    (pad 3 thru_hole circle (at -4 0 270) (size 1.15 1.15) (drill 0.7) (layers *.Cu *.Mask)
      (net 16 /PCB_top_level/+6.2V_HVPS))
    (pad 2 thru_hole circle (at -2 0 270) (size 1.15 1.15) (drill 0.7) (layers *.Cu *.Mask)
      (net 2 /PCB_top_level/HVPS_TEMP+))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.15 1.15) (drill 0.7) (layers *.Cu *.Mask)
      (net 4 /PCB_top_level/HVPS_TEMP2-))
    (model ${KIPRJMOD}/../../Libraries/Solid_models/m80-5401642_asm.stp
      (offset (xyz -7 -4.57 3.25))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Aspera_footprints:C_2220_HandSoldering (layer B.Cu) (tedit 68CDF260)
    (at 77.9 64.3)
    (descr "Capacitor SMD 2220, hand soldering")
    (tags "capacitor 2220")
    (attr smd)
    (fp_text reference C12 (at -6.6 0) (layer B.SilkS))
    (fp_text value 22uF (at 0 -3.75) (layer B.Fab) hide)
    (fp_text user %R (at 0 3.5) (layer B.Fab))
    (pad 2 smd rect (at 3.5 0) (size 2.4 5) (layers B.Cu B.Paste B.Mask)
      (net 17 /PCB_top_level/-6.2V_HVPS))
    (pad 1 smd rect (at -3.5 0) (size 2.4 5) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model ${KIPRJMOD}/../../Libraries/Solid_models/C_2220.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Aspera_footprints:C_2220_HandSoldering (layer B.Cu) (tedit 68CDF260)
    (at 64.3 73.9)
    (descr "Capacitor SMD 2220, hand soldering")
    (tags "capacitor 2220")
    (attr smd)
    (fp_text reference C11 (at 0.25 -3.75) (layer B.SilkS))
    (fp_text value 22uF (at 0 -3.75) (layer B.Fab) hide)
    (fp_text user %R (at 0 3.5) (layer B.Fab))
    (pad 2 smd rect (at 3.5 0) (size 2.4 5) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -3.5 0) (size 2.4 5) (layers B.Cu B.Paste B.Mask)
      (net 16 /PCB_top_level/+6.2V_HVPS))
    (model ${KIPRJMOD}/../../Libraries/Solid_models/C_2220.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Aspera_footprints:GUSTO_C_0603_HandSoldering (layer F.Cu) (tedit 68CDF219)
    (at 85.85 78.1 90)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C8 (at -2.75 0 90) (layer F.SilkS))
    (fp_text value 100pF (at 0 1.5 90) (layer F.Fab) hide)
    (fp_text user %R (at -0.05 0 90) (layer F.Fab))
    (pad 2 smd rect (at 0.95 0 90) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(C8-Pad2)"))
    (pad 1 smd rect (at -0.95 0 90) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 23 /PCB_top_level/HVPS_LEVSET))
    (model ${KIPRJMOD}/../../Libraries/Solid_models/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Aspera_footprints:GUSTO_C_0603_HandSoldering (layer F.Cu) (tedit 68CDF219)
    (at 64.85 78.1 90)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C7 (at -2.74 0.11 90) (layer F.SilkS))
    (fp_text value 100pF (at 0 1.5 90) (layer F.Fab) hide)
    (fp_text user %R (at -0.05 0 90) (layer F.Fab))
    (pad 2 smd rect (at 0.95 0 90) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(C7-Pad2)"))
    (pad 1 smd rect (at -0.95 0 90) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 7 /PCB_top_level/HVPS1_Imon))
    (model ${KIPRJMOD}/../../Libraries/Solid_models/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Aspera_footprints:GUSTO_C_0603_HandSoldering (layer F.Cu) (tedit 68CDF219)
    (at 64.85 71.6 270)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C6 (at -2.5 0.05 270) (layer F.SilkS))
    (fp_text value 100pF (at 0 1.5 90) (layer F.Fab) hide)
    (fp_text user %R (at -0.05 0 90) (layer F.Fab))
    (pad 2 smd rect (at 0.95 0 270) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(C6-Pad2)"))
    (pad 1 smd rect (at -0.95 0 270) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 8 /PCB_top_level/HVPS2_Vmon))
    (model ${KIPRJMOD}/../../Libraries/Solid_models/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Aspera_footprints:GUSTO_C_0603_HandSoldering (layer F.Cu) (tedit 68CDF219)
    (at 85.85 71.6 270)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C5 (at -2.6 0 90) (layer F.SilkS))
    (fp_text value 100pF (at 0 1.5 90) (layer F.Fab) hide)
    (fp_text user %R (at -0.05 0 90) (layer F.Fab))
    (pad 2 smd rect (at 0.95 0 270) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(C5-Pad2)"))
    (pad 1 smd rect (at -0.95 0 270) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 6 /PCB_top_level/HVPS1_Vmon))
    (model ${KIPRJMOD}/../../Libraries/Solid_models/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Aspera_footprints:GUSTO_C_1206_HandSoldering (layer B.Cu) (tedit 68CDF1C4)
    (at 81.4 73 90)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C4 (at -0.03 1.84 90) (layer B.SilkS))
    (fp_text value 10uF (at 0 -2 90) (layer B.Fab) hide)
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 1 smd rect (at -2 0 90) (size 2 1.6) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 2 smd rect (at 2 0 90) (size 2 1.6) (layers B.Cu B.Paste B.Mask)
      (net 11 "Net-(C2-Pad2)"))
    (model ${KIPRJMOD}/../../Libraries/Solid_models/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Aspera_footprints:GUSTO_C_1206_HandSoldering (layer B.Cu) (tedit 68CDF1C4)
    (at 76.4 82.7 180)
    (descr "Capacitor SMD 1206, hand soldering")
    (tags "capacitor 1206")
    (attr smd)
    (fp_text reference C3 (at 4.25 0) (layer B.SilkS))
    (fp_text value 10uF (at 0 -2) (layer B.Fab) hide)
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at -2 0 180) (size 2 1.6) (layers B.Cu B.Paste B.Mask)
      (net 10 "Net-(C1-Pad1)"))
    (pad 2 smd rect (at 2 0 180) (size 2 1.6) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model ${KIPRJMOD}/../../Libraries/Solid_models/C_1206.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Aspera_footprints:GUSTO_C_0805_HandSoldering (layer B.Cu) (tedit 68CDF13E)
    (at 52 65.6 90)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C10 (at 3.6 0 90) (layer B.SilkS))
    (fp_text value 0.1uF (at 0 -1.75 90) (layer B.Fab) hide)
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 2 smd rect (at 1.25 0 90) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 17 /PCB_top_level/-6.2V_HVPS))
    (pad 1 smd rect (at -1.25 0 90) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model ${KIPRJMOD}/../../Libraries/Solid_models/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Aspera_footprints:GUSTO_C_0805_HandSoldering (layer B.Cu) (tedit 68CDF13E)
    (at 52 73.1 90)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C9 (at -3.1 0 270) (layer B.SilkS))
    (fp_text value 0.1uF (at 0 -1.75 270) (layer B.Fab) hide)
    (fp_text user %R (at 0 0 270) (layer B.Fab))
    (pad 2 smd rect (at 1.25 0 90) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -1.25 0 90) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 16 /PCB_top_level/+6.2V_HVPS))
    (model ${KIPRJMOD}/../../Libraries/Solid_models/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Aspera_footprints:GUSTO_C_0805_HandSoldering (layer B.Cu) (tedit 68CDF13E)
    (at 79.2 72 90)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C2 (at 0 -1.5 90) (layer B.SilkS))
    (fp_text value 0.1uF (at 0 -1.75 90) (layer B.Fab) hide)
    (fp_text user %R (at 0 0 90) (layer B.Fab))
    (pad 2 smd rect (at 1.25 0 90) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 11 "Net-(C2-Pad2)"))
    (pad 1 smd rect (at -1.25 0 90) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (model ${KIPRJMOD}/../../Libraries/Solid_models/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Aspera_footprints:GUSTO_C_0805_HandSoldering (layer B.Cu) (tedit 68CDF13E)
    (at 77.2 80.6 180)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C1 (at 3.25 0) (layer B.SilkS))
    (fp_text value 0.1uF (at 0 -1.75) (layer B.Fab) hide)
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 2 smd rect (at 1.25 0 180) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 1 GND))
    (pad 1 smd rect (at -1.25 0 180) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 10 "Net-(C1-Pad1)"))
    (model ${KIPRJMOD}/../../Libraries/Solid_models/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Aspera_footprints:Steward_Logo (layer B.Cu) (tedit 5F2C1ACD)
    (at 89.46 75.68 180)
    (fp_text reference G1 (at 0 0 180) (layer B.SilkS) hide)
    (fp_text value STEWARD_LOGO (at 0.75 0 180) (layer B.SilkS) hide)
  )
  (gr_line (start 94.75 86.5) (end 101.1 86.5) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 94.75 86.5) (end 94.75 94.5) (layer Edge.Cuts) (width 0.1))
  (dimension 44.8 (width 0.15) (layer Dwgs.User)
    (gr_text "44.800 mm" (at 72.4 101.3) (layer Dwgs.User))
    (feature1 (pts (xy 94.8 88.4) (xy 94.8 100.586421)))
    (feature2 (pts (xy 50 88.4) (xy 50 100.586421)))
    (crossbar (pts (xy 50 100) (xy 94.8 100)))
    (arrow1a (pts (xy 94.8 100) (xy 93.673496 100.586421)))
    (arrow1b (pts (xy 94.8 100) (xy 93.673496 99.413579)))
    (arrow2a (pts (xy 50 100) (xy 51.126504 100.586421)))
    (arrow2b (pts (xy 50 100) (xy 51.126504 99.413579)))
  )
  (gr_line (start 60 50) (end 60 60.7) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 60 60.7) (end 101.1 60.7) (layer Edge.Cuts) (width 0.1))
  (gr_text "ASPERA-UA-DWG-00004a\nVersion 1.0a\n2025/10/24   D. Hamara" (at 87.1 65.4) (layer F.SilkS))
  (gr_text "Aspera Alice HVPS Interface Board" (at 77.9 62.3) (layer F.SilkS))
  (gr_text "STEWARD OBSERVATORY" (at 78.13 77.83) (layer B.SilkS))
  (gr_line (start 50 94.5) (end 50 50) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 94.75 94.5) (end 50 94.5) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 101.1 60.7) (end 101.1 86.5) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 50 50) (end 60 50) (layer Edge.Cuts) (width 0.1))
  (zone (net 1) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 101.25 86.5) (xy 94.75 86.5) (xy 94.75 94.5) (xy 50 94.5) (xy 50 50)
        (xy 60 50) (xy 60 60.75) (xy 101.25 60.75)
      )
    )
  )
  (zone (net 1) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508) (smoothing fillet) (radius 3.17))
    (polygon
      (pts
        (xy 101.165198 86.459956) (xy 94.665198 86.459956) (xy 87.16 86.46) (xy 87.16 94.43) (xy 57.52625 94.4225)
        (xy 57.53375 86.4575) (xy 50.0775 86.475) (xy 50.025 58.4175) (xy 58.335 58.4225) (xy 58.2775 61.239375)
        (xy 93.5025 61.220625) (xy 93.5525 67.928125) (xy 101.1075 67.891875)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 89.8 66.7) (xy 87.1 66.7) (xy 87.1 63) (xy 89.8 63)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 80 67) (xy 75.8 67) (xy 75.8 61.6) (xy 80 61.6)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 88.5 72.4) (xy 86.9 72.4) (xy 86.9 69.5) (xy 88.5 69.5)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 82.4 73.8) (xy 80.4 73.8) (xy 80.4 72.2) (xy 82.4 72.2)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 86.2 83.6) (xy 84.6 83.6) (xy 84.6 80.8) (xy 86.2 80.8)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 66.4 76.6) (xy 62.2 76.6) (xy 62.2 71.2) (xy 66.4 71.2)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 65.5 82.4) (xy 62.7 82.4) (xy 62.7 78.7) (xy 65.5 78.7)
      )
    )
  )
  (zone (net 0) (net_name "") (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (keepout (tracks allowed) (vias allowed) (copperpour not_allowed))
    (fill (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 77.2 83.7) (xy 75.6 83.7) (xy 75.6 81.7) (xy 77.2 81.7)
      )
    )
  )
)
