(kicad_pcb
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(general
		(thickness 4.69)
		(legacy_teardrops no)
	)
	(paper "A3")
	(title_block
		(date "2023-02-24")
		(rev "1")
	)
	(layers
		(0 "F.Cu" signal)
		(2 "B.Cu" signal)
		(9 "F.Adhes" user "F.Adhesive")
		(11 "B.Adhes" user "B.Adhesive")
		(13 "F.Paste" user)
		(15 "B.Paste" user)
		(5 "F.SilkS" user "F.Silkscreen")
		(7 "B.SilkS" user "B.Silkscreen")
		(1 "F.Mask" user)
		(3 "B.Mask" user)
		(17 "Dwgs.User" user "User.Drawings")
		(19 "Cmts.User" user "User.Comments")
		(21 "Eco1.User" user "User.Eco1")
		(23 "Eco2.User" user "User.Eco2")
		(25 "Edge.Cuts" user)
		(27 "Margin" user)
		(31 "F.CrtYd" user "F.Courtyard")
		(29 "B.CrtYd" user "B.Courtyard")
		(35 "F.Fab" user)
		(33 "B.Fab" user)
		(39 "User.1" user)
		(41 "User.2" user)
		(43 "User.3" user)
		(45 "User.4" user)
		(47 "User.5" user)
		(49 "User.6" user)
		(51 "User.7" user)
		(53 "User.8" user)
		(55 "User.9" user)
	)
	(setup
		(stackup
			(layer "F.SilkS"
				(type "Top Silk Screen")
				(color "White")
			)
			(layer "F.Paste"
				(type "Top Solder Paste")
			)
			(layer "F.Mask"
				(type "Top Solder Mask")
				(color "Green")
				(thickness 0.01)
			)
			(layer "F.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "dielectric 1"
				(type "core")
				(thickness 4.6)
				(material "FR4")
				(epsilon_r 4.5)
				(loss_tangent 0.02)
			)
			(layer "B.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "B.Mask"
				(type "Bottom Solder Mask")
				(color "Green")
				(thickness 0.01)
			)
			(layer "B.Paste"
				(type "Bottom Solder Paste")
			)
			(layer "B.SilkS"
				(type "Bottom Silk Screen")
				(color "White")
			)
			(copper_finish "None")
			(dielectric_constraints no)
		)
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(tenting front back)
		(pcbplotparams
			(layerselection 0x00000000_00000000_55555555_5755f5ff)
			(plot_on_all_layers_selection 0x00000000_00000000_00000000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 6)
			(plotframeref no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(pdf_metadata yes)
			(pdf_single_document no)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plot_black_and_white yes)
			(sketchpadsonfab no)
			(plotpadnumbers no)
			(hidednponfab no)
			(sketchdnponfab yes)
			(crossoutdnponfab yes)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 0)
			(scaleselection 1)
			(outputdirectory "gerbers/")
		)
	)
	(net 0 "")
	(net 1 "Net-(P3-Pin_2)")
	(net 2 "Net-(DB1-+)")
	(net 3 "/CA8")
	(net 4 "/CA9")
	(net 5 "/CA10")
	(net 6 "/CA11")
	(net 7 "/CA12")
	(net 8 "/CA13")
	(net 9 "/CA14")
	(net 10 "/CA15")
	(net 11 "/CA16")
	(net 12 "/CA17")
	(net 13 "/CA18")
	(net 14 "/CA19")
	(net 15 "/CA20")
	(net 16 "/CA21")
	(net 17 "/CA22")
	(net 18 "/CA23")
	(net 19 "unconnected-(U1-PP0-Pad19)")
	(net 20 "unconnected-(U1-PP1-Pad20)")
	(net 21 "unconnected-(U1-PP2-Pad21)")
	(net 22 "unconnected-(U1-PP3-Pad22)")
	(net 23 "unconnected-(U1-PP4-Pad23)")
	(net 24 "unconnected-(U1-PP5-Pad24)")
	(net 25 "Net-(P1-CIC3)")
	(net 26 "XIN")
	(net 27 "Net-(P1-CIC0)")
	(net 28 "Net-(P1-CIC2)")
	(net 29 "Net-(P1-CIC1)")
	(net 30 "Net-(U1-HBLANK)")
	(net 31 "Net-(U1-VBLANK)")
	(net 32 "Net-(U18-4.433M)")
	(net 33 "/D0")
	(net 34 "/D1")
	(net 35 "/D2")
	(net 36 "/D3")
	(net 37 "/D4")
	(net 38 "/D5")
	(net 39 "/D6")
	(net 40 "/D7")
	(net 41 "/{slash}PARD")
	(net 42 "/{slash}RAMSEL")
	(net 43 "unconnected-(U1-DMA-Pad70)")
	(net 44 "unconnected-(U1-CPUCK-Pad71)")
	(net 45 "Net-(U18-XOUT)")
	(net 46 "{slash}VAWR")
	(net 47 "{slash}VBWR")
	(net 48 "{slash}VRD")
	(net 49 "Net-(P1-REFRESH)")
	(net 50 "/{slash}PAWR")
	(net 51 "unconnected-(U1-R{slash}W-Pad80)")
	(net 52 "{slash}RESOUT0")
	(net 53 "unconnected-(U1-ML-Pad82)")
	(net 54 "unconnected-(U1-MF-Pad83)")
	(net 55 "unconnected-(U1-XF-Pad84)")
	(net 56 "unconnected-(U1-VPA-Pad86)")
	(net 57 "unconnected-(U1-VDA-Pad87)")
	(net 58 "unconnected-(U1-ALCK-Pad88)")
	(net 59 "unconnected-(U1-VP-Pad89)")
	(net 60 "/{slash}ROMSEL")
	(net 61 "/{slash}CPUWR")
	(net 62 "/CA0")
	(net 63 "/CA1")
	(net 64 "/CA2")
	(net 65 "/CA3")
	(net 66 "/CA4")
	(net 67 "/CA5")
	(net 68 "/CA6")
	(net 69 "Net-(C30-Pad1)")
	(net 70 "Net-(C30-Pad2)")
	(net 71 "/CA7")
	(net 72 "VCC")
	(net 73 "Net-(C31-Pad1)")
	(net 74 "Net-(C31-Pad2)")
	(net 75 "Net-(U3-5MOUT)")
	(net 76 "/{slash}CPURD")
	(net 77 "{slash}RESOUT1")
	(net 78 "Net-(J2-Audio)")
	(net 79 "SYSCK")
	(net 80 "unconnected-(U2-NC-Pad27)")
	(net 81 "/VA14")
	(net 82 "/VAB13")
	(net 83 "/VAB12")
	(net 84 "/VAB11")
	(net 85 "/VAB10")
	(net 86 "/VAB9")
	(net 87 "/VAB8")
	(net 88 "/VAB7")
	(net 89 "unconnected-(U2-VA15-Pad46)")
	(net 90 "/VAB6")
	(net 91 "/VAB5")
	(net 92 "/VAB4")
	(net 93 "/VAB3")
	(net 94 "/VAB2")
	(net 95 "/VAB1")
	(net 96 "/VAB0")
	(net 97 "/VAA13")
	(net 98 "/VAA12")
	(net 99 "/VAA11")
	(net 100 "/VAA10")
	(net 101 "/VAA9")
	(net 102 "/VAA8")
	(net 103 "/VAA7")
	(net 104 "/VAA6")
	(net 105 "/VAA5")
	(net 106 "/VAA4")
	(net 107 "/VAA3")
	(net 108 "/VAA2")
	(net 109 "/VAA1")
	(net 110 "/VAA0")
	(net 111 "unconnected-(U3-PED-Pad2)")
	(net 112 "unconnected-(U3-3.58M-Pad3)")
	(net 113 "unconnected-(U3-TOUMEI-Pad4)")
	(net 114 "unconnected-(U3-TST0-Pad77)")
	(net 115 "unconnected-(U3-TST1-Pad78)")
	(net 116 "unconnected-(U3-TST2-Pad79)")
	(net 117 "unconnected-(U3-TST3-Pad80)")
	(net 118 "unconnected-(U3-TST4-Pad81)")
	(net 119 "unconnected-(U3-TST5-Pad82)")
	(net 120 "unconnected-(U3-TST6-Pad84)")
	(net 121 "unconnected-(U3-TST7-Pad85)")
	(net 122 "unconnected-(U3-TST8-Pad86)")
	(net 123 "unconnected-(U3-TST9-Pad87)")
	(net 124 "unconnected-(U3-TST10-Pad88)")
	(net 125 "unconnected-(U3-TST11-Pad89)")
	(net 126 "Net-(P2-Pin_2)")
	(net 127 "GND")
	(net 128 "Net-(P2-Pin_3)")
	(net 129 "Net-(P2-Pin_4)")
	(net 130 "Net-(P2-Pin_5)")
	(net 131 "Net-(P2-Pin_6)")
	(net 132 "Net-(P2-Pin_7)")
	(net 133 "Net-(P2-Pin_8)")
	(net 134 "Net-(P2-Pin_9)")
	(net 135 "Net-(P2-Pin_10)")
	(net 136 "/VDB0")
	(net 137 "/VDB1")
	(net 138 "/VDB2")
	(net 139 "/VDB3")
	(net 140 "/VDB4")
	(net 141 "/VDB5")
	(net 142 "/VDB6")
	(net 143 "/VDB7")
	(net 144 "/VDA0")
	(net 145 "/VDA1")
	(net 146 "/VDA2")
	(net 147 "/VDA3")
	(net 148 "/VDA4")
	(net 149 "/VDA5")
	(net 150 "/VDA6")
	(net 151 "/VDA7")
	(net 152 "Net-(U7-VB)")
	(net 153 "unconnected-(U6-G-Pad55)")
	(net 154 "Net-(C9-Pad2)")
	(net 155 "Net-(U7-VC)")
	(net 156 "Net-(C11-Pad2)")
	(net 157 "Net-(U8-RES)")
	(net 158 "Net-(U8-P02)")
	(net 159 "unconnected-(U8-NC-Pad5)")
	(net 160 "unconnected-(U8-CL2-Pad6)")
	(net 161 "unconnected-(U8-P12-Pad12)")
	(net 162 "unconnected-(U8-P13-Pad13)")
	(net 163 "unconnected-(U8-NC-Pad14)")
	(net 164 "unconnected-(U8-P20-Pad15)")
	(net 165 "unconnected-(U8-P21-Pad16)")
	(net 166 "unconnected-(U8-P22-Pad17)")
	(net 167 "Net-(DA12-K)")
	(net 168 "Net-(DA15-K)")
	(net 169 "Net-(DA12-A-Pad2)")
	(net 170 "Net-(C7-Pad1)")
	(net 171 "Net-(C6-Pad1)")
	(net 172 "Net-(DA15-A-Pad2)")
	(net 173 "Net-(C13-Pad1)")
	(net 174 "Net-(U7-(B-Y)I)")
	(net 175 "Net-(U7-AR)")
	(net 176 "Net-(U7-AG)")
	(net 177 "Net-(C15-Pad1)")
	(net 178 "Net-(Q11-B)")
	(net 179 "Net-(U7-(R-Y)I)")
	(net 180 "Net-(Q10-B)")
	(net 181 "Net-(U7-YI)")
	(net 182 "Net-(J2-Video)")
	(net 183 "unconnected-(U7-VA-Pad15)")
	(net 184 "Net-(C18-Pad2)")
	(net 185 "unconnected-(U7-PHA-Pad17)")
	(net 186 "unconnected-(U7-PDO-Pad18)")
	(net 187 "Net-(Q12-B)")
	(net 188 "Net-(P1-SOUND-R)")
	(net 189 "Net-(Q10-E)")
	(net 190 "/MD0")
	(net 191 "/MD1")
	(net 192 "/MD2")
	(net 193 "/MD3")
	(net 194 "/MD4")
	(net 195 "/MD5")
	(net 196 "/MD6")
	(net 197 "/MD7")
	(net 198 "/MA0")
	(net 199 "/MA1")
	(net 200 "/MA2")
	(net 201 "/MA3")
	(net 202 "/MA4")
	(net 203 "Net-(U10D--)")
	(net 204 "/MA5")
	(net 205 "/MA6")
	(net 206 "/MA7")
	(net 207 "/MA12")
	(net 208 "/MA14")
	(net 209 "/MA10")
	(net 210 "/MA11")
	(net 211 "/MA9")
	(net 212 "/MA8")
	(net 213 "/MA13")
	(net 214 "Net-(U14-XTAL0)")
	(net 215 "Net-(U14-XTAL1)")
	(net 216 "Net-(U14-BCK)")
	(net 217 "Net-(U14-LRCK)")
	(net 218 "Net-(U14-DATA)")
	(net 219 "Net-(U10C--)")
	(net 220 "Net-(C74-Pad2)")
	(net 221 "Net-(C75-Pad2)")
	(net 222 "Net-(U10D-+)")
	(net 223 "/JPSTR")
	(net 224 "Net-(U13-CPUA4)")
	(net 225 "Net-(U13-CPUA3)")
	(net 226 "Net-(U13-CPUA2)")
	(net 227 "Net-(U13-CPUA1)")
	(net 228 "Net-(U13-CPUA0)")
	(net 229 "Net-(U13-CPUD7)")
	(net 230 "Net-(U13-CPUD6)")
	(net 231 "Net-(U13-CPUD5)")
	(net 232 "Net-(U13-CPUD4)")
	(net 233 "Net-(U13-CPUD3)")
	(net 234 "Net-(U13-CPUD2)")
	(net 235 "Net-(U13-CPUD1)")
	(net 236 "Net-(U13-CPUD0)")
	(net 237 "Net-(U13-PD3)")
	(net 238 "Net-(U13-PD2)")
	(net 239 "Net-(U13-CPUK)")
	(net 240 "Net-(U13-P57)")
	(net 241 "Net-(U13-P56)")
	(net 242 "Net-(U13-P55)")
	(net 243 "Net-(U13-P54)")
	(net 244 "Net-(U13-P53)")
	(net 245 "Net-(U13-P52)")
	(net 246 "Net-(U13-P51)")
	(net 247 "Net-(U13-P50)")
	(net 248 "unconnected-(U13-P47-Pad27)")
	(net 249 "unconnected-(U13-P46-Pad28)")
	(net 250 "unconnected-(U13-P45-Pad29)")
	(net 251 "unconnected-(U13-P44-Pad30)")
	(net 252 "unconnected-(U13-P43-Pad31)")
	(net 253 "unconnected-(U13-P42-Pad32)")
	(net 254 "unconnected-(U13-P41-Pad33)")
	(net 255 "unconnected-(U13-P40-Pad34)")
	(net 256 "Net-(U13-CPUA15)")
	(net 257 "Net-(U13-CPUA14)")
	(net 258 "Net-(U13-CPUA13)")
	(net 259 "Net-(U13-CPUA12)")
	(net 260 "Net-(U13-CPUA11)")
	(net 261 "Net-(U13-CPUA10)")
	(net 262 "Net-(U13-CPUA9)")
	(net 263 "Net-(U13-CPUA8)")
	(net 264 "Net-(U13-CPUA7)")
	(net 265 "Net-(U13-CPUA6)")
	(net 266 "Net-(U13-CPUA5)")
	(net 267 "unconnected-(U14-DKD-Pad1)")
	(net 268 "unconnected-(U14-MXK-Pad2)")
	(net 269 "unconnected-(U14-MX1-Pad3)")
	(net 270 "unconnected-(U14-MX2-Pad4)")
	(net 271 "unconnected-(U14-MX3-Pad5)")
	(net 272 "unconnected-(U14-MA15-Pad20)")
	(net 273 "unconnected-(U14-DIP-Pad21)")
	(net 274 "/JPCLK2")
	(net 275 "unconnected-(U14-MCK-Pad40)")
	(net 276 "unconnected-(U14-SCLK-Pad41)")
	(net 277 "/JPCLK1")
	(net 278 "unconnected-(U14-XCK-Pad77)")
	(net 279 "unconnected-(U14-CK1-Pad79)")
	(net 280 "unconnected-(U14-CK2-Pad80)")
	(net 281 "/4016.D1")
	(net 282 "unconnected-(U17-A.GND-Pad5)")
	(net 283 "Net-(C77-Pad2)")
	(net 284 "/4016.D0")
	(net 285 "/4017.D1")
	(net 286 "/4017.D0")
	(net 287 "EXTLATCH")
	(net 288 "/JPIO6")
	(net 289 "Net-(P4-Audio-L)")
	(net 290 "Net-(P4-Audio-R)")
	(net 291 "Net-(C1-Pad2)")
	(net 292 "Net-(C3-Pad2)")
	(net 293 "Net-(R1-Pad2)")
	(net 294 "Net-(R2-Pad1)")
	(net 295 "Net-(R3-Pad2)")
	(net 296 "Net-(U18-3.546M)")
	(net 297 "~{RESET}")
	(net 298 "+9V")
	(net 299 "Net-(U1-JOY-OUT1)")
	(net 300 "Net-(U1-JOY-OUT2)")
	(net 301 "Net-(DA11-A)")
	(net 302 "Net-(DA11-common)")
	(net 303 "Net-(DA11-K)")
	(net 304 "+12V")
	(net 305 "unconnected-(D1B-K-Pad2)")
	(net 306 "unconnected-(DA1B-K-Pad2)")
	(net 307 "/PA0")
	(net 308 "/PA2")
	(net 309 "/PA4")
	(net 310 "/PA1")
	(net 311 "/PA3")
	(net 312 "/PA5")
	(net 313 "/PA6")
	(net 314 "/PA7")
	(net 315 "Net-(P1-SOUND-L)")
	(net 316 "CHR3")
	(net 317 "CHR2")
	(net 318 "CHR1")
	(net 319 "CHR0")
	(net 320 "PRIO1")
	(net 321 "PRIO0")
	(net 322 "COLOR2")
	(net 323 "COLOR1")
	(net 324 "COLOR0")
	(net 325 "VCLD")
	(net 326 "HCLD")
	(net 327 "5MIN")
	(net 328 "OVER")
	(net 329 "FIELD")
	(net 330 "Net-(U10C-+)")
	(net 331 "Net-(U17-R.OUT)")
	(net 332 "Net-(U17-L.OUT)")
	(net 333 "Net-(C23-Pad1)")
	(net 334 "Net-(C26-Pad1)")
	(net 335 "Net-(C78-Pad2)")
	(net 336 "{slash}IRQ")
	(net 337 "Net-(P5-DOTCK)")
	(net 338 "Net-(P5-SMPCK)")
	(net 339 "Net-(P5-MONO-OUT)")
	(net 340 "Net-(P5-SL-IN)")
	(net 341 "Net-(P5-SR-IN)")
	(net 342 "Net-(C24-Pad1)")
	(net 343 "Net-(DA6A-A)")
	(net 344 "Net-(C25-Pad1)")
	(net 345 "Net-(Q9-B)")
	(net 346 "Net-(C27-Pad1)")
	(net 347 "Net-(Q3-E)")
	(net 348 "Net-(C28-Pad1)")
	(net 349 "Net-(Q3-B)")
	(net 350 "Net-(Q14-B)")
	(net 351 "Net-(Q15-B)")
	(net 352 "Net-(P1-EXPAND)")
	(net 353 "Net-(Q4-E)")
	(net 354 "Net-(Q4-B)")
	(net 355 "Net-(Q5-E)")
	(net 356 "Net-(Q5-B)")
	(net 357 "Net-(Q6-E)")
	(net 358 "Net-(Q6-B)")
	(net 359 "Net-(Q9-E)")
	(net 360 "Net-(Q11-E)")
	(net 361 "Net-(Q12-E)")
	(net 362 "Net-(U7-CO)")
	(net 363 "Net-(U7-YO)")
	(net 364 "Net-(U7-(B-Y)O)")
	(net 365 "Net-(U7-(R-Y)O)")
	(net 366 "Net-(C8-Pad1)")
	(net 367 "Net-(U7-AB)")
	(net 368 "Net-(Q14-E)")
	(net 369 "Net-(Q14-C)")
	(net 370 "Net-(Q15-E)")
	(net 371 "Net-(Q15-C)")
	(net 372 "Net-(Q16-E)")
	(net 373 "Net-(U7-BLA)")
	(net 374 "Net-(U3-BURST)")
	(net 375 "Net-(U3-CSYNC)")
	(net 376 "/{slash}SCE1")
	(net 377 "/{slash}SCE0")
	(net 378 "/{slash}SOE")
	(net 379 "/{slash}SWE")
	(net 380 "Net-(C66-Pad2)")
	(net 381 "Net-(Q13-B)")
	(net 382 "Net-(U14-~{MUTE})")
	(net 383 "Net-(Q7-E)")
	(net 384 "Net-(Q7-B)")
	(net 385 "Net-(Q8-E)")
	(net 386 "Net-(Q8-B)")
	(net 387 "Net-(Q13-C)")
	(net 388 "Net-(U13-T1)")
	(net 389 "Net-(U13-T0)")
	(net 390 "Net-(U3-RESOUT1)")
	(net 391 "unconnected-(U14-TF-Pad37)")
	(net 392 "unconnected-(U14-TK-Pad38)")
	(net 393 "unconnected-(U17-LRCK{slash}WDCK-Pad13)")
	(net 394 "Net-(Q17-E)")
	(net 395 "Net-(C65-Pad1)")
	(net 396 "Net-(Q18-B)")
	(net 397 "Net-(DA17-K)")
	(net 398 "Net-(DA17-A-Pad2)")
	(net 399 "Net-(DA16-K)")
	(net 400 "Net-(DA16-A-Pad2)")
	(net 401 "Net-(DA13-K)")
	(net 402 "Net-(DA19-K)")
	(net 403 "Net-(U18-Pad8)")
	(net 404 "Net-(DA13-A-Pad2)")
	(net 405 "Net-(DA19-A-Pad2)")
	(net 406 "Net-(C2-Pad2)")
	(net 407 "Net-(U13-P5RD)")
	(net 408 "Net-(J3-Pin_1)")
	(net 409 "Net-(J3-Pin_2)")
	(net 410 "Net-(J3-Pin_3)")
	(net 411 "Net-(J3-Pin_4)")
	(net 412 "Net-(J3-Pin_7)")
	(net 413 "Net-(J3-Pin_8)")
	(net 414 "Net-(J3-Pin_9)")
	(net 415 "Net-(J3-Pin_10)")
	(net 416 "Net-(J3-Pin_11)")
	(net 417 "Net-(J3-Pin_12)")
	(net 418 "Net-(D3-K)")
	(net 419 "Net-(LED1-A)")
	(net 420 "Net-(D2-K)")
	(net 421 "Net-(D2-A)")
	(net 422 "Net-(D4-A)")
	(net 423 "Net-(D5-A)")
	(net 424 "Net-(D6-A)")
	(net 425 "Net-(D7-A)")
	(net 426 "Net-(J4-Pin_4)")
	(net 427 "Net-(J4-Pin_6)")
	(net 428 "Net-(J5-Pin_4)")
	(net 429 "Net-(J5-Pin_5)")
	(net 430 "Net-(J4-Pin_5)")
	(net 431 "Net-(D4-K)")
	(net 432 "Net-(D5-K)")
	(net 433 "Net-(D6-K)")
	(net 434 "Net-(J5-Pin_6)")
	(footprint "SNES_Library:SOIC-18_7x12mm_P0,8mm"
		(layer "F.Cu")
		(at 225.507 188.17)
		(property "Reference" "U8"
			(at 3.601 -6.56 270)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "CIC"
			(at 0.045 -0.464 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -5.5 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -4.4 -3.6 90)
			(size 1 2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 29 "Net-(P1-CIC1)")
			(pinfunction "P00")
			(pintype "bidirectional")
		)
		(pad "2" smd rect
			(at -4.4 -2.4 90)
			(size 0.4 2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 27 "Net-(P1-CIC0)")
			(pinfunction "P01")
			(pintype "bidirectional")
		)
		(pad "3" smd rect
			(at -4.4 -1.6 90)
			(size 0.4 2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 158 "Net-(U8-P02)")
			(pinfunction "P02")
			(pintype "input")
		)
		(pad "4" smd rect
			(at -4.4 -0.8 90)
			(size 0.4 2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 72 "VCC")
			(pinfunction "P03")
			(pintype "input")
		)
		(pad "5" smd rect
			(at -4.4 0 90)
			(size 0.4 2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 159 "unconnected-(U8-NC-Pad5)")
			(pinfunction "NC")
			(pintype "no_connect")
		)
		(pad "6" smd rect
			(at -4.4 0.8 90)
			(size 0.4 2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 160 "unconnected-(U8-CL2-Pad6)")
			(pinfunction "CL2")
			(pintype "unspecified+no_connect")
		)
		(pad "7" smd rect
			(at -4.4 1.6 90)
			(size 0.4 2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 296 "Net-(U18-3.546M)")
			(pinfunction "CL1")
			(pintype "input")
		)
		(pad "8" smd rect
			(at -4.4 2.4 90)
			(size 0.4 2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 157 "Net-(U8-RES)")
			(pinfunction "RES")
			(pintype "input")
		)
		(pad "9" smd rect
			(at -4.4 3.6 90)
			(size 1 2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 127 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "10" smd rect
			(at 4.4 3.6 90)
			(size 1 2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 297 "~{RESET}")
			(pinfunction "P10")
			(pintype "output")
		)
		(pad "11" smd rect
			(at 4.4 2.4 90)
			(size 0.4 2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 28 "Net-(P1-CIC2)")
			(pinfunction "P11")
			(pintype "output")
		)
		(pad "12" smd rect
			(at 4.4 1.6 90)
			(size 0.4 2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 161 "unconnected-(U8-P12-Pad12)")
			(pinfunction "P12")
			(pintype "unspecified+no_connect")
		)
		(pad "13" smd rect
			(at 4.4 0.8 90)
			(size 0.4 2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 162 "unconnected-(U8-P13-Pad13)")
			(pinfunction "P13")
			(pintype "unspecified+no_connect")
		)
		(pad "14" smd rect
			(at 4.4 0 90)
			(size 0.4 2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 163 "unconnected-(U8-NC-Pad14)")
			(pinfunction "NC")
			(pintype "no_connect")
		)
		(pad "15" smd rect
			(at 4.4 -0.8 90)
			(size 0.4 2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 164 "unconnected-(U8-P20-Pad15)")
			(pinfunction "P20")
			(pintype "unspecified+no_connect")
		)
		(pad "16" smd rect
			(at 4.4 -1.6 90)
			(size 0.4 2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 165 "unconnected-(U8-P21-Pad16)")
			(pinfunction "P21")
			(pintype "unspecified+no_connect")
		)
		(pad "17" smd rect
			(at 4.4 -2.4 90)
			(size 0.4 2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 166 "unconnected-(U8-P22-Pad17)")
			(pinfunction "P22")
			(pintype "unspecified+no_connect")
		)
		(pad "18" smd rect
			(at 4.4 -3.6 90)
			(size 1 2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 72 "VCC")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(embedded_fonts no)
		(model "${KICAD7_3DMODEL_DIR}/Package_SO.3dshapes/ETSSOP-20-1EP_4.4x6.5mm_P0.65mm_EP3x4.2mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_THT:C_Axial_L3.8mm_D2.6mm_P7.50mm_Horizontal"
		(layer "F.Cu")
		(at 275.1074 103.4542 -90)
		(descr "C, Axial series, Axial, Horizontal, pin pitch=7.5mm, length*diameter=3.8*2.6mm^2, http://www.vishay.com/docs/45231/arseries.pdf")
		(tags "C Axial series Axial Horizontal pin pitch 7.5mm  length 3.8mm diameter 2.6mm")
		(property "Reference" "C21"
			(at -2.2352 -0.1016 90)
			(layer "F.SilkS")
		)
		(property "Value" "C"
			(at 3.75 2.42 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 3.75 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 127 "GND")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 7.5 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 423 "Net-(D5-A)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Axial_L3.8mm_D2.6mm_P7.50mm_Horizontal.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "SNES_Library:Fuse"
		(layer "F.Cu")
		(at 108.966 208.534)
		(property "Reference" "F1"
			(at 0 -3.429 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "Fuse"
			(at 0 -1.5 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Fuse"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*Fuse*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -7.62 0)
			(size 3.048 6.096)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "Net-(DB1-+)")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 7.62 0)
			(size 3.048 6.096)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "Net-(P3-Pin_2)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD7_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P7.62mm_Horizontal.wrl"
			(offset
				(xyz -3.5 0 -0.5)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MountingHole:MountingHole_2.5mm"
		(layer "F.Cu")
		(at 271.5514 172.5422 180)
		(descr "Mounting Hole 2.5mm, no annular, generated by kicad-footprint-generator mountinghole.py")
		(tags "mountinghole")
		(property "Reference" "H2"
			(at 0 -3.5 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "MountingHole"
			(at 0 3.5 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Mounting Hole without connection"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "MountingHole*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr exclude_from_pos_files)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole circle
			(at 0 0 180)
			(size 2.5 2.5)
			(drill 2.5)
			(layers "*.Cu" "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "Capacitor_THT:CP_Radial_D16.0mm_P7.50mm"
		(layer "F.Cu")
		(at 114.45 178.4)
		(descr "CP, Radial series, Radial, pin pitch=7.50mm, diameter=16mm, height=25mm, Electrolytic Capacitor")
		(tags "CP Radial series Radial pin pitch 7.50mm diameter 16mm height 25mm Electrolytic Capacitor")
		(property "Reference" "C67"
			(at 3.75 -9.25 0)
			(layer "F.SilkS")
		)
		(property "Value" "2200uF"
			(at 3.75 9.25 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Polarized capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "CP_*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 3.75 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole roundrect
			(at 0 0)
			(size 2.4 2.4)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.104167)
			(net 2 "Net-(DB1-+)")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 7.5 0)
			(size 2.4 2.4)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 127 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_THT.3dshapes/CP_Radial_D16.0mm_P7.50mm.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Diode_SMD:D_3220_8050Metric"
		(layer "F.Cu")
		(at 120.4375 190)
		(descr "Diode SMD 3220 (8050 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size from: http://datasheets.avx.com/schottky.pdf), generated with kicad-footprint-generator")
		(tags "diode")
		(property "Reference" "VA1"
			(at 0 4 0)
			(layer "F.SilkS")
		)
		(property "Value" "Varistor"
			(at 0 3.52 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Voltage dependent resistor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Device" "SUBCKT"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Library" "${KICAD7_SYMBOL_DIR}/Simulation_SPICE.sp"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Name" "kicad_builtin_varistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Params" "threshold=1k"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" "1=A 2=B"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "RV_* Varistor*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -3.1875 0)
			(size 2.475 5.15)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.10101)
			(net 303 "Net-(DA11-K)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 3.1875 0)
			(size 2.475 5.15)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.10101)
			(net 127 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Diode_SMD.3dshapes/D_3220_8050Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_Elec_6.3x5.4"
		(layer "F.Cu")
		(at 94.625 126.0875 -90)
		(descr "SMD capacitor, aluminum electrolytic nonpolar, 6.3x5.4mm")
		(tags "capacitor electrolytic nonpolar")
		(property "Reference" "C65"
			(at 0.2125 4.525 90)
			(layer "F.SilkS")
		)
		(property "Value" "10u 50V"
			(at 0 4.35 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Polarized capacitor"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "CP_*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -2.5375 0 270)
			(size 3.325 1.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.15625)
			(net 395 "Net-(C65-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 2.5375 0 270)
			(size 3.325 1.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.15625)
			(net 290 "Net-(P4-Audio-R)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_Elec_6.3x5.4.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_SO:SO-14_3.9x8.65mm_P1.27mm"
		(layer "F.Cu")
		(at 118.364 152.973 90)
		(descr "SO, 14 Pin (https://www.st.com/resource/en/datasheet/l6491.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SO SO")
		(property "Reference" "U10"
			(at 7.177 0 180)
			(layer "F.SilkS")
		)
		(property "Value" "LM324"
			(at 0 5.28 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm2902-n.pdf"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Low-Power, Quad-Operational Amplifiers, DIP-14/SOIC-14/SSOP-14"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SOIC*3.9x8.7mm*P1.27mm* DIP*W7.62mm* TSSOP*4.4x5mm*P0.65mm* SSOP*5.3x6.2mm*P0.65mm* MSOP*3x3mm*P0.5mm*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -2.475 -3.81 90)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 371 "Net-(Q15-C)")
			(pintype "output")
		)
		(pad "2" smd roundrect
			(at -2.475 -2.54 90)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 370 "Net-(Q15-E)")
			(pinfunction "-")
			(pintype "input")
		)
		(pad "3" smd roundrect
			(at -2.475 -1.27 90)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 343 "Net-(DA6A-A)")
			(pinfunction "+")
			(pintype "input")
		)
		(pad "4" smd roundrect
			(at -2.475 0 90)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 298 "+9V")
			(pinfunction "V+")
			(pintype "power_in")
		)
		(pad "5" smd roundrect
			(at -2.475 1.27 90)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 343 "Net-(DA6A-A)")
			(pinfunction "+")
			(pintype "input")
		)
		(pad "6" smd roundrect
			(at -2.475 2.54 90)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 368 "Net-(Q14-E)")
			(pinfunction "-")
			(pintype "input")
		)
		(pad "7" smd roundrect
			(at -2.475 3.81 90)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 369 "Net-(Q14-C)")
			(pintype "output")
		)
		(pad "8" smd roundrect
			(at 2.475 3.81 90)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 219 "Net-(U10C--)")
			(pintype "output")
		)
		(pad "9" smd roundrect
			(at 2.475 2.54 90)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 219 "Net-(U10C--)")
			(pinfunction "-")
			(pintype "input")
		)
		(pad "10" smd roundrect
			(at 2.475 1.27 90)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 330 "Net-(U10C-+)")
			(pinfunction "+")
			(pintype "input")
		)
		(pad "11" smd roundrect
			(at 2.475 0 90)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 127 "GND")
			(pinfunction "V-")
			(pintype "power_in")
		)
		(pad "12" smd roundrect
			(at 2.475 -1.27 90)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 222 "Net-(U10D-+)")
			(pinfunction "+")
			(pintype "input")
		)
		(pad "13" smd roundrect
			(at 2.475 -2.54 90)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 203 "Net-(U10D--)")
			(pinfunction "-")
			(pintype "input")
		)
		(pad "14" smd roundrect
			(at 2.475 -3.81 90)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 203 "Net-(U10D--)")
			(pintype "output")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Package_SO.3dshapes/SO-14_3.9x8.65mm_P1.27mm.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "SNES_Library:AVOut_Internal"
		(layer "F.Cu")
		(at 175.895 67.526 180)
		(property "Reference" "P6"
			(at 0 -0.5 180)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "~"
			(at 0 1 180)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 2.5 180)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 6.35 8.89 180)
			(size 2.032 10)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 408 "Net-(J3-Pin_1)")
			(pinfunction "Red")
			(pintype "unspecified")
		)
		(pad "2" smd rect
			(at 6.35 8.89 180)
			(size 2.032 10)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 409 "Net-(J3-Pin_2)")
			(pinfunction "Green")
			(pintype "unspecified")
		)
		(pad "3" smd rect
			(at 3.81 8.89 180)
			(size 2.032 10)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 410 "Net-(J3-Pin_3)")
			(pinfunction "CSYNC")
			(pintype "unspecified")
		)
		(pad "4" smd rect
			(at 3.81 8.89 180)
			(size 2.032 10)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 411 "Net-(J3-Pin_4)")
			(pinfunction "Blue")
			(pintype "unspecified")
		)
		(pad "5" smd rect
			(at 1.27 8.89 180)
			(size 2.032 10)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 127 "GND")
			(pinfunction "GND")
			(pintype "unspecified")
		)
		(pad "6" smd rect
			(at 1.27 8.89 180)
			(size 2.032 10)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 127 "GND")
			(pinfunction "GND")
			(pintype "unspecified")
		)
		(pad "7" smd rect
			(at -1.27 8.89 180)
			(size 2.032 10)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 412 "Net-(J3-Pin_7)")
			(pinfunction "Y-SV")
			(pintype "unspecified")
		)
		(pad "8" smd rect
			(at -1.27 8.89 180)
			(size 2.032 10)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 413 "Net-(J3-Pin_8)")
			(pinfunction "C-SV")
			(pintype "unspecified")
		)
		(pad "9" smd rect
			(at -3.81 8.89 180)
			(size 2.032 10)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 414 "Net-(J3-Pin_9)")
			(pinfunction "CV")
			(pintype "unspecified")
		)
		(pad "10" smd rect
			(at -3.81 8.89 180)
			(size 2.032 10)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 415 "Net-(J3-Pin_10)")
			(pinfunction "VCC")
			(pintype "unspecified")
		)
		(pad "11" smd rect
			(at -6.35 8.89 180)
			(size 2.032 10)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 416 "Net-(J3-Pin_11)")
			(pinfunction "Audio-L")
			(pintype "unspecified")
		)
		(pad "12" smd rect
			(at -6.35 8.89 180)
			(size 2.032 10)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 417 "Net-(J3-Pin_12)")
			(pinfunction "Audio-R")
			(pintype "unspecified")
		)
		(embedded_fonts no)
	)
	(footprint "Package_TO_SOT_THT:TO-220-3_Vertical"
		(layer "F.Cu")
		(at 113.72 201.05)
		(descr "TO-220-3, Vertical, RM 2.54mm, see https://www.vishay.com/docs/66542/to-220-1.pdf, generated with kicad-footprint-generator TO_SOT_THT_generate.py")
		(tags "TO-220-3 Vertical RM 2.54mm")
		(property "Reference" "U12"
			(at -0.055 -3.692 0)
			(layer "F.SilkS")
		)
		(property "Value" "L7805"
			(at 2.54 -1.88 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "http://www.st.com/content/ccc/resource/technical/document/datasheet/41/4f/b3/b0/12/d4/47/88/CD00000444.pdf/files/CD00000444.pdf/jcr:content/translations/en.CD00000444.pdf"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Positive 1.5A 35V Linear Regulator, Fixed Output 5V, TO-220/TO-263/TO-252"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TO?252* TO?263* TO?220*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at -0.055 -3.692 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.905 2)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 303 "Net-(DA11-K)")
			(pinfunction "IN")
			(pintype "power_in")
		)
		(pad "2" thru_hole oval
			(at 2.54 0)
			(size 1.905 2)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 127 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "3" thru_hole oval
			(at 5.08 0)
			(size 1.905 2)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 72 "VCC")
			(pinfunction "OUT")
			(pintype "power_out")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Package_TO_SOT_THT.3dshapes/TO-220-3_Vertical.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "SNES_Library:EXPANSION"
		(layer "F.Cu")
		(at 100.15 95.5 -90)
		(property "Reference" "P5"
			(at 0 -0.5 270)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "~"
			(at 0 1 270)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr through_hole)
		(fp_text user "28"
			(at -14.224 17.78 270)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "27"
			(at -14.224 2.794 270)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "1"
			(at 12.446 2.794 270)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "10"
			(at 3.81 17.78 270)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "2"
			(at 12.446 17.78 270)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "20"
			(at -6.35 17.78 270)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "5"
			(at 8.382 2.794 270)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "15"
			(at -2.286 2.794 270)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "${REFERENCE}"
			(at 0 2.5 270)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" thru_hole oval
			(at 13 5)
			(size 2 1.7)
			(drill oval 0.8 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 307 "/PA0")
			(pinfunction "PA0")
			(pintype "unspecified")
		)
		(pad "2" thru_hole oval
			(at 13 14)
			(size 2 1.7)
			(drill oval 0.8 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 310 "/PA1")
			(pinfunction "PA1")
			(pintype "unspecified")
		)
		(pad "3" thru_hole oval
			(at 11 5)
			(size 2 1.7)
			(drill oval 0.8 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 308 "/PA2")
			(pinfunction "PA2")
			(pintype "unspecified")
		)
		(pad "4" thru_hole oval
			(at 11 14)
			(size 2 1.7)
			(drill oval 0.8 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 311 "/PA3")
			(pinfunction "PA3")
			(pintype "unspecified")
		)
		(pad "5" thru_hole oval
			(at 9 5)
			(size 2 1.7)
			(drill oval 0.8 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 309 "/PA4")
			(pinfunction "PA4")
			(pintype "unspecified")
		)
		(pad "6" thru_hole oval
			(at 9 14)
			(size 2 1.7)
			(drill oval 0.8 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 312 "/PA5")
			(pinfunction "PA5")
			(pintype "unspecified")
		)
		(pad "7" thru_hole oval
			(at 7 5)
			(size 2 1.7)
			(drill oval 0.8 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 313 "/PA6")
			(pinfunction "PA6")
			(pintype "unspecified")
		)
		(pad "8" thru_hole oval
			(at 7 14)
			(size 2 1.7)
			(drill oval 0.8 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 314 "/PA7")
			(pinfunction "PA7")
			(pintype "unspecified")
		)
		(pad "9" thru_hole oval
			(at 5 5)
			(size 2 1.7)
			(drill oval 0.8 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 50 "/{slash}PAWR")
			(pinfunction "~{PAWR}")
			(pintype "unspecified")
		)
		(pad "10" thru_hole oval
			(at 5 14)
			(size 2 1.7)
			(drill oval 0.8 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 41 "/{slash}PARD")
			(pinfunction "~{PARD}")
			(pintype "unspecified")
		)
		(pad "11" thru_hole oval
			(at 3 5)
			(size 2 1.7)
			(drill oval 0.8 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 33 "/D0")
			(pinfunction "D0")
			(pintype "unspecified")
		)
		(pad "12" thru_hole oval
			(at 3 14)
			(size 2 1.7)
			(drill oval 0.8 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 34 "/D1")
			(pinfunction "D1")
			(pintype "unspecified")
		)
		(pad "13" thru_hole oval
			(at 1 5)
			(size 2 1.7)
			(drill oval 0.8 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 35 "/D2")
			(pinfunction "D2")
			(pintype "unspecified")
		)
		(pad "14" thru_hole oval
			(at 1 14)
			(size 2 1.7)
			(drill oval 0.8 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 36 "/D3")
			(pinfunction "D3")
			(pintype "unspecified")
		)
		(pad "15" thru_hole oval
			(at -1 5)
			(size 2 1.7)
			(drill oval 0.8 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 37 "/D4")
			(pinfunction "D4")
			(pintype "unspecified")
		)
		(pad "16" thru_hole oval
			(at -1 14)
			(size 2 1.7)
			(drill oval 0.8 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 38 "/D5")
			(pinfunction "D5")
			(pintype "unspecified")
		)
		(pad "17" thru_hole oval
			(at -3 5)
			(size 2 1.7)
			(drill oval 0.8 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 39 "/D6")
			(pinfunction "D6")
			(pintype "unspecified")
		)
		(pad "18" thru_hole oval
			(at -3 14)
			(size 2 1.7)
			(drill oval 0.8 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 40 "/D7")
			(pinfunction "D7")
			(pintype "unspecified")
		)
		(pad "19" thru_hole oval
			(at -5 5)
			(size 2 1.7)
			(drill oval 0.8 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 77 "{slash}RESOUT1")
			(pinfunction "~{RESET}")
			(pintype "unspecified")
		)
		(pad "20" thru_hole oval
			(at -5 14)
			(size 2 1.7)
			(drill oval 0.8 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 72 "VCC")
			(pinfunction "Vcc")
			(pintype "power_in")
		)
		(pad "21" thru_hole oval
			(at -7 5)
			(size 2 1.7)
			(drill oval 0.8 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 338 "Net-(P5-SMPCK)")
			(pinfunction "SMPCK")
			(pintype "unspecified")
		)
		(pad "22" thru_hole oval
			(at -7 14)
			(size 2 1.7)
			(drill oval 0.8 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 337 "Net-(P5-DOTCK)")
			(pinfunction "DOTCK")
			(pintype "unspecified")
		)
		(pad "23" thru_hole circle
			(at -18 5)
			(size 2 2)
			(drill oval 1 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 127 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "23" thru_hole circle
			(at -18 14)
			(size 2 2)
			(drill oval 1 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 127 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "23" thru_hole oval
			(at -9 5)
			(size 2 1.7)
			(drill oval 0.8 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 127 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "23" thru_hole circle
			(at 18 5)
			(size 2 2)
			(drill oval 1 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 127 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "23" thru_hole circle
			(at 18 14)
			(size 2 2)
			(drill oval 1 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 127 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "24" thru_hole oval
			(at -9 14)
			(size 2 1.7)
			(drill oval 0.8 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 352 "Net-(P1-EXPAND)")
			(pinfunction "EXPAND")
			(pintype "unspecified")
		)
		(pad "25" thru_hole oval
			(at -11 5)
			(size 2 1.7)
			(drill oval 0.8 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 339 "Net-(P5-MONO-OUT)")
			(pinfunction "MONO-OUT")
			(pintype "unspecified")
		)
		(pad "26" thru_hole oval
			(at -11 14)
			(size 2 1.7)
			(drill oval 0.8 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 336 "{slash}IRQ")
			(pinfunction "~{IRQ}")
			(pintype "unspecified")
		)
		(pad "27" thru_hole oval
			(at -13 5)
			(size 2 1.7)
			(drill oval 0.8 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 340 "Net-(P5-SL-IN)")
			(pinfunction "SL-IN")
			(pintype "unspecified")
		)
		(pad "28" thru_hole oval
			(at -13 14)
			(size 2 1.7)
			(drill oval 0.8 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 341 "Net-(P5-SR-IN)")
			(pinfunction "SR-IN")
			(pintype "unspecified")
		)
		(embedded_fonts no)
	)
	(footprint "MountingHole:MountingHole_2.5mm"
		(layer "F.Cu")
		(at 260.5278 83.8454 180)
		(descr "Mounting Hole 2.5mm, no annular, generated by kicad-footprint-generator mountinghole.py")
		(tags "mountinghole")
		(property "Reference" "H1"
			(at 0 -3.5 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "MountingHole"
			(at 0 3.5 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Mounting Hole without connection"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "MountingHole*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr exclude_from_pos_files)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole circle
			(at 0 0 180)
			(size 2.5 2.5)
			(drill 2.5)
			(layers "*.Cu" "*.Mask")
		)
		(embedded_fonts no)
	)
	(footprint "SNES_Library:RAM"
		(layer "F.Cu")
		(at 134.952 134.747)
		(descr "SOIC, 18 Pin (JEDEC MS-013AB, https://www.analog.com/media/en/package-pcb-resources/package/33254132129439rw_18.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOIC SO")
		(property "Reference" "U15"
			(at 8.128 -2.54 270)
			(layer "F.SilkS")
		)
		(property "Value" "MS62256CL-10FC"
			(at 0 6.72 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.futurlec.com/Datasheet/Memory/62256.pdf"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "32Kx8 bit Low Power CMOS Static RAM, 55/70ns, DIP-28"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "DIP*W15.24mm*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr smd)
		(fp_text user "14"
			(at -6.35 9.398 270)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "15"
			(at 4.826 9.398 270)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "1"
			(at -6.096 -11.176 270)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "28"
			(at 4.826 -12.446 270)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -5.6 -8.255)
			(size 1.6 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 208 "/MA14")
			(pinfunction "A14")
			(pintype "input")
		)
		(pad "2" smd roundrect
			(at -5.6 -6.985)
			(size 1.6 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 207 "/MA12")
			(pinfunction "A12")
			(pintype "input")
		)
		(pad "3" smd roundrect
			(at -5.6 -5.715)
			(size 1.6 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 206 "/MA7")
			(pinfunction "A7")
			(pintype "input")
		)
		(pad "4" smd roundrect
			(at -5.6 -4.445)
			(size 1.6 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 205 "/MA6")
			(pinfunction "A6")
			(pintype "input")
		)
		(pad "5" smd roundrect
			(at -5.6 -3.175)
			(size 1.6 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 204 "/MA5")
			(pinfunction "A5")
			(pintype "input")
		)
		(pad "6" smd roundrect
			(at -5.6 -1.905)
			(size 1.6 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 202 "/MA4")
			(pinfunction "A4")
			(pintype "input")
		)
		(pad "7" smd roundrect
			(at -5.6 -0.635)
			(size 1.6 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 201 "/MA3")
			(pinfunction "A3")
			(pintype "input")
		)
		(pad "8" smd roundrect
			(at -5.6 0.635)
			(size 1.6 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 200 "/MA2")
			(pinfunction "A2")
			(pintype "input")
		)
		(pad "9" smd roundrect
			(at -5.6 1.905)
			(size 1.6 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 199 "/MA1")
			(pinfunction "A1")
			(pintype "input")
		)
		(pad "10" smd roundrect
			(at -5.6 3.175)
			(size 1.6 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 198 "/MA0")
			(pinfunction "A0")
			(pintype "input")
		)
		(pad "11" smd roundrect
			(at -5.6 4.445)
			(size 1.6 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 190 "/MD0")
			(pinfunction "Q0")
			(pintype "tri_state")
		)
		(pad "12" smd roundrect
			(at -5.6 5.715)
			(size 1.6 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 191 "/MD1")
			(pinfunction "Q1")
			(pintype "tri_state")
		)
		(pad "13" smd roundrect
			(at -5.6 6.985)
			(size 1.6 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 192 "/MD2")
			(pinfunction "Q2")
			(pintype "tri_state")
		)
		(pad "14" smd roundrect
			(at -5.6 8.255)
			(size 1.6 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 127 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "15" smd roundrect
			(at 5.6 8.25)
			(size 1.6 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 193 "/MD3")
			(pinfunction "Q3")
			(pintype "tri_state")
		)
		(pad "16" smd roundrect
			(at 5.6 6.98)
			(size 1.6 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 194 "/MD4")
			(pinfunction "Q4")
			(pintype "tri_state")
		)
		(pad "17" smd roundrect
			(at 5.6 5.71)
			(size 1.6 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 195 "/MD5")
			(pinfunction "Q5")
			(pintype "tri_state")
		)
		(pad "18" smd roundrect
			(at 5.6 4.44)
			(size 1.6 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 196 "/MD6")
			(pinfunction "Q6")
			(pintype "tri_state")
		)
		(pad "19" smd roundrect
			(at 5.6 3.17)
			(size 1.6 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 197 "/MD7")
			(pinfunction "Q7")
			(pintype "tri_state")
		)
		(pad "20" smd roundrect
			(at 5.6 1.9)
			(size 1.6 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 377 "/{slash}SCE0")
			(pinfunction "~{CS}")
			(pintype "input")
		)
		(pad "21" smd roundrect
			(at 5.6 0.63)
			(size 1.6 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 209 "/MA10")
			(pinfunction "A10")
			(pintype "input")
		)
		(pad "22" smd roundrect
			(at 5.6 -0.64)
			(size 1.6 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 378 "/{slash}SOE")
			(pinfunction "~{OE}")
			(pintype "input")
		)
		(pad "23" smd roundrect
			(at 5.6 -1.91)
			(size 1.6 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 210 "/MA11")
			(pinfunction "A11")
			(pintype "input")
		)
		(pad "24" smd roundrect
			(at 5.6 -3.18)
			(size 1.6 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 211 "/MA9")
			(pinfunction "A9")
			(pintype "input")
		)
		(pad "25" smd roundrect
			(at 5.6 -4.45)
			(size 1.6 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 212 "/MA8")
			(pinfunction "A8")
			(pintype "input")
		)
		(pad "26" smd roundrect
			(at 5.6 -5.72)
			(size 1.6 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 213 "/MA13")
			(pinfunction "A13")
			(pintype "input")
		)
		(pad "27" smd roundrect
			(at 5.6 -6.99)
			(size 1.6 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 379 "/{slash}SWE")
			(pinfunction "~{WE}")
			(pintype "input")
		)
		(pad "28" smd roundrect
			(at 5.6 -8.26)
			(size 1.6 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 72 "VCC")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(embedded_fonts no)
		(model "${KICAD7_3DMODEL_DIR}/Package_SO.3dshapes/SOIC-28W_7.5x18.7mm_P1.27mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "SNES_Library:SOP-64_11x28mm_P0,75mm"
		(layer "F.Cu")
		(at 180.22 170.204 -90)
		(property "Reference" "U6"
			(at -0.278 -9.518 270)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "WRAM"
			(at 0 1 270)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr smd)
		(fp_text user "1"
			(at -13.994 11.31 270)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "64"
			(at -13.994 -7.74 270)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "${REFERENCE}"
			(at 0 2.5 270)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -12.4 7.2)
			(size 1.27 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 72 "VCC")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(pad "2" smd rect
			(at -11.2 7.2)
			(size 1.27 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 37 "/D4")
			(pinfunction "D4")
			(pintype "bidirectional")
		)
		(pad "3" smd rect
			(at -10.4 7.2)
			(size 1.27 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 38 "/D5")
			(pinfunction "D5")
			(pintype "bidirectional")
		)
		(pad "4" smd rect
			(at -9.6 7.2)
			(size 1.27 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 39 "/D6")
			(pinfunction "D6")
			(pintype "bidirectional")
		)
		(pad "5" smd rect
			(at -8.8 7.2)
			(size 1.27 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 40 "/D7")
			(pinfunction "D7")
			(pintype "bidirectional")
		)
		(pad "6" smd rect
			(at -8 7.2)
			(size 1.27 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 79 "SYSCK")
			(pinfunction "SYSCK")
			(pintype "input")
		)
		(pad "7" smd rect
			(at -7.2 7.2)
			(size 1.27 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 49 "Net-(P1-REFRESH)")
			(pinfunction "REFRESH")
			(pintype "input")
		)
		(pad "8" smd rect
			(at -6.4 7.2)
			(size 1.27 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 77 "{slash}RESOUT1")
			(pinfunction "RESET")
			(pintype "input")
		)
		(pad "9" smd rect
			(at -5.6 7.2)
			(size 1.27 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
		)
		(pad "10" smd rect
			(at -4.8 7.2)
			(size 1.27 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 72 "VCC")
			(pinfunction "CS1")
			(pintype "input")
		)
		(pad "11" smd rect
			(at -4 7.2)
			(size 1.27 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 72 "VCC")
			(pinfunction "CS2")
			(pintype "input")
		)
		(pad "12" smd rect
			(at -3.2 7.2)
			(size 1.27 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 72 "VCC")
			(pinfunction "CS3")
			(pintype "input")
		)
		(pad "13" smd rect
			(at -2.4 7.2)
			(size 1.27 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 127 "GND")
			(pinfunction "CS1")
			(pintype "input")
		)
		(pad "14" smd rect
			(at -1.6 7.2)
			(size 1.27 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 127 "GND")
			(pinfunction "CS2")
			(pintype "input")
		)
		(pad "15" smd rect
			(at -0.8 7.2)
			(size 1.27 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 42 "/{slash}RAMSEL")
			(pinfunction "CS3")
			(pintype "input")
		)
		(pad "16" smd rect
			(at 0 7.2)
			(size 1.27 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 72 "VCC")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(pad "17" smd rect
			(at 0.8 7.2)
			(size 1.27 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 127 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "18" smd rect
			(at 1.6 7.2)
			(size 1.27 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
		)
		(pad "19" smd rect
			(at 2.4 7.2)
			(size 1.27 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
		)
		(pad "20" smd rect
			(at 3.2 7.2)
			(size 1.27 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
		)
		(pad "21" smd rect
			(at 4 7.2)
			(size 1.27 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
		)
		(pad "22" smd rect
			(at 4.8 7.2)
			(size 1.27 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
		)
		(pad "23" smd rect
			(at 5.6 7.2)
			(size 1.27 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 62 "/CA0")
			(pinfunction "A0")
			(pintype "input")
		)
		(pad "24" smd rect
			(at 6.4 7.2)
			(size 1.27 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 4 "/CA9")
			(pinfunction "A9")
			(pintype "input")
		)
		(pad "25" smd rect
			(at 7.2 7.2)
			(size 1.27 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 63 "/CA1")
			(pinfunction "A1")
			(pintype "input")
		)
		(pad "26" smd rect
			(at 8 7.2)
			(size 1.27 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 5 "/CA10")
			(pinfunction "A10")
			(pintype "input")
		)
		(pad "27" smd rect
			(at 8.8 7.2)
			(size 1.27 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 64 "/CA2")
			(pinfunction "A2")
			(pintype "input")
		)
		(pad "28" smd rect
			(at 9.6 7.2)
			(size 1.27 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 6 "/CA11")
			(pinfunction "A11")
			(pintype "input")
		)
		(pad "29" smd rect
			(at 10.4 7.2)
			(size 1.27 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 65 "/CA3")
			(pinfunction "A3")
			(pintype "input")
		)
		(pad "30" smd rect
			(at 11.2 7.2)
			(size 1.27 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 7 "/CA12")
			(pinfunction "A12")
			(pintype "input")
		)
		(pad "31" smd rect
			(at 12 7.2)
			(size 1.27 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 66 "/CA4")
			(pinfunction "A4")
			(pintype "input")
		)
		(pad "32" smd rect
			(at 13.2 7.2)
			(size 1.27 1.27)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 72 "VCC")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(pad "33" smd rect
			(at 13.2 -6.4)
			(size 1.27 1.27)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 127 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "34" smd rect
			(at 12 -6.4)
			(size 1.27 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 8 "/CA13")
			(pinfunction "A13")
			(pintype "input")
		)
		(pad "35" smd rect
			(at 11.2 -6.4)
			(size 1.27 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 67 "/CA5")
			(pinfunction "A5")
			(pintype "input")
		)
		(pad "36" smd rect
			(at 10.4 -6.4)
			(size 1.27 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 9 "/CA14")
			(pinfunction "A14")
			(pintype "input")
		)
		(pad "37" smd rect
			(at 9.6 -6.4)
			(size 1.27 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 68 "/CA6")
			(pinfunction "A6")
			(pintype "input")
		)
		(pad "38" smd rect
			(at 8.8 -6.4)
			(size 1.27 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 10 "/CA15")
			(pinfunction "A15")
			(pintype "input")
		)
		(pad "39" smd rect
			(at 8 -6.4)
			(size 1.27 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 71 "/CA7")
			(pinfunction "A7")
			(pintype "input")
		)
		(pad "40" smd rect
			(at 7.2 -6.4)
			(size 1.27 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 11 "/CA16")
			(pinfunction "A16")
			(pintype "input")
		)
		(pad "41" smd rect
			(at 6.4 -6.4)
			(size 1.27 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 3 "/CA8")
			(pinfunction "A8")
			(pintype "input")
		)
		(pad "42" smd rect
			(at 5.6 -6.4)
			(size 1.27 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 17 "/CA22")
			(pinfunction "ENA")
			(pintype "input")
		)
		(pad "43" smd rect
			(at 4.8 -6.4)
			(size 1.27 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 308 "/PA2")
			(pinfunction "PS1")
			(pintype "input")
		)
		(pad "44" smd rect
			(at 4 -6.4)
			(size 1.27 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 311 "/PA3")
			(pinfunction "PS2")
			(pintype "input")
		)
		(pad "45" smd rect
			(at 3.2 -6.4)
			(size 1.27 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 309 "/PA4")
			(pinfunction "PS3")
			(pintype "input")
		)
		(pad "46" smd rect
			(at 2.4 -6.4)
			(size 1.27 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 312 "/PA5")
			(pinfunction "PS4")
			(pintype "input")
		)
		(pad "47" smd rect
			(at 1.6 -6.4)
			(size 1.27 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 313 "/PA6")
			(pinfunction "PS5")
			(pintype "input")
		)
		(pad "48" smd rect
			(at 0.8 -6.4)
			(size 1.27 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 127 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "49" smd rect
			(at 0 -6.4)
			(size 1.27 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 72 "VCC")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(pad "50" smd rect
			(at -0.8 -6.4)
			(size 1.27 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 314 "/PA7")
			(pinfunction "PS1")
			(pintype "input")
		)
		(pad "51" smd rect
			(at -1.6 -6.4)
			(size 1.27 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 72 "VCC")
			(pinfunction "PS2")
			(pintype "input")
		)
		(pad "52" smd rect
			(at -2.4 -6.4)
			(size 1.27 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 72 "VCC")
			(pinfunction "PS3")
			(pintype "input")
		)
		(pad "53" smd rect
			(at -3.2 -6.4)
			(size 1.27 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 307 "/PA0")
			(pinfunction "PA0")
			(pintype "input")
		)
		(pad "54" smd rect
			(at -4 -6.4)
			(size 1.27 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 310 "/PA1")
			(pinfunction "PA1")
			(pintype "input")
		)
		(pad "55" smd rect
			(at -4.8 -6.4)
			(size 1.27 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 153 "unconnected-(U6-G-Pad55)")
			(pinfunction "G")
			(pintype "no_connect")
		)
		(pad "56" smd rect
			(at -5.6 -6.4)
			(size 1.27 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 41 "/{slash}PARD")
			(pinfunction "PARD")
			(pintype "input")
		)
		(pad "57" smd rect
			(at -6.4 -6.4)
			(size 1.27 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 76 "/{slash}CPURD")
			(pinfunction "RD")
			(pintype "input")
		)
		(pad "58" smd rect
			(at -7.2 -6.4)
			(size 1.27 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 50 "/{slash}PAWR")
			(pinfunction "PAWR")
			(pintype "input")
		)
		(pad "59" smd rect
			(at -8 -6.4)
			(size 1.27 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 61 "/{slash}CPUWR")
			(pinfunction "WR")
			(pintype "input")
		)
		(pad "60" smd rect
			(at -8.8 -6.4)
			(size 1.27 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 33 "/D0")
			(pinfunction "D0")
			(pintype "bidirectional")
		)
		(pad "61" smd rect
			(at -9.6 -6.4)
			(size 1.27 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 34 "/D1")
			(pinfunction "D1")
			(pintype "bidirectional")
		)
		(pad "62" smd rect
			(at -10.4 -6.4)
			(size 1.27 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 35 "/D2")
			(pinfunction "D2")
			(pintype "bidirectional")
		)
		(pad "63" smd rect
			(at -11.2 -6.4)
			(size 1.27 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 36 "/D3")
			(pinfunction "D3")
			(pintype "bidirectional")
		)
		(pad "64" smd rect
			(at -12.4 -6.4)
			(size 1.27 1.27)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 127 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(embedded_fonts no)
		(model "${KICAD7_3DMODEL_DIR}/Package_SO.3dshapes/TSOP-II-54_22.2x10.16mm_P0.8mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 -90)
			)
		)
	)
	(footprint "Package_SO:SO-24_5.3x15mm_P1.27mm"
		(layer "F.Cu")
		(at 170.9755 97.663)
		(descr "SO, 24 Pin (https://www.ti.com/lit/ml/msop002a/msop002a.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SO SO")
		(property "Reference" "U7"
			(at 5.6815 -4.826 270)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "S-ENC"
			(at 0 8.45 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://wiki.console5.com/tw/images/e/e6/BA6592F.pdf"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -3.4625 -6.985)
			(size 1.975 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 365 "Net-(U7-(R-Y)O)")
			(pinfunction "(R-Y)O")
			(pintype "unspecified")
		)
		(pad "2" smd roundrect
			(at -3.4625 -5.715)
			(size 1.975 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 127 "GND")
			(pinfunction "GND")
			(pintype "unspecified")
		)
		(pad "3" smd roundrect
			(at -3.4625 -4.445)
			(size 1.975 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 374 "Net-(U3-BURST)")
			(pinfunction "PCP")
			(pintype "unspecified")
		)
		(pad "4" smd roundrect
			(at -3.4625 -3.175)
			(size 1.975 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 72 "VCC")
			(pinfunction "SW")
			(pintype "unspecified")
		)
		(pad "5" smd roundrect
			(at -3.4625 -1.905)
			(size 1.975 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 72 "VCC")
			(pinfunction "VCC")
			(pintype "unspecified")
		)
		(pad "6" smd roundrect
			(at -3.4625 -0.635)
			(size 1.975 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 362 "Net-(U7-CO)")
			(pinfunction "CO")
			(pintype "unspecified")
		)
		(pad "7" smd roundrect
			(at -3.4625 0.635)
			(size 1.975 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 182 "Net-(J2-Video)")
			(pinfunction "VO")
			(pintype "unspecified")
		)
		(pad "8" smd roundrect
			(at -3.4625 1.905)
			(size 1.975 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 375 "Net-(U3-CSYNC)")
			(pinfunction "SYNC")
			(pintype "unspecified")
		)
		(pad "9" smd roundrect
			(at -3.4625 3.175)
			(size 1.975 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 181 "Net-(U7-YI)")
			(pinfunction "YI")
			(pintype "unspecified")
		)
		(pad "10" smd roundrect
			(at -3.4625 4.445)
			(size 1.975 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 174 "Net-(U7-(B-Y)I)")
			(pinfunction "(B-Y)I")
			(pintype "unspecified")
		)
		(pad "11" smd roundrect
			(at -3.4625 5.715)
			(size 1.975 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 179 "Net-(U7-(R-Y)I)")
			(pinfunction "(R-Y)I")
			(pintype "unspecified")
		)
		(pad "12" smd roundrect
			(at -3.4625 6.985)
			(size 1.975 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 373 "Net-(U7-BLA)")
			(pinfunction "BLA")
			(pintype "unspecified")
		)
		(pad "13" smd roundrect
			(at 3.4625 6.985)
			(size 1.975 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 155 "Net-(U7-VC)")
			(pinfunction "VC")
			(pintype "unspecified")
		)
		(pad "14" smd roundrect
			(at 3.4625 5.715)
			(size 1.975 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 152 "Net-(U7-VB)")
			(pinfunction "VB")
			(pintype "unspecified")
		)
		(pad "15" smd roundrect
			(at 3.4625 4.445)
			(size 1.975 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 183 "unconnected-(U7-VA-Pad15)")
			(pinfunction "VA")
			(pintype "unspecified+no_connect")
		)
		(pad "16" smd roundrect
			(at 3.4625 3.175)
			(size 1.975 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 374 "Net-(U3-BURST)")
			(pinfunction "BFP")
			(pintype "unspecified")
		)
		(pad "17" smd roundrect
			(at 3.4625 1.905)
			(size 1.975 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 185 "unconnected-(U7-PHA-Pad17)")
			(pinfunction "PHA")
			(pintype "unspecified+no_connect")
		)
		(pad "18" smd roundrect
			(at 3.4625 0.635)
			(size 1.975 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 186 "unconnected-(U7-PDO-Pad18)")
			(pinfunction "PDO")
			(pintype "unspecified+no_connect")
		)
		(pad "19" smd roundrect
			(at 3.4625 -0.635)
			(size 1.975 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 127 "GND")
			(pinfunction "NTSC/PAL")
			(pintype "unspecified")
		)
		(pad "20" smd roundrect
			(at 3.4625 -1.905)
			(size 1.975 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 175 "Net-(U7-AR)")
			(pinfunction "AR")
			(pintype "unspecified")
		)
		(pad "21" smd roundrect
			(at 3.4625 -3.175)
			(size 1.975 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 176 "Net-(U7-AG)")
			(pinfunction "AG")
			(pintype "unspecified")
		)
		(pad "22" smd roundrect
			(at 3.4625 -4.445)
			(size 1.975 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 367 "Net-(U7-AB)")
			(pinfunction "AB")
			(pintype "unspecified")
		)
		(pad "23" smd roundrect
			(at 3.4625 -5.715)
			(size 1.975 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 363 "Net-(U7-YO)")
			(pinfunction "YO")
			(pintype "unspecified")
		)
		(pad "24" smd roundrect
			(at 3.4625 -6.985)
			(size 1.975 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 364 "Net-(U7-(B-Y)O)")
			(pinfunction "(B-Y)O")
			(pintype "unspecified")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Package_SO.3dshapes/SO-24_5.3x15mm_P1.27mm.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_THT:C_Axial_L3.8mm_D2.6mm_P12.50mm_Horizontal"
		(layer "F.Cu")
		(at 274.955 85.979 -90)
		(descr "C, Axial series, Axial, Horizontal, pin pitch=12.5mm, length*diameter=3.8*2.6mm^2, http://www.vishay.com/docs/45231/arseries.pdf")
		(tags "C Axial series Axial Horizontal pin pitch 12.5mm  length 3.8mm diameter 2.6mm")
		(property "Reference" "C20"
			(at -1.7272 1.3716 90)
			(layer "F.SilkS")
		)
		(property "Value" "C"
			(at 6.25 2.42 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 6.25 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 127 "GND")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 12.5 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 422 "Net-(D4-A)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Axial_L3.8mm_D2.6mm_P12.50mm_Horizontal.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Diode_THT:D_T-1_P5.08mm_Horizontal"
		(layer "F.Cu")
		(at 269.2654 145.3134 -90)
		(descr "Diode, T-1 series, Axial, Horizontal, pin pitch=5.08mm, length*diameter=3.2*2.6mm^2, http://www.diodes.com/_files/packages/T-1.pdf")
		(tags "Diode T-1 series Axial Horizontal pin pitch 5.08mm  length 3.2mm diameter 2.6mm")
		(property "Reference" "D6"
			(at 7.6708 0.508 90)
			(layer "F.SilkS")
		)
		(property "Value" "D"
			(at 2.54 2.42 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Diode"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Device" "D"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TO-???* *_Diode_* *SingleDiode* D_*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr through_hole)
		(fp_text user "K"
			(at -1.8034 0 270)
			(layer "F.SilkS")
		)
		(fp_text user "K"
			(at -1.8034 0 270)
			(layer "F.Fab")
		)
		(fp_text user "${REFERENCE}"
			(at 2.78 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole roundrect
			(at 0 0 270)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.125)
			(net 433 "Net-(D6-K)")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 5.08 0 270)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 424 "Net-(D6-A)")
			(pinfunction "A")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Diode_THT.3dshapes/D_T-1_P5.08mm_Horizontal.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Button_Switch_Keyboard:SW_Cherry_MX_1.00u_PCB"
		(layer "F.Cu")
		(at 221.869 86.106 -90)
		(descr "Cherry MX keyswitch, 1.00u, PCB mount, http://cherryamericas.com/wp-content/uploads/2014/12/mx_cat.pdf")
		(tags "Cherry MX keyswitch 1.00u PCB")
		(property "Reference" "SW1"
			(at -2.54 -2.794 90)
			(layer "F.SilkS")
		)
		(property "Value" "KB"
			(at -2.54 12.954 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Push button switch, generic, two pins"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at -2.54 -2.794 90)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole circle
			(at -7.62 5.08 270)
			(size 1.7 1.7)
			(drill 1.7)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at -2.54 5.08 270)
			(size 4 4)
			(drill 4)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 2.54 5.08 270)
			(size 1.7 1.7)
			(drill 1.7)
			(layers "*.Cu" "*.Mask")
		)
		(pad "1" thru_hole circle
			(at 0 0 270)
			(size 2.2 2.2)
			(drill 1.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 157 "Net-(U8-RES)")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at -6.35 2.54 270)
			(size 2.2 2.2)
			(drill 1.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 72 "VCC")
			(pinfunction "2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Button_Switch_Keyboard.3dshapes/SW_Cherry_MX_1.00u_PCB.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_Elec_6.3x5.4"
		(layer "F.Cu")
		(at 102.108 152.4965 -90)
		(descr "SMD capacitor, aluminum electrolytic nonpolar, 6.3x5.4mm")
		(tags "capacitor electrolytic nonpolar")
		(property "Reference" "C60"
			(at 0 -4.35 270)
			(layer "F.SilkS")
		)
		(property "Value" "10uF 50V"
			(at 0 4.35 270)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Polarized capacitor"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "CP_*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 270)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -2.5375 0 270)
			(size 3.325 1.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.15625)
			(net 301 "Net-(DA11-A)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 2.5375 0 270)
			(size 3.325 1.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.15625)
			(net 127 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_Elec_6.3x5.4.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_THT:C_Axial_L3.8mm_D2.6mm_P12.50mm_Horizontal"
		(layer "F.Cu")
		(at 275.6154 170.4626 90)
		(descr "C, Axial series, Axial, Horizontal, pin pitch=12.5mm, length*diameter=3.8*2.6mm^2, http://www.vishay.com/docs/45231/arseries.pdf")
		(tags "C Axial series Axial Horizontal pin pitch 12.5mm  length 3.8mm diameter 2.6mm")
		(property "Reference" "C55"
			(at 2.5432 1.778 90)
			(layer "F.SilkS")
		)
		(property "Value" "C"
			(at 6.25 2.42 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 6.25 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 127 "GND")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 12.5 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 425 "Net-(D7-A)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Axial_L3.8mm_D2.6mm_P12.50mm_Horizontal.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal"
		(layer "F.Cu")
		(at 255.651 170.7134 -90)
		(descr "Resistor, Axial_DIN0207 series, Axial, Horizontal, pin pitch=10.16mm, 0.25W = 1/4W, length*diameter=6.3*2.5mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0207 series Axial Horizontal pin pitch 10.16mm 0.25W = 1/4W length 6.3mm diameter 2.5mm")
		(property "Reference" "O4"
			(at 12.446 1.0668 90)
			(layer "F.SilkS")
		)
		(property "Value" "160 Ω"
			(at 5.08 2.37 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 5.08 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 421 "Net-(D2-A)")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 10.16 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 419 "Net-(LED1-A)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Crystal:Crystal_HC49-4H_Vertical"
		(layer "F.Cu")
		(at 191.97 189.865)
		(descr "HC-49-4H, Crystal, http://5hertz.com/pdfs/04404_D.pdf")
		(property "Reference" "X1"
			(at 2.44 -3.525 0)
			(layer "F.SilkS")
		)
		(property "Value" "17.734MHz"
			(at 2.44 3.525 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Two pin crystal"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Crystal*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 2.44 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1.5 1.5)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 291 "Net-(C1-Pad2)")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 4.88 0)
			(size 1.5 1.5)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 406 "Net-(C2-Pad2)")
			(pinfunction "2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Crystal.3dshapes/Crystal_HC49-4H_Vertical.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Crystal:Resonator-2Pin_W7.0mm_H2.5mm"
		(layer "F.Cu")
		(at 107.15 96.75 90)
		(descr "Ceramic Resonator/Filter, length 2.5mm, width 7.0mm, 2 pins")
		(tags "ceramic")
		(property "Reference" "X2"
			(at 2.516 3.086 90)
			(layer "F.SilkS")
		)
		(property "Value" "24.576MHz"
			(at 2.5 2.45 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Two pin crystal"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Crystal*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 2.5 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 215 "Net-(U14-XTAL1)")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 5 0 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 214 "Net-(U14-XTAL0)")
			(pinfunction "2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Crystal.3dshapes/Resonator-2Pin_W7.0mm_H2.5mm.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:CP_Elec_4x5.8"
		(layer "F.Cu")
		(at 212.35 190.7)
		(descr "SMD capacitor, aluminum electrolytic, Panasonic, 4.0x5.8mm")
		(tags "capacitor electrolytic")
		(property "Reference" "C62"
			(at 2.788 -4.01 0)
			(layer "F.SilkS")
		)
		(property "Value" "2.2uF"
			(at 0 3.2 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Polarized capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "CP_*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.8 0)
			(size 2.6 1.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.15625)
			(net 72 "VCC")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.8 0)
			(size 2.6 1.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.15625)
			(net 158 "Net-(U8-P02)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/CP_Elec_4x5.8.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "SNES_Library:Controller"
		(layer "F.Cu")
		(at 265.945 159.217 -90)
		(property "Reference" "J5"
			(at 0 -0.5 270)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "CONTROLLER 2"
			(at -3.0212 2.674 270)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Datasheet" "~"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x07, script generated"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr through_hole)
		(fp_text user "1"
			(at -14.7052 2.4708 270)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "7"
			(at 15.8764 3.0296 270)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "${REFERENCE}"
			(at 0 -2.286 270)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" thru_hole oval
			(at -12.532 0.134 270)
			(size 2 3)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 418 "Net-(D3-K)")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at -8.532 0.134 270)
			(size 2 3)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 424 "Net-(D6-A)")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at -4.532 0.134 270)
			(size 2 3)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 425 "Net-(D7-A)")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole oval
			(at -0.532 0.134 270)
			(size 2 3)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 428 "Net-(J5-Pin_4)")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(pad "5" thru_hole oval
			(at 5.97 0.134 270)
			(size 2 3)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 429 "Net-(J5-Pin_5)")
			(pinfunction "Pin_5")
			(pintype "passive")
		)
		(pad "6" thru_hole oval
			(at 9.97 0.134 270)
			(size 2 3)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 434 "Net-(J5-Pin_6)")
			(pinfunction "Pin_6")
			(pintype "passive")
		)
		(pad "7" thru_hole oval
			(at 13.97 0.134 270)
			(size 2 3)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 127 "GND")
			(pinfunction "Pin_7")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "Capacitor_SMD:CP_Elec_6.3x3"
		(layer "F.Cu")
		(at 137.5 188.4 -90)
		(descr "SMD capacitor, aluminum electrolytic, Nichicon, 6.3x3.0mm")
		(tags "capacitor electrolytic")
		(property "Reference" "C64"
			(at 0.322 -4.613 270)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "33uF 25V"
			(at 0 4.35 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Polarized capacitor"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "CP_*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -2.7 0 270)
			(size 3.5 1.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.15625)
			(net 396 "Net-(Q18-B)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 2.7 0 270)
			(size 3.5 1.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.15625)
			(net 127 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/CP_Elec_6.3x3.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Diode_THT:D_T-1_P5.08mm_Horizontal"
		(layer "F.Cu")
		(at 261.0866 110.5662 -90)
		(descr "Diode, T-1 series, Axial, Horizontal, pin pitch=5.08mm, length*diameter=3.2*2.6mm^2, http://www.diodes.com/_files/packages/T-1.pdf")
		(tags "Diode T-1 series Axial Horizontal pin pitch 5.08mm  length 3.2mm diameter 2.6mm")
		(property "Reference" "D2"
			(at 8.4328 2.8448 90)
			(layer "F.SilkS")
		)
		(property "Value" "D"
			(at 2.54 2.42 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Diode"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Device" "D"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TO-???* *_Diode_* *SingleDiode* D_*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr through_hole)
		(fp_text user "K"
			(at 0 -2 270)
			(layer "F.SilkS")
		)
		(fp_text user "K"
			(at 0 -2 270)
			(layer "F.Fab")
		)
		(fp_text user "${REFERENCE}"
			(at 2.78 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole roundrect
			(at 0 0 270)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.125)
			(net 420 "Net-(D2-K)")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 5.08 0 270)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 421 "Net-(D2-A)")
			(pinfunction "A")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Diode_THT.3dshapes/D_T-1_P5.08mm_Horizontal.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Fuse:Fuse_1210_3225Metric"
		(layer "F.Cu")
		(at 183.134 85.976 -90)
		(descr "Fuse SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
		(tags "fuse")
		(property "Reference" "L1"
			(at 0 -2.28 90)
			(layer "F.SilkS")
		)
		(property "Value" "22u"
			(at 0 2.28 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Inductor"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Choke_* *Coil* Inductor_* L_*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.4 0 270)
			(size 1.25 2.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.2)
			(net 127 "GND")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.4 0 270)
			(size 1.25 2.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.2)
			(net 156 "Net-(C11-Pad2)")
			(pinfunction "2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Fuse.3dshapes/Fuse_1210_3225Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "SNES_Library:RAM"
		(layer "F.Cu")
		(at 188.976 105.107 90)
		(descr "SOIC, 18 Pin (JEDEC MS-013AB, https://www.analog.com/media/en/package-pcb-resources/package/33254132129439rw_18.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOIC SO")
		(property "Reference" "U5"
			(at 8.128 -2.54 0)
			(layer "F.SilkS")
		)
		(property "Value" "MS62256CL-10FC"
			(at 0 6.72 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.futurlec.com/Datasheet/Memory/62256.pdf"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "32Kx8 bit Low Power CMOS Static RAM, 55/70ns, DIP-28"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "DIP*W15.24mm*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr smd)
		(fp_text user "15"
			(at 4.826 9.398 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "1"
			(at -6.096 -11.176 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "28"
			(at 4.826 -12.446 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "14"
			(at -6.35 9.398 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -5.6 -8.255 90)
			(size 1.6 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 81 "/VA14")
			(pinfunction "A14")
			(pintype "input")
		)
		(pad "2" smd roundrect
			(at -5.6 -6.985 90)
			(size 1.6 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 98 "/VAA12")
			(pinfunction "A12")
			(pintype "input")
		)
		(pad "3" smd roundrect
			(at -5.6 -5.715 90)
			(size 1.6 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 103 "/VAA7")
			(pinfunction "A7")
			(pintype "input")
		)
		(pad "4" smd roundrect
			(at -5.6 -4.445 90)
			(size 1.6 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 104 "/VAA6")
			(pinfunction "A6")
			(pintype "input")
		)
		(pad "5" smd roundrect
			(at -5.6 -3.175 90)
			(size 1.6 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 105 "/VAA5")
			(pinfunction "A5")
			(pintype "input")
		)
		(pad "6" smd roundrect
			(at -5.6 -1.905 90)
			(size 1.6 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 106 "/VAA4")
			(pinfunction "A4")
			(pintype "input")
		)
		(pad "7" smd roundrect
			(at -5.6 -0.635 90)
			(size 1.6 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 107 "/VAA3")
			(pinfunction "A3")
			(pintype "input")
		)
		(pad "8" smd roundrect
			(at -5.6 0.635 90)
			(size 1.6 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 108 "/VAA2")
			(pinfunction "A2")
			(pintype "input")
		)
		(pad "9" smd roundrect
			(at -5.6 1.905 90)
			(size 1.6 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 109 "/VAA1")
			(pinfunction "A1")
			(pintype "input")
		)
		(pad "10" smd roundrect
			(at -5.6 3.175 90)
			(size 1.6 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 110 "/VAA0")
			(pinfunction "A0")
			(pintype "input")
		)
		(pad "11" smd roundrect
			(at -5.6 4.445 90)
			(size 1.6 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 144 "/VDA0")
			(pinfunction "Q0")
			(pintype "tri_state")
		)
		(pad "12" smd roundrect
			(at -5.6 5.715 90)
			(size 1.6 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 145 "/VDA1")
			(pinfunction "Q1")
			(pintype "tri_state")
		)
		(pad "13" smd roundrect
			(at -5.6 6.985 90)
			(size 1.6 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 146 "/VDA2")
			(pinfunction "Q2")
			(pintype "tri_state")
		)
		(pad "14" smd roundrect
			(at -5.6 8.255 90)
			(size 1.6 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 127 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "15" smd roundrect
			(at 5.6 8.25 90)
			(size 1.6 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 147 "/VDA3")
			(pinfunction "Q3")
			(pintype "tri_state")
		)
		(pad "16" smd roundrect
			(at 5.6 6.98 90)
			(size 1.6 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 148 "/VDA4")
			(pinfunction "Q4")
			(pintype "tri_state")
		)
		(pad "17" smd roundrect
			(at 5.6 5.71 90)
			(size 1.6 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 149 "/VDA5")
			(pinfunction "Q5")
			(pintype "tri_state")
		)
		(pad "18" smd roundrect
			(at 5.6 4.44 90)
			(size 1.6 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 150 "/VDA6")
			(pinfunction "Q6")
			(pintype "tri_state")
		)
		(pad "19" smd roundrect
			(at 5.6 3.17 90)
			(size 1.6 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 151 "/VDA7")
			(pinfunction "Q7")
			(pintype "tri_state")
		)
		(pad "20" smd roundrect
			(at 5.6 1.9 90)
			(size 1.6 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 127 "GND")
			(pinfunction "~{CS}")
			(pintype "input")
		)
		(pad "21" smd roundrect
			(at 5.6 0.63 90)
			(size 1.6 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 100 "/VAA10")
			(pinfunction "A10")
			(pintype "input")
		)
		(pad "22" smd roundrect
			(at 5.6 -0.64 90)
			(size 1.6 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 48 "{slash}VRD")
			(pinfunction "~{OE}")
			(pintype "input")
		)
		(pad "23" smd roundrect
			(at 5.6 -1.91 90)
			(size 1.6 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 99 "/VAA11")
			(pinfunction "A11")
			(pintype "input")
		)
		(pad "24" smd roundrect
			(at 5.6 -3.18 90)
			(size 1.6 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 101 "/VAA9")
			(pinfunction "A9")
			(pintype "input")
		)
		(pad "25" smd roundrect
			(at 5.6 -4.45 90)
			(size 1.6 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 102 "/VAA8")
			(pinfunction "A8")
			(pintype "input")
		)
		(pad "26" smd roundrect
			(at 5.6 -5.72 90)
			(size 1.6 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 97 "/VAA13")
			(pinfunction "A13")
			(pintype "input")
		)
		(pad "27" smd roundrect
			(at 5.6 -6.99 90)
			(size 1.6 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 46 "{slash}VAWR")
			(pinfunction "~{WE}")
			(pintype "input")
		)
		(pad "28" smd roundrect
			(at 5.6 -8.26 90)
			(size 1.6 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 72 "VCC")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(embedded_fonts no)
		(model "${KICAD7_3DMODEL_DIR}/Package_SO.3dshapes/SOIC-28W_7.5x18.7mm_P1.27mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_THT:C_Axial_L3.8mm_D2.6mm_P7.50mm_Horizontal"
		(layer "F.Cu")
		(at 275.3614 141.732 -90)
		(descr "C, Axial series, Axial, Horizontal, pin pitch=7.5mm, length*diameter=3.8*2.6mm^2, http://www.vishay.com/docs/45231/arseries.pdf")
		(tags "C Axial series Axial Horizontal pin pitch 7.5mm  length 3.8mm diameter 2.6mm")
		(property "Reference" "C56"
			(at 11.43 0.3048 90)
			(layer "F.SilkS")
		)
		(property "Value" "C"
			(at 3.75 2.42 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 3.75 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 127 "GND")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 7.5 0 270)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 424 "Net-(D6-A)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Axial_L3.8mm_D2.6mm_P7.50mm_Horizontal.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_SO:SOIC-16_4.55x10.3mm_P1.27mm"
		(layer "F.Cu")
		(at 106.045 81.332 90)
		(descr "SOIC, 16 Pin (https://toshiba.semicon-storage.com/info/docget.jsp?did=12858&prodName=TLP291-4), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOIC SO")
		(property "Reference" "U17"
			(at 7.037 0.635 180)
			(layer "F.SilkS")
		)
		(property "Value" "uPD6376"
			(at 0 6.1 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -3.25 -4.445 90)
			(size 1.6 0.55)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 127 "GND")
			(pinfunction "4/8_fs_SEL")
			(pintype "input")
		)
		(pad "2" smd roundrect
			(at -3.25 -3.175 90)
			(size 1.6 0.55)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 127 "GND")
			(pinfunction "D.GND")
			(pintype "power_in")
		)
		(pad "3" smd roundrect
			(at -3.25 -1.905 90)
			(size 1.6 0.55)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 72 "VCC")
			(pinfunction "NC")
			(pintype "unspecified")
		)
		(pad "4" smd roundrect
			(at -3.25 -0.635 90)
			(size 1.6 0.55)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 72 "VCC")
			(pinfunction "D.Vdd")
			(pintype "power_in")
		)
		(pad "5" smd roundrect
			(at -3.25 0.635 90)
			(size 1.6 0.55)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 282 "unconnected-(U17-A.GND-Pad5)")
			(pinfunction "A.GND")
			(pintype "power_in+no_connect")
		)
		(pad "6" smd roundrect
			(at -3.25 1.905 90)
			(size 1.6 0.55)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 331 "Net-(U17-R.OUT)")
			(pinfunction "R.OUT")
			(pintype "output")
		)
		(pad "7" smd roundrect
			(at -3.25 3.175 90)
			(size 1.6 0.55)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 72 "VCC")
			(pinfunction "A.Vdd")
			(pintype "power_in")
		)
		(pad "8" smd roundrect
			(at -3.25 4.445 90)
			(size 1.6 0.55)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 72 "VCC")
			(pinfunction "A.Vdd")
			(pintype "power_in")
		)
		(pad "9" smd roundrect
			(at 3.25 4.445 90)
			(size 1.6 0.55)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 217 "Net-(U14-LRCK)")
			(pinfunction "R.REF")
			(pintype "unspecified")
		)
		(pad "10" smd roundrect
			(at 3.25 3.175 90)
			(size 1.6 0.55)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 217 "Net-(U14-LRCK)")
			(pinfunction "L.REF")
			(pintype "unspecified")
		)
		(pad "11" smd roundrect
			(at 3.25 1.905 90)
			(size 1.6 0.55)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 332 "Net-(U17-L.OUT)")
			(pinfunction "L.OUT")
			(pintype "output")
		)
		(pad "12" smd roundrect
			(at 3.25 0.635 90)
			(size 1.6 0.55)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 127 "GND")
			(pinfunction "A.GND")
			(pintype "power_in")
		)
		(pad "13" smd roundrect
			(at 3.25 -0.635 90)
			(size 1.6 0.55)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 393 "unconnected-(U17-LRCK{slash}WDCK-Pad13)")
			(pinfunction "LRCK/WDCK")
			(pintype "input+no_connect")
		)
		(pad "14" smd roundrect
			(at 3.25 -1.905 90)
			(size 1.6 0.55)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 127 "GND")
			(pinfunction "LRSEL/RSI")
			(pintype "input")
		)
		(pad "15" smd roundrect
			(at 3.25 -3.175 90)
			(size 1.6 0.55)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 218 "Net-(U14-DATA)")
			(pinfunction "SI/LSI")
			(pintype "input")
		)
		(pad "16" smd roundrect
			(at 3.25 -4.445 90)
			(size 1.6 0.55)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 216 "Net-(U14-BCK)")
			(pinfunction "CLK")
			(pintype "input")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Package_SO.3dshapes/SOIC-16_4.55x10.3mm_P1.27mm.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_Elec_6.3x5.4"
		(layer "F.Cu")
		(at 102.108 161.5135 -90)
		(descr "SMD capacitor, aluminum electrolytic nonpolar, 6.3x5.4mm")
		(tags "capacitor electrolytic nonpolar")
		(property "Reference" "C59"
			(at 0 -4.35 270)
			(layer "F.SilkS")
		)
		(property "Value" "10uF 50V"
			(at 0 4.35 270)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Polarized capacitor"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "CP_*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 270)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -2.5375 0 270)
			(size 3.325 1.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.15625)
			(net 302 "Net-(DA11-common)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 2.5375 0 270)
			(size 3.325 1.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.15625)
			(net 74 "Net-(C31-Pad2)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_Elec_6.3x5.4.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Diode_THT:D_T-1_P5.08mm_Horizontal"
		(layer "F.Cu")
		(at 272.5674 145.3134 -90)
		(descr "Diode, T-1 series, Axial, Horizontal, pin pitch=5.08mm, length*diameter=3.2*2.6mm^2, http://www.diodes.com/_files/packages/T-1.pdf")
		(tags "Diode T-1 series Axial Horizontal pin pitch 5.08mm  length 3.2mm diameter 2.6mm")
		(property "Reference" "D7"
			(at 7.6708 0.7112 90)
			(layer "F.SilkS")
		)
		(property "Value" "D"
			(at 2.54 2.42 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Diode"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Device" "D"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TO-???* *_Diode_* *SingleDiode* D_*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr through_hole)
		(fp_text user "K"
			(at -1.8034 0 270)
			(layer "F.SilkS")
		)
		(fp_text user "${REFERENCE}"
			(at 2.78 0 90)
			(layer "F.Fab")
		)
		(fp_text user "K"
			(at -1.8034 0 270)
			(layer "F.Fab")
		)
		(pad "1" thru_hole roundrect
			(at 0 0 270)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.125)
			(net 431 "Net-(D4-K)")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 5.08 0 270)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 425 "Net-(D7-A)")
			(pinfunction "A")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Diode_THT.3dshapes/D_T-1_P5.08mm_Horizontal.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "SNES_Library:DcJack"
		(layer "F.Cu")
		(at 71.795 199.39)
		(property "Reference" "J1"
			(at 7.62 -7.62 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Jack-DC"
			(at -1.27 5.08 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "DC Barrel Jack"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "BarrelJack*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at -1.27 6.35 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" thru_hole oval
			(at -3.81 0)
			(size 4.5 6.35)
			(drill oval 1.524 4.572)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 70 "Net-(C30-Pad2)")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 2.5 0)
			(size 4.5 6.35)
			(drill oval 1.524 4.572)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 69 "Net-(C30-Pad1)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD7_3DMODEL_DIR}/Connector_BarrelJack.3dshapes/BarrelJack_CUI_PJ-063AH_Horizontal.wrl"
			(offset
				(xyz 2.5 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 90)
			)
		)
	)
	(footprint "Connector_JST:JST_PH_B2B-PH-K_1x02_P2.00mm_Vertical"
		(layer "F.Cu")
		(at 103.9 202.35 180)
		(descr "JST PH series connector, B2B-PH-K (http://www.jst-mfg.com/product/pdf/eng/ePH.pdf), generated with kicad-footprint-generator")
		(tags "connector JST PH vertical")
		(property "Reference" "P3"
			(at 1.538 2.452 0)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_01x02_Pin"
			(at 1 4 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x02, script generated"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 1 1.5 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole roundrect
			(at 0 0 180)
			(size 1.2 1.75)
			(drill 0.75)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.208333)
			(net 303 "Net-(DA11-K)")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 2 0 180)
			(size 1.2 1.75)
			(drill 0.75)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "Net-(P3-Pin_2)")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_JST.3dshapes/JST_PH_B2B-PH-K_1x02_P2.00mm_Vertical.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "SNES_Library:RAM"
		(layer "F.Cu")
		(at 111.25 131.142 90)
		(descr "SOIC, 18 Pin (JEDEC MS-013AB, https://www.analog.com/media/en/package-pcb-resources/package/33254132129439rw_18.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOIC SO")
		(property "Reference" "U16"
			(at 8.128 -2.54 0)
			(layer "F.SilkS")
		)
		(property "Value" "MS62256CL-10FC"
			(at 0 6.72 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.futurlec.com/Datasheet/Memory/62256.pdf"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "32Kx8 bit Low Power CMOS Static RAM, 55/70ns, DIP-28"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "DIP*W15.24mm*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr smd)
		(fp_text user "15"
			(at 4.826 9.398 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "14"
			(at -6.35 9.398 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "1"
			(at -6.096 -11.176 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "28"
			(at 4.826 -12.446 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -5.6 -8.255 90)
			(size 1.6 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 208 "/MA14")
			(pinfunction "A14")
			(pintype "input")
		)
		(pad "2" smd roundrect
			(at -5.6 -6.985 90)
			(size 1.6 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 207 "/MA12")
			(pinfunction "A12")
			(pintype "input")
		)
		(pad "3" smd roundrect
			(at -5.6 -5.715 90)
			(size 1.6 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 206 "/MA7")
			(pinfunction "A7")
			(pintype "input")
		)
		(pad "4" smd roundrect
			(at -5.6 -4.445 90)
			(size 1.6 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 205 "/MA6")
			(pinfunction "A6")
			(pintype "input")
		)
		(pad "5" smd roundrect
			(at -5.6 -3.175 90)
			(size 1.6 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 204 "/MA5")
			(pinfunction "A5")
			(pintype "input")
		)
		(pad "6" smd roundrect
			(at -5.6 -1.905 90)
			(size 1.6 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 202 "/MA4")
			(pinfunction "A4")
			(pintype "input")
		)
		(pad "7" smd roundrect
			(at -5.6 -0.635 90)
			(size 1.6 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 201 "/MA3")
			(pinfunction "A3")
			(pintype "input")
		)
		(pad "8" smd roundrect
			(at -5.6 0.635 90)
			(size 1.6 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 200 "/MA2")
			(pinfunction "A2")
			(pintype "input")
		)
		(pad "9" smd roundrect
			(at -5.6 1.905 90)
			(size 1.6 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 199 "/MA1")
			(pinfunction "A1")
			(pintype "input")
		)
		(pad "10" smd roundrect
			(at -5.6 3.175 90)
			(size 1.6 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 198 "/MA0")
			(pinfunction "A0")
			(pintype "input")
		)
		(pad "11" smd roundrect
			(at -5.6 4.445 90)
			(size 1.6 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 190 "/MD0")
			(pinfunction "Q0")
			(pintype "tri_state")
		)
		(pad "12" smd roundrect
			(at -5.6 5.715 90)
			(size 1.6 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 191 "/MD1")
			(pinfunction "Q1")
			(pintype "tri_state")
		)
		(pad "13" smd roundrect
			(at -5.6 6.985 90)
			(size 1.6 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 192 "/MD2")
			(pinfunction "Q2")
			(pintype "tri_state")
		)
		(pad "14" smd roundrect
			(at -5.6 8.255 90)
			(size 1.6 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 127 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "15" smd roundrect
			(at 5.6 8.25 90)
			(size 1.6 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 193 "/MD3")
			(pinfunction "Q3")
			(pintype "tri_state")
		)
		(pad "16" smd roundrect
			(at 5.6 6.98 90)
			(size 1.6 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 194 "/MD4")
			(pinfunction "Q4")
			(pintype "tri_state")
		)
		(pad "17" smd roundrect
			(at 5.6 5.71 90)
			(size 1.6 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 195 "/MD5")
			(pinfunction "Q5")
			(pintype "tri_state")
		)
		(pad "18" smd roundrect
			(at 5.6 4.44 90)
			(size 1.6 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 196 "/MD6")
			(pinfunction "Q6")
			(pintype "tri_state")
		)
		(pad "19" smd roundrect
			(at 5.6 3.17 90)
			(size 1.6 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 197 "/MD7")
			(pinfunction "Q7")
			(pintype "tri_state")
		)
		(pad "20" smd roundrect
			(at 5.6 1.9 90)
			(size 1.6 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 376 "/{slash}SCE1")
			(pinfunction "~{CS}")
			(pintype "input")
		)
		(pad "21" smd roundrect
			(at 5.6 0.63 90)
			(size 1.6 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 209 "/MA10")
			(pinfunction "A10")
			(pintype "input")
		)
		(pad "22" smd roundrect
			(at 5.6 -0.64 90)
			(size 1.6 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 378 "/{slash}SOE")
			(pinfunction "~{OE}")
			(pintype "input")
		)
		(pad "23" smd roundrect
			(at 5.6 -1.91 90)
			(size 1.6 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 210 "/MA11")
			(pinfunction "A11")
			(pintype "input")
		)
		(pad "24" smd roundrect
			(at 5.6 -3.18 90)
			(size 1.6 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 211 "/MA9")
			(pinfunction "A9")
			(pintype "input")
		)
		(pad "25" smd roundrect
			(at 5.6 -4.45 90)
			(size 1.6 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 212 "/MA8")
			(pinfunction "A8")
			(pintype "input")
		)
		(pad "26" smd roundrect
			(at 5.6 -5.72 90)
			(size 1.6 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 213 "/MA13")
			(pinfunction "A13")
			(pintype "input")
		)
		(pad "27" smd roundrect
			(at 5.6 -6.99 90)
			(size 1.6 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 379 "/{slash}SWE")
			(pinfunction "~{WE}")
			(pintype "input")
		)
		(pad "28" smd roundrect
			(at 5.6 -8.26 90)
			(size 1.6 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 72 "VCC")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(embedded_fonts no)
		(model "${KICAD7_3DMODEL_DIR}/Package_SO.3dshapes/SOIC-28W_7.5x18.7mm_P1.27mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Diode_THT:D_T-1_P5.08mm_Horizontal"
		(layer "F.Cu")
		(at 271.8054 106.7054 -90)
		(descr "Diode, T-1 series, Axial, Horizontal, pin pitch=5.08mm, length*diameter=3.2*2.6mm^2, http://www.diodes.com/_files/packages/T-1.pdf")
		(tags "Diode T-1 series Axial Horizontal pin pitch 5.08mm  length 3.2mm diameter 2.6mm")
		(property "Reference" "D5"
			(at 6.2484 2.6416 90)
			(layer "F.SilkS")
		)
		(property "Value" "D"
			(at 2.54 2.42 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Diode"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Device" "D"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TO-???* *_Diode_* *SingleDiode* D_*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr through_hole)
		(fp_text user "K"
			(at 0 -2 270)
			(layer "F.SilkS")
		)
		(fp_text user "${REFERENCE}"
			(at 2.78 0 90)
			(layer "F.Fab")
		)
		(fp_text user "K"
			(at 0 -2 270)
			(layer "F.Fab")
		)
		(pad "1" thru_hole roundrect
			(at 0 0 270)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.125)
			(net 432 "Net-(D5-K)")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 5.08 0 270)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 423 "Net-(D5-A)")
			(pinfunction "A")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Diode_THT.3dshapes/D_T-1_P5.08mm_Horizontal.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Diode_THT:D_T-1_P5.08mm_Horizontal"
		(layer "F.Cu")
		(at 257.4798 110.617 -90)
		(descr "Diode, T-1 series, Axial, Horizontal, pin pitch=5.08mm, length*diameter=3.2*2.6mm^2, http://www.diodes.com/_files/packages/T-1.pdf")
		(tags "Diode T-1 series Axial Horizontal pin pitch 5.08mm  length 3.2mm diameter 2.6mm")
		(property "Reference" "D3"
			(at 8.4328 1.5748 90)
			(layer "F.SilkS")
		)
		(property "Value" "D"
			(at 2.54 2.42 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Diode"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Device" "D"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TO-???* *_Diode_* *SingleDiode* D_*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr through_hole)
		(fp_text user "K"
			(at 0 -2 270)
			(layer "F.SilkS")
		)
		(fp_text user "K"
			(at 0 -2 270)
			(layer "F.Fab")
		)
		(fp_text user "${REFERENCE}"
			(at 2.78 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole roundrect
			(at 0 0 270)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.125)
			(net 418 "Net-(D3-K)")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 5.08 0 270)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 421 "Net-(D2-A)")
			(pinfunction "A")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Diode_THT.3dshapes/D_T-1_P5.08mm_Horizontal.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "SNES_Library:AVOut"
		(layer "F.Cu")
		(at 83.439 143.764 -90)
		(property "Reference" "P4"
			(at 0 -5.54 270)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "~"
			(at 0 -4.04 270)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr through_hole)
		(fp_circle
			(center -6.27 12)
			(end -6.35 10.16)
			(fill no)
			(layer "Edge.Cuts")
		)
		(fp_circle
			(center 6.73 12)
			(end 6.73 10.16)
			(fill no)
			(layer "Edge.Cuts")
		)
		(fp_text user "1"
			(at 13.97 2.54 270)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "12"
			(at -13.208 5.08 270)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "11"
			(at -13.208 2.54 270)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "2"
			(at 13.97 5.08 270)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "2"
			(at 10.922 6.096 270)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(fp_text user "11"
			(at -7.112 3.556 270)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(fp_text user "12"
			(at -7.112 6.096 270)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(fp_text user "1"
			(at 10.922 3.556 270)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(fp_text user "${REFERENCE}"
			(at 0 -2.54 270)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" thru_hole oval
			(at 6.35 2.54 270)
			(size 1.5 2)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 167 "Net-(DA12-K)")
			(pinfunction "Red")
			(pintype "unspecified")
		)
		(pad "2" thru_hole oval
			(at 6.35 5.08 270)
			(size 1.5 2)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 402 "Net-(DA19-K)")
			(pinfunction "Green")
			(pintype "unspecified")
		)
		(pad "3" thru_hole oval
			(at 3.81 2.54 270)
			(size 1.5 2)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 304 "+12V")
			(pinfunction "CSYNC")
			(pintype "unspecified")
		)
		(pad "4" thru_hole oval
			(at 3.81 5.08 270)
			(size 1.5 2)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 401 "Net-(DA13-K)")
			(pinfunction "Blue")
			(pintype "unspecified")
		)
		(pad "5" thru_hole oval
			(at 1.27 2.54 270)
			(size 1.5 2)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 127 "GND")
			(pinfunction "GND")
			(pintype "unspecified")
		)
		(pad "6" thru_hole oval
			(at 1.27 5.08 270)
			(size 1.5 2)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 127 "GND")
			(pinfunction "GND")
			(pintype "unspecified")
		)
		(pad "7" thru_hole oval
			(at -1.27 2.54 270)
			(size 1.5 2)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 399 "Net-(DA16-K)")
			(pinfunction "Y-SV")
			(pintype "unspecified")
		)
		(pad "8" thru_hole oval
			(at -1.27 5.08 270)
			(size 1.5 2)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 397 "Net-(DA17-K)")
			(pinfunction "C-SV")
			(pintype "unspecified")
		)
		(pad "9" thru_hole oval
			(at -3.81 2.54 270)
			(size 1.5 2)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 168 "Net-(DA15-K)")
			(pinfunction "CV")
			(pintype "unspecified")
		)
		(pad "10" thru_hole oval
			(at -3.81 5.08 270)
			(size 1.5 2)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 72 "VCC")
			(pinfunction "VCC")
			(pintype "unspecified")
		)
		(pad "11" thru_hole oval
			(at -6.35 2.54 270)
			(size 1.5 2)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 289 "Net-(P4-Audio-L)")
			(pinfunction "Audio-L")
			(pintype "unspecified")
		)
		(pad "12" thru_hole oval
			(at -6.27 5.08 270)
			(size 1.5 2)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 290 "Net-(P4-Audio-R)")
			(pinfunction "Audio-R")
			(pintype "unspecified")
		)
		(embedded_fonts no)
	)
	(footprint "Package_TO_SOT_SMD:SOT-23"
		(layer "F.Cu")
		(at 224.8385 155.641)
		(descr "SOT, 3 Pin (JEDEC TO-236 Var AB https://www.jedec.org/document_search?search_api_views_fulltext=TO-236), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOT TO_SOT_SMD")
		(property "Reference" "U11"
			(at 0 -2.4 0)
			(layer "F.SilkS")
		)
		(property "Value" "LM809"
			(at 0 2.4 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm809.pdf"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Microprocessor Reset (active-low) Circuit, SOT-23"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SOT?23*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9375 -0.95)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 127 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "2" smd roundrect
			(at -0.9375 0.95)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 77 "{slash}RESOUT1")
			(pinfunction "~{RESET}")
			(pintype "output")
		)
		(pad "3" smd roundrect
			(at 0.9375 0)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 72 "VCC")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_SO:SOIC-14_3.9x8.7mm_P1.27mm"
		(layer "F.Cu")
		(at 183.134 189.549 -90)
		(descr "SOIC, 14 Pin (JEDEC MS-012AB, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_narrow-r/r_14.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOIC SO")
		(property "Reference" "U18"
			(at -0.573 6.985 180)
			(layer "F.SilkS")
		)
		(property "Value" "S-CLK"
			(at 0.062 0.254 180)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -2.475 -3.81 270)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 406 "Net-(C2-Pad2)")
			(pinfunction "XTAL")
			(pintype "unspecified")
		)
		(pad "2" smd roundrect
			(at -2.475 -2.54 270)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 293 "Net-(R1-Pad2)")
			(pinfunction "XTAL")
			(pintype "unspecified")
		)
		(pad "3" smd roundrect
			(at -2.475 -1.27 270)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 72 "VCC")
			(pinfunction "+5V")
			(pintype "power_in")
		)
		(pad "4" smd roundrect
			(at -2.475 0 270)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 45 "Net-(U18-XOUT)")
			(pinfunction "XOUT")
			(pintype "output")
		)
		(pad "5" smd roundrect
			(at -2.475 1.27 270)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 32 "Net-(U18-4.433M)")
			(pinfunction "4.433M")
			(pintype "output")
		)
		(pad "6" smd roundrect
			(at -2.475 2.54 270)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 296 "Net-(U18-3.546M)")
			(pinfunction "3.546M")
			(pintype "output")
		)
		(pad "7" smd roundrect
			(at -2.475 3.81 270)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 25 "Net-(P1-CIC3)")
			(pinfunction "CIC3")
			(pintype "unspecified")
		)
		(pad "8" smd roundrect
			(at 2.475 3.81 270)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 403 "Net-(U18-Pad8)")
			(pintype "unspecified")
		)
		(pad "9" smd roundrect
			(at 2.475 2.54 270)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 403 "Net-(U18-Pad8)")
			(pintype "unspecified")
		)
		(pad "10" smd roundrect
			(at 2.475 1.27 270)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 127 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "11" smd roundrect
			(at 2.475 0 270)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 294 "Net-(R2-Pad1)")
			(pintype "unspecified")
		)
		(pad "12" smd roundrect
			(at 2.475 -1.27 270)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 295 "Net-(R3-Pad2)")
			(pintype "unspecified")
		)
		(pad "13" smd roundrect
			(at 2.475 -2.54 270)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 295 "Net-(R3-Pad2)")
			(pintype "unspecified")
		)
		(pad "14" smd roundrect
			(at 2.475 -3.81 270)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 72 "VCC")
			(pinfunction "+5V?")
			(pintype "unspecified")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Package_SO.3dshapes/SOIC-14_3.9x8.7mm_P1.27mm.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "SNES_Library:PQFP-64_14x20mm_P1mm"
		(layer "F.Cu")
		(at 128.914 75.25)
		(property "Reference" "U13"
			(at -0.644 -1.717 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "S-SMP"
			(at 0 1 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 2.5 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -10.45 19.75 270)
			(size 1.27 1.27)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 224 "Net-(U13-CPUA4)")
			(pinfunction "CPUA4")
			(pintype "output")
		)
		(pad "2" smd rect
			(at -9 19.75)
			(size 0.6 1.27)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 225 "Net-(U13-CPUA3)")
			(pinfunction "CPUA3")
			(pintype "output")
		)
		(pad "3" smd rect
			(at -8 19.75)
			(size 0.6 1.27)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 226 "Net-(U13-CPUA2)")
			(pinfunction "CPUA2")
			(pintype "output")
		)
		(pad "4" smd rect
			(at -7 19.75)
			(size 0.6 1.27)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 227 "Net-(U13-CPUA1)")
			(pinfunction "CPUA1")
			(pintype "output")
		)
		(pad "5" smd rect
			(at -6 19.75)
			(size 0.6 1.27)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 228 "Net-(U13-CPUA0)")
			(pinfunction "CPUA0")
			(pintype "output")
		)
		(pad "6" smd rect
			(at -5 19.75)
			(size 0.6 1.27)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 229 "Net-(U13-CPUD7)")
			(pinfunction "CPUD7")
			(pintype "bidirectional")
		)
		(pad "7" smd rect
			(at -4 19.75)
			(size 0.6 1.27)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 230 "Net-(U13-CPUD6)")
			(pinfunction "CPUD6")
			(pintype "bidirectional")
		)
		(pad "8" smd rect
			(at -3 19.75)
			(size 0.6 1.27)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 231 "Net-(U13-CPUD5)")
			(pinfunction "CPUD5")
			(pintype "bidirectional")
		)
		(pad "9" smd rect
			(at -2 19.75)
			(size 0.6 1.27)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 232 "Net-(U13-CPUD4)")
			(pinfunction "CPUD4")
			(pintype "bidirectional")
		)
		(pad "10" smd rect
			(at -1 19.75)
			(size 0.6 1.27)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 233 "Net-(U13-CPUD3)")
			(pinfunction "CPUD3")
			(pintype "bidirectional")
		)
		(pad "11" smd rect
			(at 0 19.75)
			(size 0.6 1.27)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 234 "Net-(U13-CPUD2)")
			(pinfunction "CPUD2")
			(pintype "bidirectional")
		)
		(pad "12" smd rect
			(at 1 19.75)
			(size 0.6 1.27)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 235 "Net-(U13-CPUD1)")
			(pinfunction "CPUD1")
			(pintype "bidirectional")
		)
		(pad "13" smd rect
			(at 2 19.75)
			(size 0.6 1.27)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 236 "Net-(U13-CPUD0)")
			(pinfunction "CPUD0")
			(pintype "bidirectional")
		)
		(pad "14" smd rect
			(at 3 19.75)
			(size 0.6 1.27)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 237 "Net-(U13-PD3)")
			(pinfunction "PD3")
			(pintype "input")
		)
		(pad "15" smd rect
			(at 4 19.75)
			(size 0.6 1.27)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 238 "Net-(U13-PD2)")
			(pinfunction "PD2")
			(pintype "output")
		)
		(pad "16" smd rect
			(at 5 19.75)
			(size 0.6 1.27)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 239 "Net-(U13-CPUK)")
			(pinfunction "CPUK")
			(pintype "input")
		)
		(pad "17" smd rect
			(at 6 19.75)
			(size 0.6 1.27)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 407 "Net-(U13-P5RD)")
			(pinfunction "P5RD")
			(pintype "output")
		)
		(pad "18" smd rect
			(at 7 19.75)
			(size 0.6 1.27)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 240 "Net-(U13-P57)")
			(pinfunction "P57")
			(pintype "bidirectional")
		)
		(pad "19" smd rect
			(at 8.45 19.75 270)
			(size 1.27 1.27)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 241 "Net-(U13-P56)")
			(pinfunction "P56")
			(pintype "bidirectional")
		)
		(pad "20" smd rect
			(at 11 17.5 270)
			(size 1.27 1.27)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 242 "Net-(U13-P55)")
			(pinfunction "P55")
			(pintype "bidirectional")
		)
		(pad "21" smd rect
			(at 11 16 270)
			(size 0.6 1.27)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 243 "Net-(U13-P54)")
			(pinfunction "P54")
			(pintype "bidirectional")
		)
		(pad "22" smd rect
			(at 11 15 270)
			(size 0.6 1.27)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 244 "Net-(U13-P53)")
			(pinfunction "P53")
			(pintype "bidirectional")
		)
		(pad "23" smd rect
			(at 11 14 270)
			(size 0.6 1.27)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 245 "Net-(U13-P52)")
			(pinfunction "P52")
			(pintype "bidirectional")
		)
		(pad "24" smd rect
			(at 11 13 270)
			(size 0.6 1.27)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 246 "Net-(U13-P51)")
			(pinfunction "P51")
			(pintype "bidirectional")
		)
		(pad "25" smd rect
			(at 11 12 270)
			(size 0.6 1.27)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 247 "Net-(U13-P50)")
			(pinfunction "P50")
			(pintype "bidirectional")
		)
		(pad "26" smd rect
			(at 11 11 270)
			(size 0.6 1.27)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 127 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "27" smd rect
			(at 11 10 270)
			(size 0.6 1.27)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 248 "unconnected-(U13-P47-Pad27)")
			(pinfunction "P47")
			(pintype "bidirectional+no_connect")
		)
		(pad "28" smd rect
			(at 11 9 270)
			(size 0.6 1.27)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 249 "unconnected-(U13-P46-Pad28)")
			(pinfunction "P46")
			(pintype "bidirectional+no_connect")
		)
		(pad "29" smd rect
			(at 11 8 270)
			(size 0.6 1.27)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 250 "unconnected-(U13-P45-Pad29)")
			(pinfunction "P45")
			(pintype "bidirectional+no_connect")
		)
		(pad "30" smd rect
			(at 11 7 270)
			(size 0.6 1.27)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 251 "unconnected-(U13-P44-Pad30)")
			(pinfunction "P44")
			(pintype "bidirectional+no_connect")
		)
		(pad "31" smd rect
			(at 11 6 270)
			(size 0.6 1.27)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 252 "unconnected-(U13-P43-Pad31)")
			(pinfunction "P43")
			(pintype "bidirectional+no_connect")
		)
		(pad "32" smd rect
			(at 11 4.5 270)
			(size 1.27 1.27)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 253 "unconnected-(U13-P42-Pad32)")
			(pinfunction "P42")
			(pintype "bidirectional+no_connect")
		)
		(pad "33" smd rect
			(at 8.5 2.25 270)
			(size 1.27 1.27)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 254 "unconnected-(U13-P41-Pad33)")
			(pinfunction "P41")
			(pintype "bidirectional+no_connect")
		)
		(pad "34" smd rect
			(at 7 2.25)
			(size 0.6 1.27)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 255 "unconnected-(U13-P40-Pad34)")
			(pinfunction "P40")
			(pintype "bidirectional+no_connect")
		)
		(pad "35" smd rect
			(at 6 2.25)
			(size 0.6 1.27)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 388 "Net-(U13-T1)")
			(pinfunction "T1")
			(pintype "input")
		)
		(pad "36" smd rect
			(at 5 2.25)
			(size 0.6 1.27)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 389 "Net-(U13-T0)")
			(pinfunction "T0")
			(pintype "input")
		)
		(pad "37" smd rect
			(at 4 2.25)
			(size 0.6 1.27)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 77 "{slash}RESOUT1")
			(pinfunction "RESET")
			(pintype "input")
		)
		(pad "38" smd rect
			(at 3 2.25)
			(size 0.6 1.27)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 40 "/D7")
			(pinfunction "D7")
			(pintype "bidirectional")
		)
		(pad "39" smd rect
			(at 2 2.25)
			(size 0.6 1.27)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 39 "/D6")
			(pinfunction "D6")
			(pintype "bidirectional")
		)
		(pad "40" smd rect
			(at 1 2.25)
			(size 0.6 1.27)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 38 "/D5")
			(pinfunction "D5")
			(pintype "bidirectional")
		)
		(pad "41" smd rect
			(at 0 2.25)
			(size 0.6 1.27)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 37 "/D4")
			(pinfunction "D4")
			(pintype "bidirectional")
		)
		(pad "42" smd rect
			(at -1 2.25)
			(size 0.6 1.27)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 36 "/D3")
			(pinfunction "D3")
			(pintype "bidirectional")
		)
		(pad "43" smd rect
			(at -2 2.25)
			(size 0.6 1.27)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 35 "/D2")
			(pinfunction "D2")
			(pintype "bidirectional")
		)
		(pad "44" smd rect
			(at -3 2.25)
			(size 0.6 1.27)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 34 "/D1")
			(pinfunction "D1")
			(pintype "bidirectional")
		)
		(pad "45" smd rect
			(at -4 2.25)
			(size 0.6 1.27)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 33 "/D0")
			(pinfunction "D0")
			(pintype "bidirectional")
		)
		(pad "46" smd rect
			(at -5 2.25)
			(size 0.6 1.27)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 41 "/{slash}PARD")
			(pinfunction "RD")
			(pintype "input")
		)
		(pad "47" smd rect
			(at -6 2.25)
			(size 0.6 1.27)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 50 "/{slash}PAWR")
			(pinfunction "WR")
			(pintype "input")
		)
		(pad "48" smd rect
			(at -7 2.25)
			(size 0.6 1.27)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 310 "/PA1")
			(pinfunction "A1")
			(pintype "input")
		)
		(pad "49" smd rect
			(at -8 2.25)
			(size 0.6 1.27)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 307 "/PA0")
			(pinfunction "A0")
			(pintype "input")
		)
		(pad "50" smd rect
			(at -9 2.25)
			(size 0.6 1.27)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 313 "/PA6")
			(pinfunction "CS")
			(pintype "input")
		)
		(pad "51" smd rect
			(at -10.5 2.25 270)
			(size 1.27 1.27)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 314 "/PA7")
			(pinfunction "~{CS}")
			(pintype "input")
		)
		(pad "52" smd rect
			(at -13 4.5 270)
			(size 1.27 1.27)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 256 "Net-(U13-CPUA15)")
			(pinfunction "CPUA15")
			(pintype "output")
		)
		(pad "53" smd rect
			(at -13.05 6 270)
			(size 0.6 1.27)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 257 "Net-(U13-CPUA14)")
			(pinfunction "CPUA14")
			(pintype "output")
		)
		(pad "54" smd rect
			(at -13.05 7 270)
			(size 0.6 1.27)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 258 "Net-(U13-CPUA13)")
			(pinfunction "CPUA13")
			(pintype "output")
		)
		(pad "55" smd rect
			(at -13.05 8 270)
			(size 0.6 1.27)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 259 "Net-(U13-CPUA12)")
			(pinfunction "CPUA12")
			(pintype "output")
		)
		(pad "56" smd rect
			(at -13.05 9 270)
			(size 0.6 1.27)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 260 "Net-(U13-CPUA11)")
			(pinfunction "CPUA11")
			(pintype "output")
		)
		(pad "57" smd rect
			(at -13.05 10 270)
			(size 0.6 1.27)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 72 "VCC")
			(pinfunction "Vcc")
			(pintype "power_in")
		)
		(pad "58" smd rect
			(at -13.05 11 270)
			(size 0.6 1.27)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 127 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "59" smd rect
			(at -13.05 12 270)
			(size 0.6 1.27)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 261 "Net-(U13-CPUA10)")
			(pinfunction "CPUA10")
			(pintype "output")
		)
		(pad "60" smd rect
			(at -13.05 13 270)
			(size 0.6 1.27)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 262 "Net-(U13-CPUA9)")
			(pinfunction "CPUA9")
			(pintype "output")
		)
		(pad "61" smd rect
			(at -13.05 14 270)
			(size 0.6 1.27)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 263 "Net-(U13-CPUA8)")
			(pinfunction "CPUA8")
			(pintype "output")
		)
		(pad "62" smd rect
			(at -13.05 15 270)
			(size 0.6 1.27)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 264 "Net-(U13-CPUA7)")
			(pinfunction "CPUA7")
			(pintype "output")
		)
		(pad "63" smd rect
			(at -13.05 16 270)
			(size 0.6 1.27)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 265 "Net-(U13-CPUA6)")
			(pinfunction "CPUA6")
			(pintype "output")
		)
		(pad "64" smd rect
			(at -13 17.45 270)
			(size 1.27 1.27)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 266 "Net-(U13-CPUA5)")
			(pinfunction "CPUA5")
			(pintype "output")
		)
		(embedded_fonts no)
		(model "${KICAD7_3DMODEL_DIR}/Package_QFP.3dshapes/PQFP-80_14x20mm_P0.8mm.wrl"
			(offset
				(xyz -1 -11 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 -90)
			)
		)
	)
	(footprint "SNES_Library:PQFP-80_15x22mm_P0.8mm"
		(layer "F.Cu")
		(at 127.375 109.96 90)
		(descr "PQFP80 14x20 / QIP80E CASE 122BS (see ON Semiconductor 122BS.PDF)")
		(tags "QFP 0.8")
		(property "Reference" "U14"
			(at 11.916 -5.074 0)
			(layer "F.SilkS")
		)
		(property "Value" "S-DSP"
			(at 0 12.8 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -8.3 -9.5 90)
			(size 1.5 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 267 "unconnected-(U14-DKD-Pad1)")
			(pinfunction "DKD")
			(pintype "output+no_connect")
		)
		(pad "2" smd rect
			(at -8.3 -8.4 90)
			(size 1.5 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 268 "unconnected-(U14-MXK-Pad2)")
			(pinfunction "MXK")
			(pintype "output+no_connect")
		)
		(pad "3" smd rect
			(at -8.3 -7.6 90)
			(size 1.5 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 269 "unconnected-(U14-MX1-Pad3)")
			(pinfunction "MX1")
			(pintype "output+no_connect")
		)
		(pad "4" smd rect
			(at -8.3 -6.8 90)
			(size 1.5 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 270 "unconnected-(U14-MX2-Pad4)")
			(pinfunction "MX2")
			(pintype "output+no_connect")
		)
		(pad "5" smd rect
			(at -8.3 -6 90)
			(size 1.5 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 271 "unconnected-(U14-MX3-Pad5)")
			(pinfunction "MX3")
			(pintype "output+no_connect")
		)
		(pad "6" smd rect
			(at -8.3 -5.2 90)
			(size 1.5 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 192 "/MD2")
			(pinfunction "MD2")
			(pintype "bidirectional")
		)
		(pad "7" smd rect
			(at -8.3 -4.4 90)
			(size 1.5 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 191 "/MD1")
			(pinfunction "MD1")
			(pintype "bidirectional")
		)
		(pad "8" smd rect
			(at -8.3 -3.6 90)
			(size 1.5 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 190 "/MD0")
			(pinfunction "MD0")
			(pintype "bidirectional")
		)
		(pad "9" smd rect
			(at -8.3 -2.8 90)
			(size 1.5 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 198 "/MA0")
			(pinfunction "MA0")
			(pintype "output")
		)
		(pad "10" smd rect
			(at -8.3 -2 90)
			(size 1.5 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 199 "/MA1")
			(pinfunction "MA1")
			(pintype "output")
		)
		(pad "11" smd rect
			(at -8.3 -1.2 90)
			(size 1.5 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 200 "/MA2")
			(pinfunction "MA2")
			(pintype "output")
		)
		(pad "12" smd rect
			(at -8.3 -0.4 90)
			(size 1.5 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 127 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "13" smd rect
			(at -8.3 0.4 90)
			(size 1.5 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 201 "/MA3")
			(pinfunction "MA3")
			(pintype "output")
		)
		(pad "14" smd rect
			(at -8.3 1.2 90)
			(size 1.5 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 202 "/MA4")
			(pinfunction "MA4")
			(pintype "output")
		)
		(pad "15" smd rect
			(at -8.3 2 90)
			(size 1.5 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 204 "/MA5")
			(pinfunction "MA5")
			(pintype "output")
		)
		(pad "16" smd rect
			(at -8.3 2.8 90)
			(size 1.5 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 205 "/MA6")
			(pinfunction "MA6")
			(pintype "output")
		)
		(pad "17" smd rect
			(at -8.3 3.6 90)
			(size 1.5 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 206 "/MA7")
			(pinfunction "MA7")
			(pintype "output")
		)
		(pad "18" smd rect
			(at -8.3 4.4 90)
			(size 1.5 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 207 "/MA12")
			(pinfunction "MA12")
			(pintype "output")
		)
		(pad "19" smd rect
			(at -8.3 5.2 90)
			(size 1.5 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 208 "/MA14")
			(pinfunction "MA14")
			(pintype "output")
		)
		(pad "20" smd rect
			(at -8.3 6 90)
			(size 1.5 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 272 "unconnected-(U14-MA15-Pad20)")
			(pinfunction "MA15")
			(pintype "output+no_connect")
		)
		(pad "21" smd rect
			(at -8.3 6.8 90)
			(size 1.5 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 273 "unconnected-(U14-DIP-Pad21)")
			(pinfunction "DIP")
			(pintype "unspecified+no_connect")
		)
		(pad "22" smd rect
			(at -8.3 7.6 90)
			(size 1.5 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 193 "/MD3")
			(pinfunction "MD3")
			(pintype "bidirectional")
		)
		(pad "23" smd rect
			(at -8.3 8.4 90)
			(size 1.5 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 194 "/MD4")
			(pinfunction "MD4")
			(pintype "bidirectional")
		)
		(pad "24" smd rect
			(at -8.3 9.5 90)
			(size 1.5 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 195 "/MD5")
			(pinfunction "MD5")
			(pintype "bidirectional")
		)
		(pad "25" smd rect
			(at -6.3 11.3 180)
			(size 1.5 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 196 "/MD6")
			(pinfunction "MD6")
			(pintype "bidirectional")
		)
		(pad "26" smd rect
			(at -5.2 11.3 180)
			(size 1.5 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 197 "/MD7")
			(pinfunction "MD7")
			(pintype "bidirectional")
		)
		(pad "27" smd rect
			(at -4.4 11.3 180)
			(size 1.5 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 376 "/{slash}SCE1")
			(pinfunction "CE1")
			(pintype "output")
		)
		(pad "28" smd rect
			(at -3.6 11.3 180)
			(size 1.5 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 377 "/{slash}SCE0")
			(pinfunction "CE0")
			(pintype "output")
		)
		(pad "29" smd rect
			(at -2.8 11.3 180)
			(size 1.5 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 209 "/MA10")
			(pinfunction "MA10")
			(pintype "output")
		)
		(pad "30" smd rect
			(at -2 11.3 180)
			(size 1.5 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 378 "/{slash}SOE")
			(pinfunction "OE")
			(pintype "output")
		)
		(pad "31" smd rect
			(at -1.2 11.3 180)
			(size 1.5 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 210 "/MA11")
			(pinfunction "MA11")
			(pintype "output")
		)
		(pad "32" smd rect
			(at -0.4 11.3 180)
			(size 1.5 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 211 "/MA9")
			(pinfunction "MA9")
			(pintype "output")
		)
		(pad "33" smd rect
			(at 0.4 11.3 180)
			(size 1.5 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 72 "VCC")
			(pinfunction "Vcc")
			(pintype "power_in")
		)
		(pad "34" smd rect
			(at 1.2 11.3 180)
			(size 1.5 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 212 "/MA8")
			(pinfunction "MA8")
			(pintype "output")
		)
		(pad "35" smd rect
			(at 2 11.3 180)
			(size 1.5 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 213 "/MA13")
			(pinfunction "MA13")
			(pintype "output")
		)
		(pad "36" smd rect
			(at 2.8 11.3 180)
			(size 1.5 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 379 "/{slash}SWE")
			(pinfunction "WE")
			(pintype "output")
		)
		(pad "37" smd rect
			(at 3.6 11.3 180)
			(size 1.5 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 391 "unconnected-(U14-TF-Pad37)")
			(pinfunction "TF")
			(pintype "input+no_connect")
		)
		(pad "38" smd rect
			(at 4.4 11.3 180)
			(size 1.5 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 392 "unconnected-(U14-TK-Pad38)")
			(pinfunction "TK")
			(pintype "input+no_connect")
		)
		(pad "39" smd rect
			(at 5.2 11.3 180)
			(size 1.5 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 382 "Net-(U14-~{MUTE})")
			(pinfunction "~{MUTE}")
			(pintype "output")
		)
		(pad "40" smd rect
			(at 6.3 11.3 180)
			(size 1.5 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 275 "unconnected-(U14-MCK-Pad40)")
			(pinfunction "MCK")
			(pintype "unspecified+no_connect")
		)
		(pad "41" smd rect
			(at 8.3 9.5 90)
			(size 1.5 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 276 "unconnected-(U14-SCLK-Pad41)")
			(pinfunction "SCLK")
			(pintype "no_connect")
		)
		(pad "42" smd rect
			(at 8.3 8.4 90)
			(size 1.5 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 216 "Net-(U14-BCK)")
			(pinfunction "BCK")
			(pintype "output")
		)
		(pad "43" smd rect
			(at 8.3 7.6 90)
			(size 1.5 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 217 "Net-(U14-LRCK)")
			(pinfunction "LRCK")
			(pintype "output")
		)
		(pad "44" smd rect
			(at 8.3 6.8 90)
			(size 1.5 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 218 "Net-(U14-DATA)")
			(pinfunction "DATA")
			(pintype "output")
		)
		(pad "45" smd rect
			(at 8.3 6 90)
			(size 1.5 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 214 "Net-(U14-XTAL0)")
			(pinfunction "XTAL0")
			(pintype "output")
		)
		(pad "46" smd rect
			(at 8.3 5.2 90)
			(size 1.5 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 215 "Net-(U14-XTAL1)")
			(pinfunction "XTAL1")
			(pintype "input")
		)
		(pad "47" smd rect
			(at 8.3 4.4 90)
			(size 1.5 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 77 "{slash}RESOUT1")
			(pinfunction "RESET")
			(pintype "input")
		)
		(pad "48" smd rect
			(at 8.3 3.6 90)
			(size 1.5 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 239 "Net-(U13-CPUK)")
			(pinfunction "CPUK")
			(pintype "output")
		)
		(pad "49" smd rect
			(at 8.3 2.8 90)
			(size 1.5 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 238 "Net-(U13-PD2)")
			(pinfunction "PD2")
			(pintype "input")
		)
		(pad "50" smd rect
			(at 8.3 2 90)
			(size 1.5 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 237 "Net-(U13-PD3)")
			(pinfunction "PD3")
			(pintype "output")
		)
		(pad "51" smd rect
			(at 8.3 1.2 90)
			(size 1.5 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 236 "Net-(U13-CPUD0)")
			(pinfunction "D0")
			(pintype "unspecified")
		)
		(pad "52" smd rect
			(at 8.3 0.4 90)
			(size 1.5 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 127 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "53" smd rect
			(at 8.3 -0.4 90)
			(size 1.5 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 235 "Net-(U13-CPUD1)")
			(pinfunction "D1")
			(pintype "bidirectional")
		)
		(pad "54" smd rect
			(at 8.3 -1.2 90)
			(size 1.5 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 234 "Net-(U13-CPUD2)")
			(pinfunction "D2")
			(pintype "bidirectional")
		)
		(pad "55" smd rect
			(at 8.3 -2 90)
			(size 1.5 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 233 "Net-(U13-CPUD3)")
			(pinfunction "D3")
			(pintype "bidirectional")
		)
		(pad "56" smd rect
			(at 8.3 -2.8 90)
			(size 1.5 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 232 "Net-(U13-CPUD4)")
			(pinfunction "D4")
			(pintype "bidirectional")
		)
		(pad "57" smd rect
			(at 8.3 -3.6 90)
			(size 1.5 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 231 "Net-(U13-CPUD5)")
			(pinfunction "D5")
			(pintype "bidirectional")
		)
		(pad "58" smd rect
			(at 8.3 -4.4 90)
			(size 1.5 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 230 "Net-(U13-CPUD6)")
			(pinfunction "D6")
			(pintype "bidirectional")
		)
		(pad "59" smd rect
			(at 8.3 -5.2 90)
			(size 1.5 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 229 "Net-(U13-CPUD7)")
			(pinfunction "D7")
			(pintype "bidirectional")
		)
		(pad "60" smd rect
			(at 8.3 -6 90)
			(size 1.5 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 228 "Net-(U13-CPUA0)")
			(pinfunction "A0")
			(pintype "input")
		)
		(pad "61" smd rect
			(at 8.3 -6.8 90)
			(size 1.5 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 227 "Net-(U13-CPUA1)")
			(pinfunction "A1")
			(pintype "input")
		)
		(pad "62" smd rect
			(at 8.3 -7.6 90)
			(size 1.5 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 226 "Net-(U13-CPUA2)")
			(pinfunction "A2")
			(pintype "input")
		)
		(pad "63" smd rect
			(at 8.3 -8.4 90)
			(size 1.5 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 225 "Net-(U13-CPUA3)")
			(pinfunction "A3")
			(pintype "input")
		)
		(pad "64" smd rect
			(at 8.3 -9.5 90)
			(size 1.5 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 224 "Net-(U13-CPUA4)")
			(pinfunction "A4")
			(pintype "input")
		)
		(pad "65" smd rect
			(at 6.3 -11.3 180)
			(size 1.5 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 266 "Net-(U13-CPUA5)")
			(pinfunction "A5")
			(pintype "input")
		)
		(pad "66" smd rect
			(at 5.2 -11.3 180)
			(size 1.5 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 265 "Net-(U13-CPUA6)")
			(pinfunction "A6")
			(pintype "input")
		)
		(pad "67" smd rect
			(at 4.4 -11.3 180)
			(size 1.5 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 264 "Net-(U13-CPUA7)")
			(pinfunction "A7")
			(pintype "input")
		)
		(pad "68" smd rect
			(at 3.6 -11.3 180)
			(size 1.5 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 263 "Net-(U13-CPUA8)")
			(pinfunction "A8")
			(pintype "input")
		)
		(pad "69" smd rect
			(at 2.8 -11.3 180)
			(size 1.5 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 262 "Net-(U13-CPUA9)")
			(pinfunction "A9")
			(pintype "input")
		)
		(pad "70" smd rect
			(at 2 -11.3 180)
			(size 1.5 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 261 "Net-(U13-CPUA10)")
			(pinfunction "A10")
			(pintype "input")
		)
		(pad "71" smd rect
			(at 1.2 -11.3 180)
			(size 1.5 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 260 "Net-(U13-CPUA11)")
			(pinfunction "A11")
			(pintype "input")
		)
		(pad "72" smd rect
			(at 0.4 -11.3 180)
			(size 1.5 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 259 "Net-(U13-CPUA12)")
			(pinfunction "A12")
			(pintype "input")
		)
		(pad "73" smd rect
			(at -0.4 -11.3 180)
			(size 1.5 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 72 "VCC")
			(pinfunction "Vcc")
			(pintype "power_in")
		)
		(pad "74" smd rect
			(at -1.2 -11.3 180)
			(size 1.5 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 258 "Net-(U13-CPUA13)")
			(pinfunction "A13")
			(pintype "input")
		)
		(pad "75" smd rect
			(at -2 -11.3 180)
			(size 1.5 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 257 "Net-(U13-CPUA14)")
			(pinfunction "A14")
			(pintype "input")
		)
		(pad "76" smd rect
			(at -2.8 -11.3 180)
			(size 1.5 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 256 "Net-(U13-CPUA15)")
			(pinfunction "A15")
			(pintype "input")
		)
		(pad "77" smd rect
			(at -3.6 -11.3 180)
			(size 1.5 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 278 "unconnected-(U14-XCK-Pad77)")
			(pinfunction "XCK")
			(pintype "output+no_connect")
		)
		(pad "78" smd rect
			(at -4.4 -11.3 180)
			(size 1.5 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 338 "Net-(P5-SMPCK)")
			(pinfunction "DCK")
			(pintype "output")
		)
		(pad "79" smd rect
			(at -5.2 -11.3 180)
			(size 1.5 0.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 279 "unconnected-(U14-CK1-Pad79)")
			(pinfunction "CK1")
			(pintype "no_connect")
		)
		(pad "80" smd rect
			(at -6.3 -11.3 180)
			(size 1.5 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 280 "unconnected-(U14-CK2-Pad80)")
			(pinfunction "CK2")
			(pintype "no_connect")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Package_QFP.3dshapes/PQFP-80_14x20mm_P0.8mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_Elec_6.3x5.4"
		(layer "F.Cu")
		(at 94.615 135.0035 90)
		(descr "SMD capacitor, aluminum electrolytic nonpolar, 6.3x5.4mm")
		(tags "capacitor electrolytic nonpolar")
		(property "Reference" "C66"
			(at -0.1245 -4.445 90)
			(layer "F.SilkS")
		)
		(property "Value" "10uF 50V"
			(at 0 4.35 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Polarized capacitor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "CP_*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -2.5375 0 90)
			(size 3.325 1.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.15625)
			(net 289 "Net-(P4-Audio-L)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 2.5375 0 90)
			(size 3.325 1.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.15625)
			(net 380 "Net-(C66-Pad2)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_Elec_6.3x5.4.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "SNES_Library:PQFP-100_14x20mm_P0.65mm"
		(layer "F.Cu")
		(at 185.725 130.6 90)
		(descr "PQFP, 100 Pin (http://www.microsemi.com/index.php?option=com_docman&task=doc_download&gid=131095), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "PQFP QFP")
		(property "Reference" "U3"
			(at 12.109 -0.051 0)
			(layer "F.SilkS")
		)
		(property "Value" "PPU2"
			(at 1.3648 -0.0002 180)
			(layer "F.SilkS")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr smd)
		(fp_text user "50"
			(at 7.537 11.125 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "51"
			(at 10.16 9.22 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "81"
			(at 6.267 -15.799 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "80"
			(at 11.601 -11.862 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "100"
			(at -8.338 -17.45 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "30"
			(at -13.418 7.442 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "1"
			(at -12 -10.668 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "31"
			(at -8.338 13.157 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -8.75 -9.7 90)
			(size 1.75 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 374 "Net-(U3-BURST)")
			(pinfunction "BURST")
			(pintype "output")
		)
		(pad "2" smd roundrect
			(at -8.75 -8.775 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 111 "unconnected-(U3-PED-Pad2)")
			(pinfunction "PED")
			(pintype "no_connect")
		)
		(pad "3" smd roundrect
			(at -8.75 -8.125 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 112 "unconnected-(U3-3.58M-Pad3)")
			(pinfunction "3.58M")
			(pintype "output+no_connect")
		)
		(pad "4" smd roundrect
			(at -8.75 -7.475 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 113 "unconnected-(U3-TOUMEI-Pad4)")
			(pinfunction "TOUMEI")
			(pintype "no_connect")
		)
		(pad "5" smd roundrect
			(at -8.75 -6.825 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 72 "VCC")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(pad "6" smd roundrect
			(at -8.75 -6.175 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 50 "/{slash}PAWR")
			(pinfunction "PAWR")
			(pintype "input")
		)
		(pad "7" smd roundrect
			(at -8.75 -5.525 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 41 "/{slash}PARD")
			(pinfunction "PARD")
			(pintype "input")
		)
		(pad "8" smd roundrect
			(at -8.75 -4.875 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 40 "/D7")
			(pinfunction "D7")
			(pintype "bidirectional")
		)
		(pad "9" smd roundrect
			(at -8.75 -4.225 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 39 "/D6")
			(pinfunction "D6")
			(pintype "bidirectional")
		)
		(pad "10" smd roundrect
			(at -8.75 -3.575 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 38 "/D5")
			(pinfunction "D5")
			(pintype "bidirectional")
		)
		(pad "11" smd roundrect
			(at -8.75 -2.925 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 37 "/D4")
			(pinfunction "D4")
			(pintype "bidirectional")
		)
		(pad "12" smd roundrect
			(at -8.75 -2.275 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 36 "/D3")
			(pinfunction "D3")
			(pintype "bidirectional")
		)
		(pad "13" smd roundrect
			(at -8.75 -1.625 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 35 "/D2")
			(pinfunction "D2")
			(pintype "bidirectional")
		)
		(pad "14" smd roundrect
			(at -8.75 -0.975 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 34 "/D1")
			(pinfunction "D1")
			(pintype "bidirectional")
		)
		(pad "15" smd roundrect
			(at -8.75 -0.325 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 33 "/D0")
			(pinfunction "D0")
			(pintype "bidirectional")
		)
		(pad "16" smd roundrect
			(at -8.75 0.325 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 127 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "17" smd roundrect
			(at -8.75 0.975 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 314 "/PA7")
			(pinfunction "PA7")
			(pintype "input")
		)
		(pad "18" smd roundrect
			(at -8.75 1.625 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 313 "/PA6")
			(pinfunction "PA6")
			(pintype "input")
		)
		(pad "19" smd roundrect
			(at -8.75 2.275 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 312 "/PA5")
			(pinfunction "PA5")
			(pintype "input")
		)
		(pad "20" smd roundrect
			(at -8.75 2.925 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 309 "/PA4")
			(pinfunction "PA4")
			(pintype "input")
		)
		(pad "21" smd roundrect
			(at -8.75 3.575 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 311 "/PA3")
			(pinfunction "PA3")
			(pintype "input")
		)
		(pad "22" smd roundrect
			(at -8.75 4.225 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 308 "/PA2")
			(pinfunction "PA2")
			(pintype "input")
		)
		(pad "23" smd roundrect
			(at -8.75 4.875 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 310 "/PA1")
			(pinfunction "PA1")
			(pintype "input")
		)
		(pad "24" smd roundrect
			(at -8.75 5.525 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 307 "/PA0")
			(pinfunction "PA0")
			(pintype "input")
		)
		(pad "25" smd roundrect
			(at -8.75 6.175 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 30 "Net-(U1-HBLANK)")
			(pinfunction "HBLANK")
			(pintype "output")
		)
		(pad "26" smd roundrect
			(at -8.75 6.825 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 31 "Net-(U1-VBLANK)")
			(pinfunction "VBLANK")
			(pintype "output")
		)
		(pad "27" smd roundrect
			(at -8.75 7.475 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 75 "Net-(U3-5MOUT)")
			(pinfunction "5MOUT")
			(pintype "output")
		)
		(pad "28" smd roundrect
			(at -8.75 8.125 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 390 "Net-(U3-RESOUT1)")
			(pinfunction "RESOUT1")
			(pintype "output")
		)
		(pad "29" smd roundrect
			(at -8.75 8.775 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 287 "EXTLATCH")
			(pinfunction "EXTLATCH")
			(pintype "bidirectional")
		)
		(pad "30" smd roundrect
			(at -8.75 9.7 90)
			(size 1.75 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 72 "VCC")
			(pinfunction "PALMODE")
			(pintype "input")
		)
		(pad "31" smd roundrect
			(at -6.5 12.05 90)
			(size 1 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 26 "XIN")
			(pinfunction "XIN")
			(pintype "input")
		)
		(pad "32" smd roundrect
			(at -5.525 12.05 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 72 "VCC")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(pad "33" smd roundrect
			(at -4.875 12.05 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 52 "{slash}RESOUT0")
			(pinfunction "RESOUT0")
			(pintype "output")
		)
		(pad "34" smd roundrect
			(at -4.225 12.05 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 297 "~{RESET}")
			(pinfunction "~{RESET}")
			(pintype "input")
		)
		(pad "35" smd roundrect
			(at -3.575 12.05 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 127 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "36" smd roundrect
			(at -2.925 12.05 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 329 "FIELD")
			(pinfunction "FIELD")
			(pintype "unspecified")
		)
		(pad "37" smd roundrect
			(at -2.275 12.05 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 328 "OVER")
			(pinfunction "OVER1")
			(pintype "unspecified")
		)
		(pad "38" smd roundrect
			(at -1.625 12.05 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 327 "5MIN")
			(pinfunction "5MIN")
			(pintype "input")
		)
		(pad "39" smd roundrect
			(at -0.975 12.05 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 326 "HCLD")
			(pinfunction "HCLD")
			(pintype "unspecified")
		)
		(pad "40" smd roundrect
			(at -0.325 12.05 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 325 "VCLD")
			(pinfunction "VCLD")
			(pintype "unspecified")
		)
		(pad "41" smd roundrect
			(at 0.325 12.05 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 324 "COLOR0")
			(pinfunction "COLOR0")
			(pintype "unspecified")
		)
		(pad "42" smd roundrect
			(at 0.975 12.05 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 323 "COLOR1")
			(pinfunction "COLOR1")
			(pintype "unspecified")
		)
		(pad "43" smd roundrect
			(at 1.625 12.05 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 322 "COLOR2")
			(pinfunction "COLOR2")
			(pintype "unspecified")
		)
		(pad "44" smd roundrect
			(at 2.275 12.05 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 321 "PRIO0")
			(pinfunction "PRIO0")
			(pintype "unspecified")
		)
		(pad "45" smd roundrect
			(at 2.925 12.05 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 320 "PRIO1")
			(pinfunction "PRIO1")
			(pintype "unspecified")
		)
		(pad "46" smd roundrect
			(at 3.575 12.05 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 319 "CHR0")
			(pinfunction "CHR0")
			(pintype "unspecified")
		)
		(pad "47" smd roundrect
			(at 4.225 12.05 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 318 "CHR1")
			(pinfunction "CHR1")
			(pintype "unspecified")
		)
		(pad "48" smd roundrect
			(at 4.875 12.05 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 317 "CHR2")
			(pinfunction "CHR2")
			(pintype "unspecified")
		)
		(pad "49" smd roundrect
			(at 5.525 12.05 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 316 "CHR3")
			(pinfunction "CHR3")
			(pintype "unspecified")
		)
		(pad "50" smd roundrect
			(at 6.5 12.05 90)
			(size 1 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 328 "OVER")
			(pinfunction "OVER2")
			(pintype "input")
		)
		(pad "51" smd roundrect
			(at 8.8 9.7 90)
			(size 1.75 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 136 "/VDB0")
			(pinfunction "VDB0")
			(pintype "bidirectional")
		)
		(pad "52" smd roundrect
			(at 8.8 8.775 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 137 "/VDB1")
			(pinfunction "VDB1")
			(pintype "bidirectional")
		)
		(pad "53" smd roundrect
			(at 8.8 8.125 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 138 "/VDB2")
			(pinfunction "VDB2")
			(pintype "bidirectional")
		)
		(pad "54" smd roundrect
			(at 8.8 7.475 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 139 "/VDB3")
			(pinfunction "VDB3")
			(pintype "bidirectional")
		)
		(pad "55" smd roundrect
			(at 8.8 6.825 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 140 "/VDB4")
			(pinfunction "VDB4")
			(pintype "bidirectional")
		)
		(pad "56" smd roundrect
			(at 8.8 6.175 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 141 "/VDB5")
			(pinfunction "VDB5")
			(pintype "bidirectional")
		)
		(pad "57" smd roundrect
			(at 8.8 5.525 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 142 "/VDB6")
			(pinfunction "VDB6")
			(pintype "bidirectional")
		)
		(pad "58" smd roundrect
			(at 8.8 4.875 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 143 "/VDB7")
			(pinfunction "VDB7")
			(pintype "bidirectional")
		)
		(pad "59" smd roundrect
			(at 8.8 4.225 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 72 "VCC")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(pad "60" smd roundrect
			(at 8.8 3.575 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 144 "/VDA0")
			(pinfunction "VDA0")
			(pintype "bidirectional")
		)
		(pad "61" smd roundrect
			(at 8.8 2.925 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 145 "/VDA1")
			(pinfunction "VDA1")
			(pintype "bidirectional")
		)
		(pad "62" smd roundrect
			(at 8.8 2.275 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 146 "/VDA2")
			(pinfunction "VDA2")
			(pintype "bidirectional")
		)
		(pad "63" smd roundrect
			(at 8.8 1.625 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 147 "/VDA3")
			(pinfunction "VDA3")
			(pintype "bidirectional")
		)
		(pad "64" smd roundrect
			(at 8.8 0.975 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 148 "/VDA4")
			(pinfunction "VDA4")
			(pintype "bidirectional")
		)
		(pad "65" smd roundrect
			(at 8.8 0.325 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 149 "/VDA5")
			(pinfunction "VDA5")
			(pintype "bidirectional")
		)
		(pad "66" smd roundrect
			(at 8.8 -0.325 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 150 "/VDA6")
			(pinfunction "VDA6")
			(pintype "bidirectional")
		)
		(pad "67" smd roundrect
			(at 8.8 -0.975 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 151 "/VDA7")
			(pinfunction "VDA7")
			(pintype "bidirectional")
		)
		(pad "68" smd roundrect
			(at 8.8 -1.625 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 127 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "69" smd roundrect
			(at 8.8 -2.275 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 136 "/VDB0")
			(pinfunction "EXT0")
			(pintype "input")
		)
		(pad "70" smd roundrect
			(at 8.8 -2.925 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 137 "/VDB1")
			(pinfunction "EXT1")
			(pintype "input")
		)
		(pad "71" smd roundrect
			(at 8.8 -3.575 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 138 "/VDB2")
			(pinfunction "EXT2")
			(pintype "input")
		)
		(pad "72" smd roundrect
			(at 8.8 -4.225 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 139 "/VDB3")
			(pinfunction "EXT3")
			(pintype "input")
		)
		(pad "73" smd roundrect
			(at 8.8 -4.875 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 140 "/VDB4")
			(pinfunction "EXT4")
			(pintype "input")
		)
		(pad "74" smd roundrect
			(at 8.8 -5.525 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 141 "/VDB5")
			(pinfunction "EXT5")
			(pintype "input")
		)
		(pad "75" smd roundrect
			(at 8.8 -6.175 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 142 "/VDB6")
			(pinfunction "EXT6")
			(pintype "input")
		)
		(pad "76" smd roundrect
			(at 8.8 -6.825 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 143 "/VDB7")
			(pinfunction "EXT7")
			(pintype "input")
		)
		(pad "77" smd roundrect
			(at 8.8 -7.475 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 114 "unconnected-(U3-TST0-Pad77)")
			(pinfunction "TST0")
			(pintype "input+no_connect")
		)
		(pad "78" smd roundrect
			(at 8.8 -8.125 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 115 "unconnected-(U3-TST1-Pad78)")
			(pinfunction "TST1")
			(pintype "input+no_connect")
		)
		(pad "79" smd roundrect
			(at 8.8 -8.775 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 116 "unconnected-(U3-TST2-Pad79)")
			(pinfunction "TST2")
			(pintype "input+no_connect")
		)
		(pad "80" smd roundrect
			(at 8.8 -9.7 90)
			(size 1.75 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 117 "unconnected-(U3-TST3-Pad80)")
			(pinfunction "TST3")
			(pintype "input+no_connect")
		)
		(pad "81" smd roundrect
			(at 6.5 -12 90)
			(size 1 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 118 "unconnected-(U3-TST4-Pad81)")
			(pinfunction "TST4")
			(pintype "input+no_connect")
		)
		(pad "82" smd roundrect
			(at 5.525 -12 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 119 "unconnected-(U3-TST5-Pad82)")
			(pinfunction "TST5")
			(pintype "input+no_connect")
		)
		(pad "83" smd roundrect
			(at 4.875 -12 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 72 "VCC")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(pad "84" smd roundrect
			(at 4.225 -12 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 120 "unconnected-(U3-TST6-Pad84)")
			(pinfunction "TST6")
			(pintype "input+no_connect")
		)
		(pad "85" smd roundrect
			(at 3.575 -12 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 121 "unconnected-(U3-TST7-Pad85)")
			(pinfunction "TST7")
			(pintype "input+no_connect")
		)
		(pad "86" smd roundrect
			(at 2.925 -12 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 122 "unconnected-(U3-TST8-Pad86)")
			(pinfunction "TST8")
			(pintype "input+no_connect")
		)
		(pad "87" smd roundrect
			(at 2.275 -12 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 123 "unconnected-(U3-TST9-Pad87)")
			(pinfunction "TST9")
			(pintype "input+no_connect")
		)
		(pad "88" smd roundrect
			(at 1.625 -12 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 124 "unconnected-(U3-TST10-Pad88)")
			(pinfunction "TST10")
			(pintype "input+no_connect")
		)
		(pad "89" smd roundrect
			(at 0.975 -12 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 125 "unconnected-(U3-TST11-Pad89)")
			(pinfunction "TST11")
			(pintype "input+no_connect")
		)
		(pad "90" smd roundrect
			(at 0.325 -12 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 127 "GND")
			(pinfunction "TST12")
			(pintype "input")
		)
		(pad "91" smd roundrect
			(at -0.325 -12 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 127 "GND")
			(pinfunction "TST13")
			(pintype "input")
		)
		(pad "92" smd roundrect
			(at -0.975 -12 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 127 "GND")
			(pinfunction "TST14")
			(pintype "input")
		)
		(pad "93" smd roundrect
			(at -1.625 -12 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 127 "GND")
			(pinfunction "TST15")
			(pintype "unspecified")
		)
		(pad "94" smd roundrect
			(at -2.275 -12 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 72 "VCC")
			(pinfunction "AVCC")
			(pintype "unspecified")
		)
		(pad "95" smd roundrect
			(at -2.925 -12 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 349 "Net-(Q3-B)")
			(pinfunction "R")
			(pintype "output")
		)
		(pad "96" smd roundrect
			(at -3.575 -12 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 356 "Net-(Q5-B)")
			(pinfunction "G")
			(pintype "output")
		)
		(pad "97" smd roundrect
			(at -4.225 -12 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 384 "Net-(Q7-B)")
			(pinfunction "B")
			(pintype "output")
		)
		(pad "98" smd roundrect
			(at -4.875 -12 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 127 "GND")
			(pinfunction "HVCMODE")
			(pintype "input")
		)
		(pad "99" smd roundrect
			(at -5.525 -12 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 127 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "100" smd roundrect
			(at -6.5 -12 90)
			(size 1 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 375 "Net-(U3-CSYNC)")
			(pinfunction "CSYNC")
			(pintype "output")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Package_QFP.3dshapes/PQFP-100_14x20mm_P0.65mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "SNES_Library:PQFP-100_14x20mm_P0.65mm"
		(layer "F.Cu")
		(at 216.925 130.6 90)
		(descr "PQFP, 100 Pin (http://www.microsemi.com/index.php?option=com_docman&task=doc_download&gid=131095), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "PQFP QFP")
		(property "Reference" "U2"
			(at 12.109 -1.152 0)
			(layer "F.SilkS")
		)
		(property "Value" "PPU1"
			(at 0.5012 -0.009 180)
			(layer "F.SilkS")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr smd)
		(fp_text user "100"
			(at -8.719 -15.249 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "30"
			(at -13.037 8.754 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "31"
			(at -8.338 13.199 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "1"
			(at -12 -10.668 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "80"
			(at 11.347 -12.328 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "50"
			(at 6.858 13.453 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "51"
			(at 10.204 9.262 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "81"
			(at 6.775 -15.884 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -8.75 -9.7 90)
			(size 1.75 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 127 "GND")
			(pinfunction "TST1")
			(pintype "input")
		)
		(pad "2" smd roundrect
			(at -8.75 -8.775 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 127 "GND")
			(pinfunction "TST0")
			(pintype "input")
		)
		(pad "3" smd roundrect
			(at -8.75 -8.125 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 41 "/{slash}PARD")
			(pinfunction "PARD")
			(pintype "input")
		)
		(pad "4" smd roundrect
			(at -8.75 -7.475 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 50 "/{slash}PAWR")
			(pinfunction "PAWR")
			(pintype "input")
		)
		(pad "5" smd roundrect
			(at -8.75 -6.825 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 314 "/PA7")
			(pinfunction "PA7")
			(pintype "input")
		)
		(pad "6" smd roundrect
			(at -8.75 -6.175 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 313 "/PA6")
			(pinfunction "PA6")
			(pintype "input")
		)
		(pad "7" smd roundrect
			(at -8.75 -5.525 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 312 "/PA5")
			(pinfunction "PA5")
			(pintype "input")
		)
		(pad "8" smd roundrect
			(at -8.75 -4.875 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 309 "/PA4")
			(pinfunction "PA4")
			(pintype "input")
		)
		(pad "9" smd roundrect
			(at -8.75 -4.225 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 311 "/PA3")
			(pinfunction "PA3")
			(pintype "input")
		)
		(pad "10" smd roundrect
			(at -8.75 -3.575 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 308 "/PA2")
			(pinfunction "PA2")
			(pintype "input")
		)
		(pad "11" smd roundrect
			(at -8.75 -2.925 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 310 "/PA1")
			(pinfunction "PA1")
			(pintype "input")
		)
		(pad "12" smd roundrect
			(at -8.75 -2.275 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 307 "/PA0")
			(pinfunction "PA0")
			(pintype "input")
		)
		(pad "13" smd roundrect
			(at -8.75 -1.625 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 72 "VCC")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(pad "14" smd roundrect
			(at -8.75 -0.975 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 40 "/D7")
			(pinfunction "D7")
			(pintype "bidirectional")
		)
		(pad "15" smd roundrect
			(at -8.75 -0.325 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 39 "/D6")
			(pinfunction "D6")
			(pintype "bidirectional")
		)
		(pad "16" smd roundrect
			(at -8.75 0.325 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 38 "/D5")
			(pinfunction "D5")
			(pintype "bidirectional")
		)
		(pad "17" smd roundrect
			(at -8.75 0.975 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 37 "/D4")
			(pinfunction "D4")
			(pintype "bidirectional")
		)
		(pad "18" smd roundrect
			(at -8.75 1.625 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 36 "/D3")
			(pinfunction "D3")
			(pintype "bidirectional")
		)
		(pad "19" smd roundrect
			(at -8.75 2.275 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 35 "/D2")
			(pinfunction "D2")
			(pintype "bidirectional")
		)
		(pad "20" smd roundrect
			(at -8.75 2.925 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 34 "/D1")
			(pinfunction "D1")
			(pintype "bidirectional")
		)
		(pad "21" smd roundrect
			(at -8.75 3.575 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 33 "/D0")
			(pinfunction "D0")
			(pintype "bidirectional")
		)
		(pad "22" smd roundrect
			(at -8.75 4.225 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 127 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "23" smd roundrect
			(at -8.75 4.875 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 127 "GND")
			(pinfunction "HVCMODE")
			(pintype "input")
		)
		(pad "24" smd roundrect
			(at -8.75 5.525 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 72 "VCC")
			(pinfunction "PALMODE")
			(pintype "input")
		)
		(pad "25" smd roundrect
			(at -8.75 6.175 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 127 "GND")
			(pinfunction "MASTER")
			(pintype "input")
		)
		(pad "26" smd roundrect
			(at -8.75 6.825 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 72 "VCC")
			(pinfunction "EXTSYNC")
			(pintype "input")
		)
		(pad "27" smd roundrect
			(at -8.75 7.475 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 80 "unconnected-(U2-NC-Pad27)")
			(pinfunction "NC")
			(pintype "no_connect")
		)
		(pad "28" smd roundrect
			(at -8.75 8.125 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 136 "/VDB0")
			(pinfunction "VDB0")
			(pintype "bidirectional")
		)
		(pad "29" smd roundrect
			(at -8.75 8.775 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 137 "/VDB1")
			(pinfunction "VDB1")
			(pintype "bidirectional")
		)
		(pad "30" smd roundrect
			(at -8.75 9.7 90)
			(size 1.75 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 138 "/VDB2")
			(pinfunction "VDB2")
			(pintype "bidirectional")
		)
		(pad "31" smd roundrect
			(at -6.5 12.05 90)
			(size 1 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 139 "/VDB3")
			(pinfunction "VDB3")
			(pintype "bidirectional")
		)
		(pad "32" smd roundrect
			(at -5.525 12.05 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 140 "/VDB4")
			(pinfunction "VDB4")
			(pintype "bidirectional")
		)
		(pad "33" smd roundrect
			(at -4.875 12.05 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 141 "/VDB5")
			(pinfunction "VDB5")
			(pintype "bidirectional")
		)
		(pad "34" smd roundrect
			(at -4.225 12.05 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 142 "/VDB6")
			(pinfunction "VDB6")
			(pintype "bidirectional")
		)
		(pad "35" smd roundrect
			(at -3.575 12.05 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 143 "/VDB7")
			(pinfunction "VDB7")
			(pintype "bidirectional")
		)
		(pad "36" smd roundrect
			(at -2.925 12.05 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 72 "VCC")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(pad "37" smd roundrect
			(at -2.275 12.05 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 144 "/VDA0")
			(pinfunction "VDA0")
			(pintype "bidirectional")
		)
		(pad "38" smd roundrect
			(at -1.625 12.05 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 145 "/VDA1")
			(pinfunction "VDA1")
			(pintype "bidirectional")
		)
		(pad "39" smd roundrect
			(at -0.975 12.05 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 146 "/VDA2")
			(pinfunction "VDA2")
			(pintype "bidirectional")
		)
		(pad "40" smd roundrect
			(at -0.325 12.05 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 147 "/VDA3")
			(pinfunction "VDA3")
			(pintype "bidirectional")
		)
		(pad "41" smd roundrect
			(at 0.325 12.05 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 148 "/VDA4")
			(pinfunction "VDA4")
			(pintype "bidirectional")
		)
		(pad "42" smd roundrect
			(at 0.975 12.05 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 149 "/VDA5")
			(pinfunction "VDA5")
			(pintype "bidirectional")
		)
		(pad "43" smd roundrect
			(at 1.625 12.05 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 150 "/VDA6")
			(pinfunction "VDA6")
			(pintype "bidirectional")
		)
		(pad "44" smd roundrect
			(at 2.275 12.05 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 151 "/VDA7")
			(pinfunction "VDA7")
			(pintype "bidirectional")
		)
		(pad "45" smd roundrect
			(at 2.925 12.05 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 127 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "46" smd roundrect
			(at 3.575 12.05 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 89 "unconnected-(U2-VA15-Pad46)")
			(pinfunction "VA15")
			(pintype "output+no_connect")
		)
		(pad "47" smd roundrect
			(at 4.225 12.05 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 81 "/VA14")
			(pinfunction "VA15")
			(pintype "output")
		)
		(pad "48" smd roundrect
			(at 4.875 12.05 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 82 "/VAB13")
			(pinfunction "VAB13")
			(pintype "output")
		)
		(pad "49" smd roundrect
			(at 5.525 12.05 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 83 "/VAB12")
			(pinfunction "VAB12")
			(pintype "output")
		)
		(pad "50" smd roundrect
			(at 6.5 12.05 90)
			(size 1 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 84 "/VAB11")
			(pinfunction "VAB11")
			(pintype "output")
		)
		(pad "51" smd roundrect
			(at 8.8 9.7 90)
			(size 1.75 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 85 "/VAB10")
			(pinfunction "VAB10")
			(pintype "output")
		)
		(pad "52" smd roundrect
			(at 8.8 8.775 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 86 "/VAB9")
			(pinfunction "VAB9")
			(pintype "output")
		)
		(pad "53" smd roundrect
			(at 8.8 8.125 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 87 "/VAB8")
			(pinfunction "VAB8")
			(pintype "output")
		)
		(pad "54" smd roundrect
			(at 8.8 7.475 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 88 "/VAB7")
			(pinfunction "VAB7")
			(pintype "output")
		)
		(pad "55" smd roundrect
			(at 8.8 6.825 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 90 "/VAB6")
			(pinfunction "VAB6")
			(pintype "output")
		)
		(pad "56" smd roundrect
			(at 8.8 6.175 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 91 "/VAB5")
			(pinfunction "VAB5")
			(pintype "output")
		)
		(pad "57" smd roundrect
			(at 8.8 5.525 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 92 "/VAB4")
			(pinfunction "VAB4")
			(pintype "output")
		)
		(pad "58" smd roundrect
			(at 8.8 4.875 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 93 "/VAB3")
			(pinfunction "VAB3")
			(pintype "output")
		)
		(pad "59" smd roundrect
			(at 8.8 4.225 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 94 "/VAB2")
			(pinfunction "VAB2")
			(pintype "output")
		)
		(pad "60" smd roundrect
			(at 8.8 3.575 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 95 "/VAB1")
			(pinfunction "VAB1")
			(pintype "output")
		)
		(pad "61" smd roundrect
			(at 8.8 2.925 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 96 "/VAB0")
			(pinfunction "VAB0")
			(pintype "output")
		)
		(pad "62" smd roundrect
			(at 8.8 2.275 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 72 "VCC")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(pad "63" smd roundrect
			(at 8.8 1.625 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 97 "/VAA13")
			(pinfunction "VAA13")
			(pintype "output")
		)
		(pad "64" smd roundrect
			(at 8.8 0.975 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 98 "/VAA12")
			(pinfunction "VAA12")
			(pintype "output")
		)
		(pad "65" smd roundrect
			(at 8.8 0.325 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 99 "/VAA11")
			(pinfunction "VAA11")
			(pintype "output")
		)
		(pad "66" smd roundrect
			(at 8.8 -0.325 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 100 "/VAA10")
			(pinfunction "VAA10")
			(pintype "output")
		)
		(pad "67" smd roundrect
			(at 8.8 -0.975 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 101 "/VAA9")
			(pinfunction "VAA9")
			(pintype "output")
		)
		(pad "68" smd roundrect
			(at 8.8 -1.625 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 102 "/VAA8")
			(pinfunction "VAA8")
			(pintype "output")
		)
		(pad "69" smd roundrect
			(at 8.8 -2.275 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 103 "/VAA7")
			(pinfunction "VAA7")
			(pintype "output")
		)
		(pad "70" smd roundrect
			(at 8.8 -2.925 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 104 "/VAA6")
			(pinfunction "VAA6")
			(pintype "output")
		)
		(pad "71" smd roundrect
			(at 8.8 -3.575 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 105 "/VAA5")
			(pinfunction "VAA5")
			(pintype "output")
		)
		(pad "72" smd roundrect
			(at 8.8 -4.225 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 106 "/VAA4")
			(pinfunction "VAA4")
			(pintype "output")
		)
		(pad "73" smd roundrect
			(at 8.8 -4.875 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 107 "/VAA3")
			(pinfunction "VAA3")
			(pintype "output")
		)
		(pad "74" smd roundrect
			(at 8.8 -5.525 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 108 "/VAA2")
			(pinfunction "VAA2")
			(pintype "output")
		)
		(pad "75" smd roundrect
			(at 8.8 -6.175 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 109 "/VAA1")
			(pinfunction "VAA1")
			(pintype "output")
		)
		(pad "76" smd roundrect
			(at 8.8 -6.825 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 110 "/VAA0")
			(pinfunction "VAA0")
			(pintype "output")
		)
		(pad "77" smd roundrect
			(at 8.8 -7.475 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 127 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "78" smd roundrect
			(at 8.8 -8.125 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 46 "{slash}VAWR")
			(pinfunction "VAWR")
			(pintype "output")
		)
		(pad "79" smd roundrect
			(at 8.8 -8.775 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 47 "{slash}VBWR")
			(pinfunction "VBWR")
			(pintype "output")
		)
		(pad "80" smd roundrect
			(at 8.8 -9.7 90)
			(size 1.75 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 48 "{slash}VRD")
			(pinfunction "VRD")
			(pintype "output")
		)
		(pad "81" smd roundrect
			(at 6.5 -12 90)
			(size 1 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 72 "VCC")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(pad "82" smd roundrect
			(at 5.525 -12 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 316 "CHR3")
			(pinfunction "CHR3")
			(pintype "unspecified")
		)
		(pad "83" smd roundrect
			(at 4.875 -12 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 317 "CHR2")
			(pinfunction "CHR2")
			(pintype "unspecified")
		)
		(pad "84" smd roundrect
			(at 4.225 -12 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 318 "CHR1")
			(pinfunction "CHR1")
			(pintype "unspecified")
		)
		(pad "85" smd roundrect
			(at 3.575 -12 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 319 "CHR0")
			(pinfunction "CHR0")
			(pintype "unspecified")
		)
		(pad "86" smd roundrect
			(at 2.925 -12 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 320 "PRIO1")
			(pinfunction "PRIO1")
			(pintype "unspecified")
		)
		(pad "87" smd roundrect
			(at 2.275 -12 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 321 "PRIO0")
			(pinfunction "PRIO0")
			(pintype "unspecified")
		)
		(pad "88" smd roundrect
			(at 1.625 -12 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 322 "COLOR2")
			(pinfunction "COLOR2")
			(pintype "unspecified")
		)
		(pad "89" smd roundrect
			(at 0.975 -12 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 323 "COLOR1")
			(pinfunction "COLOR1")
			(pintype "unspecified")
		)
		(pad "90" smd roundrect
			(at 0.325 -12 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 324 "COLOR0")
			(pinfunction "COLOR0")
			(pintype "unspecified")
		)
		(pad "91" smd roundrect
			(at -0.325 -12 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 325 "VCLD")
			(pinfunction "VCLD")
			(pintype "unspecified")
		)
		(pad "92" smd roundrect
			(at -0.975 -12 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 326 "HCLD")
			(pinfunction "HCLD")
			(pintype "unspecified")
		)
		(pad "93" smd roundrect
			(at -1.625 -12 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 327 "5MIN")
			(pinfunction "5MOUT")
			(pintype "output")
		)
		(pad "94" smd roundrect
			(at -2.275 -12 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 328 "OVER")
			(pinfunction "~{OVER}")
			(pintype "output")
		)
		(pad "95" smd roundrect
			(at -2.925 -12 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 329 "FIELD")
			(pinfunction "FIELD")
			(pintype "unspecified")
		)
		(pad "96" smd roundrect
			(at -3.575 -12 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 127 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "97" smd roundrect
			(at -4.225 -12 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 327 "5MIN")
			(pinfunction "5MIN")
			(pintype "input")
		)
		(pad "98" smd roundrect
			(at -4.875 -12 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 52 "{slash}RESOUT0")
			(pinfunction "RESET")
			(pintype "input")
		)
		(pad "99" smd roundrect
			(at -5.525 -12 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 127 "GND")
			(pinfunction "TST2")
			(pintype "input")
		)
		(pad "100" smd roundrect
			(at -6.5 -12 90)
			(size 1 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 26 "XIN")
			(pinfunction "XIN")
			(pintype "input")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Package_QFP.3dshapes/PQFP-100_14x20mm_P0.65mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Inductor_SMD:L_CommonMode_Delevan_4222"
		(layer "F.Cu")
		(at 83.185 193.735 90)
		(descr "API Delevan, Surface Mount Common Mode Bead, 4222 4222R, http://www.delevan.com/seriesPDFs/4222.pdf")
		(tags "surface mount common mode bead")
		(property "Reference" "T1"
			(at -0.06 5.08 180)
			(layer "F.SilkS")
		)
		(property "Value" "L_Coupled"
			(at 0 4 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Coupled inductor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Choke_* *Coil* Inductor_* L_*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -3.75 -1.27 90)
			(size 3 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 70 "Net-(C30-Pad2)")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -3.75 1.27 90)
			(size 3 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 69 "Net-(C30-Pad1)")
			(pinfunction "2")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at 3.75 1.27 90)
			(size 3 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 73 "Net-(C31-Pad1)")
			(pinfunction "3")
			(pintype "passive")
		)
		(pad "4" smd rect
			(at 3.75 -1.27 90)
			(size 3 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 74 "Net-(C31-Pad2)")
			(pinfunction "4")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_CommonMode_Delevan_4222.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "SNES_Library:CASSETTE"
		(layer "F.Cu")
		(at 151.094 133 -90)
		(descr "DIN41612 connector, type R, Vertical, 3 rows 32 pins wide, https://www.erni-x-press.com/de/downloads/kataloge/englische_kataloge/erni-din41612-iec60603-2-e.pdf")
		(tags "DIN 41612 IEC 60603 R")
		(property "Reference" "P1"
			(at -0.12 -8.065 90)
			(layer "F.SilkS")
		)
		(property "Value" "CASSETTE"
			(at -6.525 0.38 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr through_hole)
		(fp_circle
			(center -47.5 0)
			(end -46 0)
			(fill no)
			(layer "Edge.Cuts")
		)
		(fp_circle
			(center 47.5 0)
			(end 49 0)
			(fill no)
			(layer "Edge.Cuts")
		)
		(fp_text user "10"
			(at 13.812 -6.132 270)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "25"
			(at -23.399 -6.132 270)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "15"
			(at 1.366 -6.132 270)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "20"
			(at -11.207 -6.513 270)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "5"
			(at 26.766 -6.767 270)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "1"
			(at 41.625 -6.386 270)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "55"
			(at -21 7.965 270)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "62"
			(at -43.5 7.5 270)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "31"
			(at -43.5 -6 270)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "${REFERENCE}"
			(at -0.12 8.445 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 42.5 -3.556 180)
			(size 1.55 1.55)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 26 "XIN")
			(pinfunction "MCK_21M")
			(pintype "unspecified")
		)
		(pad "2" thru_hole rect
			(at 40 -3.556 180)
			(size 1.55 1.55)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 352 "Net-(P1-EXPAND)")
			(pinfunction "EXPAND")
			(pintype "unspecified")
		)
		(pad "3" thru_hole rect
			(at 37.5 -3.556 180)
			(size 1.55 1.55)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 313 "/PA6")
			(pinfunction "PA6")
			(pintype "unspecified")
		)
		(pad "4" thru_hole rect
			(at 35 -3.556 180)
			(size 1.55 1.55)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 41 "/{slash}PARD")
			(pinfunction "PARD")
			(pintype "unspecified")
		)
		(pad "5" thru_hole rect
			(at 27.5 -3.556 180)
			(size 1.55 1.55)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 127 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "6" thru_hole rect
			(at 25 -3.556 180)
			(size 1.55 1.55)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "/CA11")
			(pinfunction "A11")
			(pintype "input")
		)
		(pad "7" thru_hole rect
			(at 22.5 -3.466 180)
			(size 1.55 1.55)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "/CA10")
			(pinfunction "A10")
			(pintype "input")
		)
		(pad "8" thru_hole rect
			(at 20 -3.556 180)
			(size 1.55 1.55)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "/CA9")
			(pinfunction "A9")
			(pintype "input")
		)
		(pad "9" thru_hole rect
			(at 17.5 -3.556 180)
			(size 1.55 1.55)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "/CA8")
			(pinfunction "A8")
			(pintype "input")
		)
		(pad "10" thru_hole rect
			(at 15 -3.466 180)
			(size 1.55 1.55)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 71 "/CA7")
			(pinfunction "A7")
			(pintype "input")
		)
		(pad "11" thru_hole rect
			(at 12.5 -3.556 180)
			(size 1.55 1.55)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 68 "/CA6")
			(pinfunction "A6")
			(pintype "input")
		)
		(pad "12" thru_hole rect
			(at 10 -3.466 180)
			(size 1.55 1.55)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 67 "/CA5")
			(pinfunction "A5")
			(pintype "input")
		)
		(pad "13" thru_hole rect
			(at 7.5 -3.556 180)
			(size 1.55 1.55)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 66 "/CA4")
			(pinfunction "A4")
			(pintype "input")
		)
		(pad "14" thru_hole rect
			(at 5 -3.556 180)
			(size 1.55 1.55)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 65 "/CA3")
			(pinfunction "A3")
			(pintype "input")
		)
		(pad "15" thru_hole rect
			(at 2.5 -3.556 180)
			(size 1.55 1.55)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 64 "/CA2")
			(pinfunction "A2")
			(pintype "input")
		)
		(pad "16" thru_hole rect
			(at 0 -3.556 180)
			(size 1.55 1.55)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 63 "/CA1")
			(pinfunction "A1")
			(pintype "input")
		)
		(pad "17" thru_hole rect
			(at -2.5 -3.556 180)
			(size 1.55 1.55)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 62 "/CA0")
			(pinfunction "A0")
			(pintype "input")
		)
		(pad "18" thru_hole rect
			(at -5 -3.556 180)
			(size 1.55 1.55)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 336 "{slash}IRQ")
			(pinfunction "IRQ")
			(pintype "unspecified")
		)
		(pad "19" thru_hole rect
			(at -7.5 -3.556 180)
			(size 1.55 1.55)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 33 "/D0")
			(pinfunction "D0")
			(pintype "bidirectional")
		)
		(pad "20" thru_hole rect
			(at -10 -3.556 180)
			(size 1.55 1.55)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 34 "/D1")
			(pinfunction "D1")
			(pintype "bidirectional")
		)
		(pad "21" thru_hole rect
			(at -12.5 -3.556 180)
			(size 1.55 1.55)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 35 "/D2")
			(pinfunction "D2")
			(pintype "bidirectional")
		)
		(pad "22" thru_hole rect
			(at -15 -3.556 180)
			(size 1.55 1.55)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 36 "/D3")
			(pinfunction "D3")
			(pintype "bidirectional")
		)
		(pad "23" thru_hole rect
			(at -17.5 -3.556 180)
			(size 1.55 1.55)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 76 "/{slash}CPURD")
			(pinfunction "RD")
			(pintype "unspecified")
		)
		(pad "24" thru_hole rect
			(at -20 -3.556 180)
			(size 1.55 1.55)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 27 "Net-(P1-CIC0)")
			(pinfunction "CIC0")
			(pintype "unspecified")
		)
		(pad "25" thru_hole rect
			(at -22.5 -3.556 180)
			(size 1.55 1.55)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 28 "Net-(P1-CIC2)")
			(pinfunction "CIC2")
			(pintype "unspecified")
		)
		(pad "26" thru_hole rect
			(at -25 -3.556 180)
			(size 1.55 1.55)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 77 "{slash}RESOUT1")
			(pinfunction "RESET")
			(pintype "unspecified")
		)
		(pad "27" thru_hole rect
			(at -27.5 -3.556 180)
			(size 1.55 1.55)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 72 "VCC")
			(pinfunction "+5V")
			(pintype "power_in")
		)
		(pad "28" thru_hole rect
			(at -35 -3.556 180)
			(size 1.55 1.55)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 307 "/PA0")
			(pinfunction "PA0")
			(pintype "unspecified")
		)
		(pad "29" thru_hole rect
			(at -37.5 -3.556 180)
			(size 1.55 1.55)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 308 "/PA2")
			(pinfunction "PA2")
			(pintype "unspecified")
		)
		(pad "30" thru_hole rect
			(at -40 -3.556 180)
			(size 1.55 1.55)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 309 "/PA4")
			(pinfunction "PA4")
			(pintype "unspecified")
		)
		(pad "31" thru_hole rect
			(at -42.5 -3.556 180)
			(size 1.55 1.55)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 315 "Net-(P1-SOUND-L)")
			(pinfunction "SOUND-L")
			(pintype "output")
		)
		(pad "32" thru_hole rect
			(at 42.582 3.556 180)
			(size 1.55 1.55)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 42 "/{slash}RAMSEL")
			(pinfunction "WRAMSEL")
			(pintype "unspecified")
		)
		(pad "33" thru_hole rect
			(at 40.082 3.556 180)
			(size 1.55 1.55)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 49 "Net-(P1-REFRESH)")
			(pinfunction "REFRESH")
			(pintype "unspecified")
		)
		(pad "34" thru_hole rect
			(at 37.582 3.556 180)
			(size 1.55 1.55)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 314 "/PA7")
			(pinfunction "PA7")
			(pintype "unspecified")
		)
		(pad "35" thru_hole rect
			(at 35.082 3.556 180)
			(size 1.55 1.55)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 50 "/{slash}PAWR")
			(pinfunction "PAWR")
			(pintype "unspecified")
		)
		(pad "36" thru_hole rect
			(at 27.582 3.556 180)
			(size 1.55 1.55)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 127 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "37" thru_hole rect
			(at 25.082 3.556 180)
			(size 1.55 1.55)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 7 "/CA12")
			(pinfunction "A12")
			(pintype "input")
		)
		(pad "38" thru_hole rect
			(at 22.582 3.556 180)
			(size 1.55 1.55)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 8 "/CA13")
			(pinfunction "A13")
			(pintype "input")
		)
		(pad "39" thru_hole rect
			(at 20.082 3.556 180)
			(size 1.55 1.55)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 9 "/CA14")
			(pinfunction "A14")
			(pintype "input")
		)
		(pad "40" thru_hole rect
			(at 17.582 3.556 180)
			(size 1.55 1.55)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 10 "/CA15")
			(pinfunction "A15")
			(pintype "input")
		)
		(pad "41" thru_hole rect
			(at 15.082 3.556 180)
			(size 1.55 1.55)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 11 "/CA16")
			(pinfunction "A16")
			(pintype "input")
		)
		(pad "42" thru_hole rect
			(at 12.582 3.556 180)
			(size 1.55 1.55)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 12 "/CA17")
			(pinfunction "A17")
			(pintype "input")
		)
		(pad "43" thru_hole rect
			(at 10.082 3.556 180)
			(size 1.55 1.55)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 13 "/CA18")
			(pinfunction "A18")
			(pintype "input")
		)
		(pad "44" thru_hole rect
			(at 7.582 3.556 180)
			(size 1.55 1.55)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 14 "/CA19")
			(pinfunction "A19")
			(pintype "input")
		)
		(pad "45" thru_hole rect
			(at 5.082 3.556 180)
			(size 1.55 1.55)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 15 "/CA20")
			(pinfunction "A20")
			(pintype "input")
		)
		(pad "46" thru_hole rect
			(at 2.582 3.556 180)
			(size 1.55 1.55)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 16 "/CA21")
			(pinfunction "A21")
			(pintype "input")
		)
		(pad "47" thru_hole rect
			(at 0.082 3.556 180)
			(size 1.55 1.55)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 17 "/CA22")
			(pinfunction "A22")
			(pintype "input")
		)
		(pad "48" thru_hole rect
			(at -2.418 3.556 180)
			(size 1.55 1.55)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 18 "/CA23")
			(pinfunction "A23")
			(pintype "input")
		)
		(pad "49" thru_hole rect
			(at -4.918 3.556 180)
			(size 1.55 1.55)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 60 "/{slash}ROMSEL")
			(pinfunction "ROMSEL")
			(pintype "unspecified")
		)
		(pad "50" thru_hole rect
			(at -7.418 3.556 180)
			(size 1.55 1.55)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 37 "/D4")
			(pinfunction "D4")
			(pintype "bidirectional")
		)
		(pad "51" thru_hole rect
			(at -9.918 3.556 180)
			(size 1.55 1.55)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 38 "/D5")
			(pinfunction "D5")
			(pintype "bidirectional")
		)
		(pad "52" thru_hole rect
			(at -12.418 3.556 180)
			(size 1.55 1.55)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 39 "/D6")
			(pinfunction "D6")
			(pintype "bidirectional")
		)
		(pad "53" thru_hole rect
			(at -14.918 3.556 180)
			(size 1.55 1.55)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 40 "/D7")
			(pinfunction "D7")
			(pintype "bidirectional")
		)
		(pad "54" thru_hole rect
			(at -17.418 3.556 180)
			(size 1.55 1.55)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 61 "/{slash}CPUWR")
			(pinfunction "WR")
			(pintype "unspecified")
		)
		(pad "55" thru_hole rect
			(at -19.918 3.556 180)
			(size 1.55 1.55)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 29 "Net-(P1-CIC1)")
			(pinfunction "CIC1")
			(pintype "unspecified")
		)
		(pad "56" thru_hole rect
			(at -22.418 3.556 180)
			(size 1.55 1.55)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 25 "Net-(P1-CIC3)")
			(pinfunction "CIC3")
			(pintype "unspecified")
		)
		(pad "57" thru_hole rect
			(at -24.918 3.556 180)
			(size 1.55 1.55)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 79 "SYSCK")
			(pinfunction "SYSCK")
			(pintype "unspecified")
		)
		(pad "58" thru_hole rect
			(at -27.418 3.556 180)
			(size 1.55 1.55)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 72 "VCC")
			(pinfunction "+5V")
			(pintype "power_in")
		)
		(pad "59" thru_hole rect
			(at -34.918 3.556 180)
			(size 1.55 1.55)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 310 "/PA1")
			(pinfunction "PA1")
			(pintype "unspecified")
		)
		(pad "60" thru_hole rect
			(at -37.418 3.556 180)
			(size 1.55 1.55)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 311 "/PA3")
			(pinfunction "PA3")
			(pintype "unspecified")
		)
		(pad "61" thru_hole rect
			(at -39.918 3.556 180)
			(size 1.55 1.55)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 312 "/PA5")
			(pinfunction "PA5")
			(pintype "unspecified")
		)
		(pad "62" thru_hole rect
			(at -42.418 3.556 180)
			(size 1.55 1.55)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 188 "Net-(P1-SOUND-R)")
			(pinfunction "SOUND-R")
			(pintype "output")
		)
		(embedded_fonts no)
		(model "${KICAD7_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_2x34_P2.54mm_Vertical.wrl"
			(offset
				(xyz -42 1 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 -90)
			)
		)
	)
	(footprint "SNES_Library:ResetSwitch"
		(layer "F.Cu")
		(at 216.099 72.646)
		(property "Reference" "SW2"
			(at 0 1 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Value" "Old"
			(at 9 11 270)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Push button switch, generic, two pins"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr through_hole)
		(fp_circle
			(center 1 11)
			(end 2.5 11)
			(fill no)
			(layer "Edge.Cuts")
		)
		(fp_text user "${REFERENCE}"
			(at 0 2.5 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 4.5 16)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 157 "Net-(U8-RES)")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" thru_hole rect
			(at 5 6)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 72 "VCC")
			(pinfunction "2")
			(pintype "passive")
		)
		(pad "3" thru_hole rect
			(at -2.5 6.5)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(pad "4" thru_hole rect
			(at -2.5 15.5)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
		)
		(embedded_fonts no)
	)
	(footprint "SNES_Library:JST_ZE_Controllers"
		(layer "F.Cu")
		(at 272.1718 129.3838 90)
		(descr "JST ZE series connector, B11B-ZESK-D (http://www.jst-mfg.com/product/pdf/eng/eZE.pdf), generated with kicad-footprint-generator")
		(tags "connector JST ZE side entry")
		(property "Reference" "P7"
			(at -0.508 -8.89 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "JST 11FE-BT-VK-N"
			(at 0.14 1.56 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, double row, 11 pins, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*2Rows*Pins__* *FCC*2Rows*Pins__*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr through_hole)
		(fp_text user "2"
			(at -4.318 -9.144 270)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "10"
			(at -6.8872 -3.1096 270)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "1"
			(at -5.842 1.778 270)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "11"
			(at 7.112 1.778 270)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "${REFERENCE}"
			(at 1.41 -5.69 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole custom
			(at -6.36 -0.29 90)
			(size 1.117157 1.117157)
			(drill 0.75)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 127 "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
			(options
				(clearance outline)
				(anchor circle)
			)
			(primitives
				(gr_poly
					(pts
						(xy 0.45 -0.225) (xy 0.45 0.625) (xy -0.45 0.625) (xy -0.45 -0.625) (xy 0.05 -0.625)
					)
					(width 0.5)
					(fill yes)
				)
			)
		)
		(pad "2" thru_hole oval
			(at -5 -2.5 90)
			(size 1.4 1.75)
			(drill 0.75)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 431 "Net-(D4-K)")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at -3.86 -0.29 90)
			(size 1.4 1.75)
			(drill 0.75)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 433 "Net-(D6-K)")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole oval
			(at -2.5 -2.5 90)
			(size 1.4 1.75)
			(drill 0.75)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 432 "Net-(D5-K)")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(pad "5" thru_hole oval
			(at -1.36 -0.29 90)
			(size 1.4 1.75)
			(drill 0.75)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 430 "Net-(J4-Pin_5)")
			(pinfunction "Pin_5")
			(pintype "passive")
		)
		(pad "6" thru_hole oval
			(at 0 -2.5 90)
			(size 1.4 1.75)
			(drill 0.75)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 426 "Net-(J4-Pin_4)")
			(pinfunction "Pin_6")
			(pintype "passive")
		)
		(pad "7" thru_hole oval
			(at 1.14 -0.29 90)
			(size 1.4 1.75)
			(drill 0.75)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 429 "Net-(J5-Pin_5)")
			(pinfunction "Pin_7")
			(pintype "passive")
		)
		(pad "8" thru_hole oval
			(at 2.5 -2.5 90)
			(size 1.4 1.75)
			(drill 0.75)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 428 "Net-(J5-Pin_4)")
			(pinfunction "Pin_8")
			(pintype "passive")
		)
		(pad "9" thru_hole oval
			(at 3.64 -0.29 90)
			(size 1.4 1.75)
			(drill 0.75)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 434 "Net-(J5-Pin_6)")
			(pinfunction "Pin_9")
			(pintype "passive")
		)
		(pad "10" thru_hole oval
			(at 5 -2.5 90)
			(size 1.4 1.75)
			(drill 0.75)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 427 "Net-(J4-Pin_6)")
			(pinfunction "Pin_10")
			(pintype "passive")
		)
		(pad "11" thru_hole oval
			(at 6.5 -0.29 90)
			(size 1.4 1.75)
			(drill 0.75)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 421 "Net-(D2-A)")
			(pinfunction "Pin_11")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD7_3DMODEL_DIR}/Connector_JST.3dshapes/JST_GH_BM12B-GHS-TBT_1x12-1MP_P1.25mm_Vertical.wrl"
			(offset
				(xyz 0 2 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "SNES_Library:Controller"
		(layer "F.Cu")
		(at 265.6262 99.3042 90)
		(property "Reference" "J4"
			(at 0 -0.5 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "CONTROLLER 1"
			(at -2.4228 -2.5076 270)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x07, script generated"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr through_hole)
		(fp_text user "7"
			(at 16.3224 -2.152 270)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "1"
			(at -14.3608 -1.9996 270)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "${REFERENCE}"
			(at 0 -2.286 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" thru_hole oval
			(at -12.532 0.134 90)
			(size 2 3)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 420 "Net-(D2-K)")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at -8.532 0.134 90)
			(size 2 3)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 423 "Net-(D5-A)")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at -4.532 0.134 90)
			(size 2 3)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 422 "Net-(D4-A)")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole oval
			(at -0.532 0.134 90)
			(size 2 3)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 426 "Net-(J4-Pin_4)")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(pad "5" thru_hole oval
			(at 5.97 0.134 90)
			(size 2 3)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 430 "Net-(J4-Pin_5)")
			(pinfunction "Pin_5")
			(pintype "passive")
		)
		(pad "6" thru_hole oval
			(at 9.97 0.134 90)
			(size 2 3)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 427 "Net-(J4-Pin_6)")
			(pinfunction "Pin_6")
			(pintype "passive")
		)
		(pad "7" thru_hole oval
			(at 13.97 0.134 90)
			(size 2 3)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 127 "GND")
			(pinfunction "Pin_7")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "Diode_THT:D_T-1_P5.08mm_Horizontal"
		(layer "F.Cu")
		(at 256.2098 101.1682 -90)
		(descr "Diode, T-1 series, Axial, Horizontal, pin pitch=5.08mm, length*diameter=3.2*2.6mm^2, http://www.diodes.com/_files/packages/T-1.pdf")
		(tags "Diode T-1 series Axial Horizontal pin pitch 5.08mm  length 3.2mm diameter 2.6mm")
		(property "Reference" "D4"
			(at 7.9248 1.3208 90)
			(layer "F.SilkS")
		)
		(property "Value" "D"
			(at 2.54 2.42 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Diode"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Device" "D"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TO-???* *_Diode_* *SingleDiode* D_*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr through_hole)
		(fp_text user "K"
			(at 0 -2 270)
			(layer "F.SilkS")
		)
		(fp_text user "${REFERENCE}"
			(at 2.78 0 90)
			(layer "F.Fab")
		)
		(fp_text user "K"
			(at 0 -2 270)
			(layer "F.Fab")
		)
		(pad "1" thru_hole roundrect
			(at 0 0 270)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.125)
			(net 431 "Net-(D4-K)")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 5.08 0 270)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 422 "Net-(D4-A)")
			(pinfunction "A")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Diode_THT.3dshapes/D_T-1_P5.08mm_Horizontal.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_Elec_6.3x5.4"
		(layer "F.Cu")
		(at 127.2125 162.15)
		(descr "SMD capacitor, aluminum electrolytic nonpolar, 6.3x5.4mm")
		(tags "capacitor electrolytic nonpolar")
		(property "Reference" "C61"
			(at 0.3375 4.9 0)
			(layer "F.SilkS")
		)
		(property "Value" "10uF 50V"
			(at 0 4.35 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Polarized capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "CP_*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -2.5375 0)
			(size 3.325 1.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.15625)
			(net 343 "Net-(DA6A-A)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 2.5375 0)
			(size 3.325 1.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.15625)
			(net 127 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_Elec_6.3x5.4.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "SNES_Library:RFModulator"
		(layer "F.Cu")
		(at 102.362 175.006 -90)
		(property "Reference" "J2"
			(at 0 -5.31 270)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "~"
			(at 0 -3.81 270)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr through_hole)
		(fp_circle
			(center -15.24 29)
			(end -13.24 29)
			(fill no)
			(layer "Edge.Cuts")
		)
		(fp_circle
			(center 16.002 29)
			(end 18.002 29)
			(fill no)
			(layer "Edge.Cuts")
		)
		(fp_circle
			(center -0.002517 2.286)
			(end 0 0.762)
			(fill no)
			(layer "Edge.Cuts")
		)
		(fp_text user "${REFERENCE}"
			(at 0 -4.31 270)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at -3.81 8.89 270)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 72 "VCC")
			(pinfunction "+B")
			(pintype "input")
		)
		(pad "2" thru_hole rect
			(at -1.27 8.89 270)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 182 "Net-(J2-Video)")
			(pinfunction "Video")
			(pintype "input")
		)
		(pad "3" thru_hole rect
			(at 1.27 8.89 270)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 78 "Net-(J2-Audio)")
			(pinfunction "Audio")
			(pintype "input")
		)
		(pad "4" thru_hole rect
			(at 3.81 8.89 270)
			(size 2 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 127 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(embedded_fonts no)
	)
	(footprint "Trimmer_THT:SurftrimGKG"
		(layer "F.Cu")
		(at 201.216 192.834 90)
		(property "Reference" "TC1"
			(at -1.222 -1.064 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "20p"
			(at 0 -4 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Trimmable capacitor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 -2.5 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" thru_hole oval
			(at -3 3 180)
			(size 1.6 0.6)
			(drill oval 1.2 0.24)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 127 "GND")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 3 3 180)
			(size 1.6 0.6)
			(drill oval 1.2 0.24)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 406 "Net-(C2-Pad2)")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "Capacitor_SMD:C_Elec_6.3x5.4"
		(layer "F.Cu")
		(at 111.1225 68.326)
		(descr "SMD capacitor, aluminum electrolytic nonpolar, 6.3x5.4mm")
		(tags "capacitor electrolytic nonpolar")
		(property "Reference" "C73"
			(at 6.4795 0.254 0)
			(layer "F.SilkS")
		)
		(property "Value" "47u 10V"
			(at 0 4.35 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Polarized capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "CP_*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -2.5375 0)
			(size 3.325 1.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.15625)
			(net 217 "Net-(U14-LRCK)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 2.5375 0)
			(size 3.325 1.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.15625)
			(net 127 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_Elec_6.3x5.4.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "SNES_Library:JST_ZE_Controllers"
		(layer "F.Cu")
		(at 243.8 133.049 90)
		(descr "JST ZE series connector, B11B-ZESK-D (http://www.jst-mfg.com/product/pdf/eng/eZE.pdf), generated with kicad-footprint-generator")
		(tags "connector JST ZE side entry")
		(property "Reference" "P2"
			(at -0.508 -8.89 90)
			(layer "F.SilkS")
		)
		(property "Value" "JST 11FE-BT-VK-N"
			(at 0.14 1.56 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, double row, 11 pins, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*2Rows*Pins__* *FCC*2Rows*Pins__*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr through_hole)
		(fp_text user "11"
			(at 7.112 1.778 270)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "1"
			(at -5.842 1.778 270)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "2"
			(at -4.318 -9.144 270)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "10"
			(at 6.35 -9.144 270)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "${REFERENCE}"
			(at 1.41 -5.69 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole custom
			(at -6.36 -0.29 90)
			(size 1.117157 1.117157)
			(drill 0.75)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 72 "VCC")
			(pinfunction "Pin_1")
			(pintype "passive")
			(options
				(clearance outline)
				(anchor circle)
			)
			(primitives
				(gr_poly
					(pts
						(xy 0.45 -0.225) (xy 0.45 0.625) (xy -0.45 0.625) (xy -0.45 -0.625) (xy 0.05 -0.625)
					)
					(width 0.5)
					(fill yes)
				)
			)
		)
		(pad "2" thru_hole oval
			(at -5 -2.5 90)
			(size 1.4 1.75)
			(drill 0.75)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 126 "Net-(P2-Pin_2)")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at -3.86 -0.29 90)
			(size 1.4 1.75)
			(drill 0.75)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 128 "Net-(P2-Pin_3)")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole oval
			(at -2.5 -2.5 90)
			(size 1.4 1.75)
			(drill 0.75)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 129 "Net-(P2-Pin_4)")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(pad "5" thru_hole oval
			(at -1.36 -0.29 90)
			(size 1.4 1.75)
			(drill 0.75)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 130 "Net-(P2-Pin_5)")
			(pinfunction "Pin_5")
			(pintype "passive")
		)
		(pad "6" thru_hole oval
			(at 0 -2.5 90)
			(size 1.4 1.75)
			(drill 0.75)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 131 "Net-(P2-Pin_6)")
			(pinfunction "Pin_6")
			(pintype "passive")
		)
		(pad "7" thru_hole oval
			(at 1.14 -0.29 90)
			(size 1.4 1.75)
			(drill 0.75)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 132 "Net-(P2-Pin_7)")
			(pinfunction "Pin_7")
			(pintype "passive")
		)
		(pad "8" thru_hole oval
			(at 2.5 -2.5 90)
			(size 1.4 1.75)
			(drill 0.75)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 133 "Net-(P2-Pin_8)")
			(pinfunction "Pin_8")
			(pintype "passive")
		)
		(pad "9" thru_hole oval
			(at 3.64 -0.29 90)
			(size 1.4 1.75)
			(drill 0.75)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 134 "Net-(P2-Pin_9)")
			(pinfunction "Pin_9")
			(pintype "passive")
		)
		(pad "10" thru_hole oval
			(at 5 -2.5 90)
			(size 1.4 1.75)
			(drill 0.75)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 135 "Net-(P2-Pin_10)")
			(pinfunction "Pin_10")
			(pintype "passive")
		)
		(pad "11" thru_hole oval
			(at 6.5 -0.29 90)
			(size 1.4 1.75)
			(drill 0.75)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 127 "GND")
			(pinfunction "Pin_11")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD7_3DMODEL_DIR}/Connector_JST.3dshapes/JST_GH_BM12B-GHS-TBT_1x12-1MP_P1.25mm_Vertical.wrl"
			(offset
				(xyz 0 2 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:CP_Elec_6.3x3"
		(layer "F.Cu")
		(at 129.9 188.5 -90)
		(descr "SMD capacitor, aluminum electrolytic, Nichicon, 6.3x3.0mm")
		(tags "capacitor electrolytic")
		(property "Reference" "C63"
			(at -7.05 0 270)
			(layer "F.SilkS")
		)
		(property "Value" "33uF 25V"
			(at 0 4.35 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Polarized capacitor"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "CP_*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -2.7 0 270)
			(size 3.5 1.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.15625)
			(net 303 "Net-(DA11-K)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 2.7 0 270)
			(size 3.5 1.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.15625)
			(net 127 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/CP_Elec_6.3x3.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "SNES_Library:PQFP-100_14x20mm_P0.65mm"
		(layer "F.Cu")
		(at 213.4 170.3 90)
		(descr "PQFP, 100 Pin (http://www.microsemi.com/index.php?option=com_docman&task=doc_download&gid=131095), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "PQFP QFP")
		(property "Reference" "U1"
			(at 11.684 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "CPU"
			(at 2.1012 -0.04 180)
			(layer "F.SilkS")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr smd)
		(fp_text user "1"
			(at -12 -10.668 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "31"
			(at -7.62 13.208 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "51"
			(at 10.16 8.89 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "80"
			(at 11.176 -11.684 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "30"
			(at -12.954 8.382 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "100"
			(at -8.636 -17.272 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "50"
			(at 6.858 13.208 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "81"
			(at 6.2 -17.018 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "${REFERENCE}"
			(at -12.7832 2.1444 180)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -8.75 -9.7 90)
			(size 1.75 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 72 "VCC")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(pad "2" smd roundrect
			(at -8.75 -8.775 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 3 "/CA8")
			(pinfunction "A8")
			(pintype "output")
		)
		(pad "3" smd roundrect
			(at -8.75 -8.125 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 4 "/CA9")
			(pinfunction "A9")
			(pintype "output")
		)
		(pad "4" smd roundrect
			(at -8.75 -7.475 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 5 "/CA10")
			(pinfunction "A10")
			(pintype "output")
		)
		(pad "5" smd roundrect
			(at -8.75 -6.825 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 6 "/CA11")
			(pinfunction "A11")
			(pintype "output")
		)
		(pad "6" smd roundrect
			(at -8.75 -6.175 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 7 "/CA12")
			(pinfunction "A12")
			(pintype "output")
		)
		(pad "7" smd roundrect
			(at -8.75 -5.525 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 8 "/CA13")
			(pinfunction "A13")
			(pintype "output")
		)
		(pad "8" smd roundrect
			(at -8.75 -4.875 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 9 "/CA14")
			(pinfunction "A14")
			(pintype "output")
		)
		(pad "9" smd roundrect
			(at -8.75 -4.225 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 10 "/CA15")
			(pinfunction "A15")
			(pintype "output")
		)
		(pad "10" smd roundrect
			(at -8.75 -3.575 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 11 "/CA16")
			(pinfunction "A16")
			(pintype "output")
		)
		(pad "11" smd roundrect
			(at -8.75 -2.925 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 12 "/CA17")
			(pinfunction "A17")
			(pintype "output")
		)
		(pad "12" smd roundrect
			(at -8.75 -2.275 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 13 "/CA18")
			(pinfunction "A18")
			(pintype "output")
		)
		(pad "13" smd roundrect
			(at -8.75 -1.625 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 14 "/CA19")
			(pinfunction "A19")
			(pintype "output")
		)
		(pad "14" smd roundrect
			(at -8.75 -0.975 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 15 "/CA20")
			(pinfunction "A20")
			(pintype "output")
		)
		(pad "15" smd roundrect
			(at -8.75 -0.325 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 16 "/CA21")
			(pinfunction "A21")
			(pintype "output")
		)
		(pad "16" smd roundrect
			(at -8.75 0.325 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 17 "/CA22")
			(pinfunction "A22")
			(pintype "output")
		)
		(pad "17" smd roundrect
			(at -8.75 0.975 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 18 "/CA23")
			(pinfunction "A23")
			(pintype "output")
		)
		(pad "18" smd roundrect
			(at -8.75 1.625 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 127 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "19" smd roundrect
			(at -8.75 2.275 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 19 "unconnected-(U1-PP0-Pad19)")
			(pinfunction "PP0")
			(pintype "bidirectional+no_connect")
		)
		(pad "20" smd roundrect
			(at -8.75 2.925 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 20 "unconnected-(U1-PP1-Pad20)")
			(pinfunction "PP1")
			(pintype "bidirectional+no_connect")
		)
		(pad "21" smd roundrect
			(at -8.75 3.575 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 21 "unconnected-(U1-PP2-Pad21)")
			(pinfunction "PP2")
			(pintype "bidirectional+no_connect")
		)
		(pad "22" smd roundrect
			(at -8.75 4.225 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 22 "unconnected-(U1-PP3-Pad22)")
			(pinfunction "PP3")
			(pintype "bidirectional+no_connect")
		)
		(pad "23" smd roundrect
			(at -8.75 4.875 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 23 "unconnected-(U1-PP4-Pad23)")
			(pinfunction "PP4")
			(pintype "bidirectional+no_connect")
		)
		(pad "24" smd roundrect
			(at -8.75 5.525 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 24 "unconnected-(U1-PP5-Pad24)")
			(pinfunction "PP5")
			(pintype "bidirectional+no_connect")
		)
		(pad "25" smd roundrect
			(at -8.75 6.175 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 288 "/JPIO6")
			(pinfunction "PP6")
			(pintype "bidirectional")
		)
		(pad "26" smd roundrect
			(at -8.75 6.825 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 287 "EXTLATCH")
			(pinfunction "PP7")
			(pintype "bidirectional")
		)
		(pad "27" smd roundrect
			(at -8.75 7.475 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 286 "/4017.D0")
			(pinfunction "4017D0")
			(pintype "input")
		)
		(pad "28" smd roundrect
			(at -8.75 8.125 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 285 "/4017.D1")
			(pinfunction "4017D1")
			(pintype "input")
		)
		(pad "29" smd roundrect
			(at -8.75 8.775 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 127 "GND")
			(pinfunction "4017D2")
			(pintype "input")
		)
		(pad "30" smd roundrect
			(at -8.75 9.7 90)
			(size 1.75 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 127 "GND")
			(pinfunction "4017D3")
			(pintype "input")
		)
		(pad "31" smd roundrect
			(at -6.5 12.05 90)
			(size 1 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 127 "GND")
			(pinfunction "4017D4")
			(pintype "input")
		)
		(pad "32" smd roundrect
			(at -5.525 12.05 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 284 "/4016.D0")
			(pinfunction "4016D0")
			(pintype "input")
		)
		(pad "33" smd roundrect
			(at -4.875 12.05 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 281 "/4016.D1")
			(pinfunction "4016D1")
			(pintype "input")
		)
		(pad "34" smd roundrect
			(at -4.225 12.05 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 72 "VCC")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(pad "35" smd roundrect
			(at -3.575 12.05 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 277 "/JPCLK1")
			(pinfunction "JOY-2-CLK")
			(pintype "output")
		)
		(pad "36" smd roundrect
			(at -2.925 12.05 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 274 "/JPCLK2")
			(pinfunction "JOY-1-CLK")
			(pintype "output")
		)
		(pad "37" smd roundrect
			(at -2.275 12.05 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 223 "/JPSTR")
			(pinfunction "JOY-OUT0")
			(pintype "output")
		)
		(pad "38" smd roundrect
			(at -1.625 12.05 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 299 "Net-(U1-JOY-OUT1)")
			(pinfunction "JOY-OUT1")
			(pintype "output")
		)
		(pad "39" smd roundrect
			(at -0.975 12.05 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 300 "Net-(U1-JOY-OUT2)")
			(pinfunction "JOY-OUT2")
			(pintype "output")
		)
		(pad "40" smd roundrect
			(at -0.325 12.05 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 49 "Net-(P1-REFRESH)")
			(pinfunction "REFRESH")
			(pintype "output")
		)
		(pad "41" smd roundrect
			(at 0.325 12.05 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 127 "GND")
			(pinfunction "TCKSEL0")
			(pintype "input")
		)
		(pad "42" smd roundrect
			(at 0.975 12.05 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 127 "GND")
			(pinfunction "TCKSEL1")
			(pintype "input")
		)
		(pad "43" smd roundrect
			(at 1.625 12.05 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 30 "Net-(U1-HBLANK)")
			(pinfunction "HBLANK")
			(pintype "input")
		)
		(pad "44" smd roundrect
			(at 2.275 12.05 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 31 "Net-(U1-VBLANK)")
			(pinfunction "VBLANK")
			(pintype "input")
		)
		(pad "45" smd roundrect
			(at 2.925 12.05 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 72 "VCC")
			(pinfunction "NMI")
			(pintype "input")
		)
		(pad "46" smd roundrect
			(at 3.575 12.05 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 336 "{slash}IRQ")
			(pinfunction "IRQ")
			(pintype "input")
		)
		(pad "47" smd roundrect
			(at 4.225 12.05 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 127 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "48" smd roundrect
			(at 4.875 12.05 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 26 "XIN")
			(pinfunction "MCK")
			(pintype "input")
		)
		(pad "49" smd roundrect
			(at 5.525 12.05 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 127 "GND")
			(pinfunction "DRAMMODE")
			(pintype "input")
		)
		(pad "50" smd roundrect
			(at 6.5 12.05 90)
			(size 1 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 77 "{slash}RESOUT1")
			(pinfunction "RESET")
			(pintype "input")
		)
		(pad "51" smd roundrect
			(at 8.8 9.7 90)
			(size 1.75 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 307 "/PA0")
			(pinfunction "PA0")
			(pintype "output")
		)
		(pad "52" smd roundrect
			(at 8.8 8.775 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 310 "/PA1")
			(pinfunction "PA1")
			(pintype "output")
		)
		(pad "53" smd roundrect
			(at 8.8 8.125 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 308 "/PA2")
			(pinfunction "PA2")
			(pintype "output")
		)
		(pad "54" smd roundrect
			(at 8.8 7.475 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 311 "/PA3")
			(pinfunction "PA3")
			(pintype "output")
		)
		(pad "55" smd roundrect
			(at 8.8 6.825 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 309 "/PA4")
			(pinfunction "PA4")
			(pintype "output")
		)
		(pad "56" smd roundrect
			(at 8.8 6.175 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 312 "/PA5")
			(pinfunction "PA5")
			(pintype "output")
		)
		(pad "57" smd roundrect
			(at 8.8 5.525 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 313 "/PA6")
			(pinfunction "PA6")
			(pintype "output")
		)
		(pad "58" smd roundrect
			(at 8.8 4.875 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 314 "/PA7")
			(pinfunction "PA7")
			(pintype "output")
		)
		(pad "59" smd roundrect
			(at 8.8 4.225 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 72 "VCC")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(pad "60" smd roundrect
			(at 8.8 3.575 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 33 "/D0")
			(pinfunction "D0")
			(pintype "bidirectional")
		)
		(pad "61" smd roundrect
			(at 8.8 2.925 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 34 "/D1")
			(pinfunction "D1")
			(pintype "bidirectional")
		)
		(pad "62" smd roundrect
			(at 8.8 2.275 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 35 "/D2")
			(pinfunction "D2")
			(pintype "bidirectional")
		)
		(pad "63" smd roundrect
			(at 8.8 1.625 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 36 "/D3")
			(pinfunction "D3")
			(pintype "bidirectional")
		)
		(pad "64" smd roundrect
			(at 8.8 0.975 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 37 "/D4")
			(pinfunction "D4")
			(pintype "bidirectional")
		)
		(pad "65" smd roundrect
			(at 8.8 0.325 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 38 "/D5")
			(pinfunction "D5")
			(pintype "bidirectional")
		)
		(pad "66" smd roundrect
			(at 8.8 -0.325 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 39 "/D6")
			(pinfunction "D6")
			(pintype "bidirectional")
		)
		(pad "67" smd roundrect
			(at 8.8 -0.975 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 40 "/D7")
			(pinfunction "D7")
			(pintype "bidirectional")
		)
		(pad "68" smd roundrect
			(at 8.8 -1.625 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 41 "/{slash}PARD")
			(pinfunction "PARD")
			(pintype "output")
		)
		(pad "69" smd roundrect
			(at 8.8 -2.275 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 50 "/{slash}PAWR")
			(pinfunction "PAWR")
			(pintype "output")
		)
		(pad "70" smd roundrect
			(at 8.8 -2.925 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 43 "unconnected-(U1-DMA-Pad70)")
			(pinfunction "DMA")
			(pintype "output+no_connect")
		)
		(pad "71" smd roundrect
			(at 8.8 -3.575 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 44 "unconnected-(U1-CPUCK-Pad71)")
			(pinfunction "CPUCK")
			(pintype "output+no_connect")
		)
		(pad "72" smd roundrect
			(at 8.8 -4.225 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 79 "SYSCK")
			(pinfunction "SYSCK")
			(pintype "output")
		)
		(pad "73" smd roundrect
			(at 8.8 -4.875 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 127 "GND")
			(pinfunction "TM")
			(pintype "input")
		)
		(pad "74" smd roundrect
			(at 8.8 -5.525 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 127 "GND")
			(pinfunction "HVCMODE")
			(pintype "input")
		)
		(pad "75" smd roundrect
			(at 8.8 -6.175 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 127 "GND")
			(pinfunction "HALT")
			(pintype "input")
		)
		(pad "76" smd roundrect
			(at 8.8 -6.825 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 72 "VCC")
			(pinfunction "ABORT")
			(pintype "input")
		)
		(pad "77" smd roundrect
			(at 8.8 -7.475 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 60 "/{slash}ROMSEL")
			(pinfunction "ROMSEL")
			(pintype "output")
		)
		(pad "78" smd roundrect
			(at 8.8 -8.125 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 42 "/{slash}RAMSEL")
			(pinfunction "RAMSEL")
			(pintype "output")
		)
		(pad "79" smd roundrect
			(at 8.8 -8.775 90)
			(size 1.75 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 127 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "80" smd roundrect
			(at 8.8 -9.7 90)
			(size 1.75 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 51 "unconnected-(U1-R{slash}W-Pad80)")
			(pinfunction "R/W")
			(pintype "output+no_connect")
		)
		(pad "81" smd roundrect
			(at 6.5 -12 90)
			(size 1 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 72 "VCC")
			(pinfunction "RDY")
			(pintype "input")
		)
		(pad "82" smd roundrect
			(at 5.525 -12 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 53 "unconnected-(U1-ML-Pad82)")
			(pinfunction "ML")
			(pintype "output+no_connect")
		)
		(pad "83" smd roundrect
			(at 4.875 -12 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 54 "unconnected-(U1-MF-Pad83)")
			(pinfunction "MF")
			(pintype "output+no_connect")
		)
		(pad "84" smd roundrect
			(at 4.225 -12 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 55 "unconnected-(U1-XF-Pad84)")
			(pinfunction "XF")
			(pintype "output+no_connect")
		)
		(pad "85" smd roundrect
			(at 3.575 -12 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 72 "VCC")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(pad "86" smd roundrect
			(at 2.925 -12 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 56 "unconnected-(U1-VPA-Pad86)")
			(pinfunction "VPA")
			(pintype "output+no_connect")
		)
		(pad "87" smd roundrect
			(at 2.275 -12 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 57 "unconnected-(U1-VDA-Pad87)")
			(pinfunction "VDA")
			(pintype "output+no_connect")
		)
		(pad "88" smd roundrect
			(at 1.625 -12 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 58 "unconnected-(U1-ALCK-Pad88)")
			(pinfunction "ALCK")
			(pintype "output+no_connect")
		)
		(pad "89" smd roundrect
			(at 0.975 -12 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 59 "unconnected-(U1-VP-Pad89)")
			(pinfunction "VP")
			(pintype "output+no_connect")
		)
		(pad "90" smd roundrect
			(at 0.325 -12 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 127 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "91" smd roundrect
			(at -0.325 -12 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 61 "/{slash}CPUWR")
			(pinfunction "CPUWR")
			(pintype "output")
		)
		(pad "92" smd roundrect
			(at -0.975 -12 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 76 "/{slash}CPURD")
			(pinfunction "CPURD")
			(pintype "output")
		)
		(pad "93" smd roundrect
			(at -1.625 -12 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 62 "/CA0")
			(pinfunction "A0")
			(pintype "output")
		)
		(pad "94" smd roundrect
			(at -2.275 -12 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 63 "/CA1")
			(pinfunction "A1")
			(pintype "output")
		)
		(pad "95" smd roundrect
			(at -2.925 -12 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 64 "/CA2")
			(pinfunction "A2")
			(pintype "output")
		)
		(pad "96" smd roundrect
			(at -3.575 -12 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 65 "/CA3")
			(pinfunction "A3")
			(pintype "output")
		)
		(pad "97" smd roundrect
			(at -4.225 -12 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 66 "/CA4")
			(pinfunction "A4")
			(pintype "output")
		)
		(pad "98" smd roundrect
			(at -4.875 -12 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 67 "/CA5")
			(pinfunction "A5")
			(pintype "output")
		)
		(pad "99" smd roundrect
			(at -5.525 -12 90)
			(size 0.4 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 68 "/CA6")
			(pinfunction "A6")
			(pintype "output")
		)
		(pad "100" smd roundrect
			(at -6.5 -12 90)
			(size 1 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 71 "/CA7")
			(pinfunction "A7")
			(pintype "output")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Package_QFP.3dshapes/PQFP-100_14x20mm_P0.65mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "SNES_Library:FullBridgeRectifier"
		(layer "F.Cu")
		(at 107.95 187.452)
		(property "Reference" "DB1"
			(at -0.127 6.858 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "D_Bridge_+A-A"
			(at 0 1 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Diode bridge, +ve/AC/-ve/AC"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "D*Bridge* D*Rectifier*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr through_hole)
		(fp_text user "+"
			(at -5.08 5.08 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "~"
			(at 5.08 3.81 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "~"
			(at -4.318 -4.318 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "${REFERENCE}"
			(at 0 2.5 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at -3.81 3.81)
			(size 1.524 1.524)
			(drill 0.762)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "Net-(DB1-+)")
			(pinfunction "+")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 2.54 2.54)
			(size 1.524 1.524)
			(drill 0.762)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 73 "Net-(C31-Pad1)")
			(pintype "passive")
		)
		(pad "3" thru_hole circle
			(at 2.54 -2.54)
			(size 1.524 1.524)
			(drill 0.762)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 127 "GND")
			(pinfunction "-")
			(pintype "passive")
		)
		(pad "4" thru_hole circle
			(at -2.54 -2.54)
			(size 1.524 1.524)
			(drill 0.762)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 74 "Net-(C31-Pad2)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD7_3DMODEL_DIR}/Diode_THT.3dshapes/Diode_Bridge_Round_D9.0mm.wrl"
			(offset
				(xyz -2.5 2.5 2.5)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "SNES_Library:RAM"
		(layer "F.Cu")
		(at 219.202 105.205 90)
		(descr "SOIC, 18 Pin (JEDEC MS-013AB, https://www.analog.com/media/en/package-pcb-resources/package/33254132129439rw_18.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOIC SO")
		(property "Reference" "U4"
			(at 8.128 -2.54 0)
			(layer "F.SilkS")
		)
		(property "Value" "MS62256CL-10FC"
			(at 0 6.72 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.futurlec.com/Datasheet/Memory/62256.pdf"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "32Kx8 bit Low Power CMOS Static RAM, 55/70ns, DIP-28"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "DIP*W15.24mm*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr smd)
		(fp_text user "14"
			(at -6.35 9.398 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "15"
			(at 4.826 9.398 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "1"
			(at -6.096 -11.176 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "28"
			(at 4.826 -12.446 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -5.6 -8.255 90)
			(size 1.6 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 81 "/VA14")
			(pinfunction "A14")
			(pintype "input")
		)
		(pad "2" smd roundrect
			(at -5.6 -6.985 90)
			(size 1.6 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 83 "/VAB12")
			(pinfunction "A12")
			(pintype "input")
		)
		(pad "3" smd roundrect
			(at -5.6 -5.715 90)
			(size 1.6 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 88 "/VAB7")
			(pinfunction "A7")
			(pintype "input")
		)
		(pad "4" smd roundrect
			(at -5.6 -4.445 90)
			(size 1.6 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 90 "/VAB6")
			(pinfunction "A6")
			(pintype "input")
		)
		(pad "5" smd roundrect
			(at -5.6 -3.175 90)
			(size 1.6 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 91 "/VAB5")
			(pinfunction "A5")
			(pintype "input")
		)
		(pad "6" smd roundrect
			(at -5.6 -1.905 90)
			(size 1.6 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 92 "/VAB4")
			(pinfunction "A4")
			(pintype "input")
		)
		(pad "7" smd roundrect
			(at -5.6 -0.635 90)
			(size 1.6 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 93 "/VAB3")
			(pinfunction "A3")
			(pintype "input")
		)
		(pad "8" smd roundrect
			(at -5.6 0.635 90)
			(size 1.6 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 94 "/VAB2")
			(pinfunction "A2")
			(pintype "input")
		)
		(pad "9" smd roundrect
			(at -5.6 1.905 90)
			(size 1.6 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 95 "/VAB1")
			(pinfunction "A1")
			(pintype "input")
		)
		(pad "10" smd roundrect
			(at -5.6 3.175 90)
			(size 1.6 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 96 "/VAB0")
			(pinfunction "A0")
			(pintype "input")
		)
		(pad "11" smd roundrect
			(at -5.6 4.445 90)
			(size 1.6 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 136 "/VDB0")
			(pinfunction "Q0")
			(pintype "tri_state")
		)
		(pad "12" smd roundrect
			(at -5.6 5.715 90)
			(size 1.6 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 137 "/VDB1")
			(pinfunction "Q1")
			(pintype "tri_state")
		)
		(pad "13" smd roundrect
			(at -5.6 6.985 90)
			(size 1.6 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 138 "/VDB2")
			(pinfunction "Q2")
			(pintype "tri_state")
		)
		(pad "14" smd roundrect
			(at -5.6 8.255 90)
			(size 1.6 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 127 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "15" smd roundrect
			(at 5.6 8.25 90)
			(size 1.6 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 139 "/VDB3")
			(pinfunction "Q3")
			(pintype "tri_state")
		)
		(pad "16" smd roundrect
			(at 5.6 6.98 90)
			(size 1.6 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 140 "/VDB4")
			(pinfunction "Q4")
			(pintype "tri_state")
		)
		(pad "17" smd roundrect
			(at 5.6 5.71 90)
			(size 1.6 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 141 "/VDB5")
			(pinfunction "Q5")
			(pintype "tri_state")
		)
		(pad "18" smd roundrect
			(at 5.6 4.44 90)
			(size 1.6 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 142 "/VDB6")
			(pinfunction "Q6")
			(pintype "tri_state")
		)
		(pad "19" smd roundrect
			(at 5.6 3.17 90)
			(size 1.6 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 143 "/VDB7")
			(pinfunction "Q7")
			(pintype "tri_state")
		)
		(pad "20" smd roundrect
			(at 5.6 1.9 90)
			(size 1.6 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 127 "GND")
			(pinfunction "~{CS}")
			(pintype "input")
		)
		(pad "21" smd roundrect
			(at 5.6 0.63 90)
			(size 1.6 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 85 "/VAB10")
			(pinfunction "A10")
			(pintype "input")
		)
		(pad "22" smd roundrect
			(at 5.6 -0.64 90)
			(size 1.6 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 48 "{slash}VRD")
			(pinfunction "~{OE}")
			(pintype "input")
		)
		(pad "23" smd roundrect
			(at 5.6 -1.91 90)
			(size 1.6 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 84 "/VAB11")
			(pinfunction "A11")
			(pintype "input")
		)
		(pad "24" smd roundrect
			(at 5.6 -3.18 90)
			(size 1.6 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 86 "/VAB9")
			(pinfunction "A9")
			(pintype "input")
		)
		(pad "25" smd roundrect
			(at 5.6 -4.45 90)
			(size 1.6 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 87 "/VAB8")
			(pinfunction "A8")
			(pintype "input")
		)
		(pad "26" smd roundrect
			(at 5.6 -5.72 90)
			(size 1.6 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 82 "/VAB13")
			(pinfunction "A13")
			(pintype "input")
		)
		(pad "27" smd roundrect
			(at 5.6 -6.99 90)
			(size 1.6 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 47 "{slash}VBWR")
			(pinfunction "~{WE}")
			(pintype "input")
		)
		(pad "28" smd roundrect
			(at 5.6 -8.26 90)
			(size 1.6 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 72 "VCC")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(embedded_fonts no)
		(model "${KICAD7_3DMODEL_DIR}/Package_SO.3dshapes/SOIC-28W_7.5x18.7mm_P1.27mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_SMD:SC-59"
		(layer "B.Cu")
		(at 227.273 175.453 180)
		(descr "SC-59, https://lib.chipdip.ru/images/import_diod/original/SOT-23_SC-59.jpg")
		(tags "SC-59")
		(property "Reference" "DA10"
			(at -0.565 -2.855 0)
			(layer "B.SilkS")
		)
		(property "Value" "DAN202"
			(at 0 -2.5 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Dual diode, common anode on pin 1"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.2 0.95 180)
			(size 0.9 0.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 287 "EXTLATCH")
			(pinfunction "A")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at -1.2 -0.95 180)
			(size 0.9 0.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 288 "/JPIO6")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "3" smd roundrect
			(at 1.2 0 180)
			(size 0.9 0.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 72 "VCC")
			(pinfunction "K")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SC-59.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "B.Cu")
		(at 217.297 97.282 180)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP104"
			(at 0 1.448 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 -1.55 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 1.45 180)
			(layer "B.Fab")
		)
		(pad "1" smd circle
			(at 0 0 180)
			(size 1 1)
			(layers "B.Cu" "B.Mask")
			(net 84 "/VAB11")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "B.Cu")
		(at 223.2625 158.15 180)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R74"
			(at 3.4625 -0.6 0)
			(layer "B.SilkS")
		)
		(property "Value" "2.2k"
			(at 0 -1.65 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 180)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902)
			(net 77 "{slash}RESOUT1")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 180)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902)
			(net 390 "Net-(U3-RESOUT1)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "B.Cu")
		(at 185.801 113.538 180)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP52"
			(at 0 1.448 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 -1.55 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 1.45 0)
			(layer "B.Fab")
		)
		(pad "1" smd circle
			(at 0 0 180)
			(size 1 1)
			(layers "B.Cu" "B.Mask")
			(net 105 "/VAA5")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "B.Cu")
		(at 104.8785 153.924)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R72"
			(at -8.4855 8.382 0)
			(layer "B.SilkS")
		)
		(property "Value" "1k"
			(at 0 -1.65 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902)
			(net 304 "+12V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902)
			(net 301 "Net-(DA11-A)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "B.Cu")
		(at 80.4 92.2 180)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP10"
			(at 0 1.448 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 -1.55 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 1.45 0)
			(layer "B.Fab")
		)
		(pad "1" smd circle
			(at 0 0 180)
			(size 1 1)
			(layers "B.Cu" "B.Mask")
			(net 40 "/D7")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "B.Cu")
		(at 180.7445 93.091 180)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R29"
			(at -4.9295 -0.381 0)
			(layer "B.SilkS")
		)
		(property "Value" "3.3k"
			(at 0 -1.65 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 180)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902)
			(net 32 "Net-(U18-4.433M)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 180)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902)
			(net 156 "Net-(C11-Pad2)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "B.Cu")
		(at 185.95 77.8 90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C17"
			(at 3.6 0.232 270)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "10pF"
			(at 0 -1.68 90)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0 90)
			(size 1 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 178 "Net-(Q11-B)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0 90)
			(size 1 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 127 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_SMD:SC-59"
		(layer "B.Cu")
		(at 133.1 154.55 180)
		(descr "SC-59, https://lib.chipdip.ru/images/import_diod/original/SOT-23_SC-59.jpg")
		(tags "SC-59")
		(property "Reference" "Q13"
			(at -9.4 1.388 0)
			(layer "B.SilkS")
		)
		(property "Value" "C2412K"
			(at 0 -2.5 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "NPN transistor, base/emitter/collector"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.2 0.95 180)
			(size 0.9 0.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 381 "Net-(Q13-B)")
			(pinfunction "B")
			(pintype "input")
		)
		(pad "2" smd roundrect
			(at -1.2 -0.95 180)
			(size 0.9 0.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 127 "GND")
			(pinfunction "E")
			(pintype "passive")
		)
		(pad "3" smd roundrect
			(at 1.2 0 180)
			(size 0.9 0.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 387 "Net-(Q13-C)")
			(pinfunction "C")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SC-59.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "B.Cu")
		(at 231.1 130.2 180)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP30"
			(at 0 1.448 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 -1.55 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 1.45 0)
			(layer "B.Fab")
		)
		(pad "1" smd circle
			(at 0 0 180)
			(size 1 1)
			(layers "B.Cu" "B.Mask")
			(net 132 "Net-(P2-Pin_7)")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "B.Cu")
		(at 179.95 135.3625 -90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R15"
			(at 1.9245 -2.295 270)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "10k"
			(at 0 -1.65 90)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 270)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902)
			(net 170 "Net-(C7-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 270)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902)
			(net 355 "Net-(Q5-E)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "B.Cu")
		(at 217.297 107.95 180)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP97"
			(at 0 1.448 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 -1.55 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 1.45 0)
			(layer "B.Fab")
		)
		(pad "1" smd circle
			(at 0 0 180)
			(size 1 1)
			(layers "B.Cu" "B.Mask")
			(net 92 "/VAB4")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "B.Cu")
		(at 175.961 103.251 180)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C10"
			(at -4.506 -0.762 0)
			(layer "B.SilkS")
		)
		(property "Value" "82pF"
			(at 0 -1.68 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0 180)
			(size 1 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 155 "Net-(U7-VC)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0 180)
			(size 1 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 127 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "B.Cu")
		(at 192.151 110.871 180)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP47"
			(at 0 1.448 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 -1.55 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 1.45 0)
			(layer "B.Fab")
		)
		(pad "1" smd circle
			(at 0 0 180)
			(size 1 1)
			(layers "B.Cu" "B.Mask")
			(net 110 "/VAA0")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "B.Cu")
		(at 96.1155 151.638)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R5"
			(at -0.9925 -2.032 0)
			(layer "B.SilkS")
		)
		(property "Value" "100"
			(at 0 -1.65 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr smd exclude_from_bom dnp)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902)
			(net 127 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902)
			(net 357 "Net-(Q6-E)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "B.Cu")
		(at 125.73 156.6945 90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R59"
			(at -1.5475 2.032 270)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "1k"
			(at 0 -1.65 90)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 90)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902)
			(net 351 "Net-(Q15-B)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 90)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902)
			(net 387 "Net-(Q13-C)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "B.Cu")
		(at 114.427 168.6795 -90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R70"
			(at 4.1675 0 270)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "10k"
			(at 0 -1.65 90)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 270)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902)
			(net 380 "Net-(C66-Pad2)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 270)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902)
			(net 394 "Net-(Q17-E)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "B.Cu")
		(at 87.945 127.508 180)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C52"
			(at 0.145 2.308 0)
			(layer "B.SilkS")
		)
		(property "Value" "47pF"
			(at 0 -1.68 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0 180)
			(size 1 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 290 "Net-(P4-Audio-R)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0 180)
			(size 1 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 127 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "B.Cu")
		(at 180.909 95.504 180)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C11"
			(at -4.765 -0.127 0)
			(layer "B.SilkS")
		)
		(property "Value" "82pF"
			(at 0 -1.68 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0 180)
			(size 1 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 127 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0 180)
			(size 1 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 156 "Net-(C11-Pad2)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "B.Cu")
		(at 83.693 157.033 90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C45"
			(at -4.003 -0.127 270)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "47pF"
			(at 0 -1.68 90)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0 90)
			(size 1 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 402 "Net-(DA19-K)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0 90)
			(size 1 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 127 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "B.Cu")
		(at 120.3375 168.85 180)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R51"
			(at -0.0625 -6.45 0)
			(layer "B.SilkS")
		)
		(property "Value" "33k"
			(at 0 -1.65 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 180)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902)
			(net 127 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 180)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902)
			(net 343 "Net-(DA6A-A)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "B.Cu")
		(at 80.4 87 180)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP19"
			(at 0 1.448 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 -1.55 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 1.45 0)
			(layer "B.Fab")
		)
		(pad "1" smd circle
			(at 0 0 180)
			(size 1 1)
			(layers "B.Cu" "B.Mask")
			(net 352 "Net-(P1-EXPAND)")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "B.Cu")
		(at 81.407 128.966 90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C88"
			(at -0.574 -2.707 270)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "0.1µF"
			(at 0 -1.68 90)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0 90)
			(size 1 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 72 "VCC")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0 90)
			(size 1 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 127 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "B.Cu")
		(at 112.268 143.9945 -90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R102"
			(at -12.1685 -0.889 270)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "22k"
			(at 0 -1.65 90)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 270)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902)
			(net 222 "Net-(U10D-+)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 270)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902)
			(net 221 "Net-(C75-Pad2)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "B.Cu")
		(at 121.6 139.1 180)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C79"
			(at 0.188 2.956 0)
			(layer "B.SilkS")
		)
		(property "Value" "100pF"
			(at 0 -1.68 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0 180)
			(size 1 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 127 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0 180)
			(size 1 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 330 "Net-(U10C-+)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "B.Cu")
		(at 222.377 97.409 180)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP46"
			(at 0 1.448 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 -1.55 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 1.45 0)
			(layer "B.Fab")
		)
		(pad "1" smd circle
			(at 0 0 180)
			(size 1 1)
			(layers "B.Cu" "B.Mask")
			(net 143 "/VDB7")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "B.Cu")
		(at 78.8 94.4 180)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP8"
			(at 0 1.448 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 -1.55 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 1.45 0)
			(layer "B.Fab")
		)
		(pad "1" smd circle
			(at 0 0 180)
			(size 1 1)
			(layers "B.Cu" "B.Mask")
			(net 38 "/D5")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "B.Cu")
		(at 193.294 113.284 180)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP55"
			(at 0 1.448 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 -1.55 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 1.45 0)
			(layer "B.Fab")
		)
		(pad "1" smd circle
			(at 0 0 180)
			(size 1 1)
			(layers "B.Cu" "B.Mask")
			(net 144 "/VDA0")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "B.Cu")
		(at 100.7 109.1 180)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP13"
			(at 0 1.448 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 -1.55 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 1.45 0)
			(layer "B.Fab")
		)
		(pad "1" smd circle
			(at 0 0 180)
			(size 1 1)
			(layers "B.Cu" "B.Mask")
			(net 308 "/PA2")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "B.Cu")
		(at 180.467 187.8095 -90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R73"
			(at -4.2945 -0.508 270)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "0"
			(at 0 -1.65 90)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 270)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902)
			(net 26 "XIN")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 270)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902)
			(net 45 "Net-(U18-XOUT)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "B.Cu")
		(at 190.881 113.03 180)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP48"
			(at 0 1.448 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 -1.55 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 1.45 0)
			(layer "B.Fab")
		)
		(pad "1" smd circle
			(at 0 0 180)
			(size 1 1)
			(layers "B.Cu" "B.Mask")
			(net 109 "/VAA1")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "B.Cu")
		(at 115.9 87.05 -90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C98"
			(at -4.119 0.33 270)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "0.1µF"
			(at 0 -1.68 90)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0 270)
			(size 1 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 72 "VCC")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0 270)
			(size 1 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 127 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "B.Cu")
		(at 228.6285 132.715 180)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R87"
			(at 3.81 0 0)
			(layer "B.SilkS")
		)
		(property "Value" "100"
			(at 0 -0.04 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 180)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902)
			(net 131 "Net-(P2-Pin_6)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 180)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902)
			(net 284 "/4016.D0")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "B.Cu")
		(at 173.1 77.7625 -90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R44"
			(at -3.5945 -0.763 270)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "10k"
			(at 0 -1.65 90)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 270)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902)
			(net 127 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 270)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902)
			(net 187 "Net-(Q12-B)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_SMD:SC-59"
		(layer "B.Cu")
		(at 101.403 145.415 180)
		(descr "SC-59, https://lib.chipdip.ru/images/import_diod/original/SOT-23_SC-59.jpg")
		(tags "SC-59")
		(property "Reference" "D1"
			(at -0.451 -3.175 0)
			(layer "B.SilkS")
		)
		(property "Value" "D_Zener_Dual_CommonCathode_AAK_Split"
			(at 0 -2.5 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Dual Zener diode, common anode on pin 1"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.2 0.95 180)
			(size 0.9 0.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 127 "GND")
			(pinfunction "A")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at -1.2 -0.95 180)
			(size 0.9 0.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 305 "unconnected-(D1B-K-Pad2)")
			(pinfunction "K")
			(pintype "passive+no_connect")
		)
		(pad "3" smd roundrect
			(at 1.2 0 180)
			(size 0.9 0.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 304 "+12V")
			(pinfunction "K")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SC-59.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_SMD:SC-59"
		(layer "B.Cu")
		(at 128.95 155 180)
		(descr "SC-59, https://lib.chipdip.ru/images/import_diod/original/SOT-23_SC-59.jpg")
		(tags "SC-59")
		(property "Reference" "Q14"
			(at -9.425 1.95 0)
			(layer "B.SilkS")
		)
		(property "Value" "C2412K"
			(at 0 -2.5 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "NPN transistor, base/emitter/collector"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.2 0.95 180)
			(size 0.9 0.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 350 "Net-(Q14-B)")
			(pinfunction "B")
			(pintype "input")
		)
		(pad "2" smd roundrect
			(at -1.2 -0.95 180)
			(size 0.9 0.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 368 "Net-(Q14-E)")
			(pinfunction "E")
			(pintype "passive")
		)
		(pad "3" smd roundrect
			(at 1.2 0 180)
			(size 0.9 0.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 369 "Net-(Q14-C)")
			(pinfunction "C")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SC-59.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_SMD:SC-59"
		(layer "B.Cu")
		(at 92.018 140.782 180)
		(descr "SC-59, https://lib.chipdip.ru/images/import_diod/original/SOT-23_SC-59.jpg")
		(tags "SC-59")
		(property "Reference" "DA17"
			(at -3.359 -0.442 0)
			(layer "B.SilkS")
		)
		(property "Value" "DAN202"
			(at 0 -2.5 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Dual diode, common cathode on pin 3"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.2 0.95 180)
			(size 0.9 0.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 127 "GND")
			(pinfunction "A")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at -1.2 -0.95 180)
			(size 0.9 0.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 398 "Net-(DA17-A-Pad2)")
			(pinfunction "A")
			(pintype "passive")
		)
		(pad "3" smd roundrect
			(at 1.2 0 180)
			(size 0.9 0.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 397 "Net-(DA17-K)")
			(pinfunction "K")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SC-59.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "B.Cu")
		(at 175.514 187.772 -90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C69"
			(at -4.257 -0.127 270)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "47pF"
			(at 0 -1.68 90)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr smd exclude_from_bom dnp)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0 270)
			(size 1 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 127 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0 270)
			(size 1 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 32 "Net-(U18-4.433M)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "B.Cu")
		(at 102.108 77.404 90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C102"
			(at 4.633 -0.127 270)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "0.1µF"
			(at 0 -1.68 90)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0 90)
			(size 1 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 72 "VCC")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0 90)
			(size 1 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 127 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_SMD:SC-59"
		(layer "B.Cu")
		(at 231.21 158.816 180)
		(descr "SC-59, https://lib.chipdip.ru/images/import_diod/original/SOT-23_SC-59.jpg")
		(tags "SC-59")
		(property "Reference" "DA2"
			(at -10.979 5.649 0)
			(layer "B.SilkS")
		)
		(property "Value" "DAP202"
			(at 0 -2.5 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Dual diode, common anode on pin 1"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.2 0.95 180)
			(size 0.9 0.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 274 "/JPCLK2")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at -1.2 -0.95 180)
			(size 0.9 0.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 277 "/JPCLK1")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "3" smd roundrect
			(at 1.2 0 180)
			(size 0.9 0.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 127 "GND")
			(pinfunction "A")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SC-59.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "B.Cu")
		(at 101 88.9 180)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP26"
			(at 0 1.448 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 -1.55 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 1.45 0)
			(layer "B.Fab")
		)
		(pad "1" smd circle
			(at 0 0 180)
			(size 1 1)
			(layers "B.Cu" "B.Mask")
			(net 338 "Net-(P5-SMPCK)")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "B.Cu")
		(at 224.3055 171.323)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R78"
			(at -9.6755 2.159 0)
			(layer "B.SilkS")
		)
		(property "Value" "10k"
			(at 0 -1.65 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902)
			(net 72 "VCC")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902)
			(net 287 "EXTLATCH")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "B.Cu")
		(at 130 111.2)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C99"
			(at 0.6 -2.15 0)
			(layer "B.SilkS")
		)
		(property "Value" "0.1µF"
			(at 0 -1.68 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0)
			(size 1 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 127 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0)
			(size 1 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 72 "VCC")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_SMD:SC-59"
		(layer "B.Cu")
		(at 103.2025 150.307 180)
		(descr "SC-59, https://lib.chipdip.ru/images/import_diod/original/SOT-23_SC-59.jpg")
		(tags "SC-59")
		(property "Reference" "DA11"
			(at 3.5075 -3.871 0)
			(layer "B.SilkS")
		)
		(property "Value" "DAN217"
			(at 0 -2.5 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Dual diode, cathode/anode/center"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.2 0.95 180)
			(size 0.9 0.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 303 "Net-(DA11-K)")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at -1.2 -0.95 180)
			(size 0.9 0.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 301 "Net-(DA11-A)")
			(pinfunction "A")
			(pintype "passive")
		)
		(pad "3" smd roundrect
			(at 1.2 0 180)
			(size 0.9 0.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 302 "Net-(DA11-common)")
			(pinfunction "common")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SC-59.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_SMD:SC-59"
		(layer "B.Cu")
		(at 227.146 154.498 180)
		(descr "SC-59, https://lib.chipdip.ru/images/import_diod/original/SOT-23_SC-59.jpg")
		(tags "SC-59")
		(property "Reference" "DA6"
			(at -2.089 2.987 0)
			(layer "B.SilkS")
		)
		(property "Value" "DAN202"
			(at 0 -2.5 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Dual diode, common anode on pin 1"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.2 0.95 180)
			(size 0.9 0.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 343 "Net-(DA6A-A)")
			(pinfunction "A")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at -1.2 -0.95 180)
			(size 0.9 0.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 223 "/JPSTR")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "3" smd roundrect
			(at 1.2 0 180)
			(size 0.9 0.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 72 "VCC")
			(pinfunction "K")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SC-59.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "B.Cu")
		(at 233.619 135.255)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C38"
			(at 4.13 0 0)
			(layer "B.SilkS")
		)
		(property "Value" "330pF"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0)
			(size 1 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 130 "Net-(P2-Pin_5)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0)
			(size 1 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 127 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "B.Cu")
		(at 105.537 161.0125 90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R94"
			(at -4.2145 -2.286 270)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "200"
			(at 0 -1.65 90)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 90)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902)
			(net 127 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 90)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902)
			(net 340 "Net-(P5-SL-IN)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "B.Cu")
		(at 219.837 108.077 180)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP95"
			(at 0 1.448 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 -1.55 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 1.45 180)
			(layer "B.Fab")
		)
		(pad "1" smd circle
			(at 0 0 180)
			(size 1 1)
			(layers "B.Cu" "B.Mask")
			(net 94 "/VAB2")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "B.Cu")
		(at 120.7375 166.45 180)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R50"
			(at 0.2875 -7.3 0)
			(layer "B.SilkS")
		)
		(property "Value" "33k"
			(at 0 -1.65 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 180)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902)
			(net 343 "Net-(DA6A-A)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 180)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902)
			(net 298 "+9V")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_SMD:SC-59"
		(layer "B.Cu")
		(at 232.226 167.452 180)
		(descr "SC-59, https://lib.chipdip.ru/images/import_diod/original/SOT-23_SC-59.jpg")
		(tags "SC-59")
		(property "Reference" "DA4"
			(at -10.979 -11.745 0)
			(layer "B.SilkS")
		)
		(property "Value" "DAP202"
			(at 0 -2.5 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Dual diode, common anode on pin 1"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.2 0.95 180)
			(size 0.9 0.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 285 "/4017.D1")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at -1.2 -0.95 180)
			(size 0.9 0.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 286 "/4017.D0")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "3" smd roundrect
			(at 1.2 0 180)
			(size 0.9 0.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 127 "GND")
			(pinfunction "A")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SC-59.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "B.Cu")
		(at 187.198 191.6665 -90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R2"
			(at -3.4525 -0.381 270)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "5.1k"
			(at 0 -1.65 90)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 270)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902)
			(net 294 "Net-(R2-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 270)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902)
			(net 127 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "B.Cu")
		(at 188.6 77.8125 -90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R39"
			(at -3.6125 -0.25 270)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "10k"
			(at 0 -1.65 90)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 270)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902)
			(net 127 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 270)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902)
			(net 178 "Net-(Q11-B)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_SMD:SC-59"
		(layer "B.Cu")
		(at 232.099 171.77 180)
		(descr "SC-59, https://lib.chipdip.ru/images/import_diod/original/SOT-23_SC-59.jpg")
		(tags "SC-59")
		(property "Reference" "DA5"
			(at -0.438 -3.368 0)
			(layer "B.SilkS")
		)
		(property "Value" "DAP202"
			(at 0 -2.5 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Dual diode, common anode on pin 1"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.2 0.95 180)
			(size 0.9 0.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 287 "EXTLATCH")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at -1.2 -0.95 180)
			(size 0.9 0.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 288 "/JPIO6")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "3" smd roundrect
			(at 1.2 0 180)
			(size 0.9 0.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 127 "GND")
			(pinfunction "A")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SC-59.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "B.Cu")
		(at 223.1375 175.8 180)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R77"
			(at 0.2875 -2.55 0)
			(layer "B.SilkS")
		)
		(property "Value" "10k"
			(at 0 -1.65 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 180)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902)
			(net 72 "VCC")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 180)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902)
			(net 288 "/JPIO6")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "B.Cu")
		(at 119.38 191.455 90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C34"
			(at 4.13 0.381 270)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "0.1µF"
			(at 0 -1.68 90)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0 90)
			(size 1 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 303 "Net-(DA11-K)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0 90)
			(size 1 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 127 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "B.Cu")
		(at 171.257 95.504 180)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C84"
			(at 3.998 -0.254 0)
			(layer "B.SilkS")
		)
		(property "Value" "0.1µF"
			(at 0 -1.68 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0 180)
			(size 1 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 127 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0 180)
			(size 1 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 72 "VCC")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "B.Cu")
		(at 115.062 156.7415 -90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R64"
			(at -3.3255 -0.635 270)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "1.8k"
			(at 0 -1.65 90)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 270)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902)
			(net 371 "Net-(Q15-C)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 270)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902)
			(net 127 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_SMD:SC-59"
		(layer "B.Cu")
		(at 95.955 144.211 180)
		(descr "SC-59, https://lib.chipdip.ru/images/import_diod/original/SOT-23_SC-59.jpg")
		(tags "SC-59")
		(property "Reference" "DA12"
			(at -2.724 -1.204 270)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "DAN202"
			(at 0 -2.5 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Dual diode, common cathode on pin 3"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.2 0.95 180)
			(size 0.9 0.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 127 "GND")
			(pinfunction "A")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at -1.2 -0.95 180)
			(size 0.9 0.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 169 "Net-(DA12-A-Pad2)")
			(pinfunction "A")
			(pintype "passive")
		)
		(pad "3" smd roundrect
			(at 1.2 0 180)
			(size 0.9 0.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 167 "Net-(DA12-K)")
			(pinfunction "K")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SC-59.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "B.Cu")
		(at 80.4 82 180)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP23"
			(at 0 1.448 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 -1.55 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 1.45 0)
			(layer "B.Fab")
		)
		(pad "1" smd circle
			(at 0 0 180)
			(size 1 1)
			(layers "B.Cu" "B.Mask")
			(net 341 "Net-(P5-SR-IN)")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "B.Cu")
		(at 218.9 170.6 180)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP2"
			(at 0 1.448 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 -1.55 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 1.45 0)
			(layer "B.Fab")
		)
		(pad "1" smd circle
			(at 0 0 180)
			(size 1 1)
			(layers "B.Cu" "B.Mask")
			(net 300 "Net-(U1-JOY-OUT2)")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "B.Cu")
		(at 161.163 189.23 180)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP80"
			(at 0 1.448 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 -1.55 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 1.45 0)
			(layer "B.Fab")
		)
		(pad "1" smd circle
			(at 0 0 180)
			(size 1 1)
			(layers "B.Cu" "B.Mask")
			(net 10 "/CA15")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "B.Cu")
		(at 134.239 91.948 180)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP65"
			(at 0 1.448 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 -1.55 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 1.45 0)
			(layer "B.Fab")
		)
		(pad "1" smd circle
			(at 0 0 180)
			(size 1 1)
			(layers "B.Cu" "B.Mask")
			(net 242 "Net-(U13-P55)")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "B.Cu")
		(at 173.3375 130.9)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R10"
			(at -0.0625 -15.5 0)
			(layer "B.SilkS")
		)
		(property "Value" "10k"
			(at 0 -1.65 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902)
			(net 171 "Net-(C6-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902)
			(net 347 "Net-(Q3-E)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "B.Cu")
		(at 180.782 160.528 180)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C91"
			(at -2.352 2.159 0)
			(layer "B.SilkS")
		)
		(property "Value" "0.1µF"
			(at 0 -1.68 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0 180)
			(size 1 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 127 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0 180)
			(size 1 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 72 "VCC")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "B.Cu")
		(at 169.05 145.4 180)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C8"
			(at 4.204 -0.269 0)
			(layer "B.SilkS")
		)
		(property "Value" "0.1µF"
			(at 0 -1.68 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0 180)
			(size 1 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 366 "Net-(C8-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0 180)
			(size 1 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 367 "Net-(U7-AB)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_SMD:SC-59"
		(layer "B.Cu")
		(at 87.687 136.652 180)
		(descr "SC-59, https://lib.chipdip.ru/images/import_diod/original/SOT-23_SC-59.jpg")
		(tags "SC-59")
		(property "Reference" "DA18"
			(at 3.387 1.552 0)
			(layer "B.SilkS")
		)
		(property "Value" "DAN202"
			(at 0 -2.5 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Dual diode, common cathode on pin 3"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.2 0.95 180)
			(size 0.9 0.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 168 "Net-(DA15-K)")
			(pinfunction "A")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at -1.2 -0.95 180)
			(size 0.9 0.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 399 "Net-(DA16-K)")
			(pinfunction "A")
			(pintype "passive")
		)
		(pad "3" smd roundrect
			(at 1.2 0 180)
			(size 0.9 0.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 72 "VCC")
			(pinfunction "K")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SC-59.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_SMD:SC-59"
		(layer "B.Cu")
		(at 178.05 142.35 180)
		(descr "SC-59, https://lib.chipdip.ru/images/import_diod/original/SOT-23_SC-59.jpg")
		(tags "SC-59")
		(property "Reference" "Q5"
			(at -0.512 2.777 0)
			(layer "B.SilkS")
		)
		(property "Value" "C2412K"
			(at 0 -2.5 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "NPN transistor, base/emitter/collector"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.2 0.95 180)
			(size 0.9 0.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 356 "Net-(Q5-B)")
			(pinfunction "B")
			(pintype "input")
		)
		(pad "2" smd roundrect
			(at -1.2 -0.95 180)
			(size 0.9 0.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 355 "Net-(Q5-E)")
			(pinfunction "E")
			(pintype "passive")
		)
		(pad "3" smd roundrect
			(at 1.2 0 180)
			(size 0.9 0.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 127 "GND")
			(pinfunction "C")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SC-59.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "B.Cu")
		(at 178.35 82 -90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C86"
			(at -14.055 -12.023 270)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "10pF"
			(at 0 -1.68 90)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0 270)
			(size 1 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 345 "Net-(Q9-B)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0 270)
			(size 1 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 127 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "B.Cu")
		(at 231.1 132.8 180)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP34"
			(at 0 1.448 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 -1.55 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 1.45 0)
			(layer "B.Fab")
		)
		(pad "1" smd circle
			(at 0 0 180)
			(size 1 1)
			(layers "B.Cu" "B.Mask")
			(net 131 "Net-(P2-Pin_6)")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "B.Cu")
		(at 136.906 86.995 180)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP70"
			(at 0 1.448 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 -1.55 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 1.45 0)
			(layer "B.Fab")
		)
		(pad "1" smd circle
			(at 0 0 180)
			(size 1 1)
			(layers "B.Cu" "B.Mask")
			(net 247 "Net-(U13-P50)")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "B.Cu")
		(at 181.356 175.895 180)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP86"
			(at 0 1.448 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 -1.55 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 1.45 0)
			(layer "B.Fab")
		)
		(pad "1" smd circle
			(at 0 0 180)
			(size 1 1)
			(layers "B.Cu" "B.Mask")
			(net 68 "/CA6")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "B.Cu")
		(at 101 101.5 180)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP25"
			(at 0 1.448 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 -1.55 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 1.45 0)
			(layer "B.Fab")
		)
		(pad "1" smd circle
			(at 0 0 180)
			(size 1 1)
			(layers "B.Cu" "B.Mask")
			(net 50 "/{slash}PAWR")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "B.Cu")
		(at 223.647 99.441 180)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP45"
			(at 0 1.448 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 -1.55 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 1.45 0)
			(layer "B.Fab")
		)
		(pad "1" smd circle
			(at 0 0 180)
			(size 1 1)
			(layers "B.Cu" "B.Mask")
			(net 142 "/VDB6")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "B.Cu")
		(at 166.9875 85.8)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R37"
			(at -3.9125 0.15 0)
			(layer "B.SilkS")
		)
		(property "Value" "270"
			(at 0 -1.65 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902)
			(net 365 "Net-(U7-(R-Y)O)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902)
			(net 177 "Net-(C15-Pad1)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "B.Cu")
		(at 118.05 148 90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C78"
			(at -0.59 3.997 270)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "1800pF"
			(at 0 -1.68 90)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0 90)
			(size 1 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 219 "Net-(U10C--)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0 90)
			(size 1 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 335 "Net-(C78-Pad2)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "B.Cu")
		(at 185.42 168.402)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP89"
			(at 0 1.448 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 -1.55 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 1.45 180)
			(layer "B.Fab")
		)
		(pad "1" smd circle
			(at 0 0)
			(size 1 1)
			(layers "B.Cu" "B.Mask")
			(net 61 "/{slash}CPUWR")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "B.Cu")
		(at 87.823 147.066 180)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C46"
			(at 3.622 -0.254 0)
			(layer "B.SilkS")
		)
		(property "Value" "330pF"
			(at 0 -1.68 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0 180)
			(size 1 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 304 "+12V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0 180)
			(size 1 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 127 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "B.Cu")
		(at 213.36 110.109 180)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP100"
			(at 0 1.448 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 -1.55 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 1.45 180)
			(layer "B.Fab")
		)
		(pad "1" smd circle
			(at 0 0 180)
			(size 1 1)
			(layers "B.Cu" "B.Mask")
			(net 88 "/VAB7")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "B.Cu")
		(at 169.0875 142.85 180)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R21"
			(at 4.1375 1 0)
			(layer "B.SilkS")
		)
		(property "Value" "120"
			(at 0 -1.65 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 180)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902)
			(net 366 "Net-(C8-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 180)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902)
			(net 72 "VCC")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "B.Cu")
		(at 133.924 137.922)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C101"
			(at 4.506 0.254 0)
			(layer "B.SilkS")
		)
		(property "Value" "0.1µF"
			(at 0 -1.68 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0)
			(size 1 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 127 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0)
			(size 1 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 72 "VCC")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "B.Cu")
		(at 124.46 191.455 90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C81"
			(at 4.13 -0.254 270)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "1uF"
			(at 0 -1.68 90)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0 90)
			(size 1 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 72 "VCC")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0 90)
			(size 1 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 127 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "B.Cu")
		(at 228.6285 125.095 180)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R90"
			(at 5.3575 0 0)
			(layer "B.SilkS")
		)
		(property "Value" "10"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 180)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902)
			(net 134 "Net-(P2-Pin_9)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 180)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902)
			(net 274 "/JPCLK2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "B.Cu")
		(at 80.4 100.4 180)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP24"
			(at 0 1.448 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 -1.55 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 1.45 0)
			(layer "B.Fab")
		)
		(pad "1" smd circle
			(at 0 0 180)
			(size 1 1)
			(layers "B.Cu" "B.Mask")
			(net 41 "/{slash}PARD")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "B.Cu")
		(at 117.983 143.9945 -90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R105"
			(at -8.7395 -0.635 270)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "22k"
			(at 0 -1.65 90)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 270)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902)
			(net 330 "Net-(U10C-+)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 270)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902)
			(net 335 "Net-(C78-Pad2)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "B.Cu")
		(at 195.834 173.863 180)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP88"
			(at 0 1.448 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 -1.55 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 1.45 0)
			(layer "B.Fab")
		)
		(pad "1" smd circle
			(at 0 0 180)
			(size 1 1)
			(layers "B.Cu" "B.Mask")
			(net 67 "/CA5")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "B.Cu")
		(at 80.3 108.4 180)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP12"
			(at 0 1.448 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 -1.55 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 1.45 0)
			(layer "B.Fab")
		)
		(pad "1" smd circle
			(at 0 0 180)
			(size 1 1)
			(layers "B.Cu" "B.Mask")
			(net 310 "/PA1")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "B.Cu")
		(at 224.3875 168.3)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R79"
			(at -9.8125 3.45 0)
			(layer "B.SilkS")
		)
		(property "Value" "10k"
			(at 0 -1.65 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902)
			(net 72 "VCC")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902)
			(net 286 "/4017.D0")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "B.Cu")
		(at 133.1995 141.478 180)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R68"
			(at -3.9605 0.508 0)
			(layer "B.SilkS")
		)
		(property "Value" "47k"
			(at 0 -1.65 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 180)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902)
			(net 78 "Net-(J2-Audio)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 180)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902)
			(net 372 "Net-(Q16-E)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "B.Cu")
		(at 163.703 189.484 180)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP81"
			(at 0 1.448 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 -1.55 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 1.45 0)
			(layer "B.Fab")
		)
		(pad "1" smd circle
			(at 0 0 180)
			(size 1 1)
			(layers "B.Cu" "B.Mask")
			(net 9 "/CA14")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "B.Cu")
		(at 218.567 110.236 180)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP96"
			(at 0 1.448 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 -1.55 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 1.45 180)
			(layer "B.Fab")
		)
		(pad "1" smd circle
			(at 0 0 180)
			(size 1 1)
			(layers "B.Cu" "B.Mask")
			(net 93 "/VAB3")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "B.Cu")
		(at 233.619 125.095)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C42"
			(at 4.13 0 0)
			(layer "B.SilkS")
		)
		(property "Value" "330pF"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0)
			(size 1 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 134 "Net-(P2-Pin_9)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0)
			(size 1 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 127 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "B.Cu")
		(at 100.7 106.6 180)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP15"
			(at 0 1.448 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 -1.55 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 1.45 0)
			(layer "B.Fab")
		)
		(pad "1" smd circle
			(at 0 0 180)
			(size 1 1)
			(layers "B.Cu" "B.Mask")
			(net 309 "/PA4")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "B.Cu")
		(at 175.7 81.9625 90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R23"
			(at 14.0175 12.514 270)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "10k"
			(at 0 -1.65 90)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 90)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902)
			(net 127 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 90)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902)
			(net 345 "Net-(Q9-B)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "B.Cu")
		(at 169.0875 140.5)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R14"
			(at -4.1625 -0.45 0)
			(layer "B.SilkS")
		)
		(property "Value" "1.5k"
			(at 0 -1.65 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902)
			(net 72 "VCC")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902)
			(net 358 "Net-(Q6-B)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "B.Cu")
		(at 195.961 113.919 180)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP57"
			(at 0 1.448 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 -1.55 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 1.45 0)
			(layer "B.Fab")
		)
		(pad "1" smd circle
			(at 0 0 180)
			(size 1 1)
			(layers "B.Cu" "B.Mask")
			(net 146 "/VDA2")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "B.Cu")
		(at 224.3375 163.25)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R81"
			(at -3.8625 -0.25 0)
			(layer "B.SilkS")
		)
		(property "Value" "10k"
			(at 0 -1.65 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902)
			(net 72 "VCC")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902)
			(net 284 "/4016.D0")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_SMD:SC-59"
		(layer "B.Cu")
		(at 114.75 161.65 180)
		(descr "SC-59, https://lib.chipdip.ru/images/import_diod/original/SOT-23_SC-59.jpg")
		(tags "SC-59")
		(property "Reference" "Q17"
			(at 1.974 1.376 0)
			(layer "B.SilkS")
		)
		(property "Value" "C2412K"
			(at 0 -2.5 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "NPN transistor, base/emitter/collector"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.2 0.95 180)
			(size 0.9 0.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 371 "Net-(Q15-C)")
			(pinfunction "B")
			(pintype "input")
		)
		(pad "2" smd roundrect
			(at -1.2 -0.95 180)
			(size 0.9 0.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 394 "Net-(Q17-E)")
			(pinfunction "E")
			(pintype "passive")
		)
		(pad "3" smd roundrect
			(at 1.2 0 180)
			(size 0.9 0.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 298 "+9V")
			(pinfunction "C")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SC-59.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "B.Cu")
		(at 99.7985 142.113)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R4"
			(at 3.3255 -8.382 0)
			(layer "B.SilkS")
		)
		(property "Value" "100"
			(at 0 -1.65 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr smd exclude_from_bom dnp)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902)
			(net 353 "Net-(Q4-E)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902)
			(net 127 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "B.Cu")
		(at 227.584 97.409 180)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP42"
			(at 0 1.448 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 -1.55 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 1.45 0)
			(layer "B.Fab")
		)
		(pad "1" smd circle
			(at 0 0 180)
			(size 1 1)
			(layers "B.Cu" "B.Mask")
			(net 139 "/VDB3")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "B.Cu")
		(at 103.85 112.3625 -90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R25"
			(at 0.4135 -2.195 270)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "22"
			(at 0 -1.65 90)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 270)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902)
			(net 359 "Net-(Q9-E)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 270)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902)
			(net 400 "Net-(DA16-A-Pad2)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "B.Cu")
		(at 101 91.4 180)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP9"
			(at 0 1.448 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 -1.55 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 1.45 0)
			(layer "B.Fab")
		)
		(pad "1" smd circle
			(at 0 0 180)
			(size 1 1)
			(layers "B.Cu" "B.Mask")
			(net 39 "/D6")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "B.Cu")
		(at 123.65 109.85 -90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C90"
			(at 0.513 2.492 270)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "0.1µF"
			(at 0 -1.68 90)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0 270)
			(size 1 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 72 "VCC")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0 270)
			(size 1 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 127 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "B.Cu")
		(at 103.8625 84.709)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R32"
			(at 3.8335 0.127 0)
			(layer "B.SilkS")
		)
		(property "Value" "100"
			(at 0 -1.65 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr smd exclude_from_bom dnp)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902)
			(net 127 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902)
			(net 189 "Net-(Q10-E)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "B.Cu")
		(at 228.6285 135.255 180)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R86"
			(at 3.81 0 0)
			(layer "B.SilkS")
		)
		(property "Value" "100"
			(at 0 -0.45 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 180)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902)
			(net 130 "Net-(P2-Pin_5)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 180)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902)
			(net 285 "/4017.D1")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "B.Cu")
		(at 111.379 166.7745 -90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R96"
			(at 4.8025 0.381 270)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "200"
			(at 0 -1.65 90)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 270)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902)
			(net 127 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 270)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902)
			(net 315 "Net-(P1-SOUND-L)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "B.Cu")
		(at 231.2 140.3 180)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP28"
			(at 0 1.448 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 -1.55 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 1.45 0)
			(layer "B.Fab")
		)
		(pad "1" smd circle
			(at 0 0 180)
			(size 1 1)
			(layers "B.Cu" "B.Mask")
			(net 128 "Net-(P2-Pin_3)")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "Package_TO_SOT_SMD:SC-59"
		(layer "B.Cu")
		(at 232.226 163.134 180)
		(descr "SC-59, https://lib.chipdip.ru/images/import_diod/original/SOT-23_SC-59.jpg")
		(tags "SC-59")
		(property "Reference" "DA3"
			(at -10.979 6.157 0)
			(layer "B.SilkS")
		)
		(property "Value" "DAP202"
			(at 0 -2.5 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Dual diode, common anode on pin 1"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.2 0.95 180)
			(size 0.9 0.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 281 "/4016.D1")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at -1.2 -0.95 180)
			(size 0.9 0.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 284 "/4016.D0")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "3" smd roundrect
			(at 1.2 0 180)
			(size 0.9 0.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 127 "GND")
			(pinfunction "A")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SC-59.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "B.Cu")
		(at 100.8 84.6 180)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP20"
			(at 0 1.448 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 -1.55 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 1.45 0)
			(layer "B.Fab")
		)
		(pad "1" smd circle
			(at 0 0 180)
			(size 1 1)
			(layers "B.Cu" "B.Mask")
			(net 339 "Net-(P5-MONO-OUT)")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "B.Cu")
		(at 130.617 159.004)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C23"
			(at 0.701 -1.778 0)
			(layer "B.SilkS")
		)
		(property "Value" "1uF"
			(at 0 -1.68 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0)
			(size 1 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 333 "Net-(C23-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0)
			(size 1 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 203 "Net-(U10D--)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "B.Cu")
		(at 136.906 89.535 180)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP68"
			(at 0 1.448 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 -1.55 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 1.45 0)
			(layer "B.Fab")
		)
		(pad "1" smd circle
			(at 0 0 180)
			(size 1 1)
			(layers "B.Cu" "B.Mask")
			(net 245 "Net-(U13-P52)")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "B.Cu")
		(at 202 84.3375 -90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R30"
			(at 0.5625 -2.724 270)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "470"
			(at 0 -1.65 90)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 270)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902)
			(net 182 "Net-(J2-Video)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 270)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902)
			(net 180 "Net-(Q10-B)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "B.Cu")
		(at 180.8 81.8875 90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R22"
			(at 13.9425 11.605 270)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "470"
			(at 0 -1.65 90)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 90)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902)
			(net 363 "Net-(U7-YO)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 90)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902)
			(net 345 "Net-(Q9-B)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "B.Cu")
		(at 175.7 77.75 90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C19"
			(at 3.582 0.195 270)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "10pF"
			(at 0 -1.68 90)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0 90)
			(size 1 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 187 "Net-(Q12-B)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0 90)
			(size 1 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 127 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "B.Cu")
		(at 106.299 178.115 90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C96"
			(at -2.225 -2.413 270)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "0.1µF"
			(at 0 -1.68 90)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0 90)
			(size 1 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 127 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0 90)
			(size 1 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 72 "VCC")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "B.Cu")
		(at 233.619 132.715)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C39"
			(at 4.13 0 0)
			(layer "B.SilkS")
		)
		(property "Value" "330pF"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0)
			(size 1 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 131 "Net-(P2-Pin_6)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0)
			(size 1 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 127 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "B.Cu")
		(at 233.619 127.635)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C41"
			(at 4.13 0 0)
			(layer "B.SilkS")
		)
		(property "Value" "330pF"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0)
			(size 1 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 133 "Net-(P2-Pin_8)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0)
			(size 1 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 127 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_SMD:SC-59"
		(layer "B.Cu")
		(at 127.65 149.95 180)
		(descr "SC-59, https://lib.chipdip.ru/images/import_diod/original/SOT-23_SC-59.jpg")
		(tags "SC-59")
		(property "Reference" "Q16"
			(at -2.75 -0.4 270)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "C2412K"
			(at 0 -2.5 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "NPN transistor, base/emitter/collector"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.2 0.95 180)
			(size 0.9 0.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 369 "Net-(Q14-C)")
			(pinfunction "B")
			(pintype "input")
		)
		(pad "2" smd roundrect
			(at -1.2 -0.95 180)
			(size 0.9 0.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 372 "Net-(Q16-E)")
			(pinfunction "E")
			(pintype "passive")
		)
		(pad "3" smd roundrect
			(at 1.2 0 180)
			(size 0.9 0.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 298 "+9V")
			(pinfunction "C")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SC-59.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_SMD:SC-59"
		(layer "B.Cu")
		(at 129.3645 177.353 180)
		(descr "SC-59, https://lib.chipdip.ru/images/import_diod/original/SOT-23_SC-59.jpg")
		(tags "SC-59")
		(property "Reference" "Q18"
			(at 0 2.5 0)
			(layer "B.SilkS")
		)
		(property "Value" "2SC5658"
			(at 0 -2.5 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "NPN transistor, base/emitter/collector"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.2 0.95 180)
			(size 0.9 0.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 396 "Net-(Q18-B)")
			(pinfunction "B")
			(pintype "input")
		)
		(pad "2" smd roundrect
			(at -1.2 -0.95 180)
			(size 0.9 0.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 298 "+9V")
			(pinfunction "E")
			(pintype "passive")
		)
		(pad "3" smd roundrect
			(at 1.2 0 180)
			(size 0.9 0.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 303 "Net-(DA11-K)")
			(pinfunction "C")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SC-59.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "B.Cu")
		(at 109.027 154.432 180)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C26"
			(at 1.712 -15.367 0)
			(layer "B.SilkS")
		)
		(property "Value" "1uF"
			(at 0 -1.68 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0 180)
			(size 1 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 334 "Net-(C26-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0 180)
			(size 1 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 219 "Net-(U10C--)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "B.Cu")
		(at 193.421 101.981 180)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP61"
			(at 0 1.448 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 -1.55 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 1.45 0)
			(layer "B.Fab")
		)
		(pad "1" smd circle
			(at 0 0 180)
			(size 1 1)
			(layers "B.Cu" "B.Mask")
			(net 150 "/VDA6")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "B.Cu")
		(at 161.798 186.944 180)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP78"
			(at 0 1.448 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 -1.55 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 1.45 0)
			(layer "B.Fab")
		)
		(pad "1" smd circle
			(at 0 0 180)
			(size 1 1)
			(layers "B.Cu" "B.Mask")
			(net 12 "/CA17")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "B.Cu")
		(at 104.6715 157.607 180)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R62"
			(at 8.2785 -6.858 0)
			(layer "B.SilkS")
		)
		(property "Value" "10k"
			(at 0 -1.65 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 180)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902)
			(net 370 "Net-(Q15-E)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 180)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902)
			(net 348 "Net-(C28-Pad1)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "B.Cu")
		(at 184.531 111.506 180)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP53"
			(at 0 1.448 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 -1.55 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 1.45 0)
			(layer "B.Fab")
		)
		(pad "1" smd circle
			(at 0 0 180)
			(size 1 1)
			(layers "B.Cu" "B.Mask")
			(net 104 "/VAA6")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "B.Cu")
		(at 167.0375 89.5 180)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R36"
			(at 3.9695 0.092 0)
			(layer "B.SilkS")
		)
		(property "Value" "1k"
			(at 0 -1.65 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 180)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902)
			(net 127 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 180)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902)
			(net 365 "Net-(U7-(R-Y)O)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "B.Cu")
		(at 133.731 160.4245 90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R47"
			(at -0.2305 3.556 270)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "1k"
			(at 0 -1.65 90)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr smd exclude_from_bom dnp)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 90)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902)
			(net 382 "Net-(U14-~{MUTE})")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 90)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902)
			(net 298 "+9V")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "B.Cu")
		(at 133.7075 167.513 180)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R95"
			(at -4.7225 -0.762 0)
			(layer "B.SilkS")
		)
		(property "Value" "200"
			(at 0 -1.65 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 180)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902)
			(net 127 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 180)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902)
			(net 188 "Net-(P1-SOUND-R)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_SMD:SC-59"
		(layer "B.Cu")
		(at 178.1 129 180)
		(descr "SC-59, https://lib.chipdip.ru/images/import_diod/original/SOT-23_SC-59.jpg")
		(tags "SC-59")
		(property "Reference" "Q3"
			(at -1.097 3.778 0)
			(layer "B.SilkS")
		)
		(property "Value" "C2412K"
			(at 0 -2.5 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "NPN transistor, base/emitter/collector"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.2 0.95 180)
			(size 0.9 0.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 349 "Net-(Q3-B)")
			(pinfunction "B")
			(pintype "input")
		)
		(pad "2" smd roundrect
			(at -1.2 -0.95 180)
			(size 0.9 0.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 347 "Net-(Q3-E)")
			(pinfunction "E")
			(pintype "passive")
		)
		(pad "3" smd roundrect
			(at 1.2 0 180)
			(size 0.9 0.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 127 "GND")
			(pinfunction "C")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SC-59.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "B.Cu")
		(at 166.7125 125.35)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R11"
			(at -3.7715 0.38 0)
			(layer "B.SilkS")
		)
		(property "Value" "120"
			(at 0 -1.65 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902)
			(net 72 "VCC")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902)
			(net 171 "Net-(C6-Pad1)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "B.Cu")
		(at 78.8 98.4 180)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP4"
			(at 0 1.448 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 -1.55 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 1.45 0)
			(layer "B.Fab")
		)
		(pad "1" smd circle
			(at 0 0 180)
			(size 1 1)
			(layers "B.Cu" "B.Mask")
			(net 34 "/D1")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "B.Cu")
		(at 189.103 103.8 -90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C95"
			(at 0.467 2.159 270)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "0.1µF"
			(at 0 -1.68 90)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0 270)
			(size 1 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 72 "VCC")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0 270)
			(size 1 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 127 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "B.Cu")
		(at 82.87 192.786 180)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C30"
			(at -0.315 -2.032 0)
			(layer "B.SilkS")
		)
		(property "Value" "0.01uF"
			(at 0 -1.68 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0 180)
			(size 1 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 69 "Net-(C30-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0 180)
			(size 1 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 70 "Net-(C30-Pad2)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "B.Cu")
		(at 216.027 110.236 180)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP98"
			(at 0 1.448 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 -1.55 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 1.45 180)
			(layer "B.Fab")
		)
		(pad "1" smd circle
			(at 0 0 180)
			(size 1 1)
			(layers "B.Cu" "B.Mask")
			(net 91 "/VAB5")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "B.Cu")
		(at 219.9 172.85 180)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP1"
			(at 0 1.448 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 -1.55 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 1.45 0)
			(layer "B.Fab")
		)
		(pad "1" smd circle
			(at 0 0 180)
			(size 1 1)
			(layers "B.Cu" "B.Mask")
			(net 299 "Net-(U1-JOY-OUT1)")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "B.Cu")
		(at 80.899 157.033 90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C47"
			(at -3.876 -0.127 270)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "47pF"
			(at 0 -1.68 90)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0 90)
			(size 1 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 401 "Net-(DA13-K)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0 90)
			(size 1 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 127 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "B.Cu")
		(at 194.25 77.9875 -90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R40"
			(at -3.6925 -0.441 270)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "39"
			(at 0 -1.65 90)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 270)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902)
			(net 184 "Net-(C18-Pad2)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 270)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902)
			(net 360 "Net-(Q11-E)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "B.Cu")
		(at 199.6 84.45 90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C12"
			(at 3.551 1.568 270)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "10pF"
			(at 0 -1.68 90)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0 90)
			(size 1 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 180 "Net-(Q10-B)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0 90)
			(size 1 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 127 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "B.Cu")
		(at 228.6285 142.875 180)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R83"
			(at 3.81 0 0)
			(layer "B.SilkS")
		)
		(property "Value" "100"
			(at 0 -1.65 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 180)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902)
			(net 126 "Net-(P2-Pin_2)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 180)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902)
			(net 288 "/JPIO6")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "B.Cu")
		(at 228.6285 127.635 180)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R89"
			(at 5.3575 0 0)
			(layer "B.SilkS")
		)
		(property "Value" "10"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 180)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902)
			(net 133 "Net-(P2-Pin_8)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 180)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902)
			(net 277 "/JPCLK1")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "B.Cu")
		(at 219.15 121.25 180)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C94"
			(at -0.814 2.124 0)
			(layer "B.SilkS")
		)
		(property "Value" "0.1µF"
			(at 0 -1.68 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0 180)
			(size 1 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 72 "VCC")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0 180)
			(size 1 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 127 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "B.Cu")
		(at 80.2 104.5 180)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP16"
			(at 0 1.448 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 -1.55 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 1.45 0)
			(layer "B.Fab")
		)
		(pad "1" smd circle
			(at 0 0 180)
			(size 1 1)
			(layers "B.Cu" "B.Mask")
			(net 312 "/PA5")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "B.Cu")
		(at 195.961 101.981 180)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP59"
			(at 0 1.448 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 -1.55 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 1.45 0)
			(layer "B.Fab")
		)
		(pad "1" smd circle
			(at 0 0 180)
			(size 1 1)
			(layers "B.Cu" "B.Mask")
			(net 148 "/VDA4")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "B.Cu")
		(at 129.1 167.65)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C25"
			(at -0.068 6.086 0)
			(layer "B.SilkS")
		)
		(property "Value" "1uF"
			(at 0 -1.68 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0)
			(size 1 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 344 "Net-(C25-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0)
			(size 1 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 188 "Net-(P1-SOUND-R)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "B.Cu")
		(at 124.65 145.3125 -90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R106"
			(at -7.1365 -0.064 270)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "5.1k"
			(at 0 -1.65 90)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 270)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902)
			(net 127 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 270)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902)
			(net 203 "Net-(U10D--)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "B.Cu")
		(at 135.5375 171.95)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R97"
			(at 0.5125 1.95 0)
			(layer "B.SilkS")
		)
		(property "Value" "10k"
			(at 0 -1.65 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902)
			(net 352 "Net-(P1-EXPAND)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902)
			(net 72 "VCC")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "B.Cu")
		(at 114.3 96.52 180)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP93"
			(at 0 1.448 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 -1.55 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 1.45 180)
			(layer "B.Fab")
		)
		(pad "1" smd circle
			(at 0 0 180)
			(size 1 1)
			(layers "B.Cu" "B.Mask")
			(net 214 "Net-(U14-XTAL0)")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "Package_TO_SOT_SMD:SC-59"
		(layer "B.Cu")
		(at 91.764 145.222 180)
		(descr "SC-59, https://lib.chipdip.ru/images/import_diod/original/SOT-23_SC-59.jpg")
		(tags "SC-59")
		(property "Reference" "DA20"
			(at 2.356 -3.876 0)
			(layer "B.SilkS")
		)
		(property "Value" "DAN202"
			(at 0 -2.5 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Dual diode, common cathode on pin 3"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.2 0.95 180)
			(size 0.9 0.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 397 "Net-(DA17-K)")
			(pinfunction "A")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at -1.2 -0.95 180)
			(size 0.9 0.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 167 "Net-(DA12-K)")
			(pinfunction "A")
			(pintype "passive")
		)
		(pad "3" smd roundrect
			(at 1.2 0 180)
			(size 0.9 0.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 72 "VCC")
			(pinfunction "K")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SC-59.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "B.Cu")
		(at 194.691 111.125 180)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP56"
			(at 0 1.448 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 -1.55 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 1.45 0)
			(layer "B.Fab")
		)
		(pad "1" smd circle
			(at 0 0 180)
			(size 1 1)
			(layers "B.Cu" "B.Mask")
			(net 145 "/VDA1")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "B.Cu")
		(at 133.1375 146.15 180)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R66"
			(at -4.1625 -0.25 0)
			(layer "B.SilkS")
		)
		(property "Value" "10k"
			(at 0 -1.65 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 180)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902)
			(net 339 "Net-(P5-MONO-OUT)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 180)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902)
			(net 372 "Net-(Q16-E)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "B.Cu")
		(at 194.63 192.278)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C82"
			(at 0 1.905 0)
			(layer "B.SilkS")
		)
		(property "Value" "0.1µF"
			(at 0 -1.68 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0)
			(size 1 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 127 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0)
			(size 1 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 72 "VCC")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "B.Cu")
		(at 130.5625 162.55)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R53"
			(at 6.1875 0.8 0)
			(layer "B.SilkS")
		)
		(property "Value" "10k"
			(at 0 -1.65 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902)
			(net 368 "Net-(Q14-E)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902)
			(net 333 "Net-(C23-Pad1)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "B.Cu")
		(at 228.6285 137.795 180)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R85"
			(at 3.81 0 0)
			(layer "B.SilkS")
		)
		(property "Value" "100"
			(at 0 -0.625 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 180)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902)
			(net 129 "Net-(P2-Pin_4)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 180)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902)
			(net 286 "/4017.D0")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "B.Cu")
		(at 104.6245 109.093)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R24"
			(at 3.9605 -0.889 0)
			(layer "B.SilkS")
		)
		(property "Value" "100"
			(at 0 -1.65 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr smd exclude_from_bom dnp)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902)
			(net 359 "Net-(Q9-E)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902)
			(net 127 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "B.Cu")
		(at 95.8615 147.447 180)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R7"
			(at -3.1985 -0.889 0)
			(layer "B.SilkS")
		)
		(property "Value" "30"
			(at 0 -1.65 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 180)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902)
			(net 353 "Net-(Q4-E)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 180)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902)
			(net 169 "Net-(DA12-A-Pad2)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "B.Cu")
		(at 124.8375 153.5 180)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R49"
			(at 0.7585 2.624 0)
			(layer "B.SilkS")
		)
		(property "Value" "1k"
			(at 0 -1.65 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 180)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902)
			(net 387 "Net-(Q13-C)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 180)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902)
			(net 298 "+9V")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "B.Cu")
		(at 216.027 99.695 180)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP102"
			(at 0 1.448 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 -1.55 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 1.45 180)
			(layer "B.Fab")
		)
		(pad "1" smd circle
			(at 0 0 180)
			(size 1 1)
			(layers "B.Cu" "B.Mask")
			(net 86 "/VAB9")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "B.Cu")
		(at 134.366 89.535 180)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP67"
			(at 0 1.448 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 -1.55 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 1.45 0)
			(layer "B.Fab")
		)
		(pad "1" smd circle
			(at 0 0 180)
			(size 1 1)
			(layers "B.Cu" "B.Mask")
			(net 244 "Net-(U13-P53)")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "B.Cu")
		(at 210.886 166.37 180)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C93"
			(at 0 1.68 0)
			(layer "B.SilkS")
		)
		(property "Value" "0.1µF"
			(at 0 -1.68 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0 180)
			(size 1 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 72 "VCC")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0 180)
			(size 1 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 127 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_SMD:SC-59"
		(layer "B.Cu")
		(at 87.95 154.8 180)
		(descr "SC-59, https://lib.chipdip.ru/images/import_diod/original/SOT-23_SC-59.jpg")
		(tags "SC-59")
		(property "Reference" "DA14"
			(at 0.07 -5.141 0)
			(layer "B.SilkS")
		)
		(property "Value" "DAN202"
			(at 0 -2.5 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Dual diode, common cathode on pin 3"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.2 0.95 180)
			(size 0.9 0.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 402 "Net-(DA19-K)")
			(pinfunction "A")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at -1.2 -0.95 180)
			(size 0.9 0.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 401 "Net-(DA13-K)")
			(pinfunction "A")
			(pintype "passive")
		)
		(pad "3" smd roundrect
			(at 1.2 0 180)
			(size 0.9 0.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 72 "VCC")
			(pinfunction "K")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SC-59.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "B.Cu")
		(at 165.85 105.4875 90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R26"
			(at -0.6845 -2.147 270)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "1.8k"
			(at 0 -1.65 90)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 90)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902)
			(net 127 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 90)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902)
			(net 373 "Net-(U7-BLA)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "B.Cu")
		(at 133.1 148.9)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C53"
			(at 4 -0.15 0)
			(layer "B.SilkS")
		)
		(property "Value" "1uF"
			(at 0 -1.68 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0)
			(size 1 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 350 "Net-(Q14-B)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0)
			(size 1 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 127 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "B.Cu")
		(at 80.4 89.5 180)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP27"
			(at 0 1.448 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 -1.55 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 1.45 0)
			(layer "B.Fab")
		)
		(pad "1" smd circle
			(at 0 0 180)
			(size 1 1)
			(layers "B.Cu" "B.Mask")
			(net 337 "Net-(P5-DOTCK)")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "B.Cu")
		(at 213.36 99.441 180)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP106"
			(at 0 1.448 0)
			(layer "B.SilkS")
		)
		(property "Value" "TestPoint"
			(at 0 -1.55 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 1.45 0)
			(layer "B.Fab")
		)
		(pad "1" smd circle
			(at 0 0 180)
			(size 1 1)
			(layers "B.Cu" "B.Mask")
			(net 82 "/VAB13")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "B.Cu")
		(at 111.379 148.021 90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C75"
			(at -17.714 -3.175 270)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "1800pF"
			(at 0 -1.68 90)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0 90)
			(size 1 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 203 "Net-(U10D--)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0 90)
			(size 1 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 221 "Net-(C75-Pad2)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "B.Cu")
		(at 80.3 84.4 180)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP21"
			(at 0 1.448 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 -1.55 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 1.45 0)
			(layer "B.Fab")
		)
		(pad "1" smd circle
			(at 0 0 180)
			(size 1 1)
			(layers "B.Cu" "B.Mask")
			(net 336 "{slash}IRQ")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "B.Cu")
		(at 100.9 99 180)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP3"
			(at 0 1.448 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 -1.55 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 1.45 0)
			(layer "B.Fab")
		)
		(pad "1" smd circle
			(at 0 0 180)
			(size 1 1)
			(layers "B.Cu" "B.Mask")
			(net 33 "/D0")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "B.Cu")
		(at 129.2875 180.8 180)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R76"
			(at -0.5315 -1.905 0)
			(layer "B.SilkS")
		)
		(property "Value" "1.8k"
			(at 0 -1.65 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 180)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902)
			(net 396 "Net-(Q18-B)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 180)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902)
			(net 303 "Net-(DA11-K)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "B.Cu")
		(at 108.8625 157.226)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R61"
			(at -1.5475 14.351 0)
			(layer "B.SilkS")
		)
		(property "Value" "10k"
			(at 0 -1.65 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902)
			(net 370 "Net-(Q15-E)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902)
			(net 346 "Net-(C27-Pad1)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "B.Cu")
		(at 78.8 102.4 180)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP18"
			(at 0 1.448 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 -1.55 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 1.45 0)
			(layer "B.Fab")
		)
		(pad "1" smd circle
			(at 0 0 180)
			(size 1 1)
			(layers "B.Cu" "B.Mask")
			(net 314 "/PA7")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "B.Cu")
		(at 201.295 191.455 90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C2"
			(at 0.066 2.286 270)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "15pF"
			(at 0 -1.68 90)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0 90)
			(size 1 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 127 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0 90)
			(size 1 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 406 "Net-(C2-Pad2)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_SMD:SC-59"
		(layer "B.Cu")
		(at 191.05 82.3 180)
		(descr "SC-59, https://lib.chipdip.ru/images/import_diod/original/SOT-23_SC-59.jpg")
		(tags "SC-59")
		(property "Reference" "Q11"
			(at -3.7 0.3 0)
			(layer "B.SilkS")
		)
		(property "Value" "C2412K"
			(at 0 -2.5 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "NPN transistor, base/emitter/collector"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.2 0.95 180)
			(size 0.9 0.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 178 "Net-(Q11-B)")
			(pinfunction "B")
			(pintype "input")
		)
		(pad "2" smd roundrect
			(at -1.2 -0.95 180)
			(size 0.9 0.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 360 "Net-(Q11-E)")
			(pinfunction "E")
			(pintype "passive")
		)
		(pad "3" smd roundrect
			(at 1.2 0 180)
			(size 0.9 0.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 72 "VCC")
			(pinfunction "C")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SC-59.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "B.Cu")
		(at 175.702 192.024)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C3"
			(at 0 2.032 0)
			(layer "B.SilkS")
		)
		(property "Value" "47pF"
			(at 0 -1.68 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0)
			(size 1 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 127 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0)
			(size 1 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 292 "Net-(C3-Pad2)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "B.Cu")
		(at 176.596 98.298 180)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C9"
			(at -3.744 -0.762 0)
			(layer "B.SilkS")
		)
		(property "Value" "1nF"
			(at 0 -1.68 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0 180)
			(size 1 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 152 "Net-(U7-VB)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0 180)
			(size 1 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 154 "Net-(C9-Pad2)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "B.Cu")
		(at 117.45 165.5375 90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R65"
			(at 3.3875 -0.229 270)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "1k"
			(at 0 -1.65 90)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 90)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902)
			(net 394 "Net-(Q17-E)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 90)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902)
			(net 127 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "B.Cu")
		(at 125.1 165.05)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R54"
			(at -0.2 5.9 0)
			(layer "B.SilkS")
		)
		(property "Value" "10k"
			(at 0 -1.65 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902)
			(net 368 "Net-(Q14-E)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902)
			(net 342 "Net-(C24-Pad1)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_SMD:SC-59"
		(layer "B.Cu")
		(at 228.289 167.452 180)
		(descr "SC-59, https://lib.chipdip.ru/images/import_diod/original/SOT-23_SC-59.jpg")
		(tags "SC-59")
		(property "Reference" "DA9"
			(at -10.471 -11.745 0)
			(layer "B.SilkS")
		)
		(property "Value" "DAN202"
			(at 0 -2.5 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Dual diode, common anode on pin 1"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.2 0.95 180)
			(size 0.9 0.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 285 "/4017.D1")
			(pinfunction "A")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at -1.2 -0.95 180)
			(size 0.9 0.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 286 "/4017.D0")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "3" smd roundrect
			(at 1.2 0 180)
			(size 0.9 0.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 72 "VCC")
			(pinfunction "K")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SC-59.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "B.Cu")
		(at 102.5125 138.938 180)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R45"
			(at -0.1035 1.778 0)
			(layer "B.SilkS")
		)
		(property "Value" "100"
			(at 0 -1.65 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr smd exclude_from_bom dnp)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 180)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902)
			(net 127 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 180)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902)
			(net 361 "Net-(Q12-E)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "B.Cu")
		(at 166.37 154.2015 90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R6"
			(at -3.4055 -3.048 270)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "100"
			(at 0 -1.65 90)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr smd exclude_from_bom dnp)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 90)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902)
			(net 127 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 90)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902)
			(net 385 "Net-(Q8-E)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "B.Cu")
		(at 112.6 139.8875 90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R103"
			(at 12.5065 0.43 270)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "22k"
			(at 0 -1.65 90)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 90)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902)
			(net 283 "Net-(C77-Pad2)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 90)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902)
			(net 332 "Net-(U17-L.OUT)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "B.Cu")
		(at 197.1 84.4375 -90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R31"
			(at -3.4875 -2.25 270)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "10k"
			(at 0 -1.65 90)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 270)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902)
			(net 127 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 270)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902)
			(net 180 "Net-(Q10-B)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "B.Cu")
		(at 224.917 97.409 180)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP44"
			(at 0 1.448 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 -1.55 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 1.45 0)
			(layer "B.Fab")
		)
		(pad "1" smd circle
			(at 0 0 180)
			(size 1 1)
			(layers "B.Cu" "B.Mask")
			(net 141 "/VDB5")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "B.Cu")
		(at 100.7 111.7 180)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP11"
			(at 0 1.448 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 -1.55 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 1.45 0)
			(layer "B.Fab")
		)
		(pad "1" smd circle
			(at 0 0 180)
			(size 1 1)
			(layers "B.Cu" "B.Mask")
			(net 307 "/PA0")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "B.Cu")
		(at 228.6285 130.175 180)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R88"
			(at 3.81 0 180)
			(layer "B.SilkS")
		)
		(property "Value" "100"
			(at 0 -0.625 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 180)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902)
			(net 132 "Net-(P2-Pin_7)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 180)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902)
			(net 281 "/4016.D1")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "B.Cu")
		(at 231.1 135.4 180)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP29"
			(at 0 1.448 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 -1.55 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 1.45 0)
			(layer "B.Fab")
		)
		(pad "1" smd circle
			(at 0 0 180)
			(size 1 1)
			(layers "B.Cu" "B.Mask")
			(net 130 "Net-(P2-Pin_5)")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "B.Cu")
		(at 86.5905 173.355)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R111"
			(at -2.7705 -2.413 0)
			(layer "B.SilkS")
		)
		(property "Value" "100"
			(at 0 -1.65 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr smd exclude_from_bom dnp)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902)
			(net 127 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902)
			(net 182 "Net-(J2-Video)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "B.Cu")
		(at 165.989 190.246 180)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP82"
			(at 0 1.448 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 -1.55 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 1.45 0)
			(layer "B.Fab")
		)
		(pad "1" smd circle
			(at 0 0 180)
			(size 1 1)
			(layers "B.Cu" "B.Mask")
			(net 8 "/CA13")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "B.Cu")
		(at 126.4685 162.306)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R56"
			(at 0.6585 -1.778 0)
			(layer "B.SilkS")
		)
		(property "Value" "24k"
			(at 0 -1.65 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902)
			(net 369 "Net-(Q14-C)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902)
			(net 368 "Net-(Q14-E)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_SMD:SC-59"
		(layer "B.Cu")
		(at 92.018 153.482 180)
		(descr "SC-59, https://lib.chipdip.ru/images/import_diod/original/SOT-23_SC-59.jpg")
		(tags "SC-59")
		(property "Reference" "DA19"
			(at 4.134 -4.76 0)
			(layer "B.SilkS")
		)
		(property "Value" "DAN202"
			(at 0 -2.5 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Dual diode, common cathode on pin 3"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.2 0.95 180)
			(size 0.9 0.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 127 "GND")
			(pinfunction "A")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at -1.2 -0.95 180)
			(size 0.9 0.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 405 "Net-(DA19-A-Pad2)")
			(pinfunction "A")
			(pintype "passive")
		)
		(pad "3" smd roundrect
			(at 1.2 0 180)
			(size 0.9 0.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 402 "Net-(DA19-K)")
			(pinfunction "K")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SC-59.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "B.Cu")
		(at 134 78.85 180)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP37"
			(at 0 1.448 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 -1.55 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 1.45 0)
			(layer "B.Fab")
		)
		(pad "1" smd circle
			(at 0 0 180)
			(size 1 1)
			(layers "B.Cu" "B.Mask")
			(net 388 "Net-(U13-T1)")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "B.Cu")
		(at 233.619 137.795)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C37"
			(at 4.13 0 0)
			(layer "B.SilkS")
		)
		(property "Value" "330pF"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0)
			(size 1 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 129 "Net-(P2-Pin_4)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0)
			(size 1 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 127 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "B.Cu")
		(at 108.712 149.7095 -90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R101"
			(at 16.9145 2.159 270)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "22k"
			(at 0 -1.65 90)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 270)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902)
			(net 221 "Net-(C75-Pad2)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 270)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902)
			(net 220 "Net-(C74-Pad2)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "B.Cu")
		(at 183.2875 131.75 180)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R16"
			(at -5.1625 -2.1 0)
			(layer "B.SilkS")
		)
		(property "Value" "120"
			(at 0 -1.65 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 180)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902)
			(net 72 "VCC")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 180)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902)
			(net 170 "Net-(C7-Pad1)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_SMD:SC-59"
		(layer "B.Cu")
		(at 166.825 77.85 180)
		(descr "SC-59, https://lib.chipdip.ru/images/import_diod/original/SOT-23_SC-59.jpg")
		(tags "SC-59")
		(property "Reference" "Q12"
			(at 2.487 2.158 0)
			(layer "B.SilkS")
		)
		(property "Value" "C2412K"
			(at 0 -2.5 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "NPN transistor, base/emitter/collector"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.2 0.95 180)
			(size 0.9 0.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 187 "Net-(Q12-B)")
			(pinfunction "B")
			(pintype "input")
		)
		(pad "2" smd roundrect
			(at -1.2 -0.95 180)
			(size 0.9 0.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 361 "Net-(Q12-E)")
			(pinfunction "E")
			(pintype "passive")
		)
		(pad "3" smd roundrect
			(at 1.2 0 180)
			(size 0.9 0.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 72 "VCC")
			(pinfunction "C")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SC-59.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "B.Cu")
		(at 170.688 77.8745 90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R110"
			(at 4.3415 1.397 270)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "100"
			(at 0 -1.65 90)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr smd exclude_from_bom dnp)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 90)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902)
			(net 187 "Net-(Q12-B)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 90)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902)
			(net 72 "VCC")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_SMD:SC-59"
		(layer "B.Cu")
		(at 231.083 154.498 180)
		(descr "SC-59, https://lib.chipdip.ru/images/import_diod/original/SOT-23_SC-59.jpg")
		(tags "SC-59")
		(property "Reference" "DA1"
			(at -1.962 2.987 0)
			(layer "B.SilkS")
		)
		(property "Value" "DAP202"
			(at 0 -2.5 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Dual diode, common anode on pin 1"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.2 0.95 180)
			(size 0.9 0.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 223 "/JPSTR")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at -1.2 -0.95 180)
			(size 0.9 0.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 306 "unconnected-(DA1B-K-Pad2)")
			(pinfunction "K")
			(pintype "passive+no_connect")
		)
		(pad "3" smd roundrect
			(at 1.2 0 180)
			(size 0.9 0.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 127 "GND")
			(pinfunction "A")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SC-59.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "B.Cu")
		(at 178.25 77.7875 90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R43"
			(at 3.6195 0.185 270)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "470"
			(at 0 -1.65 90)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 90)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902)
			(net 187 "Net-(Q12-B)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 90)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902)
			(net 362 "Net-(U7-CO)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "B.Cu")
		(at 178.054 187.645 -90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C5"
			(at -3.622 -0.127 270)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "47pF"
			(at 0 -1.68 90)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr smd exclude_from_bom dnp)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0 270)
			(size 1 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 127 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0 270)
			(size 1 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 26 "XIN")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "B.Cu")
		(at 159.512 185.547 180)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP77"
			(at 0 1.448 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 -1.55 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 1.45 0)
			(layer "B.Fab")
		)
		(pad "1" smd circle
			(at 0 0 180)
			(size 1 1)
			(layers "B.Cu" "B.Mask")
			(net 13 "/CA18")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "B.Cu")
		(at 161.925 180.848 180)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP72"
			(at 0 1.448 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 -1.55 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 1.45 0)
			(layer "B.Fab")
		)
		(pad "1" smd circle
			(at 0 0 180)
			(size 1 1)
			(layers "B.Cu" "B.Mask")
			(net 18 "/CA23")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "B.Cu")
		(at 183.007 188.4915 90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R1"
			(at 3.5795 0.381 270)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "270"
			(at 0 -1.65 90)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 90)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902)
			(net 291 "Net-(C1-Pad2)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 90)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902)
			(net 293 "Net-(R1-Pad2)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "B.Cu")
		(at 100.9 96.5 180)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP5"
			(at 0 1.448 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 -1.55 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 1.45 0)
			(layer "B.Fab")
		)
		(pad "1" smd circle
			(at 0 0 180)
			(size 1 1)
			(layers "B.Cu" "B.Mask")
			(net 35 "/D2")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "B.Cu")
		(at 217.932 166.2195 -90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R92"
			(at -0.2305 2.159 270)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "10k"
			(at 0 -1.65 90)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 270)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902)
			(net 72 "VCC")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 270)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902)
			(net 336 "{slash}IRQ")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "B.Cu")
		(at 101 94 180)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP7"
			(at 0 1.448 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 -1.55 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 1.45 0)
			(layer "B.Fab")
		)
		(pad "1" smd circle
			(at 0 0 180)
			(size 1 1)
			(layers "B.Cu" "B.Mask")
			(net 37 "/D4")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "B.Cu")
		(at 96.52 125.7535 -90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R33"
			(at -3.8335 -0.254 270)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "22"
			(at 0 -1.65 90)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 270)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902)
			(net 189 "Net-(Q10-E)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 270)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902)
			(net 172 "Net-(DA15-A-Pad2)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "B.Cu")
		(at 197.358 99.822 180)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP58"
			(at 0 1.448 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 -1.55 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 1.45 0)
			(layer "B.Fab")
		)
		(pad "1" smd circle
			(at 0 0 180)
			(size 1 1)
			(layers "B.Cu" "B.Mask")
			(net 147 "/VDA3")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "B.Cu")
		(at 97.4325 139.065 180)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R46"
			(at -0.6115 1.778 0)
			(layer "B.SilkS")
		)
		(property "Value" "39"
			(at 0 -1.65 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 180)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902)
			(net 361 "Net-(Q12-E)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 180)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902)
			(net 398 "Net-(DA17-A-Pad2)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "B.Cu")
		(at 228.6285 140.335 180)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R84"
			(at 3.81 0 180)
			(layer "B.SilkS")
		)
		(property "Value" "100"
			(at 0 -1.65 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 180)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902)
			(net 128 "Net-(P2-Pin_3)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 180)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902)
			(net 287 "EXTLATCH")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "B.Cu")
		(at 231 125.1 180)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP31"
			(at 0 1.448 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 -1.55 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 1.45 0)
			(layer "B.Fab")
		)
		(pad "1" smd circle
			(at 0 0 180)
			(size 1 1)
			(layers "B.Cu" "B.Mask")
			(net 134 "Net-(P2-Pin_9)")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "B.Cu")
		(at 112.3 156.5625 -90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R63"
			(at -3.1465 -0.095 270)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "24k"
			(at 0 -1.65 90)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 270)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902)
			(net 371 "Net-(Q15-C)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 270)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902)
			(net 370 "Net-(Q15-E)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "B.Cu")
		(at 137.033 91.948 180)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP66"
			(at 0 1.448 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 -1.55 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 1.45 0)
			(layer "B.Fab")
		)
		(pad "1" smd circle
			(at 0 0 180)
			(size 1 1)
			(layers "B.Cu" "B.Mask")
			(net 243 "Net-(U13-P54)")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "B.Cu")
		(at 87.823 150.876 180)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C44"
			(at 3.495 -0.381 0)
			(layer "B.SilkS")
		)
		(property "Value" "47pF"
			(at 0 -1.68 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0 180)
			(size 1 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 167 "Net-(DA12-K)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0 180)
			(size 1 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 127 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "B.Cu")
		(at 133.1125 151.55)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R52"
			(at 8.2375 -2.65 0)
			(layer "B.SilkS")
		)
		(property "Value" "1k"
			(at 0 -1.65 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902)
			(net 350 "Net-(Q14-B)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902)
			(net 387 "Net-(Q13-C)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_PinSocket_2.54mm:PinSocket_2x06_P2.54mm_Vertical"
		(layer "B.Cu")
		(at 169.545 67.691 -90)
		(descr "Through hole straight socket strip, 2x06, 2.54mm pitch, double cols (from Kicad 4.0.7), script generated")
		(tags "Through hole socket strip THT 2x06 2.54mm double row")
		(property "Reference" "J3"
			(at -1.27 2.77 90)
			(layer "B.SilkS")
		)
		(property "Value" "Conn_02x06_Odd_Even"
			(at -1.27 -15.47 90)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, double row, 02x06, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_2x??_*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at -1.27 -6.35 0)
			(layer "B.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 408 "Net-(J3-Pin_1)")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at -2.54 0 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 409 "Net-(J3-Pin_2)")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole circle
			(at 0 -2.54 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 410 "Net-(J3-Pin_3)")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole circle
			(at -2.54 -2.54 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 411 "Net-(J3-Pin_4)")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(pad "5" thru_hole circle
			(at 0 -5.08 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 127 "GND")
			(pinfunction "Pin_5")
			(pintype "passive")
		)
		(pad "6" thru_hole circle
			(at -2.54 -5.08 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 127 "GND")
			(pinfunction "Pin_6")
			(pintype "passive")
		)
		(pad "7" thru_hole circle
			(at 0 -7.62 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 412 "Net-(J3-Pin_7)")
			(pinfunction "Pin_7")
			(pintype "passive")
		)
		(pad "8" thru_hole circle
			(at -2.54 -7.62 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 413 "Net-(J3-Pin_8)")
			(pinfunction "Pin_8")
			(pintype "passive")
		)
		(pad "9" thru_hole circle
			(at 0 -10.16 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 414 "Net-(J3-Pin_9)")
			(pinfunction "Pin_9")
			(pintype "passive")
		)
		(pad "10" thru_hole circle
			(at -2.54 -10.16 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 415 "Net-(J3-Pin_10)")
			(pinfunction "Pin_10")
			(pintype "passive")
		)
		(pad "11" thru_hole circle
			(at 0 -12.7 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 416 "Net-(J3-Pin_11)")
			(pinfunction "Pin_11")
			(pintype "passive")
		)
		(pad "12" thru_hole circle
			(at -2.54 -12.7 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 417 "Net-(J3-Pin_12)")
			(pinfunction "Pin_12")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_2x06_P2.54mm_Vertical.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "LED_THT:LED_D5.0mm_Horizontal_O6.35mm_Z3.0mm"
		(layer "B.Cu")
		(at 265.43 177.165 -90)
		(descr "LED, diameter 5.0mm, horizontal offset 6.35mm, z-position of LED center 3.0mm, 2 pins, generated by kicad-footprint-generator")
		(tags "LED")
		(property "Reference" "LED1"
			(at 1.27 1.96 90)
			(layer "B.SilkS")
		)
		(property "Value" "Red"
			(at 1.27 -16.01 90)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Light emitting diode"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "LED* LED_SMD:* LED_THT:*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 1.27 -10.1294 90)
			(layer "B.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 270)
			(size 1.8 1.8)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 127 "GND")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 2.54 0 270)
			(size 1.8 1.8)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 419 "Net-(LED1-A)")
			(pinfunction "A")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/LED_THT.3dshapes/LED_D5.0mm_Horizontal_O6.35mm_Z3.0mm.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "B.Cu")
		(at 139.954 98.171 180)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP64"
			(at 0 1.448 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 -1.55 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 1.45 0)
			(layer "B.Fab")
		)
		(pad "1" smd circle
			(at 0 0 180)
			(size 1 1)
			(layers "B.Cu" "B.Mask")
			(net 241 "Net-(U13-P56)")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "B.Cu")
		(at 227.584 109.601 180)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP39"
			(at 0 1.448 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 -1.55 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 1.45 0)
			(layer "B.Fab")
		)
		(pad "1" smd circle
			(at 0 0 180)
			(size 1 1)
			(layers "B.Cu" "B.Mask")
			(net 136 "/VDB0")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "B.Cu")
		(at 188.341 113.03 180)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP50"
			(at 0 1.448 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 -1.55 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 1.45 0)
			(layer "B.Fab")
		)
		(pad "1" smd circle
			(at 0 0 180)
			(size 1 1)
			(layers "B.Cu" "B.Mask")
			(net 107 "/VAA3")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "B.Cu")
		(at 184.75 86.85)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C13"
			(at 0.2 -1.7 0)
			(layer "B.SilkS")
		)
		(property "Value" "220pF"
			(at 0 -1.68 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0)
			(size 1 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 173 "Net-(C13-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0)
			(size 1 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 127 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "B.Cu")
		(at 198.374 174.498 180)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP85"
			(at 0 1.448 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 -1.55 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 1.45 0)
			(layer "B.Fab")
		)
		(pad "1" smd circle
			(at 0 0 180)
			(size 1 1)
			(layers "B.Cu" "B.Mask")
			(net 71 "/CA7")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "B.Cu")
		(at 120.7375 163.05 180)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R69"
			(at 0.2145 -9.162 0)
			(layer "B.SilkS")
		)
		(property "Value" "10k"
			(at 0 -1.65 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 180)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902)
			(net 339 "Net-(P5-MONO-OUT)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 180)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902)
			(net 394 "Net-(Q17-E)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "B.Cu")
		(at 173.9625 138.45)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R13"
			(at 0.3125 -17.75 0)
			(layer "B.SilkS")
		)
		(property "Value" "1.1k"
			(at 0 -1.65 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902)
			(net 358 "Net-(Q6-B)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902)
			(net 355 "Net-(Q5-E)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "B.Cu")
		(at 183.134 113.538 180)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP54"
			(at 0 1.448 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 -1.55 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 1.45 0)
			(layer "B.Fab")
		)
		(pad "1" smd circle
			(at 0 0 180)
			(size 1 1)
			(layers "B.Cu" "B.Mask")
			(net 103 "/VAA7")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "B.Cu")
		(at 226.187 99.441 180)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP43"
			(at 0 1.448 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 -1.55 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 1.45 0)
			(layer "B.Fab")
		)
		(pad "1" smd circle
			(at 0 0 180)
			(size 1 1)
			(layers "B.Cu" "B.Mask")
			(net 140 "/VDB4")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "B.Cu")
		(at 101 82.3 180)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP22"
			(at 0 1.448 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 -1.55 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 1.45 0)
			(layer "B.Fab")
		)
		(pad "1" smd circle
			(at 0 0 180)
			(size 1 1)
			(layers "B.Cu" "B.Mask")
			(net 340 "Net-(P5-SL-IN)")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "B.Cu")
		(at 133.15 82.1 180)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP38"
			(at 0 1.448 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 -1.55 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 1.45 0)
			(layer "B.Fab")
		)
		(pad "1" smd circle
			(at 0 0 180)
			(size 1 1)
			(layers "B.Cu" "B.Mask")
			(net 389 "Net-(U13-T0)")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "B.Cu")
		(at 168.148 120.716 90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C83"
			(at -0.315 -2.286 270)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "0.01uF"
			(at 0 -1.68 90)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Polarized capacitor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "CP_*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0 90)
			(size 1 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 72 "VCC")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0 90)
			(size 1 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 127 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "B.Cu")
		(at 220.98 110.363 180)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP94"
			(at 0 1.448 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 -1.55 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 1.45 180)
			(layer "B.Fab")
		)
		(pad "1" smd circle
			(at 0 0 180)
			(size 1 1)
			(layers "B.Cu" "B.Mask")
			(net 95 "/VAB1")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "B.Cu")
		(at 136.4 156.6875 -90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R48"
			(at 0.1575 -2.284 270)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "33k"
			(at 0 -1.65 90)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 270)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902)
			(net 381 "Net-(Q13-B)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 270)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902)
			(net 382 "Net-(U14-~{MUTE})")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "B.Cu")
		(at 171.1 88)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C15"
			(at 0.096 2.678 0)
			(layer "B.SilkS")
		)
		(property "Value" "220pF"
			(at 0 -1.68 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0)
			(size 1 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 177 "Net-(C15-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0)
			(size 1 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 127 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "B.Cu")
		(at 87.945 130.175 180)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C50"
			(at 3.622 1.143 0)
			(layer "B.SilkS")
		)
		(property "Value" "47pF"
			(at 0 -1.68 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0 180)
			(size 1 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 168 "Net-(DA15-K)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0 180)
			(size 1 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 127 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "B.Cu")
		(at 125.0715 167.55)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R55"
			(at -0.3625 6 0)
			(layer "B.SilkS")
		)
		(property "Value" "10k"
			(at 0 -1.65 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902)
			(net 368 "Net-(Q14-E)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902)
			(net 344 "Net-(C25-Pad1)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "B.Cu")
		(at 165.735 180.086 180)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP84"
			(at 0 1.448 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 -1.55 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 1.45 0)
			(layer "B.Fab")
		)
		(pad "1" smd circle
			(at 0 0 180)
			(size 1 1)
			(layers "B.Cu" "B.Mask")
			(net 6 "/CA11")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "B.Cu")
		(at 190.05 130.3)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C92"
			(at 1.95 -1.75 0)
			(layer "B.SilkS")
		)
		(property "Value" "0.1µF"
			(at 0 -1.68 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0)
			(size 1 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 72 "VCC")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0)
			(size 1 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 127 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "B.Cu")
		(at 117.05 169.5375 90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R71"
			(at -3.5625 -0.1 270)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "10k"
			(at 0 -1.65 90)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 90)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902)
			(net 78 "Net-(J2-Audio)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 90)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902)
			(net 394 "Net-(Q17-E)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "B.Cu")
		(at 194.437 86.6375 -90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R109"
			(at 5.0565 -0.254 270)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "100"
			(at 0 -1.65 90)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr smd exclude_from_bom dnp)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 270)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902)
			(net 180 "Net-(Q10-B)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 270)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902)
			(net 72 "VCC")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "B.Cu")
		(at 233.619 130.175)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C40"
			(at 4.13 0 0)
			(layer "B.SilkS")
		)
		(property "Value" "330pF"
			(at 0 0.03 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0)
			(size 1 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 132 "Net-(P2-Pin_7)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0)
			(size 1 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 127 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "B.Cu")
		(at 97.724 192.532)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C32"
			(at -0.061 -2.159 0)
			(layer "B.SilkS")
		)
		(property "Value" "0.1µF"
			(at 0 -1.68 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0)
			(size 1 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 1 "Net-(P3-Pin_2)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0)
			(size 1 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 127 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "B.Cu")
		(at 120.396 152.593 -90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C80"
			(at 0.696 3.175 270)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "0.1µF"
			(at 0 -1.68 90)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0 270)
			(size 1 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 127 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0 270)
			(size 1 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 298 "+9V")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "B.Cu")
		(at 109.6 144.15 -90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C76"
			(at -3.45 -0.1 270)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "100pF"
			(at 0 -1.68 90)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0 270)
			(size 1 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 127 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0 270)
			(size 1 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 222 "Net-(U10D-+)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "B.Cu")
		(at 129.9 145.3875 90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R58"
			(at 3.8875 0.1 270)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "1k"
			(at 0 -1.65 90)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 90)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902)
			(net 372 "Net-(Q16-E)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 90)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902)
			(net 127 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "B.Cu")
		(at 228.6285 122.555 180)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R91"
			(at 0 1.65 0)
			(layer "B.SilkS")
		)
		(property "Value" "10"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 180)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902)
			(net 135 "Net-(P2-Pin_10)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 180)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902)
			(net 223 "/JPSTR")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "B.Cu")
		(at 127.2 145.4125 90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R57"
			(at 3.9375 -0.7 270)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "1.8k"
			(at 0 -1.65 90)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 90)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902)
			(net 369 "Net-(Q14-C)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 90)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902)
			(net 127 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "B.Cu")
		(at 165.55 149.9875 90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R17"
			(at -1.1425 -2.609 270)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "30"
			(at 0 -1.65 90)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 90)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902)
			(net 385 "Net-(Q8-E)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 90)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902)
			(net 404 "Net-(DA13-A-Pad2)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "B.Cu")
		(at 108.905 159.766 180)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C27"
			(at 1.59 -13.843 0)
			(layer "B.SilkS")
		)
		(property "Value" "1uF"
			(at 0 -1.68 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0 180)
			(size 1 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 346 "Net-(C27-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0 180)
			(size 1 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 340 "Net-(P5-SL-IN)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_SMD:SC-59"
		(layer "B.Cu")
		(at 119.35 159.45 180)
		(descr "SC-59, https://lib.chipdip.ru/images/import_diod/original/SOT-23_SC-59.jpg")
		(tags "SC-59")
		(property "Reference" "Q15"
			(at 0.1 2.732 0)
			(layer "B.SilkS")
		)
		(property "Value" "C2412K"
			(at 0 -2.5 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "NPN transistor, base/emitter/collector"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.2 0.95 180)
			(size 0.9 0.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 351 "Net-(Q15-B)")
			(pinfunction "B")
			(pintype "input")
		)
		(pad "2" smd roundrect
			(at -1.2 -0.95 180)
			(size 0.9 0.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 370 "Net-(Q15-E)")
			(pinfunction "E")
			(pintype "passive")
		)
		(pad "3" smd roundrect
			(at 1.2 0 180)
			(size 0.9 0.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 371 "Net-(Q15-C)")
			(pinfunction "C")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SC-59.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "B.Cu")
		(at 159.004 188.087 180)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP79"
			(at 0 1.448 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 -1.55 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 1.45 0)
			(layer "B.Fab")
		)
		(pad "1" smd circle
			(at 0 0 180)
			(size 1 1)
			(layers "B.Cu" "B.Mask")
			(net 11 "/CA16")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "Package_TO_SOT_SMD:SC-59"
		(layer "B.Cu")
		(at 169 137 180)
		(descr "SC-59, https://lib.chipdip.ru/images/import_diod/original/SOT-23_SC-59.jpg")
		(tags "SC-59")
		(property "Reference" "Q6"
			(at 3.55 0.3 0)
			(layer "B.SilkS")
		)
		(property "Value" "C2412K"
			(at 0 -2.5 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "NPN transistor, base/emitter/collector"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.2 0.95 180)
			(size 0.9 0.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 358 "Net-(Q6-B)")
			(pinfunction "B")
			(pintype "input")
		)
		(pad "2" smd roundrect
			(at -1.2 -0.95 180)
			(size 0.9 0.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 357 "Net-(Q6-E)")
			(pinfunction "E")
			(pintype "passive")
		)
		(pad "3" smd roundrect
			(at 1.2 0 180)
			(size 0.9 0.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 72 "VCC")
			(pinfunction "C")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SC-59.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "B.Cu")
		(at 134.366 86.995 180)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP69"
			(at 0 1.448 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 -1.55 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 1.45 0)
			(layer "B.Fab")
		)
		(pad "1" smd circle
			(at 0 0 180)
			(size 1 1)
			(layers "B.Cu" "B.Mask")
			(net 246 "Net-(U13-P51)")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "B.Cu")
		(at 99.949 151.4075 -90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R12"
			(at 7.0885 -0.127 270)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "30"
			(at 0 -1.65 90)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 270)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902)
			(net 357 "Net-(Q6-E)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 270)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902)
			(net 405 "Net-(DA19-A-Pad2)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "B.Cu")
		(at 172.974 187.772 -90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C4"
			(at -3.749 0 270)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "47pF"
			(at 0 -1.68 90)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr smd exclude_from_bom dnp)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0 270)
			(size 1 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 127 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0 270)
			(size 1 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 296 "Net-(U18-3.546M)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "B.Cu")
		(at 171.1 85.8)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C16"
			(at -0.92 -1.98 0)
			(layer "B.SilkS")
		)
		(property "Value" "1uF"
			(at 0 -1.68 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0)
			(size 1 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 177 "Net-(C15-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0)
			(size 1 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 179 "Net-(U7-(R-Y)I)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "B.Cu")
		(at 222.377 108.077 180)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP107"
			(at 0 1.448 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 -1.55 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 1.45 180)
			(layer "B.Fab")
		)
		(pad "1" smd circle
			(at 0 0 180)
			(size 1 1)
			(layers "B.Cu" "B.Mask")
			(net 96 "/VAB0")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "B.Cu")
		(at 130.495 165.1)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C24"
			(at 6.157 -0.254 0)
			(layer "B.SilkS")
		)
		(property "Value" "1uF"
			(at 0 -1.68 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0)
			(size 1 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 342 "Net-(C24-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0)
			(size 1 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 341 "Net-(P5-SR-IN)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_SMD:SC-59"
		(layer "B.Cu")
		(at 191.05 86.7 180)
		(descr "SC-59, https://lib.chipdip.ru/images/import_diod/original/SOT-23_SC-59.jpg")
		(tags "SC-59")
		(property "Reference" "Q10"
			(at -0.466 -4.232 0)
			(layer "B.SilkS")
		)
		(property "Value" "C2412K"
			(at 0 -2.5 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "NPN transistor, base/emitter/collector"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.2 0.95 180)
			(size 0.9 0.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 180 "Net-(Q10-B)")
			(pinfunction "B")
			(pintype "input")
		)
		(pad "2" smd roundrect
			(at -1.2 -0.95 180)
			(size 0.9 0.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 189 "Net-(Q10-E)")
			(pinfunction "E")
			(pintype "passive")
		)
		(pad "3" smd roundrect
			(at 1.2 0 180)
			(size 0.9 0.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 72 "VCC")
			(pinfunction "C")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SC-59.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "B.Cu")
		(at 108.8625 162.179)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R60"
			(at -1.5475 13.081 0)
			(layer "B.SilkS")
		)
		(property "Value" "10k"
			(at 0 -1.65 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902)
			(net 370 "Net-(Q15-E)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902)
			(net 334 "Net-(C26-Pad1)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "B.Cu")
		(at 137.668 97.028 180)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP71"
			(at 0 1.448 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 -1.55 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 1.45 0)
			(layer "B.Fab")
		)
		(pad "1" smd circle
			(at 0 0 180)
			(size 1 1)
			(layers "B.Cu" "B.Mask")
			(net 407 "Net-(U13-P5RD)")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "B.Cu")
		(at 163.068 184.404 180)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP75"
			(at 0 1.448 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 -1.55 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 1.45 0)
			(layer "B.Fab")
		)
		(pad "1" smd circle
			(at 0 0 180)
			(size 1 1)
			(layers "B.Cu" "B.Mask")
			(net 15 "/CA20")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "B.Cu")
		(at 95.758 130.9135 -90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R42"
			(at -0.4845 -2.032 270)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "100"
			(at 0 -1.65 90)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr smd exclude_from_bom dnp)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 270)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902)
			(net 360 "Net-(Q11-E)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 270)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902)
			(net 399 "Net-(DA16-K)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "B.Cu")
		(at 180.7229 192.3796)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R3"
			(at 0.3791 1.9304 0)
			(layer "B.SilkS")
		)
		(property "Value" "270"
			(at 0 -1.65 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902)
			(net 292 "Net-(C3-Pad2)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902)
			(net 295 "Net-(R3-Pad2)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "B.Cu")
		(at 224.4125 165.75)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R80"
			(at -9.7625 4.25 0)
			(layer "B.SilkS")
		)
		(property "Value" "10k"
			(at 0 -1.65 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902)
			(net 72 "VCC")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902)
			(net 285 "/4017.D1")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_SMD:SC-59"
		(layer "B.Cu")
		(at 91.764 136.337 180)
		(descr "SC-59, https://lib.chipdip.ru/images/import_diod/original/SOT-23_SC-59.jpg")
		(tags "SC-59")
		(property "Reference" "DA16"
			(at -2.978 2.352 0)
			(layer "B.SilkS")
		)
		(property "Value" "DAN202"
			(at 0 -2.5 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Dual diode, common cathode on pin 3"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.2 0.95 180)
			(size 0.9 0.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 127 "GND")
			(pinfunction "A")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at -1.2 -0.95 180)
			(size 0.9 0.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 400 "Net-(DA16-A-Pad2)")
			(pinfunction "A")
			(pintype "passive")
		)
		(pad "3" smd roundrect
			(at 1.2 0 180)
			(size 0.9 0.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 399 "Net-(DA16-K)")
			(pinfunction "K")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SC-59.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "B.Cu")
		(at 82.87 189.484 180)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C31"
			(at 0 1.68 0)
			(layer "B.SilkS")
		)
		(property "Value" "0.1µF"
			(at 0 -1.68 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0 180)
			(size 1 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 73 "Net-(C31-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0 180)
			(size 1 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 74 "Net-(C31-Pad2)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "B.Cu")
		(at 169.4625 133.55)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R9"
			(at -2.9655 0.181 0)
			(layer "B.SilkS")
		)
		(property "Value" "1.5k"
			(at 0 -1.65 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902)
			(net 72 "VCC")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902)
			(net 354 "Net-(Q4-B)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "B.Cu")
		(at 219.837 97.409 180)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP103"
			(at 0 1.448 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 -1.55 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 1.45 180)
			(layer "B.Fab")
		)
		(pad "1" smd circle
			(at 0 0 180)
			(size 1 1)
			(layers "B.Cu" "B.Mask")
			(net 85 "/VAB10")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "B.Cu")
		(at 164.211 182.118 180)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP73"
			(at 0 1.448 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 -1.55 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 1.45 0)
			(layer "B.Fab")
		)
		(pad "1" smd circle
			(at 0 0 180)
			(size 1 1)
			(layers "B.Cu" "B.Mask")
			(net 17 "/CA22")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "B.Cu")
		(at 173.6125 150.5 180)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R18"
			(at -0.4625 -6.8 0)
			(layer "B.SilkS")
		)
		(property "Value" "1.1k"
			(at 0 -1.65 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 180)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902)
			(net 383 "Net-(Q7-E)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 180)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902)
			(net 386 "Net-(Q8-B)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "B.Cu")
		(at 183.388 166.624)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP90"
			(at 0 1.448 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 -1.55 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 1.45 180)
			(layer "B.Fab")
		)
		(pad "1" smd circle
			(at 0 0)
			(size 1 1)
			(layers "B.Cu" "B.Mask")
			(net 76 "/{slash}CPURD")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "B.Cu")
		(at 189.611 139.0885 90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R98"
			(at -4.4215 0.254 270)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "100"
			(at 0 -1.65 90)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 90)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902)
			(net 337 "Net-(P5-DOTCK)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 90)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902)
			(net 75 "Net-(U3-5MOUT)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "B.Cu")
		(at 173.355 82.0185 -90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R108"
			(at -14.7085 -12.827 270)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "100"
			(at 0 -1.65 90)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr smd exclude_from_bom dnp)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 270)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902)
			(net 345 "Net-(Q9-B)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 270)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902)
			(net 72 "VCC")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "B.Cu")
		(at 228.25 188.65 -90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C85"
			(at 5.533 -0.096 270)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "0.1µF"
			(at 0 -1.68 90)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Polarized capacitor"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "CP_*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0 270)
			(size 1 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 72 "VCC")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0 270)
			(size 1 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 127 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "B.Cu")
		(at 115.5 147.9 90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C77"
			(at -3.738 -1.2 270)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "1nF"
			(at 0 -1.68 90)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0 90)
			(size 1 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 127 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0 90)
			(size 1 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 283 "Net-(C77-Pad2)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "B.Cu")
		(at 174.0625 135.9)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R8"
			(at 0.7875 -17.05 0)
			(layer "B.SilkS")
		)
		(property "Value" "1.1k"
			(at 0 -1.65 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902)
			(net 354 "Net-(Q4-B)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902)
			(net 347 "Net-(Q3-E)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "B.Cu")
		(at 187.071 110.871 180)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP51"
			(at 0 1.448 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 -1.55 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 1.45 0)
			(layer "B.Fab")
		)
		(pad "1" smd circle
			(at 0 0 180)
			(size 1 1)
			(layers "B.Cu" "B.Mask")
			(net 106 "/VAA4")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "B.Cu")
		(at 183.3 129.35)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C7"
			(at 1.1 -1.95 0)
			(layer "B.SilkS")
		)
		(property "Value" "0.1µF"
			(at 0 -1.68 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0)
			(size 1 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 170 "Net-(C7-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0)
			(size 1 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 176 "Net-(U7-AG)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "B.Cu")
		(at 180.3875 89.05)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R35"
			(at 4.3625 1.7 0)
			(layer "B.SilkS")
		)
		(property "Value" "270"
			(at 0 -1.65 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902)
			(net 364 "Net-(U7-(B-Y)O)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902)
			(net 173 "Net-(C13-Pad1)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "B.Cu")
		(at 169.95 124.7 90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C6"
			(at -0.4 2.5 270)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "0.1µF"
			(at 0 -1.68 90)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0 90)
			(size 1 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 171 "Net-(C6-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0 90)
			(size 1 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 175 "Net-(U7-AR)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "B.Cu")
		(at 223.1625 160.782 180)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R82"
			(at 3.1985 0 0)
			(layer "B.SilkS")
		)
		(property "Value" "10k"
			(at 0 -1.65 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 180)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902)
			(net 72 "VCC")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 180)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902)
			(net 281 "/4016.D1")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "B.Cu")
		(at 87.823 140.081 180)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C48"
			(at 3.622 -1.016 0)
			(layer "B.SilkS")
		)
		(property "Value" "47pF"
			(at 0 -1.68 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0 180)
			(size 1 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 399 "Net-(DA16-K)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0 180)
			(size 1 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 127 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "B.Cu")
		(at 176.2875 89)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R34"
			(at -1.4085 2.313 0)
			(layer "B.SilkS")
		)
		(property "Value" "1k"
			(at 0 -1.65 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902)
			(net 127 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902)
			(net 364 "Net-(U7-(B-Y)O)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "B.Cu")
		(at 111.76 86.995 180)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP92"
			(at 0 1.448 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 -1.55 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 1.45 180)
			(layer "B.Fab")
		)
		(pad "1" smd circle
			(at 0 0 180)
			(size 1 1)
			(layers "B.Cu" "B.Mask")
			(net 217 "Net-(U14-LRCK)")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "B.Cu")
		(at 121.4375 143.1)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R107"
			(at 0 2.315 0)
			(layer "B.SilkS")
		)
		(property "Value" "5.1k"
			(at 0 -1.65 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902)
			(net 219 "Net-(U10C--)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902)
			(net 127 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "B.Cu")
		(at 170.307 189.164 -90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C70"
			(at -4.379 0.635 270)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "82pF"
			(at 0 -1.68 90)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0 270)
			(size 1 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 127 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0 270)
			(size 1 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 25 "Net-(P1-CIC3)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_SMD:SC-59"
		(layer "B.Cu")
		(at 228.416 163.129 180)
		(descr "SC-59, https://lib.chipdip.ru/images/import_diod/original/SOT-23_SC-59.jpg")
		(tags "SC-59")
		(property "Reference" "DA8"
			(at -10.852 6.03 0)
			(layer "B.SilkS")
		)
		(property "Value" "DAN202"
			(at 0 -2.5 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Dual diode, common anode on pin 1"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.2 0.95 180)
			(size 0.9 0.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 281 "/4016.D1")
			(pinfunction "A")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at -1.2 -0.95 180)
			(size 0.9 0.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 284 "/4016.D0")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "3" smd roundrect
			(at 1.2 0 180)
			(size 0.9 0.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 72 "VCC")
			(pinfunction "K")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SC-59.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "B.Cu")
		(at 187.071 139.131 90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C68"
			(at -4.252 0.254 270)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "56pF"
			(at 0 -1.68 90)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0 90)
			(size 1 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 337 "Net-(P5-DOTCK)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0 90)
			(size 1 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 127 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "B.Cu")
		(at 169.05 154.1625 -90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R19"
			(at 6.1115 3.95 270)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "1.5k"
			(at 0 -1.65 90)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 270)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902)
			(net 386 "Net-(Q8-B)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 270)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902)
			(net 72 "VCC")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "B.Cu")
		(at 177.546 93.5755 -90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R28"
			(at 0.6585 2.286 270)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "3.3k"
			(at 0 -1.65 90)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 270)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902)
			(net 156 "Net-(C11-Pad2)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 270)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902)
			(net 154 "Net-(C9-Pad2)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "B.Cu")
		(at 192.278 99.822 180)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP62"
			(at 0 1.448 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 -1.55 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 1.45 0)
			(layer "B.Fab")
		)
		(pad "1" smd circle
			(at 0 0 180)
			(size 1 1)
			(layers "B.Cu" "B.Mask")
			(net 151 "/VDA7")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "B.Cu")
		(at 80.4 96.4 180)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP6"
			(at 0 1.448 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 -1.55 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 1.45 0)
			(layer "B.Fab")
		)
		(pad "1" smd circle
			(at 0 0 180)
			(size 1 1)
			(layers "B.Cu" "B.Mask")
			(net 36 "/D3")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "B.Cu")
		(at 78.5 106.4 180)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP14"
			(at 0 1.448 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 -1.55 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 1.45 0)
			(layer "B.Fab")
		)
		(pad "1" smd circle
			(at 0 0 180)
			(size 1 1)
			(layers "B.Cu" "B.Mask")
			(net 311 "/PA3")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "Package_TO_SOT_SMD:SC-59"
		(layer "B.Cu")
		(at 168.05 129.05 180)
		(descr "SC-59, https://lib.chipdip.ru/images/import_diod/original/SOT-23_SC-59.jpg")
		(tags "SC-59")
		(property "Reference" "Q4"
			(at 3.3 0.3 0)
			(layer "B.SilkS")
		)
		(property "Value" "C2412K"
			(at 0 -2.5 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "NPN transistor, base/emitter/collector"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.2 0.95 180)
			(size 0.9 0.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 354 "Net-(Q4-B)")
			(pinfunction "B")
			(pintype "input")
		)
		(pad "2" smd roundrect
			(at -1.2 -0.95 180)
			(size 0.9 0.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 353 "Net-(Q4-E)")
			(pinfunction "E")
			(pintype "passive")
		)
		(pad "3" smd roundrect
			(at 1.2 0 180)
			(size 0.9 0.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 72 "VCC")
			(pinfunction "C")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SC-59.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "B.Cu")
		(at 219.202 105.344 -90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C97"
			(at 0.188 2.413 270)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "0.1µF"
			(at 0 -1.68 90)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0 270)
			(size 1 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 72 "VCC")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0 270)
			(size 1 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 127 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "B.Cu")
		(at 87.823 142.875 180)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C49"
			(at 3.622 -1.016 0)
			(layer "B.SilkS")
		)
		(property "Value" "47pF"
			(at 0 -1.68 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0 180)
			(size 1 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 397 "Net-(DA17-K)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0 180)
			(size 1 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 127 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "B.Cu")
		(at 130.1985 170.307)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R93"
			(at 3.7865 -0.127 0)
			(layer "B.SilkS")
		)
		(property "Value" "200"
			(at 0 -1.65 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902)
			(net 127 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902)
			(net 341 "Net-(P5-SR-IN)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "B.Cu")
		(at 173.6375 145.35 180)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R20"
			(at -0.9125 -8.9 0)
			(layer "B.SilkS")
		)
		(property "Value" "10k"
			(at 0 -1.65 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 180)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902)
			(net 383 "Net-(Q7-E)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 180)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902)
			(net 366 "Net-(C8-Pad1)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_SMD:SC-59"
		(layer "B.Cu")
		(at 166.65 82.25 180)
		(descr "SC-59, https://lib.chipdip.ru/images/import_diod/original/SOT-23_SC-59.jpg")
		(tags "SC-59")
		(property "Reference" "Q9"
			(at 5.106 -1.57 0)
			(layer "B.SilkS")
		)
		(property "Value" "C2412K"
			(at 0 -2.5 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "NPN transistor, base/emitter/collector"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.2 0.95 180)
			(size 0.9 0.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 345 "Net-(Q9-B)")
			(pinfunction "B")
			(pintype "input")
		)
		(pad "2" smd roundrect
			(at -1.2 -0.95 180)
			(size 0.9 0.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 359 "Net-(Q9-E)")
			(pinfunction "E")
			(pintype "passive")
		)
		(pad "3" smd roundrect
			(at 1.2 0 180)
			(size 0.9 0.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 72 "VCC")
			(pinfunction "C")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SC-59.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "B.Cu")
		(at 225.552 186.878 -90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C29"
			(at 6.035 -0.248 270)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "0.1µF"
			(at 0 -1.68 90)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Polarized capacitor"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "CP_*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0 270)
			(size 1 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 72 "VCC")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0 270)
			(size 1 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 157 "Net-(U8-RES)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "B.Cu")
		(at 176.6335 100.838 180)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R27"
			(at -4.4685 -0.508 0)
			(layer "B.SilkS")
		)
		(property "Value" "100"
			(at 0 -1.65 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 180)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902)
			(net 152 "Net-(U7-VB)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 180)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902)
			(net 155 "Net-(U7-VC)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "B.Cu")
		(at 196.85 77.9 90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C18"
			(at 3.732 0.381 270)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "1uF"
			(at 0 -1.68 90)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0 90)
			(size 1 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 181 "Net-(U7-YI)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0 90)
			(size 1 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 184 "Net-(C18-Pad2)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "B.Cu")
		(at 229.997 109.093 180)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP40"
			(at 0 1.448 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 -1.55 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 1.45 0)
			(layer "B.Fab")
		)
		(pad "1" smd circle
			(at 0 0 180)
			(size 1 1)
			(layers "B.Cu" "B.Mask")
			(net 137 "/VDB1")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "B.Cu")
		(at 137.668 99.568 180)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP63"
			(at 0 1.448 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 -1.55 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 1.45 0)
			(layer "B.Fab")
		)
		(pad "1" smd circle
			(at 0 0 180)
			(size 1 1)
			(layers "B.Cu" "B.Mask")
			(net 240 "Net-(U13-P57)")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "B.Cu")
		(at 189.5 191.85 90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C1"
			(at 3.109 0.254 270)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "47pF"
			(at 0 -1.68 90)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0 90)
			(size 1 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 127 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0 90)
			(size 1 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 291 "Net-(C1-Pad2)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_SMD:SC-59"
		(layer "B.Cu")
		(at 169.55 148.8 180)
		(descr "SC-59, https://lib.chipdip.ru/images/import_diod/original/SOT-23_SC-59.jpg")
		(tags "SC-59")
		(property "Reference" "Q8"
			(at 7.55 1.8 0)
			(layer "B.SilkS")
		)
		(property "Value" "C2412K"
			(at 0 -2.5 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "NPN transistor, base/emitter/collector"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.2 0.95 180)
			(size 0.9 0.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 386 "Net-(Q8-B)")
			(pinfunction "B")
			(pintype "input")
		)
		(pad "2" smd roundrect
			(at -1.2 -0.95 180)
			(size 0.9 0.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 385 "Net-(Q8-E)")
			(pinfunction "E")
			(pintype "passive")
		)
		(pad "3" smd roundrect
			(at 1.2 0 180)
			(size 0.9 0.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 72 "VCC")
			(pinfunction "C")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SC-59.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "B.Cu")
		(at 87.945 132.842 180)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C51"
			(at 3.845 0.942 0)
			(layer "B.SilkS")
		)
		(property "Value" "47pF"
			(at 0 -1.68 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0 180)
			(size 1 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 289 "Net-(P4-Audio-L)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0 180)
			(size 1 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 127 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "B.Cu")
		(at 194.818 99.949 180)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP60"
			(at 0 1.448 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 -1.55 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 1.45 0)
			(layer "B.Fab")
		)
		(pad "1" smd circle
			(at 0 0 180)
			(size 1 1)
			(layers "B.Cu" "B.Mask")
			(net 149 "/VDA5")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "B.Cu")
		(at 231 137.8 180)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP33"
			(at 0 1.448 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 -1.55 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 1.45 0)
			(layer "B.Fab")
		)
		(pad "1" smd circle
			(at 0 0 180)
			(size 1 1)
			(layers "B.Cu" "B.Mask")
			(net 129 "Net-(P2-Pin_4)")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "B.Cu")
		(at 105.41 129.474 90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C100"
			(at 0.188 2.032 270)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "0.1µF"
			(at 0 -1.68 90)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0 90)
			(size 1 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 127 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0 90)
			(size 1 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 72 "VCC")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "B.Cu")
		(at 231.1 142.9 180)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP32"
			(at 0 1.448 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 -1.55 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 1.45 0)
			(layer "B.Fab")
		)
		(pad "1" smd circle
			(at 0 0 180)
			(size 1 1)
			(layers "B.Cu" "B.Mask")
			(net 126 "Net-(P2-Pin_2)")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "B.Cu")
		(at 119.761 99.187 180)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP91"
			(at 0 1.448 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 -1.55 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 1.45 180)
			(layer "B.Fab")
		)
		(pad "1" smd circle
			(at 0 0 180)
			(size 1 1)
			(layers "B.Cu" "B.Mask")
			(net 215 "Net-(U14-XTAL1)")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "Package_TO_SOT_SMD:SC-59"
		(layer "B.Cu")
		(at 92.399 130.368 180)
		(descr "SC-59, https://lib.chipdip.ru/images/import_diod/original/SOT-23_SC-59.jpg")
		(tags "SC-59")
		(property "Reference" "DA15"
			(at -0.057 7.94 0)
			(layer "B.SilkS")
		)
		(property "Value" "DAN202"
			(at 0 -2.5 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Dual diode, common cathode on pin 3"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.2 0.95 180)
			(size 0.9 0.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 127 "GND")
			(pinfunction "A")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at -1.2 -0.95 180)
			(size 0.9 0.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 172 "Net-(DA15-A-Pad2)")
			(pinfunction "A")
			(pintype "passive")
		)
		(pad "3" smd roundrect
			(at 1.2 0 180)
			(size 0.9 0.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 168 "Net-(DA15-K)")
			(pinfunction "K")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SC-59.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "B.Cu")
		(at 233.619 140.335)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C36"
			(at 4.13 0 0)
			(layer "B.SilkS")
		)
		(property "Value" "330pF"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0)
			(size 1 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 128 "Net-(P2-Pin_3)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0)
			(size 1 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 127 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "B.Cu")
		(at 223.3 151.9)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C89"
			(at -6.35 0.25 0)
			(layer "B.SilkS")
		)
		(property "Value" "0.1µF"
			(at 0 -1.68 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0)
			(size 1 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 127 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0)
			(size 1 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 72 "VCC")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "B.Cu")
		(at 159.385 191.516 180)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP83"
			(at 0 1.448 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 -1.55 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 1.45 0)
			(layer "B.Fab")
		)
		(pad "1" smd circle
			(at 0 0 180)
			(size 1 1)
			(layers "B.Cu" "B.Mask")
			(net 7 "/CA12")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "Package_TO_SOT_SMD:SC-59"
		(layer "B.Cu")
		(at 95.828 154.879 180)
		(descr "SC-59, https://lib.chipdip.ru/images/import_diod/original/SOT-23_SC-59.jpg")
		(tags "SC-59")
		(property "Reference" "DA13"
			(at 1.975 -5.649 0)
			(layer "B.SilkS")
		)
		(property "Value" "DAN202"
			(at 0 -2.5 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Dual diode, common cathode on pin 3"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.2 0.95 180)
			(size 0.9 0.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 127 "GND")
			(pinfunction "A")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at -1.2 -0.95 180)
			(size 0.9 0.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 404 "Net-(DA13-A-Pad2)")
			(pinfunction "A")
			(pintype "passive")
		)
		(pad "3" smd roundrect
			(at 1.2 0 180)
			(size 0.9 0.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 401 "Net-(DA13-K)")
			(pinfunction "K")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SC-59.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_SMD:SC-59"
		(layer "B.Cu")
		(at 227.273 158.943 180)
		(descr "SC-59, https://lib.chipdip.ru/images/import_diod/original/SOT-23_SC-59.jpg")
		(tags "SC-59")
		(property "Reference" "DA7"
			(at -10.979 5.527 0)
			(layer "B.SilkS")
		)
		(property "Value" "DAN202"
			(at 0 -2.5 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Dual diode, common anode on pin 1"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.2 0.95 180)
			(size 0.9 0.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 274 "/JPCLK2")
			(pinfunction "A")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at -1.2 -0.95 180)
			(size 0.9 0.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 277 "/JPCLK1")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "3" smd roundrect
			(at 1.2 0 180)
			(size 0.9 0.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 72 "VCC")
			(pinfunction "K")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SC-59.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "B.Cu")
		(at 189.611 110.998 180)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP49"
			(at 0 1.448 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 -1.55 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 1.45 0)
			(layer "B.Fab")
		)
		(pad "1" smd circle
			(at 0 0 180)
			(size 1 1)
			(layers "B.Cu" "B.Mask")
			(net 108 "/VAA2")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "B.Cu")
		(at 231 127.7 180)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP35"
			(at 0 1.448 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 -1.55 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 1.45 0)
			(layer "B.Fab")
		)
		(pad "1" smd circle
			(at 0 0 180)
			(size 1 1)
			(layers "B.Cu" "B.Mask")
			(net 133 "Net-(P2-Pin_8)")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "B.Cu")
		(at 115.1 142.1125 -90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R104"
			(at -9.7125 -0.4 270)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "22k"
			(at 0 -1.65 90)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 270)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902)
			(net 335 "Net-(C78-Pad2)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 270)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902)
			(net 283 "Net-(C77-Pad2)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "B.Cu")
		(at 233.619 122.555)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C43"
			(at 0 -1.905 0)
			(layer "B.SilkS")
		)
		(property "Value" "330pF"
			(at 0 0.625 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0)
			(size 1 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 135 "Net-(P2-Pin_10)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0)
			(size 1 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 127 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "B.Cu")
		(at 223.3125 154.5)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R75"
			(at -3.8625 0.6 0)
			(layer "B.SilkS")
		)
		(property "Value" "100k"
			(at 0 -1.65 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902)
			(net 77 "{slash}RESOUT1")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902)
			(net 72 "VCC")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "B.Cu")
		(at 231 122.7 180)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP36"
			(at 0 1.448 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 -1.55 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 1.45 0)
			(layer "B.Fab")
		)
		(pad "1" smd circle
			(at 0 0 180)
			(size 1 1)
			(layers "B.Cu" "B.Mask")
			(net 135 "Net-(P2-Pin_10)")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "B.Cu")
		(at 102.87 161.478 -90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C28"
			(at 3.749 1.397 270)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "1uF"
			(at 0 -1.68 90)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0 270)
			(size 1 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 348 "Net-(C28-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0 270)
			(size 1 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 315 "Net-(P1-SOUND-L)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_SMD:SC-59"
		(layer "B.Cu")
		(at 178.05 146.7 180)
		(descr "SC-59, https://lib.chipdip.ru/images/import_diod/original/SOT-23_SC-59.jpg")
		(tags "SC-59")
		(property "Reference" "Q7"
			(at -3.814 0.904 0)
			(layer "B.SilkS")
		)
		(property "Value" "C2412K"
			(at 0 -2.5 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "NPN transistor, base/emitter/collector"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.2 0.95 180)
			(size 0.9 0.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 384 "Net-(Q7-B)")
			(pinfunction "B")
			(pintype "input")
		)
		(pad "2" smd roundrect
			(at -1.2 -0.95 180)
			(size 0.9 0.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 383 "Net-(Q7-E)")
			(pinfunction "E")
			(pintype "passive")
		)
		(pad "3" smd roundrect
			(at 1.2 0 180)
			(size 0.9 0.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 127 "GND")
			(pinfunction "C")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SC-59.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "B.Cu")
		(at 214.63 97.409 180)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP101"
			(at 0 1.448 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 -1.55 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 1.45 180)
			(layer "B.Fab")
		)
		(pad "1" smd circle
			(at 0 0 180)
			(size 1 1)
			(layers "B.Cu" "B.Mask")
			(net 87 "/VAB8")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "B.Cu")
		(at 133.1995 143.764 180)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R67"
			(at -8.5325 -0.254 0)
			(layer "B.SilkS")
		)
		(property "Value" "1k"
			(at 0 -1.65 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 180)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902)
			(net 395 "Net-(C65-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 180)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902)
			(net 372 "Net-(Q16-E)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "B.Cu")
		(at 160.782 183.134 180)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP74"
			(at 0 1.448 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 -1.55 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 1.45 0)
			(layer "B.Fab")
		)
		(pad "1" smd circle
			(at 0 0 180)
			(size 1 1)
			(layers "B.Cu" "B.Mask")
			(net 16 "/CA21")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "B.Cu")
		(at 233.619 142.875)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C35"
			(at 4.13 0 0)
			(layer "B.SilkS")
		)
		(property "Value" "330pF"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0)
			(size 1 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 126 "Net-(P2-Pin_2)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0)
			(size 1 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 127 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "B.Cu")
		(at 212.217 107.95 180)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP105"
			(at 0 1.448 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 -1.55 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 1.45 180)
			(layer "B.Fab")
		)
		(pad "1" smd circle
			(at 0 0 180)
			(size 1 1)
			(layers "B.Cu" "B.Mask")
			(net 83 "/VAB12")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "B.Cu")
		(at 185.9 81.8875 -90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R38"
			(at 0.4085 -2.314 270)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "470"
			(at 0 -1.65 90)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 270)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902)
			(net 178 "Net-(Q11-B)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 270)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902)
			(net 363 "Net-(U7-YO)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "B.Cu")
		(at 106.3875 146.4 180)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R99"
			(at 1.9935 4.414 0)
			(layer "B.SilkS")
		)
		(property "Value" "22k"
			(at 0 -1.65 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 180)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902)
			(net 220 "Net-(C74-Pad2)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 180)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902)
			(net 331 "Net-(U17-R.OUT)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "B.Cu")
		(at 232.537 108.458 180)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP41"
			(at 0 1.448 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 -1.55 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 1.45 0)
			(layer "B.Fab")
		)
		(pad "1" smd circle
			(at 0 0 180)
			(size 1 1)
			(layers "B.Cu" "B.Mask")
			(net 138 "/VDB2")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "B.Cu")
		(at 83.632 176.784 180)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C22"
			(at -0.061 -2.54 0)
			(layer "B.SilkS")
		)
		(property "Value" "330pF"
			(at 0 -1.68 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0 180)
			(size 1 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 78 "Net-(J2-Audio)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0 180)
			(size 1 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 127 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "B.Cu")
		(at 180.6 86.6 180)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C14"
			(at 4.9 -0.6 0)
			(layer "B.SilkS")
		)
		(property "Value" "1uF"
			(at 0 -1.68 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0 180)
			(size 1 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 173 "Net-(C13-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0 180)
			(size 1 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 174 "Net-(U7-(B-Y)I)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "B.Cu")
		(at 107.1 143.25 -90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C74"
			(at -3.677 1.055 270)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "1nF"
			(at 0 -1.68 90)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0 270)
			(size 1 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 127 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0 270)
			(size 1 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 220 "Net-(C74-Pad2)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "B.Cu")
		(at 200.787 175.26 180)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP87"
			(at 0 1.448 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 -1.55 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 1.45 0)
			(layer "B.Fab")
		)
		(pad "1" smd circle
			(at 0 0 180)
			(size 1 1)
			(layers "B.Cu" "B.Mask")
			(net 3 "/CA8")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "B.Cu")
		(at 100.7 104.1 180)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP17"
			(at 0 1.448 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 -1.55 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 1.45 0)
			(layer "B.Fab")
		)
		(pad "1" smd circle
			(at 0 0 180)
			(size 1 1)
			(layers "B.Cu" "B.Mask")
			(net 313 "/PA6")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "B.Cu")
		(at 122.5 158.6 -90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C54"
			(at -3.533 0.199 270)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "1uF"
			(at 0 -1.68 90)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0 270)
			(size 1 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 351 "Net-(Q15-B)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0 270)
			(size 1 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 127 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "B.Cu")
		(at 199.009 179.832 180)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP76"
			(at 0 1.448 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 -1.55 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 1.45 0)
			(layer "B.Fab")
		)
		(pad "1" smd circle
			(at 0 0 180)
			(size 1 1)
			(layers "B.Cu" "B.Mask")
			(net 14 "/CA19")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "B.Cu")
		(at 214.757 108.077 180)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP99"
			(at 0 1.448 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 -1.55 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 1.45 180)
			(layer "B.Fab")
		)
		(pad "1" smd circle
			(at 0 0 180)
			(size 1 1)
			(layers "B.Cu" "B.Mask")
			(net 90 "/VAB6")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "B.Cu")
		(at 117.094 191.45 90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C33"
			(at 4.125 -0.127 270)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "0.1µF"
			(at 0 -1.68 90)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0 90)
			(size 1 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 303 "Net-(DA11-K)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0 90)
			(size 1 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 127 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "B.Cu")
		(at 191.05 77.8625 -90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R41"
			(at -3.5675 -0.212 270)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "39"
			(at 0 -1.65 90)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "nonSNES.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 270)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902)
			(net 127 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 270)
			(size 1.025 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.243902)
			(net 184 "Net-(C18-Pad2)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(gr_line
		(start 251.46 163.4744)
		(end 251.46 170.2308)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 171.45 69.977)
		(end 172.339 69.977)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 183.769 69.215)
		(end 183.769 53.34)
		(layer "Edge.Cuts")
	)
	(gr_circle
		(center 241.808 83.312)
		(end 241.808 81.788)
		(fill no)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 126.365 58.42)
		(end 126.365 53.34)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 251.46 53.34)
		(end 251.46 92.4052)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 245.745 208.28)
		(end 245.745 207.01)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 167.259 53.34)
		(end 167.259 69.977)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 104.14 212.344)
		(end 104.14 205.74)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 226.06 196.85)
		(end 236.22 196.85)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 78.105 55.88)
		(mid 80.01 57.785)
		(end 78.105 59.69)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 104.14 205.74)
		(end 114.3 205.74)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 145.415 53.34)
		(end 145.415 66.04)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 182.118 69.977)
		(mid 181.737 69.596)
		(end 182.118 69.215)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 251.46 163.4744)
		(mid 252.095 162.8394)
		(end 252.73 163.4744)
		(layer "Edge.Cuts")
	)
	(gr_rect
		(start 269.6718 156.5402)
		(end 273.1262 165.3286)
		(fill no)
		(layer "Edge.Cuts")
	)
	(gr_circle
		(center 241.935 182.88)
		(end 241.935 181.61)
		(fill no)
		(layer "Edge.Cuts")
	)
	(gr_rect
		(start 258.7498 98.0694)
		(end 262.2042 106.8578)
		(fill no)
		(layer "Edge.Cuts")
	)
	(gr_circle
		(center 137.16 198.755)
		(end 137.16 197.485)
		(fill no)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 184.531 69.977)
		(end 182.118 69.977)
		(layer "Edge.Cuts")
	)
	(gr_circle
		(center 136.525 67.31)
		(end 136.525 66.04)
		(fill no)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 72.39 60.96)
		(end 72.39 53.34)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 168.021 53.34)
		(end 168.021 69.215)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 277.241 181.6354)
		(end 277.241 186.563)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 252.73 103.9876)
		(end 252.73 97.2312)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 252.73 92.4052)
		(mid 252.095 93.0402)
		(end 251.46 92.4052)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 172.339 69.215)
		(mid 172.72 69.596)
		(end 172.339 69.977)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 72.39 53.34)
		(end 116.205 53.34)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 76.2 59.69)
		(end 78.105 59.69)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 172.339 69.215)
		(end 171.45 69.215)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 251.46 174.8028)
		(mid 252.095 174.1678)
		(end 252.73 174.8028)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 126.365 53.34)
		(end 145.415 53.34)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 175.006 69.215)
		(end 174.117 69.215)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 76.2 59.69)
		(mid 74.295 57.785)
		(end 76.2 55.88)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 169.672 69.215)
		(mid 170.053 69.596)
		(end 169.672 69.977)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 176.784 69.977)
		(mid 176.403 69.596)
		(end 176.784 69.215)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 168.021 53.34)
		(end 183.769 53.34)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 63.5 110.49)
		(end 63.5 60.96)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 146.05 198.12)
		(end 156.21 198.12)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 252.73 170.2308)
		(mid 252.095 170.8658)
		(end 251.46 170.2308)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 252.73 80.645)
		(end 252.73 92.4052)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 168.91 201.93)
		(end 182.88 201.93)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 63.5 120.65)
		(end 69.85 120.65)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 174.117 69.977)
		(end 175.006 69.977)
		(layer "Edge.Cuts")
	)
	(gr_circle
		(center 137.16 208.915)
		(end 137.16 207.645)
		(fill no)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 104.14 212.344)
		(end 78.74 212.344)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 179.451 69.977)
		(mid 179.07 69.596)
		(end 179.451 69.215)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 179.451 69.977)
		(end 180.34 69.977)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 251.46 97.2312)
		(end 251.46 103.9876)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 184.531 53.34)
		(end 251.46 53.34)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 168.021 69.215)
		(end 169.672 69.215)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 252.73 103.9876)
		(mid 252.095 104.6226)
		(end 251.46 103.9876)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 252.73 158.5468)
		(mid 252.095 159.1818)
		(end 251.46 158.5468)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 145.415 66.04)
		(end 155.575 66.04)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 174.117 69.977)
		(mid 173.736 69.596)
		(end 174.117 69.215)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 78.74 212.344)
		(end 78.74 204.47)
		(layer "Edge.Cuts")
	)
	(gr_circle
		(center 241.808 88.138)
		(end 241.808 88.9)
		(fill no)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 251.46 212.344)
		(end 251.46 174.8028)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 277.241 175.2854)
		(end 277.241 169.9006)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 226.06 212.344)
		(end 226.06 196.85)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 176.784 69.977)
		(end 177.673 69.977)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 191.77 212.344)
		(end 191.77 196.85)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 252.73 80.645)
		(end 279.2222 80.645)
		(layer "Edge.Cuts")
	)
	(gr_circle
		(center 211.709 200.025)
		(end 211.709 198.12)
		(fill no)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 248.285 208.28)
		(mid 247.015 209.55)
		(end 245.745 208.28)
		(layer "Edge.Cuts")
	)
	(gr_rect
		(start 258.7498 151.3586)
		(end 262.2042 160.147)
		(fill no)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 177.673 69.215)
		(end 176.784 69.215)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 171.45 69.977)
		(mid 171.069 69.596)
		(end 171.45 69.215)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 201.93 212.344)
		(end 226.06 212.344)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 156.21 212.344)
		(end 168.91 212.344)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 63.5 204.47)
		(end 78.74 204.47)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 277.241 175.2854)
		(end 270.4338 175.2854)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 248.285 207.01)
		(end 248.285 208.28)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 270.4338 175.2854)
		(end 270.4338 181.6354)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 245.745 207.01)
		(mid 247.015 205.74)
		(end 248.285 207.01)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 156.21 198.12)
		(end 156.21 212.344)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 184.531 69.977)
		(end 184.531 53.34)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 236.22 212.344)
		(end 251.46 212.344)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 180.34 69.215)
		(end 179.451 69.215)
		(layer "Edge.Cuts")
	)
	(gr_rect
		(start 269.5702 92.9894)
		(end 273.0246 101.7778)
		(fill no)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 277.241 186.563)
		(end 252.73 186.563)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 168.91 201.93)
		(end 168.91 212.344)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 251.46 97.2312)
		(mid 252.095 96.5962)
		(end 252.73 97.2312)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 182.118 69.215)
		(end 183.769 69.215)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 270.4338 181.6354)
		(end 277.241 181.6354)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 182.88 212.344)
		(end 191.77 212.344)
		(layer "Edge.Cuts")
	)
	(gr_circle
		(center 206.375 66.04)
		(end 206.375 64.135)
		(fill no)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 201.93 196.85)
		(end 201.93 212.344)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 69.85 110.49)
		(end 63.5 110.49)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 175.006 69.215)
		(mid 175.387 69.596)
		(end 175.006 69.977)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 177.673 69.215)
		(mid 178.054 69.596)
		(end 177.673 69.977)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 78.105 55.88)
		(end 76.2 55.88)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 251.46 108.6104)
		(mid 252.095 107.9754)
		(end 252.73 108.6104)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 116.205 58.42)
		(end 126.365 58.42)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 155.575 66.04)
		(end 155.575 53.34)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 252.73 170.2308)
		(end 252.73 163.4744)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 63.5 60.96)
		(end 72.39 60.96)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 180.34 69.215)
		(mid 180.721 69.596)
		(end 180.34 69.977)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 277.241 169.9006)
		(end 279.273 169.9006)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 169.672 69.977)
		(end 167.259 69.977)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 182.88 201.93)
		(end 182.88 212.344)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 251.46 108.6104)
		(end 251.46 158.5468)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 69.85 120.65)
		(end 69.85 110.49)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 63.5 204.47)
		(end 63.5 120.65)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 114.3 212.344)
		(end 146.05 212.344)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 116.205 53.34)
		(end 116.205 58.42)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 252.73 186.563)
		(end 252.73 174.8028)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 155.575 53.34)
		(end 167.259 53.34)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 236.22 196.85)
		(end 236.22 212.344)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 146.05 212.344)
		(end 146.05 198.12)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 279.2222 80.645)
		(end 279.273 169.9006)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 252.73 158.5468)
		(end 252.73 108.6104)
		(layer "Edge.Cuts")
	)
	(gr_circle
		(center 73.025 127)
		(end 73.025 125.095)
		(fill no)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 114.3 205.74)
		(end 114.3 212.344)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 191.77 196.85)
		(end 201.93 196.85)
		(layer "Edge.Cuts")
	)
	(gr_text "SNSP"
		(at 254.2794 151.511 -90)
		(layer "F.Cu")
	)
	(gr_text "SNSP"
		(at 253.9492 161.0106 -90)
		(layer "B.Cu")
	)
	(gr_text "黒"
		(at 107.95 201.93 0)
		(layer "F.SilkS")
	)
	(gr_text "©"
		(at 169.545 76.2 0)
		(layer "F.SilkS")
	)
	(gr_text "41-0492A"
		(at 277.2156 109.855 -90)
		(layer "F.SilkS")
	)
	(gr_text "n"
		(at 187.96 76.2 0)
		(layer "F.SilkS")
	)
	(gr_text "1992"
		(at 174.625 76.2 0)
		(layer "F.SilkS")
	)
	(gr_text "SNSP-CPU-01"
		(at 181.61 78.105 0)
		(layer "F.SilkS")
	)
	(gr_text "https://github.com/stonedDiscord/nonSNES"
		(at 150.5712 113.2332 -90)
		(layer "F.SilkS")
	)
	(gr_text "n"
		(at 195.58 76.2 0)
		(layer "F.SilkS")
	)
	(gr_text "MITSU"
		(at 277.1648 82.8802 -90)
		(layer "F.SilkS")
	)
	(gr_text "o"
		(at 201.93 76.2 0)
		(layer "F.SilkS")
	)
	(gr_text "N"
		(at 182.88 76.2 0)
		(layer "F.SilkS")
	)
	(gr_text "赤"
		(at 97.79 201.93 0)
		(layer "F.SilkS")
	)
	(gr_text "CO"
		(at 277.114 98.8314 -90)
		(layer "F.SilkS")
	)
	(gr_text "R51-1640"
		(at 277.0124 154.305 -90)
		(layer "F.SilkS")
	)
	(gr_text "CCK-N15"
		(at 276.9616 143.5354 -90)
		(layer "F.SilkS")
	)
	(gr_text "HCMK-81X 92.2"
		(at 252.7808 85.0138 -90)
		(layer "F.SilkS")
	)
	(gr_text "O"
		(at 120.65 205.105 0)
		(layer "B.SilkS")
	)
	(gr_text "G"
		(at 118.11 205.105 0)
		(layer "B.SilkS")
	)
	(gr_text "I"
		(at 114.808 205.105 0)
		(layer "B.SilkS")
	)
	(dimension
		(type aligned)
		(layer "User.1")
		(pts
			(xy 236.22 212.09) (xy 251.46 212.09)
		)
		(height 11.43)
		(format
			(prefix "")
			(suffix "")
			(units 3)
			(units_format 1)
			(precision 4)
		)
		(style
			(thickness 0.1)
			(arrow_length 1.27)
			(text_position_mode 0)
			(arrow_direction outward)
			(extension_height 0.58642)
			(extension_offset 0.5)
			(keep_text_aligned yes)
		)
		(gr_text "15.2400 mm"
			(at 243.84 222.07 0)
			(layer "User.1")
		)
	)
	(dimension
		(type aligned)
		(layer "User.1")
		(pts
			(xy 63.5 60.96) (xy 72.39 60.96)
		)
		(height -13.97)
		(format
			(prefix "")
			(suffix "")
			(units 3)
			(units_format 1)
			(precision 4)
		)
		(style
			(thickness 0.1)
			(arrow_length 1.27)
			(text_position_mode 0)
			(arrow_direction outward)
			(extension_height 0.58642)
			(extension_offset 0.5)
			(keep_text_aligned yes)
		)
		(gr_text "8.8900 mm"
			(at 67.945 45.54 0)
			(layer "User.1")
		)
	)
	(dimension
		(type aligned)
		(layer "User.1")
		(pts
			(xy 104.14 212.09) (xy 78.74 212.09)
		)
		(height -11.43)
		(format
			(prefix "")
			(suffix "")
			(units 3)
			(units_format 1)
			(precision 4)
		)
		(style
			(thickness 0.1)
			(arrow_length 1.27)
			(text_position_mode 0)
			(arrow_direction outward)
			(extension_height 0.58642)
			(extension_offset 0.5)
			(keep_text_aligned yes)
		)
		(gr_text "25.4000 mm"
			(at 91.44 222.07 0)
			(layer "User.1")
		)
	)
	(dimension
		(type aligned)
		(layer "User.1")
		(pts
			(xy 145.415 66.04) (xy 155.575 66.04)
		)
		(height -19.05)
		(format
			(prefix "")
			(suffix "")
			(units 3)
			(units_format 1)
			(precision 4)
		)
		(style
			(thickness 0.1)
			(arrow_length 1.27)
			(text_position_mode 0)
			(arrow_direction outward)
			(extension_height 0.58642)
			(extension_offset 0.5)
			(keep_text_aligned yes)
		)
		(gr_text "10.1600 mm"
			(at 150.495 45.54 0)
			(layer "User.1")
		)
	)
	(dimension
		(type aligned)
		(layer "User.1")
		(pts
			(xy 63.5 110.49) (xy 63.5 60.96)
		)
		(height -5.08)
		(format
			(prefix "")
			(suffix "")
			(units 3)
			(units_format 1)
			(precision 4)
		)
		(style
			(thickness 0.1)
			(arrow_length 1.27)
			(text_position_mode 0)
			(arrow_direction outward)
			(extension_height 0.58642)
			(extension_offset 0.5)
			(keep_text_aligned yes)
		)
		(gr_text "49.5300 mm"
			(at 56.97 85.725 90)
			(layer "User.1")
		)
	)
	(dimension
		(type aligned)
		(layer "User.1")
		(pts
			(xy 72.39 53.34) (xy 116.205 53.34)
		)
		(height -6.35)
		(format
			(prefix "")
			(suffix "")
			(units 3)
			(units_format 1)
			(precision 4)
		)
		(style
			(thickness 0.1)
			(arrow_length 1.27)
			(text_position_mode 0)
			(arrow_direction outward)
			(extension_height 0.58642)
			(extension_offset 0.5)
			(keep_text_aligned yes)
		)
		(gr_text "43.8150 mm"
			(at 94.2975 45.54 0)
			(layer "User.1")
		)
	)
	(dimension
		(type aligned)
		(layer "User.1")
		(pts
			(xy 146.05 212.09) (xy 114.3 212.09)
		)
		(height -11.43)
		(format
			(prefix "")
			(suffix "")
			(units 3)
			(units_format 1)
			(precision 4)
		)
		(style
			(thickness 0.1)
			(arrow_length 1.27)
			(text_position_mode 0)
			(arrow_direction outward)
			(extension_height 0.58642)
			(extension_offset 0.5)
			(keep_text_aligned yes)
		)
		(gr_text "31.7500 mm"
			(at 130.175 222.07 0)
			(layer "User.1")
		)
	)
	(dimension
		(type aligned)
		(layer "User.1")
		(pts
			(xy 191.77 196.85) (xy 201.93 196.85)
		)
		(height 26.67)
		(format
			(prefix "")
			(suffix "")
			(units 3)
			(units_format 1)
			(precision 4)
		)
		(style
			(thickness 0.1)
			(arrow_length 1.27)
			(text_position_mode 0)
			(arrow_direction outward)
			(extension_height 0.58642)
			(extension_offset 0.5)
			(keep_text_aligned yes)
		)
		(gr_text "10.1600 mm"
			(at 196.85 222.07 0)
			(layer "User.1")
		)
	)
	(dimension
		(type aligned)
		(layer "User.1")
		(pts
			(xy 168.91 201.93) (xy 182.88 201.93)
		)
		(height 21.59)
		(format
			(prefix "")
			(suffix "")
			(units 3)
			(units_format 1)
			(precision 4)
		)
		(style
			(thickness 0.1)
			(arrow_length 1.27)
			(text_position_mode 0)
			(arrow_direction outward)
			(extension_height 0.58642)
			(extension_offset 0.5)
			(keep_text_aligned yes)
		)
		(gr_text "13.9700 mm"
			(at 175.895 222.07 0)
			(layer "User.1")
		)
	)
	(dimension
		(type aligned)
		(layer "User.1")
		(pts
			(xy 146.05 212.09) (xy 146.05 198.12)
		)
		(height -1.27)
		(format
			(prefix "")
			(suffix "")
			(units 3)
			(units_format 1)
			(precision 4)
		)
		(style
			(thickness 0.1)
			(arrow_length 1.27)
			(text_position_mode 2)
			(arrow_direction outward)
			(extension_height 0.58642)
			(extension_offset 0.5)
			(keep_text_aligned yes)
		)
		(gr_text "13.9700 mm"
			(at 142.24 205.105 90)
			(layer "User.1")
		)
	)
	(dimension
		(type aligned)
		(layer "User.1")
		(pts
			(xy 116.205 58.42) (xy 126.365 58.42)
		)
		(height -11.43)
		(format
			(prefix "")
			(suffix "")
			(units 3)
			(units_format 1)
			(precision 4)
		)
		(style
			(thickness 0.1)
			(arrow_length 1.27)
			(text_position_mode 0)
			(arrow_direction outward)
			(extension_height 0.58642)
			(extension_offset 0.5)
			(keep_text_aligned yes)
		)
		(gr_text "10.1600 mm"
			(at 121.285 45.54 0)
			(layer "User.1")
		)
	)
	(dimension
		(type aligned)
		(layer "User.1")
		(pts
			(xy 78.74 212.09) (xy 78.74 204.47)
		)
		(height 2.54)
		(format
			(prefix "")
			(suffix "")
			(units 3)
			(units_format 1)
			(precision 4)
		)
		(style
			(thickness 0.1)
			(arrow_length 1.27)
			(text_position_mode 0)
			(arrow_direction outward)
			(extension_height 0.58642)
			(extension_offset 0.5)
			(keep_text_aligned yes)
		)
		(gr_text "7.6200 mm"
			(at 79.83 208.28 90)
			(layer "User.1")
		)
	)
	(dimension
		(type aligned)
		(layer "User.1")
		(pts
			(xy 69.85 120.65) (xy 69.85 110.49)
		)
		(height -11.43)
		(format
			(prefix "")
			(suffix "")
			(units 3)
			(units_format 1)
			(precision 4)
		)
		(style
			(thickness 0.1)
			(arrow_length 1.27)
			(text_position_mode 0)
			(arrow_direction outward)
			(extension_height 0.58642)
			(extension_offset 0.5)
			(keep_text_aligned yes)
		)
		(gr_text "10.1600 mm"
			(at 56.97 115.57 90)
			(layer "User.1")
		)
	)
	(dimension
		(type aligned)
		(layer "User.1")
		(pts
			(xy 72.39 60.96) (xy 72.39 53.34)
		)
		(height -13.97)
		(format
			(prefix "")
			(suffix "")
			(units 3)
			(units_format 1)
			(precision 4)
		)
		(style
			(thickness 0.1)
			(arrow_length 1.27)
			(text_position_mode 0)
			(arrow_direction outward)
			(extension_height 0.58642)
			(extension_offset 0.5)
			(keep_text_aligned yes)
		)
		(gr_text "7.6200 mm"
			(at 56.97 57.15 90)
			(layer "User.1")
		)
	)
	(dimension
		(type aligned)
		(layer "User.1")
		(pts
			(xy 155.575 53.34) (xy 168.275 53.34)
		)
		(height -6.35)
		(format
			(prefix "")
			(suffix "")
			(units 3)
			(units_format 1)
			(precision 4)
		)
		(style
			(thickness 0.1)
			(arrow_length 1.27)
			(text_position_mode 0)
			(arrow_direction outward)
			(extension_height 0.58642)
			(extension_offset 0.5)
			(keep_text_aligned yes)
		)
		(gr_text "12.7000 mm"
			(at 161.925 45.54 0)
			(layer "User.1")
		)
	)
	(dimension
		(type aligned)
		(layer "User.1")
		(pts
			(xy 191.77 212.09) (xy 191.77 196.85)
		)
		(height 13.97)
		(format
			(prefix "")
			(suffix "")
			(units 3)
			(units_format 1)
			(precision 4)
		)
		(style
			(thickness 0.1)
			(arrow_length 1.27)
			(text_position_mode 2)
			(arrow_direction outward)
			(extension_height 0.58642)
			(extension_offset 0.5)
			(keep_text_aligned yes)
		)
		(gr_text "15.2400 mm"
			(at 208.28 204.47 90)
			(layer "User.1")
		)
	)
	(dimension
		(type aligned)
		(layer "User.1")
		(pts
			(xy 78.74 204.47) (xy 63.5 204.47)
		)
		(height -19.05)
		(format
			(prefix "")
			(suffix "")
			(units 3)
			(units_format 1)
			(precision 4)
		)
		(style
			(thickness 0.1)
			(arrow_length 1.27)
			(text_position_mode 0)
			(arrow_direction outward)
			(extension_height 0.58642)
			(extension_offset 0.5)
			(keep_text_aligned yes)
		)
		(gr_text "15.2400 mm"
			(at 71.12 222.07 0)
			(layer "User.1")
		)
	)
	(dimension
		(type aligned)
		(layer "User.1")
		(pts
			(xy 156.21 212.09) (xy 168.91 212.09)
		)
		(height 11.43)
		(format
			(prefix "")
			(suffix "")
			(units 3)
			(units_format 1)
			(precision 4)
		)
		(style
			(thickness 0.1)
			(arrow_length 1.27)
			(text_position_mode 0)
			(arrow_direction outward)
			(extension_height 0.58642)
			(extension_offset 0.5)
			(keep_text_aligned yes)
		)
		(gr_text "12.7000 mm"
			(at 162.56 222.07 0)
			(layer "User.1")
		)
	)
	(dimension
		(type aligned)
		(layer "User.1")
		(pts
			(xy 191.77 212.09) (xy 182.88 212.09)
		)
		(height -11.43)
		(format
			(prefix "")
			(suffix "")
			(units 3)
			(units_format 1)
			(precision 4)
		)
		(style
			(thickness 0.1)
			(arrow_length 1.27)
			(text_position_mode 0)
			(arrow_direction outward)
			(extension_height 0.58642)
			(extension_offset 0.5)
			(keep_text_aligned yes)
		)
		(gr_text "8.8900 mm"
			(at 187.325 222.07 0)
			(layer "User.1")
		)
	)
	(dimension
		(type aligned)
		(layer "User.1")
		(pts
			(xy 201.93 212.09) (xy 226.06 212.09)
		)
		(height 11.43)
		(format
			(prefix "")
			(suffix "")
			(units 3)
			(units_format 1)
			(precision 4)
		)
		(style
			(thickness 0.1)
			(arrow_length 1.27)
			(text_position_mode 0)
			(arrow_direction outward)
			(extension_height 0.58642)
			(extension_offset 0.5)
			(keep_text_aligned yes)
		)
		(gr_text "24.1300 mm"
			(at 213.995 222.07 0)
			(layer "User.1")
		)
	)
	(dimension
		(type aligned)
		(layer "User.1")
		(pts
			(xy 114.3 212.09) (xy 114.3 205.74)
		)
		(height 6.35)
		(format
			(prefix "")
			(suffix "")
			(units 3)
			(units_format 1)
			(precision 4)
		)
		(style
			(thickness 0.1)
			(arrow_length 1.27)
			(text_position_mode 0)
			(arrow_direction outward)
			(extension_height 0.58642)
			(extension_offset 0.5)
			(keep_text_aligned yes)
		)
		(gr_text "6.3500 mm"
			(at 119.2 208.915 90)
			(layer "User.1")
		)
	)
	(dimension
		(type aligned)
		(layer "User.1")
		(pts
			(xy 257.02 212.35) (xy 257.02 53.6)
		)
		(height 5.08)
		(format
			(prefix "")
			(suffix "")
			(units 3)
			(units_format 1)
			(precision 4)
		)
		(style
			(thickness 0.1)
			(arrow_length 1.27)
			(text_position_mode 0)
			(arrow_direction outward)
			(extension_height 0.58642)
			(extension_offset 0.5)
			(keep_text_aligned yes)
		)
		(gr_text "158.7500 mm"
			(at 260.65 132.975 90)
			(layer "User.1")
		)
	)
	(dimension
		(type aligned)
		(layer "User.1")
		(pts
			(xy 126.365 53.34) (xy 145.415 53.34)
		)
		(height -6.35)
		(format
			(prefix "")
			(suffix "")
			(units 3)
			(units_format 1)
			(precision 4)
		)
		(style
			(thickness 0.1)
			(arrow_length 1.27)
			(text_position_mode 0)
			(arrow_direction outward)
			(extension_height 0.58642)
			(extension_offset 0.5)
			(keep_text_aligned yes)
		)
		(gr_text "19.0500 mm"
			(at 135.89 45.54 0)
			(layer "User.1")
		)
	)
	(dimension
		(type aligned)
		(layer "User.1")
		(pts
			(xy 251.46 212.09) (xy 63.5 212.09)
		)
		(height -23.876)
		(format
			(prefix "")
			(suffix "")
			(units 3)
			(units_format 1)
			(precision 4)
		)
		(style
			(thickness 0.15)
			(arrow_length 1.27)
			(text_position_mode 0)
			(arrow_direction outward)
			(extension_height 0.58642)
			(extension_offset 0.5)
			(keep_text_aligned yes)
		)
		(gr_text "187.9600 mm"
			(at 157.48 234.516 0)
			(layer "User.1")
		)
	)
	(dimension
		(type aligned)
		(layer "User.1")
		(pts
			(xy 182.245 53.34) (xy 251.46 53.34)
		)
		(height -6.35)
		(format
			(prefix "")
			(suffix "")
			(units 3)
			(units_format 1)
			(precision 4)
		)
		(style
			(thickness 0.1)
			(arrow_length 1.27)
			(text_position_mode 0)
			(arrow_direction outward)
			(extension_height 0.58642)
			(extension_offset 0.5)
			(keep_text_aligned yes)
		)
		(gr_text "69.2150 mm"
			(at 216.8525 45.54 0)
			(layer "User.1")
		)
	)
	(dimension
		(type aligned)
		(layer "User.1")
		(pts
			(xy 58.404 118.745) (xy 58.404 202.565)
		)
		(height 5.08)
		(format
			(prefix "")
			(suffix "")
			(units 3)
			(units_format 1)
			(precision 4)
		)
		(style
			(thickness 0.1)
			(arrow_length 1.27)
			(text_position_mode 0)
			(arrow_direction outward)
			(extension_height 0.58642)
			(extension_offset 0.5)
			(keep_text_aligned yes)
		)
		(gr_text "83.8200 mm"
			(at 51.874 160.655 90)
			(layer "User.1")
		)
	)
	(dimension
		(type aligned)
		(layer "User.1")
		(pts
			(xy 226.06 196.85) (xy 236.22 196.85)
		)
		(height 26.67)
		(format
			(prefix "")
			(suffix "")
			(units 3)
			(units_format 1)
			(precision 4)
		)
		(style
			(thickness 0.1)
			(arrow_length 1.27)
			(text_position_mode 0)
			(arrow_direction outward)
			(extension_height 0.58642)
			(extension_offset 0.5)
			(keep_text_aligned yes)
		)
		(gr_text "10.1600 mm"
			(at 231.14 222.07 0)
			(layer "User.1")
		)
	)
	(dimension
		(type aligned)
		(layer "User.1")
		(pts
			(xy 114.3 205.74) (xy 104.14 205.74)
		)
		(height -17.78)
		(format
			(prefix "")
			(suffix "")
			(units 3)
			(units_format 1)
			(precision 4)
		)
		(style
			(thickness 0.1)
			(arrow_length 1.27)
			(text_position_mode 0)
			(arrow_direction outward)
			(extension_height 0.58642)
			(extension_offset 0.5)
			(keep_text_aligned yes)
		)
		(gr_text "10.1600 mm"
			(at 109.22 222.07 0)
			(layer "User.1")
		)
	)
	(dimension
		(type aligned)
		(layer "User.1")
		(pts
			(xy 156.21 198.12) (xy 146.05 198.12)
		)
		(height -25.4)
		(format
			(prefix "")
			(suffix "")
			(units 3)
			(units_format 1)
			(precision 4)
		)
		(style
			(thickness 0.1)
			(arrow_length 1.27)
			(text_position_mode 0)
			(arrow_direction outward)
			(extension_height 0.58642)
			(extension_offset 0.5)
			(keep_text_aligned yes)
		)
		(gr_text "10.1600 mm"
			(at 151.13 222.07 0)
			(layer "User.1")
		)
	)
	(dimension
		(type aligned)
		(layer "User.1")
		(pts
			(xy 168.91 212.09) (xy 168.91 201.93)
		)
		(height -1.27)
		(format
			(prefix "")
			(suffix "")
			(units 3)
			(units_format 1)
			(precision 4)
		)
		(style
			(thickness 0.1)
			(arrow_length 1.27)
			(text_position_mode 2)
			(arrow_direction outward)
			(extension_height 0.58642)
			(extension_offset 0.5)
			(keep_text_aligned yes)
		)
		(gr_text "10.1600 mm"
			(at 165.1 207.01 90)
			(layer "User.1")
		)
	)
	(zone
		(net 127)
		(net_name "GND")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 81)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 218.694 122.936) (xy 218.694 123.952) (xy 219.71 124.968) (xy 222.25 124.968) (xy 224.282 126.746)
				(xy 226.822 126.746) (xy 228.092 127.762) (xy 226.568 127.762) (xy 226.314 127.508) (xy 223.52 127.508)
				(xy 221.742 125.73) (xy 213.868 125.73) (xy 212.852 126.746) (xy 212.852 128.778) (xy 214.376 130.302)
				(xy 214.376 134.366) (xy 215.9 135.89) (xy 216.916 135.89) (xy 218.186 137.16) (xy 223.774 137.16)
				(xy 224.79 138.43) (xy 207.518 138.43) (xy 207.518 141.224) (xy 206.248 142.494) (xy 206.248 144.018)
				(xy 205.74 144.526) (xy 204.978 144.526) (xy 201.676 141.224) (xy 201.676 138.176) (xy 205.994 138.176)
				(xy 205.994 133.858) (xy 206.756 133.858) (xy 207.772 132.842) (xy 207.772 122.936)
			)
		)
	)
	(zone
		(net 72)
		(net_name "VCC")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 85)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 202.946 167.64) (xy 207.264 167.64) (xy 207.264 164.592) (xy 204.724 164.592) (xy 203.708 163.576)
				(xy 202.438 163.576) (xy 202.438 167.132)
			)
		)
	)
	(zone
		(net 127)
		(net_name "GND")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 82)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 224.536 155.194) (xy 221.488 155.194) (xy 219.964 153.67) (xy 219.964 147.828) (xy 221.996 145.796)
				(xy 231.14 145.796) (xy 233.172 147.574) (xy 236.22 147.574) (xy 236.22 155.448) (xy 234.442 153.67)
				(xy 233.426 153.67) (xy 232.664 154.432) (xy 232.664 163.322) (xy 232.156 163.83) (xy 232.156 165.862)
				(xy 231.648 166.37) (xy 231.648 168.148) (xy 231.394 168.402) (xy 231.394 173.482) (xy 230.886 173.99)
				(xy 230.124 173.99) (xy 230.124 148.082) (xy 228.854 146.812) (xy 222.504 146.812) (xy 220.98 148.336)
				(xy 220.98 149.86) (xy 221.488 150.368) (xy 222.504 150.368) (xy 222.758 150.622) (xy 224.536 150.622)
			)
		)
	)
	(zone
		(net 127)
		(net_name "GND")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 20)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 144.2 153.8) (xy 140.25 149.9) (xy 130.75 149.9) (xy 130.75 150.35) (xy 133.3 152.8) (xy 133.3 156.8)
				(xy 133.8 157.4) (xy 142.95 157.45) (xy 144.2 156.4)
			)
		)
	)
	(zone
		(net 127)
		(net_name "GND")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 41)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 212.05 171.2) (xy 212.05 175.3) (xy 212.45 175.7) (xy 213.6 175.7) (xy 214 176.1) (xy 214 176.8)
				(xy 214.65 177.5) (xy 214.65 178.8) (xy 223.6 178.8) (xy 223.6 176.6) (xy 216.05 176.6) (xy 215 175.1)
				(xy 215 170.4) (xy 220.55 165.1) (xy 224.15 165.1) (xy 224.15 162.85) (xy 218.7 162.85) (xy 218.7 164.25)
				(xy 216.8 164.25) (xy 216.8 162.9) (xy 203 162.9) (xy 204.7 164.2) (xy 207.65 164.2) (xy 207.65 167.6)
				(xy 207.35 168.05) (xy 206.05 168.05) (xy 204.85 169.35) (xy 204.2 169.35) (xy 203.55 170) (xy 203.85 170.65)
				(xy 205.5 170.65) (xy 206.2 169.9) (xy 207.05 169.9) (xy 207.5 170.35) (xy 207.5 171.2)
			)
		)
	)
	(zone
		(net 72)
		(net_name "VCC")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 43)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 222.5 189.4) (xy 228.3 189.4) (xy 228.3 186.675) (xy 228.3 183.95) (xy 222.5 183.95)
			)
		)
	)
	(zone
		(net 127)
		(net_name "GND")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 75)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 162.56 105.918) (xy 171.704 105.918) (xy 171.704 102.616) (xy 173.736 102.616) (xy 173.736 105.41)
				(xy 173.228 105.41) (xy 173.228 107.95) (xy 176.53 107.95) (xy 176.53 118.364) (xy 170.942 118.364)
				(xy 170.942 122.936) (xy 162.56 122.936)
			)
		)
	)
	(zone
		(net 303)
		(net_name "Net-(DA11-K)")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 92)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 113.538 194.056) (xy 113.538 185.166) (xy 114.3 184.404) (xy 130.556 184.404) (xy 130.556 186.436)
				(xy 124.714 186.436) (xy 124.714 188.214) (xy 114.808 188.214) (xy 114.808 194.056)
			)
		)
	)
	(zone
		(net 127)
		(net_name "GND")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 16)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 126.45 91.3) (xy 117.15 91.25) (xy 117.15 85.95) (xy 119.05 85.95) (xy 119.05 87.45) (xy 122.7 87.45)
				(xy 124.2 86) (xy 124.2 83.65) (xy 131.3 83.65) (xy 133.2 81.75) (xy 135.15 81.75) (xy 135.15 84.1)
				(xy 135.6 84.5) (xy 137.75 84.5) (xy 139.3 86) (xy 139.3 86.4) (xy 135.05 86.4) (xy 134.65 86.75)
				(xy 134.65 93.75) (xy 128.35 93.75) (xy 128.35 93.1)
			)
		)
	)
	(zone
		(net 72)
		(net_name "VCC")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 39)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 204.25 172.95) (xy 207.4 172.95) (xy 207.4 171.75) (xy 211.6 171.75) (xy 211.6 175.45) (xy 205 175.45)
				(xy 203.8 176.6) (xy 203.8 180.2) (xy 202.6 180.2) (xy 202.6 180.85) (xy 206.45 180.85) (xy 206.45 184.05)
				(xy 208.05 185.7) (xy 210.45 185.7) (xy 210.45 187.9) (xy 211.35 188.85) (xy 211.35 190.8) (xy 209.6 190.8)
				(xy 209.6 188.9) (xy 205.3 184.45) (xy 197.6 184.45) (xy 197.05 183.95) (xy 197.05 177.05) (xy 197.65 176.5)
				(xy 199.65 176.5) (xy 199.65 177.85) (xy 202.55 177.85) (xy 202.55 176.15) (xy 204.25 174.45)
			)
		)
	)
	(zone
		(net 72)
		(net_name "VCC")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 80)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 219.202 122.682) (xy 219.202 123.698) (xy 219.964 124.46) (xy 222.504 124.46) (xy 224.282 126.238)
				(xy 224.79 126.238) (xy 224.79 124.46) (xy 225.298 123.952) (xy 226.822 123.952) (xy 226.822 122.682)
			)
		)
	)
	(zone
		(net 127)
		(net_name "GND")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 1)
		(connect_pads yes
			(clearance 0.63)
		)
		(min_thickness 0.63)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.63)
			(thermal_bridge_width 0.63)
		)
		(polygon
			(pts
				(xy 78.975 212.005) (xy 96.12 212.055) (xy 96.17 200.025) (xy 111.095 200.025) (xy 111.095 198.1)
				(xy 113.1 198.1) (xy 113.1 184.45) (xy 109.35 184.45) (xy 109.35 187.2) (xy 111.5 189.45) (xy 111.5 191.1)
				(xy 110.75 191.85) (xy 106.55 191.85) (xy 106.55 193.375) (xy 92.583 193.375) (xy 92.583 188.341)
				(xy 97.409 188.341) (xy 97.409 186.055) (xy 88.065 186.055) (xy 88.065 205.67) (xy 79.025 205.62)
			)
		)
	)
	(zone
		(net 127)
		(net_name "GND")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 72)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 189.992 108.712) (xy 189.992 102.108) (xy 190.5 101.6) (xy 191.262 101.6) (xy 201.93 107.442)
				(xy 201.93 108.712) (xy 200.152 108.712) (xy 199.644 111.506) (xy 197.104 111.506) (xy 197.104 109.22)
				(xy 196.596 108.712)
			)
		)
	)
	(zone
		(net 72)
		(net_name "VCC")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 89)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 98.552 116.332) (xy 98.044 116.078) (xy 91.694 116.078) (xy 91.694 119.126) (xy 101.092 119.126)
				(xy 101.092 129.032) (xy 101.6 129.54) (xy 103.378 129.54) (xy 103.886 129.032) (xy 103.886 117.602)
				(xy 102.616 116.332)
			)
		)
	)
	(zone
		(net 72)
		(net_name "VCC")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 14)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 122.8 65.15) (xy 116.15 65.15) (xy 115.75 65.55) (xy 115.75 69.9) (xy 111.4 69.9) (xy 111.4 78.3)
				(xy 112.65 79.7) (xy 115 79.7) (xy 115 77.9) (xy 113.85 77.9) (xy 113.85 74.85) (xy 116.85 74.85)
				(xy 116.85 76.25) (xy 118.4 76.25) (xy 118.4 73.25) (xy 120.25 71.4) (xy 120.25 67.6) (xy 120.8 67.05)
				(xy 122.8 67.05)
			)
		)
	)
	(zone
		(net 72)
		(net_name "VCC")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 53)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 178.8 138.25) (xy 185.5 138.25) (xy 185.5 137.6) (xy 189.85 133.35) (xy 189.85 128.25) (xy 188.85 127.2)
				(xy 177.5 127.25) (xy 177.1 127.65) (xy 177.1 131.4) (xy 176.7 131.75) (xy 175.65 131.75) (xy 174.9 132.6)
				(xy 174.9 133) (xy 175.25 133) (xy 175.65 132.55) (xy 178.5 132.55) (xy 179.85 131.25) (xy 179.85 129.35)
				(xy 180.2 129) (xy 181.05 129) (xy 181.35 129.35) (xy 181.35 131.9) (xy 181.85 132.4) (xy 186.3 132.4)
				(xy 186.75 132.8) (xy 186.75 134.45) (xy 183.9 137.25) (xy 179.85 137.25)
			)
		)
	)
	(zone
		(net 127)
		(net_name "GND")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 78)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 174.244 86.614) (xy 178.308 86.614) (xy 178.308 84.836) (xy 179.832 83.312) (xy 181.61 83.312)
				(xy 185.166 85.09) (xy 185.166 88.138) (xy 180.34 92.71) (xy 180.34 96.774) (xy 181.102 97.536)
				(xy 182.372 97.536) (xy 184.15 95.758) (xy 184.15 92.964) (xy 189.992 92.202) (xy 189.23 91.186)
				(xy 189.23 78.994) (xy 180.848 78.994) (xy 180.848 80.264) (xy 177.292 80.264) (xy 174.244 83.312)
			)
		)
	)
	(zone
		(net 72)
		(net_name "VCC")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 12)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 99.55 79.45) (xy 99.55 65.05) (xy 96.2 65.05) (xy 96.2 70.95) (xy 97 79.5)
			)
		)
	)
	(zone
		(net 127)
		(net_name "GND")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 71)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 212.598 108.204) (xy 212.598 101.854) (xy 227.838 101.854) (xy 227.838 109.728) (xy 226.822 109.728)
				(xy 223.774 108.204)
			)
		)
	)
	(zone
		(net 72)
		(net_name "VCC")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 79)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 219.202 151.384) (xy 219.202 147.828) (xy 221.996 145.034) (xy 231.394 145.034) (xy 233.426 146.812)
				(xy 235.458 146.812) (xy 235.458 143.51) (xy 227.33 143.51) (xy 224.79 140.97) (xy 220.472 140.97)
				(xy 220.472 143.764) (xy 219.202 145.034) (xy 219.202 146.05) (xy 217.932 147.32) (xy 217.932 151.384)
			)
		)
	)
	(zone
		(net 127)
		(net_name "GND")
		(layer "F.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0.508)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 250.825 53.975) (xy 250.825 212.105) (xy 121.47 212.105) (xy 121.47 198.15) (xy 113.1 198.1)
				(xy 113.1 194.65) (xy 115.55 194.65) (xy 115.55 192) (xy 125.35 192) (xy 125.35 187) (xy 128.15 187)
				(xy 128.15 193.294) (xy 131.75 193.294) (xy 131.75 183.95) (xy 116.05 183.95) (xy 116.05 177.7)
				(xy 113.55 175.15) (xy 107.35 175.15) (xy 107.35 171.4) (xy 114.6 171.4) (xy 120.85 177.5) (xy 123.4 177.5)
				(xy 123.4 180.8) (xy 133 180.8) (xy 133 177.2) (xy 130 177.2) (xy 122 169.3) (xy 122 165.7) (xy 127.85 165.65)
				(xy 130.1 163.8) (xy 133.3 163.8) (xy 134.85 162.65) (xy 138.05 159.5) (xy 141.75 159.5) (xy 142.1 159.85)
				(xy 143.65 159.85) (xy 156.75 159.85) (xy 156.75 157.85) (xy 159.1 155.5) (xy 164.9 155.5) (xy 164.9 156.7)
				(xy 159.75 161.75) (xy 143.55 161.75) (xy 140.35 165) (xy 140.35 172.4) (xy 138.75 174) (xy 138.75 177)
				(xy 139.3 177) (xy 139.3 179.5) (xy 135.85 179.5) (xy 135.85 193.294) (xy 139.246 193.294) (xy 139.3 177)
				(xy 165.65 177.015) (xy 170 181.1) (xy 170 184.2) (xy 176.8 184.2) (xy 179.7 181.35) (xy 179.7 164.35)
				(xy 180.7 163.4) (xy 180.7 160.35) (xy 183.25 160.35) (xy 184.25 161.35) (xy 183.6 163.55) (xy 183.15 164)
				(xy 183.15 170.6) (xy 185.85 170.6) (xy 185.9 183.65) (xy 181.5 183.65) (xy 179.7 185.35) (xy 178.45 185.35)
				(xy 178.45 187.55) (xy 171.952718 187.553928) (xy 166.9 191.05) (xy 170.15 194) (xy 171.35 194)
				(xy 171.35 192.2) (xy 176.95 192.2) (xy 182.1 194) (xy 189.1 194) (xy 189.1 187.65) (xy 200.55 187.7)
				(xy 200.65 193.6) (xy 205.1 193.6) (xy 205.1 194.05) (xy 208.550079 194.073816) (xy 209.25 193.35)
				(xy 214.95 193.35) (xy 216.45 190.4) (xy 219.7 190.4) (xy 223.250083 194.025093) (xy 224.350071 194.021447)
				(xy 224.35 190.15) (xy 227.15 190.15) (xy 228.05 192.95) (xy 233.85 192.95) (xy 233.849967 193.98996)
				(xy 235.95 193.983) (xy 235.952745 187.300001) (xy 234.6 187.3) (xy 234.6 184.9) (xy 233.95 184.3)
				(xy 233.95 180.85) (xy 235.956277 178.700003) (xy 235.963219 161.797999) (xy 235.458 161.29) (xy 235.458 158.242)
				(xy 235.964993 157.48) (xy 235.979648 121.799992) (xy 234.95 120.8) (xy 234.95 113.45) (xy 235.983509 112.400014)
				(xy 236 72.25) (xy 158.8 72.22) (xy 158.7 89.7) (xy 143.46 89.7) (xy 143.55 77.9) (xy 139.35 73.75)
				(xy 128.6 73.75) (xy 128.6 65.75) (xy 124.95 65.75) (xy 123.95 64.85) (xy 116 64.85) (xy 115.1 65.8)
				(xy 115.1 68.2) (xy 113.7 68.2) (xy 112.4 66.95) (xy 103.4 66.95) (xy 107.4 72.2) (xy 107.4 76.35)
				(xy 99.7 76.4) (xy 99.7 64.77) (xy 95.75 64.77) (xy 95.75 73.05) (xy 96.2 73.5) (xy 96.2 81.55)
				(xy 93.75 81.55) (xy 92.25 83.1) (xy 92.2 100.6) (xy 91.2 101.6) (xy 91.15 107.15) (xy 89.4 108.9)
				(xy 89.4 101.8) (xy 88.5 100.95) (xy 88.5 83.1) (xy 87 81.55) (xy 84.39 81.55) (xy 84.4 87.6) (xy 71.79 87.6)
				(xy 71.8 93.9) (xy 84.2 93.9) (xy 84.25 110) (xy 87.05 110) (xy 87.05 116.75) (xy 84.248652 116.750003)
				(xy 84.35 164.084) (xy 98.806 164.084) (xy 103.4 168.1) (xy 103.385 186.563) (xy 76.2 186.563) (xy 76.2 193.167)
				(xy 64.135 193.167) (xy 64.135 64.77) (xy 64.135 53.975)
			)
		)
	)
	(zone
		(net 72)
		(net_name "VCC")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 6)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 72.1 87.8) (xy 72.1 93.7) (xy 84.2 93.7) (xy 84.8 90.5) (xy 84.2 87.8)
			)
		)
	)
	(zone
		(net 2)
		(net_name "Net-(DB1-+)")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 18)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 92.9 188.7) (xy 92.9 192.95) (xy 106 192.95) (xy 106 191.2) (xy 108.9 191.2) (xy 108.9 184.55)
				(xy 109.85 183.65) (xy 114.95 183.65) (xy 115.5 183.10653) (xy 115.5 178.05) (xy 113.4 175.95) (xy 107.3 175.95)
				(xy 107.3 181.15) (xy 106.55 181.9) (xy 106.55 186.35) (xy 106 186.85) (xy 97.8 186.85) (xy 97.8 188.7)
			)
		)
	)
	(zone
		(net 298)
		(net_name "+9V")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 21)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 132.85 180.1) (xy 132.85 177.5) (xy 129.7 177.5) (xy 125.7 173.55) (xy 122.45 173.55) (xy 120.7 171.85)
				(xy 120.7 164.65) (xy 110.3 164.65) (xy 110.3 158.15) (xy 111.1 157.35) (xy 111.1 152.55) (xy 110.35 152.55)
				(xy 109.15 153.8) (xy 109.15 166.35) (xy 110.4 167.6) (xy 113.8 167.6) (xy 121.6 175.35) (xy 123.4 175.35)
				(xy 123.9 175.9) (xy 123.9 180.1)
			)
		)
	)
	(zone
		(net 72)
		(net_name "VCC")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 83)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 228.6 173.99) (xy 228.6 156.464) (xy 226.568 156.464) (xy 226.568 173.99)
			)
		)
	)
	(zone
		(net 127)
		(net_name "GND")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 34)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 136 115.9) (xy 136 113.85) (xy 136.65 113.1) (xy 137.9 113.1) (xy 137.9 110.7) (xy 136.8 110.7)
				(xy 135.2 109.05) (xy 133.25 109.05) (xy 133.25 103.95) (xy 129.45 103.95) (xy 128.75 103.2) (xy 128.75 102.35)
				(xy 127.2 102.35) (xy 118.05 102.35) (xy 118.05 112.95) (xy 118.95 113.8) (xy 118.95 116.5) (xy 123.75 116.5)
				(xy 123.75 117.6) (xy 129.7 117.6) (xy 129.7 116.3) (xy 133.45 116.3) (xy 133.9 115.9)
			)
		)
	)
	(zone
		(net 127)
		(net_name "GND")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 40)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 196.35 169.5) (xy 198.25 169.5) (xy 198.25 163.3) (xy 199.7 163.3) (xy 199.9 163.05) (xy 202.55 163.05)
				(xy 202.55 162) (xy 198.85 162) (xy 198.85 157) (xy 198.35 156.5) (xy 183.4 156.5) (xy 184.2 158.1)
				(xy 190.4 158.1) (xy 191.05 157.45) (xy 193.6 157.45) (xy 195.35 159.2) (xy 195.35 162.75) (xy 195.1 163)
				(xy 194.35 163) (xy 194.35 165.95) (xy 195.8 165.95) (xy 196.35 166.45)
			)
		)
	)
	(zone
		(net 298)
		(net_name "+9V")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 90)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 123.19 151.892) (xy 123.19 155.702) (xy 128.778 155.702) (xy 128.778 158.242) (xy 132.08 158.242)
				(xy 133.096 159.004) (xy 134.112 159.004) (xy 134.112 157.988) (xy 132.842 157.988) (xy 132.08 157.226)
				(xy 130.556 157.226) (xy 130.556 154.432) (xy 126.238 154.432) (xy 126.238 151.892)
			)
		)
	)
	(zone
		(net 72)
		(net_name "VCC")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 74)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 171.196 105.41) (xy 171.196 101.6) (xy 170.18 101.6) (xy 170.18 93.726) (xy 167.894 93.726)
				(xy 167.894 105.41)
			)
		)
	)
	(zone
		(net 127)
		(net_name "GND")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 51)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 183.3 132.9) (xy 186.35 132.9) (xy 186.35 134.3) (xy 183.75 136.8) (xy 179.7 136.8) (xy 178.2 138.2)
				(xy 174.8 138.2) (xy 174.8 135.25) (xy 183.3 135.25)
			)
		)
	)
	(zone
		(net 72)
		(net_name "VCC")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 49)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 174.95 123) (xy 174.95 125.8) (xy 175.45 125.8) (xy 176.25 125) (xy 179.5 125) (xy 180.7 123.95)
				(xy 183.45 123.95) (xy 183.45 123)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layer "F.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(keepout
			(tracks allowed)
			(vias allowed)
			(pads allowed)
			(copperpour not_allowed)
			(footprints allowed)
		)
		(placement
			(enabled no)
			(sheetname "")
		)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 71.7 80.8) (xy 75 80.8) (xy 75 87.6) (xy 71.7 87.6)
			)
		)
	)
	(zone
		(net 127)
		(net_name "GND")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 84)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 122.428 163.83) (xy 122.428 159.004) (xy 114.808 159.004) (xy 113.284 160.528) (xy 112.014 160.528)
				(xy 111.506 160.02) (xy 111.506 158.75) (xy 113.538 156.718) (xy 113.538 151.384) (xy 111.506 151.384)
				(xy 111.506 157.734) (xy 110.744 158.496) (xy 110.744 164.338) (xy 112.014 164.338) (xy 112.014 162.814)
				(xy 116.84 162.814) (xy 117.602 163.83)
			)
		)
	)
	(zone
		(net 127)
		(net_name "GND")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 50)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 185.95 138.15) (xy 190.75 138.15) (xy 190.75 137.1) (xy 191.8 136.05) (xy 194.2 136.05) (xy 195.35 134.95)
				(xy 195.35 132.65) (xy 194.7 132.05) (xy 194.7 125.5) (xy 194.45 125.25) (xy 186.95 125.25) (xy 185.95 124.2)
				(xy 181 124.2) (xy 179.65 125.5) (xy 176.45 125.5) (xy 175.1 126.85) (xy 175.1 131.4) (xy 176.75 131.4)
				(xy 176.75 127.45) (xy 177.2 126.95) (xy 189.2 126.95) (xy 190.25 127.9) (xy 190.25 133.4)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layer "F.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(keepout
			(tracks allowed)
			(vias allowed)
			(pads allowed)
			(copperpour not_allowed)
			(footprints allowed)
		)
		(placement
			(enabled no)
			(sheetname "")
		)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 240.665 140.97) (xy 245.745 140.97) (xy 245.745 127) (xy 244.475 125.73) (xy 243.205 125.73)
				(xy 241.935 124.46) (xy 240.665 124.46)
			)
		)
	)
	(zone
		(net 127)
		(net_name "GND")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 52)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 171.1 137.85) (xy 175 137.85) (xy 175 140.7) (xy 175.75 140.7) (xy 176.35 141.4) (xy 178.05 141.4)
				(xy 178.65 142) (xy 178.65 144.4) (xy 178.4 144.75) (xy 176.95 144.75) (xy 171.1 138.75)
			)
		)
	)
	(zone
		(net 72)
		(net_name "VCC")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 91)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 98.552 163.068) (xy 98.552 161.036) (xy 96.012 161.036) (xy 95.504 160.528) (xy 95.504 159.766)
				(xy 90.424 159.766) (xy 87.122 156.21) (xy 87.122 117.094) (xy 84.836 117.094) (xy 84.836 161.036)
				(xy 86.868 163.068)
			)
		)
	)
	(zone
		(net 72)
		(net_name "VCC")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 19)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 160.5 74.3) (xy 192.2 74.3) (xy 198 79.75) (xy 201.3 79.75) (xy 202.8 81.25) (xy 202.8 82.35)
				(xy 192.7 92.15) (xy 211.75 92.15) (xy 211.709 81.153) (xy 223.774 81.153) (xy 233.420249 97.129886)
				(xy 233.4 104.15) (xy 235.55 106.45) (xy 235.55 73.2) (xy 235.05 72.7) (xy 160.5 72.7)
			)
		)
	)
	(zone
		(net 72)
		(net_name "VCC")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 42)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 218.1 171.4) (xy 217.25 171.4) (xy 216.85 171.75) (xy 216.85 173.25) (xy 217.05 173.45) (xy 217.75 173.45)
				(xy 218.25 174) (xy 218.25 176.15) (xy 224.65 176.15) (xy 224.65 172.5) (xy 221.3 172.5) (xy 220.8 173)
				(xy 218.45 173) (xy 218.1 172.65)
			)
		)
	)
	(zone
		(net 127)
		(net_name "GND")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 17)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 107.5 103.85) (xy 107.5 97.3) (xy 110.05 94.55) (xy 110.05 89.35) (xy 109.15 88.2) (xy 106.9 88.2)
				(xy 106.35 87.7) (xy 106.35 85.95) (xy 103.2 85.95) (xy 103.2 79.9) (xy 98.45 79.9) (xy 98.45 88.3)
				(xy 97.9 88.85) (xy 97.9 103.2) (xy 98.5 103.85)
			)
		)
	)
	(zone
		(net 72)
		(net_name "VCC")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 77)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 161.036 78.74) (xy 163.068 76.708) (xy 175.768 76.708) (xy 175.768 83.566) (xy 161.036 83.566)
			)
		)
	)
	(zone
		(net 127)
		(net_name "GND")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 88)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 113.538 98.806) (xy 116.078 98.806) (xy 116.078 102.362) (xy 116.586 102.362) (xy 116.586 100.076)
				(xy 117.348 100.076) (xy 117.348 96.266) (xy 117.094 96.266) (xy 117.094 94.234) (xy 116.586 93.726)
				(xy 115.57 93.726) (xy 115.57 96.774)
			)
		)
	)
	(zone
		(net 127)
		(net_name "GND")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 46)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 92.85 153.3) (xy 96.2 153.3) (xy 96.2 148.05) (xy 100.3 144.05) (xy 108.05 144.05) (xy 108.05 142.8)
				(xy 95.15 142.8) (xy 95.15 140) (xy 93.15 140) (xy 93.15 128) (xy 91.6 128) (xy 91.6 148.05) (xy 92.5 148.05)
				(xy 92.85 148.5)
			)
		)
	)
	(zone
		(net 127)
		(net_name "GND")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 32)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 91.6 126.35) (xy 91.6 119.55) (xy 100.7 119.55) (xy 100.7 129.4) (xy 101.35 130) (xy 103.5 130)
				(xy 104.3 129.25) (xy 104.3 126.75) (xy 120.3 126.75) (xy 120.3 130.6) (xy 123.15 133.35) (xy 123.15 135.5)
				(xy 124.5 136.95) (xy 124.5 138.2) (xy 124.9 138.6) (xy 124.9 139.85) (xy 125.2 140.1) (xy 125.55 140.1)
				(xy 127.35 142.05) (xy 128.15 142.05) (xy 128.15 143.1) (xy 127.4 143.1) (xy 126.1 141.85) (xy 113.8 141.85)
				(xy 111.25 139.3) (xy 101.55 139.3) (xy 100.3 138.1) (xy 100.3 133.6) (xy 97.1 130.4) (xy 97.1 125.15)
				(xy 96.2 124.25) (xy 96.2 121.55) (xy 93.2 121.5) (xy 93.2 126.35)
			)
		)
	)
	(zone
		(net 72)
		(net_name "VCC")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 76)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 140.208 102.87) (xy 148.844 102.87) (xy 148.844 107.188) (xy 146.304 107.188) (xy 146.304 112.522)
				(xy 140.208 112.522)
			)
		)
	)
	(zone
		(net 72)
		(net_name "VCC")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 87)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 210.058 105.664) (xy 211.582 105.664) (xy 211.582 101.854) (xy 210.566 100.33) (xy 210.058 100.838)
			)
		)
	)
	(zone
		(net 72)
		(net_name "VCC")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 86)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 184.658 122.682) (xy 191.008 122.682) (xy 191.008 124.714) (xy 187.452 124.714) (xy 186.182 123.698)
				(xy 184.658 123.698)
			)
		)
	)
	(zone
		(net 72)
		(net_name "VCC")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 11)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 141.95 126.2) (xy 141.95 143.85) (xy 145.75 143.85) (xy 145.75 126.25)
			)
		)
	)
	(zone
		(net 72)
		(net_name "VCC")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 73)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 178.816 109.728) (xy 178.816 100.584) (xy 189.484 100.584) (xy 189.484 109.728)
			)
		)
	)
	(zone
		(net 127)
		(net_name "GND")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 35)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 110.25 121.95) (xy 110.25 112.2) (xy 106.45 108.45) (xy 97.5 108.45) (xy 95.8 110.05) (xy 91.6 110.05)
				(xy 91.6 115.4) (xy 97.4 115.4) (xy 98.3 114.55) (xy 101.9 114.55) (xy 104.3 116.95) (xy 104.3 121.95)
			)
		)
	)
	(zone
		(net 72)
		(net_name "VCC")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 15)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 117.15 78.5) (xy 117.15 85.4) (xy 119.5 85.4) (xy 119.5 86.95) (xy 121.5 86.95) (xy 121.5 85.55)
				(xy 121.75 85.3) (xy 121.75 82.5) (xy 122.75 81.45) (xy 123.8 81.45) (xy 123.8 78.6)
			)
		)
	)
	(zone
		(net 72)
		(net_name "VCC")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 13)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 139.05 176.55) (xy 143.65 176.55) (xy 144 176.25) (xy 144 170.05) (xy 146.2 167.8) (xy 146.2 166.8)
				(xy 149.85 166.8) (xy 150.65 165.95) (xy 159.65 165.95) (xy 168.95 156.75) (xy 172.45 156.75) (xy 172.45 158.15)
				(xy 176.7 158.15) (xy 176.7 160.6) (xy 178 162.1) (xy 178 171.9) (xy 177.6 172.3) (xy 175.85 172.3)
				(xy 175.85 176.8) (xy 177.1 178.1) (xy 172.45 183.6) (xy 176.8 183.6) (xy 179.3 181.15) (xy 179.3 174.15)
				(xy 179.3 164.15) (xy 180.3 163.15) (xy 180.3 158.85) (xy 179.55 158.1) (xy 179.55 156.5) (xy 177.5 156.5)
				(xy 176.8 155.8) (xy 175.45 155.8) (xy 173.95 154.25) (xy 170.4 154.25) (xy 170.4 149.4) (xy 162.25 141.45)
				(xy 162.25 131.05) (xy 159.3 131.05) (xy 159.25 143.15) (xy 164.55 148.35) (xy 164.55 153.4) (xy 165.15 154.05)
				(xy 165.15 157.15) (xy 160.05 162.15) (xy 143.75 162.15) (xy 140.75 165) (xy 140.75 172.45) (xy 139.05 174.15)
			)
		)
	)
	(zone
		(net 127)
		(net_name "GND")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 33)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 130.6 133.7) (xy 130.6 144.5) (xy 135.45 144.5) (xy 136.1 143.8) (xy 137.6 143.8) (xy 137.6 144.95)
				(xy 141.6 144.95) (xy 141.6 143.85) (xy 139.6 143.85) (xy 137.2 138.4) (xy 134.35 135.6) (xy 133.6 135.6)
				(xy 131.7 133.7)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layers "F.Cu" "B.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(keepout
			(tracks not_allowed)
			(vias not_allowed)
			(pads not_allowed)
			(copperpour not_allowed)
			(footprints allowed)
		)
		(placement
			(enabled no)
			(sheetname "/")
		)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 167.386 70.104) (xy 184.404 70.104) (xy 184.404 69.088) (xy 167.386 69.088)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layer "F.Mask")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 121.92 212.09) (xy 121.92 194.31) (xy 129.54 194.31) (xy 129.54 212.09)
			)
		)
	)
	(zone
		(net 127)
		(net_name "GND")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 96)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 103.378 199.39) (xy 104.394 199.39) (xy 106.68 197.104) (xy 106.68 196.088) (xy 99.06 196.088)
				(xy 99.06 192.024) (xy 98.298 192.024) (xy 98.298 198.12) (xy 103.378 198.12)
			)
		)
	)
	(zone
		(net 127)
		(net_name "GND")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 3)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 144.78 62.23) (xy 116.205 62.23) (xy 89.7 62.23) (xy 84.1 67.7) (xy 75 67.7) (xy 75 76.4) (xy 72.09 79.3)
				(xy 72.09 123.825) (xy 75.565 123.825) (xy 76.835 125.095) (xy 76.835 132.08) (xy 73.8 135.255)
				(xy 73.8 140.3) (xy 74.7 141.27) (xy 77 141.27) (xy 77 144.7) (xy 76 144.7) (xy 76 151.8) (xy 78.7 154.5)
				(xy 78.7 159.9) (xy 80.8 161.9) (xy 85.4 161.9) (xy 85.4 169.7) (xy 82.6 172.54) (xy 82.6 175.65)
				(xy 81.9 175.65) (xy 81.9 178.25) (xy 87.7 178.25) (xy 88.3 177.6) (xy 95.35 177.6) (xy 95.35 174.2)
				(xy 96.85 171.5) (xy 100.15 170.15) (xy 103.25 171.3) (xy 104.85 174.3) (xy 104.85 178.95) (xy 106.8 178.95)
				(xy 106.8 180.7) (xy 109.5 180.7) (xy 111.55 182.75) (xy 119.85 182.75) (xy 119.85 191) (xy 116.4 191)
				(xy 116.4 189.5) (xy 115.45 189.5) (xy 115.45 191) (xy 111.9 191) (xy 111.9 188.6) (xy 106.9 188.6)
				(xy 106.9 183.9) (xy 106.15 183.18) (xy 76.2 183.18) (xy 76.2 193.059) (xy 64.135 193.059) (xy 64.135 53.975)
				(xy 144.78 53.975)
			)
		)
	)
	(zone
		(net 127)
		(net_name "GND")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 31)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 131.05 116.1) (xy 131.05 113.45) (xy 130.45 112.8) (xy 129.25 112.8) (xy 129.25 110.5) (xy 117.15 110.5)
				(xy 114.5 113.15) (xy 108.25 113.15) (xy 108.25 119.75) (xy 107.85 120.1) (xy 102.1 120.1) (xy 99.9 122.15)
				(xy 99.9 130.65) (xy 100.75 131.4) (xy 100.75 136.15) (xy 101.55 137) (xy 103.25 137) (xy 103.25 139.6)
				(xy 104.7 139.6) (xy 104.7 143.25) (xy 105.85 143.25) (xy 105.85 141.1) (xy 109.95 141.1) (xy 109.95 139.75)
				(xy 111.15 138.5) (xy 111.15 136.35) (xy 110.6 135.75) (xy 102.35 135.75) (xy 102 135.4) (xy 102 134.45)
				(xy 105.95 131.1) (xy 104.1 131.1) (xy 104.1 129.3) (xy 102.05 129.25) (xy 102.1 125.8) (xy 103.3 125.8)
				(xy 103.3 123.1) (xy 103.85 122.45) (xy 111.4 122.45) (xy 111.4 119.8) (xy 110.45 118.95) (xy 110.45 117.7)
				(xy 112.7 117.7) (xy 112.7 116.7) (xy 116.75 116.7) (xy 117.3 116.15) (xy 117.3 113.75) (xy 117.7 113.3)
				(xy 118.9 113.3) (xy 119.2 113.6) (xy 119.2 115.8) (xy 119.55 116.15) (xy 123.85 116.15) (xy 124.2 116.45)
				(xy 124.2 118.95) (xy 124.8 119.6) (xy 127.5 119.6) (xy 127.5 118.5) (xy 130 116.1)
			)
		)
	)
	(zone
		(net 127)
		(net_name "GND")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 66)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 204.978 153.924) (xy 210.312 148.59) (xy 210.312 143.51) (xy 202.184 143.51) (xy 194.31 146.812)
				(xy 194.31 152.654) (xy 192.532 154.432) (xy 192.532 157.226) (xy 204.978 157.226)
			)
		)
	)
	(zone
		(net 303)
		(net_name "Net-(DA11-K)")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 60)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 114.554 202.184) (xy 114.554 191.77) (xy 111.506 191.77) (xy 107.442 195.58) (xy 107.442 197.612)
				(xy 103.632 201.168) (xy 103.632 203.2) (xy 105.156 203.2) (xy 105.156 202.184)
			)
		)
	)
	(zone
		(net 298)
		(net_name "+9V")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 94)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 131.318 177.292) (xy 132.842 177.292) (xy 132.842 179.832) (xy 131.318 179.832)
			)
		)
	)
	(zone
		(net 127)
		(net_name "GND")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 68)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 176.149 167.64) (xy 180.721 167.64) (xy 180.721 171.069) (xy 176.149 171.069)
			)
		)
	)
	(zone
		(net 72)
		(net_name "VCC")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 62)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 184.404 186.436) (xy 184.404 187.706) (xy 193.548 187.706) (xy 193.548 191.008) (xy 195.58 191.008)
				(xy 195.58 188.468) (xy 200.406 188.468) (xy 200.66 188.214) (xy 202.438 188.214) (xy 202.438 193.04)
				(xy 205.232 193.04) (xy 205.994 192.278) (xy 208.28 192.278) (xy 209.296 193.294) (xy 220.726 193.294)
				(xy 222.504 191.516) (xy 222.504 190.5) (xy 224.282 188.976) (xy 224.282 184.912) (xy 227.584 184.912)
				(xy 227.584 186.436) (xy 229.362 186.436) (xy 229.362 178.816) (xy 228.854 178.308) (xy 220.98 178.308)
				(xy 220.472 177.8) (xy 220.472 173.99) (xy 219.71 173.99) (xy 219.71 179.07) (xy 220.726 180.086)
				(xy 220.726 185.928) (xy 220.98 186.182) (xy 220.98 191.262) (xy 220.218 192.024) (xy 212.598 192.024)
				(xy 210.312 189.738) (xy 210.312 186.182) (xy 209.296 186.182) (xy 208.788 186.69) (xy 208.788 189.23)
				(xy 208.28 189.738) (xy 205.994 189.738) (xy 202.692 186.69) (xy 199.898 186.69) (xy 198.628 185.42)
				(xy 196.596 185.42) (xy 195.326 186.436)
			)
		)
	)
	(zone
		(net 127)
		(net_name "GND")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 38)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 128.5 128.3) (xy 134.85 128.3) (xy 134.85 136.3) (xy 131.800189 136.275986) (xy 131.8 139.75)
				(xy 131 139.75) (xy 131 143.3) (xy 125.15 143.3) (xy 123.45 144.75) (xy 123.45 151.05) (xy 122.1 152.35)
				(xy 116.85 152.35) (xy 116.25 151.8) (xy 113.15 151.8) (xy 114.8 150.1) (xy 119.75 150.1) (xy 121.9 147.95)
				(xy 121.9 144.9) (xy 122.45 144.35) (xy 122.45 137.75) (xy 119.45 137.75) (xy 119.45 136.15) (xy 124.2 136.15)
				(xy 128.5 139.85)
			)
		)
	)
	(zone
		(net 127)
		(net_name "GND")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 36)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 137.25 141.65) (xy 140.4 141.65) (xy 140.4 167.4) (xy 138.1 167.4) (xy 138.1 162.9) (xy 139.35 161.7)
				(xy 139.35 153.7) (xy 138.6 152.9) (xy 138.6 143.85) (xy 137.25 142.5)
			)
		)
	)
	(zone
		(net 127)
		(net_name "GND")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 29)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 79.5 110.3) (xy 79.5 112.4) (xy 81.6 114.6) (xy 98.15 114.6) (xy 98.55 114.25) (xy 98.55 109.3)
				(xy 97.45 109.3) (xy 96.85 109.9) (xy 94.25 109.9) (xy 93.15 108.8) (xy 93.15 102.45) (xy 92.45 101.75)
				(xy 92.45 100.4) (xy 91.6 99.55) (xy 91.6 97.1) (xy 90.6 96.05) (xy 89.75 96.05) (xy 87.75 98) (xy 87.75 104.9)
				(xy 88.4 105.65) (xy 88.4 109.35) (xy 87.5 110.3)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 5)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.5)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 250.825 63.5) (xy 245.745 63.5) (xy 245.745 78.105) (xy 250.825 78.105)
			)
		)
	)
	(zone
		(net 127)
		(net_name "GND")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 59)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 170.434 112.776) (xy 170.434 110.744) (xy 179.324 110.744) (xy 184.15 105.918) (xy 190.5 105.918)
				(xy 190.5 102.108) (xy 192.532 102.108) (xy 192.532 103.124) (xy 196.596 103.124) (xy 196.596 108.458)
				(xy 185.674 108.458) (xy 182.372 111.506) (xy 182.372 112.776)
			)
		)
	)
	(zone
		(net 72)
		(net_name "VCC")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 48)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 180.25 118.55) (xy 180.25 120.55) (xy 182.4 122.75) (xy 188.6 122.75) (xy 189.3 123.5) (xy 189.3 130.7)
				(xy 188 130.7) (xy 188 131.6) (xy 194.7 131.6) (xy 195.35 132.3) (xy 195.35 135.1) (xy 196.2 135.25)
				(xy 196.55 135.65) (xy 198.35 135.65) (xy 198.35 137.05) (xy 196.5 137.05) (xy 195.8 136.35) (xy 195.1 136.35)
				(xy 194.6 135.85) (xy 193.6 135.85) (xy 191 133.2) (xy 187.55 133.2) (xy 186.8 132.4) (xy 183.8 132.4)
				(xy 183.8 131.15) (xy 185.25 131.15) (xy 185.25 127.95) (xy 184.9 127.7) (xy 184.9 126.2) (xy 183.25 124.45)
				(xy 178.75 124.45) (xy 178.25 123.85) (xy 178.25 118.55)
			)
		)
	)
	(zone
		(net 127)
		(net_name "GND")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 28)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 91.35 79.1) (xy 91.35 75.95) (xy 99.65 75.95) (xy 100.5 75.2) (xy 107.35 75.2) (xy 107.35 77.15)
				(xy 100.95 77.15) (xy 100.45 77.65) (xy 96.75 77.65) (xy 96.1 78.3) (xy 96.1 79.1)
			)
		)
	)
	(zone
		(net 127)
		(net_name "GND")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 67)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 181.356 161.544) (xy 186.436 161.544) (xy 186.436 154.178) (xy 181.356 154.178)
			)
		)
	)
	(zone
		(net 127)
		(net_name "GND")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 63)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 213.614 191.516) (xy 220.218 191.516) (xy 220.218 189.738) (xy 218.186 189.738) (xy 218.186 188.468)
				(xy 216.662 188.468) (xy 216.662 184.912) (xy 217.678 184.912) (xy 217.678 182.626) (xy 218.186 182.118)
				(xy 218.186 176.276) (xy 214.63 176.276) (xy 214.63 178.308) (xy 215.646 179.324) (xy 215.646 184.15)
				(xy 214.63 185.166) (xy 214.63 189.484) (xy 213.614 190.5)
			)
		)
	)
	(zone
		(net 72)
		(net_name "VCC")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 7)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 101.3 168.2) (xy 99.1 168.2) (xy 98.6 167.6) (xy 96.7 167.6) (xy 94.5 169.8) (xy 94.5 172.1)
				(xy 88.6 172.1) (xy 88.6 170.2) (xy 86.7 170.2) (xy 86.7 160.3) (xy 87.7 159.3) (xy 88.5 159.3)
				(xy 89 158.8) (xy 90 158.8) (xy 91.9 160.7) (xy 93.8 160.7)
			)
		)
	)
	(zone
		(net 127)
		(net_name "GND")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 45)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 229.85 110.6) (xy 232.1 110.6) (xy 234.45 113) (xy 236.7 113) (xy 236.7 116.45) (xy 235.5 117.65)
				(xy 225.3 117.65) (xy 223.1 119.8) (xy 217.2 119.85) (xy 217.2 122.5) (xy 218.7 122.5) (xy 218.7 124.75)
				(xy 217.8 124.75) (xy 210.2 117.2) (xy 210.2 112.7) (xy 211.8 112.7) (xy 216.4 117.25) (xy 223.35 117.25)
				(xy 224.1 116.45) (xy 224.9 116.45) (xy 226.05 115.25) (xy 228.8 115.25) (xy 229.85 114.2)
			)
		)
	)
	(zone
		(net 72)
		(net_name "VCC")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 56)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 160.274 134.112) (xy 160.274 135.382) (xy 162.052 144.018) (xy 162.814 144.78) (xy 165.608 144.78)
				(xy 165.862 144.526) (xy 166.878 144.526) (xy 166.878 135.89) (xy 167.386 135.89) (xy 167.386 132.842)
				(xy 163.322 132.842) (xy 162.306 134.112)
			)
		)
	)
	(zone
		(net 127)
		(net_name "GND")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 4)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.5)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 250.825 53.975) (xy 250.825 62.865) (xy 244.81 62.915) (xy 244.85 109.55) (xy 237.15 102.177484)
				(xy 232.6 102.2) (xy 232.6 106.95) (xy 231.85 107.7) (xy 225.75 107.7) (xy 225.483421 107.311373)
				(xy 223.8 107.3) (xy 223.2 106.7) (xy 221.35 106.7) (xy 220.5 107.3) (xy 211.3 107.3) (xy 210.9 106.95)
				(xy 210.9 105.8) (xy 213.2 104.2) (xy 214.65 105.6) (xy 220.5 105.6) (xy 220.5 98.2) (xy 220.751024 98)
				(xy 220.75 96.45) (xy 221.6 96.45) (xy 221.6 101.65) (xy 228.097215 101.646823) (xy 228.55 101.25)
				(xy 228.55 94.2) (xy 221.6 94.2) (xy 221.6 96.45) (xy 220.75 96.45) (xy 219.3 96.45) (xy 219.3 94.2)
				(xy 212.35 94.2) (xy 212.35 89.2) (xy 204.9 89.2) (xy 204.9 95.4) (xy 204.3 96) (xy 204.3 103.1)
				(xy 205.3 104.2) (xy 213.2 104.2) (xy 207.85 107.95) (xy 199.45 107.95) (xy 199.45 103.1) (xy 200.25 102.3)
				(xy 200.25 98.6) (xy 199.5 97.8) (xy 199.5 94.45) (xy 201.15 94.45) (xy 201.15 86.65) (xy 205.045726 86.65)
				(xy 205.035382 83.7) (xy 202.668219 81.30349) (xy 201.422 81.28) (xy 200.152 82.55) (xy 195.707 82.55)
				(xy 195.707 84.455) (xy 194.818 84.455) (xy 194.818 81.534) (xy 198.12 81.534) (xy 198.12 77.978)
				(xy 199.644 77.978) (xy 199.644 75.565) (xy 184.404 75.565) (xy 184.404 82.042) (xy 182.118 82.042)
				(xy 182.118 79.756) (xy 180.848 79.756) (xy 180.848 76.962) (xy 179.578 75.565) (xy 171.45 75.565)
				(xy 171.45 71.755) (xy 137.16 71.755) (xy 137.16 66.04) (xy 135.255 66.04) (xy 135.255 53.975)
			)
		)
	)
	(zone
		(net 72)
		(net_name "VCC")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 69)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 176.276 167.386) (xy 180.34 167.386) (xy 181.102 168.148) (xy 181.102 170.434) (xy 184.912 170.434)
				(xy 184.912 169.418) (xy 182.88 169.418) (xy 182.88 166.116) (xy 176.276 166.116)
			)
		)
	)
	(zone
		(net 127)
		(net_name "GND")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 2)
		(connect_pads yes
			(clearance 0.5)
		)
		(min_thickness 0.5)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 238.3 174.3) (xy 238.35 159.65) (xy 240.05 158.1) (xy 240.05 150.7) (xy 237.744 148.336) (xy 232.156 147.828)
				(xy 232.156 147.066) (xy 241.4 147.1) (xy 245.4 143.1) (xy 245.618 128.27) (xy 238.125 121.285)
				(xy 238.125 120.65) (xy 240.665 118.11) (xy 240.665 110.42) (xy 238.125 107.88) (xy 238.125 92.075)
				(xy 244.86 92.075) (xy 244.86 114.935) (xy 250.825 114.935) (xy 250.825 212.055) (xy 79.375 212.055)
				(xy 79.4 206.2) (xy 85.425 206.175) (xy 87.457 204.27) (xy 87.5 192) (xy 92.583 192.024) (xy 92.583 204.008)
				(xy 107.35 204.008) (xy 107.7 203.75) (xy 115.85 203.75) (xy 115.85 193.95) (xy 120.95 193.95) (xy 120.95 188.25)
				(xy 122.6 188.25) (xy 122.6 190.2) (xy 123 190.2) (xy 123 196.15) (xy 117.3 196.15) (xy 117.3 203.75)
				(xy 134.239 203.75) (xy 134.239 191.135) (xy 145.415 191.135) (xy 145.796 190.5) (xy 145.796 176.657)
				(xy 152.4 176.657) (xy 154.305 178.435) (xy 154.305 191.135) (xy 157.48 194.31) (xy 170.815 194.31)
				(xy 172.085 193.675) (xy 205.74 193.675) (xy 206.85 194.75) (xy 234.9 194.8) (xy 235.8 193.85) (xy 235.8 176.7)
			)
		)
	)
	(zone
		(net 127)
		(net_name "GND")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 30)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 82.65 127.9) (xy 85.95 127.9) (xy 85.95 126.05) (xy 93 126.05) (xy 93 127.65) (xy 91.65 127.65)
				(xy 91.65 128.9) (xy 94 128.9) (xy 94 123.35) (xy 81.35 123.35) (xy 80.75 123.95) (xy 80.75 128.1)
				(xy 81.75 128.1) (xy 81.75 126.95) (xy 82.65 126.95)
			)
		)
	)
	(zone
		(net 72)
		(net_name "VCC")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 97)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 221.488 174.498) (xy 227.076 174.498) (xy 227.076 173.482) (xy 228.346 173.482) (xy 228.346 170.942)
				(xy 226.314 170.942) (xy 226.314 172.72) (xy 223.774 172.72) (xy 223.774 162.56) (xy 222.758 162.56)
				(xy 222.758 171.958) (xy 221.996 172.72) (xy 221.488 172.72)
			)
		)
	)
	(zone
		(net 127)
		(net_name "GND")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 26)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 154.55 77.95) (xy 158.9 82.2) (xy 158.9 85.7) (xy 155.95 88.55) (xy 139.3 88.5) (xy 139.3 86)
				(xy 133.1 86) (xy 133.1 84.8) (xy 131.05 82.85) (xy 131.05 80.8) (xy 131.75 80.8) (xy 135.6 84.15)
				(xy 144.95 84.15) (xy 144.95 81.85) (xy 147.55 81.85) (xy 147.55 77.95)
			)
		)
	)
	(zone
		(net 72)
		(net_name "VCC")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 27)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 123.75 76.9) (xy 123.75 78.2) (xy 121.85 80.1) (xy 121.85 81.15) (xy 104 81.15) (xy 102.1 79.3)
				(xy 97 79.3) (xy 97 78.15) (xy 100.55 78.15) (xy 101.15 77.6) (xy 107.8 77.6) (xy 107.8 75.2) (xy 117.9 75.2)
				(xy 119.65 76.9)
			)
		)
	)
	(zone
		(net 72)
		(net_name "VCC")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 58)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 147.066 106.68) (xy 147.066 103.124) (xy 151.13 103.124) (xy 151.13 99.314) (xy 155.956 99.314)
				(xy 155.956 89.916) (xy 156.464 89.916) (xy 160.274 86.36) (xy 160.274 82.55) (xy 162.56 80.264)
				(xy 164.592 80.264) (xy 164.592 90.678) (xy 160.02 90.678) (xy 160.02 96.266) (xy 160.782 97.028)
				(xy 160.782 103.632) (xy 164.338 103.632) (xy 164.338 107.696) (xy 168.91 107.696) (xy 168.91 105.41)
				(xy 167.386 103.378) (xy 167.386 94.996) (xy 170.18 94.996) (xy 170.18 100.33) (xy 171.45 101.6)
				(xy 171.45 107.442) (xy 177.292 107.442) (xy 177.292 106.426) (xy 179.07 104.902) (xy 179.07 102.362)
				(xy 184.15 97.282) (xy 184.15 90.17) (xy 184.912 89.662) (xy 184.912 88.392) (xy 189.992 88.392)
				(xy 191.516 90.17) (xy 192.532 90.17) (xy 193.802 88.9) (xy 196.088 88.9) (xy 196.088 86.614) (xy 200.66 86.614)
				(xy 200.66 93.98) (xy 194.818 93.98) (xy 194.31 94.488) (xy 189.23 94.488) (xy 188.722 94.996) (xy 188.722 97.028)
				(xy 185.928 99.568) (xy 185.928 101.6) (xy 187.706 103.378) (xy 187.706 105.41) (xy 183.896 105.41)
				(xy 179.07 110.236) (xy 170.18 110.236) (xy 170.18 113.284) (xy 176.276 113.284) (xy 176.276 117.602)
				(xy 177.038 118.364) (xy 177.038 124.968) (xy 175.26 124.968) (xy 173.99 123.952) (xy 173.99 119.634)
				(xy 171.196 116.84) (xy 166.624 116.84) (xy 166.624 122.428) (xy 165.862 123.19) (xy 165.862 129.794)
				(xy 166.37 130.302) (xy 166.37 132.334) (xy 160.274 132.334) (xy 160.274 127) (xy 164.084 123.19)
				(xy 164.084 114.808) (xy 158.496 114.808) (xy 156.21 112.776) (xy 156.21 106.68)
			)
		)
	)
	(zone
		(net 72)
		(net_name "VCC")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 23)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 233.05 102.6) (xy 237.1 102.6) (xy 237.75 103.25) (xy 237.75 108.3) (xy 240.25 110.8) (xy 240.25 117.8)
				(xy 237.05 121) (xy 232.95 121) (xy 232.5 121.5) (xy 226.4 121.5) (xy 226.4 123) (xy 224.85 124.1)
				(xy 224.85 127.3) (xy 223.3 127.3) (xy 223.3 121.5) (xy 225.65 119.05) (xy 236.25 119.05) (xy 238.3 117)
				(xy 238.3 111.35) (xy 235.75 108.85) (xy 235.75 106.55) (xy 233.05 106.55)
			)
		)
	)
	(zone
		(net 72)
		(net_name "VCC")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 47)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 145.25 174.55) (xy 145.25 189.6) (xy 144.6 190.35) (xy 134.4 190.35) (xy 133.75 190.95) (xy 133.75 203.1)
				(xy 118.2 203.1) (xy 118.25 196.7) (xy 123.5 196.7) (xy 123.5 193.75) (xy 125.4 193.75) (xy 125.4 187.8)
				(xy 120.3 187.75) (xy 120.3 182.05) (xy 111.45 182.05) (xy 109.6 180.25) (xy 107.55 180.25) (xy 107.55 177.55)
				(xy 105.65 177.55) (xy 105.65 174) (xy 104.75 171.65) (xy 102.9 170.1) (xy 100.4 169.5) (xy 99.1 168.2)
				(xy 103.7 168.2) (xy 110.85 175.3) (xy 112.95 175.3) (xy 112.95 178.95) (xy 113.85 179.85) (xy 125.5 179.85)
				(xy 125.5 185.55) (xy 130.1 185.55) (xy 130.1 182.15) (xy 139.25 182.15) (xy 139.241047 173.9) (xy 140.5 172.7)
				(xy 142.55 172.7) (xy 144.3 174.55)
			)
		)
	)
	(zone
		(net 72)
		(net_name "VCC")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 22)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 205.35 89.65) (xy 211.8 89.65) (xy 211.8 96.1) (xy 211.25 96.75) (xy 211.25 101.1) (xy 211.631874 101.56489)
				(xy 217.65 101.55) (xy 217.65 105.1) (xy 214.75 105.1) (xy 213.55 103.9) (xy 205.65 103.9) (xy 204.7 102.95)
				(xy 204.7 100.9) (xy 206.592418 100.893024) (xy 207 100.45) (xy 207 96.15) (xy 205.35 94.45)
			)
		)
	)
	(zone
		(net 127)
		(net_name "GND")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 54)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 189.85 125.55) (xy 195.3 125.55) (xy 195.3 130.85) (xy 189.85 130.85)
			)
		)
	)
	(zone
		(net 396)
		(net_name "Net-(Q18-B)")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 93)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 130.048 180.086) (xy 133.096 180.086) (xy 133.096 177.038) (xy 130.048 177.038) (xy 130.048 175.26)
				(xy 130.556 174.752) (xy 138.684 174.752) (xy 138.684 181.61) (xy 130.048 181.61)
			)
		)
	)
	(zone
		(net 72)
		(net_name "VCC")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 98)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 204.724 167.386) (xy 204.724 160.02) (xy 200.66 160.02) (xy 198.882 157.988) (xy 195.834 157.988)
				(xy 195.834 166.37) (xy 198.374 166.37) (xy 198.374 162.306) (xy 198.882 161.798) (xy 199.644 161.798)
				(xy 200.152 162.306) (xy 200.152 164.084) (xy 202.438 164.084)
			)
		)
	)
	(zone
		(net 127)
		(net_name "GND")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 57)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 183.896 133.096) (xy 186.69 133.096) (xy 187.198 133.604) (xy 190.754 133.604) (xy 192.024 134.874)
				(xy 192.024 135.382) (xy 189.484 135.382) (xy 188.722 136.144) (xy 188.722 139.446) (xy 185.674 139.446)
				(xy 184.15 139.446) (xy 184.15 134.112)
			)
		)
	)
	(zone
		(net 127)
		(net_name "GND")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 55)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 183.3 126.65) (xy 183.3 126.15) (xy 182.7 125.6) (xy 174.9 125.6) (xy 173.5 124.25) (xy 173.5 120.05)
				(xy 170.8 117.45) (xy 167.3 117.45) (xy 167.3 120) (xy 169.1 120) (xy 171.25 122.15) (xy 171.25 124.45)
				(xy 173.45 126.65)
			)
		)
	)
	(zone
		(net 127)
		(net_name "GND")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 64)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 206.248 167.894) (xy 211.328 167.894) (xy 211.328 168.402) (xy 208.788 170.942) (xy 207.772 170.942)
				(xy 207.01 169.672) (xy 206.248 169.672)
			)
		)
	)
	(zone
		(net 72)
		(net_name "VCC")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 44)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 219.15 122.5) (xy 221.9 122.5) (xy 221.9 128) (xy 222.8 128.85) (xy 222.8 134.1) (xy 221.45 139.95)
				(xy 221.45 144.55) (xy 221.15 144.55) (xy 220.3 143.75) (xy 220.3 142.4) (xy 219.9 141.95) (xy 218.5 141.95)
				(xy 212.6 136.1) (xy 208.1 136.1) (xy 207.35 135.35) (xy 207.35 128.1) (xy 206.1 126.9) (xy 204.7 126.9)
				(xy 204.7 123.55) (xy 205.85 123.55) (xy 208.3 125.95) (xy 208.3 129.3) (xy 214.25 135.2) (xy 215.35 135.2)
				(xy 219.7 134.75) (xy 219.7 132.6) (xy 219.15 129.05)
			)
		)
	)
	(zone
		(net 70)
		(net_name "Net-(C30-Pad2)")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 24)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 77.5 198.85) (xy 82.45 198.85) (xy 82.45 192.2) (xy 80.25 192.2) (xy 80.25 193.85) (xy 79.6 194.4)
				(xy 67.55 194.4) (xy 66.65 195.5) (xy 66.65 198.75) (xy 70.3 200.85) (xy 70.3 195.5) (xy 76.7 195.5)
				(xy 77.5 196.25)
			)
		)
	)
	(zone
		(net 127)
		(net_name "GND")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 70)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 171.958 106.934) (xy 173.228 106.934) (xy 173.228 104.902) (xy 174.498 103.632) (xy 174.498 97.028)
				(xy 175.768 95.758) (xy 175.768 87.884) (xy 178.562 87.884) (xy 178.562 83.312) (xy 172.974 83.312)
				(xy 172.974 87.63) (xy 171.704 87.63) (xy 171.704 89.408) (xy 166.624 89.408) (xy 166.624 92.964)
				(xy 171.958 92.964)
			)
		)
	)
	(zone
		(net 72)
		(net_name "VCC")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 9)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 89.8 62.7) (xy 134.85 62.7) (xy 134.85 67.7) (xy 135.5 69) (xy 137.15 69.6) (xy 137.15 72.3)
				(xy 171.196 72.39) (xy 171.196 77.216) (xy 168.402 74.168) (xy 166.624 74.168) (xy 166.624 76.708)
				(xy 164.338 76.708) (xy 164.338 78.994) (xy 161.036 78.994) (xy 160.2 74.4) (xy 135.15 74.45) (xy 133.6 72.9)
				(xy 133.6 70) (xy 130.05 66.5) (xy 130.05 65.5) (xy 128.5 64) (xy 122.525335 63.974361) (xy 119.9 66.5)
				(xy 109.35 66.55) (xy 108 65.25) (xy 100.85 65.25) (xy 99.95 66.1) (xy 88.65 66.1) (xy 74.25 80.25)
				(xy 74.25 98.4) (xy 73.6 99.1) (xy 73.6 102.8) (xy 74.8 104) (xy 74.8 111.1) (xy 80.6 116.9) (xy 95.75 116.9)
				(xy 95.75 122.75) (xy 80.150072 122.783405) (xy 77.3 125.15) (xy 75.3 123.25) (xy 72.4 123.25) (xy 72.4 79.6)
			)
		)
	)
	(zone
		(net 303)
		(net_name "Net-(DA11-K)")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 95)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 125.984 185.166) (xy 129.54 185.166) (xy 129.54 182.118) (xy 127.254 182.118) (xy 125.984 183.388)
			)
		)
	)
	(zone
		(net 72)
		(net_name "VCC")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 65)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 205.74 158.75) (xy 208.026 158.75) (xy 208.026 159.258) (xy 209.55 160.782) (xy 209.55 163.83)
				(xy 211.074 163.83) (xy 211.074 160.274) (xy 212.344 159.004) (xy 213.106 159.004) (xy 213.614 158.496)
				(xy 213.614 157.48) (xy 215.138 157.48) (xy 216.154 156.464) (xy 216.154 151.892) (xy 217.424 150.622)
				(xy 217.424 146.304) (xy 219.202 146.304) (xy 219.202 163.83) (xy 216.408 163.83) (xy 216.408 168.148)
				(xy 216.916 168.148) (xy 216.916 169.926) (xy 217.932 170.942) (xy 217.932 172.466) (xy 207.772 172.466)
				(xy 207.772 171.45) (xy 208.788 171.45) (xy 212.852 167.64) (xy 212.852 165.1) (xy 208.534 165.1)
				(xy 208.534 167.386) (xy 205.994 167.386) (xy 205.994 161.036) (xy 205.74 160.782)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 5)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.5)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 250.575 99.06) (xy 245.595 99.06) (xy 245.595 114.3) (xy 250.575 114.3)
			)
		)
	)
	(zone
		(net 127)
		(net_name "GND")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 8)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 104 88.6) (xy 104 103.6) (xy 111.4 103.6) (xy 113.8 101.3) (xy 116.6 101.3) (xy 117.7 100.2)
				(xy 117.7 98.7) (xy 117.4 98.3) (xy 112.9 98.3) (xy 112.9 88.7)
			)
		)
	)
	(zone
		(net 72)
		(net_name "VCC")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 25)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 136.35 126.6) (xy 140.3 126.6) (xy 140.3 127.6) (xy 143.45 130.75) (xy 143.45 127.8) (xy 143.15 127.45)
				(xy 143.15 125.45) (xy 142.55 124.8) (xy 142.55 102.5) (xy 138.1 102.5) (xy 138.1 108.2) (xy 137.6 108.7)
				(xy 133.75 108.7) (xy 133.346336 108.3) (xy 133.35 104) (xy 133 103.65) (xy 129.4 103.65) (xy 129.4 102.4)
				(xy 124.45 102.4) (xy 124.45 103.75) (xy 120.1 103.75) (xy 120.1 105.1) (xy 119.6 105.65) (xy 118.1 105.65)
				(xy 118.1 106.5) (xy 113.7 110.45) (xy 107.2 110.45) (xy 105.9 111.6) (xy 105.9 116.65) (xy 102.75 116.65)
				(xy 101.1 118.3) (xy 101.1 119.55) (xy 107.7 119.55) (xy 107.7 113.2) (xy 108.3 112.6) (xy 114.25 112.6)
				(xy 116.95 110) (xy 122.3 110) (xy 122.3 109) (xy 123.25 109) (xy 123.25 107.25) (xy 124.15 107.25)
				(xy 124.15 109.2) (xy 125 109.2) (xy 125 109.8) (xy 132 109.8) (xy 132 111.1) (xy 130.7 111.1) (xy 131.55 112.6)
				(xy 131.55 114.6) (xy 136.2 114.55) (xy 136.2 113.2) (xy 137.65 113.2) (xy 138.05 113.65) (xy 138.05 119.3)
				(xy 139.3 119.3) (xy 139.3 120.65) (xy 136.35 123.5)
			)
		)
	)
	(zone
		(net 72)
		(net_name "VCC")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 37)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 145.45 167.5) (xy 145.45 164.55) (xy 143.35 162.55) (xy 143.35 159.85) (xy 143.5 143.5) (xy 143.55 136.55)
				(xy 136 137.2) (xy 136 141.3) (xy 140.9 141.3) (xy 140.9 167.5)
			)
		)
	)
	(zone
		(net 127)
		(net_name "GND")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 61)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 224.282 191.516) (xy 226.822 191.516) (xy 226.822 190.5) (xy 227.33 189.992) (xy 227.33 189.484)
				(xy 225.044 189.484) (xy 224.282 190.246)
			)
		)
	)
	(zone
		(net 127)
		(net_name "GND")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 10)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 123.7 83.5) (xy 125.9 83.5) (xy 128.9 86.5) (xy 128.9 90.9) (xy 118.6 90.9) (xy 118.1 91.4)
				(xy 114.75 91.4) (xy 114.75 89.8) (xy 117.25 89.2) (xy 117.45 87.15) (xy 123.05 87.15) (xy 123.7 86.5)
			)
		)
	)
	(embedded_fonts no)
)
