(kicad_pcb
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(general
		(thickness 1.6)
		(legacy_teardrops no)
	)
	(paper "A4")
	(layers
		(0 "F.Cu" signal)
		(2 "B.Cu" signal)
		(9 "F.Adhes" user "F.Adhesive")
		(11 "B.Adhes" user "B.Adhesive")
		(13 "F.Paste" user)
		(15 "B.Paste" user)
		(5 "F.SilkS" user "F.Silkscreen")
		(7 "B.SilkS" user "B.Silkscreen")
		(1 "F.Mask" user)
		(3 "B.Mask" user)
		(17 "Dwgs.User" user "User.Drawings")
		(19 "Cmts.User" user "User.Comments")
		(21 "Eco1.User" user "User.Eco1")
		(23 "Eco2.User" user "User.Eco2")
		(25 "Edge.Cuts" user)
		(27 "Margin" user)
		(31 "F.CrtYd" user "F.Courtyard")
		(29 "B.CrtYd" user "B.Courtyard")
		(35 "F.Fab" user)
		(33 "B.Fab" user)
		(39 "User.1" user)
		(41 "User.2" user)
		(43 "User.3" user)
		(45 "User.4" user)
	)
	(setup
		(stackup
			(layer "F.SilkS"
				(type "Top Silk Screen")
			)
			(layer "F.Paste"
				(type "Top Solder Paste")
			)
			(layer "F.Mask"
				(type "Top Solder Mask")
				(color "Black")
				(thickness 0.01)
			)
			(layer "F.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "dielectric 1"
				(type "core")
				(thickness 1.51)
				(material "FR4")
				(epsilon_r 4.5)
				(loss_tangent 0.02)
			)
			(layer "B.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "B.Mask"
				(type "Bottom Solder Mask")
				(color "Black")
				(thickness 0.01)
			)
			(layer "B.Paste"
				(type "Bottom Solder Paste")
			)
			(layer "B.SilkS"
				(type "Bottom Silk Screen")
			)
			(copper_finish "None")
			(dielectric_constraints no)
		)
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(tenting front back)
		(pcbplotparams
			(layerselection 0x00000000_00000000_55555555_5755f5ff)
			(plot_on_all_layers_selection 0x00000000_00000000_00000000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 4)
			(plotframeref no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(pdf_metadata yes)
			(pdf_single_document no)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plot_black_and_white yes)
			(sketchpadsonfab no)
			(plotpadnumbers no)
			(hidednponfab no)
			(sketchdnponfab yes)
			(crossoutdnponfab yes)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 1)
			(scaleselection 1)
			(outputdirectory "")
		)
	)
	(net 0 "")
	(net 1 "GND")
	(net 2 "Net-(C1-Pad1)")
	(net 3 "Net-(C2-Pad1)")
	(net 4 "Net-(D1:1-A)")
	(net 5 "Net-(D1:2-A)")
	(net 6 "Net-(D1:3-A)")
	(net 7 "Net-(D1:4-A)")
	(net 8 "Net-(D2:1-A)")
	(net 9 "Net-(D2:2-A)")
	(net 10 "Net-(D2:3-A)")
	(net 11 "Net-(D2:4-A)")
	(net 12 "Net-(D3:1-A)")
	(net 13 "Net-(D3:2-A)")
	(net 14 "Net-(D3:3-A)")
	(net 15 "Net-(D3:4-A)")
	(net 16 "Net-(D4:1-A)")
	(net 17 "Net-(D4:2-A)")
	(net 18 "Net-(D4:3-A)")
	(net 19 "Net-(D4:4-A)")
	(net 20 "unconnected-(IC1-P3-Pad7)")
	(net 21 "unconnected-(IC1-P4-Pad8)")
	(net 22 "/SDA")
	(net 23 "/SCL")
	(net 24 "/TFTDC")
	(net 25 "/TFTRST")
	(net 26 "+3.3V")
	(net 27 "/TFTCS")
	(net 28 "/CARDCS")
	(net 29 "/MISO")
	(net 30 "/SCK")
	(net 31 "/LITE")
	(net 32 "/MOSI")
	(net 33 "/Human-Machine Interface/Keypad/COL1")
	(net 34 "/Human-Machine Interface/Keypad/COL2")
	(net 35 "/Human-Machine Interface/Keypad/COL3")
	(net 36 "/Human-Machine Interface/Keypad/COL4")
	(net 37 "/Human-Machine Interface/Keypad/ROW3")
	(net 38 "/Human-Machine Interface/TFTRST")
	(net 39 "/Human-Machine Interface/ENC_SW")
	(net 40 "/Human-Machine Interface/ENC_CLK")
	(net 41 "/Human-Machine Interface/Keypad/ROW2")
	(net 42 "/Human-Machine Interface/Keypad/ROW1")
	(net 43 "/Human-Machine Interface/Keypad/ROW4")
	(net 44 "/Human-Machine Interface/ENC_DT")
	(net 45 "/Human-Machine Interface/LITE")
	(net 46 "unconnected-(X2-Pad15)")
	(net 47 "unconnected-(X2-Pad14)")
	(net 48 "unconnected-(X2-Pad16)")
	(net 49 "unconnected-(X2-Pad12)")
	(net 50 "unconnected-(X2-Pad11)")
	(net 51 "unconnected-(X2-Pad17)")
	(net 52 "unconnected-(X2-Pad13)")
	(net 53 "unconnected-(X2-Pad18)")
	(net 54 "/Human-Machine Interface/PCF_A2")
	(net 55 "/Human-Machine Interface/PCF_A0")
	(net 56 "/Human-Machine Interface/PCF_A1")
	(net 57 "unconnected-(IC1-P1-Pad5)")
	(net 58 "Net-(JP4-C)")
	(net 59 "/Human-Machine Interface/Audio/~{SD_MODE}")
	(net 60 "/Human-Machine Interface/Audio/GAIN_SLOT")
	(net 61 "Net-(JP6-B)")
	(net 62 "Net-(U2-OUTN)")
	(net 63 "Net-(U2-OUTP)")
	(net 64 "Net-(MK1-LR)")
	(net 65 "Net-(MK1-SD)")
	(net 66 "unconnected-(U2-NC-Pad13)")
	(net 67 "unconnected-(U2-NC-Pad5)")
	(net 68 "unconnected-(U2-NC-Pad12)")
	(net 69 "unconnected-(U2-NC-Pad6)")
	(net 70 "/~{PCF_INT}")
	(net 71 "/Human-Machine Interface/BCLK")
	(net 72 "/Human-Machine Interface/~{PCF_INT}")
	(net 73 "/Human-Machine Interface/LRCLK")
	(net 74 "/Human-Machine Interface/MIC_DOUT")
	(net 75 "/Human-Machine Interface/~{AMP_SD}")
	(net 76 "/Human-Machine Interface/AMP_DIN")
	(net 77 "Net-(IC1-P0)")
	(footprint "capstone-project:434133025816"
		(layer "F.Cu")
		(at 77.346515 117.191804)
		(property "Reference" "S1"
			(at 0.115985 0.208196 0)
			(layer "F.SilkS")
		)
		(property "Value" "434133025816"
			(at 2.7768 2.7936 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/Human-Machine Interface/Keypad/")
		(sheetfile "../Projects/capstone-project/Hardware/KiCAD/system-testbed/keypad.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -2.075 -1.075)
			(size 1.05 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 12 "Net-(D3:1-A)")
			(pintype "passive")
			(solder_mask_margin 0.102)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd rect
			(at 2.075 -1.075)
			(size 1.05 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 12 "Net-(D3:1-A)")
			(pintype "passive")
			(solder_mask_margin 0.102)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "3" smd rect
			(at -2.075 1.075)
			(size 1.05 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 37 "/Human-Machine Interface/Keypad/ROW3")
			(pintype "passive")
			(solder_mask_margin 0.102)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "4" smd rect
			(at 2.075 1.075)
			(size 1.05 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 37 "/Human-Machine Interface/Keypad/ROW3")
			(pintype "passive")
			(solder_mask_margin 0.102)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "C:/Users/zackp/OneDrive/Desktop/434133025816/Download_STP_4341x30258x6+%28rev1%29.stp"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 90 -180 90)
			)
		)
	)
	(footprint "capstone-project:434133025816"
		(layer "F.Cu")
		(at 92.05 117.2)
		(property "Reference" "S11"
			(at 0.1 -0.1 0)
			(layer "F.SilkS")
		)
		(property "Value" "434133025816"
			(at 2.7768 2.7936 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/Human-Machine Interface/Keypad/")
		(sheetfile "../Projects/capstone-project/Hardware/KiCAD/system-testbed/keypad.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -2.075 -1.075)
			(size 1.05 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 14 "Net-(D3:3-A)")
			(pintype "passive")
			(solder_mask_margin 0.102)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd rect
			(at 2.075 -1.075)
			(size 1.05 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 14 "Net-(D3:3-A)")
			(pintype "passive")
			(solder_mask_margin 0.102)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "3" smd rect
			(at -2.075 1.075)
			(size 1.05 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 37 "/Human-Machine Interface/Keypad/ROW3")
			(pintype "passive")
			(solder_mask_margin 0.102)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "4" smd rect
			(at 2.075 1.075)
			(size 1.05 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 37 "/Human-Machine Interface/Keypad/ROW3")
			(pintype "passive")
			(solder_mask_margin 0.102)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "C:/Users/zackp/OneDrive/Desktop/434133025816/Download_STP_4341x30258x6+%28rev1%29.stp"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 90 -180 90)
			)
		)
	)
	(footprint "capstone-project:PEC11J9215FS0015"
		(layer "F.Cu")
		(at 109.9 115.05 90)
		(descr "PEC11J-9215F-S0015")
		(tags "Undefined or Miscellaneous")
		(property "Reference" "U1"
			(at 2.65 0.987539 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "PEC11J-9215F-S0015"
			(at 0 0.6 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" "http://www.bourns.com/docs/Product-Datasheets/PEC11J.pdf"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Rotary Encoder Mechanical 12 mm SMD Long Life Encoder"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Height" "19.5"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Part Number" "652-PEC11J9215FS0015"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Price/Stock" "https://www.mouser.co.uk/ProductDetail/Bourns/PEC11J-9215F-S0015?qs=11PymoJGorKONEyHv%252BPUyw%3D%3D"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Name" "Bourns"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Part_Number" "PEC11J-9215F-S0015"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/Human-Machine Interface/")
		(sheetfile "human-machine-interface.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 0.6 90)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole circle
			(at 0 0 90)
			(size 2.05 2.05)
			(drill 2.05)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0 4.5 90)
			(size 2.69 2.69)
			(drill 2.69)
			(layers "*.Cu" "*.Mask")
		)
		(pad "A1" smd rect
			(at -2.5 7.3 90)
			(size 1.3 2.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "Net-(C1-Pad1)")
			(pinfunction "A1")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "B1" smd rect
			(at 2.5 7.3 90)
			(size 1.3 2.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 3 "Net-(C2-Pad1)")
			(pinfunction "B1")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "C1" smd rect
			(at 0 7.3 90)
			(size 1.3 2.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 26 "+3.3V")
			(pinfunction "C1")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "D1" smd rect
			(at -2.5 -7 90)
			(size 1.3 2.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "COM")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "E1" smd rect
			(at 2.5 -7 90)
			(size 1.3 2.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 39 "/Human-Machine Interface/ENC_SW")
			(pinfunction "NO")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "MP1" smd rect
			(at -6.375 0 90)
			(size 3.75 4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "MP1")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "MP2" smd rect
			(at 6.375 0 90)
			(size 3.75 4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "MP2")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "MP3" smd rect
			(at -5 -7.9 90)
			(size 2.5 3.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "MP3")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "MP4" smd rect
			(at 5 -7.9 90)
			(size 2.5 3.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "MP4")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "MP5" smd rect
			(at -5 7.9 90)
			(size 2.5 3.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "MP5")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "MP6" smd rect
			(at 5 7.9 90)
			(size 2.5 3.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "MP6")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KIPRJMOD}/capstone-project.pretty/3dmodels/PEC11J-9215F-S0015.step"
			(offset
				(xyz 0 -0.2 2.749999959)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 0 -180)
			)
		)
	)
	(footprint "MountingHole:MountingHole_3.2mm_M3_ISO14580_Pad"
		(layer "F.Cu")
		(at 123.150188 82.499792)
		(descr "Mounting Hole 3.2mm, M3, generated by kicad-footprint-generator mountinghole.py")
		(tags "mountinghole M3 ISO14580")
		(property "Reference" "H1"
			(at 0 -3.7 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "M3"
			(at 0 3.7 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Mounting Hole with connection"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "MountingHole*Pad*")
		(sheetname "/")
		(sheetfile "HMI.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 5.5 5.5)
			(drill 3.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "1")
			(pintype "input")
			(zone_connect 2)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 119.9 86.625 90)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C4"
			(at 2.025 0.1 180)
			(layer "F.SilkS")
		)
		(property "Value" "0.1uF"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "capacitor, US symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/Human-Machine Interface/Audio/")
		(sheetfile "untitled.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 90)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 26 "+3.3V")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at 0.775 0 90)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "capstone-project:434133025816"
		(layer "F.Cu")
		(at 113.263525 98.913525)
		(property "Reference" "S13"
			(at -0.1 0.186475 0)
			(layer "F.SilkS")
		)
		(property "Value" "434133025816"
			(at 2.7768 2.7936 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/Human-Machine Interface/Keypad/")
		(sheetfile "../Projects/capstone-project/Hardware/KiCAD/system-testbed/keypad.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -2.075 -1.075)
			(size 1.05 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 7 "Net-(D1:4-A)")
			(pintype "passive")
			(solder_mask_margin 0.102)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd rect
			(at 2.075 -1.075)
			(size 1.05 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 7 "Net-(D1:4-A)")
			(pintype "passive")
			(solder_mask_margin 0.102)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "3" smd rect
			(at -2.075 1.075)
			(size 1.05 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 42 "/Human-Machine Interface/Keypad/ROW1")
			(pintype "passive")
			(solder_mask_margin 0.102)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "4" smd rect
			(at 2.075 1.075)
			(size 1.05 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 42 "/Human-Machine Interface/Keypad/ROW1")
			(pintype "passive")
			(solder_mask_margin 0.102)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "C:/Users/zackp/OneDrive/Desktop/434133025816/Download_STP_4341x30258x6+%28rev1%29.stp"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 90 -180 90)
			)
		)
	)
	(footprint "capstone-project:434133025816"
		(layer "F.Cu")
		(at 84.6834 107.9)
		(property "Reference" "S5"
			(at 0.15 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "434133025816"
			(at 2.7768 2.7936 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/Human-Machine Interface/Keypad/")
		(sheetfile "../Projects/capstone-project/Hardware/KiCAD/system-testbed/keypad.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -2.075 -1.075)
			(size 1.05 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 5 "Net-(D1:2-A)")
			(pintype "passive")
			(solder_mask_margin 0.102)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd rect
			(at 2.075 -1.075)
			(size 1.05 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 5 "Net-(D1:2-A)")
			(pintype "passive")
			(solder_mask_margin 0.102)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "3" smd rect
			(at -2.075 1.075)
			(size 1.05 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 42 "/Human-Machine Interface/Keypad/ROW1")
			(pintype "passive")
			(solder_mask_margin 0.102)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "4" smd rect
			(at 2.075 1.075)
			(size 1.05 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 42 "/Human-Machine Interface/Keypad/ROW1")
			(pintype "passive")
			(solder_mask_margin 0.102)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "C:/Users/zackp/OneDrive/Desktop/434133025816/Download_STP_4341x30258x6+%28rev1%29.stp"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 90 -180 90)
			)
		)
	)
	(footprint "capstone-project:434133025816"
		(layer "F.Cu")
		(at 101.078012 98.883471)
		(property "Reference" "S16"
			(at 0.15 0.016529 0)
			(layer "F.SilkS")
		)
		(property "Value" "434133025816"
			(at 2.7768 2.7936 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/Human-Machine Interface/Keypad/")
		(sheetfile "../Projects/capstone-project/Hardware/KiCAD/system-testbed/keypad.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -2.075 -1.075)
			(size 1.05 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 19 "Net-(D4:4-A)")
			(pintype "passive")
			(solder_mask_margin 0.102)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd rect
			(at 2.075 -1.075)
			(size 1.05 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 19 "Net-(D4:4-A)")
			(pintype "passive")
			(solder_mask_margin 0.102)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "3" smd rect
			(at -2.075 1.075)
			(size 1.05 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 43 "/Human-Machine Interface/Keypad/ROW4")
			(pintype "passive")
			(solder_mask_margin 0.102)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "4" smd rect
			(at 2.075 1.075)
			(size 1.05 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 43 "/Human-Machine Interface/Keypad/ROW4")
			(pintype "passive")
			(solder_mask_margin 0.102)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "C:/Users/zackp/OneDrive/Desktop/434133025816/Download_STP_4341x30258x6+%28rev1%29.stp"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 90 -180 90)
			)
		)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "F.Cu")
		(at 110.5 79.8)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "Vin"
			(at 1.9 0.1 0)
			(layer "F.SilkS")
		)
		(property "Value" "TestPoint"
			(at 0 1.55 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/Human-Machine Interface/")
		(sheetfile "human-machine-interface.kicad_sch")
		(attr exclude_from_pos_files)
		(pad "1" smd circle
			(at 0 0)
			(size 1 1)
			(layers "F.Cu" "F.Mask")
			(net 26 "+3.3V")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "capstone-project:434133025816"
		(layer "F.Cu")
		(at 77.3625 107.8)
		(property "Reference" "S2"
			(at 0.15 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "434133025816"
			(at 2.7768 2.7936 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/Human-Machine Interface/Keypad/")
		(sheetfile "../Projects/capstone-project/Hardware/KiCAD/system-testbed/keypad.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -2.075 -1.075)
			(size 1.05 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 4 "Net-(D1:1-A)")
			(pintype "passive")
			(solder_mask_margin 0.102)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd rect
			(at 2.075 -1.075)
			(size 1.05 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 4 "Net-(D1:1-A)")
			(pintype "passive")
			(solder_mask_margin 0.102)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "3" smd rect
			(at -2.075 1.075)
			(size 1.05 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 42 "/Human-Machine Interface/Keypad/ROW1")
			(pintype "passive")
			(solder_mask_margin 0.102)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "4" smd rect
			(at 2.075 1.075)
			(size 1.05 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 42 "/Human-Machine Interface/Keypad/ROW1")
			(pintype "passive")
			(solder_mask_margin 0.102)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "C:/Users/zackp/OneDrive/Desktop/434133025816/Download_STP_4341x30258x6+%28rev1%29.stp"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 90 -180 90)
			)
		)
	)
	(footprint "LOGO"
		(layer "F.Cu")
		(at 67.159616 130.688892)
		(property "Reference" "G***"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "LOGO"
			(at 0.75 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr board_only exclude_from_pos_files exclude_from_bom)
		(embedded_fonts no)
	)
	(footprint "LOGO"
		(layer "F.Cu")
		(at 127 129.9)
		(property "Reference" "G***"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "LOGO"
			(at 0.75 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr board_only exclude_from_pos_files exclude_from_bom)
		(embedded_fonts no)
	)
	(footprint "capstone-project:434133025816"
		(layer "F.Cu")
		(at 92.05 112.55)
		(property "Reference" "S10"
			(at 0.1 -0.15 0)
			(layer "F.SilkS")
		)
		(property "Value" "434133025816"
			(at 2.7768 2.7936 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/Human-Machine Interface/Keypad/")
		(sheetfile "../Projects/capstone-project/Hardware/KiCAD/system-testbed/keypad.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -2.075 -1.075)
			(size 1.05 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 10 "Net-(D2:3-A)")
			(pintype "passive")
			(solder_mask_margin 0.102)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd rect
			(at 2.075 -1.075)
			(size 1.05 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 10 "Net-(D2:3-A)")
			(pintype "passive")
			(solder_mask_margin 0.102)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "3" smd rect
			(at -2.075 1.075)
			(size 1.05 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 41 "/Human-Machine Interface/Keypad/ROW2")
			(pintype "passive")
			(solder_mask_margin 0.102)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "4" smd rect
			(at 2.075 1.075)
			(size 1.05 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 41 "/Human-Machine Interface/Keypad/ROW2")
			(pintype "passive")
			(solder_mask_margin 0.102)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "C:/Users/zackp/OneDrive/Desktop/434133025816/Download_STP_4341x30258x6+%28rev1%29.stp"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 90 -180 90)
			)
		)
	)
	(footprint "Package_DFN_QFN:TQFN-16-1EP_3x3mm_P0.5mm_EP1.23x1.23mm"
		(layer "F.Cu")
		(at 126.79 122.99)
		(descr "TQFN, 16 Pin (https://pdfserv.maximintegrated.com/package_dwgs/21-0136.PDF (T1633-5), https://pdfserv.maximintegrated.com/land_patterns/90-0032.PDF), generated with kicad-footprint-generator ipc_noLead_generator.py")
		(tags "TQFN NoLead")
		(property "Reference" "U2"
			(at -1.99 2.31 0)
			(layer "F.SilkS")
		)
		(property "Value" "MAX98357A"
			(at 0 2.8 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/MAX98357A-MAX98357B.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Mono DAC with amplifier, I2S, PCM, TDM, 32-bit, 96khz, 3.2W, TQFP-16"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TQFN*3x3mm*P0.5mm*EP1.23x1.23mm*")
		(sheetname "/Human-Machine Interface/Audio/")
		(sheetfile "untitled.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "" smd roundrect
			(at -0.31 -0.31)
			(size 0.5 0.5)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "" smd roundrect
			(at -0.31 0.31)
			(size 0.5 0.5)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "" smd roundrect
			(at 0.31 -0.31)
			(size 0.5 0.5)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "" smd roundrect
			(at 0.31 0.31)
			(size 0.5 0.5)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "1" smd roundrect
			(at -1.4375 -0.75)
			(size 0.825 0.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 76 "/Human-Machine Interface/AMP_DIN")
			(pinfunction "DIN")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at -1.4375 -0.25)
			(size 0.825 0.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 60 "/Human-Machine Interface/Audio/GAIN_SLOT")
			(pinfunction "GAIN_SLOT")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "3" smd roundrect
			(at -1.4375 0.25)
			(size 0.825 0.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "4" smd roundrect
			(at -1.4375 0.75)
			(size 0.825 0.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 59 "/Human-Machine Interface/Audio/~{SD_MODE}")
			(pinfunction "~{SD_MODE}")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "5" smd roundrect
			(at -0.75 1.4375)
			(size 0.25 0.825)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 67 "unconnected-(U2-NC-Pad5)")
			(pinfunction "NC")
			(pintype "no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "6" smd roundrect
			(at -0.25 1.4375)
			(size 0.25 0.825)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 69 "unconnected-(U2-NC-Pad6)")
			(pinfunction "NC")
			(pintype "no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "7" smd roundrect
			(at 0.25 1.4375)
			(size 0.25 0.825)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 26 "+3.3V")
			(pinfunction "VDD")
			(pintype "power_in")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "8" smd roundrect
			(at 0.75 1.4375)
			(size 0.25 0.825)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 26 "+3.3V")
			(pinfunction "VDD")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "9" smd roundrect
			(at 1.4375 0.75)
			(size 0.825 0.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 63 "Net-(U2-OUTP)")
			(pinfunction "OUTP")
			(pintype "output")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "10" smd roundrect
			(at 1.4375 0.25)
			(size 0.825 0.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 62 "Net-(U2-OUTN)")
			(pinfunction "OUTN")
			(pintype "output")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "11" smd roundrect
			(at 1.4375 -0.25)
			(size 0.825 0.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "12" smd roundrect
			(at 1.4375 -0.75)
			(size 0.825 0.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 68 "unconnected-(U2-NC-Pad12)")
			(pinfunction "NC")
			(pintype "no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "13" smd roundrect
			(at 0.75 -1.4375)
			(size 0.25 0.825)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 66 "unconnected-(U2-NC-Pad13)")
			(pinfunction "NC")
			(pintype "no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "14" smd roundrect
			(at 0.25 -1.4375)
			(size 0.25 0.825)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 73 "/Human-Machine Interface/LRCLK")
			(pinfunction "LRCLK")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "15" smd roundrect
			(at -0.25 -1.4375)
			(size 0.25 0.825)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "16" smd roundrect
			(at -0.75 -1.4375)
			(size 0.25 0.825)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 71 "/Human-Machine Interface/BCLK")
			(pinfunction "BCLK")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "17" smd rect
			(at 0 0)
			(size 1.23 1.23)
			(property pad_prop_heatsink)
			(layers "F.Cu" "F.Mask")
			(net 1 "GND")
			(pinfunction "PAD")
			(pintype "unspecified")
			(zone_connect 2)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Package_DFN_QFN.3dshapes/TQFN-16-1EP_3x3mm_P0.5mm_EP1.23x1.23mm.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 126.8 117.4)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C7"
			(at 0.14058 1.5 0)
			(layer "F.SilkS")
		)
		(property "Value" "22pF"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/Human-Machine Interface/Audio/")
		(sheetfile "untitled.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 71 "/Human-Machine Interface/BCLK")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at 0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "F.Cu")
		(at 109 82.9)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TPAMP1"
			(at 3.2 0.1 0)
			(layer "F.SilkS")
		)
		(property "Value" "~"
			(at 0 1.55 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/Human-Machine Interface/Audio/")
		(sheetfile "untitled.kicad_sch")
		(attr exclude_from_pos_files)
		(pad "1" smd circle
			(at 0 0)
			(size 1 1)
			(layers "F.Cu" "F.Mask")
			(net 76 "/Human-Machine Interface/AMP_DIN")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "LOGO"
		(layer "F.Cu")
		(at 125.8 86.9)
		(property "Reference" "G***"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "LOGO"
			(at 0.75 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr board_only exclude_from_pos_files exclude_from_bom)
		(embedded_fonts no)
	)
	(footprint "capstone-project:434133025816"
		(layer "F.Cu")
		(at 107.209703 102.886475)
		(property "Reference" "S15"
			(at -0.009703 0.013525 0)
			(layer "F.SilkS")
		)
		(property "Value" "434133025816"
			(at 2.7768 2.7936 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/Human-Machine Interface/Keypad/")
		(sheetfile "../Projects/capstone-project/Hardware/KiCAD/system-testbed/keypad.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -2.075 -1.075)
			(size 1.05 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 15 "Net-(D3:4-A)")
			(pintype "passive")
			(solder_mask_margin 0.102)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd rect
			(at 2.075 -1.075)
			(size 1.05 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 15 "Net-(D3:4-A)")
			(pintype "passive")
			(solder_mask_margin 0.102)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "3" smd rect
			(at -2.075 1.075)
			(size 1.05 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 37 "/Human-Machine Interface/Keypad/ROW3")
			(pintype "passive")
			(solder_mask_margin 0.102)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "4" smd rect
			(at 2.075 1.075)
			(size 1.05 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 37 "/Human-Machine Interface/Keypad/ROW3")
			(pintype "passive")
			(solder_mask_margin 0.102)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "C:/Users/zackp/OneDrive/Desktop/434133025816/Download_STP_4341x30258x6+%28rev1%29.stp"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 90 -180 90)
			)
		)
	)
	(footprint "capstone-project:434133025816"
		(layer "F.Cu")
		(at 92.05 121.85)
		(property "Reference" "S12"
			(at 0.1 -0.05 0)
			(layer "F.SilkS")
		)
		(property "Value" "434133025816"
			(at 2.7768 2.7936 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/Human-Machine Interface/Keypad/")
		(sheetfile "../Projects/capstone-project/Hardware/KiCAD/system-testbed/keypad.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -2.075 -1.075)
			(size 1.05 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 18 "Net-(D4:3-A)")
			(pintype "passive")
			(solder_mask_margin 0.102)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd rect
			(at 2.075 -1.075)
			(size 1.05 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 18 "Net-(D4:3-A)")
			(pintype "passive")
			(solder_mask_margin 0.102)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "3" smd rect
			(at -2.075 1.075)
			(size 1.05 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 43 "/Human-Machine Interface/Keypad/ROW4")
			(pintype "passive")
			(solder_mask_margin 0.102)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "4" smd rect
			(at 2.075 1.075)
			(size 1.05 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 43 "/Human-Machine Interface/Keypad/ROW4")
			(pintype "passive")
			(solder_mask_margin 0.102)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "C:/Users/zackp/OneDrive/Desktop/434133025816/Download_STP_4341x30258x6+%28rev1%29.stp"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 90 -180 90)
			)
		)
	)
	(footprint "capstone-project:434133025816"
		(layer "F.Cu")
		(at 77.3625 112.5)
		(property "Reference" "S3"
			(at 0.15 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "434133025816"
			(at 2.7768 2.7936 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/Human-Machine Interface/Keypad/")
		(sheetfile "../Projects/capstone-project/Hardware/KiCAD/system-testbed/keypad.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -2.075 -1.075)
			(size 1.05 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 8 "Net-(D2:1-A)")
			(pintype "passive")
			(solder_mask_margin 0.102)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd rect
			(at 2.075 -1.075)
			(size 1.05 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 8 "Net-(D2:1-A)")
			(pintype "passive")
			(solder_mask_margin 0.102)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "3" smd rect
			(at -2.075 1.075)
			(size 1.05 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 41 "/Human-Machine Interface/Keypad/ROW2")
			(pintype "passive")
			(solder_mask_margin 0.102)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "4" smd rect
			(at 2.075 1.075)
			(size 1.05 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 41 "/Human-Machine Interface/Keypad/ROW2")
			(pintype "passive")
			(solder_mask_margin 0.102)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "C:/Users/zackp/OneDrive/Desktop/434133025816/Download_STP_4341x30258x6+%28rev1%29.stp"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 90 -180 90)
			)
		)
	)
	(footprint "capstone-project:434133025816"
		(layer "F.Cu")
		(at 77.346515 121.841804)
		(property "Reference" "S4"
			(at 0.15 -0.041804 0)
			(layer "F.SilkS")
		)
		(property "Value" "434133025816"
			(at 2.7768 2.7936 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/Human-Machine Interface/Keypad/")
		(sheetfile "../Projects/capstone-project/Hardware/KiCAD/system-testbed/keypad.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -2.075 -1.075)
			(size 1.05 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 16 "Net-(D4:1-A)")
			(pintype "passive")
			(solder_mask_margin 0.102)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd rect
			(at 2.075 -1.075)
			(size 1.05 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 16 "Net-(D4:1-A)")
			(pintype "passive")
			(solder_mask_margin 0.102)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "3" smd rect
			(at -2.075 1.075)
			(size 1.05 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 43 "/Human-Machine Interface/Keypad/ROW4")
			(pintype "passive")
			(solder_mask_margin 0.102)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "4" smd rect
			(at 2.075 1.075)
			(size 1.05 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 43 "/Human-Machine Interface/Keypad/ROW4")
			(pintype "passive")
			(solder_mask_margin 0.102)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "C:/Users/zackp/OneDrive/Desktop/434133025816/Download_STP_4341x30258x6+%28rev1%29.stp"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 90 -180 90)
			)
		)
	)
	(footprint "capstone-project:434133025816"
		(layer "F.Cu")
		(at 92.05 107.9)
		(property "Reference" "S9"
			(at 0.15 -0.1 0)
			(layer "F.SilkS")
		)
		(property "Value" "434133025816"
			(at 2.7768 2.7936 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/Human-Machine Interface/Keypad/")
		(sheetfile "../Projects/capstone-project/Hardware/KiCAD/system-testbed/keypad.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -2.075 -1.075)
			(size 1.05 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 6 "Net-(D1:3-A)")
			(pintype "passive")
			(solder_mask_margin 0.102)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd rect
			(at 2.075 -1.075)
			(size 1.05 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 6 "Net-(D1:3-A)")
			(pintype "passive")
			(solder_mask_margin 0.102)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "3" smd rect
			(at -2.075 1.075)
			(size 1.05 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 42 "/Human-Machine Interface/Keypad/ROW1")
			(pintype "passive")
			(solder_mask_margin 0.102)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "4" smd rect
			(at 2.075 1.075)
			(size 1.05 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 42 "/Human-Machine Interface/Keypad/ROW1")
			(pintype "passive")
			(solder_mask_margin 0.102)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "C:/Users/zackp/OneDrive/Desktop/434133025816/Download_STP_4341x30258x6+%28rev1%29.stp"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 90 -180 90)
			)
		)
	)
	(footprint "Package_SO:SSOP-24_5.3x8.2mm_P0.65mm"
		(layer "F.Cu")
		(at 87 95 -90)
		(descr "SSOP, 24 Pin (JEDEC MO-150 variation AG, 1.75mm body thickness, https://www.jedec.org/document_search?search_api_views_fulltext=MO-150, https://ww1.microchip.com/downloads/en/PackagingSpec/00000049BQ.pdf#page=398, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/ltc-legacy-ssop/ssop_24_05-08-1640.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SSOP SO")
		(property "Reference" "IC1"
			(at 0 -5.05 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "PCF8575PWR"
			(at 0 5.05 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/pcf8575.pdf"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "16 Bits Port/Expander to I2C Bus, SSOP-24"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Height" "1.2"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Name" "Texas Instruments"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Part_Number" "PCF8575PWR"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Part Number" "595-PCF8575PWR"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Price/Stock" "https://www.mouser.co.uk/ProductDetail/Texas-Instruments/PCF8575PWR?qs=wgAEGBTxy7lfNLEoaenBaA%3D%3D"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Arrow Part Number" "PCF8575PWR"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Arrow Price/Stock" "https://www.arrow.com/en/products/pcf8575pwr/texas-instruments?region=nac"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SSOP*5.3x8.2mm*P0.65mm*")
		(sheetname "/Human-Machine Interface/")
		(sheetfile "human-machine-interface.kicad_sch")
		(attr smd)
		(pad "1" smd roundrect
			(at -3.5 -3.575 270)
			(size 1.9 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 72 "/Human-Machine Interface/~{PCF_INT}")
			(pinfunction "~{INT}")
			(pintype "open_collector")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at -3.5 -2.925 270)
			(size 1.9 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 56 "/Human-Machine Interface/PCF_A1")
			(pinfunction "A1")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "3" smd roundrect
			(at -3.5 -2.275 270)
			(size 1.9 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 54 "/Human-Machine Interface/PCF_A2")
			(pinfunction "A2")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "4" smd roundrect
			(at -3.5 -1.625 270)
			(size 1.9 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 77 "Net-(IC1-P0)")
			(pinfunction "P0")
			(pintype "bidirectional")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "5" smd roundrect
			(at -3.5 -0.975 270)
			(size 1.9 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 57 "unconnected-(IC1-P1-Pad5)")
			(pinfunction "P1")
			(pintype "bidirectional+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "6" smd roundrect
			(at -3.5 -0.325 270)
			(size 1.9 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 38 "/Human-Machine Interface/TFTRST")
			(pinfunction "P2")
			(pintype "bidirectional")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "7" smd roundrect
			(at -3.5 0.325 270)
			(size 1.9 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 20 "unconnected-(IC1-P3-Pad7)")
			(pinfunction "P3")
			(pintype "bidirectional")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "8" smd roundrect
			(at -3.5 0.975 270)
			(size 1.9 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 21 "unconnected-(IC1-P4-Pad8)")
			(pinfunction "P4")
			(pintype "bidirectional")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "9" smd roundrect
			(at -3.5 1.625 270)
			(size 1.9 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 39 "/Human-Machine Interface/ENC_SW")
			(pinfunction "P5")
			(pintype "bidirectional")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "10" smd roundrect
			(at -3.5 2.275 270)
			(size 1.9 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 44 "/Human-Machine Interface/ENC_DT")
			(pinfunction "P6")
			(pintype "bidirectional")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "11" smd roundrect
			(at -3.5 2.925 270)
			(size 1.9 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 40 "/Human-Machine Interface/ENC_CLK")
			(pinfunction "P7")
			(pintype "bidirectional")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "12" smd roundrect
			(at -3.5 3.575 270)
			(size 1.9 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "13" smd roundrect
			(at 3.5 3.575 270)
			(size 1.9 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 42 "/Human-Machine Interface/Keypad/ROW1")
			(pinfunction "P10")
			(pintype "bidirectional")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "14" smd roundrect
			(at 3.5 2.925 270)
			(size 1.9 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 41 "/Human-Machine Interface/Keypad/ROW2")
			(pinfunction "P11")
			(pintype "bidirectional")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "15" smd roundrect
			(at 3.5 2.275 270)
			(size 1.9 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 37 "/Human-Machine Interface/Keypad/ROW3")
			(pinfunction "P12")
			(pintype "bidirectional")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "16" smd roundrect
			(at 3.5 1.625 270)
			(size 1.9 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 43 "/Human-Machine Interface/Keypad/ROW4")
			(pinfunction "P13")
			(pintype "bidirectional")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "17" smd roundrect
			(at 3.5 0.975 270)
			(size 1.9 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 33 "/Human-Machine Interface/Keypad/COL1")
			(pinfunction "P14")
			(pintype "bidirectional")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "18" smd roundrect
			(at 3.5 0.325 270)
			(size 1.9 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 34 "/Human-Machine Interface/Keypad/COL2")
			(pinfunction "P15")
			(pintype "bidirectional")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "19" smd roundrect
			(at 3.5 -0.325 270)
			(size 1.9 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 35 "/Human-Machine Interface/Keypad/COL3")
			(pinfunction "P16")
			(pintype "bidirectional")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "20" smd roundrect
			(at 3.5 -0.975 270)
			(size 1.9 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 36 "/Human-Machine Interface/Keypad/COL4")
			(pinfunction "P17")
			(pintype "bidirectional")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "21" smd roundrect
			(at 3.5 -1.625 270)
			(size 1.9 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 55 "/Human-Machine Interface/PCF_A0")
			(pinfunction "A0")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "22" smd roundrect
			(at 3.5 -2.275 270)
			(size 1.9 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 23 "/SCL")
			(pinfunction "SCL")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "23" smd roundrect
			(at 3.5 -2.925 270)
			(size 1.9 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 22 "/SDA")
			(pinfunction "SDA")
			(pintype "bidirectional")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "24" smd roundrect
			(at 3.5 -3.575 270)
			(size 1.9 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 26 "+3.3V")
			(pinfunction "VCC")
			(pintype "power_in")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Package_SO.3dshapes/SSOP-24_5.3x8.2mm_P0.65mm.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "capstone-project:434133025816"
		(layer "F.Cu")
		(at 84.6834 117.2)
		(property "Reference" "S7"
			(at 0.1 -0.1 0)
			(layer "F.SilkS")
		)
		(property "Value" "434133025816"
			(at 2.7768 2.7936 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/Human-Machine Interface/Keypad/")
		(sheetfile "../Projects/capstone-project/Hardware/KiCAD/system-testbed/keypad.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -2.075 -1.075)
			(size 1.05 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 13 "Net-(D3:2-A)")
			(pintype "passive")
			(solder_mask_margin 0.102)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd rect
			(at 2.075 -1.075)
			(size 1.05 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 13 "Net-(D3:2-A)")
			(pintype "passive")
			(solder_mask_margin 0.102)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "3" smd rect
			(at -2.075 1.075)
			(size 1.05 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 37 "/Human-Machine Interface/Keypad/ROW3")
			(pintype "passive")
			(solder_mask_margin 0.102)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "4" smd rect
			(at 2.075 1.075)
			(size 1.05 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 37 "/Human-Machine Interface/Keypad/ROW3")
			(pintype "passive")
			(solder_mask_margin 0.102)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "C:/Users/zackp/OneDrive/Desktop/434133025816/Download_STP_4341x30258x6+%28rev1%29.stp"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 90 -180 90)
			)
		)
	)
	(footprint "capstone-project:434133025816"
		(layer "F.Cu")
		(at 84.6834 121.85)
		(property "Reference" "S8"
			(at 0.1 -0.15 0)
			(layer "F.SilkS")
		)
		(property "Value" "434133025816"
			(at 2.7768 2.7936 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/Human-Machine Interface/Keypad/")
		(sheetfile "../Projects/capstone-project/Hardware/KiCAD/system-testbed/keypad.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -2.075 -1.075)
			(size 1.05 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 17 "Net-(D4:2-A)")
			(pintype "passive")
			(solder_mask_margin 0.102)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd rect
			(at 2.075 -1.075)
			(size 1.05 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 17 "Net-(D4:2-A)")
			(pintype "passive")
			(solder_mask_margin 0.102)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "3" smd rect
			(at -2.075 1.075)
			(size 1.05 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 43 "/Human-Machine Interface/Keypad/ROW4")
			(pintype "passive")
			(solder_mask_margin 0.102)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "4" smd rect
			(at 2.075 1.075)
			(size 1.05 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 43 "/Human-Machine Interface/Keypad/ROW4")
			(pintype "passive")
			(solder_mask_margin 0.102)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "C:/Users/zackp/OneDrive/Desktop/434133025816/Download_STP_4341x30258x6+%28rev1%29.stp"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 90 -180 90)
			)
		)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "F.Cu")
		(at 80.2 82.2)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP1"
			(at 0 -1.448 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 1.55 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/Human-Machine Interface/")
		(sheetfile "human-machine-interface.kicad_sch")
		(attr exclude_from_pos_files)
		(fp_text user "${REFERENCE}"
			(at 0 -1.45 0)
			(layer "F.Fab")
		)
		(pad "1" smd circle
			(at 0 0)
			(size 1 1)
			(layers "F.Cu" "F.Mask")
			(net 45 "/Human-Machine Interface/LITE")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "capstone-project:434133025816"
		(layer "F.Cu")
		(at 107.196315 94.907244)
		(property "Reference" "S14"
			(at 0.003685 0.092756 0)
			(layer "F.SilkS")
		)
		(property "Value" "434133025816"
			(at 2.7768 2.7936 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/Human-Machine Interface/Keypad/")
		(sheetfile "../Projects/capstone-project/Hardware/KiCAD/system-testbed/keypad.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -2.075 -1.075)
			(size 1.05 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 11 "Net-(D2:4-A)")
			(pintype "passive")
			(solder_mask_margin 0.102)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd rect
			(at 2.075 -1.075)
			(size 1.05 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 11 "Net-(D2:4-A)")
			(pintype "passive")
			(solder_mask_margin 0.102)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "3" smd rect
			(at -2.075 1.075)
			(size 1.05 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 41 "/Human-Machine Interface/Keypad/ROW2")
			(pintype "passive")
			(solder_mask_margin 0.102)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "4" smd rect
			(at 2.075 1.075)
			(size 1.05 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 41 "/Human-Machine Interface/Keypad/ROW2")
			(pintype "passive")
			(solder_mask_margin 0.102)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "C:/Users/zackp/OneDrive/Desktop/434133025816/Download_STP_4341x30258x6+%28rev1%29.stp"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 90 -180 90)
			)
		)
	)
	(footprint "MountingHole:MountingHole_3.2mm_M3_ISO14580_Pad"
		(layer "F.Cu")
		(at 70.963353 82.499941)
		(descr "Mounting Hole 3.2mm, M3, generated by kicad-footprint-generator mountinghole.py")
		(tags "mountinghole M3 ISO14580")
		(property "Reference" "H2"
			(at 0 -3.7 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "M3"
			(at 0 3.7 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Mounting Hole with connection"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "MountingHole*Pad*")
		(sheetname "/")
		(sheetfile "HMI.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 5.5 5.5)
			(drill 3.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "1")
			(pintype "input")
			(zone_connect 2)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
	)
	(footprint "capstone-project:434133025816"
		(layer "F.Cu")
		(at 84.6834 112.55)
		(property "Reference" "S6"
			(at 0.1 -0.05 0)
			(layer "F.SilkS")
		)
		(property "Value" "434133025816"
			(at 2.7768 2.7936 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/Human-Machine Interface/Keypad/")
		(sheetfile "../Projects/capstone-project/Hardware/KiCAD/system-testbed/keypad.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -2.075 -1.075)
			(size 1.05 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 9 "Net-(D2:2-A)")
			(pintype "passive")
			(solder_mask_margin 0.102)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd rect
			(at 2.075 -1.075)
			(size 1.05 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 9 "Net-(D2:2-A)")
			(pintype "passive")
			(solder_mask_margin 0.102)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "3" smd rect
			(at -2.075 1.075)
			(size 1.05 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 41 "/Human-Machine Interface/Keypad/ROW2")
			(pintype "passive")
			(solder_mask_margin 0.102)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "4" smd rect
			(at 2.075 1.075)
			(size 1.05 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 41 "/Human-Machine Interface/Keypad/ROW2")
			(pintype "passive")
			(solder_mask_margin 0.102)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "C:/Users/zackp/OneDrive/Desktop/434133025816/Download_STP_4341x30258x6+%28rev1%29.stp"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 90 -180 90)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 118.3 86.625 90)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C3"
			(at 2.025 0 180)
			(layer "F.SilkS")
		)
		(property "Value" "1uF"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "capacitor, US symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/Human-Machine Interface/Audio/")
		(sheetfile "untitled.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 90)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 26 "+3.3V")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at 0.775 0 90)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Diode_SMD:D_0603_1608Metric"
		(layer "B.Cu")
		(at 84.6625 117.258 180)
		(descr "Diode SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
		(tags "diode")
		(property "Reference" "D3:2"
			(at 0 1.43 0)
			(layer "B.SilkS")
		)
		(property "Value" "D"
			(at 0 -1.43 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Diode, small symbol, filled shape"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sim.Device" "D"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TO-???* *_Diode_* *SingleDiode* D_*")
		(sheetname "/Human-Machine Interface/Keypad/")
		(sheetfile "../Projects/capstone-project/Hardware/KiCAD/system-testbed/keypad.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.7875 0 180)
			(size 0.875 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 34 "/Human-Machine Interface/Keypad/COL2")
			(pinfunction "K")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at 0.7875 0 180)
			(size 0.875 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 13 "Net-(D3:2-A)")
			(pinfunction "A")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Diode_SMD.3dshapes/D_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "capstone-project:Adafruit EYESPI FPC Connector"
		(layer "B.Cu")
		(at 86.360249 81.668651)
		(descr "WR-FPC SMT ZIF Horizontal Hinge Type")
		(tags "EYESPI, FPC")
		(property "Reference" "X2"
			(at 7.874 -2.032 0)
			(layer "B.SilkS")
		)
		(property "Value" "EYESPI"
			(at 0 -4.064 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "https://www.we-online.com/components/products/datasheet/687118149022.pdf"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "WR-FPC SMT ZIF Horizontal Hinge Type"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(sheetname "/Human-Machine Interface/")
		(sheetfile "human-machine-interface.kicad_sch")
		(attr smd allow_soldermask_bridges)
		(pad "1" smd rect
			(at -4.25 3.35)
			(size 0.3 1.3)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 26 "+3.3V")
			(pintype "passive")
			(solder_mask_margin 0.102)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd rect
			(at -3.75 3.35)
			(size 0.3 1.3)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 45 "/Human-Machine Interface/LITE")
			(pintype "passive")
			(solder_mask_margin 0.102)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "3" smd rect
			(at -3.25 3.35)
			(size 0.3 1.3)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 1 "GND")
			(pintype "passive")
			(solder_mask_margin 0.102)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "4" smd rect
			(at -2.75 3.35)
			(size 0.3 1.3)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 30 "/SCK")
			(pintype "passive")
			(solder_mask_margin 0.102)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "5" smd rect
			(at -2.25 3.35)
			(size 0.3 1.3)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 32 "/MOSI")
			(pintype "passive")
			(solder_mask_margin 0.102)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "6" smd rect
			(at -1.75 3.35)
			(size 0.3 1.3)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 29 "/MISO")
			(pintype "passive")
			(solder_mask_margin 0.102)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "7" smd rect
			(at -1.25 3.35)
			(size 0.3 1.3)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 24 "/TFTDC")
			(pintype "passive")
			(solder_mask_margin 0.102)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "8" smd rect
			(at -0.75 3.35)
			(size 0.3 1.3)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 38 "/Human-Machine Interface/TFTRST")
			(pintype "passive")
			(solder_mask_margin 0.102)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "9" smd rect
			(at -0.25 3.35)
			(size 0.3 1.3)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 27 "/TFTCS")
			(pintype "passive")
			(solder_mask_margin 0.102)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "10" smd rect
			(at 0.25 3.35)
			(size 0.3 1.3)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 28 "/CARDCS")
			(pintype "passive")
			(solder_mask_margin 0.102)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "11" smd rect
			(at 0.75 3.35)
			(size 0.3 1.3)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 50 "unconnected-(X2-Pad11)")
			(pintype "passive+no_connect")
			(solder_mask_margin 0.102)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "12" smd rect
			(at 1.25 3.35)
			(size 0.3 1.3)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 49 "unconnected-(X2-Pad12)")
			(pintype "passive+no_connect")
			(solder_mask_margin 0.102)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "13" smd rect
			(at 1.75 3.35)
			(size 0.3 1.3)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 52 "unconnected-(X2-Pad13)")
			(pintype "passive+no_connect")
			(solder_mask_margin 0.102)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "14" smd rect
			(at 2.25 3.35)
			(size 0.3 1.3)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 47 "unconnected-(X2-Pad14)")
			(pintype "passive+no_connect")
			(solder_mask_margin 0.102)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "15" smd rect
			(at 2.75 3.35)
			(size 0.3 1.3)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 46 "unconnected-(X2-Pad15)")
			(pintype "passive+no_connect")
			(solder_mask_margin 0.102)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "16" smd rect
			(at 3.25 3.35)
			(size 0.3 1.3)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 48 "unconnected-(X2-Pad16)")
			(pintype "passive+no_connect")
			(solder_mask_margin 0.102)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "17" smd rect
			(at 3.75 3.35)
			(size 0.3 1.3)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 51 "unconnected-(X2-Pad17)")
			(pintype "passive+no_connect")
			(solder_mask_margin 0.102)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "18" smd rect
			(at 4.25 3.35)
			(size 0.3 1.3)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 53 "unconnected-(X2-Pad18)")
			(pintype "passive+no_connect")
			(solder_mask_margin 0.102)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "Z1" smd rect
			(at -6.05 0.6)
			(size 2 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 1 "GND")
			(pintype "passive")
			(solder_mask_margin 0.102)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "Z2" smd rect
			(at 6.05 0.6)
			(size 2 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 1 "GND")
			(pintype "passive")
			(solder_mask_margin 0.102)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KIPRJMOD}/capstone-project.pretty/3dmodels/687118149022+(rev1).step"
			(offset
				(xyz 0 0.5 1.15)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -0 -0 -0)
			)
		)
	)
	(footprint "Diode_SMD:D_0603_1608Metric"
		(layer "B.Cu")
		(at 92.0041 107.858 180)
		(descr "Diode SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
		(tags "diode")
		(property "Reference" "D1:3"
			(at -0.0459 1.4 0)
			(layer "B.SilkS")
		)
		(property "Value" "D"
			(at 0 -1.43 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Diode, small symbol, filled shape"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sim.Device" "D"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TO-???* *_Diode_* *SingleDiode* D_*")
		(sheetname "/Human-Machine Interface/Keypad/")
		(sheetfile "../Projects/capstone-project/Hardware/KiCAD/system-testbed/keypad.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.7875 0 180)
			(size 0.875 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 35 "/Human-Machine Interface/Keypad/COL3")
			(pinfunction "K")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at 0.7875 0 180)
			(size 0.875 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 6 "Net-(D1:3-A)")
			(pinfunction "A")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Diode_SMD.3dshapes/D_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Sensor_Audio:InvenSense_ICS-43434-6_3.5x2.65mm"
		(layer "B.Cu")
		(at 122.742 87.9 -90)
		(descr "TDK InvenSense MEMS I2S Microphone: https://invensense.tdk.com/products/ics-43434/")
		(tags "microphone MEMS I2S ICS-43434 TDK InvenSense")
		(property "Reference" "MK1"
			(at -0.1 -2.558 90)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "ICS-43434"
			(at 0 -2.9 90)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Datasheet" "https://www.invensense.com/wp-content/uploads/2016/02/DS-000069-ICS-43434-v1.2.pdf"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "TDK InvenSense MEMS Microphone, 24-bit I2S, 65 dBA SNR, LGA-6"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "InvenSense*ICS*43434*")
		(sheetname "/Human-Machine Interface/Audio/")
		(sheetfile "untitled.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -0.01 0)
			(unlocked yes)
			(layer "B.Fab")
		)
		(pad "" np_thru_hole circle
			(at 0 -0.71 270)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "*.Mask")
		)
		(pad "1" smd rect
			(at -0.9 1.364 270)
			(size 0.6 0.522)
			(layers "B.Cu" "B.Mask")
			(net 73 "/Human-Machine Interface/LRCLK")
			(pinfunction "WS")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd rect
			(at -0.9 0.542 270)
			(size 0.6 0.522)
			(layers "B.Cu" "B.Mask")
			(net 64 "Net-(MK1-LR)")
			(pinfunction "LR")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "3" smd custom
			(at 0.6625 -0.71 180)
			(size 0.3 0.3)
			(layers "B.Cu" "B.Mask")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(options
				(clearance outline)
				(anchor circle)
			)
			(primitives
				(gr_circle
					(center 0 0.6625)
					(end 0.6625 0.6625)
					(width 0.3)
					(fill no)
				)
			)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "4" smd rect
			(at 0.9 0.542 270)
			(size 0.6 0.522)
			(layers "B.Cu" "B.Mask")
			(net 71 "/Human-Machine Interface/BCLK")
			(pinfunction "SCK")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "5" smd rect
			(at 0.9 1.364 270)
			(size 0.6 0.522)
			(layers "B.Cu" "B.Mask")
			(net 26 "+3.3V")
			(pinfunction "VDD")
			(pintype "power_in")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "6" smd rect
			(at 0 1.364 270)
			(size 0.6 0.522)
			(layers "B.Cu" "B.Mask")
			(net 65 "Net-(MK1-SD)")
			(pinfunction "SD")
			(pintype "output")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Sensor_Audio.3dshapes/InvenSense_ICS-43434-6_3.5x2.65mm.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "capstone-project:434133025816"
		(layer "B.Cu")
		(at 77.1 88.1 -90)
		(property "Reference" "S17"
			(at -0.1 2.8064 90)
			(layer "B.SilkS")
		)
		(property "Value" "434133025816"
			(at 2.776801 -2.7936 90)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(sheetname "/Human-Machine Interface/")
		(sheetfile "human-machine-interface.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -2.075 1.075 270)
			(size 1.05 0.65)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 26 "+3.3V")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd rect
			(at 2.075 1.075 270)
			(size 1.05 0.65)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 26 "+3.3V")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "3" smd rect
			(at -2.075 -1.075 270)
			(size 1.05 0.65)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 77 "Net-(IC1-P0)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "4" smd rect
			(at 2.075 -1.075 270)
			(size 1.05 0.65)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 77 "Net-(IC1-P0)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
		(model "C:/Users/zackp/OneDrive/Desktop/434133025816/Download_STP_4341x30258x6+%28rev1%29.stp"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 90 -180 90)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "B.Cu")
		(at 113.404634 91.120446 90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R15"
			(at 0 -1.237792 90)
			(layer "B.SilkS")
		)
		(property "Value" "2k"
			(at 0 -1.43 90)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Human-Machine Interface/Audio/")
		(sheetfile "untitled.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 90)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 59 "/Human-Machine Interface/Audio/~{SD_MODE}")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at 0.825 0 90)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 75 "/Human-Machine Interface/~{AMP_SD}")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "B.Cu")
		(at 105.610845 113.535118 -90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R7"
			(at 0 -1.389155 90)
			(layer "B.SilkS")
		)
		(property "Value" "10k"
			(at 0 -1.43 90)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Human-Machine Interface/")
		(sheetfile "human-machine-interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 270)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 3 "Net-(C2-Pad1)")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at 0.825 0 270)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 26 "+3.3V")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Diode_SMD:D_0603_1608Metric"
		(layer "B.Cu")
		(at 84.6625 121.858 180)
		(descr "Diode SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
		(tags "diode")
		(property "Reference" "D4:2"
			(at 0 1.43 0)
			(layer "B.SilkS")
		)
		(property "Value" "D"
			(at 0 -1.43 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Diode, small symbol, filled shape"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sim.Device" "D"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TO-???* *_Diode_* *SingleDiode* D_*")
		(sheetname "/Human-Machine Interface/Keypad/")
		(sheetfile "../Projects/capstone-project/Hardware/KiCAD/system-testbed/keypad.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.7875 0 180)
			(size 0.875 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 34 "/Human-Machine Interface/Keypad/COL2")
			(pinfunction "K")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at 0.7875 0 180)
			(size 0.875 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 17 "Net-(D4:2-A)")
			(pinfunction "A")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Diode_SMD.3dshapes/D_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Diode_SMD:D_0603_1608Metric"
		(layer "B.Cu")
		(at 84.675 107.858 180)
		(descr "Diode SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
		(tags "diode")
		(property "Reference" "D1:2"
			(at -0.0125 1.4 0)
			(layer "B.SilkS")
		)
		(property "Value" "D"
			(at 0 -1.43 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Diode, small symbol, filled shape"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sim.Device" "D"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TO-???* *_Diode_* *SingleDiode* D_*")
		(sheetname "/Human-Machine Interface/Keypad/")
		(sheetfile "../Projects/capstone-project/Hardware/KiCAD/system-testbed/keypad.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.7875 0 180)
			(size 0.875 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 34 "/Human-Machine Interface/Keypad/COL2")
			(pinfunction "K")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at 0.7875 0 180)
			(size 0.875 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 5 "Net-(D1:2-A)")
			(pinfunction "A")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Diode_SMD.3dshapes/D_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Jumper:SolderJumper-3_P1.3mm_Open_RoundedPad1.0x1.5mm_NumberLabels"
		(layer "B.Cu")
		(at 129.1 116.3 -90)
		(descr "SMD Solder 3-pad Jumper, 1x1.5mm rounded Pads, 0.3mm gap, open, labeled with numbers")
		(tags "solder jumper open")
		(property "Reference" "JP6"
			(at 0 -1.9 90)
			(layer "B.SilkS")
		)
		(property "Value" "GAIN_{R}"
			(at 0 -1.9 90)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Solder Jumper, 3-pole, open"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SolderJumper*Open*")
		(sheetname "/Human-Machine Interface/Audio/")
		(sheetfile "untitled.kicad_sch")
		(zone_connect 1)
		(attr exclude_from_pos_files allow_soldermask_bridges)
		(fp_text user "1"
			(at -2.6 0 90)
			(layer "B.SilkS")
		)
		(fp_text user "3"
			(at 2.6 0 90)
			(layer "B.SilkS")
		)
		(pad "1" smd custom
			(at -1.3 0 270)
			(size 1 0.5)
			(layers "B.Cu" "B.Mask")
			(net 58 "Net-(JP4-C)")
			(pinfunction "A")
			(pintype "passive")
			(zone_connect 2)
			(thermal_bridge_angle 45)
			(options
				(clearance outline)
				(anchor rect)
			)
			(primitives
				(gr_circle
					(center 0 -0.25)
					(end 0.5 -0.25)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center 0 0.25)
					(end 0.5 0.25)
					(width 0)
					(fill yes)
				)
				(gr_poly
					(pts
						(xy 0.55 -0.75) (xy 0 -0.75) (xy 0 0.75) (xy 0.55 0.75)
					)
					(width 0)
					(fill yes)
				)
			)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd rect
			(at 0 0 270)
			(size 1 1.5)
			(layers "B.Cu" "B.Mask")
			(net 60 "/Human-Machine Interface/Audio/GAIN_SLOT")
			(pinfunction "C")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "3" smd custom
			(at 1.3 0 270)
			(size 1 0.5)
			(layers "B.Cu" "B.Mask")
			(net 61 "Net-(JP6-B)")
			(pinfunction "B")
			(pintype "passive")
			(zone_connect 2)
			(thermal_bridge_angle 45)
			(options
				(clearance outline)
				(anchor rect)
			)
			(primitives
				(gr_circle
					(center 0 -0.25)
					(end 0.5 -0.25)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center 0 0.25)
					(end 0.5 0.25)
					(width 0)
					(fill yes)
				)
				(gr_poly
					(pts
						(xy 0 -0.75) (xy -0.55 -0.75) (xy -0.55 0.75) (xy 0 0.75)
					)
					(width 0)
					(fill yes)
				)
			)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
	)
	(footprint "Diode_SMD:D_0603_1608Metric"
		(layer "B.Cu")
		(at 101.078012 102.161475 180)
		(descr "Diode SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
		(tags "diode")
		(property "Reference" "D4:4"
			(at 0 1.43 0)
			(layer "B.SilkS")
		)
		(property "Value" "D"
			(at 0 -1.43 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Diode, small symbol, filled shape"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sim.Device" "D"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TO-???* *_Diode_* *SingleDiode* D_*")
		(sheetname "/Human-Machine Interface/Keypad/")
		(sheetfile "../Projects/capstone-project/Hardware/KiCAD/system-testbed/keypad.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.7875 0 180)
			(size 0.875 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 36 "/Human-Machine Interface/Keypad/COL4")
			(pinfunction "K")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at 0.7875 0 180)
			(size 0.875 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 19 "Net-(D4:4-A)")
			(pinfunction "A")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Diode_SMD.3dshapes/D_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "LOGO"
		(layer "B.Cu")
		(at 97.4 123.1 180)
		(property "Reference" "G***"
			(at 0 0 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "LOGO"
			(at 0.75 0 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(attr board_only exclude_from_pos_files exclude_from_bom)
		(embedded_fonts no)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "B.Cu")
		(at 68.5 113.7 -90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R3"
			(at -0.1 -1.4 90)
			(layer "B.SilkS")
		)
		(property "Value" "10k"
			(at 0 -1.43 90)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Human-Machine Interface/")
		(sheetfile "human-machine-interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 270)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 54 "/Human-Machine Interface/PCF_A2")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at 0.825 0 270)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "B.Cu")
		(at 101.695132 112.759843)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R5"
			(at 0 1.2 0)
			(layer "B.SilkS")
		)
		(property "Value" "10k"
			(at 0 -1.43 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Human-Machine Interface/")
		(sheetfile "human-machine-interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 44 "/Human-Machine Interface/ENC_DT")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at 0.825 0)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 3 "Net-(C2-Pad1)")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "B.Cu")
		(at 104.041716 116.674005 90)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C1"
			(at -2.325995 -0.04836 90)
			(layer "B.SilkS")
		)
		(property "Value" "0.01uF"
			(at 0 -1.43 90)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "capacitor, US symbol"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/Human-Machine Interface/")
		(sheetfile "human-machine-interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 90)
			(size 0.9 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 2 "Net-(C1-Pad1)")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at 0.775 0 90)
			(size 0.9 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Jumper:SolderJumper-2_P1.3mm_Open_TrianglePad1.0x1.5mm"
		(layer "B.Cu")
		(at 66 113.45)
		(descr "SMD Solder Jumper, 1x1.5mm Triangular Pads, 0.3mm gap, open")
		(tags "solder jumper open")
		(property "Reference" "JP3"
			(at 0 1.8 0)
			(layer "B.SilkS")
		)
		(property "Value" "SolderJumper_2_Open"
			(at 0 -1.9 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Solder Jumper, 2-pole, open"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SolderJumper*Open*")
		(sheetname "/Human-Machine Interface/")
		(sheetfile "human-machine-interface.kicad_sch")
		(zone_connect 1)
		(attr exclude_from_pos_files exclude_from_bom allow_soldermask_bridges)
		(pad "1" smd custom
			(at -0.725 0)
			(size 0.3 0.3)
			(layers "B.Cu" "B.Mask")
			(net 26 "+3.3V")
			(pinfunction "A")
			(pintype "passive")
			(zone_connect 2)
			(thermal_bridge_angle 45)
			(options
				(clearance outline)
				(anchor rect)
			)
			(primitives
				(gr_poly
					(pts
						(xy 1 0) (xy 0.5 -0.75) (xy -0.5 -0.75) (xy -0.5 0.75) (xy 0.5 0.75)
					)
					(width 0)
					(fill yes)
				)
			)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd custom
			(at 0.725 0)
			(size 0.3 0.3)
			(layers "B.Cu" "B.Mask")
			(net 54 "/Human-Machine Interface/PCF_A2")
			(pinfunction "B")
			(pintype "passive")
			(zone_connect 2)
			(thermal_bridge_angle 45)
			(options
				(clearance outline)
				(anchor rect)
			)
			(primitives
				(gr_poly
					(pts
						(xy 0.5 -0.75) (xy -0.65 -0.75) (xy -0.15 0) (xy -0.65 0.75) (xy 0.5 0.75)
					)
					(width 0)
					(fill yes)
				)
			)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
	)
	(footprint "Diode_SMD:D_0603_1608Metric"
		(layer "B.Cu")
		(at 77.400615 112.569004 180)
		(descr "Diode SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
		(tags "diode")
		(property "Reference" "D2:1"
			(at 0 1.43 0)
			(layer "B.SilkS")
		)
		(property "Value" "D"
			(at 0 -1.43 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Diode, small symbol, filled shape"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sim.Device" "D"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TO-???* *_Diode_* *SingleDiode* D_*")
		(sheetname "/Human-Machine Interface/Keypad/")
		(sheetfile "../Projects/capstone-project/Hardware/KiCAD/system-testbed/keypad.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.7875 0 180)
			(size 0.875 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 33 "/Human-Machine Interface/Keypad/COL1")
			(pinfunction "K")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at 0.7875 0 180)
			(size 0.875 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 8 "Net-(D2:1-A)")
			(pinfunction "A")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Diode_SMD.3dshapes/D_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Diode_SMD:D_0603_1608Metric"
		(layer "B.Cu")
		(at 92.0041 112.658 180)
		(descr "Diode SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
		(tags "diode")
		(property "Reference" "D2:3"
			(at 0 1.43 0)
			(layer "B.SilkS")
		)
		(property "Value" "D"
			(at 0 -1.43 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Diode, small symbol, filled shape"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sim.Device" "D"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TO-???* *_Diode_* *SingleDiode* D_*")
		(sheetname "/Human-Machine Interface/Keypad/")
		(sheetfile "../Projects/capstone-project/Hardware/KiCAD/system-testbed/keypad.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.7875 0 180)
			(size 0.875 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 35 "/Human-Machine Interface/Keypad/COL3")
			(pinfunction "K")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at 0.7875 0 180)
			(size 0.875 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 10 "Net-(D2:3-A)")
			(pinfunction "A")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Diode_SMD.3dshapes/D_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "B.Cu")
		(at 113.4 94.225 90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R16"
			(at -0.064414 -1.233158 90)
			(layer "B.SilkS")
		)
		(property "Value" "100k"
			(at 0 -1.43 90)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Human-Machine Interface/Audio/")
		(sheetfile "untitled.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 90)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at 0.825 0 90)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 59 "/Human-Machine Interface/Audio/~{SD_MODE}")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Jumper:SolderJumper-2_P1.3mm_Open_TrianglePad1.0x1.5mm"
		(layer "B.Cu")
		(at 66 117)
		(descr "SMD Solder Jumper, 1x1.5mm Triangular Pads, 0.3mm gap, open")
		(tags "solder jumper open")
		(property "Reference" "JP2"
			(at 0 1.8 0)
			(layer "B.SilkS")
		)
		(property "Value" "SolderJumper_2_Open"
			(at 0 -1.9 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Solder Jumper, 2-pole, open"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SolderJumper*Open*")
		(sheetname "/Human-Machine Interface/")
		(sheetfile "human-machine-interface.kicad_sch")
		(zone_connect 1)
		(attr exclude_from_pos_files exclude_from_bom allow_soldermask_bridges)
		(pad "1" smd custom
			(at -0.725 0)
			(size 0.3 0.3)
			(layers "B.Cu" "B.Mask")
			(net 26 "+3.3V")
			(pinfunction "A")
			(pintype "passive")
			(zone_connect 2)
			(thermal_bridge_angle 45)
			(options
				(clearance outline)
				(anchor rect)
			)
			(primitives
				(gr_poly
					(pts
						(xy 1 0) (xy 0.5 -0.75) (xy -0.5 -0.75) (xy -0.5 0.75) (xy 0.5 0.75)
					)
					(width 0)
					(fill yes)
				)
			)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd custom
			(at 0.725 0)
			(size 0.3 0.3)
			(layers "B.Cu" "B.Mask")
			(net 56 "/Human-Machine Interface/PCF_A1")
			(pinfunction "B")
			(pintype "passive")
			(zone_connect 2)
			(thermal_bridge_angle 45)
			(options
				(clearance outline)
				(anchor rect)
			)
			(primitives
				(gr_poly
					(pts
						(xy 0.5 -0.75) (xy -0.65 -0.75) (xy -0.15 0) (xy -0.65 0.75) (xy 0.5 0.75)
					)
					(width 0)
					(fill yes)
				)
			)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "B.Cu")
		(at 117.2 90.9 -90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R9"
			(at -0.05 -1.3 90)
			(layer "B.SilkS")
		)
		(property "Value" "47k"
			(at -0.1 -6.988 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Human-Machine Interface/Audio/")
		(sheetfile "untitled.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 270)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 65 "Net-(MK1-SD)")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at 0.825 0 270)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "B.Cu")
		(at 116.5 87.6 180)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R10"
			(at 0.05 1.2 0)
			(layer "B.SilkS")
		)
		(property "Value" "68"
			(at 0 -1.43 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Human-Machine Interface/Audio/")
		(sheetfile "untitled.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 180)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 65 "Net-(MK1-SD)")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at 0.825 0 180)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 74 "/Human-Machine Interface/MIC_DOUT")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Jumper:SolderJumper-3_P1.3mm_Open_RoundedPad1.0x1.5mm_NumberLabels"
		(layer "B.Cu")
		(at 123.9 116.3 -90)
		(descr "SMD Solder 3-pad Jumper, 1x1.5mm rounded Pads, 0.3mm gap, open, labeled with numbers")
		(tags "solder jumper open")
		(property "Reference" "JP4"
			(at 0 1.8 90)
			(layer "B.SilkS")
		)
		(property "Value" "GAIN_{LOGIC}"
			(at 0 -1.9 90)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Solder Jumper, 3-pole, open"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SolderJumper*Open*")
		(sheetname "/Human-Machine Interface/Audio/")
		(sheetfile "untitled.kicad_sch")
		(zone_connect 1)
		(attr exclude_from_pos_files allow_soldermask_bridges)
		(fp_text user "3"
			(at 2.6 0 90)
			(layer "B.SilkS")
		)
		(fp_text user "1"
			(at -2.6 0 90)
			(layer "B.SilkS")
		)
		(pad "1" smd custom
			(at -1.3 0 270)
			(size 1 0.5)
			(layers "B.Cu" "B.Mask")
			(net 26 "+3.3V")
			(pinfunction "A")
			(pintype "passive")
			(zone_connect 2)
			(thermal_bridge_angle 45)
			(options
				(clearance outline)
				(anchor rect)
			)
			(primitives
				(gr_circle
					(center 0 -0.25)
					(end 0.5 -0.25)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center 0 0.25)
					(end 0.5 0.25)
					(width 0)
					(fill yes)
				)
				(gr_poly
					(pts
						(xy 0.55 -0.75) (xy 0 -0.75) (xy 0 0.75) (xy 0.55 0.75)
					)
					(width 0)
					(fill yes)
				)
			)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd rect
			(at 0 0 270)
			(size 1 1.5)
			(layers "B.Cu" "B.Mask")
			(net 58 "Net-(JP4-C)")
			(pinfunction "C")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "3" smd custom
			(at 1.3 0 270)
			(size 1 0.5)
			(layers "B.Cu" "B.Mask")
			(net 1 "GND")
			(pinfunction "B")
			(pintype "passive")
			(zone_connect 2)
			(thermal_bridge_angle 45)
			(options
				(clearance outline)
				(anchor rect)
			)
			(primitives
				(gr_circle
					(center 0 -0.25)
					(end 0.5 -0.25)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center 0 0.25)
					(end 0.5 0.25)
					(width 0)
					(fill yes)
				)
				(gr_poly
					(pts
						(xy 0 -0.75) (xy -0.55 -0.75) (xy -0.55 0.75) (xy 0 0.75)
					)
					(width 0)
					(fill yes)
				)
			)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
	)
	(footprint "Jumper:SolderJumper-2_P1.3mm_Open_TrianglePad1.0x1.5mm"
		(layer "B.Cu")
		(at 66 120.55)
		(descr "SMD Solder Jumper, 1x1.5mm Triangular Pads, 0.3mm gap, open")
		(tags "solder jumper open")
		(property "Reference" "JP1"
			(at 0 1.8 0)
			(layer "B.SilkS")
		)
		(property "Value" "SolderJumper_2_Open"
			(at 0 -1.9 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Solder Jumper, 2-pole, open"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SolderJumper*Open*")
		(sheetname "/Human-Machine Interface/")
		(sheetfile "human-machine-interface.kicad_sch")
		(zone_connect 1)
		(attr exclude_from_pos_files exclude_from_bom allow_soldermask_bridges)
		(pad "1" smd custom
			(at -0.725 0)
			(size 0.3 0.3)
			(layers "B.Cu" "B.Mask")
			(net 26 "+3.3V")
			(pinfunction "A")
			(pintype "passive")
			(zone_connect 2)
			(thermal_bridge_angle 45)
			(options
				(clearance outline)
				(anchor rect)
			)
			(primitives
				(gr_poly
					(pts
						(xy 1 0) (xy 0.5 -0.75) (xy -0.5 -0.75) (xy -0.5 0.75) (xy 0.5 0.75)
					)
					(width 0)
					(fill yes)
				)
			)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd custom
			(at 0.725 0)
			(size 0.3 0.3)
			(layers "B.Cu" "B.Mask")
			(net 55 "/Human-Machine Interface/PCF_A0")
			(pinfunction "B")
			(pintype "passive")
			(zone_connect 2)
			(thermal_bridge_angle 45)
			(options
				(clearance outline)
				(anchor rect)
			)
			(primitives
				(gr_poly
					(pts
						(xy 0.5 -0.75) (xy -0.65 -0.75) (xy -0.15 0) (xy -0.65 0.75) (xy 0.5 0.75)
					)
					(width 0)
					(fill yes)
				)
			)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
	)
	(footprint "Connector_JST:JST_EH_B2B-EH-A_1x02_P2.50mm_Vertical"
		(layer "B.Cu")
		(at 119.6 131.25 90)
		(descr "JST EH series connector, B2B-EH-A (http://www.jst-mfg.com/product/pdf/eng/eEH.pdf), generated with kicad-footprint-generator")
		(tags "connector JST EH vertical")
		(property "Reference" "LS1"
			(at 1.25 2.8 90)
			(layer "B.SilkS")
		)
		(property "Value" "Speaker"
			(at 1.15 -2.8 90)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Speaker"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(sheetname "/Human-Machine Interface/Audio/")
		(sheetfile "untitled.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 1.25 -1.5 90)
			(layer "B.Fab")
		)
		(pad "1" thru_hole roundrect
			(at 0 0 90)
			(size 1.7 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.147059)
			(net 63 "Net-(U2-OUTP)")
			(pinfunction "1")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" thru_hole oval
			(at 2.5 0 90)
			(size 1.7 2)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 62 "Net-(U2-OUTN)")
			(pinfunction "2")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_JST.3dshapes/JST_EH_B2B-EH-A_1x02_P2.50mm_Vertical.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "B.Cu")
		(at 126.6 116.3 -90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R12"
			(at 3 -0.05942 90)
			(layer "B.SilkS")
		)
		(property "Value" "100k 5%"
			(at 0 -1.43 90)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Human-Machine Interface/Audio/")
		(sheetfile "untitled.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 270)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 58 "Net-(JP4-C)")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at 0.825 0 270)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 61 "Net-(JP6-B)")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Diode_SMD:D_0603_1608Metric"
		(layer "B.Cu")
		(at 77.375615 121.849804 180)
		(descr "Diode SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
		(tags "diode")
		(property "Reference" "D4:1"
			(at 0 1.43 0)
			(layer "B.SilkS")
		)
		(property "Value" "D"
			(at 0 -1.43 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Diode, small symbol, filled shape"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sim.Device" "D"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TO-???* *_Diode_* *SingleDiode* D_*")
		(sheetname "/Human-Machine Interface/Keypad/")
		(sheetfile "../Projects/capstone-project/Hardware/KiCAD/system-testbed/keypad.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.7875 0 180)
			(size 0.875 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 33 "/Human-Machine Interface/Keypad/COL1")
			(pinfunction "K")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at 0.7875 0 180)
			(size 0.875 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 16 "Net-(D4:1-A)")
			(pinfunction "A")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Diode_SMD.3dshapes/D_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "B.Cu")
		(at 68.5 116.7 -90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R2"
			(at 0 -1.4 90)
			(layer "B.SilkS")
		)
		(property "Value" "10k"
			(at 0 -1.43 90)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Human-Machine Interface/")
		(sheetfile "human-machine-interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 270)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 56 "/Human-Machine Interface/PCF_A1")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at 0.825 0 270)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Diode_SMD:D_0603_1608Metric"
		(layer "B.Cu")
		(at 92.0041 121.858 180)
		(descr "Diode SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
		(tags "diode")
		(property "Reference" "D4:3"
			(at 0 1.43 0)
			(layer "B.SilkS")
		)
		(property "Value" "D"
			(at 0 -1.43 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Diode, small symbol, filled shape"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sim.Device" "D"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TO-???* *_Diode_* *SingleDiode* D_*")
		(sheetname "/Human-Machine Interface/Keypad/")
		(sheetfile "../Projects/capstone-project/Hardware/KiCAD/system-testbed/keypad.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.7875 0 180)
			(size 0.875 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 35 "/Human-Machine Interface/Keypad/COL3")
			(pinfunction "K")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at 0.7875 0 180)
			(size 0.875 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 18 "Net-(D4:3-A)")
			(pinfunction "A")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Diode_SMD.3dshapes/D_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Diode_SMD:D_0603_1608Metric"
		(layer "B.Cu")
		(at 77.400615 107.930131 180)
		(descr "Diode SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
		(tags "diode")
		(property "Reference" "D1:1"
			(at 0 1.43 0)
			(layer "B.SilkS")
		)
		(property "Value" "D"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Diode, small symbol, filled shape"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sim.Device" "D"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TO-???* *_Diode_* *SingleDiode* D_*")
		(sheetname "/Human-Machine Interface/Keypad/")
		(sheetfile "../Projects/capstone-project/Hardware/KiCAD/system-testbed/keypad.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.7875 0 180)
			(size 0.875 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 33 "/Human-Machine Interface/Keypad/COL1")
			(pinfunction "K")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at 0.7875 0 180)
			(size 0.875 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 4 "Net-(D1:1-A)")
			(pinfunction "A")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Diode_SMD.3dshapes/D_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "LOGO"
		(layer "B.Cu")
		(at 71.583362 130.11 180)
		(property "Reference" "G***"
			(at 0 0 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "LOGO"
			(at 0.75 0 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(attr board_only exclude_from_pos_files exclude_from_bom)
		(embedded_fonts no)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "B.Cu")
		(at 105.606994 116.679017 -90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R6"
			(at 0 -1.293006 90)
			(layer "B.SilkS")
		)
		(property "Value" "10k"
			(at 0 -1.43 90)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Human-Machine Interface/")
		(sheetfile "human-machine-interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 270)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 26 "+3.3V")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at 0.825 0 270)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 2 "Net-(C1-Pad1)")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "LOGO"
		(layer "B.Cu")
		(at 88.7 96.1 180)
		(property "Reference" "G***"
			(at 0 0 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "LOGO"
			(at 0.75 0 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(attr board_only exclude_from_pos_files exclude_from_bom)
		(embedded_fonts no)
	)
	(footprint "Diode_SMD:D_0603_1608Metric"
		(layer "B.Cu")
		(at 107.245358 99.326773 180)
		(descr "Diode SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
		(tags "diode")
		(property "Reference" "D2:4"
			(at -0.008642 1.456774 0)
			(layer "B.SilkS")
		)
		(property "Value" "D"
			(at 0 -1.43 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Diode, small symbol, filled shape"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sim.Device" "D"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TO-???* *_Diode_* *SingleDiode* D_*")
		(sheetname "/Human-Machine Interface/Keypad/")
		(sheetfile "../Projects/capstone-project/Hardware/KiCAD/system-testbed/keypad.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.7875 0 180)
			(size 0.875 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 36 "/Human-Machine Interface/Keypad/COL4")
			(pinfunction "K")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at 0.7875 0 180)
			(size 0.875 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 11 "Net-(D2:4-A)")
			(pinfunction "A")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Diode_SMD.3dshapes/D_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Diode_SMD:D_0603_1608Metric"
		(layer "B.Cu")
		(at 92.05 117.2508 180)
		(descr "Diode SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
		(tags "diode")
		(property "Reference" "D3:3"
			(at 0 1.43 0)
			(layer "B.SilkS")
		)
		(property "Value" "D"
			(at 0 -1.43 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Diode, small symbol, filled shape"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sim.Device" "D"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TO-???* *_Diode_* *SingleDiode* D_*")
		(sheetname "/Human-Machine Interface/Keypad/")
		(sheetfile "../Projects/capstone-project/Hardware/KiCAD/system-testbed/keypad.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.7875 0 180)
			(size 0.875 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 35 "/Human-Machine Interface/Keypad/COL3")
			(pinfunction "K")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at 0.7875 0 180)
			(size 0.875 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 14 "Net-(D3:3-A)")
			(pinfunction "A")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Diode_SMD.3dshapes/D_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Diode_SMD:D_0603_1608Metric"
		(layer "B.Cu")
		(at 107.209703 104.361475 180)
		(descr "Diode SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
		(tags "diode")
		(property "Reference" "D3:4"
			(at 0 1.43 0)
			(layer "B.SilkS")
		)
		(property "Value" "D"
			(at 0.04192 -1.626189 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Diode, small symbol, filled shape"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sim.Device" "D"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TO-???* *_Diode_* *SingleDiode* D_*")
		(sheetname "/Human-Machine Interface/Keypad/")
		(sheetfile "../Projects/capstone-project/Hardware/KiCAD/system-testbed/keypad.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.7875 0 180)
			(size 0.875 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 36 "/Human-Machine Interface/Keypad/COL4")
			(pinfunction "K")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at 0.7875 0 180)
			(size 0.875 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 15 "Net-(D3:4-A)")
			(pinfunction "A")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Diode_SMD.3dshapes/D_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "B.Cu")
		(at 118.7 83.4 90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R8"
			(at 0 -1.3 90)
			(layer "B.SilkS")
		)
		(property "Value" "47k"
			(at 0 -1.43 90)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Human-Machine Interface/Audio/")
		(sheetfile "untitled.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 90)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 64 "Net-(MK1-LR)")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at 0.825 0 90)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "B.Cu")
		(at 68.5 119.8 90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R1"
			(at 0 1.5 90)
			(layer "B.SilkS")
		)
		(property "Value" "10k"
			(at 0 -1.43 90)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Human-Machine Interface/")
		(sheetfile "human-machine-interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 90)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 55 "/Human-Machine Interface/PCF_A0")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at 0.825 0 90)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Diode_SMD:D_0603_1608Metric"
		(layer "B.Cu")
		(at 77.388115 117.249804 180)
		(descr "Diode SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
		(tags "diode")
		(property "Reference" "D3:1"
			(at 0 1.43 0)
			(layer "B.SilkS")
		)
		(property "Value" "D"
			(at 0 -1.43 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Diode, small symbol, filled shape"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sim.Device" "D"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TO-???* *_Diode_* *SingleDiode* D_*")
		(sheetname "/Human-Machine Interface/Keypad/")
		(sheetfile "../Projects/capstone-project/Hardware/KiCAD/system-testbed/keypad.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.7875 0 180)
			(size 0.875 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 33 "/Human-Machine Interface/Keypad/COL1")
			(pinfunction "K")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at 0.7875 0 180)
			(size 0.875 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 12 "Net-(D3:1-A)")
			(pinfunction "A")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Diode_SMD.3dshapes/D_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "B.Cu")
		(at 104.039987 113.51886 -90)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C2"
			(at -2.487615 0.046631 90)
			(layer "B.SilkS")
		)
		(property "Value" "0.01uF"
			(at 0 -1.43 90)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "capacitor, US symbol"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/Human-Machine Interface/")
		(sheetfile "human-machine-interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 270)
			(size 0.9 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 3 "Net-(C2-Pad1)")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at 0.775 0 270)
			(size 0.9 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Diode_SMD:D_0603_1608Metric"
		(layer "B.Cu")
		(at 113.084703 102.161475 180)
		(descr "Diode SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
		(tags "diode")
		(property "Reference" "D1:4"
			(at 0.0433 1.6 0)
			(layer "B.SilkS")
		)
		(property "Value" "D"
			(at 0 -1.43 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Diode, small symbol, filled shape"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sim.Device" "D"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TO-???* *_Diode_* *SingleDiode* D_*")
		(sheetname "/Human-Machine Interface/Keypad/")
		(sheetfile "../Projects/capstone-project/Hardware/KiCAD/system-testbed/keypad.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.7875 0 180)
			(size 0.875 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 36 "/Human-Machine Interface/Keypad/COL4")
			(pinfunction "K")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at 0.7875 0 180)
			(size 0.875 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 7 "Net-(D1:4-A)")
			(pinfunction "A")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Diode_SMD.3dshapes/D_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "B.Cu")
		(at 101.693356 117.431245)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R4"
			(at -2.48893 -0.004979 0)
			(layer "B.SilkS")
		)
		(property "Value" "10k"
			(at 0 -1.43 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, US symbol"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Human-Machine Interface/")
		(sheetfile "human-machine-interface.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 40 "/Human-Machine Interface/ENC_CLK")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at 0.825 0)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 2 "Net-(C1-Pad1)")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "capstone-project:Adafruit EYESPI FPC Connector"
		(layer "B.Cu")
		(at 108.169254 81.668651)
		(descr "WR-FPC SMT ZIF Horizontal Hinge Type")
		(tags "EYESPI, FPC")
		(property "Reference" "X1"
			(at 7.874 -2.032 0)
			(layer "B.SilkS")
		)
		(property "Value" "EYESPI"
			(at 0 -4.064 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "https://www.we-online.com/components/products/datasheet/687118149022.pdf"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "WR-FPC SMT ZIF Horizontal Hinge Type"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "HMI.kicad_sch")
		(attr smd allow_soldermask_bridges)
		(pad "1" smd rect
			(at -4.25 3.35)
			(size 0.3 1.3)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 26 "+3.3V")
			(pintype "passive")
			(solder_mask_margin 0.102)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd rect
			(at -3.75 3.35)
			(size 0.3 1.3)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 31 "/LITE")
			(pintype "passive")
			(solder_mask_margin 0.102)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "3" smd rect
			(at -3.25 3.35)
			(size 0.3 1.3)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 1 "GND")
			(pintype "passive")
			(solder_mask_margin 0.102)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "4" smd rect
			(at -2.75 3.35)
			(size 0.3 1.3)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 30 "/SCK")
			(pintype "passive")
			(solder_mask_margin 0.102)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "5" smd rect
			(at -2.25 3.35)
			(size 0.3 1.3)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 32 "/MOSI")
			(pintype "passive")
			(solder_mask_margin 0.102)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "6" smd rect
			(at -1.75 3.35)
			(size 0.3 1.3)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 29 "/MISO")
			(pintype "passive")
			(solder_mask_margin 0.102)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "7" smd rect
			(at -1.25 3.35)
			(size 0.3 1.3)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 24 "/TFTDC")
			(pintype "passive")
			(solder_mask_margin 0.102)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "8" smd rect
			(at -0.75 3.35)
			(size 0.3 1.3)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 25 "/TFTRST")
			(pintype "passive")
			(solder_mask_margin 0.102)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "9" smd rect
			(at -0.25 3.35)
			(size 0.3 1.3)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 27 "/TFTCS")
			(pintype "passive")
			(solder_mask_margin 0.102)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "10" smd rect
			(at 0.25 3.35)
			(size 0.3 1.3)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 28 "/CARDCS")
			(pintype "passive")
			(solder_mask_margin 0.102)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "11" smd rect
			(at 0.75 3.35)
			(size 0.3 1.3)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 76 "/Human-Machine Interface/AMP_DIN")
			(pintype "passive")
			(solder_mask_margin 0.102)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "12" smd rect
			(at 1.25 3.35)
			(size 0.3 1.3)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 74 "/Human-Machine Interface/MIC_DOUT")
			(pintype "passive")
			(solder_mask_margin 0.102)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "13" smd rect
			(at 1.75 3.35)
			(size 0.3 1.3)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 23 "/SCL")
			(pintype "passive")
			(solder_mask_margin 0.102)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "14" smd rect
			(at 2.25 3.35)
			(size 0.3 1.3)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 22 "/SDA")
			(pintype "passive")
			(solder_mask_margin 0.102)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "15" smd rect
			(at 2.75 3.35)
			(size 0.3 1.3)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 70 "/~{PCF_INT}")
			(pintype "passive")
			(solder_mask_margin 0.102)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "16" smd rect
			(at 3.25 3.35)
			(size 0.3 1.3)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 75 "/Human-Machine Interface/~{AMP_SD}")
			(pintype "passive")
			(solder_mask_margin 0.102)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "17" smd rect
			(at 3.75 3.35)
			(size 0.3 1.3)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 71 "/Human-Machine Interface/BCLK")
			(pintype "passive")
			(solder_mask_margin 0.102)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "18" smd rect
			(at 4.25 3.35)
			(size 0.3 1.3)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 73 "/Human-Machine Interface/LRCLK")
			(pintype "passive")
			(solder_mask_margin 0.102)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "Z1" smd rect
			(at -6.05 0.6)
			(size 2 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 1 "GND")
			(pintype "passive")
			(solder_mask_margin 0.102)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "Z2" smd rect
			(at 6.05 0.6)
			(size 2 1.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 1 "GND")
			(pintype "passive")
			(solder_mask_margin 0.102)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KIPRJMOD}/capstone-project.pretty/3dmodels/687118149022+(rev1).step"
			(offset
				(xyz 0 0.5 1.15)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -0 -0 -0)
			)
		)
	)
	(footprint "Diode_SMD:D_0603_1608Metric"
		(layer "B.Cu")
		(at 84.6875 112.658 180)
		(descr "Diode SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
		(tags "diode")
		(property "Reference" "D2:2"
			(at 0 1.43 0)
			(layer "B.SilkS")
		)
		(property "Value" "D"
			(at 0 -1.43 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Diode, small symbol, filled shape"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sim.Device" "D"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TO-???* *_Diode_* *SingleDiode* D_*")
		(sheetname "/Human-Machine Interface/Keypad/")
		(sheetfile "../Projects/capstone-project/Hardware/KiCAD/system-testbed/keypad.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.7875 0 180)
			(size 0.875 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 34 "/Human-Machine Interface/Keypad/COL2")
			(pinfunction "K")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at 0.7875 0 180)
			(size 0.875 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 9 "Net-(D2:2-A)")
			(pinfunction "A")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges no)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Diode_SMD.3dshapes/D_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(gr_arc
		(start 123.150199 77.99999)
		(mid 126.332087 79.31801)
		(end 127.64999 82.499998)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 127.65002 86.989481)
		(mid 126.349475 90.142617)
		(end 123.20417 91.462053)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 81.024854 130.9899)
		(mid 82.351676 127.799121)
		(end 85.548704 126.489876)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 66.463422 82.509426)
		(end 66.463422 86.9523)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 70.963514 91.437404)
		(end 71.278086 91.437403)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 131.651443 108.817907)
		(mid 132.083033 109.012467)
		(end 132.265919 109.475605)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 75.778102 95.962257)
		(mid 74.45128 99.153036)
		(end 71.253248 100.462277)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 127.721713 105.011812)
		(end 127.721713 105.013257)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 66.7894 135.489974)
		(mid 63.598635 134.163152)
		(end 62.289394 131.014456)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 66.725268 104.962304)
		(mid 65.618257 107.697161)
		(end 62.920618 108.892007)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 127.65002 86.989481)
		(end 127.650041 82.499998)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 85.548704 126.489876)
		(end 109.081894 126.49978)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 123.221663 100.486958)
		(mid 120.030884 99.160136)
		(end 118.721643 95.962104)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 66.7894 135.489974)
		(end 76.54984 135.489974)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 66.725268 104.962297)
		(mid 68.05209 101.771518)
		(end 71.250122 100.462277)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 123.20417 91.462053)
		(end 123.196994 91.462053)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 131.651416 108.817907)
		(mid 128.916559 107.710896)
		(end 127.721713 105.013257)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 132.265919 130.95764)
		(mid 130.95659 134.130956)
		(end 127.796977 135.45765)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 70.963514 91.437404)
		(mid 67.790165 90.128084)
		(end 66.463422 86.9523)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 118.721643 95.962054)
		(mid 120.030969 92.78879)
		(end 123.196994 91.462053)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 81.024854 130.989954)
		(mid 79.698032 134.180733)
		(end 76.54984 135.489974)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 71.250122 100.462277)
		(end 71.253248 100.462277)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 123.221693 100.486958)
		(mid 126.412472 101.81378)
		(end 127.721713 105.011812)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 75.978021 78.000005)
		(end 71.278021 78)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 70.96335 78)
		(end 71.278021 78)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 132.265919 109.475605)
		(end 132.265919 130.95764)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 91.15 78)
		(end 75.978021 78.000005)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 71.278086 91.437403)
		(mid 74.468861 92.764225)
		(end 75.778102 95.962257)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 118.08 135.45765)
		(end 127.796977 135.45765)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 62.289394 109.568876)
		(end 62.289394 131.014456)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 118.08 135.45765)
		(mid 114.889202 134.130828)
		(end 113.579961 130.932796)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 123.150199 77.99999)
		(end 91.15 78)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 109.081894 126.49978)
		(mid 112.238185 127.793995)
		(end 113.579961 130.932252)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 62.289394 109.568876)
		(mid 62.483953 109.074957)
		(end 62.920618 108.892071)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 66.463422 82.509426)
		(mid 67.778062 79.321358)
		(end 70.96335 78)
		(layer "Edge.Cuts")
	)
	(gr_text "2"
		(at 80.267089 108.897902 0)
		(layer "F.SilkS" knockout)
	)
	(gr_text "OPENAIR LAB"
		(at 87.725076 86.7 0)
		(layer "F.SilkS" knockout)
	)
	(gr_text "Zachary Potersnak, Eric Mutton\n 	   Fall 2025 REV-B\n      	    (HMI)"
		(at 88.7 82.4 0)
		(layer "F.SilkS" knockout)
	)
	(gr_text "9"
		(at 87.6 118.3 0)
		(layer "F.SilkS" knockout)
	)
	(gr_text "Rotary "
		(at 100.1 107.6 0)
		(layer "F.SilkS" knockout)
	)
	(gr_text "  Audio \nAmplifier"
		(at 122.7 116.2 0)
		(layer "F.SilkS" knockout)
	)
	(gr_text "GPIO Expander"
		(at 92.7 99.1 90)
		(layer "F.SilkS" knockout)
	)
	(gr_text "5"
		(at 80.267089 113.697902 0)
		(layer "F.SilkS" knockout)
	)
	(gr_text "Push To \n  Talk"
		(at 73.7 89.4 0)
		(layer "F.SilkS" knockout)
	)
	(gr_text "LITE"
		(at 79 81 0)
		(layer "F.SilkS")
	)
	(gr_text "*"
		(at 72.7 123.4 0)
		(layer "F.SilkS" knockout)
	)
	(gr_text "6"
		(at 87.6 113.7 0)
		(layer "F.SilkS" knockout)
	)
	(gr_text "Encoder"
		(at 112.974649 107.764467 0)
		(layer "F.SilkS" knockout)
	)
	(gr_text "4"
		(at 72.6 113.7 0)
		(layer "F.SilkS" knockout)
	)
	(gr_text "#"
		(at 87.5 122.9 0)
		(layer "F.SilkS" knockout)
	)
	(gr_text "OpenAir Lab\nProduction"
		(at 71.244213 132.988964 0)
		(layer "F.SilkS" knockout)
	)
	(gr_text "8"
		(at 80.367089 118.397902 0)
		(layer "F.SilkS" knockout)
	)
	(gr_text "Mic"
		(at 122.3 90.3 0)
		(layer "F.SilkS" knockout)
	)
	(gr_text "0"
		(at 80.267089 122.997902 0)
		(layer "F.SilkS" knockout)
	)
	(gr_text "3"
		(at 87.6 108.9 0)
		(layer "F.SilkS" knockout)
	)
	(gr_text "1"
		(at 72.7 108.9 0)
		(layer "F.SilkS" knockout)
	)
	(gr_text "7"
		(at 72.7 118.5 0)
		(layer "F.SilkS" knockout)
	)
	(zone
		(net 12)
		(net_name "Net-(D3:1-A)")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30034)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 78.571515 116.016804) (xy 78.571515 116.216804) (xy 78.896515 116.441804) (xy 79.422515 116.116804)
				(xy 78.896515 115.791804)
			)
		)
	)
	(zone
		(net 9)
		(net_name "Net-(D2:2-A)")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30095)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 83.366306 111.597335) (xy 83.507726 111.455915) (xy 83.1334 111.181819) (xy 82.607693 111.474293)
				(xy 83.1334 111.8)
			)
		)
	)
	(zone
		(net 37)
		(net_name "/Human-Machine Interface/Keypad/ROW3")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30022)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 85.9084 118.175) (xy 85.9084 118.375) (xy 86.2334 118.6) (xy 86.7594 118.275) (xy 86.2334 117.95)
			)
		)
	)
	(zone
		(net 17)
		(net_name "Net-(D4:2-A)")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30078)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 83.383682 120.855386) (xy 83.525102 120.713966) (xy 83.1334 120.455714) (xy 82.607693 120.774293)
				(xy 83.1334 121.1)
			)
		)
	)
	(zone
		(net 34)
		(net_name "/Human-Machine Interface/Keypad/COL2")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30106)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 86.575 99.65) (xy 86.775 99.65) (xy 86.867388 99.388268) (xy 86.675 98.499) (xy 86.482612 99.388268)
			)
		)
	)
	(zone
		(net 11)
		(net_name "Net-(D2:4-A)")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30096)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 108.377732 93.827025) (xy 108.519153 93.968446) (xy 108.746315 94.157244) (xy 109.272022 93.831537)
				(xy 108.746315 93.547745)
			)
		)
	)
	(zone
		(net 36)
		(net_name "/Human-Machine Interface/Keypad/COL4")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30115)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 87.875 99.65) (xy 88.075 99.65) (xy 88.167388 99.388268) (xy 87.975 98.499) (xy 87.782612 99.388268)
			)
		)
	)
	(zone
		(net 37)
		(net_name "/Human-Machine Interface/Keypad/ROW3")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30016)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 78.571515 118.166804) (xy 78.571515 118.366804) (xy 78.896515 118.591804) (xy 79.422515 118.266804)
				(xy 78.896515 117.941804)
			)
		)
	)
	(zone
		(net 8)
		(net_name "Net-(D2:1-A)")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30075)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 76.1375 111.566804) (xy 76.1375 111.366804) (xy 75.8125 111.125446) (xy 75.2865 111.425) (xy 75.8125 111.75)
			)
		)
	)
	(zone
		(net 71)
		(net_name "/Human-Machine Interface/BCLK")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30008)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 125.925 118.325) (xy 126.125 118.325) (xy 126.457873 117.736104) (xy 126.025 117.399) (xy 125.592127 117.736104)
			)
		)
	)
	(zone
		(net 11)
		(net_name "Net-(D2:4-A)")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30010)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 105.805414 94.457764) (xy 105.946835 94.316343) (xy 105.646315 93.814681) (xy 105.120608 93.831537)
				(xy 105.014946 94.157244)
			)
		)
	)
	(zone
		(net 26)
		(net_name "+3.3V")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30006)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 119.225 87.525) (xy 119.225 87.275) (xy 118.636104 86.967127) (xy 118.299 87.4) (xy 118.636104 87.832873)
			)
		)
	)
	(zone
		(net 42)
		(net_name "/Human-Machine Interface/Keypad/ROW1")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30109)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 83.325 99.65) (xy 83.525 99.65) (xy 83.617388 99.388268) (xy 83.425 98.499) (xy 83.232612 99.388268)
			)
		)
	)
	(zone
		(net 41)
		(net_name "/Human-Machine Interface/Keypad/ROW2")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30067)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 90.825 113.725) (xy 90.825 113.525) (xy 90.5 113.3) (xy 89.974 113.625) (xy 90.5 113.95)
			)
		)
	)
	(zone
		(net 42)
		(net_name "/Human-Machine Interface/Keypad/ROW1")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30073)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 94.975 109.1) (xy 94.975 108.9) (xy 94.65 108.665312) (xy 94.124 108.975) (xy 94.65 109.3)
			)
		)
	)
	(zone
		(net 60)
		(net_name "/Human-Machine Interface/Audio/GAIN_SLOT")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30001)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 124.815 122.64) (xy 124.815 122.84) (xy 125.0025 122.865) (xy 125.3535 122.74) (xy 125.0025 122.615)
			)
		)
	)
	(zone
		(net 41)
		(net_name "/Human-Machine Interface/Keypad/ROW2")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30103)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 83.975 99.65) (xy 84.175 99.65) (xy 84.267388 99.388268) (xy 84.075 98.499) (xy 83.882612 99.388268)
			)
		)
	)
	(zone
		(net 33)
		(net_name "/Human-Machine Interface/Keypad/COL1")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30107)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 85.925 99.65) (xy 86.125 99.65) (xy 86.217388 99.388268) (xy 86.025 98.499) (xy 85.832612 99.388268)
			)
		)
	)
	(zone
		(net 43)
		(net_name "/Human-Machine Interface/Keypad/ROW4")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30040)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 99.853012 100.058471) (xy 99.853012 99.858471) (xy 99.528012 99.633471) (xy 99.002012 99.958471)
				(xy 99.528012 100.283471)
			)
		)
	)
	(zone
		(net 41)
		(net_name "/Human-Machine Interface/Keypad/ROW2")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30118)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 105.021315 96.632244) (xy 105.221315 96.632244) (xy 105.446315 96.307244) (xy 105.121315 95.981244)
				(xy 104.796315 96.307244)
			)
		)
	)
	(zone
		(net 42)
		(net_name "/Human-Machine Interface/Keypad/ROW1")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30060)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 112.038525 100.088525) (xy 112.038525 99.888525) (xy 111.713525 99.663525) (xy 111.187525 99.988525)
				(xy 111.713525 100.313525)
			)
		)
	)
	(zone
		(net 41)
		(net_name "/Human-Machine Interface/Keypad/ROW2")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30012)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 93.275 113.525) (xy 93.275 113.725) (xy 93.6 113.95) (xy 94.126 113.625) (xy 93.6 113.3)
			)
		)
	)
	(zone
		(net 37)
		(net_name "/Human-Machine Interface/Keypad/ROW3")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30015)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 93.275 118.175) (xy 93.275 118.375) (xy 93.6 118.6) (xy 94.126 118.275) (xy 93.6 117.95)
			)
		)
	)
	(zone
		(net 40)
		(net_name "/Human-Machine Interface/ENC_CLK")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30111)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 84.175 90.35) (xy 83.975 90.35) (xy 83.882612 90.611732) (xy 84.075 91.501) (xy 84.267388 90.611732)
			)
		)
	)
	(zone
		(net 42)
		(net_name "/Human-Machine Interface/Keypad/ROW1")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30044)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 87.6084 109.075) (xy 87.6084 108.875) (xy 87.2834 108.65) (xy 86.7574 108.975) (xy 87.2834 109.3)
			)
		)
	)
	(zone
		(net 15)
		(net_name "Net-(D3:4-A)")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30091)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 105.899348 101.917541) (xy 106.040769 101.77612) (xy 105.659703 101.508141) (xy 105.133996 101.810768)
				(xy 105.659703 102.136475)
			)
		)
	)
	(zone
		(net 42)
		(net_name "/Human-Machine Interface/Keypad/ROW1")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30061)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 114.488525 99.888525) (xy 114.488525 100.088525) (xy 114.813525 100.313525) (xy 115.339525 99.988525)
				(xy 114.813525 99.663525)
			)
		)
	)
	(zone
		(net 42)
		(net_name "/Human-Machine Interface/Keypad/ROW1")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30041)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 83.4584 109.075) (xy 83.4584 108.875) (xy 83.1334 108.65) (xy 82.6074 108.975) (xy 83.1334 109.3)
			)
		)
	)
	(zone
		(net 37)
		(net_name "/Human-Machine Interface/Keypad/ROW3")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30013)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 90.825 118.375) (xy 90.825 118.175) (xy 90.5 117.95) (xy 89.974 118.275) (xy 90.5 118.6)
			)
		)
	)
	(zone
		(net 42)
		(net_name "/Human-Machine Interface/Keypad/ROW1")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30059)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 114.488525 99.888525) (xy 114.488525 100.088525) (xy 114.813525 100.313525) (xy 115.339525 99.988525)
				(xy 114.813525 99.663525)
			)
		)
	)
	(zone
		(net 44)
		(net_name "/Human-Machine Interface/ENC_DT")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30114)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 84.825 90.35) (xy 84.625 90.35) (xy 84.532612 90.611732) (xy 84.725 91.501) (xy 84.917388 90.611732)
			)
		)
	)
	(zone
		(net 43)
		(net_name "/Human-Machine Interface/Keypad/ROW4")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30112)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 85.275 99.65) (xy 85.475 99.65) (xy 85.567388 99.388268) (xy 85.375 98.499) (xy 85.182612 99.388268)
			)
		)
	)
	(zone
		(net 43)
		(net_name "/Human-Machine Interface/Keypad/ROW4")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30049)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 87.6084 123.025) (xy 87.6084 122.825) (xy 87.2834 122.6) (xy 86.7574 122.925) (xy 87.2834 123.25)
			)
		)
	)
	(zone
		(net 26)
		(net_name "+3.3V")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30002)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 119.05 115.19) (xy 119.05 114.91) (xy 118.4 114.4) (xy 117.199 115.05) (xy 118.4 115.7)
			)
		)
	)
	(zone
		(net 7)
		(net_name "Net-(D1:4-A)")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30094)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 114.445985 97.758773) (xy 114.587405 97.900193) (xy 114.813525 98.157507) (xy 115.339232 97.837818)
				(xy 114.813525 97.513525)
			)
		)
	)
	(zone
		(net 38)
		(net_name "/Human-Machine Interface/TFTRST")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30113)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 87.425 90.35) (xy 87.225 90.35) (xy 87.132612 90.611732) (xy 87.325 91.501) (xy 87.517388 90.611732)
			)
		)
	)
	(zone
		(net 37)
		(net_name "/Human-Machine Interface/Keypad/ROW3")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30025)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 105.984703 104.061475) (xy 105.984703 103.861475) (xy 105.659703 103.636475) (xy 105.133703 103.961475)
				(xy 105.659703 104.286475)
			)
		)
	)
	(zone
		(net 41)
		(net_name "/Human-Machine Interface/Keypad/ROW2")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30083)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 76.1375 113.733) (xy 76.1375 113.533) (xy 75.8125 113.285095) (xy 75.2865 113.575) (xy 75.8125 113.9)
			)
		)
	)
	(zone
		(net 7)
		(net_name "Net-(D1:4-A)")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30070)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 111.672624 98.464045) (xy 111.814045 98.322624) (xy 111.713525 97.903905) (xy 111.187818 97.837818)
				(xy 111.053906 98.163525)
			)
		)
	)
	(zone
		(net 43)
		(net_name "/Human-Machine Interface/Keypad/ROW4")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30051)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 90.825 123.025) (xy 90.825 122.825) (xy 90.5 122.6) (xy 89.974 122.925) (xy 90.5 123.25)
			)
		)
	)
	(zone
		(net 63)
		(net_name "Net-(U2-OUTP)")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30006)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 128.765 123.84) (xy 128.765 123.64) (xy 128.5775 123.615) (xy 128.2265 123.74) (xy 128.5775 123.865)
			)
		)
	)
	(zone
		(net 26)
		(net_name "+3.3V")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30004)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 126.94 124.965) (xy 127.14 124.965) (xy 127.165 124.7775) (xy 127.04 124.4265) (xy 126.915 124.7775)
			)
		)
	)
	(zone
		(net 42)
		(net_name "/Human-Machine Interface/Keypad/ROW1")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30086)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 74.4375 108.833) (xy 74.4375 109.033) (xy 74.7625 109.2) (xy 75.2885 108.875) (xy 74.7625 108.585095)
			)
		)
	)
	(zone
		(net 43)
		(net_name "/Human-Machine Interface/Keypad/ROW4")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30055)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 85.9084 122.825) (xy 85.9084 123.025) (xy 86.2334 123.25) (xy 86.7594 122.925) (xy 86.2334 122.6)
			)
		)
	)
	(zone
		(net 41)
		(net_name "/Human-Machine Interface/Keypad/ROW2")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30011)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 87.6084 113.725) (xy 87.6084 113.525) (xy 87.2834 113.3) (xy 86.7574 113.625) (xy 87.2834 113.95)
			)
		)
	)
	(zone
		(net 41)
		(net_name "/Human-Machine Interface/Keypad/ROW2")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30014)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 89.125 113.525) (xy 89.125 113.725) (xy 89.45 113.95) (xy 89.976 113.625) (xy 89.45 113.3)
			)
		)
	)
	(zone
		(net 6)
		(net_name "Net-(D1:3-A)")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30037)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 93.275 106.725) (xy 93.275 106.925) (xy 93.6 107.15) (xy 94.126 106.825) (xy 93.6 106.5)
			)
		)
	)
	(zone
		(net 26)
		(net_name "+3.3V")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30098)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 90.715 97.35) (xy 90.435 97.35) (xy 90.382612 97.611732) (xy 90.575 98.501) (xy 90.767388 97.611732)
			)
		)
	)
	(zone
		(net 22)
		(net_name "/SDA")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30108)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 89.825 99.65) (xy 90.025 99.65) (xy 90.117388 99.388268) (xy 89.925 98.499) (xy 89.732612 99.388268)
			)
		)
	)
	(zone
		(net 41)
		(net_name "/Human-Machine Interface/Keypad/ROW2")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30065)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 83.4584 113.725) (xy 83.4584 113.525) (xy 83.1334 113.3) (xy 82.6074 113.625) (xy 83.1334 113.95)
			)
		)
	)
	(zone
		(net 43)
		(net_name "/Human-Machine Interface/Keypad/ROW4")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30048)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 89.125 122.825) (xy 89.125 123.025) (xy 89.45 123.25) (xy 89.976 122.925) (xy 89.45 122.6)
			)
		)
	)
	(zone
		(net 12)
		(net_name "Net-(D3:1-A)")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30035)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 76.121515 116.216804) (xy 76.121515 116.016804) (xy 75.796515 115.791804) (xy 75.270515 116.116804)
				(xy 75.796515 116.441804)
			)
		)
	)
	(zone
		(net 43)
		(net_name "/Human-Machine Interface/Keypad/ROW4")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30069)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 81.7584 122.816804) (xy 81.7584 123.016804) (xy 82.0834 123.244949) (xy 82.6094 122.925) (xy 82.0834 122.6)
			)
		)
	)
	(zone
		(net 18)
		(net_name "Net-(D4:3-A)")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30088)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 90.744983 120.868178) (xy 90.886403 120.726758) (xy 90.5 120.463649) (xy 89.974293 120.774293)
				(xy 90.5 121.1)
			)
		)
	)
	(zone
		(net 2)
		(net_name "Net-(C1-Pad1)")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30001)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 115.35 117.4) (xy 115.35 117.7) (xy 116 118.2) (xy 117.201 117.55) (xy 116 116.9)
			)
		)
	)
	(zone
		(net 3)
		(net_name "Net-(C2-Pad1)")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30000)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 115.35 112.4) (xy 115.35 112.7) (xy 116 113.2) (xy 117.201 112.55) (xy 116 111.9)
			)
		)
	)
	(zone
		(net 37)
		(net_name "/Human-Machine Interface/Keypad/ROW3")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30100)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 84.625 99.65) (xy 84.825 99.65) (xy 84.917388 99.388268) (xy 84.725 98.499) (xy 84.532612 99.388268)
			)
		)
	)
	(zone
		(net 23)
		(net_name "/SCL")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30110)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 89.175 99.65) (xy 89.375 99.65) (xy 89.467388 99.388268) (xy 89.275 98.499) (xy 89.082612 99.388268)
			)
		)
	)
	(zone
		(net 62)
		(net_name "Net-(U2-OUTN)")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30005)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 128.765 123.34) (xy 128.765 123.14) (xy 128.5775 123.115) (xy 128.2265 123.24) (xy 128.5775 123.365)
			)
		)
	)
	(zone
		(net 41)
		(net_name "/Human-Machine Interface/Keypad/ROW2")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30026)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 81.7584 113.525) (xy 81.7584 113.725) (xy 82.0834 113.95) (xy 82.6094 113.625) (xy 82.0834 113.3)
			)
		)
	)
	(zone
		(net 15)
		(net_name "Net-(D3:4-A)")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30030)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 108.434703 101.711475) (xy 108.434703 101.911475) (xy 108.759703 102.136475) (xy 109.285703 101.811475)
				(xy 108.759703 101.486475)
			)
		)
	)
	(zone
		(net 37)
		(net_name "/Human-Machine Interface/Keypad/ROW3")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30023)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 83.4584 118.375) (xy 83.4584 118.175) (xy 83.1334 117.95) (xy 82.6074 118.275) (xy 83.1334 118.6)
			)
		)
	)
	(zone
		(net 18)
		(net_name "Net-(D4:3-A)")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30027)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 93.275 120.675) (xy 93.275 120.875) (xy 93.6 121.1) (xy 94.126 120.775) (xy 93.6 120.45)
			)
		)
	)
	(zone
		(net 42)
		(net_name "/Human-Machine Interface/Keypad/ROW1")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30042)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 85.9084 108.875) (xy 85.9084 109.075) (xy 86.2334 109.3) (xy 86.7594 108.975) (xy 86.2334 108.65)
			)
		)
	)
	(zone
		(net 43)
		(net_name "/Human-Machine Interface/Keypad/ROW4")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30053)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 76.121515 123.016804) (xy 76.121515 122.816804) (xy 75.796515 122.591804) (xy 75.270515 122.916804)
				(xy 75.796515 123.241804)
			)
		)
	)
	(zone
		(net 19)
		(net_name "Net-(D4:4-A)")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30119)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 102.301042 97.903714) (xy 102.442464 98.045136) (xy 102.628012 98.133471) (xy 103.153719 97.807764)
				(xy 102.628012 97.587508)
			)
		)
	)
	(zone
		(net 10)
		(net_name "Net-(D2:3-A)")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30090)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 90.550225 112.080524) (xy 90.550225 111.880524) (xy 90.5 111.504118) (xy 89.974 111.475) (xy 89.851645 111.8)
			)
		)
	)
	(zone
		(net 14)
		(net_name "Net-(D3:3-A)")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30031)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 93.275 116.025) (xy 93.275 116.225) (xy 93.6 116.45) (xy 94.126 116.125) (xy 93.6 115.8)
			)
		)
	)
	(zone
		(net 73)
		(net_name "/Human-Machine Interface/LRCLK")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30002)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 127.14 121.015) (xy 126.94 121.015) (xy 126.915 121.2025) (xy 127.04 121.5535) (xy 127.165 121.2025)
			)
		)
	)
	(zone
		(net 6)
		(net_name "Net-(D1:3-A)")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30019)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 90.825 106.925) (xy 90.825 106.725) (xy 90.5 106.5) (xy 89.974 106.825) (xy 90.5 107.15)
			)
		)
	)
	(zone
		(net 77)
		(net_name "Net-(IC1-P0)")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30097)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 88.412867 92.52071) (xy 88.554289 92.662132) (xy 88.703669 92.45) (xy 88.625707 91.499293) (xy 88.425 91.491763)
			)
		)
	)
	(zone
		(net 37)
		(net_name "/Human-Machine Interface/Keypad/ROW3")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30024)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 108.434703 103.861475) (xy 108.434703 104.061475) (xy 108.759703 104.286475) (xy 109.285703 103.961475)
				(xy 108.759703 103.636475)
			)
		)
	)
	(zone
		(net 42)
		(net_name "/Human-Machine Interface/Keypad/ROW1")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30043)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 89.125 108.875) (xy 89.125 109.075) (xy 89.45 109.3) (xy 89.976 108.975) (xy 89.45 108.65)
			)
		)
	)
	(zone
		(net 42)
		(net_name "/Human-Machine Interface/Keypad/ROW1")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30085)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 78.5875 108.833) (xy 78.5875 109.033) (xy 78.9125 109.2) (xy 79.4385 108.875) (xy 78.9125 108.585095)
			)
		)
	)
	(zone
		(net 8)
		(net_name "Net-(D2:1-A)")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30081)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 78.5875 111.383) (xy 78.5875 111.583) (xy 78.9125 111.75) (xy 79.4385 111.425) (xy 78.9125 111.135095)
			)
		)
	)
	(zone
		(net 5)
		(net_name "Net-(D1:2-A)")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30033)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 83.4584 106.925) (xy 83.4584 106.725) (xy 83.1334 106.5) (xy 82.6074 106.825) (xy 83.1334 107.15)
			)
		)
	)
	(zone
		(net 42)
		(net_name "/Human-Machine Interface/Keypad/ROW1")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30076)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 81.7584 108.833) (xy 81.7584 109.033) (xy 82.0834 109.274435) (xy 82.6094 108.975) (xy 82.0834 108.65)
			)
		)
	)
	(zone
		(net 42)
		(net_name "/Human-Machine Interface/Keypad/ROW1")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30080)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 76.1375 109.033) (xy 76.1375 108.833) (xy 75.8125 108.585095) (xy 75.2865 108.875) (xy 75.8125 109.2)
			)
		)
	)
	(zone
		(net 39)
		(net_name "/Human-Machine Interface/ENC_SW")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30003)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 101.05 112.45) (xy 101.05 112.65) (xy 101.7 113.2) (xy 102.901 112.55) (xy 101.7 111.9)
			)
		)
	)
	(zone
		(net 14)
		(net_name "Net-(D3:3-A)")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30089)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 90.742395 116.224427) (xy 90.883815 116.083007) (xy 90.5 115.817534) (xy 89.974293 116.124293)
				(xy 90.5 116.45)
			)
		)
	)
	(zone
		(net 56)
		(net_name "/Human-Machine Interface/PCF_A1")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30099)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 89.825 92.65) (xy 90.025 92.65) (xy 90.117388 92.388268) (xy 89.925 91.499) (xy 89.732612 92.388268)
			)
		)
	)
	(zone
		(net 13)
		(net_name "Net-(D3:2-A)")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30032)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 85.9084 116.025) (xy 85.9084 116.225) (xy 86.2334 116.45) (xy 86.7594 116.125) (xy 86.2334 115.8)
			)
		)
	)
	(zone
		(net 17)
		(net_name "Net-(D4:2-A)")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30028)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 85.9084 120.675) (xy 85.9084 120.875) (xy 86.2334 121.1) (xy 86.7594 120.775) (xy 86.2334 120.45)
			)
		)
	)
	(zone
		(net 37)
		(net_name "/Human-Machine Interface/Keypad/ROW3")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30021)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 89.125 118.175) (xy 89.125 118.375) (xy 89.45 118.6) (xy 89.976 118.275) (xy 89.45 117.95)
			)
		)
	)
	(zone
		(net 10)
		(net_name "Net-(D2:3-A)")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30036)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 93.275 111.375) (xy 93.275 111.575) (xy 93.6 111.8) (xy 94.126 111.475) (xy 93.6 111.15)
			)
		)
	)
	(zone
		(net 43)
		(net_name "/Human-Machine Interface/Keypad/ROW4")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30050)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 80.271515 123.016804) (xy 80.271515 122.816804) (xy 79.946515 122.591804) (xy 79.420515 122.916804)
				(xy 79.946515 123.241804)
			)
		)
	)
	(zone
		(net 37)
		(net_name "/Human-Machine Interface/Keypad/ROW3")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30057)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 108.434703 103.861475) (xy 108.434703 104.061475) (xy 108.759703 104.286475) (xy 109.285703 103.961475)
				(xy 108.759703 103.636475)
			)
		)
	)
	(zone
		(net 54)
		(net_name "/Human-Machine Interface/PCF_A2")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30102)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 89.175 92.65) (xy 89.375 92.65) (xy 89.467388 92.388268) (xy 89.275 91.499) (xy 89.082612 92.388268)
			)
		)
	)
	(zone
		(net 41)
		(net_name "/Human-Machine Interface/Keypad/ROW2")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30072)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 74.4375 113.5) (xy 74.4375 113.7) (xy 74.7625 113.9) (xy 75.2885 113.575) (xy 74.7625 113.265312)
			)
		)
	)
	(zone
		(net 76)
		(net_name "/Human-Machine Interface/AMP_DIN")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30008)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 124.893033 122.151612) (xy 124.751612 122.293033) (xy 124.966849 122.352402) (xy 125.353207 122.240707)
				(xy 124.978582 122.119758)
			)
		)
	)
	(zone
		(net 37)
		(net_name "/Human-Machine Interface/Keypad/ROW3")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30020)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 87.6084 118.375) (xy 87.6084 118.175) (xy 87.2834 117.95) (xy 86.7574 118.275) (xy 87.2834 118.6)
			)
		)
	)
	(zone
		(net 26)
		(net_name "+3.3V")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30004)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 117.603486 86.726709) (xy 117.426709 86.903486) (xy 117.825 87.607371) (xy 118.300707 87.400707)
				(xy 118.449025 86.95)
			)
		)
	)
	(zone
		(net 26)
		(net_name "+3.3V")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30003)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 127.44 124.965) (xy 127.64 124.965) (xy 127.665 124.7775) (xy 127.54 124.4265) (xy 127.415 124.7775)
			)
		)
	)
	(zone
		(net 16)
		(net_name "Net-(D4:1-A)")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30029)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 78.571515 120.666804) (xy 78.571515 120.866804) (xy 78.896515 121.091804) (xy 79.422515 120.766804)
				(xy 78.896515 120.441804)
			)
		)
	)
	(zone
		(net 43)
		(net_name "/Human-Machine Interface/Keypad/ROW4")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30052)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 93.275 122.825) (xy 93.275 123.025) (xy 93.6 123.25) (xy 94.126 122.925) (xy 93.6 122.6)
			)
		)
	)
	(zone
		(net 41)
		(net_name "/Human-Machine Interface/Keypad/ROW2")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30064)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 108.421315 95.882244) (xy 108.421315 96.082244) (xy 108.746315 96.307244) (xy 109.272315 95.982244)
				(xy 108.746315 95.657244)
			)
		)
	)
	(zone
		(net 42)
		(net_name "/Human-Machine Interface/Keypad/ROW1")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30117)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 111.088525 100.638525) (xy 111.288525 100.638525) (xy 111.513525 100.313525) (xy 111.188525 99.987525)
				(xy 110.863525 100.313525)
			)
		)
	)
	(zone
		(net 19)
		(net_name "Net-(D4:4-A)")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30071)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 99.487111 98.433991) (xy 99.628532 98.29257) (xy 99.528012 97.873851) (xy 99.002305 97.807764)
				(xy 98.868393 98.133471)
			)
		)
	)
	(zone
		(net 37)
		(net_name "/Human-Machine Interface/Keypad/ROW3")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30074)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 94.975 118.4) (xy 94.975 118.2) (xy 94.65 117.965312) (xy 94.124 118.275) (xy 94.65 118.6)
			)
		)
	)
	(zone
		(net 43)
		(net_name "/Human-Machine Interface/Keypad/ROW4")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30054)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 78.571515 122.816804) (xy 78.571515 123.016804) (xy 78.896515 123.241804) (xy 79.422515 122.916804)
				(xy 78.896515 122.591804)
			)
		)
	)
	(zone
		(net 16)
		(net_name "Net-(D4:1-A)")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30079)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 76.045705 120.849826) (xy 76.187125 120.708406) (xy 75.796515 120.449152) (xy 75.270808 120.766097)
				(xy 75.796515 121.091804)
			)
		)
	)
	(zone
		(net 26)
		(net_name "+3.3V")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30007)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 118.975 87.275) (xy 118.975 87.525) (xy 119.563896 87.832873) (xy 119.901 87.4) (xy 119.563896 86.967127)
			)
		)
	)
	(zone
		(net 41)
		(net_name "/Human-Machine Interface/Keypad/ROW2")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30082)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 78.5875 113.533) (xy 78.5875 113.733) (xy 78.9125 113.9) (xy 79.4385 113.575) (xy 78.9125 113.285095)
			)
		)
	)
	(zone
		(net 43)
		(net_name "/Human-Machine Interface/Keypad/ROW4")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30062)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 98.153012 99.858471) (xy 98.153012 100.058471) (xy 98.478012 100.283471) (xy 99.004012 99.958471)
				(xy 98.478012 99.633471)
			)
		)
	)
	(zone
		(net 70)
		(net_name "/~{PCF_INT}")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30116)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 90.675 90.35) (xy 90.475 90.35) (xy 90.382612 90.611732) (xy 90.575 91.501) (xy 90.767388 90.611732)
			)
		)
	)
	(zone
		(net 55)
		(net_name "/Human-Machine Interface/PCF_A0")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30104)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 88.725 97.35) (xy 88.525 97.35) (xy 88.432612 97.611732) (xy 88.625 98.501) (xy 88.817388 97.611732)
			)
		)
	)
	(zone
		(net 9)
		(net_name "Net-(D2:2-A)")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30038)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 85.9084 111.375) (xy 85.9084 111.575) (xy 86.2334 111.8) (xy 86.7594 111.475) (xy 86.2334 111.15)
			)
		)
	)
	(zone
		(net 42)
		(net_name "/Human-Machine Interface/Keypad/ROW1")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30045)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 90.825 109.075) (xy 90.825 108.875) (xy 90.5 108.65) (xy 89.974 108.975) (xy 90.5 109.3)
			)
		)
	)
	(zone
		(net 42)
		(net_name "/Human-Machine Interface/Keypad/ROW1")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30046)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 93.275 108.875) (xy 93.275 109.075) (xy 93.6 109.3) (xy 94.126 108.975) (xy 93.6 108.65)
			)
		)
	)
	(zone
		(net 37)
		(net_name "/Human-Machine Interface/Keypad/ROW3")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30017)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 76.121515 118.366804) (xy 76.121515 118.166804) (xy 75.796515 117.941804) (xy 75.270515 118.266804)
				(xy 75.796515 118.591804)
			)
		)
	)
	(zone
		(net 13)
		(net_name "Net-(D3:2-A)")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30092)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 83.37238 116.232671) (xy 83.5138 116.091251) (xy 83.1334 115.822667) (xy 82.607693 116.124293)
				(xy 83.1334 116.45)
			)
		)
	)
	(zone
		(net 41)
		(net_name "/Human-Machine Interface/Keypad/ROW2")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30063)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 105.971315 96.082244) (xy 105.971315 95.882244) (xy 105.646315 95.657244) (xy 105.120315 95.982244)
				(xy 105.646315 96.307244)
			)
		)
	)
	(zone
		(net 41)
		(net_name "/Human-Machine Interface/Keypad/ROW2")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30058)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 94.975 113.725) (xy 94.975 113.525) (xy 94.65 113.3) (xy 94.124 113.625) (xy 94.65 113.95)
			)
		)
	)
	(zone
		(net 35)
		(net_name "/Human-Machine Interface/Keypad/COL3")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30105)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 87.225 99.65) (xy 87.425 99.65) (xy 87.517388 99.388268) (xy 87.325 98.499) (xy 87.132612 99.388268)
			)
		)
	)
	(zone
		(net 41)
		(net_name "/Human-Machine Interface/Keypad/ROW2")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30066)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 85.9084 113.525) (xy 85.9084 113.725) (xy 86.2334 113.95) (xy 86.7594 113.625) (xy 86.2334 113.3)
			)
		)
	)
	(zone
		(net 26)
		(net_name "+3.3V")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30005)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 119.775 88.3) (xy 120.025 88.3) (xy 120.35 87.722886) (xy 119.9 87.399) (xy 119.45 87.722886)
			)
		)
	)
	(zone
		(net 37)
		(net_name "/Human-Machine Interface/Keypad/ROW3")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30068)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 80.271515 118.375) (xy 80.271515 118.175) (xy 79.946515 117.946854) (xy 79.420515 118.266804)
				(xy 79.946515 118.591804)
			)
		)
	)
	(zone
		(net 4)
		(net_name "Net-(D1:1-A)")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30093)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 76.1375 106.916804) (xy 76.1375 106.716804) (xy 75.8125 106.454858) (xy 75.2865 106.725) (xy 75.8125 107.05)
			)
		)
	)
	(zone
		(net 42)
		(net_name "/Human-Machine Interface/Keypad/ROW1")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30084)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 80.2875 109.033) (xy 80.2875 108.833) (xy 79.9625 108.585095) (xy 79.4365 108.875) (xy 79.9625 109.2)
			)
		)
	)
	(zone
		(net 59)
		(net_name "/Human-Machine Interface/Audio/~{SD_MODE}")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30000)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 124.815 123.64) (xy 124.815 123.84) (xy 125.0025 123.865) (xy 125.3535 123.74) (xy 125.0025 123.615)
			)
		)
	)
	(zone
		(net 39)
		(net_name "/Human-Machine Interface/ENC_SW")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30101)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 85.275 92.65) (xy 85.475 92.65) (xy 85.567388 92.388268) (xy 85.375 91.499) (xy 85.182612 92.388268)
			)
		)
	)
	(zone
		(net 4)
		(net_name "Net-(D1:1-A)")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30087)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 78.5875 106.683) (xy 78.5875 106.883) (xy 78.9125 107.05) (xy 79.4385 106.725) (xy 78.9125 106.435095)
			)
		)
	)
	(zone
		(net 43)
		(net_name "/Human-Machine Interface/Keypad/ROW4")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30047)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 102.303012 99.858471) (xy 102.303012 100.058471) (xy 102.628012 100.283471) (xy 103.154012 99.958471)
				(xy 102.628012 99.633471)
			)
		)
	)
	(zone
		(net 43)
		(net_name "/Human-Machine Interface/Keypad/ROW4")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30056)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 83.4584 123.025) (xy 83.4584 122.825) (xy 83.1334 122.6) (xy 82.6074 122.925) (xy 83.1334 123.25)
			)
		)
	)
	(zone
		(net 71)
		(net_name "/Human-Machine Interface/BCLK")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30009)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 126.125 116.475) (xy 125.925 116.475) (xy 125.592127 117.063896) (xy 126.025 117.401) (xy 126.457873 117.063896)
			)
		)
	)
	(zone
		(net 41)
		(net_name "/Human-Machine Interface/Keypad/ROW2")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30077)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 80.2875 113.725) (xy 80.2875 113.525) (xy 79.9625 113.280344) (xy 79.4365 113.575) (xy 79.9625 113.9)
			)
		)
	)
	(zone
		(net 37)
		(net_name "/Human-Machine Interface/Keypad/ROW3")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30018)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 81.7584 118.175) (xy 81.7584 118.375) (xy 82.0834 118.6) (xy 82.6094 118.275) (xy 82.0834 117.95)
			)
		)
	)
	(zone
		(net 5)
		(net_name "Net-(D1:2-A)")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30039)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 85.9084 106.725) (xy 85.9084 106.925) (xy 86.2334 107.15) (xy 86.7594 106.825) (xy 86.2334 106.5)
			)
		)
	)
	(zone
		(net 71)
		(net_name "/Human-Machine Interface/BCLK")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30007)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 126.125 121.015) (xy 125.925 121.015) (xy 125.915 121.2025) (xy 126.04 121.5535) (xy 126.15436 121.169779)
			)
		)
	)
	(zone
		(net 1)
		(net_name "GND")
		(layers "F.Cu" "B.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0.25)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 57.8644 73.3) (xy 138.5 73.6) (xy 139 142) (xy 56.2 141.65)
			)
		)
	)
	(zone
		(net 75)
		(net_name "/Human-Machine Interface/~{AMP_SD}")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30090)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 111.319254 85.818651) (xy 111.519254 85.818651) (xy 111.569254 85.668651) (xy 111.419254 85.017651)
				(xy 111.269254 85.668651)
			)
		)
	)
	(zone
		(net 12)
		(net_name "Net-(D3:1-A)")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30072)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 76.673246 116.566804) (xy 76.473246 116.566804) (xy 76.227185 116.838874) (xy 76.600615 117.250804)
				(xy 76.974045 116.838874)
			)
		)
	)
	(zone
		(net 56)
		(net_name "/Human-Machine Interface/PCF_A1")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30012)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 67.689971 116.368608) (xy 67.831392 116.510029) (xy 68.635029 116.275) (xy 68.500707 115.874293)
				(xy 68.025 115.734241)
			)
		)
	)
	(zone
		(net 35)
		(net_name "/Human-Machine Interface/Keypad/COL3")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30030)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 92.6916 108.7705) (xy 92.8916 108.7705) (xy 93.212449 108.197962) (xy 92.7916 107.857) (xy 92.370751 108.197962)
			)
		)
	)
	(zone
		(net 38)
		(net_name "/Human-Machine Interface/TFTRST")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30093)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 85.510249 85.818651) (xy 85.710249 85.818651) (xy 85.760249 85.668651) (xy 85.610249 85.017651)
				(xy 85.460249 85.668651)
			)
		)
	)
	(zone
		(net 2)
		(net_name "Net-(C1-Pad1)")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30061)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 103.318356 117.531245) (xy 103.318356 117.331245) (xy 102.870749 117.031245) (xy 102.517356 117.431245)
				(xy 102.870749 117.831245)
			)
		)
	)
	(zone
		(net 58)
		(net_name "Net-(JP4-C)")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30003)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 125.132842 116.158579) (xy 124.991421 116.017158) (xy 124.65 115.8) (xy 123.899293 116.300707)
				(xy 124.65 116.671608)
			)
		)
	)
	(zone
		(net 33)
		(net_name "/Human-Machine Interface/Keypad/COL1")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30037)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 78.263115 120.937304) (xy 78.063115 120.937304) (xy 77.742266 121.509842) (xy 78.163115 121.850804)
				(xy 78.583964 121.509842)
			)
		)
	)
	(zone
		(net 27)
		(net_name "/TFTCS")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30098)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 86.210249 84.218651) (xy 86.010249 84.218651) (xy 85.960249 84.368651) (xy 86.110249 85.019651)
				(xy 86.260249 84.368651)
			)
		)
	)
	(zone
		(net 34)
		(net_name "/Human-Machine Interface/Keypad/COL2")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30032)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 85.55 120.9455) (xy 85.35 120.9455) (xy 85.029151 121.518038) (xy 85.45 121.859) (xy 85.870849 121.518038)
			)
		)
	)
	(zone
		(net 73)
		(net_name "/Human-Machine Interface/LRCLK")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30089)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 112.519254 84.218651) (xy 112.319254 84.218651) (xy 112.269254 84.368651) (xy 112.419254 85.019651)
				(xy 112.569254 84.368651)
			)
		)
	)
	(zone
		(net 10)
		(net_name "Net-(D2:3-A)")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30077)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 91.291822 111.980524) (xy 91.091822 111.980524) (xy 90.84317 112.24707) (xy 91.2166 112.659)
				(xy 91.59003 112.24707)
			)
		)
	)
	(zone
		(net 24)
		(net_name "/TFTDC")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30094)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 85.010249 85.818651) (xy 85.210249 85.818651) (xy 85.260249 85.668651) (xy 85.110249 85.017651)
				(xy 84.960249 85.668651)
			)
		)
	)
	(zone
		(net 32)
		(net_name "/MOSI")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30100)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 105.819254 85.818651) (xy 106.019254 85.818651) (xy 106.069254 85.668651) (xy 105.919254 85.017651)
				(xy 105.769254 85.668651)
			)
		)
	)
	(zone
		(net 29)
		(net_name "/MISO")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30101)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 106.319254 85.818651) (xy 106.519254 85.818651) (xy 106.569254 85.668651) (xy 106.419254 85.017651)
				(xy 106.269254 85.668651)
			)
		)
	)
	(zone
		(net 35)
		(net_name "/Human-Machine Interface/Keypad/COL3")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30016)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 92.6916 118.1633) (xy 92.8916 118.1633) (xy 93.258349 117.590762) (xy 92.8375 117.2498) (xy 92.416651 117.590762)
			)
		)
	)
	(zone
		(net 71)
		(net_name "/Human-Machine Interface/BCLK")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30106)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 111.819254 85.818651) (xy 112.019254 85.818651) (xy 112.069254 85.668651) (xy 111.919254 85.017651)
				(xy 111.769254 85.668651)
			)
		)
	)
	(zone
		(net 17)
		(net_name "Net-(D4:2-A)")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30074)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 83.949263 121.179547) (xy 83.749263 121.179547) (xy 83.50157 121.44707) (xy 83.875 121.859)
				(xy 84.24843 121.44707)
			)
		)
	)
	(zone
		(net 26)
		(net_name "+3.3V")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30083)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 120.856 88.775) (xy 120.856 89.025) (xy 121.117 89.1) (xy 121.379 88.8) (xy 121.117 88.584367)
			)
		)
	)
	(zone
		(net 59)
		(net_name "/Human-Machine Interface/Audio/~{SD_MODE}")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30048)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 114.275 93.5) (xy 114.275 93.3) (xy 113.751537 93.015224) (xy 113.399 93.4) (xy 113.751537 93.784776)
			)
		)
	)
	(zone
		(net 33)
		(net_name "/Human-Machine Interface/Keypad/COL1")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30013)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 78.063115 118.162304) (xy 78.263115 118.162304) (xy 78.596464 117.589766) (xy 78.175615 117.248804)
				(xy 77.754766 117.589766)
			)
		)
	)
	(zone
		(net 4)
		(net_name "Net-(D1:1-A)")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30075)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 76.687778 107.251726) (xy 76.487778 107.251726) (xy 76.239685 107.519201) (xy 76.613115 107.931131)
				(xy 76.986545 107.519201)
			)
		)
	)
	(zone
		(net 55)
		(net_name "/Human-Machine Interface/PCF_A0")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30052)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 69.375 120.725) (xy 69.375 120.525) (xy 68.851537 120.240224) (xy 68.499 120.625) (xy 68.851537 121.009776)
			)
		)
	)
	(zone
		(net 23)
		(net_name "/SCL")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30105)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 109.819254 85.818651) (xy 110.019254 85.818651) (xy 110.069254 85.668651) (xy 109.919254 85.017651)
				(xy 109.769254 85.668651)
			)
		)
	)
	(zone
		(net 55)
		(net_name "/Human-Machine Interface/PCF_A0")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30050)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 67.625 120.525) (xy 67.625 120.725) (xy 68.148463 121.009776) (xy 68.501 120.625) (xy 68.148463 120.240224)
			)
		)
	)
	(zone
		(net 19)
		(net_name "Net-(D4:4-A)")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30020)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 100.390512 101.248975) (xy 100.190512 101.248975) (xy 99.869663 101.821513) (xy 100.290512 102.162475)
				(xy 100.711361 101.821513)
			)
		)
	)
	(zone
		(net 76)
		(net_name "/Human-Machine Interface/AMP_DIN")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30099)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 109.019254 84.218651) (xy 108.819254 84.218651) (xy 108.769254 84.368651) (xy 108.919254 85.019651)
				(xy 109.069254 84.368651)
			)
		)
	)
	(zone
		(net 29)
		(net_name "/MISO")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30092)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 84.710249 84.218651) (xy 84.510249 84.218651) (xy 84.460249 84.368651) (xy 84.610249 85.019651)
				(xy 84.760249 84.368651)
			)
		)
	)
	(zone
		(net 35)
		(net_name "/Human-Machine Interface/Keypad/COL3")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30065)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 92.552951 107.002931) (xy 92.41153 107.144352) (xy 92.3541 107.60175) (xy 92.792307 107.858707)
				(xy 93.080305 107.396914)
			)
		)
	)
	(zone
		(net 74)
		(net_name "/Human-Machine Interface/MIC_DOUT")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30104)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 109.319254 85.818651) (xy 109.519254 85.818651) (xy 109.569254 85.668651) (xy 109.419254 85.017651)
				(xy 109.269254 85.668651)
			)
		)
	)
	(zone
		(net 16)
		(net_name "Net-(D4:1-A)")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30081)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 76.664314 121.227015) (xy 76.464314 121.227015) (xy 76.214685 121.438874) (xy 76.588115 121.850804)
				(xy 76.961545 121.438874)
			)
		)
	)
	(zone
		(net 3)
		(net_name "Net-(C2-Pad1)")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30043)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 106.485845 112.854475) (xy 106.485845 112.554475) (xy 105.962382 112.325342) (xy 105.609845 112.710118)
				(xy 105.962382 113.094894)
			)
		)
	)
	(zone
		(net 3)
		(net_name "Net-(C2-Pad1)")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30010)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 104.964987 112.804475) (xy 104.964987 112.604475) (xy 104.376091 112.310987) (xy 104.038987 112.74386)
				(xy 104.376091 113.176733)
			)
		)
	)
	(zone
		(net 22)
		(net_name "/SDA")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30086)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 110.319254 85.818651) (xy 110.519254 85.818651) (xy 110.569254 85.668651) (xy 110.419254 85.017651)
				(xy 110.269254 85.668651)
			)
		)
	)
	(zone
		(net 36)
		(net_name "/Human-Machine Interface/Keypad/COL4")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30005)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 102.634031 101.534377) (xy 102.49261 101.392956) (xy 101.721793 101.686475) (xy 101.864805 102.162182)
				(xy 102.303012 102.342693)
			)
		)
	)
	(zone
		(net 34)
		(net_name "/Human-Machine Interface/Keypad/COL2")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30026)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 85.5625 106.9455) (xy 85.3625 106.9455) (xy 85.041651 107.518038) (xy 85.4625 107.859) (xy 85.883349 107.518038)
			)
		)
	)
	(zone
		(net 34)
		(net_name "/Human-Machine Interface/Keypad/COL2")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30034)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 85.375 108.7705) (xy 85.575 108.7705) (xy 85.883349 108.197962) (xy 85.4625 107.857) (xy 85.041651 108.197962)
			)
		)
	)
	(zone
		(net 64)
		(net_name "Net-(MK1-LR)")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30046)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 119.575 84.325) (xy 119.575 84.125) (xy 119.051537 83.840224) (xy 118.699 84.225) (xy 119.051537 84.609776)
			)
		)
	)
	(zone
		(net 65)
		(net_name "Net-(MK1-SD)")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30045)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 117.937132 88.178553) (xy 118.078553 88.037132) (xy 117.725 87.398852) (xy 117.324293 87.599293)
				(xy 117.293576 88.075)
			)
		)
	)
	(zone
		(net 14)
		(net_name "Net-(D3:3-A)")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30079)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 91.333473 116.574085) (xy 91.133473 116.574085) (xy 90.88907 116.83987) (xy 91.2625 117.2518)
				(xy 91.63593 116.83987)
			)
		)
	)
	(zone
		(net 63)
		(net_name "Net-(U2-OUTP)")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30000)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 121.45 131.35) (xy 121.45 131.15) (xy 120.526777 130.473223) (xy 119.599 131.25) (xy 120.526777 132.026777)
			)
		)
	)
	(zone
		(net 54)
		(net_name "/Human-Machine Interface/PCF_A2")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30055)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 68.7 112.075) (xy 68.5 112.075) (xy 68.144746 112.492707) (xy 68.5 112.876) (xy 68.94122 112.570694)
			)
		)
	)
	(zone
		(net 58)
		(net_name "Net-(JP4-C)")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30053)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 125.725 115.375) (xy 125.725 115.575) (xy 126.248463 115.859776) (xy 126.601 115.475) (xy 126.248463 115.090224)
			)
		)
	)
	(zone
		(net 11)
		(net_name "Net-(D2:4-A)")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30014)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 106.557858 98.414273) (xy 106.357858 98.414273) (xy 106.037009 98.986811) (xy 106.457858 99.327773)
				(xy 106.878707 98.986811)
			)
		)
	)
	(zone
		(net 65)
		(net_name "Net-(MK1-SD)")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30041)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 118.028553 89.693629) (xy 117.887132 89.552208) (xy 117.090173 89.675) (xy 117.199293 90.075707)
				(xy 117.675 90.257593)
			)
		)
	)
	(zone
		(net 33)
		(net_name "/Human-Machine Interface/Keypad/COL1")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30021)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 78.288115 111.656504) (xy 78.088115 111.656504) (xy 77.767266 112.229042) (xy 78.188115 112.570004)
				(xy 78.608964 112.229042)
			)
		)
	)
	(zone
		(net 30)
		(net_name "/SCK")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30110)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 105.294937 85.725736) (xy 105.436358 85.867157) (xy 105.524928 85.668651) (xy 105.419961 85.017944)
				(xy 105.269254 85.668651)
			)
		)
	)
	(zone
		(net 56)
		(net_name "/Human-Machine Interface/PCF_A1")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30111)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 67.401776 116.939645) (xy 67.260355 116.798224) (xy 67.225 116.738473) (xy 66.724293 117.000707)
				(xy 67.225 117.045465)
			)
		)
	)
	(zone
		(net 26)
		(net_name "+3.3V")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30007)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 106.160051 115.117495) (xy 106.358041 114.919505) (xy 106.085845 114.272441) (xy 105.610138 114.359411)
				(xy 105.443322 114.760118)
			)
		)
	)
	(zone
		(net 55)
		(net_name "/Human-Machine Interface/PCF_A0")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30108)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 67.375 120.725) (xy 67.375 120.525) (xy 67.225 120.456727) (xy 66.724 120.55) (xy 67.225 120.75871)
			)
		)
	)
	(zone
		(net 36)
		(net_name "/Human-Machine Interface/Keypad/COL4")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30040)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 101.5 103.064674) (xy 101.7 103.064674) (xy 102.191145 102.604341) (xy 101.865512 102.160475)
				(xy 101.428012 102.417725)
			)
		)
	)
	(zone
		(net 13)
		(net_name "Net-(D3:2-A)")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30076)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 83.961164 116.580035) (xy 83.761164 116.580035) (xy 83.50157 116.84707) (xy 83.875 117.259)
				(xy 84.24843 116.84707)
			)
		)
	)
	(zone
		(net 45)
		(net_name "/Human-Machine Interface/LITE")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30091)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 82.710249 84.218651) (xy 82.510249 84.218651) (xy 82.460249 84.368651) (xy 82.610249 85.019651)
				(xy 82.760249 84.368651)
			)
		)
	)
	(zone
		(net 9)
		(net_name "Net-(D2:2-A)")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30078)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 83.990915 111.980524) (xy 83.790915 111.980524) (xy 83.52657 112.24707) (xy 83.9 112.659) (xy 84.27343 112.24707)
			)
		)
	)
	(zone
		(net 59)
		(net_name "/Human-Machine Interface/Audio/~{SD_MODE}")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30063)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 113.304634 92.745446) (xy 113.504634 92.745446) (xy 113.804634 92.297839) (xy 113.404634 91.944446)
				(xy 113.004634 92.297839)
			)
		)
	)
	(zone
		(net 44)
		(net_name "/Human-Machine Interface/ENC_DT")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30038)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 100.286538 112.034828) (xy 100.145117 112.176249) (xy 100.470132 112.925528) (xy 100.870839 112.76055)
				(xy 100.960817 112.284843)
			)
		)
	)
	(zone
		(net 33)
		(net_name "/Human-Machine Interface/Keypad/COL1")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30018)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 78.288115 116.337304) (xy 78.088115 116.337304) (xy 77.754766 116.909842) (xy 78.175615 117.250804)
				(xy 78.596464 116.909842)
			)
		)
	)
	(zone
		(net 28)
		(net_name "/CARDCS")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30097)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 108.319254 85.818651) (xy 108.519254 85.818651) (xy 108.569254 85.668651) (xy 108.419254 85.017651)
				(xy 108.269254 85.668651)
			)
		)
	)
	(zone
		(net 73)
		(net_name "/Human-Machine Interface/LRCLK")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30082)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 121.003156 86.483735) (xy 120.861735 86.625156) (xy 121.117 87.10811) (xy 121.378707 87.000707)
				(xy 121.44711 86.7)
			)
		)
	)
	(zone
		(net 61)
		(net_name "Net-(JP6-B)")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30044)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 127.328575 117.7) (xy 127.328575 117.5) (xy 127.075 116.9576) (xy 126.599 117.125) (xy 126.480262 117.525)
			)
		)
	)
	(zone
		(net 35)
		(net_name "/Human-Machine Interface/Keypad/COL3")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30027)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 92.9375 116.3383) (xy 92.7375 116.3383) (xy 92.416651 116.910838) (xy 92.8375 117.2518) (xy 93.258349 116.910838)
			)
		)
	)
	(zone
		(net 33)
		(net_name "/Human-Machine Interface/Keypad/COL1")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30017)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 78.288115 107.017631) (xy 78.088115 107.017631) (xy 77.767266 107.590169) (xy 78.188115 107.931131)
				(xy 78.608964 107.590169)
			)
		)
	)
	(zone
		(net 34)
		(net_name "/Human-Machine Interface/Keypad/COL2")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30035)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 85.575 111.7455) (xy 85.375 111.7455) (xy 85.054151 112.318038) (xy 85.475 112.659) (xy 85.895849 112.318038)
			)
		)
	)
	(zone
		(net 62)
		(net_name "Net-(U2-OUTN)")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30001)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 121.433667 128.85) (xy 121.433667 128.65) (xy 120.222235 128.043251) (xy 119.599 128.75) (xy 120.222235 129.456749)
			)
		)
	)
	(zone
		(net 65)
		(net_name "Net-(MK1-SD)")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30084)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 120.856 87.8) (xy 120.856 88) (xy 121.117 88.161) (xy 121.379 87.9) (xy 121.117 87.639)
			)
		)
	)
	(zone
		(net 75)
		(net_name "/Human-Machine Interface/~{AMP_SD}")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30049)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 112.529634 90.195446) (xy 112.529634 90.395446) (xy 113.053097 90.680222) (xy 113.405634 90.295446)
				(xy 113.053097 89.91067)
			)
		)
	)
	(zone
		(net 2)
		(net_name "Net-(C1-Pad1)")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30054)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 104.731994 117.390545) (xy 104.731994 117.590545) (xy 105.255457 117.888793) (xy 105.607994 117.504017)
				(xy 105.255457 117.119241)
			)
		)
	)
	(zone
		(net 2)
		(net_name "Net-(C1-Pad1)")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30042)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 106.481994 117.640545) (xy 106.481994 117.340545) (xy 105.958531 117.119241) (xy 105.605994 117.504017)
				(xy 105.958531 117.888793)
			)
		)
	)
	(zone
		(net 2)
		(net_name "Net-(C1-Pad1)")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30009)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 103.116716 117.331245) (xy 103.116716 117.531245) (xy 103.705612 117.881878) (xy 104.042716 117.449005)
				(xy 103.705612 117.016132)
			)
		)
	)
	(zone
		(net 28)
		(net_name "/CARDCS")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30088)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 86.710249 84.218651) (xy 86.510249 84.218651) (xy 86.460249 84.368651) (xy 86.610249 85.019651)
				(xy 86.760249 84.368651)
			)
		)
	)
	(zone
		(net 36)
		(net_name "/Human-Machine Interface/Keypad/COL4")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30023)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 108.097203 103.448975) (xy 107.897203 103.448975) (xy 107.576354 104.021513) (xy 107.997203 104.362475)
				(xy 108.418052 104.021513)
			)
		)
	)
	(zone
		(net 54)
		(net_name "/Human-Machine Interface/PCF_A2")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30071)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 68.118198 113.4) (xy 68.118198 113.6) (xy 68.725072 113.275) (xy 68.501 112.875) (xy 68.025 113.075)
			)
		)
	)
	(zone
		(net 33)
		(net_name "/Human-Machine Interface/Keypad/COL1")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30015)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 78.088115 113.481504) (xy 78.288115 113.481504) (xy 78.608964 112.908966) (xy 78.188115 112.568004)
				(xy 77.767266 112.908966)
			)
		)
	)
	(zone
		(net 27)
		(net_name "/TFTCS")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30103)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 107.819254 85.818651) (xy 108.019254 85.818651) (xy 108.069254 85.668651) (xy 107.919254 85.017651)
				(xy 107.769254 85.668651)
			)
		)
	)
	(zone
		(net 54)
		(net_name "/Human-Machine Interface/PCF_A2")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30109)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 67.375 113.6) (xy 67.375 113.4) (xy 67.225 113.338037) (xy 66.724 113.45) (xy 67.225 113.638921)
			)
		)
	)
	(zone
		(net 34)
		(net_name "/Human-Machine Interface/Keypad/COL2")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30025)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 85.375 113.5705) (xy 85.575 113.5705) (xy 85.895849 112.997962) (xy 85.475 112.657) (xy 85.054151 112.997962)
			)
		)
	)
	(zone
		(net 36)
		(net_name "/Human-Machine Interface/Keypad/COL4")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30004)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 113.103684 102.788573) (xy 113.245105 102.929994) (xy 114.015921 102.636475) (xy 113.87291 102.160768)
				(xy 113.434703 101.980256)
			)
		)
	)
	(zone
		(net 56)
		(net_name "/Human-Machine Interface/PCF_A1")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30051)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 69.375 115.975) (xy 69.375 115.775) (xy 68.851537 115.490224) (xy 68.499 115.875) (xy 68.851537 116.259776)
			)
		)
	)
	(zone
		(net 35)
		(net_name "/Human-Machine Interface/Keypad/COL3")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30028)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 92.8916 120.9455) (xy 92.6916 120.9455) (xy 92.370751 121.518038) (xy 92.7916 121.859) (xy 93.212449 121.518038)
			)
		)
	)
	(zone
		(net 64)
		(net_name "Net-(MK1-LR)")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30107)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 122.115148 86.432726) (xy 121.973726 86.574148) (xy 121.939 86.7) (xy 122.200707 87.000707)
				(xy 122.379792 86.7)
			)
		)
	)
	(zone
		(net 71)
		(net_name "/Human-Machine Interface/BCLK")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30085)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 122.086156 89.272423) (xy 122.227577 89.413844) (xy 122.438313 89.1) (xy 122.200707 88.799293)
				(xy 121.939 89.1)
			)
		)
	)
	(zone
		(net 26)
		(net_name "+3.3V")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30039)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 106.252546 115.34) (xy 106.252546 115.06) (xy 105.438962 115.454017) (xy 105.605994 115.854017)
				(xy 106.081994 115.941481)
			)
		)
	)
	(zone
		(net 34)
		(net_name "/Human-Machine Interface/Keypad/COL2")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30031)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 85.575 116.3455) (xy 85.375 116.3455) (xy 85.029151 116.918038) (xy 85.45 117.259) (xy 85.870849 116.918038)
			)
		)
	)
	(zone
		(net 32)
		(net_name "/MOSI")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30096)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 84.210249 84.218651) (xy 84.010249 84.218651) (xy 83.960249 84.368651) (xy 84.110249 85.019651)
				(xy 84.260249 84.368651)
			)
		)
	)
	(zone
		(net 40)
		(net_name "/Human-Machine Interface/ENC_CLK")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30062)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 100.068356 117.331245) (xy 100.068356 117.531245) (xy 100.515963 117.831245) (xy 100.869356 117.431245)
				(xy 100.515963 117.031245)
			)
		)
	)
	(zone
		(net 74)
		(net_name "/Human-Machine Interface/MIC_DOUT")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30059)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 114.875 87.5) (xy 114.875 87.7) (xy 115.322607 88) (xy 115.676 87.6) (xy 115.322607 87.2)
			)
		)
	)
	(zone
		(net 15)
		(net_name "Net-(D3:4-A)")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30006)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 107.184703 103.64904) (xy 106.984703 103.64904) (xy 106.267179 103.886475) (xy 106.422203 104.362475)
				(xy 106.859703 104.534281)
			)
		)
	)
	(zone
		(net 26)
		(net_name "+3.3V")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30057)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 105.7 115.054017) (xy 105.5 115.054017) (xy 105.20391 115.503683) (xy 105.606994 115.855017)
				(xy 106.003905 115.49956)
			)
		)
	)
	(zone
		(net 5)
		(net_name "Net-(D1:2-A)")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30066)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 83.979014 107.154904) (xy 83.779014 107.154904) (xy 83.51407 107.44707) (xy 83.8875 107.859)
				(xy 84.26093 107.44707)
			)
		)
	)
	(zone
		(net 7)
		(net_name "Net-(D1:4-A)")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30036)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 112.397203 101.248975) (xy 112.197203 101.248975) (xy 111.876354 101.821513) (xy 112.297203 102.162475)
				(xy 112.718052 101.821513)
			)
		)
	)
	(zone
		(net 35)
		(net_name "/Human-Machine Interface/Keypad/COL3")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30024)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 92.7375 113.5705) (xy 92.9375 113.5705) (xy 93.212449 112.997962) (xy 92.7916 112.657) (xy 92.370751 112.997962)
			)
		)
	)
	(zone
		(net 61)
		(net_name "Net-(JP6-B)")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30080)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 128.104278 117.5) (xy 128.104278 117.7) (xy 128.421926 117.85) (xy 129.101 117.6) (xy 128.35 117.35)
			)
		)
	)
	(zone
		(net 58)
		(net_name "Net-(JP4-C)")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30068)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 128.1 115.2) (xy 128.1 115.4) (xy 128.35 115.48606) (xy 129.101 115) (xy 128.354278 114.962807)
			)
		)
	)
	(zone
		(net 6)
		(net_name "Net-(D1:3-A)")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30073)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 91.297772 107.178704) (xy 91.097772 107.178704) (xy 90.84317 107.44707) (xy 91.2166 107.859)
				(xy 91.59003 107.44707)
			)
		)
	)
	(zone
		(net 35)
		(net_name "/Human-Machine Interface/Keypad/COL3")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30029)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 92.8916 111.7455) (xy 92.6916 111.7455) (xy 92.370751 112.318038) (xy 92.7916 112.659) (xy 93.212449 112.318038)
			)
		)
	)
	(zone
		(net 26)
		(net_name "+3.3V")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30067)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 122.904278 114.86) (xy 122.904278 115.14) (xy 123.15 115.25) (xy 123.901 115) (xy 123.221926 114.75)
			)
		)
	)
	(zone
		(net 70)
		(net_name "/~{PCF_INT}")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30087)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 110.819254 85.818651) (xy 111.019254 85.818651) (xy 111.069254 85.668651) (xy 110.919254 85.017651)
				(xy 110.769254 85.668651)
			)
		)
	)
	(zone
		(net 33)
		(net_name "/Human-Machine Interface/Keypad/COL1")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30019)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 78.088115 108.842631) (xy 78.288115 108.842631) (xy 78.608964 108.270093) (xy 78.188115 107.929131)
				(xy 77.767266 108.270093)
			)
		)
	)
	(zone
		(net 8)
		(net_name "Net-(D2:1-A)")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30069)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 76.673246 111.883989) (xy 76.473246 111.883989) (xy 76.239685 112.158074) (xy 76.613115 112.570004)
				(xy 76.986545 112.158074)
			)
		)
	)
	(zone
		(net 30)
		(net_name "/SCK")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30095)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 83.710249 84.218651) (xy 83.510249 84.218651) (xy 83.460249 84.368651) (xy 83.610249 85.019651)
				(xy 83.760249 84.368651)
			)
		)
	)
	(zone
		(net 18)
		(net_name "Net-(D4:3-A)")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30070)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 91.291822 121.173597) (xy 91.091822 121.173597) (xy 90.84317 121.44707) (xy 91.2166 121.859)
				(xy 91.59003 121.44707)
			)
		)
	)
	(zone
		(net 3)
		(net_name "Net-(C2-Pad1)")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30011)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 103.114987 112.659843) (xy 103.114987 112.859843) (xy 103.703883 113.176733) (xy 104.040987 112.74386)
				(xy 103.703883 112.310987)
			)
		)
	)
	(zone
		(net 58)
		(net_name "Net-(JP4-C)")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30064)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 127.475 115.4) (xy 127.475 115.2) (xy 126.951537 115.090224) (xy 126.599 115.475) (xy 127.029458 115.796909)
			)
		)
	)
	(zone
		(net 24)
		(net_name "/TFTDC")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30102)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 106.819254 85.818651) (xy 107.019254 85.818651) (xy 107.069254 85.668651) (xy 106.919254 85.017651)
				(xy 106.769254 85.668651)
			)
		)
	)
	(zone
		(net 59)
		(net_name "/Human-Machine Interface/Audio/~{SD_MODE}")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30058)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 113.504634 92.6) (xy 113.304634 92.6) (xy 113.002045 93.046239) (xy 113.4 93.401) (xy 113.802042 93.048971)
			)
		)
	)
	(zone
		(net 2)
		(net_name "Net-(C1-Pad1)")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30008)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 104.966716 117.590545) (xy 104.966716 117.390545) (xy 104.37782 117.016132) (xy 104.040716 117.449005)
				(xy 104.37782 117.881878)
			)
		)
	)
	(zone
		(net 3)
		(net_name "Net-(C2-Pad1)")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30060)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 103.320132 112.859843) (xy 103.320132 112.659843) (xy 102.872525 112.359843) (xy 102.519132 112.759843)
				(xy 102.872525 113.159843)
			)
		)
	)
	(zone
		(net 26)
		(net_name "+3.3V")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30056)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 105.5 115.160118) (xy 105.7 115.160118) (xy 106.006053 114.715713) (xy 105.610845 114.359118)
				(xy 105.206067 114.709318)
			)
		)
	)
	(zone
		(net 3)
		(net_name "Net-(C2-Pad1)")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30047)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 104.735845 112.604475) (xy 104.735845 112.804475) (xy 105.259308 113.094894) (xy 105.611845 112.710118)
				(xy 105.259308 112.325342)
			)
		)
	)
	(zone
		(net 36)
		(net_name "/Human-Machine Interface/Keypad/COL4")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30022)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 107.932858 100.239273) (xy 108.132858 100.239273) (xy 108.453707 99.666735) (xy 108.032858 99.325773)
				(xy 107.612009 99.666735)
			)
		)
	)
	(zone
		(net 34)
		(net_name "/Human-Machine Interface/Keypad/COL2")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30033)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 85.35 118.1705) (xy 85.55 118.1705) (xy 85.870849 117.597962) (xy 85.45 117.257) (xy 85.029151 117.597962)
			)
		)
	)
	(zone
		(net 60)
		(net_name "/Human-Machine Interface/Audio/GAIN_SLOT")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30002)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 127.85 116.2) (xy 127.85 116.4) (xy 128.35 116.8) (xy 129.101 116.3) (xy 128.35 115.8)
			)
		)
	)
	(embedded_fonts no)
)
