(kicad_pcb
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(general
		(thickness 1.6)
		(legacy_teardrops no)
	)
	(paper "A4")
	(layers
		(0 "F.Cu" signal "Top Layer")
		(2 "B.Cu" signal "Bottom Layer")
		(9 "F.Adhes" user "F.Adhesive")
		(11 "B.Adhes" user "B.Adhesive")
		(13 "F.Paste" user "Top Paste")
		(15 "B.Paste" user "Bottom Paste")
		(5 "F.SilkS" user "Top Overlay")
		(7 "B.SilkS" user "Bottom Overlay")
		(1 "F.Mask" user "Top Solder")
		(3 "B.Mask" user "Bottom Solder")
		(17 "Dwgs.User" user "User.Drawings")
		(19 "Cmts.User" user "User.Comments")
		(21 "Eco1.User" user "User.Eco1")
		(23 "Eco2.User" user "User.Eco2")
		(25 "Edge.Cuts" user)
		(27 "Margin" user)
		(31 "F.CrtYd" user "F.Courtyard")
		(29 "B.CrtYd" user "B.Courtyard")
		(35 "F.Fab" user "Mechanical 12")
		(33 "B.Fab" user "Mechanical 13")
		(39 "User.1" user "Top 3D Body")
		(41 "User.2" user "Board Outline")
		(43 "User.3" user "Top Courtyard")
		(45 "User.4" user "Bottom Courtyard")
		(47 "User.5" user "Top Assembly")
		(49 "User.6" user "Bottom 3D Body")
		(51 "User.7" user "Bottom Assembly")
		(53 "User.8" user "Top 3D Body 2")
		(55 "User.9" user "Bottom 3D Body 2")
		(57 "User.10" user "Board Outline 2")
		(59 "User.11" user "Mechanical 11")
		(61 "User.12" user "Mechanical 14")
		(63 "User.13" user "Mechanical 15")
		(65 "User.14" user "Mechanical 16")
	)
	(setup
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(tenting front back)
		(aux_axis_origin 72.3011 155.8036)
		(grid_origin 72.3011 155.8036)
		(pcbplotparams
			(layerselection 0x00000000_00000000_55555555_575555ff)
			(plot_on_all_layers_selection 0x00000000_00000000_00000000_00000000)
			(disableapertmacros no)
			(usegerberextensions yes)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 4)
			(plotframeref no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(pdf_metadata yes)
			(pdf_single_document no)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plot_black_and_white yes)
			(sketchpadsonfab no)
			(plotpadnumbers no)
			(hidednponfab no)
			(sketchdnponfab yes)
			(crossoutdnponfab yes)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 0)
			(scaleselection 1)
			(outputdirectory "CAM/")
		)
	)
	(property "ADDRESS1" "22605 Gateway Center Drive")
	(property "ADDRESS2" "Clarksburg")
	(property "ADDRESS3" "MD")
	(property "ADDRESS4" "USA 20871")
	(property "DOCUMENTNUMBER" "")
	(property "ORGANIZATION" "Thales DSI")
	(property "SHEETTOTAL" "1")
	(net 0 "")
	(net 1 "Net-(J2-Pin_10)")
	(net 2 "Net-(J2-Pin_2)")
	(net 3 "Net-(J2-Pin_9)")
	(net 4 "Net-(J2-Pin_1)")
	(net 5 "Net-(J2-Pin_4)")
	(net 6 "Net-(J1-PIN2)")
	(net 7 "Net-(J1-PIN1)")
	(net 8 "Net-(J2-Pin_7)")
	(net 9 "Net-(J2-Pin_5)")
	(net 10 "Net-(J2-Pin_8)")
	(net 11 "Net-(J3-Pin_4)")
	(net 12 "Net-(J3-Pin_3)")
	(net 13 "Net-(J3-Pin_5)")
	(net 14 "Net-(J3-Pin_8)")
	(net 15 "Net-(J3-Pin_6)")
	(net 16 "Net-(J3-Pin_7)")
	(net 17 "Net-(J3-Pin_9)")
	(net 18 "Net-(J3-Pin_2)")
	(net 19 "Net-(J3-Pin_1)")
	(net 20 "Net-(J4-Pin_4)")
	(net 21 "Net-(J4-Pin_3)")
	(net 22 "Net-(J4-Pin_7)")
	(net 23 "Net-(J4-Pin_5)")
	(net 24 "Net-(J4-Pin_8)")
	(net 25 "Net-(J4-Pin_6)")
	(net 26 "Net-(J4-Pin_9)")
	(net 27 "Net-(J4-Pin_2)")
	(net 28 "Net-(J4-Pin_1)")
	(net 29 "Net-(J2-Pin_6)")
	(net 30 "Net-(J2-Pin_3)")
	(net 31 "GND")
	(footprint "t_connectors:PinHeader_1x10_P2.54mm_small"
		(layer "F.Cu")
		(at 142.7861 84.0486)
		(descr "Through hole straight pin header, 1x10, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x10 2.54mm single row")
		(property "Reference" "J4"
			(at -2.54 -1.27 0)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_01x10"
			(at 0 25.24 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x10, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "/")
		(sheetfile "FFC_Breakout_2.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 11.43 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.7 1.4)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 28 "Net-(J4-Pin_1)")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 2.54)
			(size 1.7 1.4)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 27 "Net-(J4-Pin_2)")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 0 5.08)
			(size 1.7 1.4)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 21 "Net-(J4-Pin_3)")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole oval
			(at 0 7.62)
			(size 1.7 1.4)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 20 "Net-(J4-Pin_4)")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(pad "5" thru_hole oval
			(at 0 10.16)
			(size 1.7 1.4)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 23 "Net-(J4-Pin_5)")
			(pinfunction "Pin_5")
			(pintype "passive")
		)
		(pad "6" thru_hole oval
			(at 0 12.7)
			(size 1.7 1.4)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 25 "Net-(J4-Pin_6)")
			(pinfunction "Pin_6")
			(pintype "passive")
		)
		(pad "7" thru_hole oval
			(at 0 15.24)
			(size 1.7 1.4)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 22 "Net-(J4-Pin_7)")
			(pinfunction "Pin_7")
			(pintype "passive")
		)
		(pad "8" thru_hole oval
			(at 0 17.78)
			(size 1.7 1.4)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 24 "Net-(J4-Pin_8)")
			(pinfunction "Pin_8")
			(pintype "passive")
		)
		(pad "9" thru_hole oval
			(at 0 20.32)
			(size 1.7 1.4)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 26 "Net-(J4-Pin_9)")
			(pinfunction "Pin_9")
			(pintype "passive")
		)
		(pad "10" thru_hole oval
			(at 0 22.86)
			(size 1.7 1.4)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "Net-(J1-PIN2)")
			(pinfunction "Pin_10")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x10_P2.54mm_Vertical.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_connectors:CON_30P_FPC_5MM_C"
		(layer "F.Cu")
		(at 152.9715 95.504 90)
		(property "Reference" "J5"
			(at -12.065 1.905 180)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "~"
			(at 10.303002 -4.506365 180)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "CONN FFC FPC 30POS DUAL 0.5mm"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*CON_30P_FPC_5MM_C*")
		(sheetname "/")
		(sheetfile "FFC_Breakout_2.kicad_sch")
		(pad "1" smd rect
			(at -7.25 -1.95 90)
			(size 0.3302 0.889)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 6 "Net-(J1-PIN2)")
			(pinfunction "1")
			(pintype "passive")
			(solder_mask_margin 0.0508)
		)
		(pad "2" smd rect
			(at -6.75 -1.95 90)
			(size 0.3302 0.889)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 7 "Net-(J1-PIN1)")
			(pinfunction "2")
			(pintype "passive")
			(solder_mask_margin 0.0508)
		)
		(pad "3" smd rect
			(at -6.25 -1.95 90)
			(size 0.3302 0.889)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "Net-(J2-Pin_10)")
			(pinfunction "3")
			(pintype "passive")
			(solder_mask_margin 0.0508)
		)
		(pad "4" smd rect
			(at -5.75 -1.95 90)
			(size 0.3302 0.889)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 26 "Net-(J4-Pin_9)")
			(pinfunction "4")
			(pintype "passive")
			(solder_mask_margin 0.0508)
		)
		(pad "5" smd rect
			(at -5.25 -1.95 90)
			(size 0.3302 0.889)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 17 "Net-(J3-Pin_9)")
			(pinfunction "5")
			(pintype "passive")
			(solder_mask_margin 0.0508)
		)
		(pad "6" smd rect
			(at -4.75 -1.95 90)
			(size 0.3302 0.889)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 3 "Net-(J2-Pin_9)")
			(pinfunction "6")
			(pintype "passive")
			(solder_mask_margin 0.0508)
		)
		(pad "7" smd rect
			(at -4.25 -1.95 90)
			(size 0.3302 0.889)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 24 "Net-(J4-Pin_8)")
			(pinfunction "7")
			(pintype "passive")
			(solder_mask_margin 0.0508)
		)
		(pad "8" smd rect
			(at -3.75 -1.95 90)
			(size 0.3302 0.889)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 14 "Net-(J3-Pin_8)")
			(pinfunction "8")
			(pintype "passive")
			(solder_mask_margin 0.0508)
		)
		(pad "9" smd rect
			(at -3.25 -1.95 90)
			(size 0.3302 0.889)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 10 "Net-(J2-Pin_8)")
			(pinfunction "9")
			(pintype "passive")
			(solder_mask_margin 0.0508)
		)
		(pad "10" smd rect
			(at -2.75 -1.95 90)
			(size 0.3302 0.889)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 22 "Net-(J4-Pin_7)")
			(pinfunction "10")
			(pintype "passive")
			(solder_mask_margin 0.0508)
		)
		(pad "11" smd rect
			(at -2.25 -1.95 90)
			(size 0.3302 0.889)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 16 "Net-(J3-Pin_7)")
			(pinfunction "11")
			(pintype "passive")
			(solder_mask_margin 0.0508)
		)
		(pad "12" smd rect
			(at -1.75 -1.95 90)
			(size 0.3302 0.889)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 8 "Net-(J2-Pin_7)")
			(pinfunction "12")
			(pintype "passive")
			(solder_mask_margin 0.0508)
		)
		(pad "13" smd rect
			(at -1.25 -1.95 90)
			(size 0.3302 0.889)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 25 "Net-(J4-Pin_6)")
			(pinfunction "13")
			(pintype "passive")
			(solder_mask_margin 0.0508)
		)
		(pad "14" smd rect
			(at -0.75 -1.95 90)
			(size 0.3302 0.889)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 15 "Net-(J3-Pin_6)")
			(pinfunction "14")
			(pintype "passive")
			(solder_mask_margin 0.0508)
		)
		(pad "15" smd rect
			(at -0.25 -1.95 90)
			(size 0.3302 0.889)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 29 "Net-(J2-Pin_6)")
			(pinfunction "15")
			(pintype "passive")
			(solder_mask_margin 0.0508)
		)
		(pad "16" smd rect
			(at 0.25 -1.95 90)
			(size 0.3302 0.889)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 23 "Net-(J4-Pin_5)")
			(pinfunction "16")
			(pintype "passive")
			(solder_mask_margin 0.0508)
		)
		(pad "17" smd rect
			(at 0.75 -1.95 90)
			(size 0.3302 0.889)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 13 "Net-(J3-Pin_5)")
			(pinfunction "17")
			(pintype "passive")
			(solder_mask_margin 0.0508)
		)
		(pad "18" smd rect
			(at 1.25 -1.95 90)
			(size 0.3302 0.889)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 9 "Net-(J2-Pin_5)")
			(pinfunction "18")
			(pintype "passive")
			(solder_mask_margin 0.0508)
		)
		(pad "19" smd rect
			(at 1.75 -1.95 90)
			(size 0.3302 0.889)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 20 "Net-(J4-Pin_4)")
			(pinfunction "19")
			(pintype "passive")
			(solder_mask_margin 0.0508)
		)
		(pad "20" smd rect
			(at 2.25 -1.95 90)
			(size 0.3302 0.889)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 11 "Net-(J3-Pin_4)")
			(pinfunction "20")
			(pintype "passive")
			(solder_mask_margin 0.0508)
		)
		(pad "21" smd rect
			(at 2.75 -1.95 90)
			(size 0.3302 0.889)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 5 "Net-(J2-Pin_4)")
			(pinfunction "21")
			(pintype "passive")
			(solder_mask_margin 0.0508)
		)
		(pad "22" smd rect
			(at 3.25 -1.95 90)
			(size 0.3302 0.889)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 21 "Net-(J4-Pin_3)")
			(pinfunction "22")
			(pintype "passive")
			(solder_mask_margin 0.0508)
		)
		(pad "23" smd rect
			(at 3.75 -1.95 90)
			(size 0.3302 0.889)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 12 "Net-(J3-Pin_3)")
			(pinfunction "23")
			(pintype "passive")
			(solder_mask_margin 0.0508)
		)
		(pad "24" smd rect
			(at 4.25 -1.95 90)
			(size 0.3302 0.889)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 30 "Net-(J2-Pin_3)")
			(pinfunction "24")
			(pintype "passive")
			(solder_mask_margin 0.0508)
		)
		(pad "25" smd rect
			(at 4.75 -1.95 90)
			(size 0.3302 0.889)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 27 "Net-(J4-Pin_2)")
			(pinfunction "25")
			(pintype "passive")
			(solder_mask_margin 0.0508)
		)
		(pad "26" smd rect
			(at 5.25 -1.95 90)
			(size 0.3302 0.889)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 18 "Net-(J3-Pin_2)")
			(pinfunction "26")
			(pintype "passive")
			(solder_mask_margin 0.0508)
		)
		(pad "27" smd rect
			(at 5.75 -1.95 90)
			(size 0.3302 0.889)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "Net-(J2-Pin_2)")
			(pinfunction "27")
			(pintype "passive")
			(solder_mask_margin 0.0508)
		)
		(pad "28" smd rect
			(at 6.25 -1.95 90)
			(size 0.3302 0.889)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 28 "Net-(J4-Pin_1)")
			(pinfunction "28")
			(pintype "passive")
			(solder_mask_margin 0.0508)
		)
		(pad "29" smd rect
			(at 6.75 -1.95 90)
			(size 0.3302 0.889)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 19 "Net-(J3-Pin_1)")
			(pinfunction "PIN1")
			(pintype "passive")
			(solder_mask_margin 0.0508)
		)
		(pad "30" smd rect
			(at 7.25 -1.95 90)
			(size 0.3302 0.889)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 4 "Net-(J2-Pin_1)")
			(pinfunction "PIN2")
			(pintype "passive")
			(solder_mask_margin 0.0508)
		)
		(pad "31" smd rect
			(at -8.3 0.55 90)
			(size 0.762 1.1938)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 31 "GND")
			(pinfunction "TAB1")
			(pintype "passive")
			(solder_mask_margin 0.0508)
		)
		(pad "32" smd rect
			(at 8.3 0.55 90)
			(size 0.762 1.1938)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 31 "GND")
			(pinfunction "TAB2")
			(pintype "passive")
			(solder_mask_margin 0.0508)
		)
		(embedded_fonts no)
		(embedded_files
			(file
				(name "ayf533035-closed.step")
				(type other)
			)
		)
		(model "kicad-embed://ayf533035-closed.step"
			(offset
				(xyz 0 0.75 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 -0 0)
			)
		)
	)
	(footprint "t_connectors:PinHeader_1x10_P2.54mm_small"
		(layer "F.Cu")
		(at 132.6261 84.0486)
		(descr "Through hole straight pin header, 1x10, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x10 2.54mm single row")
		(property "Reference" "J2"
			(at -3.175 -1.38 0)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_01x10"
			(at 0 25.24 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x10, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "/")
		(sheetfile "FFC_Breakout_2.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 11.43 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.7 1.4)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "Net-(J2-Pin_1)")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 2.54)
			(size 1.7 1.4)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "Net-(J2-Pin_2)")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 0 5.08)
			(size 1.7 1.4)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 30 "Net-(J2-Pin_3)")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole oval
			(at 0 7.62)
			(size 1.7 1.4)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "Net-(J2-Pin_4)")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(pad "5" thru_hole oval
			(at 0 10.16)
			(size 1.7 1.4)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 9 "Net-(J2-Pin_5)")
			(pinfunction "Pin_5")
			(pintype "passive")
		)
		(pad "6" thru_hole oval
			(at 0 12.7)
			(size 1.7 1.4)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 29 "Net-(J2-Pin_6)")
			(pinfunction "Pin_6")
			(pintype "passive")
		)
		(pad "7" thru_hole oval
			(at 0 15.24)
			(size 1.7 1.4)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 8 "Net-(J2-Pin_7)")
			(pinfunction "Pin_7")
			(pintype "passive")
		)
		(pad "8" thru_hole oval
			(at 0 17.78)
			(size 1.7 1.4)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 10 "Net-(J2-Pin_8)")
			(pinfunction "Pin_8")
			(pintype "passive")
		)
		(pad "9" thru_hole oval
			(at 0 20.32)
			(size 1.7 1.4)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "Net-(J2-Pin_9)")
			(pinfunction "Pin_9")
			(pintype "passive")
		)
		(pad "10" thru_hole oval
			(at 0 22.86)
			(size 1.7 1.4)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "Net-(J2-Pin_10)")
			(pinfunction "Pin_10")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x10_P2.54mm_Vertical.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "t_connectors:CON_30P_FPC_5MM_C"
		(locked yes)
		(layer "F.Cu")
		(at 124.3711 95.4786 -90)
		(property "Reference" "J1"
			(at -12.065 1.905 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "~"
			(at 10.303002 -4.506365 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "CONN FFC FPC 30POS DUAL 0.5mm"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*CON_30P_FPC_5MM_C*")
		(sheetname "/")
		(sheetfile "FFC_Breakout_2.kicad_sch")
		(pad "1" smd rect
			(at -7.25 -1.95 270)
			(size 0.3302 0.889)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 4 "Net-(J2-Pin_1)")
			(pinfunction "1")
			(pintype "passive")
			(solder_mask_margin 0.0508)
		)
		(pad "2" smd rect
			(at -6.75 -1.95 270)
			(size 0.3302 0.889)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 19 "Net-(J3-Pin_1)")
			(pinfunction "2")
			(pintype "passive")
			(solder_mask_margin 0.0508)
		)
		(pad "3" smd rect
			(at -6.25 -1.95 270)
			(size 0.3302 0.889)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 28 "Net-(J4-Pin_1)")
			(pinfunction "3")
			(pintype "passive")
			(solder_mask_margin 0.0508)
		)
		(pad "4" smd rect
			(at -5.75 -1.95 270)
			(size 0.3302 0.889)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "Net-(J2-Pin_2)")
			(pinfunction "4")
			(pintype "passive")
			(solder_mask_margin 0.0508)
		)
		(pad "5" smd rect
			(at -5.25 -1.95 270)
			(size 0.3302 0.889)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 18 "Net-(J3-Pin_2)")
			(pinfunction "5")
			(pintype "passive")
			(solder_mask_margin 0.0508)
		)
		(pad "6" smd rect
			(at -4.75 -1.95 270)
			(size 0.3302 0.889)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 27 "Net-(J4-Pin_2)")
			(pinfunction "6")
			(pintype "passive")
			(solder_mask_margin 0.0508)
		)
		(pad "7" smd rect
			(at -4.25 -1.95 270)
			(size 0.3302 0.889)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 30 "Net-(J2-Pin_3)")
			(pinfunction "7")
			(pintype "passive")
			(solder_mask_margin 0.0508)
		)
		(pad "8" smd rect
			(at -3.75 -1.95 270)
			(size 0.3302 0.889)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 12 "Net-(J3-Pin_3)")
			(pinfunction "8")
			(pintype "passive")
			(solder_mask_margin 0.0508)
		)
		(pad "9" smd rect
			(at -3.25 -1.95 270)
			(size 0.3302 0.889)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 21 "Net-(J4-Pin_3)")
			(pinfunction "9")
			(pintype "passive")
			(solder_mask_margin 0.0508)
		)
		(pad "10" smd rect
			(at -2.75 -1.95 270)
			(size 0.3302 0.889)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 5 "Net-(J2-Pin_4)")
			(pinfunction "10")
			(pintype "passive")
			(solder_mask_margin 0.0508)
		)
		(pad "11" smd rect
			(at -2.25 -1.95 270)
			(size 0.3302 0.889)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 11 "Net-(J3-Pin_4)")
			(pinfunction "11")
			(pintype "passive")
			(solder_mask_margin 0.0508)
		)
		(pad "12" smd rect
			(at -1.75 -1.95 270)
			(size 0.3302 0.889)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 20 "Net-(J4-Pin_4)")
			(pinfunction "12")
			(pintype "passive")
			(solder_mask_margin 0.0508)
		)
		(pad "13" smd rect
			(at -1.25 -1.95 270)
			(size 0.3302 0.889)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 9 "Net-(J2-Pin_5)")
			(pinfunction "13")
			(pintype "passive")
			(solder_mask_margin 0.0508)
		)
		(pad "14" smd rect
			(at -0.75 -1.95 270)
			(size 0.3302 0.889)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 13 "Net-(J3-Pin_5)")
			(pinfunction "14")
			(pintype "passive")
			(solder_mask_margin 0.0508)
		)
		(pad "15" smd rect
			(at -0.25 -1.95 270)
			(size 0.3302 0.889)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 23 "Net-(J4-Pin_5)")
			(pinfunction "15")
			(pintype "passive")
			(solder_mask_margin 0.0508)
		)
		(pad "16" smd rect
			(at 0.25 -1.95 270)
			(size 0.3302 0.889)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 29 "Net-(J2-Pin_6)")
			(pinfunction "16")
			(pintype "passive")
			(solder_mask_margin 0.0508)
		)
		(pad "17" smd rect
			(at 0.75 -1.95 270)
			(size 0.3302 0.889)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 15 "Net-(J3-Pin_6)")
			(pinfunction "17")
			(pintype "passive")
			(solder_mask_margin 0.0508)
		)
		(pad "18" smd rect
			(at 1.25 -1.95 270)
			(size 0.3302 0.889)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 25 "Net-(J4-Pin_6)")
			(pinfunction "18")
			(pintype "passive")
			(solder_mask_margin 0.0508)
		)
		(pad "19" smd rect
			(at 1.75 -1.95 270)
			(size 0.3302 0.889)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 8 "Net-(J2-Pin_7)")
			(pinfunction "19")
			(pintype "passive")
			(solder_mask_margin 0.0508)
		)
		(pad "20" smd rect
			(at 2.25 -1.95 270)
			(size 0.3302 0.889)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 16 "Net-(J3-Pin_7)")
			(pinfunction "20")
			(pintype "passive")
			(solder_mask_margin 0.0508)
		)
		(pad "21" smd rect
			(at 2.75 -1.95 270)
			(size 0.3302 0.889)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 22 "Net-(J4-Pin_7)")
			(pinfunction "21")
			(pintype "passive")
			(solder_mask_margin 0.0508)
		)
		(pad "22" smd rect
			(at 3.25 -1.95 270)
			(size 0.3302 0.889)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 10 "Net-(J2-Pin_8)")
			(pinfunction "22")
			(pintype "passive")
			(solder_mask_margin 0.0508)
		)
		(pad "23" smd rect
			(at 3.75 -1.95 270)
			(size 0.3302 0.889)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 14 "Net-(J3-Pin_8)")
			(pinfunction "23")
			(pintype "passive")
			(solder_mask_margin 0.0508)
		)
		(pad "24" smd rect
			(at 4.25 -1.95 270)
			(size 0.3302 0.889)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 24 "Net-(J4-Pin_8)")
			(pinfunction "24")
			(pintype "passive")
			(solder_mask_margin 0.0508)
		)
		(pad "25" smd rect
			(at 4.75 -1.95 270)
			(size 0.3302 0.889)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 3 "Net-(J2-Pin_9)")
			(pinfunction "25")
			(pintype "passive")
			(solder_mask_margin 0.0508)
		)
		(pad "26" smd rect
			(at 5.25 -1.95 270)
			(size 0.3302 0.889)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 17 "Net-(J3-Pin_9)")
			(pinfunction "26")
			(pintype "passive")
			(solder_mask_margin 0.0508)
		)
		(pad "27" smd rect
			(at 5.75 -1.95 270)
			(size 0.3302 0.889)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 26 "Net-(J4-Pin_9)")
			(pinfunction "27")
			(pintype "passive")
			(solder_mask_margin 0.0508)
		)
		(pad "28" smd rect
			(at 6.25 -1.95 270)
			(size 0.3302 0.889)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "Net-(J2-Pin_10)")
			(pinfunction "28")
			(pintype "passive")
			(solder_mask_margin 0.0508)
		)
		(pad "29" smd rect
			(at 6.75 -1.95 270)
			(size 0.3302 0.889)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 7 "Net-(J1-PIN1)")
			(pinfunction "PIN1")
			(pintype "passive")
			(solder_mask_margin 0.0508)
		)
		(pad "30" smd rect
			(at 7.25 -1.95 270)
			(size 0.3302 0.889)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 6 "Net-(J1-PIN2)")
			(pinfunction "PIN2")
			(pintype "passive")
			(solder_mask_margin 0.0508)
		)
		(pad "31" smd rect
			(at -8.3 0.55 270)
			(size 0.762 1.1938)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 31 "GND")
			(pinfunction "TAB1")
			(pintype "passive")
			(solder_mask_margin 0.0508)
		)
		(pad "32" smd rect
			(at 8.3 0.55 270)
			(size 0.762 1.1938)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 31 "GND")
			(pinfunction "TAB2")
			(pintype "passive")
			(solder_mask_margin 0.0508)
		)
		(embedded_fonts no)
		(embedded_files
			(file
				(name "ayf533035-closed.step")
				(type other)
			)
		)
		(model "kicad-embed://ayf533035-closed.step"
			(offset
				(xyz 0 0.75 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 -0 0)
			)
		)
	)
	(footprint "footprints:CONN30_FH28D-30S-0.5SH05_HIR"
		(layer "F.Cu")
		(at 122.458288 95.483599 -90)
		(tags "FH28D-30S-0.5SH05 ")
		(property "Reference" "REF**"
			(at 0 -3.702812 270)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "CONN30_FH28D-30S-0.5SH05_HIR"
			(at 0 -3.702812 270)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -3.702812 270)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -7.250001 -3.702812 270)
			(size 0.3302 1.397)
			(layers "F.Cu" "F.Mask" "F.Paste")
		)
		(pad "2" smd rect
			(at -6.749999 -3.702812 270)
			(size 0.3302 1.397)
			(layers "F.Cu" "F.Mask" "F.Paste")
		)
		(pad "3" smd rect
			(at -6.25 -3.702812 270)
			(size 0.3302 1.397)
			(layers "F.Cu" "F.Mask" "F.Paste")
		)
		(pad "4" smd rect
			(at -5.750001 -3.702812 270)
			(size 0.3302 1.397)
			(layers "F.Cu" "F.Mask" "F.Paste")
		)
		(pad "5" smd rect
			(at -5.25 -3.702812 270)
			(size 0.3302 1.397)
			(layers "F.Cu" "F.Mask" "F.Paste")
		)
		(pad "6" smd rect
			(at -4.750001 -3.702812 270)
			(size 0.3302 1.397)
			(layers "F.Cu" "F.Mask" "F.Paste")
		)
		(pad "7" smd rect
			(at -4.249999 -3.702812 270)
			(size 0.3302 1.397)
			(layers "F.Cu" "F.Mask" "F.Paste")
		)
		(pad "8" smd rect
			(at -3.75 -3.702812 270)
			(size 0.3302 1.397)
			(layers "F.Cu" "F.Mask" "F.Paste")
		)
		(pad "9" smd rect
			(at -3.250001 -3.702812 270)
			(size 0.3302 1.397)
			(layers "F.Cu" "F.Mask" "F.Paste")
		)
		(pad "10" smd rect
			(at -2.75 -3.702812 270)
			(size 0.3302 1.397)
			(layers "F.Cu" "F.Mask" "F.Paste")
		)
		(pad "11" smd rect
			(at -2.250001 -3.702812 270)
			(size 0.3302 1.397)
			(layers "F.Cu" "F.Mask" "F.Paste")
		)
		(pad "12" smd rect
			(at -1.749999 -3.702812 270)
			(size 0.3302 1.397)
			(layers "F.Cu" "F.Mask" "F.Paste")
		)
		(pad "13" smd rect
			(at -1.25 -3.702812 270)
			(size 0.3302 1.397)
			(layers "F.Cu" "F.Mask" "F.Paste")
		)
		(pad "14" smd rect
			(at -0.750001 -3.702812 270)
			(size 0.3302 1.397)
			(layers "F.Cu" "F.Mask" "F.Paste")
		)
		(pad "15" smd rect
			(at -0.25 -3.702812 270)
			(size 0.3302 1.397)
			(layers "F.Cu" "F.Mask" "F.Paste")
		)
		(pad "16" smd rect
			(at 0.25 -3.702812 270)
			(size 0.3302 1.397)
			(layers "F.Cu" "F.Mask" "F.Paste")
		)
		(pad "17" smd rect
			(at 0.750001 -3.702812 270)
			(size 0.3302 1.397)
			(layers "F.Cu" "F.Mask" "F.Paste")
		)
		(pad "18" smd rect
			(at 1.25 -3.702812 270)
			(size 0.3302 1.397)
			(layers "F.Cu" "F.Mask" "F.Paste")
		)
		(pad "19" smd rect
			(at 1.749999 -3.702812 270)
			(size 0.3302 1.397)
			(layers "F.Cu" "F.Mask" "F.Paste")
		)
		(pad "20" smd rect
			(at 2.250001 -3.702812 270)
			(size 0.3302 1.397)
			(layers "F.Cu" "F.Mask" "F.Paste")
		)
		(pad "21" smd rect
			(at 2.75 -3.702812 270)
			(size 0.3302 1.397)
			(layers "F.Cu" "F.Mask" "F.Paste")
		)
		(pad "22" smd rect
			(at 3.250001 -3.702812 270)
			(size 0.3302 1.397)
			(layers "F.Cu" "F.Mask" "F.Paste")
		)
		(pad "23" smd rect
			(at 3.75 -3.702812 270)
			(size 0.3302 1.397)
			(layers "F.Cu" "F.Mask" "F.Paste")
		)
		(pad "24" smd rect
			(at 4.249999 -3.702812 270)
			(size 0.3302 1.397)
			(layers "F.Cu" "F.Mask" "F.Paste")
		)
		(pad "25" smd rect
			(at 4.750001 -3.702812 270)
			(size 0.3302 1.397)
			(layers "F.Cu" "F.Mask" "F.Paste")
		)
		(pad "26" smd rect
			(at 5.25 -3.702812 270)
			(size 0.3302 1.397)
			(layers "F.Cu" "F.Mask" "F.Paste")
		)
		(pad "27" smd rect
			(at 5.750001 -3.702812 270)
			(size 0.3302 1.397)
			(layers "F.Cu" "F.Mask" "F.Paste")
		)
		(pad "28" smd rect
			(at 6.25 -3.702812 270)
			(size 0.3302 1.397)
			(layers "F.Cu" "F.Mask" "F.Paste")
		)
		(pad "29" smd rect
			(at 6.749999 -3.702812 270)
			(size 0.3302 1.397)
			(layers "F.Cu" "F.Mask" "F.Paste")
		)
		(pad "30" smd rect
			(at 7.250001 -3.702812 270)
			(size 0.3302 1.397)
			(layers "F.Cu" "F.Mask" "F.Paste")
		)
		(pad "31" smd rect
			(at -9.399999 1.947187)
			(size 2.3114 1.8034)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 31 "GND")
		)
		(pad "32" smd rect
			(at 9.399999 1.947187)
			(size 2.3114 1.8034)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 31 "GND")
		)
		(embedded_fonts no)
	)
	(footprint "t_connectors:PinHeader_1x10_P2.54mm_small"
		(layer "F.Cu")
		(at 137.7061 84.0486)
		(descr "Through hole straight pin header, 1x10, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x10 2.54mm single row")
		(property "Reference" "J3"
			(at -2.54 -1.27 0)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_01x10"
			(at 0 25.24 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x10, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "/")
		(sheetfile "FFC_Breakout_2.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 11.43 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.7 1.4)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 19 "Net-(J3-Pin_1)")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 2.54)
			(size 1.7 1.4)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 18 "Net-(J3-Pin_2)")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 0 5.08)
			(size 1.7 1.4)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 12 "Net-(J3-Pin_3)")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole oval
			(at 0 7.62)
			(size 1.7 1.4)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 11 "Net-(J3-Pin_4)")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(pad "5" thru_hole oval
			(at 0 10.16)
			(size 1.7 1.4)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 13 "Net-(J3-Pin_5)")
			(pinfunction "Pin_5")
			(pintype "passive")
		)
		(pad "6" thru_hole oval
			(at 0 12.7)
			(size 1.7 1.4)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 15 "Net-(J3-Pin_6)")
			(pinfunction "Pin_6")
			(pintype "passive")
		)
		(pad "7" thru_hole oval
			(at 0 15.24)
			(size 1.7 1.4)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 16 "Net-(J3-Pin_7)")
			(pinfunction "Pin_7")
			(pintype "passive")
		)
		(pad "8" thru_hole oval
			(at 0 17.78)
			(size 1.7 1.4)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 14 "Net-(J3-Pin_8)")
			(pinfunction "Pin_8")
			(pintype "passive")
		)
		(pad "9" thru_hole oval
			(at 0 20.32)
			(size 1.7 1.4)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 17 "Net-(J3-Pin_9)")
			(pinfunction "Pin_9")
			(pintype "passive")
		)
		(pad "10" thru_hole oval
			(at 0 22.86)
			(size 1.7 1.4)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 7 "Net-(J1-PIN1)")
			(pinfunction "Pin_10")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x10_P2.54mm_Vertical.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:CONN30_FH28D-30S-0.5SH05_HIR"
		(layer "F.Cu")
		(at 154.943912 95.503599 90)
		(tags "FH28D-30S-0.5SH05 ")
		(property "Reference" "REF**"
			(at 0 -3.702812 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "CONN30_FH28D-30S-0.5SH05_HIR"
			(at 0 -3.702812 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -3.702812 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -7.250001 -3.702812 90)
			(size 0.3302 1.397)
			(layers "F.Cu" "F.Mask" "F.Paste")
		)
		(pad "2" smd rect
			(at -6.749999 -3.702812 90)
			(size 0.3302 1.397)
			(layers "F.Cu" "F.Mask" "F.Paste")
		)
		(pad "3" smd rect
			(at -6.25 -3.702812 90)
			(size 0.3302 1.397)
			(layers "F.Cu" "F.Mask" "F.Paste")
		)
		(pad "4" smd rect
			(at -5.750001 -3.702812 90)
			(size 0.3302 1.397)
			(layers "F.Cu" "F.Mask" "F.Paste")
		)
		(pad "5" smd rect
			(at -5.25 -3.702812 90)
			(size 0.3302 1.397)
			(layers "F.Cu" "F.Mask" "F.Paste")
		)
		(pad "6" smd rect
			(at -4.750001 -3.702812 90)
			(size 0.3302 1.397)
			(layers "F.Cu" "F.Mask" "F.Paste")
		)
		(pad "7" smd rect
			(at -4.249999 -3.702812 90)
			(size 0.3302 1.397)
			(layers "F.Cu" "F.Mask" "F.Paste")
		)
		(pad "8" smd rect
			(at -3.75 -3.702812 90)
			(size 0.3302 1.397)
			(layers "F.Cu" "F.Mask" "F.Paste")
		)
		(pad "9" smd rect
			(at -3.250001 -3.702812 90)
			(size 0.3302 1.397)
			(layers "F.Cu" "F.Mask" "F.Paste")
		)
		(pad "10" smd rect
			(at -2.75 -3.702812 90)
			(size 0.3302 1.397)
			(layers "F.Cu" "F.Mask" "F.Paste")
		)
		(pad "11" smd rect
			(at -2.250001 -3.702812 90)
			(size 0.3302 1.397)
			(layers "F.Cu" "F.Mask" "F.Paste")
		)
		(pad "12" smd rect
			(at -1.749999 -3.702812 90)
			(size 0.3302 1.397)
			(layers "F.Cu" "F.Mask" "F.Paste")
		)
		(pad "13" smd rect
			(at -1.25 -3.702812 90)
			(size 0.3302 1.397)
			(layers "F.Cu" "F.Mask" "F.Paste")
		)
		(pad "14" smd rect
			(at -0.750001 -3.702812 90)
			(size 0.3302 1.397)
			(layers "F.Cu" "F.Mask" "F.Paste")
		)
		(pad "15" smd rect
			(at -0.25 -3.702812 90)
			(size 0.3302 1.397)
			(layers "F.Cu" "F.Mask" "F.Paste")
		)
		(pad "16" smd rect
			(at 0.25 -3.702812 90)
			(size 0.3302 1.397)
			(layers "F.Cu" "F.Mask" "F.Paste")
		)
		(pad "17" smd rect
			(at 0.750001 -3.702812 90)
			(size 0.3302 1.397)
			(layers "F.Cu" "F.Mask" "F.Paste")
		)
		(pad "18" smd rect
			(at 1.25 -3.702812 90)
			(size 0.3302 1.397)
			(layers "F.Cu" "F.Mask" "F.Paste")
		)
		(pad "19" smd rect
			(at 1.749999 -3.702812 90)
			(size 0.3302 1.397)
			(layers "F.Cu" "F.Mask" "F.Paste")
		)
		(pad "20" smd rect
			(at 2.250001 -3.702812 90)
			(size 0.3302 1.397)
			(layers "F.Cu" "F.Mask" "F.Paste")
		)
		(pad "21" smd rect
			(at 2.75 -3.702812 90)
			(size 0.3302 1.397)
			(layers "F.Cu" "F.Mask" "F.Paste")
		)
		(pad "22" smd rect
			(at 3.250001 -3.702812 90)
			(size 0.3302 1.397)
			(layers "F.Cu" "F.Mask" "F.Paste")
		)
		(pad "23" smd rect
			(at 3.75 -3.702812 90)
			(size 0.3302 1.397)
			(layers "F.Cu" "F.Mask" "F.Paste")
		)
		(pad "24" smd rect
			(at 4.249999 -3.702812 90)
			(size 0.3302 1.397)
			(layers "F.Cu" "F.Mask" "F.Paste")
		)
		(pad "25" smd rect
			(at 4.750001 -3.702812 90)
			(size 0.3302 1.397)
			(layers "F.Cu" "F.Mask" "F.Paste")
		)
		(pad "26" smd rect
			(at 5.25 -3.702812 90)
			(size 0.3302 1.397)
			(layers "F.Cu" "F.Mask" "F.Paste")
		)
		(pad "27" smd rect
			(at 5.750001 -3.702812 90)
			(size 0.3302 1.397)
			(layers "F.Cu" "F.Mask" "F.Paste")
		)
		(pad "28" smd rect
			(at 6.25 -3.702812 90)
			(size 0.3302 1.397)
			(layers "F.Cu" "F.Mask" "F.Paste")
		)
		(pad "29" smd rect
			(at 6.749999 -3.702812 90)
			(size 0.3302 1.397)
			(layers "F.Cu" "F.Mask" "F.Paste")
		)
		(pad "30" smd rect
			(at 7.250001 -3.702812 90)
			(size 0.3302 1.397)
			(layers "F.Cu" "F.Mask" "F.Paste")
		)
		(pad "31" smd rect
			(at -9.399999 1.947187 180)
			(size 2.3114 1.8034)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 31 "GND")
		)
		(pad "32" smd rect
			(at 9.399999 1.947187 180)
			(size 2.3114 1.8034)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 31 "GND")
		)
		(embedded_fonts no)
	)
	(gr_line
		(start 158.6611 82.7786)
		(end 157.3911 81.5086)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 118.6561 108.1786)
		(end 119.9261 109.4486)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 143.4211 81.5086)
		(end 119.9261 81.5086)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 157.3911 81.5086)
		(end 143.4211 81.5086)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 158.6611 108.1786)
		(end 158.6611 82.7786)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 118.6561 82.7786)
		(end 118.6561 108.1786)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 157.3911 109.4486)
		(end 158.6611 108.1786)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 143.4211 109.4486)
		(end 119.9261 109.4486)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 143.4211 109.4486)
		(end 157.3911 109.4486)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 118.6561 82.7786)
		(end 119.9261 81.5086)
		(layer "Edge.Cuts")
	)
	(gr_text "1"
		(at 131.2291 84.6836 0)
		(layer "B.SilkS")
	)
	(gr_text "4"
		(at 131.2291 87.2236 0)
		(layer "B.SilkS")
	)
	(gr_text "8"
		(at 136.3091 89.7636 0)
		(layer "B.SilkS")
	)
	(gr_text "18"
		(at 141.3891 97.3836 0)
		(layer "B.SilkS")
	)
	(gr_text "5"
		(at 136.3091 87.2236 0)
		(layer "B.SilkS")
	)
	(gr_text "25"
		(at 131.2291 105.0036 0)
		(layer "B.SilkS")
	)
	(gr_text "16"
		(at 131.2291 97.3836 0)
		(layer "B.SilkS")
	)
	(gr_text "FFC-30 Breakout Board"
		(at 120.5611 106.9086 270)
		(layer "B.SilkS")
	)
	(gr_text "->\n"
		(at 130.0861 84.6836 0)
		(layer "B.SilkS")
	)
	(gr_text "19"
		(at 131.2291 99.9236 0)
		(layer "B.SilkS")
	)
	(gr_text "23"
		(at 136.3091 102.4636 0)
		(layer "B.SilkS")
	)
	(gr_text "17"
		(at 136.3091 97.3836 0)
		(layer "B.SilkS")
	)
	(gr_text "12"
		(at 141.3891 92.0496 0)
		(layer "B.SilkS")
	)
	(gr_text "9"
		(at 141.3891 89.7636 0)
		(layer "B.SilkS")
	)
	(gr_text "10"
		(at 131.2291 92.0496 0)
		(layer "B.SilkS")
	)
	(gr_text "13"
		(at 131.2291 94.8436 0)
		(layer "B.SilkS")
	)
	(gr_text "7"
		(at 131.2291 89.7636 0)
		(layer "B.SilkS")
	)
	(gr_text "6"
		(at 141.3891 87.2236 0)
		(layer "B.SilkS")
	)
	(gr_text "numbering for this \nconnector v"
		(at 122.4661 96.1136 270)
		(layer "B.SilkS")
	)
	(gr_text "11"
		(at 136.3091 92.0496 0)
		(layer "B.SilkS")
	)
	(gr_text "22"
		(at 131.2291 102.4636 0)
		(layer "B.SilkS")
	)
	(gr_text "3"
		(at 141.3891 84.6836 0)
		(layer "B.SilkS")
	)
	(gr_text "21"
		(at 141.3891 99.9236 0)
		(layer "B.SilkS")
	)
	(gr_text "14"
		(at 136.3091 94.8436 0)
		(layer "B.SilkS")
	)
	(gr_text "27"
		(at 141.3891 105.0036 0)
		(layer "B.SilkS")
	)
	(gr_text "28"
		(at 131.2291 107.5436 0)
		(layer "B.SilkS")
	)
	(gr_text "30\n"
		(at 141.3891 107.5436 0)
		(layer "B.SilkS")
	)
	(gr_text "26"
		(at 136.3091 105.0036 0)
		(layer "B.SilkS")
	)
	(gr_text "15"
		(at 141.3891 94.8436 0)
		(layer "B.SilkS")
	)
	(gr_text "2"
		(at 136.3091 84.6836 0)
		(layer "B.SilkS")
	)
	(gr_text "29"
		(at 136.3091 107.5436 0)
		(layer "B.SilkS")
	)
	(gr_text "20"
		(at 136.3091 99.9236 0)
		(layer "B.SilkS")
	)
	(gr_text "24"
		(at 141.3891 102.2096 0)
		(layer "B.SilkS")
	)
	(zone
		(net 31)
		(net_name "GND")
		(layer "F.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 118.4021 82.3976) (xy 119.5451 81.2546) (xy 158.788978 81.2546) (xy 160.4011 82.8036) (xy 160.620968 106.910732)
				(xy 158.9011 109.8036) (xy 119.4181 109.7026) (xy 118.4021 108.6866)
			)
		)
	)
	(embedded_fonts no)
	(embedded_files
		(file
			(name "ayf533035-closed.step")
			(type other)
		)
	)
)
