(kicad_pcb
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(general
		(thickness 1.6)
		(legacy_teardrops no)
	)
	(paper "A4")
	(title_block
		(title "MiniNDP")
		(date "2026-09-01")
		(rev "T512_08")
		(company "Brian K. White - b.kenyon.w@gmail.com")
		(comment 1 "github.com/bkw777/NODE_DATAPAC")
	)
	(layers
		(0 "F.Cu" signal)
		(2 "B.Cu" signal)
		(9 "F.Adhes" user "F.Adhesive")
		(11 "B.Adhes" user "B.Adhesive")
		(13 "F.Paste" user)
		(15 "B.Paste" user)
		(5 "F.SilkS" user "F.Silkscreen")
		(7 "B.SilkS" user "B.Silkscreen")
		(1 "F.Mask" user)
		(3 "B.Mask" user)
		(17 "Dwgs.User" user "User.Drawings")
		(19 "Cmts.User" user "User.Comments")
		(21 "Eco1.User" user "User.Eco1")
		(23 "Eco2.User" user "User.Eco2")
		(25 "Edge.Cuts" user)
		(27 "Margin" user)
		(31 "F.CrtYd" user "F.Courtyard")
		(29 "B.CrtYd" user "B.Courtyard")
		(35 "F.Fab" user)
		(33 "B.Fab" user)
		(39 "User.1" user)
		(41 "User.2" user)
		(43 "User.3" user)
		(45 "User.4" user)
		(47 "User.5" user)
		(49 "User.6" user)
		(51 "User.7" user)
		(53 "User.8" user)
		(55 "User.9" user)
	)
	(setup
		(stackup
			(layer "F.SilkS"
				(type "Top Silk Screen")
				(color "White")
			)
			(layer "F.Paste"
				(type "Top Solder Paste")
			)
			(layer "F.Mask"
				(type "Top Solder Mask")
				(color "Blue")
				(thickness 0.01)
			)
			(layer "F.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "dielectric 1"
				(type "core")
				(thickness 1.51)
				(material "FR4")
				(epsilon_r 4.5)
				(loss_tangent 0.02)
			)
			(layer "B.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "B.Mask"
				(type "Bottom Solder Mask")
				(color "Blue")
				(thickness 0.01)
			)
			(layer "B.Paste"
				(type "Bottom Solder Paste")
			)
			(layer "B.SilkS"
				(type "Bottom Silk Screen")
				(color "White")
			)
			(copper_finish "ENIG")
			(dielectric_constraints no)
		)
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(tenting front back)
		(aux_axis_origin 121.95 86.025)
		(grid_origin 151.95 115.025)
		(pcbplotparams
			(layerselection 0x00000000_00000000_55555555_f755f5ff)
			(plot_on_all_layers_selection 0x00000000_00000000_00000000_00000000)
			(disableapertmacros no)
			(usegerberextensions yes)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 4)
			(plotframeref no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(pdf_metadata yes)
			(pdf_single_document no)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plot_black_and_white yes)
			(sketchpadsonfab no)
			(plotpadnumbers no)
			(hidednponfab no)
			(sketchdnponfab yes)
			(crossoutdnponfab yes)
			(subtractmaskfromsilk yes)
			(outputformat 1)
			(mirror no)
			(drillshape 0)
			(scaleselection 1)
			(outputdirectory "GERBER_${TITLE}_${REVISION}")
		)
	)
	(net 0 "")
	(net 1 "GND")
	(net 2 "VMEM")
	(net 3 "VBUS")
	(net 4 "/AD0")
	(net 5 "/AD1")
	(net 6 "/AD2")
	(net 7 "/AD3")
	(net 8 "/AD4")
	(net 9 "/AD5")
	(net 10 "/AD6")
	(net 11 "/AD7")
	(net 12 "/A8")
	(net 13 "/A9")
	(net 14 "/A10")
	(net 15 "/A11")
	(net 16 "/A12")
	(net 17 "/A13")
	(net 18 "/A14")
	(net 19 "/A15")
	(net 20 "/~{RD}")
	(net 21 "/RAMRST")
	(net 22 "/~{Y0}")
	(net 23 "/(A)")
	(net 24 "unconnected-(J1-Pin_39-Pad39)")
	(net 25 "unconnected-(J1-Pin_40-Pad40)")
	(net 26 "unconnected-(J1-Pin_30-Pad30)")
	(net 27 "unconnected-(J1-Pin_31-Pad31)")
	(net 28 "unconnected-(J1-Pin_37-Pad37)")
	(net 29 "unconnected-(J1-Pin_15-Pad15)")
	(net 30 "/~{CE}")
	(net 31 "/A18_CE2")
	(net 32 "unconnected-(U1-Y1-Pad14)")
	(net 33 "/BUS_A10")
	(net 34 "unconnected-(U1-Y7-Pad7)")
	(net 35 "unconnected-(U1-Y0-Pad15)")
	(net 36 "unconnected-(U1-Y2-Pad13)")
	(net 37 "/A5")
	(net 38 "/A6")
	(net 39 "unconnected-(U1-Y3-Pad12)")
	(net 40 "unconnected-(U1-Y5-Pad10)")
	(net 41 "/A7")
	(net 42 "+BATT")
	(net 43 "/BUS_A8")
	(net 44 "/BUS_A9")
	(net 45 "/A16")
	(net 46 "/A17")
	(net 47 "/A3")
	(net 48 "/BYTE")
	(net 49 "unconnected-(U2-Q11-Pad1)")
	(net 50 "unconnected-(J1-Pin_17-Pad17)")
	(net 51 "unconnected-(J1-Pin_18-Pad18)")
	(net 52 "unconnected-(J1-Pin_19-Pad19)")
	(net 53 "unconnected-(J1-Pin_20-Pad20)")
	(net 54 "unconnected-(J1-Pin_25-Pad25)")
	(net 55 "unconnected-(J1-Pin_26-Pad26)")
	(net 56 "unconnected-(J1-Pin_27-Pad27)")
	(net 57 "unconnected-(J1-Pin_28-Pad28)")
	(net 58 "unconnected-(J1-Pin_33-Pad33)")
	(net 59 "unconnected-(J1-Pin_34-Pad34)")
	(net 60 "unconnected-(U2-Q10-Pad15)")
	(net 61 "/~{WR}")
	(net 62 "/BLOCK")
	(net 63 "/A0")
	(net 64 "/A2")
	(net 65 "/A4")
	(net 66 "/A1")
	(net 67 "Net-(U6-Pad6)")
	(footprint "000_LOCAL:TSSOP-16"
		(layer "F.Cu")
		(at 155.1 108.225 180)
		(descr "TSSOP, 16 Pin (JEDEC MO-153 Var AB https://www.jedec.org/document_search?search_api_views_fulltext=MO-153), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "TSSOP SO")
		(property "Reference" "U1"
			(at -1.25 -1 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "HC238"
			(at 1 0 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Datasheet" "datasheets/HC238.pdf"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "IC DECODER/DEMUX 1 X 3:8 16SO"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "74HC238PW,118"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "DIP*W7.62mm* SOIC*3.9x9.9mm*P1.27mm* TSSOP*4.4x5mm*P0.65mm*")
		(sheetname "/")
		(sheetfile "MiniNDP_T512_x.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -2.9 -2.275 180)
			(size 1.2 0.35)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "A0")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at -2.9 -1.625 180)
			(size 1.2 0.35)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 44 "/BUS_A9")
			(pinfunction "A1")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "3" smd roundrect
			(at -2.9 -0.975 180)
			(size 1.2 0.35)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 43 "/BUS_A8")
			(pinfunction "A2")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "4" smd roundrect
			(at -2.9 -0.325 180)
			(size 1.2 0.35)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "~{E1}")
			(pintype "input")
			(zone_connect 2)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "5" smd roundrect
			(at -2.9 0.325 180)
			(size 1.2 0.35)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 23 "/(A)")
			(pinfunction "~{E2}")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "6" smd roundrect
			(at -2.9 0.975 180)
			(size 1.2 0.35)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 22 "/~{Y0}")
			(pinfunction "E3")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "7" smd roundrect
			(at -2.9 1.625 180)
			(size 1.2 0.35)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 34 "unconnected-(U1-Y7-Pad7)")
			(pinfunction "Y7")
			(pintype "output+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "8" smd roundrect
			(at -2.9 2.275 180)
			(size 1.2 0.35)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "9" smd roundrect
			(at 2.9 2.275 180)
			(size 1.2 0.35)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 48 "/BYTE")
			(pinfunction "Y6")
			(pintype "output")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "10" smd roundrect
			(at 2.9 1.625 180)
			(size 1.2 0.35)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 40 "unconnected-(U1-Y5-Pad10)")
			(pinfunction "Y5")
			(pintype "output+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "11" smd roundrect
			(at 2.9 0.975 180)
			(size 1.2 0.35)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 62 "/BLOCK")
			(pinfunction "Y4")
			(pintype "output")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "12" smd roundrect
			(at 2.9 0.325 180)
			(size 1.2 0.35)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 39 "unconnected-(U1-Y3-Pad12)")
			(pinfunction "Y3")
			(pintype "output+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "13" smd roundrect
			(at 2.9 -0.325 180)
			(size 1.2 0.35)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 36 "unconnected-(U1-Y2-Pad13)")
			(pinfunction "Y2")
			(pintype "output+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "14" smd roundrect
			(at 2.9 -0.975 180)
			(size 1.2 0.35)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 32 "unconnected-(U1-Y1-Pad14)")
			(pinfunction "Y1")
			(pintype "output+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "15" smd roundrect
			(at 2.9 -1.625 180)
			(size 1.2 0.35)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 35 "unconnected-(U1-Y0-Pad15)")
			(pinfunction "Y0")
			(pintype "output+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "16" smd roundrect
			(at 2.9 -2.275 180)
			(size 1.2 0.35)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 3 "VBUS")
			(pinfunction "VCC")
			(pintype "power_in")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KIPRJMOD}/000_LOCAL.pretty/3dshapes/TSSOP-16.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "000_LOCAL:Fiducial_0.75_1.5"
		(layer "F.Cu")
		(at 179.95 88.025 180)
		(descr "Circular Fiducial, 0.75mm bare copper, 1.5mm soldermask opening (Level B)")
		(tags "fiducial")
		(property "Reference" "F3"
			(at 0 -2.000001 180)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Fiducial_0.75_1.5"
			(at 0 2.000001 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(zone_connect 0)
		(attr board_only exclude_from_bom)
		(pad "" smd circle
			(at 0 0 180)
			(size 0.75 0.75)
			(layers "F.Cu" "F.Mask")
			(solder_mask_margin 0.375)
			(clearance 0.375)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
	)
	(footprint "000_LOCAL:TSOP32-dual"
		(layer "F.Cu")
		(at 149.199 92.925 180)
		(descr "Module CMS TSOP 32 pins")
		(tags "CMS TSOP")
		(property "Reference" "U4"
			(at -0.05 -1.5 180)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "AS6C4008"
			(at -0.05 1.5 180)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Datasheet" "datasheets/AS6C4008.pdf"
			(at 3.05 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "IC SRAM 512Kx8 PARALLEL STSOP-32"
			(at 3.05 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "AS6C4008-55STIN"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SSOP*11.305x20.495mm*P1.27mm*")
		(sheetname "/")
		(sheetfile "MiniNDP_T512_x.kicad_sch")
		(attr smd)
		(pad "1" smd roundrect
			(at -6.500001 -3.75 90)
			(size 0.3 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 66 "/A1")
			(pinfunction "A11")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at -6.5 -3.25 90)
			(size 0.3 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 64 "/A2")
			(pinfunction "A9")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "3" smd roundrect
			(at -6.5 -2.75 90)
			(size 0.3 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 47 "/A3")
			(pinfunction "A8")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "4" smd roundrect
			(at -6.5 -2.25 90)
			(size 0.3 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 38 "/A6")
			(pinfunction "A13")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "5" smd roundrect
			(at -6.5 -1.75 90)
			(size 0.3 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 61 "/~{WR}")
			(pinfunction "~{WE}")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "6" smd roundrect
			(at -6.500001 -1.25 90)
			(size 0.3 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 31 "/A18_CE2")
			(pinfunction "A17")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "7" smd roundrect
			(at -6.5 -0.75 90)
			(size 0.3 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 65 "/A4")
			(pinfunction "A15")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "8" smd roundrect
			(at -6.5 -0.25 90)
			(size 0.3 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "VMEM")
			(pinfunction "VCC")
			(pintype "power_in")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "9" smd roundrect
			(at -6.5 0.25 90)
			(size 0.3 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 46 "/A17")
			(pinfunction "A18")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "10" smd roundrect
			(at -6.5 0.75 90)
			(size 0.3 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 37 "/A5")
			(pinfunction "A16")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "11" smd roundrect
			(at -6.500001 1.25 90)
			(size 0.3 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 13 "/A9")
			(pinfunction "A14")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "12" smd roundrect
			(at -6.5 1.75 90)
			(size 0.3 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 41 "/A7")
			(pinfunction "A12")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "13" smd roundrect
			(at -6.5 2.25 90)
			(size 0.3 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 12 "/A8")
			(pinfunction "A7")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "14" smd roundrect
			(at -6.5 2.75 90)
			(size 0.3 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 16 "/A12")
			(pinfunction "A6")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "15" smd roundrect
			(at -6.5 3.25 90)
			(size 0.3 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 15 "/A11")
			(pinfunction "A5")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "16" smd roundrect
			(at -6.500001 3.75 90)
			(size 0.3 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 14 "/A10")
			(pinfunction "A4")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "17" smd roundrect
			(at 6.500001 3.75 90)
			(size 0.3 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 17 "/A13")
			(pinfunction "A3")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "17" smd roundrect
			(at 13 3.75 90)
			(size 0.3 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 17 "/A13")
			(pinfunction "A3")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "18" smd roundrect
			(at 6.5 3.25 90)
			(size 0.3 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 18 "/A14")
			(pinfunction "A2")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "18" smd roundrect
			(at 13 3.25 90)
			(size 0.3 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 18 "/A14")
			(pinfunction "A2")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "19" smd roundrect
			(at 6.5 2.75 90)
			(size 0.3 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 19 "/A15")
			(pinfunction "A1")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "19" smd roundrect
			(at 13 2.75 90)
			(size 0.3 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 19 "/A15")
			(pinfunction "A1")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "20" smd roundrect
			(at 6.5 2.25 90)
			(size 0.3 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 45 "/A16")
			(pinfunction "A0")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "20" smd roundrect
			(at 13 2.25 90)
			(size 0.3 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 45 "/A16")
			(pinfunction "A0")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "21" smd roundrect
			(at 6.5 1.75 90)
			(size 0.3 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 4 "/AD0")
			(pinfunction "Q0")
			(pintype "tri_state")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "21" smd roundrect
			(at 13 1.75 90)
			(size 0.3 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 4 "/AD0")
			(pinfunction "Q0")
			(pintype "tri_state")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "22" smd roundrect
			(at 6.500001 1.25 90)
			(size 0.3 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 5 "/AD1")
			(pinfunction "Q1")
			(pintype "tri_state")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "22" smd roundrect
			(at 13 1.25 90)
			(size 0.3 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 5 "/AD1")
			(pinfunction "Q1")
			(pintype "tri_state")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "23" smd roundrect
			(at 6.5 0.75 90)
			(size 0.3 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 6 "/AD2")
			(pinfunction "Q2")
			(pintype "tri_state")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "23" smd roundrect
			(at 13 0.75 90)
			(size 0.3 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 6 "/AD2")
			(pinfunction "Q2")
			(pintype "tri_state")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "24" smd roundrect
			(at 6.5 0.25 90)
			(size 0.3 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(zone_connect 2)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "24" smd roundrect
			(at 13 0.25 90)
			(size 0.3 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(zone_connect 2)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "25" smd roundrect
			(at 6.5 -0.25 90)
			(size 0.3 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 7 "/AD3")
			(pinfunction "Q3")
			(pintype "tri_state")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "25" smd roundrect
			(at 13 -0.25 90)
			(size 0.3 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 7 "/AD3")
			(pinfunction "Q3")
			(pintype "tri_state")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "26" smd roundrect
			(at 6.5 -0.75 90)
			(size 0.3 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 8 "/AD4")
			(pinfunction "Q4")
			(pintype "tri_state")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "26" smd roundrect
			(at 13 -0.75 90)
			(size 0.3 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 8 "/AD4")
			(pinfunction "Q4")
			(pintype "tri_state")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "27" smd roundrect
			(at 6.500001 -1.25 90)
			(size 0.3 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 9 "/AD5")
			(pinfunction "Q5")
			(pintype "tri_state")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "27" smd roundrect
			(at 13 -1.25 90)
			(size 0.3 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 9 "/AD5")
			(pinfunction "Q5")
			(pintype "tri_state")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "28" smd roundrect
			(at 6.5 -1.75 90)
			(size 0.3 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 10 "/AD6")
			(pinfunction "Q6")
			(pintype "tri_state")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "28" smd roundrect
			(at 13 -1.75 90)
			(size 0.3 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 10 "/AD6")
			(pinfunction "Q6")
			(pintype "tri_state")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "29" smd roundrect
			(at 6.5 -2.25 90)
			(size 0.3 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 11 "/AD7")
			(pinfunction "Q7")
			(pintype "tri_state")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "29" smd roundrect
			(at 13 -2.25 90)
			(size 0.3 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 11 "/AD7")
			(pinfunction "Q7")
			(pintype "tri_state")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "30" smd roundrect
			(at 6.5 -2.75 90)
			(size 0.3 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 30 "/~{CE}")
			(pinfunction "~{CE}")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "30" smd roundrect
			(at 13 -2.75 90)
			(size 0.3 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 30 "/~{CE}")
			(pinfunction "~{CE}")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "31" smd roundrect
			(at 6.5 -3.25 90)
			(size 0.3 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 63 "/A0")
			(pinfunction "A10")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "31" smd roundrect
			(at 13 -3.25 90)
			(size 0.3 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 63 "/A0")
			(pinfunction "A10")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "32" smd roundrect
			(at 6.500001 -3.75 90)
			(size 0.3 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 20 "/~{RD}")
			(pinfunction "~{OE}")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "32" smd roundrect
			(at 13 -3.75 90)
			(size 0.3 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 20 "/~{RD}")
			(pinfunction "~{OE}")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KIPRJMOD}/000_LOCAL.pretty/3dshapes/TSOP32_8x14.step"
			(hide yes)
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
		(model "${KIPRJMOD}/000_LOCAL.pretty/3dshapes/TSOP32_8X20.step"
			(offset
				(xyz 3.25 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
		(model "${KIPRJMOD}/000_LOCAL.pretty/3dshapes/TSOP-I-32_11.8x8mm_P0.5mm.step"
			(hide yes)
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
		(model "${KIPRJMOD}/000_LOCAL.pretty/3dshapes/TSOP-I-32_18.4x8mm_P0.5mm.step"
			(hide yes)
			(offset
				(xyz 3.25 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "000_LOCAL:Fiducial_0.75_1.5"
		(layer "F.Cu")
		(at 123.95 88.025)
		(descr "Circular Fiducial, 0.75mm bare copper, 1.5mm soldermask opening (Level B)")
		(tags "fiducial")
		(property "Reference" "F3"
			(at 0 -2 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Fiducial_0.75_1.5"
			(at 0 2 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(zone_connect 0)
		(attr board_only exclude_from_bom)
		(pad "" smd circle
			(at 0 0)
			(size 0.75 0.75)
			(layers "F.Cu" "F.Mask")
			(solder_mask_margin 0.375)
			(clearance 0.375)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
	)
	(footprint "000_LOCAL:SolderJumper-2_P1.3mm_Open_RoundedPad1.0x1.5mm"
		(layer "F.Cu")
		(at 146.25 101.925 90)
		(descr "SMD Solder Jumper, 1x1.5mm, rounded Pads, 0.3mm gap, open")
		(tags "solder jumper open")
		(property "Reference" "JP2"
			(at -1.8 0 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "CE2"
			(at 0 1.9 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SolderJumper*Open*")
		(sheetname "/")
		(sheetfile "MiniNDP_T512_x.kicad_sch")
		(zone_connect 1)
		(attr smd exclude_from_pos_files exclude_from_bom dnp allow_soldermask_bridges)
		(pad "1" smd custom
			(at -0.65 0 90)
			(size 1 0.5)
			(layers "F.Cu" "F.Mask")
			(net 48 "/BYTE")
			(pinfunction "A")
			(pintype "passive")
			(zone_connect 2)
			(thermal_bridge_angle 45)
			(options
				(clearance outline)
				(anchor rect)
			)
			(primitives
				(gr_circle
					(center 0 0.25)
					(end 0.5 0.25)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center 0 -0.25)
					(end 0.5 -0.25)
					(width 0)
					(fill yes)
				)
				(gr_poly
					(pts
						(xy 0.5 0.75) (xy 0 0.75) (xy 0 -0.75) (xy 0.5 -0.75)
					)
					(width 0)
					(fill yes)
				)
			)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd custom
			(at 0.65 0 90)
			(size 1 0.5)
			(layers "F.Cu" "F.Mask")
			(net 31 "/A18_CE2")
			(pinfunction "B")
			(pintype "passive")
			(zone_connect 2)
			(thermal_bridge_angle 45)
			(options
				(clearance outline)
				(anchor rect)
			)
			(primitives
				(gr_circle
					(center 0 0.25)
					(end 0.5 0.25)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center 0 -0.25)
					(end 0.5 -0.25)
					(width 0)
					(fill yes)
				)
				(gr_poly
					(pts
						(xy 0 0.75) (xy -0.5 0.75) (xy -0.5 -0.75) (xy 0 -0.75)
					)
					(width 0)
					(fill yes)
				)
			)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KIPRJMOD}/000_LOCAL.pretty/3dshapes/Solder_Bridge_1.5x2.3.step"
			(offset
				(xyz -1.15 -0.75 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -0 -0 -0)
			)
		)
	)
	(footprint "000_LOCAL:R_0805"
		(layer "F.Cu")
		(at 141.85 98.975 180)
		(descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
		(tags "resistor 0805")
		(property "Reference" "R2"
			(at -1.85 0.675 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "47k"
			(at -1.875 -0.525 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Datasheet" "datasheets/sei-rmcf_rmcp.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "RES 47K OHM 1% 1/8W 0805"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "RMCF0805FT47K0"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "MiniNDP_T512_x.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.949999 0 180)
			(size 0.7 1.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.1)
			(net 2 "VMEM")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at 0.949999 0 180)
			(size 0.7 1.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.1)
			(net 21 "/RAMRST")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KIPRJMOD}/000_LOCAL.pretty/3dshapes/R_0805.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "000_LOCAL:MiniNDP_Cover_THIN"
		(layer "F.Cu")
		(at 151.95 103.025)
		(property "Reference" "N1"
			(at 0 -0.381 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Value" "MiniNDP_Cover_THIN"
			(at 0 1 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "../COVER/MiniNDP_Cover.scad"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Snap cover for MiniNDP, thin version for CR2016"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "MiniNDP_Cover_THIN.stl"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Enclosure* Housing*")
		(sheetname "/")
		(sheetfile "MiniNDP_T512_x.kicad_sch")
		(attr board_only exclude_from_pos_files exclude_from_bom allow_missing_courtyard)
		(embedded_fonts no)
		(model "${KIPRJMOD}/000_LOCAL.pretty/3dshapes/MiniNDP_Cover_THIN.step"
			(offset
				(xyz 0 0 -1.6)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "000_LOCAL:C_0805"
		(layer "F.Cu")
		(at 157.45 92.525 90)
		(descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
		(tags "capacitor 0805")
		(property "Reference" "C5"
			(at 0.65 1.1 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "1u"
			(at -0.7 1.15 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Datasheet" "datasheets/CL21B105KAFNNNE.pdf"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "CAP CER 1UF 25V X7R 0805"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "CL21B105KAFNNNE"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "MiniNDP_T512_x.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -1.5 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9 0 90)
			(size 0.8 1.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.1)
			(net 2 "VMEM")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at 0.9 0 90)
			(size 0.8 1.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.1)
			(net 1 "GND")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KIPRJMOD}/000_LOCAL.pretty/3dshapes/C_0805.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "000_LOCAL:Fiducial_0.75_1.5"
		(layer "F.Cu")
		(at 123.95 118.025)
		(descr "Circular Fiducial, 0.75mm bare copper, 1.5mm soldermask opening (Level B)")
		(tags "fiducial")
		(property "Reference" "F3"
			(at 0 -2 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Fiducial_0.75_1.5"
			(at 0 2 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(zone_connect 0)
		(attr board_only exclude_from_bom)
		(pad "" smd circle
			(at 0 0)
			(size 0.75 0.75)
			(layers "F.Cu" "F.Mask")
			(solder_mask_margin 0.375)
			(clearance 0.375)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
	)
	(footprint "000_LOCAL:TSSOP-16"
		(layer "F.Cu")
		(at 152.6 100.6 180)
		(descr "TSSOP, 16 Pin (JEDEC MO-153 Var AB https://www.jedec.org/document_search?search_api_views_fulltext=MO-153), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "TSSOP SO")
		(property "Reference" "U2"
			(at -1.25 -1 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "HC4040"
			(at 1 0 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Datasheet" "datasheets/4040.pdf"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "IC BINARY COUNTER 12-BIT 16SO"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "74HC4040PW,118"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "DIP?16* SO*16*")
		(sheetname "/")
		(sheetfile "MiniNDP_T512_x.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -2.9 -2.275 180)
			(size 1.2 0.35)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 49 "unconnected-(U2-Q11-Pad1)")
			(pinfunction "Q11")
			(pintype "output+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at -2.9 -1.625 180)
			(size 1.2 0.35)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 37 "/A5")
			(pinfunction "Q5")
			(pintype "output")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "3" smd roundrect
			(at -2.9 -0.975 180)
			(size 1.2 0.35)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 65 "/A4")
			(pinfunction "Q4")
			(pintype "output")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "4" smd roundrect
			(at -2.9 -0.325 180)
			(size 1.2 0.35)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 38 "/A6")
			(pinfunction "Q6")
			(pintype "output")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "5" smd roundrect
			(at -2.9 0.325 180)
			(size 1.2 0.35)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 47 "/A3")
			(pinfunction "Q3")
			(pintype "output")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "6" smd roundrect
			(at -2.9 0.975 180)
			(size 1.2 0.35)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 64 "/A2")
			(pinfunction "Q2")
			(pintype "output")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "7" smd roundrect
			(at -2.9 1.625 180)
			(size 1.2 0.35)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 66 "/A1")
			(pinfunction "Q1")
			(pintype "output")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "8" smd roundrect
			(at -2.9 2.275 180)
			(size 1.2 0.35)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "VSS")
			(pintype "power_in")
			(zone_connect 2)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "9" smd roundrect
			(at 2.9 2.275 180)
			(size 1.2 0.35)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 63 "/A0")
			(pinfunction "Q0")
			(pintype "output")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "10" smd roundrect
			(at 2.9 1.625 180)
			(size 1.2 0.35)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 48 "/BYTE")
			(pinfunction "CLK")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "11" smd roundrect
			(at 2.9 0.975 180)
			(size 1.2 0.35)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 62 "/BLOCK")
			(pinfunction "Reset")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "12" smd roundrect
			(at 2.9 0.325 180)
			(size 1.2 0.35)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 12 "/A8")
			(pinfunction "Q8")
			(pintype "output")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "13" smd roundrect
			(at 2.9 -0.325 180)
			(size 1.2 0.35)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 41 "/A7")
			(pinfunction "Q7")
			(pintype "output")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "14" smd roundrect
			(at 2.9 -0.975 180)
			(size 1.2 0.35)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 13 "/A9")
			(pinfunction "Q9")
			(pintype "output")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "15" smd roundrect
			(at 2.9 -1.625 180)
			(size 1.2 0.35)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 60 "unconnected-(U2-Q10-Pad15)")
			(pinfunction "Q10")
			(pintype "output+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "16" smd roundrect
			(at 2.9 -2.275 180)
			(size 1.2 0.35)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 3 "VBUS")
			(pinfunction "VDD")
			(pintype "power_in")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KIPRJMOD}/000_LOCAL.pretty/3dshapes/TSSOP-16.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "000_LOCAL:C_0805"
		(layer "F.Cu")
		(at 125.725 92.375 -90)
		(descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
		(tags "capacitor 0805")
		(property "Reference" "C3"
			(at -0.85 1.075 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "1u"
			(at 0.5 1.075 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Datasheet" "datasheets/CL21B105KAFNNNE.pdf"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "CAP CER 1UF 25V X7R 0805"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "CL21B105KAFNNNE"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "MiniNDP_T512_x.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -1.5 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9 0 270)
			(size 0.8 1.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.1)
			(net 3 "VBUS")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at 0.9 0 270)
			(size 0.8 1.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.1)
			(net 1 "GND")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KIPRJMOD}/000_LOCAL.pretty/3dshapes/C_0805.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "000_LOCAL:TSSOP-20"
		(layer "F.Cu")
		(at 130.275 94.575 90)
		(descr "TSSOP, 20 Pin (JEDEC MO-153 Var AC https://www.jedec.org/document_search?search_api_views_fulltext=MO-153), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "TSSOP SO")
		(property "Reference" "U3"
			(at -1.25 -1.5 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "HC573"
			(at 1 0 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Datasheet" "datasheets/HC573.pdf"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "8-bit Latch 3-state outputs"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "74HC573PW,118"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "MiniNDP_T512_x.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -2.9 -2.925 90)
			(size 1.2 0.35)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "~{OE}")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at -2.9 -2.275 90)
			(size 1.2 0.35)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 4 "/AD0")
			(pinfunction "D0")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "3" smd roundrect
			(at -2.9 -1.625 90)
			(size 1.2 0.35)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 5 "/AD1")
			(pinfunction "D1")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "4" smd roundrect
			(at -2.9 -0.975 90)
			(size 1.2 0.35)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 6 "/AD2")
			(pinfunction "D2")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "5" smd roundrect
			(at -2.9 -0.325 90)
			(size 1.2 0.35)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 7 "/AD3")
			(pinfunction "D3")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "6" smd roundrect
			(at -2.9 0.325 90)
			(size 1.2 0.35)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 8 "/AD4")
			(pinfunction "D4")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "7" smd roundrect
			(at -2.9 0.975 90)
			(size 1.2 0.35)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 9 "/AD5")
			(pinfunction "D5")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "8" smd roundrect
			(at -2.9 1.625 90)
			(size 1.2 0.35)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 10 "/AD6")
			(pinfunction "D6")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "9" smd roundrect
			(at -2.9 2.275 90)
			(size 1.2 0.35)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 11 "/AD7")
			(pinfunction "D7")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "10" smd roundrect
			(at -2.9 2.925 90)
			(size 1.2 0.35)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "11" smd roundrect
			(at 2.9 2.925 90)
			(size 1.2 0.35)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 62 "/BLOCK")
			(pinfunction "LE")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "12" smd roundrect
			(at 2.9 2.275 90)
			(size 1.2 0.35)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 46 "/A17")
			(pinfunction "Q7")
			(pintype "tri_state")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "13" smd roundrect
			(at 2.9 1.625 90)
			(size 1.2 0.35)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 45 "/A16")
			(pinfunction "Q6")
			(pintype "tri_state")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "14" smd roundrect
			(at 2.9 0.975 90)
			(size 1.2 0.35)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 19 "/A15")
			(pinfunction "Q5")
			(pintype "tri_state")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "15" smd roundrect
			(at 2.9 0.325 90)
			(size 1.2 0.35)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 18 "/A14")
			(pinfunction "Q4")
			(pintype "tri_state")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "16" smd roundrect
			(at 2.9 -0.325 90)
			(size 1.2 0.35)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 17 "/A13")
			(pinfunction "Q3")
			(pintype "tri_state")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "17" smd roundrect
			(at 2.9 -0.975 90)
			(size 1.2 0.35)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 16 "/A12")
			(pinfunction "Q2")
			(pintype "tri_state")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "18" smd roundrect
			(at 2.9 -1.625 90)
			(size 1.2 0.35)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 15 "/A11")
			(pinfunction "Q1")
			(pintype "tri_state")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "19" smd roundrect
			(at 2.9 -2.275 90)
			(size 1.2 0.35)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 14 "/A10")
			(pinfunction "Q0")
			(pintype "tri_state")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "20" smd roundrect
			(at 2.9 -2.925 90)
			(size 1.2 0.35)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 3 "VBUS")
			(pinfunction "VCC")
			(pintype "power_in")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KIPRJMOD}/000_LOCAL.pretty/3dshapes/TSSOP-20.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "000_LOCAL:Fiducial_0.75_1.5"
		(layer "F.Cu")
		(at 179.95 118.025 90)
		(descr "Circular Fiducial, 0.75mm bare copper, 1.5mm soldermask opening (Level B)")
		(tags "fiducial")
		(property "Reference" "F3"
			(at 0 -2.000001 270)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Fiducial_0.75_1.5"
			(at 0 2.000001 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(zone_connect 0)
		(attr board_only exclude_from_bom)
		(pad "" smd circle
			(at 0 0 90)
			(size 0.75 0.75)
			(layers "F.Cu" "F.Mask")
			(solder_mask_margin 0.375)
			(clearance 0.375)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
	)
	(footprint "000_LOCAL:TSSOP-8_3x3mm_P0.65mm"
		(layer "F.Cu")
		(at 141.85 101.925)
		(descr "TSSOP8: plastic thin shrink small outline package; 8 leads; body width 3 mm; (see NXP SSOP-TSSOP-VSO-REFLOW.pdf and sot505-1_po.pdf)")
		(tags "SSOP 0.65")
		(property "Reference" "U6"
			(at 0.325 -1.175 270)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "2G00"
			(at 0 2.55 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Datasheet" "datasheets/2G00.pdf"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Dual NAND Gate, Low-Voltage CMOS"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SSOP* VSSOP*")
		(sheetname "/")
		(sheetfile "MiniNDP_T512_x.kicad_sch")
		(clearance 0.2)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.875 -0.975)
			(size 0.8 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 21 "/RAMRST")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at -1.875 -0.325)
			(size 0.8 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 21 "/RAMRST")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "3" smd roundrect
			(at -1.875 0.325)
			(size 0.8 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 30 "/~{CE}")
			(pintype "output")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "4" smd roundrect
			(at -1.875 0.975)
			(size 0.8 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "5" smd roundrect
			(at 1.875 0.975)
			(size 0.8 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 48 "/BYTE")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "6" smd roundrect
			(at 1.875 0.325)
			(size 0.8 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 67 "Net-(U6-Pad6)")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "7" smd roundrect
			(at 1.875 -0.325)
			(size 0.8 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 67 "Net-(U6-Pad6)")
			(pintype "output")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "8" smd roundrect
			(at 1.875 -0.975)
			(size 0.8 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "VMEM")
			(pinfunction "VCC")
			(pintype "power_in")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KIPRJMOD}/000_LOCAL.pretty/3dshapes/TSSOP-8.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "000_LOCAL:SolderJumper-2_P1.3mm_Open_RoundedPad1.0x1.5mm"
		(layer "F.Cu")
		(at 137.45 101.925 -90)
		(descr "SMD Solder Jumper, 1x1.5mm, rounded Pads, 0.3mm gap, open")
		(tags "solder jumper open")
		(property "Reference" "JP1"
			(at 1.8 0.001 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "~{CE1}"
			(at 0 1.9 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SolderJumper*Open*")
		(sheetname "/")
		(sheetfile "MiniNDP_T512_x.kicad_sch")
		(zone_connect 1)
		(attr smd exclude_from_pos_files exclude_from_bom dnp allow_soldermask_bridges)
		(pad "1" smd custom
			(at -0.65 0 270)
			(size 1 0.5)
			(layers "F.Cu" "F.Mask")
			(net 21 "/RAMRST")
			(pinfunction "A")
			(pintype "passive")
			(zone_connect 2)
			(thermal_bridge_angle 45)
			(options
				(clearance outline)
				(anchor rect)
			)
			(primitives
				(gr_circle
					(center 0 0.25)
					(end 0.5 0.25)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center 0 -0.25)
					(end 0.5 -0.25)
					(width 0)
					(fill yes)
				)
				(gr_poly
					(pts
						(xy 0.5 0.75) (xy 0 0.75) (xy 0 -0.75) (xy 0.5 -0.75)
					)
					(width 0)
					(fill yes)
				)
			)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd custom
			(at 0.65 0 270)
			(size 1 0.5)
			(layers "F.Cu" "F.Mask")
			(net 30 "/~{CE}")
			(pinfunction "B")
			(pintype "passive")
			(zone_connect 2)
			(thermal_bridge_angle 45)
			(options
				(clearance outline)
				(anchor rect)
			)
			(primitives
				(gr_circle
					(center 0 0.25)
					(end 0.5 0.25)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center 0 -0.25)
					(end 0.5 -0.25)
					(width 0)
					(fill yes)
				)
				(gr_poly
					(pts
						(xy 0 0.75) (xy -0.5 0.75) (xy -0.5 -0.75) (xy 0 -0.75)
					)
					(width 0)
					(fill yes)
				)
			)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KIPRJMOD}/000_LOCAL.pretty/3dshapes/Solder_Bridge_1.5x2.3.step"
			(offset
				(xyz -1.15 -0.75 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -0 -0 -0)
			)
		)
	)
	(footprint "000_LOCAL:C_0805"
		(layer "F.Cu")
		(at 150.05 109.375 90)
		(descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
		(tags "capacitor 0805")
		(property "Reference" "C2"
			(at 2.05 0.55 270)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "1u"
			(at 2.05 -0.65 270)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Datasheet" "datasheets/CL21B105KAFNNNE.pdf"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "CAP CER 1UF 25V X7R 0805"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "CL21B105KAFNNNE"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "MiniNDP_T512_x.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -1.5 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9 0 90)
			(size 0.8 1.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.1)
			(net 3 "VBUS")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at 0.9 0 90)
			(size 0.8 1.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.1)
			(net 1 "GND")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KIPRJMOD}/000_LOCAL.pretty/3dshapes/C_0805.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "000_LOCAL:SOT-353_SC-70-5"
		(layer "F.Cu")
		(at 146.87 109.375 -90)
		(descr "SOT-353, SC-70-5")
		(tags "SOT-353 SC-70-5")
		(property "Reference" "U5"
			(at -2 -0.005 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "1G79"
			(at 2.1 0.02 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Datasheet" "datasheets/LVC1G79.pdf"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "IC FF D-TYPE SNGL 1BIT 5TSSOP"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "74LVC1G79GW,125"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SOT* SG*")
		(sheetname "/")
		(sheetfile "MiniNDP_T512_x.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 -0.65 270)
			(size 0.65 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 33 "/BUS_A10")
			(pinfunction "D")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at -0.949999 0 270)
			(size 0.65 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 62 "/BLOCK")
			(pinfunction "C")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "3" smd roundrect
			(at -0.95 0.65 270)
			(size 0.65 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "4" smd roundrect
			(at 0.95 0.65 270)
			(size 0.65 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 31 "/A18_CE2")
			(pinfunction "Q")
			(pintype "output")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "5" smd roundrect
			(at 0.95 -0.65 270)
			(size 0.65 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 3 "VBUS")
			(pinfunction "VCC")
			(pintype "power_in")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KIPRJMOD}/000_LOCAL.pretty/3dshapes/SOT-353_SC-70-5.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "000_LOCAL:C_0805"
		(layer "F.Cu")
		(at 152.675 104.275)
		(descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
		(tags "capacitor 0805")
		(property "Reference" "C4"
			(at -2.2 0 270)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "1u"
			(at -3.45 0 270)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Datasheet" "datasheets/CL21B105KAFNNNE.pdf"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "CAP CER 1UF 25V X7R 0805"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "CL21B105KAFNNNE"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "MiniNDP_T512_x.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -1.5 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9 0)
			(size 0.8 1.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.1)
			(net 3 "VBUS")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at 0.9 0)
			(size 0.8 1.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.1)
			(net 1 "GND")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KIPRJMOD}/000_LOCAL.pretty/3dshapes/C_0805.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "000_LOCAL:Keystone_3028_3034_bkw"
		(layer "F.Cu")
		(at 170.225 99.475 90)
		(descr "Keystone 3034 SMD battery holder for 2020, 2025 and 2032 coincell batteries. http://www.keyelco.com/product-pdf.cfm?p=798")
		(tags "Keystone type 3034 coin cell retainer")
		(property "Reference" "BT1"
			(at -8.75 -5.6 135)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "Keystone_3028"
			(at 9.65 0.55 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Datasheet" "datasheets/Keystone_3034.pdf"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "BATTERY RETAINER COIN 20MM x 1.6MM SMT"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "Keystone_3028"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "MiniNDP_T512_x.kicad_sch")
		(zone_connect 2)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -2.9 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at -11.275 -2.75)
			(size 0.8 0.8)
			(drill 0.6)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 42 "+BATT")
			(pinfunction "+")
			(pintype "passive")
			(solder_mask_margin -0.2)
			(clearance 0.4)
			(zone_connect 2)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "1" thru_hole circle
			(at -11.275 0)
			(size 0.8 0.8)
			(drill 0.6)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 42 "+BATT")
			(pinfunction "+")
			(pintype "passive")
			(solder_mask_margin -0.2)
			(clearance 0.4)
			(zone_connect 2)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "1" smd roundrect
			(at -11.275 0 90)
			(size 1.85 7.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.125)
			(net 42 "+BATT")
			(pinfunction "+")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "1" thru_hole circle
			(at -11.275 2.75)
			(size 0.8 0.8)
			(drill 0.6)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 42 "+BATT")
			(pinfunction "+")
			(pintype "passive")
			(solder_mask_margin -0.2)
			(clearance 0.4)
			(zone_connect 2)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "1" thru_hole circle
			(at 11.275 -2.75)
			(size 0.8 0.8)
			(drill 0.6)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 42 "+BATT")
			(pinfunction "+")
			(pintype "passive")
			(solder_mask_margin -0.2)
			(clearance 0.4)
			(zone_connect 2)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "1" thru_hole circle
			(at 11.275 0)
			(size 0.8 0.8)
			(drill 0.6)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 42 "+BATT")
			(pinfunction "+")
			(pintype "passive")
			(solder_mask_margin -0.2)
			(clearance 0.4)
			(zone_connect 2)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "1" smd roundrect
			(at 11.275 0 90)
			(size 1.85 7.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.125)
			(net 42 "+BATT")
			(pinfunction "+")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "1" thru_hole circle
			(at 11.275 2.75)
			(size 0.8 0.8)
			(drill 0.6)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 42 "+BATT")
			(pinfunction "+")
			(pintype "passive")
			(solder_mask_margin -0.2)
			(clearance 0.4)
			(zone_connect 2)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" thru_hole circle
			(at -9.007825 -3.731163 112.5)
			(size 0.5 0.5)
			(drill 0.3)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "-")
			(pintype "passive")
			(solder_mask_margin -0.15)
			(zone_connect 2)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" thru_hole circle
			(at -9.007825 3.731163 112.5)
			(size 0.5 0.5)
			(drill 0.3)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "-")
			(pintype "passive")
			(solder_mask_margin -0.15)
			(zone_connect 2)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" thru_hole circle
			(at -3.731163 -9.007825 112.5)
			(size 0.5 0.5)
			(drill 0.3)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "-")
			(pintype "passive")
			(solder_mask_margin -0.15)
			(zone_connect 2)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" thru_hole circle
			(at -3.731163 9.007825 112.5)
			(size 0.5 0.5)
			(drill 0.3)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "-")
			(pintype "passive")
			(solder_mask_margin -0.15)
			(zone_connect 2)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd circle
			(at 0 0 90)
			(size 18 18)
			(layers "F.Cu" "F.Mask")
			(net 1 "GND")
			(pinfunction "-")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" thru_hole circle
			(at 3.731163 -9.007825 112.5)
			(size 0.5 0.5)
			(drill 0.3)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "-")
			(pintype "passive")
			(solder_mask_margin -0.15)
			(zone_connect 2)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" thru_hole circle
			(at 3.731163 9.007825 112.5)
			(size 0.5 0.5)
			(drill 0.3)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "-")
			(pintype "passive")
			(solder_mask_margin -0.15)
			(zone_connect 2)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" thru_hole circle
			(at 9.007825 -3.731163 112.5)
			(size 0.5 0.5)
			(drill 0.3)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "-")
			(pintype "passive")
			(solder_mask_margin -0.15)
			(zone_connect 2)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" thru_hole circle
			(at 9.007825 3.731163 112.5)
			(size 0.5 0.5)
			(drill 0.3)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "-")
			(pintype "passive")
			(solder_mask_margin -0.15)
			(zone_connect 2)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KIPRJMOD}/000_LOCAL.pretty/3dshapes/CR2032_holder_Keystone_3034.step"
			(hide yes)
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
		(model "${KIPRJMOD}/000_LOCAL.pretty/3dshapes/CR2016_holder_BAT-HLD-002-SMT.STEP"
			(hide yes)
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 0 0)
			)
		)
		(model "${KIPRJMOD}/000_LOCAL.pretty/3dshapes/CR2012_holder_Keystone_3028.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 90)
			)
		)
		(model "${KIPRJMOD}/000_LOCAL.pretty/3dshapes/CR2012_blank.step"
			(offset
				(xyz 0 0 1.2)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 180 0 0)
			)
		)
		(model "${KIPRJMOD}/000_LOCAL.pretty/3dshapes/CR2016_blank.step"
			(hide yes)
			(offset
				(xyz 0 0 1.6)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 180 0 0)
			)
		)
		(model "${KIPRJMOD}/000_LOCAL.pretty/3dshapes/CR2032_blank.step"
			(hide yes)
			(offset
				(xyz 0 0 3.2)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 180 0 0)
			)
		)
	)
	(footprint "000_LOCAL:SOT-23"
		(layer "F.Cu")
		(at 159.55 88.875 -90)
		(descr "SOT-23, Standard")
		(tags "SOT-23")
		(property "Reference" "DA1"
			(at 0 -1.825 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "BAV70"
			(at -1.25 -1.825 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Datasheet" "datasheets/BAV70.pdf"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "DIODE ARRAY GP 75V 150MA SOT23-3"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "BAV70-7-F"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SOT?23*")
		(sheetname "/")
		(sheetfile "MiniNDP_T512_x.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at -6.15 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.15 -0.95 270)
			(size 0.8 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 42 "+BATT")
			(pinfunction "A")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at -1.15 0.95 270)
			(size 0.8 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 3 "VBUS")
			(pinfunction "A")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "3" smd roundrect
			(at 1.15 0 270)
			(size 0.8 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "VMEM")
			(pinfunction "K")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KIPRJMOD}/000_LOCAL.pretty/3dshapes/SOT-23.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "000_LOCAL:IDC-Header_2x20_P2.54mm_Vertical"
		(layer "B.Cu")
		(at 127.82 113.755 -90)
		(descr "Through hole IDC box header, 2x20, 2.54mm pitch, DIN 41651 / IEC 60603-13, double rows, https://docs.google.com/spreadsheets/d/16SsEcesNF15N3Lb4niX7dcUr-NY5_MFPQhobNuNppn4/edit#gid=0")
		(tags "Through hole vertical IDC box header THT 2x20 2.54mm double row")
		(property "Reference" "J1"
			(at -0.42 2.61 90)
			(layer "B.SilkS")
		)
		(property "Value" "Conn_02x20_Odd_Even"
			(at 1.27 -24.003 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "datasheets/2x20_male_boxed.pdf"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "CONN HEADER VERT 40POS 2.54MM"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "302-S401"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_2x??_*")
		(sheetname "/")
		(sheetfile "MiniNDP_T512_x.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at -1.905 -24.13 0)
			(layer "B.Fab")
		)
		(pad "1" thru_hole roundrect
			(at 0 0 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.147059)
			(net 3 "VBUS")
			(pinfunction "Pin_1")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" thru_hole circle
			(at 2.54 0 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "VBUS")
			(pinfunction "Pin_2")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "3" thru_hole circle
			(at 0 -2.54 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_3")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "4" thru_hole circle
			(at 2.54 -2.54 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_4")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "5" thru_hole circle
			(at 0 -5.08 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "/AD1")
			(pinfunction "Pin_5")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "6" thru_hole circle
			(at 2.54 -5.08 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "/AD0")
			(pinfunction "Pin_6")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "7" thru_hole circle
			(at 0 -7.62 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 7 "/AD3")
			(pinfunction "Pin_7")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "8" thru_hole circle
			(at 2.54 -7.62 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "/AD2")
			(pinfunction "Pin_8")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "9" thru_hole circle
			(at 0 -10.16 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 9 "/AD5")
			(pinfunction "Pin_9")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "10" thru_hole circle
			(at 2.54 -10.16 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 8 "/AD4")
			(pinfunction "Pin_10")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "11" thru_hole circle
			(at 0 -12.7 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 11 "/AD7")
			(pinfunction "Pin_11")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "12" thru_hole circle
			(at 2.54 -12.7 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 10 "/AD6")
			(pinfunction "Pin_12")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "13" thru_hole circle
			(at 0 -15.24 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 44 "/BUS_A9")
			(pinfunction "Pin_13")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "14" thru_hole circle
			(at 2.54 -15.24 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 43 "/BUS_A8")
			(pinfunction "Pin_14")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "15" thru_hole circle
			(at 0 -17.78 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 29 "unconnected-(J1-Pin_15-Pad15)")
			(pinfunction "Pin_15")
			(pintype "passive+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "16" thru_hole circle
			(at 2.54 -17.78 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 33 "/BUS_A10")
			(pinfunction "Pin_16")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "17" thru_hole circle
			(at 0 -20.32 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 50 "unconnected-(J1-Pin_17-Pad17)")
			(pinfunction "Pin_17")
			(pintype "passive+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "18" thru_hole circle
			(at 2.54 -20.32 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 51 "unconnected-(J1-Pin_18-Pad18)")
			(pinfunction "Pin_18")
			(pintype "passive+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "19" thru_hole circle
			(at 0 -22.86 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 52 "unconnected-(J1-Pin_19-Pad19)")
			(pinfunction "Pin_19")
			(pintype "passive+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "20" thru_hole circle
			(at 2.54 -22.86 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 53 "unconnected-(J1-Pin_20-Pad20)")
			(pinfunction "Pin_20")
			(pintype "passive+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "21" thru_hole circle
			(at 0 -25.4 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_21")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "22" thru_hole circle
			(at 2.54 -25.4 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_22")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "23" thru_hole circle
			(at 0 -27.94 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 61 "/~{WR}")
			(pinfunction "Pin_23")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "24" thru_hole circle
			(at 2.54 -27.94 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 20 "/~{RD}")
			(pinfunction "Pin_24")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "25" thru_hole circle
			(at 0 -30.48 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 54 "unconnected-(J1-Pin_25-Pad25)")
			(pinfunction "Pin_25")
			(pintype "passive+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "26" thru_hole circle
			(at 2.54 -30.48 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 55 "unconnected-(J1-Pin_26-Pad26)")
			(pinfunction "Pin_26")
			(pintype "passive+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "27" thru_hole circle
			(at 0 -33.02 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 56 "unconnected-(J1-Pin_27-Pad27)")
			(pinfunction "Pin_27")
			(pintype "passive+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "28" thru_hole circle
			(at 2.54 -33.02 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 57 "unconnected-(J1-Pin_28-Pad28)")
			(pinfunction "Pin_28")
			(pintype "passive+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "29" thru_hole circle
			(at 0 -35.56 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 22 "/~{Y0}")
			(pinfunction "Pin_29")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "30" thru_hole circle
			(at 2.54 -35.56 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 26 "unconnected-(J1-Pin_30-Pad30)")
			(pinfunction "Pin_30")
			(pintype "passive+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "31" thru_hole circle
			(at 0 -38.1 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 27 "unconnected-(J1-Pin_31-Pad31)")
			(pinfunction "Pin_31")
			(pintype "passive+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "32" thru_hole circle
			(at 2.54 -38.1 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 23 "/(A)")
			(pinfunction "Pin_32")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "33" thru_hole circle
			(at 0 -40.64 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 58 "unconnected-(J1-Pin_33-Pad33)")
			(pinfunction "Pin_33")
			(pintype "passive+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "34" thru_hole circle
			(at 2.54 -40.64 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 59 "unconnected-(J1-Pin_34-Pad34)")
			(pinfunction "Pin_34")
			(pintype "passive+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "35" thru_hole circle
			(at 0 -43.18 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_35")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "36" thru_hole circle
			(at 2.54 -43.18 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_36")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "37" thru_hole circle
			(at 0 -45.72 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 28 "unconnected-(J1-Pin_37-Pad37)")
			(pinfunction "Pin_37")
			(pintype "passive+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "38" thru_hole circle
			(at 2.54 -45.72 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 21 "/RAMRST")
			(pinfunction "Pin_38")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "39" thru_hole circle
			(at 0 -48.26 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 24 "unconnected-(J1-Pin_39-Pad39)")
			(pinfunction "Pin_39")
			(pintype "passive+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "40" thru_hole circle
			(at 2.54 -48.26 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 25 "unconnected-(J1-Pin_40-Pad40)")
			(pinfunction "Pin_40")
			(pintype "passive+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KIPRJMOD}/000_LOCAL.pretty/3dshapes/IDC-Header_2x20_P2.54mm_Vertical.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(gr_arc
		(start 121.95 88.025)
		(mid 122.535786 86.610786)
		(end 123.95 86.025)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 121.95 118.025)
		(end 121.95 88.025)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 123.95 86.025)
		(end 179.95 86.025)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 123.95 120.025001)
		(mid 122.535786 119.439214)
		(end 121.949999 118.025)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 179.95 86.024999)
		(mid 181.364214 86.610786)
		(end 181.950001 88.025)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 179.95 120.025)
		(end 123.95 120.025)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 181.95 88.025)
		(end 181.95 118.025)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 181.950001 118.025)
		(mid 181.364214 119.439214)
		(end 179.95 120.025001)
		(layer "Edge.Cuts")
	)
	(gr_text "128k 256k:\nDNP U5 U6\nClose JP1 JP2"
		(at 123.275 99.275 0)
		(layer "F.SilkS")
	)
	(gr_text "512k:\nPopulate U5 U6\nOpen JP1 JP2"
		(at 123.275 103.875 0)
		(layer "F.SilkS")
	)
	(gr_text "CR2016 / CR2012"
		(at 180.9 99.475 90)
		(layer "F.SilkS")
	)
	(gr_text "${TITLE} - ${REVISION} - RAM DISK for TANDY 102/200"
		(at 151.95 118.575 0)
		(layer "F.SilkS")
	)
	(gr_text "128k"
		(at 126.875 110.15 0)
		(layer "F.SilkS")
	)
	(gr_text "256k"
		(at 133.675 110.15 0)
		(layer "F.SilkS")
	)
	(gr_text "512k"
		(at 140.475 110.15 0)
		(layer "F.SilkS")
	)
	(gr_text "BASIC to bootstrap RAMxxx.CO previously saved as the first file in bank 0"
		(at 151.95 95.086 0)
		(layer "B.SilkS")
	)
	(gr_text "128k 256k 512k\nRAM DISK for\nTANDY 102/200"
		(at 132.519 88.863 0)
		(layer "B.SilkS")
	)
	(gr_text "BATTERY\nCR2016\nCR2012"
		(at 181.45 109.525 90)
		(layer "B.SilkS")
	)
	(gr_text "${COMMENT1} - ${REVISION}"
		(at 151.95 92.775 0)
		(layer "B.SilkS")
	)
	(gr_text "${TITLE}"
		(at 151.95 88.863 0)
		(layer "B.SilkS")
	)
	(gr_text "bank 0:P=129  1:P=133\nblock 0-255: OUT P,N\nread byte:   D=INP(131)\nwrite byte:  OUT 131,D"
		(at 181.18 88.915 0)
		(layer "B.SilkS")
	)
	(gr_text "100 1 CLEAR0,61558:T=61558:E=62957:OUT129,2\n200 1 CLEAR0,59715:T=59715:E=61101:OUT129,2\n    2 FORA=0TO15:N=INP(131):NEXT:FORA=TTOE\n    3 POKEA,INP(131):IFA=T+1007THENOUT129,1\n    4 ?{dblquote}.{dblquote};:NEXT:SAVEM{dblquote}RAMDSK{dblquote},T,E,T"
		(at 180.6 97.175 0)
		(layer "B.SilkS")
	)
	(gr_text "Use ENIG copper finish\nfor gold battery contact.\n"
		(at 169.7 85.025 0)
		(layer "Eco1.User")
	)
	(zone
		(net 4)
		(net_name "/AD0")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30105)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 136.749 91.075) (xy 136.713185 91.077179) (xy 136.618197 91.077612) (xy 136.577507 91.063237)
				(xy 136.552701 91.030709) (xy 136.198 91.175) (xy 136.552701 91.319291) (xy 136.58249 91.283776)
				(xy 136.641061 91.270071) (xy 136.713185 91.272822) (xy 136.749 91.275)
			)
		)
	)
	(zone
		(net 22)
		(net_name "/~{Y0}")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30083)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 158.818886 107.209819) (xy 158.768129 107.19931) (xy 158.649136 107.170258) (xy 158.60247 107.145322)
				(xy 158.58037 107.109606) (xy 157.999134 107.249501) (xy 158.545985 107.418339) (xy 158.559202 107.392705)
				(xy 158.577838 107.376394) (xy 158.629238 107.365224) (xy 158.707789 107.379962) (xy 158.718894 107.383027)
			)
		)
	)
	(zone
		(net 65)
		(net_name "/A4")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30075)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 154.699263 101.621127) (xy 154.733118 101.62543) (xy 154.848578 101.646893) (xy 154.895588 101.671959)
				(xy 154.917952 101.712884) (xy 155.500959 101.575281) (xy 154.9875 101.4) (xy 154.946698 101.43587)
				(xy 154.87992 101.446877) (xy 154.781302 101.433979) (xy 154.755609 101.429229)
			)
		)
	)
	(zone
		(net 3)
		(net_name "VBUS")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30001)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 127.52 112.055) (xy 127.51468 112.171303) (xy 127.497441 112.30908) (xy 127.46929 112.446989)
				(xy 127.427841 112.587426) (xy 127.384118 112.696453) (xy 127.330156 112.79839) (xy 127.278168 112.873415)
				(xy 127.218478 112.939104) (xy 127.161443 112.985995) (xy 127.098302 113.02338) (xy 126.98903 113.059329)
				(xy 127.82 113.756) (xy 128.65097 113.059329) (xy 128.530403 113.017688) (xy 128.42281 112.94032)
				(xy 128.325908 112.82365) (xy 128.240872 112.662287) (xy 128.172536 112.454343) (xy 128.129409 112.213165)
				(xy 128.12 112.055)
			)
		)
	)
	(zone
		(net 9)
		(net_name "/AD5")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30010)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 137.333214 112.247847) (xy 137.398623 112.341158) (xy 137.446349 112.426975) (xy 137.476045 112.500419)
				(xy 137.493374 112.569499) (xy 137.496249 112.696142) (xy 137.461851 112.827437) (xy 137.362604 113.032639)
				(xy 137.243159 113.27607) (xy 137.189262 113.421896) (xy 137.146333 113.589173) (xy 137.980608 113.755793)
				(xy 138.452235 113.048251) (xy 138.082372 112.789707) (xy 137.95939 112.687203) (xy 137.853291 112.580834)
				(xy 137.648144 112.329911) (xy 137.559414 112.214253) (xy 137.491885 112.126096)
			)
		)
	)
	(zone
		(net 10)
		(net_name "/AD6")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30162)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 135.808059 94.786209) (xy 135.807325 94.77288) (xy 135.804703 94.760031) (xy 135.804709 94.778701)
				(xy 136.199991 94.67487) (xy 135.820967 94.546967) (xy 135.810374 94.586196) (xy 135.79864 94.592818)
				(xy 135.792305 94.590503) (xy 135.781963 94.58792)
			)
		)
	)
	(zone
		(net 46)
		(net_name "/A17")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30056)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 132.65 92.45) (xy 132.649499 92.424648) (xy 132.655524 92.306364) (xy 132.676166 92.253302)
				(xy 132.718339 92.220985) (xy 132.55 91.674) (xy 132.381661 92.220985) (xy 132.423649 92.253029)
				(xy 132.446245 92.315788) (xy 132.450501 92.424647) (xy 132.45 92.45)
			)
		)
	)
	(zone
		(net 9)
		(net_name "/AD5")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30081)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 131.215305 96.673634) (xy 131.208621 96.712951) (xy 131.184041 96.823788) (xy 131.159094 96.867553)
				(xy 131.120479 96.887364) (xy 131.249691 97.475951) (xy 131.425 96.9625) (xy 131.390343 96.922194)
				(xy 131.381964 96.857487) (xy 131.399778 96.759238) (xy 131.405516 96.735435)
			)
		)
	)
	(zone
		(net 44)
		(net_name "/BUS_A9")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30089)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 158.811103 109.838773) (xy 158.751611 109.821153) (xy 158.648214 109.788126) (xy 158.61009 109.764189)
				(xy 158.594107 109.73288) (xy 157.999134 109.8495) (xy 158.5125 110.025) (xy 158.530493 110.001223)
				(xy 158.552655 109.986901) (xy 158.609595 109.980642) (xy 158.702433 110.008459) (xy 158.711103 110.011977)
			)
		)
	)
	(zone
		(net 48)
		(net_name "/BYTE")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30052)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 149.145196 98.875) (xy 149.065664 98.870332) (xy 149.005069 98.857658) (xy 148.902813 98.809439)
				(xy 148.821184 98.766714) (xy 148.698773 98.729804) (xy 148.649 98.975) (xy 148.698773 99.220196)
				(xy 148.835415 99.176905) (xy 148.902813 99.140561) (xy 148.997709 99.094647) (xy 149.060872 99.080319)
				(xy 149.145196 99.075)
			)
		)
	)
	(zone
		(net 15)
		(net_name "/A11")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30082)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 128.621945 90.882555) (xy 128.616918 90.91522) (xy 128.593893 91.021782) (xy 128.568467 91.064052)
				(xy 128.527824 91.082456) (xy 128.649793 91.675978) (xy 128.825 91.1625) (xy 128.795211 91.12279)
				(xy 128.790354 91.05533) (xy 128.809221 90.959635) (xy 128.817574 90.924137)
			)
		)
	)
	(zone
		(net 10)
		(net_name "/AD6")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30106)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 136.749 94.575) (xy 136.713185 94.577179) (xy 136.618197 94.577612) (xy 136.577507 94.563237)
				(xy 136.552701 94.530709) (xy 136.198 94.675) (xy 136.552701 94.819291) (xy 136.58249 94.783776)
				(xy 136.641061 94.770071) (xy 136.713185 94.772822) (xy 136.749 94.775)
			)
		)
	)
	(zone
		(net 3)
		(net_name "VBUS")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30044)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 151.425 110.65) (xy 151.491579 110.640878) (xy 151.604554 110.628745) (xy 151.653453 110.640592)
				(xy 151.6875 110.675) (xy 152.201 110.5) (xy 151.6875 110.325) (xy 151.649436 110.361332) (xy 151.585856 110.371559)
				(xy 151.491579 110.359122) (xy 151.425 110.35)
			)
		)
	)
	(zone
		(net 21)
		(net_name "/RAMRST")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30102)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 140.175 100.55) (xy 140.154995 100.621588) (xy 140.129021 100.657235) (xy 140.092388 100.689573)
				(xy 140.046122 100.716281) (xy 139.989603 100.736285) (xy 139.875598 100.75) (xy 139.975 100.951)
				(xy 140.349261 100.784603) (xy 140.337703 100.759607) (xy 140.357373 100.644333) (xy 140.375 100.55)
			)
		)
	)
	(zone
		(net 9)
		(net_name "/AD5")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30104)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 135.663258 94.294709) (xy 135.693273 94.289776) (xy 135.794069 94.280095) (xy 135.840818 94.291796)
				(xy 135.874 94.325) (xy 136.199991 94.17487) (xy 135.833552 94.038557) (xy 135.806737 94.07363)
				(xy 135.747321 94.091167) (xy 135.680196 94.094557) (xy 135.637151 94.096422)
			)
		)
	)
	(zone
		(net 17)
		(net_name "/A13")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30080)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 129.914103 90.877595) (xy 129.90884 90.912697) (xy 129.885888 91.023127) (xy 129.860746 91.067226)
				(xy 129.82065 91.087249) (xy 129.949742 91.675965) (xy 130.125 91.1625) (xy 130.091931 91.122299)
				(xy 130.084122 91.055926) (xy 130.100868 90.958414) (xy 130.107287 90.929361)
			)
		)
	)
	(zone
		(net 19)
		(net_name "/A15")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30121)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 135.649 90.275) (xy 135.684815 90.272822) (xy 135.779803 90.272388) (xy 135.820493 90.286763)
				(xy 135.845299 90.319291) (xy 136.2 90.175) (xy 135.845299 90.030709) (xy 135.815511 90.066224)
				(xy 135.756941 90.079929) (xy 135.684815 90.077179) (xy 135.649 90.075)
			)
		)
	)
	(zone
		(net 62)
		(net_name "/BLOCK")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30065)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 150.475 99.525) (xy 150.449647 99.525501) (xy 150.331363 99.519476) (xy 150.278301 99.498834)
				(xy 150.245985 99.456661) (xy 149.699 99.625) (xy 150.245985 99.793339) (xy 150.278029 99.751351)
				(xy 150.340788 99.728755) (xy 150.449648 99.724499) (xy 150.475 99.725)
			)
		)
	)
	(zone
		(net 23)
		(net_name "/(A)")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30072)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 158.795768 107.844052) (xy 158.749514 107.836343) (xy 158.641339 107.813742) (xy 158.598518 107.790838)
				(xy 158.577417 107.755186) (xy 157.999035 107.899742) (xy 158.5125 108.075) (xy 158.553188 108.033464)
				(xy 158.617233 108.018691) (xy 158.709446 108.029274) (xy 158.735112 108.035149) (xy 158.744013 108.037239)
			)
		)
	)
	(zone
		(net 9)
		(net_name "/AD5")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30057)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 131.35 98.25) (xy 131.349499 98.224648) (xy 131.355524 98.106364) (xy 131.376166 98.053302)
				(xy 131.418339 98.020985) (xy 131.25 97.474) (xy 131.081661 98.020985) (xy 131.123649 98.053029)
				(xy 131.146245 98.115788) (xy 131.150501 98.224647) (xy 131.15 98.25)
			)
		)
	)
	(zone
		(net 11)
		(net_name "/AD7")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30107)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 136.749 95.075) (xy 136.713185 95.077179) (xy 136.618197 95.077612) (xy 136.577507 95.063237)
				(xy 136.552701 95.030709) (xy 136.198 95.175) (xy 136.552701 95.319291) (xy 136.58249 95.283776)
				(xy 136.641061 95.270071) (xy 136.713185 95.272822) (xy 136.749 95.275)
			)
		)
	)
	(zone
		(net 7)
		(net_name "/AD3")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30122)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 142.149 93.275) (xy 142.184815 93.272822) (xy 142.279803 93.272388) (xy 142.320493 93.286763)
				(xy 142.345299 93.319291) (xy 142.7 93.175) (xy 142.345299 93.030709) (xy 142.315511 93.066224)
				(xy 142.256941 93.079929) (xy 142.184815 93.077179) (xy 142.149 93.075)
			)
		)
	)
	(zone
		(net 30)
		(net_name "/~{CE}")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30033)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 136.463855 102.332524) (xy 136.509599 102.341034) (xy 136.560393 102.360904) (xy 136.608403 102.391019)
				(xy 136.650817 102.432493) (xy 136.67734 102.474115) (xy 136.69456 102.523538) (xy 136.7 102.575)
				(xy 137.450984 102.575173) (xy 136.7 102.075) (xy 136.695291 102.099206) (xy 136.682324 102.11691)
				(xy 136.634145 102.137367) (xy 136.545847 102.139595) (xy 136.51632 102.1371) (xy 136.498585 102.135564)
			)
		)
	)
	(zone
		(net 46)
		(net_name "/A17")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30054)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 155.035874 92.575) (xy 154.830285 92.563591) (xy 154.70478 92.556633) (xy 154.526227 92.579804)
				(xy 154.574 92.825) (xy 154.713893 93.032867) (xy 154.796615 92.958208) (xy 154.844233 92.888838)
				(xy 154.873819 92.843964) (xy 154.909386 92.807842) (xy 154.960287 92.783758) (xy 155.035874 92.775)
			)
		)
	)
	(zone
		(net 7)
		(net_name "/AD3")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30108)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 136.749 93.075) (xy 136.713185 93.077179) (xy 136.618197 93.077612) (xy 136.577507 93.063237)
				(xy 136.552701 93.030709) (xy 136.198 93.175) (xy 136.552701 93.319291) (xy 136.58249 93.283776)
				(xy 136.641061 93.270071) (xy 136.713185 93.272822) (xy 136.749 93.275)
			)
		)
	)
	(zone
		(net 11)
		(net_name "/AD7")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30090)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 132.538773 96.663897) (xy 132.521153 96.723389) (xy 132.488126 96.826786) (xy 132.464189 96.86491)
				(xy 132.43288 96.880892) (xy 132.5495 97.475866) (xy 132.725 96.9625) (xy 132.701223 96.944507)
				(xy 132.686901 96.922345) (xy 132.680642 96.865405) (xy 132.708459 96.772567) (xy 132.711977 96.763897)
			)
		)
	)
	(zone
		(net 11)
		(net_name "/AD7")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30058)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 132.65 98.25) (xy 132.649499 98.224648) (xy 132.655524 98.106364) (xy 132.676166 98.053302)
				(xy 132.718339 98.020985) (xy 132.55 97.474) (xy 132.381661 98.020985) (xy 132.423649 98.053029)
				(xy 132.446245 98.115788) (xy 132.450501 98.224647) (xy 132.45 98.25)
			)
		)
	)
	(zone
		(net 16)
		(net_name "/A12")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30078)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 129.260325 90.878569) (xy 129.256297 90.910165) (xy 129.234946 91.022415) (xy 129.209609 91.067952)
				(xy 129.16803 91.089) (xy 129.299761 91.67597) (xy 129.475 91.1625) (xy 129.442141 91.122121) (xy 129.433735 91.054439)
				(xy 129.448299 90.958366) (xy 129.454512 90.926432)
			)
		)
	)
	(zone
		(net 18)
		(net_name "/A14")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30073)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 130.551037 90.871728) (xy 130.546224 90.907951) (xy 130.524262 91.024625) (xy 130.499412 91.072025)
				(xy 130.45928 91.094846) (xy 130.599691 91.675951) (xy 130.775 91.1625) (xy 130.737224 91.121482)
				(xy 130.724814 91.055468) (xy 130.737292 90.954703) (xy 130.741246 90.933532)
			)
		)
	)
	(zone
		(net 3)
		(net_name "VBUS")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30023)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 152.575 104.3) (xy 152.571294 104.300001) (xy 152.456302 104.295433) (xy 152.390622 104.284536)
				(xy 152.325973 104.263301) (xy 152.267221 104.22828) (xy 152.219231 104.176026) (xy 152.186869 104.103092)
				(xy 152.175 104.006031) (xy 151.774 104.275) (xy 152.160348 104.863429) (xy 152.166501 104.839178)
				(xy 152.180976 104.823442) (xy 152.229889 104.81312) (xy 152.329063 104.831659) (xy 152.421276 104.86072)
				(xy 152.507971 104.887954) (xy 152.575 104.9)
			)
		)
	)
	(zone
		(net 43)
		(net_name "/BUS_A8")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30009)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 144.321243 117.414822) (xy 144.212792 117.299373) (xy 144.129491 117.195373) (xy 144.073513 117.109758)
				(xy 144.032085 117.028473) (xy 143.982888 116.871082) (xy 143.958315 116.671411) (xy 143.954099 116.613921)
				(xy 143.935444 116.398628) (xy 143.893667 116.129173) (xy 143.059293 116.294293) (xy 142.894173 117.128667)
				(xy 143.205856 117.174912) (xy 143.378921 117.189099) (xy 143.582466 117.208545) (xy 143.674907 117.22667)
				(xy 143.765661 117.255561) (xy 143.85813 117.299091) (xy 143.955712 117.361133) (xy 144.061809 117.445559)
				(xy 144.179822 117.556243)
			)
		)
	)
	(zone
		(net 37)
		(net_name "/A5")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30076)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 154.703392 102.271617) (xy 154.735956 102.275558) (xy 154.849349 102.296209) (xy 154.895598 102.321153)
				(xy 154.91761 102.362372) (xy 155.50097 102.225239) (xy 154.9875 102.05) (xy 154.946878 102.084997)
				(xy 154.87937 102.095611) (xy 154.779428 102.082537) (xy 154.751252 102.077429)
			)
		)
	)
	(zone
		(net 3)
		(net_name "VBUS")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30018)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 150.52071 109.380026) (xy 150.413907 109.501896) (xy 150.305247 109.62836) (xy 150.180858 109.74904)
				(xy 150.11272 109.799551) (xy 150.040595 109.839425) (xy 149.964466 109.865595) (xy 149.884314 109.875)
				(xy 150.049293 110.275707) (xy 150.675 110.215686) (xy 150.657003 110.179713) (xy 150.649995 110.14434)
				(xy 150.664261 110.074509) (xy 150.718372 109.996286) (xy 150.825065 109.900864) (xy 150.863944 109.870831)
				(xy 150.944974 109.80429)
			)
		)
	)
	(zone
		(net 30)
		(net_name "/~{CE}")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30086)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 139.375 102.35) (xy 139.382653 102.34999) (xy 139.448933 102.351319) (xy 139.525874 102.361335)
				(xy 139.594725 102.388777) (xy 139.620256 102.411765) (xy 139.636732 102.442388) (xy 139.976 102.25)
				(xy 139.636732 102.057612) (xy 139.602649 102.105494) (xy 139.536181 102.136138) (xy 139.430447 102.149492)
				(xy 139.382653 102.15001) (xy 139.375 102.15)
			)
		)
	)
	(zone
		(net 5)
		(net_name "/AD1")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30123)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 142.148999 91.775) (xy 142.184814 91.772822) (xy 142.279802 91.772388) (xy 142.320492 91.786763)
				(xy 142.345298 91.819291) (xy 142.699999 91.675) (xy 142.345298 91.530709) (xy 142.31551 91.566224)
				(xy 142.25694 91.579929) (xy 142.184814 91.577179) (xy 142.148999 91.575)
			)
		)
	)
	(zone
		(net 30)
		(net_name "/~{CE}")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30031)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 138.45 102.15) (xy 138.427557 102.150256) (xy 138.284762 102.142675) (xy 138.224675 102.120214)
				(xy 138.206604 102.100934) (xy 138.2 102.075) (xy 137.449 102.575) (xy 138.195722 102.595404) (xy 138.214906 102.502638)
				(xy 138.26613 102.428958) (xy 138.346009 102.374915) (xy 138.440635 102.350259) (xy 138.45 102.35)
			)
		)
	)
	(zone
		(net 63)
		(net_name "/A0")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30109)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 136.749 96.075) (xy 136.713185 96.077179) (xy 136.618197 96.077612) (xy 136.577507 96.063237)
				(xy 136.552701 96.030709) (xy 136.198 96.175) (xy 136.552701 96.319291) (xy 136.58249 96.283776)
				(xy 136.641061 96.270071) (xy 136.713185 96.272822) (xy 136.749 96.275)
			)
		)
	)
	(zone
		(net 3)
		(net_name "VBUS")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30024)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 126.75 91.325) (xy 126.662702 91.319311) (xy 126.557108 91.299487) (xy 126.47601 91.272631)
				(xy 126.402199 91.233575) (xy 126.358494 91.19756) (xy 126.324979 91.1539) (xy 126.300615 91.08109)
				(xy 125.724 91.475) (xy 126.300615 91.86891) (xy 126.329177 91.789154) (xy 126.392028 91.723592)
				(xy 126.494045 91.670269) (xy 126.63641 91.634298) (xy 126.75 91.625)
			)
		)
	)
	(zone
		(net 48)
		(net_name "/BYTE")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30087)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 144.325 102.8) (xy 144.317347 102.80001) (xy 144.251067 102.798681) (xy 144.174126 102.788665)
				(xy 144.105275 102.761223) (xy 144.079744 102.738235) (xy 144.063268 102.707612) (xy 143.724 102.9)
				(xy 144.063268 103.092388) (xy 144.097351 103.044506) (xy 144.163819 103.013862) (xy 144.269553 103.000508)
				(xy 144.317347 102.99999) (xy 144.325 103)
			)
		)
	)
	(zone
		(net 65)
		(net_name "/A4")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30124)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 155.149 93.775) (xy 155.184815 93.772822) (xy 155.279803 93.772388) (xy 155.320493 93.786763)
				(xy 155.345299 93.819291) (xy 155.7 93.675) (xy 155.345299 93.530709) (xy 155.315511 93.566224)
				(xy 155.256941 93.579929) (xy 155.184815 93.577179) (xy 155.149 93.575)
			)
		)
	)
	(zone
		(net 21)
		(net_name "/RAMRST")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30032)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 138.45 101.5) (xy 138.35557 101.479242) (xy 138.305369 101.452598) (xy 138.259538 101.414362)
				(xy 138.228806 101.374256) (xy 138.206836 101.325781) (xy 138.195722 101.254595) (xy 137.449 101.275)
				(xy 138.2 101.775) (xy 138.204739 101.752678) (xy 138.217914 101.73519) (xy 138.270854 101.710383)
				(xy 138.373604 101.699532) (xy 138.427557 101.699744) (xy 138.45 101.7)
			)
		)
	)
	(zone
		(net 21)
		(net_name "/RAMRST")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30097)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 140.567774 101.595366) (xy 140.546113 101.589364) (xy 140.433363 101.548872) (xy 140.387133 101.512578)
				(xy 140.366703 101.460706) (xy 139.974041 101.599719) (xy 140.275 101.8) (xy 140.318321 101.764862)
				(xy 140.384289 101.757383) (xy 140.494883 101.782229) (xy 140.511427 101.787264)
			)
		)
	)
	(zone
		(net 10)
		(net_name "/AD6")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30071)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 131.834535 96.683511) (xy 131.829244 96.724548) (xy 131.809495 96.835069) (xy 131.786553 96.879976)
				(xy 131.748961 96.903121) (xy 131.899805 97.47598) (xy 132.075 96.9625) (xy 132.033274 96.92164)
				(xy 132.016588 96.855428) (xy 132.024105 96.758618) (xy 132.028529 96.734224) (xy 132.030691 96.722532)
			)
		)
	)
	(zone
		(net 62)
		(net_name "/BLOCK")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30099)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 146.879035 107.876711) (xy 146.869826 107.905578) (xy 146.820209 108.034064) (xy 146.781024 108.086309)
				(xy 146.756838 108.102457) (xy 146.729209 108.109298) (xy 146.869658 108.42594) (xy 147.07 108.200001)
				(xy 147.035954 108.15794) (xy 147.028973 108.091445) (xy 147.050762 107.992904) (xy 147.062508 107.95807)
				(xy 147.066973 107.945114)
			)
		)
	)
	(zone
		(net 63)
		(net_name "/A0")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30125)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 142.149 96.275) (xy 142.184815 96.272822) (xy 142.279803 96.272388) (xy 142.320493 96.286763)
				(xy 142.345299 96.319291) (xy 142.7 96.175) (xy 142.345299 96.030709) (xy 142.315511 96.066224)
				(xy 142.256941 96.079929) (xy 142.184815 96.077179) (xy 142.149 96.075)
			)
		)
	)
	(zone
		(net 42)
		(net_name "+BATT")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30020)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 169.629437 88.025) (xy 169.686573 88.029847) (xy 169.729039 88.043773) (xy 169.776648 88.088042)
				(xy 169.804283 88.164276) (xy 169.81299 88.205253) (xy 169.838633 88.309633) (xy 169.892412 88.422228)
				(xy 170.226 88.2) (xy 170.447228 87.867412) (xy 170.260683 87.724246) (xy 170.168865 87.639944)
				(xy 170.069222 87.550559) (xy 169.96338 87.482872) (xy 169.900036 87.458135) (xy 169.825424 87.439985)
				(xy 169.629437 87.425)
			)
		)
	)
	(zone
		(net 17)
		(net_name "/A13")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30126)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 135.649 89.275) (xy 135.684815 89.272822) (xy 135.779803 89.272388) (xy 135.820493 89.286763)
				(xy 135.845299 89.319291) (xy 136.2 89.175) (xy 135.845299 89.030709) (xy 135.815511 89.066224)
				(xy 135.756941 89.079929) (xy 135.684815 89.077179) (xy 135.649 89.075)
			)
		)
	)
	(zone
		(net 45)
		(net_name "/A16")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30091)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 131.888773 90.863897) (xy 131.871153 90.923389) (xy 131.838126 91.026786) (xy 131.814189 91.06491)
				(xy 131.78288 91.080892) (xy 131.8995 91.675866) (xy 132.075 91.1625) (xy 132.051223 91.144507)
				(xy 132.036901 91.122345) (xy 132.030642 91.065405) (xy 132.058459 90.972567) (xy 132.061977 90.963897)
			)
		)
	)
	(zone
		(net 62)
		(net_name "/BLOCK")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30041)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 150.6 99.030764) (xy 150.595292 99.113989) (xy 150.582338 99.179514) (xy 150.537978 99.27831)
				(xy 150.511952 99.318409) (xy 150.4538 99.416663) (xy 150.427548 99.482406) (xy 150.405764 99.566473)
				(xy 150.7 99.626) (xy 150.994236 99.566473) (xy 150.973493 99.485601) (xy 150.948581 99.421727)
				(xy 150.888048 99.318409) (xy 150.854617 99.265883) (xy 150.826536 99.206776) (xy 150.8072 99.131574)
				(xy 150.8 99.030764)
			)
		)
	)
	(zone
		(net 62)
		(net_name "/BLOCK")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30038)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 150.105764 107.175) (xy 150.188989 107.179708) (xy 150.254514 107.192662) (xy 150.35331 107.237022)
				(xy 150.393409 107.263048) (xy 150.491663 107.3212) (xy 150.557406 107.347452) (xy 150.641473 107.369236)
				(xy 150.701 107.075) (xy 150.641473 106.780764) (xy 150.560601 106.801507) (xy 150.496727 106.826418)
				(xy 150.393409 106.886952) (xy 150.340883 106.920383) (xy 150.281776 106.948464) (xy 150.206574 106.9678)
				(xy 150.105764 106.975)
			)
		)
	)
	(zone
		(net 9)
		(net_name "/AD5")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30127)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 142.148999 94.275) (xy 142.184814 94.272822) (xy 142.279802 94.272388) (xy 142.320492 94.286763)
				(xy 142.345298 94.319291) (xy 142.699999 94.175) (xy 142.345298 94.030709) (xy 142.31551 94.066224)
				(xy 142.25694 94.079929) (xy 142.184814 94.077179) (xy 142.148999 94.075)
			)
		)
	)
	(zone
		(net 45)
		(net_name "/A16")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30110)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 136.749 90.575) (xy 136.713185 90.577179) (xy 136.618197 90.577612) (xy 136.577507 90.563237)
				(xy 136.552701 90.530709) (xy 136.198 90.675) (xy 136.552701 90.819291) (xy 136.58249 90.783776)
				(xy 136.641061 90.770071) (xy 136.713185 90.772822) (xy 136.749 90.775)
			)
		)
	)
	(zone
		(net 6)
		(net_name "/AD2")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30150)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 135.67617 92.308913) (xy 135.711818 92.301795) (xy 135.802213 92.288894) (xy 135.8437 92.297284)
				(xy 135.874 92.325) (xy 136.199965 92.174742) (xy 135.818631 92.050461) (xy 135.795889 92.0867)
				(xy 135.739694 92.106791) (xy 135.663922 92.113167) (xy 135.624407 92.115728)
			)
		)
	)
	(zone
		(net 12)
		(net_name "/A8")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30128)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 155.149 90.775) (xy 155.184815 90.772822) (xy 155.279803 90.772388) (xy 155.320493 90.786763)
				(xy 155.345299 90.819291) (xy 155.7 90.675) (xy 155.345299 90.530709) (xy 155.315511 90.566224)
				(xy 155.256941 90.579929) (xy 155.184815 90.577179) (xy 155.149 90.575)
			)
		)
	)
	(zone
		(net 4)
		(net_name "/AD0")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30084)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 127.976621 96.683719) (xy 127.971757 96.71513) (xy 127.948537 96.821044) (xy 127.922802 96.863066)
				(xy 127.881635 96.881139) (xy 127.999805 97.47598) (xy 128.175 96.9625) (xy 128.14694 96.922972)
				(xy 128.143751 96.854907) (xy 128.163325 96.761843) (xy 128.172777 96.722737)
			)
		)
	)
	(zone
		(net 4)
		(net_name "/AD0")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30013)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 131.726233 115.209032) (xy 131.827416 115.418599) (xy 131.895461 115.585078) (xy 131.933667 115.70484)
				(xy 131.960003 115.816811) (xy 131.994399 116.030789) (xy 132.066333 116.460827) (xy 132.900454 116.29589)
				(xy 133.065827 115.461333) (xy 132.841017 115.433977) (xy 132.605491 115.437067) (xy 132.545207 115.440847)
				(xy 132.354794 115.447522) (xy 132.269461 115.439547) (xy 132.189473 115.41842) (xy 132.113904 115.379933)
				(xy 132.041825 115.319878) (xy 131.97231 115.234046) (xy 131.904431 115.11823)
			)
		)
	)
	(zone
		(net 37)
		(net_name "/A5")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30129)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 155.149 92.275) (xy 155.184815 92.272822) (xy 155.279803 92.272388) (xy 155.320493 92.286763)
				(xy 155.345299 92.319291) (xy 155.7 92.175) (xy 155.345299 92.030709) (xy 155.315511 92.066224)
				(xy 155.256941 92.079929) (xy 155.184815 92.077179) (xy 155.149 92.075)
			)
		)
	)
	(zone
		(net 19)
		(net_name "/A15")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30130)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 142.149 90.275) (xy 142.184815 90.272822) (xy 142.279803 90.272388) (xy 142.320493 90.286763)
				(xy 142.345299 90.319291) (xy 142.7 90.175) (xy 142.345299 90.030709) (xy 142.315511 90.066224)
				(xy 142.256941 90.079929) (xy 142.184815 90.077179) (xy 142.149 90.075)
			)
		)
	)
	(zone
		(net 31)
		(net_name "/A18_CE2")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30049)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 154.75 96.929804) (xy 154.745332 97.009336) (xy 154.732658 97.069931) (xy 154.684439 97.172186)
				(xy 154.641714 97.253815) (xy 154.604804 97.376227) (xy 154.85 97.426) (xy 155.095196 97.376227)
				(xy 155.051905 97.239584) (xy 155.015561 97.172187) (xy 154.969647 97.077291) (xy 154.955319 97.014128)
				(xy 154.95 96.929804)
			)
		)
	)
	(zone
		(net 64)
		(net_name "/A2")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30079)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 156.231596 99.480167) (xy 156.217154 99.483703) (xy 156.16607 99.495096) (xy 156.107889 99.500321)
				(xy 156.053176 99.488811) (xy 156.0125 99.45) (xy 155.499077 99.625382) (xy 156.08348 99.760739)
				(xy 156.105593 99.72257) (xy 156.166112 99.69331) (xy 156.263708 99.673007) (xy 156.308132 99.664942)
			)
		)
	)
	(zone
		(net 3)
		(net_name "VBUS")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30019)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 149.556645 111.185238) (xy 149.666995 111.061515) (xy 149.781598 110.930775) (xy 149.911971 110.805727)
				(xy 149.982716 110.753329) (xy 150.056979 110.711944) (xy 150.134617 110.684769) (xy 150.215488 110.675)
				(xy 150.050809 110.274413) (xy 149.425 110.333318) (xy 149.444652 110.371874) (xy 149.452658 110.408648)
				(xy 149.439735 110.476992) (xy 149.388887 110.548541) (xy 149.273007 110.644687) (xy 149.203963 110.699838)
			)
		)
	)
	(zone
		(net 2)
		(net_name "VMEM")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30036)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 143.499999 98.875) (xy 143.37784 98.854337) (xy 143.307296 98.827182) (xy 143.241569 98.788108)
				(xy 143.199992 98.75044) (xy 143.16905 98.705471) (xy 143.154991 98.667343) (xy 143.149999 98.625)
				(xy 142.798999 98.975) (xy 143.149999 99.325) (xy 143.168278 99.246081) (xy 143.221711 99.177997)
				(xy 143.313265 99.120032) (xy 143.437187 99.081284) (xy 143.499999 99.075)
			)
		)
	)
	(zone
		(net 4)
		(net_name "/AD0")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30131)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 142.149 91.275) (xy 142.184815 91.272822) (xy 142.279803 91.272388) (xy 142.320493 91.286763)
				(xy 142.345299 91.319291) (xy 142.7 91.175) (xy 142.345299 91.030709) (xy 142.315511 91.066224)
				(xy 142.256941 91.079929) (xy 142.184815 91.077179) (xy 142.149 91.075)
			)
		)
	)
	(zone
		(net 62)
		(net_name "/BLOCK")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30048)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 148.270867 91.654446) (xy 148.21793 91.594908) (xy 148.184045 91.543098) (xy 148.145835 91.436696)
				(xy 148.118326 91.348765) (xy 148.057867 91.236107) (xy 147.849293 91.374293) (xy 147.711107 91.582867)
				(xy 147.838338 91.648876) (xy 147.911696 91.670835) (xy 148.011264 91.705471) (xy 148.066059 91.740002)
				(xy 148.129446 91.795867)
			)
		)
	)
	(zone
		(net 11)
		(net_name "/AD7")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30007)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 139.258757 112.635178) (xy 139.367208 112.750627) (xy 139.450509 112.854626) (xy 139.506487 112.940241)
				(xy 139.547915 113.021526) (xy 139.597111 113.178917) (xy 139.621684 113.378589) (xy 139.6259 113.436078)
				(xy 139.644556 113.651371) (xy 139.686333 113.920827) (xy 140.520707 113.755707) (xy 140.685827 112.921333)
				(xy 140.374143 112.875087) (xy 140.201078 112.8609) (xy 139.997533 112.841454) (xy 139.905092 112.823329)
				(xy 139.814338 112.794438) (xy 139.721869 112.750908) (xy 139.624287 112.688867) (xy 139.51819 112.604441)
				(xy 139.400178 112.493757)
			)
		)
	)
	(zone
		(net 5)
		(net_name "/AD1")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30017)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 132.797923 112.363521) (xy 132.803423 112.469203) (xy 132.797979 112.558809) (xy 132.784001 112.629462)
				(xy 132.762179 112.6903) (xy 132.696913 112.791282) (xy 132.590077 112.89052) (xy 132.536581 112.932552)
				(xy 132.3691 113.073141) (xy 132.281061 113.166317) (xy 132.193251 113.282765) (xy 132.900098 113.755995)
				(xy 133.606749 113.282765) (xy 133.460094 113.093278) (xy 133.291299 112.927773) (xy 133.185983 112.827279)
				(xy 133.099963 112.714588) (xy 133.06506 112.645176) (xy 133.036026 112.562525) (xy 133.013209 112.463238)
				(xy 132.996959 112.343917)
			)
		)
	)
	(zone
		(net 2)
		(net_name "VMEM")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30030)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 143.925 100.269236) (xy 143.929761 100.134041) (xy 143.943092 100.039009) (xy 143.968901 99.938694)
				(xy 144.019236 99.733527) (xy 143.725 99.674) (xy 143.430764 99.733527) (xy 143.481099 99.938696)
				(xy 143.513028 100.072951) (xy 143.525 100.269236)
			)
		)
	)
	(zone
		(net 47)
		(net_name "/A3")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30074)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 156.241124 100.133942) (xy 156.221359 100.137768) (xy 156.108128 100.150448) (xy 156.052865 100.137889)
				(xy 156.0125 100.1) (xy 155.499049 100.275309) (xy 156.080067 100.415848) (xy 156.103046 100.375936)
				(xy 156.162394 100.347577) (xy 156.265295 100.329364) (xy 156.302927 100.324152)
			)
		)
	)
	(zone
		(net 3)
		(net_name "VBUS")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30158)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 127.010355 91.625) (xy 127.023375 91.626835) (xy 127.071355 91.635344) (xy 127.120778 91.65597)
				(xy 127.159405 91.698969) (xy 127.175 91.774599) (xy 127.351 91.675) (xy 127.175 91.368733) (xy 127.170322 91.385237)
				(xy 127.157576 91.390506) (xy 127.112629 91.375973) (xy 127.07317 91.354564) (xy 127.010355 91.325)
			)
		)
	)
	(zone
		(net 13)
		(net_name "/A9")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30132)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 155.149001 91.775) (xy 155.184816 91.772822) (xy 155.279804 91.772388) (xy 155.320494 91.786763)
				(xy 155.3453 91.819291) (xy 155.700001 91.675) (xy 155.3453 91.530709) (xy 155.315512 91.566224)
				(xy 155.256942 91.579929) (xy 155.184816 91.577179) (xy 155.149001 91.575)
			)
		)
	)
	(zone
		(net 21)
		(net_name "/RAMRST")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30008)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 172.420178 117.556243) (xy 172.535627 117.447792) (xy 172.639626 117.364491) (xy 172.725241 117.308513)
				(xy 172.806526 117.267085) (xy 172.963917 117.217888) (xy 173.163588 117.193315) (xy 173.221079 117.189099)
				(xy 173.436371 117.170444) (xy 173.705827 117.128667) (xy 173.540707 116.294293) (xy 172.706333 116.129173)
				(xy 172.660087 116.440856) (xy 172.6459 116.613922) (xy 172.626454 116.817466) (xy 172.608329 116.909907)
				(xy 172.579438 117.000662) (xy 172.535908 117.09313) (xy 172.473866 117.190712) (xy 172.38944 117.29681)
				(xy 172.278757 117.414822)
			)
		)
	)
	(zone
		(net 44)
		(net_name "/BUS_A9")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30005)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 144.172396 115.034336) (xy 144.095605 114.863725) (xy 144.04099 114.718357) (xy 144.006104 114.598568)
				(xy 143.984039 114.490689) (xy 143.9638 114.269075) (xy 143.961275 114.202989) (xy 143.946205 113.942863)
				(xy 143.926874 113.781142) (xy 143.893667 113.589173) (xy 143.059567 113.7541) (xy 142.587765 114.461749)
				(xy 142.780483 114.56864) (xy 142.972483 114.63483) (xy 143.179142 114.670676) (xy 143.305873 114.682174)
				(xy 143.501583 114.703933) (xy 143.592664 114.725507) (xy 143.679625 114.760237) (xy 143.762763 114.812642)
				(xy 143.842374 114.887243) (xy 143.918755 114.98856) (xy 143.992202 115.121112)
			)
		)
	)
	(zone
		(net 19)
		(net_name "/A15")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30077)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 131.209935 90.866506) (xy 131.202273 90.909832) (xy 131.176621 91.024863) (xy 131.151799 91.070365)
				(xy 131.114145 91.091595) (xy 131.249618 91.675923) (xy 131.425 91.1625) (xy 131.386322 91.121545)
				(xy 131.374938 91.058144) (xy 131.391059 90.958368) (xy 131.394711 90.943038)
			)
		)
	)
	(zone
		(net 45)
		(net_name "/A16")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30133)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 135.649 90.775) (xy 135.684815 90.772822) (xy 135.779803 90.772388) (xy 135.820493 90.786763)
				(xy 135.845299 90.819291) (xy 136.2 90.675) (xy 135.845299 90.530709) (xy 135.815511 90.566224)
				(xy 135.756941 90.579929) (xy 135.684815 90.577179) (xy 135.649 90.575)
			)
		)
	)
	(zone
		(net 3)
		(net_name "VBUS")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30028)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 151.075 110.35) (xy 150.951375 110.329097) (xy 150.882 110.301818) (xy 150.814887 110.262408)
				(xy 150.765308 110.220554) (xy 150.723828 110.169703) (xy 150.697581 110.120168) (xy 150.680735 110.0639)
				(xy 150.675 110.002775) (xy 150.049 110.275) (xy 150.595 110.675) (xy 150.628605 110.645744) (xy 150.709182 110.629717)
				(xy 150.869677 110.63392) (xy 150.948691 110.641011) (xy 151.075 110.65)
			)
		)
	)
	(zone
		(net 33)
		(net_name "/BUS_A10")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30098)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 147.561019 108.982784) (xy 147.56724 108.953622) (xy 147.606389 108.810622) (xy 147.64162 108.749698)
				(xy 147.66472 108.729375) (xy 147.692075 108.718668) (xy 147.520382 108.424077) (xy 147.327612 108.688268)
				(xy 147.354036 108.702025) (xy 147.372478 108.721806) (xy 147.390742 108.779566) (xy 147.38474 108.866293)
				(xy 147.376738 108.904086) (xy 147.376243 108.906251)
			)
		)
	)
	(zone
		(net 61)
		(net_name "/~{WR}")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30006)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 155.66 112.071333) (xy 155.655052 112.229654) (xy 155.640415 112.362095) (xy 155.619459 112.462216)
				(xy 155.591276 112.548987) (xy 155.514771 112.695066) (xy 155.390958 112.853631) (xy 155.353288 112.897263)
				(xy 155.214244 113.06269) (xy 155.053251 113.282765) (xy 155.76 113.756) (xy 156.466749 113.282765)
				(xy 156.279056 113.029671) (xy 156.166712 112.897263) (xy 156.036535 112.739586) (xy 155.983985 112.661403)
				(xy 155.940242 112.576801) (xy 155.905637 112.480636) (xy 155.880506 112.367765) (xy 155.865182 112.233045)
				(xy 155.86 112.071333)
			)
		)
	)
	(zone
		(net 48)
		(net_name "/BYTE")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30069)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 148.925 99.075) (xy 148.950352 99.074499) (xy 149.068637 99.080524) (xy 149.121699 99.101166)
				(xy 149.154015 99.143339) (xy 149.701 98.975) (xy 149.154015 98.806661) (xy 149.121972 98.848649)
				(xy 149.059213 98.871245) (xy 148.950353 98.875501) (xy 148.925 98.875)
			)
		)
	)
	(zone
		(net 62)
		(net_name "/BLOCK")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30039)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 150.105764 99.725) (xy 150.188989 99.729708) (xy 150.254514 99.742662) (xy 150.35331 99.787022)
				(xy 150.393409 99.813048) (xy 150.491663 99.8712) (xy 150.557406 99.897452) (xy 150.641473 99.919236)
				(xy 150.701 99.625) (xy 150.641473 99.330764) (xy 150.560601 99.351507) (xy 150.496727 99.376418)
				(xy 150.393409 99.436952) (xy 150.340883 99.470383) (xy 150.281776 99.498464) (xy 150.206574 99.5178)
				(xy 150.105764 99.525)
			)
		)
	)
	(zone
		(net 30)
		(net_name "/~{CE}")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30134)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 142.149 95.775) (xy 142.184815 95.772822) (xy 142.279803 95.772388) (xy 142.320493 95.786763)
				(xy 142.345299 95.819291) (xy 142.7 95.675) (xy 142.345299 95.530709) (xy 142.315511 95.566224)
				(xy 142.256941 95.579929) (xy 142.184815 95.577179) (xy 142.149 95.575)
			)
		)
	)
	(zone
		(net 18)
		(net_name "/A14")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30135)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 142.149 89.775) (xy 142.184815 89.772822) (xy 142.279803 89.772388) (xy 142.320493 89.786763)
				(xy 142.345299 89.819291) (xy 142.7 89.675) (xy 142.345299 89.530709) (xy 142.315511 89.566224)
				(xy 142.256941 89.579929) (xy 142.184815 89.577179) (xy 142.149 89.575)
			)
		)
	)
	(zone
		(net 11)
		(net_name "/AD7")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30136)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 142.149 95.275) (xy 142.184815 95.272822) (xy 142.279803 95.272388) (xy 142.320493 95.286763)
				(xy 142.345299 95.319291) (xy 142.7 95.175) (xy 142.345299 95.030709) (xy 142.315511 95.066224)
				(xy 142.256941 95.079929) (xy 142.184815 95.077179) (xy 142.149 95.075)
			)
		)
	)
	(zone
		(net 16)
		(net_name "/A12")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30137)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 155.149 90.275) (xy 155.184815 90.272822) (xy 155.279803 90.272388) (xy 155.320493 90.286763)
				(xy 155.345299 90.319291) (xy 155.7 90.175) (xy 155.345299 90.030709) (xy 155.315511 90.066224)
				(xy 155.256941 90.079929) (xy 155.184815 90.077179) (xy 155.149 90.075)
			)
		)
	)
	(zone
		(net 3)
		(net_name "VBUS")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30029)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 147.32 110.650764) (xy 147.313399 110.870748) (xy 147.287193 111.033046) (xy 147.278984 111.07275)
				(xy 147.255764 111.186473) (xy 147.55 111.246) (xy 147.844236 111.186473) (xy 147.79266 111.00084)
				(xy 147.775882 110.956865) (xy 147.736228 110.834638) (xy 147.724339 110.755846) (xy 147.72 110.650764)
			)
		)
	)
	(zone
		(net 6)
		(net_name "/AD2")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30111)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 136.749 92.075) (xy 136.713185 92.077179) (xy 136.618197 92.077612) (xy 136.577507 92.063237)
				(xy 136.552701 92.030709) (xy 136.198 92.175) (xy 136.552701 92.319291) (xy 136.58249 92.283776)
				(xy 136.641061 92.270071) (xy 136.713185 92.272822) (xy 136.749 92.275)
			)
		)
	)
	(zone
		(net 3)
		(net_name "VBUS")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30026)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 125.425 90.675) (xy 125.435067 90.76466) (xy 125.447994 90.867352) (xy 125.445942 90.968009)
				(xy 125.433682 91.010682) (xy 125.410936 91.044576) (xy 125.375458 91.066935) (xy 125.325 91.075)
				(xy 125.725 91.476) (xy 126.125 91.075) (xy 126.084931 91.070206) (xy 126.053957 91.056651) (xy 126.016133 91.010261)
				(xy 126.000373 90.931465) (xy 126.009133 90.804439) (xy 126.014933 90.76466) (xy 126.025 90.675)
			)
		)
	)
	(zone
		(net 63)
		(net_name "/A0")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30070)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 148.929041 98.135776) (xy 148.98882 98.175964) (xy 149.068157 98.229666) (xy 149.093928 98.258164)
				(xy 149.1 98.286799) (xy 149.700755 98.325654) (xy 149.730816 98.15) (xy 149.598922 98.150997) (xy 149.476592 98.142104)
				(xy 149.367528 98.124414) (xy 149.269322 98.098288) (xy 149.187351 98.066298) (xy 149.116583 98.027598)
				(xy 149.060013 97.984626)
			)
		)
	)
	(zone
		(net 5)
		(net_name "/AD1")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30059)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 128.75 98.25) (xy 128.749499 98.224648) (xy 128.755524 98.106364) (xy 128.776166 98.053302)
				(xy 128.818339 98.020985) (xy 128.65 97.474) (xy 128.481661 98.020985) (xy 128.523649 98.053029)
				(xy 128.546245 98.115788) (xy 128.550501 98.224647) (xy 128.55 98.25)
			)
		)
	)
	(zone
		(net 31)
		(net_name "/A18_CE2")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30053)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 146.32 110.020196) (xy 146.324668 109.940664) (xy 146.337342 109.880069) (xy 146.385561 109.777813)
				(xy 146.428285 109.696184) (xy 146.465196 109.573773) (xy 146.22 109.524) (xy 145.974804 109.573773)
				(xy 146.018094 109.710415) (xy 146.054439 109.777813) (xy 146.100353 109.872709) (xy 146.114681 109.935872)
				(xy 146.12 110.020196)
			)
		)
	)
	(zone
		(net 10)
		(net_name "/AD6")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30138)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 142.149 94.775) (xy 142.184815 94.772822) (xy 142.279803 94.772388) (xy 142.320493 94.786763)
				(xy 142.345299 94.819291) (xy 142.7 94.675) (xy 142.345299 94.530709) (xy 142.315511 94.566224)
				(xy 142.256941 94.579929) (xy 142.184815 94.577179) (xy 142.149 94.575)
			)
		)
	)
	(zone
		(net 7)
		(net_name "/AD3")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30157)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 135.693765 93.291392) (xy 135.720767 93.286945) (xy 135.804341 93.279755) (xy 135.843903 93.292152)
				(xy 135.874 93.325) (xy 136.199993 93.174889) (xy 135.8361 93.036855) (xy 135.825337 93.059619)
				(xy 135.808249 93.075079) (xy 135.753907 93.090574) (xy 135.705731 93.091816) (xy 135.671373 93.09265)
			)
		)
	)
	(zone
		(net 8)
		(net_name "/AD4")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30112)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 136.749 93.575) (xy 136.713185 93.577179) (xy 136.618197 93.577612) (xy 136.577507 93.563237)
				(xy 136.552701 93.530709) (xy 136.198 93.675) (xy 136.552701 93.819291) (xy 136.58249 93.783776)
				(xy 136.641061 93.770071) (xy 136.713185 93.772822) (xy 136.749 93.775)
			)
		)
	)
	(zone
		(net 30)
		(net_name "/~{CE}")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30149)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 135.678252 95.798367) (xy 135.702705 95.793051) (xy 135.796676 95.780253) (xy 135.841332 95.791172)
				(xy 135.874 95.825) (xy 136.199965 95.674742) (xy 135.826943 95.542973) (xy 135.801914 95.576395)
				(xy 135.741361 95.595229) (xy 135.675401 95.600898) (xy 135.62649 95.605183)
			)
		)
	)
	(zone
		(net 2)
		(net_name "VMEM")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30040)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 143.130764 99.075) (xy 143.213989 99.079708) (xy 143.279514 99.092662) (xy 143.37831 99.137022)
				(xy 143.418409 99.163048) (xy 143.516663 99.2212) (xy 143.582406 99.247452) (xy 143.666473 99.269236)
				(xy 143.726 98.975) (xy 143.666473 98.680764) (xy 143.585601 98.701507) (xy 143.521727 98.726418)
				(xy 143.418409 98.786952) (xy 143.365883 98.820383) (xy 143.306776 98.848464) (xy 143.231574 98.8678)
				(xy 143.130764 98.875)
			)
		)
	)
	(zone
		(net 5)
		(net_name "/AD1")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30113)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 136.749 91.575) (xy 136.713185 91.577179) (xy 136.618197 91.577612) (xy 136.577507 91.563237)
				(xy 136.552701 91.530709) (xy 136.198 91.675) (xy 136.552701 91.819291) (xy 136.58249 91.783776)
				(xy 136.641061 91.770071) (xy 136.713185 91.772822) (xy 136.749 91.775)
			)
		)
	)
	(zone
		(net 17)
		(net_name "/A13")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30139)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 142.148999 89.275) (xy 142.184814 89.272822) (xy 142.279802 89.272388) (xy 142.320492 89.286763)
				(xy 142.345298 89.319291) (xy 142.699999 89.175) (xy 142.345298 89.030709) (xy 142.31551 89.066224)
				(xy 142.25694 89.079929) (xy 142.184814 89.077179) (xy 142.148999 89.075)
			)
		)
	)
	(zone
		(net 8)
		(net_name "/AD4")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30140)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 142.149 93.775) (xy 142.184815 93.772822) (xy 142.279803 93.772388) (xy 142.320493 93.786763)
				(xy 142.345299 93.819291) (xy 142.7 93.675) (xy 142.345299 93.530709) (xy 142.315511 93.566224)
				(xy 142.256941 93.579929) (xy 142.184815 93.577179) (xy 142.149 93.575)
			)
		)
	)
	(zone
		(net 4)
		(net_name "/AD0")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30060)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 128.1 98.25) (xy 128.099499 98.224648) (xy 128.105524 98.106364) (xy 128.126166 98.053302) (xy 128.168339 98.020985)
				(xy 128 97.474) (xy 127.831661 98.020985) (xy 127.873649 98.053029) (xy 127.896245 98.115788) (xy 127.900501 98.224647)
				(xy 127.9 98.25)
			)
		)
	)
	(zone
		(net 4)
		(net_name "/AD0")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30101)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 135.673407 91.325399) (xy 135.701271 91.320811) (xy 135.80838 91.304414) (xy 135.931088 91.293654)
				(xy 136.064801 91.29752) (xy 136.204924 91.325) (xy 136.199974 91.174778) (xy 135.811108 91.061721)
				(xy 135.804589 91.083001) (xy 135.790364 91.098833) (xy 135.736745 91.119628) (xy 135.666966 91.127028)
				(xy 135.628913 91.130412)
			)
		)
	)
	(zone
		(net 21)
		(net_name "/RAMRST")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30151)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 140.075 101.35) (xy 140.076563 101.295167) (xy 140.0875 101.229037) (xy 140.117188 101.173389)
				(xy 140.141992 101.156301) (xy 140.175 101.15) (xy 139.975 100.949) (xy 139.775 101.15) (xy 139.803918 101.154711)
				(xy 139.826643 101.167688) (xy 139.858209 101.215955) (xy 139.873737 101.299533) (xy 139.875 101.35)
			)
		)
	)
	(zone
		(net 45)
		(net_name "/A16")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30141)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 142.149 90.775) (xy 142.184815 90.772822) (xy 142.279803 90.772388) (xy 142.320493 90.786763)
				(xy 142.345299 90.819291) (xy 142.7 90.675) (xy 142.345299 90.530709) (xy 142.315511 90.566224)
				(xy 142.256941 90.579929) (xy 142.184815 90.577179) (xy 142.149 90.575)
			)
		)
	)
	(zone
		(net 2)
		(net_name "VMEM")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30022)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 156.425 93.325) (xy 156.545501 93.345731) (xy 156.613702 93.373005) (xy 156.679937 93.412321)
				(xy 156.730111 93.454808) (xy 156.772471 93.506435) (xy 156.799851 93.557066) (xy 156.817927 93.614569)
				(xy 156.825 93.684168) (xy 157.451 93.425) (xy 157.499028 93.025) (xy 157.289119 93.053446) (xy 157.004807 93.056004)
				(xy 156.714695 93.039381) (xy 156.425 93.025)
			)
		)
	)
	(zone
		(net 48)
		(net_name "/BYTE")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30043)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 149.195641 105.724257) (xy 149.122246 105.695268) (xy 149.07053 105.663505) (xy 149.013121 105.596459)
				(xy 148.980546 105.531697) (xy 148.899441 105.383329) (xy 148.649049 105.549691) (xy 148.591473 105.844236)
				(xy 148.738138 105.878122) (xy 148.837076 105.910401) (xy 148.896615 105.933912) (xy 149.102933 106.009571)
			)
		)
	)
	(zone
		(net 48)
		(net_name "/BYTE")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30045)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 151.425 106.1) (xy 151.491579 106.090878) (xy 151.604554 106.078745) (xy 151.653453 106.090592)
				(xy 151.6875 106.125) (xy 152.201 105.95) (xy 151.6875 105.775) (xy 151.649436 105.811332) (xy 151.585856 105.821559)
				(xy 151.491579 105.809122) (xy 151.425 105.8)
			)
		)
	)
	(zone
		(net 62)
		(net_name "/BLOCK")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30037)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 151.241112 107.1) (xy 151.175651 107.095199) (xy 151.125756 107.081589) (xy 151.06085 107.036667)
				(xy 151.014582 106.977283) (xy 150.957146 106.903294) (xy 150.866671 106.825559) (xy 150.699 107.075)
				(xy 150.641473 107.369236) (xy 150.813196 107.398265) (xy 150.932718 107.406532) (xy 151.042931 107.404129)
				(xy 151.241112 107.4)
			)
		)
	)
	(zone
		(net 31)
		(net_name "/A18_CE2")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30156)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 155.203723 94.299548) (xy 155.220994 94.294715) (xy 155.302347 94.280368) (xy 155.342651 94.290851)
				(xy 155.374001 94.325) (xy 155.699867 94.1745) (xy 155.318279 94.050991) (xy 155.295477 94.082997)
				(xy 155.232101 94.106117) (xy 155.159097 94.117529) (xy 155.103724 94.126345)
			)
		)
	)
	(zone
		(net 8)
		(net_name "/AD4")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30061)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 130.7 98.25) (xy 130.699499 98.224648) (xy 130.705524 98.106364) (xy 130.726166 98.053302) (xy 130.768339 98.020985)
				(xy 130.6 97.474) (xy 130.431661 98.020985) (xy 130.473649 98.053029) (xy 130.496245 98.115788)
				(xy 130.500501 98.224647) (xy 130.5 98.25)
			)
		)
	)
	(zone
		(net 8)
		(net_name "/AD4")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30014)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 136.806233 115.209032) (xy 136.907416 115.418599) (xy 136.975461 115.585078) (xy 137.013667 115.70484)
				(xy 137.040003 115.816811) (xy 137.074399 116.030789) (xy 137.146333 116.460827) (xy 137.980454 116.29589)
				(xy 138.145827 115.461333) (xy 137.921017 115.433977) (xy 137.685491 115.437067) (xy 137.625207 115.440847)
				(xy 137.434794 115.447522) (xy 137.349461 115.439547) (xy 137.269473 115.41842) (xy 137.193904 115.379933)
				(xy 137.121825 115.319878) (xy 137.05231 115.234046) (xy 136.984431 115.11823)
			)
		)
	)
	(zone
		(net 64)
		(net_name "/A2")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30155)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 156.284092 96.1251) (xy 156.236422 96.119275) (xy 156.138064 96.10373) (xy 156.099963 96.08514)
				(xy 156.081863 96.054196) (xy 155.698077 96.174618) (xy 156.024 96.325) (xy 156.040516 96.304437)
				(xy 156.061468 96.29252) (xy 156.118993 96.288844) (xy 156.180326 96.302827) (xy 156.207556 96.309875)
			)
		)
	)
	(zone
		(net 8)
		(net_name "/AD4")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30103)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 135.663017 93.791218) (xy 135.693815 93.7868) (xy 135.794449 93.779103) (xy 135.840977 93.791555)
				(xy 135.874 93.825) (xy 136.199991 93.67487) (xy 135.837163 93.536145) (xy 135.809383 93.57155)
				(xy 135.749353 93.588931) (xy 135.678885 93.591742) (xy 135.636914 93.59293)
			)
		)
	)
	(zone
		(net 67)
		(net_name "Net-(U6-Pad6)")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30152)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 143.825 102) (xy 143.826563 101.945167) (xy 143.8375 101.879037) (xy 143.867188 101.823389)
				(xy 143.891992 101.806301) (xy 143.925 101.8) (xy 143.725 101.599) (xy 143.525 101.8) (xy 143.553918 101.804711)
				(xy 143.576643 101.817688) (xy 143.608209 101.865955) (xy 143.623737 101.949533) (xy 143.625 102)
			)
		)
	)
	(zone
		(net 14)
		(net_name "/A10")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30093)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 127.97241 90.923968) (xy 127.968603 90.948333) (xy 127.948196 91.032972) (xy 127.923126 91.066522)
				(xy 127.881386 91.081189) (xy 127.999805 91.67598) (xy 128.175 91.1625) (xy 128.145638 91.121851)
				(xy 128.144363 91.059795) (xy 128.159735 90.996555) (xy 128.168566 90.962986)
			)
		)
	)
	(zone
		(net 12)
		(net_name "/A8")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30066)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 150.475 100.175) (xy 150.449647 100.175501) (xy 150.331363 100.169476) (xy 150.278301 100.148834)
				(xy 150.245985 100.106661) (xy 149.699 100.275) (xy 150.245985 100.443339) (xy 150.278029 100.401351)
				(xy 150.340788 100.378755) (xy 150.449648 100.374499) (xy 150.475 100.375)
			)
		)
	)
	(zone
		(net 15)
		(net_name "/A11")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30142)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 155.149 89.775) (xy 155.184815 89.772822) (xy 155.279803 89.772388) (xy 155.320493 89.786763)
				(xy 155.345299 89.819291) (xy 155.7 89.675) (xy 155.345299 89.530709) (xy 155.315511 89.566224)
				(xy 155.256941 89.579929) (xy 155.184815 89.577179) (xy 155.149 89.575)
			)
		)
	)
	(zone
		(net 46)
		(net_name "/A17")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30143)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 155.149 92.775) (xy 155.184815 92.772822) (xy 155.279803 92.772388) (xy 155.320493 92.786763)
				(xy 155.345299 92.819291) (xy 155.7 92.675) (xy 155.345299 92.530709) (xy 155.315511 92.566224)
				(xy 155.256941 92.579929) (xy 155.184815 92.577179) (xy 155.149 92.575)
			)
		)
	)
	(zone
		(net 2)
		(net_name "VMEM")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30021)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 158.475 93.125) (xy 158.373878 93.135984) (xy 158.263853 93.149578) (xy 158.155107 93.148397)
				(xy 158.107788 93.136748) (xy 158.06868 93.114786) (xy 158.040412 93.080302) (xy 158.025615 93.03109)
				(xy 157.449 93.425) (xy 158.025615 93.81891) (xy 158.03523 93.780821) (xy 158.052668 93.751191)
				(xy 158.106695 93.713668) (xy 158.194574 93.698302) (xy 158.332316 93.708105) (xy 158.373878 93.714016)
				(xy 158.475 93.725)
			)
		)
	)
	(zone
		(net 48)
		(net_name "/BYTE")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30034)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 145.373942 103) (xy 145.473194 102.994115) (xy 145.644077 102.986352) (xy 145.719919 102.994506)
				(xy 145.775516 103.017805) (xy 146.251 102.575) (xy 145.504278 102.58509) (xy 145.51752 102.633203)
				(xy 145.519311 102.674478) (xy 145.49644 102.737846) (xy 145.445021 102.781378) (xy 145.373942 102.8)
			)
		)
	)
	(zone
		(net 6)
		(net_name "/AD2")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30100)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 129.272175 96.792462) (xy 129.269719 96.806705) (xy 129.253701 96.853996) (xy 129.22964 96.871999)
				(xy 129.18678 96.880116) (xy 129.299778 97.475974) (xy 129.475 96.9625) (xy 129.45412 96.941465)
				(xy 129.445353 96.919986) (xy 129.452104 96.87532) (xy 129.458493 96.860071) (xy 129.46716 96.836967)
			)
		)
	)
	(zone
		(net 14)
		(net_name "/A10")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30144)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 155.149001 89.275) (xy 155.184816 89.272822) (xy 155.279804 89.272388) (xy 155.320494 89.286763)
				(xy 155.3453 89.319291) (xy 155.700001 89.175) (xy 155.3453 89.030709) (xy 155.315512 89.066224)
				(xy 155.256942 89.079929) (xy 155.184816 89.077179) (xy 155.149001 89.075)
			)
		)
	)
	(zone
		(net 22)
		(net_name "/~{Y0}")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30002)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 162.978161 112.138416) (xy 163.014934 112.253727) (xy 163.037309 112.35666) (xy 163.046436 112.444078)
				(xy 163.045029 112.52328) (xy 163.015004 112.663024) (xy 162.948504 112.799518) (xy 162.848437 112.946276)
				(xy 162.762677 113.069095) (xy 162.678411 113.210692) (xy 162.603633 113.380805) (xy 162.546333 113.589173)
				(xy 163.380342 113.755939) (xy 164.086749 113.282765) (xy 163.901163 113.036017) (xy 163.720329 112.848216)
				(xy 163.636398 112.771766) (xy 163.509839 112.653667) (xy 163.391812 112.517071) (xy 163.278503 112.332383)
				(xy 163.166099 112.070012)
			)
		)
	)
	(zone
		(net 3)
		(net_name "VBUS")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30047)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 150.504181 103.042049) (xy 150.452162 103.012524) (xy 150.408757 102.995716) (xy 150.329891 102.962059)
				(xy 150.30567 102.943106) (xy 150.3 102.921715) (xy 149.699293 102.874293) (xy 149.668036 103.05)
				(xy 149.775775 103.050266) (xy 149.874637 103.05981) (xy 150.051426 103.104211) (xy 150.197824 103.177735)
				(xy 150.292049 103.254181)
			)
		)
	)
	(zone
		(net 62)
		(net_name "/BLOCK")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30051)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 133.354804 91.475) (xy 133.434336 91.479668) (xy 133.494931 91.492342) (xy 133.597187 91.540561)
				(xy 133.678815 91.583285) (xy 133.801227 91.620196) (xy 133.851 91.375) (xy 133.801227 91.129804)
				(xy 133.664585 91.173094) (xy 133.597186 91.209439) (xy 133.50229 91.255353) (xy 133.439128 91.269681)
				(xy 133.354804 91.275)
			)
		)
	)
	(zone
		(net 66)
		(net_name "/A1")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30092)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 156.211103 98.813023) (xy 156.202433 98.816541) (xy 156.157478 98.833425) (xy 156.104188 98.844892)
				(xy 156.052536 98.838048) (xy 156.030443 98.82373) (xy 156.0125 98.8) (xy 155.499134 98.9755) (xy 156.094107 99.092119)
				(xy 156.113439 99.057797) (xy 156.175524 99.026029) (xy 156.25161 99.003847) (xy 156.311103 98.986227)
			)
		)
	)
	(zone
		(net 46)
		(net_name "/A17")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30050)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 132.45 92.179804) (xy 132.445332 92.259336) (xy 132.432658 92.319931) (xy 132.384439 92.422186)
				(xy 132.341714 92.503815) (xy 132.304804 92.626227) (xy 132.55 92.676) (xy 132.795196 92.626227)
				(xy 132.751905 92.489584) (xy 132.715561 92.422187) (xy 132.669647 92.327291) (xy 132.655319 92.264128)
				(xy 132.65 92.179804)
			)
		)
	)
	(zone
		(net 41)
		(net_name "/A7")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30145)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 155.149 91.275) (xy 155.184815 91.272822) (xy 155.279803 91.272388) (xy 155.320493 91.286763)
				(xy 155.345299 91.319291) (xy 155.7 91.175) (xy 155.345299 91.030709) (xy 155.315511 91.066224)
				(xy 155.256941 91.079929) (xy 155.184815 91.077179) (xy 155.149 91.075)
			)
		)
	)
	(zone
		(net 6)
		(net_name "/AD2")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30062)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 129.4 98.25) (xy 129.399499 98.224648) (xy 129.405524 98.106364) (xy 129.426166 98.053302) (xy 129.468339 98.020985)
				(xy 129.3 97.474) (xy 129.131661 98.020985) (xy 129.173649 98.053029) (xy 129.196245 98.115788)
				(xy 129.200501 98.224647) (xy 129.2 98.25)
			)
		)
	)
	(zone
		(net 31)
		(net_name "/A18_CE2")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30095)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 146.12 109.8) (xy 146.12001 109.807653) (xy 146.118681 109.873933) (xy 146.108665 109.950874)
				(xy 146.081223 110.019725) (xy 146.058235 110.045256) (xy 146.027612 110.061732) (xy 146.22 110.326)
				(xy 146.412388 110.061732) (xy 146.364506 110.027649) (xy 146.333862 109.961181) (xy 146.320508 109.855447)
				(xy 146.31999 109.807653) (xy 146.32 109.8)
			)
		)
	)
	(zone
		(net 33)
		(net_name "/BUS_A10")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30012)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 146.59554 115.118212) (xy 146.542241 115.21199) (xy 146.488051 115.286653) (xy 146.437321 115.339951)
				(xy 146.385122 115.380539) (xy 146.276696 115.429373) (xy 146.145361 115.447504) (xy 145.95477 115.44084)
				(xy 145.717175 115.432202) (xy 145.581903 115.439538) (xy 145.434173 115.461333) (xy 145.599546 116.29589)
				(xy 146.433667 116.460827) (xy 146.505604 116.030723) (xy 146.534639 115.844731) (xy 146.575962 115.671261)
				(xy 146.649139 115.472094) (xy 146.773738 115.209014)
			)
		)
	)
	(zone
		(net 7)
		(net_name "/AD3")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30003)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 135.056284 112.134548) (xy 135.092676 112.248815) (xy 135.114743 112.350905) (xy 135.12363 112.4377)
				(xy 135.122006 112.516358) (xy 135.091574 112.654994) (xy 135.024745 112.789647) (xy 134.918441 112.940986)
				(xy 134.829392 113.064375) (xy 134.742077 113.206824) (xy 134.664918 113.378402) (xy 134.606333 113.589173)
				(xy 135.440342 113.755939) (xy 136.146749 113.282765) (xy 135.95702 113.029557) (xy 135.772774 112.835499)
				(xy 135.708446 112.774871) (xy 135.583987 112.654209) (xy 135.468064 112.515777) (xy 135.356277 112.329711)
				(xy 135.244223 112.066146)
			)
		)
	)
	(zone
		(net 21)
		(net_name "/RAMRST")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30027)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 140.464301 99.92479) (xy 140.516772 99.85936) (xy 140.58748 99.787812) (xy 140.665875 99.723588)
				(xy 140.751922 99.669938) (xy 140.818822 99.641354) (xy 140.886058 99.626201) (xy 140.927848 99.625)
				(xy 140.900383 98.974077) (xy 140.550001 98.880697) (xy 140.538008 99.114555) (xy 140.487253 99.372189)
				(xy 140.399526 99.626807) (xy 140.34629 99.738365) (xy 140.289879 99.833198) (xy 140.279525 99.848256)
			)
		)
	)
	(zone
		(net 18)
		(net_name "/A14")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30114)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 136.749 89.575) (xy 136.713185 89.577179) (xy 136.618197 89.577612) (xy 136.577507 89.563237)
				(xy 136.552701 89.530709) (xy 136.198 89.675) (xy 136.552701 89.819291) (xy 136.58249 89.783776)
				(xy 136.641061 89.770071) (xy 136.713185 89.772822) (xy 136.749 89.775)
			)
		)
	)
	(zone
		(net 7)
		(net_name "/AD3")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30063)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 130.05 98.25) (xy 130.049499 98.224648) (xy 130.055524 98.106364) (xy 130.076166 98.053302)
				(xy 130.118339 98.020985) (xy 129.95 97.474) (xy 129.781661 98.020985) (xy 129.823649 98.053029)
				(xy 129.846245 98.115788) (xy 129.850501 98.224647) (xy 129.85 98.25)
			)
		)
	)
	(zone
		(net 7)
		(net_name "/AD3")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30096)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 129.927935 96.754322) (xy 129.92392 96.775362) (xy 129.904068 96.842448) (xy 129.879411 96.868523)
				(xy 129.838052 96.879863) (xy 129.949761 97.47597) (xy 130.125 96.9625) (xy 130.10568 96.943163)
				(xy 130.096257 96.921202) (xy 130.099831 96.867491) (xy 130.112581 96.830168) (xy 130.122122 96.802187)
			)
		)
	)
	(zone
		(net 11)
		(net_name "/AD7")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30161)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 135.735238 95.294067) (xy 135.755287 95.2884) (xy 135.804652 95.27965) (xy 135.827667 95.290047)
				(xy 135.845299 95.319291) (xy 136.199987 95.174844) (xy 135.830749 95.04043) (xy 135.820326 95.065953)
				(xy 135.804122 95.082073) (xy 135.757239 95.095031) (xy 135.731514 95.095459) (xy 135.703947 95.096531)
			)
		)
	)
	(zone
		(net 66)
		(net_name "/A1")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30159)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 156.288557 96.650756) (xy 156.229179 96.636855) (xy 156.13891 96.614397) (xy 156.105984 96.595837)
				(xy 156.091952 96.569294) (xy 155.698135 96.6745) (xy 156.024001 96.825) (xy 156.040519 96.804145)
				(xy 156.060721 96.793246) (xy 156.11188 96.794381) (xy 156.168034 96.81532) (xy 156.188558 96.82396)
			)
		)
	)
	(zone
		(net 20)
		(net_name "/~{RD}")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30004)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 154.65511 115.009669) (xy 154.730489 115.177341) (xy 154.784173 115.320737) (xy 154.81856 115.439583)
				(xy 154.840175 115.546631) (xy 154.859003 115.764585) (xy 154.861164 115.839273) (xy 154.874151 116.102476)
				(xy 154.892956 116.266208) (xy 154.926333 116.460827) (xy 155.760433 116.2959) (xy 156.232235 115.588251)
				(xy 156.03862 115.480734) (xy 155.845808 115.413908) (xy 155.63795 115.377125) (xy 155.519296 115.365511)
				(xy 155.32434 115.34222) (xy 155.233636 115.31999) (xy 155.14703 115.2847) (xy 155.064208 115.231848)
				(xy 154.984855 115.156931) (xy 154.908658 115.055447) (xy 154.835303 114.922892)
			)
		)
	)
	(zone
		(net 62)
		(net_name "/BLOCK")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30160)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 133.55 91.275) (xy 133.479349 91.290603) (xy 133.408305 91.307556) (xy 133.384228 91.30671)
				(xy 133.375 91.294362) (xy 133.199 91.675) (xy 133.375 91.754782) (xy 133.379752 91.683695) (xy 133.393017 91.623272)
				(xy 133.413525 91.572948) (xy 133.439661 91.533189) (xy 133.470244 91.503579) (xy 133.503435 91.484457)
				(xy 133.55 91.475)
			)
		)
	)
	(zone
		(net 21)
		(net_name "/RAMRST")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30153)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 139.875 101.2) (xy 139.873438 101.254833) (xy 139.8625 101.320963) (xy 139.832813 101.376611)
				(xy 139.808008 101.393699) (xy 139.775 101.4) (xy 139.975 101.601) (xy 140.175 101.4) (xy 140.146082 101.395289)
				(xy 140.123357 101.382312) (xy 140.091791 101.334045) (xy 140.076263 101.250467) (xy 140.075 101.2)
			)
		)
	)
	(zone
		(net 9)
		(net_name "/AD5")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30115)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 136.749 94.075) (xy 136.713185 94.077179) (xy 136.618197 94.077612) (xy 136.577507 94.063237)
				(xy 136.552701 94.030709) (xy 136.198 94.175) (xy 136.552701 94.319291) (xy 136.58249 94.283776)
				(xy 136.641061 94.270071) (xy 136.713185 94.272822) (xy 136.749 94.275)
			)
		)
	)
	(zone
		(net 5)
		(net_name "/AD1")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30094)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 128.62713 96.724603) (xy 128.622978 96.749363) (xy 128.601868 96.833113) (xy 128.576673 96.866145)
				(xy 128.53513 96.880444) (xy 128.649793 97.475978) (xy 128.825 96.9625) (xy 128.796776 96.922019)
				(xy 128.797046 96.860665) (xy 128.813128 96.800258) (xy 128.822759 96.766186)
			)
		)
	)
	(zone
		(net 18)
		(net_name "/A14")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30146)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 135.649 89.775) (xy 135.684815 89.772822) (xy 135.779803 89.772388) (xy 135.820493 89.786763)
				(xy 135.845299 89.819291) (xy 136.2 89.675) (xy 135.845299 89.530709) (xy 135.815511 89.566224)
				(xy 135.756941 89.579929) (xy 135.684815 89.577179) (xy 135.649 89.575)
			)
		)
	)
	(zone
		(net 10)
		(net_name "/AD6")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30064)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 132 98.25) (xy 131.999499 98.224648) (xy 132.005524 98.106364) (xy 132.026166 98.053302) (xy 132.068339 98.020985)
				(xy 131.9 97.474) (xy 131.731661 98.020985) (xy 131.773649 98.053029) (xy 131.796245 98.115788)
				(xy 131.800501 98.224647) (xy 131.8 98.25)
			)
		)
	)
	(zone
		(net 67)
		(net_name "Net-(U6-Pad6)")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30154)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 143.625 101.85) (xy 143.623438 101.904833) (xy 143.6125 101.970963) (xy 143.582813 102.026611)
				(xy 143.558008 102.043699) (xy 143.525 102.05) (xy 143.725 102.251) (xy 143.925 102.05) (xy 143.896082 102.045289)
				(xy 143.873357 102.032312) (xy 143.841791 101.984045) (xy 143.826263 101.900467) (xy 143.825 101.85)
			)
		)
	)
	(zone
		(net 21)
		(net_name "/RAMRST")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30088)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 139.375 101.7) (xy 139.382653 101.69999) (xy 139.448933 101.701319) (xy 139.525874 101.711335)
				(xy 139.594725 101.738777) (xy 139.620256 101.761765) (xy 139.636732 101.792388) (xy 139.976 101.6)
				(xy 139.636732 101.407612) (xy 139.602649 101.455494) (xy 139.536181 101.486138) (xy 139.430447 101.499492)
				(xy 139.382653 101.50001) (xy 139.375 101.5)
			)
		)
	)
	(zone
		(net 19)
		(net_name "/A15")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30116)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 136.749 90.075) (xy 136.713185 90.077179) (xy 136.618197 90.077612) (xy 136.577507 90.063237)
				(xy 136.552701 90.030709) (xy 136.198 90.175) (xy 136.552701 90.319291) (xy 136.58249 90.283776)
				(xy 136.641061 90.270071) (xy 136.713185 90.272822) (xy 136.749 90.275)
			)
		)
	)
	(zone
		(net 17)
		(net_name "/A13")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30117)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 136.749 89.075) (xy 136.713185 89.077179) (xy 136.618197 89.077612) (xy 136.577507 89.063237)
				(xy 136.552701 89.030709) (xy 136.198 89.175) (xy 136.552701 89.319291) (xy 136.58249 89.283776)
				(xy 136.641061 89.270071) (xy 136.713185 89.272822) (xy 136.749 89.275)
			)
		)
	)
	(zone
		(net 20)
		(net_name "/~{RD}")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30118)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 136.749 96.575) (xy 136.713185 96.577179) (xy 136.618197 96.577612) (xy 136.577507 96.563237)
				(xy 136.552701 96.530709) (xy 136.198 96.675) (xy 136.552701 96.819291) (xy 136.58249 96.783776)
				(xy 136.641061 96.770071) (xy 136.713185 96.772822) (xy 136.749 96.775)
			)
		)
	)
	(zone
		(net 48)
		(net_name "/BYTE")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30035)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 147.098016 103.031595) (xy 147.09748 103.031059) (xy 147.045799 102.977184) (xy 146.989281 102.905302)
				(xy 146.953574 102.827891) (xy 146.95154 102.79101) (xy 146.964328 102.757427) (xy 146.249293 102.574293)
				(xy 146.535576 103.070722) (xy 146.632225 103.04615) (xy 146.741132 103.055869) (xy 146.858001 103.101421)
				(xy 146.956595 103.173016)
			)
		)
	)
	(zone
		(net 20)
		(net_name "/~{RD}")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30147)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 142.148999 96.775) (xy 142.184814 96.772822) (xy 142.279802 96.772388) (xy 142.320492 96.786763)
				(xy 142.345298 96.819291) (xy 142.699999 96.675) (xy 142.345298 96.530709) (xy 142.31551 96.566224)
				(xy 142.25694 96.579929) (xy 142.184814 96.577179) (xy 142.148999 96.575)
			)
		)
	)
	(zone
		(net 6)
		(net_name "/AD2")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30148)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 142.149 92.275) (xy 142.184815 92.272822) (xy 142.279803 92.272388) (xy 142.320493 92.286763)
				(xy 142.345299 92.319291) (xy 142.7 92.175) (xy 142.345299 92.030709) (xy 142.315511 92.066224)
				(xy 142.256941 92.079929) (xy 142.184815 92.077179) (xy 142.149 92.075)
			)
		)
	)
	(zone
		(net 6)
		(net_name "/AD2")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30015)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 134.266233 115.209032) (xy 134.367416 115.418599) (xy 134.435461 115.585078) (xy 134.473667 115.70484)
				(xy 134.500003 115.816811) (xy 134.534399 116.030789) (xy 134.606333 116.460827) (xy 135.440454 116.29589)
				(xy 135.605827 115.461333) (xy 135.381017 115.433977) (xy 135.145491 115.437067) (xy 135.085207 115.440847)
				(xy 134.894794 115.447522) (xy 134.809461 115.439547) (xy 134.729473 115.41842) (xy 134.653904 115.379933)
				(xy 134.581825 115.319878) (xy 134.51231 115.234046) (xy 134.444431 115.11823)
			)
		)
	)
	(zone
		(net 8)
		(net_name "/AD4")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30085)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 130.576087 96.679001) (xy 130.569205 96.716607) (xy 130.544059 96.82247) (xy 130.518896 96.863729)
				(xy 130.480199 96.881425) (xy 130.599742 97.475965) (xy 130.775 96.9625) (xy 130.744343 96.922898)
				(xy 130.739792 96.857596) (xy 130.761083 96.761243) (xy 130.769272 96.730764)
			)
		)
	)
	(zone
		(net 10)
		(net_name "/AD6")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30016)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 139.346233 115.209032) (xy 139.447416 115.418599) (xy 139.515461 115.585078) (xy 139.553667 115.70484)
				(xy 139.580003 115.816811) (xy 139.614399 116.030789) (xy 139.686333 116.460827) (xy 140.520454 116.29589)
				(xy 140.685827 115.461333) (xy 140.461017 115.433977) (xy 140.225491 115.437067) (xy 140.165207 115.440847)
				(xy 139.974794 115.447522) (xy 139.889461 115.439547) (xy 139.809473 115.41842) (xy 139.733904 115.379933)
				(xy 139.661825 115.319878) (xy 139.59231 115.234046) (xy 139.524431 115.11823)
			)
		)
	)
	(zone
		(net 43)
		(net_name "/BUS_A8")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30055)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 158.799994 109.196429) (xy 158.753197 109.184568) (xy 158.650824 109.154467) (xy 158.612273 109.129436)
				(xy 158.596344 109.094123) (xy 157.999061 109.199658) (xy 157.991633 109.375) (xy 158.24523 109.335843)
				(xy 158.481944 109.335821) (xy 158.591099 109.349696) (xy 158.688581 109.371371) (xy 158.73159 109.384367)
			)
		)
	)
	(zone
		(net 48)
		(net_name "/BYTE")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30042)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 148.159102 105.200523) (xy 148.214622 105.262701) (xy 148.251795 105.318194) (xy 148.290287 105.41942)
				(xy 148.300238 105.466178) (xy 148.328594 105.576773) (xy 148.356519 105.641823) (xy 148.400559 105.716671)
				(xy 148.650707 105.550707) (xy 148.816671 105.300559) (xy 148.744819 105.258042) (xy 148.682038 105.230491)
				(xy 148.566178 105.200238) (xy 148.505397 105.186736) (xy 148.443746 105.164797) (xy 148.376897 105.125294)
				(xy 148.300523 105.059102)
			)
		)
	)
	(zone
		(net 63)
		(net_name "/A0")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30119)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 143.249 96.075) (xy 143.213185 96.077179) (xy 143.118197 96.077612) (xy 143.077507 96.063237)
				(xy 143.052701 96.030709) (xy 142.698 96.175) (xy 143.052701 96.319291) (xy 143.08249 96.283776)
				(xy 143.141061 96.270071) (xy 143.213185 96.272822) (xy 143.249 96.275)
			)
		)
	)
	(zone
		(net 3)
		(net_name "VBUS")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30025)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 150.928404 103.791747) (xy 151.044924 103.850784) (xy 151.109288 103.900453) (xy 151.171456 103.961265)
				(xy 151.22883 104.031755) (xy 151.27967 104.111375) (xy 151.319113 104.192644) (xy 151.349309 104.280239)
				(xy 151.367281 104.364812) (xy 151.374844 104.453449) (xy 151.375 104.468189) (xy 151.77589 104.275454)
				(xy 151.630492 103.65) (xy 151.558508 103.666647) (xy 151.442894 103.653797) (xy 151.264708 103.599352)
				(xy 151.16903 103.56311) (xy 151.06461 103.52445)
			)
		)
	)
	(zone
		(net 42)
		(net_name "+BATT")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30000)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 165.55 88.025) (xy 165.73273 88.045492) (xy 165.843943 88.073463) (xy 165.959109 88.113852)
				(xy 166.06268 88.161435) (xy 166.162034 88.219853) (xy 166.241233 88.278856) (xy 166.312487 88.346274)
				(xy 166.366069 88.411643) (xy 166.410559 88.483612) (xy 166.441497 88.553783) (xy 166.462932 88.629451)
				(xy 166.475 88.748724) (xy 170.226 88.2) (xy 166.70625 87.275) (xy 166.65534 87.332629) (xy 166.559547 87.380585)
				(xy 166.3989 87.417065) (xy 166.149188 87.435815) (xy 165.739077 87.429876) (xy 165.55 87.425)
			)
		)
	)
	(zone
		(net 62)
		(net_name "/BLOCK")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30046)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 151.425 107.4) (xy 151.491579 107.390878) (xy 151.604554 107.378745) (xy 151.653453 107.390592)
				(xy 151.6875 107.425) (xy 152.201 107.25) (xy 151.6875 107.075) (xy 151.649436 107.111332) (xy 151.585856 107.121559)
				(xy 151.491579 107.109122) (xy 151.425 107.1)
			)
		)
	)
	(zone
		(net 23)
		(net_name "/(A)")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30011)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 164.74323 115.299431) (xy 164.837007 115.35273) (xy 164.911669 115.406919) (xy 164.964966 115.457649)
				(xy 165.005553 115.509847) (xy 165.054387 115.618273) (xy 165.072516 115.749606) (xy 165.065847 115.940207)
				(xy 165.057204 116.177813) (xy 165.064538 116.313091) (xy 165.086333 116.460827) (xy 165.92089 116.295454)
				(xy 166.085827 115.461333) (xy 165.655789 115.389399) (xy 165.469778 115.360354) (xy 165.2963 115.319024)
				(xy 165.097126 115.24584) (xy 164.834032 115.121233)
			)
		)
	)
	(zone
		(net 30)
		(net_name "/~{CE}")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30120)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 136.749 95.575) (xy 136.713185 95.577179) (xy 136.618197 95.577612) (xy 136.577507 95.563237)
				(xy 136.552701 95.530709) (xy 136.198 95.675) (xy 136.552701 95.819291) (xy 136.58249 95.783776)
				(xy 136.641061 95.770071) (xy 136.713185 95.772822) (xy 136.749 95.775)
			)
		)
	)
	(zone
		(net 13)
		(net_name "/A9")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30067)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 150.475 101.475) (xy 150.449647 101.475501) (xy 150.331363 101.469476) (xy 150.278301 101.448834)
				(xy 150.245985 101.406661) (xy 149.699 101.575) (xy 150.245985 101.743339) (xy 150.278029 101.701351)
				(xy 150.340788 101.678755) (xy 150.449648 101.674499) (xy 150.475 101.675)
			)
		)
	)
	(zone
		(net 41)
		(net_name "/A7")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30068)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 150.475 100.825) (xy 150.449647 100.825501) (xy 150.331363 100.819476) (xy 150.278301 100.798834)
				(xy 150.245985 100.756661) (xy 149.699 100.925) (xy 150.245985 101.093339) (xy 150.278029 101.051351)
				(xy 150.340788 101.028755) (xy 150.449648 101.024499) (xy 150.475 101.025)
			)
		)
	)
	(zone
		(net 1)
		(net_name "GND")
		(layers "F.Cu" "B.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0.2)
		)
		(min_thickness 0.2)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.2)
			(thermal_bridge_width 0.2)
			(smoothing fillet)
			(radius 0.1)
		)
		(polygon
			(pts
				(xy 181.95 120.025) (xy 181.95 86.025) (xy 121.95 86.025) (xy 121.95 120.025)
			)
		)
	)
	(zone
		(net 46)
		(net_name "/A17")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30013)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 154.114073 92.775) (xy 154.172288 92.779784) (xy 154.215897 92.793274) (xy 154.271233 92.837666)
				(xy 154.305749 92.888839) (xy 154.354855 92.960002) (xy 154.436107 93.032867) (xy 154.576 92.825)
				(xy 154.623773 92.579804) (xy 154.503166 92.560618) (xy 154.415847 92.556494) (xy 154.319683 92.56359)
				(xy 154.114073 92.575)
			)
		)
	)
	(zone
		(net 62)
		(net_name "/BLOCK")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30007)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 147.354804 91.475) (xy 147.434336 91.479668) (xy 147.494931 91.492342) (xy 147.597187 91.540561)
				(xy 147.678815 91.583285) (xy 147.801227 91.620196) (xy 147.851 91.375) (xy 147.801227 91.129804)
				(xy 147.664585 91.173094) (xy 147.597186 91.209439) (xy 147.50229 91.255353) (xy 147.439128 91.269681)
				(xy 147.354804 91.275)
			)
		)
	)
	(zone
		(net 62)
		(net_name "/BLOCK")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30004)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 150.8 100.219236) (xy 150.804708 100.136011) (xy 150.817662 100.070485) (xy 150.862022 99.971689)
				(xy 150.888048 99.93159) (xy 150.9462 99.833336) (xy 150.972452 99.767593) (xy 150.994236 99.683527)
				(xy 150.7 99.624) (xy 150.405764 99.683527) (xy 150.426507 99.764398) (xy 150.451418 99.828272)
				(xy 150.511952 99.93159) (xy 150.545383 99.984116) (xy 150.573464 100.043223) (xy 150.5928 100.118425)
				(xy 150.6 100.219236)
			)
		)
	)
	(zone
		(net 31)
		(net_name "/A18_CE2")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30006)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 146.15 100.779804) (xy 146.145332 100.859336) (xy 146.132658 100.919931) (xy 146.084439 101.022186)
				(xy 146.041714 101.103815) (xy 146.004804 101.226227) (xy 146.25 101.276) (xy 146.495196 101.226227)
				(xy 146.451905 101.089584) (xy 146.415561 101.022187) (xy 146.369647 100.927291) (xy 146.355319 100.864128)
				(xy 146.35 100.779804)
			)
		)
	)
	(zone
		(net 3)
		(net_name "VBUS")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30001)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 128.12 115.455) (xy 128.12532 115.338697) (xy 128.142559 115.20092) (xy 128.170709 115.063012)
				(xy 128.212159 114.922574) (xy 128.255882 114.813548) (xy 128.309844 114.71161) (xy 128.361832 114.636586)
				(xy 128.421522 114.570897) (xy 128.478557 114.524005) (xy 128.541698 114.48662) (xy 128.65097 114.450671)
				(xy 127.82 113.754) (xy 126.98903 114.450671) (xy 127.109597 114.492312) (xy 127.21719 114.569681)
				(xy 127.314092 114.686351) (xy 127.399129 114.847714) (xy 127.467464 115.055659) (xy 127.510591 115.296836)
				(xy 127.52 115.455)
			)
		)
	)
	(zone
		(net 3)
		(net_name "VBUS")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30000)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 127.52 114.611333) (xy 127.515176 114.760689) (xy 127.501404 114.889765) (xy 127.480163 114.999884)
				(xy 127.452292 115.096304) (xy 127.37535 115.269577) (xy 127.278362 115.428743) (xy 127.198167 115.557405)
				(xy 127.119334 115.706999) (xy 127.047008 115.892573) (xy 126.986333 116.129173) (xy 127.82 116.296)
				(xy 128.653667 116.129173) (xy 128.619968 115.984033) (xy 128.581572 115.858406) (xy 128.489125 115.642722)
				(xy 128.361638 115.428744) (xy 128.26977 115.27886) (xy 128.192719 115.110666) (xy 128.162636 115.011264)
				(xy 128.139718 114.897158) (xy 128.125122 114.764973) (xy 128.12 114.611333)
			)
		)
	)
	(zone
		(net 48)
		(net_name "/BYTE")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30009)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 148.75 99.470196) (xy 148.754668 99.390664) (xy 148.767342 99.330069) (xy 148.815561 99.227813)
				(xy 148.858285 99.146184) (xy 148.895196 99.023773) (xy 148.65 98.974) (xy 148.404804 99.023773)
				(xy 148.448094 99.160415) (xy 148.484439 99.227813) (xy 148.530353 99.322709) (xy 148.544681 99.385872)
				(xy 148.55 99.470196)
			)
		)
	)
	(zone
		(net 62)
		(net_name "/BLOCK")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30002)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 150.6 106.480764) (xy 150.595292 106.563989) (xy 150.582338 106.629514) (xy 150.537978 106.72831)
				(xy 150.511952 106.768409) (xy 150.4538 106.866663) (xy 150.427548 106.932406) (xy 150.405764 107.016473)
				(xy 150.7 107.076) (xy 150.994236 107.016473) (xy 150.973493 106.935601) (xy 150.948581 106.871727)
				(xy 150.888048 106.768409) (xy 150.854617 106.715883) (xy 150.826536 106.656776) (xy 150.8072 106.581574)
				(xy 150.8 106.480764)
			)
		)
	)
	(zone
		(net 48)
		(net_name "/BYTE")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30003)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 148.55 104.955764) (xy 148.545292 105.038989) (xy 148.532338 105.104514) (xy 148.487978 105.20331)
				(xy 148.461952 105.243409) (xy 148.4038 105.341663) (xy 148.377548 105.407406) (xy 148.355764 105.491473)
				(xy 148.65 105.551) (xy 148.944236 105.491473) (xy 148.923493 105.410601) (xy 148.898581 105.346727)
				(xy 148.838048 105.243409) (xy 148.804617 105.190883) (xy 148.776536 105.131776) (xy 148.7572 105.056574)
				(xy 148.75 104.955764)
			)
		)
	)
	(zone
		(net 62)
		(net_name "/BLOCK")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30010)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 134.345196 91.275) (xy 134.265664 91.270332) (xy 134.205069 91.257658) (xy 134.102813 91.209439)
				(xy 134.021184 91.166714) (xy 133.898773 91.129804) (xy 133.849 91.375) (xy 133.898773 91.620196)
				(xy 134.035415 91.576905) (xy 134.102813 91.540561) (xy 134.197709 91.494647) (xy 134.260872 91.480319)
				(xy 134.345196 91.475)
			)
		)
	)
	(zone
		(net 46)
		(net_name "/A17")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30011)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 133.045196 92.575) (xy 132.965664 92.570332) (xy 132.905069 92.557658) (xy 132.802813 92.509439)
				(xy 132.721184 92.466714) (xy 132.598773 92.429804) (xy 132.549 92.675) (xy 132.598773 92.920196)
				(xy 132.735415 92.876905) (xy 132.802813 92.840561) (xy 132.897709 92.794647) (xy 132.960872 92.780319)
				(xy 133.045196 92.775)
			)
		)
	)
	(zone
		(net 31)
		(net_name "/A18_CE2")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30008)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 154.354804 97.525) (xy 154.434336 97.529668) (xy 154.494931 97.542342) (xy 154.597187 97.590561)
				(xy 154.678815 97.633285) (xy 154.801227 97.670196) (xy 154.851 97.425) (xy 154.801227 97.179804)
				(xy 154.664585 97.223094) (xy 154.597186 97.259439) (xy 154.50229 97.305353) (xy 154.439128 97.319681)
				(xy 154.354804 97.325)
			)
		)
	)
	(zone
		(net 31)
		(net_name "/A18_CE2")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30012)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 146.35 101.770196) (xy 146.354668 101.690664) (xy 146.367342 101.630069) (xy 146.415561 101.527813)
				(xy 146.458285 101.446184) (xy 146.495196 101.323773) (xy 146.25 101.274) (xy 146.004804 101.323773)
				(xy 146.048094 101.460415) (xy 146.084439 101.527813) (xy 146.130353 101.622709) (xy 146.144681 101.685872)
				(xy 146.15 101.770196)
			)
		)
	)
	(zone
		(net 31)
		(net_name "/A18_CE2")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30005)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 146.15 109.029804) (xy 146.145311 109.102095) (xy 146.132485 109.158211) (xy 146.088655 109.242551)
				(xy 146.070348 109.267832) (xy 146.017298 109.34969) (xy 145.993784 109.404973) (xy 145.974804 109.476227)
				(xy 146.22 109.526) (xy 146.465196 109.476227) (xy 146.419441 109.321106) (xy 146.401747 109.279933)
				(xy 146.365225 109.180603) (xy 146.354092 109.115924) (xy 146.35 109.029804)
			)
		)
	)
	(embedded_fonts yes)
	(embedded_files
		(file
			(name "ProggyVector.ttf")
			(type font)
		)
	)
)
