(kicad_pcb
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(general
		(thickness 1.5424)
		(legacy_teardrops no)
	)
	(paper "A4")
	(layers
		(0 "F.Cu" signal)
		(1 "In1.Cu" power)
		(2 "In2.Cu" power)
		(31 "B.Cu" signal)
		(32 "B.Adhes" user "B.Adhesive")
		(33 "F.Adhes" user "F.Adhesive")
		(34 "B.Paste" user)
		(35 "F.Paste" user)
		(36 "B.SilkS" user "B.Silkscreen")
		(37 "F.SilkS" user "F.Silkscreen")
		(38 "B.Mask" user)
		(39 "F.Mask" user)
		(40 "Dwgs.User" user "User.Drawings")
		(41 "Cmts.User" user "User.Comments")
		(42 "Eco1.User" user "User.Eco1")
		(43 "Eco2.User" user "User.Eco2")
		(44 "Edge.Cuts" user)
		(45 "Margin" user)
		(46 "B.CrtYd" user "B.Courtyard")
		(47 "F.CrtYd" user "F.Courtyard")
		(48 "B.Fab" user)
		(49 "F.Fab" user)
		(50 "User.1" user)
		(51 "User.2" user)
		(52 "User.3" user)
		(53 "User.4" user)
		(54 "User.5" user)
		(55 "User.6" user)
		(56 "User.7" user)
		(57 "User.8" user)
		(58 "User.9" user)
	)
	(setup
		(stackup
			(layer "F.SilkS"
				(type "Top Silk Screen")
			)
			(layer "F.Paste"
				(type "Top Solder Paste")
			)
			(layer "F.Mask"
				(type "Top Solder Mask")
				(thickness 0.0152)
			)
			(layer "F.Cu"
				(type "copper")
				(thickness 0.0432)
			)
			(layer "dielectric 1"
				(type "prepreg")
				(color "FR4 natural")
				(thickness 0.2)
				(material "FR408-HR")
				(epsilon_r 3.69)
				(loss_tangent 0.0091)
			)
			(layer "In1.Cu"
				(type "copper")
				(thickness 0.0175)
			)
			(layer "dielectric 2"
				(type "core")
				(color "FR4 natural")
				(thickness 0.9906)
				(material "FR408-HR")
				(epsilon_r 3.69)
				(loss_tangent 0.0091)
			)
			(layer "In2.Cu"
				(type "copper")
				(thickness 0.0175)
			)
			(layer "dielectric 3"
				(type "prepreg")
				(color "FR4 natural")
				(thickness 0.2)
				(material "FR408-HR")
				(epsilon_r 3.69)
				(loss_tangent 0.0091)
			)
			(layer "B.Cu"
				(type "copper")
				(thickness 0.0432)
			)
			(layer "B.Mask"
				(type "Bottom Solder Mask")
				(thickness 0.0152)
			)
			(layer "B.Paste"
				(type "Bottom Solder Paste")
			)
			(layer "B.SilkS"
				(type "Bottom Silk Screen")
			)
			(copper_finish "None")
			(dielectric_constraints yes)
		)
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(pcbplotparams
			(layerselection 0x00010fc_ffffffff)
			(plot_on_all_layers_selection 0x0000000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 4)
			(plotframeref no)
			(viasonmask no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plotreference yes)
			(plotvalue yes)
			(plotfptext yes)
			(plotinvisibletext no)
			(sketchpadsonfab no)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 1)
			(scaleselection 1)
			(outputdirectory "")
		)
	)
	(net 0 "")
	(net 1 "Net-(U1-VBAT)")
	(net 2 "GND")
	(net 3 "Net-(C10-Pad2)")
	(net 4 "Net-(U2-NR{slash}FB)")
	(net 5 "Net-(J1-~{RESET})")
	(net 6 "Net-(U1-OSC0)")
	(net 7 "Net-(Y1-OUT{slash}IN)")
	(net 8 "Net-(U1-PC3_TDO_SWO)")
	(net 9 "Net-(U1-PC2_TDI)")
	(net 10 "Net-(J1-NC{slash}TDI)")
	(net 11 "Net-(J1-SWDIO{slash}TMS)")
	(net 12 "Net-(J1-SWO{slash}TDO)")
	(net 13 "Net-(J1-VTref)")
	(net 14 "unconnected-(J1-KEY-Pad7)")
	(net 15 "Net-(J1-SWCLK{slash}TCK)")
	(net 16 "Net-(U1-PB0_USB0VID)")
	(net 17 "Net-(C7-Pad2)")
	(net 18 "Net-(U2-EN)")
	(net 19 "Net-(U1-WAKE_N)")
	(net 20 "Net-D+")
	(net 21 "Net-(U1-OSC1)")
	(net 22 "Net-(U1-PC0_TCK_SWCLK)")
	(net 23 "Net-(U1-PC1_TMS_SWDIO)")
	(net 24 "unconnected-(U1-PD0-Pad61)")
	(net 25 "unconnected-(U1-PE4-Pad59)")
	(net 26 "unconnected-(U1-PF1-Pad29)")
	(net 27 "unconnected-(U1-PA4_SSI0Rx-Pad21)")
	(net 28 "unconnected-(U1-PD2-Pad63)")
	(net 29 "unconnected-(U1-PA0_U0Rx-Pad17)")
	(net 30 "unconnected-(U1-PB5-Pad57)")
	(net 31 "unconnected-(U1-HIB_N-Pad33)")
	(net 32 "unconnected-(U1-PB1_USB0VBUS-Pad46)")
	(net 33 "unconnected-(U1-PA5_SSI0Tx-Pad22)")
	(net 34 "unconnected-(U1-PC7-Pad13)")
	(net 35 "unconnected-(U1-PA7-Pad24)")
	(net 36 "unconnected-(U1-PE0-Pad9)")
	(net 37 "unconnected-(U1-PC4-Pad16)")
	(net 38 "unconnected-(U1-PE3-Pad6)")
	(net 39 "unconnected-(U1-PB2_I2C0SCL-Pad47)")
	(net 40 "unconnected-(U1-PD6-Pad53)")
	(net 41 "unconnected-(U1-PF2-Pad30)")
	(net 42 "unconnected-(U1-PB7-Pad4)")
	(net 43 "unconnected-(U1-PF3-Pad31)")
	(net 44 "unconnected-(U1-PE5-Pad60)")
	(net 45 "unconnected-(U1-PA6-Pad23)")
	(net 46 "unconnected-(U1-PA3_SSI0Fss-Pad20)")
	(net 47 "unconnected-(U1-PD1-Pad62)")
	(net 48 "unconnected-(U1-PB3_I2C0SDA-Pad48)")
	(net 49 "unconnected-(U1-PC6-Pad14)")
	(net 50 "unconnected-(U1-PD7-Pad10)")
	(net 51 "unconnected-(U1-PA2_SSI0Clk-Pad19)")
	(net 52 "unconnected-(U1-PF4-Pad5)")
	(net 53 "unconnected-(U1-PB4-Pad58)")
	(net 54 "unconnected-(U1-PA1_U0Tx-Pad18)")
	(net 55 "unconnected-(U1-PE1-Pad8)")
	(net 56 "unconnected-(U1-PF0-Pad28)")
	(net 57 "unconnected-(U1-PE2-Pad7)")
	(net 58 "unconnected-(U1-PC5-Pad15)")
	(net 59 "unconnected-(U1-PB6-Pad1)")
	(net 60 "Net-(U1-XOSC1)")
	(net 61 "Net-(U1-XOSC0)")
	(net 62 "Net-(D2-A)")
	(net 63 "Net-(D1-A)")
	(net 64 "Net-(U1-PD3)")
	(net 65 "Net-D-")
	(net 66 "Net-(J3-Pad4)")
	(footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder"
		(layer "F.Cu")
		(at 130.55 81.85 90)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C13"
			(at 0.25 1.6 90)
			(layer "F.SilkS")
		)
		(property "Value" "12pF"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "test jtag board.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.8625 0 90)
			(size 1.075 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 6 "Net-(U1-OSC0)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.8625 0 90)
			(size 1.075 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "hibernation oscillator:XTAL_ECS-.327-12.5-13FLX"
		(layer "F.Cu")
		(at 122.4721 91.9 180)
		(property "Reference" "Y2"
			(at -2.6279 2.1 0)
			(layer "F.SilkS")
		)
		(property "Value" "ECS-.327-12.5-13FLX"
			(at 2.998394 2.638619 360)
			(layer "F.Fab")
		)
		(property "Footprint" "hibernation oscillator:XTAL_ECS-.327-12.5-13FLX"
			(at 0 0 360)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 360)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 360)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTREV" "2016"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER" "ECS Inc."
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "STANDARD" "Manufacturer Recommendations"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "test jtag board.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at 2 1.25 180)
			(size 2.5 1)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 61 "Net-(U1-XOSC0)")
			(pinfunction "IN/OUT")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd rect
			(at 2 -1.25 180)
			(size 2.5 1)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 60 "Net-(U1-XOSC1)")
			(pinfunction "OUT/IN")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "3" smd rect
			(at -3.75 0 180)
			(size 6 2.5)
			(layers "F.Cu" "F.Mask")
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(solder_mask_margin 0.102)
		)
		(model "C:/Users/christopher.oelkers/Documents/KiCad Symbols/ECS__327_12_5_13FLX_TR/ECS-.327-12.5-13FLX.step"
			(offset
				(xyz 0 0 -0.1)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 90 -90)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder"
		(layer "F.Cu")
		(at 122.35 66.45 180)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R7"
			(at 0 -1.43 0)
			(layer "F.SilkS")
		)
		(property "Value" "10k"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "test jtag board.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 180)
			(size 0.975 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "Net-(U1-VBAT)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 180)
			(size 0.975 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 23 "Net-(U1-PC1_TMS_SWDIO)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder"
		(layer "F.Cu")
		(at 112.25 62.25 180)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R11"
			(at 0.4 -1.45 0)
			(layer "F.SilkS")
		)
		(property "Value" "10k"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "test jtag board.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 180)
			(size 0.975 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 8 "Net-(U1-PC3_TDO_SWO)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 180)
			(size 0.975 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder"
		(layer "F.Cu")
		(at 125.4 88.35 180)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R1"
			(at -0.25 1.35 0)
			(layer "F.SilkS")
		)
		(property "Value" "10k"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "test jtag board.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 180)
			(size 0.975 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "Net-(U1-VBAT)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 180)
			(size 0.975 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 5 "Net-(J1-~{RESET})")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "LED_THT:LED_D3.0mm"
		(layer "F.Cu")
		(at 102.3 65.375 -90)
		(descr "LED, diameter 3.0mm, 2 pins")
		(tags "LED diameter 3.0mm 2 pins")
		(property "Reference" "D2"
			(at 1.27 -2.96 90)
			(layer "F.SilkS")
		)
		(property "Value" "LED"
			(at 1.27 2.96 90)
			(layer "F.Fab")
		)
		(property "Footprint" "LED_THT:LED_D3.0mm"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Light emitting diode"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "LED* LED_SMD:* LED_THT:*")
		(sheetname "Root")
		(sheetfile "test jtag board.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole rect
			(at 0 0 270)
			(size 1.8 1.8)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 2.54 0 270)
			(size 1.8 1.8)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 62 "Net-(D2-A)")
			(pinfunction "A")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/LED_THT.3dshapes/LED_D3.0mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder"
		(layer "F.Cu")
		(at 102.4 83.15 90)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C1"
			(at -0.9 -1.43 90)
			(layer "F.SilkS")
		)
		(property "Value" "0.1uF"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "test jtag board.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.8625 0 90)
			(size 1.075 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.8625 0 90)
			(size 1.075 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "Net-(U1-VBAT)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder"
		(layer "F.Cu")
		(at 101.65 78.35)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C5"
			(at 0 -1.43 0)
			(layer "F.SilkS")
		)
		(property "Value" "0.1uF"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "test jtag board.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.8625 0)
			(size 1.075 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.8625 0)
			(size 1.075 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "Net-(U1-VBAT)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "16mhz oscillator:XTAL_ECS-160-9-42-CKM-TR"
		(layer "F.Cu")
		(at 127.9 81.65 90)
		(property "Reference" "Y1"
			(at 1.55 -2.25 90)
			(layer "F.SilkS")
		)
		(property "Value" "ECS-160-9-42-CKM-TR"
			(at 4.82721 2.20067 90)
			(layer "F.Fab")
		)
		(property "Footprint" "16mhz oscillator:XTAL_ECS-160-9-42-CKM-TR"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTREV" "11/11"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER" "ECS Inc."
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "STANDARD" "MAnufacturer Recommendations"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "test jtag board.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -1.5 0.8 90)
			(size 1.4 1.15)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 6 "Net-(U1-OSC0)")
			(pinfunction "IN/OUT")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd rect
			(at 1.5 0.8 90)
			(size 1.4 1.15)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(solder_mask_margin 0.102)
		)
		(pad "3" smd rect
			(at 1.5 -0.8 90)
			(size 1.4 1.15)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 7 "Net-(Y1-OUT{slash}IN)")
			(pinfunction "OUT/IN")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "4" smd rect
			(at -1.5 -0.8 90)
			(size 1.4 1.15)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pinfunction "GND__1")
			(pintype "power_in")
			(solder_mask_margin 0.102)
		)
		(model "C:/Users/christopher.oelkers/Documents/KiCad Symbols/ECS_160_9_42_CKM_TR/ECS-160-9-42-CKM-TR.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder"
		(layer "F.Cu")
		(at 117.1 93.3 180)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C16"
			(at 3.15 -0.3 360)
			(layer "F.SilkS")
		)
		(property "Value" "20pF"
			(at 0 1.43 360)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "test jtag board.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0.05 1.5 360)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.8625 0 180)
			(size 1.075 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 60 "Net-(U1-XOSC1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.8625 0 180)
			(size 1.075 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder"
		(layer "F.Cu")
		(at 124.2 63.65 180)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R9"
			(at 0.1 1.4 0)
			(layer "F.SilkS")
		)
		(property "Value" "100"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "test jtag board.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 180)
			(size 0.975 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "Net-(U1-VBAT)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 180)
			(size 0.975 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 13 "Net-(J1-VTref)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder"
		(layer "F.Cu")
		(at 115.65 67.55 180)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R5"
			(at 0.45 -1.5 0)
			(layer "F.SilkS")
		)
		(property "Value" "10k"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "test jtag board.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 180)
			(size 0.975 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "Net-(U1-VBAT)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 180)
			(size 0.975 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 22 "Net-(U1-PC0_TCK_SWCLK)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_PinHeader_1.27mm:PinHeader_2x05_P1.27mm_Vertical"
		(layer "F.Cu")
		(at 120.8 64.29 180)
		(descr "Through hole straight pin header, 2x05, 1.27mm pitch, double rows")
		(tags "Through hole pin header THT 2x05 1.27mm double row")
		(property "Reference" "J1"
			(at -0.5 6.99 0)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_ARM_JTAG_SWD_10"
			(at 0.635 6.775 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Connector_PinHeader_1.27mm:PinHeader_2x05_P1.27mm_Vertical"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "http://infocenter.arm.com/help/topic/com.arm.doc.ddi0314h/DDI0314H_coresight_components_trm.pdf"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Cortex Debug Connector, standard ARM Cortex-M SWD and JTAG interface"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "PinHeader?2x05?P1.27mm*")
		(sheetname "Root")
		(sheetfile "test jtag board.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0.635 2.54 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 180)
			(size 1 1)
			(drill 0.65)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 13 "Net-(J1-VTref)")
			(pinfunction "VTref")
			(pintype "power_in")
		)
		(pad "2" thru_hole oval
			(at 1.27 0 180)
			(size 1 1)
			(drill 0.65)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 11 "Net-(J1-SWDIO{slash}TMS)")
			(pinfunction "SWDIO/TMS")
			(pintype "bidirectional")
		)
		(pad "3" thru_hole oval
			(at 0 1.27 180)
			(size 1 1)
			(drill 0.65)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "4" thru_hole oval
			(at 1.27 1.27 180)
			(size 1 1)
			(drill 0.65)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 15 "Net-(J1-SWCLK{slash}TCK)")
			(pinfunction "SWCLK/TCK")
			(pintype "output")
		)
		(pad "5" thru_hole oval
			(at 0 2.54 180)
			(size 1 1)
			(drill 0.65)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "6" thru_hole oval
			(at 1.27 2.54 180)
			(size 1 1)
			(drill 0.65)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 12 "Net-(J1-SWO{slash}TDO)")
			(pinfunction "SWO/TDO")
			(pintype "input")
		)
		(pad "7" thru_hole oval
			(at 0 3.81 180)
			(size 1 1)
			(drill 0.65)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 14 "unconnected-(J1-KEY-Pad7)")
			(pinfunction "KEY")
			(pintype "no_connect")
		)
		(pad "8" thru_hole oval
			(at 1.27 3.81 180)
			(size 1 1)
			(drill 0.65)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 10 "Net-(J1-NC{slash}TDI)")
			(pinfunction "NC/TDI")
			(pintype "output")
		)
		(pad "9" thru_hole oval
			(at 0 5.08 180)
			(size 1 1)
			(drill 0.65)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "GNDDetect")
			(pintype "passive")
		)
		(pad "10" thru_hole oval
			(at 1.27 5.08 180)
			(size 1 1)
			(drill 0.65)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "Net-(J1-~{RESET})")
			(pinfunction "~{RESET}")
			(pintype "open_collector")
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_PinHeader_1.27mm.3dshapes/PinHeader_2x05_P1.27mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "LED_THT:LED_D3.0mm"
		(layer "F.Cu")
		(at 136.5 78.275 90)
		(descr "LED, diameter 3.0mm, 2 pins")
		(tags "LED diameter 3.0mm 2 pins")
		(property "Reference" "D1"
			(at 1.27 -2.96 90)
			(layer "F.SilkS")
		)
		(property "Value" "LED"
			(at 1.27 2.96 90)
			(layer "F.Fab")
		)
		(property "Footprint" "LED_THT:LED_D3.0mm"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Light emitting diode"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "LED* LED_SMD:* LED_THT:*")
		(sheetname "Root")
		(sheetfile "test jtag board.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole rect
			(at 0 0 90)
			(size 1.8 1.8)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 2.54 0 90)
			(size 1.8 1.8)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 63 "Net-(D1-A)")
			(pinfunction "A")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/LED_THT.3dshapes/LED_D3.0mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder"
		(layer "F.Cu")
		(at 121.4 87.9)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C15"
			(at -1.15 1.4 360)
			(layer "F.SilkS")
		)
		(property "Value" "20pF"
			(at 0 1.43 360)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "test jtag board.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 360)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.8625 0)
			(size 1.075 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 61 "Net-(U1-XOSC0)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.8625 0)
			(size 1.075 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder"
		(layer "F.Cu")
		(at 115.85 58.5)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R6"
			(at 0 -1.43 0)
			(layer "F.SilkS")
		)
		(property "Value" "10k"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "test jtag board.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0)
			(size 0.975 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "Net-(U1-VBAT)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0)
			(size 0.975 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 5 "Net-(J1-~{RESET})")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder"
		(layer "F.Cu")
		(at 127.5 75.15)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C11"
			(at -1.65 -1.43 0)
			(layer "F.SilkS")
		)
		(property "Value" "10nF"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "test jtag board.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.8625 0)
			(size 1.075 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 4 "Net-(U2-NR{slash}FB)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.8625 0)
			(size 1.075 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder"
		(layer "F.Cu")
		(at 136.45 71.95 90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R14"
			(at 0.1 1.4 90)
			(layer "F.SilkS")
		)
		(property "Value" "470"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "test jtag board.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 90)
			(size 0.975 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 63 "Net-(D1-A)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 90)
			(size 0.975 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "Net-(U1-VBAT)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder"
		(layer "F.Cu")
		(at 101.6875 80.1)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C6"
			(at -1.1875 1.45 0)
			(layer "F.SilkS")
		)
		(property "Value" "1uF"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "test jtag board.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.8625 0)
			(size 1.075 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.8625 0)
			(size 1.075 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "Net-(U1-VBAT)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder"
		(layer "F.Cu")
		(at 126.0875 77.85)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C14"
			(at -1.5875 -1.5 0)
			(layer "F.SilkS")
		)
		(property "Value" "12pF"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "test jtag board.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.8625 0)
			(size 1.075 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 7 "Net-(Y1-OUT{slash}IN)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.8625 0)
			(size 1.075 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder"
		(layer "F.Cu")
		(at 122.15 85.55)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C12"
			(at -3.05 0.5 0)
			(layer "F.SilkS")
		)
		(property "Value" "10nF"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "test jtag board.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.8625 0)
			(size 1.075 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 5 "Net-(J1-~{RESET})")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.8625 0)
			(size 1.075 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder"
		(layer "F.Cu")
		(at 129 86.15 90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R3"
			(at 0.15 -1.35 90)
			(layer "F.SilkS")
		)
		(property "Value" "470"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "test jtag board.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 90)
			(size 0.975 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 5 "Net-(J1-~{RESET})")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 90)
			(size 0.975 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 66 "Net-(J3-Pad4)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder"
		(layer "F.Cu")
		(at 108.9 90.05)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C7"
			(at 0.5 1.45 0)
			(layer "F.SilkS")
		)
		(property "Value" "0.1uF"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "test jtag board.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.8625 0)
			(size 1.075 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.8625 0)
			(size 1.075 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 17 "Net-(C7-Pad2)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "tm4c123gh6pm:PM0064A_N"
		(layer "F.Cu")
		(at 110.8 81.65)
		(tags "TM4C123GH6PMT ")
		(property "Reference" "U1"
			(at -5.55 -5.85 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "TM4C123GH6PMT"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" "tm4c123gh6pm:PM0064A_N"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.ti.com/lit/gpn/tm4c123gh6pm"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "PM0064A_N PM0064A_M PM0064A_L")
		(sheetname "Root")
		(sheetfile "test jtag board.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd oval
			(at -5.549999 -3.750003 90)
			(size 0.299999 1.799999)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 59 "unconnected-(U1-PB6-Pad1)")
			(pinfunction "PB6")
			(pintype "bidirectional")
		)
		(pad "2" smd oval
			(at -5.549999 -3.250001 90)
			(size 0.299999 1.799999)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "Net-(U1-VBAT)")
			(pinfunction "VDDA")
			(pintype "power_in")
		)
		(pad "3" smd oval
			(at -5.549999 -2.750002 90)
			(size 0.299999 1.799999)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pinfunction "GNDA")
			(pintype "power_in")
		)
		(pad "4" smd oval
			(at -5.549999 -2.250001 90)
			(size 0.299999 1.799999)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 42 "unconnected-(U1-PB7-Pad4)")
			(pinfunction "PB7")
			(pintype "bidirectional")
		)
		(pad "5" smd oval
			(at -5.549999 -1.750002 90)
			(size 0.299999 1.799999)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 52 "unconnected-(U1-PF4-Pad5)")
			(pinfunction "PF4")
			(pintype "bidirectional")
		)
		(pad "6" smd oval
			(at -5.549999 -1.250003 90)
			(size 0.299999 1.799999)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 38 "unconnected-(U1-PE3-Pad6)")
			(pinfunction "PE3")
			(pintype "bidirectional")
		)
		(pad "7" smd oval
			(at -5.549999 -0.750001 90)
			(size 0.299999 1.799999)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 57 "unconnected-(U1-PE2-Pad7)")
			(pinfunction "PE2")
			(pintype "bidirectional")
		)
		(pad "8" smd oval
			(at -5.549999 -0.250002 90)
			(size 0.299999 1.799999)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 55 "unconnected-(U1-PE1-Pad8)")
			(pinfunction "PE1")
			(pintype "bidirectional")
		)
		(pad "9" smd oval
			(at -5.549999 0.25 90)
			(size 0.299999 1.799999)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 36 "unconnected-(U1-PE0-Pad9)")
			(pinfunction "PE0")
			(pintype "bidirectional")
		)
		(pad "10" smd oval
			(at -5.549999 0.749998 90)
			(size 0.299999 1.799999)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 50 "unconnected-(U1-PD7-Pad10)")
			(pinfunction "PD7")
			(pintype "bidirectional")
		)
		(pad "11" smd oval
			(at -5.549999 1.249997 90)
			(size 0.299999 1.799999)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "Net-(U1-VBAT)")
			(pinfunction "VDD")
			(pintype "power_in")
		)
		(pad "12" smd oval
			(at -5.549999 1.749999 90)
			(size 0.299999 1.799999)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "13" smd oval
			(at -5.549999 2.249998 90)
			(size 0.299999 1.799999)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 34 "unconnected-(U1-PC7-Pad13)")
			(pinfunction "PC7")
			(pintype "bidirectional")
		)
		(pad "14" smd oval
			(at -5.549999 2.75 90)
			(size 0.299999 1.799999)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 49 "unconnected-(U1-PC6-Pad14)")
			(pinfunction "PC6")
			(pintype "bidirectional")
		)
		(pad "15" smd oval
			(at -5.549999 3.249999 90)
			(size 0.299999 1.799999)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 58 "unconnected-(U1-PC5-Pad15)")
			(pinfunction "PC5")
			(pintype "bidirectional")
		)
		(pad "16" smd oval
			(at -5.549999 3.749998 90)
			(size 0.299999 1.799999)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 37 "unconnected-(U1-PC4-Pad16)")
			(pinfunction "PC4")
			(pintype "bidirectional")
		)
		(pad "17" smd oval
			(at -3.75 5.549999)
			(size 0.299999 1.799999)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 29 "unconnected-(U1-PA0_U0Rx-Pad17)")
			(pinfunction "PA0_U0Rx")
			(pintype "bidirectional")
		)
		(pad "18" smd oval
			(at -3.249999 5.549999)
			(size 0.299999 1.799999)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 54 "unconnected-(U1-PA1_U0Tx-Pad18)")
			(pinfunction "PA1_U0Tx")
			(pintype "bidirectional")
		)
		(pad "19" smd oval
			(at -2.75 5.549999)
			(size 0.299999 1.799999)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 51 "unconnected-(U1-PA2_SSI0Clk-Pad19)")
			(pinfunction "PA2_SSI0Clk")
			(pintype "bidirectional")
		)
		(pad "20" smd oval
			(at -2.249998 5.549999)
			(size 0.299999 1.799999)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 46 "unconnected-(U1-PA3_SSI0Fss-Pad20)")
			(pinfunction "PA3_SSI0Fss")
			(pintype "bidirectional")
		)
		(pad "21" smd oval
			(at -1.749999 5.549999)
			(size 0.299999 1.799999)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 27 "unconnected-(U1-PA4_SSI0Rx-Pad21)")
			(pinfunction "PA4_SSI0Rx")
			(pintype "bidirectional")
		)
		(pad "22" smd oval
			(at -1.25 5.549999)
			(size 0.299999 1.799999)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 33 "unconnected-(U1-PA5_SSI0Tx-Pad22)")
			(pinfunction "PA5_SSI0Tx")
			(pintype "bidirectional")
		)
		(pad "23" smd oval
			(at -0.749998 5.549999)
			(size 0.299999 1.799999)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 45 "unconnected-(U1-PA6-Pad23)")
			(pinfunction "PA6")
			(pintype "bidirectional")
		)
		(pad "24" smd oval
			(at -0.25 5.549999)
			(size 0.299999 1.799999)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 35 "unconnected-(U1-PA7-Pad24)")
			(pinfunction "PA7")
			(pintype "bidirectional")
		)
		(pad "25" smd oval
			(at 0.250002 5.549999)
			(size 0.299999 1.799999)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 17 "Net-(C7-Pad2)")
			(pinfunction "VDDC")
			(pintype "power_in")
		)
		(pad "26" smd oval
			(at 0.750001 5.549999)
			(size 0.299999 1.799999)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "Net-(U1-VBAT)")
			(pinfunction "VDD")
			(pintype "power_in")
		)
		(pad "27" smd oval
			(at 1.25 5.549999)
			(size 0.299999 1.799999)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "28" smd oval
			(at 1.750002 5.549999)
			(size 0.299999 1.799999)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 56 "unconnected-(U1-PF0-Pad28)")
			(pinfunction "PF0")
			(pintype "bidirectional")
		)
		(pad "29" smd oval
			(at 2.250001 5.549999)
			(size 0.299999 1.799999)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 26 "unconnected-(U1-PF1-Pad29)")
			(pinfunction "PF1")
			(pintype "bidirectional")
		)
		(pad "30" smd oval
			(at 2.750002 5.549999)
			(size 0.299999 1.799999)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 41 "unconnected-(U1-PF2-Pad30)")
			(pinfunction "PF2")
			(pintype "bidirectional")
		)
		(pad "31" smd oval
			(at 3.250001 5.549999)
			(size 0.299999 1.799999)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 43 "unconnected-(U1-PF3-Pad31)")
			(pinfunction "PF3")
			(pintype "bidirectional")
		)
		(pad "32" smd oval
			(at 3.75 5.549999)
			(size 0.299999 1.799999)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 19 "Net-(U1-WAKE_N)")
			(pinfunction "WAKE_N")
			(pintype "input")
		)
		(pad "33" smd oval
			(at 5.550002 3.749998 90)
			(size 0.299999 1.799999)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 31 "unconnected-(U1-HIB_N-Pad33)")
			(pinfunction "HIB_N")
			(pintype "output")
		)
		(pad "34" smd oval
			(at 5.550002 3.249999 90)
			(size 0.299999 1.799999)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 61 "Net-(U1-XOSC0)")
			(pinfunction "XOSC0")
			(pintype "input")
		)
		(pad "35" smd oval
			(at 5.550002 2.75 90)
			(size 0.299999 1.799999)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pinfunction "GNDX")
			(pintype "power_in")
		)
		(pad "36" smd oval
			(at 5.550002 2.249998 90)
			(size 0.299999 1.799999)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 60 "Net-(U1-XOSC1)")
			(pinfunction "XOSC1")
			(pintype "output")
		)
		(pad "37" smd oval
			(at 5.550002 1.749999 90)
			(size 0.299999 1.799999)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "Net-(U1-VBAT)")
			(pinfunction "VBAT")
			(pintype "power_in")
		)
		(pad "38" smd oval
			(at 5.550002 1.249997 90)
			(size 0.299999 1.799999)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 5 "Net-(J1-~{RESET})")
			(pinfunction "RST_N")
			(pintype "input")
		)
		(pad "39" smd oval
			(at 5.550002 0.749998 90)
			(size 0.299999 1.799999)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "40" smd oval
			(at 5.550002 0.25 90)
			(size 0.299999 1.799999)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 6 "Net-(U1-OSC0)")
			(pinfunction "OSC0")
			(pintype "input")
		)
		(pad "41" smd oval
			(at 5.550002 -0.250002 90)
			(size 0.299999 1.799999)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 21 "Net-(U1-OSC1)")
			(pinfunction "OSC1")
			(pintype "output")
		)
		(pad "42" smd oval
			(at 5.550002 -0.750001 90)
			(size 0.299999 1.799999)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "Net-(U1-VBAT)")
			(pinfunction "VDD")
			(pintype "power_in")
		)
		(pad "43" smd oval
			(at 5.550002 -1.250003 90)
			(size 0.299999 1.799999)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 65 "Net-D-")
			(pinfunction "PD4")
			(pintype "bidirectional")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 0)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "44" smd oval
			(at 5.550002 -1.750002 90)
			(size 0.299999 1.799999)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 20 "Net-D+")
			(pinfunction "PD5")
			(pintype "bidirectional")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 0)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "45" smd oval
			(at 5.550002 -2.250001 90)
			(size 0.299999 1.799999)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 16 "Net-(U1-PB0_USB0VID)")
			(pinfunction "PB0_USB0VID")
			(pintype "bidirectional")
		)
		(pad "46" smd oval
			(at 5.550002 -2.750002 90)
			(size 0.299999 1.799999)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 32 "unconnected-(U1-PB1_USB0VBUS-Pad46)")
			(pinfunction "PB1_USB0VBUS")
			(pintype "bidirectional")
		)
		(pad "47" smd oval
			(at 5.550002 -3.250001 90)
			(size 0.299999 1.799999)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 39 "unconnected-(U1-PB2_I2C0SCL-Pad47)")
			(pinfunction "PB2_I2C0SCL")
			(pintype "bidirectional")
		)
		(pad "48" smd oval
			(at 5.550002 -3.750003 90)
			(size 0.299999 1.799999)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 48 "unconnected-(U1-PB3_I2C0SDA-Pad48)")
			(pinfunction "PB3_I2C0SDA")
			(pintype "bidirectional")
		)
		(pad "49" smd oval
			(at 3.75 -5.550002)
			(size 0.299999 1.799999)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 8 "Net-(U1-PC3_TDO_SWO)")
			(pinfunction "PC3_TDO_SWO")
			(pintype "bidirectional")
		)
		(pad "50" smd oval
			(at 3.250001 -5.550002)
			(size 0.299999 1.799999)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 9 "Net-(U1-PC2_TDI)")
			(pinfunction "PC2_TDI")
			(pintype "bidirectional")
		)
		(pad "51" smd oval
			(at 2.750002 -5.550002)
			(size 0.299999 1.799999)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 23 "Net-(U1-PC1_TMS_SWDIO)")
			(pinfunction "PC1_TMS_SWDIO")
			(pintype "bidirectional")
		)
		(pad "52" smd oval
			(at 2.250001 -5.550002)
			(size 0.299999 1.799999)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 22 "Net-(U1-PC0_TCK_SWCLK)")
			(pinfunction "PC0_TCK_SWCLK")
			(pintype "bidirectional")
		)
		(pad "53" smd oval
			(at 1.750002 -5.550002)
			(size 0.299999 1.799999)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 40 "unconnected-(U1-PD6-Pad53)")
			(pinfunction "PD6")
			(pintype "bidirectional")
		)
		(pad "54" smd oval
			(at 1.25 -5.550002)
			(size 0.299999 1.799999)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "Net-(U1-VBAT)")
			(pinfunction "VDD")
			(pintype "power_in")
		)
		(pad "55" smd oval
			(at 0.750001 -5.550002)
			(size 0.299999 1.799999)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "56" smd oval
			(at 0.250002 -5.550002)
			(size 0.299999 1.799999)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 3 "Net-(C10-Pad2)")
			(pinfunction "VDDC")
			(pintype "power_in")
		)
		(pad "57" smd oval
			(at -0.25 -5.550002)
			(size 0.299999 1.799999)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 30 "unconnected-(U1-PB5-Pad57)")
			(pinfunction "PB5")
			(pintype "bidirectional")
		)
		(pad "58" smd oval
			(at -0.749998 -5.550002)
			(size 0.299999 1.799999)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 53 "unconnected-(U1-PB4-Pad58)")
			(pinfunction "PB4")
			(pintype "bidirectional")
		)
		(pad "59" smd oval
			(at -1.25 -5.550002)
			(size 0.299999 1.799999)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 25 "unconnected-(U1-PE4-Pad59)")
			(pinfunction "PE4")
			(pintype "bidirectional")
		)
		(pad "60" smd oval
			(at -1.749999 -5.550002)
			(size 0.299999 1.799999)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 44 "unconnected-(U1-PE5-Pad60)")
			(pinfunction "PE5")
			(pintype "bidirectional")
		)
		(pad "61" smd oval
			(at -2.249998 -5.550002)
			(size 0.299999 1.799999)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 24 "unconnected-(U1-PD0-Pad61)")
			(pinfunction "PD0")
			(pintype "bidirectional")
		)
		(pad "62" smd oval
			(at -2.75 -5.550002)
			(size 0.299999 1.799999)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 47 "unconnected-(U1-PD1-Pad62)")
			(pinfunction "PD1")
			(pintype "bidirectional")
		)
		(pad "63" smd oval
			(at -3.249999 -5.550002)
			(size 0.299999 1.799999)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 28 "unconnected-(U1-PD2-Pad63)")
			(pinfunction "PD2")
			(pintype "bidirectional")
		)
		(pad "64" smd oval
			(at -3.75 -5.550002)
			(size 0.299999 1.799999)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 64 "Net-(U1-PD3)")
			(pinfunction "PD3")
			(pintype "bidirectional")
		)
		(model "C:/Users/christopher.oelkers/Documents/KiCad Symbols/TM4C123GH6PMT/PM0064A.stp"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "linear regulator:DBV5"
		(layer "F.Cu")
		(at 129.3 71.1 -90)
		(tags "TPS73633DBVR ")
		(property "Reference" "U2"
			(at 0.35 -2.5 -90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "TPS73633DBVR"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" "linear regulator:DBV5"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.ti.com/lit/gpn/tps736"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "DBV5 DBV5-M DBV5-L")
		(sheetname "Root")
		(sheetfile "test jtag board.kicad_sch")
		(attr smd)
		(fp_text user "*"
			(at -1.7 -1.9 -90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "*"
			(at -1.4478 -2.6518 90)
			(layer "F.Fab")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(fp_text user "*"
			(at -1.4478 -2.6518 -90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.1938 -0.950001 270)
			(size 1.4732 0.5588)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 18 "Net-(U2-EN)")
			(pinfunction "IN")
			(pintype "input")
		)
		(pad "2" smd rect
			(at -1.1938 0 270)
			(size 1.4732 0.5588)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "3" smd rect
			(at -1.1938 0.950001 270)
			(size 1.4732 0.5588)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 18 "Net-(U2-EN)")
			(pinfunction "EN")
			(pintype "unspecified")
		)
		(pad "4" smd rect
			(at 1.1938 0.950001 270)
			(size 1.4732 0.5588)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 4 "Net-(U2-NR{slash}FB)")
			(pinfunction "NR/FB")
			(pintype "bidirectional")
		)
		(pad "5" smd rect
			(at 1.1938 -0.950001 270)
			(size 1.4732 0.5588)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "Net-(U1-VBAT)")
			(pinfunction "OUT")
			(pintype "output")
		)
		(model "C:/Users/christopher.oelkers/Documents/KiCad Symbols/TPS73633DBVR/DBV0005A.stp"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder"
		(layer "F.Cu")
		(at 131.15 75.15 180)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C18"
			(at 0 -1.43 0)
			(layer "F.SilkS")
		)
		(property "Value" "0.1uF"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "test jtag board.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.8625 0 180)
			(size 1.075 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "Net-(U1-VBAT)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.8625 0 180)
			(size 1.075 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder"
		(layer "F.Cu")
		(at 110.4 71.45 180)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C9"
			(at 2.65 -0.05 0)
			(layer "F.SilkS")
		)
		(property "Value" "1uF"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "test jtag board.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.8625 0 180)
			(size 1.075 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.8625 0 180)
			(size 1.075 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 3 "Net-(C10-Pad2)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder"
		(layer "F.Cu")
		(at 115.9875 64.35)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R8"
			(at -0.1875 -3.5 0)
			(layer "F.SilkS")
		)
		(property "Value" "33"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "test jtag board.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0)
			(size 0.975 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 22 "Net-(U1-PC0_TCK_SWCLK)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0)
			(size 0.975 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 15 "Net-(J1-SWCLK{slash}TCK)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder"
		(layer "F.Cu")
		(at 122.1 81.75)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C3"
			(at 0 -1.43 0)
			(layer "F.SilkS")
		)
		(property "Value" "0.1uF"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "test jtag board.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.8625 0)
			(size 1.075 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "Net-(U1-VBAT)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.8625 0)
			(size 1.075 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder"
		(layer "F.Cu")
		(at 112.5 89.95 180)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C2"
			(at 0 -1.43 0)
			(layer "F.SilkS")
		)
		(property "Value" "0.1uF"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "test jtag board.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.8625 0 180)
			(size 1.075 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.8625 0 180)
			(size 1.075 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "Net-(U1-VBAT)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder"
		(layer "F.Cu")
		(at 119.55 67.35 90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R10"
			(at 0 -1.43 90)
			(layer "F.SilkS")
		)
		(property "Value" "33"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "test jtag board.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 90)
			(size 0.975 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 23 "Net-(U1-PC1_TMS_SWDIO)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 90)
			(size 0.975 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 11 "Net-(J1-SWDIO{slash}TMS)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder"
		(layer "F.Cu")
		(at 115.4 90.55 90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R2"
			(at 0.7 1.4 90)
			(layer "F.SilkS")
		)
		(property "Value" "1M"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "test jtag board.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 90)
			(size 0.975 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "Net-(U1-VBAT)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 90)
			(size 0.975 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 19 "Net-(U1-WAKE_N)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder"
		(layer "F.Cu")
		(at 102.3 71.9 90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R15"
			(at 0 -1.43 90)
			(layer "F.SilkS")
		)
		(property "Value" "470"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "test jtag board.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 90)
			(size 0.975 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 64 "Net-(U1-PD3)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 90)
			(size 0.975 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 62 "Net-(D2-A)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder"
		(layer "F.Cu")
		(at 110.5 73.45 180)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C8"
			(at 2.7 -0.15 0)
			(layer "F.SilkS")
		)
		(property "Value" "2.2uF"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "test jtag board.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.8625 0 180)
			(size 1.075 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.8625 0 180)
			(size 1.075 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 3 "Net-(C10-Pad2)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder"
		(layer "F.Cu")
		(at 113.3 72.7 -90)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C4"
			(at -0.2 -1.45 90)
			(layer "F.SilkS")
		)
		(property "Value" "0.1uF"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "test jtag board.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.8625 0 270)
			(size 1.075 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.8625 0 270)
			(size 1.075 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "Net-(U1-VBAT)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder"
		(layer "F.Cu")
		(at 112.2375 60.5)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R13"
			(at -0.7875 -1.35 0)
			(layer "F.SilkS")
		)
		(property "Value" "33"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "test jtag board.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0)
			(size 0.975 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 9 "Net-(U1-PC2_TDI)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0)
			(size 0.975 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 10 "Net-(J1-NC{slash}TDI)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder"
		(layer "F.Cu")
		(at 115.8875 62.25 180)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R12"
			(at 2.0875 -3.6 0)
			(layer "F.SilkS")
		)
		(property "Value" "33"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "test jtag board.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 180)
			(size 0.975 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 12 "Net-(J1-SWO{slash}TDO)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 180)
			(size 0.975 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 8 "Net-(U1-PC3_TDO_SWO)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder"
		(layer "F.Cu")
		(at 131.25 65.8 -90)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C17"
			(at 0 -1.43 90)
			(layer "F.SilkS")
		)
		(property "Value" "1uF"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "test jtag board.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.8625 0 270)
			(size 1.075 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 18 "Net-(U2-EN)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.8625 0 270)
			(size 1.075 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "tactile switch:CONN_P1236C_APM"
		(layer "F.Cu")
		(at 134.298299 92.415601 90)
		(tags "MJTP1236C ")
		(property "Reference" "J3"
			(at 8.915601 2.001701 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "MJTP1236C"
			(at 3.500001 1.25 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" "tactile switch:CONN_P1236C_APM"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "MJTP1236C"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "CONN_P1236C_APM")
		(sheetname "Root")
		(sheetfile "test jtag board.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 3.500001 1.25 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 90)
			(size 1.8034 1.8034)
			(drill 1.2954)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "1")
			(pintype "unspecified")
		)
		(pad "2" thru_hole circle
			(at 7.000001 0 90)
			(size 1.8034 1.8034)
			(drill 1.2954)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "2")
			(pintype "unspecified")
		)
		(pad "3" thru_hole circle
			(at 1.25 2.5 90)
			(size 1.4986 1.4986)
			(drill 0.9906)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "3")
			(pintype "unspecified")
		)
		(pad "4" thru_hole circle
			(at 5.750001 2.5 90)
			(size 1.4986 1.4986)
			(drill 0.9906)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 66 "Net-(J3-Pad4)")
			(pinfunction "4")
			(pintype "unspecified")
		)
	)
	(footprint "usb connector:CONN5_ZX62-AB-5PA_HIR"
		(layer "F.Cu")
		(at 138.2 62.8 90)
		(tags "ZX62-AB-5PA31 ")
		(property "Reference" "J2"
			(at 3.8 -4.25 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "ZX62-AB-5PA31"
			(at 0 -2.5019 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" "usb connector:CONN5_ZX62-AB-5PA_HIR"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "ZX62-AB-5PA31"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "CONN5_ZX62-AB-5PA_HIR")
		(sheetname "Root")
		(sheetfile "test jtag board.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -2.5019 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.3 -2.5019 90)
			(size 0.4064 1.3462)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 18 "Net-(U2-EN)")
			(pinfunction "1")
			(pintype "unspecified")
		)
		(pad "2" smd rect
			(at -0.649999 -2.5019 90)
			(size 0.4064 1.3462)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 65 "Net-D-")
			(pinfunction "2")
			(pintype "unspecified")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 0)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "3" smd rect
			(at 0 -2.5019 90)
			(size 0.4064 1.3462)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 20 "Net-D+")
			(pinfunction "3")
			(pintype "unspecified")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 0)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "4" smd rect
			(at 0.649999 -2.5019 90)
			(size 0.4064 1.3462)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 16 "Net-(U1-PB0_USB0VID)")
			(pinfunction "4")
			(pintype "unspecified")
		)
		(pad "5" smd rect
			(at 1.3 -2.5019 90)
			(size 0.4064 1.3462)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pinfunction "5")
			(pintype "unspecified")
		)
		(pad "6" smd rect
			(at -3.0988 -2.3749 180)
			(size 2.1082 1.6002)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 0)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "7" smd rect
			(at 3.0988 -2.3749 180)
			(size 2.1082 1.6002)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 0)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "8" smd rect
			(at -4.0005 0.1651 180)
			(size 1.8034 1.905)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 0)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "9" smd rect
			(at 4.0005 0.1651 180)
			(size 1.8034 1.905)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curve_points 0)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(model "C:/Users/christopher.oelkers/Documents/KiCad Symbols/ul_ZX62-AB-5PA-31-/KiCADv6/footprints.pretty/CONN5_ZX62-AB-5PA_HIR.kicad_mod"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder"
		(layer "F.Cu")
		(at 110.4 69.55 180)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C10"
			(at 3.15 -0.1 0)
			(layer "F.SilkS")
		)
		(property "Value" "0.1uF"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "test jtag board.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.8625 0 180)
			(size 1.075 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.8625 0 180)
			(size 1.075 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 3 "Net-(C10-Pad2)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder"
		(layer "F.Cu")
		(at 122.1 83.3)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R4"
			(at -2.6 0.1 0)
			(layer "F.SilkS")
		)
		(property "Value" "500"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric_Pad0.98x0.95mm_HandSolder"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "test jtag board.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0)
			(size 0.975 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 21 "Net-(U1-OSC1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0)
			(size 0.975 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 7 "Net-(Y1-OUT{slash}IN)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(gr_rect
		(start 96.7 53.6)
		(end 139.9 98.7)
		(fill none)
		(layer "Edge.Cuts")
	)
	(gr_text_box "TM4C Programming proof of concept\ncb: C. E. Oelkers"
		(start 97.325 94.5)
		(end 131.375 98.25)
		(layer "F.SilkS")
		(border yes)
	)
	(gr_text_box "Net-D+ and Net-D- are impedance controlled to 90 Ohms"
		(start 126.5 48.3)
		(end 146.2 54.6)
		(layer "F.Fab")
		(border yes)
	)
	(gr_text_box "Board Thickness: 1.6mm nominal\nOuter layer Copper Weight: 1oz\nInner Layer Copper Weight: 1/2oz"
		(start 86.1 48.375)
		(end 115.35 54.275)
		(layer "F.Fab")
		(border yes)
	)
	(zone
		(net 65)
		(net_name "Net-D-")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30000)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 134.8218 63.267499) (xy 134.8218 63.632499) (xy 135.025 63.653199) (xy 135.6991 63.449999) (xy 135.025 63.246799)
			)
		)
	)
	(zone
		(net 20)
		(net_name "Net-D+")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch full 0.1)
		(priority 30001)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 134.8218 62.6175) (xy 134.8218 62.9825) (xy 135.025 63.0032) (xy 135.6991 62.8) (xy 135.025 62.5968)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layer "In1.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 96.95 53.85) (xy 139.7 53.8) (xy 139.7 98.4) (xy 97.1 98.35)
			)
		)
	)
	(zone
		(net 1)
		(net_name "Net-(U1-VBAT)")
		(layer "In2.Cu")
		(hatch edge 0.5)
		(priority 1)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 96.9 53.8) (xy 139.7 53.8) (xy 139.7 98.4) (xy 97.15 98.45)
			)
		)
	)
)
