(kicad_pcb
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(general
		(thickness 1.6)
		(legacy_teardrops no)
	)
	(paper "A4")
	(layers
		(0 "F.Cu" signal)
		(2 "B.Cu" signal)
		(9 "F.Adhes" user "F.Adhesive")
		(11 "B.Adhes" user "B.Adhesive")
		(13 "F.Paste" user)
		(15 "B.Paste" user)
		(5 "F.SilkS" user "F.Silkscreen")
		(7 "B.SilkS" user "B.Silkscreen")
		(1 "F.Mask" user)
		(3 "B.Mask" user)
		(17 "Dwgs.User" user "User.Drawings")
		(19 "Cmts.User" user "User.Comments")
		(21 "Eco1.User" user "User.Eco1")
		(23 "Eco2.User" user "User.Eco2")
		(25 "Edge.Cuts" user)
		(27 "Margin" user)
		(31 "F.CrtYd" user "F.Courtyard")
		(29 "B.CrtYd" user "B.Courtyard")
		(35 "F.Fab" user)
		(33 "B.Fab" user)
		(39 "User.1" user)
		(41 "User.2" user)
		(43 "User.3" user)
		(45 "User.4" user)
	)
	(setup
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(tenting front back)
		(pcbplotparams
			(layerselection 0x00000000_00000000_55555555_5755f5ff)
			(plot_on_all_layers_selection 0x00000000_00000000_00000000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 4)
			(plotframeref no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(pdf_metadata yes)
			(pdf_single_document no)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plot_black_and_white yes)
			(sketchpadsonfab no)
			(plotpadnumbers no)
			(hidednponfab no)
			(sketchdnponfab yes)
			(crossoutdnponfab yes)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 1)
			(scaleselection 1)
			(outputdirectory "")
		)
	)
	(net 0 "")
	(net 1 "Net-(H1-Pin_32)")
	(net 2 "Net-(H1-Pin_24)")
	(net 3 "Net-(H1-Pin_12)")
	(net 4 "Net-(H1-Pin_22)")
	(net 5 "Net-(H1-Pin_5)")
	(net 6 "Net-(H1-Pin_2)")
	(net 7 "Net-(H1-Pin_26)")
	(net 8 "Net-(H1-Pin_18)")
	(net 9 "Net-(H1-Pin_14)")
	(net 10 "GND")
	(net 11 "Net-(H1-Pin_19)")
	(net 12 "Net-(H1-Pin_28)")
	(net 13 "Net-(H1-Pin_4)")
	(net 14 "+5V")
	(net 15 "Net-(H1-Pin_13)")
	(net 16 "Net-(H1-Pin_6)")
	(net 17 "Net-(H1-Pin_10)")
	(net 18 "Net-(H1-Pin_31)")
	(net 19 "Net-(H1-Pin_25)")
	(net 20 "Net-(H1-Pin_3)")
	(net 21 "Net-(H1-Pin_17)")
	(net 22 "Net-(H1-Pin_8)")
	(net 23 "Net-(H1-Pin_15)")
	(net 24 "Net-(H1-Pin_11)")
	(net 25 "Net-(H1-Pin_21)")
	(net 26 "Net-(H1-Pin_27)")
	(net 27 "Net-(H1-Pin_16)")
	(net 28 "Net-(H1-Pin_7)")
	(net 29 "Net-(H1-Pin_30)")
	(net 30 "Net-(H1-Pin_29)")
	(net 31 "Net-(H1-Pin_9)")
	(net 32 "Net-(H1-Pin_23)")
	(net 33 "Net-(J1-Pin_16)")
	(net 34 "Net-(H1-Pin_34)")
	(net 35 "Net-(H1-Pin_33)")
	(net 36 "Net-(H1-Pin_40)")
	(net 37 "Net-(H1-Pin_35)")
	(net 38 "Net-(H1-Pin_37)")
	(net 39 "Net-(H1-Pin_38)")
	(net 40 "Net-(H1-Pin_36)")
	(net 41 "Net-(J1-Pin_15)")
	(net 42 "Net-(H1-Pin_39)")
	(net 43 "Net-(J2-Pin_1)")
	(net 44 "Net-(J3-Pin_1)")
	(net 45 "Net-(U1-Za)")
	(net 46 "unconnected-(U1-I1b-Pad6)")
	(net 47 "unconnected-(U1-I0d-Pad11)")
	(net 48 "unconnected-(U1-Zc-Pad12)")
	(net 49 "unconnected-(U1-I1d-Pad10)")
	(net 50 "unconnected-(U1-Zb-Pad7)")
	(net 51 "unconnected-(U1-I1c-Pad13)")
	(net 52 "unconnected-(U1-I0b-Pad5)")
	(net 53 "unconnected-(U1-I0c-Pad14)")
	(net 54 "unconnected-(U1-Zd-Pad9)")
	(net 55 "Net-(U1-I0a)")
	(net 56 "Net-(U1-I1a)")
	(footprint "Package_SO:SOIC-16_3.9x9.9mm_P1.27mm"
		(layer "F.Cu")
		(at 152.05 89.635)
		(descr "SOIC, 16 Pin (JEDEC MS-012, variation AC, https://www.jedec.org/document_search?search_api_views_fulltext=MS-012, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_narrow-r/r_16.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOIC SO 16-pin-NSOP R-16 R-16-S D0016A M2B SO16 SOT109-1 751B SOIC_N narrow")
		(property "Reference" "U1"
			(at -0.025 0 270)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "74LS158"
			(at 0 5.9 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/sn74LS158"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Quad 2 to 1 multiplexer"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "DIP?16*")
		(sheetname "/")
		(sheetfile "RamUp320 (130XE) 2.0.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -2.475 -4.445)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 19 "Net-(H1-Pin_25)")
			(pinfunction "S")
			(pintype "input")
		)
		(pad "2" smd roundrect
			(at -2.475 -3.175)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 55 "Net-(U1-I0a)")
			(pinfunction "I0a")
			(pintype "input")
		)
		(pad "3" smd roundrect
			(at -2.475 -1.905)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 56 "Net-(U1-I1a)")
			(pinfunction "I1a")
			(pintype "input")
		)
		(pad "4" smd roundrect
			(at -2.475 -0.635)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 45 "Net-(U1-Za)")
			(pinfunction "Za")
			(pintype "output")
		)
		(pad "5" smd roundrect
			(at -2.475 0.635)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 52 "unconnected-(U1-I0b-Pad5)")
			(pinfunction "I0b")
			(pintype "input+no_connect")
		)
		(pad "6" smd roundrect
			(at -2.475 1.905)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 46 "unconnected-(U1-I1b-Pad6)")
			(pinfunction "I1b")
			(pintype "input+no_connect")
		)
		(pad "7" smd roundrect
			(at -2.475 3.175)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 50 "unconnected-(U1-Zb-Pad7)")
			(pinfunction "Zb")
			(pintype "output+no_connect")
		)
		(pad "8" smd roundrect
			(at -2.475 4.445)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 10 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "9" smd roundrect
			(at 2.475 4.445)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 54 "unconnected-(U1-Zd-Pad9)")
			(pinfunction "Zd")
			(pintype "output+no_connect")
		)
		(pad "10" smd roundrect
			(at 2.475 3.175)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 49 "unconnected-(U1-I1d-Pad10)")
			(pinfunction "I1d")
			(pintype "input+no_connect")
		)
		(pad "11" smd roundrect
			(at 2.475 1.905)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 47 "unconnected-(U1-I0d-Pad11)")
			(pinfunction "I0d")
			(pintype "input+no_connect")
		)
		(pad "12" smd roundrect
			(at 2.475 0.635)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 48 "unconnected-(U1-Zc-Pad12)")
			(pinfunction "Zc")
			(pintype "output+no_connect")
		)
		(pad "13" smd roundrect
			(at 2.475 -0.635)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 51 "unconnected-(U1-I1c-Pad13)")
			(pinfunction "I1c")
			(pintype "input+no_connect")
		)
		(pad "14" smd roundrect
			(at 2.475 -1.905)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 53 "unconnected-(U1-I0c-Pad14)")
			(pinfunction "I0c")
			(pintype "input+no_connect")
		)
		(pad "15" smd roundrect
			(at 2.475 -3.175)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 10 "GND")
			(pinfunction "E")
			(pintype "input")
		)
		(pad "16" smd roundrect
			(at 2.475 -4.445)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 14 "+5V")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Package_SO.3dshapes/SOIC-16_3.9x9.9mm_P1.27mm.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_DIP:DIP-40_W15.24mm_Socket"
		(layer "F.Cu")
		(at 143.285 72.16)
		(descr "40-lead though-hole mounted DIP package, row spacing 15.24mm (600 mils), Socket")
		(tags "THT DIP DIL PDIP 2.54mm 15.24mm 600mil Socket")
		(property "Reference" "J1"
			(at 7.62 -2.33 0)
			(layer "F.SilkS")
		)
		(property "Value" "Socket"
			(at 7.62 50.59 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, double row, 02x20, counter clockwise pin numbering scheme (similar to DIP package numbering), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_2x??_*")
		(sheetname "/")
		(sheetfile "RamUp320 (130XE) 2.0.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 7.62 24.13 270)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" thru_hole roundrect
			(at 0 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.15625)
			(net 10 "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 0 2.54)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "Net-(H1-Pin_2)")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole circle
			(at 0 5.08)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 20 "Net-(H1-Pin_3)")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole circle
			(at 0 7.62)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 13 "Net-(H1-Pin_4)")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(pad "5" thru_hole circle
			(at 0 10.16)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "Net-(H1-Pin_5)")
			(pinfunction "Pin_5")
			(pintype "passive")
		)
		(pad "6" thru_hole circle
			(at 0 12.7)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 16 "Net-(H1-Pin_6)")
			(pinfunction "Pin_6")
			(pintype "passive")
		)
		(pad "7" thru_hole circle
			(at 0 15.24)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 28 "Net-(H1-Pin_7)")
			(pinfunction "Pin_7")
			(pintype "passive")
		)
		(pad "8" thru_hole circle
			(at 0 17.78)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 22 "Net-(H1-Pin_8)")
			(pinfunction "Pin_8")
			(pintype "passive")
		)
		(pad "9" thru_hole circle
			(at 0 20.32)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 31 "Net-(H1-Pin_9)")
			(pinfunction "Pin_9")
			(pintype "passive")
		)
		(pad "10" thru_hole circle
			(at 0 22.86)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 17 "Net-(H1-Pin_10)")
			(pinfunction "Pin_10")
			(pintype "passive")
		)
		(pad "11" thru_hole circle
			(at 0 25.4)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 24 "Net-(H1-Pin_11)")
			(pinfunction "Pin_11")
			(pintype "passive")
		)
		(pad "12" thru_hole circle
			(at 0 27.94)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "Net-(H1-Pin_12)")
			(pinfunction "Pin_12")
			(pintype "passive")
		)
		(pad "13" thru_hole circle
			(at 0 30.48)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 15 "Net-(H1-Pin_13)")
			(pinfunction "Pin_13")
			(pintype "passive")
		)
		(pad "14" thru_hole circle
			(at 0 33.02)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 9 "Net-(H1-Pin_14)")
			(pinfunction "Pin_14")
			(pintype "passive")
		)
		(pad "15" thru_hole circle
			(at 0 35.56)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 41 "Net-(J1-Pin_15)")
			(pinfunction "Pin_15")
			(pintype "passive")
		)
		(pad "16" thru_hole circle
			(at 0 38.1)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 33 "Net-(J1-Pin_16)")
			(pinfunction "Pin_16")
			(pintype "passive")
		)
		(pad "17" thru_hole circle
			(at 0 40.64)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 21 "Net-(H1-Pin_17)")
			(pinfunction "Pin_17")
			(pintype "passive")
		)
		(pad "18" thru_hole circle
			(at 0 43.18)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 8 "Net-(H1-Pin_18)")
			(pinfunction "Pin_18")
			(pintype "passive")
		)
		(pad "19" thru_hole circle
			(at 0 45.72)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 11 "Net-(H1-Pin_19)")
			(pinfunction "Pin_19")
			(pintype "passive")
		)
		(pad "20" thru_hole circle
			(at 0 48.26)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 14 "+5V")
			(pinfunction "Pin_20")
			(pintype "passive")
		)
		(pad "21" thru_hole circle
			(at 15.24 48.26)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 25 "Net-(H1-Pin_21)")
			(pinfunction "Pin_21")
			(pintype "passive")
		)
		(pad "22" thru_hole circle
			(at 15.24 45.72)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "Net-(H1-Pin_22)")
			(pinfunction "Pin_22")
			(pintype "passive")
		)
		(pad "23" thru_hole circle
			(at 15.24 43.18)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 32 "Net-(H1-Pin_23)")
			(pinfunction "Pin_23")
			(pintype "passive")
		)
		(pad "24" thru_hole circle
			(at 15.24 40.64)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "Net-(H1-Pin_24)")
			(pinfunction "Pin_24")
			(pintype "passive")
		)
		(pad "25" thru_hole circle
			(at 15.24 38.1)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 19 "Net-(H1-Pin_25)")
			(pinfunction "Pin_25")
			(pintype "passive")
		)
		(pad "26" thru_hole circle
			(at 15.24 35.56)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 7 "Net-(H1-Pin_26)")
			(pinfunction "Pin_26")
			(pintype "passive")
		)
		(pad "27" thru_hole circle
			(at 15.24 33.02)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 26 "Net-(H1-Pin_27)")
			(pinfunction "Pin_27")
			(pintype "passive")
		)
		(pad "28" thru_hole circle
			(at 15.24 30.48)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 12 "Net-(H1-Pin_28)")
			(pinfunction "Pin_28")
			(pintype "passive")
		)
		(pad "29" thru_hole circle
			(at 15.24 27.94)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 30 "Net-(H1-Pin_29)")
			(pinfunction "Pin_29")
			(pintype "passive")
		)
		(pad "30" thru_hole circle
			(at 15.24 25.4)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 29 "Net-(H1-Pin_30)")
			(pinfunction "Pin_30")
			(pintype "passive")
		)
		(pad "31" thru_hole circle
			(at 15.24 22.86)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 18 "Net-(H1-Pin_31)")
			(pinfunction "Pin_31")
			(pintype "passive")
		)
		(pad "32" thru_hole circle
			(at 15.24 20.32)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "Net-(H1-Pin_32)")
			(pinfunction "Pin_32")
			(pintype "passive")
		)
		(pad "33" thru_hole circle
			(at 15.24 17.78)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 35 "Net-(H1-Pin_33)")
			(pinfunction "Pin_33")
			(pintype "passive")
		)
		(pad "34" thru_hole circle
			(at 15.24 15.24)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 34 "Net-(H1-Pin_34)")
			(pinfunction "Pin_34")
			(pintype "passive")
		)
		(pad "35" thru_hole circle
			(at 15.24 12.7)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 37 "Net-(H1-Pin_35)")
			(pinfunction "Pin_35")
			(pintype "passive")
		)
		(pad "36" thru_hole circle
			(at 15.24 10.16)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 40 "Net-(H1-Pin_36)")
			(pinfunction "Pin_36")
			(pintype "passive")
		)
		(pad "37" thru_hole circle
			(at 15.24 7.62)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 38 "Net-(H1-Pin_37)")
			(pinfunction "Pin_37")
			(pintype "passive")
		)
		(pad "38" thru_hole circle
			(at 15.24 5.08)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 39 "Net-(H1-Pin_38)")
			(pinfunction "Pin_38")
			(pintype "passive")
		)
		(pad "39" thru_hole circle
			(at 15.24 2.54)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 42 "Net-(H1-Pin_39)")
			(pinfunction "Pin_39")
			(pintype "passive")
		)
		(pad "40" thru_hole circle
			(at 15.24 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 36 "Net-(H1-Pin_40)")
			(pinfunction "Pin_40")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Package_DIP.3dshapes/DIP-40_W15.24mm_Socket.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_SO:SOIC-16_3.9x9.9mm_P1.27mm"
		(layer "F.Cu")
		(at 151.9 109.31)
		(descr "SOIC, 16 Pin (JEDEC MS-012, variation AC, https://www.jedec.org/document_search?search_api_views_fulltext=MS-012, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_narrow-r/r_16.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOIC SO 16-pin-NSOP R-16 R-16-S D0016A M2B SO16 SOT109-1 751B SOIC_N narrow")
		(property "Reference" "U2"
			(at 0.125 -0.275 270)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "SN74LS157DR"
			(at 4.325 0.075 270)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/sn74LS157"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Quad 2 to 1 line Multiplexer"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "DIP?16*")
		(sheetname "/")
		(sheetfile "RamUp320 (130XE) 2.0.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -2.475 -4.445)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 44 "Net-(J3-Pin_1)")
			(pinfunction "S")
			(pintype "input")
		)
		(pad "2" smd roundrect
			(at -2.475 -3.175)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 14 "+5V")
			(pinfunction "I0a")
			(pintype "input")
		)
		(pad "3" smd roundrect
			(at -2.475 -1.905)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 41 "Net-(J1-Pin_15)")
			(pinfunction "I1a")
			(pintype "input")
		)
		(pad "4" smd roundrect
			(at -2.475 -0.635)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 23 "Net-(H1-Pin_15)")
			(pinfunction "Za")
			(pintype "output")
		)
		(pad "5" smd roundrect
			(at -2.475 0.635)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 41 "Net-(J1-Pin_15)")
			(pinfunction "I0b")
			(pintype "input")
		)
		(pad "6" smd roundrect
			(at -2.475 1.905)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 14 "+5V")
			(pinfunction "I1b")
			(pintype "input")
		)
		(pad "7" smd roundrect
			(at -2.475 3.175)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 55 "Net-(U1-I0a)")
			(pinfunction "Zb")
			(pintype "output")
		)
		(pad "8" smd roundrect
			(at -2.475 4.445)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 10 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "9" smd roundrect
			(at 2.475 4.445)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 27 "Net-(H1-Pin_16)")
			(pinfunction "Zc")
			(pintype "output")
		)
		(pad "10" smd roundrect
			(at 2.475 3.175)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 33 "Net-(J1-Pin_16)")
			(pinfunction "I1c")
			(pintype "input")
		)
		(pad "11" smd roundrect
			(at 2.475 1.905)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 14 "+5V")
			(pinfunction "I0c")
			(pintype "input")
		)
		(pad "12" smd roundrect
			(at 2.475 0.635)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 56 "Net-(U1-I1a)")
			(pinfunction "Zd")
			(pintype "output")
		)
		(pad "13" smd roundrect
			(at 2.475 -0.635)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 14 "+5V")
			(pinfunction "I1d")
			(pintype "input")
		)
		(pad "14" smd roundrect
			(at 2.475 -1.905)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 33 "Net-(J1-Pin_16)")
			(pinfunction "I0d")
			(pintype "input")
		)
		(pad "15" smd roundrect
			(at 2.475 -3.175)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 10 "GND")
			(pinfunction "E")
			(pintype "input")
		)
		(pad "16" smd roundrect
			(at 2.475 -4.445)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 14 "+5V")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Package_SO.3dshapes/SOIC-16_3.9x9.9mm_P1.27mm.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_DIP:DIP-40_W15.24mm"
		(layer "F.Cu")
		(at 145.955 72.1)
		(descr "40-lead though-hole mounted DIP package, row spacing 15.24mm (600 mils)")
		(tags "THT DIP DIL PDIP 2.54mm 15.24mm 600mil")
		(property "Reference" "H1"
			(at 7.62 -2.33 0)
			(layer "B.SilkS")
		)
		(property "Value" "Header"
			(at 7.62 50.59 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, double row, 02x20, counter clockwise pin numbering scheme (similar to DIP package numbering), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_2x??_*")
		(sheetname "/")
		(sheetfile "RamUp320 (130XE) 2.0.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 7.62 24.13 270)
			(unlocked yes)
			(layer "B.Fab")
		)
		(pad "1" thru_hole roundrect
			(at 0 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.15625)
			(net 10 "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 0 2.54)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "Net-(H1-Pin_2)")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole circle
			(at 0 5.08)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 20 "Net-(H1-Pin_3)")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole circle
			(at 0 7.62)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 13 "Net-(H1-Pin_4)")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(pad "5" thru_hole circle
			(at 0 10.16)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "Net-(H1-Pin_5)")
			(pinfunction "Pin_5")
			(pintype "passive")
		)
		(pad "6" thru_hole circle
			(at 0 12.7)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 16 "Net-(H1-Pin_6)")
			(pinfunction "Pin_6")
			(pintype "passive")
		)
		(pad "7" thru_hole circle
			(at 0 15.24)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 28 "Net-(H1-Pin_7)")
			(pinfunction "Pin_7")
			(pintype "passive")
		)
		(pad "8" thru_hole circle
			(at 0 17.78)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 22 "Net-(H1-Pin_8)")
			(pinfunction "Pin_8")
			(pintype "passive")
		)
		(pad "9" thru_hole circle
			(at 0 20.32)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 31 "Net-(H1-Pin_9)")
			(pinfunction "Pin_9")
			(pintype "passive")
		)
		(pad "10" thru_hole circle
			(at 0 22.86)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 17 "Net-(H1-Pin_10)")
			(pinfunction "Pin_10")
			(pintype "passive")
		)
		(pad "11" thru_hole circle
			(at 0 25.4)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 24 "Net-(H1-Pin_11)")
			(pinfunction "Pin_11")
			(pintype "passive")
		)
		(pad "12" thru_hole circle
			(at 0 27.94)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "Net-(H1-Pin_12)")
			(pinfunction "Pin_12")
			(pintype "passive")
		)
		(pad "13" thru_hole circle
			(at 0 30.48)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 15 "Net-(H1-Pin_13)")
			(pinfunction "Pin_13")
			(pintype "passive")
		)
		(pad "14" thru_hole circle
			(at 0 33.02)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 9 "Net-(H1-Pin_14)")
			(pinfunction "Pin_14")
			(pintype "passive")
		)
		(pad "15" thru_hole circle
			(at 0 35.56)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 23 "Net-(H1-Pin_15)")
			(pinfunction "Pin_15")
			(pintype "passive")
		)
		(pad "16" thru_hole circle
			(at 0 38.1)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 27 "Net-(H1-Pin_16)")
			(pinfunction "Pin_16")
			(pintype "passive")
		)
		(pad "17" thru_hole circle
			(at 0 40.64)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 21 "Net-(H1-Pin_17)")
			(pinfunction "Pin_17")
			(pintype "passive")
		)
		(pad "18" thru_hole circle
			(at 0 43.18)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 8 "Net-(H1-Pin_18)")
			(pinfunction "Pin_18")
			(pintype "passive")
		)
		(pad "19" thru_hole circle
			(at 0 45.72)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 11 "Net-(H1-Pin_19)")
			(pinfunction "Pin_19")
			(pintype "passive")
		)
		(pad "20" thru_hole circle
			(at 0 48.26)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 14 "+5V")
			(pinfunction "Pin_20")
			(pintype "passive")
		)
		(pad "21" thru_hole circle
			(at 15.24 48.26)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 25 "Net-(H1-Pin_21)")
			(pinfunction "Pin_21")
			(pintype "passive")
		)
		(pad "22" thru_hole circle
			(at 15.24 45.72)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "Net-(H1-Pin_22)")
			(pinfunction "Pin_22")
			(pintype "passive")
		)
		(pad "23" thru_hole circle
			(at 15.24 43.18)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 32 "Net-(H1-Pin_23)")
			(pinfunction "Pin_23")
			(pintype "passive")
		)
		(pad "24" thru_hole circle
			(at 15.24 40.64)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "Net-(H1-Pin_24)")
			(pinfunction "Pin_24")
			(pintype "passive")
		)
		(pad "25" thru_hole circle
			(at 15.24 38.1)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 19 "Net-(H1-Pin_25)")
			(pinfunction "Pin_25")
			(pintype "passive")
		)
		(pad "26" thru_hole circle
			(at 15.24 35.56)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 7 "Net-(H1-Pin_26)")
			(pinfunction "Pin_26")
			(pintype "passive")
		)
		(pad "27" thru_hole circle
			(at 15.24 33.02)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 26 "Net-(H1-Pin_27)")
			(pinfunction "Pin_27")
			(pintype "passive")
		)
		(pad "28" thru_hole circle
			(at 15.24 30.48)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 12 "Net-(H1-Pin_28)")
			(pinfunction "Pin_28")
			(pintype "passive")
		)
		(pad "29" thru_hole circle
			(at 15.24 27.94)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 30 "Net-(H1-Pin_29)")
			(pinfunction "Pin_29")
			(pintype "passive")
		)
		(pad "30" thru_hole circle
			(at 15.24 25.4)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 29 "Net-(H1-Pin_30)")
			(pinfunction "Pin_30")
			(pintype "passive")
		)
		(pad "31" thru_hole circle
			(at 15.24 22.86)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 18 "Net-(H1-Pin_31)")
			(pinfunction "Pin_31")
			(pintype "passive")
		)
		(pad "32" thru_hole circle
			(at 15.24 20.32)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "Net-(H1-Pin_32)")
			(pinfunction "Pin_32")
			(pintype "passive")
		)
		(pad "33" thru_hole circle
			(at 15.24 17.78)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 35 "Net-(H1-Pin_33)")
			(pinfunction "Pin_33")
			(pintype "passive")
		)
		(pad "34" thru_hole circle
			(at 15.24 15.24)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 34 "Net-(H1-Pin_34)")
			(pinfunction "Pin_34")
			(pintype "passive")
		)
		(pad "35" thru_hole circle
			(at 15.24 12.7)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 37 "Net-(H1-Pin_35)")
			(pinfunction "Pin_35")
			(pintype "passive")
		)
		(pad "36" thru_hole circle
			(at 15.24 10.16)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 40 "Net-(H1-Pin_36)")
			(pinfunction "Pin_36")
			(pintype "passive")
		)
		(pad "37" thru_hole circle
			(at 15.24 7.62)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 38 "Net-(H1-Pin_37)")
			(pinfunction "Pin_37")
			(pintype "passive")
		)
		(pad "38" thru_hole circle
			(at 15.24 5.08)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 39 "Net-(H1-Pin_38)")
			(pinfunction "Pin_38")
			(pintype "passive")
		)
		(pad "39" thru_hole circle
			(at 15.24 2.54)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 42 "Net-(H1-Pin_39)")
			(pinfunction "Pin_39")
			(pintype "passive")
		)
		(pad "40" thru_hole circle
			(at 15.24 0)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 36 "Net-(H1-Pin_40)")
			(pinfunction "Pin_40")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Package_DIP.3dshapes/DIP-40_W15.24mm.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Horizontal"
		(layer "F.Cu")
		(at 164.315 106.685)
		(descr "Through hole angled pin header, 1x02, 2.54mm pitch, 6mm pin length, single row")
		(tags "Through hole angled pin header THT 1x02 2.54mm single row")
		(property "Reference" "J3"
			(at -0.265 -2.475 0)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_01x02"
			(at 4.385 4.81 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "/")
		(sheetfile "RamUp320 (130XE) 2.0.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 2.77 1.27 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 44 "Net-(J3-Pin_1)")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 0 2.54)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 10 "GND")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Horizontal.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_PinHeader_2.54mm:PinHeader_1x01_P2.54mm_Horizontal"
		(layer "F.Cu")
		(at 164.075 81.06)
		(descr "Through hole angled pin header, 1x01, 2.54mm pitch, 6mm pin length, single row")
		(tags "Through hole angled pin header THT 1x01 2.54mm single row")
		(property "Reference" "J2"
			(at 0.025 -2.435 0)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_01x01"
			(at 4.385 2.27 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x01, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "/")
		(sheetfile "RamUp320 (130XE) 2.0.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 2.77 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 43 "Net-(J2-Pin_1)")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Horizontal.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
		(layer "F.Cu")
		(at 152.05 81.61)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R1"
			(at 0 -1.83 0)
			(layer "F.SilkS")
		)
		(property "Value" "33R"
			(at 0 1.83 0)
			(layer "F.SilkS")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "RamUp320 (130XE) 2.0.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.55 0)
			(size 1.3 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.192308)
			(net 45 "Net-(U1-Za)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.55 0)
			(size 1.3 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.192308)
			(net 43 "Net-(J2-Pin_1)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_1206_3216Metric_Pad1.30x1.75mm_HandSolder"
		(layer "F.Cu")
		(at 152.075 101.11 180)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC-7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R2"
			(at 0 1.75 0)
			(layer "F.SilkS")
		)
		(property "Value" "1K"
			(at -0.05 -2 0)
			(layer "F.SilkS")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "RamUp320 (130XE) 2.0.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.55 0 180)
			(size 1.3 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.192308)
			(net 14 "+5V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.55 0 180)
			(size 1.3 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.192308)
			(net 44 "Net-(J3-Pin_1)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(gr_rect
		(start 140.6 68.71)
		(end 167.7 123.11)
		(fill no)
		(layer "Edge.Cuts")
	)
	(gr_text "Memory MUX concept by S.Peterson"
		(at 153.375 97.175 270)
		(layer "B.Cu")
	)
	(gr_text "\n\n128K/320K switch module\n©2026 Wayne Thomason"
		(at 148.375 97.575 270)
		(layer "B.Cu")
	)
	(gr_text "130XE 320K Upgrade"
		(at 155.45 109.625 270)
		(layer "B.Cu")
	)
	(gr_text "v2.2"
		(at 155.65 82.85 270)
		(layer "B.Cu")
	)
	(gr_text "\n\n128K/320K switch module\n©2026 Wayne Thomason"
		(at 148.375 97.575 270)
		(layer "B.Mask")
	)
	(gr_text "v2.2"
		(at 155.65 82.85 270)
		(layer "B.Mask")
	)
	(gr_text "130XE 320K Upgrade"
		(at 155.45 109.625 270)
		(layer "B.Mask")
	)
	(gr_text "Memory MUX concept by S.Peterson"
		(at 153.375 97.175 270)
		(layer "B.Mask")
	)
	(gr_text "130XE 320K\nUpgrade"
		(at 162.7 88.06 270)
		(layer "F.SilkS")
	)
	(gr_text "©2026 Wayne\nThomason"
		(at 163.425 116.775 270)
		(layer "F.SilkS")
	)
	(gr_text "PIA (6520)\nSOCKET"
		(at 151.45 118.175 0)
		(layer "F.SilkS")
	)
	(gr_text "v2.2"
		(at 162.775 100.285 270)
		(layer "F.SilkS")
	)
	(gr_text "SN74LS158DR"
		(at 156 89.65 270)
		(layer "F.SilkS")
	)
	(gr_text "RA8"
		(at 165.45 79.81 270)
		(layer "F.SilkS")
	)
	(gr_text "TO SPST"
		(at 165.75 107.71 270)
		(layer "F.SilkS")
	)
	(gr_text "To 130XE\nMainboard\nPIA (6520)\nSocket"
		(at 152.6375 120.25625 0)
		(layer "B.SilkS")
	)
	(gr_text "J2"
		(at 163.525 84.5 270)
		(layer "B.SilkS")
	)
	(gr_text "RA8"
		(at 165.625 82.16 270)
		(layer "B.SilkS")
	)
	(gr_text "J3"
		(at 163.675 112.96 270)
		(layer "B.SilkS")
	)
	(gr_text "TO SPST"
		(at 165.725 107.81 270)
		(layer "B.SilkS")
	)
	(embedded_fonts no)
)
