(kicad_pcb
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(general
		(thickness 1.6)
		(legacy_teardrops no)
	)
	(paper "A4")
	(title_block
		(title "ATF150x_uPRG")
		(date "2026-09-12")
		(rev "010")
		(company "Brian K. White")
		(comment 1 "CC-BY-SA")
		(comment 2 "github.com/bkw777/ATF150x_uPRG")
	)
	(layers
		(0 "F.Cu" signal)
		(2 "B.Cu" signal)
		(9 "F.Adhes" user "F.Adhesive")
		(11 "B.Adhes" user "B.Adhesive")
		(13 "F.Paste" user)
		(15 "B.Paste" user)
		(5 "F.SilkS" user "F.Silkscreen")
		(7 "B.SilkS" user "B.Silkscreen")
		(1 "F.Mask" user)
		(3 "B.Mask" user)
		(17 "Dwgs.User" user "User.Drawings")
		(19 "Cmts.User" user "User.Comments")
		(21 "Eco1.User" user "User.Eco1")
		(23 "Eco2.User" user "User.Eco2")
		(25 "Edge.Cuts" user)
		(27 "Margin" user)
		(31 "F.CrtYd" user "F.Courtyard")
		(29 "B.CrtYd" user "B.Courtyard")
		(35 "F.Fab" user)
		(33 "B.Fab" user)
	)
	(setup
		(stackup
			(layer "F.SilkS"
				(type "Top Silk Screen")
			)
			(layer "F.Paste"
				(type "Top Solder Paste")
			)
			(layer "F.Mask"
				(type "Top Solder Mask")
				(thickness 0.01)
			)
			(layer "F.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "dielectric 1"
				(type "core")
				(thickness 1.51)
				(material "FR4")
				(epsilon_r 4.5)
				(loss_tangent 0.02)
			)
			(layer "B.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "B.Mask"
				(type "Bottom Solder Mask")
				(thickness 0.01)
			)
			(layer "B.Paste"
				(type "Bottom Solder Paste")
			)
			(layer "B.SilkS"
				(type "Bottom Silk Screen")
			)
			(copper_finish "ENIG")
			(dielectric_constraints no)
		)
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(tenting front back)
		(pcbplotparams
			(layerselection 0x00000000_00000000_55555555_f755f5ff)
			(plot_on_all_layers_selection 0x00000000_00000000_00000000_00000000)
			(disableapertmacros no)
			(usegerberextensions yes)
			(usegerberattributes no)
			(usegerberadvancedattributes no)
			(creategerberjobfile no)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 4)
			(plotframeref no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(pdf_metadata yes)
			(pdf_single_document no)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plot_black_and_white yes)
			(sketchpadsonfab no)
			(plotpadnumbers no)
			(hidednponfab no)
			(sketchdnponfab yes)
			(crossoutdnponfab yes)
			(subtractmaskfromsilk yes)
			(outputformat 1)
			(mirror no)
			(drillshape 0)
			(scaleselection 1)
			(outputdirectory "GERBER_${TITLE}_${REVISION}")
		)
	)
	(net 0 "")
	(net 1 "TCK")
	(net 2 "TDI")
	(net 3 "TDO")
	(net 4 "TMS")
	(net 5 "Net-(C7-Pad1)")
	(net 6 "Net-(C7-Pad2)")
	(net 7 "unconnected-(J1-AC1-Pad13)")
	(net 8 "unconnected-(J1-AD4-Pad8)")
	(net 9 "+5V")
	(net 10 "GND")
	(net 11 "unconnected-(J1-AD6-Pad10)")
	(net 12 "unconnected-(J1-AC0-Pad12)")
	(net 13 "unconnected-(J1-AC5-Pad17)")
	(net 14 "unconnected-(J1-AC3-Pad15)")
	(net 15 "unconnected-(J1-AC6-Pad18)")
	(net 16 "unconnected-(J1-AC4-Pad16)")
	(net 17 "unconnected-(J1-AC8-Pad20)")
	(net 18 "unconnected-(J1-AD5-Pad9)")
	(net 19 "unconnected-(J1-AC9-Pad21)")
	(net 20 "unconnected-(J1-AC7-Pad19)")
	(net 21 "unconnected-(J1-AC2-Pad14)")
	(net 22 "+12V")
	(net 23 "unconnected-(J1-AD7-Pad11)")
	(net 24 "+3V3")
	(net 25 "unconnected-(JP1-Pad1)")
	(net 26 "unconnected-(JP2-Pad1)")
	(net 27 "Net-(JP2-Pad3)")
	(net 28 "Net-(LED1-A)")
	(net 29 "Net-(LED2-A)")
	(net 30 "Net-(LED3-A)")
	(net 31 "VCC")
	(net 32 "Net-(C6-Pad2)")
	(net 33 "Net-(C6-Pad1)")
	(net 34 "VPP")
	(net 35 "unconnected-(J2-nc-Pad7)")
	(net 36 "unconnected-(J2-nc-Pad8)")
	(footprint "000_LOCAL:R_0805"
		(layer "F.Cu")
		(at 131.572 95.885)
		(descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
		(tags "resistor 0805")
		(property "Reference" "R2"
			(at 1.905 -0.508 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "10k"
			(at 1.905 0.635 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "ATF150x_uPRG.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0)
			(size 0.7 1.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.1)
			(net 28 "Net-(LED1-A)")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at 0.95 0)
			(size 0.7 1.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.1)
			(net 31 "VCC")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KIPRJMOD}/000_LOCAL.pretty/3dshapes/R_0805.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "000_LOCAL:C_0805"
		(layer "F.Cu")
		(at 140.649999 99.441)
		(descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
		(tags "capacitor 0805")
		(property "Reference" "C1"
			(at 2.650001 -0.491 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "1u"
			(at 2.650001 0.659 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "ATF150x_uPRG.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -1.270001 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9 0)
			(size 0.8 1.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.1)
			(net 9 "+5V")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at 0.9 0)
			(size 0.8 1.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.1)
			(net 10 "GND")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KIPRJMOD}/000_LOCAL.pretty/3dshapes/C_0805.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "000_LOCAL:Fiducial_0.5_1.0"
		(layer "F.Cu")
		(at 159.76 87.23)
		(descr "Circular Fiducial, 0.5mm bare copper, 1mm soldermask opening (Level C)")
		(tags "fiducial")
		(property "Reference" "REF**"
			(at 0 -1.5 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Fiducial_0.5_1.0"
			(at 0 1.5 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "" smd circle
			(at 0 0)
			(size 0.5 0.5)
			(layers "F.Cu" "F.Mask")
			(solder_mask_margin 0.25)
			(clearance 0.25)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
	)
	(footprint "000_LOCAL:SOIC-8"
		(layer "F.Cu")
		(at 137.225 91.186)
		(descr "SOIC, 8 Pin (JEDEC MS-012AA, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_narrow-r/r_8.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOIC SO")
		(property "Reference" "U2"
			(at -1.208 -2.427 270)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "MAX662A"
			(at 0.443 0 270)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "ATF150x_uPRG.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -2.667 -1.905)
			(size 1.5 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 33 "Net-(C6-Pad1)")
			(pinfunction "C1-")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at -2.667 -0.635)
			(size 1.5 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 32 "Net-(C6-Pad2)")
			(pinfunction "C1+")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "3" smd roundrect
			(at -2.667 0.635)
			(size 1.5 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 5 "Net-(C7-Pad1)")
			(pinfunction "C1-")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "4" smd roundrect
			(at -2.667 1.905)
			(size 1.5 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 6 "Net-(C7-Pad2)")
			(pinfunction "C1+")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "5" smd roundrect
			(at 2.667 1.905)
			(size 1.5 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 9 "+5V")
			(pinfunction "Vcc")
			(pintype "power_in")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "6" smd roundrect
			(at 2.667 0.635)
			(size 1.5 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 22 "+12V")
			(pinfunction "Vout")
			(pintype "power_out")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "7" smd roundrect
			(at 2.667 -0.635)
			(size 1.5 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 10 "GND")
			(pinfunction "GND")
			(pintype "power_in")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "8" smd roundrect
			(at 2.667 -1.905)
			(size 1.5 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 10 "GND")
			(pinfunction "SHDN")
			(pintype "input")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KIPRJMOD}/000_LOCAL.pretty/3dshapes/SO-8_3.9x4.9mm_P1.27mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "000_LOCAL:Fiducial_0.5_1.0"
		(layer "F.Cu")
		(at 128.16 88.79)
		(descr "Circular Fiducial, 0.5mm bare copper, 1mm soldermask opening (Level C)")
		(tags "fiducial")
		(property "Reference" "REF**"
			(at 0 -1.5 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Fiducial_0.5_1.0"
			(at 0 1.5 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "" smd circle
			(at 0 0)
			(size 0.5 0.5)
			(layers "F.Cu" "F.Mask")
			(solder_mask_margin 0.25)
			(clearance 0.25)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
	)
	(footprint "000_LOCAL:C_0805"
		(layer "F.Cu")
		(at 142.15 90.825 90)
		(descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
		(tags "capacitor 0805")
		(property "Reference" "C4"
			(at 3.525 0 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "1u"
			(at 2.425 0 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "ATF150x_uPRG.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -1.270001 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9 0 90)
			(size 0.8 1.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.1)
			(net 22 "+12V")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at 0.9 0 90)
			(size 0.8 1.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.1)
			(net 10 "GND")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KIPRJMOD}/000_LOCAL.pretty/3dshapes/C_0805.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "000_LOCAL:IDC-Header_2x05_P2.54mm pcb-edge"
		(layer "F.Cu")
		(at 165.09 95.25)
		(descr "Through hole IDC box header, 2x05, 2.54mm pitch, DIN 41651 / IEC 60603-13, double rows, https://docs.google.com/spreadsheets/d/16SsEcesNF15N3Lb4niX7dcUr-NY5_MFPQhobNuNppn4/edit#gid=0")
		(tags "Through hole horizontal IDC box header THT 2x05 2.54mm double row")
		(property "Reference" "J2"
			(at -4.689 -6.985 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Altera JTAG-A+VPP"
			(at -6.096 0 270)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "datasheets/JTAG-A.pdf"
			(at -4.318 -5.08 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, double row, 02x05, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at -4.318 -5.08 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_2x??_*")
		(sheetname "Root")
		(sheetfile "ATF150x_uPRG.kicad_sch")
		(attr through_hole)
		(fp_text user "PCB EDGE"
			(at 4.445 11.303 0)
			(unlocked yes)
			(layer "Dwgs.User")
		)
		(fp_text user "PCB EDGE"
			(at -0.889 9.271 270)
			(unlocked yes)
			(layer "Dwgs.User")
		)
		(fp_text user "${REFERENCE}"
			(at 4.512 0 90)
			(layer "F.Fab")
		)
		(pad "1" connect roundrect
			(at -1.905 -5.08)
			(size 3.81 1.905)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(chamfer_ratio 0)
			(chamfer top_right bottom_right)
			(net 1 "TCK")
			(pinfunction "TCK")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" connect roundrect
			(at -1.905 -5.08)
			(size 3.81 1.905)
			(layers "B.Cu" "B.Mask")
			(roundrect_rratio 0.25)
			(chamfer_ratio 0)
			(chamfer top_right bottom_right)
			(net 10 "GND")
			(pinfunction "GND")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "3" connect roundrect
			(at -1.905 -2.54)
			(size 3.81 1.905)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(chamfer_ratio 0)
			(chamfer top_right bottom_right)
			(net 3 "TDO")
			(pinfunction "TDO")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "4" connect roundrect
			(at -1.905 -2.54)
			(size 3.81 1.905)
			(layers "B.Cu" "B.Mask")
			(roundrect_rratio 0.25)
			(chamfer_ratio 0)
			(chamfer top_right bottom_right)
			(net 31 "VCC")
			(pinfunction "VREF")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "5" connect roundrect
			(at -1.905 0)
			(size 3.81 1.905)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(chamfer_ratio 0)
			(chamfer top_right bottom_right)
			(net 4 "TMS")
			(pinfunction "TMS")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "6" connect roundrect
			(at -1.905 0)
			(size 3.81 1.905)
			(layers "B.Cu" "B.Mask")
			(roundrect_rratio 0.25)
			(chamfer_ratio 0)
			(chamfer top_right bottom_right)
			(net 34 "VPP")
			(pinfunction "VPP")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "7" connect roundrect
			(at -1.905 2.54)
			(size 3.81 1.905)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(chamfer_ratio 0)
			(chamfer top_right bottom_right)
			(net 35 "unconnected-(J2-nc-Pad7)")
			(pinfunction "nc")
			(pintype "passive+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "8" connect roundrect
			(at -1.905 2.54)
			(size 3.81 1.905)
			(layers "B.Cu" "B.Mask")
			(roundrect_rratio 0.25)
			(chamfer_ratio 0)
			(chamfer top_right bottom_right)
			(net 36 "unconnected-(J2-nc-Pad8)")
			(pinfunction "nc")
			(pintype "passive+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "9" connect roundrect
			(at -1.905 5.08)
			(size 3.81 1.905)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(chamfer_ratio 0)
			(chamfer top_right bottom_right)
			(net 2 "TDI")
			(pinfunction "TDI")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "10" connect roundrect
			(at -1.905 5.08)
			(size 3.81 1.905)
			(layers "B.Cu" "B.Mask")
			(roundrect_rratio 0.25)
			(chamfer_ratio 0)
			(chamfer top_right bottom_right)
			(net 10 "GND")
			(pinfunction "GND")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KIPRJMOD}/000_LOCAL.pretty/3dshapes/IDC-Header_2x05_P2.54mm_Vertical.step"
			(offset
				(xyz -0.2032 5.08 0.4318)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 -90 0)
			)
		)
	)
	(footprint "000_LOCAL:R_0805"
		(layer "F.Cu")
		(at 146.812 92.725 90)
		(descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
		(tags "resistor 0805")
		(property "Reference" "R1"
			(at 0.416597 1.016 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "2k2"
			(at -0.726403 1.016 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "ATF150x_uPRG.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -1.270001 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0 90)
			(size 0.7 1.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.1)
			(net 27 "Net-(JP2-Pad3)")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at 0.95 0 90)
			(size 0.7 1.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.1)
			(net 22 "+12V")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KIPRJMOD}/000_LOCAL.pretty/3dshapes/R_0805.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "000_LOCAL:Fiducial_0.5_1.0"
		(layer "F.Cu")
		(at 131.86 102.67)
		(descr "Circular Fiducial, 0.5mm bare copper, 1mm soldermask opening (Level C)")
		(tags "fiducial")
		(property "Reference" "REF**"
			(at 0 -1.5 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Fiducial_0.5_1.0"
			(at 0 1.5 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "" smd circle
			(at 0 0)
			(size 0.5 0.5)
			(layers "F.Cu" "F.Mask")
			(solder_mask_margin 0.25)
			(clearance 0.25)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
	)
	(footprint "000_LOCAL:Adafruit_2264"
		(layer "F.Cu")
		(at 146.05 95.251)
		(property "Reference" "J1"
			(at 8.89 -6.604 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Adafruit_2264"
			(at 4.445 0.381 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Adafruit FT232H Breakout v2"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "ATF150x_uPRG.kicad_sch")
		(fp_line
			(start -19.05 -8.89)
			(end -19.05 8.89)
			(layer "Edge.Cuts")
		)
		(fp_line
			(start -16.51 11.43)
			(end 16.51 11.43)
			(layer "Edge.Cuts")
		)
		(fp_line
			(start 16.51 -11.43)
			(end -16.51 -11.43)
			(layer "Edge.Cuts")
		)
		(fp_line
			(start 19.05 8.89)
			(end 19.05 -8.89)
			(layer "Edge.Cuts")
		)
		(fp_arc
			(start -19.05 -8.89)
			(mid -18.306051 -10.686051)
			(end -16.51 -11.43)
			(layer "Edge.Cuts")
		)
		(fp_arc
			(start -16.51 11.43)
			(mid -18.306051 10.686051)
			(end -19.05 8.89)
			(layer "Edge.Cuts")
		)
		(fp_arc
			(start 16.51 -11.43)
			(mid 18.306051 -10.686051)
			(end 19.05 -8.89)
			(layer "Edge.Cuts")
		)
		(fp_arc
			(start 19.05 8.89)
			(mid 18.306051 10.686051)
			(end 16.51 11.43)
			(layer "Edge.Cuts")
		)
		(pad "1" thru_hole circle
			(at -12.7 10.033)
			(size 1.6 1.6)
			(drill 0.94)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 24 "+3V3")
			(pinfunction "3V3")
			(pintype "power_out")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" thru_hole circle
			(at -10.16 10.287)
			(size 1.6 1.6)
			(drill 0.94)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 9 "+5V")
			(pinfunction "5V")
			(pintype "power_out")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "3" thru_hole circle
			(at -7.62 10.033)
			(size 1.6 1.6)
			(drill 0.94)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 10 "GND")
			(pinfunction "GND")
			(pintype "power_out")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "4" thru_hole circle
			(at -5.08 10.287)
			(size 1.6 1.6)
			(drill 0.94)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "TCK")
			(pinfunction "AD0")
			(pintype "bidirectional")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "5" thru_hole circle
			(at -2.54 10.033)
			(size 1.6 1.6)
			(drill 0.94)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "TDI")
			(pinfunction "AD1")
			(pintype "bidirectional")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "6" thru_hole circle
			(at 0 10.287)
			(size 1.6 1.6)
			(drill 0.94)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "TDO")
			(pinfunction "AD2")
			(pintype "bidirectional")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "7" thru_hole circle
			(at 2.54 10.033)
			(size 1.6 1.6)
			(drill 0.94)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "TMS")
			(pinfunction "AD3")
			(pintype "bidirectional")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "8" thru_hole circle
			(at 5.08 10.287)
			(size 1.6 1.6)
			(drill 0.94)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 8 "unconnected-(J1-AD4-Pad8)")
			(pinfunction "AD4")
			(pintype "bidirectional+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "9" thru_hole circle
			(at 7.62 10.033)
			(size 1.6 1.6)
			(drill 0.94)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 18 "unconnected-(J1-AD5-Pad9)")
			(pinfunction "AD5")
			(pintype "bidirectional+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "10" thru_hole circle
			(at 10.16 10.287)
			(size 1.6 1.6)
			(drill 0.94)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 11 "unconnected-(J1-AD6-Pad10)")
			(pinfunction "AD6")
			(pintype "bidirectional+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "11" thru_hole circle
			(at 12.7 10.033)
			(size 1.6 1.6)
			(drill 0.94)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 23 "unconnected-(J1-AD7-Pad11)")
			(pinfunction "AD7")
			(pintype "bidirectional+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "12" thru_hole circle
			(at 12.7 -10.287)
			(size 1.6 1.6)
			(drill 0.94)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 12 "unconnected-(J1-AC0-Pad12)")
			(pinfunction "AC0")
			(pintype "bidirectional+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "13" thru_hole circle
			(at 10.16 -10.033)
			(size 1.6 1.6)
			(drill 0.94)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 7 "unconnected-(J1-AC1-Pad13)")
			(pinfunction "AC1")
			(pintype "bidirectional+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "14" thru_hole circle
			(at 7.62 -10.287)
			(size 1.6 1.6)
			(drill 0.94)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 21 "unconnected-(J1-AC2-Pad14)")
			(pinfunction "AC2")
			(pintype "bidirectional+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "15" thru_hole circle
			(at 5.08 -10.033)
			(size 1.6 1.6)
			(drill 0.94)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 14 "unconnected-(J1-AC3-Pad15)")
			(pinfunction "AC3")
			(pintype "bidirectional+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "16" thru_hole circle
			(at 2.54 -10.287)
			(size 1.6 1.6)
			(drill 0.94)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 16 "unconnected-(J1-AC4-Pad16)")
			(pinfunction "AC4")
			(pintype "bidirectional+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "17" thru_hole circle
			(at 0 -10.033)
			(size 1.6 1.6)
			(drill 0.94)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 13 "unconnected-(J1-AC5-Pad17)")
			(pinfunction "AC5")
			(pintype "bidirectional+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "18" thru_hole circle
			(at -2.54 -10.287)
			(size 1.6 1.6)
			(drill 0.94)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 15 "unconnected-(J1-AC6-Pad18)")
			(pinfunction "AC6")
			(pintype "bidirectional+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "19" thru_hole circle
			(at -5.08 -10.033)
			(size 1.6 1.6)
			(drill 0.94)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 20 "unconnected-(J1-AC7-Pad19)")
			(pinfunction "AC7")
			(pintype "bidirectional+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "20" thru_hole circle
			(at -7.62 -10.287)
			(size 1.6 1.6)
			(drill 0.94)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 17 "unconnected-(J1-AC8-Pad20)")
			(pinfunction "AC8")
			(pintype "bidirectional+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "21" thru_hole circle
			(at -10.16 -10.033)
			(size 1.6 1.6)
			(drill 0.94)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 19 "unconnected-(J1-AC9-Pad21)")
			(pinfunction "AC9")
			(pintype "bidirectional+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "22" thru_hole circle
			(at -12.7 -10.287)
			(size 1.6 1.6)
			(drill 0.94)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 10 "GND")
			(pinfunction "GND")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "M" thru_hole circle
			(at -16.51 -8.89)
			(size 3.2 3.2)
			(drill 2.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 10 "GND")
			(pinfunction "M")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "M" thru_hole circle
			(at -16.51 8.89)
			(size 3.2 3.2)
			(drill 2.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 10 "GND")
			(pinfunction "M")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "M" thru_hole circle
			(at 16.51 -8.89)
			(size 3.2 3.2)
			(drill 2.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 10 "GND")
			(pinfunction "M")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "M" thru_hole circle
			(at 16.51 8.89)
			(size 3.2 3.2)
			(drill 2.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 10 "GND")
			(pinfunction "M")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KIPRJMOD}/000_LOCAL.pretty/3dshapes/Adafruit_2264.step"
			(offset
				(xyz 0 0 2.54)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
		(model "${KIPRJMOD}/000_LOCAL.pretty/3dshapes/PinHeader_1x11_P2.54mm_Vertical.step"
			(offset
				(xyz 12.7 -10.16 2.54)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 180 90)
			)
		)
		(model "${KIPRJMOD}/000_LOCAL.pretty/3dshapes/PinHeader_1x11_P2.54mm_Vertical.step"
			(offset
				(xyz 12.7 10.16 2.54)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 180 90)
			)
		)
	)
	(footprint "000_LOCAL:R_0805"
		(layer "F.Cu")
		(at 131.572 100.711)
		(descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
		(tags "resistor 0805")
		(property "Reference" "R4"
			(at -1.778 0 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "10k"
			(at -1.651 1.143 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "ATF150x_uPRG.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0)
			(size 0.7 1.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.1)
			(net 30 "Net-(LED3-A)")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at 0.95 0)
			(size 0.7 1.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.1)
			(net 9 "+5V")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KIPRJMOD}/000_LOCAL.pretty/3dshapes/R_0805.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "000_LOCAL:C_0805"
		(layer "F.Cu")
		(at 132.271997 89.448602 -90)
		(descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
		(tags "capacitor 0805")
		(property "Reference" "C6"
			(at -0.548602 1.842997 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "1u"
			(at 0.594398 1.842997 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "ATF150x_uPRG.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -1.270001 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9 0 270)
			(size 0.8 1.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.1)
			(net 33 "Net-(C6-Pad1)")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at 0.9 0 270)
			(size 0.8 1.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.1)
			(net 32 "Net-(C6-Pad2)")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KIPRJMOD}/000_LOCAL.pretty/3dshapes/C_0805.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "000_LOCAL:C_0805"
		(layer "F.Cu")
		(at 132.271997 92.923401 -90)
		(descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
		(tags "capacitor 0805")
		(property "Reference" "C7"
			(at -0.623401 1.921997 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "1u"
			(at 0.548599 1.842997 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "ATF150x_uPRG.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -1.270001 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9 0 270)
			(size 0.8 1.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.1)
			(net 5 "Net-(C7-Pad1)")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at 0.9 0 270)
			(size 0.8 1.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.1)
			(net 6 "Net-(C7-Pad2)")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KIPRJMOD}/000_LOCAL.pretty/3dshapes/C_0805.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "000_LOCAL:Fiducial_0.5_1.0"
		(layer "F.Cu")
		(at 160.38 102.43)
		(descr "Circular Fiducial, 0.5mm bare copper, 1mm soldermask opening (Level C)")
		(tags "fiducial")
		(property "Reference" "REF**"
			(at 0 -1.5 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Fiducial_0.5_1.0"
			(at 0 1.5 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "" smd circle
			(at 0 0)
			(size 0.5 0.5)
			(layers "F.Cu" "F.Mask")
			(solder_mask_margin 0.25)
			(clearance 0.25)
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
	)
	(footprint "000_LOCAL:C_0805"
		(layer "F.Cu")
		(at 144.45 90.825 90)
		(descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
		(tags "capacitor 0805")
		(property "Reference" "C5"
			(at 3.518599 0 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "1u"
			(at 2.418599 0 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "ATF150x_uPRG.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -1.270001 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9 0 90)
			(size 0.8 1.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.1)
			(net 22 "+12V")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at 0.9 0 90)
			(size 0.8 1.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.1)
			(net 10 "GND")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KIPRJMOD}/000_LOCAL.pretty/3dshapes/C_0805.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "000_LOCAL:C_0805"
		(layer "F.Cu")
		(at 140.649999 97.282)
		(descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
		(tags "capacitor 0805")
		(property "Reference" "C2"
			(at 2.650001 -0.532 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "1u"
			(at 2.650001 0.568 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "ATF150x_uPRG.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -1.270001 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9 0)
			(size 0.8 1.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.1)
			(net 9 "+5V")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at 0.9 0)
			(size 0.8 1.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.1)
			(net 10 "GND")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KIPRJMOD}/000_LOCAL.pretty/3dshapes/C_0805.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "000_LOCAL:C_0805"
		(layer "F.Cu")
		(at 140.649999 95.123)
		(descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
		(tags "capacitor 0805")
		(property "Reference" "C3"
			(at 2.650001 -0.623 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "1u"
			(at 2.650001 0.477 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "ATF150x_uPRG.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -1.270001 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9 0)
			(size 0.8 1.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.1)
			(net 9 "+5V")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at 0.9 0)
			(size 0.8 1.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.1)
			(net 10 "GND")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KIPRJMOD}/000_LOCAL.pretty/3dshapes/C_0805.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "000_LOCAL:R_0805"
		(layer "F.Cu")
		(at 131.572 98.298)
		(descr "Resistor SMD 0805, reflow soldering, Vishay (see dcrcw.pdf)")
		(tags "resistor 0805")
		(property "Reference" "R3"
			(at 1.905 -0.508 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "10k"
			(at 1.905 0.635 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "ATF150x_uPRG.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0)
			(size 0.7 1.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.1)
			(net 29 "Net-(LED2-A)")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at 0.95 0)
			(size 0.7 1.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.1)
			(net 34 "VPP")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KIPRJMOD}/000_LOCAL.pretty/3dshapes/R_0805.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "000_LOCAL:LED_0805"
		(layer "B.Cu")
		(at 128.778 99.06)
		(descr "LED SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "LED")
		(property "Reference" "LED3"
			(at 0 1.65 180)
			(unlocked yes)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "PWR"
			(at 1.524 0 0)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Light emitting diode"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "LED* LED_SMD:* LED_THT:*")
		(sheetname "Root")
		(sheetfile "ATF150x_uPRG.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9375 0)
			(size 0.975 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 10 "GND")
			(pinfunction "K")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at 0.9375 0)
			(size 0.975 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 30 "Net-(LED3-A)")
			(pinfunction "A")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KIPRJMOD}/000_LOCAL.pretty/3dshapes/LED_0805.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "000_LOCAL:LED_0805"
		(layer "B.Cu")
		(at 128.778 95.25)
		(descr "LED SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "LED")
		(property "Reference" "LED2"
			(at 0 1.65 180)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "VPP"
			(at 1.524 0 0)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Light emitting diode"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "LED* LED_SMD:* LED_THT:*")
		(sheetname "Root")
		(sheetfile "ATF150x_uPRG.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9375 0)
			(size 0.975 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 10 "GND")
			(pinfunction "K")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at 0.9375 0)
			(size 0.975 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 29 "Net-(LED2-A)")
			(pinfunction "A")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KIPRJMOD}/000_LOCAL.pretty/3dshapes/LED_0805.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "000_LOCAL:LED_0805"
		(layer "B.Cu")
		(at 128.778 91.44)
		(descr "LED SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "LED")
		(property "Reference" "LED1"
			(at 0 1.65 180)
			(unlocked yes)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "VCC"
			(at 1.524 0 0)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Light emitting diode"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "LED* LED_SMD:* LED_THT:*")
		(sheetname "Root")
		(sheetfile "ATF150x_uPRG.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9375 0)
			(size 0.975 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 10 "GND")
			(pinfunction "K")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" smd roundrect
			(at 0.9375 0)
			(size 0.975 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 28 "Net-(LED1-A)")
			(pinfunction "A")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KIPRJMOD}/000_LOCAL.pretty/3dshapes/LED_0805.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "000_LOCAL:PinHeader_1x03_P2.54mm_Horizontal"
		(layer "B.Cu")
		(at 154.94 101.854 90)
		(descr "Through hole angled pin header, 1x03, 2.54mm pitch, 6mm pin length, single row")
		(tags "Through hole angled pin header THT 1x03 2.54mm single row")
		(property "Reference" "JP2"
			(at 2.794 -2.54 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "VPP"
			(at 14.732 -2.54 0)
			(unlocked yes)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Jumper, 3-pole, pins 1+2 closed/bridged"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Jumper* TestPoint*3Pads* TestPoint*Bridge*")
		(sheetname "Root")
		(sheetfile "ATF150x_uPRG.kicad_sch")
		(attr through_hole exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 2.77 -2.54 0)
			(layer "B.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 90)
			(size 1.6 1.6)
			(drill 0.95)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 26 "unconnected-(JP2-Pad1)")
			(pintype "passive+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" thru_hole circle
			(at 0 -2.54 90)
			(size 1.6 1.6)
			(drill 0.95)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 34 "VPP")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "3" thru_hole circle
			(at 0 -5.079999 90)
			(size 1.6 1.6)
			(drill 0.95)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 27 "Net-(JP2-Pad3)")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KIPRJMOD}/000_LOCAL.pretty/3dshapes/PinHeader_1x03_P2.54mm_Horizontal.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
		(model "${KIPRJMOD}/000_LOCAL.pretty/3dshapes/jumper.step"
			(offset
				(xyz 4.064 0 1.27)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 90 0 90)
			)
		)
	)
	(footprint "000_LOCAL:PinHeader_1x04_P2.54mm_Horizontal"
		(layer "B.Cu")
		(at 142.24 101.854 90)
		(descr "Through hole angled pin header, 1x04, 2.54mm pitch, 6mm pin length, single row")
		(tags "Through hole angled pin header THT 1x04 2.54mm single row")
		(property "Reference" "JP1"
			(at 4.385 2.27 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "VCC"
			(at 14.732 -3.81 0)
			(unlocked yes)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Jumper, 4-pole, pins 1+2 closed/bridged"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Jumper* TestPoint*3Pads* TestPoint*Bridge*")
		(sheetname "Root")
		(sheetfile "ATF150x_uPRG.kicad_sch")
		(attr through_hole exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 2.77 -3.81 0)
			(layer "B.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0 90)
			(size 1.6 1.6)
			(drill 0.95)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 25 "unconnected-(JP1-Pad1)")
			(pintype "passive+no_connect")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "2" thru_hole circle
			(at 0 -2.54 90)
			(size 1.6 1.6)
			(drill 0.95)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 9 "+5V")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "3" thru_hole circle
			(at 0 -5.079999 90)
			(size 1.6 1.6)
			(drill 0.95)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 31 "VCC")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(pad "4" thru_hole circle
			(at 0 -7.62 90)
			(size 1.6 1.6)
			(drill 0.95)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 24 "+3V3")
			(pintype "passive")
			(teardrops
				(best_length_ratio 0.5)
				(max_length 1)
				(best_width_ratio 1)
				(max_width 2)
				(curved_edges yes)
				(filter_ratio 0.9)
				(enabled yes)
				(allow_two_segments yes)
				(prefer_zone_connections yes)
			)
		)
		(embedded_fonts no)
		(model "${KIPRJMOD}/000_LOCAL.pretty/3dshapes/PinHeader_1x04_P2.54mm_Horizontal.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
		(model "${KIPRJMOD}/000_LOCAL.pretty/3dshapes/jumper.step"
			(offset
				(xyz 4.064 0 1.27)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 90 0 90)
			)
		)
	)
	(gr_text "THIS SIDE\nFACE UP\n<-USB"
		(at 150.495 96.52 0)
		(layer "F.SilkS")
	)
	(gr_text "GND"
		(at 133.35 86.995 0)
		(layer "F.SilkS")
	)
	(gr_text "github.com/bkw777/\nATF150x_uPRG"
		(at 152.4 88.265 0)
		(layer "F.SilkS")
	)
	(gr_text "3V3"
		(at 133.477 104.013 90)
		(layer "F.SilkS")
	)
	(gr_text "5V"
		(at 135.89 104.013 90)
		(layer "F.SilkS")
	)
	(gr_text "GND"
		(at 138.43 104.013 90)
		(layer "F.SilkS")
	)
	(gr_text "TCK"
		(at 140.97 104.013 90)
		(layer "F.SilkS")
	)
	(gr_text "TDI"
		(at 143.51 104.013 90)
		(layer "F.SilkS")
	)
	(gr_text "TDO"
		(at 146.05 104.013 90)
		(layer "F.SilkS")
	)
	(gr_text "TMS"
		(at 148.59 104.013 90)
		(layer "F.SilkS")
	)
	(gr_text "TCK"
		(at 160.909 90.17 0)
		(layer "F.SilkS")
	)
	(gr_text "TDO"
		(at 160.909 92.71 0)
		(layer "F.SilkS")
	)
	(gr_text "TMS"
		(at 160.909 95.25 0)
		(layer "F.SilkS")
	)
	(gr_text "TDI"
		(at 160.909 100.33 0)
		(layer "F.SilkS")
	)
	(gr_text "USBC"
		(at 128.016 95.25 90)
		(layer "F.SilkS")
	)
	(gr_text "v${REVISION}"
		(at 160.655 102.743 0)
		(layer "B.SilkS")
	)
	(gr_text "3V3"
		(at 133.35 104.394 270)
		(layer "B.SilkS")
	)
	(gr_text "5V"
		(at 135.89 104.394 270)
		(layer "B.SilkS")
	)
	(gr_text "GND"
		(at 138.43 104.394 270)
		(layer "B.SilkS")
	)
	(gr_text "TCK"
		(at 140.97 104.394 270)
		(layer "B.SilkS")
	)
	(gr_text "TDI"
		(at 143.51 104.394 270)
		(layer "B.SilkS")
	)
	(gr_text "TDO"
		(at 146.05 104.394 270)
		(layer "B.SilkS")
	)
	(gr_text "TMS"
		(at 148.336 104.394 270)
		(layer "B.SilkS")
	)
	(gr_text "GND"
		(at 132.334 85.725 270)
		(layer "B.SilkS")
	)
	(gr_text "GND"
		(at 160.909 90.17 0)
		(layer "B.SilkS")
	)
	(gr_text "VCC"
		(at 160.909 92.71 0)
		(layer "B.SilkS")
	)
	(gr_text "VPP"
		(at 160.909 95.25 0)
		(layer "B.SilkS")
	)
	(gr_text "GND"
		(at 160.909 100.33 0)
		(layer "B.SilkS")
	)
	(gr_text "ATF150x_uPRG"
		(at 155.194 103.632 0)
		(layer "B.SilkS")
	)
	(gr_text "3V3"
		(at 134.62 90.805 270)
		(layer "B.SilkS")
	)
	(gr_text "VCC"
		(at 137.16 90.805 270)
		(layer "B.SilkS")
	)
	(gr_text "5V"
		(at 139.7 90.805 270)
		(layer "B.SilkS")
	)
	(gr_text "N/C"
		(at 142.24 90.805 270)
		(layer "B.SilkS")
	)
	(gr_text "12V"
		(at 149.86 90.805 270)
		(layer "B.SilkS")
	)
	(gr_text "VPP"
		(at 152.4 90.805 270)
		(layer "B.SilkS")
	)
	(gr_text "N/C"
		(at 154.94 90.805 270)
		(layer "B.SilkS")
	)
	(zone
		(net 33)
		(net_name "Net-(C6-Pad1)")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30016)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 133.414782 88.489666) (xy 133.302988 88.459452) (xy 133.245852 88.448273) (xy 133.124425 88.42319)
				(xy 133.011942 88.389084) (xy 132.9292 88.339206) (xy 132.905481 88.306243) (xy 132.896997 88.266807)
				(xy 132.271131 88.548103) (xy 132.233468 88.948602) (xy 132.382975 88.889764) (xy 132.541716 88.866854)
				(xy 132.713416 88.878705) (xy 132.902124 88.926283) (xy 133.104315 89.004851) (xy 133.114784 89.009281)
			)
		)
	)
	(zone
		(net 9)
		(net_name "+5V")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30019)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 140 98.307) (xy 139.992357 98.222247) (xy 139.981947 98.114839) (xy 139.987452 98.007799) (xy 140.00201 97.961645)
				(xy 140.027551 97.924256) (xy 140.066411 97.898524) (xy 140.120925 97.887338) (xy 139.749999 97.281)
				(xy 139.349999 97.827) (xy 139.382525 97.839365) (xy 139.407085 97.858979) (xy 139.436288 97.917903)
				(xy 139.442308 98.015045) (xy 139.418016 98.18028) (xy 139.4 98.307)
			)
		)
	)
	(zone
		(net 9)
		(net_name "+5V")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30022)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 139.4 96.257) (xy 139.418016 96.38372) (xy 139.436884 96.494554) (xy 139.442546 96.602425) (xy 139.435405 96.649603)
				(xy 139.418939 96.689264) (xy 139.39114 96.719149) (xy 139.349999 96.737) (xy 139.749999 97.283)
				(xy 140.120925 96.676661) (xy 140.078981 96.669899) (xy 140.045944 96.654758) (xy 140.003369 96.605201)
				(xy 139.982891 96.524158) (xy 139.985942 96.397862) (xy 139.992357 96.341753) (xy 140 96.257)
			)
		)
	)
	(zone
		(net 2)
		(net_name "TDI")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30037)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 158.895196 100.992) (xy 158.815664 100.987332) (xy 158.755069 100.974658) (xy 158.652813 100.926439)
				(xy 158.571184 100.883714) (xy 158.448773 100.846804) (xy 158.399 101.092) (xy 158.448773 101.337196)
				(xy 158.585415 101.293905) (xy 158.652813 101.257561) (xy 158.747709 101.211647) (xy 158.810872 101.197319)
				(xy 158.895196 101.192)
			)
		)
	)
	(zone
		(net 22)
		(net_name "+12V")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30013)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 145.475 91.525) (xy 145.400715 91.530603) (xy 145.294341 91.53866) (xy 145.187444 91.529835)
				(xy 145.141509 91.51301) (xy 145.104695 91.484669) (xy 145.080085 91.442377) (xy 145.070763 91.383704)
				(xy 144.449 91.725) (xy 144.429557 92.125) (xy 144.574485 92.077953) (xy 144.754458 92.058692) (xy 144.983774 92.069608)
				(xy 145.191995 92.096238) (xy 145.343724 92.116248) (xy 145.475 92.125)
			)
		)
	)
	(zone
		(net 4)
		(net_name "TMS")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30003)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 160.432906 94.588) (xy 160.559847 94.607388) (xy 160.709763 94.671096) (xy 160.871722 94.78405)
				(xy 160.951185 94.857957) (xy 161.025931 94.941516) (xy 161.092762 95.031572) (xy 161.151996 95.129225)
				(xy 161.199469 95.227449) (xy 161.237562 95.331051) (xy 161.263428 95.431561) (xy 161.279061 95.535613)
				(xy 161.28 95.710769) (xy 163.186 95.25) (xy 161.75625 94.2975) (xy 161.651147 94.330603) (xy 161.416504 94.362262)
				(xy 160.990319 94.383534) (xy 160.478206 94.388018) (xy 160.432906 94.388)
			)
		)
	)
	(zone
		(net 28)
		(net_name "Net-(LED1-A)")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30026)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 130.0155 95.156897) (xy 130.104809 95.273801) (xy 130.185176 95.446057) (xy 130.244841 95.670646)
				(xy 130.262921 95.797958) (xy 130.271458 95.931022) (xy 130.272 95.991161) (xy 130.622694 95.885719)
				(xy 130.607782 95.235) (xy 130.508433 95.229565) (xy 130.38946 95.186147) (xy 130.253882 95.100194)
				(xy 130.159448 95.018051)
			)
		)
	)
	(zone
		(net 1)
		(net_name "TCK")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30007)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 142.09079 104.417788) (xy 141.990975 104.510668) (xy 141.899365 104.582017) (xy 141.820603 104.631056)
				(xy 141.745584 104.666391) (xy 141.599942 104.704742) (xy 141.423863 104.714158) (xy 141.351316 104.713222)
				(xy 141.114706 104.715436) (xy 140.973945 104.727667) (xy 140.813928 104.753372) (xy 140.969293 105.538707)
				(xy 141.635176 105.982456) (xy 141.70524 105.869028) (xy 141.759562 105.763735) (xy 141.832902 105.565018)
				(xy 141.873406 105.361328) (xy 141.88352 105.284109) (xy 141.908673 105.116734) (xy 141.958214 104.947143)
				(xy 142.000079 104.858227) (xy 142.057581 104.76481) (xy 142.133898 104.665576) (xy 142.232212 104.55921)
			)
		)
	)
	(zone
		(net 9)
		(net_name "+5V")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30023)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 139.4 98.416) (xy 139.418016 98.54272) (xy 139.436884 98.653554) (xy 139.442546 98.761425) (xy 139.435405 98.808603)
				(xy 139.418939 98.848264) (xy 139.39114 98.878149) (xy 139.349999 98.896) (xy 139.749999 99.442)
				(xy 140.120925 98.835661) (xy 140.078981 98.828899) (xy 140.045944 98.813758) (xy 140.003369 98.764201)
				(xy 139.982891 98.683158) (xy 139.985942 98.556862) (xy 139.992357 98.500753) (xy 140 98.416)
			)
		)
	)
	(zone
		(net 1)
		(net_name "TCK")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30000)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 160.3275 90.27) (xy 160.497392 90.289344) (xy 160.723335 90.355972) (xy 160.850533 90.409171)
				(xy 160.977807 90.473413) (xy 161.099267 90.546108) (xy 161.214493 90.627643) (xy 161.311481 90.708958)
				(xy 161.398329 90.796253) (xy 161.464619 90.877674) (xy 161.519562 90.962789) (xy 161.573997 91.086248)
				(xy 163.186 90.17) (xy 161.573997 89.253752) (xy 161.508072 89.396995) (xy 161.39718 89.545023)
				(xy 161.236618 89.694984) (xy 161.026893 89.838652) (xy 160.781605 89.960994) (xy 160.655468 90.007966)
				(xy 160.534569 90.042404) (xy 160.427746 90.062651) (xy 160.331527 90.069986) (xy 160.3275 90.07)
			)
		)
	)
	(zone
		(net 9)
		(net_name "+5V")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30004)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 139.4 100.269372) (xy 139.395183 100.416808) (xy 139.381465 100.543337) (xy 139.360366 100.65064)
				(xy 139.332769 100.74422) (xy 139.256054 100.914512) (xy 139.180851 101.041488) (xy 139.108574 101.162556)
				(xy 139.03725 101.303132) (xy 138.971358 101.476996) (xy 138.915372 101.697928) (xy 139.7 101.855)
				(xy 140.484628 101.697928) (xy 140.4513 101.554563) (xy 140.413505 101.43133) (xy 140.32257 101.219993)
				(xy 140.219149 101.041489) (xy 140.135695 100.899257) (xy 140.06583 100.74016) (xy 140.038582 100.646318)
				(xy 140.017838 100.538697) (xy 140.004632 100.414111) (xy 140 100.269372)
			)
		)
	)
	(zone
		(net 3)
		(net_name "TDO")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30009)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 146.585 104.216397) (xy 146.580097 104.311219) (xy 146.565777 104.390381) (xy 146.545056 104.450245)
				(xy 146.517461 104.499858) (xy 146.44498 104.572402) (xy 146.339741 104.624281) (xy 146.139063 104.67491)
				(xy 146.014657 104.702441) (xy 145.882573 104.739611) (xy 145.745355 104.79391) (xy 145.605544 104.872824)
				(xy 146.05 105.539) (xy 146.834628 105.381928) (xy 146.792638 105.145539) (xy 146.772086 104.967697)
				(xy 146.769698 104.71384) (xy 146.773722 104.627267) (xy 146.785 104.216397)
			)
		)
	)
	(zone
		(net 30)
		(net_name "Net-(LED3-A)")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30038)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 130.289196 100.103) (xy 130.209664 100.098332) (xy 130.149069 100.085658) (xy 130.046813 100.037439)
				(xy 129.965184 99.994714) (xy 129.842773 99.957804) (xy 129.793 100.203) (xy 129.842773 100.448196)
				(xy 129.979415 100.404905) (xy 130.046813 100.368561) (xy 130.141709 100.322647) (xy 130.204872 100.308319)
				(xy 130.289196 100.303)
			)
		)
	)
	(zone
		(net 22)
		(net_name "+12V")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30015)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 143.425 92.125) (xy 143.613793 92.109216) (xy 143.708005 92.096238) (xy 143.898863 92.071441)
				(xy 144.096729 92.058437) (xy 144.290843 92.071523) (xy 144.38313 92.092319) (xy 144.470443 92.125)
				(xy 144.451 91.725) (xy 143.829236 91.383704) (xy 143.824011 91.42848) (xy 143.810103 91.464077)
				(xy 143.762718 91.510686) (xy 143.685219 91.534962) (xy 143.565469 91.53665) (xy 143.499284 91.530603)
				(xy 143.425 91.525)
			)
		)
	)
	(zone
		(net 31)
		(net_name "VCC")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30005)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 136.860001 100.269372) (xy 136.855184 100.416808) (xy 136.841466 100.543337) (xy 136.820367 100.65064)
				(xy 136.79277 100.74422) (xy 136.716055 100.914512) (xy 136.640852 101.041488) (xy 136.568575 101.162556)
				(xy 136.497251 101.303132) (xy 136.431359 101.476996) (xy 136.375373 101.697928) (xy 137.160001 101.855)
				(xy 137.944629 101.697928) (xy 137.911301 101.554563) (xy 137.873506 101.43133) (xy 137.782571 101.219993)
				(xy 137.67915 101.041489) (xy 137.595696 100.899257) (xy 137.525831 100.74016) (xy 137.498583 100.646318)
				(xy 137.477839 100.538697) (xy 137.464633 100.414111) (xy 137.460001 100.269372)
			)
		)
	)
	(zone
		(net 30)
		(net_name "Net-(LED3-A)")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30029)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 129.922 100.303) (xy 130.006657 100.32235) (xy 130.093674 100.383568) (xy 130.175659 100.491642)
				(xy 130.21077 100.563419) (xy 130.239025 100.644517) (xy 130.259223 100.733877) (xy 130.270257 100.830754)
				(xy 130.272 100.888878) (xy 130.623 100.711) (xy 130.326706 100.064041) (xy 130.296864 100.089976)
				(xy 130.214715 100.106793) (xy 130.001999 100.105686) (xy 129.922 100.103)
			)
		)
	)
	(zone
		(net 22)
		(net_name "+12V")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30018)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 145.812 92.125) (xy 145.992432 92.109216) (xy 146.081855 92.096237) (xy 146.26319 92.071441)
				(xy 146.452722 92.058437) (xy 146.64179 92.071523) (xy 146.733443 92.092319) (xy 146.821732 92.125)
				(xy 146.813 91.775) (xy 146.175206 91.456421) (xy 146.169052 91.494617) (xy 146.154555 91.522847)
				(xy 146.108204 91.553516) (xy 146.030297 91.560134) (xy 145.904322 91.539678) (xy 145.812 91.525)
			)
		)
	)
	(zone
		(net 34)
		(net_name "VPP")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30006)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 152.1 100.269372) (xy 152.095183 100.416808) (xy 152.081465 100.543337) (xy 152.060366 100.65064)
				(xy 152.032769 100.74422) (xy 151.956054 100.914512) (xy 151.880851 101.041488) (xy 151.808574 101.162556)
				(xy 151.73725 101.303132) (xy 151.671358 101.476996) (xy 151.615372 101.697928) (xy 152.4 101.855)
				(xy 153.184628 101.697928) (xy 153.1513 101.554563) (xy 153.113505 101.43133) (xy 153.02257 101.219993)
				(xy 152.919149 101.041489) (xy 152.835695 100.899257) (xy 152.76583 100.74016) (xy 152.738582 100.646318)
				(xy 152.717838 100.538697) (xy 152.704632 100.414111) (xy 152.7 100.269372)
			)
		)
	)
	(zone
		(net 2)
		(net_name "TDI")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30002)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 160.432906 101.192) (xy 160.478206 101.191982) (xy 160.802488 101.19322) (xy 161.183609 101.20298)
				(xy 161.53154 101.229871) (xy 161.664924 101.25243) (xy 161.75625 101.2825) (xy 163.186 100.33)
				(xy 161.28 99.86923) (xy 161.277397 100.060303) (xy 161.236775 100.25147) (xy 161.157948 100.439667)
				(xy 161.042093 100.618231) (xy 160.894817 100.775863) (xy 160.813037 100.842322) (xy 160.729366 100.897683)
				(xy 160.647144 100.940339) (xy 160.566233 100.97073) (xy 160.432906 100.992)
			)
		)
	)
	(zone
		(net 34)
		(net_name "VPP")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30035)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 134.251804 97.89) (xy 134.331336 97.894668) (xy 134.391931 97.907342) (xy 134.494187 97.955561)
				(xy 134.575815 97.998285) (xy 134.698227 98.035196) (xy 134.748 97.79) (xy 134.698227 97.544804)
				(xy 134.561585 97.588094) (xy 134.494186 97.624439) (xy 134.39929 97.670353) (xy 134.336128 97.684681)
				(xy 134.251804 97.69)
			)
		)
	)
	(zone
		(net 2)
		(net_name "TDI")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30034)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 145.008554 103.925867) (xy 145.068092 103.87293) (xy 145.119901 103.839045) (xy 145.226304 103.800835)
				(xy 145.314235 103.773326) (xy 145.426893 103.712867) (xy 145.288707 103.504293) (xy 145.080133 103.366107)
				(xy 145.014123 103.493338) (xy 144.992164 103.566697) (xy 144.957529 103.666264) (xy 144.922998 103.721059)
				(xy 144.867133 103.784446)
			)
		)
	)
	(zone
		(net 9)
		(net_name "+5V")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30033)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 134.274439 99.699988) (xy 134.344692 99.690852) (xy 134.399737 99.693385) (xy 134.481981 99.722165)
				(xy 134.514378 99.740397) (xy 134.58975 99.779824) (xy 134.698227 99.813196) (xy 134.74798 99.567805)
				(xy 134.698227 99.322804) (xy 134.611142 99.344754) (xy 134.546306 99.369657) (xy 134.466821 99.413318)
				(xy 134.376273 99.461912) (xy 134.235419 99.503832)
			)
		)
	)
	(zone
		(net 9)
		(net_name "+5V")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30020)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 140 96.148) (xy 139.992357 96.063247) (xy 139.981947 95.955839) (xy 139.987452 95.848799) (xy 140.00201 95.802645)
				(xy 140.027551 95.765256) (xy 140.066411 95.739524) (xy 140.120925 95.728338) (xy 139.749999 95.122)
				(xy 139.349999 95.668) (xy 139.382525 95.680365) (xy 139.407085 95.699979) (xy 139.436288 95.758903)
				(xy 139.442308 95.856045) (xy 139.418016 96.02128) (xy 139.4 96.148)
			)
		)
	)
	(zone
		(net 34)
		(net_name "VPP")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30030)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 133.222 97.69) (xy 133.142001 97.692686) (xy 132.941523 97.694719) (xy 132.859862 97.681689)
				(xy 132.832439 97.668954) (xy 132.817293 97.651041) (xy 132.521 98.298) (xy 132.872 98.475878) (xy 132.890652 98.289716)
				(xy 132.913456 98.20382) (xy 132.943742 98.126467) (xy 132.980965 98.057578) (xy 133.02354 97.999279)
				(xy 133.068847 97.953684) (xy 133.116993 97.919732) (xy 133.16306 97.899426) (xy 133.20977 97.890413)
				(xy 133.222 97.89)
			)
		)
	)
	(zone
		(net 2)
		(net_name "TDI")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30008)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 144.55929 104.092288) (xy 144.446344 104.198231) (xy 144.345059 104.278779) (xy 144.262335 104.331992)
				(xy 144.183714 104.37093) (xy 144.029508 104.41657) (xy 143.80339 104.441806) (xy 143.603562 104.460174)
				(xy 143.353928 104.499372) (xy 143.509293 105.284707) (xy 144.294628 105.440072) (xy 144.339574 105.136223)
				(xy 144.352052 104.989141) (xy 144.371312 104.79676) (xy 144.388774 104.709586) (xy 144.416334 104.624083)
				(xy 144.457651 104.536999) (xy 144.516381 104.445078) (xy 144.596182 104.345066) (xy 144.700712 104.23371)
			)
		)
	)
	(zone
		(net 22)
		(net_name "+12V")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30014)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 143.175 91.525) (xy 143.100715 91.530603) (xy 142.994341 91.53866) (xy 142.887444 91.529835)
				(xy 142.841509 91.51301) (xy 142.804695 91.484669) (xy 142.780085 91.442377) (xy 142.770763 91.383704)
				(xy 142.149 91.725) (xy 142.129557 92.125) (xy 142.274485 92.077953) (xy 142.454458 92.058692) (xy 142.683774 92.069608)
				(xy 142.891995 92.096238) (xy 143.043724 92.116248) (xy 143.175 92.125)
			)
		)
	)
	(zone
		(net 22)
		(net_name "+12V")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30025)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 141.125 92.121) (xy 141.273694 92.093222) (xy 141.379667 92.068888) (xy 141.480525 92.056445)
				(xy 141.5242 92.059195) (xy 141.560793 92.070335) (xy 141.588372 92.091668) (xy 141.605 92.125)
				(xy 142.151 91.725) (xy 141.529697 91.381386) (xy 141.524426 91.425949) (xy 141.510481 91.461346)
				(xy 141.463041 91.507605) (xy 141.385398 91.531555) (xy 141.26528 91.532852) (xy 141.20001 91.526756)
				(xy 141.125 91.521)
			)
		)
	)
	(zone
		(net 29)
		(net_name "Net-(LED2-A)")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30040)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 129.865749 97.472167) (xy 129.80067 97.433599) (xy 129.757278 97.3961) (xy 129.710473 97.321553)
				(xy 129.697302 97.290532) (xy 129.667998 97.224483) (xy 129.620867 97.143107) (xy 129.41211 97.281546)
				(xy 129.364227 97.527196) (xy 129.47656 97.547989) (xy 129.611107 97.57787) (xy 129.774942 97.650363)
			)
		)
	)
	(zone
		(net 28)
		(net_name "Net-(LED1-A)")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30039)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 129.8155 93.205196) (xy 129.820168 93.125664) (xy 129.832842 93.065069) (xy 129.881061 92.962813)
				(xy 129.923785 92.881184) (xy 129.960696 92.758773) (xy 129.7155 92.709) (xy 129.470304 92.758773)
				(xy 129.513594 92.895415) (xy 129.549939 92.962813) (xy 129.595853 93.057709) (xy 129.610181 93.120872)
				(xy 129.6155 93.205196)
			)
		)
	)
	(zone
		(net 6)
		(net_name "Net-(C7-Pad2)")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30017)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 133.114777 93.36274) (xy 133.104326 93.367162) (xy 132.927774 93.437013) (xy 132.824835 93.468993)
				(xy 132.714453 93.493141) (xy 132.598378 93.505057) (xy 132.478357 93.50034) (xy 132.356141 93.474588)
				(xy 132.233477 93.423401) (xy 132.271131 93.823901) (xy 132.896997 94.105204) (xy 132.901815 94.075033)
				(xy 132.915542 94.048611) (xy 132.971462 94.002075) (xy 133.081324 93.95985) (xy 133.245845 93.923746)
				(xy 133.341187 93.904333) (xy 133.414781 93.882351)
			)
		)
	)
	(zone
		(net 31)
		(net_name "VCC")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30036)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 134.251804 95.604) (xy 134.331336 95.608668) (xy 134.391931 95.621342) (xy 134.494187 95.669561)
				(xy 134.575815 95.712285) (xy 134.698227 95.749196) (xy 134.748 95.504) (xy 134.698227 95.258804)
				(xy 134.561585 95.302094) (xy 134.494186 95.338439) (xy 134.39929 95.384353) (xy 134.336128 95.398681)
				(xy 134.251804 95.404)
			)
		)
	)
	(zone
		(net 31)
		(net_name "VCC")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30031)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 133.209159 95.404) (xy 133.106335 95.406742) (xy 132.981824 95.391292) (xy 132.927823 95.371991)
				(xy 132.888315 95.342455) (xy 132.874529 95.319535) (xy 132.869421 95.292034) (xy 132.521 95.885)
				(xy 132.872 96.09073) (xy 132.890472 95.943837) (xy 132.943901 95.810801) (xy 133.027097 95.700865)
				(xy 133.076454 95.658824) (xy 133.127619 95.628007) (xy 133.209159 95.604)
			)
		)
	)
	(zone
		(net 29)
		(net_name "Net-(LED2-A)")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30027)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 129.915618 97.702365) (xy 130.005769 97.739574) (xy 130.093985 97.819398) (xy 130.175082 97.947698)
				(xy 130.238062 98.124291) (xy 130.25869 98.227704) (xy 130.270169 98.337863) (xy 130.272 98.440125)
				(xy 130.622951 98.298309) (xy 130.476166 97.648) (xy 130.39889 97.640839) (xy 130.176391 97.572814)
				(xy 129.977428 97.512157)
			)
		)
	)
	(zone
		(net 9)
		(net_name "+5V")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30021)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 140 100.466) (xy 139.992357 100.381247) (xy 139.981947 100.273839) (xy 139.987452 100.166799)
				(xy 140.00201 100.120645) (xy 140.027551 100.083256) (xy 140.066411 100.057524) (xy 140.120925 100.046338)
				(xy 139.749999 99.44) (xy 139.349999 99.986) (xy 139.382525 99.998365) (xy 139.407085 100.017979)
				(xy 139.436288 100.076903) (xy 139.442308 100.174045) (xy 139.418016 100.33928) (xy 139.4 100.466)
			)
		)
	)
	(zone
		(net 27)
		(net_name "Net-(JP2-Pad3)")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30028)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 147.112 94.375) (xy 147.094167 94.278765) (xy 147.075219 94.192566) (xy 147.069425 94.110506)
				(xy 147.076516 94.0762) (xy 147.092961 94.049135) (xy 147.120782 94.031378) (xy 147.162 94.025)
				(xy 146.812 93.674) (xy 146.462 94.025) (xy 146.498386 94.029779) (xy 146.524602 94.043231) (xy 146.550912 94.08743)
				(xy 146.552883 94.16471) (xy 146.529833 94.278765) (xy 146.512 94.375)
			)
		)
	)
	(zone
		(net 3)
		(net_name "TDO")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30001)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 160.3275 92.81) (xy 160.497392 92.829344) (xy 160.723335 92.895972) (xy 160.850533 92.949171)
				(xy 160.977807 93.013413) (xy 161.099267 93.086108) (xy 161.214493 93.167643) (xy 161.311481 93.248958)
				(xy 161.398329 93.336253) (xy 161.464619 93.417674) (xy 161.519562 93.502789) (xy 161.573997 93.626248)
				(xy 163.186 92.71) (xy 161.573997 91.793752) (xy 161.508072 91.936995) (xy 161.39718 92.085023)
				(xy 161.236618 92.234984) (xy 161.026893 92.378652) (xy 160.781605 92.500994) (xy 160.655468 92.547966)
				(xy 160.534569 92.582404) (xy 160.427746 92.602651) (xy 160.331527 92.609986) (xy 160.3275 92.61)
			)
		)
	)
	(zone
		(net 9)
		(net_name "+5V")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30024)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 139.4 94.098) (xy 139.418016 94.22472) (xy 139.436884 94.335554) (xy 139.442546 94.443425) (xy 139.435405 94.490603)
				(xy 139.418939 94.530264) (xy 139.39114 94.560149) (xy 139.349999 94.578) (xy 139.749999 95.124)
				(xy 140.120925 94.517661) (xy 140.078981 94.510899) (xy 140.045944 94.495758) (xy 140.003369 94.446201)
				(xy 139.982891 94.365158) (xy 139.985942 94.238862) (xy 139.992357 94.182753) (xy 140 94.098)
			)
		)
	)
	(zone
		(net 32)
		(net_name "Net-(C6-Pad2)")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30011)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 133.296997 90.251001) (xy 133.241278 90.253363) (xy 133.132563 90.256474) (xy 133.020319 90.240181)
				(xy 132.971604 90.218118) (xy 132.932484 90.183235) (xy 132.906451 90.132876) (xy 132.896997 90.064384)
				(xy 132.270998 90.348602) (xy 132.23192 90.748602) (xy 132.381911 90.723144) (xy 132.572111 90.728539)
				(xy 132.823945 90.769859) (xy 132.937402 90.794134) (xy 133.13112 90.83365) (xy 133.296996 90.851)
			)
		)
	)
	(zone
		(net 5)
		(net_name "Net-(C7-Pad1)")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30012)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 133.296997 91.521) (xy 133.133275 91.537977) (xy 132.937399 91.577867) (xy 132.758582 91.615132)
				(xy 132.5762 91.643034) (xy 132.398048 91.649736) (xy 132.312993 91.641438) (xy 132.23192 91.623401)
				(xy 132.270998 92.023401) (xy 132.896997 92.307618) (xy 132.901792 92.257272) (xy 132.915359 92.216349)
				(xy 132.962517 92.160027) (xy 133.0379 92.1269) (xy 133.150356 92.115274) (xy 133.241278 92.118638)
				(xy 133.296996 92.120999)
			)
		)
	)
	(zone
		(net 4)
		(net_name "TMS")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30010)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 147.855 103.962397) (xy 147.866277 104.373266) (xy 147.872615 104.53381) (xy 147.869551 104.68978)
				(xy 147.849625 104.876158) (xy 147.805372 105.127928) (xy 148.59 105.285) (xy 149.034456 104.618824)
				(xy 148.863487 104.525827) (xy 148.671236 104.460079) (xy 148.500936 104.42091) (xy 148.322087 104.377556)
				(xy 148.246118 104.348031) (xy 148.180926 104.307955) (xy 148.127865 104.253342) (xy 148.088287 104.180203)
				(xy 148.063547 104.08455) (xy 148.055 103.962397)
			)
		)
	)
	(zone
		(net 9)
		(net_name "+5V")
		(layer "F.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30032)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 133.079063 100.10196) (xy 133.030099 100.104632) (xy 132.89627 100.106541) (xy 132.838208 100.092912)
				(xy 132.802 100.061) (xy 132.52102 100.711195) (xy 132.872 100.867954) (xy 132.876934 100.738592)
				(xy 132.89147 100.621941) (xy 132.913205 100.526827) (xy 132.94255 100.446027) (xy 132.974027 100.388634)
				(xy 133.010816 100.344371) (xy 133.046143 100.317849) (xy 133.085035 100.302262) (xy 133.118086 100.298115)
			)
		)
	)
	(zone
		(net 10)
		(net_name "GND")
		(layers "F.Cu" "B.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0.2032)
		)
		(min_thickness 0.2032)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.2032)
			(thermal_bridge_width 0.4064)
			(smoothing fillet)
			(radius 0.1016)
		)
		(polygon
			(pts
				(xy 165.1 106.68) (xy 127 106.68) (xy 127 83.82) (xy 165.1 83.82)
			)
		)
	)
	(zone
		(net 24)
		(net_name "+3V3")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30004)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 133.802366 103.121411) (xy 133.857319 103.024301) (xy 133.913365 102.945396) (xy 133.967694 102.885529)
				(xy 134.023345 102.838433) (xy 134.14068 102.775014) (xy 134.282443 102.739412) (xy 134.42387 102.723106)
				(xy 134.565949 102.70726) (xy 134.719227 102.676979) (xy 134.884973 102.618779) (xy 135.064456 102.519176)
				(xy 134.620454 101.85311) (xy 133.954824 101.409544) (xy 133.826383 101.610334) (xy 133.730994 101.777046)
				(xy 133.606724 102.044893) (xy 133.545303 102.207589) (xy 133.440743 102.478147) (xy 133.26777 102.849003)
			)
		)
	)
	(zone
		(net 28)
		(net_name "Net-(LED1-A)")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30007)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 129.8155 92.6275) (xy 129.835119 92.481032) (xy 129.863207 92.384663) (xy 129.903046 92.286321)
				(xy 129.949346 92.199902) (xy 130.00478 92.121477) (xy 130.056949 92.06625) (xy 130.114895 92.022084)
				(xy 130.184446 91.989529) (xy 129.7155 91.439) (xy 129.246554 91.989529) (xy 129.341826 92.039636)
				(xy 129.433922 92.131046) (xy 129.519328 92.268392) (xy 129.586404 92.444258) (xy 129.607061 92.536247)
				(xy 129.615349 92.616594) (xy 129.6155 92.6275)
			)
		)
	)
	(zone
		(net 2)
		(net_name "TDI")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30011)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 158.120554 101.512867) (xy 158.180092 101.45993) (xy 158.231901 101.426045) (xy 158.338304 101.387835)
				(xy 158.426235 101.360326) (xy 158.538893 101.299867) (xy 158.400707 101.091293) (xy 158.192133 100.953107)
				(xy 158.126123 101.080338) (xy 158.104164 101.153697) (xy 158.069529 101.253264) (xy 158.034998 101.308059)
				(xy 157.979133 101.371446)
			)
		)
	)
	(zone
		(net 30)
		(net_name "Net-(LED3-A)")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30009)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 129.894 100.203) (xy 129.914088 100.041048) (xy 129.942003 99.938242) (xy 129.981996 99.835731)
				(xy 130.024191 99.757212) (xy 130.074732 99.689269) (xy 130.119972 99.646639) (xy 130.17034 99.615523)
				(xy 130.184446 99.609529) (xy 129.7155 99.059) (xy 129.299393 99.688607) (xy 129.404429 99.722499)
				(xy 129.503227 99.793658) (xy 129.592913 99.903799) (xy 129.662621 100.046222) (xy 129.684256 100.121286)
				(xy 129.69363 100.188536) (xy 129.694 100.203)
			)
		)
	)
	(zone
		(net 24)
		(net_name "+3V3")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30002)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 133.05 103.699372) (xy 133.045183 103.846808) (xy 133.031465 103.973337) (xy 133.010366 104.08064)
				(xy 132.982769 104.17422) (xy 132.906054 104.344512) (xy 132.830851 104.471488) (xy 132.758574 104.592556)
				(xy 132.68725 104.733132) (xy 132.621358 104.906996) (xy 132.565372 105.127928) (xy 133.35 105.285)
				(xy 134.134628 105.127928) (xy 134.1013 104.984563) (xy 134.063505 104.86133) (xy 133.97257 104.649993)
				(xy 133.869149 104.471489) (xy 133.785695 104.329257) (xy 133.71583 104.17016) (xy 133.688582 104.076318)
				(xy 133.667838 103.968697) (xy 133.654632 103.844111) (xy 133.65 103.699372)
			)
		)
	)
	(zone
		(net 9)
		(net_name "+5V")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30006)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 138.855829 103.122387) (xy 138.959089 103.028872) (xy 139.054243 102.955573) (xy 139.141707 102.90005)
				(xy 139.224227 102.858282) (xy 139.393696 102.800748) (xy 139.519293 102.77283) (xy 139.650927 102.743646)
				(xy 139.794694 102.7003) (xy 139.957051 102.629806) (xy 140.144456 102.519176) (xy 139.700717 101.853304)
				(xy 139.034824 101.409544) (xy 138.964203 101.523747) (xy 138.909894 101.628608) (xy 138.835742 101.826623)
				(xy 138.789709 102.032572) (xy 138.757372 102.184827) (xy 138.703479 102.338488) (xy 138.661178 102.419111)
				(xy 138.604763 102.504005) (xy 138.531325 102.594474) (xy 138.437957 102.691827)
			)
		)
	)
	(zone
		(net 31)
		(net_name "VCC")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30016)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 136.664805 95.604) (xy 136.744337 95.608668) (xy 136.804932 95.621342) (xy 136.907188 95.669561)
				(xy 136.988816 95.712285) (xy 137.111228 95.749196) (xy 137.161001 95.504) (xy 137.111228 95.258804)
				(xy 136.974586 95.302094) (xy 136.907187 95.338439) (xy 136.812291 95.384353) (xy 136.749129 95.398681)
				(xy 136.664805 95.404)
			)
		)
	)
	(zone
		(net 31)
		(net_name "VCC")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30001)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 160.359077 92.375) (xy 160.522104 92.395023) (xy 160.62032 92.42249) (xy 160.721864 92.461663)
				(xy 160.820814 92.510933) (xy 160.917318 92.571285) (xy 161.000681 92.635845) (xy 161.077668 92.709611)
				(xy 161.139501 92.783498) (xy 161.19307 92.864792) (xy 161.233263 92.944946) (xy 161.26432 93.031211)
				(xy 161.284036 93.116963) (xy 161.293987 93.208018) (xy 161.294959 93.261457) (xy 163.186 92.71)
				(xy 161.75625 91.7575) (xy 161.66662 91.79836) (xy 161.509515 91.82582) (xy 161.253121 91.831887)
				(xy 160.75503 91.799727) (xy 160.359077 91.775)
			)
		)
	)
	(zone
		(net 9)
		(net_name "+5V")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30005)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 136.325181 103.975555) (xy 136.018123 104.26067) (xy 135.85054 104.399164) (xy 135.703814 104.520883)
				(xy 135.562508 104.655823) (xy 135.408789 104.836028) (xy 135.224824 105.093544) (xy 135.889293 105.538707)
				(xy 136.674628 105.694072) (xy 136.695411 105.497208) (xy 136.679851 105.312908) (xy 136.631302 105.120475)
				(xy 136.614321 105.066717) (xy 136.568079 104.90471) (xy 136.556008 104.826399) (xy 136.55608 104.747818)
				(xy 136.571878 104.667418) (xy 136.606983 104.583651) (xy 136.664978 104.494968) (xy 136.749445 104.399819)
			)
		)
	)
	(zone
		(net 31)
		(net_name "VCC")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30017)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 135.242196 95.404) (xy 135.162664 95.399332) (xy 135.102069 95.386658) (xy 134.999813 95.338439)
				(xy 134.918184 95.295714) (xy 134.795773 95.258804) (xy 134.746 95.504) (xy 134.795773 95.749196)
				(xy 134.932415 95.705905) (xy 134.999813 95.669561) (xy 135.094709 95.623647) (xy 135.157872 95.609319)
				(xy 135.242196 95.604)
			)
		)
	)
	(zone
		(net 2)
		(net_name "TDI")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30020)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 145.702425 103.6) (xy 145.651805 103.595159) (xy 145.615808 103.581273) (xy 145.575851 103.536893)
				(xy 145.552585 103.482606) (xy 145.529959 103.42745) (xy 145.495867 103.366107) (xy 145.287 103.505)
				(xy 145.239227 103.750196) (xy 145.289296 103.760203) (xy 145.482944 103.793638) (xy 145.702425 103.8)
			)
		)
	)
	(zone
		(net 27)
		(net_name "Net-(JP2-Pad3)")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30003)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 149.560001 100.269372) (xy 149.555184 100.416808) (xy 149.541466 100.543337) (xy 149.520367 100.65064)
				(xy 149.49277 100.74422) (xy 149.416055 100.914512) (xy 149.340852 101.041488) (xy 149.268575 101.162556)
				(xy 149.197251 101.303132) (xy 149.131359 101.476996) (xy 149.075373 101.697928) (xy 149.860001 101.855)
				(xy 150.644629 101.697928) (xy 150.611301 101.554563) (xy 150.573506 101.43133) (xy 150.482571 101.219993)
				(xy 150.37915 101.041489) (xy 150.295696 100.899257) (xy 150.225831 100.74016) (xy 150.198583 100.646318)
				(xy 150.177839 100.538697) (xy 150.164633 100.414111) (xy 150.160001 100.269372)
			)
		)
	)
	(zone
		(net 30)
		(net_name "Net-(LED3-A)")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30013)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 129.694 99.707804) (xy 129.689332 99.787336) (xy 129.676658 99.847931) (xy 129.628439 99.950186)
				(xy 129.585714 100.031815) (xy 129.548804 100.154227) (xy 129.794 100.204) (xy 130.039196 100.154227)
				(xy 129.995905 100.017584) (xy 129.959561 99.950187) (xy 129.913647 99.855291) (xy 129.899319 99.792128)
				(xy 129.894 99.707804)
			)
		)
	)
	(zone
		(net 34)
		(net_name "VPP")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30000)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 160.359077 96.185) (xy 160.75503 96.160273) (xy 161.049549 96.13756) (xy 161.33885 96.127111)
				(xy 161.470173 96.131133) (xy 161.586546 96.143799) (xy 161.683421 96.166968) (xy 161.75625 96.2025)
				(xy 163.186 95.25) (xy 161.294959 94.698542) (xy 161.278417 94.872627) (xy 161.225425 95.032649)
				(xy 161.136883 95.179989) (xy 161.012519 95.313826) (xy 160.853493 95.43012) (xy 160.667166 95.520806)
				(xy 160.474173 95.574499) (xy 160.359077 95.585)
			)
		)
	)
	(zone
		(net 9)
		(net_name "+5V")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30012)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 139.420554 98.769667) (xy 139.480092 98.71673) (xy 139.531901 98.682845) (xy 139.638304 98.644635)
				(xy 139.726235 98.617126) (xy 139.838893 98.556667) (xy 139.700707 98.348093) (xy 139.492133 98.209907)
				(xy 139.426123 98.337138) (xy 139.404164 98.410497) (xy 139.369529 98.510064) (xy 139.334998 98.564859)
				(xy 139.279133 98.628246)
			)
		)
	)
	(zone
		(net 34)
		(net_name "VPP")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30018)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 135.242196 97.69) (xy 135.162664 97.685332) (xy 135.102069 97.672658) (xy 134.999813 97.624439)
				(xy 134.918184 97.581714) (xy 134.795773 97.544804) (xy 134.746 97.79) (xy 134.795773 98.035196)
				(xy 134.932415 97.991905) (xy 134.999813 97.955561) (xy 135.094709 97.909647) (xy 135.157872 97.895319)
				(xy 135.242196 97.89)
			)
		)
	)
	(zone
		(net 29)
		(net_name "Net-(LED2-A)")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30014)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 129.313 96.786804) (xy 129.308332 96.866336) (xy 129.295658 96.926931) (xy 129.247439 97.029186)
				(xy 129.204714 97.110815) (xy 129.167804 97.233227) (xy 129.413 97.283) (xy 129.658196 97.233227)
				(xy 129.614905 97.096584) (xy 129.578561 97.029187) (xy 129.532647 96.934291) (xy 129.518319 96.871128)
				(xy 129.513 96.786804)
			)
		)
	)
	(zone
		(net 28)
		(net_name "Net-(LED1-A)")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30015)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 129.6155 92.214804) (xy 129.610832 92.294336) (xy 129.598158 92.354931) (xy 129.549939 92.457186)
				(xy 129.507214 92.538815) (xy 129.470304 92.661227) (xy 129.7155 92.711) (xy 129.960696 92.661227)
				(xy 129.917405 92.524584) (xy 129.881061 92.457187) (xy 129.835147 92.362291) (xy 129.820819 92.299128)
				(xy 129.8155 92.214804)
			)
		)
	)
	(zone
		(net 34)
		(net_name "VPP")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30010)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 151.979133 98.780554) (xy 152.032069 98.840092) (xy 152.065954 98.891901) (xy 152.104164 98.998303)
				(xy 152.131674 99.086234) (xy 152.192133 99.198893) (xy 152.400707 99.060707) (xy 152.538893 98.852133)
				(xy 152.411662 98.786123) (xy 152.338303 98.764164) (xy 152.238735 98.729529) (xy 152.183941 98.694998)
				(xy 152.120554 98.639133)
			)
		)
	)
	(zone
		(net 29)
		(net_name "Net-(LED2-A)")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30008)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 129.513 96.425814) (xy 129.532372 96.320707) (xy 129.597819 96.190887) (xy 129.647171 96.126754)
				(xy 129.706403 96.067502) (xy 129.76918 96.019522) (xy 129.839187 95.980147) (xy 129.907321 95.954006)
				(xy 129.980364 95.937941) (xy 130.042934 95.933354) (xy 129.7155 95.249) (xy 129.228 95.70625) (xy 129.264661 95.781662)
				(xy 129.295137 95.933828) (xy 129.311675 96.191083) (xy 129.313066 96.387567) (xy 129.313 96.425814)
			)
		)
	)
	(zone
		(net 9)
		(net_name "+5V")
		(layer "B.Cu")
		(name "$teardrop_padvia$")
		(hatch none 0.1)
		(priority 30019)
		(attr
			(teardrop
				(type padvia)
			)
		)
		(connect_pads yes
			(clearance 0)
		)
		(min_thickness 0.0254)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 135.242196 99.468) (xy 135.162664 99.463332) (xy 135.102069 99.450658) (xy 134.999813 99.402439)
				(xy 134.918184 99.359714) (xy 134.795773 99.322804) (xy 134.746 99.568) (xy 134.795773 99.813196)
				(xy 134.932415 99.769905) (xy 134.999813 99.733561) (xy 135.094709 99.687647) (xy 135.157872 99.673319)
				(xy 135.242196 99.668)
			)
		)
	)
	(embedded_fonts no)
)
