(kicad_pcb
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(general
		(thickness 1.6)
		(legacy_teardrops no)
	)
	(paper "A4")
	(layers
		(0 "F.Cu" signal)
		(2 "B.Cu" signal)
		(9 "F.Adhes" user "F.Adhesive")
		(11 "B.Adhes" user "B.Adhesive")
		(13 "F.Paste" user)
		(15 "B.Paste" user)
		(5 "F.SilkS" user "F.Silkscreen")
		(7 "B.SilkS" user "B.Silkscreen")
		(1 "F.Mask" user)
		(3 "B.Mask" user)
		(17 "Dwgs.User" user "User.Drawings")
		(19 "Cmts.User" user "User.Comments")
		(21 "Eco1.User" user "User.Eco1")
		(23 "Eco2.User" user "User.Eco2")
		(25 "Edge.Cuts" user)
		(27 "Margin" user)
		(31 "F.CrtYd" user "F.Courtyard")
		(29 "B.CrtYd" user "B.Courtyard")
		(35 "F.Fab" user)
		(33 "B.Fab" user)
		(39 "User.1" user)
		(41 "User.2" user)
		(43 "User.3" user)
		(45 "User.4" user)
	)
	(setup
		(stackup
			(layer "F.SilkS"
				(type "Top Silk Screen")
			)
			(layer "F.Paste"
				(type "Top Solder Paste")
			)
			(layer "F.Mask"
				(type "Top Solder Mask")
				(thickness 0.01)
			)
			(layer "F.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "dielectric 1"
				(type "core")
				(thickness 1.51)
				(material "FR4")
				(epsilon_r 4.5)
				(loss_tangent 0.02)
			)
			(layer "B.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "B.Mask"
				(type "Bottom Solder Mask")
				(thickness 0.01)
			)
			(layer "B.Paste"
				(type "Bottom Solder Paste")
			)
			(layer "B.SilkS"
				(type "Bottom Silk Screen")
			)
			(copper_finish "None")
			(dielectric_constraints no)
		)
		(pad_to_mask_clearance 0.0508)
		(allow_soldermask_bridges_in_footprints no)
		(tenting front back)
		(pcbplotparams
			(layerselection 0x00000000_00000000_55555555_5755f5ff)
			(plot_on_all_layers_selection 0x00000000_00000000_00000000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 4)
			(plotframeref no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(pdf_metadata yes)
			(pdf_single_document no)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plot_black_and_white yes)
			(sketchpadsonfab no)
			(plotpadnumbers no)
			(hidednponfab no)
			(sketchdnponfab yes)
			(crossoutdnponfab yes)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 1)
			(scaleselection 1)
			(outputdirectory "")
		)
	)
	(net 0 "")
	(net 1 "/GPIO_0")
	(net 2 "/SWCLK")
	(net 3 "/VDD")
	(net 4 "/RST")
	(net 5 "/GND")
	(net 6 "/GPIO_1")
	(net 7 "/SWDIO")
	(net 8 "unconnected-(U1-TRACEDATA3{slash}P0.14-Pad28)")
	(net 9 "unconnected-(U1-P0.17-Pad31)")
	(net 10 "unconnected-(U1-P0.07-Pad20)")
	(net 11 "/GPIO_2")
	(net 12 "unconnected-(U1-P0.26-Pad3)")
	(net 13 "unconnected-(U1-P0.27-Pad4)")
	(net 14 "unconnected-(U1-DEC4-Pad9)")
	(net 15 "unconnected-(U1-P0.24-Pad40)")
	(net 16 "unconnected-(U1-NFC1{slash}P0.09-Pad22)")
	(net 17 "unconnected-(U1-DCC-Pad10)")
	(net 18 "unconnected-(U1-P0.19-Pad33)")
	(net 19 "unconnected-(U1-P0.08-Pad21)")
	(net 20 "unconnected-(U1-P0.01{slash}XL2-Pad14)")
	(net 21 "unconnected-(U1-P0.06-Pad19)")
	(net 22 "unconnected-(U1-P0.25-Pad2)")
	(net 23 "unconnected-(U1-P0.11-Pad25)")
	(net 24 "unconnected-(U1-P0.13-Pad27)")
	(net 25 "/GPIO_3")
	(net 26 "unconnected-(U1-P0.23-Pad41)")
	(net 27 "unconnected-(U1-TRACEDATA2{slash}P0.15-Pad29)")
	(net 28 "unconnected-(U1-AIN6{slash}P0.30-Pad7)")
	(net 29 "unconnected-(U1-P0.00{slash}XL1-Pad13)")
	(net 30 "unconnected-(U1-TRACECLK{slash}P0.20-Pad34)")
	(net 31 "unconnected-(U1-AIN5{slash}P0.29-Pad6)")
	(net 32 "unconnected-(U1-AIN7{slash}P0.31-Pad8)")
	(net 33 "unconnected-(U1-TRACEDATA1{slash}P0.16-Pad30)")
	(net 34 "unconnected-(U1-P0.22-Pad38)")
	(net 35 "unconnected-(U1-P0.12-Pad26)")
	(net 36 "unconnected-(U1-AIN4{slash}P0.28-Pad5)")
	(net 37 "unconnected-(U1-NFC2{slash}P0.10-Pad23)")
	(net 38 "unconnected-(U1-TRACEDATA0{slash}P0.18-Pad32)")
	(footprint "Connector_PinHeader_1.27mm:PinHeader_1x06_P1.27mm_Vertical"
		(layer "F.Cu")
		(at 135.5 93.025)
		(descr "Through hole straight pin header, 1x06, 1.27mm pitch, single row")
		(tags "Through hole pin header THT 1x06 1.27mm single row")
		(property "Reference" "J2"
			(at -0.372 -2.855 0)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_01x06_Pin"
			(at 0 8.095 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x06, script generated"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "/")
		(sheetfile "mu.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1 1)
			(drill 0.65)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "/GPIO_1")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 0 1.27)
			(size 1 1)
			(drill 0.65)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 25 "/GPIO_3")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole circle
			(at 0 2.54)
			(size 1 1)
			(drill 0.65)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 11 "/GPIO_2")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole circle
			(at 0 3.81)
			(size 1 1)
			(drill 0.65)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "/GPIO_0")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(pad "5" thru_hole circle
			(at 0 5.08)
			(size 1 1)
			(drill 0.65)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "/GND")
			(pinfunction "Pin_5")
			(pintype "passive")
		)
		(pad "6" thru_hole circle
			(at 0 6.35)
			(size 1 1)
			(drill 0.65)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "/VDD")
			(pinfunction "Pin_6")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_PinHeader_1.27mm.3dshapes/PinHeader_1x06_P1.27mm_Vertical.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_PinHeader_1.27mm:PinHeader_1x07_P1.27mm_Vertical"
		(layer "F.Cu")
		(at 149.75 93.025)
		(descr "Through hole straight pin header, 1x07, 1.27mm pitch, single row")
		(tags "Through hole pin header THT 1x07 1.27mm single row")
		(property "Reference" "J3"
			(at 0.11 -2.855 0)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_01x07_Pin"
			(at 0 9.365 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x07, script generated"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "/")
		(sheetfile "mu.kicad_sch")
		(attr through_hole)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1 1)
			(drill 0.65)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "/GND")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 0 1.27)
			(size 1 1)
			(drill 0.65)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "/GND")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole circle
			(at 0 2.54)
			(size 1 1)
			(drill 0.65)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "/VDD")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole circle
			(at 0 3.81)
			(size 1 1)
			(drill 0.65)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "/GND")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(pad "5" thru_hole circle
			(at 0 5.08)
			(size 1 1)
			(drill 0.65)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 7 "/SWDIO")
			(pinfunction "Pin_5")
			(pintype "passive")
		)
		(pad "6" thru_hole circle
			(at 0 6.35)
			(size 1 1)
			(drill 0.65)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "/SWCLK")
			(pinfunction "Pin_6")
			(pintype "passive")
		)
		(pad "7" thru_hole circle
			(at 0 7.62)
			(size 1 1)
			(drill 0.65)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "/RST")
			(pinfunction "Pin_7")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_PinHeader_1.27mm.3dshapes/PinHeader_1x07_P1.27mm_Vertical.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "RF_Module:Raytac_MDBT42Q"
		(layer "F.Cu")
		(at 142.612 96.032)
		(descr "Multiprotocol radio SoC module https://www.raytac.com/download/index.php?index_id=27")
		(tags "wireless 2.4 GHz Bluetooth ble zigbee 802.15.4 thread nordic raytac nrf52832")
		(property "Reference" "U1"
			(at -0.118 -7.64 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "MDBT42Q-512K"
			(at -0.02 9.6 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.raytac.com/download/index.php?index_id=27"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Multiprotocol BLE/ANT/2.4 GHz/802.15.4 Cortex-M4F SoC, nRF52832 module, ceramic antenna"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Raytac?MDBT42Q*")
		(sheetname "/")
		(sheetfile "mu.kicad_sch")
		(attr smd)
		(fp_text_box "No Ground-Pad Area"
			(start -0.5 -4.2)
			(end 3.9 -1.1)
			(margins 0.35 0.35 0.35 0.35)
			(layer "Dwgs.User")
			(border yes)
		)
		(fp_text_box "KEEP-OUT AREA"
			(start -6 -9)
			(end 6 -4.2)
			(margins 0.35 0.35 0.35 0.35)
			(layer "Dwgs.User")
			(border yes)
		)
		(pad "1" smd rect
			(at -4.6 -3.8)
			(size 1.4 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 5 "/GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "2" smd rect
			(at -4.6 -0.8)
			(size 1.4 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 22 "unconnected-(U1-P0.25-Pad2)")
			(pinfunction "P0.25")
			(pintype "bidirectional")
		)
		(pad "3" smd rect
			(at -4.6 -0.1)
			(size 1.4 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 12 "unconnected-(U1-P0.26-Pad3)")
			(pinfunction "P0.26")
			(pintype "bidirectional")
		)
		(pad "4" smd rect
			(at -4.6 0.6)
			(size 1.4 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 13 "unconnected-(U1-P0.27-Pad4)")
			(pinfunction "P0.27")
			(pintype "bidirectional")
		)
		(pad "5" smd rect
			(at -4.6 1.3)
			(size 1.4 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 36 "unconnected-(U1-AIN4{slash}P0.28-Pad5)")
			(pinfunction "AIN4/P0.28")
			(pintype "bidirectional")
		)
		(pad "6" smd rect
			(at -4.6 2)
			(size 1.4 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 31 "unconnected-(U1-AIN5{slash}P0.29-Pad6)")
			(pinfunction "AIN5/P0.29")
			(pintype "bidirectional")
		)
		(pad "7" smd rect
			(at -4.6 2.7)
			(size 1.4 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 28 "unconnected-(U1-AIN6{slash}P0.30-Pad7)")
			(pinfunction "AIN6/P0.30")
			(pintype "bidirectional")
		)
		(pad "8" smd rect
			(at -4.6 3.4)
			(size 1.4 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 32 "unconnected-(U1-AIN7{slash}P0.31-Pad8)")
			(pinfunction "AIN7/P0.31")
			(pintype "bidirectional")
		)
		(pad "9" smd rect
			(at -4.6 4.1)
			(size 1.4 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 14 "unconnected-(U1-DEC4-Pad9)")
			(pinfunction "DEC4")
			(pintype "power_out")
		)
		(pad "10" smd rect
			(at -4.6 4.8)
			(size 1.4 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 17 "unconnected-(U1-DCC-Pad10)")
			(pinfunction "DCC")
			(pintype "power_out")
		)
		(pad "11" smd rect
			(at -4.6 5.5)
			(size 1.4 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 3 "/VDD")
			(pinfunction "VDD")
			(pintype "power_in")
		)
		(pad "12" smd rect
			(at -4.2 7.6 90)
			(size 1.4 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 5 "/GND")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "13" smd rect
			(at -3.5 7.6 90)
			(size 1.4 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 29 "unconnected-(U1-P0.00{slash}XL1-Pad13)")
			(pinfunction "P0.00/XL1")
			(pintype "bidirectional")
		)
		(pad "14" smd rect
			(at -2.8 7.6 90)
			(size 1.4 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 20 "unconnected-(U1-P0.01{slash}XL2-Pad14)")
			(pinfunction "P0.01/XL2")
			(pintype "bidirectional")
		)
		(pad "15" smd rect
			(at -2.1 7.6 90)
			(size 1.4 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "/GPIO_0")
			(pinfunction "AIN0/P0.02")
			(pintype "bidirectional")
		)
		(pad "16" smd rect
			(at -1.4 7.6 90)
			(size 1.4 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 6 "/GPIO_1")
			(pinfunction "AIN1/P0.03")
			(pintype "bidirectional")
		)
		(pad "17" smd rect
			(at -0.7 7.6 90)
			(size 1.4 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 11 "/GPIO_2")
			(pinfunction "AIN2/P0.04")
			(pintype "bidirectional")
		)
		(pad "18" smd rect
			(at 0 7.6 90)
			(size 1.4 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 25 "/GPIO_3")
			(pinfunction "AIN3/P0.05")
			(pintype "bidirectional")
		)
		(pad "19" smd rect
			(at 0.7 7.6 90)
			(size 1.4 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 21 "unconnected-(U1-P0.06-Pad19)")
			(pinfunction "P0.06")
			(pintype "bidirectional")
		)
		(pad "20" smd rect
			(at 1.4 7.6 90)
			(size 1.4 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 10 "unconnected-(U1-P0.07-Pad20)")
			(pinfunction "P0.07")
			(pintype "bidirectional")
		)
		(pad "21" smd rect
			(at 2.1 7.6 90)
			(size 1.4 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 19 "unconnected-(U1-P0.08-Pad21)")
			(pinfunction "P0.08")
			(pintype "bidirectional")
		)
		(pad "22" smd rect
			(at 2.8 7.6 90)
			(size 1.4 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 16 "unconnected-(U1-NFC1{slash}P0.09-Pad22)")
			(pinfunction "NFC1/P0.09")
			(pintype "bidirectional")
		)
		(pad "23" smd rect
			(at 3.5 7.6 90)
			(size 1.4 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 37 "unconnected-(U1-NFC2{slash}P0.10-Pad23)")
			(pinfunction "NFC2/P0.10")
			(pintype "bidirectional")
		)
		(pad "24" smd rect
			(at 4.2 7.6 90)
			(size 1.4 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 5 "/GND")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "25" smd rect
			(at 4.6 6.2)
			(size 1.4 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 23 "unconnected-(U1-P0.11-Pad25)")
			(pinfunction "P0.11")
			(pintype "bidirectional")
		)
		(pad "26" smd rect
			(at 4.6 5.5)
			(size 1.4 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 35 "unconnected-(U1-P0.12-Pad26)")
			(pinfunction "P0.12")
			(pintype "bidirectional")
		)
		(pad "27" smd rect
			(at 4.6 4.8)
			(size 1.4 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 24 "unconnected-(U1-P0.13-Pad27)")
			(pinfunction "P0.13")
			(pintype "bidirectional")
		)
		(pad "28" smd rect
			(at 4.6 4.1)
			(size 1.4 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 8 "unconnected-(U1-TRACEDATA3{slash}P0.14-Pad28)")
			(pinfunction "TRACEDATA3/P0.14")
			(pintype "bidirectional")
		)
		(pad "29" smd rect
			(at 4.6 3.4)
			(size 1.4 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 27 "unconnected-(U1-TRACEDATA2{slash}P0.15-Pad29)")
			(pinfunction "TRACEDATA2/P0.15")
			(pintype "bidirectional")
		)
		(pad "30" smd rect
			(at 4.6 2.7)
			(size 1.4 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 33 "unconnected-(U1-TRACEDATA1{slash}P0.16-Pad30)")
			(pinfunction "TRACEDATA1/P0.16")
			(pintype "bidirectional")
		)
		(pad "31" smd rect
			(at 4.6 2)
			(size 1.4 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 9 "unconnected-(U1-P0.17-Pad31)")
			(pinfunction "P0.17")
			(pintype "bidirectional")
		)
		(pad "32" smd rect
			(at 4.6 1.3)
			(size 1.4 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 38 "unconnected-(U1-TRACEDATA0{slash}P0.18-Pad32)")
			(pinfunction "TRACEDATA0/P0.18")
			(pintype "bidirectional")
		)
		(pad "33" smd rect
			(at 4.6 0.6)
			(size 1.4 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 18 "unconnected-(U1-P0.19-Pad33)")
			(pinfunction "P0.19")
			(pintype "bidirectional")
		)
		(pad "34" smd rect
			(at 4.6 -0.1)
			(size 1.4 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 30 "unconnected-(U1-TRACECLK{slash}P0.20-Pad34)")
			(pinfunction "TRACECLK/P0.20")
			(pintype "bidirectional")
		)
		(pad "35" smd rect
			(at 4.6 -0.8)
			(size 1.4 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 4 "/RST")
			(pinfunction "P0.21/~{RESET}")
			(pintype "bidirectional")
		)
		(pad "36" smd rect
			(at 4.6 -1.5)
			(size 1.4 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "/SWCLK")
			(pinfunction "SWDCLK")
			(pintype "input")
		)
		(pad "37" smd rect
			(at 4.6 -2.2)
			(size 1.4 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 7 "/SWDIO")
			(pinfunction "SWDIO")
			(pintype "bidirectional")
		)
		(pad "38" smd rect
			(at 4.6 -2.9)
			(size 1.4 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 34 "unconnected-(U1-P0.22-Pad38)")
			(pinfunction "P0.22")
			(pintype "bidirectional")
		)
		(pad "39" smd rect
			(at 4.6 -3.8)
			(size 1.4 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 5 "/GND")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "40" smd rect
			(at 2.9 -3.25)
			(size 1 0.4)
			(layers "B.Cu")
			(net 15 "unconnected-(U1-P0.24-Pad40)")
			(pinfunction "P0.24")
			(pintype "bidirectional")
		)
		(pad "41" smd rect
			(at 2.9 -1.85)
			(size 1 0.4)
			(layers "B.Cu")
			(net 26 "unconnected-(U1-P0.23-Pad41)")
			(pinfunction "P0.23")
			(pintype "bidirectional")
		)
		(zone
			(net 0)
			(net_name "")
			(layers "F.Cu" "B.Cu" "Dwgs.User")
			(hatch full 0.5)
			(connect_pads
				(clearance 0)
			)
			(min_thickness 0.25)
			(filled_areas_thickness no)
			(keepout
				(tracks not_allowed)
				(vias not_allowed)
				(pads not_allowed)
				(copperpour not_allowed)
				(footprints not_allowed)
			)
			(placement
				(enabled no)
				(sheetname "")
			)
			(fill
				(thermal_gap 0.5)
				(thermal_bridge_width 0.5)
			)
			(polygon
				(pts
					(xy 136.612 87.032) (xy 136.612 91.832) (xy 148.612 91.832) (xy 148.612 87.032)
				)
			)
		)
		(zone
			(net 0)
			(net_name "")
			(layers "F.Cu" "Dwgs.User")
			(hatch full 0.5)
			(connect_pads
				(clearance 0)
			)
			(min_thickness 0.25)
			(filled_areas_thickness no)
			(keepout
				(tracks not_allowed)
				(vias not_allowed)
				(pads not_allowed)
				(copperpour not_allowed)
				(footprints not_allowed)
			)
			(placement
				(enabled no)
				(sheetname "")
			)
			(fill
				(thermal_gap 0.5)
				(thermal_bridge_width 0.5)
			)
			(polygon
				(pts
					(xy 142.112 91.832) (xy 142.112 94.932) (xy 146.512 94.932) (xy 146.512 91.832)
				)
			)
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/RF_Module.3dshapes/Raytac_MDBT42Q.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(gr_rect
		(start 133.096 86.36)
		(end 152.146 106.172)
		(fill no)
		(layer "Edge.Cuts")
	)
	(zone
		(net 5)
		(net_name "/GND")
		(layers "F.Cu" "B.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 133.604 86.868) (xy 133.604 105.664) (xy 151.638 105.664) (xy 151.638 91.694) (xy 146.812 91.694)
				(xy 146.812 95.25) (xy 141.732 95.25) (xy 141.732 91.44) (xy 146.812 91.44) (xy 146.812 91.694)
				(xy 151.638 91.694) (xy 151.638 86.868)
			)
		)
	)
	(embedded_fonts no)
)
