(kicad_pcb
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(general
		(thickness 1.6)
		(legacy_teardrops no)
	)
	(paper "A4")
	(layers
		(0 "F.Cu" signal)
		(2 "B.Cu" signal)
		(9 "F.Adhes" user "F.Adhesive")
		(11 "B.Adhes" user "B.Adhesive")
		(13 "F.Paste" user)
		(15 "B.Paste" user)
		(5 "F.SilkS" user "F.Silkscreen")
		(7 "B.SilkS" user "B.Silkscreen")
		(1 "F.Mask" user)
		(3 "B.Mask" user)
		(17 "Dwgs.User" user "User.Drawings")
		(19 "Cmts.User" user "User.Comments")
		(21 "Eco1.User" user "User.Eco1")
		(23 "Eco2.User" user "User.Eco2")
		(25 "Edge.Cuts" user)
		(27 "Margin" user)
		(31 "F.CrtYd" user "F.Courtyard")
		(29 "B.CrtYd" user "B.Courtyard")
		(35 "F.Fab" user)
		(33 "B.Fab" user)
		(39 "User.1" user)
		(41 "User.2" user)
		(43 "User.3" user)
		(45 "User.4" user)
	)
	(setup
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(tenting front back)
		(pcbplotparams
			(layerselection 0x00000000_00000000_55555555_5755f5ff)
			(plot_on_all_layers_selection 0x00000000_00000000_00000000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 4)
			(plotframeref no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(pdf_metadata yes)
			(pdf_single_document no)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plot_black_and_white yes)
			(sketchpadsonfab no)
			(plotpadnumbers no)
			(hidednponfab no)
			(sketchdnponfab yes)
			(crossoutdnponfab yes)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 0)
			(scaleselection 1)
			(outputdirectory "")
		)
	)
	(net 0 "")
	(net 1 "Net-(D1-K)")
	(net 2 "GND")
	(net 3 "Net-(IC2-RAMP)")
	(net 4 "Net-(IC2-SS)")
	(net 5 "+24V")
	(net 6 "Net-(D2-K)")
	(net 7 "Net-(IC2-SW)")
	(net 8 "/Power Supply/VCC")
	(net 9 "+5V")
	(net 10 "Net-(IC2-FB)")
	(net 11 "Net-(IC2-COMP)")
	(net 12 "Net-(C10-Pad2)")
	(net 13 "+12V")
	(net 14 "+5.5V")
	(net 15 "+3.3V")
	(net 16 "Net-(U3-VI+)")
	(net 17 "GNDA")
	(net 18 "Net-(C17-Pad1)")
	(net 19 "+12VA")
	(net 20 "Net-(U2-ENN)")
	(net 21 "Net-(Q3-D)")
	(net 22 "Net-(U2-CP)")
	(net 23 "Net-(U2-CN)")
	(net 24 "-12V")
	(net 25 "Net-(U2-VREF)")
	(net 26 "Net-(U2-VNEG)")
	(net 27 "Net-(U2-FBP)")
	(net 28 "/0-10V INPUTS/AIN0")
	(net 29 "/0-10V INPUTS/AIN1")
	(net 30 "/0-10V INPUTS/AIN2")
	(net 31 "/0-10V INPUTS/AIN3")
	(net 32 "Net-(Q4-B)")
	(net 33 "Net-(U6D--)")
	(net 34 "Net-(RN2A-R1.1)")
	(net 35 "/4-20mA Inputs/AIN3")
	(net 36 "Net-(U6C--)")
	(net 37 "Net-(Q7-B)")
	(net 38 "Net-(RN2C-R3.1)")
	(net 39 "/4-20mA Inputs/AIN2")
	(net 40 "Net-(Q6-B)")
	(net 41 "Net-(U6B--)")
	(net 42 "Net-(RN3A-R1.1)")
	(net 43 "/4-20mA Inputs/AIN1")
	(net 44 "Net-(Q5-B)")
	(net 45 "Net-(U6A--)")
	(net 46 "Net-(RN3C-R3.1)")
	(net 47 "/4-20mA Inputs/AIN0")
	(net 48 "Net-(C46-Pad1)")
	(net 49 "Net-(IC4-IN1+)")
	(net 50 "Net-(C48-Pad1)")
	(net 51 "Net-(IC4-IN2+)")
	(net 52 "Net-(C52-Pad1)")
	(net 53 "Net-(C53-Pad1)")
	(net 54 "Net-(IC5-IN1+)")
	(net 55 "Net-(IC5-IN2+)")
	(net 56 "Net-(RN5A-R1.1)")
	(net 57 "Net-(IC6-IN1+)")
	(net 58 "Net-(RN5C-R3.1)")
	(net 59 "Net-(IC6-IN2+)")
	(net 60 "/O_CHECK1")
	(net 61 "/O_CHECK2")
	(net 62 "/O_CHECK4")
	(net 63 "Net-(RN8C-R3.1)")
	(net 64 "/O_CHECK3")
	(net 65 "Net-(RN8A-R1.1)")
	(net 66 "Net-(IC7-IN2+)")
	(net 67 "Net-(IC7-IN1+)")
	(net 68 "Net-(D3-A)")
	(net 69 "Net-(D4-K)")
	(net 70 "/4-20mA Inputs/IN1N")
	(net 71 "/4-20mA Inputs/IN1P")
	(net 72 "/4-20mA Inputs/IN2N")
	(net 73 "/4-20mA Inputs/IN2P")
	(net 74 "/4-20mA Inputs/IN3N")
	(net 75 "/4-20mA Inputs/IN3P")
	(net 76 "/4-20mA Inputs/IN4P")
	(net 77 "/4-20mA Inputs/IN4N")
	(net 78 "Net-(D9-K)")
	(net 79 "/DigitalIO/VEX4")
	(net 80 "Net-(D10-K)")
	(net 81 "/DigitalIO/VEX3")
	(net 82 "/DigitalIO/VEX2")
	(net 83 "Net-(D11-K)")
	(net 84 "Net-(D12-K)")
	(net 85 "/DigitalIO/VEX1")
	(net 86 "Net-(D13-A)")
	(net 87 "Net-(D14-A)")
	(net 88 "Net-(D15-A)")
	(net 89 "Net-(D16-A)")
	(net 90 "/Communication/RS485B")
	(net 91 "/Communication/RS485A")
	(net 92 "/DigitalIO/OP2")
	(net 93 "Net-(HY1-ANODE_4)")
	(net 94 "/DigitalIO/OP1")
	(net 95 "Net-(HY1-ANODE_3)")
	(net 96 "/DigitalIO/OP3")
	(net 97 "/OPTO_IN3")
	(net 98 "Net-(HY1-ANODE_1)")
	(net 99 "/OPTO_IN4")
	(net 100 "Net-(HY1-ANODE_2)")
	(net 101 "/OPTO_IN1")
	(net 102 "/OPTO_IN2")
	(net 103 "/DigitalIO/OP4")
	(net 104 "/OD2")
	(net 105 "Net-(HY2-ANODE_2)")
	(net 106 "Net-(HY2-ANODE_4)")
	(net 107 "/OD4")
	(net 108 "Net-(HY2-EMITTER_2)")
	(net 109 "/OD3")
	(net 110 "Net-(HY2-EMITTER_4)")
	(net 111 "Net-(HY2-ANODE_3)")
	(net 112 "Net-(HY2-EMITTER_3)")
	(net 113 "Net-(HY2-EMITTER_1)")
	(net 114 "Net-(HY2-ANODE_1)")
	(net 115 "/OD1")
	(net 116 "unconnected-(IC1-NC_1-Pad5)")
	(net 117 "Net-(IC1-ADJ)")
	(net 118 "unconnected-(IC1-NC_2-Pad8)")
	(net 119 "Net-(IC2-RT{slash}SYNC)")
	(net 120 "Net-(IC2-CSG)")
	(net 121 "Net-(IC2-EN)")
	(net 122 "Net-(IC2-LO)")
	(net 123 "Net-(IC2-CS)")
	(net 124 "Net-(IC2-HO)")
	(net 125 "Net-(IC2-UVLO)")
	(net 126 "/0-10V INPUTS/-IN_A")
	(net 127 "/0-10V INPUTS/-IN_C")
	(net 128 "/0-10V INPUTS/+IN_D")
	(net 129 "/0-10V INPUTS/-IN_D")
	(net 130 "/0-10V INPUTS/+IN_B")
	(net 131 "/0-10V INPUTS/-IN_B")
	(net 132 "/0-10V INPUTS/+IN_A")
	(net 133 "/0-10V INPUTS/+IN_C")
	(net 134 "Net-(IC4-IN2-)")
	(net 135 "Net-(IC4-IN1-)")
	(net 136 "/0-10VOutput/10V OUT1")
	(net 137 "/0-10VOutput/10V OUT2")
	(net 138 "/0-10VOutput/10V OUT4")
	(net 139 "Net-(IC5-IN2-)")
	(net 140 "Net-(IC5-IN1-)")
	(net 141 "/0-10VOutput/10V OUT3")
	(net 142 "Net-(IC6-OUT1)")
	(net 143 "Net-(IC6-IN1-)")
	(net 144 "Net-(IC6-OUT2)")
	(net 145 "Net-(IC6-IN2-)")
	(net 146 "Net-(IC7-OUT2)")
	(net 147 "Net-(IC7-OUT1)")
	(net 148 "Net-(IC7-IN2-)")
	(net 149 "Net-(IC7-IN1-)")
	(net 150 "/0-10V INPUTS/IN10V1")
	(net 151 "/0-10V INPUTS/IN10V2")
	(net 152 "/0-10V INPUTS/IN10V3")
	(net 153 "/0-10V INPUTS/IN10V4")
	(net 154 "/SCL")
	(net 155 "/PWM_IOUT5")
	(net 156 "/PWM_IOUT6")
	(net 157 "/PWM_VOUT3")
	(net 158 "/PWM_VOUT2")
	(net 159 "/PWM_VOUT1")
	(net 160 "/SDA")
	(net 161 "/A2INT_I")
	(net 162 "/RST")
	(net 163 "/A2INT_V")
	(net 164 "/PWM_IOUT8")
	(net 165 "/PWM_VOUT4")
	(net 166 "/RS485_DE")
	(net 167 "/PWM_IOUT7")
	(net 168 "/RS485_RX")
	(net 169 "/RS485_TX")
	(net 170 "/GPIO37")
	(net 171 "/GPIO21")
	(net 172 "/GPIO38")
	(net 173 "/GPIO0")
	(net 174 "/GPIO20")
	(net 175 "/GPIO36")
	(net 176 "/GPIO19")
	(net 177 "/GPIO35")
	(net 178 "/GPIO45")
	(net 179 "/4-20mAOutput/OUT1")
	(net 180 "/DigitalIO/OD_OUT1")
	(net 181 "Net-(Q3-G)")
	(net 182 "Net-(Q4-E)")
	(net 183 "Net-(Q5-E)")
	(net 184 "Net-(Q6-E)")
	(net 185 "Net-(Q7-E)")
	(net 186 "Net-(Q8-G)")
	(net 187 "/4-20mAOutput/OUT2")
	(net 188 "Net-(Q9-G)")
	(net 189 "/4-20mAOutput/OUT3")
	(net 190 "Net-(Q10-G)")
	(net 191 "/4-20mAOutput/OUT4")
	(net 192 "Net-(Q11-G)")
	(net 193 "/DigitalIO/OD_OUT2")
	(net 194 "/DigitalIO/OD_OUT3")
	(net 195 "/DigitalIO/OD_OUT4")
	(net 196 "Net-(U2-FBN)")
	(net 197 "Net-(R27-Pad2)")
	(net 198 "Net-(U6D-+)")
	(net 199 "Net-(RN2A-R1.2)")
	(net 200 "Net-(R31-Pad1)")
	(net 201 "Net-(R35-Pad2)")
	(net 202 "Net-(U6C-+)")
	(net 203 "Net-(RN2C-R3.2)")
	(net 204 "Net-(R39-Pad1)")
	(net 205 "Net-(R41-Pad2)")
	(net 206 "Net-(U6B-+)")
	(net 207 "Net-(RN3A-R1.2)")
	(net 208 "Net-(R45-Pad1)")
	(net 209 "Net-(R47-Pad2)")
	(net 210 "Net-(U6A-+)")
	(net 211 "Net-(RN3C-R3.2)")
	(net 212 "Net-(R51-Pad1)")
	(net 213 "Net-(U9-RO)")
	(net 214 "Net-(U9-DI)")
	(net 215 "unconnected-(U1-NC-Pad4)")
	(net 216 "unconnected-(U2-NC-Pad20)")
	(net 217 "unconnected-(U2-NC-Pad12)")
	(footprint "SamacSys_Parts:DMG4800LFG7"
		(layer "F.Cu")
		(at 157.66 119.8475)
		(descr "DMG4800LFG-7")
		(tags "MOSFET (N-Channel)")
		(property "Reference" "Q13"
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "DMG4800LFG-7"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" "https://www.diodes.com//assets/Datasheets/ds31785.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "N-Channel 30 V 7.44A (Ta) 940mW (Ta) Surface Mount U-DFN3030-8"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Height" "0.63"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Part Number" "621-DMG4800LFG-7"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Price/Stock" "https://www.mouser.co.uk/ProductDetail/Diodes-Incorporated/DMG4800LFG-7?qs=f4CYDwCO%252B%2FEVatAzjmPrMQ%3D%3D"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Name" "Diodes Incorporated"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Part_Number" "DMG4800LFG-7"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/DigitalIO/")
		(sheetfile "DigitalIO.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -0.975 1.3)
			(size 0.39 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 17 "GNDA")
			(pinfunction "S_1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.325 1.3)
			(size 0.39 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 17 "GNDA")
			(pinfunction "S_2")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at 0.325 1.3)
			(size 0.39 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 17 "GNDA")
			(pinfunction "S_3")
			(pintype "passive")
		)
		(pad "4" smd rect
			(at 0.975 1.3)
			(size 0.39 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 112 "Net-(HY2-EMITTER_3)")
			(pinfunction "G")
			(pintype "passive")
		)
		(pad "5" smd rect
			(at 0 -0.38 90)
			(size 2.49 2.59)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 193 "/DigitalIO/OD_OUT2")
			(pinfunction "D")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "C:\\Users\\ESpurbeck\\Documents\\KiCad\\3rdparty\\SamacSys_Parts.3dshapes\\DMG4800LFG-7.stp"
			(offset
				(xyz -74.85999949 42.70000012 0.6000000148)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 -180 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 161.3 64.7)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R53"
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "2.2k"
			(at 0 1.43 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/0-10VOutput/")
		(sheetfile "0-10VOutput.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 48 "Net-(C46-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 49 "Net-(IC4-IN1+)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Diode_SMD:D_SOD-323"
		(layer "F.Cu")
		(at 134.45 67.325 90)
		(descr "SOD-323")
		(tags "SOD-323")
		(property "Reference" "D4"
			(at -0.0225 0 90)
			(layer "F.SilkS")
		)
		(property "Value" "1N5819WS"
			(at 0.1 1.9 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://datasheet.lcsc.com/lcsc/2204281430_Guangdong-Hottech-1N5819WS_C191023.pdf"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "40V 600mV@1A 1A SOD-323 Schottky Barrier Diodes, SOD-323"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "D*SOD?323*")
		(sheetname "/Power Supply/")
		(sheetfile "Power Supply.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at -0.0225 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.05 0 90)
			(size 0.6 0.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 69 "Net-(D4-K)")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.05 0 90)
			(size 0.6 0.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 24 "-12V")
			(pinfunction "A")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SOD-323.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 144.65 67.35 -90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R12"
			(at 0 0 90)
			(layer "F.SilkS")
		)
		(property "Value" "1M"
			(at 0 1.43 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Power Supply/")
		(sheetfile "Power Supply.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 270)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 13 "+12V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0 270)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 27 "Net-(U2-FBP)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "SamacSys_Parts:L_Bourns_SRR4528A"
		(layer "F.Cu")
		(at 129.25 66.375 -90)
		(property "Reference" "L5"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "4.7uH"
			(at 0 1 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Inductor, small symbol"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Choke_* *Coil* Inductor_* L_*")
		(sheetname "/Power Supply/")
		(sheetfile "Power Supply.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -2.1 0 270)
			(size 1.6 5.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 2.1 0 270)
			(size 1.6 5.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.15)
			(net 69 "Net-(D4-K)")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "F.Cu")
		(at 192.4675 105.74 -90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C68"
			(at 0 0 90)
			(layer "F.SilkS")
		)
		(property "Value" "1uF"
			(at 0 1.68 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/4-20mAOutput/")
		(sheetfile "4-20mAOutput.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0 270)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 66 "Net-(IC7-IN2+)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0 270)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 75.255 128.675)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R48"
			(at -0.03 1.375 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "1M"
			(at 0 1.43 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/4-20mA Inputs/")
		(sheetfile "4-20mA Inputs.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 70 "/4-20mA Inputs/IN1N")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "F.Cu")
		(at 140 55.175)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C19"
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "4.7uF"
			(at 0 1.68 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/Power Supply/")
		(sheetfile "Power Supply.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 9 "+5V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 170.1 62.175 180)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R57"
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "6.49k"
			(at 0 1.43 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/0-10VOutput/")
		(sheetfile "0-10VOutput.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 180)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 134 "Net-(IC4-IN2-)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0 180)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "F.Cu")
		(at 192.0675 76.59 90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C59"
			(at 0 0 90)
			(layer "F.SilkS")
		)
		(property "Value" "1uF"
			(at 0 1.68 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/4-20mAOutput/")
		(sheetfile "4-20mAOutput.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0 90)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 57 "Net-(IC6-IN1+)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0 90)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 179.055 131.4675 -90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R87"
			(at 0 0 90)
			(layer "F.SilkS")
		)
		(property "Value" "15k"
			(at 0 -1.4 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/DigitalIO/")
		(sheetfile "DigitalIO.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 270)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 79 "/DigitalIO/VEX4")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0 270)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 84 "Net-(D12-K)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_Cat16-4"
		(layer "F.Cu")
		(at 188.5075 100.19)
		(descr "SMT resistor net, Bourns CAT16 series, 4 way")
		(tags "SMT resistor net Bourns CAT16 series 4 way")
		(property "Reference" "RN8"
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "2.2k"
			(at 0 2.55 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "4 resistor network, parallel topology, split"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "DIP* SOIC* R*Array*Concave* R*Array*Convex* MSOP*")
		(sheetname "/4-20mAOutput/")
		(sheetfile "4-20mAOutput.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -0.76 -1.2 180)
			(size 0.76 0.43)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 65 "Net-(RN8A-R1.1)")
			(pinfunction "R1.1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.76 -0.4 180)
			(size 0.76 0.43)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 67 "Net-(IC7-IN1+)")
			(pinfunction "R2.1")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at -0.76 0.4 180)
			(size 0.76 0.43)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 63 "Net-(RN8C-R3.1)")
			(pinfunction "R3.1")
			(pintype "passive")
		)
		(pad "4" smd rect
			(at -0.76 1.2 180)
			(size 0.76 0.43)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 66 "Net-(IC7-IN2+)")
			(pinfunction "R4.1")
			(pintype "passive")
		)
		(pad "5" smd rect
			(at 0.76 1.2 180)
			(size 0.76 0.43)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 63 "Net-(RN8C-R3.1)")
			(pinfunction "R4.2")
			(pintype "passive")
		)
		(pad "6" smd rect
			(at 0.76 0.4 180)
			(size 0.76 0.43)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 164 "/PWM_IOUT8")
			(pinfunction "R3.2")
			(pintype "passive")
		)
		(pad "7" smd rect
			(at 0.76 -0.4 180)
			(size 0.76 0.43)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 65 "Net-(RN8A-R1.1)")
			(pinfunction "R2.2")
			(pintype "passive")
		)
		(pad "8" smd rect
			(at 0.76 -1.2 180)
			(size 0.76 0.43)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 167 "/PWM_IOUT7")
			(pinfunction "R1.2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_Cat16-4.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "F.Cu")
		(at 196.8675 88.39 90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R75"
			(at 0 0 90)
			(layer "F.SilkS")
		)
		(property "Value" "10"
			(at 0 1.65 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/4-20mAOutput/")
		(sheetfile "4-20mAOutput.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 90)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net 144 "Net-(IC6-OUT2)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 90)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net 188 "Net-(Q9-G)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_SMD:SOT-23"
		(layer "F.Cu")
		(at 88.5375 119.925 180)
		(descr "SOT, 3 Pin (JEDEC TO-236 Var AB https://www.jedec.org/document_search?search_api_views_fulltext=TO-236), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOT TO_SOT_SMD")
		(property "Reference" "Q4"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "MMBT3904"
			(at 0 2.4 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.onsemi.com/pdf/datasheet/pzt3904-d.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "0.2A Ic, 40V Vce, Small Signal NPN Transistor, SOT-23"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SOT?23*")
		(sheetname "/4-20mA Inputs/")
		(sheetfile "4-20mA Inputs.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9375 -0.95 180)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 32 "Net-(Q4-B)")
			(pinfunction "B")
			(pintype "input")
		)
		(pad "2" smd roundrect
			(at -0.9375 0.95 180)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 182 "Net-(Q4-E)")
			(pinfunction "E")
			(pintype "passive")
		)
		(pad "3" smd roundrect
			(at 0.9375 0 180)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 9 "+5V")
			(pinfunction "C")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 170.1 58.1 180)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R61"
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "15k"
			(at 0 1.43 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/0-10VOutput/")
		(sheetfile "0-10VOutput.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 180)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 134 "Net-(IC4-IN2-)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0 180)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 137 "/0-10VOutput/10V OUT2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 157.875 58.375)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R60"
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "15k"
			(at 0 1.43 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/0-10VOutput/")
		(sheetfile "0-10VOutput.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 135 "Net-(IC4-IN1-)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 136 "/0-10VOutput/10V OUT1")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "F.Cu")
		(at 167.15 67.1 180)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C48"
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "1uF"
			(at 0 1.68 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/0-10VOutput/")
		(sheetfile "0-10VOutput.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0 180)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 50 "Net-(C48-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0 180)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_SO:SO-14_3.9x8.65mm_P1.27mm"
		(layer "F.Cu")
		(at 100.785 120.45 90)
		(descr "SO, 14 Pin (https://www.st.com/resource/en/datasheet/l6491.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SO SO")
		(property "Reference" "U6"
			(at 0 -0.0775 180)
			(layer "F.SilkS")
		)
		(property "Value" "LM324"
			(at 0 5.28 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/lm2902-n.pdf"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Low-Power, Quad-Operational Amplifiers, DIP-14/SOIC-14/SSOP-14"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SOIC*3.9x8.7mm*P1.27mm* DIP*W7.62mm* TSSOP*4.4x5mm*P0.65mm* SSOP*5.3x6.2mm*P0.65mm* MSOP*3x3mm*P0.5mm*")
		(sheetname "/4-20mA Inputs/")
		(sheetfile "4-20mA Inputs.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -0.0775 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -2.475 -3.81 90)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 44 "Net-(Q5-B)")
			(pintype "output")
		)
		(pad "2" smd roundrect
			(at -2.475 -2.54 90)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 45 "Net-(U6A--)")
			(pinfunction "-")
			(pintype "input")
		)
		(pad "3" smd roundrect
			(at -2.475 -1.27 90)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 210 "Net-(U6A-+)")
			(pinfunction "+")
			(pintype "input")
		)
		(pad "4" smd roundrect
			(at -2.475 0 90)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 14 "+5.5V")
			(pinfunction "V+")
			(pintype "power_in")
		)
		(pad "5" smd roundrect
			(at -2.475 1.27 90)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 206 "Net-(U6B-+)")
			(pinfunction "+")
			(pintype "input")
		)
		(pad "6" smd roundrect
			(at -2.475 2.54 90)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 41 "Net-(U6B--)")
			(pinfunction "-")
			(pintype "input")
		)
		(pad "7" smd roundrect
			(at -2.475 3.81 90)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 40 "Net-(Q6-B)")
			(pintype "output")
		)
		(pad "8" smd roundrect
			(at 2.475 3.81 90)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 37 "Net-(Q7-B)")
			(pintype "output")
		)
		(pad "9" smd roundrect
			(at 2.475 2.54 90)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 36 "Net-(U6C--)")
			(pinfunction "-")
			(pintype "input")
		)
		(pad "10" smd roundrect
			(at 2.475 1.27 90)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 202 "Net-(U6C-+)")
			(pinfunction "+")
			(pintype "input")
		)
		(pad "11" smd roundrect
			(at 2.475 0 90)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "V-")
			(pintype "power_in")
		)
		(pad "12" smd roundrect
			(at 2.475 -1.27 90)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 198 "Net-(U6D-+)")
			(pinfunction "+")
			(pintype "input")
		)
		(pad "13" smd roundrect
			(at 2.475 -2.54 90)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 33 "Net-(U6D--)")
			(pinfunction "-")
			(pintype "input")
		)
		(pad "14" smd roundrect
			(at 2.475 -3.81 90)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 32 "Net-(Q4-B)")
			(pintype "output")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Package_SO.3dshapes/SO-14_3.9x8.65mm_P1.27mm.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "SamacSys_Parts:APTD1608ZGCK"
		(layer "F.Cu")
		(at 182.9717 131.4675 180)
		(descr "APTD1608ZGCK-1")
		(tags "LED")
		(property "Reference" "D11"
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "LED_Small"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Light emitting diode, small symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pin" "1=K 2=A"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "LED* LED_SMD:* LED_THT:*")
		(sheetname "/DigitalIO/")
		(sheetfile "DigitalIO.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -0.825 0 270)
			(size 0.8 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 83 "Net-(D11-K)")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 0.825 0 270)
			(size 0.8 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 96 "/DigitalIO/OP3")
			(pinfunction "A")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "C:\\Users\\ESpurbeck\\Documents\\KiCad\\3rdparty\\SamacSys_Parts.3dshapes\\APTD1608ZGCK.stp"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 90 -180 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "F.Cu")
		(at 157.5 64.7 180)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C47"
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "1uF"
			(at 0 1.68 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/0-10VOutput/")
		(sheetfile "0-10VOutput.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0 180)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 49 "Net-(IC4-IN1+)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0 180)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "F.Cu")
		(at 175.975 67.3)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C52"
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "1uF"
			(at 0 1.68 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/0-10VOutput/")
		(sheetfile "0-10VOutput.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 52 "Net-(C52-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "SamacSys_Parts:APTD1608ZGCK"
		(layer "F.Cu")
		(at 142.26 130.8675)
		(descr "APTD1608ZGCK-1")
		(tags "LED")
		(property "Reference" "D15"
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "LED_Small"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Light emitting diode, small symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pin" "1=K 2=A"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "LED* LED_SMD:* LED_THT:*")
		(sheetname "/DigitalIO/")
		(sheetfile "DigitalIO.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -0.825 0 90)
			(size 0.8 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 17 "GNDA")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 0.825 0 90)
			(size 0.8 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 88 "Net-(D15-A)")
			(pinfunction "A")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "C:\\Users\\ESpurbeck\\Documents\\KiCad\\3rdparty\\SamacSys_Parts.3dshapes\\APTD1608ZGCK.stp"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 90 -180 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 81.545 82.175 -90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R24"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "22k"
			(at 0 1.43 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/0-10V INPUTS/")
		(sheetfile "0-10V INPUTS.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 270)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 153 "/0-10V INPUTS/IN10V4")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0 270)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 133 "/0-10V INPUTS/+IN_C")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 95.675 135 90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R45"
			(at 0 0 90)
			(layer "F.SilkS")
		)
		(property "Value" "100"
			(at 0 1.43 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/4-20mA Inputs/")
		(sheetfile "4-20mA Inputs.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 90)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 208 "Net-(R45-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0 90)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 41 "Net-(U6B--)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "SamacSys_Parts:APTD1608ZGCK"
		(layer "F.Cu")
		(at 157.7267 130.8675)
		(descr "APTD1608ZGCK-1")
		(tags "LED")
		(property "Reference" "D14"
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "LED_Small"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Light emitting diode, small symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pin" "1=K 2=A"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "LED* LED_SMD:* LED_THT:*")
		(sheetname "/DigitalIO/")
		(sheetfile "DigitalIO.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -0.825 0 90)
			(size 0.8 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 17 "GNDA")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 0.825 0 90)
			(size 0.8 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 87 "Net-(D14-A)")
			(pinfunction "A")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "C:\\Users\\ESpurbeck\\Documents\\KiCad\\3rdparty\\SamacSys_Parts.3dshapes\\APTD1608ZGCK.stp"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 90 -180 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 161.3 66.9 180)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R28"
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "2.2k"
			(at 0 1.43 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/0-10VOutput/")
		(sheetfile "0-10VOutput.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 180)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 159 "/PWM_VOUT1")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0 180)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 48 "Net-(C46-Pad1)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 201.43 131.4425 90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R84"
			(at 0 0 90)
			(layer "F.SilkS")
		)
		(property "Value" "15k"
			(at 0 1.43 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/DigitalIO/")
		(sheetfile "DigitalIO.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 90)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 78 "Net-(D9-K)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0 90)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 85 "/DigitalIO/VEX1")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_Cat16-4"
		(layer "F.Cu")
		(at 86.565 88.05 180)
		(descr "SMT resistor net, Bourns CAT16 series, 4 way")
		(tags "SMT resistor net Bourns CAT16 series 4 way")
		(property "Reference" "RN1"
			(at 0 0 90)
			(layer "F.SilkS")
		)
		(property "Value" "4.7k"
			(at 0 2.55 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "4 resistor network, parallel topology, split"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "DIP* SOIC* R*Array*Concave* R*Array*Convex* MSOP*")
		(sheetname "/0-10V INPUTS/")
		(sheetfile "0-10V INPUTS.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -0.76 -1.2)
			(size 0.76 0.43)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 31 "/0-10V INPUTS/AIN3")
			(pinfunction "R1.1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.76 -0.4)
			(size 0.76 0.43)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 30 "/0-10V INPUTS/AIN2")
			(pinfunction "R2.1")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at -0.76 0.4)
			(size 0.76 0.43)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 29 "/0-10V INPUTS/AIN1")
			(pinfunction "R3.1")
			(pintype "passive")
		)
		(pad "4" smd rect
			(at -0.76 1.2)
			(size 0.76 0.43)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 28 "/0-10V INPUTS/AIN0")
			(pinfunction "R4.1")
			(pintype "passive")
		)
		(pad "5" smd rect
			(at 0.76 1.2)
			(size 0.76 0.43)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 127 "/0-10V INPUTS/-IN_C")
			(pinfunction "R4.2")
			(pintype "passive")
		)
		(pad "6" smd rect
			(at 0.76 0.4)
			(size 0.76 0.43)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 129 "/0-10V INPUTS/-IN_D")
			(pinfunction "R3.2")
			(pintype "passive")
		)
		(pad "7" smd rect
			(at 0.76 -0.4)
			(size 0.76 0.43)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 126 "/0-10V INPUTS/-IN_A")
			(pinfunction "R2.2")
			(pintype "passive")
		)
		(pad "8" smd rect
			(at 0.76 -1.2)
			(size 0.76 0.43)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 131 "/0-10V INPUTS/-IN_B")
			(pinfunction "R1.2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_Cat16-4.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 86.675 91.5 -90)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C31"
			(at 0 0 90)
			(layer "F.SilkS")
		)
		(property "Value" "470nF"
			(at 0 1.43 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/0-10V INPUTS/")
		(sheetfile "0-10V INPUTS.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 270)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 31 "/0-10V INPUTS/AIN3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 270)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 187.65 58.55 180)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R71"
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "15k"
			(at 0 1.43 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/0-10VOutput/")
		(sheetfile "0-10VOutput.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 180)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 139 "Net-(IC5-IN2-)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0 180)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 138 "/0-10VOutput/10V OUT4")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 83.85 83)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R25"
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "10k"
			(at 0 1.43 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/0-10V INPUTS/")
		(sheetfile "0-10V INPUTS.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 133 "/0-10V INPUTS/+IN_C")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 92.1875 93.075 -90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R18"
			(at 0 0 90)
			(layer "F.SilkS")
		)
		(property "Value" "2.2k"
			(at 0 1.43 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/0-10V INPUTS/")
		(sheetfile "0-10V INPUTS.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 270)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 160 "/SDA")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0 270)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 15 "+3.3V")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "SamacSys_Parts:SOIC127P700X230-16N"
		(layer "F.Cu")
		(at 146.4 108.2 -90)
		(descr "TLP293-4(GB-TP,E-1")
		(tags "Circulator or Directional Coupler")
		(property "Reference" "HY2"
			(at 0 0 90)
			(layer "F.SilkS")
		)
		(property "Value" "TLP293-4_GB-TP,E"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" "https://componentsearchengine.com/Datasheets/1/TLP293-4(GB-TP,E.pdf"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Transistor Output Optocouplers 4ch Transistor opto coupler"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Height" "2.3"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Part Number" "757-TLP293-4GB-TPE"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Price/Stock" "https://www.mouser.co.uk/ProductDetail/Toshiba/TLP293-4GB-TPE?qs=U6BGiFaJGDs%252BkJtAfW6%2FTw%3D%3D"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Name" "Toshiba"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Part_Number" "TLP293-4(GB-TP,E"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/DigitalIO/")
		(sheetfile "DigitalIO.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -3.25 -4.445)
			(size 0.65 1.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 114 "Net-(HY2-ANODE_1)")
			(pinfunction "ANODE_1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -3.25 -3.175)
			(size 0.65 1.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 115 "/OD1")
			(pinfunction "CATHODE_1")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at -3.25 -1.905)
			(size 0.65 1.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 105 "Net-(HY2-ANODE_2)")
			(pinfunction "ANODE_2")
			(pintype "passive")
		)
		(pad "4" smd rect
			(at -3.25 -0.635)
			(size 0.65 1.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 104 "/OD2")
			(pinfunction "CATHODE_2")
			(pintype "passive")
		)
		(pad "5" smd rect
			(at -3.25 0.635)
			(size 0.65 1.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 111 "Net-(HY2-ANODE_3)")
			(pinfunction "ANODE_3")
			(pintype "passive")
		)
		(pad "6" smd rect
			(at -3.25 1.905)
			(size 0.65 1.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 109 "/OD3")
			(pinfunction "CATHODE_3")
			(pintype "passive")
		)
		(pad "7" smd rect
			(at -3.25 3.175)
			(size 0.65 1.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 106 "Net-(HY2-ANODE_4)")
			(pinfunction "ANODE_4")
			(pintype "passive")
		)
		(pad "8" smd rect
			(at -3.25 4.445)
			(size 0.65 1.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 107 "/OD4")
			(pinfunction "CATHODE_4")
			(pintype "passive")
		)
		(pad "9" smd rect
			(at 3.25 4.445)
			(size 0.65 1.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 113 "Net-(HY2-EMITTER_1)")
			(pinfunction "EMITTER_1")
			(pintype "passive")
		)
		(pad "10" smd rect
			(at 3.25 3.175)
			(size 0.65 1.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 19 "+12VA")
			(pinfunction "COLLECTOR_1")
			(pintype "passive")
		)
		(pad "11" smd rect
			(at 3.25 1.905)
			(size 0.65 1.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 108 "Net-(HY2-EMITTER_2)")
			(pinfunction "EMITTER_2")
			(pintype "passive")
		)
		(pad "12" smd rect
			(at 3.25 0.635)
			(size 0.65 1.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 19 "+12VA")
			(pinfunction "COLLECTOR_2")
			(pintype "passive")
		)
		(pad "13" smd rect
			(at 3.25 -0.635)
			(size 0.65 1.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 112 "Net-(HY2-EMITTER_3)")
			(pinfunction "EMITTER_3")
			(pintype "passive")
		)
		(pad "14" smd rect
			(at 3.25 -1.905)
			(size 0.65 1.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 19 "+12VA")
			(pinfunction "COLLECTOR_3")
			(pintype "passive")
		)
		(pad "15" smd rect
			(at 3.25 -3.175)
			(size 0.65 1.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 110 "Net-(HY2-EMITTER_4)")
			(pinfunction "EMITTER_4")
			(pintype "passive")
		)
		(pad "16" smd rect
			(at 3.25 -4.445)
			(size 0.65 1.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 19 "+12VA")
			(pinfunction "COLLECTOR_4")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "C:\\Users\\ESpurbeck\\Documents\\KiCad\\3rdparty\\SamacSys_Parts.3dshapes\\TLP293-4_GB-TP,E.stp"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 101.725 126.25 90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R51"
			(at 0 0 90)
			(layer "F.SilkS")
		)
		(property "Value" "100"
			(at 0 1.43 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/4-20mA Inputs/")
		(sheetfile "4-20mA Inputs.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 90)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 212 "Net-(R51-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0 90)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 45 "Net-(U6A--)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "F.Cu")
		(at 185.55 67.5)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C53"
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "1uF"
			(at 0 1.68 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/0-10VOutput/")
		(sheetfile "0-10VOutput.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 53 "Net-(C53-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 96.75 110.4 180)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R29"
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "49.9"
			(at 0 1.43 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/4-20mA Inputs/")
		(sheetfile "4-20mA Inputs.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 180)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0 180)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 198 "Net-(U6D-+)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 103.4 126.25 90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R52"
			(at 0 0 90)
			(layer "F.SilkS")
		)
		(property "Value" "49.9"
			(at 0 1.43 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/4-20mA Inputs/")
		(sheetfile "4-20mA Inputs.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 90)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0 90)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 212 "Net-(R51-Pad1)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_Cat16-4"
		(layer "F.Cu")
		(at 182.8425 86.19)
		(descr "SMT resistor net, Bourns CAT16 series, 4 way")
		(tags "SMT resistor net Bourns CAT16 series 4 way")
		(property "Reference" "RN6"
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "4.7k"
			(at 0 2.55 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "4 resistor network, parallel topology, split"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "DIP* SOIC* R*Array*Concave* R*Array*Convex* MSOP*")
		(sheetname "/4-20mAOutput/")
		(sheetfile "4-20mAOutput.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -0.76 -1.2 180)
			(size 0.76 0.43)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 143 "Net-(IC6-IN1-)")
			(pinfunction "R1.1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.76 -0.4 180)
			(size 0.76 0.43)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 145 "Net-(IC6-IN2-)")
			(pinfunction "R2.1")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at -0.76 0.4 180)
			(size 0.76 0.43)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 149 "Net-(IC7-IN1-)")
			(pinfunction "R3.1")
			(pintype "passive")
		)
		(pad "4" smd rect
			(at -0.76 1.2 180)
			(size 0.76 0.43)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 148 "Net-(IC7-IN2-)")
			(pinfunction "R4.1")
			(pintype "passive")
		)
		(pad "5" smd rect
			(at 0.76 1.2 180)
			(size 0.76 0.43)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 62 "/O_CHECK4")
			(pinfunction "R4.2")
			(pintype "passive")
		)
		(pad "6" smd rect
			(at 0.76 0.4 180)
			(size 0.76 0.43)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 64 "/O_CHECK3")
			(pinfunction "R3.2")
			(pintype "passive")
		)
		(pad "7" smd rect
			(at 0.76 -0.4 180)
			(size 0.76 0.43)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 61 "/O_CHECK2")
			(pinfunction "R2.2")
			(pintype "passive")
		)
		(pad "8" smd rect
			(at 0.76 -1.2 180)
			(size 0.76 0.43)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 60 "/O_CHECK1")
			(pinfunction "R1.2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_Cat16-4.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0201_0603Metric"
		(layer "F.Cu")
		(at 108.75 126.495 -90)
		(descr "Resistor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R34"
			(at 0 0 90)
			(layer "F.SilkS")
		)
		(property "Value" "2.2k"
			(at 0 1.05 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/4-20mA Inputs/")
		(sheetfile "4-20mA Inputs.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "" smd roundrect
			(at -0.345 0 270)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0.345 0 270)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "1" smd roundrect
			(at -0.32 0 270)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 154 "/SCL")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.32 0 270)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 15 "+3.3V")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0201_0603Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Diode_SMD:D_SMA"
		(layer "F.Cu")
		(at 65.075 130.15 90)
		(descr "Diode SMA (DO-214AC)")
		(tags "Diode SMA (DO-214AC)")
		(property "Reference" "D5"
			(at -0.0225 0 90)
			(layer "F.SilkS")
		)
		(property "Value" "SMAJ18A"
			(at 0 2.6 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.littelfuse.com/media?resourcetype=datasheets&itemid=75e32973-b177-4ee3-a0ff-cedaf1abdb93&filename=smaj-datasheet"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "400W unidirectional Transient Voltage Suppressor, 18.0Vr, SMA(DO-214AC)"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "D*SMA*")
		(sheetname "/4-20mA Inputs/")
		(sheetfile "4-20mA Inputs.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at -0.0225 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -2 0 90)
			(size 2.5 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.1388888889)
			(net 71 "/4-20mA Inputs/IN1P")
			(pinfunction "A1")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 2 0 90)
			(size 2.5 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.1388888889)
			(net 70 "/4-20mA Inputs/IN1N")
			(pinfunction "A2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SMA.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_SMD:SOT-23"
		(layer "F.Cu")
		(at 89.375 135.7375 -90)
		(descr "SOT, 3 Pin (JEDEC TO-236 Var AB https://www.jedec.org/document_search?search_api_views_fulltext=TO-236), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOT TO_SOT_SMD")
		(property "Reference" "Q6"
			(at 0 0 90)
			(layer "F.SilkS")
		)
		(property "Value" "MMBT3904"
			(at 0 2.4 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.onsemi.com/pdf/datasheet/pzt3904-d.pdf"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "0.2A Ic, 40V Vce, Small Signal NPN Transistor, SOT-23"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SOT?23*")
		(sheetname "/4-20mA Inputs/")
		(sheetfile "4-20mA Inputs.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9375 -0.95 270)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 40 "Net-(Q6-B)")
			(pinfunction "B")
			(pintype "input")
		)
		(pad "2" smd roundrect
			(at -0.9375 0.95 270)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 184 "Net-(Q6-E)")
			(pinfunction "E")
			(pintype "passive")
		)
		(pad "3" smd roundrect
			(at 0.9375 0 270)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 9 "+5V")
			(pinfunction "C")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 96.21 126.43 90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R49"
			(at 0 0 90)
			(layer "F.SilkS")
		)
		(property "Value" "49.9"
			(at 0 1.43 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/4-20mA Inputs/")
		(sheetfile "4-20mA Inputs.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 90)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0 90)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 210 "Net-(U6A-+)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 138.95 71.55 90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R13"
			(at 0 0 90)
			(layer "F.SilkS")
		)
		(property "Value" "100k"
			(at 0 1.43 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Power Supply/")
		(sheetfile "Power Supply.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 90)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 25 "Net-(U2-VREF)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0 90)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 196 "Net-(U2-FBN)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 157.875 61.975)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R56"
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "6.49k"
			(at 0 1.43 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/0-10VOutput/")
		(sheetfile "0-10VOutput.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 135 "Net-(IC4-IN1-)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "SamacSys_Parts:DMG4800LFG7"
		(layer "F.Cu")
		(at 205.6875 107.99 -90)
		(descr "DMG4800LFG-7")
		(tags "MOSFET (N-Channel)")
		(property "Reference" "Q11"
			(at 0 0 90)
			(layer "F.SilkS")
		)
		(property "Value" "DMG4800LFG-7"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" "https://www.diodes.com//assets/Datasheets/ds31785.pdf"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "N-Channel 30 V 7.44A (Ta) 940mW (Ta) Surface Mount U-DFN3030-8"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Height" "0.63"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Part Number" "621-DMG4800LFG-7"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Price/Stock" "https://www.mouser.co.uk/ProductDetail/Diodes-Incorporated/DMG4800LFG-7?qs=f4CYDwCO%252B%2FEVatAzjmPrMQ%3D%3D"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Name" "Diodes Incorporated"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Part_Number" "DMG4800LFG-7"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/4-20mAOutput/")
		(sheetfile "4-20mAOutput.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -0.975 1.3 270)
			(size 0.39 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 148 "Net-(IC7-IN2-)")
			(pinfunction "S_1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.325 1.3 270)
			(size 0.39 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 148 "Net-(IC7-IN2-)")
			(pinfunction "S_2")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at 0.325 1.3 270)
			(size 0.39 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 148 "Net-(IC7-IN2-)")
			(pinfunction "S_3")
			(pintype "passive")
		)
		(pad "4" smd rect
			(at 0.975 1.3 270)
			(size 0.39 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 192 "Net-(Q11-G)")
			(pinfunction "G")
			(pintype "passive")
		)
		(pad "5" smd rect
			(at 0 -0.38)
			(size 2.49 2.59)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 191 "/4-20mAOutput/OUT4")
			(pinfunction "D")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "C:\\Users\\ESpurbeck\\Documents\\KiCad\\3rdparty\\SamacSys_Parts.3dshapes\\DMG4800LFG-7.stp"
			(offset
				(xyz -74.85999949 42.70000012 0.6000000148)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 -180 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 170.775 64.9 180)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R59"
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "2.2k"
			(at 0 1.43 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/0-10VOutput/")
		(sheetfile "0-10VOutput.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 180)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 50 "Net-(C48-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0 180)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 51 "Net-(IC4-IN2+)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 170.1 59.875 180)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R55"
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "4.53k"
			(at 0 1.43 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/0-10VOutput/")
		(sheetfile "0-10VOutput.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 180)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 15 "+3.3V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0 180)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 134 "Net-(IC4-IN2-)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "F.Cu")
		(at 175.925 64.9 180)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C54"
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "1uF"
			(at 0 1.68 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/0-10VOutput/")
		(sheetfile "0-10VOutput.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0 180)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 54 "Net-(IC5-IN1+)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0 180)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_1206_3216Metric"
		(layer "F.Cu")
		(at 75.1 124.8075)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R41"
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "140"
			(at 0 1.83 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/4-20mA Inputs/")
		(sheetfile "4-20mA Inputs.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.4625 0)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.222222)
			(net 73 "/4-20mA Inputs/IN2P")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.4625 0)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.222222)
			(net 205 "Net-(R41-Pad2)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 176.1 58.3)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R70"
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "15k"
			(at 0 1.43 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/0-10VOutput/")
		(sheetfile "0-10VOutput.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 140 "Net-(IC5-IN1-)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 141 "/0-10VOutput/10V OUT3")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 102.57 111.95)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C40"
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "220nF"
			(at 0 1.43 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/4-20mA Inputs/")
		(sheetfile "4-20mA Inputs.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 41 "Net-(U6B--)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 40 "Net-(Q6-B)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_1206_3216Metric"
		(layer "F.Cu")
		(at 75.2 132.4275)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R47"
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "140"
			(at 0 1.83 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/4-20mA Inputs/")
		(sheetfile "4-20mA Inputs.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.4625 0)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.222222)
			(net 71 "/4-20mA Inputs/IN1P")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.4625 0)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.222222)
			(net 209 "Net-(R47-Pad2)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 176.2 73.65 -90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R9"
			(at 0 0 90)
			(layer "F.SilkS")
		)
		(property "Value" "1k"
			(at 0 1.43 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Power Supply/")
		(sheetfile "Power Supply.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 270)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0 270)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 117 "Net-(IC1-ADJ)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 103.275 114.85 -90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R39"
			(at 0 0 90)
			(layer "F.SilkS")
		)
		(property "Value" "100"
			(at 0 1.43 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/4-20mA Inputs/")
		(sheetfile "4-20mA Inputs.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 270)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 204 "Net-(R39-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0 270)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 36 "Net-(U6C--)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_SO:TSSOP-10_3x3mm_P0.5mm"
		(layer "F.Cu")
		(at 92.15 88.075 -90)
		(descr "TSSOP10: plastic thin shrink small outline package; 10 leads; body width 3 mm; (see NXP SSOP-TSSOP-VSO-REFLOW.pdf and sot552-1_po.pdf)")
		(tags "SSOP 0.5")
		(property "Reference" "U4"
			(at 0 0 90)
			(layer "F.SilkS")
		)
		(property "Value" "ADS1115IDGS"
			(at 0 2.55 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/ads1113.pdf"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Ultra-Small, Low-Power, I2C-Compatible, 860-SPS, 16-Bit ADCs With Internal Reference, Oscillator, and Programmable Comparator, VSSOP-10"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TSSOP*3x3mm*P0.5mm*")
		(sheetname "/0-10V INPUTS/")
		(sheetfile "0-10V INPUTS.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -2.15 -1 270)
			(size 1.1 0.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "GND")
			(pinfunction "ADDR")
			(pintype "input")
		)
		(pad "2" smd rect
			(at -2.15 -0.5 270)
			(size 1.1 0.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 163 "/A2INT_V")
			(pinfunction "ALERT/RDY")
			(pintype "output")
		)
		(pad "3" smd rect
			(at -2.15 0 270)
			(size 1.1 0.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "4" smd rect
			(at -2.15 0.5 270)
			(size 1.1 0.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 28 "/0-10V INPUTS/AIN0")
			(pinfunction "AIN0")
			(pintype "input")
		)
		(pad "5" smd rect
			(at -2.15 1 270)
			(size 1.1 0.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 29 "/0-10V INPUTS/AIN1")
			(pinfunction "AIN1")
			(pintype "input")
		)
		(pad "6" smd rect
			(at 2.15 1 270)
			(size 1.1 0.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 30 "/0-10V INPUTS/AIN2")
			(pinfunction "AIN2")
			(pintype "input")
		)
		(pad "7" smd rect
			(at 2.15 0.5 270)
			(size 1.1 0.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 31 "/0-10V INPUTS/AIN3")
			(pinfunction "AIN3")
			(pintype "input")
		)
		(pad "8" smd rect
			(at 2.15 0 270)
			(size 1.1 0.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 15 "+3.3V")
			(pinfunction "VDD")
			(pintype "power_in")
		)
		(pad "9" smd rect
			(at 2.15 -0.5 270)
			(size 1.1 0.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 160 "/SDA")
			(pinfunction "SDA")
			(pintype "bidirectional")
		)
		(pad "10" smd rect
			(at 2.15 -1 270)
			(size 1.1 0.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 154 "/SCL")
			(pinfunction "SCL")
			(pintype "input")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Package_SO.3dshapes/TSSOP-10_3x3mm_P0.5mm.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_1206_3216Metric"
		(layer "F.Cu")
		(at 205.3175 77.59)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R73"
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "140"
			(at 3.3375 -1.2 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/4-20mAOutput/")
		(sheetfile "4-20mAOutput.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.4625 0)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.222222)
			(net 143 "Net-(IC6-IN1-)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.4625 0)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.222222)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "F.Cu")
		(at 167.15 64.9 180)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C49"
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "1uF"
			(at 0 1.68 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/0-10VOutput/")
		(sheetfile "0-10VOutput.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0 180)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 51 "Net-(IC4-IN2+)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0 180)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "SamacSys_Parts:SOIC127P600X175-14N"
		(layer "F.Cu")
		(at 80.275 87.95 90)
		(descr "D")
		(tags "Integrated Circuit")
		(property "Reference" "IC3"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "OPA4330AIDR"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/opa4330"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "1.8V, 35A, microPower, Precision, Zero Drift CMOS Op Amp"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Height" "1.75"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Part Number" "595-OPA4330AIDR"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Price/Stock" "https://www.mouser.co.uk/ProductDetail/Texas-Instruments/OPA4330AIDR?qs=EuM%2FBx4ov4R6DjwOW%252BMW9A%3D%3D"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Name" "Texas Instruments"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Part_Number" "OPA4330AIDR"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/0-10V INPUTS/")
		(sheetfile "0-10V INPUTS.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -2.712 -3.81 180)
			(size 0.65 1.525)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 126 "/0-10V INPUTS/-IN_A")
			(pinfunction "OUT_A")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -2.712 -2.54 180)
			(size 0.65 1.525)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 126 "/0-10V INPUTS/-IN_A")
			(pinfunction "-IN_A")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at -2.712 -1.27 180)
			(size 0.65 1.525)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 132 "/0-10V INPUTS/+IN_A")
			(pinfunction "+IN_A")
			(pintype "passive")
		)
		(pad "4" smd rect
			(at -2.712 0 180)
			(size 0.65 1.525)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 15 "+3.3V")
			(pinfunction "V+")
			(pintype "passive")
		)
		(pad "5" smd rect
			(at -2.712 1.27 180)
			(size 0.65 1.525)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 130 "/0-10V INPUTS/+IN_B")
			(pinfunction "+IN_B")
			(pintype "passive")
		)
		(pad "6" smd rect
			(at -2.712 2.54 180)
			(size 0.65 1.525)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 131 "/0-10V INPUTS/-IN_B")
			(pinfunction "-IN_B")
			(pintype "passive")
		)
		(pad "7" smd rect
			(at -2.712 3.81 180)
			(size 0.65 1.525)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 131 "/0-10V INPUTS/-IN_B")
			(pinfunction "OUT_B")
			(pintype "passive")
		)
		(pad "8" smd rect
			(at 2.712 3.81 180)
			(size 0.65 1.525)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 127 "/0-10V INPUTS/-IN_C")
			(pinfunction "OUT_C")
			(pintype "passive")
		)
		(pad "9" smd rect
			(at 2.712 2.54 180)
			(size 0.65 1.525)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 127 "/0-10V INPUTS/-IN_C")
			(pinfunction "-IN_C")
			(pintype "passive")
		)
		(pad "10" smd rect
			(at 2.712 1.27 180)
			(size 0.65 1.525)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 133 "/0-10V INPUTS/+IN_C")
			(pinfunction "+IN_C")
			(pintype "passive")
		)
		(pad "11" smd rect
			(at 2.712 0 180)
			(size 0.65 1.525)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "GND")
			(pinfunction "V-")
			(pintype "passive")
		)
		(pad "12" smd rect
			(at 2.712 -1.27 180)
			(size 0.65 1.525)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 128 "/0-10V INPUTS/+IN_D")
			(pinfunction "+IN_D")
			(pintype "passive")
		)
		(pad "13" smd rect
			(at 2.712 -2.54 180)
			(size 0.65 1.525)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 129 "/0-10V INPUTS/-IN_D")
			(pinfunction "-IN_D")
			(pintype "passive")
		)
		(pad "14" smd rect
			(at 2.712 -3.81 180)
			(size 0.65 1.525)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 129 "/0-10V INPUTS/-IN_D")
			(pinfunction "OUT_D")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "C:\\Users\\ESpurbeck\\Documents\\KiCad\\3rdparty\\SamacSys_Parts.3dshapes\\OPA4330AIDR.stp"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_1206_3216Metric"
		(layer "F.Cu")
		(at 81.18 111.38)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R44"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "140"
			(at 0 1.83 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/4-20mA Inputs/")
		(sheetfile "4-20mA Inputs.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.4625 0)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.222222)
			(net 2 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.4625 0)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.222222)
			(net 207 "Net-(RN3A-R1.2)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 185.8675 84.19)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C63"
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "220nF"
			(at 0 1.43 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/4-20mAOutput/")
		(sheetfile "4-20mAOutput.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 61 "/O_CHECK2")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 142.825 69.975)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C23"
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "10nF"
			(at 0 1.43 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/Power Supply/")
		(sheetfile "Power Supply.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 23 "Net-(U2-CN)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "F.Cu")
		(at 187.0675 79.79)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C58"
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "1uF"
			(at 0 1.68 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/4-20mAOutput/")
		(sheetfile "4-20mAOutput.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 56 "Net-(RN5A-R1.1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 146.45 67.4 -90)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C27"
			(at 0 0 90)
			(layer "F.SilkS")
		)
		(property "Value" "7.5pF"
			(at 0 1.43 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/Power Supply/")
		(sheetfile "Power Supply.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 270)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 13 "+12V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 270)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 27 "Net-(U2-FBP)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 189.8 64.5 90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R65"
			(at 0 0 90)
			(layer "F.SilkS")
		)
		(property "Value" "2.2k"
			(at 0 1.43 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/0-10VOutput/")
		(sheetfile "0-10VOutput.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 90)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 53 "Net-(C53-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0 90)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 55 "Net-(IC5-IN2+)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "F.Cu")
		(at 161.5 100.125 90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C15"
			(at 0 0 90)
			(layer "F.SilkS")
		)
		(property "Value" "4.7uF"
			(at 0 1.68 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/Power Supply/")
		(sheetfile "Power Supply.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0 90)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 9 "+5V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0 90)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 101.45 114.875 90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R40"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "49.9"
			(at 0 1.43 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/4-20mA Inputs/")
		(sheetfile "4-20mA Inputs.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 90)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0 90)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 204 "Net-(R39-Pad1)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "F.Cu")
		(at 190.1175 89.19)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C60"
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "1uF"
			(at 0 1.68 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/4-20mAOutput/")
		(sheetfile "4-20mAOutput.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 58 "Net-(RN5C-R3.1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 92.65 120 -90)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C34"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "220nF"
			(at 0 1.43 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/4-20mA Inputs/")
		(sheetfile "4-20mA Inputs.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 270)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 33 "Net-(U6D--)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 270)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 32 "Net-(Q4-B)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 93.9 135 90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R46"
			(at 0 0 90)
			(layer "F.SilkS")
		)
		(property "Value" "49.9"
			(at 0 1.43 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/4-20mA Inputs/")
		(sheetfile "4-20mA Inputs.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 90)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0 90)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 208 "Net-(R45-Pad1)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 96.825 131.95)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R37"
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "49.9"
			(at 0 1.43 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/4-20mA Inputs/")
		(sheetfile "4-20mA Inputs.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 202 "Net-(U6C-+)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 176.1 60.1)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R66"
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "4.53k"
			(at 0 1.43 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/0-10VOutput/")
		(sheetfile "0-10VOutput.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 15 "+3.3V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 140 "Net-(IC5-IN1-)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 200.0925 87.59 180)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C70"
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "100nF"
			(at 0 1.43 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/4-20mAOutput/")
		(sheetfile "4-20mAOutput.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 180)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 5 "+24V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 180)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_1206_3216Metric"
		(layer "F.Cu")
		(at 75.275 117.1875)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R35"
			(at -0.025 2.0125 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "140"
			(at 0 1.83 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/4-20mA Inputs/")
		(sheetfile "4-20mA Inputs.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.4625 0)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.222222)
			(net 75 "/4-20mA Inputs/IN3P")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.4625 0)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.222222)
			(net 201 "Net-(R35-Pad2)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "SamacSys_Parts:APTD1608ZGCK"
		(layer "F.Cu")
		(at 149.9933 130.8675)
		(descr "APTD1608ZGCK-1")
		(tags "LED")
		(property "Reference" "D13"
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "LED_Small"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Light emitting diode, small symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pin" "1=K 2=A"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "LED* LED_SMD:* LED_THT:*")
		(sheetname "/DigitalIO/")
		(sheetfile "DigitalIO.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -0.825 0 90)
			(size 0.8 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 17 "GNDA")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 0.825 0 90)
			(size 0.8 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 86 "Net-(D13-A)")
			(pinfunction "A")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "C:\\Users\\ESpurbeck\\Documents\\KiCad\\3rdparty\\SamacSys_Parts.3dshapes\\APTD1608ZGCK.stp"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 90 -180 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_1206_3216Metric"
		(layer "F.Cu")
		(at 205.3175 86.39)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R74"
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "140"
			(at 2.6 -1.8 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/4-20mAOutput/")
		(sheetfile "4-20mAOutput.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.4625 0)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.222222)
			(net 145 "Net-(IC6-IN2-)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.4625 0)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.222222)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 95.975 113.8 -90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R31"
			(at 0 0 90)
			(layer "F.SilkS")
		)
		(property "Value" "100"
			(at 0 1.43 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/4-20mA Inputs/")
		(sheetfile "4-20mA Inputs.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 270)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 200 "Net-(R31-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0 270)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 33 "Net-(U6D--)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 179.125 55.9)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C56"
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "220nF"
			(at 0 1.43 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/0-10VOutput/")
		(sheetfile "0-10VOutput.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 13 "+12V")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_1210_3225Metric"
		(layer "F.Cu")
		(at 182.59 120.99)
		(descr "Resistor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R81"
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "4.7k"
			(at 0 2.28 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/DigitalIO/")
		(sheetfile "DigitalIO.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.4625 0)
			(size 1.125 2.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.222222)
			(net 96 "/DigitalIO/OP3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.4625 0)
			(size 1.125 2.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.222222)
			(net 100 "Net-(HY1-ANODE_2)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1210_3225Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Diode_SMD:D_SMA"
		(layer "F.Cu")
		(at 65.075 122.75 90)
		(descr "Diode SMA (DO-214AC)")
		(tags "Diode SMA (DO-214AC)")
		(property "Reference" "D6"
			(at -0.0225 0 90)
			(layer "F.SilkS")
		)
		(property "Value" "SMAJ18A"
			(at 0 2.6 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.littelfuse.com/media?resourcetype=datasheets&itemid=75e32973-b177-4ee3-a0ff-cedaf1abdb93&filename=smaj-datasheet"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "400W unidirectional Transient Voltage Suppressor, 18.0Vr, SMA(DO-214AC)"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "D*SMA*")
		(sheetname "/4-20mA Inputs/")
		(sheetfile "4-20mA Inputs.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at -0.0225 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -2 0 90)
			(size 2.5 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.1388888889)
			(net 73 "/4-20mA Inputs/IN2P")
			(pinfunction "A1")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 2 0 90)
			(size 2.5 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.1388888889)
			(net 72 "/4-20mA Inputs/IN2N")
			(pinfunction "A2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SMA.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_1210_3225Metric"
		(layer "F.Cu")
		(at 190.17 120.96)
		(descr "Resistor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R82"
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "4.7k"
			(at 0 2.28 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/DigitalIO/")
		(sheetfile "DigitalIO.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.4625 0)
			(size 1.125 2.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.222222)
			(net 92 "/DigitalIO/OP2")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.4625 0)
			(size 1.125 2.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.222222)
			(net 95 "Net-(HY1-ANODE_3)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1210_3225Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 100.675 133.75)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C37"
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "220nF"
			(at 0 1.43 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/4-20mA Inputs/")
		(sheetfile "4-20mA Inputs.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 36 "Net-(U6C--)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 37 "Net-(Q7-B)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 83.85 92.775)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R17"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "10k"
			(at 0 1.43 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/0-10V INPUTS/")
		(sheetfile "0-10V INPUTS.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 130 "/0-10V INPUTS/+IN_B")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1206_3216Metric"
		(layer "F.Cu")
		(at 180.82 81.7675 180)
		(descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C12"
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "10uF/16V"
			(at 0 1.85 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/Power Supply/")
		(sheetfile "Power Supply.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.475 0 180)
			(size 1.15 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.217391)
			(net 14 "+5.5V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.475 0 180)
			(size 1.15 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.217391)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1206_3216Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_1206_3216Metric"
		(layer "F.Cu")
		(at 205.3175 94.99)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R78"
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "140"
			(at 0 1.83 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/4-20mAOutput/")
		(sheetfile "4-20mAOutput.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.4625 0)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.222222)
			(net 149 "Net-(IC7-IN1-)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.4625 0)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.222222)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 140.525 71.55 90)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C25"
			(at 0 0 90)
			(layer "F.SilkS")
		)
		(property "Value" "220nF"
			(at 0 1.43 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/Power Supply/")
		(sheetfile "Power Supply.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 90)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 25 "Net-(U2-VREF)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 90)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_PinSocket_2.54mm:PinSocket_1x22_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 137.75 99.36 -90)
		(descr "Through hole straight socket strip, 1x22, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
		(tags "Through hole socket strip THT 1x22 2.54mm single row")
		(property "Reference" "J5"
			(at -0.025 26.65 90)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_01x22_Socket"
			(at 0 56.11 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x22, script generated"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "/")
		(sheetfile "universal-io-board-Hat.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at -0.025 26.65 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 0 2.54 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 169 "/RS485_TX")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole circle
			(at 0 5.08 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 168 "/RS485_RX")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole circle
			(at 0 7.62 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 60 "/O_CHECK1")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(pad "5" thru_hole circle
			(at 0 10.16 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 61 "/O_CHECK2")
			(pinfunction "Pin_5")
			(pintype "passive")
		)
		(pad "6" thru_hole circle
			(at 0 12.7 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 99 "/OPTO_IN4")
			(pinfunction "Pin_6")
			(pintype "passive")
		)
		(pad "7" thru_hole circle
			(at 0 15.24 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 97 "/OPTO_IN3")
			(pinfunction "Pin_7")
			(pintype "passive")
		)
		(pad "8" thru_hole circle
			(at 0 17.78 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 102 "/OPTO_IN2")
			(pinfunction "Pin_8")
			(pintype "passive")
		)
		(pad "9" thru_hole circle
			(at 0 20.32 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 101 "/OPTO_IN1")
			(pinfunction "Pin_9")
			(pintype "passive")
		)
		(pad "10" thru_hole circle
			(at 0 22.86 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 172 "/GPIO38")
			(pinfunction "Pin_10")
			(pintype "passive")
		)
		(pad "11" thru_hole circle
			(at 0 25.4 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 170 "/GPIO37")
			(pinfunction "Pin_11")
			(pintype "passive")
		)
		(pad "12" thru_hole circle
			(at 0 27.94 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 175 "/GPIO36")
			(pinfunction "Pin_12")
			(pintype "passive")
		)
		(pad "13" thru_hole circle
			(at 0 30.48 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 177 "/GPIO35")
			(pinfunction "Pin_13")
			(pintype "passive")
		)
		(pad "14" thru_hole circle
			(at 0 33.02 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 173 "/GPIO0")
			(pinfunction "Pin_14")
			(pintype "passive")
		)
		(pad "15" thru_hole circle
			(at 0 35.56 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 178 "/GPIO45")
			(pinfunction "Pin_15")
			(pintype "passive")
		)
		(pad "16" thru_hole circle
			(at 0 38.1 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 109 "/OD3")
			(pinfunction "Pin_16")
			(pintype "passive")
		)
		(pad "17" thru_hole circle
			(at 0 40.64 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 107 "/OD4")
			(pinfunction "Pin_17")
			(pintype "passive")
		)
		(pad "18" thru_hole circle
			(at 0 43.18 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 171 "/GPIO21")
			(pinfunction "Pin_18")
			(pintype "passive")
		)
		(pad "19" thru_hole circle
			(at 0 45.72 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 174 "/GPIO20")
			(pinfunction "Pin_19")
			(pintype "passive")
		)
		(pad "20" thru_hole circle
			(at 0 48.26 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 176 "/GPIO19")
			(pinfunction "Pin_20")
			(pintype "passive")
		)
		(pad "21" thru_hole circle
			(at 0 50.8 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "Pin_21")
			(pintype "passive")
		)
		(pad "22" thru_hole circle
			(at 0 53.34 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "Pin_22")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x22_P2.54mm_Vertical.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_1206_3216Metric"
		(layer "F.Cu")
		(at 80.5975 126.19)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R50"
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "140"
			(at 0 1.83 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/4-20mA Inputs/")
		(sheetfile "4-20mA Inputs.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.4625 0)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.222222)
			(net 2 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.4625 0)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.222222)
			(net 211 "Net-(RN3C-R3.2)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "SamacSys_Parts:APTD1608ZGCK"
		(layer "F.Cu")
		(at 175.43 131.4675 180)
		(descr "APTD1608ZGCK-1")
		(tags "LED")
		(property "Reference" "D12"
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "LED_Small"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Light emitting diode, small symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pin" "1=K 2=A"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "LED* LED_SMD:* LED_THT:*")
		(sheetname "/DigitalIO/")
		(sheetfile "DigitalIO.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -0.825 0 270)
			(size 0.8 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 84 "Net-(D12-K)")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 0.825 0 270)
			(size 0.8 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 103 "/DigitalIO/OP4")
			(pinfunction "A")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "C:\\Users\\ESpurbeck\\Documents\\KiCad\\3rdparty\\SamacSys_Parts.3dshapes\\APTD1608ZGCK.stp"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 90 -180 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "F.Cu")
		(at 190.7175 84.79 180)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C61"
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "1uF"
			(at 0 1.68 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/4-20mAOutput/")
		(sheetfile "4-20mAOutput.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0 180)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 59 "Net-(IC6-IN2+)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0 180)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 187.675 62.1 180)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R69"
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "6.49k"
			(at 0 1.43 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/0-10VOutput/")
		(sheetfile "0-10VOutput.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 180)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 139 "Net-(IC5-IN2-)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0 180)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 91.15 83.325 90)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C33"
			(at 0 0 90)
			(layer "F.SilkS")
		)
		(property "Value" "470nF"
			(at 0 1.43 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/0-10V INPUTS/")
		(sheetfile "0-10V INPUTS.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 90)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 29 "/0-10V INPUTS/AIN1")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 90)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_SO:SOIC-16_4.55x10.3mm_P1.27mm"
		(layer "F.Cu")
		(at 89.725 127.9)
		(descr "SOIC, 16 Pin (https://toshiba.semicon-storage.com/info/docget.jsp?did=12858&prodName=TLP291-4), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOIC SO")
		(property "Reference" "U5"
			(at 0.24 0.4 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "TLP293-4"
			(at 0 6.1 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://toshiba.semicon-storage.com/info/TLP293-4_datasheet_en_20190520.pdf?did=15287&prodName=TLP293-4"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Quad DC Optocoupler, Vce 80V, CTR 50-100%, SOP16"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SOIC*4.55x10.3mm*P1.27mm*")
		(sheetname "/4-20mA Inputs/")
		(sheetfile "4-20mA Inputs.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -0.0475 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -3.25 -4.445)
			(size 1.6 0.55)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 205 "Net-(R41-Pad2)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at -3.25 -3.175)
			(size 1.6 0.55)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 72 "/4-20mA Inputs/IN2N")
			(pintype "passive")
		)
		(pad "3" smd roundrect
			(at -3.25 -1.905)
			(size 1.6 0.55)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 183 "Net-(Q5-E)")
			(pintype "passive")
		)
		(pad "4" smd roundrect
			(at -3.25 -0.635)
			(size 1.6 0.55)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 211 "Net-(RN3C-R3.2)")
			(pintype "passive")
		)
		(pad "5" smd roundrect
			(at -3.25 0.635)
			(size 1.6 0.55)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 209 "Net-(R47-Pad2)")
			(pintype "passive")
		)
		(pad "6" smd roundrect
			(at -3.25 1.905)
			(size 1.6 0.55)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 70 "/4-20mA Inputs/IN1N")
			(pintype "passive")
		)
		(pad "7" smd roundrect
			(at -3.25 3.175)
			(size 1.6 0.55)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 184 "Net-(Q6-E)")
			(pintype "passive")
		)
		(pad "8" smd roundrect
			(at -3.25 4.445)
			(size 1.6 0.55)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 207 "Net-(RN3A-R1.2)")
			(pintype "passive")
		)
		(pad "9" smd roundrect
			(at 3.25 4.445)
			(size 1.6 0.55)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 208 "Net-(R45-Pad1)")
			(pintype "passive")
		)
		(pad "10" smd roundrect
			(at 3.25 3.175)
			(size 1.6 0.55)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 9 "+5V")
			(pintype "passive")
		)
		(pad "11" smd roundrect
			(at 3.25 1.905)
			(size 1.6 0.55)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 210 "Net-(U6A-+)")
			(pintype "passive")
		)
		(pad "12" smd roundrect
			(at 3.25 0.635)
			(size 1.6 0.55)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 9 "+5V")
			(pintype "passive")
		)
		(pad "13" smd roundrect
			(at 3.25 -0.635)
			(size 1.6 0.55)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 212 "Net-(R51-Pad1)")
			(pintype "passive")
		)
		(pad "14" smd roundrect
			(at 3.25 -1.905)
			(size 1.6 0.55)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 9 "+5V")
			(pintype "passive")
		)
		(pad "15" smd roundrect
			(at 3.25 -3.175)
			(size 1.6 0.55)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 206 "Net-(U6B-+)")
			(pintype "passive")
		)
		(pad "16" smd roundrect
			(at 3.25 -4.445)
			(size 1.6 0.55)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 9 "+5V")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Package_SO.3dshapes/SOIC-16_4.55x10.3mm_P1.27mm.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Diode_SMD:D_SMA"
		(layer "F.Cu")
		(at 65.075 115.35 90)
		(descr "Diode SMA (DO-214AC)")
		(tags "Diode SMA (DO-214AC)")
		(property "Reference" "D7"
			(at -0.0225 0 90)
			(layer "F.SilkS")
		)
		(property "Value" "SMAJ18A"
			(at 0 2.6 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.littelfuse.com/media?resourcetype=datasheets&itemid=75e32973-b177-4ee3-a0ff-cedaf1abdb93&filename=smaj-datasheet"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "400W unidirectional Transient Voltage Suppressor, 18.0Vr, SMA(DO-214AC)"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "D*SMA*")
		(sheetname "/4-20mA Inputs/")
		(sheetfile "4-20mA Inputs.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at -0.0225 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -2 0 90)
			(size 2.5 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.1388888889)
			(net 75 "/4-20mA Inputs/IN3P")
			(pinfunction "A1")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 2 0 90)
			(size 2.5 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.1388888889)
			(net 74 "/4-20mA Inputs/IN3N")
			(pinfunction "A2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SMA.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "F.Cu")
		(at 200.955 80.99)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R72"
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "10"
			(at 0 1.65 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/4-20mAOutput/")
		(sheetfile "4-20mAOutput.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net 142 "Net-(IC6-OUT1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net 186 "Net-(Q8-G)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "SamacSys_Parts:SOIC127P600X175-8N"
		(layer "F.Cu")
		(at 181.9 60.5)
		(descr "SO 8_")
		(tags "Integrated Circuit")
		(property "Reference" "IC5"
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "LM258DT"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/lm158.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "LM258DT, Dual Operational Amplifier 1.1MHz 5 to 28V, 8-Pin SO"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Height" "1.75"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Part Number" "511-LM258D-TR"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Price/Stock" "https://www.mouser.co.uk/ProductDetail/STMicroelectronics/LM258DT?qs=EhGjr%2F0Q%252Bo8damG9%252BR9%2FhA%3D%3D"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Name" "STMicroelectronics"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Part_Number" "LM258DT"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/0-10VOutput/")
		(sheetfile "0-10VOutput.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -2.712 -1.905 90)
			(size 0.65 1.525)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 141 "/0-10VOutput/10V OUT3")
			(pinfunction "OUT1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -2.712 -0.635 90)
			(size 0.65 1.525)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 140 "Net-(IC5-IN1-)")
			(pinfunction "IN1-")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at -2.712 0.635 90)
			(size 0.65 1.525)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 54 "Net-(IC5-IN1+)")
			(pinfunction "IN1+")
			(pintype "passive")
		)
		(pad "4" smd rect
			(at -2.712 1.905 90)
			(size 0.65 1.525)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 24 "-12V")
			(pinfunction "VCC-")
			(pintype "passive")
		)
		(pad "5" smd rect
			(at 2.712 1.905 90)
			(size 0.65 1.525)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 55 "Net-(IC5-IN2+)")
			(pinfunction "IN2+")
			(pintype "passive")
		)
		(pad "6" smd rect
			(at 2.712 0.635 90)
			(size 0.65 1.525)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 139 "Net-(IC5-IN2-)")
			(pinfunction "IN2-")
			(pintype "passive")
		)
		(pad "7" smd rect
			(at 2.712 -0.635 90)
			(size 0.65 1.525)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 138 "/0-10VOutput/10V OUT4")
			(pinfunction "OUT2")
			(pintype "passive")
		)
		(pad "8" smd rect
			(at 2.712 -1.905 90)
			(size 0.65 1.525)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 13 "+12V")
			(pinfunction "VCC+")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "C:\\Users\\ESpurbeck\\Documents\\KiCad\\3rdparty\\SamacSys_Parts.3dshapes\\LM258DT.stp"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 190.5 66.9 180)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R63"
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "2.2k"
			(at 0 1.43 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/0-10VOutput/")
		(sheetfile "0-10VOutput.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 180)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 165 "/PWM_VOUT4")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0 180)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 53 "Net-(C53-Pad1)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "SamacSys_Parts:SOT95P237X112-3N"
		(layer "F.Cu")
		(at 132.4 57.05)
		(descr "-SOT-23")
		(tags "MOSFET (P-Channel)")
		(property "Reference" "Q3"
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "Si2323DDS-T1-GE3"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" "https://altium.componentsearchengine.com/Datasheets/2/SI2323DDS-T1-GE3.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "VISHAY - SI2323DDS-T1-GE3 - Power MOSFET, P Channel, 20 V, 5.3 A, 0.032 ohm, SOT-23, Surface Mount"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Height" "1.12"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Part Number" "78-SI2323DDS-T1-GE3"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Price/Stock" "https://www.mouser.co.uk/ProductDetail/Vishay-Semiconductors/SI2323DDS-T1-GE3?qs=vgn07B5hXavjZXK0uPQNiA%3D%3D"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Name" "Vishay"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Part_Number" "Si2323DDS-T1-GE3"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/Power Supply/")
		(sheetfile "Power Supply.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.05 -0.95 90)
			(size 0.6 1.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 181 "Net-(Q3-G)")
			(pinfunction "G")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -1.05 0.95 90)
			(size 0.6 1.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 9 "+5V")
			(pinfunction "S")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at 1.05 0 90)
			(size 0.6 1.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 21 "Net-(Q3-D)")
			(pinfunction "D")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "C:\\Users\\ESpurbeck\\Documents\\KiCad\\3rdparty\\SamacSys_Parts.3dshapes\\Si2323DDS-T1-GE3.stp"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 167.7 56.6 180)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C51"
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "220nF"
			(at 0 1.43 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/0-10VOutput/")
		(sheetfile "0-10VOutput.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 180)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 180)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 13 "+12V")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "F.Cu")
		(at 108.1 130.7)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C36"
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "1uF"
			(at 0 1.68 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/4-20mA Inputs/")
		(sheetfile "4-20mA Inputs.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 35 "/4-20mA Inputs/AIN3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_SO:TSSOP-10_3x3mm_P0.5mm"
		(layer "F.Cu")
		(at 107.6 121.1 -90)
		(descr "TSSOP10: plastic thin shrink small outline package; 10 leads; body width 3 mm; (see NXP SSOP-TSSOP-VSO-REFLOW.pdf and sot552-1_po.pdf)")
		(tags "SSOP 0.5")
		(property "Reference" "U8"
			(at 0 0 90)
			(layer "F.SilkS")
		)
		(property "Value" "ADS1115IDGS"
			(at 0 2.55 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/ads1113.pdf"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Ultra-Small, Low-Power, I2C-Compatible, 860-SPS, 16-Bit ADCs With Internal Reference, Oscillator, and Programmable Comparator, VSSOP-10"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TSSOP*3x3mm*P0.5mm*")
		(sheetname "/4-20mA Inputs/")
		(sheetfile "4-20mA Inputs.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -2.15 -1 270)
			(size 1.1 0.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 15 "+3.3V")
			(pinfunction "ADDR")
			(pintype "input")
		)
		(pad "2" smd rect
			(at -2.15 -0.5 270)
			(size 1.1 0.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 161 "/A2INT_I")
			(pinfunction "ALERT/RDY")
			(pintype "output")
		)
		(pad "3" smd rect
			(at -2.15 0 270)
			(size 1.1 0.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "4" smd rect
			(at -2.15 0.5 270)
			(size 1.1 0.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 47 "/4-20mA Inputs/AIN0")
			(pinfunction "AIN0")
			(pintype "input")
		)
		(pad "5" smd rect
			(at -2.15 1 270)
			(size 1.1 0.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 43 "/4-20mA Inputs/AIN1")
			(pinfunction "AIN1")
			(pintype "input")
		)
		(pad "6" smd rect
			(at 2.15 1 270)
			(size 1.1 0.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 39 "/4-20mA Inputs/AIN2")
			(pinfunction "AIN2")
			(pintype "input")
		)
		(pad "7" smd rect
			(at 2.15 0.5 270)
			(size 1.1 0.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 35 "/4-20mA Inputs/AIN3")
			(pinfunction "AIN3")
			(pintype "input")
		)
		(pad "8" smd rect
			(at 2.15 0 270)
			(size 1.1 0.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 15 "+3.3V")
			(pinfunction "VDD")
			(pintype "power_in")
		)
		(pad "9" smd rect
			(at 2.15 -0.5 270)
			(size 1.1 0.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 160 "/SDA")
			(pinfunction "SDA")
			(pintype "bidirectional")
		)
		(pad "10" smd rect
			(at 2.15 -1 270)
			(size 1.1 0.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 154 "/SCL")
			(pinfunction "SCL")
			(pintype "input")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Package_SO.3dshapes/TSSOP-10_3x3mm_P0.5mm.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1210_3225Metric"
		(layer "F.Cu")
		(at 131.925 60.975 180)
		(descr "Capacitor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C24"
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "22uF"
			(at 0 2.3 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/Power Supply/")
		(sheetfile "Power Supply.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.475 0 180)
			(size 1.15 2.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.217391)
			(net 24 "-12V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.475 0 180)
			(size 1.15 2.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.217391)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1210_3225Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 78.55 95.05 -90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R21"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "10k"
			(at 0 1.43 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/0-10V INPUTS/")
		(sheetfile "0-10V INPUTS.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 270)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 132 "/0-10V INPUTS/+IN_A")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0 270)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 137.225 60.775)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R11"
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "100"
			(at 0 1.43 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Power Supply/")
		(sheetfile "Power Supply.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 9 "+5V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 20 "Net-(U2-ENN)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 186.0675 86.59)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C66"
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "220nF"
			(at 0 1.43 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/4-20mAOutput/")
		(sheetfile "4-20mAOutput.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 64 "/O_CHECK3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 79.005 82.075 90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R23"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "10k"
			(at 0 1.43 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/0-10V INPUTS/")
		(sheetfile "0-10V INPUTS.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 90)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 128 "/0-10V INPUTS/+IN_D")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0 90)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 170.775 67.1)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R58"
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "2.2k"
			(at 0 1.43 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/0-10VOutput/")
		(sheetfile "0-10VOutput.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 158 "/PWM_VOUT2")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 50 "Net-(C48-Pad1)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "SamacSys_Parts:L_Bourns_SRR4528A"
		(layer "F.Cu")
		(at 155.825 109.925 180)
		(property "Reference" "L3"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "4.7uH"
			(at 0 1 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Inductor, small symbol"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Choke_* *Coil* Inductor_* L_*")
		(sheetname "/Power Supply/")
		(sheetfile "Power Supply.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -2.1 0 180)
			(size 1.6 5.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 18 "Net-(C17-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 2.1 0 180)
			(size 1.6 5.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.15)
			(net 19 "+12VA")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 75.255 121.4167 180)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R42"
			(at 0 0 180)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "1M"
			(at 0 1.43 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/4-20mA Inputs/")
		(sheetfile "4-20mA Inputs.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 180)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 72 "/4-20mA Inputs/IN2N")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0 180)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "F.Cu")
		(at 106.125 128.525 180)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C39"
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "1uF"
			(at 0 1.68 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/4-20mA Inputs/")
		(sheetfile "4-20mA Inputs.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0 180)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 39 "/4-20mA Inputs/AIN2")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0 180)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_1206_3216Metric"
		(layer "F.Cu")
		(at 82.125 115.725)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R30"
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "140"
			(at 0 1.83 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/4-20mA Inputs/")
		(sheetfile "4-20mA Inputs.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.4625 0)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.222222)
			(net 2 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.4625 0)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.222222)
			(net 199 "Net-(RN2A-R1.2)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Samacsys:SOIC127P600X175-8N"
		(layer "F.Cu")
		(at 181.66 75.9675 -90)
		(descr "SO-8 batwing")
		(tags "Integrated Circuit")
		(property "Reference" "IC1"
			(at 0 0 90)
			(layer "F.SilkS")
		)
		(property "Value" "LM317LD13TR"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/lm217l.pdf"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "LM317LD13TR, Voltage Regulator, 0.2A Adjustable 1.2  37 V, 8-Pin, SOIC"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Height" "1.75"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Part Number" "511-LM317LD13TR"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Price/Stock" "https://www.mouser.co.uk/ProductDetail/STMicroelectronics/LM317LD13TR?qs=01cQMEOqxGSoMXHqAObrAA%3D%3D"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Name" "STMicroelectronics"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Part_Number" "LM317LD13TR"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/Power Supply/")
		(sheetfile "Power Supply.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -2.712 -1.905)
			(size 0.65 1.525)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 13 "+12V")
			(pinfunction "VIN")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -2.712 -0.635)
			(size 0.65 1.525)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 14 "+5.5V")
			(pinfunction "VOUT_1")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at -2.712 0.635)
			(size 0.65 1.525)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 14 "+5.5V")
			(pinfunction "VOUT_2")
			(pintype "passive")
		)
		(pad "4" smd rect
			(at -2.712 1.905)
			(size 0.65 1.525)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 117 "Net-(IC1-ADJ)")
			(pinfunction "ADJ")
			(pintype "passive")
		)
		(pad "5" smd rect
			(at 2.712 1.905)
			(size 0.65 1.525)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 116 "unconnected-(IC1-NC_1-Pad5)")
			(pinfunction "NC_1")
			(pintype "passive+no_connect")
		)
		(pad "6" smd rect
			(at 2.712 0.635)
			(size 0.65 1.525)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 14 "+5.5V")
			(pinfunction "VOUT_3")
			(pintype "passive")
		)
		(pad "7" smd rect
			(at 2.712 -0.635)
			(size 0.65 1.525)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 14 "+5.5V")
			(pinfunction "VOUT_4")
			(pintype "passive")
		)
		(pad "8" smd rect
			(at 2.712 -1.905)
			(size 0.65 1.525)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 118 "unconnected-(IC1-NC_2-Pad8)")
			(pinfunction "NC_2")
			(pintype "passive+no_connect")
		)
		(embedded_fonts no)
		(model "${KIPRJMOD}/Samacsys.3dshapes/LM317LD13TR.stp"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "F.Cu")
		(at 157.5 66.9 180)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C46"
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "1uF"
			(at 0 1.68 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/0-10VOutput/")
		(sheetfile "0-10VOutput.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0 180)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 48 "Net-(C46-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0 180)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Diode_SMD:D_SOD-323"
		(layer "F.Cu")
		(at 142.65 62.575 180)
		(descr "SOD-323")
		(tags "SOD-323")
		(property "Reference" "D3"
			(at -0.0225 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "1N5819WS"
			(at 0.1 1.9 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://datasheet.lcsc.com/lcsc/2204281430_Guangdong-Hottech-1N5819WS_C191023.pdf"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "40V 600mV@1A 1A SOD-323 Schottky Barrier Diodes, SOD-323"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "D*SOD?323*")
		(sheetname "/Power Supply/")
		(sheetfile "Power Supply.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at -0.0225 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.05 0 180)
			(size 0.6 0.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 13 "+12V")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.05 0 180)
			(size 0.6 0.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 68 "Net-(D3-A)")
			(pinfunction "A")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SOD-323.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 184.575 71.45)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C11"
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "100nF"
			(at 0 1.43 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/Power Supply/")
		(sheetfile "Power Supply.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 13 "+12V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 187.675 60.1 180)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R68"
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "4.53k"
			(at 0 1.43 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/0-10VOutput/")
		(sheetfile "0-10VOutput.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 180)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 15 "+3.3V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0 180)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 139 "Net-(IC5-IN2-)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 75.255 106.9)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R26"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "1M"
			(at 0 1.43 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/4-20mA Inputs/")
		(sheetfile "4-20mA Inputs.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 77 "/4-20mA Inputs/IN4N")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "F.Cu")
		(at 188.6175 95.99)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C67"
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "1uF"
			(at 0 1.68 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/4-20mAOutput/")
		(sheetfile "4-20mAOutput.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 65 "Net-(RN8A-R1.1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 99.975 126.25 -90)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C43"
			(at 0 0 90)
			(layer "F.SilkS")
		)
		(property "Value" "220nF"
			(at 0 1.43 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/4-20mA Inputs/")
		(sheetfile "4-20mA Inputs.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 270)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 45 "Net-(U6A--)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 270)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 44 "Net-(Q5-B)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "F.Cu")
		(at 195.8675 105.19)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R77"
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "10"
			(at 0 1.65 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/4-20mAOutput/")
		(sheetfile "4-20mAOutput.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net 146 "Net-(IC7-OUT2)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net 192 "Net-(Q11-G)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "SamacSys_Parts:DMG4800LFG7"
		(layer "F.Cu")
		(at 205.6875 98.99 -90)
		(descr "DMG4800LFG-7")
		(tags "MOSFET (N-Channel)")
		(property "Reference" "Q10"
			(at 0 0 90)
			(layer "F.SilkS")
		)
		(property "Value" "DMG4800LFG-7"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" "https://www.diodes.com//assets/Datasheets/ds31785.pdf"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "N-Channel 30 V 7.44A (Ta) 940mW (Ta) Surface Mount U-DFN3030-8"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Height" "0.63"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Part Number" "621-DMG4800LFG-7"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Price/Stock" "https://www.mouser.co.uk/ProductDetail/Diodes-Incorporated/DMG4800LFG-7?qs=f4CYDwCO%252B%2FEVatAzjmPrMQ%3D%3D"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Name" "Diodes Incorporated"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Part_Number" "DMG4800LFG-7"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/4-20mAOutput/")
		(sheetfile "4-20mAOutput.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -0.975 1.3 270)
			(size 0.39 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 149 "Net-(IC7-IN1-)")
			(pinfunction "S_1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.325 1.3 270)
			(size 0.39 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 149 "Net-(IC7-IN1-)")
			(pinfunction "S_2")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at 0.325 1.3 270)
			(size 0.39 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 149 "Net-(IC7-IN1-)")
			(pinfunction "S_3")
			(pintype "passive")
		)
		(pad "4" smd rect
			(at 0.975 1.3 270)
			(size 0.39 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 190 "Net-(Q10-G)")
			(pinfunction "G")
			(pintype "passive")
		)
		(pad "5" smd rect
			(at 0 -0.38)
			(size 2.49 2.59)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 189 "/4-20mAOutput/OUT3")
			(pinfunction "D")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "C:\\Users\\ESpurbeck\\Documents\\KiCad\\3rdparty\\SamacSys_Parts.3dshapes\\DMG4800LFG-7.stp"
			(offset
				(xyz -74.85999949 42.70000012 0.6000000148)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 -180 0)
			)
		)
	)
	(footprint "Package_SO:SOIC-16_4.55x10.3mm_P1.27mm"
		(layer "F.Cu")
		(at 89.425 111.475)
		(descr "SOIC, 16 Pin (https://toshiba.semicon-storage.com/info/docget.jsp?did=12858&prodName=TLP291-4), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOIC SO")
		(property "Reference" "U7"
			(at 0 -0.0475 0)
			(layer "F.SilkS")
		)
		(property "Value" "TLP293-4"
			(at 0 6.1 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://toshiba.semicon-storage.com/info/TLP293-4_datasheet_en_20190520.pdf?did=15287&prodName=TLP293-4"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Quad DC Optocoupler, Vce 80V, CTR 50-100%, SOP16"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SOIC*4.55x10.3mm*P1.27mm*")
		(sheetname "/4-20mA Inputs/")
		(sheetfile "4-20mA Inputs.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -0.0475 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -3.25 -4.445)
			(size 1.6 0.55)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 197 "Net-(R27-Pad2)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at -3.25 -3.175)
			(size 1.6 0.55)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 77 "/4-20mA Inputs/IN4N")
			(pintype "passive")
		)
		(pad "3" smd roundrect
			(at -3.25 -1.905)
			(size 1.6 0.55)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 185 "Net-(Q7-E)")
			(pintype "passive")
		)
		(pad "4" smd roundrect
			(at -3.25 -0.635)
			(size 1.6 0.55)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 203 "Net-(RN2C-R3.2)")
			(pintype "passive")
		)
		(pad "5" smd roundrect
			(at -3.25 0.635)
			(size 1.6 0.55)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 201 "Net-(R35-Pad2)")
			(pintype "passive")
		)
		(pad "6" smd roundrect
			(at -3.25 1.905)
			(size 1.6 0.55)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 74 "/4-20mA Inputs/IN3N")
			(pintype "passive")
		)
		(pad "7" smd roundrect
			(at -3.25 3.175)
			(size 1.6 0.55)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 182 "Net-(Q4-E)")
			(pintype "passive")
		)
		(pad "8" smd roundrect
			(at -3.25 4.445)
			(size 1.6 0.55)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 199 "Net-(RN2A-R1.2)")
			(pintype "passive")
		)
		(pad "9" smd roundrect
			(at 3.25 4.445)
			(size 1.6 0.55)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 200 "Net-(R31-Pad1)")
			(pintype "passive")
		)
		(pad "10" smd roundrect
			(at 3.25 3.175)
			(size 1.6 0.55)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 9 "+5V")
			(pintype "passive")
		)
		(pad "11" smd roundrect
			(at 3.25 1.905)
			(size 1.6 0.55)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 202 "Net-(U6C-+)")
			(pintype "passive")
		)
		(pad "12" smd roundrect
			(at 3.25 0.635)
			(size 1.6 0.55)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 9 "+5V")
			(pintype "passive")
		)
		(pad "13" smd roundrect
			(at 3.25 -0.635)
			(size 1.6 0.55)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 204 "Net-(R39-Pad1)")
			(pintype "passive")
		)
		(pad "14" smd roundrect
			(at 3.25 -1.905)
			(size 1.6 0.55)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 9 "+5V")
			(pintype "passive")
		)
		(pad "15" smd roundrect
			(at 3.25 -3.175)
			(size 1.6 0.55)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 198 "Net-(U6D-+)")
			(pintype "passive")
		)
		(pad "16" smd roundrect
			(at 3.25 -4.445)
			(size 1.6 0.55)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 9 "+5V")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Package_SO.3dshapes/SOIC-16_4.55x10.3mm_P1.27mm.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 77.8 92.775)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R20"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "22k"
			(at 0 1.43 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/0-10V INPUTS/")
		(sheetfile "0-10V INPUTS.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 151 "/0-10V INPUTS/IN10V2")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 132 "/0-10V INPUTS/+IN_A")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "F.Cu")
		(at 165.05 111.55 -90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C17"
			(at 0 0 90)
			(layer "F.SilkS")
		)
		(property "Value" "1uF"
			(at 0 1.68 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/Power Supply/")
		(sheetfile "Power Supply.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0 270)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 18 "Net-(C17-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0 270)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 17 "GNDA")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0201_0603Metric"
		(layer "F.Cu")
		(at 107.95 126.495 -90)
		(descr "Resistor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R33"
			(at 0 0 90)
			(layer "F.SilkS")
		)
		(property "Value" "2.2k"
			(at 0 1.05 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/4-20mA Inputs/")
		(sheetfile "4-20mA Inputs.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "" smd roundrect
			(at -0.345 0 270)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0.345 0 270)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "1" smd roundrect
			(at -0.32 0 270)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 160 "/SDA")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.32 0 270)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 15 "+3.3V")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0201_0603Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "SamacSys_Parts:DMG4800LFG7"
		(layer "F.Cu")
		(at 165.17 120 -90)
		(descr "DMG4800LFG-7")
		(tags "MOSFET (N-Channel)")
		(property "Reference" "Q12"
			(at 0 0 90)
			(layer "F.SilkS")
		)
		(property "Value" "DMG4800LFG-7"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" "https://www.diodes.com//assets/Datasheets/ds31785.pdf"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "N-Channel 30 V 7.44A (Ta) 940mW (Ta) Surface Mount U-DFN3030-8"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Height" "0.63"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Part Number" "621-DMG4800LFG-7"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Price/Stock" "https://www.mouser.co.uk/ProductDetail/Diodes-Incorporated/DMG4800LFG-7?qs=f4CYDwCO%252B%2FEVatAzjmPrMQ%3D%3D"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Name" "Diodes Incorporated"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Part_Number" "DMG4800LFG-7"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/DigitalIO/")
		(sheetfile "DigitalIO.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -0.975 1.3 270)
			(size 0.39 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 17 "GNDA")
			(pinfunction "S_1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.325 1.3 270)
			(size 0.39 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 17 "GNDA")
			(pinfunction "S_2")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at 0.325 1.3 270)
			(size 0.39 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 17 "GNDA")
			(pinfunction "S_3")
			(pintype "passive")
		)
		(pad "4" smd rect
			(at 0.975 1.3 270)
			(size 0.39 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 110 "Net-(HY2-EMITTER_4)")
			(pinfunction "G")
			(pintype "passive")
		)
		(pad "5" smd rect
			(at 0 -0.38)
			(size 2.49 2.59)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 180 "/DigitalIO/OD_OUT1")
			(pinfunction "D")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "C:\\Users\\ESpurbeck\\Documents\\KiCad\\3rdparty\\SamacSys_Parts.3dshapes\\DMG4800LFG-7.stp"
			(offset
				(xyz -74.85999949 42.70000012 0.6000000148)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 -180 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "F.Cu")
		(at 185.55 65.1)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C55"
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "1uF"
			(at 0 1.68 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/0-10VOutput/")
		(sheetfile "0-10VOutput.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 55 "Net-(IC5-IN2+)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 135.525 71.5 90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R14"
			(at 0 0 90)
			(layer "F.SilkS")
		)
		(property "Value" "1M"
			(at 0 1.43 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Power Supply/")
		(sheetfile "Power Supply.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 90)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 26 "Net-(U2-VNEG)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0 90)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 24 "-12V")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_1206_3216Metric"
		(layer "F.Cu")
		(at 75.275 109.5675)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R27"
			(at 0.275 1.5075 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "140"
			(at 0 1.83 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/4-20mA Inputs/")
		(sheetfile "4-20mA Inputs.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.4625 0)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.222222)
			(net 76 "/4-20mA Inputs/IN4P")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.4625 0)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.222222)
			(net 197 "Net-(R27-Pad2)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "SamacSys_Parts:L_Bourns_SRR4528A"
		(layer "F.Cu")
		(at 134.55 51.175)
		(property "Reference" "L4"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "4.7uH"
			(at 0 1 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Inductor, small symbol"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Choke_* *Coil* Inductor_* L_*")
		(sheetname "/Power Supply/")
		(sheetfile "Power Supply.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -2.1 0)
			(size 1.6 5.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 21 "Net-(Q3-D)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 2.1 0)
			(size 1.6 5.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.15)
			(net 68 "Net-(D3-A)")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "Resistor_SMD:R_1210_3225Metric"
		(layer "F.Cu")
		(at 175.0092 121.21)
		(descr "Resistor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R80"
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "4.7k"
			(at 0 2.28 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/DigitalIO/")
		(sheetfile "DigitalIO.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.4625 0)
			(size 1.125 2.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.222222)
			(net 103 "/DigitalIO/OP4")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.4625 0)
			(size 1.125 2.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.222222)
			(net 98 "Net-(HY1-ANODE_1)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1210_3225Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 75.1 112.575 90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R36"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "1M"
			(at 0 1.43 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/4-20mA Inputs/")
		(sheetfile "4-20mA Inputs.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 90)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 74 "/4-20mA Inputs/IN3N")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0 90)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 140.05 53.175)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C30"
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "220nF"
			(at 0 1.43 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/0-10V INPUTS/")
		(sheetfile "0-10V INPUTS.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 9 "+5V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 162.15 55.5 180)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C50"
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "220nF"
			(at 0 1.43 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/0-10VOutput/")
		(sheetfile "0-10VOutput.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 180)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 180)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 24 "-12V")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "F.Cu")
		(at 185.2675 99.19 90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C65"
			(at 0 0 90)
			(layer "F.SilkS")
		)
		(property "Value" "1uF"
			(at 0 1.68 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/4-20mAOutput/")
		(sheetfile "4-20mAOutput.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0 90)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 63 "Net-(RN8C-R3.1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0 90)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "SamacSys_Parts:L_Bourns_SRR4528A"
		(layer "F.Cu")
		(at 163.625 105.3)
		(property "Reference" "L2"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "4.7uH"
			(at 0 1 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Inductor, small symbol"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Choke_* *Coil* Inductor_* L_*")
		(sheetname "/Power Supply/")
		(sheetfile "Power Supply.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -2.1 0)
			(size 1.6 5.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 9 "+5V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 2.1 0)
			(size 1.6 5.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.15)
			(net 16 "Net-(U3-VI+)")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "SamacSys_Parts:APTD1608ZGCK"
		(layer "F.Cu")
		(at 190.455 131.4675 180)
		(descr "APTD1608ZGCK-1")
		(tags "LED")
		(property "Reference" "D10"
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "LED_Small"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Light emitting diode, small symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pin" "1=K 2=A"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "LED* LED_SMD:* LED_THT:*")
		(sheetname "/DigitalIO/")
		(sheetfile "DigitalIO.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -0.825 0 270)
			(size 0.8 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 80 "Net-(D10-K)")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 0.825 0 270)
			(size 0.8 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 92 "/DigitalIO/OP2")
			(pinfunction "A")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "C:\\Users\\ESpurbeck\\Documents\\KiCad\\3rdparty\\SamacSys_Parts.3dshapes\\APTD1608ZGCK.stp"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 90 -180 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "F.Cu")
		(at 130.125 52.275 -90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C21"
			(at 0 0 90)
			(layer "F.SilkS")
		)
		(property "Value" "4.7uF"
			(at 0 1.68 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/Power Supply/")
		(sheetfile "Power Supply.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0 270)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 21 "Net-(Q3-D)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0 270)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 194.255 131.4675 -90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R85"
			(at 0 0 90)
			(layer "F.SilkS")
		)
		(property "Value" "15k"
			(at 0 -1.4 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/DigitalIO/")
		(sheetfile "DigitalIO.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 270)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 82 "/DigitalIO/VEX2")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0 270)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 80 "Net-(D10-K)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "F.Cu")
		(at 165.175 100.55 180)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C16"
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "2.2uF"
			(at 0 1.68 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/Power Supply/")
		(sheetfile "Power Supply.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0 180)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 16 "Net-(U3-VI+)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0 180)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "F.Cu")
		(at 194.7175 93.59)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C69"
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "1uF"
			(at 0 1.68 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/4-20mAOutput/")
		(sheetfile "4-20mAOutput.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 67 "Net-(IC7-IN1+)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "F.Cu")
		(at 104.425 106.8 90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C45"
			(at 0 0 90)
			(layer "F.SilkS")
		)
		(property "Value" "1uF"
			(at 0 1.68 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/4-20mA Inputs/")
		(sheetfile "4-20mA Inputs.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0 90)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 47 "/4-20mA Inputs/AIN0")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0 90)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 182.85 83.65 180)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C62"
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "220nF"
			(at 0 1.43 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/4-20mAOutput/")
		(sheetfile "4-20mAOutput.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 180)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 60 "/O_CHECK1")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 180)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Diode_SMD:D_SMA"
		(layer "F.Cu")
		(at 65.075 107.5675 90)
		(descr "Diode SMA (DO-214AC)")
		(tags "Diode SMA (DO-214AC)")
		(property "Reference" "D8"
			(at -0.0225 0 90)
			(layer "F.SilkS")
		)
		(property "Value" "SMAJ18A"
			(at 0 2.6 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.littelfuse.com/media?resourcetype=datasheets&itemid=75e32973-b177-4ee3-a0ff-cedaf1abdb93&filename=smaj-datasheet"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "400W unidirectional Transient Voltage Suppressor, 18.0Vr, SMA(DO-214AC)"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "D*SMA*")
		(sheetname "/4-20mA Inputs/")
		(sheetfile "4-20mA Inputs.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at -0.0225 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -2 0 90)
			(size 2.5 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.1388888889)
			(net 76 "/4-20mA Inputs/IN4P")
			(pinfunction "A1")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 2 0 90)
			(size 2.5 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.1388888889)
			(net 77 "/4-20mA Inputs/IN4N")
			(pinfunction "A2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SMA.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 99.18 114.45 90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R32"
			(at 0 0 90)
			(layer "F.SilkS")
		)
		(property "Value" "49.9"
			(at 0 1.43 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/4-20mA Inputs/")
		(sheetfile "4-20mA Inputs.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 90)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0 90)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 200 "Net-(R31-Pad1)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 184.2675 89.19)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C64"
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "220nF"
			(at 0 1.43 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/4-20mAOutput/")
		(sheetfile "4-20mAOutput.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 62 "/O_CHECK4")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_1206_3216Metric"
		(layer "F.Cu")
		(at 205.3175 103.79)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R79"
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "140"
			(at 0 1.83 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/4-20mAOutput/")
		(sheetfile "4-20mAOutput.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.4625 0)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.222222)
			(net 148 "Net-(IC7-IN2-)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.4625 0)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.222222)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 93.8 93.075 -90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R19"
			(at 0 0 90)
			(layer "F.SilkS")
		)
		(property "Value" "2.2k"
			(at 0 1.43 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/0-10V INPUTS/")
		(sheetfile "0-10V INPUTS.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 270)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 154 "/SCL")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0 270)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 15 "+3.3V")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "SamacSys_Parts:DMG4800LFG7"
		(layer "F.Cu")
		(at 142.3267 119.8475)
		(descr "DMG4800LFG-7")
		(tags "MOSFET (N-Channel)")
		(property "Reference" "Q15"
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "DMG4800LFG-7"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" "https://www.diodes.com//assets/Datasheets/ds31785.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "N-Channel 30 V 7.44A (Ta) 940mW (Ta) Surface Mount U-DFN3030-8"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Height" "0.63"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Part Number" "621-DMG4800LFG-7"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Price/Stock" "https://www.mouser.co.uk/ProductDetail/Diodes-Incorporated/DMG4800LFG-7?qs=f4CYDwCO%252B%2FEVatAzjmPrMQ%3D%3D"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Name" "Diodes Incorporated"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Part_Number" "DMG4800LFG-7"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/DigitalIO/")
		(sheetfile "DigitalIO.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -0.975 1.3)
			(size 0.39 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 17 "GNDA")
			(pinfunction "S_1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.325 1.3)
			(size 0.39 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 17 "GNDA")
			(pinfunction "S_2")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at 0.325 1.3)
			(size 0.39 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 17 "GNDA")
			(pinfunction "S_3")
			(pintype "passive")
		)
		(pad "4" smd rect
			(at 0.975 1.3)
			(size 0.39 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 113 "Net-(HY2-EMITTER_1)")
			(pinfunction "G")
			(pintype "passive")
		)
		(pad "5" smd rect
			(at 0 -0.38 90)
			(size 2.49 2.59)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 195 "/DigitalIO/OD_OUT4")
			(pinfunction "D")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "C:\\Users\\ESpurbeck\\Documents\\KiCad\\3rdparty\\SamacSys_Parts.3dshapes\\DMG4800LFG-7.stp"
			(offset
				(xyz -74.85999949 42.70000012 0.6000000148)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 -180 0)
			)
		)
	)
	(footprint "SamacSys_Parts:SOIC127P600X175-8N"
		(layer "F.Cu")
		(at 196.0675 81.99 -90)
		(descr "SO 8_")
		(tags "Integrated Circuit")
		(property "Reference" "IC6"
			(at 0 0 90)
			(layer "F.SilkS")
		)
		(property "Value" "LM258DT"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/lm158.pdf"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "LM258DT, Dual Operational Amplifier 1.1MHz 5 to 28V, 8-Pin SO"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Height" "1.75"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Part Number" "511-LM258D-TR"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Price/Stock" "https://www.mouser.co.uk/ProductDetail/STMicroelectronics/LM258DT?qs=EhGjr%2F0Q%252Bo8damG9%252BR9%2FhA%3D%3D"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Name" "STMicroelectronics"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Part_Number" "LM258DT"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/4-20mAOutput/")
		(sheetfile "4-20mAOutput.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -2.712 -1.905)
			(size 0.65 1.525)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 142 "Net-(IC6-OUT1)")
			(pinfunction "OUT1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -2.712 -0.635)
			(size 0.65 1.525)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 143 "Net-(IC6-IN1-)")
			(pinfunction "IN1-")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at -2.712 0.635)
			(size 0.65 1.525)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 57 "Net-(IC6-IN1+)")
			(pinfunction "IN1+")
			(pintype "passive")
		)
		(pad "4" smd rect
			(at -2.712 1.905)
			(size 0.65 1.525)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "GND")
			(pinfunction "VCC-")
			(pintype "passive")
		)
		(pad "5" smd rect
			(at 2.712 1.905)
			(size 0.65 1.525)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 59 "Net-(IC6-IN2+)")
			(pinfunction "IN2+")
			(pintype "passive")
		)
		(pad "6" smd rect
			(at 2.712 0.635)
			(size 0.65 1.525)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 145 "Net-(IC6-IN2-)")
			(pinfunction "IN2-")
			(pintype "passive")
		)
		(pad "7" smd rect
			(at 2.712 -0.635)
			(size 0.65 1.525)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 144 "Net-(IC6-OUT2)")
			(pinfunction "OUT2")
			(pintype "passive")
		)
		(pad "8" smd rect
			(at 2.712 -1.905)
			(size 0.65 1.525)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 5 "+24V")
			(pinfunction "VCC+")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "C:\\Users\\ESpurbeck\\Documents\\KiCad\\3rdparty\\SamacSys_Parts.3dshapes\\LM258DT.stp"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 138.075 57.575 180)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C20"
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "100nF"
			(at 0 1.43 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/Power Supply/")
		(sheetfile "Power Supply.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 180)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 20 "Net-(U2-ENN)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 180)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "SamacSys_Parts:DMG4800LFG7"
		(layer "F.Cu")
		(at 149.9933 119.8475)
		(descr "DMG4800LFG-7")
		(tags "MOSFET (N-Channel)")
		(property "Reference" "Q14"
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "DMG4800LFG-7"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" "https://www.diodes.com//assets/Datasheets/ds31785.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "N-Channel 30 V 7.44A (Ta) 940mW (Ta) Surface Mount U-DFN3030-8"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Height" "0.63"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Part Number" "621-DMG4800LFG-7"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Price/Stock" "https://www.mouser.co.uk/ProductDetail/Diodes-Incorporated/DMG4800LFG-7?qs=f4CYDwCO%252B%2FEVatAzjmPrMQ%3D%3D"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Name" "Diodes Incorporated"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Part_Number" "DMG4800LFG-7"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/DigitalIO/")
		(sheetfile "DigitalIO.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -0.975 1.3)
			(size 0.39 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 17 "GNDA")
			(pinfunction "S_1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.325 1.3)
			(size 0.39 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 17 "GNDA")
			(pinfunction "S_2")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at 0.325 1.3)
			(size 0.39 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 17 "GNDA")
			(pinfunction "S_3")
			(pintype "passive")
		)
		(pad "4" smd rect
			(at 0.975 1.3)
			(size 0.39 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 108 "Net-(HY2-EMITTER_2)")
			(pinfunction "G")
			(pintype "passive")
		)
		(pad "5" smd rect
			(at 0 -0.38 90)
			(size 2.49 2.59)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 194 "/DigitalIO/OD_OUT3")
			(pinfunction "D")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "C:\\Users\\ESpurbeck\\Documents\\KiCad\\3rdparty\\SamacSys_Parts.3dshapes\\DMG4800LFG-7.stp"
			(offset
				(xyz -74.85999949 42.70000012 0.6000000148)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 -180 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 137.225 71.5 90)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C26"
			(at 0 0 90)
			(layer "F.SilkS")
		)
		(property "Value" "7.5pF"
			(at 0 1.43 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/Power Supply/")
		(sheetfile "Power Supply.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 90)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 26 "Net-(U2-VNEG)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 90)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 24 "-12V")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_SMD:SOT-23"
		(layer "F.Cu")
		(at 130.4 118.52 -90)
		(descr "SOT, 3 Pin (JEDEC TO-236 Var AB https://www.jedec.org/document_search?search_api_views_fulltext=TO-236), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOT TO_SOT_SMD")
		(property "Reference" "D17"
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "SM712_SOT23"
			(at 0 2.4 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.littelfuse.com/~/media/electronics/datasheets/tvs_diode_arrays/littelfuse_tvs_diode_array_sm712_datasheet.pdf.pdf"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "7V/12V, 600W Asymmetrical TVS Diode Array, SOT-23"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SOT?23*")
		(sheetname "/Communication/")
		(sheetfile "Communication.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9375 -0.95 270)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 91 "/Communication/RS485A")
			(pinfunction "A1")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at -0.9375 0.95 270)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 90 "/Communication/RS485B")
			(pinfunction "A2")
			(pintype "passive")
		)
		(pad "3" smd roundrect
			(at 0.9375 0 270)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "common")
			(pintype "input")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "SamacSys_Parts:SOIC127P700X230-16N"
		(layer "F.Cu")
		(at 185.66 112.535 90)
		(descr "TLP293-4(GB-TP,E-1")
		(tags "Circulator or Directional Coupler")
		(property "Reference" "HY1"
			(at 0 0 90)
			(layer "F.SilkS")
		)
		(property "Value" "TLP293-4_GB-TP,E"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" "https://componentsearchengine.com/Datasheets/1/TLP293-4(GB-TP,E.pdf"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Transistor Output Optocouplers 4ch Transistor opto coupler"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Height" "2.3"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Part Number" "757-TLP293-4GB-TPE"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Price/Stock" "https://www.mouser.co.uk/ProductDetail/Toshiba/TLP293-4GB-TPE?qs=U6BGiFaJGDs%252BkJtAfW6%2FTw%3D%3D"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Name" "Toshiba"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Part_Number" "TLP293-4(GB-TP,E"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/DigitalIO/")
		(sheetfile "DigitalIO.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -3.25 -4.445 180)
			(size 0.65 1.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 98 "Net-(HY1-ANODE_1)")
			(pinfunction "ANODE_1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -3.25 -3.175 180)
			(size 0.65 1.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 79 "/DigitalIO/VEX4")
			(pinfunction "CATHODE_1")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at -3.25 -1.905 180)
			(size 0.65 1.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 100 "Net-(HY1-ANODE_2)")
			(pinfunction "ANODE_2")
			(pintype "passive")
		)
		(pad "4" smd rect
			(at -3.25 -0.635 180)
			(size 0.65 1.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 81 "/DigitalIO/VEX3")
			(pinfunction "CATHODE_2")
			(pintype "passive")
		)
		(pad "5" smd rect
			(at -3.25 0.635 180)
			(size 0.65 1.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 95 "Net-(HY1-ANODE_3)")
			(pinfunction "ANODE_3")
			(pintype "passive")
		)
		(pad "6" smd rect
			(at -3.25 1.905 180)
			(size 0.65 1.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 82 "/DigitalIO/VEX2")
			(pinfunction "CATHODE_3")
			(pintype "passive")
		)
		(pad "7" smd rect
			(at -3.25 3.175 180)
			(size 0.65 1.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 93 "Net-(HY1-ANODE_4)")
			(pinfunction "ANODE_4")
			(pintype "passive")
		)
		(pad "8" smd rect
			(at -3.25 4.445 180)
			(size 0.65 1.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 85 "/DigitalIO/VEX1")
			(pinfunction "CATHODE_4")
			(pintype "passive")
		)
		(pad "9" smd rect
			(at 3.25 4.445 180)
			(size 0.65 1.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "GND")
			(pinfunction "EMITTER_1")
			(pintype "passive")
		)
		(pad "10" smd rect
			(at 3.25 3.175 180)
			(size 0.65 1.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 99 "/OPTO_IN4")
			(pinfunction "COLLECTOR_1")
			(pintype "passive")
		)
		(pad "11" smd rect
			(at 3.25 1.905 180)
			(size 0.65 1.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "GND")
			(pinfunction "EMITTER_2")
			(pintype "passive")
		)
		(pad "12" smd rect
			(at 3.25 0.635 180)
			(size 0.65 1.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 97 "/OPTO_IN3")
			(pinfunction "COLLECTOR_2")
			(pintype "passive")
		)
		(pad "13" smd rect
			(at 3.25 -0.635 180)
			(size 0.65 1.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "GND")
			(pinfunction "EMITTER_3")
			(pintype "passive")
		)
		(pad "14" smd rect
			(at 3.25 -1.905 180)
			(size 0.65 1.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 102 "/OPTO_IN2")
			(pinfunction "COLLECTOR_3")
			(pintype "passive")
		)
		(pad "15" smd rect
			(at 3.25 -3.175 180)
			(size 0.65 1.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "GND")
			(pinfunction "EMITTER_4")
			(pintype "passive")
		)
		(pad "16" smd rect
			(at 3.25 -4.445 180)
			(size 0.65 1.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 101 "/OPTO_IN1")
			(pinfunction "COLLECTOR_4")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "C:\\Users\\ESpurbeck\\Documents\\KiCad\\3rdparty\\SamacSys_Parts.3dshapes\\TLP293-4_GB-TP,E.stp"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 176.1 61.9)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R67"
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "6.49k"
			(at 0 1.43 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/0-10VOutput/")
		(sheetfile "0-10VOutput.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 140 "Net-(IC5-IN1-)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "SamacSys_Parts:APTD1608ZGCK"
		(layer "F.Cu")
		(at 198.055 131.4675 180)
		(descr "APTD1608ZGCK-1")
		(tags "LED")
		(property "Reference" "D9"
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "LED_Small"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Light emitting diode, small symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pin" "1=K 2=A"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "LED* LED_SMD:* LED_THT:*")
		(sheetname "/DigitalIO/")
		(sheetfile "DigitalIO.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -0.825 0 270)
			(size 0.8 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 78 "Net-(D9-K)")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 0.825 0 270)
			(size 0.8 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 94 "/DigitalIO/OP1")
			(pinfunction "A")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "C:\\Users\\ESpurbeck\\Documents\\KiCad\\3rdparty\\SamacSys_Parts.3dshapes\\APTD1608ZGCK.stp"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 90 -180 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "F.Cu")
		(at 166.025 114.725 180)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C18"
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "4.7uF"
			(at 0 1.68 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/Power Supply/")
		(sheetfile "Power Supply.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0 180)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 19 "+12VA")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0 180)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 17 "GNDA")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_1210_3225Metric"
		(layer "F.Cu")
		(at 197.82 120.96)
		(descr "Resistor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R83"
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "4.7k"
			(at 0 2.28 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/DigitalIO/")
		(sheetfile "DigitalIO.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.4625 0)
			(size 1.125 2.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.222222)
			(net 94 "/DigitalIO/OP1")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.4625 0)
			(size 1.125 2.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.222222)
			(net 93 "Net-(HY1-ANODE_4)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1210_3225Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 179.975 67.1 180)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R62"
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "2.2k"
			(at 0 1.43 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/0-10VOutput/")
		(sheetfile "0-10VOutput.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 180)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 157 "/PWM_VOUT3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0 180)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 52 "Net-(C52-Pad1)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "SamacSys_Parts:APTD1608ZGCK"
		(layer "F.Cu")
		(at 165.46 130.8675 180)
		(descr "APTD1608ZGCK-1")
		(tags "LED")
		(property "Reference" "D16"
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "LED_Small"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Light emitting diode, small symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pin" "1=K 2=A"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "LED* LED_SMD:* LED_THT:*")
		(sheetname "/DigitalIO/")
		(sheetfile "DigitalIO.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -0.825 0 270)
			(size 0.8 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 17 "GNDA")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 0.825 0 270)
			(size 0.8 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 89 "Net-(D16-A)")
			(pinfunction "A")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "C:\\Users\\ESpurbeck\\Documents\\KiCad\\3rdparty\\SamacSys_Parts.3dshapes\\APTD1608ZGCK.stp"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 90 -180 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 178 73.65 90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R10"
			(at 0 0 90)
			(layer "F.SilkS")
		)
		(property "Value" "300"
			(at 0 1.43 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Power Supply/")
		(sheetfile "Power Supply.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 90)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 117 "Net-(IC1-ADJ)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0 90)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 14 "+5.5V")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1210_3225Metric"
		(layer "F.Cu")
		(at 148.85 68.175 -90)
		(descr "Capacitor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C28"
			(at 0 0 90)
			(layer "F.SilkS")
		)
		(property "Value" "22uF"
			(at 0 2.3 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/Power Supply/")
		(sheetfile "Power Supply.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.475 0 270)
			(size 1.15 2.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.217391)
			(net 13 "+12V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.475 0 270)
			(size 1.15 2.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.217391)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1210_3225Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "F.Cu")
		(at 199.8675 96.79)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R76"
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "10"
			(at 0 1.65 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/4-20mAOutput/")
		(sheetfile "4-20mAOutput.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net 147 "Net-(IC7-OUT1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net 190 "Net-(Q10-G)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 186.735 131.4675 -90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R86"
			(at 0 0 90)
			(layer "F.SilkS")
		)
		(property "Value" "15k"
			(at 0 1.43 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/DigitalIO/")
		(sheetfile "DigitalIO.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 270)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 81 "/DigitalIO/VEX3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0 270)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 83 "Net-(D11-K)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 96.275 103.4 -90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R43"
			(at 0 0 90)
			(layer "F.SilkS")
		)
		(property "Value" "49.9"
			(at 0 1.43 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/4-20mA Inputs/")
		(sheetfile "4-20mA Inputs.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 270)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0 270)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 206 "Net-(U6B-+)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_1206_3216Metric"
		(layer "F.Cu")
		(at 82.275 130.15)
		(descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R38"
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "140"
			(at 0 1.83 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/4-20mA Inputs/")
		(sheetfile "4-20mA Inputs.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.4625 0)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.222222)
			(net 2 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.4625 0)
			(size 1.125 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.222222)
			(net 203 "Net-(RN2C-R3.2)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_1206_3216Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "SamacSys_Parts:SOIC127P600X175-8N"
		(layer "F.Cu")
		(at 194.3625 99.678 -90)
		(descr "SO 8_")
		(tags "Integrated Circuit")
		(property "Reference" "IC7"
			(at 0 0 90)
			(layer "F.SilkS")
		)
		(property "Value" "LM258DT"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/lm158.pdf"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "LM258DT, Dual Operational Amplifier 1.1MHz 5 to 28V, 8-Pin SO"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Height" "1.75"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Part Number" "511-LM258D-TR"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Price/Stock" "https://www.mouser.co.uk/ProductDetail/STMicroelectronics/LM258DT?qs=EhGjr%2F0Q%252Bo8damG9%252BR9%2FhA%3D%3D"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Name" "STMicroelectronics"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Part_Number" "LM258DT"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/4-20mAOutput/")
		(sheetfile "4-20mAOutput.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -2.712 -1.905)
			(size 0.65 1.525)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 147 "Net-(IC7-OUT1)")
			(pinfunction "OUT1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -2.712 -0.635)
			(size 0.65 1.525)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 149 "Net-(IC7-IN1-)")
			(pinfunction "IN1-")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at -2.712 0.635)
			(size 0.65 1.525)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 67 "Net-(IC7-IN1+)")
			(pinfunction "IN1+")
			(pintype "passive")
		)
		(pad "4" smd rect
			(at -2.712 1.905)
			(size 0.65 1.525)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "GND")
			(pinfunction "VCC-")
			(pintype "passive")
		)
		(pad "5" smd rect
			(at 2.712 1.905)
			(size 0.65 1.525)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 66 "Net-(IC7-IN2+)")
			(pinfunction "IN2+")
			(pintype "passive")
		)
		(pad "6" smd rect
			(at 2.712 0.635)
			(size 0.65 1.525)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 148 "Net-(IC7-IN2-)")
			(pinfunction "IN2-")
			(pintype "passive")
		)
		(pad "7" smd rect
			(at 2.712 -0.635)
			(size 0.65 1.525)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 146 "Net-(IC7-OUT2)")
			(pinfunction "OUT2")
			(pintype "passive")
		)
		(pad "8" smd rect
			(at 2.712 -1.905)
			(size 0.65 1.525)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 5 "+24V")
			(pinfunction "VCC+")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "C:\\Users\\ESpurbeck\\Documents\\KiCad\\3rdparty\\SamacSys_Parts.3dshapes\\LM258DT.stp"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 81.525 93.525 90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R16"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "22k"
			(at 0 1.43 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/0-10V INPUTS/")
		(sheetfile "0-10V INPUTS.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 90)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 150 "/0-10V INPUTS/IN10V1")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0 90)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 130 "/0-10V INPUTS/+IN_B")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "F.Cu")
		(at 145.85 70.7 -90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R15"
			(at 0 0 90)
			(layer "F.SilkS")
		)
		(property "Value" "110k"
			(at 0 1.65 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Power Supply/")
		(sheetfile "Power Supply.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 270)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net 27 "Net-(U2-FBP)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 270)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 90.575 93.075 -90)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C29"
			(at 0 0 90)
			(layer "F.SilkS")
		)
		(property "Value" "470nF"
			(at 0 1.43 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/0-10V INPUTS/")
		(sheetfile "0-10V INPUTS.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 270)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 30 "/0-10V INPUTS/AIN2")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 270)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 86.675 84.575 90)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C32"
			(at 0 0 90)
			(layer "F.SilkS")
		)
		(property "Value" "470nF"
			(at 0 1.43 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/0-10V INPUTS/")
		(sheetfile "0-10V INPUTS.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 90)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 28 "/0-10V INPUTS/AIN0")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 90)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "SamacSys_Parts:DMG4800LFG7"
		(layer "F.Cu")
		(at 205.6875 90.365 -90)
		(descr "DMG4800LFG-7")
		(tags "MOSFET (N-Channel)")
		(property "Reference" "Q9"
			(at 0 0 90)
			(layer "F.SilkS")
		)
		(property "Value" "DMG4800LFG-7"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" "https://www.diodes.com//assets/Datasheets/ds31785.pdf"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "N-Channel 30 V 7.44A (Ta) 940mW (Ta) Surface Mount U-DFN3030-8"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Height" "0.63"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Part Number" "621-DMG4800LFG-7"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Price/Stock" "https://www.mouser.co.uk/ProductDetail/Diodes-Incorporated/DMG4800LFG-7?qs=f4CYDwCO%252B%2FEVatAzjmPrMQ%3D%3D"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Name" "Diodes Incorporated"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Part_Number" "DMG4800LFG-7"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/4-20mAOutput/")
		(sheetfile "4-20mAOutput.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -0.975 1.3 270)
			(size 0.39 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 145 "Net-(IC6-IN2-)")
			(pinfunction "S_1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.325 1.3 270)
			(size 0.39 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 145 "Net-(IC6-IN2-)")
			(pinfunction "S_2")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at 0.325 1.3 270)
			(size 0.39 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 145 "Net-(IC6-IN2-)")
			(pinfunction "S_3")
			(pintype "passive")
		)
		(pad "4" smd rect
			(at 0.975 1.3 270)
			(size 0.39 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 188 "Net-(Q9-G)")
			(pinfunction "G")
			(pintype "passive")
		)
		(pad "5" smd rect
			(at 0 -0.38)
			(size 2.49 2.59)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 187 "/4-20mAOutput/OUT2")
			(pinfunction "D")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "C:\\Users\\ESpurbeck\\Documents\\KiCad\\3rdparty\\SamacSys_Parts.3dshapes\\DMG4800LFG-7.stp"
			(offset
				(xyz -74.85999949 42.70000012 0.6000000148)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 -180 0)
			)
		)
	)
	(footprint "Connector_PinSocket_2.54mm:PinSocket_1x22_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 137.75 76.5 -90)
		(descr "Through hole straight socket strip, 1x22, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
		(tags "Through hole socket strip THT 1x22 2.54mm single row")
		(property "Reference" "J4"
			(at -0.025 26.65 90)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_01x22_Socket"
			(at 0 56.11 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x22, script generated"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "/")
		(sheetfile "universal-io-board-Hat.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at -0.025 26.65 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 15 "+3.3V")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 0 2.54 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 15 "+3.3V")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole circle
			(at 0 5.08 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 162 "/RST")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole circle
			(at 0 7.62 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 165 "/PWM_VOUT4")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(pad "5" thru_hole circle
			(at 0 10.16 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 157 "/PWM_VOUT3")
			(pinfunction "Pin_5")
			(pintype "passive")
		)
		(pad "6" thru_hole circle
			(at 0 12.7 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 158 "/PWM_VOUT2")
			(pinfunction "Pin_6")
			(pintype "passive")
		)
		(pad "7" thru_hole circle
			(at 0 15.24 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 159 "/PWM_VOUT1")
			(pinfunction "Pin_7")
			(pintype "passive")
		)
		(pad "8" thru_hole circle
			(at 0 17.78 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 155 "/PWM_IOUT5")
			(pinfunction "Pin_8")
			(pintype "passive")
		)
		(pad "9" thru_hole circle
			(at 0 20.32 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 156 "/PWM_IOUT6")
			(pinfunction "Pin_9")
			(pintype "passive")
		)
		(pad "10" thru_hole circle
			(at 0 22.86 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 167 "/PWM_IOUT7")
			(pinfunction "Pin_10")
			(pintype "passive")
		)
		(pad "11" thru_hole circle
			(at 0 25.4 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 164 "/PWM_IOUT8")
			(pinfunction "Pin_11")
			(pintype "passive")
		)
		(pad "12" thru_hole circle
			(at 0 27.94 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 64 "/O_CHECK3")
			(pinfunction "Pin_12")
			(pintype "passive")
		)
		(pad "13" thru_hole circle
			(at 0 30.48 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 62 "/O_CHECK4")
			(pinfunction "Pin_13")
			(pintype "passive")
		)
		(pad "14" thru_hole circle
			(at 0 33.02 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 166 "/RS485_DE")
			(pinfunction "Pin_14")
			(pintype "passive")
		)
		(pad "15" thru_hole circle
			(at 0 35.56 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 104 "/OD2")
			(pinfunction "Pin_15")
			(pintype "passive")
		)
		(pad "16" thru_hole circle
			(at 0 38.1 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 115 "/OD1")
			(pinfunction "Pin_16")
			(pintype "passive")
		)
		(pad "17" thru_hole circle
			(at 0 40.64 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 154 "/SCL")
			(pinfunction "Pin_17")
			(pintype "passive")
		)
		(pad "18" thru_hole circle
			(at 0 43.18 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 160 "/SDA")
			(pinfunction "Pin_18")
			(pintype "passive")
		)
		(pad "19" thru_hole circle
			(at 0 45.72 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 161 "/A2INT_I")
			(pinfunction "Pin_19")
			(pintype "passive")
		)
		(pad "20" thru_hole circle
			(at 0 48.26 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 163 "/A2INT_V")
			(pinfunction "Pin_20")
			(pintype "passive")
		)
		(pad "21" thru_hole circle
			(at 0 50.8 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 9 "+5V")
			(pinfunction "Pin_21")
			(pintype "passive")
		)
		(pad "22" thru_hole circle
			(at 0 53.34 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "Pin_22")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x22_P2.54mm_Vertical.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 200.8675 84.59 90)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C71"
			(at 0 0 90)
			(layer "F.SilkS")
		)
		(property "Value" "100nF"
			(at 0 1.43 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/4-20mAOutput/")
		(sheetfile "4-20mAOutput.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 90)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 5 "+24V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 90)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "SamacSys_Parts:SOIC127P600X175-8N"
		(layer "F.Cu")
		(at 164.3 60.3)
		(descr "SO 8_")
		(tags "Integrated Circuit")
		(property "Reference" "IC4"
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "LM258DT"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/lm158.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "LM258DT, Dual Operational Amplifier 1.1MHz 5 to 28V, 8-Pin SO"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Height" "1.75"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Part Number" "511-LM258D-TR"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Price/Stock" "https://www.mouser.co.uk/ProductDetail/STMicroelectronics/LM258DT?qs=EhGjr%2F0Q%252Bo8damG9%252BR9%2FhA%3D%3D"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Name" "STMicroelectronics"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Part_Number" "LM258DT"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/0-10VOutput/")
		(sheetfile "0-10VOutput.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -2.712 -1.905 90)
			(size 0.65 1.525)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 136 "/0-10VOutput/10V OUT1")
			(pinfunction "OUT1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -2.712 -0.635 90)
			(size 0.65 1.525)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 135 "Net-(IC4-IN1-)")
			(pinfunction "IN1-")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at -2.712 0.635 90)
			(size 0.65 1.525)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 49 "Net-(IC4-IN1+)")
			(pinfunction "IN1+")
			(pintype "passive")
		)
		(pad "4" smd rect
			(at -2.712 1.905 90)
			(size 0.65 1.525)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 24 "-12V")
			(pinfunction "VCC-")
			(pintype "passive")
		)
		(pad "5" smd rect
			(at 2.712 1.905 90)
			(size 0.65 1.525)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 51 "Net-(IC4-IN2+)")
			(pinfunction "IN2+")
			(pintype "passive")
		)
		(pad "6" smd rect
			(at 2.712 0.635 90)
			(size 0.65 1.525)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 134 "Net-(IC4-IN2-)")
			(pinfunction "IN2-")
			(pintype "passive")
		)
		(pad "7" smd rect
			(at 2.712 -0.635 90)
			(size 0.65 1.525)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 137 "/0-10VOutput/10V OUT2")
			(pinfunction "OUT2")
			(pintype "passive")
		)
		(pad "8" smd rect
			(at 2.712 -1.905 90)
			(size 0.65 1.525)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 13 "+12V")
			(pinfunction "VCC+")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "C:\\Users\\ESpurbeck\\Documents\\KiCad\\3rdparty\\SamacSys_Parts.3dshapes\\LM258DT.stp"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 76.725 82.825)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R22"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "22k"
			(at 0 1.43 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/0-10V INPUTS/")
		(sheetfile "0-10V INPUTS.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 152 "/0-10V INPUTS/IN10V3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 128 "/0-10V INPUTS/+IN_D")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_DFN_QFN:VQFN-24-1EP_4x4mm_P0.5mm_EP2.45x2.45mm_ThermalVias"
		(layer "F.Cu")
		(at 138.1825 67.285 -90)
		(descr "VQFN, 24 Pin (http://www.ti.com/lit/ds/symlink/msp430f1101a.pdf), generated with kicad-footprint-generator ipc_noLead_generator.py")
		(tags "VQFN NoLead")
		(property "Reference" "U2"
			(at -0.1875 0 90)
			(layer "F.SilkS")
		)
		(property "Value" "TPS65131RGE"
			(at 0 3.33 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tps65130.pdf"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Split-Rail Converter with Dual, Positive and Negative Outputs (750mA typ, Switch Current Limit 1950mA typ),), 2.7-5.5V, VQFN-24"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "VQFN*1EP*4x4mm*P0.5mm*")
		(sheetname "/Power Supply/")
		(sheetfile "Power Supply.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at -0.1875 0 90)
			(layer "F.Fab")
		)
		(pad "" smd roundrect
			(at -0.82 -0.82 270)
			(size 0.61 0.61)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at -0.82 0 270)
			(size 0.61 0.61)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at -0.82 0.82 270)
			(size 0.61 0.61)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0 -0.82 270)
			(size 0.61 0.61)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0 0 270)
			(size 0.61 0.61)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0 0.82 270)
			(size 0.61 0.61)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0.82 -0.82 270)
			(size 0.61 0.61)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0.82 0 270)
			(size 0.61 0.61)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0.82 0.82 270)
			(size 0.61 0.61)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "1" smd roundrect
			(at -1.9875 -1.25 270)
			(size 0.775 0.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 68 "Net-(D3-A)")
			(pinfunction "INP")
			(pintype "input")
		)
		(pad "2" smd roundrect
			(at -1.9875 -0.75 270)
			(size 0.775 0.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "PGND")
			(pintype "power_in")
		)
		(pad "3" smd roundrect
			(at -1.9875 -0.25 270)
			(size 0.775 0.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "PGND")
			(pintype "passive")
		)
		(pad "4" smd roundrect
			(at -1.9875 0.25 270)
			(size 0.775 0.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 20 "Net-(U2-ENN)")
			(pinfunction "VIN")
			(pintype "power_in")
		)
		(pad "5" smd roundrect
			(at -1.9875 0.75 270)
			(size 0.775 0.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 9 "+5V")
			(pinfunction "INN")
			(pintype "input")
		)
		(pad "6" smd roundrect
			(at -1.9875 1.25 270)
			(size 0.775 0.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 9 "+5V")
			(pinfunction "INN")
			(pintype "input")
		)
		(pad "7" smd roundrect
			(at -1.25 1.9875 270)
			(size 0.25 0.775)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 181 "Net-(Q3-G)")
			(pinfunction "BSW")
			(pintype "output")
		)
		(pad "8" smd roundrect
			(at -0.75 1.9875 270)
			(size 0.25 0.775)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 20 "Net-(U2-ENN)")
			(pinfunction "ENP")
			(pintype "input")
		)
		(pad "9" smd roundrect
			(at -0.25 1.9875 270)
			(size 0.25 0.775)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 20 "Net-(U2-ENN)")
			(pinfunction "PSP")
			(pintype "input")
		)
		(pad "10" smd roundrect
			(at 0.25 1.9875 270)
			(size 0.25 0.775)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 20 "Net-(U2-ENN)")
			(pinfunction "ENN")
			(pintype "input")
		)
		(pad "11" smd roundrect
			(at 0.75 1.9875 270)
			(size 0.25 0.775)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 20 "Net-(U2-ENN)")
			(pinfunction "PSN")
			(pintype "input")
		)
		(pad "12" smd roundrect
			(at 1.25 1.9875 270)
			(size 0.25 0.775)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 217 "unconnected-(U2-NC-Pad12)")
			(pinfunction "NC")
			(pintype "no_connect")
		)
		(pad "13" smd roundrect
			(at 1.9875 1.25 270)
			(size 0.775 0.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 69 "Net-(D4-K)")
			(pinfunction "OUTN")
			(pintype "output")
		)
		(pad "14" smd roundrect
			(at 1.9875 0.75 270)
			(size 0.775 0.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 69 "Net-(D4-K)")
			(pinfunction "OUTN")
			(pintype "passive")
		)
		(pad "15" smd roundrect
			(at 1.9875 0.25 270)
			(size 0.775 0.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 26 "Net-(U2-VNEG)")
			(pinfunction "VNEG")
			(pintype "input")
		)
		(pad "16" smd roundrect
			(at 1.9875 -0.25 270)
			(size 0.775 0.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 196 "Net-(U2-FBN)")
			(pinfunction "FBN")
			(pintype "input")
		)
		(pad "17" smd roundrect
			(at 1.9875 -0.75 270)
			(size 0.775 0.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 25 "Net-(U2-VREF)")
			(pinfunction "VREF")
			(pintype "output")
		)
		(pad "18" smd roundrect
			(at 1.9875 -1.25 270)
			(size 0.775 0.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 23 "Net-(U2-CN)")
			(pinfunction "CN")
			(pintype "passive")
		)
		(pad "19" smd roundrect
			(at 1.25 -1.9875 270)
			(size 0.25 0.775)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "AGND")
			(pintype "power_in")
		)
		(pad "20" smd roundrect
			(at 0.75 -1.9875 270)
			(size 0.25 0.775)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 216 "unconnected-(U2-NC-Pad20)")
			(pinfunction "NC")
			(pintype "no_connect")
		)
		(pad "21" smd roundrect
			(at 0.25 -1.9875 270)
			(size 0.25 0.775)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 22 "Net-(U2-CP)")
			(pinfunction "CP")
			(pintype "passive")
		)
		(pad "22" smd roundrect
			(at -0.25 -1.9875 270)
			(size 0.25 0.775)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 27 "Net-(U2-FBP)")
			(pinfunction "FBP")
			(pintype "input")
		)
		(pad "23" smd roundrect
			(at -0.75 -1.9875 270)
			(size 0.25 0.775)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 13 "+12V")
			(pinfunction "VPOS")
			(pintype "input")
		)
		(pad "24" smd roundrect
			(at -1.25 -1.9875 270)
			(size 0.25 0.775)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 68 "Net-(D3-A)")
			(pinfunction "INP")
			(pintype "input")
		)
		(pad "25" thru_hole circle
			(at -0.975 -0.975 270)
			(size 0.5 0.5)
			(drill 0.2)
			(property pad_prop_heatsink)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "EP")
			(pintype "passive")
		)
		(pad "25" thru_hole circle
			(at -0.975 0 270)
			(size 0.5 0.5)
			(drill 0.2)
			(property pad_prop_heatsink)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "EP")
			(pintype "passive")
		)
		(pad "25" thru_hole circle
			(at -0.975 0.975 270)
			(size 0.5 0.5)
			(drill 0.2)
			(property pad_prop_heatsink)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "EP")
			(pintype "passive")
		)
		(pad "25" thru_hole circle
			(at 0 -0.975 270)
			(size 0.5 0.5)
			(drill 0.2)
			(property pad_prop_heatsink)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "EP")
			(pintype "passive")
		)
		(pad "25" thru_hole circle
			(at 0 0 270)
			(size 0.5 0.5)
			(drill 0.2)
			(property pad_prop_heatsink)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "EP")
			(pintype "passive")
		)
		(pad "25" smd rect
			(at 0 0 270)
			(size 2.45 2.45)
			(property pad_prop_heatsink)
			(layers "F.Cu" "F.Mask")
			(net 2 "GND")
			(pinfunction "EP")
			(pintype "passive")
			(zone_connect 2)
		)
		(pad "25" smd rect
			(at 0 0 270)
			(size 2.45 2.45)
			(property pad_prop_heatsink)
			(layers "B.Cu")
			(net 2 "GND")
			(pinfunction "EP")
			(pintype "passive")
			(zone_connect 2)
		)
		(pad "25" thru_hole circle
			(at 0 0.975 270)
			(size 0.5 0.5)
			(drill 0.2)
			(property pad_prop_heatsink)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "EP")
			(pintype "passive")
		)
		(pad "25" thru_hole circle
			(at 0.975 -0.975 270)
			(size 0.5 0.5)
			(drill 0.2)
			(property pad_prop_heatsink)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "EP")
			(pintype "passive")
		)
		(pad "25" thru_hole circle
			(at 0.975 0 270)
			(size 0.5 0.5)
			(drill 0.2)
			(property pad_prop_heatsink)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "EP")
			(pintype "passive")
		)
		(pad "25" thru_hole circle
			(at 0.975 0.975 270)
			(size 0.5 0.5)
			(drill 0.2)
			(property pad_prop_heatsink)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "EP")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Package_DFN_QFN.3dshapes/VQFN-24-1EP_4x4mm_P0.5mm_EP2.45x2.45mm.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "SamacSys_Parts:DMG4800LFG7"
		(layer "F.Cu")
		(at 205.6875 81.565 -90)
		(descr "DMG4800LFG-7")
		(tags "MOSFET (N-Channel)")
		(property "Reference" "Q8"
			(at 0 0 90)
			(layer "F.SilkS")
		)
		(property "Value" "DMG4800LFG-7"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" "https://www.diodes.com//assets/Datasheets/ds31785.pdf"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "N-Channel 30 V 7.44A (Ta) 940mW (Ta) Surface Mount U-DFN3030-8"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Height" "0.63"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Part Number" "621-DMG4800LFG-7"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Price/Stock" "https://www.mouser.co.uk/ProductDetail/Diodes-Incorporated/DMG4800LFG-7?qs=f4CYDwCO%252B%2FEVatAzjmPrMQ%3D%3D"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Name" "Diodes Incorporated"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Part_Number" "DMG4800LFG-7"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/4-20mAOutput/")
		(sheetfile "4-20mAOutput.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -0.975 1.3 270)
			(size 0.39 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 143 "Net-(IC6-IN1-)")
			(pinfunction "S_1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.325 1.3 270)
			(size 0.39 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 143 "Net-(IC6-IN1-)")
			(pinfunction "S_2")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at 0.325 1.3 270)
			(size 0.39 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 143 "Net-(IC6-IN1-)")
			(pinfunction "S_3")
			(pintype "passive")
		)
		(pad "4" smd rect
			(at 0.975 1.3 270)
			(size 0.39 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 186 "Net-(Q8-G)")
			(pinfunction "G")
			(pintype "passive")
		)
		(pad "5" smd rect
			(at 0 -0.38)
			(size 2.49 2.59)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 179 "/4-20mAOutput/OUT1")
			(pinfunction "D")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "C:\\Users\\ESpurbeck\\Documents\\KiCad\\3rdparty\\SamacSys_Parts.3dshapes\\DMG4800LFG-7.stp"
			(offset
				(xyz -74.85999949 42.70000012 0.6000000148)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 -180 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 180 64.9)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R64"
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "2.2k"
			(at 0 1.43 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/0-10VOutput/")
		(sheetfile "0-10VOutput.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 52 "Net-(C52-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 54 "Net-(IC5-IN1+)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 157.875 60.175 180)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R54"
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "4.53k"
			(at 0 1.43 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/0-10VOutput/")
		(sheetfile "0-10VOutput.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 180)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 15 "+3.3V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0 180)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 135 "Net-(IC4-IN1-)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "B.Cu")
		(at 154.05 90.35 90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C13"
			(at 0 0 90)
			(layer "B.SilkS")
		)
		(property "Value" "1uF"
			(at 0 -1.68 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/Power Supply/")
		(sheetfile "Power Supply.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0 90)
			(size 1 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 15 "+3.3V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0 90)
			(size 1 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_SO:ONSemi_SO-8FL_488AA"
		(layer "B.Cu")
		(at 92.875 54.1 90)
		(descr "ON Semi DFN5 5x6mm 1.27P SO-8FL CASE 488A https://www.onsemi.com/pub/Collateral/488AA.PDF")
		(tags "ON Semi DFN5 5x6mm 1.27P SO-8FL CASE 488A ")
		(property "Reference" "Q1"
			(at 0 4 90)
			(layer "B.SilkS")
		)
		(property "Value" "NTMFS5C670NLT1G"
			(at 0.05 -4.475 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/NTMFS5C670NL-D.PDF"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Low RDS(on); Low input capacitance; RoHS Compliant"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Height" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Mouser Part Number" "863-NTMFS5C670NLT1G"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Mouser Price/Stock" "https://www.mouser.co.uk/ProductDetail/onsemi/NTMFS5C670NLT1G?qs=85c0ukccmxF7%2F53ox6Y1og%3D%3D"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer_Name" "onsemi"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer_Part_Number" "NTMFS5C670NLT1G"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(sheetname "/Power Supply/")
		(sheetfile "Power Supply.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0.04775 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -2.74725 1.905 90)
			(size 1 0.75)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 7 "Net-(IC2-SW)")
			(pinfunction "S_1")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at -2.74725 0.635 90)
			(size 1 0.75)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 7 "Net-(IC2-SW)")
			(pinfunction "S_2")
			(pintype "passive")
		)
		(pad "3" smd roundrect
			(at -2.74725 -0.635 90)
			(size 1 0.75)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 7 "Net-(IC2-SW)")
			(pinfunction "S_3")
			(pintype "passive")
		)
		(pad "4" smd roundrect
			(at -2.74725 -1.905 90)
			(size 1 0.75)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 124 "Net-(IC2-HO)")
			(pinfunction "G")
			(pintype "passive")
		)
		(pad "5" smd custom
			(at 0.745 0 90)
			(size 4.055 4.56)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 1 "Net-(D1-K)")
			(pinfunction "D")
			(pintype "passive")
			(zone_connect 0)
			(thermal_bridge_angle 45)
			(options
				(clearance outline)
				(anchor rect)
			)
			(primitives
				(gr_poly
					(pts
						(xy -0.6975 2.28) (xy 2.5025 2.28) (xy 2.5025 1.53) (xy 1.905 1.53) (xy 1.905 -1.53) (xy 2.5025 -1.53)
						(xy 2.5025 -2.28) (xy -0.6975 -2.28) (xy -0.6975 -2.775) (xy -1.6025 -2.775) (xy -1.6025 2.775)
						(xy -0.6975 2.775)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Package_SO.3dshapes/ONSemi_SO-8FL_488AA.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_Cat16-4"
		(layer "B.Cu")
		(at 153.8 114.98 -90)
		(descr "SMT resistor net, Bourns CAT16 series, 4 way")
		(tags "SMT resistor net Bourns CAT16 series 4 way")
		(property "Reference" "RN13"
			(at 0 0 90)
			(layer "B.SilkS")
		)
		(property "Value" "4.7k"
			(at 0 -2.55 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "4 resistor network, parallel topology, split"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "DIP* SOIC* R*Array*Concave* R*Array*Convex* MSOP*")
		(sheetname "/DigitalIO/")
		(sheetfile "DigitalIO.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd rect
			(at -0.76 1.2 90)
			(size 0.76 0.43)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 110 "Net-(HY2-EMITTER_4)")
			(pinfunction "R1.1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.76 0.4 90)
			(size 0.76 0.43)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 87 "Net-(D14-A)")
			(pinfunction "R2.1")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at -0.76 -0.4 90)
			(size 0.76 0.43)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 88 "Net-(D15-A)")
			(pinfunction "R3.1")
			(pintype "passive")
		)
		(pad "4" smd rect
			(at -0.76 -1.2 90)
			(size 0.76 0.43)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 89 "Net-(D16-A)")
			(pinfunction "R4.1")
			(pintype "passive")
		)
		(pad "5" smd rect
			(at 0.76 -1.2 90)
			(size 0.76 0.43)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 113 "Net-(HY2-EMITTER_1)")
			(pinfunction "R4.2")
			(pintype "passive")
		)
		(pad "6" smd rect
			(at 0.76 -0.4 90)
			(size 0.76 0.43)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 108 "Net-(HY2-EMITTER_2)")
			(pinfunction "R3.2")
			(pintype "passive")
		)
		(pad "7" smd rect
			(at 0.76 0.4 90)
			(size 0.76 0.43)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 112 "Net-(HY2-EMITTER_3)")
			(pinfunction "R2.2")
			(pintype "passive")
		)
		(pad "8" smd rect
			(at 0.76 1.2 90)
			(size 0.76 0.43)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 86 "Net-(D13-A)")
			(pinfunction "R1.2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_Cat16-4.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_SMD:SOT-23-5"
		(layer "B.Cu")
		(at 153.08 94.4525 90)
		(descr "SOT, 5 Pin (JEDEC MO-178 Var AA https://www.jedec.org/document_search?search_api_views_fulltext=MO-178), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOT TO_SOT_SMD")
		(property "Reference" "U1"
			(at 0 0.0875 90)
			(layer "B.SilkS")
		)
		(property "Value" "ME6211C33M5"
			(at 0 -2.4 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.lcsc.com/datasheet/lcsc_datasheet_2304140030_MICRONE-Nanjing-Micro-One-Elec-ME6211C33R5G_C235316.pdf"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "500mA low dropout linear regulator, shutdown pin, 6.5V max input voltage, 3.3V fixed positive output, SOT-23-5"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SOT?23?5*")
		(sheetname "/Power Supply/")
		(sheetfile "Power Supply.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0.0875 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.1375 0.95 90)
			(size 1.325 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 9 "+5V")
			(pinfunction "V_{IN}")
			(pintype "power_in")
		)
		(pad "2" smd roundrect
			(at -1.1375 0 90)
			(size 1.325 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "V_{SS}")
			(pintype "power_in")
		)
		(pad "3" smd roundrect
			(at -1.1375 -0.95 90)
			(size 1.325 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 9 "+5V")
			(pinfunction "CE")
			(pintype "input")
		)
		(pad "4" smd roundrect
			(at 1.1375 -0.95 90)
			(size 1.325 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 215 "unconnected-(U1-NC-Pad4)")
			(pinfunction "NC")
			(pintype "no_connect")
		)
		(pad "5" smd roundrect
			(at 1.1375 0.95 90)
			(size 1.325 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 15 "+3.3V")
			(pinfunction "V_{OUT}")
			(pintype "power_out")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "B.Cu")
		(at 141.65 66.6 90)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C22"
			(at 0 0 90)
			(layer "B.SilkS")
		)
		(property "Value" "4.7nF"
			(at 0 -1.43 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/Power Supply/")
		(sheetfile "Power Supply.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 90)
			(size 0.9 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 22 "Net-(U2-CP)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 90)
			(size 0.9 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "SamacSys_Parts:SOP65P640X110-21N"
		(layer "B.Cu")
		(at 106.075 54.375 -90)
		(descr "htssop -pwp")
		(tags "Integrated Circuit")
		(property "Reference" "IC2"
			(at 0 0.0125 90)
			(layer "B.SilkS")
		)
		(property "Value" "LM5116MHX_NOPB"
			(at 0 0 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/lm5116"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "6-100V Wide Vin, Current Mode Synchronous Buck Controller"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Height" "1.1"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Mouser Part Number" "926-LM5116MHX/NOPB"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Mouser Price/Stock" "https://www.mouser.co.uk/ProductDetail/Texas-Instruments/LM5116MHX-NOPB?qs=QbsRYf82W3EaCl%2FW15P7yA%3D%3D"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer_Name" "Texas Instruments"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer_Part_Number" "LM5116MHX/NOPB"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(sheetname "/Power Supply/")
		(sheetfile "Power Supply.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0.0125 90)
			(layer "B.Fab")
		)
		(pad "1" smd rect
			(at -2.925 2.925 180)
			(size 0.45 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 1 "Net-(D1-K)")
			(pinfunction "VIN")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -2.925 2.275 180)
			(size 0.45 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 125 "Net-(IC2-UVLO)")
			(pinfunction "UVLO")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at -2.925 1.625 180)
			(size 0.45 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 119 "Net-(IC2-RT{slash}SYNC)")
			(pinfunction "RT/SYNC")
			(pintype "passive")
		)
		(pad "4" smd rect
			(at -2.925 0.975 180)
			(size 0.45 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 121 "Net-(IC2-EN)")
			(pinfunction "EN")
			(pintype "passive")
		)
		(pad "5" smd rect
			(at -2.925 0.325 180)
			(size 0.45 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 3 "Net-(IC2-RAMP)")
			(pinfunction "RAMP")
			(pintype "passive")
		)
		(pad "6" smd rect
			(at -2.925 -0.325 180)
			(size 0.45 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 2 "GND")
			(pinfunction "AGND")
			(pintype "passive")
		)
		(pad "7" smd rect
			(at -2.925 -0.975 180)
			(size 0.45 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 4 "Net-(IC2-SS)")
			(pinfunction "SS")
			(pintype "passive")
		)
		(pad "8" smd rect
			(at -2.925 -1.625 180)
			(size 0.45 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 10 "Net-(IC2-FB)")
			(pinfunction "FB")
			(pintype "passive")
		)
		(pad "9" smd rect
			(at -2.925 -2.275 180)
			(size 0.45 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 11 "Net-(IC2-COMP)")
			(pinfunction "COMP")
			(pintype "passive")
		)
		(pad "10" smd rect
			(at -2.925 -2.925 180)
			(size 0.45 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 9 "+5V")
			(pinfunction "VOUT")
			(pintype "passive")
		)
		(pad "11" smd rect
			(at 2.925 -2.925 180)
			(size 0.45 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 120 "Net-(IC2-CSG)")
			(pinfunction "DEMB")
			(pintype "passive")
		)
		(pad "12" smd rect
			(at 2.925 -2.275 180)
			(size 0.45 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 123 "Net-(IC2-CS)")
			(pinfunction "CS")
			(pintype "passive")
		)
		(pad "13" smd rect
			(at 2.925 -1.625 180)
			(size 0.45 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 120 "Net-(IC2-CSG)")
			(pinfunction "CSG")
			(pintype "passive")
		)
		(pad "14" smd rect
			(at 2.925 -0.975 180)
			(size 0.45 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 2 "GND")
			(pinfunction "PGND")
			(pintype "passive")
		)
		(pad "15" smd rect
			(at 2.925 -0.325 180)
			(size 0.45 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 122 "Net-(IC2-LO)")
			(pinfunction "LO")
			(pintype "passive")
		)
		(pad "16" smd rect
			(at 2.925 0.325 180)
			(size 0.45 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 8 "/Power Supply/VCC")
			(pinfunction "VCC")
			(pintype "passive")
		)
		(pad "17" smd rect
			(at 2.925 0.975 180)
			(size 0.45 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 2 "GND")
			(pinfunction "VCCX")
			(pintype "passive")
		)
		(pad "18" smd rect
			(at 2.925 1.625 180)
			(size 0.45 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 6 "Net-(D2-K)")
			(pinfunction "HB")
			(pintype "passive")
		)
		(pad "19" smd rect
			(at 2.925 2.275 180)
			(size 0.45 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 124 "Net-(IC2-HO)")
			(pinfunction "HO")
			(pintype "passive")
		)
		(pad "20" smd rect
			(at 2.925 2.925 180)
			(size 0.45 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 7 "Net-(IC2-SW)")
			(pinfunction "SW")
			(pintype "passive")
		)
		(pad "21" smd rect
			(at 0 0 270)
			(size 3.15 4.35)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 2 "GND")
			(pinfunction "EP")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "C:\\Users\\ESpurbeck\\Documents\\KiCad\\3rdparty\\SamacSys_Parts.3dshapes\\LM5116MHX_NOPB.stp"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_Cat16-4"
		(layer "B.Cu")
		(at 191.3075 80.19 180)
		(descr "SMT resistor net, Bourns CAT16 series, 4 way")
		(tags "SMT resistor net Bourns CAT16 series 4 way")
		(property "Reference" "RN5"
			(at 0 0 0)
			(layer "B.SilkS")
		)
		(property "Value" "2.2k"
			(at 0 -2.55 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "4 resistor network, parallel topology, split"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "DIP* SOIC* R*Array*Concave* R*Array*Convex* MSOP*")
		(sheetname "/4-20mAOutput/")
		(sheetfile "4-20mAOutput.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd rect
			(at -0.76 1.2)
			(size 0.76 0.43)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 56 "Net-(RN5A-R1.1)")
			(pinfunction "R1.1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.76 0.4)
			(size 0.76 0.43)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 57 "Net-(IC6-IN1+)")
			(pinfunction "R2.1")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at -0.76 -0.4)
			(size 0.76 0.43)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 58 "Net-(RN5C-R3.1)")
			(pinfunction "R3.1")
			(pintype "passive")
		)
		(pad "4" smd rect
			(at -0.76 -1.2)
			(size 0.76 0.43)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 59 "Net-(IC6-IN2+)")
			(pinfunction "R4.1")
			(pintype "passive")
		)
		(pad "5" smd rect
			(at 0.76 -1.2)
			(size 0.76 0.43)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 58 "Net-(RN5C-R3.1)")
			(pinfunction "R4.2")
			(pintype "passive")
		)
		(pad "6" smd rect
			(at 0.76 -0.4)
			(size 0.76 0.43)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 156 "/PWM_IOUT6")
			(pinfunction "R3.2")
			(pintype "passive")
		)
		(pad "7" smd rect
			(at 0.76 0.4)
			(size 0.76 0.43)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 56 "Net-(RN5A-R1.1)")
			(pinfunction "R2.2")
			(pintype "passive")
		)
		(pad "8" smd rect
			(at 0.76 1.2)
			(size 0.76 0.43)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 155 "/PWM_IOUT5")
			(pinfunction "R1.2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_Cat16-4.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_Phoenix_MC:PhoenixContact_MC_1,5_8-G-3.81_1x08_P3.81mm_Horizontal"
		(layer "B.Cu")
		(at 167.08 126.4675 180)
		(descr "Generic Phoenix Contact connector footprint for: MC_1,5/8-G-3.81; number of pins: 08; pin pitch: 3.81mm; Angled || order number: 1803332 8A 160V")
		(tags "phoenix_contact connector MC_01x08_G_3.81mm")
		(property "Reference" "J9"
			(at 13.28 -2.9325 0)
			(layer "B.SilkS")
		)
		(property "Value" "Conn_01x08_Socket"
			(at 13.33 -9.2 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x08, script generated"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "/DigitalIO/")
		(sheetfile "DigitalIO.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 13.28 -2.9325 0)
			(layer "B.Fab")
		)
		(pad "1" thru_hole roundrect
			(at 0 0 180)
			(size 1.8 3.6)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.138889)
			(net 180 "/DigitalIO/OD_OUT1")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 3.81 0 180)
			(size 1.8 3.6)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 17 "GNDA")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 7.62 0 180)
			(size 1.8 3.6)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 193 "/DigitalIO/OD_OUT2")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole oval
			(at 11.43 0 180)
			(size 1.8 3.6)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 17 "GNDA")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(pad "5" thru_hole oval
			(at 15.24 0 180)
			(size 1.8 3.6)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 194 "/DigitalIO/OD_OUT3")
			(pinfunction "Pin_5")
			(pintype "passive")
		)
		(pad "6" thru_hole oval
			(at 19.05 0 180)
			(size 1.8 3.6)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 17 "GNDA")
			(pinfunction "Pin_6")
			(pintype "passive")
		)
		(pad "7" thru_hole oval
			(at 22.86 0 180)
			(size 1.8 3.6)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 195 "/DigitalIO/OD_OUT4")
			(pinfunction "Pin_7")
			(pintype "passive")
		)
		(pad "8" thru_hole oval
			(at 26.67 0 180)
			(size 1.8 3.6)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 17 "GNDA")
			(pinfunction "Pin_8")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_Phoenix_MC.3dshapes/PhoenixContact_MC_1,5_8-G-3.81_1x08_P3.81mm_Horizontal.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "SamacSys_Parts:DIOM5436X244N"
		(layer "B.Cu")
		(at 94.3 47.825 180)
		(descr "SMB (DO-214AA)_2024")
		(tags "TVS Diode (Uni-directional)")
		(property "Reference" "D1"
			(at 0 0 0)
			(layer "B.SilkS")
		)
		(property "Value" "SMBJ30A"
			(at 0 0 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Datasheet" "https://bourns.com/docs/product-datasheets/smbj.pdf?sfvrsn=34552159_18"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "ESD Suppressors / TVS Diodes 30volts 5uA 12.4 Amps Uni-Dir"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Height" "2.44"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Mouser Part Number" "652-SMBJ30A"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Mouser Price/Stock" "https://www.mouser.co.uk/ProductDetail/Bourns/SMBJ30A?qs=%252Bf8Cd6aE5by%252B8DX3Y6MgHw%3D%3D"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer_Name" "Bourns"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer_Part_Number" "SMBJ30A"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(sheetname "/Power Supply/")
		(sheetfile "Power Supply.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd rect
			(at -2.2 0 90)
			(size 2.15 2.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 1 "Net-(D1-K)")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 2.2 0 90)
			(size 2.15 2.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 2 "GND")
			(pinfunction "A")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "C:\\Users\\ESpurbeck\\Documents\\KiCad\\3rdparty\\SamacSys_Parts.3dshapes\\SMBJ30A.stp"
			(offset
				(xyz 0 0 1.309999923)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "B.Cu")
		(at 156.28 96.5025 -90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C14"
			(at 0 0 90)
			(layer "B.SilkS")
		)
		(property "Value" "1uF"
			(at 0 -1.68 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/Power Supply/")
		(sheetfile "Power Supply.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0 270)
			(size 1 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 9 "+5V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0 270)
			(size 1 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_SMD:SOT-23"
		(layer "B.Cu")
		(at 96.9873 110.9225)
		(descr "SOT, 3 Pin (JEDEC TO-236 Var AB https://www.jedec.org/document_search?search_api_views_fulltext=TO-236), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOT TO_SOT_SMD")
		(property "Reference" "Q7"
			(at 0 0 0)
			(layer "B.SilkS")
		)
		(property "Value" "MMBT3904"
			(at 0 -2.4 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.onsemi.com/pdf/datasheet/pzt3904-d.pdf"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "0.2A Ic, 40V Vce, Small Signal NPN Transistor, SOT-23"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SOT?23*")
		(sheetname "/4-20mA Inputs/")
		(sheetfile "4-20mA Inputs.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9375 0.95)
			(size 1.475 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 37 "Net-(Q7-B)")
			(pinfunction "B")
			(pintype "input")
		)
		(pad "2" smd roundrect
			(at -0.9375 -0.95)
			(size 1.475 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 185 "Net-(Q7-E)")
			(pinfunction "E")
			(pintype "passive")
		)
		(pad "3" smd roundrect
			(at 0.9375 0)
			(size 1.475 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 9 "+5V")
			(pinfunction "C")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_Cat16-4"
		(layer "B.Cu")
		(at 146.4 114.98 90)
		(descr "SMT resistor net, Bourns CAT16 series, 4 way")
		(tags "SMT resistor net Bourns CAT16 series 4 way")
		(property "Reference" "RN14"
			(at 0 0 90)
			(layer "B.SilkS")
		)
		(property "Value" "4.7k"
			(at 0 -2.55 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "4 resistor network, parallel topology, split"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "DIP* SOIC* R*Array*Concave* R*Array*Convex* MSOP*")
		(sheetname "/DigitalIO/")
		(sheetfile "DigitalIO.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd rect
			(at -0.76 1.2 270)
			(size 0.76 0.43)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 17 "GNDA")
			(pinfunction "R1.1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.76 0.4 270)
			(size 0.76 0.43)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 17 "GNDA")
			(pinfunction "R2.1")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at -0.76 -0.4 270)
			(size 0.76 0.43)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 17 "GNDA")
			(pinfunction "R3.1")
			(pintype "passive")
		)
		(pad "4" smd rect
			(at -0.76 -1.2 270)
			(size 0.76 0.43)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 17 "GNDA")
			(pinfunction "R4.1")
			(pintype "passive")
		)
		(pad "5" smd rect
			(at 0.76 -1.2 270)
			(size 0.76 0.43)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 113 "Net-(HY2-EMITTER_1)")
			(pinfunction "R4.2")
			(pintype "passive")
		)
		(pad "6" smd rect
			(at 0.76 -0.4 270)
			(size 0.76 0.43)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 108 "Net-(HY2-EMITTER_2)")
			(pinfunction "R3.2")
			(pintype "passive")
		)
		(pad "7" smd rect
			(at 0.76 0.4 270)
			(size 0.76 0.43)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 112 "Net-(HY2-EMITTER_3)")
			(pinfunction "R2.2")
			(pintype "passive")
		)
		(pad "8" smd rect
			(at 0.76 1.2 270)
			(size 0.76 0.43)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 110 "Net-(HY2-EMITTER_4)")
			(pinfunction "R1.2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_Cat16-4.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "B.Cu")
		(at 89.95 103.175 90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C42"
			(at 0 0 90)
			(layer "B.SilkS")
		)
		(property "Value" "1uF"
			(at 0 -1.68 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/4-20mA Inputs/")
		(sheetfile "4-20mA Inputs.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0 90)
			(size 1 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 43 "/4-20mA Inputs/AIN1")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0 90)
			(size 1 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "B.Cu")
		(at 125.825 120.025 90)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C73"
			(at 0 0 90)
			(layer "B.SilkS")
		)
		(property "Value" "220nF"
			(at 0 -1.43 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/Communication/")
		(sheetfile "Communication.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 90)
			(size 0.9 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 15 "+3.3V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 90)
			(size 0.9 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_Phoenix_MC:PhoenixContact_MC_1,5_3-G-3.81_1x03_P3.81mm_Horizontal"
		(layer "B.Cu")
		(at 132.355 126.8675 180)
		(descr "Generic Phoenix Contact connector footprint for: MC_1,5/3-G-3.81; number of pins: 03; pin pitch: 3.81mm; Angled || order number: 1803280 8A 160V")
		(tags "phoenix_contact connector MC_01x03_G_3.81mm")
		(property "Reference" "J10"
			(at 3.755 -2.9325 0)
			(layer "B.SilkS")
		)
		(property "Value" "Conn_01x03_Socket"
			(at 3.81 -9.2 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x03, script generated"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "/Communication/")
		(sheetfile "Communication.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 3.755 -2.9325 0)
			(layer "B.Fab")
		)
		(pad "1" thru_hole roundrect
			(at 0 0 180)
			(size 1.8 3.6)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.138889)
			(net 91 "/Communication/RS485A")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 3.81 0 180)
			(size 1.8 3.6)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 90 "/Communication/RS485B")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 7.62 0 180)
			(size 1.8 3.6)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_Phoenix_MC.3dshapes/PhoenixContact_MC_1,5_3-G-3.81_1x03_P3.81mm_Horizontal.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "B.Cu")
		(at 110.9 49.525)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R7"
			(at 0 0 0)
			(layer "B.SilkS")
		)
		(property "Value" "78.7k"
			(at 0 -1.43 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Power Supply/")
		(sheetfile "Power Supply.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 11 "Net-(IC2-COMP)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 12 "Net-(C10-Pad2)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_Cat16-4"
		(layer "B.Cu")
		(at 89.965 128.3 180)
		(descr "SMT resistor net, Bourns CAT16 series, 4 way")
		(tags "SMT resistor net Bourns CAT16 series 4 way")
		(property "Reference" "RN2"
			(at 0 0 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "2.2k"
			(at 0 -2.55 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "4 resistor network, parallel topology, split"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "DIP* SOIC* R*Array*Concave* R*Array*Convex* MSOP*")
		(sheetname "/4-20mA Inputs/")
		(sheetfile "4-20mA Inputs.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd rect
			(at -0.76 1.2)
			(size 0.76 0.43)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 34 "Net-(RN2A-R1.1)")
			(pinfunction "R1.1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.76 0.4)
			(size 0.76 0.43)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 35 "/4-20mA Inputs/AIN3")
			(pinfunction "R2.1")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at -0.76 -0.4)
			(size 0.76 0.43)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 38 "Net-(RN2C-R3.1)")
			(pinfunction "R3.1")
			(pintype "passive")
		)
		(pad "4" smd rect
			(at -0.76 -1.2)
			(size 0.76 0.43)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 39 "/4-20mA Inputs/AIN2")
			(pinfunction "R4.1")
			(pintype "passive")
		)
		(pad "5" smd rect
			(at 0.76 -1.2)
			(size 0.76 0.43)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 38 "Net-(RN2C-R3.1)")
			(pinfunction "R4.2")
			(pintype "passive")
		)
		(pad "6" smd rect
			(at 0.76 -0.4)
			(size 0.76 0.43)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 203 "Net-(RN2C-R3.2)")
			(pinfunction "R3.2")
			(pintype "passive")
		)
		(pad "7" smd rect
			(at 0.76 0.4)
			(size 0.76 0.43)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 34 "Net-(RN2A-R1.1)")
			(pinfunction "R2.2")
			(pintype "passive")
		)
		(pad "8" smd rect
			(at 0.76 1.2)
			(size 0.76 0.43)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 199 "Net-(RN2A-R1.2)")
			(pinfunction "R1.2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_Cat16-4.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "B.Cu")
		(at 87.75 103.15 90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C41"
			(at 0 0 90)
			(layer "B.SilkS")
		)
		(property "Value" "1uF"
			(at 0 -1.68 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/4-20mA Inputs/")
		(sheetfile "4-20mA Inputs.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0 90)
			(size 1 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 42 "Net-(RN3A-R1.1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0 90)
			(size 1 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_SO:ONSemi_SO-8FL_488AA"
		(layer "B.Cu")
		(at 93.02 61.5472 -90)
		(descr "ON Semi DFN5 5x6mm 1.27P SO-8FL CASE 488A https://www.onsemi.com/pub/Collateral/488AA.PDF")
		(tags "ON Semi DFN5 5x6mm 1.27P SO-8FL CASE 488A ")
		(property "Reference" "Q2"
			(at 0 4 90)
			(layer "B.SilkS")
		)
		(property "Value" "NTMFS5C670NLT1G"
			(at 0 -4 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/NTMFS5C670NL-D.PDF"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Low RDS(on); Low input capacitance; RoHS Compliant"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Height" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Mouser Part Number" "863-NTMFS5C670NLT1G"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Mouser Price/Stock" "https://www.mouser.co.uk/ProductDetail/onsemi/NTMFS5C670NLT1G?qs=85c0ukccmxF7%2F53ox6Y1og%3D%3D"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer_Name" "onsemi"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer_Part_Number" "NTMFS5C670NLT1G"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(sheetname "/Power Supply/")
		(sheetfile "Power Supply.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0.04775 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -2.74725 1.905 270)
			(size 1 0.75)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 123 "Net-(IC2-CS)")
			(pinfunction "S_1")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at -2.74725 0.635 270)
			(size 1 0.75)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 123 "Net-(IC2-CS)")
			(pinfunction "S_2")
			(pintype "passive")
		)
		(pad "3" smd roundrect
			(at -2.74725 -0.635 270)
			(size 1 0.75)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 123 "Net-(IC2-CS)")
			(pinfunction "S_3")
			(pintype "passive")
		)
		(pad "4" smd roundrect
			(at -2.74725 -1.905 270)
			(size 1 0.75)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 122 "Net-(IC2-LO)")
			(pinfunction "G")
			(pintype "passive")
		)
		(pad "5" smd custom
			(at 0.745 0 270)
			(size 4.055 4.56)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 7 "Net-(IC2-SW)")
			(pinfunction "D")
			(pintype "passive")
			(zone_connect 0)
			(thermal_bridge_angle 45)
			(options
				(clearance outline)
				(anchor rect)
			)
			(primitives
				(gr_poly
					(pts
						(xy -0.6975 2.28) (xy 2.5025 2.28) (xy 2.5025 1.53) (xy 1.905 1.53) (xy 1.905 -1.53) (xy 2.5025 -1.53)
						(xy 2.5025 -2.28) (xy -0.6975 -2.28) (xy -0.6975 -2.775) (xy -1.6025 -2.775) (xy -1.6025 2.775)
						(xy -0.6975 2.775)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Package_SO.3dshapes/ONSemi_SO-8FL_488AA.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "B.Cu")
		(at 103.15 60.55 -90)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C6"
			(at 0 0 90)
			(layer "B.SilkS")
		)
		(property "Value" "33nF"
			(at 0 -1.43 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/Power Supply/")
		(sheetfile "Power Supply.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 270)
			(size 0.9 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 7 "Net-(IC2-SW)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 270)
			(size 0.9 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 6 "Net-(D2-K)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_Cat16-4"
		(layer "B.Cu")
		(at 89.625 110.71 -90)
		(descr "SMT resistor net, Bourns CAT16 series, 4 way")
		(tags "SMT resistor net Bourns CAT16 series 4 way")
		(property "Reference" "RN3"
			(at 0 0 90)
			(layer "B.SilkS")
		)
		(property "Value" "2.2k"
			(at 0 -2.55 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "4 resistor network, parallel topology, split"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "DIP* SOIC* R*Array*Concave* R*Array*Convex* MSOP*")
		(sheetname "/4-20mA Inputs/")
		(sheetfile "4-20mA Inputs.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd rect
			(at -0.76 1.2 90)
			(size 0.76 0.43)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 42 "Net-(RN3A-R1.1)")
			(pinfunction "R1.1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.76 0.4 90)
			(size 0.76 0.43)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 43 "/4-20mA Inputs/AIN1")
			(pinfunction "R2.1")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at -0.76 -0.4 90)
			(size 0.76 0.43)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 46 "Net-(RN3C-R3.1)")
			(pinfunction "R3.1")
			(pintype "passive")
		)
		(pad "4" smd rect
			(at -0.76 -1.2 90)
			(size 0.76 0.43)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 47 "/4-20mA Inputs/AIN0")
			(pinfunction "R4.1")
			(pintype "passive")
		)
		(pad "5" smd rect
			(at 0.76 -1.2 90)
			(size 0.76 0.43)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 46 "Net-(RN3C-R3.1)")
			(pinfunction "R4.2")
			(pintype "passive")
		)
		(pad "6" smd rect
			(at 0.76 -0.4 90)
			(size 0.76 0.43)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 211 "Net-(RN3C-R3.2)")
			(pinfunction "R3.2")
			(pintype "passive")
		)
		(pad "7" smd rect
			(at 0.76 0.4 90)
			(size 0.76 0.43)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 42 "Net-(RN3A-R1.1)")
			(pinfunction "R2.2")
			(pintype "passive")
		)
		(pad "8" smd rect
			(at 0.76 1.2 90)
			(size 0.76 0.43)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 207 "Net-(RN3A-R1.2)")
			(pinfunction "R1.2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_Cat16-4.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_Phoenix_MC:PhoenixContact_MC_1,5_8-G-3.81_1x08_P3.81mm_Horizontal"
		(layer "B.Cu")
		(at 69.91 99.0175 90)
		(descr "Generic Phoenix Contact connector footprint for: MC_1,5/8-G-3.81; number of pins: 08; pin pitch: 3.81mm; Angled || order number: 1803332 8A 160V")
		(tags "phoenix_contact connector MC_01x08_G_3.81mm")
		(property "Reference" "J2"
			(at 13.28 -2.9325 90)
			(layer "B.SilkS")
		)
		(property "Value" "Conn_01x08_Socket"
			(at 13.33 -9.2 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x08, script generated"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "/0-10V INPUTS/")
		(sheetfile "0-10V INPUTS.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 13.28 -2.9325 90)
			(layer "B.Fab")
		)
		(pad "1" thru_hole roundrect
			(at 0 0 90)
			(size 1.8 3.6)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.138889)
			(net 150 "/0-10V INPUTS/IN10V1")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 3.81 0 90)
			(size 1.8 3.6)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 7.62 0 90)
			(size 1.8 3.6)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 151 "/0-10V INPUTS/IN10V2")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole oval
			(at 11.43 0 90)
			(size 1.8 3.6)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(pad "5" thru_hole oval
			(at 15.24 0 90)
			(size 1.8 3.6)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 152 "/0-10V INPUTS/IN10V3")
			(pinfunction "Pin_5")
			(pintype "passive")
		)
		(pad "6" thru_hole oval
			(at 19.05 0 90)
			(size 1.8 3.6)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "Pin_6")
			(pintype "passive")
		)
		(pad "7" thru_hole oval
			(at 22.86 0 90)
			(size 1.8 3.6)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 153 "/0-10V INPUTS/IN10V4")
			(pinfunction "Pin_7")
			(pintype "passive")
		)
		(pad "8" thru_hole oval
			(at 26.67 0 90)
			(size 1.8 3.6)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "Pin_8")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_Phoenix_MC.3dshapes/PhoenixContact_MC_1,5_8-G-3.81_1x08_P3.81mm_Horizontal.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "B.Cu")
		(at 110.9 47.975)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C9"
			(at 0 0 0)
			(layer "B.SilkS")
		)
		(property "Value" "5.1pF"
			(at 0 -1.43 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/Power Supply/")
		(sheetfile "Power Supply.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0)
			(size 0.9 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 10 "Net-(IC2-FB)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0)
			(size 0.9 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 11 "Net-(IC2-COMP)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "B.Cu")
		(at 85.45 52.425)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C1"
			(at 0 0 0)
			(layer "B.SilkS")
		)
		(property "Value" "4.7uF"
			(at 0 -1.68 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/Power Supply/")
		(sheetfile "Power Supply.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0)
			(size 1 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 1 "Net-(D1-K)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0)
			(size 1 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "B.Cu")
		(at 102.65 48.775 90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R1"
			(at 0 0 90)
			(layer "B.SilkS")
		)
		(property "Value" "10k"
			(at 0 -1.43 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Power Supply/")
		(sheetfile "Power Supply.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 90)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 125 "Net-(IC2-UVLO)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0 90)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "B.Cu")
		(at 85.275 50.575)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C2"
			(at 0 0 0)
			(layer "B.SilkS")
		)
		(property "Value" "100nF"
			(at 0 -1.43 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/Power Supply/")
		(sheetfile "Power Supply.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0)
			(size 0.9 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 1 "Net-(D1-K)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0)
			(size 0.9 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_Phoenix_MC:PhoenixContact_MC_1,5_2-G-3.81_1x02_P3.81mm_Horizontal"
		(layer "B.Cu")
		(at 68.6575 49.95 90)
		(descr "Generic Phoenix Contact connector footprint for: MC_1,5/2-G-3.81; number of pins: 02; pin pitch: 3.81mm; Angled || order number: 1803277 8A 160V")
		(tags "phoenix_contact connector MC_01x02_G_3.81mm")
		(property "Reference" "J1"
			(at 1.85 -2.9325 90)
			(layer "B.SilkS")
		)
		(property "Value" "Conn_01x02_Socket"
			(at 1.9 -9.2 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x02, script generated"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "/Power Supply/")
		(sheetfile "Power Supply.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 1.85 -2.9325 90)
			(layer "B.Fab")
		)
		(pad "1" thru_hole roundrect
			(at 0 0 90)
			(size 1.8 3.6)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.138889)
			(net 5 "+24V")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 3.81 0 90)
			(size 1.8 3.6)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_Phoenix_MC.3dshapes/PhoenixContact_MC_1,5_2-G-3.81_1x02_P3.81mm_Horizontal.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_Cat16-4"
		(layer "B.Cu")
		(at 174.7 52.26 -90)
		(descr "SMT resistor net, Bourns CAT16 series, 4 way")
		(tags "SMT resistor net Bourns CAT16 series 4 way")
		(property "Reference" "RN4"
			(at 0 0 90)
			(layer "B.SilkS")
		)
		(property "Value" "10k"
			(at 0 -2.55 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "4 resistor network, parallel topology"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "DIP* SOIC* R*Array*Concave* R*Array*Convex* MSOP*")
		(sheetname "/0-10VOutput/")
		(sheetfile "0-10VOutput.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd rect
			(at -0.76 1.2 90)
			(size 0.76 0.43)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 136 "/0-10VOutput/10V OUT1")
			(pinfunction "R1.1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.76 0.4 90)
			(size 0.76 0.43)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 137 "/0-10VOutput/10V OUT2")
			(pinfunction "R2.1")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at -0.76 -0.4 90)
			(size 0.76 0.43)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 141 "/0-10VOutput/10V OUT3")
			(pinfunction "R3.1")
			(pintype "passive")
		)
		(pad "4" smd rect
			(at -0.76 -1.2 90)
			(size 0.76 0.43)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 138 "/0-10VOutput/10V OUT4")
			(pinfunction "R4.1")
			(pintype "passive")
		)
		(pad "5" smd rect
			(at 0.76 -1.2 90)
			(size 0.76 0.43)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 2 "GND")
			(pinfunction "R4.2")
			(pintype "passive")
		)
		(pad "6" smd rect
			(at 0.76 -0.4 90)
			(size 0.76 0.43)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 2 "GND")
			(pinfunction "R3.2")
			(pintype "passive")
		)
		(pad "7" smd rect
			(at 0.76 0.4 90)
			(size 0.76 0.43)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 2 "GND")
			(pinfunction "R2.2")
			(pintype "passive")
		)
		(pad "8" smd rect
			(at 0.76 1.2 90)
			(size 0.76 0.43)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 2 "GND")
			(pinfunction "R1.2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_Cat16-4.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_2512_6332Metric"
		(layer "B.Cu")
		(at 111.68 60.4 90)
		(descr "Resistor SMD 2512 (6332 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R8"
			(at 0 0 90)
			(layer "B.SilkS")
		)
		(property "Value" "10m"
			(at 0 -2.63 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Power Supply/")
		(sheetfile "Power Supply.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -2.9625 0 90)
			(size 1.225 3.35)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.204082)
			(net 123 "Net-(IC2-CS)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 2.9625 0 90)
			(size 1.225 3.35)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.204082)
			(net 120 "Net-(IC2-CSG)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_2512_6332Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "B.Cu")
		(at 114.575 51.4)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R6"
			(at 0 0 0)
			(layer "B.SilkS")
		)
		(property "Value" "10k"
			(at 0 -1.43 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Power Supply/")
		(sheetfile "Power Supply.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 10 "Net-(IC2-FB)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
		(layer "B.Cu")
		(at 130.4 118.32 -90)
		(descr "SOIC, 8 Pin (JEDEC MS-012AA, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_narrow-r/r_8.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOIC SO")
		(property "Reference" "U9"
			(at 0 0.0675 90)
			(layer "B.SilkS")
		)
		(property "Value" "SP3485EN"
			(at 0 -3.4 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "http://www.icbase.com/pdf/SPX/SPX00480106.pdf"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Industrial 3.3V Low Power Half-Duplex RS-485 Transceiver 10Mbps, SOIC-8"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SOIC*3.9x4.9mm*P1.27mm*")
		(sheetname "/Communication/")
		(sheetfile "Communication.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0.0675 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -2.475 1.905 270)
			(size 1.95 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 213 "Net-(U9-RO)")
			(pinfunction "RO")
			(pintype "output")
		)
		(pad "2" smd roundrect
			(at -2.475 0.635 270)
			(size 1.95 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 166 "/RS485_DE")
			(pinfunction "~{RE}")
			(pintype "input")
		)
		(pad "3" smd roundrect
			(at -2.475 -0.635 270)
			(size 1.95 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 166 "/RS485_DE")
			(pinfunction "DE")
			(pintype "input")
		)
		(pad "4" smd roundrect
			(at -2.475 -1.905 270)
			(size 1.95 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 214 "Net-(U9-DI)")
			(pinfunction "DI")
			(pintype "input")
		)
		(pad "5" smd roundrect
			(at 2.475 -1.905 270)
			(size 1.95 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "6" smd roundrect
			(at 2.475 -0.635 270)
			(size 1.95 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 91 "/Communication/RS485A")
			(pinfunction "A")
			(pintype "bidirectional")
		)
		(pad "7" smd roundrect
			(at 2.475 0.635 270)
			(size 1.95 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 90 "/Communication/RS485B")
			(pinfunction "B")
			(pintype "bidirectional")
		)
		(pad "8" smd roundrect
			(at 2.475 1.905 270)
			(size 1.95 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 15 "+3.3V")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Package_SO.3dshapes/SOIC-8_3.9x4.9mm_P1.27mm.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "B.Cu")
		(at 113.975 49.5 180)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C10"
			(at 0 0 0)
			(layer "B.SilkS")
		)
		(property "Value" "180pF"
			(at 0 -1.43 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/Power Supply/")
		(sheetfile "Power Supply.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 180)
			(size 0.9 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 10 "Net-(IC2-FB)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 180)
			(size 0.9 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 12 "Net-(C10-Pad2)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "B.Cu")
		(at 106.075 48.85 90)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C3"
			(at 0 0 90)
			(layer "B.SilkS")
		)
		(property "Value" "150pF"
			(at 0 -1.43 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/Power Supply/")
		(sheetfile "Power Supply.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 90)
			(size 0.9 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 3 "Net-(IC2-RAMP)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 90)
			(size 0.9 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_Cat16-4"
		(layer "B.Cu")
		(at 146.6 107.915 -90)
		(descr "SMT resistor net, Bourns CAT16 series, 4 way")
		(tags "SMT resistor net Bourns CAT16 series 4 way")
		(property "Reference" "RN12"
			(at 0 0 90)
			(layer "B.SilkS")
		)
		(property "Value" "1k"
			(at 0 -2.55 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "4 resistor network, parallel topology"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "DIP* SOIC* R*Array*Concave* R*Array*Convex* MSOP*")
		(sheetname "/DigitalIO/")
		(sheetfile "DigitalIO.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd rect
			(at -0.76 1.2 90)
			(size 0.76 0.43)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 106 "Net-(HY2-ANODE_4)")
			(pinfunction "R1.1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.76 0.4 90)
			(size 0.76 0.43)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 111 "Net-(HY2-ANODE_3)")
			(pinfunction "R2.1")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at -0.76 -0.4 90)
			(size 0.76 0.43)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 105 "Net-(HY2-ANODE_2)")
			(pinfunction "R3.1")
			(pintype "passive")
		)
		(pad "4" smd rect
			(at -0.76 -1.2 90)
			(size 0.76 0.43)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 114 "Net-(HY2-ANODE_1)")
			(pinfunction "R4.1")
			(pintype "passive")
		)
		(pad "5" smd rect
			(at 0.76 -1.2 90)
			(size 0.76 0.43)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 15 "+3.3V")
			(pinfunction "R4.2")
			(pintype "passive")
		)
		(pad "6" smd rect
			(at 0.76 -0.4 90)
			(size 0.76 0.43)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 15 "+3.3V")
			(pinfunction "R3.2")
			(pintype "passive")
		)
		(pad "7" smd rect
			(at 0.76 0.4 90)
			(size 0.76 0.43)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 15 "+3.3V")
			(pinfunction "R2.2")
			(pintype "passive")
		)
		(pad "8" smd rect
			(at 0.76 1.2 90)
			(size 0.76 0.43)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 15 "+3.3V")
			(pinfunction "R1.2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_Cat16-4.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_Phoenix_MC:PhoenixContact_MC_1,5_8-G-3.81_1x08_P3.81mm_Horizontal"
		(layer "B.Cu")
		(at 69.91 132.4275 90)
		(descr "Generic Phoenix Contact connector footprint for: MC_1,5/8-G-3.81; number of pins: 08; pin pitch: 3.81mm; Angled || order number: 1803332 8A 160V")
		(tags "phoenix_contact connector MC_01x08_G_3.81mm")
		(property "Reference" "J3"
			(at 13.28 -2.9325 0)
			(layer "B.SilkS")
		)
		(property "Value" "Conn_01x08_Socket"
			(at 13.33 -9.2 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x08, script generated"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "/4-20mA Inputs/")
		(sheetfile "4-20mA Inputs.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 13.28 -2.9325 90)
			(layer "B.Fab")
		)
		(pad "1" thru_hole roundrect
			(at 0 0 90)
			(size 1.8 3.6)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.138889)
			(net 71 "/4-20mA Inputs/IN1P")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 3.81 0 90)
			(size 1.8 3.6)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 70 "/4-20mA Inputs/IN1N")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 7.62 0 90)
			(size 1.8 3.6)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 73 "/4-20mA Inputs/IN2P")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole oval
			(at 11.43 0 90)
			(size 1.8 3.6)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 72 "/4-20mA Inputs/IN2N")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(pad "5" thru_hole oval
			(at 15.24 0 90)
			(size 1.8 3.6)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 75 "/4-20mA Inputs/IN3P")
			(pinfunction "Pin_5")
			(pintype "passive")
		)
		(pad "6" thru_hole oval
			(at 19.05 0 90)
			(size 1.8 3.6)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 74 "/4-20mA Inputs/IN3N")
			(pinfunction "Pin_6")
			(pintype "passive")
		)
		(pad "7" thru_hole oval
			(at 22.86 0 90)
			(size 1.8 3.6)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 76 "/4-20mA Inputs/IN4P")
			(pinfunction "Pin_7")
			(pintype "passive")
		)
		(pad "8" thru_hole oval
			(at 26.67 0 90)
			(size 1.8 3.6)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 77 "/4-20mA Inputs/IN4N")
			(pinfunction "Pin_8")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_Phoenix_MC.3dshapes/PhoenixContact_MC_1,5_8-G-3.81_1x08_P3.81mm_Horizontal.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "B.Cu")
		(at 92.125 103.2 90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C44"
			(at 0 0 90)
			(layer "B.SilkS")
		)
		(property "Value" "1uF"
			(at 0 -1.68 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/4-20mA Inputs/")
		(sheetfile "4-20mA Inputs.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0 90)
			(size 1 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 46 "Net-(RN3C-R3.1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0 90)
			(size 1 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_Phoenix_MC:PhoenixContact_MC_1,5_8-G-3.81_1x08_P3.81mm_Horizontal"
		(layer "B.Cu")
		(at 157.69 48.4)
		(descr "Generic Phoenix Contact connector footprint for: MC_1,5/8-G-3.81; number of pins: 08; pin pitch: 3.81mm; Angled || order number: 1803332 8A 160V")
		(tags "phoenix_contact connector MC_01x08_G_3.81mm")
		(property "Reference" "J6"
			(at 13.28 -2.9325 0)
			(layer "B.SilkS")
		)
		(property "Value" "Conn_01x08_Socket"
			(at 13.33 -9.2 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x08, script generated"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "/0-10VOutput/")
		(sheetfile "0-10VOutput.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 13.28 -2.9325 0)
			(layer "B.Fab")
		)
		(pad "1" thru_hole roundrect
			(at 0 0)
			(size 1.8 3.6)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.138889)
			(net 136 "/0-10VOutput/10V OUT1")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 3.81 0)
			(size 1.8 3.6)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 7.62 0)
			(size 1.8 3.6)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 137 "/0-10VOutput/10V OUT2")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole oval
			(at 11.43 0)
			(size 1.8 3.6)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(pad "5" thru_hole oval
			(at 15.24 0)
			(size 1.8 3.6)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 141 "/0-10VOutput/10V OUT3")
			(pinfunction "Pin_5")
			(pintype "passive")
		)
		(pad "6" thru_hole oval
			(at 19.05 0)
			(size 1.8 3.6)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "Pin_6")
			(pintype "passive")
		)
		(pad "7" thru_hole oval
			(at 22.86 0)
			(size 1.8 3.6)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 138 "/0-10VOutput/10V OUT4")
			(pinfunction "Pin_7")
			(pintype "passive")
		)
		(pad "8" thru_hole oval
			(at 26.67 0)
			(size 1.8 3.6)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "Pin_8")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_Phoenix_MC.3dshapes/PhoenixContact_MC_1,5_8-G-3.81_1x08_P3.81mm_Horizontal.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "B.Cu")
		(at 134.39 114.94 -90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R90"
			(at 0 0 90)
			(layer "B.SilkS")
		)
		(property "Value" "120"
			(at 0 -1.43 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Communication/")
		(sheetfile "Communication.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 270)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 169 "/RS485_TX")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0 270)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 214 "Net-(U9-DI)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_SMD:SOT-23"
		(layer "B.Cu")
		(at 97.24 127.2623)
		(descr "SOT, 3 Pin (JEDEC TO-236 Var AB https://www.jedec.org/document_search?search_api_views_fulltext=TO-236), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOT TO_SOT_SMD")
		(property "Reference" "Q5"
			(at 0 0 0)
			(layer "B.SilkS")
		)
		(property "Value" "MMBT3904"
			(at 0 -2.4 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.onsemi.com/pdf/datasheet/pzt3904-d.pdf"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "0.2A Ic, 40V Vce, Small Signal NPN Transistor, SOT-23"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SOT?23*")
		(sheetname "/4-20mA Inputs/")
		(sheetfile "4-20mA Inputs.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9375 0.95)
			(size 1.475 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 44 "Net-(Q5-B)")
			(pinfunction "B")
			(pintype "input")
		)
		(pad "2" smd roundrect
			(at -0.9375 -0.95)
			(size 1.475 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 183 "Net-(Q5-E)")
			(pinfunction "E")
			(pintype "passive")
		)
		(pad "3" smd roundrect
			(at 0.9375 0)
			(size 1.475 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 9 "+5V")
			(pinfunction "C")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1210_3225Metric"
		(layer "B.Cu")
		(at 101.71 70.39 -90)
		(descr "Capacitor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C8"
			(at 0 0 90)
			(layer "B.SilkS")
		)
		(property "Value" "47uF"
			(at 0 -2.3 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/Power Supply/")
		(sheetfile "Power Supply.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.475 0 270)
			(size 1.15 2.7)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.217391)
			(net 9 "+5V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.475 0 270)
			(size 1.15 2.7)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.217391)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1210_3225Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "B.Cu")
		(at 179.7 61.075 180)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C57"
			(at 0 0 0)
			(layer "B.SilkS")
		)
		(property "Value" "220nF"
			(at 0 -1.43 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/0-10VOutput/")
		(sheetfile "0-10VOutput.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 180)
			(size 0.9 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 180)
			(size 0.9 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 24 "-12V")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "B.Cu")
		(at 106.875 45.775 -90)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C5"
			(at 0 0 90)
			(layer "B.SilkS")
		)
		(property "Value" "150pF"
			(at 0 -1.43 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/Power Supply/")
		(sheetfile "Power Supply.kicad_sch")
		(attr smd)
		(pad "1" smd roundrect
			(at -0.775 0 270)
			(size 0.9 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 5 "+24V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 270)
			(size 0.9 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "footprints:EDJ4"
		(layer "B.Cu")
		(at 175.265 108.795 -90)
		(tags "DCH010512SN7 ")
		(property "Reference" "U3"
			(at -7.62 2.54 90)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "DCH010512SN7"
			(at -7.62 2.54 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.ti.com/lit/gpn/dch010512s"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "EDJ4")
		(sheetname "/Power Supply/")
		(sheetfile "Power Supply.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at -7.62 2.54 90)
			(unlocked yes)
			(layer "B.Fab")
		)
		(pad "1" thru_hole circle
			(at -15.24 5.08 270)
			(size 1.2446 1.2446)
			(drill 0.9652)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 16 "Net-(U3-VI+)")
			(pinfunction "VI+")
			(pintype "input")
		)
		(pad "2" thru_hole circle
			(at -12.7 5.08 270)
			(size 1.2446 1.2446)
			(drill 0.9652)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "VI-")
			(pintype "input")
		)
		(pad "3" thru_hole circle
			(at -5.08 5.08 270)
			(size 1.2446 1.2446)
			(drill 0.9652)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 17 "GNDA")
			(pinfunction "3")
			(pintype "unspecified")
		)
		(pad "4" thru_hole circle
			(at 0 5.08 270)
			(size 1.2446 1.2446)
			(drill 0.9652)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 18 "Net-(C17-Pad1)")
			(pinfunction "4")
			(pintype "unspecified")
		)
		(embedded_fonts no)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "B.Cu")
		(at 104.25 48.8 90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R3"
			(at 0 0 90)
			(layer "B.SilkS")
		)
		(property "Value" "3.09k"
			(at 0 -1.43 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Power Supply/")
		(sheetfile "Power Supply.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 90)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 119 "Net-(IC2-RT{slash}SYNC)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0 90)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_Phoenix_MC:PhoenixContact_MC_1,5_8-G-3.81_1x08_P3.81mm_Horizontal"
		(layer "B.Cu")
		(at 212.5925 79.77 -90)
		(descr "Generic Phoenix Contact connector footprint for: MC_1,5/8-G-3.81; number of pins: 08; pin pitch: 3.81mm; Angled || order number: 1803332 8A 160V")
		(tags "phoenix_contact connector MC_01x08_G_3.81mm")
		(property "Reference" "J7"
			(at 13.28 -2.9325 90)
			(layer "B.SilkS")
		)
		(property "Value" "Conn_01x08_Socket"
			(at 13.33 -9.2 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x08, script generated"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "/4-20mAOutput/")
		(sheetfile "4-20mAOutput.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 13.28 -2.9325 90)
			(layer "B.Fab")
		)
		(pad "1" thru_hole roundrect
			(at 0 0 270)
			(size 1.8 3.6)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.138889)
			(net 179 "/4-20mAOutput/OUT1")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 3.81 0 270)
			(size 1.8 3.6)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "+24V")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 7.62 0 270)
			(size 1.8 3.6)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 187 "/4-20mAOutput/OUT2")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole oval
			(at 11.43 0 270)
			(size 1.8 3.6)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "+24V")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(pad "5" thru_hole oval
			(at 15.24 0 270)
			(size 1.8 3.6)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 189 "/4-20mAOutput/OUT3")
			(pinfunction "Pin_5")
			(pintype "passive")
		)
		(pad "6" thru_hole oval
			(at 19.05 0 270)
			(size 1.8 3.6)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "+24V")
			(pinfunction "Pin_6")
			(pintype "passive")
		)
		(pad "7" thru_hole oval
			(at 22.86 0 270)
			(size 1.8 3.6)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 191 "/4-20mAOutput/OUT4")
			(pinfunction "Pin_7")
			(pintype "passive")
		)
		(pad "8" thru_hole oval
			(at 26.67 0 270)
			(size 1.8 3.6)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "+24V")
			(pinfunction "Pin_8")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_Phoenix_MC.3dshapes/PhoenixContact_MC_1,5_8-G-3.81_1x08_P3.81mm_Horizontal.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "SamacSys_Parts:L_Bourns_SRR4528A"
		(layer "B.Cu")
		(at 93.01 68.94)
		(property "Reference" "L1"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(property "Value" "2.7uH"
			(at 0 -1 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Inductor, small symbol"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Choke_* *Coil* Inductor_* L_*")
		(sheetname "/Power Supply/")
		(sheetfile "Power Supply.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
		)
		(pad "1" smd rect
			(at -2.1 0)
			(size 1.6 5.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 7 "Net-(IC2-SW)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 2.1 0)
			(size 1.6 5.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.15)
			(net 9 "+5V")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "SamacSys_Parts:00318201G"
		(layer "B.Cu")
		(at 62.125 60.075)
		(descr "0031.8201.G-4")
		(tags "Hardware")
		(property "Reference" "F1"
			(at 11.25 0 0)
			(layer "B.SilkS")
		)
		(property "Value" "Fuse"
			(at 11.25 0 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Fuse"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*Fuse*")
		(sheetname "/Power Supply/")
		(sheetfile "Power Supply.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 11.25 0 0)
			(layer "B.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.95 1.95)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "+24V")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 22.5 0)
			(size 1.95 1.95)
			(drill 1.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "Net-(D1-K)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "C:\\Users\\ESpurbeck\\Documents\\KiCad\\3rdparty\\SamacSys_Parts.3dshapes\\0031.8201.G.stp"
			(offset
				(xyz 11.25 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 -0 -0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "B.Cu")
		(at 126.4 115.945 -90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R89"
			(at 0 0 90)
			(layer "B.SilkS")
		)
		(property "Value" "120"
			(at 0 -1.43 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Communication/")
		(sheetfile "Communication.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 270)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 168 "/RS485_RX")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0 270)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 213 "Net-(U9-RO)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "B.Cu")
		(at 106.7 60.4)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C7"
			(at 0 0 0)
			(layer "B.SilkS")
		)
		(property "Value" "1uF"
			(at 0 -1.68 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/Power Supply/")
		(sheetfile "Power Supply.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0)
			(size 1 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 8 "/Power Supply/VCC")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0)
			(size 1 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_SMD:SOT-23"
		(layer "B.Cu")
		(at 106.6875 63.625)
		(descr "SOT, 3 Pin (JEDEC TO-236 Var AB https://www.jedec.org/document_search?search_api_views_fulltext=TO-236), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOT TO_SOT_SMD")
		(property "Reference" "D2"
			(at 0 0 0)
			(layer "B.SilkS")
		)
		(property "Value" "CMPD2003"
			(at 0 -2.4 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Diode, small symbol"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sim.Device" "D"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TO-???* *_Diode_* *SingleDiode* D_*")
		(sheetname "/Power Supply/")
		(sheetfile "Power Supply.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9375 0.95)
			(size 1.475 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 6 "Net-(D2-K)")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at -0.9375 -0.95)
			(size 1.475 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 8 "/Power Supply/VCC")
			(pinfunction "A")
			(pintype "passive")
		)
		(pad "3" smd roundrect
			(at 0.9375 0)
			(size 1.475 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_Cat16-4"
		(layer "B.Cu")
		(at 186.06 112.535 -90)
		(descr "SMT resistor net, Bourns CAT16 series, 4 way")
		(tags "SMT resistor net Bourns CAT16 series 4 way")
		(property "Reference" "RN11"
			(at 0 0 90)
			(layer "B.SilkS")
		)
		(property "Value" "4.7k"
			(at 0 -2.55 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "4 resistor network, parallel topology"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "DIP* SOIC* R*Array*Concave* R*Array*Convex* MSOP*")
		(sheetname "/DigitalIO/")
		(sheetfile "DigitalIO.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd rect
			(at -0.76 1.2 90)
			(size 0.76 0.43)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 101 "/OPTO_IN1")
			(pinfunction "R1.1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -0.76 0.4 90)
			(size 0.76 0.43)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 102 "/OPTO_IN2")
			(pinfunction "R2.1")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at -0.76 -0.4 90)
			(size 0.76 0.43)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 97 "/OPTO_IN3")
			(pinfunction "R3.1")
			(pintype "passive")
		)
		(pad "4" smd rect
			(at -0.76 -1.2 90)
			(size 0.76 0.43)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 99 "/OPTO_IN4")
			(pinfunction "R4.1")
			(pintype "passive")
		)
		(pad "5" smd rect
			(at 0.76 -1.2 90)
			(size 0.76 0.43)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 15 "+3.3V")
			(pinfunction "R4.2")
			(pintype "passive")
		)
		(pad "6" smd rect
			(at 0.76 -0.4 90)
			(size 0.76 0.43)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 15 "+3.3V")
			(pinfunction "R3.2")
			(pintype "passive")
		)
		(pad "7" smd rect
			(at 0.76 0.4 90)
			(size 0.76 0.43)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 15 "+3.3V")
			(pinfunction "R2.2")
			(pintype "passive")
		)
		(pad "8" smd rect
			(at 0.76 1.2 90)
			(size 0.76 0.43)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 15 "+3.3V")
			(pinfunction "R1.2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_Cat16-4.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "B.Cu")
		(at 105.4 45.75 -90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R4"
			(at 0 0 90)
			(layer "B.SilkS")
		)
		(property "Value" "33k"
			(at 0 -1.43 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Power Supply/")
		(sheetfile "Power Supply.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 270)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 5 "+24V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0 270)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 121 "Net-(IC2-EN)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_Phoenix_MC:PhoenixContact_MC_1,5_8-G-3.81_1x08_P3.81mm_Horizontal"
		(layer "B.Cu")
		(at 200.11 126.335 180)
		(descr "Generic Phoenix Contact connector footprint for: MC_1,5/8-G-3.81; number of pins: 08; pin pitch: 3.81mm; Angled || order number: 1803332 8A 160V")
		(tags "phoenix_contact connector MC_01x08_G_3.81mm")
		(property "Reference" "J8"
			(at 13.28 -2.9325 0)
			(layer "B.SilkS")
		)
		(property "Value" "Conn_01x08_Socket"
			(at 13.33 -9.2 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x08, script generated"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "/DigitalIO/")
		(sheetfile "DigitalIO.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 13.28 -2.9325 0)
			(layer "B.Fab")
		)
		(pad "1" thru_hole roundrect
			(at 0 0 180)
			(size 1.8 3.6)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.138889)
			(net 85 "/DigitalIO/VEX1")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 3.81 0 180)
			(size 1.8 3.6)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 94 "/DigitalIO/OP1")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 7.62 0 180)
			(size 1.8 3.6)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 82 "/DigitalIO/VEX2")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole oval
			(at 11.43 0 180)
			(size 1.8 3.6)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 92 "/DigitalIO/OP2")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(pad "5" thru_hole oval
			(at 15.24 0 180)
			(size 1.8 3.6)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 81 "/DigitalIO/VEX3")
			(pinfunction "Pin_5")
			(pintype "passive")
		)
		(pad "6" thru_hole oval
			(at 19.05 0 180)
			(size 1.8 3.6)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 96 "/DigitalIO/OP3")
			(pinfunction "Pin_6")
			(pintype "passive")
		)
		(pad "7" thru_hole oval
			(at 22.86 0 180)
			(size 1.8 3.6)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 79 "/DigitalIO/VEX4")
			(pinfunction "Pin_7")
			(pintype "passive")
		)
		(pad "8" thru_hole oval
			(at 26.67 0 180)
			(size 1.8 3.6)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 103 "/DigitalIO/OP4")
			(pinfunction "Pin_8")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_Phoenix_MC.3dshapes/PhoenixContact_MC_1,5_8-G-3.81_1x08_P3.81mm_Horizontal.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "B.Cu")
		(at 101.1 48.8 90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R2"
			(at 0 0 90)
			(layer "B.SilkS")
		)
		(property "Value" "33k"
			(at 0 -1.43 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Power Supply/")
		(sheetfile "Power Supply.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 90)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 1 "Net-(D1-K)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0 90)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 125 "Net-(IC2-UVLO)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "B.Cu")
		(at 90.125 131.9)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C38"
			(at 0 0 0)
			(layer "B.SilkS")
		)
		(property "Value" "1uF"
			(at 0 -1.68 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/4-20mA Inputs/")
		(sheetfile "4-20mA Inputs.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0)
			(size 1 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 38 "Net-(RN2C-R3.1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0)
			(size 1 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "B.Cu")
		(at 108.425 47.675 90)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C4"
			(at 0 0 90)
			(layer "B.SilkS")
		)
		(property "Value" "33nF"
			(at 0 -1.43 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/Power Supply/")
		(sheetfile "Power Supply.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 90)
			(size 0.9 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 4 "Net-(IC2-SS)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 90)
			(size 0.9 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "B.Cu")
		(at 111.45 51.4)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R5"
			(at 0 0 0)
			(layer "B.SilkS")
		)
		(property "Value" "33k"
			(at 0 -1.43 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/Power Supply/")
		(sheetfile "Power Supply.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 9 "+5V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0)
			(size 0.8 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 10 "Net-(IC2-FB)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "B.Cu")
		(at 91 124.55 90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C35"
			(at 0 0 90)
			(layer "B.SilkS")
		)
		(property "Value" "1uF"
			(at 0 -1.68 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/4-20mA Inputs/")
		(sheetfile "4-20mA Inputs.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0 90)
			(size 1 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 34 "Net-(RN2A-R1.1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0 90)
			(size 1 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(gr_arc
		(start 59.99 141.41)
		(mid 59.282893 141.117107)
		(end 58.99 140.41)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 58.99 140.41)
		(end 58.99 38)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 222.99 140.41)
		(mid 222.697107 141.117107)
		(end 221.99 141.41)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 222.99 38)
		(end 222.99 140.41)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 221.99 141.41)
		(end 59.99 141.41)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 59.99 37)
		(end 221.99 37)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 221.99 37)
		(mid 222.697107 37.292893)
		(end 222.99 38)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 58.99 38)
		(mid 59.282893 37.292893)
		(end 59.99 37)
		(layer "Edge.Cuts")
	)
	(zone
		(net 2)
		(net_name "GND")
		(layers "F.Cu" "B.Cu")
		(hatch edge 0.5)
		(connect_pads yes
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 60 38) (xy 222.08 38) (xy 222.08 140.4) (xy 60 140.4)
			)
		)
	)
	(embedded_fonts no)
)
