(kicad_pcb
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(general
		(thickness 1.6)
		(legacy_teardrops no)
	)
	(paper "A4")
	(layers
		(0 "F.Cu" signal)
		(2 "B.Cu" signal)
		(9 "F.Adhes" user "F.Adhesive")
		(11 "B.Adhes" user "B.Adhesive")
		(13 "F.Paste" user)
		(15 "B.Paste" user)
		(5 "F.SilkS" user "F.Silkscreen")
		(7 "B.SilkS" user "B.Silkscreen")
		(1 "F.Mask" user)
		(3 "B.Mask" user)
		(17 "Dwgs.User" user "User.Drawings")
		(19 "Cmts.User" user "User.Comments")
		(21 "Eco1.User" user "User.Eco1")
		(23 "Eco2.User" user "User.Eco2")
		(25 "Edge.Cuts" user)
		(27 "Margin" user)
		(31 "F.CrtYd" user "F.Courtyard")
		(29 "B.CrtYd" user "B.Courtyard")
		(35 "F.Fab" user)
		(33 "B.Fab" user)
		(39 "User.1" user)
		(41 "User.2" user)
		(43 "User.3" user)
		(45 "User.4" user)
		(47 "User.5" user)
		(49 "User.6" user)
		(51 "User.7" user)
		(53 "User.8" user)
		(55 "User.9" user)
	)
	(setup
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(tenting front back)
		(pcbplotparams
			(layerselection 0x00000000_00000000_55555555_5755f5ff)
			(plot_on_all_layers_selection 0x00000000_00000000_00000000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 4)
			(plotframeref no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(pdf_metadata yes)
			(pdf_single_document no)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plot_black_and_white yes)
			(sketchpadsonfab no)
			(plotpadnumbers no)
			(hidednponfab no)
			(sketchdnponfab yes)
			(crossoutdnponfab yes)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 1)
			(scaleselection 1)
			(outputdirectory "")
		)
	)
	(net 0 "")
	(net 1 "GNDREF")
	(net 2 "Net-(J1-Pin_1)")
	(net 3 "Net-(U1-13_SCK_CRX1_LED)")
	(net 4 "Net-(U2-SCK)")
	(net 5 "Net-(U1-11_MOSI_CTX1)")
	(net 6 "Net-(U2-MOSI)")
	(net 7 "Net-(U2-VCC)")
	(net 8 "unconnected-(U1-9_OUT1C-Pad11)")
	(net 9 "unconnected-(U1-ON_OFF-Pad19)")
	(net 10 "unconnected-(U1-3_LRCLK2-Pad5)")
	(net 11 "unconnected-(U1-25_A11_RX6_SDA2-Pad36)")
	(net 12 "unconnected-(U1-27_A13_SCK1-Pad38)")
	(net 13 "unconnected-(U1-29_TX7-Pad40)")
	(net 14 "unconnected-(U1-17_A3_TX4_SDA1-Pad24)")
	(net 15 "unconnected-(U1-28_RX7-Pad39)")
	(net 16 "Net-(U1-12_MISO_MQSL)")
	(net 17 "unconnected-(U1-31_CTX3-Pad42)")
	(net 18 "unconnected-(U1-22_A8_CTX1-Pad29)")
	(net 19 "unconnected-(U1-16_A2_RX4_SCL1-Pad23)")
	(net 20 "unconnected-(U1-26_A12_MOSI1-Pad37)")
	(net 21 "unconnected-(U1-1_TX1_CTX2_MISO1-Pad3)")
	(net 22 "unconnected-(U1-23_A9_CRX1_MCLK1-Pad30)")
	(net 23 "unconnected-(U1-21_A7_RX5_BCLK1-Pad28)")
	(net 24 "unconnected-(U1-PROGRAM-Pad18)")
	(net 25 "unconnected-(U1-0_RX1_CRX2_CS1-Pad2)")
	(net 26 "unconnected-(U1-15_A1_RX3_SPDIF_IN-Pad22)")
	(net 27 "Net-(U1-7_RX2_OUT1A)")
	(net 28 "unconnected-(U1-VBAT-Pad15)")
	(net 29 "unconnected-(U1-20_A6_TX5_LRCLK1-Pad27)")
	(net 30 "unconnected-(U1-18_A4_SDA0-Pad25)")
	(net 31 "unconnected-(U1-33_MCLK2-Pad44)")
	(net 32 "unconnected-(U1-14_A0_TX3_SPDIF_OUT-Pad21)")
	(net 33 "unconnected-(U1-19_A5_SCL0-Pad26)")
	(net 34 "unconnected-(U1-VUSB-Pad34)")
	(net 35 "unconnected-(U1-30_CRX3-Pad41)")
	(net 36 "unconnected-(U1-24_A10_TX6_SCL2-Pad35)")
	(net 37 "unconnected-(U1-4_BCLK2-Pad6)")
	(net 38 "unconnected-(U1-10_CS_MQSR-Pad12)")
	(net 39 "Net-(U1-6_OUT1D)")
	(net 40 "unconnected-(U1-2_OUT2-Pad4)")
	(net 41 "unconnected-(U1-32_OUT1B-Pad43)")
	(net 42 "unconnected-(U1-5_IN2-Pad7)")
	(net 43 "unconnected-(U2-IRQ-Pad8)")
	(net 44 "Net-(J2-Pin_2)")
	(footprint "Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal"
		(layer "F.Cu")
		(at 109.22 96.52)
		(descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=5.08mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 5.08mm 0.167W length 3.6mm diameter 1.6mm")
		(property "Reference" "R2"
			(at -0.055772 2.473973 0)
			(layer "F.SilkS")
		)
		(property "Value" "100"
			(at 5.05801 2.473973 0)
			(layer "F.SilkS")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, small US symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "Teensy-RV-Leveling-Helper-Pair-LED-Controller.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 2.54 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1.4 1.4)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "Net-(U1-11_MOSI_CTX1)")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 5.08 0)
			(size 1.4 1.4)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "Net-(U2-MOSI)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal"
		(layer "F.Cu")
		(at 129.54 91.44)
		(descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=5.08mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
		(tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 5.08mm 0.167W length 3.6mm diameter 1.6mm")
		(property "Reference" "R1"
			(at -0.064696 2.531338 0)
			(layer "F.SilkS")
		)
		(property "Value" "100"
			(at 5.049086 2.531338 0)
			(layer "F.SilkS")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor, small US symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "Teensy-RV-Leveling-Helper-Pair-LED-Controller.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 2.54 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 1.4 1.4)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "Net-(U1-13_SCK_CRX1_LED)")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 5.08 0)
			(size 1.4 1.4)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "Net-(U2-SCK)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P5.08mm_Horizontal.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MountingHole:MountingHole_2.7mm_M2.5_DIN965_Pad_TopBottom"
		(layer "F.Cu")
		(at 144.78 91.44)
		(descr "Mounting Hole 2.7mm, M2.5, generated by kicad-footprint-generator mountinghole.py")
		(tags "mountinghole M2.5 DIN965")
		(property "Reference" "H4"
			(at 0 -3.3 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "MountingHole"
			(at 0 3.3 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Mounting Hole without connection"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "MountingHole*")
		(sheetname "/")
		(sheetfile "Teensy-RV-Leveling-Helper-Pair-LED-Controller.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 3.1 3.1)
			(drill 2.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(zone_connect 2)
		)
		(pad "1" connect circle
			(at 0 0)
			(size 4.7 4.7)
			(layers "F.Cu" "F.Mask")
			(zone_connect 2)
		)
		(pad "1" connect circle
			(at 0 0)
			(size 4.7 4.7)
			(layers "B.Cu" "B.Mask")
			(zone_connect 2)
		)
		(embedded_fonts no)
	)
	(footprint "MountingHole:MountingHole_2.7mm_M2.5_DIN965_Pad_TopBottom"
		(layer "F.Cu")
		(at 106.68 55.88)
		(descr "Mounting Hole 2.7mm, M2.5, generated by kicad-footprint-generator mountinghole.py")
		(tags "mountinghole M2.5 DIN965")
		(property "Reference" "H2"
			(at 0 -3.3 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "MountingHole"
			(at 0 3.3 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Mounting Hole without connection"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "MountingHole*")
		(sheetname "/")
		(sheetfile "Teensy-RV-Leveling-Helper-Pair-LED-Controller.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 3.1 3.1)
			(drill 2.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(zone_connect 2)
		)
		(pad "1" connect circle
			(at 0 0)
			(size 4.7 4.7)
			(layers "F.Cu" "F.Mask")
			(zone_connect 2)
		)
		(pad "1" connect circle
			(at 0 0)
			(size 4.7 4.7)
			(layers "B.Cu" "B.Mask")
			(zone_connect 2)
		)
		(embedded_fonts no)
	)
	(footprint "Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 142.2073 104.0757 -90)
		(descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x03 2.54mm single row")
		(property "Reference" "J2"
			(at 2.6043 5.0473 0)
			(layer "F.SilkS")
		)
		(property "Value" "WS2812B"
			(at 2.6043 -0.0327 0)
			(layer "F.SilkS")
		)
		(property "Datasheet" "~"
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x03, script generated"
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "/")
		(sheetfile "Teensy-RV-Leveling-Helper-Pair-LED-Controller.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 2.54 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "Net-(J1-Pin_1)")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 0 2.54 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 44 "Net-(J2-Pin_2)")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole circle
			(at 0 5.08 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GNDREF")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_THT:CP_Radial_Tantal_D4.5mm_P2.50mm"
		(layer "F.Cu")
		(at 124.3978 104.0757 90)
		(descr "CP, Radial_Tantal series, Radial, pin pitch=2.50mm, diameter=4.5mm, height=10mm, Tantal Electrolytic Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/TANTAL-TB-Serie%23.pdf")
		(tags "CP Radial_Tantal series Radial pin pitch 2.50mm diameter 4.5mm height 10mm Tantal Electrolytic Capacitor")
		(property "Reference" "C2"
			(at -2.383948 0 180)
			(layer "F.SilkS")
		)
		(property "Value" "100uF"
			(at 5.25871 0 180)
			(layer "F.SilkS")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "capacitor, US symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "Teensy-RV-Leveling-Helper-Pair-LED-Controller.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 1.25 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole roundrect
			(at 0 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.15625)
			(net 2 "Net-(J1-Pin_1)")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 2.5 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GNDREF")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_THT.3dshapes/CP_Radial_Tantal_D4.5mm_P2.50mm.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MountingHole:MountingHole_2.7mm_M2.5_DIN965_Pad_TopBottom"
		(layer "F.Cu")
		(at 144.78 55.88)
		(descr "Mounting Hole 2.7mm, M2.5, generated by kicad-footprint-generator mountinghole.py")
		(tags "mountinghole M2.5 DIN965")
		(property "Reference" "H1"
			(at 0 -3.3 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "MountingHole"
			(at 0 3.3 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Mounting Hole without connection"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "MountingHole*")
		(sheetname "/")
		(sheetfile "Teensy-RV-Leveling-Helper-Pair-LED-Controller.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 3.1 3.1)
			(drill 2.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(zone_connect 2)
		)
		(pad "1" connect circle
			(at 0 0)
			(size 4.7 4.7)
			(layers "F.Cu" "F.Mask")
			(zone_connect 2)
		)
		(pad "1" connect circle
			(at 0 0)
			(size 4.7 4.7)
			(layers "B.Cu" "B.Mask")
			(zone_connect 2)
		)
		(embedded_fonts no)
	)
	(footprint "Capacitor_THT:CP_Radial_Tantal_D4.5mm_P2.50mm"
		(layer "F.Cu")
		(at 132.0405 104.0757 90)
		(descr "CP, Radial_Tantal series, Radial, pin pitch=2.50mm, diameter=4.5mm, height=10mm, Tantal Electrolytic Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/TANTAL-TB-Serie%23.pdf")
		(tags "CP Radial_Tantal series Radial pin pitch 2.50mm diameter 4.5mm height 10mm Tantal Electrolytic Capacitor")
		(property "Reference" "C1"
			(at -2.548361 0 180)
			(layer "F.SilkS")
		)
		(property "Value" "0.1uF"
			(at 5.024181 0 0)
			(layer "F.SilkS")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "capacitor, US symbol"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "Teensy-RV-Leveling-Helper-Pair-LED-Controller.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 1.25 0 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole roundrect
			(at 0 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.15625)
			(net 2 "Net-(J1-Pin_1)")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 2.5 0 90)
			(size 1.6 1.6)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GNDREF")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_THT.3dshapes/CP_Radial_Tantal_D4.5mm_P2.50mm.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "RF_Module:nRF24L01_Breakout"
		(layer "F.Cu")
		(at 129.54 86.36 90)
		(descr "nRF24L01 breakout board")
		(tags "nRF24L01 adapter breakout")
		(property "Reference" "U2"
			(at 0 -3 90)
			(layer "F.SilkS")
		)
		(property "Value" "NRF24L01_Breakout"
			(at 13 5 90)
			(layer "F.SilkS")
		)
		(property "Datasheet" "http://www.nordicsemi.com/eng/content/download/2730/34105/file/nRF24L01_Product_Specification_v2_0.pdf"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "nRF24L01*Breakout*")
		(sheetname "/")
		(sheetfile "Teensy-RV-Leveling-Helper-Pair-LED-Controller.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 12.5 2.5 90)
			(layer "F.SilkS")
		)
		(pad "1" thru_hole rect
			(at 0 0 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GNDREF")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "2" thru_hole circle
			(at 2.54 0 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 7 "Net-(U2-VCC)")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(pad "3" thru_hole circle
			(at 0 2.54 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 27 "Net-(U1-7_RX2_OUT1A)")
			(pinfunction "CE")
			(pintype "input")
		)
		(pad "4" thru_hole circle
			(at 2.54 2.54 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 39 "Net-(U1-6_OUT1D)")
			(pinfunction "~{CSN}")
			(pintype "input")
		)
		(pad "5" thru_hole circle
			(at 0 5.08 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 4 "Net-(U2-SCK)")
			(pinfunction "SCK")
			(pintype "input")
		)
		(pad "6" thru_hole circle
			(at 2.54 5.08 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 6 "Net-(U2-MOSI)")
			(pinfunction "MOSI")
			(pintype "input")
		)
		(pad "7" thru_hole circle
			(at 0 7.62 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 16 "Net-(U1-12_MISO_MQSL)")
			(pinfunction "MISO")
			(pintype "output")
		)
		(pad "8" thru_hole circle
			(at 2.54 7.62 90)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 43 "unconnected-(U2-IRQ-Pad8)")
			(pinfunction "IRQ")
			(pintype "output+no_connect")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/RF_Module.3dshapes/nRF24L01_Breakout.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 144.78 96.52)
		(descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x02 2.54mm single row")
		(property "Reference" "J1"
			(at -5.096891 -0.004271 0)
			(layer "F.SilkS")
		)
		(property "Value" "POWER INPUT"
			(at 0 4.92 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x02, script generated"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "/")
		(sheetfile "Teensy-RV-Leveling-Helper-Pair-LED-Controller.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 1.27 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "Net-(J1-Pin_1)")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 0 2.54)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GNDREF")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "teensy:Teensy40"
		(layer "F.Cu")
		(at 116.84 76.2 -90)
		(property "Reference" "U1"
			(at 6.112801 10.722289 90)
			(layer "F.SilkS")
		)
		(property "Value" "Teensy4.0"
			(at -1.529857 10.722289 90)
			(layer "F.SilkS")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "Teensy-RV-Leveling-Helper-Pair-LED-Controller.kicad_sch")
		(attr through_hole)
		(fp_text user "DVL6A"
			(at 1.778 0 0)
			(layer "F.SilkS")
		)
		(fp_text user "MIMXRT1062"
			(at 0.254 0 0)
			(layer "F.SilkS")
		)
		(pad "1" thru_hole circle
			(at -16.51 7.62 270)
			(size 1.6 1.6)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GNDREF")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "2" thru_hole circle
			(at -13.97 7.62 270)
			(size 1.6 1.6)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 25 "unconnected-(U1-0_RX1_CRX2_CS1-Pad2)")
			(pinfunction "0_RX1_CRX2_CS1")
			(pintype "bidirectional+no_connect")
		)
		(pad "3" thru_hole circle
			(at -11.43 7.62 270)
			(size 1.6 1.6)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 21 "unconnected-(U1-1_TX1_CTX2_MISO1-Pad3)")
			(pinfunction "1_TX1_CTX2_MISO1")
			(pintype "bidirectional+no_connect")
		)
		(pad "4" thru_hole circle
			(at -8.89 7.62 270)
			(size 1.6 1.6)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 40 "unconnected-(U1-2_OUT2-Pad4)")
			(pinfunction "2_OUT2")
			(pintype "bidirectional+no_connect")
		)
		(pad "5" thru_hole circle
			(at -6.35 7.62 270)
			(size 1.6 1.6)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 10 "unconnected-(U1-3_LRCLK2-Pad5)")
			(pinfunction "3_LRCLK2")
			(pintype "bidirectional+no_connect")
		)
		(pad "6" thru_hole circle
			(at -3.81 7.62 270)
			(size 1.6 1.6)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 37 "unconnected-(U1-4_BCLK2-Pad6)")
			(pinfunction "4_BCLK2")
			(pintype "bidirectional+no_connect")
		)
		(pad "7" thru_hole circle
			(at -1.27 7.62 270)
			(size 1.6 1.6)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 42 "unconnected-(U1-5_IN2-Pad7)")
			(pinfunction "5_IN2")
			(pintype "bidirectional+no_connect")
		)
		(pad "8" thru_hole circle
			(at 1.27 7.62 270)
			(size 1.6 1.6)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 39 "Net-(U1-6_OUT1D)")
			(pinfunction "6_OUT1D")
			(pintype "bidirectional")
		)
		(pad "9" thru_hole circle
			(at 3.81 7.62 270)
			(size 1.6 1.6)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 27 "Net-(U1-7_RX2_OUT1A)")
			(pinfunction "7_RX2_OUT1A")
			(pintype "bidirectional")
		)
		(pad "10" thru_hole circle
			(at 6.35 7.62 270)
			(size 1.6 1.6)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 44 "Net-(J2-Pin_2)")
			(pinfunction "8_TX2_IN1")
			(pintype "bidirectional")
		)
		(pad "11" thru_hole circle
			(at 8.89 7.62 270)
			(size 1.6 1.6)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 8 "unconnected-(U1-9_OUT1C-Pad11)")
			(pinfunction "9_OUT1C")
			(pintype "bidirectional+no_connect")
		)
		(pad "12" thru_hole circle
			(at 11.43 7.62 270)
			(size 1.6 1.6)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 38 "unconnected-(U1-10_CS_MQSR-Pad12)")
			(pinfunction "10_CS_MQSR")
			(pintype "bidirectional+no_connect")
		)
		(pad "13" thru_hole circle
			(at 13.97 7.62 270)
			(size 1.6 1.6)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "Net-(U1-11_MOSI_CTX1)")
			(pinfunction "11_MOSI_CTX1")
			(pintype "bidirectional")
		)
		(pad "14" thru_hole circle
			(at 16.51 7.62 270)
			(size 1.6 1.6)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 16 "Net-(U1-12_MISO_MQSL)")
			(pinfunction "12_MISO_MQSL")
			(pintype "bidirectional")
		)
		(pad "15" thru_hole circle
			(at 16.51 5.08 270)
			(size 1.6 1.6)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 28 "unconnected-(U1-VBAT-Pad15)")
			(pinfunction "VBAT")
			(pintype "power_in+no_connect")
		)
		(pad "16" thru_hole circle
			(at 16.51 2.54 270)
			(size 1.6 1.6)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 7 "Net-(U2-VCC)")
			(pinfunction "3V3")
			(pintype "power_in")
		)
		(pad "17" thru_hole circle
			(at 16.51 0 270)
			(size 1.6 1.6)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GNDREF")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "18" thru_hole circle
			(at 16.51 -2.54 270)
			(size 1.6 1.6)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 24 "unconnected-(U1-PROGRAM-Pad18)")
			(pinfunction "PROGRAM")
			(pintype "input+no_connect")
		)
		(pad "19" thru_hole circle
			(at 16.51 -5.08 270)
			(size 1.6 1.6)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 9 "unconnected-(U1-ON_OFF-Pad19)")
			(pinfunction "ON_OFF")
			(pintype "input+no_connect")
		)
		(pad "20" thru_hole circle
			(at 16.51 -7.62 270)
			(size 1.6 1.6)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "Net-(U1-13_SCK_CRX1_LED)")
			(pinfunction "13_SCK_CRX1_LED")
			(pintype "bidirectional")
		)
		(pad "21" thru_hole circle
			(at 13.97 -7.62 270)
			(size 1.6 1.6)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 32 "unconnected-(U1-14_A0_TX3_SPDIF_OUT-Pad21)")
			(pinfunction "14_A0_TX3_SPDIF_OUT")
			(pintype "bidirectional+no_connect")
		)
		(pad "22" thru_hole circle
			(at 11.43 -7.62 270)
			(size 1.6 1.6)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 26 "unconnected-(U1-15_A1_RX3_SPDIF_IN-Pad22)")
			(pinfunction "15_A1_RX3_SPDIF_IN")
			(pintype "bidirectional+no_connect")
		)
		(pad "23" thru_hole circle
			(at 8.89 -7.62 270)
			(size 1.6 1.6)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 19 "unconnected-(U1-16_A2_RX4_SCL1-Pad23)")
			(pinfunction "16_A2_RX4_SCL1")
			(pintype "bidirectional+no_connect")
		)
		(pad "24" thru_hole circle
			(at 6.35 -7.62 270)
			(size 1.6 1.6)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 14 "unconnected-(U1-17_A3_TX4_SDA1-Pad24)")
			(pinfunction "17_A3_TX4_SDA1")
			(pintype "bidirectional+no_connect")
		)
		(pad "25" thru_hole circle
			(at 3.81 -7.62 270)
			(size 1.6 1.6)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 30 "unconnected-(U1-18_A4_SDA0-Pad25)")
			(pinfunction "18_A4_SDA0")
			(pintype "bidirectional+no_connect")
		)
		(pad "26" thru_hole circle
			(at 1.27 -7.62 270)
			(size 1.6 1.6)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 33 "unconnected-(U1-19_A5_SCL0-Pad26)")
			(pinfunction "19_A5_SCL0")
			(pintype "bidirectional+no_connect")
		)
		(pad "27" thru_hole circle
			(at -1.27 -7.62 270)
			(size 1.6 1.6)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 29 "unconnected-(U1-20_A6_TX5_LRCLK1-Pad27)")
			(pinfunction "20_A6_TX5_LRCLK1")
			(pintype "bidirectional+no_connect")
		)
		(pad "28" thru_hole circle
			(at -3.81 -7.62 270)
			(size 1.6 1.6)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 23 "unconnected-(U1-21_A7_RX5_BCLK1-Pad28)")
			(pinfunction "21_A7_RX5_BCLK1")
			(pintype "bidirectional+no_connect")
		)
		(pad "29" thru_hole circle
			(at -6.35 -7.62 270)
			(size 1.6 1.6)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 18 "unconnected-(U1-22_A8_CTX1-Pad29)")
			(pinfunction "22_A8_CTX1")
			(pintype "bidirectional+no_connect")
		)
		(pad "30" thru_hole circle
			(at -8.89 -7.62 270)
			(size 1.6 1.6)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 22 "unconnected-(U1-23_A9_CRX1_MCLK1-Pad30)")
			(pinfunction "23_A9_CRX1_MCLK1")
			(pintype "bidirectional+no_connect")
		)
		(pad "31" thru_hole circle
			(at -11.43 -7.62 270)
			(size 1.6 1.6)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 7 "Net-(U2-VCC)")
			(pinfunction "3V3")
			(pintype "power_out")
		)
		(pad "32" thru_hole circle
			(at -13.97 -7.62 270)
			(size 1.6 1.6)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GNDREF")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "33" thru_hole circle
			(at -16.51 -7.62 270)
			(size 1.6 1.6)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "Net-(J1-Pin_1)")
			(pinfunction "VIN")
			(pintype "power_in")
		)
		(pad "34" thru_hole circle
			(at -13.97 -5.08 270)
			(size 1.6 1.6)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 34 "unconnected-(U1-VUSB-Pad34)")
			(pinfunction "VUSB")
			(pintype "power_out+no_connect")
		)
		(pad "35" thru_hole circle
			(at 11.43 -5.08 270)
			(size 1.6 1.6)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 36 "unconnected-(U1-24_A10_TX6_SCL2-Pad35)")
			(pinfunction "24_A10_TX6_SCL2")
			(pintype "bidirectional+no_connect")
		)
		(pad "36" thru_hole circle
			(at 8.89 -5.08 270)
			(size 1.6 1.6)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 11 "unconnected-(U1-25_A11_RX6_SDA2-Pad36)")
			(pinfunction "25_A11_RX6_SDA2")
			(pintype "bidirectional+no_connect")
		)
		(pad "37" thru_hole circle
			(at 11.43 -2.54 270)
			(size 1.6 1.6)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 20 "unconnected-(U1-26_A12_MOSI1-Pad37)")
			(pinfunction "26_A12_MOSI1")
			(pintype "bidirectional+no_connect")
		)
		(pad "38" thru_hole circle
			(at 8.89 -2.54 270)
			(size 1.6 1.6)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 12 "unconnected-(U1-27_A13_SCK1-Pad38)")
			(pinfunction "27_A13_SCK1")
			(pintype "bidirectional+no_connect")
		)
		(pad "39" thru_hole circle
			(at 11.43 0 270)
			(size 1.6 1.6)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 15 "unconnected-(U1-28_RX7-Pad39)")
			(pinfunction "28_RX7")
			(pintype "bidirectional+no_connect")
		)
		(pad "40" thru_hole circle
			(at 8.89 0 270)
			(size 1.6 1.6)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 13 "unconnected-(U1-29_TX7-Pad40)")
			(pinfunction "29_TX7")
			(pintype "bidirectional+no_connect")
		)
		(pad "41" thru_hole circle
			(at 11.43 2.54 270)
			(size 1.6 1.6)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 35 "unconnected-(U1-30_CRX3-Pad41)")
			(pinfunction "30_CRX3")
			(pintype "bidirectional+no_connect")
		)
		(pad "42" thru_hole circle
			(at 8.89 2.54 270)
			(size 1.6 1.6)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 17 "unconnected-(U1-31_CTX3-Pad42)")
			(pinfunction "31_CTX3")
			(pintype "bidirectional+no_connect")
		)
		(pad "43" thru_hole circle
			(at 11.43 5.08 270)
			(size 1.6 1.6)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 41 "unconnected-(U1-32_OUT1B-Pad43)")
			(pinfunction "32_OUT1B")
			(pintype "bidirectional+no_connect")
		)
		(pad "44" thru_hole circle
			(at 8.89 5.08 270)
			(size 1.6 1.6)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 31 "unconnected-(U1-33_MCLK2-Pad44)")
			(pinfunction "33_MCLK2")
			(pintype "bidirectional+no_connect")
		)
		(embedded_fonts no)
		(model "${KICAD_USER_DIR}/teensy.pretty/Teensy_4.0_Assembly.STEP"
			(offset
				(xyz 33 9.5 -11)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 0 0)
			)
		)
	)
	(footprint "MountingHole:MountingHole_2.7mm_M2.5_DIN965_Pad_TopBottom"
		(layer "F.Cu")
		(at 106.68 109.22)
		(descr "Mounting Hole 2.7mm, M2.5, generated by kicad-footprint-generator mountinghole.py")
		(tags "mountinghole M2.5 DIN965")
		(property "Reference" "H3"
			(at 0 -3.3 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "MountingHole"
			(at 0 3.3 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Mounting Hole without connection"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "MountingHole*")
		(sheetname "/")
		(sheetfile "Teensy-RV-Leveling-Helper-Pair-LED-Controller.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 3.1 3.1)
			(drill 2.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(zone_connect 2)
		)
		(pad "1" connect circle
			(at 0 0)
			(size 4.7 4.7)
			(layers "F.Cu" "F.Mask")
			(zone_connect 2)
		)
		(pad "1" connect circle
			(at 0 0)
			(size 4.7 4.7)
			(layers "B.Cu" "B.Mask")
			(zone_connect 2)
		)
		(embedded_fonts no)
	)
	(gr_line
		(start 104.14 111.76)
		(end 104.14 53.34)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 147.32 111.76)
		(end 104.14 111.76)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 104.14 53.34)
		(end 147.32 53.34)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 147.32 53.34)
		(end 147.32 111.76)
		(layer "Edge.Cuts")
	)
	(gr_text "POWER\nIN/OUT"
		(at 139.683109 99.03991 0)
		(layer "F.SilkS")
	)
	(gr_text "Teensy LED Controller V1.1 20251208"
		(at 114.27801 109.168633 0)
		(layer "F.SilkS")
	)
	(gr_text "Teensy LED Controller V1.1 20251208"
		(at 142.223746 109.168633 0)
		(layer "B.SilkS")
	)
	(embedded_fonts no)
)
