(kicad_pcb
	(version 20260206)
	(generator "pcbnew")
	(generator_version "10.0")
	(general
		(thickness 1.6)
		(legacy_teardrops no)
	)
	(paper "A4")
	(layers
		(0 "F.Cu" signal)
		(4 "In1.Cu" signal)
		(6 "In2.Cu" signal)
		(2 "B.Cu" signal)
		(9 "F.Adhes" user "F.Adhesive")
		(11 "B.Adhes" user "B.Adhesive")
		(13 "F.Paste" user)
		(15 "B.Paste" user)
		(5 "F.SilkS" user "F.Silkscreen")
		(7 "B.SilkS" user "B.Silkscreen")
		(1 "F.Mask" user)
		(3 "B.Mask" user)
		(17 "Dwgs.User" user "User.Drawings")
		(19 "Cmts.User" user "User.Comments")
		(21 "Eco1.User" user "User.Eco1")
		(23 "Eco2.User" user "User.Eco2")
		(25 "Edge.Cuts" user)
		(27 "Margin" user)
		(31 "F.CrtYd" user "F.Courtyard")
		(29 "B.CrtYd" user "B.Courtyard")
		(35 "F.Fab" user)
		(33 "B.Fab" user)
		(39 "User.1" user)
		(41 "User.2" user)
		(43 "User.3" user)
		(45 "User.4" user)
	)
	(setup
		(stackup
			(layer "F.SilkS"
				(type "Top Silk Screen")
			)
			(layer "F.Paste"
				(type "Top Solder Paste")
			)
			(layer "F.Mask"
				(type "Top Solder Mask")
				(thickness 0.01)
			)
			(layer "F.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "dielectric 1"
				(type "prepreg")
				(thickness 0.1)
				(material "FR4")
				(epsilon_r 4.5)
				(loss_tangent 0.02)
			)
			(layer "In1.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "dielectric 2"
				(type "core")
				(thickness 1.24)
				(material "FR4")
				(epsilon_r 4.5)
				(loss_tangent 0.02)
			)
			(layer "In2.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "dielectric 3"
				(type "prepreg")
				(thickness 0.1)
				(material "FR4")
				(epsilon_r 4.5)
				(loss_tangent 0.02)
			)
			(layer "B.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "B.Mask"
				(type "Bottom Solder Mask")
				(thickness 0.01)
			)
			(layer "B.Paste"
				(type "Bottom Solder Paste")
			)
			(layer "B.SilkS"
				(type "Bottom Silk Screen")
			)
			(copper_finish "None")
			(dielectric_constraints no)
		)
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(tenting
			(front yes)
			(back yes)
		)
		(covering
			(front no)
			(back no)
		)
		(plugging
			(front no)
			(back no)
		)
		(capping no)
		(filling no)
		(pcbplotparams
			(layerselection 0x00000000_00000000_55555555_5755f5ff)
			(plot_on_all_layers_selection 0x00000000_00000000_00000000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12)
			(dashed_line_gap_ratio 3)
			(svgprecision 4)
			(plotframeref no)
			(mode 1)
			(useauxorigin no)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(pdf_metadata yes)
			(pdf_single_document no)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plot_black_and_white yes)
			(sketchpadsonfab no)
			(plotpadnumbers no)
			(hidednponfab no)
			(sketchdnponfab yes)
			(crossoutdnponfab yes)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 1)
			(scaleselection 1)
			(outputdirectory "")
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "F.Cu")
		(at 117.6 118.7 180)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "resistor")
		(property "Reference" "R4"
			(at -2.7 0 180)
			(layer "F.SilkS")
		)
		(property "Value" "10k"
			(at 0 1.65 180)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/esp/")
		(sheetfile "esp.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1" "2")
			)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 180)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net "+3.3V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 180)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net "Net-(U1-IO0)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "F.Cu")
		(at 123.4 101.2 180)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "resistor")
		(property "Reference" "R5"
			(at 2.4 0 90)
			(layer "F.SilkS")
		)
		(property "Value" "R"
			(at 0 1.65 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/esp/")
		(sheetfile "esp.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1" "2")
			)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 180)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net "Net-(D1-RK)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 180)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "F.Cu")
		(at 116.6525 115.8 -90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing)")
		(tags "capacitor")
		(property "Reference" "C1"
			(at -2.55 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "4.7uF"
			(at 0 1.68 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/power/")
		(sheetfile "mini.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1" "2")
			)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0 270)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "+5V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0 270)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "F.Cu")
		(at 124.1525 117)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing)")
		(tags "capacitor")
		(property "Reference" "C2"
			(at 2.8 0.1 0)
			(layer "F.SilkS")
		)
		(property "Value" "10uF"
			(at 0 1.68 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/power/")
		(sheetfile "mini.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1" "2")
			)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "+3.3V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "RVL:DBV0006A_N"
		(layer "F.Cu")
		(at 131.6 115.8 90)
		(tags "SN74LVC1T45DBVR ")
		(property "Reference" "U3"
			(at 0.2 -2.8 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "SN74LVC1T45DBVR"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://www.ti.com/lit/gpn/sn74lvc1t45"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "DBV0006A_N DBV0006A_M DBV0006A_L")
		(sheetname "/leds/")
		(sheetfile "leds.kicad_sch")
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.2 -0.950001 180)
			(size 0.650001 1.1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "+5V")
			(pinfunction "VCCA_1")
			(pintype "power_in")
		)
		(pad "2" smd rect
			(at -1.2 0 180)
			(size 0.650001 1.1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "GND")
			(pinfunction "GND_2")
			(pintype "power_in")
		)
		(pad "3" smd rect
			(at -1.2 0.949998 180)
			(size 0.650001 1.1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "Net-(U3-A)")
			(pinfunction "A_3")
			(pintype "bidirectional")
		)
		(pad "4" smd rect
			(at 1.2 0.949998 180)
			(size 0.650001 1.1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "LED_DATA")
			(pinfunction "B_4")
			(pintype "bidirectional")
		)
		(pad "5" smd rect
			(at 1.2 0 180)
			(size 0.650001 1.1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "GND")
			(pinfunction "DIR_5")
			(pintype "input")
		)
		(pad "6" smd rect
			(at 1.2 -0.950001 180)
			(size 0.650001 1.1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "+3.3V")
			(pinfunction "VCCB_6")
			(pintype "power_in")
		)
		(embedded_fonts no)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "F.Cu")
		(at 127 101.2)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "resistor")
		(property "Reference" "R6"
			(at 2.5 0 90)
			(layer "F.SilkS")
		)
		(property "Value" "R"
			(at 0 1.65 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/esp/")
		(sheetfile "esp.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1" "2")
			)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net "Net-(D1-GK)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "F.Cu")
		(at 131.4 105.1 -90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing)")
		(tags "capacitor")
		(property "Reference" "C3"
			(at 2.5 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "1uF"
			(at 0 1.68 270)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/esp/")
		(sheetfile "esp.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1" "2")
			)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 270)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0 270)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "Net-(U1-EN)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0 270)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "RVL:MF05A"
		(layer "F.Cu")
		(at 120 115.8)
		(tags "LM3671MF-3.3/NOPB ")
		(property "Reference" "U2"
			(at 0.75 0 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "LM3671MF-3.3/NOPB"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.ti.com/lit/gpn/lm3671"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "MF05A MF05A-M MF05A-L")
		(sheetname "/power/")
		(sheetfile "mini.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1" "2" "5" "4" "3")
			)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "*"
			(at -1.4732 -2.1209 0)
			(layer "F.SilkS")
		)
		(fp_text user "*"
			(at -1.4732 -2.1209 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(fp_text user "*"
			(at -1.4732 -2.1209 0)
			(layer "F.Fab")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.2192 -0.9525)
			(size 1.27 0.5588)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "+5V")
			(pinfunction "VIN_1")
			(pintype "input")
		)
		(pad "2" smd rect
			(at -1.2192 0)
			(size 1.27 0.5588)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "GND")
			(pinfunction "GND_2")
			(pintype "power_in")
		)
		(pad "3" smd rect
			(at -1.2192 0.9525)
			(size 1.27 0.5588)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "+5V")
			(pinfunction "EN_3")
			(pintype "unspecified")
		)
		(pad "4" smd rect
			(at 1.2192 0.9525)
			(size 1.27 0.5588)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "+3.3V")
			(pinfunction "FB_4")
			(pintype "input")
		)
		(pad "5" smd rect
			(at 1.2192 -0.9525)
			(size 1.27 0.5588)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "Net-(U2-SW)")
			(pinfunction "SW_5")
			(pintype "unspecified")
		)
		(embedded_fonts no)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "F.Cu")
		(at 131.7 119)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing)")
		(tags "capacitor")
		(property "Reference" "C4"
			(at 2.4 0 90)
			(layer "F.SilkS")
		)
		(property "Value" "0.1uF"
			(at 0 1.68 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/leds/")
		(sheetfile "leds.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1" "2")
			)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "+5V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "F.Cu")
		(at 131.1 101.4 90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing)")
		(tags "capacitor")
		(property "Reference" "C5"
			(at 0 2.4 90)
			(layer "F.SilkS")
		)
		(property "Value" "0.1uF"
			(at 0 1.68 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/esp/")
		(sheetfile "esp.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1" "2")
			)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0 90)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "+3.3V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0 90)
			(size 1 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "F.Cu")
		(at 128.6 118.3615 90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "resistor")
		(property "Reference" "R1"
			(at -0.8385 -2 180)
			(layer "F.SilkS")
		)
		(property "Value" "68"
			(at 0 1.65 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/leds/")
		(sheetfile "leds.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1" "2")
			)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 90)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net "Net-(J2-Pin_2)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 90)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net "Net-(U3-A)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "RVL:CONN_10118194-0001LF_AMP"
		(layer "F.Cu")
		(at 118.081402 124.1049 -90)
		(tags "10118194-0001LF ")
		(property "Reference" "J1"
			(at 0.1451 1.831402 270)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "10118194-0001LF"
			(at 0 -2.593599 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "10118194-0001LF"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "CONN_10118194-0001LF_AMP")
		(sheetname "/power/")
		(sheetfile "mini.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1" "2" "3" "4" "5")
			)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 -2.593599 270)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole oval
			(at -3.5 0.081402)
			(size 1.651 1.016)
			(drill oval 1.1938 0.5588)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole oval
			(at -2.5 -2.593599 270)
			(size 1.2954 1.016)
			(drill oval 0.889 0.6096)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole oval
			(at 2.5 -2.593599 270)
			(size 1.2954 1.016)
			(drill oval 0.889 0.6096)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole oval
			(at 3.500001 0.081402)
			(size 1.651 1.016)
			(drill oval 1.1938 0.5588)
			(layers "*.Cu" "*.Mask")
		)
		(pad "1" smd rect
			(at -1.3 -2.593599 270)
			(size 0.4572 1.3462)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "+5V")
			(pinfunction "1_1")
			(pintype "unspecified")
		)
		(pad "2" smd rect
			(at -0.649999 -2.593599 270)
			(size 0.4572 1.3462)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "unconnected-(J1-Pad2)")
			(pinfunction "2_2")
			(pintype "unspecified+no_connect")
		)
		(pad "3" smd rect
			(at 0 -2.593599 270)
			(size 0.4572 1.3462)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "unconnected-(J1-Pad3)")
			(pinfunction "3_3")
			(pintype "unspecified+no_connect")
		)
		(pad "4" smd rect
			(at 0.649999 -2.593599 270)
			(size 0.4572 1.3462)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "unconnected-(J1-Pad4)")
			(pinfunction "4_4")
			(pintype "unspecified+no_connect")
		)
		(pad "5" smd rect
			(at 1.3 -2.593599 270)
			(size 0.4572 1.3462)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "GND")
			(pinfunction "5_5")
			(pintype "unspecified")
		)
		(pad "10" smd rect
			(at -1.000001 0.081402 270)
			(size 1.4986 1.651)
			(layers "F.Cu" "F.Mask" "F.Paste")
		)
		(pad "11" smd rect
			(at 1.000001 0.081402 270)
			(size 1.4986 1.651)
			(layers "F.Cu" "F.Mask" "F.Paste")
		)
		(embedded_fonts no)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "F.Cu")
		(at 123.1 108.4875 -90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "resistor")
		(property "Reference" "R7"
			(at 1.4125 1.5 90)
			(layer "F.SilkS")
		)
		(property "Value" "R"
			(at 0 1.65 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/esp/")
		(sheetfile "esp.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1" "2")
			)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 270)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net "Net-(D1-BK)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 270)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric"
		(layer "F.Cu")
		(at 129.2 105.1 90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "resistor")
		(property "Reference" "R3"
			(at -2.5 0 180)
			(layer "F.SilkS")
		)
		(property "Value" "12k"
			(at 0 1.65 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/esp/")
		(sheetfile "esp.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1" "2")
			)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9125 0 90)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net "+3.3V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.9125 0 90)
			(size 1.025 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.243902)
			(net "Net-(U1-EN)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "RVL:LED_RGB_PLCC-6"
		(layer "F.Cu")
		(at 125.3 104.5)
		(descr "RGB LED PLCC-6")
		(tags "RGB LED PLCC-6")
		(property "Reference" "D1"
			(at 0 0 270)
			(layer "F.SilkS")
		)
		(property "Value" "LED_RGB"
			(at 0 2.8 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "RGB LED, 6 pin package"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "LED* LED_SMD:* LED_THT:*")
		(sheetname "/esp/")
		(sheetfile "esp.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "2" "4" "6" "1" "3" "5")
			)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(pad "1" smd rect
			(at -1.55 -1.1 90)
			(size 0.7 1.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "Net-(D1-RA)")
			(pinfunction "RA_1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.55 -1.1 90)
			(size 0.7 1.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "Net-(D1-RK)")
			(pinfunction "RK_2")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at -1.55 0 90)
			(size 0.7 1.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "Net-(D1-GA)")
			(pinfunction "GA_3")
			(pintype "passive")
		)
		(pad "4" smd rect
			(at 1.55 0 90)
			(size 0.7 1.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "Net-(D1-GK)")
			(pinfunction "GK_4")
			(pintype "passive")
		)
		(pad "5" smd rect
			(at -1.55 1.1 90)
			(size 0.7 1.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "Net-(D1-BA)")
			(pinfunction "BA_5")
			(pintype "passive")
		)
		(pad "6" smd rect
			(at 1.55 1.1 90)
			(size 0.7 1.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "Net-(D1-BK)")
			(pinfunction "BK_6")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/LED_SMD.3dshapes/LED_RGB_PLCC-6.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Inductor_SMD:L_0805_2012Metric"
		(layer "F.Cu")
		(at 124.1525 114.9)
		(descr "Inductor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 80, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "inductor")
		(property "Reference" "L1"
			(at 2.75 0.1 180)
			(layer "F.SilkS")
		)
		(property "Value" "2.2uH"
			(at 0 1.55 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Inductor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Choke_* *Coil* Inductor_* L_*")
		(sheetname "/power/")
		(sheetfile "mini.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1" "2")
			)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.0625 0)
			(size 0.875 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "Net-(U2-SW)")
			(pinfunction "1_1")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.0625 0)
			(size 0.875 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "+3.3V")
			(pinfunction "2_2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_0805_2012Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TerminalBlock_4Ucon:TerminalBlock_4Ucon_1x03_P3.50mm_Horizontal"
		(layer "F.Cu")
		(at 124.75 124.1675)
		(descr "Terminal Block 4Ucon ItemNo. 20193, 3 pins, pitch 3.5mm, size 11.2x7mm, drill diameter 1.2mm, pad diameter 2.4mm, http://www.4uconnector.com/online/object/4udrawing/20193.pdf")
		(tags "THT Terminal Block 4Ucon ItemNo. 20193 pitch 3.5mm size 11.2x7mm drill 1.2mm pad 2.4mm")
		(property "Reference" "J2"
			(at 3.5 3 0)
			(layer "F.SilkS")
		)
		(property "Value" "Screw_Terminal_01x03"
			(at 3.5 4.72 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic screw terminal, single row, 01x03, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TerminalBlock*:*")
		(sheetname "/leds/")
		(sheetfile "leds.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1" "2" "3")
			)
		)
		(attr through_hole)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 3.5 2.9 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole roundrect
			(at 0 0)
			(size 2.4 2.4)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.104167)
			(net "+5V")
			(pinfunction "Pin_1_1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 3.5 0)
			(size 2.4 2.4)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "Net-(J2-Pin_2)")
			(pinfunction "Pin_2_2")
			(pintype "passive")
		)
		(pad "3" thru_hole circle
			(at 7 0)
			(size 2.4 2.4)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "GND")
			(pinfunction "Pin_3_3")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/TerminalBlock_4Ucon.3dshapes/TerminalBlock_4Ucon_1x03_P3.50mm_Horizontal.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "RVL:CONN_532610001-SD_05_MOL"
		(layer "F.Cu")
		(at 117.5 106 90)
		(tags "532610571 ")
		(property "Reference" "J3"
			(at 0 0.794199 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "532610571"
			(at 0 2.9045 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://www.molex.com/en-us/products/part-detail-pdf/532610571?display=pdf"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "CONN_532610001-SD_05_MOL")
		(sheetname "/esp/")
		(sheetfile "esp.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1" "2" "3" "4" "5")
			)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 2.9045 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at 2.5 2.9045 90)
			(size 0.8128 1.7018)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "Net-(U1-EN)")
			(pinfunction "1_1")
			(pintype "unspecified")
		)
		(pad "2" smd rect
			(at 1.25 2.9045 90)
			(size 0.8128 1.7018)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "Net-(U1-IO0)")
			(pinfunction "2_2")
			(pintype "unspecified")
		)
		(pad "3" smd rect
			(at 0 2.9045 90)
			(size 0.8128 1.7018)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "Net-(U1-TXD0{slash}IO1)")
			(pinfunction "3_3")
			(pintype "unspecified")
		)
		(pad "4" smd rect
			(at -1.25 2.9045 90)
			(size 0.8128 1.7018)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "Net-(U1-RXD0{slash}IO3)")
			(pinfunction "4_4")
			(pintype "unspecified")
		)
		(pad "5" smd rect
			(at -2.5 2.9045 90)
			(size 0.8128 1.7018)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "GND")
			(pinfunction "5_5")
			(pintype "unspecified")
		)
		(pad "6" smd rect
			(at -5.05 0.004501 90)
			(size 2.2098 3.0988)
			(layers "F.Cu" "F.Mask" "F.Paste")
		)
		(pad "7" smd rect
			(at 5.05 0.004501 90)
			(size 2.2098 3.0988)
			(layers "F.Cu" "F.Mask" "F.Paste")
		)
		(zone
			(layer "F.Cu")
			(hatch full 0.508)
			(connect_pads
				(clearance 0)
			)
			(min_thickness 0.254)
			(keepout
				(tracks not_allowed)
				(vias not_allowed)
				(pads allowed)
				(copperpour not_allowed)
				(footprints allowed)
			)
			(placement
				(enabled no)
				(sheetname "")
			)
			(fill
				(thermal_gap 0.508)
				(thermal_bridge_width 0.508)
				(island_removal_mode 0)
			)
			(polygon
				(pts
					(xy 115.002799 102.995299) (xy 116.806199 102.995299) (xy 116.806199 102.004699) (xy 115.002799 102.004699)
				)
			)
		)
		(zone
			(layer "F.Cu")
			(hatch full 0.508)
			(connect_pads
				(clearance 0)
			)
			(min_thickness 0.254)
			(keepout
				(tracks not_allowed)
				(vias not_allowed)
				(pads allowed)
				(copperpour not_allowed)
				(footprints allowed)
			)
			(placement
				(enabled no)
				(sheetname "")
			)
			(fill
				(thermal_gap 0.508)
				(thermal_bridge_width 0.508)
				(island_removal_mode 0)
			)
			(polygon
				(pts
					(xy 115.002799 109.995301) (xy 116.806199 109.995301) (xy 116.806199 109.004701) (xy 115.002799 109.004701)
				)
			)
		)
		(zone
			(layer "F.Cu")
			(hatch full 0.508)
			(connect_pads
				(clearance 0)
			)
			(min_thickness 0.254)
			(keepout
				(tracks not_allowed)
				(vias not_allowed)
				(pads allowed)
				(copperpour not_allowed)
				(footprints allowed)
			)
			(placement
				(enabled no)
				(sheetname "")
			)
			(fill
				(thermal_gap 0.508)
				(thermal_bridge_width 0.508)
				(island_removal_mode 0)
			)
			(polygon
				(pts
					(xy 118.2028 102.995299) (xy 120.0062 102.995299) (xy 120.0062 102.004699) (xy 118.2028 102.004699)
				)
			)
		)
		(zone
			(layer "F.Cu")
			(hatch full 0.508)
			(connect_pads
				(clearance 0)
			)
			(min_thickness 0.254)
			(keepout
				(tracks not_allowed)
				(vias not_allowed)
				(pads allowed)
				(copperpour not_allowed)
				(footprints allowed)
			)
			(placement
				(enabled no)
				(sheetname "")
			)
			(fill
				(thermal_gap 0.508)
				(thermal_bridge_width 0.508)
				(island_removal_mode 0)
			)
			(polygon
				(pts
					(xy 118.2028 109.995301) (xy 120.0062 109.995301) (xy 120.0062 109.004701) (xy 118.2028 109.004701)
				)
			)
		)
		(embedded_fonts no)
	)
	(footprint "RF_Module:ESP32-WROOM-32E"
		(layer "B.Cu")
		(at 124.775 106.025 180)
		(descr "2.4 GHz Wi­-Fi and Bluetooth 5 (LE) module: https://www.espressif.com/sites/default/files/documentation/esp32-wroom-32e_esp32-wroom-32ue_datasheet_en.pdf")
		(tags "Bluetooth WiFi Wi-Fi ESP32 WROOM Xtensa LX6")
		(property "Reference" "U1"
			(at -0.825 1.025 180)
			(layer "B.SilkS")
		)
		(property "Value" "ESP32-WROOM-32E"
			(at 0 -14.5 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.espressif.com/sites/default/files/documentation/esp32-wroom-32e_esp32-wroom-32ue_datasheet_en.pdf"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "RF Module, ESP32-D0WD-V3 SoC, without PSRAM, Wi-Fi 802.11b/g/n, Bluetooth, BLE, 32-bit, 2.7-3.6V, onboard antenna, SMD"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "ESP32?WROOM?32E*")
		(sheetname "/esp/")
		(sheetfile "esp.kicad_sch")
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 1 0)
			(layer "B.Fab")
		)
		(pad "1" smd rect
			(at -8.75 5.26 180)
			(size 1.5 0.9)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net "GND")
			(pinfunction "GND_1")
			(pintype "power_in")
		)
		(pad "2" smd rect
			(at -8.75 3.99 180)
			(size 1.5 0.9)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net "+3.3V")
			(pinfunction "VDD_2")
			(pintype "power_in")
		)
		(pad "3" smd rect
			(at -8.75 2.72 180)
			(size 1.5 0.9)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net "Net-(U1-EN)")
			(pinfunction "EN_3")
			(pintype "input")
		)
		(pad "4" smd rect
			(at -8.75 1.45 180)
			(size 1.5 0.9)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net "unconnected-(U1-SENSOR_VP-Pad4)")
			(pinfunction "SENSOR_VP_4")
			(pintype "input+no_connect")
		)
		(pad "5" smd rect
			(at -8.75 0.18 180)
			(size 1.5 0.9)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net "unconnected-(U1-SENSOR_VN-Pad5)")
			(pinfunction "SENSOR_VN_5")
			(pintype "input+no_connect")
		)
		(pad "6" smd rect
			(at -8.75 -1.09 180)
			(size 1.5 0.9)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net "unconnected-(U1-IO34-Pad6)")
			(pinfunction "IO34_6")
			(pintype "input+no_connect")
		)
		(pad "7" smd rect
			(at -8.75 -2.36 180)
			(size 1.5 0.9)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net "unconnected-(U1-IO35-Pad7)")
			(pinfunction "IO35_7")
			(pintype "input+no_connect")
		)
		(pad "8" smd rect
			(at -8.75 -3.63 180)
			(size 1.5 0.9)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net "unconnected-(U1-IO32-Pad8)")
			(pinfunction "IO32_8")
			(pintype "bidirectional+no_connect")
		)
		(pad "9" smd rect
			(at -8.75 -4.9 180)
			(size 1.5 0.9)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net "LED_DATA")
			(pinfunction "IO33_9")
			(pintype "bidirectional")
		)
		(pad "10" smd rect
			(at -8.75 -6.17 180)
			(size 1.5 0.9)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net "unconnected-(U1-IO25-Pad10)")
			(pinfunction "IO25_10")
			(pintype "bidirectional+no_connect")
		)
		(pad "11" smd rect
			(at -8.75 -7.44 180)
			(size 1.5 0.9)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net "unconnected-(U1-IO26-Pad11)")
			(pinfunction "IO26_11")
			(pintype "bidirectional+no_connect")
		)
		(pad "12" smd rect
			(at -8.75 -8.71 180)
			(size 1.5 0.9)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net "unconnected-(U1-IO27-Pad12)")
			(pinfunction "IO27_12")
			(pintype "bidirectional+no_connect")
		)
		(pad "13" smd rect
			(at -8.75 -9.98 180)
			(size 1.5 0.9)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net "unconnected-(U1-IO14-Pad13)")
			(pinfunction "IO14_13")
			(pintype "bidirectional+no_connect")
		)
		(pad "14" smd rect
			(at -8.75 -11.25 180)
			(size 1.5 0.9)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net "unconnected-(U1-IO12-Pad14)")
			(pinfunction "IO12_14")
			(pintype "bidirectional+no_connect")
		)
		(pad "15" smd rect
			(at -5.715 -12.5 90)
			(size 1.5 0.9)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net "GND")
			(pinfunction "GND_15")
			(pintype "power_in")
		)
		(pad "16" smd rect
			(at -4.445 -12.5 90)
			(size 1.5 0.9)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net "unconnected-(U1-IO13-Pad16)")
			(pinfunction "IO13_16")
			(pintype "bidirectional+no_connect")
		)
		(pad "17" smd rect
			(at -3.175 -12.5 90)
			(size 1.5 0.9)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net "unconnected-(U1-NC-Pad17)")
			(pinfunction "NC_17")
			(pintype "no_connect")
		)
		(pad "18" smd rect
			(at -1.905 -12.5 90)
			(size 1.5 0.9)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net "unconnected-(U1-NC-Pad18)")
			(pinfunction "NC_18")
			(pintype "no_connect")
		)
		(pad "19" smd rect
			(at -0.635 -12.5 90)
			(size 1.5 0.9)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net "unconnected-(U1-NC-Pad19)")
			(pinfunction "NC_19")
			(pintype "no_connect")
		)
		(pad "20" smd rect
			(at 0.635 -12.5 90)
			(size 1.5 0.9)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net "unconnected-(U1-NC-Pad20)")
			(pinfunction "NC_20")
			(pintype "no_connect")
		)
		(pad "21" smd rect
			(at 1.905 -12.5 90)
			(size 1.5 0.9)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net "unconnected-(U1-NC-Pad21)")
			(pinfunction "NC_21")
			(pintype "no_connect")
		)
		(pad "22" smd rect
			(at 3.175 -12.5 90)
			(size 1.5 0.9)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net "unconnected-(U1-NC-Pad22)")
			(pinfunction "NC_22")
			(pintype "no_connect")
		)
		(pad "23" smd rect
			(at 4.445 -12.5 90)
			(size 1.5 0.9)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net "unconnected-(U1-IO15-Pad23)")
			(pinfunction "IO15_23")
			(pintype "bidirectional+no_connect")
		)
		(pad "24" smd rect
			(at 5.715 -12.5 90)
			(size 1.5 0.9)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net "unconnected-(U1-IO2-Pad24)")
			(pinfunction "IO2_24")
			(pintype "bidirectional+no_connect")
		)
		(pad "25" smd rect
			(at 8.75 -11.25 180)
			(size 1.5 0.9)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net "Net-(U1-IO0)")
			(pinfunction "IO0_25")
			(pintype "bidirectional")
		)
		(pad "26" smd rect
			(at 8.75 -9.98 180)
			(size 1.5 0.9)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net "unconnected-(U1-IO4-Pad26)")
			(pinfunction "IO4_26")
			(pintype "bidirectional+no_connect")
		)
		(pad "27" smd rect
			(at 8.75 -8.71 180)
			(size 1.5 0.9)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net "unconnected-(U1-IO16-Pad27)")
			(pinfunction "IO16_27")
			(pintype "bidirectional+no_connect")
		)
		(pad "28" smd rect
			(at 8.75 -7.44 180)
			(size 1.5 0.9)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net "unconnected-(U1-IO17-Pad28)")
			(pinfunction "IO17_28")
			(pintype "bidirectional+no_connect")
		)
		(pad "29" smd rect
			(at 8.75 -6.17 180)
			(size 1.5 0.9)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net "unconnected-(U1-IO5-Pad29)")
			(pinfunction "IO5_29")
			(pintype "bidirectional+no_connect")
		)
		(pad "30" smd rect
			(at 8.75 -4.9 180)
			(size 1.5 0.9)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net "unconnected-(U1-IO18-Pad30)")
			(pinfunction "IO18_30")
			(pintype "bidirectional+no_connect")
		)
		(pad "31" smd rect
			(at 8.75 -3.63 180)
			(size 1.5 0.9)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net "unconnected-(U1-IO19-Pad31)")
			(pinfunction "IO19_31")
			(pintype "bidirectional+no_connect")
		)
		(pad "32" smd rect
			(at 8.75 -2.36 180)
			(size 1.5 0.9)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net "unconnected-(U1-NC-Pad32)")
			(pinfunction "NC_32")
			(pintype "no_connect")
		)
		(pad "33" smd rect
			(at 8.75 -1.09 180)
			(size 1.5 0.9)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net "Net-(D1-BA)")
			(pinfunction "IO21_33")
			(pintype "bidirectional")
		)
		(pad "34" smd rect
			(at 8.75 0.18 180)
			(size 1.5 0.9)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net "Net-(U1-RXD0{slash}IO3)")
			(pinfunction "RXD0/IO3_34")
			(pintype "bidirectional")
		)
		(pad "35" smd rect
			(at 8.75 1.45 180)
			(size 1.5 0.9)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net "Net-(U1-TXD0{slash}IO1)")
			(pinfunction "TXD0/IO1_35")
			(pintype "bidirectional")
		)
		(pad "36" smd rect
			(at 8.75 2.72 180)
			(size 1.5 0.9)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net "Net-(D1-GA)")
			(pinfunction "IO22_36")
			(pintype "bidirectional")
		)
		(pad "37" smd rect
			(at 8.75 3.99 180)
			(size 1.5 0.9)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net "Net-(D1-RA)")
			(pinfunction "IO23_37")
			(pintype "bidirectional")
		)
		(pad "38" smd rect
			(at 8.75 5.26 180)
			(size 1.5 0.9)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net "GND")
			(pinfunction "GND_38")
			(pintype "power_in")
		)
		(pad "39" smd rect
			(at -2.9 -3.86 180)
			(size 0.9 0.9)
			(property pad_prop_heatsink)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net "GND")
			(pinfunction "GND_39")
			(pintype "power_in")
			(zone_connect 2)
		)
		(pad "39" thru_hole circle
			(at -2.9 -3.16 180)
			(size 0.654 0.654)
			(drill 0.254)
			(property pad_prop_heatsink)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "GND")
			(pinfunction "GND_39")
			(pintype "power_in")
			(zone_connect 2)
		)
		(pad "39" smd rect
			(at -2.9 -2.46 180)
			(size 0.9 0.9)
			(property pad_prop_heatsink)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net "GND")
			(pinfunction "GND_39")
			(pintype "power_in")
			(zone_connect 2)
		)
		(pad "39" thru_hole circle
			(at -2.9 -1.76 180)
			(size 0.654 0.654)
			(drill 0.254)
			(property pad_prop_heatsink)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "GND")
			(pinfunction "GND_39")
			(pintype "power_in")
			(zone_connect 2)
		)
		(pad "39" smd rect
			(at -2.9 -1.06 180)
			(size 0.9 0.9)
			(property pad_prop_heatsink)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net "GND")
			(pinfunction "GND_39")
			(pintype "power_in")
			(zone_connect 2)
		)
		(pad "39" thru_hole circle
			(at -2.2 -3.86 180)
			(size 0.6 0.6)
			(drill 0.254)
			(property pad_prop_heatsink)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "GND")
			(pinfunction "GND_39")
			(pintype "power_in")
			(zone_connect 2)
		)
		(pad "39" thru_hole circle
			(at -2.2 -2.46 180)
			(size 0.654 0.654)
			(drill 0.254)
			(property pad_prop_heatsink)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "GND")
			(pinfunction "GND_39")
			(pintype "power_in")
			(zone_connect 2)
		)
		(pad "39" thru_hole circle
			(at -2.2 -1.06)
			(size 0.654 0.654)
			(drill 0.254)
			(property pad_prop_heatsink)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "GND")
			(pinfunction "GND_39")
			(pintype "power_in")
			(zone_connect 2)
		)
		(pad "39" smd rect
			(at -1.5 -3.86 180)
			(size 0.9 0.9)
			(property pad_prop_heatsink)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net "GND")
			(pinfunction "GND_39")
			(pintype "power_in")
			(zone_connect 2)
		)
		(pad "39" thru_hole circle
			(at -1.5 -3.16 90)
			(size 0.654 0.654)
			(drill 0.254)
			(property pad_prop_heatsink)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "GND")
			(pinfunction "GND_39")
			(pintype "power_in")
			(zone_connect 2)
		)
		(pad "39" smd rect
			(at -1.5 -2.46 180)
			(size 0.9 0.9)
			(property pad_prop_heatsink)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net "GND")
			(pinfunction "GND_39")
			(pintype "power_in")
			(zone_connect 2)
		)
		(pad "39" thru_hole circle
			(at -1.5 -1.76 180)
			(size 0.654 0.654)
			(drill 0.254)
			(property pad_prop_heatsink)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "GND")
			(pinfunction "GND_39")
			(pintype "power_in")
			(zone_connect 2)
		)
		(pad "39" smd rect
			(at -1.5 -1.06 180)
			(size 0.9 0.9)
			(property pad_prop_heatsink)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net "GND")
			(pinfunction "GND_39")
			(pintype "power_in")
			(zone_connect 2)
		)
		(pad "39" thru_hole circle
			(at -0.8 -3.86 90)
			(size 0.654 0.654)
			(drill 0.254)
			(property pad_prop_heatsink)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "GND")
			(pinfunction "GND_39")
			(pintype "power_in")
			(zone_connect 2)
		)
		(pad "39" thru_hole circle
			(at -0.8 -2.46 90)
			(size 0.654 0.654)
			(drill 0.254)
			(property pad_prop_heatsink)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "GND")
			(pinfunction "GND_39")
			(pintype "power_in")
			(zone_connect 2)
		)
		(pad "39" thru_hole circle
			(at -0.8 -1.06 90)
			(size 0.654 0.654)
			(drill 0.254)
			(property pad_prop_heatsink)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "GND")
			(pinfunction "GND_39")
			(pintype "power_in")
			(zone_connect 2)
		)
		(pad "39" smd rect
			(at -0.1 -3.86 180)
			(size 0.9 0.9)
			(property pad_prop_heatsink)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net "GND")
			(pinfunction "GND_39")
			(pintype "power_in")
			(zone_connect 2)
		)
		(pad "39" thru_hole circle
			(at -0.1 -3.16 90)
			(size 0.654 0.654)
			(drill 0.254)
			(property pad_prop_heatsink)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "GND")
			(pinfunction "GND_39")
			(pintype "power_in")
			(zone_connect 2)
		)
		(pad "39" smd rect
			(at -0.1 -2.46 180)
			(size 0.9 0.9)
			(property pad_prop_heatsink)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net "GND")
			(pinfunction "GND_39")
			(pintype "power_in")
			(zone_connect 2)
		)
		(pad "39" thru_hole circle
			(at -0.1 -1.76 180)
			(size 0.654 0.654)
			(drill 0.254)
			(property pad_prop_heatsink)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "GND")
			(pinfunction "GND_39")
			(pintype "power_in")
			(zone_connect 2)
		)
		(pad "39" smd rect
			(at -0.1 -1.06 180)
			(size 0.9 0.9)
			(property pad_prop_heatsink)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net "GND")
			(pinfunction "GND_39")
			(pintype "power_in")
			(zone_connect 2)
		)
		(zone
			(layers "F.Cu" "B.Cu" "In1.Cu" "In2.Cu")
			(hatch full 0.5)
			(connect_pads
				(clearance 0)
			)
			(min_thickness 0.25)
			(keepout
				(tracks not_allowed)
				(vias not_allowed)
				(pads not_allowed)
				(copperpour not_allowed)
				(footprints not_allowed)
			)
			(placement
				(enabled no)
				(sheetname "")
			)
			(fill
				(thermal_gap 0.5)
				(thermal_bridge_width 0.5)
				(island_removal_mode 0)
			)
			(polygon
				(pts
					(xy 148.775 78.275) (xy 100.775 78.275) (xy 100.775 99.465) (xy 148.775 99.465)
				)
			)
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/RF_Module.3dshapes/ESP32-WROOM-32E.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(gr_line
		(start 114.7 99.3)
		(end 114.7 128.7)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 114.7 128.7)
		(end 134.8 128.7)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 134.8 99.3)
		(end 114.7 99.3)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 134.8 128.7)
		(end 134.8 99.3)
		(layer "Edge.Cuts")
	)
	(gr_text "RVL Mini v1.0\n© Bryan Hughes"
		(at 121.9 113.3 0)
		(layer "F.SilkS")
	)
	(zone
		(net "GND")
		(layer "In1.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 0)
		)
		(polygon
			(pts
				(xy 114 130) (xy 136 130) (xy 136 98.3) (xy 114 98.3)
			)
		)
	)
	(zone
		(net "+3.3V")
		(layer "In2.Cu")
		(hatch edge 0.5)
		(priority 2)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 0)
		)
		(polygon
			(pts
				(xy 114 113.3) (xy 121.4 113.3) (xy 121.4 118.9) (xy 136 118.9) (xy 136 98.3) (xy 114 98.3)
			)
		)
	)
	(zone
		(net "+5V")
		(layer "In2.Cu")
		(hatch edge 0.5)
		(priority 1)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 0)
		)
		(polygon
			(pts
				(xy 114 130) (xy 114 114) (xy 120.7 114) (xy 120.7 119.6) (xy 136 119.6) (xy 136 130)
			)
		)
	)
	(embedded_fonts no)
)
