(kicad_pcb
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(general
		(thickness 1.5422)
		(legacy_teardrops no)
	)
	(paper "A4")
	(layers
		(0 "F.Cu" signal)
		(4 "In1.Cu" power)
		(6 "In2.Cu" power)
		(2 "B.Cu" signal)
		(9 "F.Adhes" user "F.Adhesive")
		(11 "B.Adhes" user "B.Adhesive")
		(13 "F.Paste" user)
		(15 "B.Paste" user)
		(5 "F.SilkS" user "F.Silkscreen")
		(7 "B.SilkS" user "B.Silkscreen")
		(1 "F.Mask" user)
		(3 "B.Mask" user)
		(17 "Dwgs.User" user "User.Drawings")
		(19 "Cmts.User" user "User.Comments")
		(21 "Eco1.User" user "User.Eco1")
		(23 "Eco2.User" user "User.Eco2")
		(25 "Edge.Cuts" user)
		(27 "Margin" user)
		(31 "F.CrtYd" user "F.Courtyard")
		(29 "B.CrtYd" user "B.Courtyard")
		(35 "F.Fab" user "Mechanical 12")
		(33 "B.Fab" user "Top Assembly")
		(39 "User.1" user "Top 3D Body")
		(41 "User.2" user "Top Designator")
		(43 "User.3" user "Route Tool Path")
		(45 "User.4" user "Board")
		(47 "User.5" user "Mechanical 5")
		(49 "User.6" user "Bottom Courtyard")
		(51 "User.7" user "Mechanical 7")
		(53 "User.8" user "Bottom 3D Body")
		(55 "User.9" user "Mechanical 9")
		(57 "User.10" user "Bottom Assembly")
		(59 "User.11" user "Mechanical 11")
		(61 "User.12" user "Mechanical 14")
		(63 "User.13" user "Top Courtyard")
		(65 "User.14" user "Mechanical 16")
	)
	(setup
		(stackup
			(layer "F.SilkS"
				(type "Top Silk Screen")
				(color "White")
				(material "Liquid Photo")
			)
			(layer "F.Paste"
				(type "Top Solder Paste")
			)
			(layer "F.Mask"
				(type "Top Solder Mask")
				(color "Purple")
				(thickness 0.0152)
				(material "SMOBC")
				(epsilon_r 3.9)
				(loss_tangent 0.033)
			)
			(layer "F.Cu"
				(type "copper")
				(thickness 0.0432)
			)
			(layer "dielectric 1"
				(type "prepreg")
				(color "FR4 natural")
				(thickness 0.1999 locked)
				(material "FR408-HR")
				(epsilon_r 3.61)
				(loss_tangent 0.0091)
			)
			(layer "In1.Cu"
				(type "copper")
				(thickness 0.0175)
			)
			(layer "dielectric 2"
				(type "core")
				(color "FR4 natural")
				(thickness 0.9906 locked)
				(material "FR408-HR")
				(epsilon_r 3.87)
				(loss_tangent 0.0091)
			)
			(layer "In2.Cu"
				(type "copper")
				(thickness 0.0175)
			)
			(layer "dielectric 3"
				(type "prepreg")
				(color "FR4 natural")
				(thickness 0.1999 locked)
				(material "FR408-HR")
				(epsilon_r 3.61)
				(loss_tangent 0.0091)
			)
			(layer "B.Cu"
				(type "copper")
				(thickness 0.0432)
			)
			(layer "B.Mask"
				(type "Bottom Solder Mask")
				(color "Purple")
				(thickness 0.0152)
				(material "SMOBC")
				(epsilon_r 3.9)
				(loss_tangent 0.033)
			)
			(layer "B.Paste"
				(type "Bottom Solder Paste")
			)
			(layer "B.SilkS"
				(type "Bottom Silk Screen")
				(color "White")
				(material "Liquid Photo")
			)
			(copper_finish "ENIG")
			(dielectric_constraints yes)
		)
		(pad_to_mask_clearance 0.0762)
		(solder_mask_min_width 0.1016)
		(allow_soldermask_bridges_in_footprints no)
		(tenting front back)
		(aux_axis_origin 127.20111 115.16359)
		(grid_origin 127.20111 115.16359)
		(pcbplotparams
			(layerselection 0x00000000_00000000_55555555_5755f5ff)
			(plot_on_all_layers_selection 0x00000000_00000000_00000000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 4)
			(plotframeref no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(pdf_metadata yes)
			(pdf_single_document no)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plot_black_and_white yes)
			(sketchpadsonfab no)
			(plotpadnumbers no)
			(hidednponfab no)
			(sketchdnponfab yes)
			(crossoutdnponfab yes)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 1)
			(scaleselection 1)
			(outputdirectory "")
		)
	)
	(net 0 "")
	(net 1 "GND")
	(net 2 "/EN")
	(net 3 "/BCLK")
	(net 4 "/RF_INT")
	(net 5 "/LRCLK")
	(net 6 "/BMS_INT")
	(net 7 "/HMI_INT")
	(net 8 "/SCL")
	(net 9 "/AUDIO_INT")
	(net 10 "/SDA")
	(net 11 "unconnected-(X6-Pad2)")
	(net 12 "unconnected-(X6-Pad6)")
	(net 13 "unconnected-(X7-Pad2)")
	(net 14 "unconnected-(X7-Pad4)")
	(net 15 "unconnected-(X7-Pad5)")
	(net 16 "unconnected-(X7-Pad6)")
	(net 17 "unconnected-(X7-Pad7)")
	(net 18 "unconnected-(X7-Pad8)")
	(net 19 "unconnected-(X7-Pad9)")
	(net 20 "unconnected-(X7-Pad16)")
	(net 21 "unconnected-(U5-DCD-Pad1)")
	(net 22 "unconnected-(U5-RI{slash}CLK-Pad2)")
	(net 23 "unconnected-(U5-NC-Pad10)")
	(net 24 "unconnected-(U5-SUSPEND-Pad12)")
	(net 25 "unconnected-(U5-CHREN-Pad13)")
	(net 26 "unconnected-(U5-CHR1-Pad14)")
	(net 27 "unconnected-(U5-CHR0-Pad15)")
	(net 28 "unconnected-(U5-GPIO.3{slash}WAKEUP-Pad16)")
	(net 29 "unconnected-(U5-GPIO.2{slash}RS485-Pad17)")
	(net 30 "unconnected-(U5-GPIO.6-Pad20)")
	(net 31 "unconnected-(U5-GPIO.5-Pad21)")
	(net 32 "unconnected-(U5-GPIO.4-Pad22)")
	(net 33 "unconnected-(U5-CTS-Pad23)")
	(net 34 "unconnected-(U5-DSR-Pad27)")
	(net 35 "unconnected-(U8-NC-Pad17)")
	(net 36 "unconnected-(U8-NC-Pad18)")
	(net 37 "unconnected-(U8-NC-Pad19)")
	(net 38 "unconnected-(U8-NC-Pad20)")
	(net 39 "unconnected-(U8-NC-Pad21)")
	(net 40 "unconnected-(U8-NC-Pad22)")
	(net 41 "Net-(Q1-B)")
	(net 42 "unconnected-(U8-NC-Pad27)")
	(net 43 "unconnected-(U8-NC-Pad28)")
	(net 44 "unconnected-(U8-NC-Pad32)")
	(net 45 "/HSPI_CS")
	(net 46 "/VSPI_CS")
	(net 47 "unconnected-(X5-Pad4)")
	(net 48 "unconnected-(X5-Pad5)")
	(net 49 "unconnected-(X5-Pad6)")
	(net 50 "unconnected-(X5-Pad8)")
	(net 51 "Net-(Q2-B)")
	(net 52 "/VSPI_MISO")
	(net 53 "/VSPI_SCLK")
	(net 54 "/X_INT")
	(net 55 "/VSPI_GDO2")
	(net 56 "/HSPI_DC")
	(net 57 "/HSPI_SCLK")
	(net 58 "/HSPI_MOSI")
	(net 59 "/VSPI_MOSI")
	(net 60 "/VSPI_GDO0")
	(net 61 "/D-")
	(net 62 "/D+")
	(net 63 "Net-(JP2-A)")
	(net 64 "/DIN")
	(net 65 "/DOUT")
	(net 66 "Net-(D1-A)")
	(net 67 "/IO0")
	(net 68 "Net-(D2-K)")
	(net 69 "Net-(D2-A)")
	(net 70 "Net-(D3-K)")
	(net 71 "Net-(D3-A)")
	(net 72 "/CC1200_RST")
	(net 73 "RXD0")
	(net 74 "RXD")
	(net 75 "Net-(J3-Pin_1)")
	(net 76 "Net-(J4-Pin_1)")
	(net 77 "/RTS")
	(net 78 "/DTR")
	(net 79 "Net-(U5-SUSPENDb)")
	(net 80 "Net-(U5-RSTb)")
	(net 81 "Net-(U8-RXD0)")
	(net 82 "Net-(U8-TXD0)")
	(net 83 "/AMP_SD")
	(net 84 "+3.3V")
	(net 85 "/TFT_RST")
	(net 86 "/CARD_CS")
	(net 87 "/BAT_LOW")
	(net 88 "Net-(J3-Pin_2)")
	(net 89 "Net-(J3-Pin_3)")
	(net 90 "Net-(J4-Pin_8)")
	(net 91 "Net-(J4-Pin_5)")
	(net 92 "Net-(J4-Pin_7)")
	(net 93 "Net-(J4-Pin_3)")
	(net 94 "Net-(J4-Pin_6)")
	(net 95 "Net-(J4-Pin_4)")
	(net 96 "Net-(J4-Pin_2)")
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 203.2 105.5 180)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R3"
			(at -0.025 -1.3 0)
			(layer "F.SilkS")
		)
		(property "Value" "10k"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "testbed-mcu copy.kicad_sch")
		(attr smd)
		(pad "1" smd roundrect
			(at -0.825 0 180)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 84 "+3.3V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0 180)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 45 "/HSPI_CS")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "F.Cu")
		(at 208.400882 93.989596)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP2"
			(at -2.360435 -0.001559 0)
			(layer "F.SilkS")
		)
		(property "Value" "TestPoint"
			(at 0 1.55 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/")
		(sheetfile "testbed-mcu copy.kicad_sch")
		(attr exclude_from_pos_files)
		(fp_text user "${REFERENCE}"
			(at 0 -1.45 0)
			(layer "F.Fab")
		)
		(pad "1" smd circle
			(at 0 0)
			(size 1 1)
			(layers "F.Cu" "F.Mask")
			(net 84 "+3.3V")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "LOGO"
		(layer "F.Cu")
		(at 150.85 110.5 -90)
		(property "Reference" "G***"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "LOGO"
			(at 0.75 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(attr board_only exclude_from_pos_files exclude_from_bom)
		(embedded_fonts no)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "F.Cu")
		(at 169.1 131.3)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP7"
			(at 0 -1.448 0)
			(layer "F.SilkS")
		)
		(property "Value" "TestPoint"
			(at 0 1.55 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/")
		(sheetfile "testbed-mcu copy.kicad_sch")
		(attr exclude_from_pos_files)
		(pad "1" smd circle
			(at 0 0)
			(size 1 1)
			(layers "F.Cu" "F.Mask")
			(net 84 "+3.3V")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 176.976 87.6 -90)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C2"
			(at 2.1 0.276 0)
			(layer "F.SilkS")
		)
		(property "Value" "10u"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "testbed-mcu copy.kicad_sch")
		(attr smd)
		(pad "1" smd roundrect
			(at -0.775 0 270)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 84 "+3.3V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 270)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "F.Cu")
		(at 176.98511 111.09959)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP3"
			(at 0 -1.448 0)
			(layer "F.SilkS")
		)
		(property "Value" "TestPoint"
			(at 0 1.55 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/")
		(sheetfile "testbed-mcu copy.kicad_sch")
		(attr exclude_from_pos_files)
		(fp_text user "${REFERENCE}"
			(at 0 -1.45 0)
			(layer "F.Fab")
		)
		(pad "1" smd circle
			(at 0 0)
			(size 1 1)
			(layers "F.Cu" "F.Mask")
			(net 84 "+3.3V")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "LOGO"
		(layer "F.Cu")
		(at 187.45 87.3)
		(property "Reference" "G***"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "LOGO"
			(at 0.75 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr board_only exclude_from_pos_files exclude_from_bom)
		(embedded_fonts no)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 197.3 121.095387 180)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R13"
			(at -2.6111 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "10k"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "testbed-mcu copy.kicad_sch")
		(attr smd)
		(pad "1" smd roundrect
			(at -0.825 0 180)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 77 "/RTS")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0 180)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 51 "Net-(Q2-B)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "capstone-project:Adafruit EYESPI FPC Connector"
		(layer "F.Cu")
		(at 152.973601 94.113826 -90)
		(descr "WR-FPC SMT ZIF Horizontal Hinge Type")
		(tags "EYESPI, FPC")
		(property "Reference" "X8"
			(at 7.874 2.032 90)
			(layer "F.SilkS")
		)
		(property "Value" "EYESPI"
			(at 0 4.064 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://www.we-online.com/components/products/datasheet/687118149022.pdf"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "WR-FPC SMT ZIF Horizontal Hinge Type"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Assignment" "CC1200_VSPI"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "testbed-mcu copy.kicad_sch")
		(attr smd allow_soldermask_bridges)
		(pad "1" smd rect
			(at -4.25 -3.35 270)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 84 "+3.3V")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd rect
			(at -3.75 -3.35 270)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 84 "+3.3V")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "3" smd rect
			(at -3.25 -3.35 270)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "4" smd rect
			(at -2.75 -3.35 270)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 53 "/VSPI_SCLK")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "5" smd rect
			(at -2.25 -3.35 270)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 59 "/VSPI_MOSI")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "6" smd rect
			(at -1.75 -3.35 270)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 52 "/VSPI_MISO")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "7" smd rect
			(at -1.25 -3.35 270)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 84 "+3.3V")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "8" smd rect
			(at -0.75 -3.35 270)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 72 "/CC1200_RST")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "9" smd rect
			(at -0.25 -3.35 270)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 46 "/VSPI_CS")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "10" smd rect
			(at 0.25 -3.35 270)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "11" smd rect
			(at 0.75 -3.35 270)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "12" smd rect
			(at 1.25 -3.35 270)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "13" smd rect
			(at 1.75 -3.35 270)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 8 "/SCL")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "14" smd rect
			(at 2.25 -3.35 270)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 10 "/SDA")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "15" smd rect
			(at 2.75 -3.35 270)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 4 "/RF_INT")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "16" smd rect
			(at 3.25 -3.35 270)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 84 "+3.3V")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "17" smd rect
			(at 3.75 -3.35 270)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 60 "/VSPI_GDO0")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "18" smd rect
			(at 4.25 -3.35 270)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 55 "/VSPI_GDO2")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "Z1" smd rect
			(at -6.05 -0.6 270)
			(size 2 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "Z2" smd rect
			(at 6.05 -0.6 270)
			(size 2 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
		(model "${KIPRJMOD}/capstone-project.pretty/3dmodels/687118149022+(rev1).step"
			(offset
				(xyz 0 0.5 1.15)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -0 -0 -0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 195.2 131.7 180)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R7"
			(at 0 -1.43 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "1k"
			(at 3.85 -0.3 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "testbed-mcu copy.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -1.35 0)
			(layer "F.SilkS")
		)
		(pad "1" smd roundrect
			(at -0.825 0 180)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 80 "Net-(U5-RSTb)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0 180)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 84 "+3.3V")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 198.3 131.7)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R6"
			(at -0.063278 -1.336064 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "10k"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "testbed-mcu copy.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 1.297173 0)
			(layer "F.SilkS")
		)
		(pad "1" smd roundrect
			(at -0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 79 "Net-(U5-SUSPENDb)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "LED_SMD:LED_0603_1608Metric"
		(layer "F.Cu")
		(at 167.55 87.325)
		(descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
		(tags "LED")
		(property "Reference" "D1"
			(at -0.25 1.375 0)
			(layer "F.SilkS")
		)
		(property "Value" "LTST-C190KRKT"
			(at 0 1.43 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://componentsearchengine.com/Datasheets/1/LTST-C190KRKT.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "LED,SMD,0603,Red,54mcd,130deg Lite-On LTST-C190KRKT Red LED, 631 nm, 1608 (0603), Rectangle Lens SMD Package"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Height" "0.8"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Part Number" "859-LTST-C190KRKT"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Price/Stock" "https://www.mouser.co.uk/ProductDetail/LITEON/LTST-C190KRKT?qs=kAD5fFa1n5VY3YYNWPC1Fg%3D%3D"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Name" "Lite-On"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Part_Number" "LTST-C190KRKT"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "testbed-mcu copy.kicad_sch")
		(attr smd)
		(pad "1" smd roundrect
			(at -0.7875 0)
			(size 0.875 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.7875 0)
			(size 0.875 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 66 "Net-(D1-A)")
			(pinfunction "A")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Button_Switch_SMD:SW_SPST_EVQP2_MiddlePushTravel_H2.5mm"
		(layer "F.Cu")
		(at 210.15 107.35 -90)
		(descr "Tactile switch, 4.7 x 3.5 mm, middle push travel, H2.5mm, https://industry.panasonic.com/ac/cdn/e/control/switch/light-touch/catalog/sw_lt_eng_4735s.pdf")
		(tags "SMD SMT SPST EVQP2")
		(property "Reference" "SW1"
			(at 0 -2.75 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "SW_Push"
			(at 0 3 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Push button switch, generic, two pins"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "testbed-mcu copy.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.SilkS")
		)
		(pad "1" smd roundrect
			(at -2.575 -0.85 270)
			(size 1.45 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "1" smd roundrect
			(at 2.575 -0.85 270)
			(size 1.45 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at -2.575 0.85 270)
			(size 1.45 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "/EN")
			(pinfunction "2")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 2.575 0.85 270)
			(size 1.45 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "/EN")
			(pinfunction "2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Button_Switch_SMD.3dshapes/SW_SPST_EVQP2_MiddlePushTravel_H2.5mm.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "F.Cu")
		(at 157.3 102.8)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP1"
			(at 0 -1.448 0)
			(layer "F.SilkS")
		)
		(property "Value" "TestPoint"
			(at 0 1.55 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/")
		(sheetfile "testbed-mcu copy.kicad_sch")
		(attr exclude_from_pos_files)
		(pad "1" smd circle
			(at 0 0)
			(size 1 1)
			(layers "F.Cu" "F.Mask")
			(net 84 "+3.3V")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "capstone-project:LTST-C191GKT"
		(layer "F.Cu")
		(at 203.7741 128.4)
		(descr "LTST-C191GKT")
		(tags "LED")
		(property "Reference" "D3"
			(at -2.40499 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "LTST-C191GKT"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" "https://componentsearchengine.com/Datasheets/1/LTST-C191GKT.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Lite-On 569 nm Green LED, 1608 (0603) SMD package"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Height" "0.65"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Part Number" "859-LTST-C191GKT"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Price/Stock" "https://www.mouser.co.uk/ProductDetail/LITEON/LTST-C191GKT?qs=wp3idE545Uf460CSMpWzfQ%3D%3D"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Name" "Lite-On"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Part_Number" "LTST-C191GKT"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "testbed-mcu copy.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -0.75 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 70 "Net-(D3-K)")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 0.75 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 71 "Net-(D3-A)")
			(pinfunction "A")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_JST:JST_SH_SM04B-SRSS-TB_1x04-1MP_P1.00mm_Horizontal"
		(layer "F.Cu")
		(at 212.473097 90.970028 90)
		(descr "JST SH series connector, SM04B-SRSS-TB (http://www.jst-mfg.com/product/pdf/eng/eSH.pdf), generated with kicad-footprint-generator")
		(tags "connector JST SH horizontal")
		(property "Reference" "J8"
			(at 0 -3.98 90)
			(layer "F.SilkS")
		)
		(property "Value" "Stemma QT"
			(at 0 3.98 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://cdn-shop.adafruit.com/product-files/4208/4208_Kaweei_C13396_diagram.pdf"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic shielded connector, single row, 01x04, script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??-1SH*")
		(sheetname "/")
		(sheetfile "testbed-mcu copy.kicad_sch")
		(attr smd)
		(pad "1" smd roundrect
			(at -1.5 -2 90)
			(size 0.6 1.55)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at -0.5 -2 90)
			(size 0.6 1.55)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 84 "+3.3V")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" smd roundrect
			(at 0.5 -2 90)
			(size 0.6 1.55)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 10 "/SDA")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" smd roundrect
			(at 1.5 -2 90)
			(size 0.6 1.55)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 8 "/SCL")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(pad "MP" smd roundrect
			(at -2.8 1.875 90)
			(size 1.2 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
		)
		(pad "MP" smd roundrect
			(at 2.8 1.875 90)
			(size 1.2 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_JST.3dshapes/JST_SH_SM04B-SRSS-TB_1x04-1MP_P1.00mm_Horizontal.step"
			(hide yes)
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_PinHeader_1.00mm:PinHeader_1x06_P1.00mm_Vertical"
		(layer "F.Cu")
		(at 204.1 87.22359 90)
		(descr "Through hole straight pin header, 1x06, 1.00mm pitch, single row")
		(tags "Through hole pin header THT 1x06 1.00mm single row")
		(property "Reference" "J2"
			(at 0 -1.61 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Conn_01x06_Socket"
			(at 0 6.61 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x06, script generated"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "/")
		(sheetfile "testbed-mcu copy.kicad_sch")
		(clearance 0.15)
		(attr through_hole allow_soldermask_bridges)
		(fp_text user "${REFERENCE}"
			(at 0 -1.46089 90)
			(layer "F.SilkS")
		)
		(pad "1" thru_hole rect
			(at 0 0 90)
			(size 0.85 0.85)
			(drill 0.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 84 "+3.3V")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 0 1 90)
			(size 0.85 0.85)
			(drill 0.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 74 "RXD")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole circle
			(at 0 2 90)
			(size 0.85 0.85)
			(drill 0.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 73 "RXD0")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole circle
			(at 0 3 90)
			(size 0.85 0.85)
			(drill 0.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 8 "/SCL")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(pad "5" thru_hole circle
			(at 0 4 90)
			(size 0.85 0.85)
			(drill 0.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 10 "/SDA")
			(pinfunction "Pin_5")
			(pintype "passive")
		)
		(pad "6" thru_hole circle
			(at 0 5 90)
			(size 0.85 0.85)
			(drill 0.5)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_6")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_PinHeader_1.00mm.3dshapes/PinHeader_1x06_P1.00mm_Vertical.step"
			(hide yes)
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 170.85 87.325 180)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R5"
			(at 0 -1.43 0)
			(layer "F.SilkS")
		)
		(property "Value" "680"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "PWR LED R"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "testbed-mcu copy.kicad_sch")
		(attr smd)
		(pad "1" smd roundrect
			(at -0.825 0 180)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 63 "Net-(JP2-A)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0 180)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 66 "Net-(D1-A)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MountingHole:MountingHole_3.2mm_M3_ISO14580_Pad"
		(layer "F.Cu")
		(at 215.59311 130.3883)
		(descr "Mounting Hole 3.2mm, M3, generated by kicad-footprint-generator mountinghole.py")
		(tags "mountinghole M3 ISO14580")
		(property "Reference" "H20"
			(at 0 -3.7 0)
			(layer "F.SilkS")
		)
		(property "Value" "M3"
			(at 0 3.7 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Mounting Hole with connection"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "MountingHole*Pad*")
		(sheetname "/")
		(sheetfile "testbed-mcu copy.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 5.5 5.5)
			(drill 3.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "1")
			(pintype "input")
			(zone_connect 2)
		)
		(embedded_fonts no)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 206.274162 128.38652 -90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R11"
			(at 0 -1.43 90)
			(layer "F.SilkS")
		)
		(property "Value" "680"
			(at 0 1.43 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "PWR LED R"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "testbed-mcu copy.kicad_sch")
		(attr smd)
		(pad "1" smd roundrect
			(at -0.825 0 270)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 84 "+3.3V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0 270)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 71 "Net-(D3-A)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MountingHole:MountingHole_3.2mm_M3_ISO14580_Pad"
		(layer "F.Cu")
		(at 215.577221 102.456235)
		(descr "Mounting Hole 3.2mm, M3, generated by kicad-footprint-generator mountinghole.py")
		(tags "mountinghole M3 ISO14580")
		(property "Reference" "H18"
			(at 0.322779 3.492648 0)
			(layer "F.SilkS")
		)
		(property "Value" "M3"
			(at 0 3.7 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Mounting Hole with connection"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "MountingHole*Pad*")
		(sheetname "/")
		(sheetfile "testbed-mcu copy.kicad_sch")
		(attr exclude_from_pos_files exclude_from_bom)
		(pad "1" thru_hole circle
			(at 0 0)
			(size 5.5 5.5)
			(drill 3.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "1")
			(pintype "input")
			(zone_connect 2)
		)
		(embedded_fonts no)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "F.Cu")
		(at 157.3 118.6)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP5"
			(at 2.41311 -1.448 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 1.55 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/")
		(sheetfile "testbed-mcu copy.kicad_sch")
		(attr exclude_from_pos_files)
		(fp_text user "${REFERENCE}"
			(at 0 -1.45 0)
			(layer "F.SilkS")
		)
		(pad "1" smd circle
			(at 0 0)
			(size 1 1)
			(layers "F.Cu" "F.Mask")
			(net 84 "+3.3V")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 191.1 129.6 90)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C6"
			(at -2.1 0 180)
			(layer "F.SilkS")
		)
		(property "Value" "0.1uF"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "testbed-mcu copy.kicad_sch")
		(attr smd)
		(pad "1" smd roundrect
			(at -0.775 0 90)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 90)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 84 "+3.3V")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "capstone-project:ESP32-WROVER-IE"
		(layer "F.Cu")
		(at 190.6 97.892)
		(property "Reference" "U8"
			(at -0.16 2.06 0)
			(layer "F.SilkS")
		)
		(property "Value" "ESP32-WROVER-E"
			(at -0.02 0.32 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "kicad-embed://esp32-wrover-e_esp32-wrover-ie_datasheet_en.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "WROVER-E & WROVER-IE Footprint"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "testbed-mcu copy.kicad_sch")
		(attr through_hole)
		(fp_text user "Keep Out Area"
			(at -0.61 -15.68 0)
			(layer "F.SilkS")
		)
		(fp_text user "Keep Out Area"
			(at -0.61 -15.68 0)
			(layer "F.SilkS")
		)
		(pad "1" smd rect
			(at -8.75 -11.43)
			(size 1.5 0.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "2" smd rect
			(at -8.75 -10.16)
			(size 1.5 0.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 84 "+3.3V")
			(pinfunction "3V3")
			(pintype "power_in")
		)
		(pad "3" smd rect
			(at -8.75 -8.89)
			(size 1.5 0.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "/EN")
			(pinfunction "EN")
			(pintype "input")
		)
		(pad "4" smd rect
			(at -8.75 -7.62)
			(size 1.5 0.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 6 "/BMS_INT")
			(pinfunction "GPIO36")
			(pintype "output")
		)
		(pad "5" smd rect
			(at -8.75 -6.35)
			(size 1.5 0.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 4 "/RF_INT")
			(pinfunction "GPIO39")
			(pintype "output")
		)
		(pad "6" smd rect
			(at -8.75 -5.08)
			(size 1.5 0.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 64 "/DIN")
			(pinfunction "GPIO34")
			(pintype "bidirectional")
		)
		(pad "7" smd rect
			(at -8.75 -3.81)
			(size 1.5 0.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 7 "/HMI_INT")
			(pinfunction "GPIO35")
			(pintype "bidirectional")
		)
		(pad "8" smd rect
			(at -8.75 -2.54)
			(size 1.5 0.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 60 "/VSPI_GDO0")
			(pinfunction "GPIO32")
			(pintype "bidirectional")
		)
		(pad "9" smd rect
			(at -8.75 -1.27)
			(size 1.5 0.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 55 "/VSPI_GDO2")
			(pinfunction "GPIO33")
			(pintype "input")
		)
		(pad "10" smd rect
			(at -8.75 0)
			(size 1.5 0.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 5 "/LRCLK")
			(pinfunction "GPIO25")
			(pintype "output")
		)
		(pad "11" smd rect
			(at -8.75 1.27)
			(size 1.5 0.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 3 "/BCLK")
			(pinfunction "GPIO26")
			(pintype "bidirectional")
		)
		(pad "12" smd rect
			(at -8.75 2.54)
			(size 1.5 0.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 65 "/DOUT")
			(pinfunction "GPIO27")
			(pintype "output")
		)
		(pad "13" smd rect
			(at -8.75 3.81)
			(size 1.5 0.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 57 "/HSPI_SCLK")
			(pinfunction "GPIO14")
			(pintype "bidirectional")
		)
		(pad "14" smd rect
			(at -8.75 5.08)
			(size 1.5 0.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 54 "/X_INT")
			(pinfunction "IO12")
			(pintype "bidirectional")
		)
		(pad "15" smd rect
			(at -8.75 6.35)
			(size 1.5 0.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "16" smd rect
			(at -8.75 7.62)
			(size 1.5 0.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 58 "/HSPI_MOSI")
			(pinfunction "GPIO13")
			(pintype "bidirectional")
		)
		(pad "17" smd rect
			(at -8.75 8.89)
			(size 1.5 0.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 35 "unconnected-(U8-NC-Pad17)")
			(pinfunction "NC")
			(pintype "no_connect")
		)
		(pad "18" smd rect
			(at -8.75 10.16)
			(size 1.5 0.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 36 "unconnected-(U8-NC-Pad18)")
			(pinfunction "NC")
			(pintype "no_connect")
		)
		(pad "19" smd rect
			(at -8.75 11.43)
			(size 1.5 0.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 37 "unconnected-(U8-NC-Pad19)")
			(pinfunction "NC")
			(pintype "no_connect")
		)
		(pad "20" smd rect
			(at 8.75 11.43)
			(size 1.5 0.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 38 "unconnected-(U8-NC-Pad20)")
			(pinfunction "NC")
			(pintype "no_connect")
		)
		(pad "21" smd rect
			(at 8.75 10.16)
			(size 1.5 0.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 39 "unconnected-(U8-NC-Pad21)")
			(pinfunction "NC")
			(pintype "no_connect")
		)
		(pad "22" smd rect
			(at 8.75 8.89)
			(size 1.5 0.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 40 "unconnected-(U8-NC-Pad22)")
			(pinfunction "NC")
			(pintype "no_connect")
		)
		(pad "23" smd rect
			(at 8.75 7.62)
			(size 1.5 0.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 45 "/HSPI_CS")
			(pinfunction "IO15")
			(pintype "bidirectional")
		)
		(pad "24" smd rect
			(at 8.75 6.35)
			(size 1.5 0.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 9 "/AUDIO_INT")
			(pinfunction "IO2")
			(pintype "bidirectional")
		)
		(pad "25" smd rect
			(at 8.75 5.08)
			(size 1.5 0.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 67 "/IO0")
			(pinfunction "IO0")
			(pintype "bidirectional")
		)
		(pad "26" smd rect
			(at 8.75 3.81)
			(size 1.5 0.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 56 "/HSPI_DC")
			(pinfunction "GPIO4")
			(pintype "bidirectional")
		)
		(pad "27" smd rect
			(at 8.75 2.54)
			(size 1.5 0.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 42 "unconnected-(U8-NC-Pad27)")
			(pinfunction "NC")
			(pintype "no_connect")
		)
		(pad "28" smd rect
			(at 8.75 1.27)
			(size 1.5 0.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 43 "unconnected-(U8-NC-Pad28)")
			(pinfunction "NC")
			(pintype "no_connect")
		)
		(pad "29" smd rect
			(at 8.75 0)
			(size 1.5 0.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 46 "/VSPI_CS")
			(pinfunction "IO5")
			(pintype "bidirectional")
		)
		(pad "30" smd rect
			(at 8.75 -1.27)
			(size 1.5 0.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 53 "/VSPI_SCLK")
			(pinfunction "GPIO18")
			(pintype "bidirectional")
		)
		(pad "31" smd rect
			(at 8.75 -2.54)
			(size 1.5 0.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 52 "/VSPI_MISO")
			(pinfunction "GPIO19")
			(pintype "bidirectional")
		)
		(pad "32" smd rect
			(at 8.75 -3.81)
			(size 1.5 0.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 44 "unconnected-(U8-NC-Pad32)")
			(pinfunction "NC")
			(pintype "no_connect")
		)
		(pad "33" smd rect
			(at 8.75 -5.08)
			(size 1.5 0.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 10 "/SDA")
			(pinfunction "GPIO21")
			(pintype "bidirectional")
		)
		(pad "34" smd rect
			(at 8.75 -6.35)
			(size 1.5 0.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 81 "Net-(U8-RXD0)")
			(pinfunction "RXD0")
			(pintype "output")
		)
		(pad "35" smd rect
			(at 8.75 -7.62)
			(size 1.5 0.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 82 "Net-(U8-TXD0)")
			(pinfunction "TXD0")
			(pintype "output")
		)
		(pad "36" smd rect
			(at 8.75 -8.89)
			(size 1.5 0.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 8 "/SCL")
			(pinfunction "GPIO22")
			(pintype "bidirectional")
		)
		(pad "37" smd rect
			(at 8.75 -10.16)
			(size 1.5 0.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 59 "/VSPI_MOSI")
			(pinfunction "GPIO23")
			(pintype "bidirectional")
		)
		(pad "38" smd rect
			(at 8.75 -11.43)
			(size 1.5 0.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "39" smd rect
			(at -2.9 -4.42)
			(size 0.9 0.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "Pad39")
			(pintype "unspecified")
		)
		(pad "39" smd rect
			(at -2.9 -3.02)
			(size 0.9 0.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "Pad39")
			(pintype "unspecified")
		)
		(pad "39" smd rect
			(at -2.9 -1.62)
			(size 0.9 0.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "Pad39")
			(pintype "unspecified")
		)
		(pad "39" smd rect
			(at -1.5 -4.42)
			(size 0.9 0.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "Pad39")
			(pintype "unspecified")
		)
		(pad "39" smd rect
			(at -1.5 -3.02)
			(size 0.9 0.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "Pad39")
			(pintype "unspecified")
		)
		(pad "39" smd rect
			(at -1.5 -1.62)
			(size 0.9 0.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "Pad39")
			(pintype "unspecified")
		)
		(pad "39" smd rect
			(at -0.1 -4.42)
			(size 0.9 0.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "Pad39")
			(pintype "unspecified")
		)
		(pad "39" smd rect
			(at -0.1 -3.02)
			(size 0.9 0.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "Pad39")
			(pintype "unspecified")
		)
		(pad "39" smd rect
			(at -0.1 -1.62)
			(size 0.9 0.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "Pad39")
			(pintype "unspecified")
		)
		(embedded_fonts no)
		(model "${KIPRJMOD}/capstone-project.pretty/3dmodels/ESP32-WROVER-E.step"
			(offset
				(xyz -9 -12.5 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -0 -0 -0)
			)
		)
	)
	(footprint "Jumper:SolderJumper-2_P1.3mm_Bridged_RoundedPad1.0x1.5mm"
		(layer "F.Cu")
		(at 174.275 87.325)
		(descr "SMD Solder Jumper, 1x1.5mm, rounded Pads, 0.3mm gap, bridged with 1 copper strip")
		(tags "net tie solder jumper bridged")
		(property "Reference" "JP2"
			(at 0 -1.8 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "PWR LED"
			(at -0.025 1.7 0)
			(layer "F.SilkS")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Solder Jumper, 2-pole, closed/bridged"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SolderJumper*Bridged*")
		(sheetname "/")
		(sheetfile "testbed-mcu copy.kicad_sch")
		(zone_connect 1)
		(attr exclude_from_pos_files exclude_from_bom allow_soldermask_bridges)
		(net_tie_pad_groups "1, 2")
		(pad "1" smd custom
			(at -0.65 0)
			(size 1 0.5)
			(layers "F.Cu" "F.Mask")
			(net 63 "Net-(JP2-A)")
			(pinfunction "A")
			(pintype "passive")
			(zone_connect 2)
			(thermal_bridge_angle 45)
			(options
				(clearance outline)
				(anchor rect)
			)
			(primitives
				(gr_circle
					(center 0 0.25)
					(end 0.5 0.25)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center 0 -0.25)
					(end 0.5 -0.25)
					(width 0)
					(fill yes)
				)
				(gr_poly
					(pts
						(xy 0.5 0.75) (xy 0 0.75) (xy 0 -0.75) (xy 0.5 -0.75)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "2" smd custom
			(at 0.65 0)
			(size 1 0.5)
			(layers "F.Cu" "F.Mask")
			(net 84 "+3.3V")
			(pinfunction "B")
			(pintype "passive")
			(zone_connect 2)
			(thermal_bridge_angle 45)
			(options
				(clearance outline)
				(anchor rect)
			)
			(primitives
				(gr_circle
					(center 0 0.25)
					(end 0.5 0.25)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center 0 -0.25)
					(end 0.5 -0.25)
					(width 0)
					(fill yes)
				)
				(gr_poly
					(pts
						(xy 0 0.75) (xy -0.5 0.75) (xy -0.5 -0.75) (xy 0 -0.75)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(embedded_fonts no)
	)
	(footprint "Connector_PinSocket_1.27mm:PinSocket_1x03_P1.27mm_Vertical"
		(layer "F.Cu")
		(at 165.35 117.08)
		(descr "Through hole straight socket strip, 1x03, 1.27mm pitch, single row (from Kicad 4.0.7), script generated")
		(tags "Through hole socket strip THT 1x03 1.27mm single row")
		(property "Reference" "J3"
			(at 0 -2.135 0)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_01x03_Socket"
			(at 0 4.675 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x03, script generated"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "/")
		(sheetfile "testbed-mcu copy.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 1.27 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1 1)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 75 "Net-(J3-Pin_1)")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 0 1.27)
			(size 1 1)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 88 "Net-(J3-Pin_2)")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole circle
			(at 0 2.54)
			(size 1 1)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 89 "Net-(J3-Pin_3)")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_PinSocket_1.27mm.3dshapes/PinSocket_1x03_P1.27mm_Vertical.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 178.5 87.6 -90)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C3"
			(at 2.1 -0.2 0)
			(layer "F.SilkS")
		)
		(property "Value" "0.1u"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "testbed-mcu copy.kicad_sch")
		(attr smd)
		(pad "1" smd roundrect
			(at -0.775 0 270)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 84 "+3.3V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 270)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 202.7 90.1 180)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R9"
			(at -2.22511 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "0"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "testbed-mcu copy.kicad_sch")
		(attr smd)
		(pad "1" smd roundrect
			(at -0.825 0 180)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 74 "RXD")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0 180)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 82 "Net-(U8-TXD0)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 203.175 97.925 180)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R4"
			(at 0 -1.43 0)
			(layer "F.SilkS")
		)
		(property "Value" "10k"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "testbed-mcu copy.kicad_sch")
		(attr smd)
		(pad "1" smd roundrect
			(at -0.825 0 180)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 84 "+3.3V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0 180)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 46 "/VSPI_CS")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 210.15 103.003575)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C4"
			(at 0.019656 1.197355 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "0.1u"
			(at 0 1.43 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "testbed-mcu copy.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at -2.042804 -0.010199 90)
			(layer "F.SilkS")
		)
		(pad "1" smd roundrect
			(at -0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 67 "/IO0")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "LOGO"
		(layer "F.Cu")
		(at 160.75 134.2)
		(property "Reference" "G***"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "LOGO"
			(at 0.75 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr board_only exclude_from_pos_files exclude_from_bom)
		(embedded_fonts no)
	)
	(footprint "Button_Switch_SMD:SW_SPST_EVQP2_MiddlePushTravel_H2.5mm"
		(layer "F.Cu")
		(at 210.15 98.675 90)
		(descr "Tactile switch, 4.7 x 3.5 mm, middle push travel, H2.5mm, https://industry.panasonic.com/ac/cdn/e/control/switch/light-touch/catalog/sw_lt_eng_4735s.pdf")
		(tags "SMD SMT SPST EVQP2")
		(property "Reference" "SW2"
			(at 0 -2.75 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "SW_Push"
			(at 0 3 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Push button switch, generic, two pins"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "testbed-mcu copy.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.SilkS")
		)
		(pad "1" smd roundrect
			(at -2.575 -0.85 90)
			(size 1.45 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 67 "/IO0")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "1" smd roundrect
			(at 2.575 -0.85 90)
			(size 1.45 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 67 "/IO0")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at -2.575 0.85 90)
			(size 1.45 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "2")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 2.575 0.85 90)
			(size 1.45 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Button_Switch_SMD.3dshapes/SW_SPST_EVQP2_MiddlePushTravel_H2.5mm.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "capstone-project:Adafruit EYESPI FPC Connector"
		(layer "F.Cu")
		(at 152.908 125.476 -90)
		(descr "WR-FPC SMT ZIF Horizontal Hinge Type")
		(tags "EYESPI, FPC")
		(property "Reference" "X6"
			(at 7.674 1.808 90)
			(layer "F.SilkS")
		)
		(property "Value" "EYESPI"
			(at 0 4.064 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://www.we-online.com/components/products/datasheet/687118149022.pdf"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "WR-FPC SMT ZIF Horizontal Hinge Type"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Assignment" "DISPLAY_HSPI"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "testbed-mcu copy.kicad_sch")
		(attr smd allow_soldermask_bridges)
		(pad "1" smd rect
			(at -4.25 -3.35 270)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 84 "+3.3V")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd rect
			(at -3.75 -3.35 270)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 11 "unconnected-(X6-Pad2)")
			(pintype "passive+no_connect")
			(solder_mask_margin 0.102)
		)
		(pad "3" smd rect
			(at -3.25 -3.35 270)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "4" smd rect
			(at -2.75 -3.35 270)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 57 "/HSPI_SCLK")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "5" smd rect
			(at -2.25 -3.35 270)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 58 "/HSPI_MOSI")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "6" smd rect
			(at -1.75 -3.35 270)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 12 "unconnected-(X6-Pad6)")
			(pintype "passive+no_connect")
			(solder_mask_margin 0.102)
		)
		(pad "7" smd rect
			(at -1.25 -3.35 270)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 56 "/HSPI_DC")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "8" smd rect
			(at -0.75 -3.35 270)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 85 "/TFT_RST")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "9" smd rect
			(at -0.25 -3.35 270)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 45 "/HSPI_CS")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "10" smd rect
			(at 0.25 -3.35 270)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 86 "/CARD_CS")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "11" smd rect
			(at 0.75 -3.35 270)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 64 "/DIN")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "12" smd rect
			(at 1.25 -3.35 270)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 65 "/DOUT")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "13" smd rect
			(at 1.75 -3.35 270)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 8 "/SCL")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "14" smd rect
			(at 2.25 -3.35 270)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 10 "/SDA")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "15" smd rect
			(at 2.75 -3.35 270)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 7 "/HMI_INT")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "16" smd rect
			(at 3.25 -3.35 270)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 83 "/AMP_SD")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "17" smd rect
			(at 3.75 -3.35 270)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 3 "/BCLK")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "18" smd rect
			(at 4.25 -3.35 270)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 5 "/LRCLK")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "Z1" smd rect
			(at -6.05 -0.6 270)
			(size 2 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "Z2" smd rect
			(at 6.05 -0.6 270)
			(size 2 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
		(model "${KIPRJMOD}/capstone-project.pretty/3dmodels/687118149022+(rev1).step"
			(offset
				(xyz 0 0.5 1.15)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -0 -0 -0)
			)
		)
	)
	(footprint "Package_SO:SSOP-24_5.3x8.2mm_P0.65mm"
		(layer "F.Cu")
		(at 173.35 116.55)
		(descr "SSOP, 24 Pin (JEDEC MO-150 variation AG, 1.75mm body thickness, https://www.jedec.org/document_search?search_api_views_fulltext=MO-150, https://ww1.microchip.com/downloads/en/PackagingSpec/00000049BQ.pdf#page=398, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/ltc-legacy-ssop/ssop_24_05-08-1640.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SSOP SO")
		(property "Reference" "U6"
			(at 0 -5.05 0)
			(layer "F.SilkS")
		)
		(property "Value" "PCF8575DBR"
			(at 0 5.05 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/pcf8575.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "16 Bits Port/Expander to I2C Bus, SSOP-24"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SSOP*5.3x8.2mm*P0.65mm*")
		(sheetname "/")
		(sheetfile "testbed-mcu copy.kicad_sch")
		(attr smd allow_soldermask_bridges)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.SilkS")
		)
		(pad "1" smd roundrect
			(at -3.5 -3.575)
			(size 1.9 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 54 "/X_INT")
			(pinfunction "~{INT}")
			(pintype "open_collector")
		)
		(pad "2" smd roundrect
			(at -3.5 -2.925)
			(size 1.9 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "A1")
			(pintype "input")
		)
		(pad "3" smd roundrect
			(at -3.5 -2.275)
			(size 1.9 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "A2")
			(pintype "input")
		)
		(pad "4" smd roundrect
			(at -3.5 -1.625)
			(size 1.9 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 72 "/CC1200_RST")
			(pinfunction "P0")
			(pintype "bidirectional")
		)
		(pad "5" smd roundrect
			(at -3.5 -0.975)
			(size 1.9 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 83 "/AMP_SD")
			(pinfunction "P1")
			(pintype "bidirectional")
		)
		(pad "6" smd roundrect
			(at -3.5 -0.325)
			(size 1.9 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 87 "/BAT_LOW")
			(pinfunction "P2")
			(pintype "bidirectional")
		)
		(pad "7" smd roundrect
			(at -3.5 0.325)
			(size 1.9 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 86 "/CARD_CS")
			(pinfunction "P3")
			(pintype "bidirectional")
		)
		(pad "8" smd roundrect
			(at -3.5 0.975)
			(size 1.9 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 85 "/TFT_RST")
			(pinfunction "P4")
			(pintype "bidirectional")
		)
		(pad "9" smd roundrect
			(at -3.5 1.625)
			(size 1.9 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 75 "Net-(J3-Pin_1)")
			(pinfunction "P5")
			(pintype "bidirectional")
		)
		(pad "10" smd roundrect
			(at -3.5 2.275)
			(size 1.9 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 88 "Net-(J3-Pin_2)")
			(pinfunction "P6")
			(pintype "bidirectional")
		)
		(pad "11" smd roundrect
			(at -3.5 2.925)
			(size 1.9 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 89 "Net-(J3-Pin_3)")
			(pinfunction "P7")
			(pintype "bidirectional")
		)
		(pad "12" smd roundrect
			(at -3.5 3.575)
			(size 1.9 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "13" smd roundrect
			(at 3.5 3.575)
			(size 1.9 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 76 "Net-(J4-Pin_1)")
			(pinfunction "P10")
			(pintype "bidirectional")
		)
		(pad "14" smd roundrect
			(at 3.5 2.925)
			(size 1.9 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 96 "Net-(J4-Pin_2)")
			(pinfunction "P11")
			(pintype "bidirectional")
		)
		(pad "15" smd roundrect
			(at 3.5 2.275)
			(size 1.9 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 93 "Net-(J4-Pin_3)")
			(pinfunction "P12")
			(pintype "bidirectional")
		)
		(pad "16" smd roundrect
			(at 3.5 1.625)
			(size 1.9 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 95 "Net-(J4-Pin_4)")
			(pinfunction "P13")
			(pintype "bidirectional")
		)
		(pad "17" smd roundrect
			(at 3.5 0.975)
			(size 1.9 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 91 "Net-(J4-Pin_5)")
			(pinfunction "P14")
			(pintype "bidirectional")
		)
		(pad "18" smd roundrect
			(at 3.5 0.325)
			(size 1.9 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 94 "Net-(J4-Pin_6)")
			(pinfunction "P15")
			(pintype "bidirectional")
		)
		(pad "19" smd roundrect
			(at 3.5 -0.325)
			(size 1.9 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 92 "Net-(J4-Pin_7)")
			(pinfunction "P16")
			(pintype "bidirectional")
		)
		(pad "20" smd roundrect
			(at 3.5 -0.975)
			(size 1.9 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 90 "Net-(J4-Pin_8)")
			(pinfunction "P17")
			(pintype "bidirectional")
		)
		(pad "21" smd roundrect
			(at 3.5 -1.625)
			(size 1.9 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "A0")
			(pintype "input")
		)
		(pad "22" smd roundrect
			(at 3.5 -2.275)
			(size 1.9 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 8 "/SCL")
			(pinfunction "SCL")
			(pintype "input")
		)
		(pad "23" smd roundrect
			(at 3.5 -2.925)
			(size 1.9 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 10 "/SDA")
			(pinfunction "SDA")
			(pintype "bidirectional")
		)
		(pad "24" smd roundrect
			(at 3.5 -3.575)
			(size 1.9 0.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 84 "+3.3V")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Package_SO.3dshapes/SSOP-24_5.3x8.2mm_P0.65mm.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 189.4 129.6 90)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C7"
			(at -2.1 0 180)
			(layer "F.SilkS")
		)
		(property "Value" "4.7uF"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "testbed-mcu copy.kicad_sch")
		(attr smd)
		(pad "1" smd roundrect
			(at -0.775 0 90)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 90)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 84 "+3.3V")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "capstone-project:LTST-C191GKT"
		(layer "F.Cu")
		(at 203.7741 124.99307)
		(descr "LTST-C191GKT")
		(tags "LED")
		(property "Reference" "D2"
			(at -2.40499 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "LTST-C191GKT"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" "https://componentsearchengine.com/Datasheets/1/LTST-C191GKT.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Lite-On 569 nm Green LED, 1608 (0603) SMD package"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Height" "0.65"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Part Number" "859-LTST-C191GKT"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Price/Stock" "https://www.mouser.co.uk/ProductDetail/LITEON/LTST-C191GKT?qs=wp3idE545Uf460CSMpWzfQ%3D%3D"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Name" "Lite-On"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Part_Number" "LTST-C191GKT"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "testbed-mcu copy.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -0.75 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 68 "Net-(D2-K)")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 0.75 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 69 "Net-(D2-A)")
			(pinfunction "A")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_SMD:SOT-23"
		(layer "F.Cu")
		(at 194.8 117.3759 90)
		(descr "SOT, 3 Pin (JEDEC TO-236 Var AB https://www.jedec.org/document_search?search_api_views_fulltext=TO-236), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOT TO_SOT_SMD")
		(property "Reference" "Q2"
			(at 0 -2.6 0)
			(layer "F.SilkS")
		)
		(property "Value" "SS8050"
			(at 0 -1.7 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "http://www.secosgmbh.com/datasheet/products/SSMPTransistor/SOT-23/SS8050.pdf"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "General Purpose NPN Transistor, 1.5A Ic, 25V Vce, SOT-23"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SOT?23*")
		(sheetname "/")
		(sheetfile "testbed-mcu copy.kicad_sch")
		(attr smd)
		(pad "1" smd roundrect
			(at -0.9375 -0.95 90)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 51 "Net-(Q2-B)")
			(pinfunction "B")
			(pintype "input")
		)
		(pad "2" smd roundrect
			(at -0.9375 0.95 90)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 78 "/DTR")
			(pinfunction "E")
			(pintype "passive")
		)
		(pad "3" smd roundrect
			(at 0.9375 0 90)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 67 "/IO0")
			(pinfunction "C")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_PinSocket_1.27mm:PinSocket_1x08_P1.27mm_Vertical"
		(layer "F.Cu")
		(at 185.275 122.55 180)
		(descr "Through hole straight socket strip, 1x08, 1.27mm pitch, single row (from Kicad 4.0.7), script generated")
		(tags "Through hole socket strip THT 1x08 1.27mm single row")
		(property "Reference" "J4"
			(at 0 -2.135 0)
			(layer "F.SilkS")
		)
		(property "Value" "Conn_01x08_Socket"
			(at 0 11.025 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x08, script generated"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "/")
		(sheetfile "testbed-mcu copy.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 4.445 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 180)
			(size 1 1)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 76 "Net-(J4-Pin_1)")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 0 1.27 180)
			(size 1 1)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 96 "Net-(J4-Pin_2)")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole circle
			(at 0 2.54 180)
			(size 1 1)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 93 "Net-(J4-Pin_3)")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole circle
			(at 0 3.81 180)
			(size 1 1)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 95 "Net-(J4-Pin_4)")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(pad "5" thru_hole circle
			(at 0 5.08 180)
			(size 1 1)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 91 "Net-(J4-Pin_5)")
			(pinfunction "Pin_5")
			(pintype "passive")
		)
		(pad "6" thru_hole circle
			(at 0 6.35 180)
			(size 1 1)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 94 "Net-(J4-Pin_6)")
			(pinfunction "Pin_6")
			(pintype "passive")
		)
		(pad "7" thru_hole circle
			(at 0 7.62 180)
			(size 1 1)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 92 "Net-(J4-Pin_7)")
			(pinfunction "Pin_7")
			(pintype "passive")
		)
		(pad "8" thru_hole circle
			(at 0 8.89 180)
			(size 1 1)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 90 "Net-(J4-Pin_8)")
			(pinfunction "Pin_8")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_PinSocket_1.27mm.3dshapes/PinSocket_1x08_P1.27mm_Vertical.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 207.2 107.9 90)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C1"
			(at -2.075 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "0.1u"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "testbed-mcu copy.kicad_sch")
		(attr smd)
		(pad "1" smd roundrect
			(at -0.775 0 90)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 90)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "/EN")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "capstone-project:QFN28_5X5_SIL"
		(layer "F.Cu")
		(at 197.2 127)
		(tags "CP2102N-A02-GQFN28 ")
		(property "Reference" "U5"
			(at 3.66111 2.64159 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(property "Value" "CP2102N-A02-GQFN28"
			(at 35.573085 -42.357592 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "CP2102N-A02-GQFN28"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "QFN28_5X5_SIL QFN28_5X5_SIL-M QFN28_5X5_SIL-L")
		(sheetname "/")
		(sheetfile "testbed-mcu copy.kicad_sch")
		(clearance 0.1651)
		(attr smd allow_soldermask_bridges)
		(fp_text user "*"
			(at -3.4009 -2.55 0)
			(layer "F.SilkS")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(fp_text user "*"
			(at -1.8415 -1.75 0)
			(layer "F.Fab")
		)
		(fp_text user "*"
			(at -1.8415 -1.75 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -2.3241 -1.5 90)
			(size 0.254 0.9652)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 21 "unconnected-(U5-DCD-Pad1)")
			(pinfunction "DCD")
			(pintype "input+no_connect")
		)
		(pad "2" smd rect
			(at -2.3241 -1.000001 90)
			(size 0.254 0.9652)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 22 "unconnected-(U5-RI{slash}CLK-Pad2)")
			(pinfunction "RI/CLK")
			(pintype "bidirectional+no_connect")
		)
		(pad "3" smd rect
			(at -2.3241 -0.499999 90)
			(size 0.254 0.9652)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "4" smd rect
			(at -2.3241 0 90)
			(size 0.254 0.9652)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 62 "/D+")
			(pinfunction "D+")
			(pintype "input")
		)
		(pad "5" smd rect
			(at -2.3241 0.499999 90)
			(size 0.254 0.9652)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 61 "/D-")
			(pinfunction "D-")
			(pintype "input")
		)
		(pad "6" smd rect
			(at -2.3241 1.000001 90)
			(size 0.254 0.9652)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 84 "+3.3V")
			(pinfunction "VDD")
			(pintype "power_in")
		)
		(pad "7" smd rect
			(at -2.3241 1.5 90)
			(size 0.254 0.9652)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 84 "+3.3V")
			(pinfunction "VREGIN")
			(pintype "power_in")
		)
		(pad "8" smd rect
			(at -1.5 2.3241)
			(size 0.254 0.9652)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 84 "+3.3V")
			(pinfunction "VBUS")
			(pintype "input")
		)
		(pad "9" smd rect
			(at -1.000001 2.3241)
			(size 0.254 0.9652)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 80 "Net-(U5-RSTb)")
			(pinfunction "RSTb")
			(pintype "unspecified")
		)
		(pad "10" smd rect
			(at -0.499999 2.3241)
			(size 0.254 0.9652)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 23 "unconnected-(U5-NC-Pad10)")
			(pinfunction "NC")
			(pintype "no_connect")
		)
		(pad "11" smd rect
			(at 0 2.3241)
			(size 0.254 0.9652)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 79 "Net-(U5-SUSPENDb)")
			(pinfunction "SUSPENDb")
			(pintype "output")
		)
		(pad "12" smd rect
			(at 0.499999 2.3241)
			(size 0.254 0.9652)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 24 "unconnected-(U5-SUSPEND-Pad12)")
			(pinfunction "SUSPEND")
			(pintype "output+no_connect")
		)
		(pad "13" smd rect
			(at 1.000001 2.3241)
			(size 0.254 0.9652)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 25 "unconnected-(U5-CHREN-Pad13)")
			(pinfunction "CHREN")
			(pintype "output+no_connect")
		)
		(pad "14" smd rect
			(at 1.5 2.3241)
			(size 0.254 0.9652)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 26 "unconnected-(U5-CHR1-Pad14)")
			(pinfunction "CHR1")
			(pintype "output+no_connect")
		)
		(pad "15" smd rect
			(at 2.3241 1.5 90)
			(size 0.254 0.9652)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 27 "unconnected-(U5-CHR0-Pad15)")
			(pinfunction "CHR0")
			(pintype "output+no_connect")
		)
		(pad "16" smd rect
			(at 2.3241 1.000001 90)
			(size 0.254 0.9652)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 28 "unconnected-(U5-GPIO.3{slash}WAKEUP-Pad16)")
			(pinfunction "GPIO.3/WAKEUP")
			(pintype "bidirectional+no_connect")
		)
		(pad "17" smd rect
			(at 2.3241 0.499999 90)
			(size 0.254 0.9652)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 29 "unconnected-(U5-GPIO.2{slash}RS485-Pad17)")
			(pinfunction "GPIO.2/RS485")
			(pintype "bidirectional+no_connect")
		)
		(pad "18" smd rect
			(at 2.3241 0 90)
			(size 0.254 0.9652)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 70 "Net-(D3-K)")
			(pinfunction "GPIO.1/RXT")
			(pintype "bidirectional")
		)
		(pad "19" smd rect
			(at 2.3241 -0.499999 90)
			(size 0.254 0.9652)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 68 "Net-(D2-K)")
			(pinfunction "GPIO.0/TXT")
			(pintype "bidirectional")
		)
		(pad "20" smd rect
			(at 2.3241 -1.000001 90)
			(size 0.254 0.9652)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 30 "unconnected-(U5-GPIO.6-Pad20)")
			(pinfunction "GPIO.6")
			(pintype "bidirectional+no_connect")
		)
		(pad "21" smd rect
			(at 2.3241 -1.5 90)
			(size 0.254 0.9652)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 31 "unconnected-(U5-GPIO.5-Pad21)")
			(pinfunction "GPIO.5")
			(pintype "bidirectional+no_connect")
		)
		(pad "22" smd rect
			(at 1.5 -2.3241)
			(size 0.254 0.9652)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 32 "unconnected-(U5-GPIO.4-Pad22)")
			(pinfunction "GPIO.4")
			(pintype "bidirectional+no_connect")
		)
		(pad "23" smd rect
			(at 1.000001 -2.3241)
			(size 0.254 0.9652)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 33 "unconnected-(U5-CTS-Pad23)")
			(pinfunction "CTS")
			(pintype "input+no_connect")
		)
		(pad "24" smd rect
			(at 0.499999 -2.3241)
			(size 0.254 0.9652)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 77 "/RTS")
			(pinfunction "RTS")
			(pintype "output")
		)
		(pad "25" smd rect
			(at 0 -2.3241)
			(size 0.254 0.9652)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 74 "RXD")
			(pinfunction "RXD")
			(pintype "input")
		)
		(pad "26" smd rect
			(at -0.499999 -2.3241)
			(size 0.254 0.9652)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 73 "RXD0")
			(pinfunction "TXD")
			(pintype "output")
		)
		(pad "27" smd rect
			(at -1.000001 -2.3241)
			(size 0.254 0.9652)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 34 "unconnected-(U5-DSR-Pad27)")
			(pinfunction "DSR")
			(pintype "input+no_connect")
		)
		(pad "28" smd rect
			(at -1.5 -2.3241)
			(size 0.254 0.9652)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 78 "/DTR")
			(pinfunction "DTR")
			(pintype "output")
		)
		(pad "29" smd rect
			(at 0 0)
			(size 3.3528 3.3528)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(embedded_fonts no)
	)
	(footprint "capstone-project:Adafruit EYESPI FPC Connector"
		(layer "F.Cu")
		(at 152.908 109.728 -90)
		(descr "WR-FPC SMT ZIF Horizontal Hinge Type")
		(tags "EYESPI, FPC")
		(property "Reference" "X7"
			(at 7.874 2.032 90)
			(layer "F.SilkS")
		)
		(property "Value" "EYESPI"
			(at 0 4.064 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://www.we-online.com/components/products/datasheet/687118149022.pdf"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "WR-FPC SMT ZIF Horizontal Hinge Type"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Assignment" "AUDIO_I2S"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "testbed-mcu copy.kicad_sch")
		(attr smd allow_soldermask_bridges)
		(pad "1" smd rect
			(at -4.25 -3.35 270)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 84 "+3.3V")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd rect
			(at -3.75 -3.35 270)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 13 "unconnected-(X7-Pad2)")
			(pintype "passive+no_connect")
			(solder_mask_margin 0.102)
		)
		(pad "3" smd rect
			(at -3.25 -3.35 270)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "4" smd rect
			(at -2.75 -3.35 270)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 14 "unconnected-(X7-Pad4)")
			(pintype "passive+no_connect")
			(solder_mask_margin 0.102)
		)
		(pad "5" smd rect
			(at -2.25 -3.35 270)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 15 "unconnected-(X7-Pad5)")
			(pintype "passive+no_connect")
			(solder_mask_margin 0.102)
		)
		(pad "6" smd rect
			(at -1.75 -3.35 270)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 16 "unconnected-(X7-Pad6)")
			(pintype "passive+no_connect")
			(solder_mask_margin 0.102)
		)
		(pad "7" smd rect
			(at -1.25 -3.35 270)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 17 "unconnected-(X7-Pad7)")
			(pintype "passive+no_connect")
			(solder_mask_margin 0.102)
		)
		(pad "8" smd rect
			(at -0.75 -3.35 270)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 18 "unconnected-(X7-Pad8)")
			(pintype "passive+no_connect")
			(solder_mask_margin 0.102)
		)
		(pad "9" smd rect
			(at -0.25 -3.35 270)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 19 "unconnected-(X7-Pad9)")
			(pintype "passive+no_connect")
			(solder_mask_margin 0.102)
		)
		(pad "10" smd rect
			(at 0.25 -3.35 270)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 83 "/AMP_SD")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "11" smd rect
			(at 0.75 -3.35 270)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 65 "/DOUT")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "12" smd rect
			(at 1.25 -3.35 270)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 64 "/DIN")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "13" smd rect
			(at 1.75 -3.35 270)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 8 "/SCL")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "14" smd rect
			(at 2.25 -3.35 270)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 10 "/SDA")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "15" smd rect
			(at 2.75 -3.35 270)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 9 "/AUDIO_INT")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "16" smd rect
			(at 3.25 -3.35 270)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 20 "unconnected-(X7-Pad16)")
			(pintype "passive+no_connect")
			(solder_mask_margin 0.102)
		)
		(pad "17" smd rect
			(at 3.75 -3.35 270)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 3 "/BCLK")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "18" smd rect
			(at 4.25 -3.35 270)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 5 "/LRCLK")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "Z1" smd rect
			(at -6.05 -0.6 270)
			(size 2 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "Z2" smd rect
			(at 6.05 -0.6 270)
			(size 2 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
		(model "${KIPRJMOD}/capstone-project.pretty/3dmodels/687118149022+(rev1).step"
			(offset
				(xyz 0 0.5 1.15)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -0 -0 -0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 197.252647 114.668158)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R12"
			(at 0 -1.292258 0)
			(layer "F.SilkS")
		)
		(property "Value" "10k"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "testbed-mcu copy.kicad_sch")
		(attr smd)
		(pad "1" smd roundrect
			(at -0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 78 "/DTR")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 41 "Net-(Q1-B)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "F.Cu")
		(at 187.39911 129.64159)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP4"
			(at 0 -1.448 0)
			(layer "F.SilkS")
		)
		(property "Value" "TestPoint"
			(at 0 1.55 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/")
		(sheetfile "testbed-mcu copy.kicad_sch")
		(attr exclude_from_pos_files)
		(fp_text user "${REFERENCE}"
			(at 0 -1.45 0)
			(layer "F.Fab")
		)
		(pad "1" smd circle
			(at 0 0)
			(size 1 1)
			(layers "F.Cu" "F.Mask")
			(net 84 "+3.3V")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "capstone-project:LOGO"
		(layer "F.Cu")
		(at 209.905327 116.652728)
		(property "Reference" "G"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "LOGO"
			(at 0.75 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr smd board_only exclude_from_pos_files exclude_from_bom)
		(embedded_fonts no)
	)
	(footprint "Package_TO_SOT_SMD:SOT-23"
		(layer "F.Cu")
		(at 199.704691 117.364689 90)
		(descr "SOT, 3 Pin (JEDEC TO-236 Var AB https://www.jedec.org/document_search?search_api_views_fulltext=TO-236), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOT TO_SOT_SMD")
		(property "Reference" "Q1"
			(at 0.015616 2.533253 0)
			(layer "F.SilkS")
		)
		(property "Value" "SS8050"
			(at 0 2.4 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "http://www.secosgmbh.com/datasheet/products/SSMPTransistor/SOT-23/SS8050.pdf"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "General Purpose NPN Transistor, 1.5A Ic, 25V Vce, SOT-23"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SOT?23*")
		(sheetname "/")
		(sheetfile "testbed-mcu copy.kicad_sch")
		(attr smd)
		(pad "1" smd roundrect
			(at -0.9375 -0.95 90)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 41 "Net-(Q1-B)")
			(pinfunction "B")
			(pintype "input")
		)
		(pad "2" smd roundrect
			(at -0.9375 0.95 90)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 77 "/RTS")
			(pinfunction "E")
			(pintype "passive")
		)
		(pad "3" smd roundrect
			(at 0.9375 0 90)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "/EN")
			(pinfunction "C")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 206.274162 125.08652 90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R10"
			(at 0 1.27 90)
			(layer "F.SilkS")
		)
		(property "Value" "680"
			(at 0 1.43 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "PWR LED R"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "testbed-mcu copy.kicad_sch")
		(attr smd)
		(pad "1" smd roundrect
			(at -0.825 0 90)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 84 "+3.3V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0 90)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 69 "Net-(D2-A)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "capstone-project:Adafruit EYESPI FPC Connector"
		(layer "F.Cu")
		(at 175.768 135.636)
		(descr "WR-FPC SMT ZIF Horizontal Hinge Type")
		(tags "EYESPI, FPC")
		(property "Reference" "X5"
			(at 7.874 2.032 0)
			(layer "F.SilkS")
		)
		(property "Value" "EYESPI"
			(at 0 4.064 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://www.we-online.com/components/products/datasheet/687118149022.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "WR-FPC SMT ZIF Horizontal Hinge Type"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Assignment" "PSU_I2C+INT"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "testbed-mcu copy.kicad_sch")
		(attr smd allow_soldermask_bridges)
		(pad "1" smd rect
			(at -4.25 -3.35)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 84 "+3.3V")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd rect
			(at -3.75 -3.35)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 84 "+3.3V")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "3" smd rect
			(at -3.25 -3.35)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "4" smd rect
			(at -2.75 -3.35)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 47 "unconnected-(X5-Pad4)")
			(pintype "passive+no_connect")
			(solder_mask_margin 0.102)
		)
		(pad "5" smd rect
			(at -2.25 -3.35)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 48 "unconnected-(X5-Pad5)")
			(pintype "passive+no_connect")
			(solder_mask_margin 0.102)
		)
		(pad "6" smd rect
			(at -1.75 -3.35)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 49 "unconnected-(X5-Pad6)")
			(pintype "passive+no_connect")
			(solder_mask_margin 0.102)
		)
		(pad "7" smd rect
			(at -1.25 -3.35)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 84 "+3.3V")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "8" smd rect
			(at -0.75 -3.35)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 50 "unconnected-(X5-Pad8)")
			(pintype "passive+no_connect")
			(solder_mask_margin 0.102)
		)
		(pad "9" smd rect
			(at -0.25 -3.35)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 87 "/BAT_LOW")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "10" smd rect
			(at 0.25 -3.35)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 84 "+3.3V")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "11" smd rect
			(at 0.75 -3.35)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "12" smd rect
			(at 1.25 -3.35)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "13" smd rect
			(at 1.75 -3.35)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 8 "/SCL")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "14" smd rect
			(at 2.25 -3.35)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 10 "/SDA")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "15" smd rect
			(at 2.75 -3.35)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 6 "/BMS_INT")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "16" smd rect
			(at 3.25 -3.35)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "17" smd rect
			(at 3.75 -3.35)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 62 "/D+")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "18" smd rect
			(at 4.25 -3.35)
			(size 0.3 1.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 61 "/D-")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "Z1" smd rect
			(at -6.05 -0.6)
			(size 2 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "Z2" smd rect
			(at 6.05 -0.6)
			(size 2 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "GND")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
		(model "${KIPRJMOD}/capstone-project.pretty/3dmodels/687118149022+(rev1).step"
			(offset
				(xyz 0 0.5 1.15)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -0 -0 -0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "F.Cu")
		(at 157.48 87.884)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP6"
			(at 0 -1.448 0)
			(layer "F.SilkS")
		)
		(property "Value" "TestPoint"
			(at 0 1.55 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/")
		(sheetfile "testbed-mcu copy.kicad_sch")
		(attr exclude_from_pos_files)
		(pad "1" smd circle
			(at 0 0)
			(size 1 1)
			(layers "F.Cu" "F.Mask")
			(net 84 "+3.3V")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 205.5 106.3 90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R2"
			(at 2 0 180)
			(layer "F.SilkS")
		)
		(property "Value" "10k"
			(at 0 1.43 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "testbed-mcu copy.kicad_sch")
		(attr smd)
		(pad "1" smd roundrect
			(at -0.825 0 90)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "/EN")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0 90)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 84 "+3.3V")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 202.7 91.7 180)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R8"
			(at -2.22511 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "0"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "testbed-mcu copy.kicad_sch")
		(attr smd)
		(pad "1" smd roundrect
			(at -0.825 0 180)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 73 "RXD0")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0 180)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 81 "Net-(U8-RXD0)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "LOGO"
		(layer "B.Cu")
		(at 151.9 137 180)
		(property "Reference" "G***"
			(at 0 0 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "LOGO"
			(at 0.75 0 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(attr board_only exclude_from_pos_files exclude_from_bom)
		(embedded_fonts no)
	)
	(footprint "LOGO"
		(layer "B.Cu")
		(at 151.600011 87.200001 180)
		(property "Reference" "G***"
			(at 0 0 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "LOGO"
			(at 0.75 0 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(attr board_only exclude_from_pos_files exclude_from_bom)
		(embedded_fonts no)
	)
	(footprint "LOGO"
		(layer "B.Cu")
		(at 213 118.65 180)
		(property "Reference" "G***"
			(at 0 0 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "LOGO"
			(at 0.75 0 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(attr board_only exclude_from_pos_files exclude_from_bom)
		(embedded_fonts no)
	)
	(gr_line
		(start 218.711069 133.60223)
		(end 215.9 136.144)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 149.86 137.668)
		(end 149.86 86.36)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 215.9 136.144)
		(end 215.9 137.668)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 218.711069 100.83623)
		(end 218.711069 133.60223)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 215.9 137.668)
		(mid 215.60242 138.38642)
		(end 214.884 138.684)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 149.86 86.36)
		(mid 150.15758 85.64158)
		(end 150.876 85.344)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 214.884 138.684)
		(end 150.876 138.684)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 215.9 98.298)
		(end 218.711069 100.83623)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 150.876 138.684)
		(mid 150.15758 138.38642)
		(end 149.86 137.668)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 214.376 85.344)
		(end 215.9 86.868)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 150.876 85.344)
		(end 214.376 85.344)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 215.9 86.868)
		(end 215.9 98.298)
		(layer "Edge.Cuts")
	)
	(gr_text "OPENAIR LAB"
		(at 204.8 121.1 0)
		(layer "F.SilkS" knockout)
	)
	(gr_text "I2C"
		(at 210.82 86.868 0)
		(layer "F.SilkS")
	)
	(gr_text "TXD"
		(at 202.530062 123.895283 0)
		(layer "F.SilkS")
	)
	(gr_text "Audio Connector"
		(at 157.6 105 270)
		(layer "F.SilkS")
	)
	(gr_text "Power\nConnector"
		(at 172.212 130.048 0)
		(layer "F.SilkS")
	)
	(gr_text "HMI Connector\n"
		(at 157.988 121.412 270)
		(layer "F.SilkS")
	)
	(gr_text "Adrianne Quick, Zachary Potersnak, Eric Mutton\n                FALL 2025 Rev B\n                 MCU MODULINO"
		(at 185.6 137.7 0)
		(layer "F.SilkS" knockout)
	)
	(gr_text "RF \nConnector"
		(at 157.988 90.424 270)
		(layer "F.SilkS")
	)
	(gr_text "RXD"
		(at 202.276062 130.753283 0)
		(layer "F.SilkS")
	)
	(gr_text "ESP32 Modulino"
		(at 14.82746 15.119573 0)
		(layer "F.SilkS")
	)
	(gr_text "TX"
		(at 207.6 87.7 90)
		(layer "B.SilkS")
	)
	(gr_text "did.. did we do it?"
		(at 160.8 138.1 0)
		(layer "B.SilkS")
	)
	(gr_text "3.3V\n"
		(at 204.4 87.8 90)
		(layer "B.SilkS")
	)
	(gr_text "Holy Moly"
		(at 214.95 137.9 0)
		(layer "B.SilkS")
	)
	(gr_text "SDA"
		(at 205.5 87.7 90)
		(layer "B.SilkS")
	)
	(gr_text "GND"
		(at 209.6 87.7 90)
		(layer "B.SilkS")
	)
	(gr_text "RX"
		(at 208.6 87.7 90)
		(layer "B.SilkS")
	)
	(gr_text "SCL"
		(at 206.6 87.7 90)
		(layer "B.SilkS")
	)
	(zone
		(net 1)
		(net_name "GND")
		(layers "F.Cu" "B.Cu" "In1.Cu" "In2.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0.2)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 149.86 85.344) (xy 215.9 85.344) (xy 215.9 98.277286) (xy 218.704512 100.820418) (xy 218.712234 133.579441)
				(xy 215.9 136.144) (xy 215.912107 137.764862) (xy 215.805339 138.105004) (xy 215.600243 138.388985)
				(xy 215.253156 138.617746) (xy 214.961287 138.688741) (xy 149.86 138.684)
			)
		)
	)
	(zone
		(net 84)
		(net_name "+3.3V")
		(layer "In2.Cu")
		(hatch edge 0.5)
		(priority 1)
		(connect_pads
			(clearance 0.2)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 152.34711 89.50959) (xy 157.17311 89.50959) (xy 157.17311 131.16559) (xy 183.08111 131.16559)
				(xy 183.08111 135.99159) (xy 152.34711 135.99159)
			)
		)
	)
	(embedded_fonts no)
)
