# Design Rule Verification Report

Date: |  | 4/15/2026
Time: |  | 9:22:16 AM
Elapsed Time: |  | 00:00:01
Filename: |  | C:\Users\brand\AppData\Local\TempReleases\Snapshot\1\2.4 GHz Radio Transmitter.PcbDoc
Warnings: |  | 0
Rule Violations: |  | 0
Waived Violations: |  | 142

## Summary

Warnings | Count
--- | ---
Total | 0

Rule Violations | Count
--- | ---
Clearance Constraint (Gap=5mil) (All),(All) | 0
Clearance Constraint (Gap=10mil) (InPolygon),(All) | 0
Short-Circuit Constraint (Allowed=No) (All),(All) | 0
Un-Routed Net Constraint ( (All) ) | 0
Modified Polygon (Allow modified: No), (Allow shelved: No) | 0
Width Constraint (Min=6mil) (Max=400mil) (Preferred=8mil) (All) | 0
Width Constraint (Min=20mil) (Max=40mil) (Preferred=30mil) (InNetClass('Power')) | 0
Width Constraint (Min=10mil) (Max=30mil) (Preferred=20mil) (InNet('GND')) | 0
Width Constraint (Min=10mil) (Max=30mil) (Preferred=20mil) (InNetClass('3V3')) | 0
Routing Topology Rule(Topology=Shortest) (All) | 0
Power Plane Connect Rule(Relief Connect )(Expansion=4mil) (Conductor Width=6mil) (Air Gap=6mil) (Entries=4) (All) | 0
Minimum Annular Ring (Minimum=4mil) (All) | 0
Hole Size Constraint (Min=10mil) (Max=265mil) (All) | 0
Hole To Hole Clearance (Gap=10mil) (All),(All) | 0
Minimum Solder Mask Sliver (Gap=0mil) (All),(All) | 0
Silk To Solder Mask (Clearance=5mil) (IsPad),(All) | 0
Silk to Silk (Clearance=0mil) (All),(All) | 0
Net Antennae (Tolerance=0mil) (All) | 0
Board Clearance Constraint (Gap=0mil) (All) | 0
Height Constraint (Min=0mil) (Max=1000mil) (Prefered=500mil) (All) | 0
Total | 0

Waived Violations | Count
--- | ---
Clearance Constraint (Gap=5mil) (All),(All) | 73
Short-Circuit Constraint (Allowed=No) (All),(All) | 52
Minimum Annular Ring (Minimum=4mil) (All) | 5
Hole Size Constraint (Min=10mil) (Max=265mil) (All) | 9
Board Clearance Constraint (Gap=0mil) (All) | 3
Total | 142

## Rule Violations

## Waived Violations

Clearance Constraint (Gap=5mil) (All),(All)
Clearance Constraint: (Collision < 5mil) Between Pad L1-1(658.82mil,-1507.87mil) on Top Layer And Region (0 hole(s)) Top Layer Waived by Brandon Velasquez at 4/10/2026 4:13:25 PM
Clearance Constraint: (Collision < 5mil) Between Pad L1-2(734.608mil,-1516.236mil) on Top Layer And Region (0 hole(s)) Top Layer Waived by Brandon Velasquez at 4/10/2026 4:13:48 PM
Clearance Constraint: (Collision < 5mil) Between Pad L1-3(734.608mil,-1373.028mil) on Top Layer And Region (0 hole(s)) Top Layer Waived by Brandon Velasquez at 4/10/2026 4:15:48 PM
Clearance Constraint: (Collision < 5mil) Between Pad L1-4(658.82mil,-1398.126mil) on Top Layer And Region (0 hole(s)) Top Layer Waived by Brandon Velasquez at 4/10/2026 4:15:32 PM
Clearance Constraint: (Collision < 5mil) Between Pad L2-1(2136.664mil,-1451.364mil) on Top Layer And Region (0 hole(s)) Top Layer Waived by Brandon Velasquez at 4/10/2026 4:17:09 PM
Clearance Constraint: (Collision < 5mil) Between Pad L2-2(2212.452mil,-1459.73mil) on Top Layer And Region (0 hole(s)) Top Layer Waived by Brandon Velasquez at 4/10/2026 4:16:46 PM
Clearance Constraint: (Collision < 5mil) Between Pad L2-3(2212.452mil,-1316.522mil) on Top Layer And Region (0 hole(s)) Top Layer Waived by Brandon Velasquez at 4/10/2026 4:16:27 PM
Clearance Constraint: (Collision < 5mil) Between Pad L2-4(2136.664mil,-1341.62mil) on Top Layer And Region (0 hole(s)) Top Layer Waived by Brandon Velasquez at 4/10/2026 4:16:07 PM
Clearance Constraint: (Collision < 5mil) Between Pad L3-1(3656.664mil,-1476.364mil) on Top Layer And Region (0 hole(s)) Top Layer Waived by Brandon Velasquez at 4/10/2026 4:18:59 PM
Clearance Constraint: (Collision < 5mil) Between Pad L3-2(3732.452mil,-1484.73mil) on Top Layer And Region (0 hole(s)) Top Layer Waived by Brandon Velasquez at 4/10/2026 4:18:46 PM
Clearance Constraint: (Collision < 5mil) Between Pad L3-3(3732.452mil,-1341.522mil) on Top Layer And Region (0 hole(s)) Top Layer Waived by Brandon Velasquez at 4/10/2026 4:18:38 PM
Clearance Constraint: (Collision < 5mil) Between Pad L3-4(3656.664mil,-1366.62mil) on Top Layer And Region (0 hole(s)) Top Layer Waived by Brandon Velasquez at 4/10/2026 4:17:46 PM
Clearance Constraint: (Collision < 5mil) Between Pad L4-1(34.143mil,-1429.754mil) on Top Layer And Region (0 hole(s)) Top Layer Waived by Brandon Velasquez at 4/10/2026 9:46:29 PM
Clearance Constraint: (Collision < 5mil) Between Pad L4-2(42.509mil,-1353.966mil) on Top Layer And Region (0 hole(s)) Top Layer Waived by Brandon Velasquez at 4/10/2026 9:46:05 PM
Clearance Constraint: (Collision < 5mil) Between Pad L4-3(-100.699mil,-1353.966mil) on Top Layer And Region (0 hole(s)) Top Layer Waived by Brandon Velasquez at 4/10/2026 9:45:48 PM
Clearance Constraint: (Collision < 5mil) Between Pad L4-4(-75.601mil,-1429.754mil) on Top Layer And Region (0 hole(s)) Top Layer Waived by Brandon Velasquez at 4/10/2026 9:46:42 PM
Clearance Constraint: (Collision < 5mil) Between Pad L5-3(5283.73mil,-1460.138mil) on Top Layer And Region (0 hole(s)) Top Layer Waived by Brandon Velasquez at 4/6/2026 1:54:49 PM
Clearance Constraint: (Collision < 5mil) Between Pad L5-4(5308.828mil,-1535.926mil) on Top Layer And Region (0 hole(s)) Top Layer Waived by Brandon Velasquez at 4/6/2026 1:54:40 PM
Clearance Constraint: (Collision < 5mil) Between Pad L7-3(631.604mil,961.368mil) on Top Layer And Region (0 hole(s)) Top Layer Waived by Brandon Velasquez at 4/6/2026 1:52:43 PM
Clearance Constraint: (4.744mil < 5mil) Between Pad U8-4(1149.274mil,-485.728mil) on Top Layer And Track (1154.636mil,-504.682mil)(1191.5mil,-504.682mil) on Top Layer Waived by Brandon Velasquez at 4/6/2026 1:37:34 PM
Clearance Constraint: (4.78mil < 5mil) Between Pad U9-2(2850.574mil,-650.056mil) on Top Layer And Track (2870.26mil,-687.98mil)(2870.26mil,-650.056mil) on Top Layer Waived by Brandon Velasquez at 4/6/2026 1:38:55 PM
Clearance Constraint: (4.779mil < 5mil) Between Pad U9-4(2889.944mil,-650.056mil) on Top Layer And Track (2870.26mil,-687.98mil)(2870.26mil,-650.056mil) on Top Layer Waived by Brandon Velasquez at 4/6/2026 1:38:57 PM
Clearance Constraint: (4.779mil < 5mil) Between Pad U9-7(2955mil,-624.37mil) on Top Layer And Track (2955mil,-604.686mil)(3077.792mil,-604.686mil) on Top Layer Waived by Brandon Velasquez at 4/6/2026 5:06:08 PM
Clearance Constraint: (4.78mil < 5mil) Between Pad U9-9(2955mil,-585mil) on Top Layer And Track (2955mil,-604.686mil)(3077.792mil,-604.686mil) on Top Layer Waived by Brandon Velasquez at 4/6/2026 5:06:10 PM
Clearance Constraint: (Collision < 5mil) Between Region (0 hole(s)) Top Layer And Track (-100.699mil,-1353.966mil)(-100.699mil,-1092.631mil) on Top Layer Waived by Brandon Velasquez at 4/10/2026 9:45:46 PM
Clearance Constraint: (Collision < 5mil) Between Region (0 hole(s)) Top Layer And Track (2136.664mil,-1341.62mil)(2136.664mil,-1250.97mil) on Top Layer Waived by Brandon Velasquez at 4/10/2026 9:48:32 PM
Clearance Constraint: (Collision < 5mil) Between Region (0 hole(s)) Top Layer And Track (2136.664mil,-1495.97mil)(2136.664mil,-1451.364mil) on Top Layer Waived by Brandon Velasquez at 4/10/2026 9:49:19 PM
Clearance Constraint: (Collision < 5mil) Between Region (0 hole(s)) Top Layer And Track (2197.749mil,-1495.646mil)(2206.536mil,-1486.859mil) on Top Layer Waived by Brandon Velasquez at 4/10/2026 9:48:57 PM
Clearance Constraint: (Collision < 5mil) Between Region (0 hole(s)) Top Layer And Track (2206.536mil,-1472.716mil)(2212.452mil,-1466.8mil) on Top Layer Waived by Brandon Velasquez at 4/10/2026 9:48:55 PM
Clearance Constraint: (Collision < 5mil) Between Region (0 hole(s)) Top Layer And Track (2206.536mil,-1486.859mil)(2206.536mil,-1472.716mil) on Top Layer Waived by Brandon Velasquez at 4/10/2026 9:48:59 PM
Clearance Constraint: (Collision < 5mil) Between Region (0 hole(s)) Top Layer And Track (2212.452mil,-1316.522mil)(2470.598mil,-1316.522mil) on Top Layer Waived by Brandon Velasquez at 4/10/2026 9:48:44 PM
Clearance Constraint: (Collision < 5mil) Between Region (0 hole(s)) Top Layer And Track (2212.452mil,-1466.8mil)(2212.452mil,-1459.73mil) on Top Layer Waived by Brandon Velasquez at 4/10/2026 9:49:01 PM
Clearance Constraint: (Collision < 5mil) Between Region (0 hole(s)) Top Layer And Track (34.143mil,-1429.754mil)(118.284mil,-1429.754mil) on Top Layer Waived by Brandon Velasquez at 4/10/2026 9:46:31 PM
Clearance Constraint: (Collision < 5mil) Between Region (0 hole(s)) Top Layer And Track (3656.664mil,-1325.97mil)(3656.664mil,-1244.771mil) on Top Layer Waived by Brandon Velasquez at 4/10/2026 9:52:33 PM
Clearance Constraint: (Collision < 5mil) Between Region (0 hole(s)) Top Layer And Track (3656.664mil,-1366.62mil)(3656.664mil,-1325.97mil) on Top Layer Waived by Brandon Velasquez at 4/10/2026 9:52:36 PM
Clearance Constraint: (Collision < 5mil) Between Region (0 hole(s)) Top Layer And Track (3656.664mil,-1565.97mil)(3656.664mil,-1476.364mil) on Top Layer Waived by Brandon Velasquez at 4/10/2026 9:53:47 PM
Clearance Constraint: (Collision < 5mil) Between Region (0 hole(s)) Top Layer And Track (3732.452mil,-1341.522mil)(4038.805mil,-1341.522mil) on Top Layer Waived by Brandon Velasquez at 4/10/2026 9:53:23 PM
Clearance Constraint: (Collision < 5mil) Between Region (0 hole(s)) Top Layer And Track (3732.452mil,-1571.758mil)(3732.452mil,-1484.73mil) on Top Layer Waived by Brandon Velasquez at 4/10/2026 9:53:34 PM
Clearance Constraint: (Collision < 5mil) Between Region (0 hole(s)) Top Layer And Track (42.509mil,-1353.966mil)(49.579mil,-1353.966mil) on Top Layer Waived by Brandon Velasquez at 4/10/2026 9:46:14 PM
Clearance Constraint: (Collision < 5mil) Between Region (0 hole(s)) Top Layer And Track (49.579mil,-1353.966mil)(55.494mil,-1359.881mil) on Top Layer Waived by Brandon Velasquez at 4/10/2026 9:46:07 PM
Clearance Constraint: (Collision < 5mil) Between Region (0 hole(s)) Top Layer And Track (5283.73mil,-1460.138mil)(5283.73mil,-1217.887mil) on Top Layer Waived by Brandon Velasquez at 4/10/2026 9:54:15 PM
Clearance Constraint: (Collision < 5mil) Between Region (0 hole(s)) Top Layer And Track (55.494mil,-1359.881mil)(69.637mil,-1359.881mil) on Top Layer Waived by Brandon Velasquez at 4/10/2026 9:46:09 PM
Clearance Constraint: (Collision < 5mil) Between Region (0 hole(s)) Top Layer And Track (631.604mil,961.368mil)(845.321mil,961.368mil) on Top Layer Waived by Brandon Velasquez at 4/10/2026 9:54:29 PM
Clearance Constraint: (Collision < 5mil) Between Region (0 hole(s)) Top Layer And Track (658.82mil,-1514.794mil)(658.82mil,-1507.87mil) on Top Layer Waived by Brandon Velasquez at 4/10/2026 9:47:16 PM
Clearance Constraint: (Collision < 5mil) Between Region (0 hole(s)) Top Layer And Track (658.82mil,-1514.794mil)(663.259mil,-1519.234mil) on Top Layer Waived by Brandon Velasquez at 4/10/2026 9:47:11 PM
Clearance Constraint: (Collision < 5mil) Between Region (0 hole(s)) Top Layer And Track (663.259mil,-1543.365mil)(663.259mil,-1519.234mil) on Top Layer Waived by Brandon Velasquez at 4/10/2026 9:47:13 PM
Clearance Constraint: (Collision < 5mil) Between Region (0 hole(s)) Top Layer And Track (663.259mil,-1543.365mil)(672.046mil,-1552.152mil) on Top Layer Waived by Brandon Velasquez at 4/10/2026 9:47:15 PM
Clearance Constraint: (Collision < 5mil) Between Region (0 hole(s)) Top Layer And Track (69.637mil,-1359.881mil)(89.756mil,-1380mil) on Top Layer Waived by Brandon Velasquez at 4/10/2026 9:46:11 PM
Clearance Constraint: (Collision < 5mil) Between Region (0 hole(s)) Top Layer And Track (717.757mil,-1554.3mil)(728.692mil,-1543.365mil) on Top Layer Waived by Brandon Velasquez at 4/10/2026 9:47:43 PM
Clearance Constraint: (Collision < 5mil) Between Region (0 hole(s)) Top Layer And Track (728.692mil,-1529.222mil)(734.608mil,-1523.306mil) on Top Layer Waived by Brandon Velasquez at 4/10/2026 9:47:41 PM
Clearance Constraint: (Collision < 5mil) Between Region (0 hole(s)) Top Layer And Track (728.692mil,-1543.365mil)(728.692mil,-1529.222mil) on Top Layer Waived by Brandon Velasquez at 4/10/2026 9:47:36 PM
Clearance Constraint: (Collision < 5mil) Between Region (0 hole(s)) Top Layer And Track (734.608mil,-1373.028mil)(739.832mil,-1367.803mil) on Top Layer Waived by Brandon Velasquez at 4/10/2026 9:48:01 PM
Clearance Constraint: (Collision < 5mil) Between Region (0 hole(s)) Top Layer And Track (734.608mil,-1523.306mil)(734.608mil,-1516.236mil) on Top Layer Waived by Brandon Velasquez at 4/10/2026 9:47:39 PM
Clearance Constraint: (Collision < 5mil) Between Region (0 hole(s)) Top Layer And Track (739.832mil,-1367.803mil)(846.987mil,-1367.803mil) on Top Layer Waived by Brandon Velasquez at 4/10/2026 9:48:10 PM
Clearance Constraint: (Collision < 5mil) Between Region (0 hole(s)) Top Layer And Via (5310mil,-1535.931mil) from Top Layer to Bottom Layer Waived by Brandon Velasquez at 4/10/2026 9:53:58 PM
Clearance Constraint: (Collision < 5mil) Between Region (0 hole(s)) Top Layer And Via (658.82mil,-1398.126mil) from Top Layer to Bottom Layer Waived by Brandon Velasquez at 4/10/2026 9:46:59 PM
Clearance Constraint: (Collision < 5mil) Between Region (0 hole(s)) Top Layer And Via (-75.601mil,-1429.754mil) from Top Layer to Bottom Layer Waived by Brandon Velasquez at 4/10/2026 9:46:40 PM
Clearance Constraint: (4.684mil < 5mil) Between Track (2859.553mil,-419.553mil)(2870.26mil,-430.26mil) on Top Layer And Track (2889.944mil,-500.26mil)(2889.944mil,-370.49mil) on Top Layer Waived by Brandon Velasquez at 4/6/2026 5:05:33 PM
Clearance Constraint: (4.684mil < 5mil) Between Track (2870.26mil,-500.26mil)(2870.26mil,-430.26mil) on Top Layer And Track (2889.944mil,-500.26mil)(2889.944mil,-370.49mil) on Top Layer Waived by Brandon Velasquez at 4/6/2026 5:05:27 PM
Clearance Constraint: (4.684mil < 5mil) Between Track (2909.63mil,-714.197mil)(2909.63mil,-650.056mil) on Top Layer And Track (2929.314mil,-674.314mil)(2929.314mil,-650.056mil) on Top Layer Waived by Brandon Velasquez at 4/6/2026 5:05:48 PM
Clearance Constraint: (4.684mil < 5mil) Between Track (2909.63mil,-714.197mil)(2909.63mil,-650.056mil) on Top Layer And Track (2929.314mil,-674.314mil)(2940mil,-685mil) on Top Layer Waived by Brandon Velasquez at 4/6/2026 5:05:54 PM
Clearance Constraint: (4.686mil < 5mil) Between Track (2955mil,-545.63mil)(3033.594mil,-545.63mil) on Top Layer And Track (2955mil,-565.316mil)(3001.08mil,-565.316mil) on Top Layer Waived by Brandon Velasquez at 4/6/2026 5:06:20 PM
Clearance Constraint: (4.686mil < 5mil) Between Track (2955mil,-545.63mil)(3033.594mil,-545.63mil) on Top Layer And Track (3001.08mil,-565.316mil)(3009.882mil,-574.117mil) on Top Layer Waived by Brandon Velasquez at 4/6/2026 5:06:33 PM
Clearance Constraint: (4.687mil < 5mil) Between Track (2989.488mil,1160.158mil)(2989.646mil,1160mil) on Top Layer And Track (2989.488mil,1180.158mil)(2989.804mil,1179.842mil) on Top Layer Waived by Brandon Velasquez at 4/6/2026 4:29:10 PM
Clearance Constraint: (4.687mil < 5mil) Between Track (2989.488mil,1160.158mil)(2989.646mil,1160mil) on Top Layer And Track (2989.804mil,1179.842mil)(2997.736mil,1179.842mil) on Top Layer Waived by Brandon Velasquez at 4/6/2026 4:29:08 PM
Clearance Constraint: (4.842mil < 5mil) Between Track (2989.488mil,1180.158mil)(2989.804mil,1179.842mil) on Top Layer And Track (2989.646mil,1160mil)(3020.306mil,1160mil) on Top Layer Waived by Brandon Velasquez at 4/6/2026 4:29:06 PM
Clearance Constraint: (4.842mil < 5mil) Between Track (2989.646mil,1160mil)(3020.306mil,1160mil) on Top Layer And Track (2989.804mil,1179.842mil)(2997.736mil,1179.842mil) on Top Layer Waived by Brandon Velasquez at 4/6/2026 4:29:04 PM
Clearance Constraint: (4.686mil < 5mil) Between Track (3773.543mil,1356.457mil)(3795.944mil,1334.056mil) on Top Layer And Track (3815.63mil,1238.544mil)(3815.63mil,1335.63mil) on Top Layer Waived by Brandon Velasquez at 4/6/2026 11:59:15 AM
Clearance Constraint: (4.749mil < 5mil) Between Track (3773.543mil,1356.457mil)(3795.944mil,1334.056mil) on Top Layer And Track (3815.63mil,1335.63mil)(3842.087mil,1362.087mil) on Top Layer Waived by Brandon Velasquez at 4/6/2026 11:59:02 AM
Clearance Constraint: (4.686mil < 5mil) Between Track (3795.944mil,1036.366mil)(3795.944mil,1085mil) on Top Layer And Track (3815.63mil,1042.35mil)(3815.63mil,1085mil) on Top Layer Waived by Brandon Velasquez at 4/6/2026 4:27:03 PM
Clearance Constraint: (4.686mil < 5mil) Between Track (3795.944mil,1036.366mil)(3795.944mil,1085mil) on Top Layer And Track (3815.63mil,1042.35mil)(3841.456mil,1016.524mil) on Top Layer Waived by Brandon Velasquez at 4/6/2026 4:27:10 PM
Clearance Constraint: (4.686mil < 5mil) Between Track (3795.944mil,1238.544mil)(3795.944mil,1334.056mil) on Top Layer And Track (3815.63mil,1238.544mil)(3815.63mil,1335.63mil) on Top Layer Waived by Brandon Velasquez at 4/6/2026 11:59:43 AM
Clearance Constraint: (4.749mil < 5mil) Between Track (3795.944mil,1238.544mil)(3795.944mil,1334.056mil) on Top Layer And Track (3815.63mil,1335.63mil)(3842.087mil,1362.087mil) on Top Layer Waived by Brandon Velasquez at 4/6/2026 12:00:01 PM

Back to top

Short-Circuit Constraint (Allowed=No) (All),(All)
Short-Circuit Constraint: Between Pad L1-1(658.82mil,-1507.87mil) on Top Layer And Region (0 hole(s)) Top Layer Location : [X = 978.82mil][Y = 1617.13mil] Waived by Brandon Velasquez at 4/10/2026 4:13:36 PM
Short-Circuit Constraint: Between Pad L1-2(734.608mil,-1516.236mil) on Top Layer And Region (0 hole(s)) Top Layer Location : [X = 1054.608mil][Y = 1608.764mil] Waived by Brandon Velasquez at 4/10/2026 4:14:11 PM
Short-Circuit Constraint: Between Pad L1-3(734.608mil,-1373.028mil) on Top Layer And Region (0 hole(s)) Top Layer Location : [X = 1054.608mil][Y = 1751.972mil] Waived by Brandon Velasquez at 4/10/2026 4:15:54 PM
Short-Circuit Constraint: Between Pad L1-4(658.82mil,-1398.126mil) on Top Layer And Region (0 hole(s)) Top Layer Location : [X = 978.82mil][Y = 1726.874mil] Waived by Brandon Velasquez at 4/10/2026 4:15:36 PM
Short-Circuit Constraint: Between Pad L2-1(2136.664mil,-1451.364mil) on Top Layer And Region (0 hole(s)) Top Layer Location : [X = 2456.664mil][Y = 1673.636mil] Waived by Brandon Velasquez at 4/10/2026 4:17:13 PM
Short-Circuit Constraint: Between Pad L2-2(2212.452mil,-1459.73mil) on Top Layer And Region (0 hole(s)) Top Layer Location : [X = 2532.452mil][Y = 1665.27mil] Waived by Brandon Velasquez at 4/10/2026 4:16:57 PM
Short-Circuit Constraint: Between Pad L2-3(2212.452mil,-1316.522mil) on Top Layer And Region (0 hole(s)) Top Layer Location : [X = 2532.452mil][Y = 1808.478mil] Waived by Brandon Velasquez at 4/10/2026 4:16:25 PM
Short-Circuit Constraint: Between Pad L2-4(2136.664mil,-1341.62mil) on Top Layer And Region (0 hole(s)) Top Layer Location : [X = 2456.664mil][Y = 1783.38mil] Waived by Brandon Velasquez at 4/10/2026 4:16:11 PM
Short-Circuit Constraint: Between Pad L3-1(3656.664mil,-1476.364mil) on Top Layer And Region (0 hole(s)) Top Layer Location : [X = 3976.664mil][Y = 1648.636mil] Waived by Brandon Velasquez at 4/10/2026 4:19:02 PM
Short-Circuit Constraint: Between Pad L3-2(3732.452mil,-1484.73mil) on Top Layer And Region (0 hole(s)) Top Layer Location : [X = 4052.452mil][Y = 1640.27mil] Waived by Brandon Velasquez at 4/10/2026 4:18:50 PM
Short-Circuit Constraint: Between Pad L3-3(3732.452mil,-1341.522mil) on Top Layer And Region (0 hole(s)) Top Layer Location : [X = 4052.452mil][Y = 1783.478mil] Waived by Brandon Velasquez at 4/10/2026 4:18:34 PM
Short-Circuit Constraint: Between Pad L3-4(3656.664mil,-1366.62mil) on Top Layer And Region (0 hole(s)) Top Layer Location : [X = 3976.664mil][Y = 1758.38mil] Waived by Brandon Velasquez at 4/10/2026 4:18:24 PM
Short-Circuit Constraint: Between Pad L4-1(34.143mil,-1429.754mil) on Top Layer And Region (0 hole(s)) Top Layer Location : [X = 354.143mil][Y = 1695.246mil] Waived by Brandon Velasquez at 4/10/2026 9:46:33 PM
Short-Circuit Constraint: Between Pad L4-2(42.509mil,-1353.966mil) on Top Layer And Region (0 hole(s)) Top Layer Location : [X = 362.509mil][Y = 1771.034mil] Waived by Brandon Velasquez at 4/10/2026 9:46:17 PM
Short-Circuit Constraint: Between Pad L4-3(-100.699mil,-1353.966mil) on Top Layer And Region (0 hole(s)) Top Layer Location : [X = 219.301mil][Y = 1771.034mil] Waived by Brandon Velasquez at 4/10/2026 9:45:51 PM
Short-Circuit Constraint: Between Pad L4-4(-75.601mil,-1429.754mil) on Top Layer And Region (0 hole(s)) Top Layer Location : [X = 244.399mil][Y = 1695.246mil] Waived by Brandon Velasquez at 4/10/2026 9:46:46 PM
Short-Circuit Constraint: Between Pad L5-3(5283.73mil,-1460.138mil) on Top Layer And Region (0 hole(s)) Top Layer Location : [X = 5603.73mil][Y = 1664.862mil] Waived by Brandon Velasquez at 4/6/2026 1:54:53 PM
Short-Circuit Constraint: Between Pad L5-4(5308.828mil,-1535.926mil) on Top Layer And Region (0 hole(s)) Top Layer Location : [X = 5628.828mil][Y = 1589.074mil] Waived by Brandon Velasquez at 4/10/2026 9:54:04 PM
Short-Circuit Constraint: Between Pad L7-3(631.604mil,961.368mil) on Top Layer And Region (0 hole(s)) Top Layer Location : [X = 951.604mil][Y = 4086.368mil] Waived by Brandon Velasquez at 4/6/2026 1:52:47 PM
Short-Circuit Constraint: Between Region (0 hole(s)) Top Layer And Track (-100.699mil,-1353.966mil)(-100.699mil,-1092.631mil) on Top Layer Location : [X = 219.301mil][Y = 1798.316mil] Waived by Brandon Velasquez at 4/10/2026 9:45:50 PM
Short-Circuit Constraint: Between Region (0 hole(s)) Top Layer And Track (2136.664mil,-1341.62mil)(2136.664mil,-1250.97mil) on Top Layer Location : [X = 2456.664mil][Y = 1798.851mil] Waived by Brandon Velasquez at 4/10/2026 9:48:35 PM
Short-Circuit Constraint: Between Region (0 hole(s)) Top Layer And Track (2136.664mil,-1495.97mil)(2136.664mil,-1451.364mil) on Top Layer Location : [X = 2456.664mil][Y = 1664.038mil] Waived by Brandon Velasquez at 4/10/2026 9:49:22 PM
Short-Circuit Constraint: Between Region (0 hole(s)) Top Layer And Track (2197.749mil,-1495.646mil)(2206.536mil,-1486.859mil) on Top Layer Location : [X = 2526.429mil][Y = 1646.291mil] Waived by Brandon Velasquez at 4/10/2026 9:49:10 PM
Short-Circuit Constraint: Between Region (0 hole(s)) Top Layer And Track (2206.536mil,-1472.716mil)(2212.452mil,-1466.8mil) on Top Layer Location : [X = 2529.494mil][Y = 1656.32mil] Waived by Brandon Velasquez at 4/10/2026 9:49:04 PM
Short-Circuit Constraint: Between Region (0 hole(s)) Top Layer And Track (2206.536mil,-1486.859mil)(2206.536mil,-1472.716mil) on Top Layer Location : [X = 2526.536mil][Y = 1653.362mil] Waived by Brandon Velasquez at 4/10/2026 9:49:08 PM
Short-Circuit Constraint: Between Region (0 hole(s)) Top Layer And Track (2212.452mil,-1316.522mil)(2470.598mil,-1316.522mil) on Top Layer Location : [X = 2559.733mil][Y = 1808.478mil] Waived by Brandon Velasquez at 4/10/2026 9:48:47 PM
Short-Circuit Constraint: Between Region (0 hole(s)) Top Layer And Track (2212.452mil,-1466.8mil)(2212.452mil,-1459.73mil) on Top Layer Location : [X = 2532.452mil][Y = 1661.735mil] Waived by Brandon Velasquez at 4/10/2026 9:49:12 PM
Short-Circuit Constraint: Between Region (0 hole(s)) Top Layer And Track (34.143mil,-1429.754mil)(118.284mil,-1429.754mil) on Top Layer Location : [X = 363.74mil][Y = 1695.246mil] Waived by Brandon Velasquez at 4/10/2026 9:46:34 PM
Short-Circuit Constraint: Between Region (0 hole(s)) Top Layer And Track (3656.664mil,-1325.97mil)(3656.664mil,-1244.771mil) on Top Layer Location : [X = 3976.664mil][Y = 1794.176mil] Waived by Brandon Velasquez at 4/10/2026 9:52:39 PM
Short-Circuit Constraint: Between Region (0 hole(s)) Top Layer And Track (3656.664mil,-1366.62mil)(3656.664mil,-1325.97mil) on Top Layer Location : [X = 3976.664mil][Y = 1773.851mil] Waived by Brandon Velasquez at 4/10/2026 9:52:40 PM
Short-Circuit Constraint: Between Region (0 hole(s)) Top Layer And Track (3656.664mil,-1565.97mil)(3656.664mil,-1476.364mil) on Top Layer Location : [X = 3976.664mil][Y = 1639.038mil] Waived by Brandon Velasquez at 4/10/2026 9:53:44 PM
Short-Circuit Constraint: Between Region (0 hole(s)) Top Layer And Track (3732.452mil,-1341.522mil)(4038.805mil,-1341.522mil) on Top Layer Location : [X = 4079.733mil][Y = 1783.478mil] Waived by Brandon Velasquez at 4/10/2026 9:53:26 PM
Short-Circuit Constraint: Between Region (0 hole(s)) Top Layer And Track (3732.452mil,-1571.758mil)(3732.452mil,-1484.73mil) on Top Layer Location : [X = 4052.452mil][Y = 1634.855mil] Waived by Brandon Velasquez at 4/10/2026 9:53:37 PM
Short-Circuit Constraint: Between Region (0 hole(s)) Top Layer And Track (42.509mil,-1353.966mil)(49.579mil,-1353.966mil) on Top Layer Location : [X = 366.044mil][Y = 1771.034mil] Waived by Brandon Velasquez at 4/10/2026 9:46:15 PM
Short-Circuit Constraint: Between Region (0 hole(s)) Top Layer And Track (49.579mil,-1353.966mil)(55.494mil,-1359.881mil) on Top Layer Location : [X = 371.458mil][Y = 1768.076mil] Waived by Brandon Velasquez at 4/10/2026 9:46:19 PM
Short-Circuit Constraint: Between Region (0 hole(s)) Top Layer And Track (5283.73mil,-1460.138mil)(5283.73mil,-1217.887mil) on Top Layer Location : [X = 5603.73mil][Y = 1692.143mil] Waived by Brandon Velasquez at 4/10/2026 9:54:18 PM
Short-Circuit Constraint: Between Region (0 hole(s)) Top Layer And Track (55.494mil,-1359.881mil)(69.637mil,-1359.881mil) on Top Layer Location : [X = 374.416mil][Y = 1765.119mil] Waived by Brandon Velasquez at 4/10/2026 9:46:21 PM
Short-Circuit Constraint: Between Region (0 hole(s)) Top Layer And Track (631.604mil,961.368mil)(845.321mil,961.368mil) on Top Layer Location : [X = 954.525mil][Y = 4086.368mil] Waived by Brandon Velasquez at 4/10/2026 9:54:32 PM
Short-Circuit Constraint: Between Region (0 hole(s)) Top Layer And Track (658.82mil,-1514.794mil)(658.82mil,-1507.87mil) on Top Layer Location : [X = 978.82mil][Y = 1613.668mil] Waived by Brandon Velasquez at 4/10/2026 9:47:28 PM
Short-Circuit Constraint: Between Region (0 hole(s)) Top Layer And Track (658.82mil,-1514.794mil)(663.259mil,-1519.234mil) on Top Layer Location : [X = 981.039mil][Y = 1607.986mil] Waived by Brandon Velasquez at 4/10/2026 9:47:22 PM
Short-Circuit Constraint: Between Region (0 hole(s)) Top Layer And Track (663.259mil,-1543.365mil)(663.259mil,-1519.234mil) on Top Layer Location : [X = 983.259mil][Y = 1601.85mil] Waived by Brandon Velasquez at 4/10/2026 9:47:24 PM
Short-Circuit Constraint: Between Region (0 hole(s)) Top Layer And Track (663.259mil,-1543.365mil)(672.046mil,-1552.152mil) on Top Layer Location : [X = 983.366mil][Y = 1589.785mil] Waived by Brandon Velasquez at 4/10/2026 9:47:26 PM
Short-Circuit Constraint: Between Region (0 hole(s)) Top Layer And Track (69.637mil,-1359.881mil)(89.756mil,-1380mil) on Top Layer Location : [X = 381.488mil][Y = 1765.012mil] Waived by Brandon Velasquez at 4/10/2026 9:46:23 PM
Short-Circuit Constraint: Between Region (0 hole(s)) Top Layer And Track (717.757mil,-1554.3mil)(728.692mil,-1543.365mil) on Top Layer Location : [X = 1048.585mil][Y = 1589.785mil] Waived by Brandon Velasquez at 4/10/2026 9:47:52 PM
Short-Circuit Constraint: Between Region (0 hole(s)) Top Layer And Track (728.692mil,-1529.222mil)(734.608mil,-1523.306mil) on Top Layer Location : [X = 1051.65mil][Y = 1599.814mil] Waived by Brandon Velasquez at 4/10/2026 9:47:51 PM
Short-Circuit Constraint: Between Region (0 hole(s)) Top Layer And Track (728.692mil,-1543.365mil)(728.692mil,-1529.222mil) on Top Layer Location : [X = 1048.692mil][Y = 1596.857mil] Waived by Brandon Velasquez at 4/10/2026 9:47:47 PM
Short-Circuit Constraint: Between Region (0 hole(s)) Top Layer And Track (734.608mil,-1373.028mil)(739.832mil,-1367.803mil) on Top Layer Location : [X = 1057.22mil][Y = 1754.584mil] Waived by Brandon Velasquez at 4/10/2026 9:48:08 PM
Short-Circuit Constraint: Between Region (0 hole(s)) Top Layer And Track (734.608mil,-1523.306mil)(734.608mil,-1516.236mil) on Top Layer Location : [X = 1054.608mil][Y = 1605.229mil] Waived by Brandon Velasquez at 4/10/2026 9:47:49 PM
Short-Circuit Constraint: Between Region (0 hole(s)) Top Layer And Track (739.832mil,-1367.803mil)(846.987mil,-1367.803mil) on Top Layer Location : [X = 1084.502mil][Y = 1757.197mil] Waived by Brandon Velasquez at 4/10/2026 9:48:02 PM
Short-Circuit Constraint: Between Region (0 hole(s)) Top Layer And Via (5310mil,-1535.931mil) from Top Layer to Bottom Layer Location : [X = 5630mil][Y = 1589.069mil] Waived by Brandon Velasquez at 4/10/2026 9:54:01 PM
Short-Circuit Constraint: Between Region (0 hole(s)) Top Layer And Via (658.82mil,-1398.126mil) from Top Layer to Bottom Layer Location : [X = 978.82mil][Y = 1726.874mil] Waived by Brandon Velasquez at 4/10/2026 9:47:02 PM
Short-Circuit Constraint: Between Region (0 hole(s)) Top Layer And Via (-75.601mil,-1429.754mil) from Top Layer to Bottom Layer Location : [X = 244.399mil][Y = 1695.246mil] Waived by Brandon Velasquez at 4/10/2026 9:46:44 PM

Back to top

Minimum Annular Ring (Minimum=4mil) (All)
Minimum Annular Ring: (No Ring) Pad J5-1(5400mil,860mil) on Multi-Layer (Annular Ring missing on Mid Layer 1) Waived by Brandon Velasquez at 4/6/2026 1:56:01 PM
Minimum Annular Ring: (No Ring) Pad J5-2(5500mil,960mil) on Multi-Layer (Annular Ring missing on Mid Layer 1) Waived by Brandon Velasquez at 4/6/2026 1:55:42 PM
Minimum Annular Ring: (No Ring) Pad J5-3(5300mil,960mil) on Multi-Layer (Annular Ring missing on Mid Layer 1) Waived by Brandon Velasquez at 4/6/2026 1:55:31 PM
Minimum Annular Ring: (No Ring) Pad J5-4(5300mil,760mil) on Multi-Layer (Annular Ring missing on Mid Layer 1) Waived by Brandon Velasquez at 4/6/2026 1:55:20 PM
Minimum Annular Ring: (No Ring) Pad J5-5(5500mil,760mil) on Multi-Layer (Annular Ring missing on Mid Layer 1) Waived by Brandon Velasquez at 4/6/2026 1:55:51 PM

Back to top

Hole Size Constraint (Min=10mil) (Max=265mil) (All)
Hole Size Constraint: (7.874mil < 10mil) Via (2851.692mil,1126.692mil) from Top Layer to Bottom Layer Actual Hole Size = 7.874mil Waived by Brandon Velasquez at 4/6/2026 10:32:27 PM
Hole Size Constraint: (7.874mil < 10mil) Via (2851.692mil,1170mil) from Top Layer to Bottom Layer Actual Hole Size = 7.874mil Waived by Brandon Velasquez at 4/6/2026 10:32:09 PM
Hole Size Constraint: (7.874mil < 10mil) Via (2851.692mil,1213.308mil) from Top Layer to Bottom Layer Actual Hole Size = 7.874mil Waived by Brandon Velasquez at 4/6/2026 10:31:11 PM
Hole Size Constraint: (7.874mil < 10mil) Via (2895mil,1126.692mil) from Top Layer to Bottom Layer Actual Hole Size = 7.874mil Waived by Brandon Velasquez at 4/6/2026 10:32:33 PM
Hole Size Constraint: (7.874mil < 10mil) Via (2895mil,1170mil) from Top Layer to Bottom Layer Actual Hole Size = 7.874mil Waived by Brandon Velasquez at 4/6/2026 10:32:15 PM
Hole Size Constraint: (7.874mil < 10mil) Via (2895mil,1213.308mil) from Top Layer to Bottom Layer Actual Hole Size = 7.874mil Waived by Brandon Velasquez at 4/6/2026 10:31:16 PM
Hole Size Constraint: (7.874mil < 10mil) Via (2938.308mil,1126.692mil) from Top Layer to Bottom Layer Actual Hole Size = 7.874mil Waived by Brandon Velasquez at 4/6/2026 10:32:39 PM
Hole Size Constraint: (7.874mil < 10mil) Via (2938.308mil,1170mil) from Top Layer to Bottom Layer Actual Hole Size = 7.874mil Waived by Brandon Velasquez at 4/6/2026 10:32:20 PM
Hole Size Constraint: (7.874mil < 10mil) Via (2938.308mil,1213.308mil) from Top Layer to Bottom Layer Actual Hole Size = 7.874mil Waived by Brandon Velasquez at 4/6/2026 10:31:21 PM

Back to top

Board Clearance Constraint (Gap=0mil) (All)
Board Outline Clearance(Outline Edge): (Collision < 15mil) Between Board Edge And Track (5545.944mil,730.5mil)(5866mil,730.5mil) on Top Overlay Waived by Brandon Velasquez at 4/6/2026 1:56:30 PM
Board Outline Clearance(Outline Edge): (Collision < 15mil) Between Board Edge And Track (5545.944mil,989.5mil)(5866mil,989.5mil) on Top Overlay Waived by Brandon Velasquez at 4/6/2026 1:56:22 PM
Board Outline Clearance(Outline Edge): (Collision < 15mil) Between Board Edge And Track (5866mil,730.5mil)(5866mil,989.5mil) on Top Overlay Waived by Brandon Velasquez at 4/6/2026 1:56:08 PM

Back to top