<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<board>
<plain>
<text>D1</text>
<text>D8</text>
<circle x="16.51" y="16.51" radius="14.986" width="0.0254" layer="20"/>
<text>GND</text>
<text>B2</text>
<text>B1</text>
<text>A2</text>
<text>A1</text>
<text>V+</text>
<text>SWITEC_X27.168_BREAKOUT_V1.1
https://tinyurl.com/mrd9ty5f 20251023</text>
<text>4</text>
<text>3</text>
<text>2</text>
<text>1</text>
</plain>
<libraries>
<library name="SparkFun-DiscreteSemi">
<description>&lt;h3&gt;SparkFun Discrete Semiconductors&lt;/h3&gt;
This library contains diodes, optoisolators, TRIACs, MOSFETs, transistors, etc. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="DIODE-1N4148">
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Connectors&lt;/h3&gt;
This library contains electrically-functional connectors. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X06">
<description>&lt;h3&gt;Plated Through Hole - 6 Pin&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:6&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_06&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="Pete's-Switec">
<description>&lt;h1&gt;&lt;strong&gt;Pete's Very Tasty EAGLE Library&lt;/strong&gt;&lt;/h1&gt;
&lt;p&gt;Most of these components have been tested but some have not.&lt;/p&gt;
&lt;p style="text-align: center;"&gt;&lt;span class="st"&gt;"doveryai no proveryai" (&lt;em&gt;trust&lt;/em&gt;, but &lt;em&gt;verify&lt;/em&gt;)&lt;br /&gt;-Russian Proverb&lt;br /&gt;&lt;/span&gt;&lt;/p&gt;
&lt;p style="text-align: center;"&gt;&lt;span class="st"&gt;"... whatever you do, do it all for the glory of God."&lt;br /&gt;1 Corinthians 10:31&lt;/span&gt;&lt;/p&gt;</description>
<packages>
<package name="X27.168">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="D1" library="SparkFun-DiscreteSemi" package="DIODE-1N4148" value="">
<attribute name="PROD_ID" value="DIO-08378"/>
<attribute name="VALUE"/>
</element>
<element name="D2" library="SparkFun-DiscreteSemi" package="DIODE-1N4148" value="">
<attribute name="PROD_ID" value="DIO-08378"/>
<attribute name="VALUE"/>
</element>
<element name="D3" library="SparkFun-DiscreteSemi" package="DIODE-1N4148" value="">
<attribute name="PROD_ID" value="DIO-08378"/>
<attribute name="VALUE"/>
</element>
<element name="D4" library="SparkFun-DiscreteSemi" package="DIODE-1N4148" value="">
<attribute name="PROD_ID" value="DIO-08378"/>
<attribute name="VALUE"/>
</element>
<element name="D5" library="SparkFun-DiscreteSemi" package="DIODE-1N4148" value="">
<attribute name="PROD_ID" value="DIO-08378"/>
<attribute name="VALUE"/>
</element>
<element name="D6" library="SparkFun-DiscreteSemi" package="DIODE-1N4148" value="">
<attribute name="PROD_ID" value="DIO-08378"/>
<attribute name="VALUE"/>
</element>
<element name="D7" library="SparkFun-DiscreteSemi" package="DIODE-1N4148" value="">
<attribute name="PROD_ID" value="DIO-08378"/>
<attribute name="VALUE"/>
</element>
<element name="D8" library="SparkFun-DiscreteSemi" package="DIODE-1N4148" value="">
<attribute name="PROD_ID" value="DIO-08378"/>
<attribute name="VALUE"/>
</element>
<element name="J1" library="SparkFun-Connectors" package="1X06" value="">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CONN-08437"/>
<attribute name="VALUE"/>
</element>
<element name="U$1" library="Pete's-Switec" package="X27.168" value=""/>
</elements>
<signals>
<signal name="VCC">
<contactref element="J1" pad="1"/>
<contactref element="D1" pad="C"/>
<contactref element="D3" pad="C"/>
<contactref element="D5" pad="C"/>
<contactref element="D7" pad="C"/>
</signal>
<signal name="A1">
<contactref element="D1" pad="A"/>
<contactref element="D2" pad="C"/>
<contactref element="J1" pad="2"/>
<contactref element="U$1" pad="P$1"/>
</signal>
<signal name="A2">
<contactref element="D3" pad="A"/>
<contactref element="D4" pad="C"/>
<contactref element="J1" pad="3"/>
<contactref element="U$1" pad="P$2"/>
</signal>
<signal name="B1">
<contactref element="D5" pad="A"/>
<contactref element="D6" pad="C"/>
<contactref element="J1" pad="4"/>
<contactref element="U$1" pad="P$3"/>
</signal>
<signal name="B2">
<contactref element="D8" pad="C"/>
<contactref element="D7" pad="A"/>
<contactref element="J1" pad="5"/>
<contactref element="U$1" pad="P$4"/>
</signal>
<signal name="GND">
<contactref element="J1" pad="6"/>
<contactref element="D2" pad="A"/>
<contactref element="D4" pad="A"/>
<contactref element="D8" pad="A"/>
<contactref element="D6" pad="A"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
